(export (version D)
  (design
    (source /home/eddy/Docs/SAO/ELECTRONICS/STM8/stepper/schematic/stepper.sch)
    (date "Ср 12 фев 2014 12:08:20")
    (tool "eeschema (2013-feb-26)-stable"))
  (components
    (comp (ref U1)
      (value STM8S105K4T6C)
      (libsource (lib stm8s105k4t6c) (part STM8S105K4T6C))
      (sheetpath (names /) (tstamps /))
      (tstamp 52FB03A2))
    (comp (ref C1)
      (value 1u)
      (libsource (lib device) (part C))
      (sheetpath (names /) (tstamps /))
      (tstamp 52FB0413))
    (comp (ref C2)
      (value 104)
      (libsource (lib device) (part C))
      (sheetpath (names /) (tstamps /))
      (tstamp 52FB0426))
    (comp (ref P2)
      (value CONN_4)
      (libsource (lib conn) (part CONN_4))
      (sheetpath (names /) (tstamps /))
      (tstamp 52FB0A49))
    (comp (ref P1)
      (value CONN_14)
      (libsource (lib conn) (part CONN_14))
      (sheetpath (names /) (tstamps /))
      (tstamp 52FB0A6A))
    (comp (ref P3)
      (value CONN_14)
      (libsource (lib conn) (part CONN_14))
      (sheetpath (names /) (tstamps /))
      (tstamp 52FB0A79))
    (comp (ref D1)
      (value LED)
      (libsource (lib device) (part LED))
      (sheetpath (names /) (tstamps /))
      (tstamp 52FB0DD3))
    (comp (ref R1)
      (value 1k)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 52FB0DE2))
    (comp (ref D2)
      (value LED)
      (libsource (lib device) (part LED))
      (sheetpath (names /) (tstamps /))
      (tstamp 52FB0ECD))
    (comp (ref R2)
      (value 1k)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 52FB0ED3))
    (comp (ref R3)
      (value 10k)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 52FB0EFD))
    (comp (ref SW1)
      (value SW_PUSH)
      (libsource (lib device) (part SW_PUSH))
      (sheetpath (names /) (tstamps /))
      (tstamp 52FB0F3B))
    (comp (ref C3)
      (value 104)
      (libsource (lib device) (part C))
      (sheetpath (names /) (tstamps /))
      (tstamp 52FB0F99))
    (comp (ref P4)
      (value CONN_5)
      (libsource (lib conn) (part CONN_6))
      (sheetpath (names /) (tstamps /))
      (tstamp 52FB29A7))
    (comp (ref K1)
      (value CONN_3)
      (libsource (lib conn) (part CONN_3))
      (sheetpath (names /) (tstamps /))
      (tstamp 52FB2C32)))
  (libparts
    (libpart (lib device) (part C)
      (description "Condensateur non polarise")
      (footprints
        (fp SM*)
        (fp C?)
        (fp C1-1))
      (fields
        (field (name Reference) C)
        (field (name Value) C)
        (field (name Footprint) ~)
        (field (name Datasheet) ~))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib device) (part LED)
      (footprints
        (fp LED-3MM)
        (fp LED-5MM)
        (fp LED-10MM)
        (fp LED-0603)
        (fp LED-0805)
        (fp LED-1206)
        (fp LEDV))
      (fields
        (field (name Reference) D)
        (field (name Value) LED)
        (field (name Footprint) ~)
        (field (name Datasheet) ~))
      (pins
        (pin (num 1) (name A) (type passive))
        (pin (num 2) (name K) (type passive))))
    (libpart (lib device) (part R)
      (description Resistance)
      (footprints
        (fp R?)
        (fp SM0603)
        (fp SM0805)
        (fp R?-*)
        (fp SM1206))
      (fields
        (field (name Reference) R)
        (field (name Value) R)
        (field (name Footprint) ~)
        (field (name Datasheet) ~))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib device) (part SW_PUSH)
      (description "Push Button")
      (fields
        (field (name Reference) SW)
        (field (name Value) SW_PUSH)
        (field (name Footprint) ~)
        (field (name Datasheet) ~))
      (pins
        (pin (num 1) (name 1) (type passive))
        (pin (num 2) (name 2) (type passive))))
    (libpart (lib conn) (part CONN_14)
      (description "Symbole general de connexion")
      (fields
        (field (name Reference) P)
        (field (name Value) CONN_14))
      (pins
        (pin (num 1) (name P1) (type passive))
        (pin (num 2) (name P2) (type passive))
        (pin (num 3) (name P3) (type passive))
        (pin (num 4) (name P4) (type passive))
        (pin (num 5) (name P5) (type passive))
        (pin (num 6) (name P6) (type passive))
        (pin (num 7) (name P7) (type passive))
        (pin (num 8) (name P8) (type passive))
        (pin (num 9) (name P9) (type passive))
        (pin (num 10) (name P10) (type passive))
        (pin (num 11) (name P11) (type passive))
        (pin (num 12) (name P12) (type passive))
        (pin (num 13) (name P13) (type passive))
        (pin (num 14) (name P14) (type passive))))
    (libpart (lib conn) (part CONN_3)
      (description "Symbole general de connecteur")
      (fields
        (field (name Reference) K)
        (field (name Value) CONN_3))
      (pins
        (pin (num 1) (name P1) (type passive))
        (pin (num 2) (name PM) (type passive))
        (pin (num 3) (name P3) (type passive))))
    (libpart (lib conn) (part CONN_4)
      (description "Symbole general de connecteur")
      (fields
        (field (name Reference) P)
        (field (name Value) CONN_4))
      (pins
        (pin (num 1) (name P1) (type passive))
        (pin (num 2) (name P2) (type passive))
        (pin (num 3) (name P3) (type passive))
        (pin (num 4) (name P4) (type passive))))
    (libpart (lib conn) (part CONN_6)
      (description "ymbole general de connecteur")
      (fields
        (field (name Reference) P)
        (field (name Value) CONN_6))
      (pins
        (pin (num 1) (name 1) (type passive))
        (pin (num 2) (name 2) (type passive))
        (pin (num 3) (name 3) (type passive))
        (pin (num 4) (name 4) (type passive))
        (pin (num 5) (name 5) (type passive))
        (pin (num 6) (name 6) (type passive))))
    (libpart (lib stm8s105k4t6c) (part STM8S105K4T6C)
      (footprints
        (fp lqfp32*))
      (fields
        (field (name Reference) U)
        (field (name Value) STM8S105K4T6C)
        (field (name Footprint) ~)
        (field (name Datasheet) ~))
      (pins
        (pin (num 1) (name NRST) (type input))
        (pin (num 2) (name OSCIN/PA1) (type 3state))
        (pin (num 3) (name OSCOUT/PA2) (type 3state))
        (pin (num 4) (name VSS) (type power_in))
        (pin (num 5) (name VCAP) (type power_out))
        (pin (num 6) (name "VDD(3.3-5v)") (type power_in))
        (pin (num 7) (name VDDio) (type power_in))
        (pin (num 8) (name PF4/AIN12) (type 3state))
        (pin (num 9) (name VDDA) (type power_in))
        (pin (num 10) (name VSSA) (type power_in))
        (pin (num 11) (name PB5/AIN5[I2X_SDA]) (type 3state))
        (pin (num 12) (name PB4/AIN4[I2C_SCL]) (type 3state))
        (pin (num 13) (name PB3/AIN3[TIM1_ETR]) (type 3state))
        (pin (num 14) (name PB2/AIN2[TIM1_CH3N]) (type 3state))
        (pin (num 15) (name PB1/AIN1_[TIM1_CH2N]) (type 3state))
        (pin (num 16) (name PB0/AIN0_[TIM1_CH1N]) (type 3state))
        (pin (num 17) (name PE5/SPI_NSS) (type 3state))
        (pin (num 18) (name "PC1(HS)/TIM1_CH1") (type 3state))
        (pin (num 19) (name "PC2(HS)/TIM1_CH2") (type 3state))
        (pin (num 20) (name "PC3(HS)/TIM1_CH3") (type 3state))
        (pin (num 21) (name "PC4(HS)/TIM1_CH4") (type 3state))
        (pin (num 22) (name "PC5(HS)/SPI_SCK") (type 3state))
        (pin (num 23) (name "PC6(HS)/SPI_MOSI") (type 3state))
        (pin (num 24) (name "PC7(HS)/SPI_MISO") (type 3state))
        (pin (num 25) (name "PD0(HS)/TIM3_CH2[TIM1_BKIN][CLK_CCO]") (type 3state))
        (pin (num 26) (name "PD1(HS)/SWIM") (type 3state))
        (pin (num 27) (name "PD2(HS)/TIM3_CH1[TIM2_CH3]") (type 3state))
        (pin (num 28) (name "PD3(HS)/TIM2_CH2[ADC_ETR]") (type 3state))
        (pin (num 29) (name "PD4(HS)/TIM2_CH1[BEEP]") (type 3state))
        (pin (num 30) (name PD5/UART2_TX) (type 3state))
        (pin (num 31) (name PD6/UART2_RX) (type 3state))
        (pin (num 32) (name PD7/TLI[TIM1_CH4]) (type 3state)))))
  (libraries
    (library (logical device)
      (uri /usr/share/kicad/library/device.lib))
    (library (logical conn)
      (uri /usr/share/kicad/library/conn.lib))
    (library (logical stm8s105k4t6c)
      (uri stm8s105k4t6c.lib)))
  (nets
    (net (code 1) (name +3.3V)
      (node (ref R3) (pin 1))
      (node (ref U1) (pin 6))
      (node (ref C2) (pin 2))
      (node (ref D1) (pin 1))
      (node (ref P2) (pin 1))
      (node (ref D2) (pin 1))
      (node (ref P1) (pin 1))
      (node (ref U1) (pin 7))
      (node (ref U1) (pin 9))
      (node (ref K1) (pin 1)))
    (net (code 2) (name "")
      (node (ref D1) (pin 2))
      (node (ref R1) (pin 1)))
    (net (code 3) (name "")
      (node (ref R2) (pin 1))
      (node (ref D2) (pin 2)))
    (net (code 4) (name GND)
      (node (ref C1) (pin 1))
      (node (ref SW1) (pin 1))
      (node (ref C3) (pin 2))
      (node (ref R2) (pin 2))
      (node (ref P2) (pin 4))
      (node (ref P1) (pin 2))
      (node (ref U1) (pin 10))
      (node (ref U1) (pin 4))
      (node (ref C2) (pin 1))
      (node (ref P4) (pin 6)))
    (net (code 5) (name /PC2)
      (node (ref R1) (pin 2))
      (node (ref U1) (pin 19))
      (node (ref P3) (pin 14)))
    (net (code 6) (name "")
      (node (ref U1) (pin 5))
      (node (ref C1) (pin 2)))
    (net (code 7) (name /PC1)
      (node (ref P1) (pin 14))
      (node (ref U1) (pin 18)))
    (net (code 8) (name /OSC1IN)
      (node (ref U1) (pin 2))
      (node (ref P1) (pin 4)))
    (net (code 9) (name /OSC2IN)
      (node (ref P1) (pin 5))
      (node (ref U1) (pin 3)))
    (net (code 10) (name /PF4)
      (node (ref P1) (pin 6))
      (node (ref U1) (pin 8)))
    (net (code 11) (name /PB5)
      (node (ref U1) (pin 11))
      (node (ref P1) (pin 7))
      (node (ref K1) (pin 2)))
    (net (code 12) (name /PB4)
      (node (ref U1) (pin 12))
      (node (ref P4) (pin 5))
      (node (ref P1) (pin 8)))
    (net (code 13) (name /PB3)
      (node (ref U1) (pin 13))
      (node (ref P1) (pin 9))
      (node (ref P4) (pin 4)))
    (net (code 14) (name /PB2)
      (node (ref P1) (pin 10))
      (node (ref P4) (pin 3))
      (node (ref U1) (pin 14)))
    (net (code 15) (name /PB1)
      (node (ref P4) (pin 2))
      (node (ref P1) (pin 11))
      (node (ref U1) (pin 15)))
    (net (code 16) (name /PB0)
      (node (ref P4) (pin 1))
      (node (ref U1) (pin 16))
      (node (ref P1) (pin 12)))
    (net (code 17) (name /PE5)
      (node (ref U1) (pin 17))
      (node (ref P1) (pin 13)))
    (net (code 18) (name /PD7)
      (node (ref U1) (pin 32))
      (node (ref P3) (pin 1)))
    (net (code 19) (name /PD6)
      (node (ref P3) (pin 2))
      (node (ref U1) (pin 31)))
    (net (code 20) (name /PD5)
      (node (ref U1) (pin 30))
      (node (ref P3) (pin 3)))
    (net (code 21) (name /PD4)
      (node (ref K1) (pin 3))
      (node (ref U1) (pin 29))
      (node (ref P3) (pin 4)))
    (net (code 22) (name /PD3)
      (node (ref U1) (pin 28))
      (node (ref P3) (pin 5)))
    (net (code 23) (name /PD2)
      (node (ref P3) (pin 6))
      (node (ref U1) (pin 27)))
    (net (code 24) (name /PD0)
      (node (ref U1) (pin 25))
      (node (ref P3) (pin 8)))
    (net (code 25) (name /PC7)
      (node (ref U1) (pin 24))
      (node (ref P3) (pin 9)))
    (net (code 26) (name /PC6)
      (node (ref P3) (pin 10))
      (node (ref U1) (pin 23)))
    (net (code 27) (name /PC5)
      (node (ref P3) (pin 11))
      (node (ref U1) (pin 22)))
    (net (code 28) (name /PC4)
      (node (ref U1) (pin 21))
      (node (ref P3) (pin 12)))
    (net (code 29) (name /PC3)
      (node (ref P3) (pin 13))
      (node (ref U1) (pin 20)))
    (net (code 30) (name /SWIM/PD1)
      (node (ref P2) (pin 2))
      (node (ref U1) (pin 26))
      (node (ref P3) (pin 7)))
    (net (code 31) (name /NRST)
      (node (ref R3) (pin 2))
      (node (ref P2) (pin 3))
      (node (ref SW1) (pin 2))
      (node (ref P1) (pin 3))
      (node (ref C3) (pin 1))
      (node (ref U1) (pin 1)))))