(kicad_pcb (version 3) (host pcbnew "(2013-feb-26)-stable")

  (general
    (links 70)
    (no_connects 70)
    (area 0 0 0 0)
    (thickness 1.6)
    (drawings 0)
    (tracks 0)
    (zones 0)
    (modules 15)
    (nets 32)
  )

  (page A3)
  (layers
    (15 F.Cu signal)
    (0 B.Cu signal)
    (16 B.Adhes user)
    (17 F.Adhes user)
    (18 B.Paste user)
    (19 F.Paste user)
    (20 B.SilkS user)
    (21 F.SilkS user)
    (22 B.Mask user)
    (23 F.Mask user)
    (24 Dwgs.User user)
    (25 Cmts.User user)
    (26 Eco1.User user)
    (27 Eco2.User user)
    (28 Edge.Cuts user)
  )

  (setup
    (last_trace_width 0.254)
    (trace_clearance 0.254)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.254)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.889)
    (via_drill 0.635)
    (via_min_size 0.889)
    (via_min_drill 0.508)
    (uvia_size 0.508)
    (uvia_drill 0.127)
    (uvias_allowed no)
    (uvia_min_size 0.508)
    (uvia_min_drill 0.127)
    (pcb_text_width 0.3)
    (pcb_text_size 1 1)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1 1)
    (pad_drill 0.6)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFFBF)
    (pcbplotparams
      (layerselection 3178497)
      (usegerberextensions true)
      (excludeedgelayer true)
      (linewidth 152400)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotothertext true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )

  (net 0 "")
  (net 1 +3.3V)
  (net 2 "/A DIR")
  (net 3 /NRST)
  (net 4 /OSC1IN)
  (net 5 /OSC2IN)
  (net 6 /PB0)
  (net 7 /PB1)
  (net 8 /PB2)
  (net 9 /PB4)
  (net 10 /PB5)
  (net 11 /PC1)
  (net 12 /PC2)
  (net 13 /PC3)
  (net 14 /PC4)
  (net 15 /PC5)
  (net 16 /PC6)
  (net 17 /PC7)
  (net 18 /PD0)
  (net 19 /PD2)
  (net 20 /PD3)
  (net 21 /PD4)
  (net 22 /PD5)
  (net 23 /PD6)
  (net 24 /PD7)
  (net 25 /PE5)
  (net 26 /PF4)
  (net 27 /SWIM/PD1)
  (net 28 GND)
  (net 29 N-0000021)
  (net 30 N-0000026)
  (net 31 N-0000042)

  (net_class Default "This is the default net class."
    (clearance 0.254)
    (trace_width 0.254)
    (via_dia 0.889)
    (via_drill 0.635)
    (uvia_dia 0.508)
    (uvia_drill 0.127)
    (add_net "")
    (add_net +3.3V)
    (add_net "/A DIR")
    (add_net /NRST)
    (add_net /OSC1IN)
    (add_net /OSC2IN)
    (add_net /PB0)
    (add_net /PB1)
    (add_net /PB2)
    (add_net /PB4)
    (add_net /PB5)
    (add_net /PC1)
    (add_net /PC2)
    (add_net /PC3)
    (add_net /PC4)
    (add_net /PC5)
    (add_net /PC6)
    (add_net /PC7)
    (add_net /PD0)
    (add_net /PD2)
    (add_net /PD3)
    (add_net /PD4)
    (add_net /PD5)
    (add_net /PD6)
    (add_net /PD7)
    (add_net /PE5)
    (add_net /PF4)
    (add_net /SWIM/PD1)
    (add_net GND)
    (add_net N-0000021)
    (add_net N-0000026)
    (add_net N-0000042)
  )

  (module TQFP32 (layer F.Cu) (tedit 43A670DA) (tstamp 52FB46F3)
    (at 239.268 53.34)
    (path /52FB03A2)
    (fp_text reference U1 (at 0 -1.27) (layer F.SilkS)
      (effects (font (size 1.27 1.016) (thickness 0.2032)))
    )
    (fp_text value STM8S105K4T6C (at 0 1.905) (layer F.SilkS)
      (effects (font (size 1.27 1.016) (thickness 0.2032)))
    )
    (fp_line (start 5.0292 2.7686) (end 3.8862 2.7686) (layer F.SilkS) (width 0.1524))
    (fp_line (start 5.0292 -2.7686) (end 3.9116 -2.7686) (layer F.SilkS) (width 0.1524))
    (fp_line (start 5.0292 2.7686) (end 5.0292 -2.7686) (layer F.SilkS) (width 0.1524))
    (fp_line (start 2.794 3.9624) (end 2.794 5.0546) (layer F.SilkS) (width 0.1524))
    (fp_line (start -2.8194 3.9878) (end -2.8194 5.0546) (layer F.SilkS) (width 0.1524))
    (fp_line (start -2.8448 5.0546) (end 2.794 5.08) (layer F.SilkS) (width 0.1524))
    (fp_line (start -2.794 -5.0292) (end 2.7178 -5.0546) (layer F.SilkS) (width 0.1524))
    (fp_line (start -3.8862 -3.2766) (end -3.8862 3.9116) (layer F.SilkS) (width 0.1524))
    (fp_line (start 2.7432 -5.0292) (end 2.7432 -3.9878) (layer F.SilkS) (width 0.1524))
    (fp_line (start -3.2512 -3.8862) (end 3.81 -3.8862) (layer F.SilkS) (width 0.1524))
    (fp_line (start 3.8608 3.937) (end 3.8608 -3.7846) (layer F.SilkS) (width 0.1524))
    (fp_line (start -3.8862 3.937) (end 3.7338 3.937) (layer F.SilkS) (width 0.1524))
    (fp_line (start -5.0292 -2.8448) (end -5.0292 2.794) (layer F.SilkS) (width 0.1524))
    (fp_line (start -5.0292 2.794) (end -3.8862 2.794) (layer F.SilkS) (width 0.1524))
    (fp_line (start -3.87604 -3.302) (end -3.29184 -3.8862) (layer F.SilkS) (width 0.1524))
    (fp_line (start -5.02412 -2.8448) (end -3.87604 -2.8448) (layer F.SilkS) (width 0.1524))
    (fp_line (start -2.794 -3.8862) (end -2.794 -5.03428) (layer F.SilkS) (width 0.1524))
    (fp_circle (center -2.83972 -2.86004) (end -2.43332 -2.60604) (layer F.SilkS) (width 0.1524))
    (pad 8 smd rect (at -4.81584 2.77622) (size 1.99898 0.44958)
      (layers F.Cu F.Paste F.Mask)
      (net 26 /PF4)
    )
    (pad 7 smd rect (at -4.81584 1.97612) (size 1.99898 0.44958)
      (layers F.Cu F.Paste F.Mask)
      (net 1 +3.3V)
    )
    (pad 6 smd rect (at -4.81584 1.17602) (size 1.99898 0.44958)
      (layers F.Cu F.Paste F.Mask)
      (net 1 +3.3V)
    )
    (pad 5 smd rect (at -4.81584 0.37592) (size 1.99898 0.44958)
      (layers F.Cu F.Paste F.Mask)
      (net 30 N-0000026)
    )
    (pad 4 smd rect (at -4.81584 -0.42418) (size 1.99898 0.44958)
      (layers F.Cu F.Paste F.Mask)
      (net 28 GND)
    )
    (pad 3 smd rect (at -4.81584 -1.22428) (size 1.99898 0.44958)
      (layers F.Cu F.Paste F.Mask)
      (net 5 /OSC2IN)
    )
    (pad 2 smd rect (at -4.81584 -2.02438) (size 1.99898 0.44958)
      (layers F.Cu F.Paste F.Mask)
      (net 4 /OSC1IN)
    )
    (pad 1 smd rect (at -4.81584 -2.82448) (size 1.99898 0.44958)
      (layers F.Cu F.Paste F.Mask)
      (net 3 /NRST)
    )
    (pad 24 smd rect (at 4.7498 -2.8194) (size 1.99898 0.44958)
      (layers F.Cu F.Paste F.Mask)
      (net 17 /PC7)
    )
    (pad 17 smd rect (at 4.7498 2.794) (size 1.99898 0.44958)
      (layers F.Cu F.Paste F.Mask)
      (net 25 /PE5)
    )
    (pad 18 smd rect (at 4.7498 1.9812) (size 1.99898 0.44958)
      (layers F.Cu F.Paste F.Mask)
      (net 11 /PC1)
    )
    (pad 19 smd rect (at 4.7498 1.1684) (size 1.99898 0.44958)
      (layers F.Cu F.Paste F.Mask)
      (net 12 /PC2)
    )
    (pad 20 smd rect (at 4.7498 0.381) (size 1.99898 0.44958)
      (layers F.Cu F.Paste F.Mask)
      (net 13 /PC3)
    )
    (pad 21 smd rect (at 4.7498 -0.4318) (size 1.99898 0.44958)
      (layers F.Cu F.Paste F.Mask)
      (net 14 /PC4)
    )
    (pad 22 smd rect (at 4.7498 -1.2192) (size 1.99898 0.44958)
      (layers F.Cu F.Paste F.Mask)
      (net 15 /PC5)
    )
    (pad 23 smd rect (at 4.7498 -2.032) (size 1.99898 0.44958)
      (layers F.Cu F.Paste F.Mask)
      (net 16 /PC6)
    )
    (pad 32 smd rect (at -2.82448 -4.826) (size 0.44958 1.99898)
      (layers F.Cu F.Paste F.Mask)
      (net 24 /PD7)
    )
    (pad 31 smd rect (at -2.02692 -4.826) (size 0.44958 1.99898)
      (layers F.Cu F.Paste F.Mask)
      (net 23 /PD6)
    )
    (pad 30 smd rect (at -1.22428 -4.826) (size 0.44958 1.99898)
      (layers F.Cu F.Paste F.Mask)
      (net 22 /PD5)
    )
    (pad 29 smd rect (at -0.42672 -4.826) (size 0.44958 1.99898)
      (layers F.Cu F.Paste F.Mask)
      (net 21 /PD4)
    )
    (pad 28 smd rect (at 0.37592 -4.826) (size 0.44958 1.99898)
      (layers F.Cu F.Paste F.Mask)
      (net 20 /PD3)
    )
    (pad 27 smd rect (at 1.17348 -4.826) (size 0.44958 1.99898)
      (layers F.Cu F.Paste F.Mask)
      (net 19 /PD2)
    )
    (pad 26 smd rect (at 1.97612 -4.826) (size 0.44958 1.99898)
      (layers F.Cu F.Paste F.Mask)
      (net 27 /SWIM/PD1)
    )
    (pad 25 smd rect (at 2.77368 -4.826) (size 0.44958 1.99898)
      (layers F.Cu F.Paste F.Mask)
      (net 18 /PD0)
    )
    (pad 9 smd rect (at -2.8194 4.7752) (size 0.44958 1.99898)
      (layers F.Cu F.Paste F.Mask)
      (net 1 +3.3V)
    )
    (pad 10 smd rect (at -2.032 4.7752) (size 0.44958 1.99898)
      (layers F.Cu F.Paste F.Mask)
      (net 28 GND)
    )
    (pad 11 smd rect (at -1.2192 4.7752) (size 0.44958 1.99898)
      (layers F.Cu F.Paste F.Mask)
      (net 10 /PB5)
    )
    (pad 12 smd rect (at -0.4318 4.7752) (size 0.44958 1.99898)
      (layers F.Cu F.Paste F.Mask)
      (net 9 /PB4)
    )
    (pad 13 smd rect (at 0.3556 4.7752) (size 0.44958 1.99898)
      (layers F.Cu F.Paste F.Mask)
      (net 2 "/A DIR")
    )
    (pad 14 smd rect (at 1.1684 4.7752) (size 0.44958 1.99898)
      (layers F.Cu F.Paste F.Mask)
      (net 8 /PB2)
    )
    (pad 15 smd rect (at 1.9812 4.7752) (size 0.44958 1.99898)
      (layers F.Cu F.Paste F.Mask)
      (net 7 /PB1)
    )
    (pad 16 smd rect (at 2.794 4.7752) (size 0.44958 1.99898)
      (layers F.Cu F.Paste F.Mask)
      (net 6 /PB0)
    )
    (model smd/tqfp32.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module SM2010 (layer F.Cu) (tedit 4EFC4DD5) (tstamp 52FB4700)
    (at 207.518 73.66)
    (tags "CMS SM")
    (path /52FB0F3B)
    (attr smd)
    (fp_text reference SW1 (at -0.50038 0 90) (layer F.SilkS)
      (effects (font (size 0.70104 0.70104) (thickness 0.127)))
    )
    (fp_text value SW_PUSH (at 0.8001 0 90) (layer F.SilkS)
      (effects (font (size 0.70104 0.70104) (thickness 0.127)))
    )
    (fp_line (start 3.50012 -1.6002) (end 3.50012 1.6002) (layer F.SilkS) (width 0.11938))
    (fp_line (start -3.50012 -1.6002) (end -3.50012 1.6002) (layer F.SilkS) (width 0.11938))
    (fp_text user + (at -4.30022 1.80086) (layer F.SilkS)
      (effects (font (size 1.524 1.524) (thickness 0.29972)))
    )
    (fp_line (start 1.19634 1.60528) (end 3.48234 1.60528) (layer F.SilkS) (width 0.11938))
    (fp_line (start 3.48234 -1.60528) (end 1.19634 -1.60528) (layer F.SilkS) (width 0.11938))
    (fp_line (start -1.19888 -1.60528) (end -3.48488 -1.60528) (layer F.SilkS) (width 0.11938))
    (fp_line (start -3.48488 1.60528) (end -1.19888 1.60528) (layer F.SilkS) (width 0.11938))
    (pad 1 smd rect (at -2.4003 0) (size 1.80086 2.70002)
      (layers F.Cu F.Paste F.Mask)
      (net 28 GND)
    )
    (pad 2 smd rect (at 2.4003 0) (size 1.80086 2.70002)
      (layers F.Cu F.Paste F.Mask)
      (net 3 /NRST)
    )
    (model smd\chip_smd_pol_wide.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.35 0.35 0.35))
      (rotate (xyz 0 0 0))
    )
  )

  (module SM1206 (layer F.Cu) (tedit 42806E24) (tstamp 52FB470C)
    (at 214.884 73.406)
    (path /52FB0413)
    (attr smd)
    (fp_text reference C1 (at 0 0) (layer F.SilkS)
      (effects (font (size 0.762 0.762) (thickness 0.127)))
    )
    (fp_text value 1u (at 0 0) (layer F.SilkS) hide
      (effects (font (size 0.762 0.762) (thickness 0.127)))
    )
    (fp_line (start -2.54 -1.143) (end -2.54 1.143) (layer F.SilkS) (width 0.127))
    (fp_line (start -2.54 1.143) (end -0.889 1.143) (layer F.SilkS) (width 0.127))
    (fp_line (start 0.889 -1.143) (end 2.54 -1.143) (layer F.SilkS) (width 0.127))
    (fp_line (start 2.54 -1.143) (end 2.54 1.143) (layer F.SilkS) (width 0.127))
    (fp_line (start 2.54 1.143) (end 0.889 1.143) (layer F.SilkS) (width 0.127))
    (fp_line (start -0.889 -1.143) (end -2.54 -1.143) (layer F.SilkS) (width 0.127))
    (pad 1 smd rect (at -1.651 0) (size 1.524 2.032)
      (layers F.Cu F.Paste F.Mask)
      (net 28 GND)
    )
    (pad 2 smd rect (at 1.651 0) (size 1.524 2.032)
      (layers F.Cu F.Paste F.Mask)
      (net 30 N-0000026)
    )
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.17 0.16 0.16))
      (rotate (xyz 0 0 0))
    )
  )

  (module SM1206 (layer F.Cu) (tedit 42806E24) (tstamp 52FB4718)
    (at 220.98 73.406)
    (path /52FB0426)
    (attr smd)
    (fp_text reference C2 (at 0 0) (layer F.SilkS)
      (effects (font (size 0.762 0.762) (thickness 0.127)))
    )
    (fp_text value 104 (at 0 0) (layer F.SilkS) hide
      (effects (font (size 0.762 0.762) (thickness 0.127)))
    )
    (fp_line (start -2.54 -1.143) (end -2.54 1.143) (layer F.SilkS) (width 0.127))
    (fp_line (start -2.54 1.143) (end -0.889 1.143) (layer F.SilkS) (width 0.127))
    (fp_line (start 0.889 -1.143) (end 2.54 -1.143) (layer F.SilkS) (width 0.127))
    (fp_line (start 2.54 -1.143) (end 2.54 1.143) (layer F.SilkS) (width 0.127))
    (fp_line (start 2.54 1.143) (end 0.889 1.143) (layer F.SilkS) (width 0.127))
    (fp_line (start -0.889 -1.143) (end -2.54 -1.143) (layer F.SilkS) (width 0.127))
    (pad 1 smd rect (at -1.651 0) (size 1.524 2.032)
      (layers F.Cu F.Paste F.Mask)
      (net 28 GND)
    )
    (pad 2 smd rect (at 1.651 0) (size 1.524 2.032)
      (layers F.Cu F.Paste F.Mask)
      (net 1 +3.3V)
    )
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.17 0.16 0.16))
      (rotate (xyz 0 0 0))
    )
  )

  (module SM1206 (layer F.Cu) (tedit 42806E24) (tstamp 52FB4724)
    (at 227.076 73.406)
    (path /52FB0DD3)
    (attr smd)
    (fp_text reference D1 (at 0 0) (layer F.SilkS)
      (effects (font (size 0.762 0.762) (thickness 0.127)))
    )
    (fp_text value LED (at 0 0) (layer F.SilkS) hide
      (effects (font (size 0.762 0.762) (thickness 0.127)))
    )
    (fp_line (start -2.54 -1.143) (end -2.54 1.143) (layer F.SilkS) (width 0.127))
    (fp_line (start -2.54 1.143) (end -0.889 1.143) (layer F.SilkS) (width 0.127))
    (fp_line (start 0.889 -1.143) (end 2.54 -1.143) (layer F.SilkS) (width 0.127))
    (fp_line (start 2.54 -1.143) (end 2.54 1.143) (layer F.SilkS) (width 0.127))
    (fp_line (start 2.54 1.143) (end 0.889 1.143) (layer F.SilkS) (width 0.127))
    (fp_line (start -0.889 -1.143) (end -2.54 -1.143) (layer F.SilkS) (width 0.127))
    (pad 1 smd rect (at -1.651 0) (size 1.524 2.032)
      (layers F.Cu F.Paste F.Mask)
      (net 1 +3.3V)
    )
    (pad 2 smd rect (at 1.651 0) (size 1.524 2.032)
      (layers F.Cu F.Paste F.Mask)
      (net 31 N-0000042)
    )
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.17 0.16 0.16))
      (rotate (xyz 0 0 0))
    )
  )

  (module SM1206 (layer F.Cu) (tedit 42806E24) (tstamp 52FB4730)
    (at 233.172 73.406)
    (path /52FB0DE2)
    (attr smd)
    (fp_text reference R1 (at 0 0) (layer F.SilkS)
      (effects (font (size 0.762 0.762) (thickness 0.127)))
    )
    (fp_text value 1k (at 0 0) (layer F.SilkS) hide
      (effects (font (size 0.762 0.762) (thickness 0.127)))
    )
    (fp_line (start -2.54 -1.143) (end -2.54 1.143) (layer F.SilkS) (width 0.127))
    (fp_line (start -2.54 1.143) (end -0.889 1.143) (layer F.SilkS) (width 0.127))
    (fp_line (start 0.889 -1.143) (end 2.54 -1.143) (layer F.SilkS) (width 0.127))
    (fp_line (start 2.54 -1.143) (end 2.54 1.143) (layer F.SilkS) (width 0.127))
    (fp_line (start 2.54 1.143) (end 0.889 1.143) (layer F.SilkS) (width 0.127))
    (fp_line (start -0.889 -1.143) (end -2.54 -1.143) (layer F.SilkS) (width 0.127))
    (pad 1 smd rect (at -1.651 0) (size 1.524 2.032)
      (layers F.Cu F.Paste F.Mask)
      (net 31 N-0000042)
    )
    (pad 2 smd rect (at 1.651 0) (size 1.524 2.032)
      (layers F.Cu F.Paste F.Mask)
      (net 12 /PC2)
    )
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.17 0.16 0.16))
      (rotate (xyz 0 0 0))
    )
  )

  (module SM1206 (layer F.Cu) (tedit 42806E24) (tstamp 52FB473C)
    (at 182.626 76.962)
    (path /52FB0ECD)
    (attr smd)
    (fp_text reference D2 (at 0 0) (layer F.SilkS)
      (effects (font (size 0.762 0.762) (thickness 0.127)))
    )
    (fp_text value LED (at 0 0) (layer F.SilkS) hide
      (effects (font (size 0.762 0.762) (thickness 0.127)))
    )
    (fp_line (start -2.54 -1.143) (end -2.54 1.143) (layer F.SilkS) (width 0.127))
    (fp_line (start -2.54 1.143) (end -0.889 1.143) (layer F.SilkS) (width 0.127))
    (fp_line (start 0.889 -1.143) (end 2.54 -1.143) (layer F.SilkS) (width 0.127))
    (fp_line (start 2.54 -1.143) (end 2.54 1.143) (layer F.SilkS) (width 0.127))
    (fp_line (start 2.54 1.143) (end 0.889 1.143) (layer F.SilkS) (width 0.127))
    (fp_line (start -0.889 -1.143) (end -2.54 -1.143) (layer F.SilkS) (width 0.127))
    (pad 1 smd rect (at -1.651 0) (size 1.524 2.032)
      (layers F.Cu F.Paste F.Mask)
      (net 1 +3.3V)
    )
    (pad 2 smd rect (at 1.651 0) (size 1.524 2.032)
      (layers F.Cu F.Paste F.Mask)
      (net 29 N-0000021)
    )
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.17 0.16 0.16))
      (rotate (xyz 0 0 0))
    )
  )

  (module SM1206 (layer F.Cu) (tedit 42806E24) (tstamp 52FB4748)
    (at 188.722 76.962)
    (path /52FB0ED3)
    (attr smd)
    (fp_text reference R2 (at 0 0) (layer F.SilkS)
      (effects (font (size 0.762 0.762) (thickness 0.127)))
    )
    (fp_text value 1k (at 0 0) (layer F.SilkS) hide
      (effects (font (size 0.762 0.762) (thickness 0.127)))
    )
    (fp_line (start -2.54 -1.143) (end -2.54 1.143) (layer F.SilkS) (width 0.127))
    (fp_line (start -2.54 1.143) (end -0.889 1.143) (layer F.SilkS) (width 0.127))
    (fp_line (start 0.889 -1.143) (end 2.54 -1.143) (layer F.SilkS) (width 0.127))
    (fp_line (start 2.54 -1.143) (end 2.54 1.143) (layer F.SilkS) (width 0.127))
    (fp_line (start 2.54 1.143) (end 0.889 1.143) (layer F.SilkS) (width 0.127))
    (fp_line (start -0.889 -1.143) (end -2.54 -1.143) (layer F.SilkS) (width 0.127))
    (pad 1 smd rect (at -1.651 0) (size 1.524 2.032)
      (layers F.Cu F.Paste F.Mask)
      (net 29 N-0000021)
    )
    (pad 2 smd rect (at 1.651 0) (size 1.524 2.032)
      (layers F.Cu F.Paste F.Mask)
      (net 28 GND)
    )
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.17 0.16 0.16))
      (rotate (xyz 0 0 0))
    )
  )

  (module SM1206 (layer F.Cu) (tedit 42806E24) (tstamp 52FB4754)
    (at 194.818 76.962)
    (path /52FB0EFD)
    (attr smd)
    (fp_text reference R3 (at 0 0) (layer F.SilkS)
      (effects (font (size 0.762 0.762) (thickness 0.127)))
    )
    (fp_text value 10k (at 0 0) (layer F.SilkS) hide
      (effects (font (size 0.762 0.762) (thickness 0.127)))
    )
    (fp_line (start -2.54 -1.143) (end -2.54 1.143) (layer F.SilkS) (width 0.127))
    (fp_line (start -2.54 1.143) (end -0.889 1.143) (layer F.SilkS) (width 0.127))
    (fp_line (start 0.889 -1.143) (end 2.54 -1.143) (layer F.SilkS) (width 0.127))
    (fp_line (start 2.54 -1.143) (end 2.54 1.143) (layer F.SilkS) (width 0.127))
    (fp_line (start 2.54 1.143) (end 0.889 1.143) (layer F.SilkS) (width 0.127))
    (fp_line (start -0.889 -1.143) (end -2.54 -1.143) (layer F.SilkS) (width 0.127))
    (pad 1 smd rect (at -1.651 0) (size 1.524 2.032)
      (layers F.Cu F.Paste F.Mask)
      (net 1 +3.3V)
    )
    (pad 2 smd rect (at 1.651 0) (size 1.524 2.032)
      (layers F.Cu F.Paste F.Mask)
      (net 3 /NRST)
    )
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.17 0.16 0.16))
      (rotate (xyz 0 0 0))
    )
  )

  (module SM1206 (layer F.Cu) (tedit 42806E24) (tstamp 52FB4760)
    (at 200.914 76.962)
    (path /52FB0F99)
    (attr smd)
    (fp_text reference C3 (at 0 0) (layer F.SilkS)
      (effects (font (size 0.762 0.762) (thickness 0.127)))
    )
    (fp_text value 104 (at 0 0) (layer F.SilkS) hide
      (effects (font (size 0.762 0.762) (thickness 0.127)))
    )
    (fp_line (start -2.54 -1.143) (end -2.54 1.143) (layer F.SilkS) (width 0.127))
    (fp_line (start -2.54 1.143) (end -0.889 1.143) (layer F.SilkS) (width 0.127))
    (fp_line (start 0.889 -1.143) (end 2.54 -1.143) (layer F.SilkS) (width 0.127))
    (fp_line (start 2.54 -1.143) (end 2.54 1.143) (layer F.SilkS) (width 0.127))
    (fp_line (start 2.54 1.143) (end 0.889 1.143) (layer F.SilkS) (width 0.127))
    (fp_line (start -0.889 -1.143) (end -2.54 -1.143) (layer F.SilkS) (width 0.127))
    (pad 1 smd rect (at -1.651 0) (size 1.524 2.032)
      (layers F.Cu F.Paste F.Mask)
      (net 3 /NRST)
    )
    (pad 2 smd rect (at 1.651 0) (size 1.524 2.032)
      (layers F.Cu F.Paste F.Mask)
      (net 28 GND)
    )
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.17 0.16 0.16))
      (rotate (xyz 0 0 0))
    )
  )

  (module SIL-5 (layer F.Cu) (tedit 200000) (tstamp 52FB476E)
    (at 187.452 73.66)
    (descr "Connecteur 5 pins")
    (tags "CONN DEV")
    (path /52FB4AA7)
    (fp_text reference P4 (at -0.635 -2.54) (layer F.SilkS)
      (effects (font (size 1.72974 1.08712) (thickness 0.3048)))
    )
    (fp_text value CONN_5 (at 0 -2.54) (layer F.SilkS) hide
      (effects (font (size 1.524 1.016) (thickness 0.3048)))
    )
    (fp_line (start -7.62 1.27) (end -7.62 -1.27) (layer F.SilkS) (width 0.3048))
    (fp_line (start -7.62 -1.27) (end 5.08 -1.27) (layer F.SilkS) (width 0.3048))
    (fp_line (start 5.08 -1.27) (end 5.08 1.27) (layer F.SilkS) (width 0.3048))
    (fp_line (start 5.08 1.27) (end -7.62 1.27) (layer F.SilkS) (width 0.3048))
    (fp_line (start -5.08 1.27) (end -5.08 -1.27) (layer F.SilkS) (width 0.3048))
    (pad 1 thru_hole rect (at -6.35 0) (size 1.397 1.397) (drill 0.8128)
      (layers *.Cu *.Mask F.SilkS)
      (net 1 +3.3V)
    )
    (pad 2 thru_hole circle (at -3.81 0) (size 1.397 1.397) (drill 0.8128)
      (layers *.Cu *.Mask F.SilkS)
    )
    (pad 3 thru_hole circle (at -1.27 0) (size 1.397 1.397) (drill 0.8128)
      (layers *.Cu *.Mask F.SilkS)
      (net 23 /PD6)
    )
    (pad 4 thru_hole circle (at 1.27 0) (size 1.397 1.397) (drill 0.8128)
      (layers *.Cu *.Mask F.SilkS)
      (net 22 /PD5)
    )
    (pad 5 thru_hole circle (at 3.81 0) (size 1.397 1.397) (drill 0.8128)
      (layers *.Cu *.Mask F.SilkS)
      (net 28 GND)
    )
  )

  (module SIL-4 (layer F.Cu) (tedit 200000) (tstamp 52FB477D)
    (at 198.12 73.66)
    (descr "Connecteur 4 pibs")
    (tags "CONN DEV")
    (path /52FB0A49)
    (fp_text reference P2 (at 0 -2.54) (layer F.SilkS)
      (effects (font (size 1.73482 1.08712) (thickness 0.3048)))
    )
    (fp_text value CONN_4 (at 0 -2.54) (layer F.SilkS) hide
      (effects (font (size 1.524 1.016) (thickness 0.3048)))
    )
    (fp_line (start -5.08 -1.27) (end -5.08 -1.27) (layer F.SilkS) (width 0.3048))
    (fp_line (start -5.08 1.27) (end -5.08 -1.27) (layer F.SilkS) (width 0.3048))
    (fp_line (start -5.08 -1.27) (end -5.08 -1.27) (layer F.SilkS) (width 0.3048))
    (fp_line (start -5.08 -1.27) (end 5.08 -1.27) (layer F.SilkS) (width 0.3048))
    (fp_line (start 5.08 -1.27) (end 5.08 1.27) (layer F.SilkS) (width 0.3048))
    (fp_line (start 5.08 1.27) (end -5.08 1.27) (layer F.SilkS) (width 0.3048))
    (fp_line (start -2.54 1.27) (end -2.54 -1.27) (layer F.SilkS) (width 0.3048))
    (pad 1 thru_hole rect (at -3.81 0) (size 1.397 1.397) (drill 0.8128)
      (layers *.Cu *.Mask F.SilkS)
      (net 1 +3.3V)
    )
    (pad 2 thru_hole circle (at -1.27 0) (size 1.397 1.397) (drill 0.8128)
      (layers *.Cu *.Mask F.SilkS)
      (net 27 /SWIM/PD1)
    )
    (pad 3 thru_hole circle (at 1.27 0) (size 1.397 1.397) (drill 0.8128)
      (layers *.Cu *.Mask F.SilkS)
      (net 3 /NRST)
    )
    (pad 4 thru_hole circle (at 3.81 0) (size 1.397 1.397) (drill 0.8128)
      (layers *.Cu *.Mask F.SilkS)
      (net 28 GND)
    )
  )

  (module SIL-14 (layer F.Cu) (tedit 200000) (tstamp 52FB4793)
    (at 197.612 70.358)
    (descr "Connecteur 14 pins")
    (tags "CONN DEV")
    (path /52FB0A6A)
    (fp_text reference P1 (at -10.16 -2.54) (layer F.SilkS)
      (effects (font (size 1.72974 1.08712) (thickness 0.3048)))
    )
    (fp_text value CONN_14 (at 7.62 -2.54) (layer F.SilkS)
      (effects (font (size 1.524 1.016) (thickness 0.3048)))
    )
    (fp_line (start -17.78 -1.27) (end 17.78 -1.27) (layer F.SilkS) (width 0.3048))
    (fp_line (start 17.78 -1.27) (end 17.78 1.27) (layer F.SilkS) (width 0.3048))
    (fp_line (start 17.78 1.27) (end -17.78 1.27) (layer F.SilkS) (width 0.3048))
    (fp_line (start -17.78 1.27) (end -17.78 -1.27) (layer F.SilkS) (width 0.3048))
    (pad 1 thru_hole rect (at -16.51 0) (size 1.397 1.397) (drill 0.8128)
      (layers *.Cu *.Mask F.SilkS)
      (net 1 +3.3V)
    )
    (pad 2 thru_hole circle (at -13.97 0) (size 1.397 1.397) (drill 0.8128)
      (layers *.Cu *.Mask F.SilkS)
      (net 28 GND)
    )
    (pad 3 thru_hole circle (at -11.43 0) (size 1.397 1.397) (drill 0.8128)
      (layers *.Cu *.Mask F.SilkS)
      (net 3 /NRST)
    )
    (pad 4 thru_hole circle (at -8.89 0) (size 1.397 1.397) (drill 0.8128)
      (layers *.Cu *.Mask F.SilkS)
      (net 4 /OSC1IN)
    )
    (pad 5 thru_hole circle (at -6.35 0) (size 1.397 1.397) (drill 0.8128)
      (layers *.Cu *.Mask F.SilkS)
      (net 5 /OSC2IN)
    )
    (pad 6 thru_hole circle (at -3.81 0) (size 1.397 1.397) (drill 0.8128)
      (layers *.Cu *.Mask F.SilkS)
      (net 26 /PF4)
    )
    (pad 7 thru_hole circle (at -1.27 0) (size 1.397 1.397) (drill 0.8128)
      (layers *.Cu *.Mask F.SilkS)
      (net 10 /PB5)
    )
    (pad 8 thru_hole circle (at 1.27 0) (size 1.397 1.397) (drill 0.8128)
      (layers *.Cu *.Mask F.SilkS)
      (net 9 /PB4)
    )
    (pad 9 thru_hole circle (at 3.81 0) (size 1.397 1.397) (drill 0.8128)
      (layers *.Cu *.Mask F.SilkS)
      (net 2 "/A DIR")
    )
    (pad 10 thru_hole circle (at 6.35 0) (size 1.397 1.397) (drill 0.8128)
      (layers *.Cu *.Mask F.SilkS)
      (net 8 /PB2)
    )
    (pad 11 thru_hole circle (at 8.89 0) (size 1.397 1.397) (drill 0.8128)
      (layers *.Cu *.Mask F.SilkS)
      (net 7 /PB1)
    )
    (pad 12 thru_hole circle (at 11.43 0) (size 1.397 1.397) (drill 0.8128)
      (layers *.Cu *.Mask F.SilkS)
      (net 6 /PB0)
    )
    (pad 13 thru_hole circle (at 13.97 0) (size 1.397 1.397) (drill 0.8128)
      (layers *.Cu *.Mask F.SilkS)
      (net 25 /PE5)
    )
    (pad 14 thru_hole circle (at 16.51 0) (size 1.397 1.397) (drill 0.8128)
      (layers *.Cu *.Mask F.SilkS)
      (net 11 /PC1)
    )
  )

  (module SIL-14 (layer F.Cu) (tedit 200000) (tstamp 52FB47A9)
    (at 233.68 70.358)
    (descr "Connecteur 14 pins")
    (tags "CONN DEV")
    (path /52FB0A79)
    (fp_text reference P3 (at -10.16 -2.54) (layer F.SilkS)
      (effects (font (size 1.72974 1.08712) (thickness 0.3048)))
    )
    (fp_text value CONN_14 (at 7.62 -2.54) (layer F.SilkS)
      (effects (font (size 1.524 1.016) (thickness 0.3048)))
    )
    (fp_line (start -17.78 -1.27) (end 17.78 -1.27) (layer F.SilkS) (width 0.3048))
    (fp_line (start 17.78 -1.27) (end 17.78 1.27) (layer F.SilkS) (width 0.3048))
    (fp_line (start 17.78 1.27) (end -17.78 1.27) (layer F.SilkS) (width 0.3048))
    (fp_line (start -17.78 1.27) (end -17.78 -1.27) (layer F.SilkS) (width 0.3048))
    (pad 1 thru_hole rect (at -16.51 0) (size 1.397 1.397) (drill 0.8128)
      (layers *.Cu *.Mask F.SilkS)
      (net 24 /PD7)
    )
    (pad 2 thru_hole circle (at -13.97 0) (size 1.397 1.397) (drill 0.8128)
      (layers *.Cu *.Mask F.SilkS)
      (net 23 /PD6)
    )
    (pad 3 thru_hole circle (at -11.43 0) (size 1.397 1.397) (drill 0.8128)
      (layers *.Cu *.Mask F.SilkS)
      (net 22 /PD5)
    )
    (pad 4 thru_hole circle (at -8.89 0) (size 1.397 1.397) (drill 0.8128)
      (layers *.Cu *.Mask F.SilkS)
      (net 21 /PD4)
    )
    (pad 5 thru_hole circle (at -6.35 0) (size 1.397 1.397) (drill 0.8128)
      (layers *.Cu *.Mask F.SilkS)
      (net 20 /PD3)
    )
    (pad 6 thru_hole circle (at -3.81 0) (size 1.397 1.397) (drill 0.8128)
      (layers *.Cu *.Mask F.SilkS)
      (net 19 /PD2)
    )
    (pad 7 thru_hole circle (at -1.27 0) (size 1.397 1.397) (drill 0.8128)
      (layers *.Cu *.Mask F.SilkS)
      (net 27 /SWIM/PD1)
    )
    (pad 8 thru_hole circle (at 1.27 0) (size 1.397 1.397) (drill 0.8128)
      (layers *.Cu *.Mask F.SilkS)
      (net 18 /PD0)
    )
    (pad 9 thru_hole circle (at 3.81 0) (size 1.397 1.397) (drill 0.8128)
      (layers *.Cu *.Mask F.SilkS)
      (net 17 /PC7)
    )
    (pad 10 thru_hole circle (at 6.35 0) (size 1.397 1.397) (drill 0.8128)
      (layers *.Cu *.Mask F.SilkS)
      (net 16 /PC6)
    )
    (pad 11 thru_hole circle (at 8.89 0) (size 1.397 1.397) (drill 0.8128)
      (layers *.Cu *.Mask F.SilkS)
      (net 15 /PC5)
    )
    (pad 12 thru_hole circle (at 11.43 0) (size 1.397 1.397) (drill 0.8128)
      (layers *.Cu *.Mask F.SilkS)
      (net 14 /PC4)
    )
    (pad 13 thru_hole circle (at 13.97 0) (size 1.397 1.397) (drill 0.8128)
      (layers *.Cu *.Mask F.SilkS)
      (net 13 /PC3)
    )
    (pad 14 thru_hole circle (at 16.51 0) (size 1.397 1.397) (drill 0.8128)
      (layers *.Cu *.Mask F.SilkS)
      (net 12 /PC2)
    )
  )

  (module DB25FC (layer F.Cu) (tedit 200000) (tstamp 52FB47DC)
    (at 206.502 66.04)
    (descr "Connecteur DB25 femelle couche")
    (tags "CONN DB25")
    (path /52FB403E)
    (fp_text reference J1 (at 0 -15.24) (layer F.SilkS)
      (effects (font (size 1.524 1.524) (thickness 0.3048)))
    )
    (fp_text value DB25 (at 0 -6.35) (layer F.SilkS)
      (effects (font (size 1.524 1.524) (thickness 0.3048)))
    )
    (fp_line (start 26.67 -11.43) (end 26.67 2.54) (layer F.SilkS) (width 0.3048))
    (fp_line (start 19.05 -6.35) (end 19.05 2.54) (layer F.SilkS) (width 0.3048))
    (fp_line (start 20.955 -11.43) (end 20.955 -6.35) (layer F.SilkS) (width 0.3048))
    (fp_line (start -20.955 -11.43) (end -20.955 -6.35) (layer F.SilkS) (width 0.3048))
    (fp_line (start -19.05 -6.35) (end -19.05 2.54) (layer F.SilkS) (width 0.3048))
    (fp_line (start -26.67 2.54) (end -26.67 -11.43) (layer F.SilkS) (width 0.3048))
    (fp_line (start 26.67 -6.35) (end 19.05 -6.35) (layer F.SilkS) (width 0.3048))
    (fp_line (start -26.67 -6.35) (end -19.05 -6.35) (layer F.SilkS) (width 0.3048))
    (fp_line (start 20.32 -8.255) (end 20.32 -11.43) (layer F.SilkS) (width 0.3048))
    (fp_line (start -20.32 -8.255) (end -20.32 -11.43) (layer F.SilkS) (width 0.3048))
    (fp_line (start 20.32 -18.415) (end 20.32 -12.7) (layer F.SilkS) (width 0.3048))
    (fp_line (start -20.32 -18.415) (end -20.32 -12.7) (layer F.SilkS) (width 0.3048))
    (fp_line (start 26.67 -11.43) (end 26.67 -12.7) (layer F.SilkS) (width 0.3048))
    (fp_line (start 26.67 -12.7) (end -26.67 -12.7) (layer F.SilkS) (width 0.3048))
    (fp_line (start -26.67 -12.7) (end -26.67 -11.43) (layer F.SilkS) (width 0.3048))
    (fp_line (start -26.67 -11.43) (end 26.67 -11.43) (layer F.SilkS) (width 0.3048))
    (fp_line (start 19.05 2.54) (end 26.67 2.54) (layer F.SilkS) (width 0.3048))
    (fp_line (start -20.32 -8.255) (end 20.32 -8.255) (layer F.SilkS) (width 0.3048))
    (fp_line (start -20.32 -18.415) (end 20.32 -18.415) (layer F.SilkS) (width 0.3048))
    (fp_line (start -26.67 2.54) (end -19.05 2.54) (layer F.SilkS) (width 0.3048))
    (pad "" thru_hole circle (at 23.495 -1.27) (size 3.81 3.81) (drill 3.048)
      (layers *.Cu *.Mask F.SilkS)
    )
    (pad "" thru_hole circle (at -23.495 -1.27) (size 3.81 3.81) (drill 3.048)
      (layers *.Cu *.Mask F.SilkS)
    )
    (pad 1 thru_hole rect (at -16.51 1.27) (size 1.524 1.524) (drill 1.016)
      (layers *.Cu *.Mask F.SilkS)
    )
    (pad 2 thru_hole circle (at -13.716 1.27) (size 1.524 1.524) (drill 1.016)
      (layers *.Cu *.Mask F.SilkS)
      (net 11 /PC1)
    )
    (pad 3 thru_hole circle (at -11.049 1.27) (size 1.524 1.524) (drill 1.016)
      (layers *.Cu *.Mask F.SilkS)
      (net 6 /PB0)
    )
    (pad 4 thru_hole circle (at -8.255 1.27) (size 1.524 1.524) (drill 1.016)
      (layers *.Cu *.Mask F.SilkS)
      (net 21 /PD4)
    )
    (pad 5 thru_hole circle (at -5.461 1.27) (size 1.524 1.524) (drill 1.016)
      (layers *.Cu *.Mask F.SilkS)
      (net 7 /PB1)
    )
    (pad 6 thru_hole circle (at -2.667 1.27) (size 1.524 1.524) (drill 1.016)
      (layers *.Cu *.Mask F.SilkS)
      (net 19 /PD2)
    )
    (pad 7 thru_hole circle (at 0 1.27) (size 1.524 1.524) (drill 1.016)
      (layers *.Cu *.Mask F.SilkS)
      (net 8 /PB2)
    )
    (pad 8 thru_hole circle (at 2.794 1.27) (size 1.524 1.524) (drill 1.016)
      (layers *.Cu *.Mask F.SilkS)
    )
    (pad 9 thru_hole circle (at 5.588 1.27) (size 1.524 1.524) (drill 1.016)
      (layers *.Cu *.Mask F.SilkS)
      (net 2 "/A DIR")
    )
    (pad 10 thru_hole circle (at 8.382 1.27) (size 1.524 1.524) (drill 1.016)
      (layers *.Cu *.Mask F.SilkS)
    )
    (pad 11 thru_hole circle (at 11.049 1.27) (size 1.524 1.524) (drill 1.016)
      (layers *.Cu *.Mask F.SilkS)
    )
    (pad 12 thru_hole circle (at 13.843 1.27) (size 1.524 1.524) (drill 1.016)
      (layers *.Cu *.Mask F.SilkS)
    )
    (pad 13 thru_hole circle (at 16.637 1.27) (size 1.524 1.524) (drill 1.016)
      (layers *.Cu *.Mask F.SilkS)
    )
    (pad 14 thru_hole circle (at -14.9352 -1.27) (size 1.524 1.524) (drill 1.016)
      (layers *.Cu *.Mask F.SilkS)
    )
    (pad 15 thru_hole circle (at -12.3952 -1.27) (size 1.524 1.524) (drill 1.016)
      (layers *.Cu *.Mask F.SilkS)
    )
    (pad 16 thru_hole circle (at -9.6012 -1.27) (size 1.524 1.524) (drill 1.016)
      (layers *.Cu *.Mask F.SilkS)
    )
    (pad 17 thru_hole circle (at -6.858 -1.27) (size 1.524 1.524) (drill 1.016)
      (layers *.Cu *.Mask F.SilkS)
    )
    (pad 18 thru_hole circle (at -4.1148 -1.27) (size 1.524 1.524) (drill 1.016)
      (layers *.Cu *.Mask F.SilkS)
      (net 28 GND)
    )
    (pad 19 thru_hole circle (at -1.3208 -1.27) (size 1.524 1.524) (drill 1.016)
      (layers *.Cu *.Mask F.SilkS)
      (net 28 GND)
    )
    (pad 20 thru_hole circle (at 1.4224 -1.27) (size 1.524 1.524) (drill 1.016)
      (layers *.Cu *.Mask F.SilkS)
      (net 28 GND)
    )
    (pad 21 thru_hole circle (at 4.1656 -1.27) (size 1.524 1.524) (drill 1.016)
      (layers *.Cu *.Mask F.SilkS)
      (net 28 GND)
    )
    (pad 22 thru_hole circle (at 7.0104 -1.27) (size 1.524 1.524) (drill 1.016)
      (layers *.Cu *.Mask F.SilkS)
      (net 28 GND)
    )
    (pad 23 thru_hole circle (at 9.7028 -1.27) (size 1.524 1.524) (drill 1.016)
      (layers *.Cu *.Mask F.SilkS)
      (net 28 GND)
    )
    (pad 24 thru_hole circle (at 12.446 -1.27) (size 1.524 1.524) (drill 1.016)
      (layers *.Cu *.Mask F.SilkS)
      (net 28 GND)
    )
    (pad 25 thru_hole circle (at 15.24 -1.27) (size 1.524 1.524) (drill 1.016)
      (layers *.Cu *.Mask F.SilkS)
      (net 28 GND)
    )
    (model conn_DBxx/db25_female_pin90deg.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

)
