(kicad_pcb (version 4) (host pcbnew 4.0.7)

  (general
    (links 6)
    (no_connects 0)
    (area 99.924999 77.525 115.325 100.575)
    (thickness 0.6)
    (drawings 9)
    (tracks 14)
    (zones 0)
    (modules 6)
    (nets 5)
  )

  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu jumper)
    (33 F.Adhes user)
    (35 F.Paste user)
    (37 F.SilkS user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (47 F.CrtYd user)
    (49 F.Fab user)
  )

  (setup
    (last_trace_width 0.5)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 5 5)
    (pad_drill 3)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 100 100)
    (grid_origin 100 100)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.150000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )

  (net 0 "")
  (net 1 GND)
  (net 2 "Net-(J1-Pad1)")
  (net 3 "Net-(J1-Pad2)")
  (net 4 "Net-(J1-Pad5)")

  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.5)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net GND)
    (add_net "Net-(J1-Pad1)")
    (add_net "Net-(J1-Pad2)")
    (add_net "Net-(J1-Pad5)")
  )

  (module my_footprints:Hole_2mm (layer F.Cu) (tedit 5A1C037C) (tstamp 5A1BFC1C)
    (at 103.5 95)
    (path /591446F9)
    (fp_text reference P1 (at 0 3.81) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value Hole (at 0 -3.81) (layer F.Fab) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad "" np_thru_hole circle (at -1 0) (size 4 4) (drill 0.8) (layers *.Cu *.Mask))
  )

  (module my_footprints:Hole_2mm (layer F.Cu) (tedit 5A1C0382) (tstamp 5A1BFC21)
    (at 111.5 95)
    (path /59143415)
    (fp_text reference P4 (at 0 3.81) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value Hole (at 0 -3.81) (layer F.Fab) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad "" np_thru_hole circle (at 1 0) (size 4 4) (drill 0.8) (layers *.Cu *.Mask))
  )

  (module Resistors_SMD.pretty:R_0805_HandSoldering (layer F.Cu) (tedit 5A1C0709) (tstamp 5A1BFC32)
    (at 112.5 81 90)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (path /5A1C0C88)
    (attr smd)
    (fp_text reference R1 (at 0 1.75 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 47k (at 0 1.75 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.5 0.5) (thickness 0.075)))
    )
    (fp_line (start -1 0.62) (end -1 -0.62) (layer F.Fab) (width 0.1))
    (fp_line (start 1 0.62) (end -1 0.62) (layer F.Fab) (width 0.1))
    (fp_line (start 1 -0.62) (end 1 0.62) (layer F.Fab) (width 0.1))
    (fp_line (start -1 -0.62) (end 1 -0.62) (layer F.Fab) (width 0.1))
    (fp_line (start 0.6 0.88) (end -0.6 0.88) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.6 -0.88) (end 0.6 -0.88) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.35 -0.9) (end 2.35 -0.9) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.35 -0.9) (end -2.35 0.9) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2.35 0.9) (end 2.35 -0.9) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2.35 0.9) (end -2.35 0.9) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(J1-Pad5)"))
    (pad 2 smd rect (at 1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module TO_SOT_Packages_SMD.pretty:SOT-23W_Handsoldering (layer F.Cu) (tedit 5A1C070E) (tstamp 5A1BFC47)
    (at 107.5 81)
    (descr "SOT-23W http://www.allegromicro.com/~/media/Files/Datasheets/A112x-Datasheet.ashx?la=en&hash=7BC461E058CC246E0BAB62433B2F1ECA104CA9D3")
    (tags "SOT-23W for handsoldering")
    (path /5A1C0A65)
    (attr smd)
    (fp_text reference U1 (at 0 -2.25) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value A3212LH (at 0 -2.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.075 0.7) (end 1.075 1.61) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.075 -1.6) (end 1.075 -0.7) (layer F.SilkS) (width 0.12))
    (fp_line (start -2 -1.61) (end 1.075 -1.61) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.075 1.61) (end 1.075 1.61) (layer F.SilkS) (width 0.12))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.5 0.5) (thickness 0.075)))
    )
    (fp_line (start -0.955 -0.49) (end -0.955 1.49) (layer F.Fab) (width 0.1))
    (fp_line (start 0.045 -1.49) (end 0.955 -1.49) (layer F.Fab) (width 0.1))
    (fp_line (start -0.955 -0.49) (end 0.045 -1.49) (layer F.Fab) (width 0.1))
    (fp_line (start 0.955 -1.49) (end 0.955 1.49) (layer F.Fab) (width 0.1))
    (fp_line (start -0.955 1.49) (end 0.955 1.49) (layer F.Fab) (width 0.1))
    (fp_line (start -2.95 -1.74) (end 2.95 -1.74) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2.95 -1.74) (end 2.95 1.74) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2.95 1.74) (end -2.95 1.74) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.95 1.74) (end -2.95 -1.74) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -1.7 -0.95) (size 2 0.7) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(J1-Pad1)"))
    (pad 2 smd rect (at -1.7 0.95) (size 2 0.7) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(J1-Pad2)"))
    (pad 3 smd rect (at 1.7 0) (size 2 0.7) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes/SOT-23W_Handsoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module my_footprints:SMD5pin (layer F.Cu) (tedit 5A1C0D07) (tstamp 5A23F1B2)
    (at 107.5 88.5)
    (path /5A1C0D39)
    (fp_text reference J1 (at 1.898 5.404) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value Conn_01x05 (at 0 -4.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 smd rect (at -5 0) (size 2 7.5) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(J1-Pad1)"))
    (pad 2 smd rect (at -2.5 0) (size 2 7.5) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(J1-Pad2)"))
    (pad 3 smd rect (at 0 0) (size 2 7.5) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(J1-Pad2)"))
    (pad 4 smd rect (at 2.5 0) (size 2 7.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 5 smd rect (at 5 0) (size 2 7.5) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(J1-Pad5)"))
  )

  (module Connectors.pretty:1pin (layer F.Cu) (tedit 5A1C06EA) (tstamp 5A40E4AE)
    (at 107.5 97)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference REF** (at 4.5 2.5) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 1pin (at -3.5 2) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_circle (center 0 0) (end 2 0.8) (layer F.Fab) (width 0.1))
    (fp_circle (center 0 0) (end 2.6 0) (layer F.CrtYd) (width 0.05))
    (fp_circle (center 0 0) (end 0 -2.286) (layer F.SilkS) (width 0.12))
    (pad "" np_thru_hole circle (at 0 0) (size 5 5) (drill 3) (layers *.Cu *.Mask))
  )

  (gr_text out (at 105.207 93.904 90) (layer F.Cu)
    (effects (font (size 1 1) (thickness 0.25)))
  )
  (gr_text Vcc (at 100.762 88.316 90) (layer F.Cu)
    (effects (font (size 1 1) (thickness 0.25)))
  )
  (gr_text gnd (at 109.652 93.777 45) (layer F.Cu)
    (effects (font (size 1 1) (thickness 0.25)))
  )
  (gr_text btn (at 107.366 93.269) (layer F.Cu)
    (effects (font (size 1 1) (thickness 0.25)))
  )
  (gr_text button (at 114.351 88.697 90) (layer F.Cu)
    (effects (font (size 1 1) (thickness 0.25)))
  )
  (gr_line (start 115 100) (end 100 100) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 115 78) (end 115 100) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 100 78) (end 115 78) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 100 100) (end 100 78) (angle 90) (layer Edge.Cuts) (width 0.15))

  (segment (start 109.2 81) (end 109.2 80.3) (width 0.5) (layer F.Cu) (net 1))
  (segment (start 109.85 79.65) (end 112.5 79.65) (width 0.5) (layer F.Cu) (net 1) (tstamp 5A23F2B8))
  (segment (start 109.2 80.3) (end 109.85 79.65) (width 0.5) (layer F.Cu) (net 1) (tstamp 5A23F2B7))
  (segment (start 110 88.5) (end 110 81.8) (width 0.5) (layer F.Cu) (net 1))
  (segment (start 110 81.8) (end 109.2 81) (width 0.5) (layer F.Cu) (net 1) (tstamp 5A23F2A1))
  (segment (start 105.8 80.05) (end 103.45 80.05) (width 0.5) (layer F.Cu) (net 2))
  (segment (start 102.5 81) (end 102.5 88.5) (width 0.5) (layer F.Cu) (net 2) (tstamp 5A23F252))
  (segment (start 103.45 80.05) (end 102.5 81) (width 0.5) (layer F.Cu) (net 2) (tstamp 5A23F251))
  (segment (start 107.5 88.5) (end 107.5 83.5) (width 0.5) (layer F.Cu) (net 3))
  (segment (start 107.5 83.5) (end 105 83.5) (width 0.5) (layer F.Cu) (net 3) (tstamp 5A23F25B))
  (segment (start 105 88.5) (end 105 83.5) (width 0.5) (layer F.Cu) (net 3))
  (segment (start 105 83.5) (end 105 82.75) (width 0.5) (layer F.Cu) (net 3) (tstamp 5A23F25E))
  (segment (start 105 82.75) (end 105.8 81.95) (width 0.5) (layer F.Cu) (net 3) (tstamp 5A23F255))
  (segment (start 112.5 88.5) (end 112.5 82.35) (width 0.5) (layer F.Cu) (net 4))

)
