(kicad_pcb (version 4) (host pcbnew 4.0.7)

  (general
    (links 5)
    (no_connects 1)
    (area 0 0 0 0)
    (thickness 0.6)
    (drawings 10)
    (tracks 14)
    (zones 0)
    (modules 6)
    (nets 6)
  )

  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )

  (setup
    (last_trace_width 1)
    (user_trace_width 0.5)
    (user_trace_width 1)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 5 5)
    (pad_drill 3)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )

  (net 0 "")
  (net 1 "Net-(J1-Pad2)")
  (net 2 "Net-(J1-Pad1)")
  (net 3 "Net-(J1-Pad4)")
  (net 4 "Net-(J1-Pad3)")
  (net 5 "Net-(J1-Pad5)")

  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.5)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net "Net-(J1-Pad1)")
    (add_net "Net-(J1-Pad2)")
    (add_net "Net-(J1-Pad3)")
    (add_net "Net-(J1-Pad4)")
    (add_net "Net-(J1-Pad5)")
  )

  (net_class 1 ""
    (clearance 0.5)
    (trace_width 1.5)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
  )

  (module Connectors.pretty:1pin (layer F.Cu) (tedit 5A1C0B7C) (tstamp 5A411FCE)
    (at 162 110)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference REF** (at 0 -3.048) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 1pin (at 0 3) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_circle (center 0 0) (end 2 0.8) (layer F.Fab) (width 0.1))
    (fp_circle (center 0 0) (end 2.6 0) (layer F.CrtYd) (width 0.05))
    (fp_circle (center 0 0) (end 0 -2.286) (layer F.SilkS) (width 0.12))
    (pad 1 thru_hole circle (at 0 0) (size 5 5) (drill 3) (layers *.Cu *.Mask))
  )

  (module Connectors.pretty:1pin (layer F.Cu) (tedit 5A1C0B7C) (tstamp 5A411FC6)
    (at 137 110)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference REF** (at 0 -3.048) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 1pin (at 0 3) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_circle (center 0 0) (end 2 0.8) (layer F.Fab) (width 0.1))
    (fp_circle (center 0 0) (end 2.6 0) (layer F.CrtYd) (width 0.05))
    (fp_circle (center 0 0) (end 0 -2.286) (layer F.SilkS) (width 0.12))
    (pad 1 thru_hole circle (at 0 0) (size 5 5) (drill 3) (layers *.Cu *.Mask))
  )

  (module Connectors.pretty:1pin (layer F.Cu) (tedit 5A1C0B7C) (tstamp 5A411FBE)
    (at 137 98)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference REF** (at 0 -3.048) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 1pin (at 0 3) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_circle (center 0 0) (end 2 0.8) (layer F.Fab) (width 0.1))
    (fp_circle (center 0 0) (end 2.6 0) (layer F.CrtYd) (width 0.05))
    (fp_circle (center 0 0) (end 0 -2.286) (layer F.SilkS) (width 0.12))
    (pad 1 thru_hole circle (at 0 0) (size 5 5) (drill 3) (layers *.Cu *.Mask))
  )

  (module Connectors.pretty:USB_B (layer B.Cu) (tedit 55B36073) (tstamp 5A411E62)
    (at 150.495 95.631 90)
    (descr "USB B connector")
    (tags "USB_B USB_DEV")
    (path /5A1C0904)
    (fp_text reference J1 (at 11.05 -1.27 360) (layer B.SilkS)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_text value USB_B (at 4.7 -1.27 360) (layer B.Fab)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_line (start 15.25 -8.9) (end -2.3 -8.9) (layer B.CrtYd) (width 0.05))
    (fp_line (start -2.3 -8.9) (end -2.3 6.35) (layer B.CrtYd) (width 0.05))
    (fp_line (start -2.3 6.35) (end 15.25 6.35) (layer B.CrtYd) (width 0.05))
    (fp_line (start 15.25 6.35) (end 15.25 -8.9) (layer B.CrtYd) (width 0.05))
    (fp_line (start 6.35 -7.37) (end 14.99 -7.37) (layer B.SilkS) (width 0.12))
    (fp_line (start -2.03 -7.37) (end 3.05 -7.37) (layer B.SilkS) (width 0.12))
    (fp_line (start 6.35 4.83) (end 14.99 4.83) (layer B.SilkS) (width 0.12))
    (fp_line (start -2.03 4.83) (end 3.05 4.83) (layer B.SilkS) (width 0.12))
    (fp_line (start 14.99 4.83) (end 14.99 -7.37) (layer B.SilkS) (width 0.12))
    (fp_line (start -2.03 -7.37) (end -2.03 4.83) (layer B.SilkS) (width 0.12))
    (pad 2 thru_hole circle (at 0 -2.54 180) (size 1.52 1.52) (drill 0.81) (layers *.Cu *.Mask)
      (net 1 "Net-(J1-Pad2)"))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.52 1.52) (drill 0.81) (layers *.Cu *.Mask)
      (net 2 "Net-(J1-Pad1)"))
    (pad 4 thru_hole circle (at 2 0 180) (size 1.52 1.52) (drill 0.81) (layers *.Cu *.Mask)
      (net 3 "Net-(J1-Pad4)"))
    (pad 3 thru_hole circle (at 2 -2.54 180) (size 1.52 1.52) (drill 0.81) (layers *.Cu *.Mask)
      (net 4 "Net-(J1-Pad3)"))
    (pad 5 thru_hole circle (at 4.7 -7.27 180) (size 2.7 2.7) (drill 2.3) (layers *.Cu *.Mask)
      (net 5 "Net-(J1-Pad5)"))
    (pad 5 thru_hole circle (at 4.7 4.73 180) (size 2.7 2.7) (drill 2.3) (layers *.Cu *.Mask)
      (net 5 "Net-(J1-Pad5)"))
    (model ${KISYS3DMOD}/Connectors.3dshapes/USB_B.wrl
      (at (xyz 0.18 -0.05 0))
      (scale (xyz 0.39 0.39 0.39))
      (rotate (xyz 0 0 -90))
    )
  )

  (module my_footprints:SMD5pin (layer F.Cu) (tedit 5A1BFD2F) (tstamp 5A411E6B)
    (at 149.25 105)
    (path /5A1C0988)
    (fp_text reference J2 (at 0 5) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value Conn_01x05 (at 0 -5.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 smd rect (at -5 0) (size 2 7.5) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(J1-Pad3)"))
    (pad 2 smd rect (at -2.5 0) (size 2 7.5) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(J1-Pad2)"))
    (pad 3 smd rect (at 0 0) (size 2 7.5) (layers F.Cu F.Paste F.Mask))
    (pad 4 smd rect (at 2.5 0) (size 2 7.5) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(J1-Pad1)"))
    (pad 5 smd rect (at 5 0) (size 2 7.5) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(J1-Pad4)"))
  )

  (module Connectors.pretty:1pin (layer F.Cu) (tedit 5A1C0B7C) (tstamp 5A411FA4)
    (at 162 98)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference REF** (at 0 -3.048) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 1pin (at 0 3) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_circle (center 0 0) (end 2 0.8) (layer F.Fab) (width 0.1))
    (fp_circle (center 0 0) (end 2.6 0) (layer F.CrtYd) (width 0.05))
    (fp_circle (center 0 0) (end 0 -2.286) (layer F.SilkS) (width 0.12))
    (pad 1 thru_hole circle (at 0 0) (size 5 5) (drill 3) (layers *.Cu *.Mask))
  )

  (dimension 26 (width 0.3) (layer Dwgs.User)
    (gr_text "26.000 mm" (at 127.65 101 90) (layer Dwgs.User)
      (effects (font (size 1.5 1.5) (thickness 0.3)))
    )
    (feature1 (pts (xy 133 88) (xy 126.3 88)))
    (feature2 (pts (xy 133 114) (xy 126.3 114)))
    (crossbar (pts (xy 129 114) (xy 129 88)))
    (arrow1a (pts (xy 129 88) (xy 129.586421 89.126504)))
    (arrow1b (pts (xy 129 88) (xy 128.413579 89.126504)))
    (arrow2a (pts (xy 129 114) (xy 129.586421 112.873496)))
    (arrow2b (pts (xy 129 114) (xy 128.413579 112.873496)))
  )
  (dimension 33 (width 0.3) (layer Dwgs.User)
    (gr_text "33.000 mm" (at 149.5 117.349999) (layer Dwgs.User)
      (effects (font (size 1.5 1.5) (thickness 0.3)))
    )
    (feature1 (pts (xy 166 114) (xy 166 118.699999)))
    (feature2 (pts (xy 133 114) (xy 133 118.699999)))
    (crossbar (pts (xy 133 115.999999) (xy 166 115.999999)))
    (arrow1a (pts (xy 166 115.999999) (xy 164.873496 116.58642)))
    (arrow1b (pts (xy 166 115.999999) (xy 164.873496 115.413578)))
    (arrow2a (pts (xy 133 115.999999) (xy 134.126504 116.58642)))
    (arrow2b (pts (xy 133 115.999999) (xy 134.126504 115.413578)))
  )
  (gr_line (start 133 114) (end 133 88) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 166 114) (end 133 114) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 166 88) (end 166 114) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 133 88) (end 166 88) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_text Gnd (at 158 105.5) (layer F.Cu)
    (effects (font (size 1.5 1.5) (thickness 0.3)))
  )
  (gr_text Vcc (at 152.5 110.5) (layer F.Cu)
    (effects (font (size 1.5 1.5) (thickness 0.3)))
  )
  (gr_text D- (at 147 110.5) (layer F.Cu)
    (effects (font (size 1.5 1.5) (thickness 0.3)))
  )
  (gr_text D+ (at 141 105.5) (layer F.Cu)
    (effects (font (size 1.5 1.5) (thickness 0.3)))
  )

  (segment (start 146.75 105) (end 146.75 99.25) (width 1) (layer F.Cu) (net 1))
  (segment (start 147.955 98.045) (end 147.955 95.631) (width 1) (layer F.Cu) (net 1) (tstamp 5A411F89))
  (segment (start 146.75 99.25) (end 147.955 98.045) (width 1) (layer F.Cu) (net 1) (tstamp 5A411F88))
  (segment (start 146.71 104.96) (end 146.75 105) (width 1) (layer F.Cu) (net 1) (tstamp 5A411F5A))
  (segment (start 150.495 95.631) (end 150.495 97.995) (width 1) (layer F.Cu) (net 2))
  (segment (start 151.75 99.25) (end 151.75 105) (width 1) (layer F.Cu) (net 2) (tstamp 5A411F8D))
  (segment (start 150.495 97.995) (end 151.75 99.25) (width 1) (layer F.Cu) (net 2) (tstamp 5A411F8C))
  (segment (start 154.25 105) (end 154.25 95.25) (width 1) (layer F.Cu) (net 3))
  (segment (start 152.631 93.631) (end 150.495 93.631) (width 1) (layer F.Cu) (net 3) (tstamp 5A411F91))
  (segment (start 154.25 95.25) (end 152.631 93.631) (width 1) (layer F.Cu) (net 3) (tstamp 5A411F90))
  (segment (start 144.25 105) (end 144.25 95.25) (width 1) (layer F.Cu) (net 4))
  (segment (start 145.869 93.631) (end 147.955 93.631) (width 1) (layer F.Cu) (net 4) (tstamp 5A411F95))
  (segment (start 144.25 95.25) (end 145.869 93.631) (width 1) (layer F.Cu) (net 4) (tstamp 5A411F94))
  (segment (start 144.25 105) (end 143.75 105) (width 0.5) (layer F.Cu) (net 4))

)
