(kicad_pcb (version 20211014) (generator pcbnew)

  (general
    (thickness 1.6)
  )

  (paper "A4")
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
    (50 "User.1" user)
    (51 "User.2" user)
    (52 "User.3" user)
    (53 "User.4" user)
    (54 "User.5" user)
    (55 "User.6" user)
    (56 "User.7" user)
    (57 "User.8" user)
    (58 "User.9" user)
  )

  (setup
    (stackup
      (layer "F.SilkS" (type "Top Silk Screen"))
      (layer "F.Paste" (type "Top Solder Paste"))
      (layer "F.Mask" (type "Top Solder Mask") (thickness 0.01))
      (layer "F.Cu" (type "copper") (thickness 0.035))
      (layer "dielectric 1" (type "core") (thickness 1.51) (material "FR4") (epsilon_r 4.5) (loss_tangent 0.02))
      (layer "B.Cu" (type "copper") (thickness 0.035))
      (layer "B.Mask" (type "Bottom Solder Mask") (thickness 0.01))
      (layer "B.Paste" (type "Bottom Solder Paste"))
      (layer "B.SilkS" (type "Bottom Silk Screen"))
      (copper_finish "None")
      (dielectric_constraints no)
    )
    (pad_to_mask_clearance 0)
    (pcbplotparams
      (layerselection 0x00010fc_ffffffff)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (svguseinch false)
      (svgprecision 6)
      (excludeedgelayer true)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "heaters_gerber/")
    )
  )

  (net 0 "")
  (net 1 "/A1")
  (net 2 "/A2")
  (net 3 "/B1")
  (net 4 "/B2")

  (footprint "MountingHole:MountingHole_2mm" (layer "F.Cu")
    (tedit 5B924920) (tstamp 1848127b-6dc8-4336-8219-7beff7a23ab3)
    (at 243.5 46.5)
    (descr "Mounting Hole 2mm, no annular")
    (tags "mounting hole 2mm no annular")
    (property "Sheetfile" "heaters.kicad_sch")
    (property "Sheetname" "")
    (path "/8a444c7f-4e59-4eb3-af78-38e4895cec8d")
    (attr exclude_from_pos_files)
    (fp_text reference "H4" (at 0 -3.2) (layer "F.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp ec2d4dbc-ce1f-474b-abf1-0a7e1ab271c9)
    )
    (fp_text value "MountingHole" (at 0 3.1) (layer "F.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp b324a88e-056e-4a5b-952a-f52166477d46)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp bdf92eec-edc3-4cdc-bf92-1bf52507edad)
    )
    (fp_circle (center 0 0) (end 2 0) (layer "Cmts.User") (width 0.15) (fill none) (tstamp e63d0173-110b-4b6a-bcb7-ec53bf7f584a))
    (fp_circle (center 0 0) (end 2.25 0) (layer "F.CrtYd") (width 0.05) (fill none) (tstamp 56413015-3efb-430d-9c26-cb160ddfdf46))
    (pad "" np_thru_hole circle (at 0 0) (size 2 2) (drill 2) (layers *.Cu *.Mask) (tstamp 23fd5288-4cd5-482c-bc5c-d28bd0e70321))
  )

  (footprint "MountingHole:MountingHole_2mm" (layer "F.Cu")
    (tedit 5B924920) (tstamp 267e9aa1-961b-4385-9825-92576ad5885b)
    (at 48.5 60.5)
    (descr "Mounting Hole 2mm, no annular")
    (tags "mounting hole 2mm no annular")
    (property "Sheetfile" "heaters.kicad_sch")
    (property "Sheetname" "")
    (path "/018a6c0a-9e2f-4a7f-b97f-552cbe26bd38")
    (attr exclude_from_pos_files)
    (fp_text reference "H3" (at 0 -3.2) (layer "F.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 61bba478-a2a9-4bb4-acc4-8bb2f70fd641)
    )
    (fp_text value "MountingHole" (at 0 3.1) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp ceaec275-f5b1-4d5c-bba9-81a58474fef6)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp a48537c4-bc1f-4de9-bed9-1e57262d32dd)
    )
    (fp_circle (center 0 0) (end 2 0) (layer "Cmts.User") (width 0.15) (fill none) (tstamp db97869e-edcc-4d38-a28e-ed2bc30b747e))
    (fp_circle (center 0 0) (end 2.25 0) (layer "F.CrtYd") (width 0.05) (fill none) (tstamp e4205f21-0eed-437a-8005-8141b0f34673))
    (pad "" np_thru_hole circle (at 0 0) (size 2 2) (drill 2) (layers *.Cu *.Mask) (tstamp 61620f21-dd79-4af8-a0c1-17e6cf02c5f9))
  )

  (footprint "Connector_PinSocket_2.54mm:PinSocket_1x01_P2.54mm_Vertical" (layer "F.Cu")
    (tedit 5A19A434) (tstamp 4512adf5-cecc-46d4-bc53-bc82fef9cdda)
    (at 98 55.5)
    (descr "Through hole straight socket strip, 1x01, 2.54mm pitch, single row (from Kicad 4.0.7), script generated")
    (tags "Through hole socket strip THT 1x01 2.54mm single row")
    (property "Sheetfile" "heaters.kicad_sch")
    (property "Sheetname" "")
    (path "/296c1c37-fb28-4c48-9cac-0f3641fd6144")
    (attr through_hole)
    (fp_text reference "J4" (at 0 -2.77) (layer "F.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 28c37493-c727-4bec-b820-db2ef6eef2be)
    )
    (fp_text value "Conn_01x01" (at 0 2.77) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 0eec24e4-f6b1-4492-ba4d-1a69fa0021d6)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 24d25b72-0b6e-4557-b742-642fccc0c7e1)
    )
    (fp_line (start -1.33 1.21) (end -1.33 1.33) (layer "F.SilkS") (width 0.12) (tstamp 13f3ac41-1850-47f7-a486-79ff40cdfd2c))
    (fp_line (start 0 -1.33) (end 1.33 -1.33) (layer "F.SilkS") (width 0.12) (tstamp 26ffead6-ad75-4e6a-9d64-d6b97d9ec6db))
    (fp_line (start 1.33 1.21) (end 1.33 1.33) (layer "F.SilkS") (width 0.12) (tstamp 66645510-3b48-44fa-8ec1-8f8b93e0c362))
    (fp_line (start 1.33 -1.33) (end 1.33 0) (layer "F.SilkS") (width 0.12) (tstamp c4e13af5-6633-48f1-8629-b8152134479a))
    (fp_line (start -1.33 1.33) (end 1.33 1.33) (layer "F.SilkS") (width 0.12) (tstamp e074bd3d-52bd-4e41-82cd-414b78f1f604))
    (fp_line (start -1.8 1.75) (end -1.8 -1.8) (layer "F.CrtYd") (width 0.05) (tstamp 5685e210-c974-4840-9435-b9d0020cc825))
    (fp_line (start 1.75 1.75) (end -1.8 1.75) (layer "F.CrtYd") (width 0.05) (tstamp 9471fa6b-ed19-4db6-9a11-19f6c348bda8))
    (fp_line (start 1.75 -1.8) (end 1.75 1.75) (layer "F.CrtYd") (width 0.05) (tstamp cb33e669-03e7-4837-bac2-5e2fd82aee65))
    (fp_line (start -1.8 -1.8) (end 1.75 -1.8) (layer "F.CrtYd") (width 0.05) (tstamp d3ccd58b-22f4-498a-8266-0e1ad455732e))
    (fp_line (start 1.27 1.27) (end -1.27 1.27) (layer "F.Fab") (width 0.1) (tstamp 314e63cb-26d9-43b6-ade2-57b55fdc20f1))
    (fp_line (start 1.27 -0.635) (end 1.27 1.27) (layer "F.Fab") (width 0.1) (tstamp 7fd5ea97-b884-4dfc-b16b-112f94672aa4))
    (fp_line (start -1.27 1.27) (end -1.27 -1.27) (layer "F.Fab") (width 0.1) (tstamp b4389b70-5e9d-4ec2-a19a-edc38a0a0e5e))
    (fp_line (start 0.635 -1.27) (end 1.27 -0.635) (layer "F.Fab") (width 0.1) (tstamp c45d4a7b-620e-414d-98e6-d2cfd4b3eb78))
    (fp_line (start -1.27 -1.27) (end 0.635 -1.27) (layer "F.Fab") (width 0.1) (tstamp f9c9517c-a7e0-4faa-9a6a-cc97580e54b5))
    (pad "1" thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 "/B2") (pinfunction "Pin_1") (pintype "passive") (tstamp fb43dd2a-3665-4a07-9a1c-9466a55acca2))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x01_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "MountingHole:MountingHole_2mm" (layer "F.Cu")
    (tedit 5B924920) (tstamp 4b3bd353-e23b-4381-a49d-331e8e7f8e36)
    (at 48.5 46.5)
    (descr "Mounting Hole 2mm, no annular")
    (tags "mounting hole 2mm no annular")
    (property "Sheetfile" "heaters.kicad_sch")
    (property "Sheetname" "")
    (path "/7bd85fc7-0166-4e29-a2c6-e5ce5ba3ac69")
    (attr exclude_from_pos_files)
    (fp_text reference "H1" (at 0 -3.2) (layer "F.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp dec6cb8d-ab2c-4726-aeaf-565ec70a4173)
    )
    (fp_text value "MountingHole" (at 0 3.1) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 3d0a9aef-4558-4807-bd14-0822793332e4)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 51c33f27-873c-4956-b44e-87b5bf9d68ad)
    )
    (fp_circle (center 0 0) (end 2 0) (layer "Cmts.User") (width 0.15) (fill none) (tstamp 6e473a15-1e6f-4ec7-b210-2edc99dd0470))
    (fp_circle (center 0 0) (end 2.25 0) (layer "F.CrtYd") (width 0.05) (fill none) (tstamp 514239ff-97a6-4f50-99ac-0a6fdaeceb0e))
    (pad "" np_thru_hole circle (at 0 0) (size 2 2) (drill 2) (layers *.Cu *.Mask) (tstamp d5963364-7a3c-4e41-a3b3-3295149fa97c))
  )

  (footprint "MountingHole:MountingHole_3.2mm_M3" (layer "F.Cu")
    (tedit 56D1B4CB) (tstamp 554ec71b-aa51-4917-b165-421fadcef4d3)
    (at 168 53.5)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (property "Sheetfile" "heaters.kicad_sch")
    (property "Sheetname" "")
    (path "/19e980a7-c598-45a0-b341-97e0237187de")
    (attr exclude_from_pos_files)
    (fp_text reference "H8" (at 0 -4.2) (layer "F.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 54546705-0ccc-4586-97a2-ee539852d3da)
    )
    (fp_text value "MountingHole" (at 0 4.2) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 60503685-c766-436f-9aaf-4765b229fa38)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp e6b7dd81-f393-4d11-9834-87b03373d535)
    )
    (fp_circle (center 0 0) (end 3.2 0) (layer "Cmts.User") (width 0.15) (fill none) (tstamp dd4aeb9c-fce7-4857-bf0b-1b64da9fee3f))
    (fp_circle (center 0 0) (end 3.45 0) (layer "F.CrtYd") (width 0.05) (fill none) (tstamp cc73d9c7-ac96-4256-9d80-b752f07957dd))
    (pad "" np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask) (tstamp 512d0664-6bf5-4718-b17a-84db1e69da2c))
  )

  (footprint "J8:avia8" (layer "F.Cu")
    (tedit 0) (tstamp 6001f7f8-fd60-4aae-9f98-e881e3218432)
    (at 234.73 53.5 -90)
    (property "Sheetfile" "heaters.kicad_sch")
    (property "Sheetname" "")
    (path "/a7cf3f80-74d7-4eb9-a9c6-6f537f05d948")
    (attr through_hole)
    (fp_text reference "J5" (at -0.0508 -4.4196 -90 unlocked) (layer "F.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 6ea82021-9e23-49f6-8f06-9acb6a0226ef)
    )
    (fp_text value "Conn_01x08" (at 0.0254 4.2926 -90 unlocked) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 357fe868-b5fb-4257-a969-7960eb8fe134)
    )
    (pad "" np_thru_hole circle (at -8.382 -5.2832 270) (size 2.8 2.8) (drill 2.4) (layers F&B.Cu *.Mask) (tstamp 49423981-2164-4449-8a44-a5303637dad7))
    (pad "" np_thru_hole circle (at 7.5184 -1.27 270) (size 2.5 2.5) (drill 2.2) (layers F&B.Cu *.Mask) (tstamp a5f966ab-658c-44cc-9803-7e303723400e))
    (pad "" np_thru_hole circle (at -7.5184 -1.27 270) (size 2.5 2.5) (drill 2.2) (layers F&B.Cu *.Mask) (tstamp f1aed676-378d-4cc8-98ad-4880ebb93fdf))
    (pad "" np_thru_hole circle (at 8.382 -5.2832 270) (size 2.8 2.8) (drill 2.4) (layers F&B.Cu *.Mask) (tstamp f5c5ea99-15f3-4af7-996a-1d9ad7a111e3))
    (pad "1" thru_hole circle (at -2.0828 -2.54 270) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 1 "/A1") (pinfunction "Pin_1") (pintype "passive") (tstamp ecdd6e3d-f2a0-4903-a6fb-3120eb0047d9))
    (pad "2" thru_hole circle (at 0 -2.54 270) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 1 "/A1") (pinfunction "Pin_2") (pintype "passive") (tstamp d1a622dd-515b-4f59-969f-2a54d36f5be2))
    (pad "3" thru_hole circle (at 2.0828 -2.54 270) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 2 "/A2") (pinfunction "Pin_3") (pintype "passive") (tstamp 407e264d-8a10-4f11-a576-f100857c11af))
    (pad "4" thru_hole circle (at -2.7178 0 270) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 4 "/B2") (pinfunction "Pin_4") (pintype "passive") (tstamp 13912a32-6e61-44a5-8669-322ff4388ad3))
    (pad "5" thru_hole circle (at 0 0 270) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 4 "/B2") (pinfunction "Pin_5") (pintype "passive") (tstamp 6a08f3b1-efd6-4261-a745-16c0fe608e81))
    (pad "6" thru_hole circle (at 2.7178 0 270) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 2 "/A2") (pinfunction "Pin_6") (pintype "passive") (tstamp cabcb6a7-9ad9-46da-9a77-0f3c8633a9b2))
    (pad "7" thru_hole circle (at -1.4986 2.54 270) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 3 "/B1") (pinfunction "Pin_7") (pintype "passive") (tstamp 1c0c55ce-fcbe-4f43-bbd8-33e98eba8f2f))
    (pad "8" thru_hole circle (at 1.4986 2.54 270) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 3 "/B1") (pinfunction "Pin_8") (pintype "passive") (tstamp 17d84e33-3e84-41e6-b1b3-27874be7877b))
  )

  (footprint "Connector_PinSocket_2.54mm:PinSocket_1x01_P2.54mm_Vertical" (layer "F.Cu")
    (tedit 5A19A434) (tstamp 76884387-867c-49ea-b6ad-1b4c7b0691d6)
    (at 94 46)
    (descr "Through hole straight socket strip, 1x01, 2.54mm pitch, single row (from Kicad 4.0.7), script generated")
    (tags "Through hole socket strip THT 1x01 2.54mm single row")
    (property "Sheetfile" "heaters.kicad_sch")
    (property "Sheetname" "")
    (path "/ce4a47b3-c029-4ade-bf61-efd39dc93791")
    (attr through_hole)
    (fp_text reference "J1" (at 0 -2.77) (layer "F.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 4618513c-0cb5-4f10-a336-953d9128b247)
    )
    (fp_text value "Conn_01x01" (at 0 2.77) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp db72bedd-ff1a-49b6-a2ea-7e44df618c87)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp e26e0753-2683-4b55-8d7c-d6d743bc0d10)
    )
    (fp_line (start 0 -1.33) (end 1.33 -1.33) (layer "F.SilkS") (width 0.12) (tstamp 1855cb5c-c8eb-487e-a056-0bbf96f0958e))
    (fp_line (start 1.33 1.21) (end 1.33 1.33) (layer "F.SilkS") (width 0.12) (tstamp 4f395c06-9346-48ed-9e72-5b1a08b51dd1))
    (fp_line (start -1.33 1.21) (end -1.33 1.33) (layer "F.SilkS") (width 0.12) (tstamp 7ed9b45d-27bc-4e5d-b53f-d4260362f79f))
    (fp_line (start 1.33 -1.33) (end 1.33 0) (layer "F.SilkS") (width 0.12) (tstamp 862d8f16-5a06-4ecd-8fb3-76a322098df7))
    (fp_line (start -1.33 1.33) (end 1.33 1.33) (layer "F.SilkS") (width 0.12) (tstamp cd45b4d0-9aae-4278-aa6b-9cb3d3f8ade3))
    (fp_line (start 1.75 1.75) (end -1.8 1.75) (layer "F.CrtYd") (width 0.05) (tstamp 5c7afdf5-c150-4ad6-9041-c98bdbcbf42d))
    (fp_line (start -1.8 -1.8) (end 1.75 -1.8) (layer "F.CrtYd") (width 0.05) (tstamp 77eea4c0-5d0d-476d-a797-7cf21c9f013f))
    (fp_line (start -1.8 1.75) (end -1.8 -1.8) (layer "F.CrtYd") (width 0.05) (tstamp 85b9e30b-e61d-4c66-9f6d-88fcfd81e67a))
    (fp_line (start 1.75 -1.8) (end 1.75 1.75) (layer "F.CrtYd") (width 0.05) (tstamp 8b16d322-b854-44b1-b76c-9a1caa15c27a))
    (fp_line (start 1.27 1.27) (end -1.27 1.27) (layer "F.Fab") (width 0.1) (tstamp 0c81af18-b6aa-4163-8111-a40391300750))
    (fp_line (start 0.635 -1.27) (end 1.27 -0.635) (layer "F.Fab") (width 0.1) (tstamp c6e0b33a-0148-4473-b9dc-61b1bea3728c))
    (fp_line (start -1.27 -1.27) (end 0.635 -1.27) (layer "F.Fab") (width 0.1) (tstamp e2f488bd-298e-4cad-8968-2f1dfd3ae6f1))
    (fp_line (start -1.27 1.27) (end -1.27 -1.27) (layer "F.Fab") (width 0.1) (tstamp e3efd6b9-59eb-4af8-84a1-efc64b739564))
    (fp_line (start 1.27 -0.635) (end 1.27 1.27) (layer "F.Fab") (width 0.1) (tstamp f80c7adf-54f9-4d6f-bb79-9973c03e38e3))
    (pad "1" thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "/A1") (pinfunction "Pin_1") (pintype "passive") (tstamp 9829ad21-e846-4faf-884c-160a20b8af4b))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x01_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "MountingHole:MountingHole_3.2mm_M3" (layer "F.Cu")
    (tedit 56D1B4CB) (tstamp 8c1775d7-c302-4d77-8542-6bb27789b556)
    (at 124 53.5)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (property "Sheetfile" "heaters.kicad_sch")
    (property "Sheetname" "")
    (path "/115c0ca5-b5d5-45b8-9907-1a92b1479d9a")
    (attr exclude_from_pos_files)
    (fp_text reference "H5" (at 0 -4.2) (layer "F.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp e6f33c9a-d5c1-4e66-a9bf-be62ef6d8b83)
    )
    (fp_text value "MountingHole" (at 0 4.2) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 6e7a00ce-d442-43e5-a529-8fc586fc5f55)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 01f0362d-33a7-47da-8d09-9d5bfdd7ce93)
    )
    (fp_circle (center 0 0) (end 3.2 0) (layer "Cmts.User") (width 0.15) (fill none) (tstamp 8604e778-e830-4a54-8546-b66a81bcfdbf))
    (fp_circle (center 0 0) (end 3.45 0) (layer "F.CrtYd") (width 0.05) (fill none) (tstamp 0b6d851b-54eb-49e4-8828-378243970e72))
    (pad "" np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask) (tstamp c870eee1-ed7a-4c1d-97e7-0964a62c592f))
  )

  (footprint "MountingHole:MountingHole_3.2mm_M3" (layer "F.Cu")
    (tedit 56D1B4CB) (tstamp 9204441e-1cd5-4125-bc55-fb320654d811)
    (at 86 53.5)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (property "Sheetfile" "heaters.kicad_sch")
    (property "Sheetname" "")
    (path "/90d62700-4d23-4d16-b6fa-43f7008b64dd")
    (attr exclude_from_pos_files)
    (fp_text reference "H7" (at 0 -4.2) (layer "F.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp cdc2b836-47bb-4a7c-9afc-18c4cf69b540)
    )
    (fp_text value "MountingHole" (at 0 4.2) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 42d91210-189a-4632-acb1-4d6b2ea8ca87)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp b2800f4d-684e-44f0-8a6f-7e1764fdc844)
    )
    (fp_circle (center 0 0) (end 3.2 0) (layer "Cmts.User") (width 0.15) (fill none) (tstamp bc9b92f8-8678-45f0-968f-e3d9936c6fda))
    (fp_circle (center 0 0) (end 3.45 0) (layer "F.CrtYd") (width 0.05) (fill none) (tstamp bcb55865-23eb-44e1-bbbf-78e2959176e1))
    (pad "" np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask) (tstamp 69ed75f9-0b23-411f-b3e8-124c98a6dce8))
  )

  (footprint "MountingHole:MountingHole_3.2mm_M3" (layer "F.Cu")
    (tedit 56D1B4CB) (tstamp ab44ffc8-3f7b-4462-a9b4-0614782151e5)
    (at 206 53.5)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (property "Sheetfile" "heaters.kicad_sch")
    (property "Sheetname" "")
    (path "/ed304870-922d-4c72-a05c-e9b1b5b0b3bf")
    (attr exclude_from_pos_files)
    (fp_text reference "H6" (at 0 -4.2) (layer "F.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp d6ae9ae1-23bd-471a-bcc6-2faf344fbda7)
    )
    (fp_text value "MountingHole" (at 0 4.2) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 244c566d-76d0-4491-8b11-e5ba17a04afa)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp f575e2a8-a156-43e0-88ad-897c38df2116)
    )
    (fp_circle (center 0 0) (end 3.2 0) (layer "Cmts.User") (width 0.15) (fill none) (tstamp 19e0c92b-c86b-4f11-ad00-7241c9abcfa3))
    (fp_circle (center 0 0) (end 3.45 0) (layer "F.CrtYd") (width 0.05) (fill none) (tstamp aaf7b51f-3149-41cf-9ddf-e7991194d9eb))
    (pad "" np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask) (tstamp 18fff2b8-6933-40db-8239-efe6f18672f1))
  )

  (footprint "Connector_PinSocket_2.54mm:PinSocket_1x01_P2.54mm_Vertical" (layer "F.Cu")
    (tedit 5A19A434) (tstamp b9b16cc6-5c12-45aa-918c-41be5eac6b47)
    (at 94 61)
    (descr "Through hole straight socket strip, 1x01, 2.54mm pitch, single row (from Kicad 4.0.7), script generated")
    (tags "Through hole socket strip THT 1x01 2.54mm single row")
    (property "Sheetfile" "heaters.kicad_sch")
    (property "Sheetname" "")
    (path "/0b2abee9-81dd-4993-b536-bdb1cab9295c")
    (attr through_hole)
    (fp_text reference "J3" (at 0 -2.77) (layer "F.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp b4ad0e3d-eb7a-4984-ab77-4b9e5a2800e2)
    )
    (fp_text value "Conn_01x01" (at 0 2.77) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 9176273b-c1be-4da2-93c2-2d839dd34cca)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 81ddf5ed-c95c-4864-8dc2-b5b24d2f1717)
    )
    (fp_line (start -1.33 1.33) (end 1.33 1.33) (layer "F.SilkS") (width 0.12) (tstamp 3d46e8d0-59a8-4af1-8f73-42b68842ca09))
    (fp_line (start 1.33 -1.33) (end 1.33 0) (layer "F.SilkS") (width 0.12) (tstamp 3d486377-4aa3-4103-aa92-7a7e2fedb4d7))
    (fp_line (start -1.33 1.21) (end -1.33 1.33) (layer "F.SilkS") (width 0.12) (tstamp 656d8a99-6b13-4d3b-a419-6759692cfd7c))
    (fp_line (start 1.33 1.21) (end 1.33 1.33) (layer "F.SilkS") (width 0.12) (tstamp dad01a7c-74e2-4348-883c-d07f79b56765))
    (fp_line (start 0 -1.33) (end 1.33 -1.33) (layer "F.SilkS") (width 0.12) (tstamp e618be82-2b33-46b6-81df-09c27af13066))
    (fp_line (start -1.8 -1.8) (end 1.75 -1.8) (layer "F.CrtYd") (width 0.05) (tstamp 074334e5-6a9c-45a9-b21e-c95c67ff0c18))
    (fp_line (start 1.75 1.75) (end -1.8 1.75) (layer "F.CrtYd") (width 0.05) (tstamp 0f27de26-17fc-42be-84f2-d5db048b95b0))
    (fp_line (start -1.8 1.75) (end -1.8 -1.8) (layer "F.CrtYd") (width 0.05) (tstamp 47e85a54-ccae-4dbb-a8c4-d3ed51b927e0))
    (fp_line (start 1.75 -1.8) (end 1.75 1.75) (layer "F.CrtYd") (width 0.05) (tstamp f45a26a0-0c00-4ec6-ac6b-3c4c07edca12))
    (fp_line (start 1.27 1.27) (end -1.27 1.27) (layer "F.Fab") (width 0.1) (tstamp 08422067-45be-4f72-9223-fef53879fbd1))
    (fp_line (start -1.27 1.27) (end -1.27 -1.27) (layer "F.Fab") (width 0.1) (tstamp 276af1be-5b06-4dd9-bbeb-d21042e1b393))
    (fp_line (start -1.27 -1.27) (end 0.635 -1.27) (layer "F.Fab") (width 0.1) (tstamp 29a86320-d03f-4354-8746-290faaeac863))
    (fp_line (start 0.635 -1.27) (end 1.27 -0.635) (layer "F.Fab") (width 0.1) (tstamp 2d38630d-2f56-42fa-8477-4a37fe0f5d20))
    (fp_line (start 1.27 -0.635) (end 1.27 1.27) (layer "F.Fab") (width 0.1) (tstamp 5e86399d-3739-497b-a8cf-42c840644ca9))
    (pad "1" thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 "/B1") (pinfunction "Pin_1") (pintype "passive") (tstamp 020b1542-051b-4822-bab0-3068037413b4))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x01_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "MountingHole:MountingHole_2mm" (layer "F.Cu")
    (tedit 5B924920) (tstamp f31372cc-b034-4ef2-84e5-208d90625b5e)
    (at 243.5 60.5)
    (descr "Mounting Hole 2mm, no annular")
    (tags "mounting hole 2mm no annular")
    (property "Sheetfile" "heaters.kicad_sch")
    (property "Sheetname" "")
    (path "/df93f598-22b2-427e-bf55-35c5f913b5a2")
    (attr exclude_from_pos_files)
    (fp_text reference "H2" (at 0 -3.2) (layer "F.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 2092912f-2167-4b6e-9bec-5b8d5d1eb44f)
    )
    (fp_text value "MountingHole" (at 0 3.1) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp fd5b68d0-adad-4809-959a-6170db65ac08)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 071870f8-b260-4a06-b477-98c3bc2ec3ec)
    )
    (fp_circle (center 0 0) (end 2 0) (layer "Cmts.User") (width 0.15) (fill none) (tstamp 231f3dc9-c522-472b-abcc-0d06596ce442))
    (fp_circle (center 0 0) (end 2.25 0) (layer "F.CrtYd") (width 0.05) (fill none) (tstamp 2a36e62d-99f3-4471-b917-5441027c4c0e))
    (pad "" np_thru_hole circle (at 0 0) (size 2 2) (drill 2) (layers *.Cu *.Mask) (tstamp eb1aa9c8-af12-495a-9e06-3aec79f1f3eb))
  )

  (footprint "Connector_PinSocket_2.54mm:PinSocket_1x01_P2.54mm_Vertical" (layer "F.Cu")
    (tedit 5A19A434) (tstamp f786872e-cb1f-401e-9197-d54c772f639d)
    (at 98 51.5)
    (descr "Through hole straight socket strip, 1x01, 2.54mm pitch, single row (from Kicad 4.0.7), script generated")
    (tags "Through hole socket strip THT 1x01 2.54mm single row")
    (property "Sheetfile" "heaters.kicad_sch")
    (property "Sheetname" "")
    (path "/f36eef0a-0e0b-427f-9631-756b2d2f0d43")
    (attr through_hole)
    (fp_text reference "J2" (at 0 -2.77) (layer "F.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 41fe4597-67f7-46cd-bfb8-a512f7834363)
    )
    (fp_text value "Conn_01x01" (at 0 2.77) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 442c03f6-b474-4427-8a5b-909cd76fe338)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 7195f5c5-6f08-44bb-98cb-f57eef73501f)
    )
    (fp_line (start 0 -1.33) (end 1.33 -1.33) (layer "F.SilkS") (width 0.12) (tstamp 39665140-9bd7-494e-875e-8fc786bf3406))
    (fp_line (start 1.33 -1.33) (end 1.33 0) (layer "F.SilkS") (width 0.12) (tstamp 9d7b2920-d125-4443-b7dd-a4040a757e38))
    (fp_line (start -1.33 1.21) (end -1.33 1.33) (layer "F.SilkS") (width 0.12) (tstamp a24346f4-c1ab-4dd2-8e62-b51cbea2cf9c))
    (fp_line (start 1.33 1.21) (end 1.33 1.33) (layer "F.SilkS") (width 0.12) (tstamp aa24fcff-ace7-453e-829f-302b33864352))
    (fp_line (start -1.33 1.33) (end 1.33 1.33) (layer "F.SilkS") (width 0.12) (tstamp e920c67e-5a53-4dce-8a9a-605b7dedb31a))
    (fp_line (start 1.75 -1.8) (end 1.75 1.75) (layer "F.CrtYd") (width 0.05) (tstamp 43103909-33a0-4f89-bc29-b3cbc6c408a2))
    (fp_line (start -1.8 1.75) (end -1.8 -1.8) (layer "F.CrtYd") (width 0.05) (tstamp 4fe87a72-c79d-4d35-85e3-52296faee68d))
    (fp_line (start -1.8 -1.8) (end 1.75 -1.8) (layer "F.CrtYd") (width 0.05) (tstamp b1bab0c2-d7e0-4cc6-affe-3572032353f5))
    (fp_line (start 1.75 1.75) (end -1.8 1.75) (layer "F.CrtYd") (width 0.05) (tstamp d49abc19-c285-4fc8-8911-220f95c77959))
    (fp_line (start 1.27 -0.635) (end 1.27 1.27) (layer "F.Fab") (width 0.1) (tstamp 0100720b-5770-48de-80f8-ea588c81d514))
    (fp_line (start -1.27 -1.27) (end 0.635 -1.27) (layer "F.Fab") (width 0.1) (tstamp 200e9aad-d0c2-4fd6-a3d3-e799b52f1e26))
    (fp_line (start 1.27 1.27) (end -1.27 1.27) (layer "F.Fab") (width 0.1) (tstamp 54972670-0399-4512-97cf-a265d475ad26))
    (fp_line (start 0.635 -1.27) (end 1.27 -0.635) (layer "F.Fab") (width 0.1) (tstamp 93940992-36d5-4843-9042-1ce5454dfb77))
    (fp_line (start -1.27 1.27) (end -1.27 -1.27) (layer "F.Fab") (width 0.1) (tstamp e7f35687-b9e4-4873-98a9-e7a8e7226b80))
    (pad "1" thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 "/A2") (pinfunction "Pin_1") (pintype "passive") (tstamp d05aac1a-9d25-4195-85d5-1b47b9392b77))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x01_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (gr_line (start 46 64) (end 46 43) (layer "Dwgs.User") (width 0.2) (tstamp 053cc865-4039-435f-8e39-4a6d26d10ff8))
  (gr_circle (center 234.73 50.77676) (end 235.23 50.77676) (layer "Dwgs.User") (width 0.2) (fill none) (tstamp 05ad1eff-e556-4b51-892e-29eefb8d7ed1))
  (gr_arc (start 52 58.7) (mid 50.3 57) (end 52 55.3) (layer "Dwgs.User") (width 0.2) (tstamp 0f5f900c-b072-46cc-a57a-cc4dda0a3b27))
  (gr_circle (center 168 53.5) (end 169.7 53.5) (layer "Dwgs.User") (width 0.2) (fill none) (tstamp 10b2dca2-d3f9-4672-9d03-49943fb627e9))
  (gr_line (start 52 55.3) (end 73 55.3) (layer "Dwgs.User") (width 0.2) (tstamp 121d06f4-373c-4845-b5e3-0390519a8bf2))
  (gr_circle (center 48.5 46.5) (end 49.5 46.5) (layer "Dwgs.User") (width 0.2) (fill none) (tstamp 14e89a80-5745-47e6-a7e5-f477e562442c))
  (gr_circle (center 240 61.889089) (end 241.2 61.889089) (layer "Dwgs.User") (width 0.2) (fill none) (tstamp 2c90f0e8-f568-48d9-ac15-33eea0c9e2b7))
  (gr_circle (center 124 53.5) (end 125.7 53.5) (layer "Dwgs.User") (width 0.2) (fill none) (tstamp 2cc562b1-9016-434e-9a5d-12b3567c4873))
  (gr_arc (start 52 51.7) (mid 50.3 50) (end 52 48.3) (layer "Dwgs.User") (width 0.2) (tstamp 37cb69d2-07c0-4f4b-bad3-eb0a3b509135))
  (gr_circle (center 236 61) (end 237.1 61) (layer "Dwgs.User") (width 0.2) (fill none) (tstamp 3db12966-abeb-4709-bd28-d69c5bd17882))
  (gr_arc (start 73 55.3) (mid 74.7 57) (end 73 58.7) (layer "Dwgs.User") (width 0.2) (tstamp 408883b0-ceb5-4ec9-a6dd-360973b16c1c))
  (gr_line (start 52 48.3) (end 73 48.3) (layer "Dwgs.User") (width 0.2) (tstamp 41def56d-5288-4403-bf75-7653a969f34b))
  (gr_circle (center 86 53.5) (end 87.7 53.5) (layer "Dwgs.User") (width 0.2) (fill none) (tstamp 4e38b072-9092-482e-aafe-7a23bad88d6a))
  (gr_arc (start 73 48.3) (mid 74.7 50) (end 73 51.7) (layer "Dwgs.User") (width 0.2) (tstamp 6161a890-143c-4d39-8928-40f8e873ede6))
  (gr_line (start 73 51.7) (end 52 51.7) (layer "Dwgs.User") (width 0.2) (tstamp 6292207a-889b-49d4-ae8d-9bee24d0546d))
  (gr_line (start 46 43) (end 246 43) (layer "Dwgs.User") (width 0.2) (tstamp 63106a6d-65bd-4224-b386-fb65eae1d712))
  (gr_line (start 246 64) (end 46 64) (layer "Dwgs.User") (width 0.2) (tstamp 664e2d08-e933-46a5-8b6f-9ddfb61b89a0))
  (gr_circle (center 236 46) (end 237.1 46) (layer "Dwgs.User") (width 0.2) (fill none) (tstamp 668362f3-d1fc-471b-bd2e-a0918aa19f31))
  (gr_circle (center 232.19 54.99776) (end 232.69 54.99776) (layer "Dwgs.User") (width 0.2) (fill none) (tstamp 748f7619-97f1-4d7e-a6dc-01c6ead56dfb))
  (gr_circle (center 232.19 52.00224) (end 232.69 52.00224) (layer "Dwgs.User") (width 0.2) (fill none) (tstamp 7b8e0df8-1270-49b1-b601-5ba2c6e1e9fe))
  (gr_circle (center 206 53.5) (end 207.7 53.5) (layer "Dwgs.User") (width 0.2) (fill none) (tstamp 7c2a7a78-2959-4595-b8e0-f300e6055de2))
  (gr_line (start 234.73 50.77676) (end 234.73 56.22324) (layer "Dwgs.User") (width 0.13) (tstamp 7dc94ddd-ad0b-43f6-bf2e-b3e6ca70b254))
  (gr_line (start 246 43) (end 246 64) (layer "Dwgs.User") (width 0.2) (tstamp 851d27f1-7919-4a57-ba0b-d9740ad24862))
  (gr_circle (center 243.5 46.5) (end 244.5 46.5) (layer "Dwgs.User") (width 0.2) (fill none) (tstamp 8801c231-e21a-406f-b098-f9bc0c6e0b65))
  (gr_circle (center 234.73 53.5) (end 235.23 53.5) (layer "Dwgs.User") (width 0.2) (fill none) (tstamp 8bef6a00-8ec1-4bd9-acb0-a555a18a0605))
  (gr_circle (center 48.5 60.5) (end 49.5 60.5) (layer "Dwgs.User") (width 0.2) (fill none) (tstamp 91f57ccb-cdec-45f6-b4de-432cdfa12358))
  (gr_line (start 231.73 53.5) (end 237.73 53.5) (layer "Dwgs.User") (width 0.13) (tstamp 924bbcd7-a043-49aa-9cef-3219085c9b77))
  (gr_circle (center 237.27 53.5) (end 237.77 53.5) (layer "Dwgs.User") (width 0.2) (fill none) (tstamp 9fb9d60f-fad6-4f7a-a9c4-8bf6268eeb68))
  (gr_line (start 73 58.7) (end 52 58.7) (layer "Dwgs.User") (width 0.2) (tstamp baba43c8-6c30-413b-8b44-b52e6b9012e8))
  (gr_circle (center 243.5 60.5) (end 244.5 60.5) (layer "Dwgs.User") (width 0.2) (fill none) (tstamp c558fc51-f980-4e1d-924d-e99f70525276))
  (gr_circle (center 234.73 56.22324) (end 235.23 56.22324) (layer "Dwgs.User") (width 0.2) (fill none) (tstamp e05b4046-5141-41bc-864d-ccb50d5cc5d9))
  (gr_circle (center 237.27 55.57545) (end 237.77 55.57545) (layer "Dwgs.User") (width 0.2) (fill none) (tstamp e5d2747d-c035-42ce-8136-9a3472be4673))
  (gr_circle (center 240 45.110911) (end 241.2 45.110911) (layer "Dwgs.User") (width 0.2) (fill none) (tstamp e8e9656b-dba4-4f4e-b534-c0b42de4f3ae))
  (gr_circle (center 237.27 51.42455) (end 237.77 51.42455) (layer "Dwgs.User") (width 0.2) (fill none) (tstamp ff5662c8-eef4-4ebf-87ec-4227e8d02aeb))
  (gr_line (start 52 58.7) (end 73 58.7) (layer "Edge.Cuts") (width 0.1) (tstamp 16a9c69f-25a4-44e6-829c-d96d846391a7))
  (gr_line (start 52 51.7) (end 73 51.7) (layer "Edge.Cuts") (width 0.1) (tstamp 351dcc6e-f5c0-4f60-998f-da8529278dad))
  (gr_arc (start 52 58.7) (mid 50.3 57) (end 52 55.3) (layer "Edge.Cuts") (width 0.1) (tstamp 3e665cd5-b83d-4b5d-8eaa-d8bd17f95c85))
  (gr_arc (start 52 51.7) (mid 50.3 50) (end 52 48.3) (layer "Edge.Cuts") (width 0.1) (tstamp 5c1006e5-630a-4421-af09-8aea0f56830b))
  (gr_line (start 73 55.3) (end 52 55.3) (layer "Edge.Cuts") (width 0.1) (tstamp 6c6c46e2-655c-417f-a1a0-8f649a538cce))
  (gr_rect (start 46 43) (end 246 64) (layer "Edge.Cuts") (width 0.1) (fill none) (tstamp 6ef0cff2-99dd-4922-afc5-fdb5297faffe))
  (gr_arc (start 73 48.3) (mid 74.7 50) (end 73 51.7) (layer "Edge.Cuts") (width 0.1) (tstamp d4678258-e0d1-43d4-b76d-c5cf44da2327))
  (gr_arc (start 73 55.3) (mid 74.7 57) (end 73 58.7) (layer "Edge.Cuts") (width 0.1) (tstamp e9daf7f4-c667-461b-ace1-7f014143d6ab))
  (gr_line (start 73 48.3) (end 52 48.3) (layer "Edge.Cuts") (width 0.1) (tstamp f9a51828-d774-48d8-9741-7094ccfc541b))
  (gr_text "B1" (at 222.6 52) (layer "F.SilkS") (tstamp 1d190d7b-bbbd-407a-ae5a-001db751acbb)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (gr_text "B2" (at 225.1 50.8) (layer "F.SilkS") (tstamp 2450a825-ba9d-4a16-91d9-74a4a77f3d20)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (gr_text "A1" (at 227.7 51.7) (layer "F.SilkS") (tstamp 4b540318-9205-47a1-8baf-f66ec5c6938c)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (gr_text "A2" (at 225.1 56.3) (layer "F.SilkS") (tstamp 6a2d6e94-6dea-43b7-be79-75e0105b603b)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (gr_text "B2" (at 225.1 53.5) (layer "F.SilkS") (tstamp c34f27e4-3e96-4ec2-b389-7f3f12e38420)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (gr_text "A1\nA2" (at 94.2 49.6) (layer "F.SilkS") (tstamp c87d2da3-7c61-4c7e-b351-fb50b65dfd45)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (gr_text "A2\n" (at 227.7 55.6) (layer "F.SilkS") (tstamp cc07c2ec-4db3-4418-b40b-f8c4685bc15d)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (gr_text "B1" (at 222.6 55) (layer "F.SilkS") (tstamp d6d224f1-a95c-4675-a950-7ca0e405dde8)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (gr_text "B2\nB1" (at 94.7 57.3) (layer "F.SilkS") (tstamp e2937757-3fd7-458b-8298-3decacde12f8)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (gr_text "A1" (at 227.7 53.5) (layer "F.SilkS") (tstamp f5ea0a76-d8ad-4181-9719-1a0cc4969a36)
    (effects (font (size 1 1) (thickness 0.15)))
  )

  (segment (start 237.27 51.4172) (end 237.27 49.77) (width 1.5) (layer "F.Cu") (net 1) (tstamp 1c1ab6d1-42ca-408f-aa4e-c7763a26246f))
  (segment (start 102.5 47.5) (end 101 46) (width 1.5) (layer "F.Cu") (net 1) (tstamp 2e7b5e8e-7285-4e40-a073-816e1755459c))
  (segment (start 232 47.5) (end 229.5 47.5) (width 1.5) (layer "F.Cu") (net 1) (tstamp 33aaf488-02ba-4e75-81ca-539896b1ef02))
  (segment (start 236 48.5) (end 233 48.5) (width 1.5) (layer "F.Cu") (net 1) (tstamp 98a18886-b5f5-4efb-9635-d8341d983460))
  (segment (start 229.5 47.5) (end 102.5 47.5) (width 7) (layer "F.Cu") (net 1) (tstamp bdd4731d-d289-4592-9228-288abea020c5))
  (segment (start 237.27 49.77) (end 236 48.5) (width 1.5) (layer "F.Cu") (net 1) (tstamp c92ac374-837f-4632-85b5-78675890696c))
  (segment (start 233 48.5) (end 232 47.5) (width 1.5) (layer "F.Cu") (net 1) (tstamp cc52ac22-16c1-46c6-86ee-163715fed720))
  (segment (start 101 46) (end 94 46) (width 1.5) (layer "F.Cu") (net 1) (tstamp d05d0475-d046-4a1d-8e04-132adb69224c))
  (segment (start 237.27 51.4172) (end 237.27 53.5) (width 1.5) (layer "F.Cu") (net 1) (tstamp efc2bd25-e74e-4e0e-bdac-6c29777601f4))
  (segment (start 231.4478 59.5) (end 229.5 59.5) (width 1.5) (layer "F.Cu") (net 2) (tstamp 063f0413-2b6b-4128-931c-9bd22eb5646d))
  (segment (start 234.73 56.2178) (end 231.4478 59.5) (width 1.5) (layer "F.Cu") (net 2) (tstamp 08590297-e688-43d9-b0e5-d83ef4036e4e))
  (segment (start 236.635 56.2178) (end 237.27 55.5828) (width 1.5) (layer "F.Cu") (net 2) (tstamp 7d2b7c2e-e569-4333-ab76-8ad507b33603))
  (segment (start 102.5 56) (end 102.5 59.5) (width 1.5) (layer "F.Cu") (net 2) (tstamp a5104945-ed9e-45db-98df-849bb278a868))
  (segment (start 98 51.5) (end 102.5 56) (width 1.5) (layer "F.Cu") (net 2) (tstamp c1b0e8c1-cf04-4f8d-be27-afaa411dbc35))
  (segment (start 229.5 59.5) (end 102.5 59.5) (width 7) (layer "F.Cu") (net 2) (tstamp e5216910-ec9d-49e4-b257-d1bfccdf7a02))
  (segment (start 234.73 56.2178) (end 236.635 56.2178) (width 1.5) (layer "F.Cu") (net 2) (tstamp efad08e3-9a49-4348-97e0-3ddb35928d4a))
  (segment (start 232.19 52.0014) (end 232.19 54.9986) (width 1.5) (layer "B.Cu") (net 3) (tstamp 54d5aaee-d7ab-4b89-a05f-f5dc929b9e69))
  (segment (start 109 59.5) (end 102.5 59.5) (width 7) (layer "B.Cu") (net 3) (tstamp 5fd409a6-9ef2-4877-8b0d-7adc63a7325c))
  (segment (start 232.19 57.31) (end 230 59.5) (width 1.5) (layer "B.Cu") (net 3) (tstamp 7801c604-d09e-4edc-a5dc-3dc1de8308db))
  (segment (start 230 59.5) (end 109 59.5) (width 7) (layer "B.Cu") (net 3) (tstamp 9d9dab93-ee00-4c5d-9ddb-ed6f0c31070c))
  (segment (start 232.19 54.9986) (end 232.19 57.31) (width 1.5) (layer "B.Cu") (net 3) (tstamp dc50d3df-44b9-42c2-bce0-999562831c9d))
  (segment (start 101 61) (end 102.5 59.5) (width 1.5) (layer "B.Cu") (net 3) (tstamp e1576dd4-8ed1-4c0e-bc5a-c5cf14327c16))
  (segment (start 94 61) (end 101 61) (width 1.5) (layer "B.Cu") (net 3) (tstamp f9d4db64-0f26-4f7b-8a6a-e760f0a81b96))
  (segment (start 102.5 51) (end 102.5 47.5) (width 1.5) (layer "B.Cu") (net 4) (tstamp 18ac3c34-8a29-425e-a55a-3f489e73c432))
  (segment (start 227.5 47.5) (end 102.5 47.5) (width 7) (layer "B.Cu") (net 4) (tstamp 31f97889-a162-4ad5-aa50-5c9483c2b298))
  (segment (start 234.73 53.5) (end 234.73 50.7822) (width 1.5) (layer "B.Cu") (net 4) (tstamp 468aec13-7239-4e1e-a07b-4ac821f26eb4))
  (segment (start 227.5 47.5) (end 231.4478 47.5) (width 1.5) (layer "B.Cu") (net 4) (tstamp a238886b-821e-4393-a494-fbd3211b5396))
  (segment (start 98 55.5) (end 102.5 51) (width 1.5) (layer "B.Cu") (net 4) (tstamp a8c2a198-6597-4837-9a62-37fc06152598))
  (segment (start 231.4478 47.5) (end 234.73 50.7822) (width 1.5) (layer "B.Cu") (net 4) (tstamp ac11368e-901f-4899-9671-ed6687329c8f))

  (group "" (id b9ce0b43-b999-4703-8c4c-3c4e53290169)
    (members
      053cc865-4039-435f-8e39-4a6d26d10ff8
      05ad1eff-e556-4b51-892e-29eefb8d7ed1
      0f5f900c-b072-46cc-a57a-cc4dda0a3b27
      10b2dca2-d3f9-4672-9d03-49943fb627e9
      121d06f4-373c-4845-b5e3-0390519a8bf2
      14e89a80-5745-47e6-a7e5-f477e562442c
      2c90f0e8-f568-48d9-ac15-33eea0c9e2b7
      2cc562b1-9016-434e-9a5d-12b3567c4873
      37cb69d2-07c0-4f4b-bad3-eb0a3b509135
      3db12966-abeb-4709-bd28-d69c5bd17882
      408883b0-ceb5-4ec9-a6dd-360973b16c1c
      41def56d-5288-4403-bf75-7653a969f34b
      4e38b072-9092-482e-aafe-7a23bad88d6a
      6161a890-143c-4d39-8928-40f8e873ede6
      6292207a-889b-49d4-ae8d-9bee24d0546d
      63106a6d-65bd-4224-b386-fb65eae1d712
      664e2d08-e933-46a5-8b6f-9ddfb61b89a0
      668362f3-d1fc-471b-bd2e-a0918aa19f31
      748f7619-97f1-4d7e-a6dc-01c6ead56dfb
      7b8e0df8-1270-49b1-b601-5ba2c6e1e9fe
      7c2a7a78-2959-4595-b8e0-f300e6055de2
      7dc94ddd-ad0b-43f6-bf2e-b3e6ca70b254
      851d27f1-7919-4a57-ba0b-d9740ad24862
      8801c231-e21a-406f-b098-f9bc0c6e0b65
      8bef6a00-8ec1-4bd9-acb0-a555a18a0605
      91f57ccb-cdec-45f6-b4de-432cdfa12358
      924bbcd7-a043-49aa-9cef-3219085c9b77
      9fb9d60f-fad6-4f7a-a9c4-8bf6268eeb68
      baba43c8-6c30-413b-8b44-b52e6b9012e8
      c558fc51-f980-4e1d-924d-e99f70525276
      e05b4046-5141-41bc-864d-ccb50d5cc5d9
      e5d2747d-c035-42ce-8136-9a3472be4673
      e8e9656b-dba4-4f4e-b534-c0b42de4f3ae
      ff5662c8-eef4-4ebf-87ec-4227e8d02aeb
    )
  )
)
