(footprint "Pin1.5x2mm" (version 20211014) (generator pcbnew)
  (layer "F.Cu")
  (tedit 5A0F774F)
  (descr "THT pad as test Point, diameter 2.0mm, hole diameter 1.0mm")
  (tags "test point THT pad")
  (property "Sheetfile" "Canon_manage.kicad_sch")
  (property "Sheetname" "")
  (attr exclude_from_pos_files)
  (fp_text reference "J2" (at 0 -1.998) (layer "F.SilkS") hide
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp ee4fdc2c-dd6e-4f61-a237-e1523368de8c)
  )
  (fp_text value "PV" (at 0.06 -2.54 90) (layer "F.SilkS")
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 6f55ed98-044f-47d4-b2b3-7ec0112cb2ba)
  )
  (fp_text user "${REFERENCE}" (at 0 -2) (layer "F.Fab")
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 26797848-8297-40fa-8e97-1810875b684a)
  )
  (pad "1" thru_hole circle (at 0 0) (size 2 2) (drill 1.5) (layers *.Cu *.Mask) (tstamp 579e99a4-eccc-4bf4-8621-efff1fa6c28f))
)
