(module Potentiometer (layer F.Cu) (tedit 5CDABBAE)
  (descr http://www.ttelectronics.com/sites/default/files/download-files/Datasheet_PanelPot_P09xSeries.pdf)
  (tags "potentiometer vertical TT P0915N single")
  (fp_text reference REF** (at 2.5 -13.5) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text value Potentiometer (at 2.5 2) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_line (start -3.1 -9.75) (end -3.1 -12.6) (layer F.CrtYd) (width 0.05))
  (fp_line (start 8.1 -0.75) (end 6.15 -0.75) (layer F.CrtYd) (width 0.05))
  (fp_line (start -3.1 -12.6) (end 8.1 -12.6) (layer F.CrtYd) (width 0.05))
  (fp_line (start 7.97 -0.88) (end 6.15 -0.88) (layer F.SilkS) (width 0.12))
  (fp_line (start -2.97 -12.47) (end -2.97 -9.75) (layer F.SilkS) (width 0.12))
  (fp_line (start 7.97 -12.47) (end -2.97 -12.47) (layer F.SilkS) (width 0.12))
  (fp_circle (center 2.5 -7.5) (end 5.5 -7.5) (layer F.Fab) (width 0.12))
  (fp_line (start -2.85 -12.35) (end 7.85 -12.35) (layer F.Fab) (width 0.1))
  (fp_line (start -2.85 -1) (end -2.85 -12.35) (layer F.Fab) (width 0.1))
  (fp_line (start 7.85 -1) (end -2.85 -1) (layer F.Fab) (width 0.1))
  (fp_line (start 7.85 -12.35) (end 7.85 -1) (layer F.Fab) (width 0.1))
  (fp_text user %R (at 2.5 -7.5) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_line (start -1.15 -0.88) (end -2.97 -0.88) (layer F.SilkS) (width 0.12))
  (fp_line (start 6.15 1.15) (end 6.15 -0.75) (layer F.CrtYd) (width 0.05))
  (fp_line (start -1.15 -0.75) (end -3.1 -0.75) (layer F.CrtYd) (width 0.05))
  (fp_line (start -1.15 1.15) (end -1.15 -0.75) (layer F.CrtYd) (width 0.05))
  (fp_line (start 6.15 1.15) (end -1.15 1.15) (layer F.CrtYd) (width 0.05))
  (fp_line (start -3.1 -9.75) (end -4.5 -9.75) (layer F.CrtYd) (width 0.05))
  (fp_line (start -4.5 -5.25) (end -4.5 -9.75) (layer F.CrtYd) (width 0.05))
  (fp_line (start -3.1 -0.75) (end -3.1 -5.25) (layer F.CrtYd) (width 0.05))
  (fp_line (start -3.1 -5.25) (end -4.5 -5.25) (layer F.CrtYd) (width 0.05))
  (fp_line (start 8.1 -0.75) (end 8.1 -5.25) (layer F.CrtYd) (width 0.05))
  (fp_line (start 8.1 -9.75) (end 8.1 -12.6) (layer F.CrtYd) (width 0.05))
  (fp_line (start 9.5 -9.75) (end 8.1 -9.75) (layer F.CrtYd) (width 0.05))
  (fp_line (start 9.5 -5.25) (end 8.1 -5.25) (layer F.CrtYd) (width 0.05))
  (fp_line (start 9.5 -5.25) (end 9.5 -9.75) (layer F.CrtYd) (width 0.05))
  (fp_line (start -2.97 -5.25) (end -2.97 -0.88) (layer F.SilkS) (width 0.12))
  (fp_line (start 7.97 -5.25) (end 7.97 -0.88) (layer F.SilkS) (width 0.12))
  (fp_line (start 7.97 -12.47) (end 7.97 -9.75) (layer F.SilkS) (width 0.12))
  (pad "" thru_hole oval (at -2.66 -7) (size 4.5 4.5) (drill 2.2) (layers *.Cu *.Mask))
  (pad 3 thru_hole circle (at 5 0) (size 2 2) (drill 0.9) (layers *.Cu *.Mask))
  (pad 2 thru_hole circle (at 2.54 0) (size 2 2) (drill 0.9) (layers *.Cu *.Mask))
  (pad 1 thru_hole rect (at 0 0) (size 2 3) (drill 0.9) (layers *.Cu *.Mask))
  (pad "" thru_hole oval (at 7.74 -7) (size 4.5 4.5) (drill 2.2) (layers *.Cu *.Mask))
  (model ${KISYS3DMOD}/Potentiometer_THT.3dshapes/Potentiometer_TT_P0915N.wrl
    (at (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
