"Source:","/home/eddy/Docs/SAO/ELECTRONICS/STM32/F0-srcs/F0_F1_testboard/kicad/stm32.sch"
"Date:","ώΤ 16 ΝΑΡ 2019 13:55:26"
"Tool:","Eeschema (6.0.0-rc1-dev-1613-ga55d9819b)"
"Generator:","/usr/local/share/kicad/plugins/bom_csv_grouped_by_value.py"
"Component Count:","35"

"Individual Components:"

"Item","Qty","Reference(s)","Value","LibPart","Footprint","Datasheet"
"","","C1","0.1","stm32-rescue:C","Capacitor_SMD:C_0603_1608Metric_Pad1.05x0.95mm_HandSolder",""
"","","C2","0.1","stm32-rescue:C","Capacitor_SMD:C_0603_1608Metric_Pad1.05x0.95mm_HandSolder",""
"","","C3","0.1","stm32-rescue:C","Capacitor_SMD:C_0603_1608Metric_Pad1.05x0.95mm_HandSolder",""
"","","C4","47u","stm32-rescue:CP","Capacitor_Tantalum_SMD:CP_EIA-3216-18_Kemet-A_Pad1.58x1.35mm_HandSolder",""
"","","C5","12","stm32-rescue:C","Capacitor_SMD:C_0603_1608Metric_Pad1.05x0.95mm_HandSolder",""
"","","C6","12","stm32-rescue:C","Capacitor_SMD:C_0603_1608Metric_Pad1.05x0.95mm_HandSolder",""
"","","C7","0.1","stm32-rescue:C","Capacitor_SMD:C_0603_1608Metric_Pad1.05x0.95mm_HandSolder",""
"","","C8","0.1","stm32-rescue:C","Capacitor_SMD:C_0603_1608Metric_Pad1.05x0.95mm_HandSolder",""
"","","C9","0.1","stm32-rescue:C","Capacitor_SMD:C_0603_1608Metric_Pad1.05x0.95mm_HandSolder",""
"","","C10","0.1","stm32-rescue:C","Capacitor_SMD:C_0603_1608Metric_Pad1.05x0.95mm_HandSolder",""
"","","D1","LED","stm32-rescue:LED-RESCUE-stm32","LED_THT:LED_D3.0mm",""
"","","D2","IP4220CZ6","Power_Protection:SP0505BAHT","TO_SOT_Packages_SMD:SOT-23-6_Handsoldering","http://www.littelfuse.com/~/media/files/littelfuse/technical%20resources/documents/data%20sheets/sp05xxba.pdf"
"","","D3","LED","stm32-rescue:LED-RESCUE-stm32","LED_THT:LED_D5.0mm",""
"","","D4","LED","stm32-rescue:LED-RESCUE-stm32","LED_THT:LED_D5.0mm",""
"","","P1","USART1","stm32-rescue:CONN_01X03","Connector_PinHeader_2.54mm:PinHeader_1x03_P2.54mm_Vertical",""
"","","P2","USB_B","stm32-rescue:USB_A-RESCUE-stm32","Connectors_USB:USB_Micro-B_Wuerth_629105150521",""
"","","Q1","DTA114Y","Transistor_BJT:DTA114Y","TO_SOT_Packages_SMD:SOT-323_SC-70_Handsoldering",""
"","","R1","10k","stm32-rescue:R","Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder",""
"","","R2","10k","stm32-rescue:R","Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder",""
"","","R3","100k","stm32-rescue:R","Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder",""
"","","R4","220","stm32-rescue:R","Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder",""
"","","R5","220","stm32-rescue:R","Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder",""
"","","R6","220","stm32-rescue:R","Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder",""
"","","R7","22","stm32-rescue:R","Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder",""
"","","R8","22","stm32-rescue:R","Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder",""
"","","R9","1k5","stm32-rescue:R","Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder",""
"","","RV1","10k","Device:R_POT","my_footprints:Potentiometer","~"
"","","SW1","Reset","stm32-rescue:SW_Push","Button_Switch_THT:SW_PUSH_6mm",""
"","","SW2","Boot","stm32-rescue:SW_Push","Button_Switch_THT:SW_PUSH_6mm",""
"","","SW3","Button0","stm32-rescue:SW_Push","Button_Switch_THT:SW_PUSH_6mm",""
"","","SW4","Button1","stm32-rescue:SW_Push","Button_Switch_THT:SW_PUSH_6mm",""
"","","U1","LM1117-3.3","stm32-rescue:LM1117-3.3-RESCUE-stm32","TO_SOT_Packages_SMD:SOT-223",""
"","","U2","STM32F042C6Tx","stm32-rescue:STM32F042C6Tx","Package_DIP:DIP-48_W15.24mm_Socket_LongPads",""
"","","U3","USBLC6-2SC6","Power_Protection:USBLC6-2SC6","TO_SOT_Packages_SMD:SOT-23-6_Handsoldering","http://www2.st.com/resource/en/datasheet/CD00050750.pdf"
"","","Y1","8MHz","Device:Crystal","Crystal:Crystal_HC49-U_Vertical","~"



"Collated Components:"

"Item","Qty","Reference(s)","Value","LibPart","Footprint","Datasheet"
"1","7","C1, C2, C3, C7, C8, C9, C10","0.1","stm32-rescue:C","Capacitor_SMD:C_0603_1608Metric_Pad1.05x0.95mm_HandSolder",""
"2","1","C4","47u","stm32-rescue:CP","Capacitor_Tantalum_SMD:CP_EIA-3216-18_Kemet-A_Pad1.58x1.35mm_HandSolder",""
"3","2","C5, C6","12","stm32-rescue:C","Capacitor_SMD:C_0603_1608Metric_Pad1.05x0.95mm_HandSolder",""
"4","1","D1","LED","stm32-rescue:LED-RESCUE-stm32","LED_THT:LED_D3.0mm",""
"5","1","D2","IP4220CZ6","Power_Protection:SP0505BAHT","TO_SOT_Packages_SMD:SOT-23-6_Handsoldering","http://www.littelfuse.com/~/media/files/littelfuse/technical%20resources/documents/data%20sheets/sp05xxba.pdf"
"6","2","D3, D4","LED","stm32-rescue:LED-RESCUE-stm32","LED_THT:LED_D5.0mm",""
"7","1","P1","USART1","stm32-rescue:CONN_01X03","Connector_PinHeader_2.54mm:PinHeader_1x03_P2.54mm_Vertical",""
"8","1","P2","USB_B","stm32-rescue:USB_A-RESCUE-stm32","Connectors_USB:USB_Micro-B_Wuerth_629105150521",""
"9","1","Q1","DTA114Y","Transistor_BJT:DTA114Y","TO_SOT_Packages_SMD:SOT-323_SC-70_Handsoldering",""
"10","2","R1, R2","10k","stm32-rescue:R","Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder",""
"11","1","R3","100k","stm32-rescue:R","Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder",""
"12","3","R4, R5, R6","220","stm32-rescue:R","Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder",""
"13","2","R7, R8","22","stm32-rescue:R","Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder",""
"14","1","R9","1k5","stm32-rescue:R","Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder",""
"15","1","RV1","10k","Device:R_POT","my_footprints:Potentiometer","~"
"16","1","SW1","Reset","stm32-rescue:SW_Push","Button_Switch_THT:SW_PUSH_6mm",""
"17","1","SW2","Boot","stm32-rescue:SW_Push","Button_Switch_THT:SW_PUSH_6mm",""
"18","1","SW3","Button0","stm32-rescue:SW_Push","Button_Switch_THT:SW_PUSH_6mm",""
"19","1","SW4","Button1","stm32-rescue:SW_Push","Button_Switch_THT:SW_PUSH_6mm",""
"20","1","U1","LM1117-3.3","stm32-rescue:LM1117-3.3-RESCUE-stm32","TO_SOT_Packages_SMD:SOT-223",""
"21","1","U2","STM32F042C6Tx","stm32-rescue:STM32F042C6Tx","Package_DIP:DIP-48_W15.24mm_Socket_LongPads",""
"22","1","U3","USBLC6-2SC6","Power_Protection:USBLC6-2SC6","TO_SOT_Packages_SMD:SOT-23-6_Handsoldering","http://www2.st.com/resource/en/datasheet/CD00050750.pdf"
"23","1","Y1","8MHz","Device:Crystal","Crystal:Crystal_HC49-U_Vertical","~"
