(module L80-R (layer F.Cu) (tedit 5D162F3C)
  (fp_text reference U3 (at 0 4) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text value L80-R (at 0 -15) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_line (start -8 -14) (end -8 3) (layer F.SilkS) (width 0.15))
  (fp_line (start -8 3) (end 8 3) (layer F.SilkS) (width 0.15))
  (fp_line (start 8 3) (end 8 -14) (layer F.SilkS) (width 0.15))
  (fp_line (start 8 -14) (end -8 -14) (layer F.SilkS) (width 0.15))
  (fp_text user 1 (at 10 3) (layer F.SilkS)
    (effects (font (size 2.5 2.5) (thickness 0.15)))
  )
  (fp_line (start -4 3) (end -4 1) (layer F.SilkS) (width 0.15))
  (fp_line (start -4 1) (end -8 1) (layer F.SilkS) (width 0.15))
  (fp_line (start 8 2) (end 7 3) (layer F.SilkS) (width 0.15))
  (fp_text user Keepout (at 0 -8) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text user area (at 0 -3.5) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_line (start -18 -24) (end -18 13) (layer F.SilkS) (width 0.15))
  (fp_line (start -18 13) (end 18 13) (layer F.SilkS) (width 0.15))
  (fp_line (start 18 13) (end 18 -24) (layer F.SilkS) (width 0.15))
  (fp_line (start 18 -24) (end -18 -24) (layer F.SilkS) (width 0.15))
  (fp_text user "Clear area" (at 0 -22) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text user "Clear area" (at 0 -22) (layer B.SilkS)
    (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
  )
  (fp_line (start -18 -24) (end -18 13) (layer B.SilkS) (width 0.15))
  (fp_line (start -18 13) (end 18 13) (layer B.SilkS) (width 0.15))
  (fp_line (start 18 13) (end 18 -24) (layer B.SilkS) (width 0.15))
  (fp_line (start 18 -24) (end -18 -24) (layer B.SilkS) (width 0.15))
  (pad 1 smd rect (at 8 0) (size 4 2) (layers F.Cu F.Paste F.Mask))
  (pad 2 smd rect (at 8 -2.54) (size 4 2) (layers F.Cu F.Paste F.Mask))
  (pad 3 smd rect (at 8 -5.08) (size 4 2) (layers F.Cu F.Paste F.Mask))
  (pad 4 smd rect (at 8 -7.62) (size 4 2) (layers F.Cu F.Paste F.Mask))
  (pad 5 smd rect (at 8 -10.16) (size 4 2) (layers F.Cu F.Paste F.Mask))
  (pad 6 smd rect (at 8 -12.7) (size 4 2) (layers F.Cu F.Paste F.Mask))
  (pad 12 smd rect (at -8 0) (size 4 2) (layers F.Cu F.Paste F.Mask))
  (pad 11 smd rect (at -8 -2.54) (size 4 2) (layers F.Cu F.Paste F.Mask))
  (pad 10 smd rect (at -8 -5.08) (size 4 2) (layers F.Cu F.Paste F.Mask))
  (pad 9 smd rect (at -8 -7.62) (size 4 2) (layers F.Cu F.Paste F.Mask))
  (pad 8 smd rect (at -8 -10.16) (size 4 2) (layers F.Cu F.Paste F.Mask))
  (pad 7 smd rect (at -8 -12.7) (size 4 2) (layers F.Cu F.Paste F.Mask))
  (pad ~ smd circle (at 0 -5.5) (size 0.1 0.1) (layers B.Cu)
    (solder_mask_margin 1.5) (solder_paste_margin 1.5) (clearance 1.3) (zone_connect 0))
  (pad ~ smd circle (at 0 -5.5) (size 0.1 0.1) (layers F.Cu)
    (solder_mask_margin 1.5) (solder_paste_margin 1.5) (clearance 1.3) (zone_connect 0))
)
