(footprint "stepper_module" (version 20211014) (generator pcbnew)
  (layer "F.Cu")
  (tedit 0)
  (attr through_hole)
  (fp_text reference "REF**" (at 0 12.7 unlocked) (layer "F.SilkS")
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp e9ef268d-483a-4357-91b1-139955764430)
  )
  (fp_text value "stepper_module" (at 0 -11.43 unlocked) (layer "F.Fab")
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp d370eb84-6ba4-4370-bc52-6d2acc57d74c)
  )
  (pad "1" thru_hole circle (at -6.35 -8.89) (size 2 2) (drill 1.02) (layers *.Cu *.Mask) (tstamp a2d33da2-d563-436b-a1a3-758acdeb565b))
  (pad "2" thru_hole circle (at -6.35 -6.35) (size 2 2) (drill 1.02) (layers *.Cu *.Mask) (tstamp dd85fb9a-8fc2-4bdc-84a6-0d46d5a07a32))
  (pad "3" thru_hole circle (at -6.35 -3.81) (size 2 2) (drill 1.02) (layers *.Cu *.Mask) (tstamp 782cab60-593e-4433-892f-4979dff713df))
  (pad "4" thru_hole circle (at -6.35 -1.27) (size 2 2) (drill 1.02) (layers *.Cu *.Mask) (tstamp a54d6c88-d4cf-4649-a8bd-4080c645a69d))
  (pad "5" thru_hole circle (at -6.35 1.27) (size 2 2) (drill 1.02) (layers *.Cu *.Mask) (tstamp 3b8de550-2ff5-4367-ab82-0c9980ec1402))
  (pad "6" thru_hole circle (at -6.35 3.81) (size 2 2) (drill 1.02) (layers *.Cu *.Mask) (tstamp a1d8d556-ef91-446b-97cc-8ed0fd3171f7))
  (pad "7" thru_hole circle (at -6.35 6.35) (size 2 2) (drill 1.02) (layers *.Cu *.Mask) (tstamp 9589bae7-96ae-4b4a-8f9f-7ec8b63b2798))
  (pad "8" thru_hole circle (at -6.35 8.89) (size 2 2) (drill 1.02) (layers *.Cu *.Mask) (tstamp 33da6e13-2d55-4a8a-aa6f-288eb76d90b5))
  (pad "9" thru_hole circle (at 6.35 8.89) (size 2 2) (drill 1.02) (layers *.Cu *.Mask) (tstamp d887e952-00b6-438b-afe4-4b398e1effba))
  (pad "10" thru_hole circle (at 6.35 6.35) (size 2 2) (drill 1.02) (layers *.Cu *.Mask) (tstamp 8f79dd42-d977-4cdc-9d7c-c4c09f487f19))
  (pad "11" thru_hole circle (at 6.35 3.81) (size 2 2) (drill 1.02) (layers *.Cu *.Mask) (tstamp dd6131dc-e2aa-4e84-93d7-122c66847d26))
  (pad "12" thru_hole circle (at 6.35 1.27) (size 2 2) (drill 1.02) (layers *.Cu *.Mask) (tstamp ebf0dacd-1b50-4d42-9727-0c549f6416f6))
  (pad "13" thru_hole circle (at 6.35 -1.27) (size 2 2) (drill 1.02) (layers *.Cu *.Mask) (tstamp 957b7297-8b22-4062-ba89-8de011c84426))
  (pad "14" thru_hole circle (at 6.35 -3.81) (size 2 2) (drill 1.02) (layers *.Cu *.Mask) (tstamp d30d1577-c0ae-4a8e-a010-ed557135026f))
  (pad "15" thru_hole circle (at 6.35 -6.35) (size 2 2) (drill 1.02) (layers *.Cu *.Mask) (tstamp 5381b559-d206-493c-b00d-4ebf32f8f613))
  (pad "16" thru_hole circle (at 6.35 -8.89) (size 2 2) (drill 1.02) (layers *.Cu *.Mask) (tstamp 744dd6a8-522e-44e2-a16e-3c91f4ef1fb5))
  (pad "17" thru_hole circle (at -3.81 -8.89) (size 2 2) (drill 1.02) (layers *.Cu *.Mask) (tstamp a2266a45-8777-41b0-90ef-b53559c13973))
  (pad "18" thru_hole circle (at -1.27 -8.89) (size 2 2) (drill 1.02) (layers *.Cu *.Mask) (tstamp d5432cc5-d4e6-4a3f-98bd-24fa4f2661f5))
)
