"Source:","/Big/Data/00__Electronics/STM32/F0_F1_F3-LQFP48_testboard/stm32.sch"
"Date:","þÔ 24 ÉÀÎ 2021 22:21:07"
"Tool:","Eeschema 5.1.10"
"Generator:","/usr/share/kicad/plugins/bom_csv_grouped_by_value_with_fp.py"
"Component Count:","54"
"Ref","Qnty","Value","Cmp name","Footprint","Description","Vendor"
"C1, C2, C3, C7, C8, C9, C10, ","7","0.1","C","Capacitor_SMD:C_0603_1608Metric_Pad1.05x0.95mm_HandSolder","",""
"C4, ","1","47u","CP","Capacitor_Tantalum_SMD:CP_EIA-6032-28_Kemet-C_Pad2.25x2.35mm_HandSolder","",""
"C5, C6, ","2","12","C","Capacitor_SMD:C_0603_1608Metric_Pad1.05x0.95mm_HandSolder","",""
"D1, D2, D3, D4, D5, D6, ","6","LED","LED-RESCUE-stm32","LED_THT:LED_D3.0mm","",""
"J1, J5, J6, J7, J8, J9, J11, ","7","Conn_01x04_Female","Conn_01x04_Female","Connector_PinSocket_2.54mm:PinSocket_1x04_P2.54mm_Vertical","Generic connector, single row, 01x04, script generated (kicad-library-utils/schlib/autogen/connector/)",""
"J2, J4, J10, J12, ","4","Conn_01x01_Female","Conn_01x01_Female","Connector_PinSocket_2.54mm:PinSocket_1x01_P2.54mm_Vertical","Generic connector, single row, 01x01, script generated (kicad-library-utils/schlib/autogen/connector/)",""
"J3, ","1","Conn_01x02_Female","Conn_01x02_Female","Connector_PinSocket_2.54mm:PinSocket_1x02_P2.54mm_Vertical","Generic connector, single row, 01x02, script generated (kicad-library-utils/schlib/autogen/connector/)",""
"P1, ","1","USART1","Conn_01x03_Female","Connector_PinSocket_2.54mm:PinSocket_1x03_P2.54mm_Vertical","Generic connector, single row, 01x03, script generated (kicad-library-utils/schlib/autogen/connector/)",""
"P2, ","1","USART2/3","Conn_01x03_Female","Connector_PinSocket_2.54mm:PinSocket_1x03_P2.54mm_Vertical","Generic connector, single row, 01x03, script generated (kicad-library-utils/schlib/autogen/connector/)",""
"P3, ","1","USB_B","USB_A-RESCUE-stm32","Connector_USB:USB_B_OST_USB-B1HSxx_Horizontal","",""
"Q1, ","1","DTA114Y","DTA114Y","Package_TO_SOT_SMD:SOT-323_SC-70_Handsoldering","Digital PNP Transistor, 10k/47k, SOT-23",""
"R1, R2, R14, R15, ","4","4k7","R","Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder","",""
"R3, ","1","10k","R","Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder","",""
"R5, ","1","100k","R","Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder","",""
"R6, R7, R8, R9, R10, R11, ","6","220","R","Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder","",""
"R12, R13, ","2","22","R","Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder","",""
"R16, ","1","1k5","R","Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder","",""
"RV1, ","1","20k","R_POT","my_footprints:Potentiometer","Potentiometer",""
"SW1, ","1","Reset","SW_Push","Button_Switch_THT:SW_PUSH_6mm","",""
"SW2, ","1","Boot","SW_Push","Button_Switch_THT:SW_PUSH_6mm","",""
"U1, ","1","LM1117-3.3","LM1117-3.3-RESCUE-stm32","Package_TO_SOT_SMD:SOT-223","",""
"U2, ","1","STM32LQFP48","STM32F042C6Tx","Package_DIP:DIP-48_W15.24mm_Socket_LongPads","",""
"U3, ","1","USBLC6-2SC6","USBLC6-2SC6","Package_TO_SOT_SMD:SOT-23-6_Handsoldering","Bidirectional ESD Protection Diode, SOT-23-6",""
"Y1, ","1","8MHz","Crystal","Crystal:Crystal_HC49-U_Vertical","Two pin crystal",""
