(export (version D)
  (design
    (source /Big/Data/00__Electronics/STM32/F0-nolib/Servo/kicad/Servo_control.sch)
    (date "Вт 12 мар 2019 21:12:54")
    (tool "Eeschema 5.0.1")
    (sheet (number 1) (name /) (tstamps /)
      (title_block
        (title)
        (company)
        (rev)
        (date)
        (source Servo_control.sch)
        (comment (number 1) (value ""))
        (comment (number 2) (value ""))
        (comment (number 3) (value ""))
        (comment (number 4) (value "")))))
  (components
    (comp (ref C4)
      (value 47u)
      (footprint Capacitor_Tantalum_SMD:CP_EIA-3216-18_Kemet-A_Pad1.53x1.40mm_HandSolder)
      (libsource (lib Servo_control-rescue) (part CP-Chiller_control-rescue) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 58C454F6))
    (comp (ref C3)
      (value 0.1)
      (footprint Capacitor_SMD:C_0603_1608Metric_Pad0.84x1.00mm_HandSolder)
      (libsource (lib Servo_control-rescue) (part C-Chiller_control-rescue) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 590D4150))
    (comp (ref C2)
      (value 0.1)
      (footprint Capacitor_SMD:C_0603_1608Metric_Pad0.84x1.00mm_HandSolder)
      (libsource (lib Servo_control-rescue) (part C-Chiller_control-rescue) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 590D4832))
    (comp (ref SW2)
      (value Boot)
      (footprint Button_Switch_SMD:SW_SPST_FSMSM)
      (libsource (lib Servo_control-rescue) (part SW_Push-Chiller_control-rescue) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5909F6B6))
    (comp (ref SW1)
      (value Reset)
      (footprint Button_Switch_SMD:SW_SPST_FSMSM)
      (libsource (lib Servo_control-rescue) (part SW_Push-Chiller_control-rescue) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 590A0134))
    (comp (ref C1)
      (value 0.1)
      (footprint Capacitor_SMD:C_0603_1608Metric_Pad0.84x1.00mm_HandSolder)
      (libsource (lib Servo_control-rescue) (part C-Chiller_control-rescue) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5A178C32))
    (comp (ref C13)
      (value 1u)
      (footprint Capacitor_SMD:C_0805_2012Metric_Pad1.15x1.50mm_HandSolder)
      (libsource (lib Servo_control-rescue) (part C-Chiller_control-rescue) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5A1AB970))
    (comp (ref U1)
      (value LM1117-3.3)
      (footprint Package_TO_SOT_SMD:SOT-223-3_TabPin2)
      (libsource (lib Servo_control-rescue) (part LM1117-3.3-Chiller_control-rescue) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5A2588E7))
    (comp (ref C5)
      (value 0.1)
      (footprint Capacitor_SMD:C_0603_1608Metric_Pad0.84x1.00mm_HandSolder)
      (libsource (lib Servo_control-rescue) (part C-Chiller_control-rescue) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5BEE1D09))
    (comp (ref L1)
      (value "BMBA 0.1mH")
      (footprint Inductor_SMD:L_0805_2012Metric_Pad1.15x1.50mm_HandSolder)
      (libsource (lib Servo_control-rescue) (part L-Chiller_control-rescue) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5BEE7949))
    (comp (ref C14)
      (value 10u)
      (footprint Capacitor_SMD:C_1206_3216Metric_Pad1.24x1.80mm_HandSolder)
      (libsource (lib Servo_control-rescue) (part C-Chiller_control-rescue) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5BEE8065))
    (comp (ref R15)
      (value 10k)
      (footprint Resistor_SMD:R_0805_2012Metric_Pad1.15x1.50mm_HandSolder)
      (libsource (lib Servo_control-rescue) (part R-Chiller_control-rescue) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5BEEBD18))
    (comp (ref R12)
      (value 510)
      (footprint Resistor_SMD:R_0805_2012Metric_Pad1.15x1.50mm_HandSolder)
      (libsource (lib Servo_control-rescue) (part R-Chiller_control-rescue) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5BEEBD1E))
    (comp (ref Q3)
      (value 2N7002)
      (footprint Package_TO_SOT_SMD:SOT-23)
      (libsource (lib Servo_control-rescue) (part Q_NMOS_GSD-Chiller_control-rescue) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5BEEBD24))
    (comp (ref Q2)
      (value SI2300)
      (footprint Package_TO_SOT_SMD:SOT-23)
      (libsource (lib Servo_control-rescue) (part Q_NMOS_GSD-Chiller_control-rescue) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5BEEB585))
    (comp (ref BZ1)
      (value Buzzer)
      (footprint Buzzer_Beeper:Buzzer_12x9.5RM7.6)
      (datasheet ~)
      (libsource (lib Device) (part Buzzer) (description "Buzzer, polar"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C83133C))
    (comp (ref Q4)
      (value 2N7002)
      (footprint Package_TO_SOT_SMD:SOT-23)
      (libsource (lib Servo_control-rescue) (part Q_NMOS_GSD-Chiller_control-rescue) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C8882AE))
    (comp (ref Q5)
      (value 2N7002)
      (footprint Package_TO_SOT_SMD:SOT-23)
      (libsource (lib Servo_control-rescue) (part Q_NMOS_GSD-Chiller_control-rescue) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C888320))
    (comp (ref J7)
      (value Servo1)
      (footprint Connector_PinHeader_2.54mm:PinHeader_1x03_P2.54mm_Vertical)
      (datasheet ~)
      (libsource (lib Connector_Generic) (part Conn_01x03) (description "Generic connector, single row, 01x03, script generated (kicad-library-utils/schlib/autogen/connector/)"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C88A162))
    (comp (ref J8)
      (value Servo2)
      (footprint Connector_PinHeader_2.54mm:PinHeader_1x03_P2.54mm_Vertical)
      (datasheet ~)
      (libsource (lib Connector_Generic) (part Conn_01x03) (description "Generic connector, single row, 01x03, script generated (kicad-library-utils/schlib/autogen/connector/)"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C83F212))
    (comp (ref J9)
      (value Servo3)
      (footprint Connector_PinHeader_2.54mm:PinHeader_1x03_P2.54mm_Vertical)
      (datasheet ~)
      (libsource (lib Connector_Generic) (part Conn_01x03) (description "Generic connector, single row, 01x03, script generated (kicad-library-utils/schlib/autogen/connector/)"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C83F4E9))
    (comp (ref R13)
      (value 510)
      (footprint Resistor_SMD:R_0805_2012Metric_Pad1.15x1.50mm_HandSolder)
      (libsource (lib Servo_control-rescue) (part R-Chiller_control-rescue) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C84B03F))
    (comp (ref R14)
      (value 510)
      (footprint Resistor_SMD:R_0805_2012Metric_Pad1.15x1.50mm_HandSolder)
      (libsource (lib Servo_control-rescue) (part R-Chiller_control-rescue) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C84B0D1))
    (comp (ref R16)
      (value 10k)
      (footprint Resistor_SMD:R_0805_2012Metric_Pad1.15x1.50mm_HandSolder)
      (libsource (lib Servo_control-rescue) (part R-Chiller_control-rescue) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C84B278))
    (comp (ref R17)
      (value 10k)
      (footprint Resistor_SMD:R_0805_2012Metric_Pad1.15x1.50mm_HandSolder)
      (libsource (lib Servo_control-rescue) (part R-Chiller_control-rescue) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C84B3BD))
    (comp (ref D2)
      (value SP0504BAHT)
      (footprint Package_TO_SOT_SMD:SOT-23-5)
      (datasheet http://www.littelfuse.com/~/media/files/littelfuse/technical%20resources/documents/data%20sheets/sp05xxba.pdf)
      (libsource (lib Power_Protection) (part SP0504BAHT) (description "TVS Diode Array, 5.5V Standoff, 4 Channels, SOT-23-5 package"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C8580E1))
    (comp (ref J2)
      (value ADC_in)
      (footprint Connector_PinHeader_2.54mm:PinHeader_1x06_P2.54mm_Vertical)
      (datasheet ~)
      (libsource (lib Connector_Generic) (part Conn_01x06) (description "Generic connector, single row, 01x06, script generated (kicad-library-utils/schlib/autogen/connector/)"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C85A71E))
    (comp (ref R3)
      (value 220)
      (footprint Resistor_SMD:R_0805_2012Metric_Pad1.15x1.50mm_HandSolder)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C85BD06))
    (comp (ref R4)
      (value 220)
      (footprint Resistor_SMD:R_0805_2012Metric_Pad1.15x1.50mm_HandSolder)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C85C1A1))
    (comp (ref R5)
      (value 220)
      (footprint Resistor_SMD:R_0805_2012Metric_Pad1.15x1.50mm_HandSolder)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C85C24A))
    (comp (ref R2)
      (value 220)
      (footprint Resistor_SMD:R_0805_2012Metric_Pad1.15x1.50mm_HandSolder)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C85C2A8))
    (comp (ref C8)
      (value 0.1)
      (footprint Capacitor_SMD:C_0603_1608Metric_Pad0.84x1.00mm_HandSolder)
      (libsource (lib Servo_control-rescue) (part C-Chiller_control-rescue) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C86267B))
    (comp (ref C10)
      (value 0.1)
      (footprint Capacitor_SMD:C_0603_1608Metric_Pad0.84x1.00mm_HandSolder)
      (libsource (lib Servo_control-rescue) (part C-Chiller_control-rescue) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C862E72))
    (comp (ref C11)
      (value 0.1)
      (footprint Capacitor_SMD:C_0603_1608Metric_Pad0.84x1.00mm_HandSolder)
      (libsource (lib Servo_control-rescue) (part C-Chiller_control-rescue) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C862EDE))
    (comp (ref C12)
      (value 0.1)
      (footprint Capacitor_SMD:C_0603_1608Metric_Pad0.84x1.00mm_HandSolder)
      (libsource (lib Servo_control-rescue) (part C-Chiller_control-rescue) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C864D09))
    (comp (ref U2)
      (value CH340G)
      (footprint Package_SOIC:SOIC-16_3.9x9.9mm_P1.27mm)
      (libsource (lib ch34x) (part CH340G) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C891E7A))
    (comp (ref C6)
      (value 0.1)
      (footprint Capacitor_SMD:C_0603_1608Metric_Pad0.84x1.00mm_HandSolder)
      (libsource (lib Servo_control-rescue) (part C-Chiller_control-rescue) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C8AFE6B))
    (comp (ref Y1)
      (value 12MHz)
      (footprint Crystal:Crystal_HC49-U_Vertical)
      (libsource (lib Device) (part Crystal) (description "Two pin crystal"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C8CDA20))
    (comp (ref C7)
      (value 22p)
      (footprint Capacitor_SMD:C_0603_1608Metric_Pad0.84x1.00mm_HandSolder)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C8CDF63))
    (comp (ref C9)
      (value 22p)
      (footprint Capacitor_SMD:C_0603_1608Metric_Pad0.84x1.00mm_HandSolder)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C8CE285))
    (comp (ref Q1)
      (value 2N7002)
      (footprint Package_TO_SOT_SMD:SOT-23)
      (libsource (lib Servo_control-rescue) (part Q_NMOS_GSD-Chiller_control-rescue) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C9233AA))
    (comp (ref R8)
      (value 510)
      (footprint Resistor_SMD:R_0805_2012Metric_Pad1.15x1.50mm_HandSolder)
      (libsource (lib Servo_control-rescue) (part R-Chiller_control-rescue) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C924EC0))
    (comp (ref R9)
      (value 10k)
      (footprint Resistor_SMD:R_0805_2012Metric_Pad1.15x1.50mm_HandSolder)
      (libsource (lib Servo_control-rescue) (part R-Chiller_control-rescue) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C924F9E))
    (comp (ref R6)
      (value 510)
      (footprint Resistor_SMD:R_0805_2012Metric_Pad1.15x1.50mm_HandSolder)
      (libsource (lib Servo_control-rescue) (part R-Chiller_control-rescue) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C929CAD))
    (comp (ref R7)
      (value 10k)
      (footprint Resistor_SMD:R_0805_2012Metric_Pad1.15x1.50mm_HandSolder)
      (libsource (lib Servo_control-rescue) (part R-Chiller_control-rescue) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C929D7F))
    (comp (ref J6)
      (value Ext_LED)
      (footprint Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical)
      (datasheet ~)
      (libsource (lib Connector_Generic) (part Conn_01x02) (description "Generic connector, single row, 01x02, script generated (kicad-library-utils/schlib/autogen/connector/)"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C93CB05))
    (comp (ref R1)
      (value 10k)
      (footprint Resistor_SMD:R_0805_2012Metric_Pad1.15x1.50mm_HandSolder)
      (libsource (lib Servo_control-rescue) (part R-Chiller_control-rescue) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C943CF3))
    (comp (ref D3)
      (value SMAJ5.0)
      (footprint Diode_SMD:D_SMA_Handsoldering)
      (libsource (lib Device) (part D) (description Diode))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C95243A))
    (comp (ref D4)
      (value SMAJ5.0)
      (footprint Diode_SMD:D_SMA_Handsoldering)
      (libsource (lib Device) (part D) (description Diode))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C952A1B))
    (comp (ref R10)
      (value 1k)
      (footprint Resistor_SMD:R_0805_2012Metric_Pad1.15x1.50mm_HandSolder)
      (libsource (lib Servo_control-rescue) (part R-Chiller_control-rescue) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C957A49))
    (comp (ref R11)
      (value 1k)
      (footprint Resistor_SMD:R_0805_2012Metric_Pad1.15x1.50mm_HandSolder)
      (libsource (lib Servo_control-rescue) (part R-Chiller_control-rescue) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C957B70))
    (comp (ref J5)
      (value Dig_In)
      (footprint Connector_PinHeader_2.54mm:PinHeader_1x03_P2.54mm_Vertical)
      (datasheet ~)
      (libsource (lib Connector_Generic) (part Conn_01x03) (description "Generic connector, single row, 01x03, script generated (kicad-library-utils/schlib/autogen/connector/)"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C9581BA))
    (comp (ref J3)
      (value Jumper0)
      (footprint Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical)
      (datasheet ~)
      (libsource (lib Connector_Generic) (part Conn_01x02) (description "Generic connector, single row, 01x02, script generated (kicad-library-utils/schlib/autogen/connector/)"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C98F117))
    (comp (ref J4)
      (value Jumper1)
      (footprint Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical)
      (datasheet ~)
      (libsource (lib Connector_Generic) (part Conn_01x02) (description "Generic connector, single row, 01x02, script generated (kicad-library-utils/schlib/autogen/connector/)"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C98F3D6))
    (comp (ref J1)
      (value USB_B_Micro)
      (footprint Connector_USB:USB_Micro-B_Wuerth-629105150521)
      (datasheet ~)
      (libsource (lib Connector_Specialized) (part USB_B_Micro) (description "USB Micro Type B connector"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C8BC41C))
    (comp (ref D1)
      (value USB6B1)
      (footprint Package_SOIC:SOIC-8_3.9x4.9mm_P1.27mm)
      (libsource (lib elements) (part USB6B1) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C9BF24E))
    (comp (ref U3)
      (value STM32F030F4Px)
      (footprint Package_SSOP:TSSOP-20_4.4x6.5mm_P0.65mm)
      (libsource (lib Servo_control-rescue) (part STM32F030F4Px-Chiller_control-rescue) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5A189F52))
    (comp (ref D5)
      (value SS14)
      (footprint Diode_SMD:D_SMA_Handsoldering)
      (libsource (lib Device) (part D_Schottky) (description "Schottky diode"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C886D5C))
    (comp (ref J10)
      (value 5V)
      (footprint Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical)
      (datasheet ~)
      (libsource (lib Connector_Generic) (part Conn_01x02) (description "Generic connector, single row, 01x02, script generated (kicad-library-utils/schlib/autogen/connector/)"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C8877B6)))
  (libparts
    (libpart (lib Connector_Generic) (part Conn_01x02)
      (description "Generic connector, single row, 01x02, script generated (kicad-library-utils/schlib/autogen/connector/)")
      (docs ~)
      (footprints
        (fp Connector*:*_1x??_*))
      (fields
        (field (name Reference) J)
        (field (name Value) Conn_01x02))
      (pins
        (pin (num 1) (name Pin_1) (type passive))
        (pin (num 2) (name Pin_2) (type passive))))
    (libpart (lib Connector_Generic) (part Conn_01x03)
      (description "Generic connector, single row, 01x03, script generated (kicad-library-utils/schlib/autogen/connector/)")
      (docs ~)
      (footprints
        (fp Connector*:*_1x??_*))
      (fields
        (field (name Reference) J)
        (field (name Value) Conn_01x03))
      (pins
        (pin (num 1) (name Pin_1) (type passive))
        (pin (num 2) (name Pin_2) (type passive))
        (pin (num 3) (name Pin_3) (type passive))))
    (libpart (lib Connector_Generic) (part Conn_01x06)
      (description "Generic connector, single row, 01x06, script generated (kicad-library-utils/schlib/autogen/connector/)")
      (docs ~)
      (footprints
        (fp Connector*:*_1x??_*))
      (fields
        (field (name Reference) J)
        (field (name Value) Conn_01x06))
      (pins
        (pin (num 1) (name Pin_1) (type passive))
        (pin (num 2) (name Pin_2) (type passive))
        (pin (num 3) (name Pin_3) (type passive))
        (pin (num 4) (name Pin_4) (type passive))
        (pin (num 5) (name Pin_5) (type passive))
        (pin (num 6) (name Pin_6) (type passive))))
    (libpart (lib Connector_Specialized) (part USB_B_Micro)
      (aliases
        (alias USB_B_Mini))
      (description "USB Micro Type B connector")
      (docs ~)
      (footprints
        (fp USB*))
      (fields
        (field (name Reference) J)
        (field (name Value) USB_B_Micro))
      (pins
        (pin (num 1) (name VBUS) (type power_out))
        (pin (num 2) (name D-) (type passive))
        (pin (num 3) (name D+) (type passive))
        (pin (num 4) (name ID) (type passive))
        (pin (num 5) (name GND) (type power_out))
        (pin (num 6) (name Shield) (type passive))))
    (libpart (lib Device) (part Buzzer)
      (description "Buzzer, polar")
      (footprints
        (fp *Buzzer*))
      (fields
        (field (name Reference) BZ)
        (field (name Value) Buzzer))
      (pins
        (pin (num 1) (name -) (type passive))
        (pin (num 2) (name +) (type passive))))
    (libpart (lib Device) (part C)
      (description "Unpolarized capacitor")
      (footprints
        (fp C_*))
      (fields
        (field (name Reference) C)
        (field (name Value) C))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib Device) (part Crystal)
      (description "Two pin crystal")
      (footprints
        (fp Crystal*))
      (fields
        (field (name Reference) Y)
        (field (name Value) Crystal))
      (pins
        (pin (num 1) (name 1) (type passive))
        (pin (num 2) (name 2) (type passive))))
    (libpart (lib Device) (part D)
      (description Diode)
      (footprints
        (fp TO-???*)
        (fp *SingleDiode)
        (fp *_Diode_*)
        (fp *SingleDiode*)
        (fp D_*))
      (fields
        (field (name Reference) D)
        (field (name Value) D))
      (pins
        (pin (num 1) (name K) (type passive))
        (pin (num 2) (name A) (type passive))))
    (libpart (lib Device) (part D_Schottky)
      (description "Schottky diode")
      (footprints
        (fp TO-???*)
        (fp *SingleDiode)
        (fp *_Diode_*)
        (fp *SingleDiode*)
        (fp D_*))
      (fields
        (field (name Reference) D)
        (field (name Value) D_Schottky))
      (pins
        (pin (num 1) (name K) (type passive))
        (pin (num 2) (name A) (type passive))))
    (libpart (lib Device) (part R)
      (description Resistor)
      (footprints
        (fp R_*)
        (fp R_*))
      (fields
        (field (name Reference) R)
        (field (name Value) R))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib Power_Protection) (part SP0504BAHT)
      (description "TVS Diode Array, 5.5V Standoff, 4 Channels, SOT-23-5 package")
      (docs http://www.littelfuse.com/~/media/files/littelfuse/technical%20resources/documents/data%20sheets/sp05xxba.pdf)
      (footprints
        (fp SOT?23*))
      (fields
        (field (name Reference) D)
        (field (name Value) SP0504BAHT)
        (field (name Footprint) Package_TO_SOT_SMD:SOT-23-5))
      (pins
        (pin (num 1) (name K) (type input))
        (pin (num 2) (name A) (type input))
        (pin (num 3) (name K) (type input))
        (pin (num 4) (name K) (type input))
        (pin (num 5) (name K) (type input))))
    (libpart (lib Servo_control-rescue) (part C-Chiller_control-rescue)
      (footprints
        (fp C_*))
      (fields
        (field (name Reference) C)
        (field (name Value) C-Chiller_control-rescue))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib Servo_control-rescue) (part CP-Chiller_control-rescue)
      (footprints
        (fp CP_*))
      (fields
        (field (name Reference) C)
        (field (name Value) CP-Chiller_control-rescue))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib Servo_control-rescue) (part L-Chiller_control-rescue)
      (footprints
        (fp Choke_*)
        (fp *Coil*)
        (fp Inductor_*)
        (fp L_*))
      (fields
        (field (name Reference) L)
        (field (name Value) L-Chiller_control-rescue))
      (pins
        (pin (num 1) (name 1) (type passive))
        (pin (num 2) (name 2) (type passive))))
    (libpart (lib Servo_control-rescue) (part LM1117-3.3-Chiller_control-rescue)
      (footprints
        (fp SOT?223*)
        (fp TO?263*)
        (fp TO?252*)
        (fp TO?220*))
      (fields
        (field (name Reference) U)
        (field (name Value) LM1117-3.3-Chiller_control-rescue))
      (pins
        (pin (num 1) (name GND) (type power_in))
        (pin (num 2) (name VO) (type power_out))
        (pin (num 3) (name VI) (type power_in))))
    (libpart (lib Servo_control-rescue) (part Q_NMOS_GSD-Chiller_control-rescue)
      (fields
        (field (name Reference) Q)
        (field (name Value) Q_NMOS_GSD-Chiller_control-rescue))
      (pins
        (pin (num 1) (name G) (type input))
        (pin (num 2) (name S) (type passive))
        (pin (num 3) (name D) (type passive))))
    (libpart (lib Servo_control-rescue) (part R-Chiller_control-rescue)
      (footprints
        (fp R_*)
        (fp R_*))
      (fields
        (field (name Reference) R)
        (field (name Value) R-Chiller_control-rescue))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib Servo_control-rescue) (part STM32F030F4Px-Chiller_control-rescue)
      (fields
        (field (name Reference) U)
        (field (name Value) STM32F030F4Px-Chiller_control-rescue)
        (field (name Footprint) Housings_SSOP:TSSOP-20_4.4x6.5mm_Pitch0.65mm))
      (pins
        (pin (num 1) (name BOOT0) (type input))
        (pin (num 2) (name PF0/RCC_OSC_IN) (type input))
        (pin (num 3) (name PF1/RCC_OSC_OUT) (type input))
        (pin (num 4) (name NRST) (type input))
        (pin (num 5) (name VDDA) (type power_in))
        (pin (num 6) (name ADC_IN0/RTC_TAMP2/SYS_WKUP1/USART1_CTS/PA0) (type BiDi))
        (pin (num 7) (name ADC_IN1/USART1_DE/USART1_RTS/PA1) (type BiDi))
        (pin (num 8) (name ADC_IN2/USART1_TX/PA2) (type BiDi))
        (pin (num 9) (name ADC_IN3/USART1_RX/PA3) (type BiDi))
        (pin (num 10) (name ADC_IN4/SPI1_NSS/TIM14_CH1/USART1_CK/PA4) (type BiDi))
        (pin (num 11) (name ADC_IN5/SPI1_SCK/PA5) (type BiDi))
        (pin (num 12) (name ADC_IN6/SPI1_MISO/TIM16_CH1/TIM1_BKIN/TIM3_CH1/PA6) (type BiDi))
        (pin (num 13) (name ADC_IN7/SPI1_MOSI/TIM14_CH1/TIM17_CH1/TIM1_CH1N/TIM3_CH2/PA7) (type BiDi))
        (pin (num 14) (name PB1/ADC_IN9/TIM14_CH1/TIM1_CH3N/TIM3_CH4) (type BiDi))
        (pin (num 15) (name VSS) (type power_in))
        (pin (num 16) (name VDD) (type power_in))
        (pin (num 17) (name I2C1_SCL/TIM1_CH2/USART1_TX/PA9) (type BiDi))
        (pin (num 18) (name I2C1_SDA/TIM17_BKIN/TIM1_CH3/USART1_RX/PA10) (type BiDi))
        (pin (num 19) (name IR_OUT/SYS_SWDIO/PA13) (type BiDi))
        (pin (num 20) (name SYS_SWCLK/USART1_TX/PA14) (type BiDi))))
    (libpart (lib Servo_control-rescue) (part SW_Push-Chiller_control-rescue)
      (fields
        (field (name Reference) SW)
        (field (name Value) SW_Push-Chiller_control-rescue))
      (pins
        (pin (num 1) (name 1) (type passive))
        (pin (num 2) (name 2) (type passive))))
    (libpart (lib ch34x) (part CH340G)
      (fields
        (field (name Reference) U)
        (field (name Value) CH340G))
      (pins
        (pin (num 1) (name GND) (type power_in))
        (pin (num 2) (name TX) (type output))
        (pin (num 3) (name RX) (type input))
        (pin (num 4) (name V3) (type passive))
        (pin (num 5) (name D+) (type BiDi))
        (pin (num 6) (name D-) (type BiDi))
        (pin (num 7) (name XI) (type input))
        (pin (num 8) (name XO) (type input))
        (pin (num 9) (name CTS) (type output))
        (pin (num 10) (name DSR) (type output))
        (pin (num 11) (name RI) (type output))
        (pin (num 12) (name DCD) (type output))
        (pin (num 13) (name DTR) (type output))
        (pin (num 14) (name RTS) (type output))
        (pin (num 15) (name RS232) (type input))
        (pin (num 16) (name VCC) (type power_in))))
    (libpart (lib elements) (part USB6B1)
      (footprints
        (fp SO8))
      (fields
        (field (name Reference) D)
        (field (name Value) USB6B1))
      (pins
        (pin (num 1) (name VCC) (type passive))
        (pin (num 2) (name I/O1) (type passive))
        (pin (num 3) (name I/O2) (type passive))
        (pin (num 4) (name GND) (type passive))
        (pin (num 5) (name GND) (type passive))
        (pin (num 6) (name I/O2) (type passive))
        (pin (num 7) (name I/O1) (type passive))
        (pin (num 8) (name VCC) (type passive)))))
  (libraries
    (library (logical Connector_Generic)
      (uri /usr/share/kicad/library/Connector_Generic.lib))
    (library (logical Connector_Specialized)
      (uri /usr/share/kicad/library/Connector_Specialized.lib))
    (library (logical Device)
      (uri /usr/share/kicad/library/Device.lib))
    (library (logical Power_Protection)
      (uri /usr/share/kicad/library/Power_Protection.lib))
    (library (logical Servo_control-rescue)
      (uri /Big/Data/00__Electronics/STM32/F0-nolib/Servo/kicad/Servo_control-rescue.lib))
    (library (logical ch34x)
      (uri /Big/Data/00__Electronics/STM32/F0-nolib/Servo/kicad/ch34x.lib))
    (library (logical elements)
      (uri /Big/Data/00__Electronics/STM32/F0-nolib/Servo/kicad/elements.lib)))
  (nets
    (net (code 1) (name "Net-(Q2-Pad1)")
      (node (ref R8) (pin 1))
      (node (ref Q2) (pin 1)))
    (net (code 2) (name "Net-(BZ1-Pad2)")
      (node (ref BZ1) (pin 2))
      (node (ref Q1) (pin 3)))
    (net (code 3) (name "Net-(Q1-Pad1)")
      (node (ref Q1) (pin 1))
      (node (ref R6) (pin 1)))
    (net (code 4) (name "Net-(J1-Pad4)")
      (node (ref J1) (pin 4)))
    (net (code 5) (name "Net-(C7-Pad1)")
      (node (ref C7) (pin 1))
      (node (ref Y1) (pin 1))
      (node (ref U2) (pin 7)))
    (net (code 6) (name /DigOut1)
      (node (ref R8) (pin 2))
      (node (ref R9) (pin 2))
      (node (ref U3) (pin 3)))
    (net (code 7) (name "Net-(C9-Pad1)")
      (node (ref C9) (pin 1))
      (node (ref U2) (pin 8))
      (node (ref Y1) (pin 2)))
    (net (code 8) (name GND)
      (node (ref U3) (pin 15))
      (node (ref SW1) (pin 2))
      (node (ref Q3) (pin 2))
      (node (ref Q5) (pin 2))
      (node (ref J10) (pin 2))
      (node (ref J4) (pin 1))
      (node (ref J3) (pin 1))
      (node (ref J5) (pin 1))
      (node (ref D1) (pin 5))
      (node (ref C12) (pin 2))
      (node (ref C11) (pin 2))
      (node (ref C10) (pin 2))
      (node (ref C8) (pin 2))
      (node (ref Q4) (pin 2))
      (node (ref Q2) (pin 2))
      (node (ref R16) (pin 1))
      (node (ref J9) (pin 1))
      (node (ref J8) (pin 1))
      (node (ref J7) (pin 1))
      (node (ref R15) (pin 1))
      (node (ref C13) (pin 2))
      (node (ref C1) (pin 2))
      (node (ref C2) (pin 2))
      (node (ref C3) (pin 2))
      (node (ref C4) (pin 2))
      (node (ref C14) (pin 1))
      (node (ref C5) (pin 2))
      (node (ref U1) (pin 1))
      (node (ref J2) (pin 1))
      (node (ref D2) (pin 2))
      (node (ref R17) (pin 1))
      (node (ref R1) (pin 1))
      (node (ref C6) (pin 2))
      (node (ref Q1) (pin 2))
      (node (ref U2) (pin 1))
      (node (ref R9) (pin 1))
      (node (ref R7) (pin 1))
      (node (ref C9) (pin 2))
      (node (ref C7) (pin 2))
      (node (ref D3) (pin 2))
      (node (ref D4) (pin 2)))
    (net (code 9) (name "Net-(J5-Pad3)")
      (node (ref J5) (pin 3))
      (node (ref R10) (pin 2)))
    (net (code 10) (name +3.3VADC)
      (node (ref L1) (pin 2))
      (node (ref C14) (pin 2))
      (node (ref U3) (pin 5))
      (node (ref J2) (pin 6)))
    (net (code 11) (name "Net-(J6-Pad2)")
      (node (ref J6) (pin 2))
      (node (ref Q2) (pin 3)))
    (net (code 12) (name "Net-(U2-Pad9)")
      (node (ref U2) (pin 9)))
    (net (code 13) (name "Net-(D1-Pad7)")
      (node (ref D1) (pin 7))
      (node (ref U2) (pin 5)))
    (net (code 14) (name "Net-(C6-Pad1)")
      (node (ref U2) (pin 4))
      (node (ref C6) (pin 1)))
    (net (code 15) (name /USART_Tx)
      (node (ref U2) (pin 3))
      (node (ref U3) (pin 17)))
    (net (code 16) (name /USART_Rx)
      (node (ref U3) (pin 18))
      (node (ref U2) (pin 2)))
    (net (code 17) (name "Net-(U2-Pad10)")
      (node (ref U2) (pin 10)))
    (net (code 18) (name +3V3)
      (node (ref U2) (pin 16))
      (node (ref U3) (pin 16))
      (node (ref U1) (pin 2))
      (node (ref C5) (pin 1))
      (node (ref L1) (pin 1))
      (node (ref C4) (pin 1))
      (node (ref C13) (pin 1))
      (node (ref SW2) (pin 2)))
    (net (code 19) (name "Net-(D1-Pad6)")
      (node (ref D1) (pin 6))
      (node (ref U2) (pin 6)))
    (net (code 20) (name "Net-(J5-Pad2)")
      (node (ref R11) (pin 2))
      (node (ref J5) (pin 2)))
    (net (code 21) (name "Net-(U2-Pad15)")
      (node (ref U2) (pin 15)))
    (net (code 22) (name "Net-(U2-Pad14)")
      (node (ref U2) (pin 14)))
    (net (code 23) (name "Net-(U2-Pad13)")
      (node (ref U2) (pin 13)))
    (net (code 24) (name "Net-(U2-Pad12)")
      (node (ref U2) (pin 12)))
    (net (code 25) (name "Net-(U2-Pad11)")
      (node (ref U2) (pin 11)))
    (net (code 26) (name /ADC3)
      (node (ref C8) (pin 1))
      (node (ref U3) (pin 9))
      (node (ref D2) (pin 4))
      (node (ref R5) (pin 1)))
    (net (code 27) (name /ADC2)
      (node (ref D2) (pin 5))
      (node (ref R4) (pin 1))
      (node (ref C10) (pin 1))
      (node (ref U3) (pin 8)))
    (net (code 28) (name /ADC1)
      (node (ref D2) (pin 1))
      (node (ref U3) (pin 7))
      (node (ref C11) (pin 1))
      (node (ref R3) (pin 1)))
    (net (code 29) (name /ADC0)
      (node (ref R2) (pin 1))
      (node (ref C12) (pin 1))
      (node (ref D2) (pin 3))
      (node (ref U3) (pin 6)))
    (net (code 30) (name /DigOut0)
      (node (ref R6) (pin 2))
      (node (ref R7) (pin 2))
      (node (ref U3) (pin 2)))
    (net (code 31) (name /TIM3_CH1)
      (node (ref R15) (pin 2))
      (node (ref R12) (pin 2))
      (node (ref U3) (pin 12)))
    (net (code 32) (name "Net-(D1-Pad3)")
      (node (ref D1) (pin 3))
      (node (ref J1) (pin 3)))
    (net (code 33) (name "Net-(D1-Pad2)")
      (node (ref J1) (pin 2))
      (node (ref D1) (pin 2)))
    (net (code 34) (name +5V)
      (node (ref BZ1) (pin 1))
      (node (ref D5) (pin 1))
      (node (ref J6) (pin 1))
      (node (ref U1) (pin 3))
      (node (ref J10) (pin 1))
      (node (ref C1) (pin 1))
      (node (ref J9) (pin 2))
      (node (ref J8) (pin 2))
      (node (ref J7) (pin 2)))
    (net (code 35) (name "Net-(D1-Pad8)")
      (node (ref D1) (pin 8))
      (node (ref D5) (pin 2)))
    (net (code 36) (name /DigIn1)
      (node (ref U3) (pin 20))
      (node (ref R10) (pin 1))
      (node (ref D4) (pin 1)))
    (net (code 37) (name /Jumper1)
      (node (ref U3) (pin 11))
      (node (ref J4) (pin 2)))
    (net (code 38) (name /Jumper0)
      (node (ref U3) (pin 10))
      (node (ref J3) (pin 2)))
    (net (code 39) (name /DigIn0)
      (node (ref U3) (pin 19))
      (node (ref D3) (pin 1))
      (node (ref R11) (pin 1)))
    (net (code 40) (name "Net-(D1-Pad1)")
      (node (ref J1) (pin 1))
      (node (ref D1) (pin 1)))
    (net (code 41) (name "Net-(D1-Pad4)")
      (node (ref J1) (pin 5))
      (node (ref D1) (pin 4))
      (node (ref J1) (pin 6)))
    (net (code 42) (name /NRST)
      (node (ref SW1) (pin 1))
      (node (ref C2) (pin 1))
      (node (ref U3) (pin 4)))
    (net (code 43) (name /BOOT0)
      (node (ref U3) (pin 1))
      (node (ref R1) (pin 2))
      (node (ref SW2) (pin 1))
      (node (ref C3) (pin 1)))
    (net (code 44) (name "Net-(J7-Pad3)")
      (node (ref Q3) (pin 3))
      (node (ref J7) (pin 3)))
    (net (code 45) (name "Net-(Q3-Pad1)")
      (node (ref Q3) (pin 1))
      (node (ref R12) (pin 1)))
    (net (code 46) (name "Net-(J2-Pad4)")
      (node (ref R3) (pin 2))
      (node (ref J2) (pin 4)))
    (net (code 47) (name /TIM3_CH4)
      (node (ref R14) (pin 2))
      (node (ref U3) (pin 14))
      (node (ref R17) (pin 2)))
    (net (code 48) (name /TIM3_CH2)
      (node (ref R16) (pin 2))
      (node (ref R13) (pin 2))
      (node (ref U3) (pin 13)))
    (net (code 49) (name "Net-(Q5-Pad1)")
      (node (ref R14) (pin 1))
      (node (ref Q5) (pin 1)))
    (net (code 50) (name "Net-(Q4-Pad1)")
      (node (ref Q4) (pin 1))
      (node (ref R13) (pin 1)))
    (net (code 51) (name "Net-(J2-Pad5)")
      (node (ref R2) (pin 2))
      (node (ref J2) (pin 5)))
    (net (code 52) (name "Net-(J2-Pad3)")
      (node (ref R4) (pin 2))
      (node (ref J2) (pin 3)))
    (net (code 53) (name "Net-(J2-Pad2)")
      (node (ref R5) (pin 2))
      (node (ref J2) (pin 2)))
    (net (code 54) (name "Net-(J8-Pad3)")
      (node (ref J8) (pin 3))
      (node (ref Q4) (pin 3)))
    (net (code 55) (name "Net-(J9-Pad3)")
      (node (ref J9) (pin 3))
      (node (ref Q5) (pin 3)))))