(export (version D)
  (design
    (source /home/eddy/Docs/SAO/ELECTRONICS/Chiller/kicad/Chiller_control.sch)
    (date "Вс 27 янв 2019 17:08:13")
    (tool "Eeschema 6.0.0-rc1-unknown")
    (sheet (number 1) (name /) (tstamps /)
      (title_block
        (title)
        (company)
        (rev)
        (date)
        (source Chiller_control.sch)
        (comment (number 1) (value ""))
        (comment (number 2) (value ""))
        (comment (number 3) (value ""))
        (comment (number 4) (value "")))))
  (components
    (comp (ref C4)
      (value 47u)
      (footprint Capacitor_Tantalum_SMD.pretty:CP_Tantalum_Case-A_EIA-3216-18_Hand)
      (libsource (lib Chiller_control-rescue) (part CP) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 58C454F6))
    (comp (ref R1)
      (value 10k)
      (footprint Resistors_SMD.pretty:R_0603_HandSoldering)
      (libsource (lib Chiller_control-rescue) (part R) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 590D30C8))
    (comp (ref C2)
      (value 0.1)
      (footprint Capacitor_SMD:C_0603_1608Metric_Pad0.99x1.00mm_HandSolder)
      (libsource (lib Chiller_control-rescue) (part C) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 590D4150))
    (comp (ref C1)
      (value 0.1)
      (footprint Capacitor_SMD:C_0603_1608Metric_Pad0.99x1.00mm_HandSolder)
      (libsource (lib Chiller_control-rescue) (part C) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 590D4832))
    (comp (ref SW2)
      (value Boot)
      (footprint Buttons_Switches_SMD:SW_SPST_FSMSM)
      (libsource (lib Chiller_control-rescue) (part SW_Push) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5909F6B6))
    (comp (ref SW1)
      (value Reset)
      (footprint Buttons_Switches_SMD:SW_SPST_FSMSM)
      (libsource (lib Chiller_control-rescue) (part SW_Push) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 590A0134))
    (comp (ref J2)
      (value 12VIN)
      (footprint Connectors_Terminal_Blocks:TerminalBlock_Pheonix_MKDS1.5-2pol)
      (libsource (lib Chiller_control-rescue) (part Conn_01x02) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5A170C1F))
    (comp (ref C3)
      (value 0.1)
      (footprint Capacitor_SMD:C_0603_1608Metric_Pad0.99x1.00mm_HandSolder)
      (libsource (lib Chiller_control-rescue) (part C) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5A178C32))
    (comp (ref U3)
      (value STM32F030F4Px)
      (footprint Housings_SSOP:TSSOP-20_4.4x6.5mm_Pitch0.65mm)
      (libsource (lib Chiller_control-rescue) (part STM32F030F4Px) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5A189F52))
    (comp (ref C6)
      (value 1u)
      (footprint Capacitor_SMD.pretty:C_0805_HandSoldering)
      (libsource (lib Chiller_control-rescue) (part C) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5A1AB970))
    (comp (ref U1)
      (value LM1117-3.3)
      (footprint TO_SOT_Packages_SMD:SOT-223)
      (libsource (lib Chiller_control-rescue) (part LM1117-3.3) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5A2588E7))
    (comp (ref C5)
      (value 0.1)
      (footprint Capacitor_SMD:C_0603_1608Metric_Pad0.99x1.00mm_HandSolder)
      (libsource (lib Chiller_control-rescue) (part C) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5BEE1D09))
    (comp (ref D1)
      (value SS14)
      (footprint Diode_SMD.pretty:D_SMA_Handsoldering)
      (libsource (lib Chiller_control-rescue) (part D) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5BEE236F))
    (comp (ref L1)
      (value "BMBA 0.1mH")
      (footprint Resistors_SMD.pretty:R_0805_HandSoldering)
      (libsource (lib Chiller_control-rescue) (part L) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5BEE7949))
    (comp (ref C7)
      (value 10u)
      (footprint Capacitor_SMD.pretty:C_1206_HandSoldering)
      (libsource (lib Chiller_control-rescue) (part C) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5BEE8065))
    (comp (ref R8)
      (value 10k)
      (footprint Resistors_SMD.pretty:R_0603_HandSoldering)
      (libsource (lib Chiller_control-rescue) (part R) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5BEEA391))
    (comp (ref R6)
      (value 10k)
      (footprint Resistors_SMD.pretty:R_0603_HandSoldering)
      (libsource (lib Chiller_control-rescue) (part R) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5BEEA7BE))
    (comp (ref Q2)
      (value SI2300)
      (footprint TO_SOT_Packages_SMD:SOT-23_Handsoldering)
      (libsource (lib Chiller_control-rescue) (part Q_NMOS_GSD) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5BEDCAD0))
    (comp (ref R14)
      (value 10k)
      (footprint Resistors_SMD.pretty:R_0603_HandSoldering)
      (libsource (lib Chiller_control-rescue) (part R) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5BEDD4AE))
    (comp (ref R15)
      (value 10k)
      (footprint Resistors_SMD.pretty:R_0603_HandSoldering)
      (libsource (lib Chiller_control-rescue) (part R) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5BEDD8A0))
    (comp (ref R19)
      (value 10k)
      (footprint Resistors_SMD.pretty:R_0603_HandSoldering)
      (libsource (lib Chiller_control-rescue) (part R) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5BEEBD18))
    (comp (ref R16)
      (value 510)
      (footprint Resistors_SMD.pretty:R_0603_HandSoldering)
      (libsource (lib Chiller_control-rescue) (part R) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5BEEBD1E))
    (comp (ref Q3)
      (value SI2300)
      (footprint TO_SOT_Packages_SMD:SOT-23_Handsoldering)
      (libsource (lib Chiller_control-rescue) (part Q_NMOS_GSD) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5BEEBD24))
    (comp (ref R20)
      (value 10k)
      (footprint Resistors_SMD.pretty:R_0603_HandSoldering)
      (libsource (lib Chiller_control-rescue) (part R) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5BEEC934))
    (comp (ref R17)
      (value 510)
      (footprint Resistors_SMD.pretty:R_0603_HandSoldering)
      (libsource (lib Chiller_control-rescue) (part R) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5BEEC93A))
    (comp (ref Q4)
      (value IRL3303)
      (footprint TO_SOT_Packages_THT:TO-220-3_Vertical)
      (libsource (lib Chiller_control-rescue) (part Q_NMOS_GDS) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5BEEC940))
    (comp (ref R21)
      (value 10k)
      (footprint Resistors_SMD.pretty:R_0603_HandSoldering)
      (libsource (lib Chiller_control-rescue) (part R) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5BEED557))
    (comp (ref R18)
      (value 510)
      (footprint Resistors_SMD.pretty:R_0603_HandSoldering)
      (libsource (lib Chiller_control-rescue) (part R) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5BEED55D))
    (comp (ref Q5)
      (value IRL3303)
      (footprint TO_SOT_Packages_THT:TO-220-3_Vertical)
      (libsource (lib Chiller_control-rescue) (part Q_NMOS_GDS) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5BEED563))
    (comp (ref R2)
      (value 1k0.1%)
      (footprint Resistors_SMD.pretty:R_0805_HandSoldering)
      (libsource (lib Chiller_control-rescue) (part R) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5BEF45BA))
    (comp (ref R3)
      (value 1k0.1%)
      (footprint Resistors_SMD.pretty:R_0805_HandSoldering)
      (libsource (lib Chiller_control-rescue) (part R) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5BEF7CBC))
    (comp (ref R4)
      (value 1k0.1%)
      (footprint Resistors_SMD.pretty:R_0805_HandSoldering)
      (libsource (lib Chiller_control-rescue) (part R) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5BEF8256))
    (comp (ref R5)
      (value 1k0.1%)
      (footprint Resistors_SMD.pretty:R_0805_HandSoldering)
      (libsource (lib Chiller_control-rescue) (part R) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5BEFAAF1))
    (comp (ref U2)
      (value MAX3232)
      (footprint Housings_SOIC:SOIC-16_3.9x9.9mm_Pitch1.27mm)
      (libsource (lib Chiller_control-rescue) (part MAX3232) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5BEFC197))
    (comp (ref C11)
      (value 0.47)
      (footprint Capacitor_SMD.pretty:C_0805_HandSoldering)
      (libsource (lib Chiller_control-rescue) (part C) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5BEFD47C))
    (comp (ref C10)
      (value 0.47)
      (footprint Capacitor_SMD.pretty:C_0805_HandSoldering)
      (libsource (lib Chiller_control-rescue) (part C) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5BEFD7DB))
    (comp (ref C13)
      (value 0.47)
      (footprint Capacitor_SMD.pretty:C_0805_HandSoldering)
      (libsource (lib Chiller_control-rescue) (part C) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5BEFD89D))
    (comp (ref C9)
      (value 0.1)
      (footprint Capacitor_SMD:C_0603_1608Metric_Pad0.99x1.00mm_HandSolder)
      (libsource (lib Chiller_control-rescue) (part C) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5BEFF11C))
    (comp (ref C8)
      (value 0.1)
      (footprint Capacitor_SMD:C_0603_1608Metric_Pad0.99x1.00mm_HandSolder)
      (libsource (lib Chiller_control-rescue) (part C) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5BF0257F))
    (comp (ref J1)
      (value DB9_Female)
      (footprint modules:DB9-F)
      (libsource (lib Chiller_control-rescue) (part DB9_Female) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5BF02D65))
    (comp (ref J5)
      (value Cooler)
      (footprint Connectors_Terminal_Blocks:TerminalBlock_Pheonix_MKDS1.5-2pol)
      (libsource (lib Chiller_control-rescue) (part Conn_01x02) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5BF1B9CF))
    (comp (ref J6)
      (value Heater)
      (footprint Connectors_Terminal_Blocks:TerminalBlock_Pheonix_MKDS1.5-2pol)
      (libsource (lib Chiller_control-rescue) (part Conn_01x02) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5BF1EE9B))
    (comp (ref J7)
      (value Pump)
      (footprint Connectors_Terminal_Blocks:TerminalBlock_Pheonix_MKDS1.5-2pol)
      (libsource (lib Chiller_control-rescue) (part Conn_01x02) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5BF1F6CF))
    (comp (ref R13)
      (value 10k)
      (footprint Resistors_SMD.pretty:R_0603_HandSoldering)
      (libsource (lib Chiller_control-rescue) (part R) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5BEE33E1))
    (comp (ref R11)
      (value 220)
      (footprint Resistors_SMD.pretty:R_0805_HandSoldering)
      (libsource (lib Chiller_control-rescue) (part R) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5BEDB615))
    (comp (ref Q1)
      (value SI2300)
      (footprint TO_SOT_Packages_SMD:SOT-23_Handsoldering)
      (libsource (lib Chiller_control-rescue) (part Q_NMOS_GSD) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5BEEB585))
    (comp (ref R10)
      (value 510)
      (footprint Resistors_SMD.pretty:R_0603_HandSoldering)
      (libsource (lib Chiller_control-rescue) (part R) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5BEEB37B))
    (comp (ref R12)
      (value 10k)
      (footprint Resistors_SMD.pretty:R_0603_HandSoldering)
      (libsource (lib Chiller_control-rescue) (part R) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5BEEB2E1))
    (comp (ref C12)
      (value 0.1)
      (footprint Capacitor_SMD:C_0603_1608Metric_Pad0.99x1.00mm_HandSolder)
      (libsource (lib Chiller_control-rescue) (part C) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5A386BD0))
    (comp (ref R9)
      (value 10k)
      (footprint Resistors_SMD.pretty:R_0603_HandSoldering)
      (libsource (lib Chiller_control-rescue) (part R) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5BEE5083))
    (comp (ref R7)
      (value 220)
      (footprint Resistor_SMD:R_0805_2012Metric_Pad1.29x1.40mm_HandSolder)
      (libsource (lib Chiller_control-rescue) (part R) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5BEDA6BA))
    (comp (ref R22)
      (value 220)
      (footprint Resistor_SMD:R_0805_2012Metric_Pad1.29x1.40mm_HandSolder)
      (libsource (lib Chiller_control-rescue) (part R) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C509370))
    (comp (ref R23)
      (value 220)
      (footprint Resistor_SMD:R_0805_2012Metric_Pad1.29x1.40mm_HandSolder)
      (libsource (lib Chiller_control-rescue) (part R) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C50F547))
    (comp (ref C15)
      (value 100u)
      (footprint Capacitor_THT:CP_Radial_D8.0mm_P3.50mm)
      (libsource (lib Chiller_control-rescue) (part CP) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C53FDA9))
    (comp (ref R26)
      (value 220)
      (footprint Resistor_SMD:R_0805_2012Metric_Pad1.29x1.40mm_HandSolder)
      (libsource (lib Chiller_control-rescue) (part R) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C5422DE))
    (comp (ref C16)
      (value 1u)
      (footprint Capacitor_SMD:C_0805_2012Metric_Pad1.29x1.40mm_HandSolder)
      (libsource (lib Chiller_control-rescue) (part C) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C548AFE))
    (comp (ref R25)
      (value 0)
      (footprint Resistor_SMD:R_0805_2012Metric_Pad1.29x1.40mm_HandSolder)
      (libsource (lib Chiller_control-rescue) (part R) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C565B8F))
    (comp (ref R24)
      (value 0)
      (footprint Resistor_SMD:R_0805_2012Metric_Pad1.29x1.40mm_HandSolder)
      (libsource (lib Chiller_control-rescue) (part R) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C56BFDC))
    (comp (ref U4)
      (value L7805)
      (footprint TO_SOT_Packages_THT:TO-220-3_Vertical)
      (datasheet http://www.st.com/content/ccc/resource/technical/document/datasheet/41/4f/b3/b0/12/d4/47/88/CD00000444.pdf/files/CD00000444.pdf/jcr:content/translations/en.CD00000444.pdf)
      (libsource (lib Regulator_Linear) (part L7805) (description "Positive 1.5A 35V Linear Regulator, Fixed Output 5V, TO-220/TO-263/TO-252"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C573DC9))
    (comp (ref C14)
      (value 1u)
      (footprint Capacitor_SMD:C_0805_2012Metric_Pad1.29x1.40mm_HandSolder)
      (libsource (lib Chiller_control-rescue) (part C) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C574153))
    (comp (ref C18)
      (value 0.1)
      (footprint Capacitor_SMD:C_0603_1608Metric_Pad0.99x1.00mm_HandSolder)
      (libsource (lib Chiller_control-rescue) (part C) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C5C6D73))
    (comp (ref C20)
      (value 0.1)
      (footprint Capacitor_SMD:C_0603_1608Metric_Pad0.99x1.00mm_HandSolder)
      (libsource (lib Chiller_control-rescue) (part C) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C5D4FAB))
    (comp (ref C17)
      (value 0.1)
      (footprint Capacitor_SMD:C_0603_1608Metric_Pad0.99x1.00mm_HandSolder)
      (libsource (lib Chiller_control-rescue) (part C) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C5D51AF))
    (comp (ref C19)
      (value 0.1)
      (footprint Capacitor_SMD:C_0603_1608Metric_Pad0.99x1.00mm_HandSolder)
      (libsource (lib Chiller_control-rescue) (part C) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C5D5336))
    (comp (ref C21)
      (value 0.1)
      (footprint Capacitor_SMD:C_0603_1608Metric_Pad0.99x1.00mm_HandSolder)
      (libsource (lib Chiller_control-rescue) (part C) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C6511ED))
    (comp (ref J4)
      (value DC3-10P)
      (footprint Connector_IDC:IDC-Header_2x05_P2.54mm_Vertical)
      (datasheet ~)
      (libsource (lib Connector_Generic) (part Conn_02x05_Odd_Even) (description "Generic connector, double row, 02x05, odd/even pin numbering scheme (row 1 odd numbers, row 2 even numbers), script generated (kicad-library-utils/schlib/autogen/connector/)"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C71D1DB))
    (comp (ref J3)
      (value DC3-10P)
      (footprint Connector_IDC:IDC-Header_2x05_P2.54mm_Vertical)
      (datasheet ~)
      (libsource (lib Connector_Generic) (part Conn_02x05_Odd_Even) (description "Generic connector, double row, 02x05, odd/even pin numbering scheme (row 1 odd numbers, row 2 even numbers), script generated (kicad-library-utils/schlib/autogen/connector/)"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C81FA0E))
    (comp (ref BZ1)
      (value Buzzer)
      (footprint Buzzer_Beeper:Buzzer_12x9.5RM7.6)
      (datasheet ~)
      (libsource (lib Device) (part Buzzer) (description "Buzzer, polar"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C83133C)))
  (libparts
    (libpart (lib Chiller_control-rescue) (part C)
      (footprints
        (fp C_*))
      (fields
        (field (name Reference) C)
        (field (name Value) C))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib Chiller_control-rescue) (part CP)
      (footprints
        (fp CP_*))
      (fields
        (field (name Reference) C)
        (field (name Value) CP))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib Chiller_control-rescue) (part Conn_01x02)
      (footprints
        (fp Connector*:*_??x*mm*)
        (fp Connector*:*1x??x*mm*)
        (fp Pin?Header?Straight?1X*)
        (fp Pin?Header?Angled?1X*)
        (fp Socket?Strip?Straight?1X*)
        (fp Socket?Strip?Angled?1X*))
      (fields
        (field (name Reference) J)
        (field (name Value) Conn_01x02))
      (pins
        (pin (num 1) (name Pin_1) (type passive))
        (pin (num 2) (name Pin_2) (type passive))))
    (libpart (lib Chiller_control-rescue) (part D)
      (footprints
        (fp TO-???*)
        (fp *SingleDiode)
        (fp *_Diode_*)
        (fp *SingleDiode*)
        (fp D_*))
      (fields
        (field (name Reference) D)
        (field (name Value) D))
      (pins
        (pin (num 1) (name K) (type passive))
        (pin (num 2) (name A) (type passive))))
    (libpart (lib Chiller_control-rescue) (part DB9_Female)
      (footprints
        (fp DB*F*))
      (fields
        (field (name Reference) J)
        (field (name Value) DB9_Female))
      (pins
        (pin (num 1) (name 1) (type passive))
        (pin (num 2) (name 2) (type passive))
        (pin (num 3) (name 3) (type passive))
        (pin (num 4) (name 4) (type passive))
        (pin (num 5) (name 5) (type passive))
        (pin (num 6) (name 6) (type passive))
        (pin (num 7) (name 7) (type passive))
        (pin (num 8) (name 8) (type passive))
        (pin (num 9) (name 9) (type passive))))
    (libpart (lib Chiller_control-rescue) (part L)
      (footprints
        (fp Choke_*)
        (fp *Coil*)
        (fp Inductor_*)
        (fp L_*))
      (fields
        (field (name Reference) L)
        (field (name Value) L))
      (pins
        (pin (num 1) (name 1) (type passive))
        (pin (num 2) (name 2) (type passive))))
    (libpart (lib Chiller_control-rescue) (part LM1117-3.3)
      (footprints
        (fp SOT?223*)
        (fp TO?263*)
        (fp TO?252*)
        (fp TO?220*))
      (fields
        (field (name Reference) U)
        (field (name Value) LM1117-3.3))
      (pins
        (pin (num 1) (name GND) (type power_in))
        (pin (num 2) (name VO) (type power_out))
        (pin (num 3) (name VI) (type power_in))))
    (libpart (lib Chiller_control-rescue) (part MAX3232)
      (footprints
        (fp SOIC*Pitch1.27mm*)
        (fp DIP*W7.62mm*)
        (fp TSSOP*4.4x5mm*Pitch0.65mm*))
      (fields
        (field (name Reference) U)
        (field (name Value) MAX3232))
      (pins
        (pin (num 1) (name C1+) (type passive))
        (pin (num 2) (name VS+) (type power_out))
        (pin (num 3) (name C1-) (type passive))
        (pin (num 4) (name C2+) (type passive))
        (pin (num 5) (name C2-) (type passive))
        (pin (num 6) (name VS-) (type power_out))
        (pin (num 7) (name T2OUT) (type output))
        (pin (num 8) (name R2IN) (type input))
        (pin (num 9) (name R2OUT) (type output))
        (pin (num 10) (name T2IN) (type input))
        (pin (num 11) (name T1IN) (type input))
        (pin (num 12) (name R1OUT) (type output))
        (pin (num 13) (name R1IN) (type input))
        (pin (num 14) (name T1OUT) (type output))
        (pin (num 15) (name GND) (type power_in))
        (pin (num 16) (name VCC) (type power_in))))
    (libpart (lib Chiller_control-rescue) (part Q_NMOS_GDS)
      (fields
        (field (name Reference) Q)
        (field (name Value) Q_NMOS_GDS))
      (pins
        (pin (num 1) (name G) (type input))
        (pin (num 2) (name D) (type passive))
        (pin (num 3) (name S) (type passive))))
    (libpart (lib Chiller_control-rescue) (part Q_NMOS_GSD)
      (fields
        (field (name Reference) Q)
        (field (name Value) Q_NMOS_GSD))
      (pins
        (pin (num 1) (name G) (type input))
        (pin (num 2) (name S) (type passive))
        (pin (num 3) (name D) (type passive))))
    (libpart (lib Chiller_control-rescue) (part R)
      (footprints
        (fp R_*)
        (fp R_*))
      (fields
        (field (name Reference) R)
        (field (name Value) R))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib Chiller_control-rescue) (part STM32F030F4Px)
      (fields
        (field (name Reference) U)
        (field (name Value) STM32F030F4Px)
        (field (name Footprint) Housings_SSOP:TSSOP-20_4.4x6.5mm_Pitch0.65mm))
      (pins
        (pin (num 1) (name BOOT0) (type input))
        (pin (num 2) (name PF0/RCC_OSC_IN) (type input))
        (pin (num 3) (name PF1/RCC_OSC_OUT) (type input))
        (pin (num 4) (name NRST) (type input))
        (pin (num 5) (name VDDA) (type power_in))
        (pin (num 6) (name ADC_IN0/RTC_TAMP2/SYS_WKUP1/USART1_CTS/PA0) (type BiDi))
        (pin (num 7) (name ADC_IN1/USART1_DE/USART1_RTS/PA1) (type BiDi))
        (pin (num 8) (name ADC_IN2/USART1_TX/PA2) (type BiDi))
        (pin (num 9) (name ADC_IN3/USART1_RX/PA3) (type BiDi))
        (pin (num 10) (name ADC_IN4/SPI1_NSS/TIM14_CH1/USART1_CK/PA4) (type BiDi))
        (pin (num 11) (name ADC_IN5/SPI1_SCK/PA5) (type BiDi))
        (pin (num 12) (name ADC_IN6/SPI1_MISO/TIM16_CH1/TIM1_BKIN/TIM3_CH1/PA6) (type BiDi))
        (pin (num 13) (name ADC_IN7/SPI1_MOSI/TIM14_CH1/TIM17_CH1/TIM1_CH1N/TIM3_CH2/PA7) (type BiDi))
        (pin (num 14) (name PB1/ADC_IN9/TIM14_CH1/TIM1_CH3N/TIM3_CH4) (type BiDi))
        (pin (num 15) (name VSS) (type power_in))
        (pin (num 16) (name VDD) (type power_in))
        (pin (num 17) (name I2C1_SCL/TIM1_CH2/USART1_TX/PA9) (type BiDi))
        (pin (num 18) (name I2C1_SDA/TIM17_BKIN/TIM1_CH3/USART1_RX/PA10) (type BiDi))
        (pin (num 19) (name IR_OUT/SYS_SWDIO/PA13) (type BiDi))
        (pin (num 20) (name SYS_SWCLK/USART1_TX/PA14) (type BiDi))))
    (libpart (lib Chiller_control-rescue) (part SW_Push)
      (fields
        (field (name Reference) SW)
        (field (name Value) SW_Push))
      (pins
        (pin (num 1) (name 1) (type passive))
        (pin (num 2) (name 2) (type passive))))
    (libpart (lib Connector_Generic) (part Conn_02x05_Odd_Even)
      (description "Generic connector, double row, 02x05, odd/even pin numbering scheme (row 1 odd numbers, row 2 even numbers), script generated (kicad-library-utils/schlib/autogen/connector/)")
      (docs ~)
      (footprints
        (fp Connector*:*_2x??_*))
      (fields
        (field (name Reference) J)
        (field (name Value) Conn_02x05_Odd_Even))
      (pins
        (pin (num 1) (name Pin_1) (type passive))
        (pin (num 2) (name Pin_2) (type passive))
        (pin (num 3) (name Pin_3) (type passive))
        (pin (num 4) (name Pin_4) (type passive))
        (pin (num 5) (name Pin_5) (type passive))
        (pin (num 6) (name Pin_6) (type passive))
        (pin (num 7) (name Pin_7) (type passive))
        (pin (num 8) (name Pin_8) (type passive))
        (pin (num 9) (name Pin_9) (type passive))
        (pin (num 10) (name Pin_10) (type passive))))
    (libpart (lib Device) (part Buzzer)
      (description "Buzzer, polar")
      (docs ~)
      (footprints
        (fp *Buzzer*))
      (fields
        (field (name Reference) BZ)
        (field (name Value) Buzzer))
      (pins
        (pin (num 1) (name -) (type passive))
        (pin (num 2) (name +) (type passive))))
    (libpart (lib Regulator_Linear) (part L7805)
      (aliases
        (alias L7806)
        (alias L7808)
        (alias L7885)
        (alias L7809)
        (alias L7812)
        (alias L7815)
        (alias L7818)
        (alias L7824))
      (description "Positive 1.5A 35V Linear Regulator, Fixed Output 5V, TO-220/TO-263/TO-252")
      (docs http://www.st.com/content/ccc/resource/technical/document/datasheet/41/4f/b3/b0/12/d4/47/88/CD00000444.pdf/files/CD00000444.pdf/jcr:content/translations/en.CD00000444.pdf)
      (footprints
        (fp TO?252*)
        (fp TO?263*)
        (fp TO?220*))
      (fields
        (field (name Reference) U)
        (field (name Value) L7805))
      (pins
        (pin (num 1) (name IN) (type power_in))
        (pin (num 2) (name GND) (type power_in))
        (pin (num 3) (name OUT) (type power_out)))))
  (libraries
    (library (logical Chiller_control-rescue)
      (uri /home/eddy/Docs/SAO/ELECTRONICS/Chiller/kicad/Chiller_control-rescue.lib))
    (library (logical Connector_Generic)
      (uri /usr/share/kicad/kicad-symbols//Connector_Generic.lib))
    (library (logical Device)
      (uri /usr/share/kicad/kicad-symbols//Device.lib))
    (library (logical Regulator_Linear)
      (uri /usr/share/kicad/kicad-symbols//Regulator_Linear.lib)))
  (nets
    (net (code 1) (name /W.levl)
      (node (ref R13) (pin 2))
      (node (ref R11) (pin 1))
      (node (ref J3) (pin 5)))
    (net (code 2) (name +3V3)
      (node (ref R9) (pin 1))
      (node (ref L1) (pin 1))
      (node (ref U3) (pin 16))
      (node (ref R14) (pin 2))
      (node (ref U2) (pin 16))
      (node (ref Q2) (pin 1))
      (node (ref R6) (pin 1))
      (node (ref BZ1) (pin 1))
      (node (ref R8) (pin 1))
      (node (ref SW2) (pin 2))
      (node (ref C5) (pin 1))
      (node (ref U1) (pin 2))
      (node (ref R13) (pin 1))
      (node (ref C4) (pin 1))
      (node (ref C6) (pin 1))
      (node (ref C9) (pin 2)))
    (net (code 3) (name /DigIn0)
      (node (ref R11) (pin 2))
      (node (ref C12) (pin 1))
      (node (ref U3) (pin 2)))
    (net (code 4) (name "Net-(Q1-Pad1)")
      (node (ref Q1) (pin 1))
      (node (ref R10) (pin 1)))
    (net (code 5) (name GND)
      (node (ref Q3) (pin 2))
      (node (ref R1) (pin 2))
      (node (ref R21) (pin 1))
      (node (ref C4) (pin 2))
      (node (ref U3) (pin 15))
      (node (ref SW1) (pin 2))
      (node (ref U1) (pin 1))
      (node (ref C3) (pin 2))
      (node (ref J2) (pin 2))
      (node (ref C2) (pin 2))
      (node (ref C1) (pin 2))
      (node (ref C18) (pin 2))
      (node (ref U4) (pin 2))
      (node (ref C21) (pin 1))
      (node (ref C14) (pin 2))
      (node (ref C20) (pin 2))
      (node (ref C16) (pin 1))
      (node (ref J3) (pin 4))
      (node (ref J3) (pin 6))
      (node (ref J3) (pin 10))
      (node (ref R19) (pin 1))
      (node (ref Q5) (pin 3))
      (node (ref Q4) (pin 3))
      (node (ref R20) (pin 1))
      (node (ref C7) (pin 1))
      (node (ref C19) (pin 1))
      (node (ref C17) (pin 1))
      (node (ref R4) (pin 2))
      (node (ref R3) (pin 2))
      (node (ref R2) (pin 2))
      (node (ref C11) (pin 1))
      (node (ref R5) (pin 2))
      (node (ref U2) (pin 15))
      (node (ref R12) (pin 1))
      (node (ref C12) (pin 2))
      (node (ref Q1) (pin 2))
      (node (ref C9) (pin 1))
      (node (ref C13) (pin 1))
      (node (ref J1) (pin 5))
      (node (ref C6) (pin 2))
      (node (ref C5) (pin 2)))
    (net (code 6) (name /DigOut1)
      (node (ref U3) (pin 19))
      (node (ref R6) (pin 2))
      (node (ref R22) (pin 2)))
    (net (code 7) (name /Out2)
      (node (ref J3) (pin 3))
      (node (ref R23) (pin 1)))
    (net (code 8) (name /DigOut2)
      (node (ref R23) (pin 2))
      (node (ref R8) (pin 2))
      (node (ref U3) (pin 20)))
    (net (code 9) (name /Out1)
      (node (ref J3) (pin 1))
      (node (ref R22) (pin 1)))
    (net (code 10) (name +12V)
      (node (ref J5) (pin 1))
      (node (ref J6) (pin 1))
      (node (ref J7) (pin 1))
      (node (ref J2) (pin 1))
      (node (ref C15) (pin 1))
      (node (ref R25) (pin 2))
      (node (ref D1) (pin 2)))
    (net (code 11) (name "Net-(C15-Pad2)")
      (node (ref C15) (pin 2))
      (node (ref J5) (pin 2))
      (node (ref Q3) (pin 3)))
    (net (code 12) (name /IN)
      (node (ref R9) (pin 2))
      (node (ref R7) (pin 1))
      (node (ref J3) (pin 2)))
    (net (code 13) (name /DigOut0)
      (node (ref R12) (pin 2))
      (node (ref U3) (pin 3))
      (node (ref R10) (pin 2)))
    (net (code 14) (name "Net-(J6-Pad2)")
      (node (ref J6) (pin 2))
      (node (ref Q4) (pin 2)))
    (net (code 15) (name "Net-(J7-Pad2)")
      (node (ref Q5) (pin 2))
      (node (ref J7) (pin 2)))
    (net (code 16) (name "Net-(J1-Pad2)")
      (node (ref J1) (pin 2))
      (node (ref U2) (pin 7)))
    (net (code 17) (name "Net-(J1-Pad3)")
      (node (ref J1) (pin 3))
      (node (ref U2) (pin 8)))
    (net (code 18) (name "Net-(C10-Pad1)")
      (node (ref C10) (pin 1))
      (node (ref U2) (pin 4)))
    (net (code 19) (name "Net-(C10-Pad2)")
      (node (ref C10) (pin 2))
      (node (ref U2) (pin 5)))
    (net (code 20) (name "Net-(C13-Pad2)")
      (node (ref C13) (pin 2))
      (node (ref U2) (pin 6)))
    (net (code 21) (name "Net-(C11-Pad2)")
      (node (ref U2) (pin 2))
      (node (ref C11) (pin 2)))
    (net (code 22) (name /Yellow)
      (node (ref J3) (pin 9))
      (node (ref R26) (pin 1)))
    (net (code 23) (name "Net-(C8-Pad1)")
      (node (ref C8) (pin 1))
      (node (ref U2) (pin 3)))
    (net (code 24) (name "Net-(C8-Pad2)")
      (node (ref U2) (pin 1))
      (node (ref C8) (pin 2)))
    (net (code 25) (name "Net-(J4-Pad10)")
      (node (ref J4) (pin 10)))
    (net (code 26) (name /ADC2)
      (node (ref R4) (pin 1))
      (node (ref J4) (pin 3))
      (node (ref U3) (pin 8))
      (node (ref C20) (pin 1)))
    (net (code 27) (name +3.3VADC)
      (node (ref J4) (pin 6))
      (node (ref J4) (pin 4))
      (node (ref J4) (pin 2))
      (node (ref J4) (pin 8))
      (node (ref U3) (pin 5))
      (node (ref L1) (pin 2))
      (node (ref C7) (pin 2)))
    (net (code 28) (name "Net-(J4-Pad9)")
      (node (ref J4) (pin 9)))
    (net (code 29) (name "Net-(J3-Pad8)")
      (node (ref J3) (pin 8)))
    (net (code 30) (name "Net-(BZ1-Pad2)")
      (node (ref Q1) (pin 3))
      (node (ref BZ1) (pin 2)))
    (net (code 31) (name /ADC3)
      (node (ref U3) (pin 9))
      (node (ref C18) (pin 1))
      (node (ref R5) (pin 1))
      (node (ref J4) (pin 1)))
    (net (code 32) (name /ADC1)
      (node (ref J4) (pin 5))
      (node (ref U3) (pin 7))
      (node (ref R3) (pin 1))
      (node (ref C19) (pin 2)))
    (net (code 33) (name /Red)
      (node (ref J3) (pin 7))
      (node (ref R15) (pin 1))
      (node (ref R25) (pin 1))
      (node (ref R24) (pin 1)))
    (net (code 34) (name +5V)
      (node (ref R24) (pin 2))
      (node (ref U4) (pin 3))
      (node (ref C3) (pin 1))
      (node (ref U1) (pin 3)))
    (net (code 35) (name "Net-(C14-Pad1)")
      (node (ref U4) (pin 1))
      (node (ref C14) (pin 1))
      (node (ref D1) (pin 1)))
    (net (code 36) (name "Net-(C16-Pad2)")
      (node (ref R26) (pin 2))
      (node (ref R15) (pin 2))
      (node (ref Q2) (pin 3))
      (node (ref C16) (pin 2)))
    (net (code 37) (name /ADC0)
      (node (ref U3) (pin 6))
      (node (ref C17) (pin 2))
      (node (ref R2) (pin 1))
      (node (ref J4) (pin 7)))
    (net (code 38) (name "Net-(Q4-Pad1)")
      (node (ref Q4) (pin 1))
      (node (ref R17) (pin 1)))
    (net (code 39) (name "Net-(Q5-Pad1)")
      (node (ref R18) (pin 1))
      (node (ref Q5) (pin 1)))
    (net (code 40) (name "Net-(Q3-Pad1)")
      (node (ref Q3) (pin 1))
      (node (ref R16) (pin 1)))
    (net (code 41) (name /BOOT0)
      (node (ref SW2) (pin 1))
      (node (ref C2) (pin 1))
      (node (ref R1) (pin 1))
      (node (ref U3) (pin 1)))
    (net (code 42) (name /Tim14Ch1)
      (node (ref R16) (pin 2))
      (node (ref R19) (pin 2))
      (node (ref U3) (pin 10)))
    (net (code 43) (name /DigIn1)
      (node (ref C21) (pin 2))
      (node (ref U3) (pin 11))
      (node (ref R7) (pin 2)))
    (net (code 44) (name /TIM16_Ch1)
      (node (ref R20) (pin 2))
      (node (ref R17) (pin 2))
      (node (ref U3) (pin 12)))
    (net (code 45) (name /TIM17_Ch1)
      (node (ref R18) (pin 2))
      (node (ref R21) (pin 2))
      (node (ref U3) (pin 13)))
    (net (code 46) (name /TIM3_Ch4)
      (node (ref U3) (pin 14))
      (node (ref Q2) (pin 2))
      (node (ref R14) (pin 1)))
    (net (code 47) (name /USART_Tx)
      (node (ref U3) (pin 17))
      (node (ref U2) (pin 10)))
    (net (code 48) (name /USART_Rx)
      (node (ref U2) (pin 9))
      (node (ref U3) (pin 18)))
    (net (code 49) (name /NRST)
      (node (ref SW1) (pin 1))
      (node (ref C1) (pin 1))
      (node (ref U3) (pin 4)))
    (net (code 50) (name "Net-(U2-Pad14)")
      (node (ref U2) (pin 14)))
    (net (code 51) (name "Net-(U2-Pad13)")
      (node (ref U2) (pin 13)))
    (net (code 52) (name "Net-(J1-Pad9)")
      (node (ref J1) (pin 9)))
    (net (code 53) (name "Net-(U2-Pad11)")
      (node (ref U2) (pin 11)))
    (net (code 54) (name "Net-(U2-Pad12)")
      (node (ref U2) (pin 12)))
    (net (code 55) (name "Net-(J1-Pad4)")
      (node (ref J1) (pin 4)))
    (net (code 56) (name "Net-(J1-Pad6)")
      (node (ref J1) (pin 6)))
    (net (code 57) (name "Net-(J1-Pad7)")
      (node (ref J1) (pin 7)))
    (net (code 58) (name "Net-(J1-Pad8)")
      (node (ref J1) (pin 8)))
    (net (code 59) (name "Net-(J1-Pad1)")
      (node (ref J1) (pin 1)))))