(kicad_pcb (version 20211014) (generator pcbnew)

  (general
    (thickness 1.6)
  )

  (paper "A4")
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
    (50 "User.1" user)
    (51 "User.2" user)
    (52 "User.3" user)
    (53 "User.4" user)
    (54 "User.5" user)
    (55 "User.6" user)
    (56 "User.7" user)
    (57 "User.8" user)
    (58 "User.9" user)
  )

  (setup
    (stackup
      (layer "F.SilkS" (type "Top Silk Screen"))
      (layer "F.Paste" (type "Top Solder Paste"))
      (layer "F.Mask" (type "Top Solder Mask") (thickness 0.01))
      (layer "F.Cu" (type "copper") (thickness 0.035))
      (layer "dielectric 1" (type "core") (thickness 1.51) (material "FR4") (epsilon_r 4.5) (loss_tangent 0.02))
      (layer "B.Cu" (type "copper") (thickness 0.035))
      (layer "B.Mask" (type "Bottom Solder Mask") (thickness 0.01))
      (layer "B.Paste" (type "Bottom Solder Paste"))
      (layer "B.SilkS" (type "Bottom Silk Screen"))
      (copper_finish "None")
      (dielectric_constraints no)
    )
    (pad_to_mask_clearance 0)
    (pcbplotparams
      (layerselection 0x00010fc_ffffffff)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (svguseinch false)
      (svgprecision 6)
      (excludeedgelayer true)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "sensors_gerber/")
    )
  )

  (net 0 "")
  (net 1 "/S1")
  (net 2 "/S3")
  (net 3 "/S5")
  (net 4 "GND")
  (net 5 "/Sa0")
  (net 6 "/Sa2")
  (net 7 "/Sa4")
  (net 8 "/Sa6")
  (net 9 "/Sa1")
  (net 10 "/Sa3")
  (net 11 "/Sa5")

  (footprint "MountingHole:MountingHole_2mm" (layer "F.Cu")
    (tedit 5B924920) (tstamp 0009af96-15fd-406c-a152-9fa815dda016)
    (at 32.07 57.8)
    (descr "Mounting Hole 2mm, no annular")
    (tags "mounting hole 2mm no annular")
    (property "Sheetfile" "sensors.kicad_sch")
    (property "Sheetname" "")
    (path "/8a444c7f-4e59-4eb3-af78-38e4895cec8d")
    (attr exclude_from_pos_files)
    (fp_text reference "H4" (at 0 -3.2) (layer "F.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 6fe09487-b88e-47ff-aa3a-1e3a438847ce)
    )
    (fp_text value "MountingHole" (at 0 3.1) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 47174dfa-da7f-49a6-91e7-812208d8a089)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 2d93296a-10c6-4147-aa63-989a54f58317)
    )
    (fp_circle (center 0 0) (end 2 0) (layer "Cmts.User") (width 0.15) (fill none) (tstamp 84d23ad9-e945-491c-82a9-59706fd616d2))
    (fp_circle (center 0 0) (end 2.25 0) (layer "F.CrtYd") (width 0.05) (fill none) (tstamp 42f908b2-564c-481a-9988-d81802b26fe9))
    (pad "" np_thru_hole circle (at 0 0) (size 2 2) (drill 2) (layers *.Cu *.Mask) (tstamp 06ae87a6-9cfb-46d5-baf1-19b687441759))
  )

  (footprint "MountingHole:MountingHole_2mm" (layer "F.Cu")
    (tedit 5B924920) (tstamp 17f73842-84d5-4eee-a609-7172ddb9f167)
    (at 227.07 57.8)
    (descr "Mounting Hole 2mm, no annular")
    (tags "mounting hole 2mm no annular")
    (property "Sheetfile" "sensors.kicad_sch")
    (property "Sheetname" "")
    (path "/7bd85fc7-0166-4e29-a2c6-e5ce5ba3ac69")
    (attr exclude_from_pos_files)
    (fp_text reference "H1" (at 0 -3.2) (layer "F.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 15efa5a1-018d-4b37-9a0e-3f7115b2b69d)
    )
    (fp_text value "MountingHole" (at 0 3.1) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 6a501c8c-8f40-4d26-a79b-7eb51dc720a3)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp be49d73e-962b-4aad-9264-4ddf5298558b)
    )
    (fp_circle (center 0 0) (end 2 0) (layer "Cmts.User") (width 0.15) (fill none) (tstamp d1a68cf2-98e0-490d-ac97-ecd2ac126a5c))
    (fp_circle (center 0 0) (end 2.25 0) (layer "F.CrtYd") (width 0.05) (fill none) (tstamp c80aa4c2-4fd7-4f6e-ada5-f502700dd9cb))
    (pad "" np_thru_hole circle (at 0 0) (size 2 2) (drill 2) (layers *.Cu *.Mask) (tstamp def4a2e6-1f9e-4dc0-9bb5-05f215767f37))
  )

  (footprint "Connector_PinSocket_2.00mm:PinSocket_1x02_P2.00mm_Vertical" (layer "F.Cu")
    (tedit 5A19A42F) (tstamp 1ba8d335-6df5-4c0a-8605-d0877d2d055a)
    (at 212.72 49.8)
    (descr "Through hole straight socket strip, 1x02, 2.00mm pitch, single row (from Kicad 4.0.7), script generated")
    (tags "Through hole socket strip THT 1x02 2.00mm single row")
    (property "Sheetfile" "sensors.kicad_sch")
    (property "Sheetname" "")
    (path "/c3c36384-a6d3-49bf-aeb2-d528362983db")
    (attr through_hole)
    (fp_text reference "TH1" (at 0 -2.5) (layer "F.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 7e89b224-66fe-4aff-9a87-8def590f364b)
    )
    (fp_text value "PT1000" (at 0 4.5) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 1e065112-ff85-4a5c-9d6c-c312500ef605)
    )
    (fp_text user "${REFERENCE}" (at 0 1 90) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 79545e69-1d5c-4d6c-bb4f-a085bc10bb74)
    )
    (fp_line (start 1.06 1) (end 1.06 3.06) (layer "F.SilkS") (width 0.12) (tstamp 3796939f-3f85-4cc0-9d50-c268d9201d7d))
    (fp_line (start -1.06 1) (end 1.06 1) (layer "F.SilkS") (width 0.12) (tstamp 597ee87d-0612-4e5b-9d1b-682cd9cc6212))
    (fp_line (start 0 -1.06) (end 1.06 -1.06) (layer "F.SilkS") (width 0.12) (tstamp 92f2a8a2-f7af-4199-aca8-cdbdaedd5603))
    (fp_line (start -1.06 1) (end -1.06 3.06) (layer "F.SilkS") (width 0.12) (tstamp ba1e0708-462c-417b-b386-0a90710f8623))
    (fp_line (start 1.06 -1.06) (end 1.06 0) (layer "F.SilkS") (width 0.12) (tstamp bcc9267c-7bfa-4c6a-8b5b-424abe049e41))
    (fp_line (start -1.06 3.06) (end 1.06 3.06) (layer "F.SilkS") (width 0.12) (tstamp bfbddcf4-41a8-4456-a394-98735075d4af))
    (fp_line (start -1.5 3.5) (end -1.5 -1.5) (layer "F.CrtYd") (width 0.05) (tstamp 2a3e2d22-6dd1-474a-ae73-c818baa17d4a))
    (fp_line (start 1.5 -1.5) (end 1.5 3.5) (layer "F.CrtYd") (width 0.05) (tstamp 2ded0f1a-bbd5-4ee0-a0f5-1501ef0da3f9))
    (fp_line (start 1.5 3.5) (end -1.5 3.5) (layer "F.CrtYd") (width 0.05) (tstamp d0bc6230-e328-4f47-a293-2e467ea8fdda))
    (fp_line (start -1.5 -1.5) (end 1.5 -1.5) (layer "F.CrtYd") (width 0.05) (tstamp e459f708-fab3-4c1f-a249-acf8b4686945))
    (fp_line (start -1 -1) (end 0.5 -1) (layer "F.Fab") (width 0.1) (tstamp 2213375d-9924-4b9e-8169-6bc7dfdd509a))
    (fp_line (start 1 3) (end -1 3) (layer "F.Fab") (width 0.1) (tstamp 47505588-2305-4a54-8384-065119a07704))
    (fp_line (start 0.5 -1) (end 1 -0.5) (layer "F.Fab") (width 0.1) (tstamp 92ffbdda-080e-455b-b1dd-f656d9b7af5a))
    (fp_line (start 1 -0.5) (end 1 3) (layer "F.Fab") (width 0.1) (tstamp 98ec2c2c-5990-4b08-8846-b41ded2a0bf6))
    (fp_line (start -1 3) (end -1 -1) (layer "F.Fab") (width 0.1) (tstamp bf5230b9-b0c9-4528-9ac2-9e79b7b57ee7))
    (pad "1" thru_hole rect (at 0 0) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 "GND") (pintype "passive") (tstamp bd2322f3-7666-4455-9e7a-581ce5b8eb3a))
    (pad "2" thru_hole oval (at 0 2) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 9 "/Sa1") (pintype "passive") (tstamp d3703ebe-9b0a-472c-abf6-17a5d1dc297e))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinSocket_2.00mm.3dshapes/PinSocket_1x02_P2.00mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Jumper:SolderJumper-2_P1.3mm_Open_TrianglePad1.0x1.5mm" (layer "F.Cu")
    (tedit 5A64794F) (tstamp 1cbc2c25-ec50-4cbc-b48b-832e7114feb1)
    (at 116.4 53.4)
    (descr "SMD Solder Jumper, 1x1.5mm Triangular Pads, 0.3mm gap, open")
    (tags "solder jumper open")
    (property "Sheetfile" "sensors.kicad_sch")
    (property "Sheetname" "")
    (path "/a3a0fab8-d1da-40c6-a29d-fc8ec4303c6c")
    (attr exclude_from_pos_files)
    (fp_text reference "JP6" (at 0 -1.8) (layer "F.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 94ffa7fc-247c-4ea8-b294-78b1c1750a99)
    )
    (fp_text value "5" (at 2.25 0.1) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 0b4f7747-dc2d-428f-9a28-3900007e4ce7)
    )
    (fp_line (start 1.4 1) (end -1.4 1) (layer "F.SilkS") (width 0.12) (tstamp 9a8735a7-fa07-4100-8641-9e1d1c1cdc9f))
    (fp_line (start -1.4 -1) (end 1.4 -1) (layer "F.SilkS") (width 0.12) (tstamp 9b973ec1-37fa-4e4c-b947-c6872d47f070))
    (fp_line (start 1.4 -1) (end 1.4 1) (layer "F.SilkS") (width 0.12) (tstamp a8fcb922-89fe-4706-af4f-a315507e8af0))
    (fp_line (start -1.4 1) (end -1.4 -1) (layer "F.SilkS") (width 0.12) (tstamp e26b88e6-4a49-4666-b41c-ece50ff4a328))
    (fp_line (start 1.65 1.25) (end -1.65 1.25) (layer "F.CrtYd") (width 0.05) (tstamp 5476ef01-2a47-49cd-b5e7-8fe41c4773e3))
    (fp_line (start -1.65 -1.25) (end 1.65 -1.25) (layer "F.CrtYd") (width 0.05) (tstamp 67fbdc15-466e-42c6-a041-f716cb28b19e))
    (fp_line (start -1.65 -1.25) (end -1.65 1.25) (layer "F.CrtYd") (width 0.05) (tstamp b30b63ca-c30a-4817-9fb2-62dca3eb1b90))
    (fp_line (start 1.65 1.25) (end 1.65 -1.25) (layer "F.CrtYd") (width 0.05) (tstamp e3352c30-e7d8-435b-9102-f9f261eac32b))
    (pad "1" smd custom (at -0.725 0) (size 0.3 0.3) (layers "F.Cu" "F.Mask")
      (net 2 "/S3") (pinfunction "A") (pintype "passive") (zone_connect 2)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_poly (pts
            (xy 1 0)
            (xy 0.5 0.75)
            (xy -0.5 0.75)
            (xy -0.5 -0.75)
            (xy 0.5 -0.75)
          ) (width 0) (fill yes))
      ) (tstamp 79ad5f80-c9e9-41d2-ae41-58c2c9b1985c))
    (pad "2" smd custom (at 0.725 0) (size 0.3 0.3) (layers "F.Cu" "F.Mask")
      (net 11 "/Sa5") (pinfunction "B") (pintype "passive") (zone_connect 2)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_poly (pts
            (xy 0.5 0.75)
            (xy -0.65 0.75)
            (xy -0.15 0)
            (xy -0.65 -0.75)
            (xy 0.5 -0.75)
          ) (width 0) (fill yes))
      ) (tstamp a22d4e62-c9ec-44f6-9e5a-16b54078866e))
  )

  (footprint "Jumper:SolderJumper-2_P1.3mm_Open_TrianglePad1.0x1.5mm" (layer "F.Cu")
    (tedit 5A64794F) (tstamp 51f19916-a268-4788-bb1f-d635c14b27ce)
    (at 49.6 53.4)
    (descr "SMD Solder Jumper, 1x1.5mm Triangular Pads, 0.3mm gap, open")
    (tags "solder jumper open")
    (property "Sheetfile" "sensors.kicad_sch")
    (property "Sheetname" "")
    (path "/36cda546-00d0-4e00-b704-8da079c36193")
    (attr exclude_from_pos_files)
    (fp_text reference "JP9" (at 0 -1.8) (layer "F.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 66ae5036-b628-4f34-be9c-7be2269d8982)
    )
    (fp_text value "6" (at 2.1 -0.05) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp d244daa5-d63d-4d98-86f1-9f23a5214468)
    )
    (fp_line (start 1.4 1) (end -1.4 1) (layer "F.SilkS") (width 0.12) (tstamp 193f7ae0-8470-4d21-9ca3-63dad08ead23))
    (fp_line (start -1.4 -1) (end 1.4 -1) (layer "F.SilkS") (width 0.12) (tstamp 5d290ad5-813a-4783-b59a-a5968847e2cf))
    (fp_line (start 1.4 -1) (end 1.4 1) (layer "F.SilkS") (width 0.12) (tstamp 8fada9c7-8125-4deb-bb22-bfbb2b8c342d))
    (fp_line (start -1.4 1) (end -1.4 -1) (layer "F.SilkS") (width 0.12) (tstamp 95ec9e59-210c-40b6-b555-d2dd0f8466fa))
    (fp_line (start -1.65 -1.25) (end -1.65 1.25) (layer "F.CrtYd") (width 0.05) (tstamp 36073fc2-ca0d-405f-b3d4-5ce2111f2b0c))
    (fp_line (start -1.65 -1.25) (end 1.65 -1.25) (layer "F.CrtYd") (width 0.05) (tstamp b2bc5282-ee59-465b-8150-cd8a9ea238ef))
    (fp_line (start 1.65 1.25) (end 1.65 -1.25) (layer "F.CrtYd") (width 0.05) (tstamp b3f0994c-5770-43a0-8903-4c6345970763))
    (fp_line (start 1.65 1.25) (end -1.65 1.25) (layer "F.CrtYd") (width 0.05) (tstamp b761fdf9-76c2-4d93-8c6e-4338842888ca))
    (pad "1" smd custom (at -0.725 0) (size 0.3 0.3) (layers "F.Cu" "F.Mask")
      (net 3 "/S5") (pinfunction "A") (pintype "passive") (zone_connect 2)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_poly (pts
            (xy 1 0)
            (xy 0.5 0.75)
            (xy -0.5 0.75)
            (xy -0.5 -0.75)
            (xy 0.5 -0.75)
          ) (width 0) (fill yes))
      ) (tstamp 57dd3e63-e1c1-4a8a-92db-33531eae23e0))
    (pad "2" smd custom (at 0.725 0) (size 0.3 0.3) (layers "F.Cu" "F.Mask")
      (net 8 "/Sa6") (pinfunction "B") (pintype "passive") (zone_connect 2)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_poly (pts
            (xy 0.5 0.75)
            (xy -0.65 0.75)
            (xy -0.15 0)
            (xy -0.65 -0.75)
            (xy 0.5 -0.75)
          ) (width 0) (fill yes))
      ) (tstamp 0a8686a8-ae36-465f-bc2d-75ba6635302a))
  )

  (footprint "MountingHole:MountingHole_3.2mm_M3" (layer "F.Cu")
    (tedit 56D1B4CB) (tstamp 53c4d283-7966-456b-87d0-058f4542ce30)
    (at 69.57 50.8)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (property "Sheetfile" "sensors.kicad_sch")
    (property "Sheetname" "")
    (path "/ed304870-922d-4c72-a05c-e9b1b5b0b3bf")
    (attr exclude_from_pos_files)
    (fp_text reference "H6" (at 0 -4.2) (layer "F.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 49bac374-083b-420f-94da-dfb771257142)
    )
    (fp_text value "MountingHole" (at 0 4.2) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 0c10a4ea-027e-4078-8745-8cc87df138ae)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 37e1080e-1bdd-4e67-b3fe-f6c76fd1678d)
    )
    (fp_circle (center 0 0) (end 3.2 0) (layer "Cmts.User") (width 0.15) (fill none) (tstamp f60ac08a-e194-4426-a046-b51741b47900))
    (fp_circle (center 0 0) (end 3.45 0) (layer "F.CrtYd") (width 0.05) (fill none) (tstamp 4ae03562-81e6-4c00-b38e-74516caf6e79))
    (pad "" np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask) (tstamp 1076d752-38d4-4274-9c63-d84299bb6c11))
  )

  (footprint "MountingHole:MountingHole_3.2mm_M3" (layer "F.Cu")
    (tedit 56D1B4CB) (tstamp 63adbb99-81bd-4dca-b43f-283ba8293aa1)
    (at 107.57 50.8)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (property "Sheetfile" "sensors.kicad_sch")
    (property "Sheetname" "")
    (path "/19e980a7-c598-45a0-b341-97e0237187de")
    (attr exclude_from_pos_files)
    (fp_text reference "H8" (at 0 -4.2) (layer "F.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp dd0dd8b6-6dcc-4434-b3fe-e2de1e8c8537)
    )
    (fp_text value "MountingHole" (at 0 4.2) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp cec4b52f-5496-4b3a-af16-3b39b8989a19)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 85b7f862-f381-4bff-b3fc-2f66b23cb858)
    )
    (fp_circle (center 0 0) (end 3.2 0) (layer "Cmts.User") (width 0.15) (fill none) (tstamp 172fa3e1-bfdc-4e69-8f53-3b5100b50fe1))
    (fp_circle (center 0 0) (end 3.45 0) (layer "F.CrtYd") (width 0.05) (fill none) (tstamp f1bc43db-0280-4829-ac16-9eb94a1d2130))
    (pad "" np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask) (tstamp 14a385fd-d4eb-4fdf-bb56-0de853391147))
  )

  (footprint "Jumper:SolderJumper-2_P1.3mm_Open_TrianglePad1.0x1.5mm" (layer "F.Cu")
    (tedit 5A64794F) (tstamp 78afe069-a583-4362-86e0-1eaa8ccd5f47)
    (at 182.8 48.2)
    (descr "SMD Solder Jumper, 1x1.5mm Triangular Pads, 0.3mm gap, open")
    (tags "solder jumper open")
    (property "Sheetfile" "sensors.kicad_sch")
    (property "Sheetname" "")
    (path "/c3463576-ff8b-4b2b-9d5a-3dc566f9bd7b")
    (attr exclude_from_pos_files)
    (fp_text reference "JP1" (at 0 -1.8) (layer "F.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 8cb2d9d2-54c7-4709-a166-d5645124f185)
    )
    (fp_text value "1" (at 2.2 -0.05) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp b259f425-5eb9-4675-bea0-ae55bde99ab3)
    )
    (fp_line (start 1.4 1) (end -1.4 1) (layer "F.SilkS") (width 0.12) (tstamp 9009c92e-56b9-43be-9dfc-4838c191cf5d))
    (fp_line (start -1.4 -1) (end 1.4 -1) (layer "F.SilkS") (width 0.12) (tstamp b2903c64-901c-433a-9d27-8450ed62cd3e))
    (fp_line (start 1.4 -1) (end 1.4 1) (layer "F.SilkS") (width 0.12) (tstamp df6fe31c-a865-484e-93a0-d140b105665f))
    (fp_line (start -1.4 1) (end -1.4 -1) (layer "F.SilkS") (width 0.12) (tstamp e0c41c0d-96fd-4f47-92a7-82fda17f13b7))
    (fp_line (start 1.65 1.25) (end 1.65 -1.25) (layer "F.CrtYd") (width 0.05) (tstamp 39d930c1-3505-4108-ae4b-0bdede0f0a4e))
    (fp_line (start -1.65 -1.25) (end -1.65 1.25) (layer "F.CrtYd") (width 0.05) (tstamp 4eb325b6-a027-4858-b723-2551fdb8a3b6))
    (fp_line (start -1.65 -1.25) (end 1.65 -1.25) (layer "F.CrtYd") (width 0.05) (tstamp 65b593ca-dd52-48ce-a1d6-0ce697f2907b))
    (fp_line (start 1.65 1.25) (end -1.65 1.25) (layer "F.CrtYd") (width 0.05) (tstamp 9c269dad-ac04-4d99-be6d-586589e5410b))
    (pad "1" smd custom (at -0.725 0) (size 0.3 0.3) (layers "F.Cu" "F.Mask")
      (net 1 "/S1") (pinfunction "A") (pintype "passive") (zone_connect 2)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_poly (pts
            (xy 1 0)
            (xy 0.5 0.75)
            (xy -0.5 0.75)
            (xy -0.5 -0.75)
            (xy 0.5 -0.75)
          ) (width 0) (fill yes))
      ) (tstamp 8c0b7a65-0cce-4d9f-86c8-afd43397e397))
    (pad "2" smd custom (at 0.725 0) (size 0.3 0.3) (layers "F.Cu" "F.Mask")
      (net 9 "/Sa1") (pinfunction "B") (pintype "passive") (zone_connect 2)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_poly (pts
            (xy 0.5 0.75)
            (xy -0.65 0.75)
            (xy -0.15 0)
            (xy -0.65 -0.75)
            (xy 0.5 -0.75)
          ) (width 0) (fill yes))
      ) (tstamp 4fa3ffce-6d51-4faa-8376-50b07008c845))
  )

  (footprint "Jumper:SolderJumper-2_P1.3mm_Open_TrianglePad1.0x1.5mm" (layer "F.Cu")
    (tedit 5A64794F) (tstamp 7e9c9a63-f462-4d35-bda4-6f87746ca516)
    (at 49.6 50.8)
    (descr "SMD Solder Jumper, 1x1.5mm Triangular Pads, 0.3mm gap, open")
    (tags "solder jumper open")
    (property "Sheetfile" "sensors.kicad_sch")
    (property "Sheetname" "")
    (path "/5b00e6e1-cb61-49d8-b8d1-bd81fc3a70c1")
    (attr exclude_from_pos_files)
    (fp_text reference "JP8" (at 0 -1.8) (layer "F.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 78eb0d01-33ec-49ff-b8c2-2261bdc4affa)
    )
    (fp_text value "3" (at 2.15 -0.05) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 3e11c4ec-6ecf-463e-a507-04c71d275323)
    )
    (fp_line (start 1.4 1) (end -1.4 1) (layer "F.SilkS") (width 0.12) (tstamp 37160243-52bd-4101-b7c0-7dbb7a631965))
    (fp_line (start -1.4 -1) (end 1.4 -1) (layer "F.SilkS") (width 0.12) (tstamp 3c24f6bf-e7c2-4923-9922-15cf1d43671e))
    (fp_line (start -1.4 1) (end -1.4 -1) (layer "F.SilkS") (width 0.12) (tstamp b36303a5-3600-4d4c-86c7-cafbe7173303))
    (fp_line (start 1.4 -1) (end 1.4 1) (layer "F.SilkS") (width 0.12) (tstamp f7169570-778d-444c-b5af-b51b764b3aac))
    (fp_line (start -1.65 -1.25) (end 1.65 -1.25) (layer "F.CrtYd") (width 0.05) (tstamp 3035ec7a-0278-4d35-94dd-4f43cb80bdc0))
    (fp_line (start 1.65 1.25) (end 1.65 -1.25) (layer "F.CrtYd") (width 0.05) (tstamp 86dfb5d6-00b2-493c-b05e-58bfb21dc235))
    (fp_line (start -1.65 -1.25) (end -1.65 1.25) (layer "F.CrtYd") (width 0.05) (tstamp e574820a-96bc-48d2-969f-0d2be5a57d71))
    (fp_line (start 1.65 1.25) (end -1.65 1.25) (layer "F.CrtYd") (width 0.05) (tstamp fbc96cac-7591-4c55-95c9-12d7e5bacef4))
    (pad "1" smd custom (at -0.725 0) (size 0.3 0.3) (layers "F.Cu" "F.Mask")
      (net 3 "/S5") (pinfunction "A") (pintype "passive") (zone_connect 2)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_poly (pts
            (xy 1 0)
            (xy 0.5 0.75)
            (xy -0.5 0.75)
            (xy -0.5 -0.75)
            (xy 0.5 -0.75)
          ) (width 0) (fill yes))
      ) (tstamp fc7d05a5-b286-430d-ae98-43b3cbbed34f))
    (pad "2" smd custom (at 0.725 0) (size 0.3 0.3) (layers "F.Cu" "F.Mask")
      (net 10 "/Sa3") (pinfunction "B") (pintype "passive") (zone_connect 2)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_poly (pts
            (xy 0.5 0.75)
            (xy -0.65 0.75)
            (xy -0.15 0)
            (xy -0.65 -0.75)
            (xy 0.5 -0.75)
          ) (width 0) (fill yes))
      ) (tstamp 193559a5-5542-4af7-90b1-341fbdf566b8))
  )

  (footprint "Jumper:SolderJumper-2_P1.3mm_Open_TrianglePad1.0x1.5mm" (layer "F.Cu")
    (tedit 5A64794F) (tstamp 885ea355-4623-4a20-b1a0-7bd79fe3127e)
    (at 116.4 50.8)
    (descr "SMD Solder Jumper, 1x1.5mm Triangular Pads, 0.3mm gap, open")
    (tags "solder jumper open")
    (property "Sheetfile" "sensors.kicad_sch")
    (property "Sheetname" "")
    (path "/5a32a366-55c9-44ab-adc2-ed65c9032b82")
    (attr exclude_from_pos_files)
    (fp_text reference "JP5" (at 0 -1.8) (layer "F.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 7777d436-24e8-4a01-b4a8-06bbf1e601a2)
    )
    (fp_text value "4" (at 2.2 0) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 1d092029-eb94-4dbf-9abb-936498fec884)
    )
    (fp_line (start -1.4 -1) (end 1.4 -1) (layer "F.SilkS") (width 0.12) (tstamp 4410edf2-55ff-4d3e-80af-7e3e1d1b5ad7))
    (fp_line (start 1.4 1) (end -1.4 1) (layer "F.SilkS") (width 0.12) (tstamp 4981f1db-c9f1-453f-8310-12fa847f7963))
    (fp_line (start 1.4 -1) (end 1.4 1) (layer "F.SilkS") (width 0.12) (tstamp 517626c0-4db4-4cf8-a6e5-2a8513e78519))
    (fp_line (start -1.4 1) (end -1.4 -1) (layer "F.SilkS") (width 0.12) (tstamp d61c17e5-360e-46a1-95be-59251432bc79))
    (fp_line (start -1.65 -1.25) (end -1.65 1.25) (layer "F.CrtYd") (width 0.05) (tstamp 1c8c9292-3d41-4979-8be5-9834592ac415))
    (fp_line (start 1.65 1.25) (end 1.65 -1.25) (layer "F.CrtYd") (width 0.05) (tstamp 8e7c8e37-a2a0-4977-bec4-9a4dbb18175b))
    (fp_line (start -1.65 -1.25) (end 1.65 -1.25) (layer "F.CrtYd") (width 0.05) (tstamp 95e62747-ec99-482f-bc01-5bc8c901c3c5))
    (fp_line (start 1.65 1.25) (end -1.65 1.25) (layer "F.CrtYd") (width 0.05) (tstamp a75c5e2c-64aa-4d88-94e1-bf99c1872f81))
    (pad "1" smd custom (at -0.725 0) (size 0.3 0.3) (layers "F.Cu" "F.Mask")
      (net 2 "/S3") (pinfunction "A") (pintype "passive") (zone_connect 2)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_poly (pts
            (xy 1 0)
            (xy 0.5 0.75)
            (xy -0.5 0.75)
            (xy -0.5 -0.75)
            (xy 0.5 -0.75)
          ) (width 0) (fill yes))
      ) (tstamp 6abc2b7f-d5e9-4803-b051-aa0b4fbc5f0c))
    (pad "2" smd custom (at 0.725 0) (size 0.3 0.3) (layers "F.Cu" "F.Mask")
      (net 7 "/Sa4") (pinfunction "B") (pintype "passive") (zone_connect 2)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_poly (pts
            (xy 0.5 0.75)
            (xy -0.65 0.75)
            (xy -0.15 0)
            (xy -0.65 -0.75)
            (xy 0.5 -0.75)
          ) (width 0) (fill yes))
      ) (tstamp d48f37d5-df18-4413-8da2-8d215a4f235a))
  )

  (footprint "MountingHole:MountingHole_3.2mm_M3" (layer "F.Cu")
    (tedit 56D1B4CB) (tstamp 94dda981-189e-4bf4-9a41-b68cfe0aa4fa)
    (at 151.57 50.8)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (property "Sheetfile" "sensors.kicad_sch")
    (property "Sheetname" "")
    (path "/115c0ca5-b5d5-45b8-9907-1a92b1479d9a")
    (attr exclude_from_pos_files)
    (fp_text reference "H5" (at 0 -4.2) (layer "F.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp b72f8761-6138-4a77-844d-be853ba4eb10)
    )
    (fp_text value "MountingHole" (at 0 4.2) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp d0243077-a556-4a2d-a967-1a723004c1bc)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp d9147773-1936-4a19-a410-dc23a55d5a79)
    )
    (fp_circle (center 0 0) (end 3.2 0) (layer "Cmts.User") (width 0.15) (fill none) (tstamp e47ab037-66dd-41ad-93cb-826862c591b7))
    (fp_circle (center 0 0) (end 3.45 0) (layer "F.CrtYd") (width 0.05) (fill none) (tstamp a9a2ab94-bcea-4897-a064-8afdf8960b95))
    (pad "" np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask) (tstamp 4be34232-df00-4cde-a3d3-b26b3c5bdb00))
  )

  (footprint "Jumper:SolderJumper-2_P1.3mm_Open_TrianglePad1.0x1.5mm" (layer "F.Cu")
    (tedit 5A64794F) (tstamp a04f48ac-af67-47e7-8b05-7bc5f4270fed)
    (at 116.4 48.2)
    (descr "SMD Solder Jumper, 1x1.5mm Triangular Pads, 0.3mm gap, open")
    (tags "solder jumper open")
    (property "Sheetfile" "sensors.kicad_sch")
    (property "Sheetname" "")
    (path "/0861f0d1-87bd-4423-beb3-c2b3d2a16d26")
    (attr exclude_from_pos_files)
    (fp_text reference "JP4" (at 0 -1.8) (layer "F.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp dd2f2542-74ea-4549-918d-ad2fae204f92)
    )
    (fp_text value "2" (at 2.2 0.05) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 207065a8-de2d-4bab-b834-4f538f313837)
    )
    (fp_line (start -1.4 -1) (end 1.4 -1) (layer "F.SilkS") (width 0.12) (tstamp 1426eae0-3172-4b1e-87eb-451c6ab6cb2e))
    (fp_line (start -1.4 1) (end -1.4 -1) (layer "F.SilkS") (width 0.12) (tstamp 6e6c8690-5556-48fd-b277-7ecc372858f3))
    (fp_line (start 1.4 1) (end -1.4 1) (layer "F.SilkS") (width 0.12) (tstamp 8ffaa809-e55e-4fc8-b450-41bd972b2310))
    (fp_line (start 1.4 -1) (end 1.4 1) (layer "F.SilkS") (width 0.12) (tstamp db510f9b-16b7-469e-8e3d-472d5093fcc9))
    (fp_line (start -1.65 -1.25) (end -1.65 1.25) (layer "F.CrtYd") (width 0.05) (tstamp 4f9dcea1-d3f2-4c1c-a45d-979dead63c0b))
    (fp_line (start -1.65 -1.25) (end 1.65 -1.25) (layer "F.CrtYd") (width 0.05) (tstamp 736a8d9a-8959-4373-b5a4-2cb82ef7e139))
    (fp_line (start 1.65 1.25) (end -1.65 1.25) (layer "F.CrtYd") (width 0.05) (tstamp ebe125c3-1607-4618-ae9b-d1d7002faa89))
    (fp_line (start 1.65 1.25) (end 1.65 -1.25) (layer "F.CrtYd") (width 0.05) (tstamp f03d51b4-b5b6-478d-abab-cc2ce9860069))
    (pad "1" smd custom (at -0.725 0) (size 0.3 0.3) (layers "F.Cu" "F.Mask")
      (net 2 "/S3") (pinfunction "A") (pintype "passive") (zone_connect 2)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_poly (pts
            (xy 1 0)
            (xy 0.5 0.75)
            (xy -0.5 0.75)
            (xy -0.5 -0.75)
            (xy 0.5 -0.75)
          ) (width 0) (fill yes))
      ) (tstamp be94f073-ea93-434f-bc3c-77109d7bdb60))
    (pad "2" smd custom (at 0.725 0) (size 0.3 0.3) (layers "F.Cu" "F.Mask")
      (net 6 "/Sa2") (pinfunction "B") (pintype "passive") (zone_connect 2)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_poly (pts
            (xy 0.5 0.75)
            (xy -0.65 0.75)
            (xy -0.15 0)
            (xy -0.65 -0.75)
            (xy 0.5 -0.75)
          ) (width 0) (fill yes))
      ) (tstamp 9c236696-d944-417c-884f-acbfc7f010d6))
  )

  (footprint "Connector_PinSocket_2.00mm:PinSocket_1x02_P2.00mm_Vertical" (layer "F.Cu")
    (tedit 5A19A42F) (tstamp ae09c41c-3bb2-40c3-a765-8f058de750d0)
    (at 146.06 49.8)
    (descr "Through hole straight socket strip, 1x02, 2.00mm pitch, single row (from Kicad 4.0.7), script generated")
    (tags "Through hole socket strip THT 1x02 2.00mm single row")
    (property "Sheetfile" "sensors.kicad_sch")
    (property "Sheetname" "")
    (path "/db3e444a-55f3-4a55-80ad-ca2b02421013")
    (attr through_hole)
    (fp_text reference "TH3" (at 0 -2.5) (layer "F.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 696784d1-a0d5-475e-8275-2717d724d1f9)
    )
    (fp_text value "PT1000" (at 0 4.5) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp ce555cf4-e677-47f2-9740-ba43b51ce779)
    )
    (fp_text user "${REFERENCE}" (at 0 1 90) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 0e5bf35d-1bfc-4a67-89b8-e3e1479bc988)
    )
    (fp_line (start 1.06 1) (end 1.06 3.06) (layer "F.SilkS") (width 0.12) (tstamp 0be4718c-702c-4882-9ca3-9d8aba29614d))
    (fp_line (start -1.06 1) (end 1.06 1) (layer "F.SilkS") (width 0.12) (tstamp c55e06b4-6732-4c5a-b003-8dd536ccb8fb))
    (fp_line (start -1.06 1) (end -1.06 3.06) (layer "F.SilkS") (width 0.12) (tstamp de0d2e57-29dc-4f7f-bdfa-6a10a18c609f))
    (fp_line (start 0 -1.06) (end 1.06 -1.06) (layer "F.SilkS") (width 0.12) (tstamp e198fe00-b9ac-4eaa-945d-209dfa8d1c43))
    (fp_line (start 1.06 -1.06) (end 1.06 0) (layer "F.SilkS") (width 0.12) (tstamp e7bd17f7-be8e-4e5d-996e-5aef763f8593))
    (fp_line (start -1.06 3.06) (end 1.06 3.06) (layer "F.SilkS") (width 0.12) (tstamp ef4d8e85-f36e-4e23-bd40-e8e2dac8d926))
    (fp_line (start 1.5 3.5) (end -1.5 3.5) (layer "F.CrtYd") (width 0.05) (tstamp 15d25102-ebb9-49aa-952e-e6dee25f8177))
    (fp_line (start -1.5 -1.5) (end 1.5 -1.5) (layer "F.CrtYd") (width 0.05) (tstamp 2d074f63-cbb3-466d-a6d4-d5261e679bff))
    (fp_line (start -1.5 3.5) (end -1.5 -1.5) (layer "F.CrtYd") (width 0.05) (tstamp bbced34d-ba3c-4c54-ada9-2adc7f70f4a4))
    (fp_line (start 1.5 -1.5) (end 1.5 3.5) (layer "F.CrtYd") (width 0.05) (tstamp e3cc484a-aa41-45fd-b03a-308a5cd234dd))
    (fp_line (start 0.5 -1) (end 1 -0.5) (layer "F.Fab") (width 0.1) (tstamp 00869d66-ebe4-4ca8-bf2b-e7a1dbaa7135))
    (fp_line (start -1 3) (end -1 -1) (layer "F.Fab") (width 0.1) (tstamp 11dfcccc-2098-4b85-99f1-56ed6335a7a6))
    (fp_line (start 1 -0.5) (end 1 3) (layer "F.Fab") (width 0.1) (tstamp 355b9f34-729c-49d1-b8f4-73f1a9758684))
    (fp_line (start -1 -1) (end 0.5 -1) (layer "F.Fab") (width 0.1) (tstamp 5c7b9110-994c-418f-b05c-1e412409ea9e))
    (fp_line (start 1 3) (end -1 3) (layer "F.Fab") (width 0.1) (tstamp aa3152ce-d773-4204-a8ef-eff4db8610c5))
    (pad "1" thru_hole rect (at 0 0) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 "GND") (pintype "passive") (tstamp cb7cab46-239f-4137-8893-d7fea9875352))
    (pad "2" thru_hole oval (at 0 2) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 10 "/Sa3") (pintype "passive") (tstamp 22ebbdda-ed16-4314-8829-99f8c93676bd))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinSocket_2.00mm.3dshapes/PinSocket_1x02_P2.00mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "J8:avia8" (layer "F.Cu")
    (tedit 0) (tstamp b58ac950-1d04-41ea-bb84-ff3398cd891e)
    (at 218.3 50.8 -90)
    (property "Sheetfile" "sensors.kicad_sch")
    (property "Sheetname" "")
    (path "/861db8d1-20ac-49af-a86d-49db3f8a7d40")
    (attr through_hole)
    (fp_text reference "J1" (at -0.0508 -4.4196 -90 unlocked) (layer "F.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 80dd8091-be64-46f0-97ec-c1fd134ce5ab)
    )
    (fp_text value "Conn_01x08" (at 0.0254 4.2926 -90 unlocked) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp a7d74016-fa1a-4b62-a669-2d9a8bf375eb)
    )
    (pad "" np_thru_hole circle (at -7.5184 -1.27 270) (size 2.5 2.5) (drill 2.2) (layers F&B.Cu *.Mask) (tstamp 09c100c1-8ad5-492c-b3a6-bbe95107e03e))
    (pad "" np_thru_hole circle (at 7.5184 -1.27 270) (size 2.5 2.5) (drill 2.2) (layers F&B.Cu *.Mask) (tstamp 3b9c3e89-aa80-4b66-a875-d9d17f75b939))
    (pad "" np_thru_hole circle (at -8.382 -5.2832 270) (size 2.8 2.8) (drill 2.4) (layers F&B.Cu *.Mask) (tstamp 9e4f0613-fbec-4ac1-9d52-d7ab637167f0))
    (pad "" np_thru_hole circle (at 8.382 -5.2832 270) (size 2.8 2.8) (drill 2.4) (layers F&B.Cu *.Mask) (tstamp c9161e72-29f6-48b4-8553-20bae1837876))
    (pad "1" thru_hole circle (at -2.0828 -2.54 270) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 5 "/Sa0") (pinfunction "Pin_1") (pintype "passive") (tstamp 1a16fee9-a785-4812-896a-e5a03e8c22b9))
    (pad "2" thru_hole circle (at 0 -2.54 270) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 9 "/Sa1") (pinfunction "Pin_2") (pintype "passive") (tstamp e87e50df-cdbd-466d-91de-5c8a58fe0c6b))
    (pad "3" thru_hole circle (at 2.0828 -2.54 270) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 6 "/Sa2") (pinfunction "Pin_3") (pintype "passive") (tstamp b5a15c55-ed01-409b-9983-3a2755e914a3))
    (pad "4" thru_hole circle (at -2.7178 0 270) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 10 "/Sa3") (pinfunction "Pin_4") (pintype "passive") (tstamp d35070bc-a663-461b-b114-716bb420e2bb))
    (pad "5" thru_hole circle (at 0 0 270) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 4 "GND") (pinfunction "Pin_5") (pintype "passive") (tstamp da64eec1-0448-43f3-be58-60bc2dc183c6))
    (pad "6" thru_hole circle (at 2.7178 0 270) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 7 "/Sa4") (pinfunction "Pin_6") (pintype "passive") (tstamp 83ccb5d4-5eb4-4e37-b063-c60c86d0599d))
    (pad "7" thru_hole circle (at -1.4986 2.54 270) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 11 "/Sa5") (pinfunction "Pin_7") (pintype "passive") (tstamp 8ba01976-489a-48ae-8385-c0b38af2ad9b))
    (pad "8" thru_hole circle (at 1.4986 2.54 270) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 8 "/Sa6") (pinfunction "Pin_8") (pintype "passive") (tstamp 6c888e6d-e47f-4b1b-8a7a-e51fbfcef897))
  )

  (footprint "Connector_PinSocket_2.00mm:PinSocket_1x02_P2.00mm_Vertical" (layer "F.Cu")
    (tedit 5A19A42F) (tstamp c8dca831-ef86-488d-9122-6b53aab225c2)
    (at 46.07 49.8)
    (descr "Through hole straight socket strip, 1x02, 2.00mm pitch, single row (from Kicad 4.0.7), script generated")
    (tags "Through hole socket strip THT 1x02 2.00mm single row")
    (property "Sheetfile" "sensors.kicad_sch")
    (property "Sheetname" "")
    (path "/16c1b640-5e73-403f-8060-6a32c823f7df")
    (attr through_hole)
    (fp_text reference "TH6" (at 0 -2.5) (layer "F.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 05085b76-2f5a-4f03-87a0-071536feaa66)
    )
    (fp_text value "PT1000" (at 0 4.5) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp ef7a8fcc-a523-4749-8e5b-4cdd537619f5)
    )
    (fp_text user "${REFERENCE}" (at 0 1 90) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 36b94c2b-ef4a-4e84-adbf-e87883d16eb8)
    )
    (fp_line (start -1.06 3.06) (end 1.06 3.06) (layer "F.SilkS") (width 0.12) (tstamp 37cf6073-bf98-47cf-bc85-5d78691a8e53))
    (fp_line (start 1.06 -1.06) (end 1.06 0) (layer "F.SilkS") (width 0.12) (tstamp 42bf11ce-bfe9-49f6-8b7b-2b05bb51bfb7))
    (fp_line (start -1.06 1) (end -1.06 3.06) (layer "F.SilkS") (width 0.12) (tstamp 9c084e44-cc34-4517-8f6c-de70520c80ac))
    (fp_line (start -1.06 1) (end 1.06 1) (layer "F.SilkS") (width 0.12) (tstamp c70529c6-2a5d-4505-a1b4-c0ab7598da9c))
    (fp_line (start 0 -1.06) (end 1.06 -1.06) (layer "F.SilkS") (width 0.12) (tstamp de0ef650-ab2b-4695-8d6e-63dc13b804c0))
    (fp_line (start 1.06 1) (end 1.06 3.06) (layer "F.SilkS") (width 0.12) (tstamp f21188f9-2dbb-4d1d-a258-155c46386e90))
    (fp_line (start -1.5 -1.5) (end 1.5 -1.5) (layer "F.CrtYd") (width 0.05) (tstamp 15741c0c-857b-41cd-9692-165dbad37c23))
    (fp_line (start 1.5 -1.5) (end 1.5 3.5) (layer "F.CrtYd") (width 0.05) (tstamp 319bbf78-92bd-4186-84a2-04d7e9db591e))
    (fp_line (start -1.5 3.5) (end -1.5 -1.5) (layer "F.CrtYd") (width 0.05) (tstamp c63ed440-a3e3-4c32-8103-4684ddb3a680))
    (fp_line (start 1.5 3.5) (end -1.5 3.5) (layer "F.CrtYd") (width 0.05) (tstamp fb54b096-a03c-4519-8c8c-1b2fc889cc1a))
    (fp_line (start -1 3) (end -1 -1) (layer "F.Fab") (width 0.1) (tstamp 4fb7b951-652e-41a0-85dd-b52b45857eaf))
    (fp_line (start 1 3) (end -1 3) (layer "F.Fab") (width 0.1) (tstamp 5739dc05-c6d1-4674-a30e-08d9eb5c129f))
    (fp_line (start -1 -1) (end 0.5 -1) (layer "F.Fab") (width 0.1) (tstamp 714a0f3c-cc81-4725-a957-6389c6adfe8f))
    (fp_line (start 0.5 -1) (end 1 -0.5) (layer "F.Fab") (width 0.1) (tstamp a0a3be5a-eef2-4487-a145-36bceb71d29b))
    (fp_line (start 1 -0.5) (end 1 3) (layer "F.Fab") (width 0.1) (tstamp c2bc37ee-2a38-486f-922a-5d545a48412e))
    (pad "1" thru_hole rect (at 0 0) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 "GND") (pintype "passive") (tstamp bf7101e3-ac6e-4500-b005-fde2d2f1e18f))
    (pad "2" thru_hole oval (at 0 2) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 "/S5") (pintype "passive") (tstamp 2cba6635-34dc-43d1-9a98-763446741388))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinSocket_2.00mm.3dshapes/PinSocket_1x02_P2.00mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "MountingHole:MountingHole_2mm" (layer "F.Cu")
    (tedit 5B924920) (tstamp d478ecf0-dbcb-4dcc-a30d-6c13db7921e8)
    (at 227.07 43.8)
    (descr "Mounting Hole 2mm, no annular")
    (tags "mounting hole 2mm no annular")
    (property "Sheetfile" "sensors.kicad_sch")
    (property "Sheetname" "")
    (path "/018a6c0a-9e2f-4a7f-b97f-552cbe26bd38")
    (attr exclude_from_pos_files)
    (fp_text reference "H3" (at 0 -3.2) (layer "F.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp f4565626-8851-4112-b35c-490240071c3a)
    )
    (fp_text value "MountingHole" (at 0 3.1) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 4cbed584-1506-41f8-83e8-b1506162fd12)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 31764dcb-8dc7-4d04-adfb-52182dd9ebdc)
    )
    (fp_circle (center 0 0) (end 2 0) (layer "Cmts.User") (width 0.15) (fill none) (tstamp ddc4d40e-61b5-40ac-a778-a065fc1b5694))
    (fp_circle (center 0 0) (end 2.25 0) (layer "F.CrtYd") (width 0.05) (fill none) (tstamp 50f0e003-4b18-4743-96b3-82a41bed794b))
    (pad "" np_thru_hole circle (at 0 0) (size 2 2) (drill 2) (layers *.Cu *.Mask) (tstamp 31ec83d0-0e63-4f4e-9a68-46d624470342))
  )

  (footprint "Connector_PinSocket_2.00mm:PinSocket_1x02_P2.00mm_Vertical" (layer "F.Cu")
    (tedit 5A19A42F) (tstamp e55fae2d-e54f-41d0-b163-0a4f12b6846a)
    (at 79.4 49.8)
    (descr "Through hole straight socket strip, 1x02, 2.00mm pitch, single row (from Kicad 4.0.7), script generated")
    (tags "Through hole socket strip THT 1x02 2.00mm single row")
    (property "Sheetfile" "sensors.kicad_sch")
    (property "Sheetname" "")
    (path "/e2800ae7-764e-496f-aa74-3c0a3492ebd1")
    (attr through_hole)
    (fp_text reference "TH5" (at 0 -2.5) (layer "F.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp d2430977-7fbf-45a5-aa48-b2f401e14807)
    )
    (fp_text value "PT1000" (at 0 4.5) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 4c438854-85da-4d61-8f9e-2280b3c2b4c3)
    )
    (fp_text user "${REFERENCE}" (at 0 1 90) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 34f4d4ca-ef8e-48cd-a34b-2443c593fe6e)
    )
    (fp_line (start 1.06 -1.06) (end 1.06 0) (layer "F.SilkS") (width 0.12) (tstamp 16a932e9-eab9-416a-9dc6-e6dce47c21d1))
    (fp_line (start -1.06 1) (end -1.06 3.06) (layer "F.SilkS") (width 0.12) (tstamp 37cb53d2-2648-450a-9ee7-cb9afc9db230))
    (fp_line (start -1.06 1) (end 1.06 1) (layer "F.SilkS") (width 0.12) (tstamp 9e77766b-5c27-4a6d-a85c-42f5f668b703))
    (fp_line (start -1.06 3.06) (end 1.06 3.06) (layer "F.SilkS") (width 0.12) (tstamp a56e25dc-7674-4aeb-9812-e18a49290a9c))
    (fp_line (start 1.06 1) (end 1.06 3.06) (layer "F.SilkS") (width 0.12) (tstamp c476deb4-929b-49bb-8636-76edc0845c9e))
    (fp_line (start 0 -1.06) (end 1.06 -1.06) (layer "F.SilkS") (width 0.12) (tstamp fb5479a5-89b7-42cb-9168-e1e492643e20))
    (fp_line (start 1.5 -1.5) (end 1.5 3.5) (layer "F.CrtYd") (width 0.05) (tstamp 11d34507-ea6c-47cc-9dbb-2b738cc10734))
    (fp_line (start -1.5 -1.5) (end 1.5 -1.5) (layer "F.CrtYd") (width 0.05) (tstamp 60d2fec4-1ada-45df-9fbf-15b135db52a2))
    (fp_line (start 1.5 3.5) (end -1.5 3.5) (layer "F.CrtYd") (width 0.05) (tstamp a3d4769a-71f3-4cf0-addd-a7c14fb7360c))
    (fp_line (start -1.5 3.5) (end -1.5 -1.5) (layer "F.CrtYd") (width 0.05) (tstamp aa8b8d7c-861a-4c0b-badd-12d3ed943e74))
    (fp_line (start 1 3) (end -1 3) (layer "F.Fab") (width 0.1) (tstamp 3a1ac587-b0df-44a7-95d9-b69d33dbd105))
    (fp_line (start 0.5 -1) (end 1 -0.5) (layer "F.Fab") (width 0.1) (tstamp 4afcb04a-1df0-4ffb-aa62-89f7b59ef8cd))
    (fp_line (start 1 -0.5) (end 1 3) (layer "F.Fab") (width 0.1) (tstamp 690761cf-dfbe-487f-804f-c4eaad2a39c0))
    (fp_line (start -1 3) (end -1 -1) (layer "F.Fab") (width 0.1) (tstamp 973037a7-9b99-4f95-987e-0687e655f16e))
    (fp_line (start -1 -1) (end 0.5 -1) (layer "F.Fab") (width 0.1) (tstamp cef103b0-3ebb-4556-b8dd-cc900b09d4e0))
    (pad "1" thru_hole rect (at 0 0) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 "GND") (pintype "passive") (tstamp 40bba0e5-1db7-456d-b9ec-ea1557b3a420))
    (pad "2" thru_hole oval (at 0 2) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 11 "/Sa5") (pintype "passive") (tstamp 6ded0065-567c-4158-808e-46b51c029249))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinSocket_2.00mm.3dshapes/PinSocket_1x02_P2.00mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "MountingHole:MountingHole_3.2mm_M3" (layer "F.Cu")
    (tedit 56D1B4CB) (tstamp e56821d4-c826-40df-973c-6cb7bdda61a8)
    (at 189.57 50.8)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (property "Sheetfile" "sensors.kicad_sch")
    (property "Sheetname" "")
    (path "/90d62700-4d23-4d16-b6fa-43f7008b64dd")
    (attr exclude_from_pos_files)
    (fp_text reference "H7" (at 0 -4.2) (layer "F.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 4025b10b-1424-43b5-a0b4-88de105cccd0)
    )
    (fp_text value "MountingHole" (at 0 4.2) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp f0b47c18-81ea-439a-968a-99723ad03a92)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp c042dbeb-19cd-4a67-817f-4276d111c28e)
    )
    (fp_circle (center 0 0) (end 3.2 0) (layer "Cmts.User") (width 0.15) (fill none) (tstamp 7ff1e29c-d2f1-440e-86af-c01b1b6c5fa5))
    (fp_circle (center 0 0) (end 3.45 0) (layer "F.CrtYd") (width 0.05) (fill none) (tstamp c575391f-b198-4ffa-aa6c-eb86e62aaa18))
    (pad "" np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask) (tstamp 46d485b0-bcc7-4533-9ab1-b2a43dac7fa7))
  )

  (footprint "Jumper:SolderJumper-2_P1.3mm_Open_TrianglePad1.0x1.5mm" (layer "F.Cu")
    (tedit 5A64794F) (tstamp ea965e5c-39ea-46d1-9fa3-7e2b350042d2)
    (at 49.6 48.2)
    (descr "SMD Solder Jumper, 1x1.5mm Triangular Pads, 0.3mm gap, open")
    (tags "solder jumper open")
    (property "Sheetfile" "sensors.kicad_sch")
    (property "Sheetname" "")
    (path "/dbf8af5d-2868-4d31-9fc8-cb6463f97d6f")
    (attr exclude_from_pos_files)
    (fp_text reference "JP7" (at 0 -1.8) (layer "F.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp f1476288-0651-42ef-b25f-edbda07282a8)
    )
    (fp_text value "0" (at 2.2 0 180) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 9f8a8fe7-247a-4d72-a60b-393b6124dbd8)
    )
    (fp_line (start -1.4 1) (end -1.4 -1) (layer "F.SilkS") (width 0.12) (tstamp 4614f9b8-d909-4a81-a815-a7f310cd9060))
    (fp_line (start -1.4 -1) (end 1.4 -1) (layer "F.SilkS") (width 0.12) (tstamp a03019ab-2649-4f6c-a558-360aa89a7b83))
    (fp_line (start 1.4 -1) (end 1.4 1) (layer "F.SilkS") (width 0.12) (tstamp c3cace4d-c525-49d8-9bb2-4f89a99e73e8))
    (fp_line (start 1.4 1) (end -1.4 1) (layer "F.SilkS") (width 0.12) (tstamp d4c384b5-613c-491c-89a2-04266af400da))
    (fp_line (start -1.65 -1.25) (end 1.65 -1.25) (layer "F.CrtYd") (width 0.05) (tstamp 1dc8d23c-5dd6-4df1-8c30-39469751fb5a))
    (fp_line (start -1.65 -1.25) (end -1.65 1.25) (layer "F.CrtYd") (width 0.05) (tstamp 2444a679-806c-4277-87b4-00b0b78958a3))
    (fp_line (start 1.65 1.25) (end -1.65 1.25) (layer "F.CrtYd") (width 0.05) (tstamp 2692e2a1-555b-4c5b-99a6-ae06ab7d76ea))
    (fp_line (start 1.65 1.25) (end 1.65 -1.25) (layer "F.CrtYd") (width 0.05) (tstamp 2beb4f29-217b-411c-b412-92c9ba17a417))
    (pad "1" smd custom (at -0.725 0) (size 0.3 0.3) (layers "F.Cu" "F.Mask")
      (net 3 "/S5") (pinfunction "A") (pintype "passive") (zone_connect 2)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_poly (pts
            (xy 1 0)
            (xy 0.5 0.75)
            (xy -0.5 0.75)
            (xy -0.5 -0.75)
            (xy 0.5 -0.75)
          ) (width 0) (fill yes))
      ) (tstamp e1c616a1-8fdc-4819-b610-e263068f1a0e))
    (pad "2" smd custom (at 0.725 0) (size 0.3 0.3) (layers "F.Cu" "F.Mask")
      (net 5 "/Sa0") (pinfunction "B") (pintype "passive") (zone_connect 2)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_poly (pts
            (xy 0.5 0.75)
            (xy -0.65 0.75)
            (xy -0.15 0)
            (xy -0.65 -0.75)
            (xy 0.5 -0.75)
          ) (width 0) (fill yes))
      ) (tstamp 3027c3f1-e470-43c6-ab35-c24589c5d634))
  )

  (footprint "Jumper:SolderJumper-2_P1.3mm_Open_TrianglePad1.0x1.5mm" (layer "F.Cu")
    (tedit 5A64794F) (tstamp ecbbad83-6ede-4f3d-8db7-50dc8ab81418)
    (at 182.8 50.8)
    (descr "SMD Solder Jumper, 1x1.5mm Triangular Pads, 0.3mm gap, open")
    (tags "solder jumper open")
    (property "Sheetfile" "sensors.kicad_sch")
    (property "Sheetname" "")
    (path "/24636705-80a7-4124-baac-8a399a6655ef")
    (attr exclude_from_pos_files)
    (fp_text reference "JP2" (at 0 -1.8) (layer "F.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 0ca68b2f-5450-4eed-8350-3bd245d9ee87)
    )
    (fp_text value "2" (at 2.25 0) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 26991657-3549-4201-9258-99b15ae49879)
    )
    (fp_line (start 1.4 1) (end -1.4 1) (layer "F.SilkS") (width 0.12) (tstamp 908b2c4e-9cbe-4a52-8ef2-87bca9227772))
    (fp_line (start -1.4 1) (end -1.4 -1) (layer "F.SilkS") (width 0.12) (tstamp a7f482e0-6aaa-4610-b7e1-da5549dace9f))
    (fp_line (start 1.4 -1) (end 1.4 1) (layer "F.SilkS") (width 0.12) (tstamp bcffdf52-8ef5-4444-aba3-79da8b5826c9))
    (fp_line (start -1.4 -1) (end 1.4 -1) (layer "F.SilkS") (width 0.12) (tstamp d746187d-467d-4361-825f-6ceeaac1d5f3))
    (fp_line (start -1.65 -1.25) (end -1.65 1.25) (layer "F.CrtYd") (width 0.05) (tstamp 4db6981d-eecd-4e16-8672-8978da945371))
    (fp_line (start 1.65 1.25) (end 1.65 -1.25) (layer "F.CrtYd") (width 0.05) (tstamp 5eeadde4-fdd0-48e9-b08a-54f36ca50bdf))
    (fp_line (start 1.65 1.25) (end -1.65 1.25) (layer "F.CrtYd") (width 0.05) (tstamp 89508bcf-d8aa-4510-a999-b42502a8aff4))
    (fp_line (start -1.65 -1.25) (end 1.65 -1.25) (layer "F.CrtYd") (width 0.05) (tstamp b76f37b2-d981-4a89-b1cc-13f0f7181856))
    (pad "1" smd custom (at -0.725 0) (size 0.3 0.3) (layers "F.Cu" "F.Mask")
      (net 1 "/S1") (pinfunction "A") (pintype "passive") (zone_connect 2)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_poly (pts
            (xy 1 0)
            (xy 0.5 0.75)
            (xy -0.5 0.75)
            (xy -0.5 -0.75)
            (xy 0.5 -0.75)
          ) (width 0) (fill yes))
      ) (tstamp b800c22e-ad0c-4df6-b837-5d74993e9186))
    (pad "2" smd custom (at 0.725 0) (size 0.3 0.3) (layers "F.Cu" "F.Mask")
      (net 6 "/Sa2") (pinfunction "B") (pintype "passive") (zone_connect 2)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_poly (pts
            (xy 0.5 0.75)
            (xy -0.65 0.75)
            (xy -0.15 0)
            (xy -0.65 -0.75)
            (xy 0.5 -0.75)
          ) (width 0) (fill yes))
      ) (tstamp 38ce7aba-5800-4669-823b-f5fb5d89d93f))
  )

  (footprint "Jumper:SolderJumper-2_P1.3mm_Open_TrianglePad1.0x1.5mm" (layer "F.Cu")
    (tedit 5A64794F) (tstamp ef175744-c97f-451c-a305-e4cfc8a03662)
    (at 182.8 53.4)
    (descr "SMD Solder Jumper, 1x1.5mm Triangular Pads, 0.3mm gap, open")
    (tags "solder jumper open")
    (property "Sheetfile" "sensors.kicad_sch")
    (property "Sheetname" "")
    (path "/4e90159d-3533-4996-93b4-6e946359432e")
    (attr exclude_from_pos_files)
    (fp_text reference "JP3" (at 0 -1.8) (layer "F.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp aebc431e-8d70-450f-ac0f-adce3a231b9a)
    )
    (fp_text value "4" (at 2.225 -0.1) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 8bf18280-aabf-4517-a685-82e5341b386c)
    )
    (fp_line (start 1.4 1) (end -1.4 1) (layer "F.SilkS") (width 0.12) (tstamp 0e3d3419-b845-44c3-b5f4-28f1673a1580))
    (fp_line (start -1.4 -1) (end 1.4 -1) (layer "F.SilkS") (width 0.12) (tstamp 3987bee7-f189-4758-a30d-c3b3b2966521))
    (fp_line (start 1.4 -1) (end 1.4 1) (layer "F.SilkS") (width 0.12) (tstamp 5e5d7961-f37e-4993-8c22-1359c20673b9))
    (fp_line (start -1.4 1) (end -1.4 -1) (layer "F.SilkS") (width 0.12) (tstamp c3c1744d-7970-4b1c-8972-a3070632bf06))
    (fp_line (start -1.65 -1.25) (end -1.65 1.25) (layer "F.CrtYd") (width 0.05) (tstamp 06ce9a0e-8d4b-4fbc-9b73-980f818dd3cb))
    (fp_line (start 1.65 1.25) (end 1.65 -1.25) (layer "F.CrtYd") (width 0.05) (tstamp 32f9473a-4d2d-4952-99be-5537ec79b2d3))
    (fp_line (start -1.65 -1.25) (end 1.65 -1.25) (layer "F.CrtYd") (width 0.05) (tstamp 392c2aa7-8c3a-4ab3-a7b2-eac2f687b50e))
    (fp_line (start 1.65 1.25) (end -1.65 1.25) (layer "F.CrtYd") (width 0.05) (tstamp 794f4674-f76f-4880-b991-41b362ba5666))
    (pad "1" smd custom (at -0.725 0) (size 0.3 0.3) (layers "F.Cu" "F.Mask")
      (net 1 "/S1") (pinfunction "A") (pintype "passive") (zone_connect 2)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_poly (pts
            (xy 1 0)
            (xy 0.5 0.75)
            (xy -0.5 0.75)
            (xy -0.5 -0.75)
            (xy 0.5 -0.75)
          ) (width 0) (fill yes))
      ) (tstamp 7ddebb8a-0be3-4acc-a3dc-7d944fe7b604))
    (pad "2" smd custom (at 0.725 0) (size 0.3 0.3) (layers "F.Cu" "F.Mask")
      (net 7 "/Sa4") (pinfunction "B") (pintype "passive") (zone_connect 2)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_poly (pts
            (xy 0.5 0.75)
            (xy -0.65 0.75)
            (xy -0.15 0)
            (xy -0.65 -0.75)
            (xy 0.5 -0.75)
          ) (width 0) (fill yes))
      ) (tstamp c72cbd24-a0a4-4987-b904-0e7d2490334d))
  )

  (footprint "Connector_PinSocket_2.00mm:PinSocket_1x02_P2.00mm_Vertical" (layer "F.Cu")
    (tedit 5A19A42F) (tstamp ef181e38-c018-4429-b5ce-9c7512bbebfa)
    (at 112.73 49.8)
    (descr "Through hole straight socket strip, 1x02, 2.00mm pitch, single row (from Kicad 4.0.7), script generated")
    (tags "Through hole socket strip THT 1x02 2.00mm single row")
    (property "Sheetfile" "sensors.kicad_sch")
    (property "Sheetname" "")
    (path "/e930f7f7-be78-4520-99ca-cbb7c5f0aecf")
    (attr through_hole)
    (fp_text reference "TH4" (at 0 -2.5) (layer "F.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp ebd3409b-6d59-44eb-b45f-bae76df28ae3)
    )
    (fp_text value "PT1000" (at 0 4.5) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp f12e363d-66f4-49b2-bc6a-4fe8b7a2c4ac)
    )
    (fp_text user "${REFERENCE}" (at 0 1 90) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp d7253882-1b67-40ac-aa27-ce6a9b01031c)
    )
    (fp_line (start -1.06 3.06) (end 1.06 3.06) (layer "F.SilkS") (width 0.12) (tstamp 2f291af2-9eb1-41d5-989e-378303606cb7))
    (fp_line (start 1.06 1) (end 1.06 3.06) (layer "F.SilkS") (width 0.12) (tstamp 47b01fbd-f17b-4c66-841a-6006dc5ef3c0))
    (fp_line (start 1.06 -1.06) (end 1.06 0) (layer "F.SilkS") (width 0.12) (tstamp 70175b0a-be43-4dd7-9137-62fb9e3badfe))
    (fp_line (start 0 -1.06) (end 1.06 -1.06) (layer "F.SilkS") (width 0.12) (tstamp 9368eb7f-1edf-42f1-9578-747e7fa588c6))
    (fp_line (start -1.06 1) (end -1.06 3.06) (layer "F.SilkS") (width 0.12) (tstamp d211c5a4-d9a1-4746-9fac-fd522a044144))
    (fp_line (start -1.06 1) (end 1.06 1) (layer "F.SilkS") (width 0.12) (tstamp f9411e77-ad06-462e-8c3f-c1390d24c014))
    (fp_line (start -1.5 -1.5) (end 1.5 -1.5) (layer "F.CrtYd") (width 0.05) (tstamp 34667ddc-0dc0-4106-aace-94db75fa8fbd))
    (fp_line (start -1.5 3.5) (end -1.5 -1.5) (layer "F.CrtYd") (width 0.05) (tstamp 447ec32e-1564-4067-be3f-0cc652838403))
    (fp_line (start 1.5 -1.5) (end 1.5 3.5) (layer "F.CrtYd") (width 0.05) (tstamp a88431da-bdce-4e23-998f-35ee8034f388))
    (fp_line (start 1.5 3.5) (end -1.5 3.5) (layer "F.CrtYd") (width 0.05) (tstamp e1f292bc-8832-4580-bd89-01348ceb78ac))
    (fp_line (start 0.5 -1) (end 1 -0.5) (layer "F.Fab") (width 0.1) (tstamp 069d83ad-0fb2-4043-8de4-4ed24c3686d2))
    (fp_line (start -1 -1) (end 0.5 -1) (layer "F.Fab") (width 0.1) (tstamp 0c2c5d55-5104-4c7a-8fd8-035d30bcbf77))
    (fp_line (start 1 -0.5) (end 1 3) (layer "F.Fab") (width 0.1) (tstamp 3a788853-a678-4156-b482-57a51288bd70))
    (fp_line (start -1 3) (end -1 -1) (layer "F.Fab") (width 0.1) (tstamp 987aa555-6bf9-4885-82a5-78cafaffd786))
    (fp_line (start 1 3) (end -1 3) (layer "F.Fab") (width 0.1) (tstamp f8909ae0-eec2-4e73-8a80-b3606d389bb3))
    (pad "1" thru_hole rect (at 0 0) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 "GND") (pintype "passive") (tstamp ce8a3b02-8179-4986-9bbc-77b66b96876d))
    (pad "2" thru_hole oval (at 0 2) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "/S3") (pintype "passive") (tstamp 133b2ba8-ef0a-4d41-9db4-96b53fcd8de8))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinSocket_2.00mm.3dshapes/PinSocket_1x02_P2.00mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "MountingHole:MountingHole_2mm" (layer "F.Cu")
    (tedit 5B924920) (tstamp f42e3e35-2a94-4c6e-a5f4-e3b954b6a34d)
    (at 32.07 43.8)
    (descr "Mounting Hole 2mm, no annular")
    (tags "mounting hole 2mm no annular")
    (property "Sheetfile" "sensors.kicad_sch")
    (property "Sheetname" "")
    (path "/df93f598-22b2-427e-bf55-35c5f913b5a2")
    (attr exclude_from_pos_files)
    (fp_text reference "H2" (at 0 -3.2) (layer "F.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 44e5694a-15af-41c7-803a-dfd8a8166a75)
    )
    (fp_text value "MountingHole" (at 0 3.1) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 8b37242a-5a4b-4e1a-9e12-434c36d9683c)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 4219b606-6029-4f18-be40-717208d3dee4)
    )
    (fp_circle (center 0 0) (end 2 0) (layer "Cmts.User") (width 0.15) (fill none) (tstamp 5851a64a-d1b4-4185-834b-7edde18a004c))
    (fp_circle (center 0 0) (end 2.25 0) (layer "F.CrtYd") (width 0.05) (fill none) (tstamp 32107452-e2c8-43f6-9a03-5612f4df0291))
    (pad "" np_thru_hole circle (at 0 0) (size 2 2) (drill 2) (layers *.Cu *.Mask) (tstamp 56f0268b-fb71-431d-b677-b9bc9be60ac2))
  )

  (footprint "Connector_PinHeader_2.00mm:PinHeader_1x07_P2.00mm_Vertical" (layer "F.Cu")
    (tedit 59FED667) (tstamp fc7c80d3-9b86-4f2f-8dc4-ac098672dce8)
    (at 36 44.8)
    (descr "Through hole straight pin header, 1x07, 2.00mm pitch, single row")
    (tags "Through hole pin header THT 1x07 2.00mm single row")
    (property "Sheetfile" "sensors.kicad_sch")
    (property "Sheetname" "")
    (path "/91a07226-6cc4-4fe7-b3ca-9c5341507169")
    (attr through_hole)
    (fp_text reference "J2" (at 0 -2.06) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 8132128e-c953-4ba4-bee3-234e04f05ae6)
    )
    (fp_text value "Conn_01x08" (at 0 14.06) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp a7ce7c95-9c44-4273-b96d-8eef1e87a9df)
    )
    (fp_text user "${REFERENCE}" (at 0 6 90) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp c5792476-68f3-42a4-adf2-ea3458ff0872)
    )
    (fp_line (start -1.06 0) (end -1.06 -1.06) (layer "F.SilkS") (width 0.12) (tstamp 017256d9-6651-4f85-a502-135f6d3a8301))
    (fp_line (start -1.06 1) (end -1.06 13.06) (layer "F.SilkS") (width 0.12) (tstamp 03a0936c-0d0b-4d64-99f5-f902fe066caa))
    (fp_line (start 1.06 1) (end 1.06 13.06) (layer "F.SilkS") (width 0.12) (tstamp 2ea4b5eb-3165-4159-8c05-ee29384dc885))
    (fp_line (start -1.06 13.06) (end 1.06 13.06) (layer "F.SilkS") (width 0.12) (tstamp 3064d8d1-9998-44b7-a684-06b407da8f4b))
    (fp_line (start -1.06 -1.06) (end 0 -1.06) (layer "F.SilkS") (width 0.12) (tstamp 4570730f-f7bd-45ad-a2b7-d679726f0ed7))
    (fp_line (start -1.06 1) (end 1.06 1) (layer "F.SilkS") (width 0.12) (tstamp f5755b52-3b66-4806-94b5-9ade2d039713))
    (fp_line (start 1.5 13.5) (end 1.5 -1.5) (layer "F.CrtYd") (width 0.05) (tstamp 2721bd01-5e1b-4a47-93e4-b18f009fbcf0))
    (fp_line (start 1.5 -1.5) (end -1.5 -1.5) (layer "F.CrtYd") (width 0.05) (tstamp 2f975306-8b69-4740-b3b5-22476d4918c0))
    (fp_line (start -1.5 13.5) (end 1.5 13.5) (layer "F.CrtYd") (width 0.05) (tstamp 440b882c-12cb-4e87-83c5-a01d988a85d5))
    (fp_line (start -1.5 -1.5) (end -1.5 13.5) (layer "F.CrtYd") (width 0.05) (tstamp beb6be08-a61c-48e7-b0e6-69cc2386333b))
    (fp_line (start -1 13) (end -1 -0.5) (layer "F.Fab") (width 0.1) (tstamp 366bb5f0-5d19-49d6-9294-a2ebaf4e81ce))
    (fp_line (start -0.5 -1) (end 1 -1) (layer "F.Fab") (width 0.1) (tstamp 504d2814-cf36-4bb7-acd4-64054f03460b))
    (fp_line (start 1 -1) (end 1 13) (layer "F.Fab") (width 0.1) (tstamp 51bcf966-b520-40d0-a939-30725ecaeddb))
    (fp_line (start -1 -0.5) (end -0.5 -1) (layer "F.Fab") (width 0.1) (tstamp 5e7cf0f2-ed13-44ce-8033-1937d0f60f6a))
    (fp_line (start 1 13) (end -1 13) (layer "F.Fab") (width 0.1) (tstamp a37153fb-d387-4f38-ab84-3b7aed7526ec))
    (pad "1" thru_hole rect (at 0 0) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 "GND") (pinfunction "Pin_1") (pintype "passive") (tstamp 76da25df-be9e-4c14-9729-267c6b6faff6))
    (pad "2" thru_hole oval (at 0 2) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 9 "/Sa1") (pinfunction "Pin_2") (pintype "passive") (tstamp e7bc868b-e485-4baf-8eef-bc585a33abcc))
    (pad "3" thru_hole oval (at 0 4) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 "/Sa2") (pinfunction "Pin_3") (pintype "passive") (tstamp 816f8799-72e6-475e-be17-03b16474f7b7))
    (pad "4" thru_hole oval (at 0 6) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 10 "/Sa3") (pinfunction "Pin_4") (pintype "passive") (tstamp 932e2d7f-a391-4e21-8b2f-7059bb008315))
    (pad "5" thru_hole oval (at 0 8) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 "/Sa4") (pinfunction "Pin_5") (pintype "passive") (tstamp a221271c-631f-47ce-aade-0b54eca78cc7))
    (pad "6" thru_hole oval (at 0 10) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 11 "/Sa5") (pinfunction "Pin_6") (pintype "passive") (tstamp 293aba78-d79f-426b-8fd7-e573ba0c2da5))
    (pad "7" thru_hole oval (at 0 12) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 8 "/Sa6") (pinfunction "Pin_7") (pintype "passive") (tstamp 26c4c6c5-f319-48fc-82bc-ec06b1fa18bc))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.00mm.3dshapes/PinHeader_1x07_P2.00mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Connector_PinSocket_2.00mm:PinSocket_1x02_P2.00mm_Vertical" (layer "F.Cu")
    (tedit 5A19A42F) (tstamp fdca3422-4c4c-488f-9a43-bfe3fba9c81d)
    (at 179.39 49.8)
    (descr "Through hole straight socket strip, 1x02, 2.00mm pitch, single row (from Kicad 4.0.7), script generated")
    (tags "Through hole socket strip THT 1x02 2.00mm single row")
    (property "Sheetfile" "sensors.kicad_sch")
    (property "Sheetname" "")
    (path "/f279e4c3-7d51-4873-a499-e471cfbc1089")
    (attr through_hole)
    (fp_text reference "TH2" (at 0 -2.5) (layer "F.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp ab9b7199-9419-4d80-b269-d27bb64532ef)
    )
    (fp_text value "PT1000" (at 0 4.5) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 19bbdd64-9c80-4c27-bba8-cfe73e6324ab)
    )
    (fp_text user "${REFERENCE}" (at 0 1 90) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp af86b714-e4e4-4a62-ad9e-a8172d9547c5)
    )
    (fp_line (start -1.06 1) (end -1.06 3.06) (layer "F.SilkS") (width 0.12) (tstamp 01fa7e2b-d8d6-4962-8a7c-d302203127ae))
    (fp_line (start 1.06 1) (end 1.06 3.06) (layer "F.SilkS") (width 0.12) (tstamp 2712940a-139a-4109-a605-4c9c4fcab6aa))
    (fp_line (start 0 -1.06) (end 1.06 -1.06) (layer "F.SilkS") (width 0.12) (tstamp 5700e0ec-02cf-4d98-a19e-34022a4d4fab))
    (fp_line (start 1.06 -1.06) (end 1.06 0) (layer "F.SilkS") (width 0.12) (tstamp 68a9e698-3aa0-45ea-b72c-523f192f7912))
    (fp_line (start -1.06 1) (end 1.06 1) (layer "F.SilkS") (width 0.12) (tstamp 9470b782-c84f-4d11-8697-ed6614ea0db2))
    (fp_line (start -1.06 3.06) (end 1.06 3.06) (layer "F.SilkS") (width 0.12) (tstamp e8a7a047-dfec-4469-8412-0398dc7fb999))
    (fp_line (start -1.5 3.5) (end -1.5 -1.5) (layer "F.CrtYd") (width 0.05) (tstamp 7f642b0a-9401-40f8-9132-6d9f84d4d283))
    (fp_line (start 1.5 3.5) (end -1.5 3.5) (layer "F.CrtYd") (width 0.05) (tstamp 870348c9-ba79-4daa-be3a-d5b641bad105))
    (fp_line (start 1.5 -1.5) (end 1.5 3.5) (layer "F.CrtYd") (width 0.05) (tstamp b279d08b-fa04-42a6-a6e4-c91b8b7dd10c))
    (fp_line (start -1.5 -1.5) (end 1.5 -1.5) (layer "F.CrtYd") (width 0.05) (tstamp bdaa294c-4dc6-46b5-ba81-05f99700059c))
    (fp_line (start 1 3) (end -1 3) (layer "F.Fab") (width 0.1) (tstamp 0097205b-c8aa-4580-b61f-ae0f3d86b2ff))
    (fp_line (start -1 -1) (end 0.5 -1) (layer "F.Fab") (width 0.1) (tstamp 31836183-5e3a-4b4b-b7e3-c1c65b681c7a))
    (fp_line (start -1 3) (end -1 -1) (layer "F.Fab") (width 0.1) (tstamp 8903688d-2767-4d69-8aae-ac7b4a3bbfc6))
    (fp_line (start 1 -0.5) (end 1 3) (layer "F.Fab") (width 0.1) (tstamp 96799c22-5256-4c51-b67a-238ce9f4a4ec))
    (fp_line (start 0.5 -1) (end 1 -0.5) (layer "F.Fab") (width 0.1) (tstamp c7ffb6f4-91b2-4a66-b186-59f04dac565a))
    (pad "1" thru_hole rect (at 0 0) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 "GND") (pintype "passive") (tstamp 1c5627f4-06d9-4aa0-a26c-0af8ae4a1dda))
    (pad "2" thru_hole oval (at 0 2) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 "/S1") (pintype "passive") (tstamp c964ad3f-3fc3-4a27-94ff-b63f743d2ae4))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinSocket_2.00mm.3dshapes/PinSocket_1x02_P2.00mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (gr_circle (center 46.07 42.8) (end 46.57 42.8) (layer "Dwgs.User") (width 0.2) (fill none) (tstamp 0047f0c9-3b2c-4443-8afb-b2362e86442f))
  (gr_circle (center 209.57 50.8) (end 210.57 50.8) (layer "Dwgs.User") (width 0.2) (fill none) (tstamp 00894004-0bed-4e00-9387-c3670b4dbfbc))
  (gr_circle (center 112.73 58.8) (end 113.23 58.8) (layer "Dwgs.User") (width 0.2) (fill none) (tstamp 021252fc-87aa-4568-ab64-f6daeda8f1a1))
  (gr_circle (center 220.84 48.72455) (end 221.34 48.72455) (layer "Dwgs.User") (width 0.2) (fill none) (tstamp 09ac629f-19ab-44e2-9904-4a329c06094f))
  (gr_circle (center 179.39 42.8) (end 179.89 42.8) (layer "Dwgs.User") (width 0.2) (fill none) (tstamp 0b8a5046-61c7-45b4-98db-f797865f0113))
  (gr_circle (center 227.07 57.8) (end 228.07 57.8) (layer "Dwgs.User") (width 0.2) (fill none) (tstamp 1e960de3-12ce-4fc1-b09b-6c478419e1a5))
  (gr_circle (center 215.76 52.29776) (end 216.26 52.29776) (layer "Dwgs.User") (width 0.2) (fill none) (tstamp 2061e762-df9e-4f9d-aaa7-955826d6bdaf))
  (gr_line (start 146.06 42.8) (end 146.06 58.8) (layer "Dwgs.User") (width 0.13) (tstamp 2dde4e68-37ea-49e6-8fc1-521c1e7cb467))
  (gr_circle (center 212.72 42.8) (end 213.22 42.8) (layer "Dwgs.User") (width 0.2) (fill none) (tstamp 41e29983-3597-43de-b83c-fb444f45602d))
  (gr_circle (center 32.07 43.8) (end 33.07 43.8) (layer "Dwgs.User") (width 0.2) (fill none) (tstamp 46489458-cfad-474c-a600-638f8d2ec302))
  (gr_circle (center 219.57 43.3) (end 220.67 43.3) (layer "Dwgs.User") (width 0.2) (fill none) (tstamp 5ea9ffd7-f9ba-45b5-ad13-479b230bea8a))
  (gr_line (start 229.57 61.3) (end 29.57 61.3) (layer "Dwgs.User") (width 0.2) (tstamp 600f6659-add5-457f-879f-20e97955a6e9))
  (gr_circle (center 218.3 53.52324) (end 218.8 53.52324) (layer "Dwgs.User") (width 0.2) (fill none) (tstamp 609883f5-9a11-4a1f-aa88-f933ef9109bf))
  (gr_circle (center 218.3 50.8) (end 218.8 50.8) (layer "Dwgs.User") (width 0.2) (fill none) (tstamp 6a617ee0-518c-42bf-a6ae-e939e9d3e391))
  (gr_circle (center 220.84 50.8) (end 221.34 50.8) (layer "Dwgs.User") (width 0.2) (fill none) (tstamp 6e9cd428-49d3-40de-adb4-d43792452ae6))
  (gr_line (start 46.07 42.8) (end 46.07 58.8) (layer "Dwgs.User") (width 0.13) (tstamp 71f885c8-78fe-4703-b807-34974bae3876))
  (gr_line (start 212.72 42.8) (end 212.72 58.8) (layer "Dwgs.User") (width 0.13) (tstamp 7e0ba7fc-feb5-459e-a53b-f8b87bc8f072))
  (gr_circle (center 225.07 50.8) (end 225.62 50.8) (layer "Dwgs.User") (width 0.2) (fill none) (tstamp 7ec6c691-91b4-4eba-be9e-16d23d3aa9da))
  (gr_circle (center 227.07 43.8) (end 228.07 43.8) (layer "Dwgs.User") (width 0.2) (fill none) (tstamp 7fb259cf-5e06-4ca8-b332-d6d9f170db05))
  (gr_line (start 29.57 50.8) (end 229.57 50.8) (layer "Dwgs.User") (width 0.13) (tstamp 8d1fc0c3-b66c-4813-bd13-925b3edcccc1))
  (gr_line (start 229.57 40.3) (end 229.57 61.3) (layer "Dwgs.User") (width 0.2) (tstamp 94e3a8ea-72c5-4fbf-9bbc-f97c70918301))
  (gr_line (start 225.07 52.3) (end 225.07 49.3) (layer "Dwgs.User") (width 0.13) (tstamp 97dd3b74-3be0-4ff2-8ff5-470557f05d54))
  (gr_line (start 79.4 42.8) (end 79.4 58.8) (layer "Dwgs.User") (width 0.13) (tstamp 9b171ba1-8bc0-47d4-b532-6e59ee9b77fb))
  (gr_circle (center 79.4 42.8) (end 79.9 42.8) (layer "Dwgs.User") (width 0.2) (fill none) (tstamp 9e7faef0-4946-420e-bb26-0036e1923500))
  (gr_circle (center 219.57 58.3) (end 220.67 58.3) (layer "Dwgs.User") (width 0.2) (fill none) (tstamp 9eacb89c-59f2-4413-af4f-d6ebbe9ab969))
  (gr_circle (center 146.06 42.8) (end 146.56 42.8) (layer "Dwgs.User") (width 0.2) (fill none) (tstamp a1364d3b-2849-4615-a88c-e71077fe41dd))
  (gr_line (start 179.39 42.8) (end 179.39 58.8) (layer "Dwgs.User") (width 0.13) (tstamp a762787f-5b2d-4f23-bc5e-5db774e6d8a4))
  (gr_line (start 218.3 48.07676) (end 218.3 53.52324) (layer "Dwgs.User") (width 0.13) (tstamp b2a9ee71-5b5b-4c94-94c2-acc171f0c09f))
  (gr_circle (center 32.07 57.8) (end 33.07 57.8) (layer "Dwgs.User") (width 0.2) (fill none) (tstamp b60cc5b4-04de-4066-a50a-0c9f7f08aac4))
  (gr_line (start 112.73 42.8) (end 112.73 58.8) (layer "Dwgs.User") (width 0.13) (tstamp b728ad10-b421-48ee-bb8f-40b278bd5297))
  (gr_circle (center 109.57 50.8) (end 111.27 50.8) (layer "Dwgs.User") (width 0.2) (fill none) (tstamp b8edca37-9148-49eb-9006-1551558982e8))
  (gr_circle (center 46.07 58.8) (end 46.57 58.8) (layer "Dwgs.User") (width 0.2) (fill none) (tstamp b97b2ef9-c503-4dbc-a7b5-33fc6f674438))
  (gr_circle (center 215.76 49.30224) (end 216.26 49.30224) (layer "Dwgs.User") (width 0.2) (fill none) (tstamp bc4ff724-3128-494a-83cd-b609a4ab231c))
  (gr_circle (center 79.4 58.8) (end 79.9 58.8) (layer "Dwgs.User") (width 0.2) (fill none) (tstamp bd081d0f-76e8-4e05-9405-5fb583864f00))
  (gr_circle (center 218.3 48.07676) (end 218.8 48.07676) (layer "Dwgs.User") (width 0.2) (fill none) (tstamp c41bdfea-2191-4e7a-8fdc-7cde7612c3ce))
  (gr_circle (center 223.57 42.410911) (end 224.77 42.410911) (layer "Dwgs.User") (width 0.2) (fill none) (tstamp cb3c41c5-5070-45c8-bd9b-4179ad5af47a))
  (gr_circle (center 112.73 42.8) (end 113.23 42.8) (layer "Dwgs.User") (width 0.2) (fill none) (tstamp d2d82093-3866-4fa5-a13e-c20ec08c9d6e))
  (gr_circle (center 212.72 58.8) (end 213.22 58.8) (layer "Dwgs.User") (width 0.2) (fill none) (tstamp d8dfd1f2-4111-46c8-b0c5-2ab35b0f1777))
  (gr_line (start 29.57 61.3) (end 29.57 40.3) (layer "Dwgs.User") (width 0.2) (tstamp e048529c-f07c-45aa-9694-650430f67b8c))
  (gr_circle (center 223.57 59.189089) (end 224.77 59.189089) (layer "Dwgs.User") (width 0.2) (fill none) (tstamp e28a2d0a-51e9-4945-8a63-4b5b6f924421))
  (gr_circle (center 220.84 52.87545) (end 221.34 52.87545) (layer "Dwgs.User") (width 0.2) (fill none) (tstamp e750ed77-8733-4646-b481-016ae8f110eb))
  (gr_circle (center 149.57 50.8) (end 151.27 50.8) (layer "Dwgs.User") (width 0.2) (fill none) (tstamp e7767b6d-b4f3-4261-9d72-d04496b0742e))
  (gr_line (start 29.57 40.3) (end 229.57 40.3) (layer "Dwgs.User") (width 0.2) (tstamp ebb71dd9-bd81-42a6-b257-4f8c8146557d))
  (gr_circle (center 179.39 58.8) (end 179.89 58.8) (layer "Dwgs.User") (width 0.2) (fill none) (tstamp ee17a97b-a93a-4233-8464-8168bdc9c133))
  (gr_circle (center 146.06 58.8) (end 146.56 58.8) (layer "Dwgs.User") (width 0.2) (fill none) (tstamp f1e72335-b8e4-42e7-ad22-34fa0e6f5bb9))
  (gr_circle (center 189.57 50.8) (end 191.27 50.8) (layer "Dwgs.User") (width 0.2) (fill none) (tstamp f6155092-0719-4eff-aa79-c27b8b3956cc))
  (gr_circle (center 69.57 50.8) (end 71.27 50.8) (layer "Dwgs.User") (width 0.2) (fill none) (tstamp fbcd3696-1ea1-416d-802b-069a258fc679))
  (gr_rect (start 29.6 40.3) (end 229.6 61.3) (layer "Edge.Cuts") (width 0.1) (fill none) (tstamp 2357cfed-4acd-466a-8e2c-1d63ce38207e))
  (gr_text "0" (at 206.8 48.7) (layer "F.SilkS") (tstamp 012c58b2-168b-4d4f-bfd6-c11a1fb544ee)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (gr_text "1" (at 206.8 50.8) (layer "F.SilkS") (tstamp 02ddd4f4-12e7-48f0-8508-d0d094e146ac)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (gr_text "Long &\nshort" (at 45.2 55.1) (layer "F.SilkS") (tstamp 0600336a-d17c-4dda-a95a-2de7e77fd06b)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (gr_text "3" (at 203.9 48.1) (layer "F.SilkS") (tstamp 0c9740a9-cdb6-4225-91e8-cd56f352dd27)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (gr_text "1" (at 214.5 47.5) (layer "F.SilkS") (tstamp 1db7d033-54a9-4592-969d-86c583be260b)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (gr_text "Long &\nshort" (at 178.5 54.9) (layer "F.SilkS") (tstamp 2d21bf74-7c66-4c28-a872-0a8df3b9f6e0)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (gr_text "4" (at 203.9 53.5) (layer "F.SilkS") (tstamp 2e8fc93c-211b-4c87-9073-9487e5801a72)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (gr_text "Short" (at 146 53.9) (layer "F.SilkS") (tstamp 3256fdab-8d21-4555-b45e-2de4ab1a557a)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (gr_text "5" (at 81.4 47.6) (layer "F.SilkS") (tstamp 3afc3850-77e2-4b40-9d94-2289168e98bf)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (gr_text "6" (at 201.3 52.3) (layer "F.SilkS") (tstamp 42d0e37b-0f32-4ab4-8f11-d80c00c69977)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (gr_text "3" (at 148.2 47.8) (layer "F.SilkS") (tstamp 602ebd76-4b14-408f-b9cb-1ec9dd9462ac)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (gr_text "Short" (at 79.4 54) (layer "F.SilkS") (tstamp 76a1d35c-346f-4ecc-b805-4d9a9c74afec)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (gr_text "Short" (at 212.5 54.3) (layer "F.SilkS") (tstamp 78ce407f-b8eb-4ce2-94e3-17d108d1270c)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (gr_text "5" (at 201.3 49.3) (layer "F.SilkS") (tstamp 87d76963-689d-4baa-8110-a945323b4018)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (gr_text "2" (at 206.7 52.9) (layer "F.SilkS") (tstamp 9e6428c0-77b2-46e9-9f11-602fbbfc7ca6)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (gr_text "Long &\nshort" (at 112.2 55.1) (layer "F.SilkS") (tstamp c09ed9cd-074a-4454-ad7b-baf7ef937171)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (gr_text "Gnd" (at 203.8 50.8) (layer "F.SilkS") (tstamp d70c9649-4061-42a2-aca2-317bab406871)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (gr_text "Gnd\n1\n2\n3\n4\n5\n6" (at 38.2 50.8) (layer "F.SilkS") (tstamp ef549bc0-3570-4aad-9272-f93499939507)
    (effects (font (size 1.2 1.2) (thickness 0.2)) (justify left))
  )

  (segment (start 182.075 53.4) (end 182.075 48.2) (width 0.25) (layer "F.Cu") (net 1) (tstamp 621f3553-9c77-4a3f-85c3-89c68835ebe2))
  (segment (start 179.39 51.8) (end 181.075 51.8) (width 0.25) (layer "F.Cu") (net 1) (tstamp ade1be1d-88de-45dd-931d-b9a2a46baedc))
  (segment (start 181.075 51.8) (end 182.075 50.8) (width 0.25) (layer "F.Cu") (net 1) (tstamp d685d340-0747-4165-9c4d-7e4cad8117a7))
  (segment (start 114.675 51.8) (end 115.675 50.8) (width 0.25) (layer "F.Cu") (net 2) (tstamp 817992ff-cd86-470c-942f-d8a956d50c19))
  (segment (start 112.73 51.8) (end 114.675 51.8) (width 0.25) (layer "F.Cu") (net 2) (tstamp c722d46a-198a-4ffa-8bb2-c56642dd1556))
  (segment (start 115.675 53.4) (end 115.675 48.2) (width 0.25) (layer "F.Cu") (net 2) (tstamp e76424c3-9975-4a9d-9e56-1560c9849ee9))
  (segment (start 46.07 51.8) (end 47.875 51.8) (width 0.25) (layer "F.Cu") (net 3) (tstamp 00c2bd22-718b-4636-8c49-9ce75c3ae932))
  (segment (start 47.875 51.8) (end 48.875 50.8) (width 0.25) (layer "F.Cu") (net 3) (tstamp 12a5d7ae-1b69-4375-842a-ccea7bb4c5bc))
  (segment (start 48.875 53.4) (end 48.875 48.2) (width 0.25) (layer "F.Cu") (net 3) (tstamp 9ff67658-0de7-4523-9602-559b61564b58))
  (segment (start 146.06 49.8) (end 146.06 43.84) (width 0.25) (layer "F.Cu") (net 4) (tstamp 0d5155dd-d927-4859-8812-da4a5a64287b))
  (segment (start 146.06 43.84) (end 146.1 43.8) (width 0.25) (layer "F.Cu") (net 4) (tstamp 37b6ae06-6bcb-4de3-93fe-2aabaf6d9dc7))
  (segment (start 179.39 49.8) (end 179.39 43.81) (width 0.25) (layer "F.Cu") (net 4) (tstamp 3af7ee74-ae1d-400f-b7a4-c4a03e7b5ca7))
  (segment (start 79.4 49.8) (end 79.4 43.8) (width 0.25) (layer "F.Cu") (net 4) (tstamp 456764d3-2f20-4e4e-844c-ea2a12c1a683))
  (segment (start 46.07 49.8) (end 46.07 43.83) (width 0.25) (layer "F.Cu") (net 4) (tstamp 71c27af5-1fb4-4cef-8e1e-c4e8e3ca89ce))
  (segment (start 179.39 43.81) (end 179.4 43.8) (width 0.25) (layer "F.Cu") (net 4) (tstamp 9bd9c4d9-8e69-4f52-bd3d-755e53e30cbb))
  (segment (start 112.73 49.8) (end 112.73 43.83) (width 0.25) (layer "F.Cu") (net 4) (tstamp b99c1024-f3da-446d-91d1-9ff498e9a11d))
  (segment (start 212.72 43.82) (end 212.7 43.8) (width 0.25) (layer "F.Cu") (net 4) (tstamp c10d9af0-2ca0-4cb5-b2c5-8ff7df42d7e7))
  (segment (start 212.72 49.8) (end 212.72 43.82) (width 0.25) (layer "F.Cu") (net 4) (tstamp c4113362-3f6e-49ed-b2f4-73e177494631))
  (segment (start 112.73 43.83) (end 112.7 43.8) (width 0.25) (layer "F.Cu") (net 4) (tstamp cba4927e-6861-4b6b-9fbf-df81f65512a3))
  (segment (start 46.07 43.83) (end 46.1 43.8) (width 0.25) (layer "F.Cu") (net 4) (tstamp f5d27585-f5c1-4e98-9b11-ebe4d274c2a2))
  (via (at 212.7 43.8) (size 0.8) (drill 0.4) (layers "F.Cu" "B.Cu") (net 4) (tstamp 3484e8f1-3331-4891-8a35-597facdc3d19))
  (via (at 146.1 43.8) (size 0.8) (drill 0.4) (layers "F.Cu" "B.Cu") (net 4) (tstamp 503498fc-1f44-427f-bebd-d6695c607698))
  (via (at 46.1 43.8) (size 0.8) (drill 0.4) (layers "F.Cu" "B.Cu") (net 4) (tstamp 764db7e7-1026-4205-8a76-1a0c6790b3ad))
  (via (at 112.7 43.8) (size 0.8) (drill 0.4) (layers "F.Cu" "B.Cu") (net 4) (tstamp cbc702ad-fbe2-405d-8d73-c8ea7371bf0f))
  (via (at 179.4 43.8) (size 0.8) (drill 0.4) (layers "F.Cu" "B.Cu") (net 4) (tstamp de60e938-f206-4dbd-a73b-92f4677e8035))
  (via (at 79.4 43.8) (size 0.8) (drill 0.4) (layers "F.Cu" "B.Cu") (net 4) (tstamp fd2709e7-6f86-4ec6-886e-203fc5363117))
  (segment (start 179.4 43.8) (end 212.143967 43.8) (width 0.25) (layer "B.Cu") (net 4) (tstamp 07a332e1-abb3-4231-a643-315913041984))
  (segment (start 215.3 43.8) (end 216.121984 44.621984) (width 0.25) (layer "B.Cu") (net 4) (tstamp 14a4e24f-6048-4637-9c7f-ae648ce51755))
  (segment (start 216.121984 47.778016) (end 218.3 49.956033) (width 0.25) (layer "B.Cu") (net 4) (tstamp 212a9701-b3fc-4a16-b6fc-1ee27533d115))
  (segment (start 112.7 43.8) (end 146.1 43.8) (width 0.25) (layer "B.Cu") (net 4) (tstamp 3f729551-86e7-4f32-91bb-ca6e9867e274))
  (segment (start 212.143967 43.8) (end 212.7 43.8) (width 0.25) (layer "B.Cu") (net 4) (tstamp 4181cb9c-a7ec-4c7b-9ac6-70b145078e99))
  (segment (start 36 44.8) (end 45.1 44.8) (width 0.25) (layer "B.Cu") (net 4) (tstamp 4a96f759-78ba-4e2b-b84b-b3c473746fe5))
  (segment (start 218.3 49.956033) (end 218.3 50.8) (width 0.25) (layer "B.Cu") (net 4) (tstamp 526a86f4-f4c0-45ee-9728-0856b0ddb24e))
  (segment (start 212.7 43.8) (end 215.3 43.8) (width 0.25) (layer "B.Cu") (net 4) (tstamp 7498e8fb-21a0-4a4e-a81a-0dc6e8c26c55))
  (segment (start 79.4 43.8) (end 112.7 43.8) (width 0.25) (layer "B.Cu") (net 4) (tstamp 82939fd9-84af-4abd-a233-fc9cf7b2f3d7))
  (segment (start 46.1 43.8) (end 79.4 43.8) (width 0.25) (layer "B.Cu") (net 4) (tstamp a5f86cbd-51ea-4aeb-9f2c-23365079a3d5))
  (segment (start 216.121984 44.621984) (end 216.121984 47.778016) (width 0.25) (layer "B.Cu") (net 4) (tstamp b191b0b1-4dbc-4e4a-ad2f-c408324b2f14))
  (segment (start 45.1 44.8) (end 46.1 43.8) (width 0.25) (layer "B.Cu") (net 4) (tstamp ef2a12ce-b3bc-44cc-a309-bcffb913bd01))
  (segment (start 146.1 43.8) (end 179.4 43.8) (width 0.25) (layer "B.Cu") (net 4) (tstamp f921edcb-b62e-4109-b761-1d8476232107))
  (segment (start 50.325 48.2) (end 50.4 48.125) (width 0.25) (layer "F.Cu") (net 5) (tstamp 475568bd-c8f1-45c6-bbd5-2b3b6b86d268))
  (segment (start 215.2 45.8) (end 220 45.8) (width 0.25) (layer "F.Cu") (net 5) (tstamp 6e9efd4b-d197-447e-852f-3813e73af3c1))
  (segment (start 220.84 46.64) (end 220.84 48.7172) (width 0.25) (layer "F.Cu") (net 5) (tstamp 714e41db-3a29-4419-b0bf-47795d87975a))
  (segment (start 50.4 48.125) (end 50.4 44.8) (width 0.25) (layer "F.Cu") (net 5) (tstamp 7fc3a8e1-da85-4a6f-867f-7a9fb5bcbff8))
  (segment (start 220 45.8) (end 220.84 46.64) (width 0.25) (layer "F.Cu") (net 5) (tstamp eb1de472-fc0c-4407-86f7-82f1454bea17))
  (via (at 50.4 44.8) (size 0.8) (drill 0.4) (layers "F.Cu" "B.Cu") (net 5) (tstamp d119fd66-d8c6-433f-b368-279e730820e7))
  (via (at 215.2 45.8) (size 0.8) (drill 0.4) (layers "F.Cu" "B.Cu") (net 5) (tstamp f1cc4edf-fdc5-4ec3-99f9-6de504c97f2b))
  (segment (start 50.4 44.8) (end 214.2 44.8) (width 0.25) (layer "B.Cu") (net 5) (tstamp 4eebaf53-a4fb-4023-85a5-dbca05f8778e))
  (segment (start 214.2 44.8) (end 215.2 45.8) (width 0.25) (layer "B.Cu") (net 5) (tstamp 654d2e58-f2a9-48b0-935d-b1cf606abf5e))
  (segment (start 118.525 46.8) (end 119.4 46.8) (width 0.25) (layer "F.Cu") (net 6) (tstamp 3abb73d8-73be-4de2-bd83-24b2edb31917))
  (segment (start 183.525 50.8) (end 184.4 50.8) (width 0.25) (layer "F.Cu") (net 6) (tstamp 82297d68-b230-4caf-a25c-d08016fb8c6d))
  (segment (start 185.6 49.6) (end 185.6 46.8) (width 0.25) (layer "F.Cu") (net 6) (tstamp bdbea0e1-82bc-41c3-8bf1-645e1f3e5c08))
  (segment (start 184.4 50.8) (end 185.6 49.6) (width 0.25) (layer "F.Cu") (net 6) (tstamp d12af640-c520-45f4-852b-0f5b26d6d1f6))
  (segment (start 117.125 48.2) (end 118.525 46.8) (width 0.25) (layer "F.Cu") (net 6) (tstamp e5648e05-f104-4d85-88eb-019f8c36de79))
  (via (at 119.4 46.8) (size 0.8) (drill 0.4) (layers "F.Cu" "B.Cu") (net 6) (tstamp 22204270-f171-4c3c-9ca6-b3799d6ced11))
  (via (at 185.6 46.8) (size 0.8) (drill 0.4) (layers "F.Cu" "B.Cu") (net 6) (tstamp 6a4088da-14ee-416a-8725-f4bf10648d92))
  (segment (start 214.3 49.715233) (end 215.558367 50.9736) (width 0.25) (layer "B.Cu") (net 6) (tstamp 0eb812f2-3d38-4a62-b4b3-5e1faa277359))
  (segment (start 38.2 48.8) (end 40.2 46.8) (width 0.25) (layer "B.Cu") (net 6) (tstamp 2bd3405d-b592-480c-9748-c222514f3519))
  (segment (start 217.751167 52.125) (end 220.0822 52.125) (width 0.25) (layer "B.Cu") (net 6) (tstamp 3c9ba630-b7ca-4869-a57c-6ba8807e5871))
  (segment (start 214.3 47.6) (end 214.3 49.715233) (width 0.25) (layer "B.Cu") (net 6) (tstamp 3fa78abd-05e1-4d73-8f6b-724757a7605c))
  (segment (start 119.4 46.8) (end 185.6 46.8) (width 0.25) (layer "B.Cu") (net 6) (tstamp 4c91c76b-2f24-4394-8095-914e8badbfee))
  (segment (start 185.6 46.8) (end 213.5 46.8) (width 0.25) (layer "B.Cu") (net 6) (tstamp 73d83fbe-3da8-47f6-89e3-08465bcabd70))
  (segment (start 36 48.8) (end 38.2 48.8) (width 0.25) (layer "B.Cu") (net 6) (tstamp 93a4ea81-dad0-4515-8028-e5366240e7da))
  (segment (start 215.558367 50.9736) (end 216.599767 50.9736) (width 0.25) (layer "B.Cu") (net 6) (tstamp aa391d47-2b4a-4168-b338-54b26ecaf3a9))
  (segment (start 40.2 46.8) (end 119.4 46.8) (width 0.25) (layer "B.Cu") (net 6) (tstamp dca23837-bc55-4f04-9db8-7c29307a8cca))
  (segment (start 213.5 46.8) (end 214.3 47.6) (width 0.25) (layer "B.Cu") (net 6) (tstamp ef0a0f09-939a-44bc-9eb9-5102a9142e9f))
  (segment (start 220.0822 52.125) (end 220.84 52.8828) (width 0.25) (layer "B.Cu") (net 6) (tstamp f689b417-f943-48b9-8f12-3a1c1f19eb88))
  (segment (start 216.599767 50.9736) (end 217.751167 52.125) (width 0.25) (layer "B.Cu") (net 6) (tstamp ffc465db-bd5d-48e3-9ef9-c0ddcbb69044))
  (segment (start 216.6933 55.1245) (end 218.3 53.5178) (width 0.25) (layer "F.Cu") (net 7) (tstamp 8e3df2cb-7903-437d-a20a-8a005318cd9f))
  (segment (start 183.525 55.725) (end 183.6 55.8) (width 0.25) (layer "F.Cu") (net 7) (tstamp 97f414eb-f6cc-4ebb-845f-8d9715d5b1cf))
  (segment (start 118 50.8) (end 119.6 52.4) (width 0.25) (layer "F.Cu") (net 7) (tstamp af63d7d4-97ad-4bff-b6ae-ea9ef560029c))
  (segment (start 183.525 53.4) (end 183.525 55.725) (width 0.25) (layer "F.Cu") (net 7) (tstamp ca91af6a-6778-43c9-b400-ce9310828874))
  (segment (start 119.6 52.4) (end 119.6 55.8) (width 0.25) (layer "F.Cu") (net 7) (tstamp cfbc1aca-2c52-4e20-80e1-6af58486e490))
  (segment (start 216 55.1245) (end 216.6933 55.1245) (width 0.25) (layer "F.Cu") (net 7) (tstamp e533b060-aa5f-4fd9-8665-c9e82107135d))
  (segment (start 117.125 50.8) (end 118 50.8) (width 0.25) (layer "F.Cu") (net 7) (tstamp f92693b0-e7b5-4b15-b751-ae368eef6790))
  (via (at 183.6 55.8) (size 0.8) (drill 0.4) (layers "F.Cu" "B.Cu") (net 7) (tstamp 8fa51c4d-ed9f-413d-95dd-e0833e1594ef))
  (via (at 119.6 55.8) (size 0.8) (drill 0.4) (layers "F.Cu" "B.Cu") (net 7) (tstamp dbff6e36-852f-4d1b-bf48-62de069e454a))
  (via (at 216 55.1245) (size 0.8) (drill 0.4) (layers "F.Cu" "B.Cu") (net 7) (tstamp f78e2241-4a71-4e45-b641-e63e11805293))
  (segment (start 40 55.8) (end 119.6 55.8) (width 0.25) (layer "B.Cu") (net 7) (tstamp 2a5d8c52-f6ba-4092-ab6e-a8a7a4343032))
  (segment (start 36 52.8) (end 39 55.8) (width 0.25) (layer "B.Cu") (net 7) (tstamp 348577b3-c60b-4e23-bfdb-6401683de951))
  (segment (start 39 55.8) (end 40 55.8) (width 0.25) (layer "B.Cu") (net 7) (tstamp 48a47ab0-82c1-45ad-9ab1-25aadb0d66c3))
  (segment (start 211.8 55.8) (end 212.5 55.1) (width 0.25) (layer "B.Cu") (net 7) (tstamp 50b27649-87c8-402a-bb53-113f479ba2aa))
  (segment (start 183.6 55.8) (end 211.8 55.8) (width 0.25) (layer "B.Cu") (net 7) (tstamp 6f4f4a5b-67bc-4476-97be-18782bc6effc))
  (segment (start 119.6 55.8) (end 183.6 55.8) (width 0.25) (layer "B.Cu") (net 7) (tstamp 7aa47b23-6af9-4ea3-bdba-65c6a24944f4))
  (segment (start 212.5 55.1) (end 215.9755 55.1) (width 0.25) (layer "B.Cu") (net 7) (tstamp 97e6cade-e032-45ca-82b7-d06a50fc24ab))
  (segment (start 215.9755 55.1) (end 216 55.1245) (width 0.25) (layer "B.Cu") (net 7) (tstamp a092f7c7-e180-46c7-a955-0459cce85f3e))
  (segment (start 39.2 55.8) (end 40 55.8) (width 0.25) (layer "B.Cu") (net 7) (tstamp c7711ede-8268-46a7-8c2b-92d8bd6ca124))
  (segment (start 214.9 53.1586) (end 214.9 56) (width 0.25) (layer "F.Cu") (net 8) (tstamp 1581eb95-fc8e-4428-ad03-08b1e8d8e57e))
  (segment (start 50.325 57.675) (end 50.2 57.8) (width 0.25) (layer "F.Cu") (net 8) (tstamp 523248b8-d5ed-42be-ad92-94f48534bdba))
  (segment (start 50.325 53.4) (end 50.325 57.675) (width 0.25) (layer "F.Cu") (net 8) (tstamp 81ac8394-e44b-4804-99a2-81772d431e83))
  (segment (start 215.76 52.2986) (end 214.9 53.1586) (width 0.25) (layer "F.Cu") (net 8) (tstamp e9ec6c4d-cfc5-4467-9637-508e5fc12679))
  (via (at 50.2 57.8) (size 0.8) (drill 0.4) (layers "F.Cu" "B.Cu") (net 8) (tstamp 79e48c0f-f666-4d35-895a-1bfb456f3ea9))
  (via (at 214.9 56) (size 0.8) (drill 0.4) (layers "F.Cu" "B.Cu") (net 8) (tstamp e8e046ae-f125-4bca-9138-5637482e6ce4))
  (segment (start 37 57.8) (end 50.2 57.8) (width 0.25) (layer "B.Cu") (net 8) (tstamp 03e0183c-94d1-41d1-a60b-588491a40d52))
  (segment (start 214.9 56.8) (end 214.9 56) (width 0.25) (layer "B.Cu") (net 8) (tstamp 365c7414-ee3f-4b38-8e22-83ee9bf05a4c))
  (segment (start 50.2 57.8) (end 209.1 57.8) (width 0.25) (layer "B.Cu") (net 8) (tstamp 624eebcd-7a44-461c-84cb-0ad5932fdc19))
  (segment (start 209.1 57.8) (end 213.9 57.8) (width 0.25) (layer "B.Cu") (net 8) (tstamp 98ff784a-bff1-4f2d-91c7-8092cad6e05e))
  (segment (start 36 56.8) (end 37 57.8) (width 0.25) (layer "B.Cu") (net 8) (tstamp a13b6309-9ae0-4a65-b4df-c20c62b1d7c8))
  (segment (start 213.9 57.8) (end 214.9 56.8) (width 0.25) (layer "B.Cu") (net 8) (tstamp e5b073fb-81a4-4f11-979b-69272e5c7b4b))
  (segment (start 212 51.8) (end 211.2 51) (width 0.25) (layer "F.Cu") (net 9) (tstamp 337f0e67-475e-4301-9de5-d1fe3f264fa6))
  (segment (start 217.807433 49.475) (end 219.515 49.475) (width 0.25) (layer "F.Cu") (net 9) (tstamp 460d098f-d737-4db4-b9c6-71ab435fb38a))
  (segment (start 219.515 49.475) (end 220.84 50.8) (width 0.25) (layer "F.Cu") (net 9) (tstamp 47a41e8e-ff53-44d8-9faa-5de762419fd5))
  (segment (start 211.2 51) (end 211.2 45.8) (width 0.25) (layer "F.Cu") (net 9) (tstamp 74d8b89b-fbe6-4bf3-bc55-1ca78aab4bf7))
  (segment (start 215.232433 46.9) (end 217.807433 49.475) (width 0.25) (layer "F.Cu") (net 9) (tstamp c1fc6218-0f69-4856-b2c9-f28d817afed2))
  (segment (start 215.2 46.9) (end 215.232433 46.9) (width 0.25) (layer "F.Cu") (net 9) (tstamp db6427d3-f247-4dcb-98c4-7977d47c3afe))
  (segment (start 212.72 51.8) (end 212 51.8) (width 0.25) (layer "F.Cu") (net 9) (tstamp e6169d70-99ef-421f-beb2-3047507e4fea))
  (segment (start 183.525 48.2) (end 183.525 45.875) (width 0.25) (layer "F.Cu") (net 9) (tstamp ed21281f-34c3-4bb1-81b4-acdd55c4ee8d))
  (segment (start 183.525 45.875) (end 183.6 45.8) (width 0.25) (layer "F.Cu") (net 9) (tstamp f71cfcd6-0f3a-4e82-9222-0e91405209a2))
  (via (at 183.6 45.8) (size 0.8) (drill 0.4) (layers "F.Cu" "B.Cu") (net 9) (tstamp dfaa1563-c208-4ceb-bf3a-c1f26f1cf318))
  (via (at 215.2 46.9) (size 0.8) (drill 0.4) (layers "F.Cu" "B.Cu") (net 9) (tstamp e7326ec3-20a2-46d9-b729-f99c37cacba8))
  (via (at 211.2 45.8) (size 0.8) (drill 0.4) (layers "F.Cu" "B.Cu") (net 9) (tstamp eece58ae-372d-4371-9f99-39eedff7e6ca))
  (segment (start 38.2 46.8) (end 39.2 45.8) (width 0.25) (layer "B.Cu") (net 9) (tstamp 06fedb2e-c1b3-4989-b8b3-a81c62f0ad02))
  (segment (start 36 46.8) (end 38.2 46.8) (width 0.25) (layer "B.Cu") (net 9) (tstamp 19851f00-57d7-4994-a449-80695d765cf2))
  (segment (start 39.2 45.8) (end 183.6 45.8) (width 0.25) (layer "B.Cu") (net 9) (tstamp 35f43e89-c703-4f2c-9963-9f4a09f7b369))
  (segment (start 211.2 45.8) (end 214.1 45.8) (width 0.25) (layer "B.Cu") (net 9) (tstamp 429c5610-90e2-47fb-ad86-2eff4b958c38))
  (segment (start 183.6 45.8) (end 211.2 45.8) (width 0.25) (layer "B.Cu") (net 9) (tstamp 618e2a3f-b9f1-4024-90d6-aaf1cb9e4e41))
  (segment (start 214.1 45.8) (end 215.2 46.9) (width 0.25) (layer "B.Cu") (net 9) (tstamp fee08a83-6ea2-4680-9d19-a0dfb705e0a5))
  (segment (start 51.8 50.8) (end 52.4 51.4) (width 0.25) (layer "F.Cu") (net 10) (tstamp 312bcfda-354d-4ee8-9350-8ef817ddf43d))
  (segment (start 50.325 50.8) (end 51.8 50.8) (width 0.25) (layer "F.Cu") (net 10) (tstamp 68c5308f-864a-4f0b-bb4f-48434b3c0d8a))
  (segment (start 146.06 51.8) (end 146.06 54.74) (width 0.25) (layer "F.Cu") (net 10) (tstamp af871609-48e6-403b-8537-45fdc8b71714))
  (segment (start 52.4 51.4) (end 52.4 54.8) (width 0.25) (layer "F.Cu") (net 10) (tstamp dc1a3ac1-0a19-454a-a5c1-38ca0abf0fd2))
  (segment (start 146.06 54.74) (end 146 54.8) (width 0.25) (layer "F.Cu") (net 10) (tstamp f4846183-6877-4459-b436-20cc4d9df3bd))
  (via (at 146 54.8) (size 0.8) (drill 0.4) (layers "F.Cu" "B.Cu") (net 10) (tstamp 5ee1b86c-7912-4cf1-a52c-d9d1b465d6ec))
  (via (at 52.4 54.8) (size 0.8) (drill 0.4) (layers "F.Cu" "B.Cu") (net 10) (tstamp 81701b6c-bafe-445f-9c90-4da99b179758))
  (segment (start 221.5 47.2) (end 222.5 48.2) (width 0.25) (layer "B.Cu") (net 10) (tstamp 11411458-e06d-4e2c-a419-ab03b1d845ad))
  (segment (start 40 54.8) (end 52.4 54.8) (width 0.25) (layer "B.Cu") (net 10) (tstamp 1635c8ca-afcc-4b8b-95f3-d1f9ea267c16))
  (segment (start 221.1 55) (end 217.3 55) (width 0.25) (layer "B.Cu") (net 10) (tstamp 2395aa27-29c7-4512-893c-2c0fcdd3000b))
  (segment (start 211.2 54.8) (end 146 54.8) (width 0.25) (layer "B.Cu") (net 10) (tstamp 3055c5b0-eb93-4aff-8e4d-b4b895b17d6b))
  (segment (start 222.5 48.2) (end 222.5 53.6) (width 0.25) (layer "B.Cu") (net 10) (tstamp 4727d44c-05dc-4a7a-907a-a9d2cc9f7687))
  (segment (start 36 50.8) (end 40 54.8) (width 0.25) (layer "B.Cu") (net 10) (tstamp 49aab7bd-b398-491d-b4d4-97afef179fd4))
  (segment (start 216.7 54.4) (end 211.6 54.4) (width 0.25) (layer "B.Cu") (net 10) (tstamp 5ae9b7a8-5963-4d44-93b1-bd9faf3eb337))
  (segment (start 222.5 53.6) (end 221.1 55) (width 0.25) (layer "B.Cu") (net 10) (tstamp 5cb6b7c6-71b0-45ed-9833-c80545314403))
  (segment (start 218.3 48.0822) (end 219.1822 47.2) (width 0.25) (layer "B.Cu") (net 10) (tstamp 69d2d7fc-64ba-4219-b0b9-2ded66d287d6))
  (segment (start 146 54.8) (end 52.4 54.8) (width 0.25) (layer "B.Cu") (net 10) (tstamp 6c033dd6-7403-4755-b5ff-acb03630d939))
  (segment (start 211.6 54.4) (end 211.2 54.8) (width 0.25) (layer "B.Cu") (net 10) (tstamp 8df052f4-f97b-4ae0-83f2-9bda305a79a1))
  (segment (start 217.3 55) (end 216.7 54.4) (width 0.25) (layer "B.Cu") (net 10) (tstamp f297f282-d2b4-41dd-87d9-bff5c9121f11))
  (segment (start 219.1822 47.2) (end 221.5 47.2) (width 0.25) (layer "B.Cu") (net 10) (tstamp fcb14149-6052-469a-869c-1abd7a3110da))
  (segment (start 213.2 55.8245) (end 213.2755 55.8245) (width 0.25) (layer "F.Cu") (net 11) (tstamp 0b2527a0-6267-4619-a0e5-fa6379407ef0))
  (segment (start 79.4 51.8) (end 79.4 56.8) (width 0.25) (layer "F.Cu") (net 11) (tstamp 2cbb4697-acf7-4a1d-af5d-87eea21b79bb))
  (segment (start 214.2 50.8614) (end 215.76 49.3014) (width 0.25) (layer "F.Cu") (net 11) (tstamp 351d9f46-f8b9-47bd-9916-00d37276f28f))
  (segment (start 214.2 54.9) (end 214.2 50.8614) (width 0.25) (layer "F.Cu") (net 11) (tstamp 435f4c49-4545-4b7f-bc24-0bb78e2e9080))
  (segment (start 213.2755 55.8245) (end 214.2 54.9) (width 0.25) (layer "F.Cu") (net 11) (tstamp 79b17162-bf6a-4ecc-894e-1d81779f90fd))
  (segment (start 117.125 53.4) (end 117 53.525) (width 0.25) (layer "F.Cu") (net 11) (tstamp 8665e1b9-b85a-4567-a5d6-3ed1ed6409db))
  (segment (start 117 53.525) (end 117 56.8) (width 0.25) (layer "F.Cu") (net 11) (tstamp 952a1bd3-fc95-488e-92f7-4845dda98802))
  (via (at 79.4 56.8) (size 0.8) (drill 0.4) (layers "F.Cu" "B.Cu") (net 11) (tstamp 2a648a38-814b-435d-bc9a-360b2a0b75e6))
  (via (at 213.2 55.8245) (size 0.8) (drill 0.4) (layers "F.Cu" "B.Cu") (net 11) (tstamp 851bd27c-5928-4668-9526-5145f86d3ec8))
  (via (at 117 56.8) (size 0.8) (drill 0.4) (layers "F.Cu" "B.Cu") (net 11) (tstamp b82194a9-3136-4551-ae61-e7611dc2ce0e))
  (segment (start 117 56.8) (end 212.2245 56.8) (width 0.25) (layer "B.Cu") (net 11) (tstamp 0bb9bace-9604-4a99-8311-53c290759ed3))
  (segment (start 79.4 56.8) (end 117 56.8) (width 0.25) (layer "B.Cu") (net 11) (tstamp 0d1ed058-8921-491a-b7e5-f90352184f42))
  (segment (start 38.7 56.8) (end 79.4 56.8) (width 0.25) (layer "B.Cu") (net 11) (tstamp 49a33a57-b9d1-4117-af70-a16fe3202cee))
  (segment (start 212.2245 56.8) (end 213.2 55.8245) (width 0.25) (layer "B.Cu") (net 11) (tstamp 5a91fabb-37fd-4000-aebc-7f4cb6dfb8f9))
  (segment (start 38 56.8) (end 38.7 56.8) (width 0.25) (layer "B.Cu") (net 11) (tstamp 5ab4677b-065a-4db6-aabd-affd6fceff58))
  (segment (start 36 54.8) (end 38 56.8) (width 0.25) (layer "B.Cu") (net 11) (tstamp afcf7f8e-aba1-48c9-ba5a-f43562b5bb64))

  (group "" (id 70967a14-c508-4b13-88c0-e35e8f224c6f)
    (members
      0047f0c9-3b2c-4443-8afb-b2362e86442f
      00894004-0bed-4e00-9387-c3670b4dbfbc
      021252fc-87aa-4568-ab64-f6daeda8f1a1
      09ac629f-19ab-44e2-9904-4a329c06094f
      0b8a5046-61c7-45b4-98db-f797865f0113
      1e960de3-12ce-4fc1-b09b-6c478419e1a5
      2061e762-df9e-4f9d-aaa7-955826d6bdaf
      2dde4e68-37ea-49e6-8fc1-521c1e7cb467
      41e29983-3597-43de-b83c-fb444f45602d
      46489458-cfad-474c-a600-638f8d2ec302
      5ea9ffd7-f9ba-45b5-ad13-479b230bea8a
      600f6659-add5-457f-879f-20e97955a6e9
      609883f5-9a11-4a1f-aa88-f933ef9109bf
      6a617ee0-518c-42bf-a6ae-e939e9d3e391
      6e9cd428-49d3-40de-adb4-d43792452ae6
      71f885c8-78fe-4703-b807-34974bae3876
      7e0ba7fc-feb5-459e-a53b-f8b87bc8f072
      7ec6c691-91b4-4eba-be9e-16d23d3aa9da
      7fb259cf-5e06-4ca8-b332-d6d9f170db05
      8d1fc0c3-b66c-4813-bd13-925b3edcccc1
      94e3a8ea-72c5-4fbf-9bbc-f97c70918301
      97dd3b74-3be0-4ff2-8ff5-470557f05d54
      9b171ba1-8bc0-47d4-b532-6e59ee9b77fb
      9e7faef0-4946-420e-bb26-0036e1923500
      9eacb89c-59f2-4413-af4f-d6ebbe9ab969
      a1364d3b-2849-4615-a88c-e71077fe41dd
      a762787f-5b2d-4f23-bc5e-5db774e6d8a4
      b2a9ee71-5b5b-4c94-94c2-acc171f0c09f
      b60cc5b4-04de-4066-a50a-0c9f7f08aac4
      b728ad10-b421-48ee-bb8f-40b278bd5297
      b8edca37-9148-49eb-9006-1551558982e8
      b97b2ef9-c503-4dbc-a7b5-33fc6f674438
      bc4ff724-3128-494a-83cd-b609a4ab231c
      bd081d0f-76e8-4e05-9405-5fb583864f00
      c41bdfea-2191-4e7a-8fdc-7cde7612c3ce
      cb3c41c5-5070-45c8-bd9b-4179ad5af47a
      d2d82093-3866-4fa5-a13e-c20ec08c9d6e
      d8dfd1f2-4111-46c8-b0c5-2ab35b0f1777
      e048529c-f07c-45aa-9694-650430f67b8c
      e28a2d0a-51e9-4945-8a63-4b5b6f924421
      e750ed77-8733-4646-b481-016ae8f110eb
      e7767b6d-b4f3-4261-9d72-d04496b0742e
      ebb71dd9-bd81-42a6-b257-4f8c8146557d
      ee17a97b-a93a-4233-8464-8168bdc9c133
      f1e72335-b8e4-42e7-ad22-34fa0e6f5bb9
      f6155092-0719-4eff-aa79-c27b8b3956cc
      fbcd3696-1ea1-416d-802b-069a258fc679
    )
  )
)
