(kicad_pcb (version 4) (host pcbnew 4.0.7)

  (general
    (links 17)
    (no_connects 0)
    (area 111.899999 37.06238 175.157143 83.985)
    (thickness 1.6)
    (drawings 13)
    (tracks 88)
    (zones 0)
    (modules 7)
    (nets 6)
  )

  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )

  (setup
    (last_trace_width 1)
    (user_trace_width 0.5)
    (user_trace_width 1)
    (user_trace_width 2)
    (trace_clearance 0.3)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 2)
    (via_drill 0.8)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (user_via 2 0.8)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x00000_00000001)
      (usegerberextensions false)
      (excludeedgelayer false)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative true)
      (psa4output false)
      (plotreference false)
      (plotvalue false)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 5)
      (mirror true)
      (drillshape 2)
      (scaleselection 1)
      (outputdirectory ""))
  )

  (net 0 "")
  (net 1 "Net-(J1-Pad1)")
  (net 2 "Net-(J1-Pad2)")
  (net 3 "Net-(J1-Pad3)")
  (net 4 "Net-(F1-Pad1)")
  (net 5 "Net-(F1-Pad2)")

  (net_class Default "This is the default net class."
    (clearance 0.3)
    (trace_width 0.5)
    (via_dia 2)
    (via_drill 0.8)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net "Net-(F1-Pad1)")
    (add_net "Net-(F1-Pad2)")
    (add_net "Net-(J1-Pad1)")
    (add_net "Net-(J1-Pad2)")
    (add_net "Net-(J1-Pad3)")
  )

  (module Connector_PinHeader_2.54mm.pretty:PinHeader_1x04_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC) (tstamp 5B68A033)
    (at 129.286 41.91 90)
    (descr "Through hole straight pin header, 1x04, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x04 2.54mm single row")
    (path /5B67E004)
    (fp_text reference J1 (at 0 -2.33 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value Conn_01x04 (at 0 9.95 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -0.635 -1.27) (end 1.27 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start 1.27 -1.27) (end 1.27 8.89) (layer F.Fab) (width 0.1))
    (fp_line (start 1.27 8.89) (end -1.27 8.89) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 8.89) (end -1.27 -0.635) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 -0.635) (end -0.635 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -1.33 8.95) (end 1.33 8.95) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.33 1.27) (end -1.33 8.95) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.33 1.27) (end 1.33 8.95) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.33 1.27) (end 1.33 1.27) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.33 0) (end -1.33 -1.33) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.33 -1.33) (end 0 -1.33) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.8 -1.8) (end -1.8 9.4) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 9.4) (end 1.8 9.4) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 9.4) (end 1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 -1.8) (end -1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 0 3.81 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "Net-(J1-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 "Net-(J1-Pad2)"))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 "Net-(J1-Pad3)"))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 "Net-(F1-Pad2)"))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x04_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module RJ45:RJ45 (layer F.Cu) (tedit 5AD06174) (tstamp 5B68A04F)
    (at 139.5 53.5)
    (descr "RJ45 connector, 8-pin")
    (tags RJ45)
    (path /5B67DE38)
    (fp_text reference J2 (at 3.25 -4.25) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value RJ45 (at 2.8 5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -6.25 -3.25) (end 12.25 -3.25) (layer F.CrtYd) (width 0.15))
    (fp_line (start 12.25 -3.25) (end 12.25 7.25) (layer F.CrtYd) (width 0.15))
    (fp_line (start 12.25 7.25) (end -6.25 7.25) (layer F.CrtYd) (width 0.15))
    (fp_line (start -6.25 7.25) (end -6.25 -3.25) (layer F.CrtYd) (width 0.15))
    (fp_line (start -5.8 6.8) (end 11.8 6.8) (layer F.Fab) (width 0.15))
    (fp_line (start 11.8 6.8) (end 11.8 -2.8) (layer F.Fab) (width 0.15))
    (fp_line (start 11.8 -2.8) (end -4.8 -2.8) (layer F.Fab) (width 0.15))
    (fp_line (start -4.8 -2.8) (end -5.8 -1.8) (layer F.Fab) (width 0.15))
    (fp_line (start -5.8 -1.8) (end -5.8 6.8) (layer F.Fab) (width 0.15))
    (fp_line (start -6 7) (end 12 7) (layer F.SilkS) (width 0.15))
    (fp_line (start 12 7) (end 12 -3) (layer F.SilkS) (width 0.15))
    (fp_line (start 12 -3) (end -6 -3) (layer F.SilkS) (width 0.15))
    (fp_line (start -6 -3) (end -6 7) (layer F.SilkS) (width 0.15))
    (fp_text user %R (at 3.25 -4.25) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad "" np_thru_hole circle (at 10.4 4.5) (size 2.2 2.2) (drill 2) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at -4.4 4.5) (size 2.2 2.2) (drill 2) (layers *.Cu *.Mask))
    (pad 1 thru_hole rect (at 0 0) (size 1.5 1.5) (drill 0.9) (layers *.Cu *.Mask)
      (net 4 "Net-(F1-Pad1)"))
    (pad 2 thru_hole circle (at 1 2.5) (size 1.5 1.5) (drill 0.9) (layers *.Cu *.Mask)
      (net 4 "Net-(F1-Pad1)"))
    (pad 3 thru_hole circle (at 2 0) (size 1.5 1.5) (drill 0.9) (layers *.Cu *.Mask)
      (net 4 "Net-(F1-Pad1)"))
    (pad 4 thru_hole circle (at 3 2.5) (size 1.5 1.5) (drill 0.9) (layers *.Cu *.Mask)
      (net 3 "Net-(J1-Pad3)"))
    (pad 5 thru_hole circle (at 4 0) (size 1.5 1.5) (drill 0.9) (layers *.Cu *.Mask)
      (net 2 "Net-(J1-Pad2)"))
    (pad 6 thru_hole circle (at 5 2.5) (size 1.5 1.5) (drill 0.9) (layers *.Cu *.Mask)
      (net 1 "Net-(J1-Pad1)"))
    (pad 7 thru_hole circle (at 6 0) (size 1.5 1.5) (drill 0.9) (layers *.Cu *.Mask)
      (net 1 "Net-(J1-Pad1)"))
    (pad 8 thru_hole circle (at 7 2.5) (size 1.5 1.5) (drill 0.9) (layers *.Cu *.Mask)
      (net 1 "Net-(J1-Pad1)"))
    (model ${KISYS3DMOD}/Connector_RJ.3dshapes/RJ45_8.wrl
      (at (xyz 116.128797 -161.289995 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )

  (module RJ45:RJ45 (layer F.Cu) (tedit 5AD06174) (tstamp 5B68A06B)
    (at 120.5 53.5)
    (descr "RJ45 connector, 8-pin")
    (tags RJ45)
    (path /5B67DF3D)
    (fp_text reference J3 (at 3.25 -4.25) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value RJ45 (at 2.8 5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -6.25 -3.25) (end 12.25 -3.25) (layer F.CrtYd) (width 0.15))
    (fp_line (start 12.25 -3.25) (end 12.25 7.25) (layer F.CrtYd) (width 0.15))
    (fp_line (start 12.25 7.25) (end -6.25 7.25) (layer F.CrtYd) (width 0.15))
    (fp_line (start -6.25 7.25) (end -6.25 -3.25) (layer F.CrtYd) (width 0.15))
    (fp_line (start -5.8 6.8) (end 11.8 6.8) (layer F.Fab) (width 0.15))
    (fp_line (start 11.8 6.8) (end 11.8 -2.8) (layer F.Fab) (width 0.15))
    (fp_line (start 11.8 -2.8) (end -4.8 -2.8) (layer F.Fab) (width 0.15))
    (fp_line (start -4.8 -2.8) (end -5.8 -1.8) (layer F.Fab) (width 0.15))
    (fp_line (start -5.8 -1.8) (end -5.8 6.8) (layer F.Fab) (width 0.15))
    (fp_line (start -6 7) (end 12 7) (layer F.SilkS) (width 0.15))
    (fp_line (start 12 7) (end 12 -3) (layer F.SilkS) (width 0.15))
    (fp_line (start 12 -3) (end -6 -3) (layer F.SilkS) (width 0.15))
    (fp_line (start -6 -3) (end -6 7) (layer F.SilkS) (width 0.15))
    (fp_text user %R (at 3.25 -4.25) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad "" np_thru_hole circle (at 10.4 4.5) (size 2.2 2.2) (drill 2) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at -4.4 4.5) (size 2.2 2.2) (drill 2) (layers *.Cu *.Mask))
    (pad 1 thru_hole rect (at 0 0) (size 1.5 1.5) (drill 0.9) (layers *.Cu *.Mask)
      (net 4 "Net-(F1-Pad1)"))
    (pad 2 thru_hole circle (at 1 2.5) (size 1.5 1.5) (drill 0.9) (layers *.Cu *.Mask)
      (net 4 "Net-(F1-Pad1)"))
    (pad 3 thru_hole circle (at 2 0) (size 1.5 1.5) (drill 0.9) (layers *.Cu *.Mask)
      (net 4 "Net-(F1-Pad1)"))
    (pad 4 thru_hole circle (at 3 2.5) (size 1.5 1.5) (drill 0.9) (layers *.Cu *.Mask)
      (net 3 "Net-(J1-Pad3)"))
    (pad 5 thru_hole circle (at 4 0) (size 1.5 1.5) (drill 0.9) (layers *.Cu *.Mask)
      (net 2 "Net-(J1-Pad2)"))
    (pad 6 thru_hole circle (at 5 2.5) (size 1.5 1.5) (drill 0.9) (layers *.Cu *.Mask)
      (net 1 "Net-(J1-Pad1)"))
    (pad 7 thru_hole circle (at 6 0) (size 1.5 1.5) (drill 0.9) (layers *.Cu *.Mask)
      (net 1 "Net-(J1-Pad1)"))
    (pad 8 thru_hole circle (at 7 2.5) (size 1.5 1.5) (drill 0.9) (layers *.Cu *.Mask)
      (net 1 "Net-(J1-Pad1)"))
    (model ${KISYS3DMOD}/Connector_RJ.3dshapes/RJ45_8.wrl
      (at (xyz 116.128797 -161.289995 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )

  (module RJ45:Hole_3mm (layer F.Cu) (tedit 5B67E153) (tstamp 5B67E16B)
    (at 171 79)
    (fp_text reference REF** (at 0 3.81) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value Hole_3mm (at 0 -7.62) (layer F.Fab) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
  )

  (module RJ45:Hole_3mm (layer F.Cu) (tedit 5B67E17F) (tstamp 5B67E190)
    (at 117.75 48)
    (fp_text reference REF** (at 0 3.81) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value Hole_3mm (at 0 -7.62) (layer F.Fab) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole circle (at 0 0) (size 5 5) (drill 1) (layers *.Cu *.Mask))
  )

  (module RJ45:Hole_3mm (layer F.Cu) (tedit 5B67E17F) (tstamp 5B67E19A)
    (at 148.25 48)
    (fp_text reference REF** (at 0 3.81) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value Hole_3mm (at 0 -7.62) (layer F.Fab) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole circle (at 0 0) (size 5 5) (drill 1) (layers *.Cu *.Mask))
  )

  (module RJ45:FUSE (layer F.Cu) (tedit 5B686345) (tstamp 5B6873A7)
    (at 126.238 47.371)
    (path /5B685A07)
    (fp_text reference F1 (at 8.255 3.937) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value Fuse (at 7.874 -4.064) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 2 smd rect (at 14.25 0) (size 6 5) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(F1-Pad2)"))
    (pad 1 smd rect (at 0 0) (size 6 5) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(F1-Pad1)"))
  )

  (dimension 22 (width 0.3) (layer Dwgs.User)
    (gr_text "22.000 mm" (at 156.85 51 90) (layer Dwgs.User)
      (effects (font (size 1.5 1.5) (thickness 0.3)))
    )
    (feature1 (pts (xy 152 40) (xy 158.2 40)))
    (feature2 (pts (xy 152 62) (xy 158.2 62)))
    (crossbar (pts (xy 155.5 62) (xy 155.5 40)))
    (arrow1a (pts (xy 155.5 40) (xy 156.086421 41.126504)))
    (arrow1b (pts (xy 155.5 40) (xy 154.913579 41.126504)))
    (arrow2a (pts (xy 155.5 62) (xy 156.086421 60.873496)))
    (arrow2b (pts (xy 155.5 62) (xy 154.913579 60.873496)))
  )
  (dimension 38 (width 0.3) (layer Dwgs.User)
    (gr_text "38.000 mm" (at 133 65.349999) (layer Dwgs.User)
      (effects (font (size 1.5 1.5) (thickness 0.3)))
    )
    (feature1 (pts (xy 152 62) (xy 152 66.699999)))
    (feature2 (pts (xy 114 62) (xy 114 66.699999)))
    (crossbar (pts (xy 114 63.999999) (xy 152 63.999999)))
    (arrow1a (pts (xy 152 63.999999) (xy 150.873496 64.58642)))
    (arrow1b (pts (xy 152 63.999999) (xy 150.873496 63.413578)))
    (arrow2a (pts (xy 114 63.999999) (xy 115.126504 64.58642)))
    (arrow2b (pts (xy 114 63.999999) (xy 115.126504 63.413578)))
  )
  (gr_text 3-CANL (at 146.431 41.529) (layer B.Cu)
    (effects (font (size 1.5 1.5) (thickness 0.3)) (justify mirror))
  )
  (gr_text 2CANH (at 117.856 41.529) (layer B.Cu)
    (effects (font (size 1.5 1.5) (thickness 0.3)) (justify mirror))
  )
  (gr_text "4 +12V" (at 145.923 41.783) (layer F.Cu)
    (effects (font (size 1.5 1.5) (thickness 0.3)))
  )
  (gr_text "1 Gnd" (at 117.856 41.783) (layer F.Cu)
    (effects (font (size 1.5 1.5) (thickness 0.3)))
  )
  (gr_line (start 152 62) (end 152 61) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 114 62) (end 152 62) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 114 61) (end 114 62) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 114 40) (end 152 40) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 114 40) (end 114 61) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 152 40) (end 152 61) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 112 48) (end 154 48) (angle 90) (layer Dwgs.User) (width 0.2))

  (segment (start 122.682 42.545) (end 122.682 42.037) (width 1) (layer B.Cu) (net 1))
  (segment (start 122.682 42.037) (end 123.698 41.021) (width 1) (layer B.Cu) (net 1) (tstamp 5B6874D9))
  (segment (start 121.298822 50.718325) (end 121.298822 43.928178) (width 1) (layer F.Cu) (net 1))
  (segment (start 121.298822 43.928178) (end 122.682 42.545) (width 1) (layer F.Cu) (net 1) (tstamp 5B6874D6))
  (segment (start 128.27 51.435) (end 144.272 51.435) (width 1) (layer F.Cu) (net 1))
  (segment (start 145.5 50.885) (end 145.5 53.5) (width 1) (layer B.Cu) (net 1) (tstamp 5B687478))
  (segment (start 144.399 49.784) (end 145.5 50.885) (width 1) (layer B.Cu) (net 1) (tstamp 5B687477))
  (segment (start 144.399 46.101) (end 144.399 49.784) (width 1) (layer B.Cu) (net 1) (tstamp 5B687476))
  (segment (start 146.431 44.069) (end 144.399 46.101) (width 1) (layer B.Cu) (net 1) (tstamp 5B687475))
  (via (at 146.431 44.069) (size 2) (drill 0.8) (layers F.Cu B.Cu) (net 1))
  (segment (start 144.907 45.593) (end 146.431 44.069) (width 1) (layer F.Cu) (net 1) (tstamp 5B687473))
  (segment (start 144.907 50.8) (end 144.907 45.593) (width 1) (layer F.Cu) (net 1) (tstamp 5B687472))
  (segment (start 144.272 51.435) (end 144.907 50.8) (width 1) (layer F.Cu) (net 1) (tstamp 5B687471))
  (segment (start 126.5 53.5) (end 128.491 53.5) (width 1) (layer B.Cu) (net 1))
  (segment (start 128.397 41.021) (end 129.286 41.91) (width 1) (layer B.Cu) (net 1) (tstamp 5B68744D))
  (via (at 122.682 42.545) (size 2) (drill 0.8) (layers F.Cu B.Cu) (net 1))
  (segment (start 123.698 41.021) (end 128.397 41.021) (width 1) (layer B.Cu) (net 1) (tstamp 5B6874DC))
  (segment (start 121.285 50.8) (end 121.298822 50.718325) (width 1) (layer F.Cu) (net 1) (tstamp 5B687448))
  (segment (start 121.92 51.435) (end 121.285 50.8) (width 1) (layer F.Cu) (net 1) (tstamp 5B687447))
  (segment (start 129.794 51.435) (end 128.27 51.435) (width 1) (layer F.Cu) (net 1) (tstamp 5B687446))
  (segment (start 128.27 51.435) (end 121.92 51.435) (width 1) (layer F.Cu) (net 1) (tstamp 5B68746F))
  (segment (start 130.81 50.419) (end 129.794 51.435) (width 1) (layer F.Cu) (net 1) (tstamp 5B687445))
  (segment (start 130.81 49.657) (end 130.81 50.419) (width 1) (layer F.Cu) (net 1) (tstamp 5B687444))
  (segment (start 131.064 49.403) (end 130.81 49.657) (width 1) (layer F.Cu) (net 1) (tstamp 5B687443))
  (via (at 131.064 49.403) (size 2) (drill 0.8) (layers F.Cu B.Cu) (net 1))
  (segment (start 131.064 50.927) (end 131.064 49.403) (width 1) (layer B.Cu) (net 1) (tstamp 5B687441))
  (segment (start 128.491 53.5) (end 131.064 50.927) (width 1) (layer B.Cu) (net 1) (tstamp 5B687440))
  (segment (start 125.5 56) (end 127.5 56) (width 1) (layer B.Cu) (net 1))
  (segment (start 127.5 56) (end 126.5 55) (width 1) (layer B.Cu) (net 1) (tstamp 5B67E503))
  (segment (start 126.5 55) (end 126.5 53.5) (width 1) (layer B.Cu) (net 1) (tstamp 5B67E504))
  (segment (start 144.5 56) (end 146.5 56) (width 1) (layer B.Cu) (net 1))
  (segment (start 146.5 56) (end 145.5 55) (width 1) (layer B.Cu) (net 1) (tstamp 5B67E4FA))
  (segment (start 145.5 55) (end 145.5 53.5) (width 1) (layer B.Cu) (net 1) (tstamp 5B67E4FB))
  (segment (start 126.5 53.5) (end 126.5 53.078) (width 1) (layer B.Cu) (net 1))
  (segment (start 143.5 53.5) (end 143.5 52.06) (width 1) (layer B.Cu) (net 2))
  (segment (start 136.906 45.466) (end 135.636 45.466) (width 1) (layer B.Cu) (net 2) (tstamp 5B687451))
  (segment (start 143.5 52.06) (end 136.906 45.466) (width 1) (layer B.Cu) (net 2) (tstamp 5B687450))
  (segment (start 124.5 53.5) (end 124.5 47.585) (width 1) (layer B.Cu) (net 2))
  (segment (start 126.619 45.466) (end 131.064 45.466) (width 1) (layer B.Cu) (net 2) (tstamp 5B68741E))
  (segment (start 124.5 47.585) (end 126.619 45.466) (width 1) (layer B.Cu) (net 2) (tstamp 5B68741D))
  (segment (start 131.826 41.91) (end 131.826 44.704) (width 1) (layer B.Cu) (net 2))
  (segment (start 131.826 44.704) (end 131.064 45.466) (width 1) (layer B.Cu) (net 2) (tstamp 5B68741A))
  (via (at 131.064 45.466) (size 2) (drill 0.8) (layers F.Cu B.Cu) (net 2))
  (via (at 135.636 45.466) (size 2) (drill 0.8) (layers F.Cu B.Cu) (net 2))
  (segment (start 131.064 45.466) (end 135.636 45.466) (width 1) (layer F.Cu) (net 2) (tstamp 5B6873DF))
  (segment (start 133.731 45.212) (end 133.731 52.07) (width 1) (layer B.Cu) (net 3))
  (segment (start 133.731 52.07) (end 136.271 54.61) (width 1) (layer B.Cu) (net 3) (tstamp 5B687427))
  (segment (start 134.366 41.91) (end 134.366 43.561) (width 1) (layer B.Cu) (net 3))
  (segment (start 133.731 44.196) (end 133.731 45.212) (width 1) (layer B.Cu) (net 3) (tstamp 5B687404))
  (segment (start 134.366 43.561) (end 133.731 44.196) (width 1) (layer B.Cu) (net 3) (tstamp 5B687403))
  (segment (start 138.176 56.515) (end 138.176 60.452) (width 1) (layer B.Cu) (net 3) (tstamp 5B6873D7))
  (segment (start 136.271 54.61) (end 138.176 56.515) (width 1) (layer B.Cu) (net 3) (tstamp 5B68742A))
  (segment (start 123.5 56) (end 123.5 57.206) (width 1) (layer B.Cu) (net 3))
  (segment (start 139.827 60.452) (end 142.5 57.779) (width 1) (layer B.Cu) (net 3) (tstamp 5B67E537))
  (segment (start 126.746 60.452) (end 138.176 60.452) (width 1) (layer B.Cu) (net 3) (tstamp 5B67E536))
  (segment (start 138.176 60.452) (end 139.827 60.452) (width 1) (layer B.Cu) (net 3) (tstamp 5B6873DA))
  (segment (start 123.5 57.206) (end 126.746 60.452) (width 1) (layer B.Cu) (net 3) (tstamp 5B67E535))
  (segment (start 142.5 57.779) (end 142.5 56) (width 1) (layer B.Cu) (net 3) (tstamp 5B67E50D))
  (segment (start 126.238 47.371) (end 135.128 47.371) (width 1) (layer F.Cu) (net 4))
  (segment (start 135.128 47.371) (end 135.763 48.006) (width 1) (layer F.Cu) (net 4) (tstamp 5B6874B5))
  (segment (start 125.476 43.307) (end 125.476 46.609) (width 1) (layer F.Cu) (net 4))
  (segment (start 125.476 46.609) (end 126.238 47.371) (width 1) (layer F.Cu) (net 4) (tstamp 5B6874B1))
  (segment (start 139.5 53.5) (end 139.5 52.759) (width 1) (layer B.Cu) (net 4))
  (segment (start 139.5 52.759) (end 135.763 49.022) (width 1) (layer B.Cu) (net 4) (tstamp 5B687467))
  (segment (start 135.128 47.371) (end 125.73 47.371) (width 1) (layer F.Cu) (net 4) (tstamp 5B68746B))
  (segment (start 135.763 48.006) (end 135.128 47.371) (width 1) (layer F.Cu) (net 4) (tstamp 5B68746A))
  (via (at 135.763 48.006) (size 2) (drill 0.8) (layers F.Cu B.Cu) (net 4))
  (segment (start 135.763 49.022) (end 135.763 48.006) (width 1) (layer B.Cu) (net 4) (tstamp 5B687468))
  (segment (start 139.5 53.5) (end 141.5 53.5) (width 1) (layer B.Cu) (net 4))
  (segment (start 122.5 53.5) (end 122.5 46.283) (width 1) (layer B.Cu) (net 4))
  (segment (start 122.5 46.283) (end 125.476 43.307) (width 1) (layer B.Cu) (net 4) (tstamp 5B68743D))
  (segment (start 125.476 43.307) (end 125.476 47.117) (width 1) (layer F.Cu) (net 4))
  (via (at 125.476 43.307) (size 2) (drill 0.8) (layers F.Cu B.Cu) (net 4))
  (segment (start 125.476 47.117) (end 125.73 47.371) (width 1) (layer F.Cu) (net 4) (tstamp 5B687438))
  (segment (start 124.079 47.371) (end 125.73 47.371) (width 1) (layer F.Cu) (net 4) (tstamp 5B6873B5))
  (segment (start 120.5 53.5) (end 122.5 53.5) (width 1) (layer B.Cu) (net 4))
  (segment (start 122.5 53.5) (end 121.5 54.5) (width 1) (layer B.Cu) (net 4) (tstamp 5B67E4FF))
  (segment (start 121.5 54.5) (end 121.5 56) (width 1) (layer B.Cu) (net 4) (tstamp 5B67E500))
  (segment (start 141.5 53.5) (end 140.5 54.5) (width 1) (layer B.Cu) (net 4) (tstamp 5B67E4F5))
  (segment (start 140.5 54.5) (end 140.5 56) (width 1) (layer B.Cu) (net 4) (tstamp 5B67E4F6))
  (segment (start 121.5 56) (end 121.292 56) (width 1) (layer B.Cu) (net 4))
  (segment (start 140.716 43.18) (end 140.716 47.143) (width 1) (layer F.Cu) (net 5))
  (segment (start 140.716 47.143) (end 140.488 47.371) (width 1) (layer F.Cu) (net 5) (tstamp 5B6874AE))
  (segment (start 140.73 47.371) (end 140.73 43.194) (width 1) (layer F.Cu) (net 5))
  (segment (start 139.446 41.91) (end 136.906 41.91) (width 1) (layer B.Cu) (net 5) (tstamp 5B6873BB))
  (segment (start 140.716 43.18) (end 139.446 41.91) (width 1) (layer B.Cu) (net 5) (tstamp 5B6873BA))
  (via (at 140.716 43.18) (size 2) (drill 0.8) (layers F.Cu B.Cu) (net 5))
  (segment (start 140.73 43.194) (end 140.716 43.18) (width 1) (layer F.Cu) (net 5) (tstamp 5B6873B8))

)
