(export (version D)
  (design
    (source /home/eddy/Dropbox/Projects/tsys01/kicad/stm32/stm32.sch)
    (date "Пт 13 апр 2018 10:55:28")
    (tool "Eeschema 4.0.7")
    (sheet (number 1) (name /) (tstamps /)
      (title_block
        (title)
        (company)
        (rev)
        (date)
        (source stm32.sch)
        (comment (number 1) (value ""))
        (comment (number 2) (value ""))
        (comment (number 3) (value ""))
        (comment (number 4) (value "")))))
  (components
    (comp (ref U7)
      (value STM32F042C6Tx)
      (footprint Package_QFP:LQFP-48_7x7mm_P0.5mm)
      (libsource (lib stm32-cache) (part STM32F042C6Tx))
      (sheetpath (names /) (tstamps /))
      (tstamp 58C42C0E))
    (comp (ref C11)
      (value 0.1)
      (footprint Capacitor_SMD:C_0603_1608Metric_Pad0.84x1.00mm_HandSolder)
      (libsource (lib stm32-cache) (part C))
      (sheetpath (names /) (tstamps /))
      (tstamp 58C42D39))
    (comp (ref U1)
      (value LM2576HV)
      (footprint Package_TO_SOT_THT:TO-220-5_Vertical_StaggeredType2)
      (fields
        (field (name Manufacturer) "Texas Instruments"))
      (libsource (lib stm32-cache) (part LM2576HV))
      (sheetpath (names /) (tstamps /))
      (tstamp 58C43093))
    (comp (ref U2)
      (value LM1117-3.3)
      (footprint Package_TO_SOT_SMD:SOT-223)
      (libsource (lib stm32-rescue) (part LM1117-3.3-RESCUE-stm32))
      (sheetpath (names /) (tstamps /))
      (tstamp 58C431FC))
    (comp (ref U4)
      (value MCP2551-I/SN)
      (footprint Package_SOIC:SOIC-8_3.9x4.9mm_P1.27mm)
      (libsource (lib stm32-cache) (part MCP2551-I/SN))
      (sheetpath (names /) (tstamps /))
      (tstamp 58C43297))
    (comp (ref P13)
      (value USB_A)
      (footprint Connector_USB:USB_Mini-B_Lumber_2486_Horizontal)
      (libsource (lib stm32-cache) (part USB_A-RESCUE-stm32))
      (sheetpath (names /) (tstamps /))
      (tstamp 58C433D0))
    (comp (ref D1)
      (value 1n5822)
      (footprint Diode_THT:D_DO-201_P12.70mm_Horizontal)
      (libsource (lib stm32-cache) (part D))
      (sheetpath (names /) (tstamps /))
      (tstamp 58C43816))
    (comp (ref L1)
      (value 100u)
      (footprint Capacitor_THT:C_Rect_L9.0mm_W2.5mm_P7.50mm_MKT)
      (libsource (lib stm32-cache) (part L))
      (sheetpath (names /) (tstamps /))
      (tstamp 58C43929))
    (comp (ref C4)
      (value 100u)
      (footprint Capacitor_THT:CP_Radial_D8.0mm_P3.50mm)
      (libsource (lib stm32-cache) (part CP))
      (sheetpath (names /) (tstamps /))
      (tstamp 58C4396A))
    (comp (ref C1)
      (value 47u)
      (footprint Capacitor_Tantalum_SMD:CP_EIA-3216-18_Kemet-A_Pad1.53x1.40mm_HandSolder)
      (libsource (lib stm32-cache) (part CP))
      (sheetpath (names /) (tstamps /))
      (tstamp 58C43A3B))
    (comp (ref C2)
      (value 47u)
      (footprint Capacitor_Tantalum_SMD:CP_EIA-3216-18_Kemet-A_Pad1.53x1.40mm_HandSolder)
      (libsource (lib stm32-cache) (part CP))
      (sheetpath (names /) (tstamps /))
      (tstamp 58C454F6))
    (comp (ref D3)
      (value PESD1CAN)
      (footprint Package_TO_SOT_SMD:SOT-23)
      (libsource (lib stm32-cache) (part PESD1CAN))
      (sheetpath (names /) (tstamps /))
      (tstamp 58C46522))
    (comp (ref R8)
      (value 4k7)
      (footprint Resistor_SMD:R_0603_1608Metric_Pad0.84x1.00mm_HandSolder)
      (libsource (lib stm32-cache) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 58C47F04))
    (comp (ref R9)
      (value 120)
      (footprint Resistor_SMD:R_0603_1608Metric_Pad0.84x1.00mm_HandSolder)
      (libsource (lib stm32-cache) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 58C488C6))
    (comp (ref JP1)
      (value Terminal)
      (footprint Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical)
      (libsource (lib stm32-cache) (part Jumper_NO_Small))
      (sheetpath (names /) (tstamps /))
      (tstamp 58C4940D))
    (comp (ref P2)
      (value RJ9-sensor)
      (footprint my_footprints:RJ9-4P4C)
      (libsource (lib stm32-cache) (part CONN_01X04))
      (sheetpath (names /) (tstamps /))
      (tstamp 590237E6))
    (comp (ref U5)
      (value 74HC4051)
      (footprint Package_SOIC:SOIC-16_3.9x9.9mm_P1.27mm)
      (libsource (lib stm32-cache) (part 74HC4051))
      (sheetpath (names /) (tstamps /))
      (tstamp 5908AF06))
    (comp (ref U6)
      (value 74HC4051)
      (footprint Package_SOIC:SOIC-16_3.9x9.9mm_P1.27mm)
      (libsource (lib stm32-cache) (part 74HC4051))
      (sheetpath (names /) (tstamps /))
      (tstamp 5908B293))
    (comp (ref D5)
      (value LED0)
      (footprint LED_SMD:LED_0805_2012Metric_Pad0.97x1.50mm_HandSolder)
      (libsource (lib stm32-cache) (part LED-RESCUE-stm32))
      (sheetpath (names /) (tstamps /))
      (tstamp 5908EA64))
    (comp (ref R29)
      (value 330)
      (footprint Resistor_SMD:R_0603_1608Metric_Pad0.84x1.00mm_HandSolder)
      (libsource (lib stm32-cache) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 5908EB17))
    (comp (ref C12)
      (value 0.1)
      (footprint Capacitor_SMD:C_0603_1608Metric_Pad0.84x1.00mm_HandSolder)
      (libsource (lib stm32-cache) (part C))
      (sheetpath (names /) (tstamps /))
      (tstamp 590935EA))
    (comp (ref C13)
      (value 0.1)
      (footprint Capacitor_SMD:C_0603_1608Metric_Pad0.84x1.00mm_HandSolder)
      (libsource (lib stm32-cache) (part C))
      (sheetpath (names /) (tstamps /))
      (tstamp 59093675))
    (comp (ref D7)
      (value USB6B1)
      (footprint Package_SOIC:SOIC-8_3.9x4.9mm_P1.27mm)
      (libsource (lib stm32-cache) (part USB6B1))
      (sheetpath (names /) (tstamps /))
      (tstamp 59098D4D))
    (comp (ref D6)
      (value LED1)
      (footprint LED_SMD:LED_0805_2012Metric_Pad0.97x1.50mm_HandSolder)
      (libsource (lib stm32-cache) (part LED-RESCUE-stm32))
      (sheetpath (names /) (tstamps /))
      (tstamp 5909AF9A))
    (comp (ref R30)
      (value 330)
      (footprint Resistor_SMD:R_0603_1608Metric_Pad0.84x1.00mm_HandSolder)
      (libsource (lib stm32-cache) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 5909AFA0))
    (comp (ref D2)
      (value LED)
      (footprint LED_SMD:LED_0805_2012Metric_Pad0.97x1.50mm_HandSolder)
      (libsource (lib stm32-cache) (part LED-RESCUE-stm32))
      (sheetpath (names /) (tstamps /))
      (tstamp 5909BFFC))
    (comp (ref R5)
      (value 330)
      (footprint Resistor_SMD:R_0603_1608Metric_Pad0.84x1.00mm_HandSolder)
      (libsource (lib stm32-cache) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 5909C002))
    (comp (ref C14)
      (value 0.1)
      (footprint Capacitor_SMD:C_0603_1608Metric_Pad0.84x1.00mm_HandSolder)
      (libsource (lib stm32-cache) (part C))
      (sheetpath (names /) (tstamps /))
      (tstamp 590A8102))
    (comp (ref P12)
      (value USART_BOOT)
      (footprint Connector_PinHeader_2.54mm:PinHeader_1x03_P2.54mm_Vertical)
      (libsource (lib stm32-cache) (part CONN_01X03))
      (sheetpath (names /) (tstamps /))
      (tstamp 590AD3A7))
    (comp (ref P3)
      (value RJ9-sensor)
      (footprint my_footprints:RJ9-4P4C)
      (libsource (lib stm32-cache) (part CONN_01X04))
      (sheetpath (names /) (tstamps /))
      (tstamp 590B3758))
    (comp (ref P4)
      (value RJ9-sensor)
      (footprint my_footprints:RJ9-4P4C)
      (libsource (lib stm32-cache) (part CONN_01X04))
      (sheetpath (names /) (tstamps /))
      (tstamp 590B3802))
    (comp (ref P5)
      (value RJ9-sensor)
      (footprint my_footprints:RJ9-4P4C)
      (libsource (lib stm32-cache) (part CONN_01X04))
      (sheetpath (names /) (tstamps /))
      (tstamp 590B391A))
    (comp (ref P6)
      (value RJ9-sensor)
      (footprint my_footprints:RJ9-4P4C)
      (libsource (lib stm32-cache) (part CONN_01X04))
      (sheetpath (names /) (tstamps /))
      (tstamp 590B3CF4))
    (comp (ref P7)
      (value RJ9-sensor)
      (footprint my_footprints:RJ9-4P4C)
      (libsource (lib stm32-cache) (part CONN_01X04))
      (sheetpath (names /) (tstamps /))
      (tstamp 590B3CFA))
    (comp (ref P8)
      (value RJ9-sensor)
      (footprint my_footprints:RJ9-4P4C)
      (libsource (lib stm32-cache) (part CONN_01X04))
      (sheetpath (names /) (tstamps /))
      (tstamp 590B3D00))
    (comp (ref P9)
      (value RJ9-sensor)
      (footprint my_footprints:RJ9-4P4C)
      (libsource (lib stm32-cache) (part CONN_01X04))
      (sheetpath (names /) (tstamps /))
      (tstamp 590B3D06))
    (comp (ref R10)
      (value 4k7)
      (footprint Resistor_SMD:R_0603_1608Metric_Pad0.84x1.00mm_HandSolder)
      (libsource (lib stm32-cache) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 590B7EE1))
    (comp (ref R11)
      (value 4k7)
      (footprint Resistor_SMD:R_0603_1608Metric_Pad0.84x1.00mm_HandSolder)
      (libsource (lib stm32-cache) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 590B8C78))
    (comp (ref R12)
      (value 4k7)
      (footprint Resistor_SMD:R_0603_1608Metric_Pad0.84x1.00mm_HandSolder)
      (libsource (lib stm32-cache) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 590C0F54))
    (comp (ref R13)
      (value 4k7)
      (footprint Resistor_SMD:R_0603_1608Metric_Pad0.84x1.00mm_HandSolder)
      (libsource (lib stm32-cache) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 590C0F5A))
    (comp (ref R14)
      (value 4k7)
      (footprint Resistor_SMD:R_0603_1608Metric_Pad0.84x1.00mm_HandSolder)
      (libsource (lib stm32-cache) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 590C467B))
    (comp (ref R15)
      (value 4k7)
      (footprint Resistor_SMD:R_0603_1608Metric_Pad0.84x1.00mm_HandSolder)
      (libsource (lib stm32-cache) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 590C4681))
    (comp (ref R16)
      (value 4k7)
      (footprint Resistor_SMD:R_0603_1608Metric_Pad0.84x1.00mm_HandSolder)
      (libsource (lib stm32-cache) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 590C4690))
    (comp (ref R17)
      (value 4k7)
      (footprint Resistor_SMD:R_0603_1608Metric_Pad0.84x1.00mm_HandSolder)
      (libsource (lib stm32-cache) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 590C4696))
    (comp (ref R18)
      (value 4k7)
      (footprint Resistor_SMD:R_0603_1608Metric_Pad0.84x1.00mm_HandSolder)
      (libsource (lib stm32-cache) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 590C549D))
    (comp (ref R19)
      (value 4k7)
      (footprint Resistor_SMD:R_0603_1608Metric_Pad0.84x1.00mm_HandSolder)
      (libsource (lib stm32-cache) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 590C54A3))
    (comp (ref R20)
      (value 4k7)
      (footprint Resistor_SMD:R_0603_1608Metric_Pad0.84x1.00mm_HandSolder)
      (libsource (lib stm32-cache) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 590C54B2))
    (comp (ref R21)
      (value 4k7)
      (footprint Resistor_SMD:R_0603_1608Metric_Pad0.84x1.00mm_HandSolder)
      (libsource (lib stm32-cache) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 590C54B8))
    (comp (ref R22)
      (value 4k7)
      (footprint Resistor_SMD:R_0603_1608Metric_Pad0.84x1.00mm_HandSolder)
      (libsource (lib stm32-cache) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 590C54C7))
    (comp (ref R23)
      (value 4k7)
      (footprint Resistor_SMD:R_0603_1608Metric_Pad0.84x1.00mm_HandSolder)
      (libsource (lib stm32-cache) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 590C54CD))
    (comp (ref R24)
      (value 4k7)
      (footprint Resistor_SMD:R_0603_1608Metric_Pad0.84x1.00mm_HandSolder)
      (libsource (lib stm32-cache) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 590C54DC))
    (comp (ref R25)
      (value 4k7)
      (footprint Resistor_SMD:R_0603_1608Metric_Pad0.84x1.00mm_HandSolder)
      (libsource (lib stm32-cache) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 590C54E2))
    (comp (ref U3)
      (value LM1117-3.3)
      (footprint Package_TO_SOT_SMD:SOT-223)
      (libsource (lib stm32-rescue) (part LM1117-3.3-RESCUE-stm32))
      (sheetpath (names /) (tstamps /))
      (tstamp 590EB986))
    (comp (ref C3)
      (value 47u)
      (footprint Capacitor_Tantalum_SMD:CP_EIA-3216-18_Kemet-A_Pad1.53x1.40mm_HandSolder)
      (libsource (lib stm32-cache) (part CP))
      (sheetpath (names /) (tstamps /))
      (tstamp 590EB998))
    (comp (ref P1)
      (value RJ45-CAN_power)
      (footprint RJ45:RJ45)
      (libsource (lib stm32-cache) (part CONN_01X08))
      (sheetpath (names /) (tstamps /))
      (tstamp 5910AA04))
    (comp (ref Q1)
      (value AO3407)
      (footprint Package_TO_SOT_SMD:SOT-23_Handsoldering)
      (libsource (lib stm32-cache) (part Q_PMOS_GSD))
      (sheetpath (names /) (tstamps /))
      (tstamp 5910E2F2))
    (comp (ref R1)
      (value 47k)
      (footprint Resistor_SMD:R_0603_1608Metric_Pad0.84x1.00mm_HandSolder)
      (libsource (lib stm32-cache) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 590A5C84))
    (comp (ref R2)
      (value 47k)
      (footprint Resistor_SMD:R_0603_1608Metric_Pad0.84x1.00mm_HandSolder)
      (libsource (lib stm32-cache) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 590A6068))
    (comp (ref R3)
      (value 220k)
      (footprint Resistor_SMD:R_0603_1608Metric_Pad0.84x1.00mm_HandSolder)
      (libsource (lib stm32-cache) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 590A6DD4))
    (comp (ref R4)
      (value 56k)
      (footprint Resistor_SMD:R_0603_1608Metric_Pad0.84x1.00mm_HandSolder)
      (libsource (lib stm32-cache) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 590A6DDA))
    (comp (ref R6)
      (value 47k)
      (footprint Resistor_SMD:R_0603_1608Metric_Pad0.84x1.00mm_HandSolder)
      (libsource (lib stm32-cache) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 590A6F68))
    (comp (ref R7)
      (value 47k)
      (footprint Resistor_SMD:R_0603_1608Metric_Pad0.84x1.00mm_HandSolder)
      (libsource (lib stm32-cache) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 590A6F6E))
    (comp (ref R27)
      (value 10k)
      (footprint Resistor_SMD:R_0603_1608Metric_Pad0.84x1.00mm_HandSolder)
      (libsource (lib stm32-cache) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 590D30C8))
    (comp (ref R28)
      (value 10k)
      (footprint Resistor_SMD:R_0603_1608Metric_Pad0.84x1.00mm_HandSolder)
      (libsource (lib stm32-cache) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 590D3334))
    (comp (ref C6)
      (value 0.1)
      (footprint Capacitor_SMD:C_0603_1608Metric_Pad0.84x1.00mm_HandSolder)
      (libsource (lib stm32-cache) (part C))
      (sheetpath (names /) (tstamps /))
      (tstamp 590D4150))
    (comp (ref C5)
      (value 0.1)
      (footprint Capacitor_SMD:C_0603_1608Metric_Pad0.84x1.00mm_HandSolder)
      (libsource (lib stm32-cache) (part C))
      (sheetpath (names /) (tstamps /))
      (tstamp 590D4832))
    (comp (ref SW2)
      (value Boot)
      (footprint Button_Switch_SMD:SW_SPST_FSMSM)
      (libsource (lib stm32-cache) (part SW_Push))
      (sheetpath (names /) (tstamps /))
      (tstamp 5909F6B6))
    (comp (ref SW1)
      (value Reset)
      (footprint Button_Switch_SMD:SW_SPST_FSMSM)
      (libsource (lib stm32-cache) (part SW_Push))
      (sheetpath (names /) (tstamps /))
      (tstamp 590A0134))
    (comp (ref P15)
      (value Hole)
      (footprint my_footprints:Hole_3mm)
      (libsource (lib stm32-cache) (part CONN_01X01))
      (sheetpath (names /) (tstamps /))
      (tstamp 59143415))
    (comp (ref P16)
      (value Hole)
      (footprint my_footprints:Hole_3mm)
      (libsource (lib stm32-cache) (part CONN_01X01))
      (sheetpath (names /) (tstamps /))
      (tstamp 5914456D))
    (comp (ref P17)
      (value Hole)
      (footprint my_footprints:Hole_3mm)
      (libsource (lib stm32-cache) (part CONN_01X01))
      (sheetpath (names /) (tstamps /))
      (tstamp 591446F3))
    (comp (ref P18)
      (value Hole)
      (footprint my_footprints:Hole_3mm)
      (libsource (lib stm32-cache) (part CONN_01X01))
      (sheetpath (names /) (tstamps /))
      (tstamp 591446F9))
    (comp (ref C15)
      (value 0.1)
      (footprint Capacitor_SMD:C_0603_1608Metric_Pad0.84x1.00mm_HandSolder)
      (libsource (lib stm32-cache) (part C))
      (sheetpath (names /) (tstamps /))
      (tstamp 596772D4))
    (comp (ref D9)
      (value MM3Z3V6)
      (footprint Diode_SMD:D_0805_2012Metric_Pad0.97x1.50mm_HandSolder)
      (libsource (lib stm32-cache) (part D_Zener))
      (sheetpath (names /) (tstamps /))
      (tstamp 5968325A))
    (comp (ref D8)
      (value MM3Z3V6)
      (footprint Diode_SMD:D_0805_2012Metric_Pad0.97x1.50mm_HandSolder)
      (libsource (lib stm32-cache) (part D_Zener))
      (sheetpath (names /) (tstamps /))
      (tstamp 59684468))
    (comp (ref R34)
      (value 22)
      (footprint Resistor_SMD:R_0603_1608Metric_Pad0.84x1.00mm_HandSolder)
      (libsource (lib stm32-cache) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 5968E385))
    (comp (ref R35)
      (value 22)
      (footprint Resistor_SMD:R_0603_1608Metric_Pad0.84x1.00mm_HandSolder)
      (libsource (lib stm32-cache) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 5968E83B))
    (comp (ref R32)
      (value 22)
      (footprint Resistor_SMD:R_0603_1608Metric_Pad0.84x1.00mm_HandSolder)
      (libsource (lib stm32-cache) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 5968FBD4))
    (comp (ref D10)
      (value MM3Z3V6)
      (footprint Diode_SMD:D_0805_2012Metric_Pad0.97x1.50mm_HandSolder)
      (libsource (lib stm32-cache) (part D_Zener))
      (sheetpath (names /) (tstamps /))
      (tstamp 59691FAC))
    (comp (ref R33)
      (value 22)
      (footprint Resistor_SMD:R_0603_1608Metric_Pad0.84x1.00mm_HandSolder)
      (libsource (lib stm32-cache) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 59698620))
    (comp (ref D11)
      (value MM3Z3V6)
      (footprint Diode_SMD:D_0805_2012Metric_Pad0.97x1.50mm_HandSolder)
      (libsource (lib stm32-cache) (part D_Zener))
      (sheetpath (names /) (tstamps /))
      (tstamp 59698626))
    (comp (ref U8)
      (value TPS2051)
      (footprint Package_SOIC:SOIC-8_3.9x4.9mm_P1.27mm)
      (libsource (lib stm32-cache) (part TPS2051))
      (sheetpath (names /) (tstamps /))
      (tstamp 5A4B00CC))
    (comp (ref C7)
      (value 0.1)
      (footprint Capacitor_SMD:C_0603_1608Metric_Pad0.84x1.00mm_HandSolder)
      (libsource (lib stm32-cache) (part C))
      (sheetpath (names /) (tstamps /))
      (tstamp 5A4B116A))
    (comp (ref R26)
      (value 10k)
      (footprint Resistor_SMD:R_0603_1608Metric_Pad0.84x1.00mm_HandSolder)
      (libsource (lib stm32-cache) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 5A4B561C))
    (comp (ref U9)
      (value MAX471)
      (footprint Package_SOIC:SOIC-8_3.9x4.9mm_P1.27mm)
      (libsource (lib stm32-rescue) (part MAX471-RESCUE-stm32))
      (sheetpath (names /) (tstamps /))
      (tstamp 5A4C9EB5))
    (comp (ref R31)
      (value "2k 1%")
      (footprint Resistor_SMD:R_0603_1608Metric_Pad0.84x1.00mm_HandSolder)
      (libsource (lib stm32-cache) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 5A4CCE57))
    (comp (ref P14)
      (value RJ45-CAN_power)
      (footprint RJ45:RJ45)
      (libsource (lib stm32-cache) (part CONN_01X08))
      (sheetpath (names /) (tstamps /))
      (tstamp 590E9D66))
    (comp (ref C8)
      (value 0.1)
      (footprint Capacitor_SMD:C_0603_1608Metric_Pad0.84x1.00mm_HandSolder)
      (libsource (lib stm32-cache) (part C))
      (sheetpath (names /) (tstamps /))
      (tstamp 5A4FA4E4))
    (comp (ref J1)
      (value CONN_02X03)
      (footprint Connector_PinHeader_2.54mm:PinHeader_2x03_P2.54mm_Vertical)
      (libsource (lib stm32-cache) (part CONN_02X03))
      (sheetpath (names /) (tstamps /))
      (tstamp 5A50A198))
    (comp (ref R36)
      (value 10k)
      (footprint Resistor_SMD:R_0603_1608Metric_Pad0.84x1.00mm_HandSolder)
      (libsource (lib stm32-cache) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 5A51A823))
    (comp (ref C9)
      (value 0.1)
      (footprint Capacitor_SMD:C_0603_1608Metric_Pad0.84x1.00mm_HandSolder)
      (libsource (lib stm32-cache) (part C))
      (sheetpath (names /) (tstamps /))
      (tstamp 5A51B421))
    (comp (ref D4)
      (value MBRS130L)
      (footprint Diode_SMD:D_SMB_Handsoldering)
      (libsource (lib stm32-cache) (part D_Schottky))
      (sheetpath (names /) (tstamps /))
      (tstamp 5A545B43)))
  (libparts
    (libpart (lib stm32-cache) (part 74HC4051)
      (footprints
        (fp SO16)
        (fp TSSOP16)
        (fp SSOP16)
        (fp DHVQFN16))
      (fields
        (field (name Reference) U)
        (field (name Value) 74HC4051))
      (pins
        (pin (num 1) (name Y4) (type BiDi))
        (pin (num 2) (name Y6) (type BiDi))
        (pin (num 3) (name Z) (type BiDi))
        (pin (num 4) (name Y7) (type BiDi))
        (pin (num 5) (name Y5) (type BiDi))
        (pin (num 6) (name ~E) (type input))
        (pin (num 7) (name VEE) (type power_in))
        (pin (num 8) (name GND) (type power_in))
        (pin (num 9) (name S2) (type input))
        (pin (num 10) (name S1) (type input))
        (pin (num 11) (name S0) (type input))
        (pin (num 12) (name Y3) (type BiDi))
        (pin (num 13) (name Y0) (type BiDi))
        (pin (num 14) (name Y1) (type BiDi))
        (pin (num 15) (name Y2) (type BiDi))
        (pin (num 16) (name VCC) (type power_in))))
    (libpart (lib stm32-cache) (part C)
      (footprints
        (fp C_*))
      (fields
        (field (name Reference) C)
        (field (name Value) C))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib stm32-cache) (part CONN_01X01)
      (footprints
        (fp Pin_Header_Straight_1X*)
        (fp Pin_Header_Angled_1X*)
        (fp Socket_Strip_Straight_1X*)
        (fp Socket_Strip_Angled_1X*))
      (fields
        (field (name Reference) J)
        (field (name Value) CONN_01X01))
      (pins
        (pin (num 1) (name P1) (type passive))))
    (libpart (lib stm32-cache) (part CONN_01X03)
      (footprints
        (fp Pin_Header_Straight_1X*)
        (fp Pin_Header_Angled_1X*)
        (fp Socket_Strip_Straight_1X*)
        (fp Socket_Strip_Angled_1X*))
      (fields
        (field (name Reference) J)
        (field (name Value) CONN_01X03))
      (pins
        (pin (num 1) (name P1) (type passive))
        (pin (num 2) (name P2) (type passive))
        (pin (num 3) (name P3) (type passive))))
    (libpart (lib stm32-cache) (part CONN_01X04)
      (footprints
        (fp Pin_Header_Straight_1X*)
        (fp Pin_Header_Angled_1X*)
        (fp Socket_Strip_Straight_1X*)
        (fp Socket_Strip_Angled_1X*))
      (fields
        (field (name Reference) J)
        (field (name Value) CONN_01X04))
      (pins
        (pin (num 1) (name P1) (type passive))
        (pin (num 2) (name P2) (type passive))
        (pin (num 3) (name P3) (type passive))
        (pin (num 4) (name P4) (type passive))))
    (libpart (lib stm32-cache) (part CONN_01X08)
      (footprints
        (fp Pin_Header_Straight_1X*)
        (fp Pin_Header_Angled_1X*)
        (fp Socket_Strip_Straight_1X*)
        (fp Socket_Strip_Angled_1X*))
      (fields
        (field (name Reference) J)
        (field (name Value) CONN_01X08))
      (pins
        (pin (num 1) (name P1) (type passive))
        (pin (num 2) (name P2) (type passive))
        (pin (num 3) (name P3) (type passive))
        (pin (num 4) (name P4) (type passive))
        (pin (num 5) (name P5) (type passive))
        (pin (num 6) (name P6) (type passive))
        (pin (num 7) (name P7) (type passive))
        (pin (num 8) (name P8) (type passive))))
    (libpart (lib stm32-cache) (part CONN_02X03)
      (footprints
        (fp Pin_Header_Straight_2X*)
        (fp Pin_Header_Angled_2X*)
        (fp Socket_Strip_Straight_2X*)
        (fp Socket_Strip_Angled_2X*)
        (fp IDC_Header_Straight_*))
      (fields
        (field (name Reference) J)
        (field (name Value) CONN_02X03))
      (pins
        (pin (num 1) (name P1) (type passive))
        (pin (num 2) (name P2) (type passive))
        (pin (num 3) (name P3) (type passive))
        (pin (num 4) (name P4) (type passive))
        (pin (num 5) (name P5) (type passive))
        (pin (num 6) (name P6) (type passive))))
    (libpart (lib stm32-cache) (part CP)
      (footprints
        (fp CP_*))
      (fields
        (field (name Reference) C)
        (field (name Value) CP))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib stm32-cache) (part D)
      (footprints
        (fp TO-???*)
        (fp *SingleDiode)
        (fp *_Diode_*)
        (fp *SingleDiode*)
        (fp D_*))
      (fields
        (field (name Reference) D)
        (field (name Value) D))
      (pins
        (pin (num 1) (name K) (type passive))
        (pin (num 2) (name A) (type passive))))
    (libpart (lib stm32-cache) (part D_Schottky)
      (footprints
        (fp TO-???*)
        (fp *SingleDiode)
        (fp *_Diode_*)
        (fp *SingleDiode*)
        (fp D_*))
      (fields
        (field (name Reference) D)
        (field (name Value) D_Schottky))
      (pins
        (pin (num 1) (name K) (type passive))
        (pin (num 2) (name A) (type passive))))
    (libpart (lib stm32-cache) (part D_Zener)
      (footprints
        (fp TO-???*)
        (fp *SingleDiode)
        (fp *_Diode_*)
        (fp *SingleDiode*)
        (fp D_*))
      (fields
        (field (name Reference) D)
        (field (name Value) D_Zener))
      (pins
        (pin (num 1) (name K) (type passive))
        (pin (num 2) (name A) (type passive))))
    (libpart (lib stm32-cache) (part Jumper_NO_Small)
      (fields
        (field (name Reference) JP)
        (field (name Value) Jumper_NO_Small))
      (pins
        (pin (num 1) (name 1) (type passive))
        (pin (num 2) (name 2) (type passive))))
    (libpart (lib stm32-cache) (part L)
      (footprints
        (fp Choke_*)
        (fp *Coil*)
        (fp Inductor_*)
        (fp L_*))
      (fields
        (field (name Reference) L)
        (field (name Value) L))
      (pins
        (pin (num 1) (name 1) (type passive))
        (pin (num 2) (name 2) (type passive))))
    (libpart (lib stm32-cache) (part LED-RESCUE-stm32)
      (footprints
        (fp LED*))
      (fields
        (field (name Reference) D)
        (field (name Value) LED-RESCUE-stm32))
      (pins
        (pin (num 1) (name K) (type passive))
        (pin (num 2) (name A) (type passive))))
    (libpart (lib stm32-rescue) (part LM1117-3.3-RESCUE-stm32)
      (footprints
        (fp SOT-223*)
        (fp TO-263*)
        (fp TO-252*))
      (fields
        (field (name Reference) U)
        (field (name Value) LM1117-3.3-RESCUE-stm32))
      (pins
        (pin (num 1) (name GND/ADJ) (type power_in))
        (pin (num 2) (name VO) (type passive))
        (pin (num 3) (name VI) (type power_in))
        (pin (num 4) (name VO) (type power_out))))
    (libpart (lib stm32-cache) (part LM2576)
      (aliases
        (alias LM2576HV))
      (footprints
        (fp *DIP8)
        (fp SOIC8))
      (fields
        (field (name Reference) U)
        (field (name Value) LM2576)
        (field (name Manufacturer) "Texas Instruments"))
      (pins
        (pin (num 1) (name VIN) (type power_in))
        (pin (num 2) (name VOUT) (type power_out))
        (pin (num 3) (name GND) (type power_in))
        (pin (num 4) (name FB) (type input))
        (pin (num 5) (name ON/OFF) (type input))))
    (libpart (lib stm32-rescue) (part MAX471-RESCUE-stm32)
      (fields
        (field (name Reference) U)
        (field (name Value) MAX471-RESCUE-stm32))
      (pins
        (pin (num 1) (name SHDN) (type input))
        (pin (num 2) (name RS+) (type power_in))
        (pin (num 3) (name RS+) (type passive))
        (pin (num 4) (name GND) (type power_in))
        (pin (num 5) (name SIGN) (type openCol))
        (pin (num 6) (name RS-) (type power_out))
        (pin (num 7) (name RS-) (type passive))
        (pin (num 8) (name OUT) (type output))))
    (libpart (lib stm32-cache) (part MCP2551-I/SN)
      (footprints
        (fp SOIC*Pitch1.27mm*))
      (fields
        (field (name Reference) U)
        (field (name Value) MCP2551-I/SN)
        (field (name Footprint) Housings_SOIC:SOIC-8_3.9x4.9mm_Pitch1.27mm))
      (pins
        (pin (num 1) (name TXD) (type input))
        (pin (num 2) (name VSS) (type power_in))
        (pin (num 3) (name VDD) (type power_in))
        (pin (num 4) (name RXD) (type output))
        (pin (num 5) (name Vref) (type power_out))
        (pin (num 6) (name CANL) (type BiDi))
        (pin (num 7) (name CANH) (type BiDi))
        (pin (num 8) (name Rs) (type input))))
    (libpart (lib stm32-cache) (part PESD1CAN)
      (footprints
        (fp SOT23))
      (fields
        (field (name Reference) D)
        (field (name Value) PESD1CAN))
      (pins
        (pin (num 1) (name K) (type passive))
        (pin (num 2) (name K) (type passive))
        (pin (num 3) (name O) (type passive))))
    (libpart (lib stm32-cache) (part Q_PMOS_GSD)
      (fields
        (field (name Reference) Q)
        (field (name Value) Q_PMOS_GSD))
      (pins
        (pin (num 1) (name G) (type input))
        (pin (num 2) (name S) (type passive))
        (pin (num 3) (name D) (type passive))))
    (libpart (lib stm32-cache) (part R)
      (footprints
        (fp R_*)
        (fp R_*))
      (fields
        (field (name Reference) R)
        (field (name Value) R))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib stm32-cache) (part STM32F042C4Tx)
      (aliases
        (alias STM32F042C6Tx))
      (fields
        (field (name Reference) U)
        (field (name Value) STM32F042C4Tx)
        (field (name Footprint) LQFP48))
      (pins
        (pin (num 1) (name VBAT) (type power_in))
        (pin (num 2) (name PC13/RTC_OUT_ALARM/RTC_OUT_CALIB/RTC_TAMP1/RTC_TS/SYS_WKUP2) (type BiDi))
        (pin (num 3) (name PC14/RCC_OSC32_IN) (type BiDi))
        (pin (num 4) (name PC15/RCC_OSC32_OUT) (type BiDi))
        (pin (num 5) (name PF0/CRS_SYNC/I2C1_SDA/RCC_OSC_IN) (type input))
        (pin (num 6) (name PF1/I2C1_SCL/RCC_OSC_OUT) (type input))
        (pin (num 7) (name NRST) (type input))
        (pin (num 8) (name VSSA) (type power_in))
        (pin (num 9) (name VDDA) (type power_in))
        (pin (num 10) (name ADC_IN0/RTC_TAMP2/SYS_WKUP1/TIM2_CH1/TIM2_ETR/TSC_G1_IO1/USART2_CTS/PA0) (type BiDi))
        (pin (num 11) (name ADC_IN1/TIM2_CH2/TSC_G1_IO2/USART2_DE/USART2_RTS/PA1) (type BiDi))
        (pin (num 12) (name ADC_IN2/SYS_WKUP4/TIM2_CH3/TSC_G1_IO3/USART2_TX/PA2) (type BiDi))
        (pin (num 13) (name ADC_IN3/TIM2_CH4/TSC_G1_IO4/USART2_RX/PA3) (type BiDi))
        (pin (num 14) (name ADC_IN4/I2S1_WS/SPI1_NSS/TIM14_CH1/TSC_G2_IO1/USART2_CK/USB_OE/PA4) (type BiDi))
        (pin (num 15) (name ADC_IN5/CEC/I2S1_CK/SPI1_SCK/TIM2_CH1/TIM2_ETR/TSC_G2_IO2/PA5) (type BiDi))
        (pin (num 16) (name ADC_IN6/I2S1_MCK/SPI1_MISO/TIM16_CH1/TIM1_BKIN/TIM3_CH1/TSC_G2_IO3/PA6) (type BiDi))
        (pin (num 17) (name ADC_IN7/I2S1_SD/SPI1_MOSI/TIM14_CH1/TIM17_CH1/TIM1_CH1N/TIM3_CH2/TSC_G2_IO4/PA7) (type BiDi))
        (pin (num 18) (name PB0/ADC_IN8/TIM1_CH2N/TIM3_CH3/TSC_G3_IO2) (type BiDi))
        (pin (num 19) (name PB1/ADC_IN9/TIM14_CH1/TIM1_CH3N/TIM3_CH4/TSC_G3_IO3) (type BiDi))
        (pin (num 20) (name PB2/TSC_G3_IO4) (type BiDi))
        (pin (num 21) (name PB10/CEC/I2C1_SCL/SPI2_SCK/TIM2_CH3/TSC_SYNC) (type BiDi))
        (pin (num 22) (name PB11/I2C1_SDA/TIM2_CH4) (type BiDi))
        (pin (num 23) (name VSS) (type power_in))
        (pin (num 24) (name VDD) (type power_in))
        (pin (num 25) (name PB12/SPI2_NSS/TIM1_BKIN) (type BiDi))
        (pin (num 26) (name PB13/I2C1_SCL/SPI2_SCK/TIM1_CH1N) (type BiDi))
        (pin (num 27) (name PB14/I2C1_SDA/SPI2_MISO/TIM1_CH2N) (type BiDi))
        (pin (num 28) (name PB15/RTC_REFIN/SPI2_MOSI/SYS_WKUP7/TIM1_CH3N) (type BiDi))
        (pin (num 29) (name CRS_SYNC/RCC_MCO/TIM1_CH1/USART1_CK/PA8) (type BiDi))
        (pin (num 30) (name I2C1_SCL/TIM1_CH2/TSC_G4_IO1/USART1_TX/PA9) (type BiDi))
        (pin (num 31) (name I2C1_SDA/TIM17_BKIN/TIM1_CH3/TSC_G4_IO2/USART1_RX/PA10) (type BiDi))
        (pin (num 32) (name CAN_RX/I2C1_SCL/TIM1_CH4/TSC_G4_IO3/USART1_CTS/USB_DM/PA11) (type BiDi))
        (pin (num 33) (name CAN_TX/I2C1_SDA/TIM1_ETR/TSC_G4_IO4/USART1_DE/USART1_RTS/USB_DP/PA12) (type BiDi))
        (pin (num 34) (name IR_OUT/SYS_SWDIO/USB_OE/PA13) (type BiDi))
        (pin (num 35) (name VSS) (type power_in))
        (pin (num 36) (name VDDIO2) (type power_in))
        (pin (num 37) (name SYS_SWCLK/USART2_TX/PA14) (type BiDi))
        (pin (num 38) (name I2S1_WS/SPI1_NSS/TIM2_CH1/TIM2_ETR/USART2_RX/USB_OE/PA15) (type BiDi))
        (pin (num 39) (name PB3/I2S1_CK/SPI1_SCK/TIM2_CH2/TSC_G5_IO1) (type BiDi))
        (pin (num 40) (name PB4/I2S1_MCK/SPI1_MISO/TIM17_BKIN/TIM3_CH1/TSC_G5_IO2) (type BiDi))
        (pin (num 41) (name PB5/I2C1_SMBA/I2S1_SD/SPI1_MOSI/SYS_WKUP6/TIM16_BKIN/TIM3_CH2) (type BiDi))
        (pin (num 42) (name PB6/I2C1_SCL/TIM16_CH1N/TSC_G5_IO3/USART1_TX) (type BiDi))
        (pin (num 43) (name PB7/I2C1_SDA/TIM17_CH1N/TSC_G5_IO4/USART1_RX) (type BiDi))
        (pin (num 44) (name PF11) (type BiDi))
        (pin (num 45) (name PB8/CAN_RX/CEC/I2C1_SCL/TIM16_CH1/TSC_SYNC) (type BiDi))
        (pin (num 46) (name PB9/CAN_TX/I2C1_SDA/IR_OUT/SPI2_NSS/TIM17_CH1) (type BiDi))
        (pin (num 47) (name VSS) (type power_in))
        (pin (num 48) (name VDD) (type power_in))))
    (libpart (lib stm32-cache) (part SW_Push)
      (fields
        (field (name Reference) SW)
        (field (name Value) SW_Push))
      (pins
        (pin (num 1) (name 1) (type passive))
        (pin (num 2) (name 2) (type passive))))
    (libpart (lib stm32-cache) (part TPS2051)
      (fields
        (field (name Reference) U)
        (field (name Value) TPS2051))
      (pins
        (pin (num 1) (name GND) (type power_in))
        (pin (num 2) (name IN) (type power_in))
        (pin (num 3) (name IN) (type passive))
        (pin (num 4) (name EN) (type input))
        (pin (num 5) (name ~OC) (type output))
        (pin (num 6) (name OUT) (type passive))
        (pin (num 7) (name OUT) (type passive))
        (pin (num 8) (name OUT) (type power_out))))
    (libpart (lib stm32-cache) (part USB6B1)
      (footprints
        (fp SO8))
      (fields
        (field (name Reference) D)
        (field (name Value) USB6B1))
      (pins
        (pin (num 1) (name VCC) (type passive))
        (pin (num 2) (name I/O1) (type passive))
        (pin (num 3) (name I/O2) (type passive))
        (pin (num 4) (name GND) (type passive))
        (pin (num 5) (name GND) (type passive))
        (pin (num 6) (name I/O2) (type passive))
        (pin (num 7) (name I/O1) (type passive))
        (pin (num 8) (name VCC) (type passive))))
    (libpart (lib stm32-cache) (part USB_A-RESCUE-stm32)
      (footprints
        (fp USB*))
      (fields
        (field (name Reference) P)
        (field (name Value) USB_A-RESCUE-stm32))
      (pins
        (pin (num 1) (name VBUS) (type power_in))
        (pin (num 2) (name D-) (type passive))
        (pin (num 3) (name D+) (type passive))
        (pin (num 4) (name GND) (type power_in))
        (pin (num 5) (name shield) (type passive)))))
  (libraries
    (library (logical stm32-rescue)
      (uri stm32-rescue.lib))
    (library (logical stm32-cache)
      (uri /home/eddy/Dropbox/Projects/tsys01/kicad/stm32/stm32-cache.lib)))
  (nets
    (net (code 1) (name /C7)
      (node (ref U6) (pin 4))
      (node (ref R25) (pin 1))
      (node (ref P9) (pin 2)))
    (net (code 2) (name /C4)
      (node (ref R19) (pin 1))
      (node (ref P6) (pin 2))
      (node (ref U6) (pin 1)))
    (net (code 3) (name /C5)
      (node (ref R21) (pin 1))
      (node (ref P7) (pin 2))
      (node (ref U6) (pin 5)))
    (net (code 4) (name /C6)
      (node (ref U6) (pin 2))
      (node (ref P8) (pin 2))
      (node (ref R23) (pin 1)))
    (net (code 5) (name GND)
      (node (ref J1) (pin 5))
      (node (ref J1) (pin 1))
      (node (ref P14) (pin 6))
      (node (ref P14) (pin 7))
      (node (ref P14) (pin 8))
      (node (ref U9) (pin 4))
      (node (ref U5) (pin 7))
      (node (ref C2) (pin 2))
      (node (ref SW1) (pin 2))
      (node (ref C5) (pin 2))
      (node (ref U9) (pin 1))
      (node (ref R27) (pin 2))
      (node (ref J1) (pin 3))
      (node (ref C8) (pin 2))
      (node (ref D11) (pin 2))
      (node (ref Q1) (pin 1))
      (node (ref P13) (pin 5))
      (node (ref P12) (pin 1))
      (node (ref P1) (pin 8))
      (node (ref R8) (pin 2))
      (node (ref P3) (pin 4))
      (node (ref C4) (pin 2))
      (node (ref U5) (pin 8))
      (node (ref U4) (pin 2))
      (node (ref D1) (pin 2))
      (node (ref P1) (pin 6))
      (node (ref P1) (pin 7))
      (node (ref D10) (pin 2))
      (node (ref D9) (pin 2))
      (node (ref D8) (pin 2))
      (node (ref P2) (pin 4))
      (node (ref C15) (pin 2))
      (node (ref D3) (pin 3))
      (node (ref D7) (pin 5))
      (node (ref R5) (pin 1))
      (node (ref C9) (pin 2))
      (node (ref P4) (pin 4))
      (node (ref R7) (pin 2))
      (node (ref C13) (pin 1))
      (node (ref C14) (pin 1))
      (node (ref R31) (pin 2))
      (node (ref P5) (pin 4))
      (node (ref C1) (pin 2))
      (node (ref P6) (pin 4))
      (node (ref P8) (pin 4))
      (node (ref C11) (pin 1))
      (node (ref U1) (pin 3))
      (node (ref U6) (pin 7))
      (node (ref U6) (pin 8))
      (node (ref U7) (pin 47))
      (node (ref P9) (pin 4))
      (node (ref U7) (pin 35))
      (node (ref P7) (pin 4))
      (node (ref U8) (pin 1))
      (node (ref U1) (pin 5))
      (node (ref U2) (pin 1))
      (node (ref U7) (pin 23))
      (node (ref C12) (pin 1))
      (node (ref U3) (pin 1))
      (node (ref C7) (pin 1))
      (node (ref R2) (pin 2))
      (node (ref C3) (pin 2))
      (node (ref U7) (pin 8))
      (node (ref R4) (pin 2)))
    (net (code 6) (name "Net-(R31-Pad1)")
      (node (ref U9) (pin 8))
      (node (ref R31) (pin 1))
      (node (ref R36) (pin 2)))
    (net (code 7) (name "Net-(U9-Pad5)")
      (node (ref U9) (pin 5)))
    (net (code 8) (name "Net-(R8-Pad1)")
      (node (ref U4) (pin 8))
      (node (ref R8) (pin 1)))
    (net (code 9) (name /T_pow_EN)
      (node (ref U8) (pin 4))
      (node (ref U7) (pin 29)))
    (net (code 10) (name /T_overcurnt)
      (node (ref U7) (pin 39))
      (node (ref U8) (pin 5))
      (node (ref R26) (pin 1)))
    (net (code 11) (name /12Vin)
      (node (ref R3) (pin 1))
      (node (ref Q1) (pin 2))
      (node (ref U9) (pin 3))
      (node (ref U9) (pin 2)))
    (net (code 12) (name /12Vout)
      (node (ref U1) (pin 1))
      (node (ref U9) (pin 6))
      (node (ref C1) (pin 1))
      (node (ref U9) (pin 7))
      (node (ref C15) (pin 1)))
    (net (code 13) (name "Net-(D5-Pad2)")
      (node (ref R29) (pin 1))
      (node (ref D5) (pin 2)))
    (net (code 14) (name /LED1)
      (node (ref D6) (pin 1))
      (node (ref U7) (pin 22)))
    (net (code 15) (name "Net-(D6-Pad2)")
      (node (ref R30) (pin 1))
      (node (ref D6) (pin 2)))
    (net (code 16) (name "Net-(D2-Pad1)")
      (node (ref D2) (pin 1))
      (node (ref R5) (pin 2)))
    (net (code 17) (name "Net-(D7-Pad1)")
      (node (ref P13) (pin 1))
      (node (ref D7) (pin 1)))
    (net (code 18) (name "Net-(D7-Pad4)")
      (node (ref D7) (pin 4))
      (node (ref P13) (pin 4)))
    (net (code 19) (name "Net-(JP1-Pad2)")
      (node (ref JP1) (pin 2))
      (node (ref R9) (pin 2)))
    (net (code 20) (name /CAN_Tx)
      (node (ref U7) (pin 46))
      (node (ref U4) (pin 1)))
    (net (code 21) (name /CAN_Rx)
      (node (ref U4) (pin 4))
      (node (ref U7) (pin 45)))
    (net (code 22) (name "Net-(R34-Pad2)")
      (node (ref R34) (pin 2))
      (node (ref U7) (pin 32)))
    (net (code 23) (name "Net-(R35-Pad2)")
      (node (ref U7) (pin 33))
      (node (ref R35) (pin 2)))
    (net (code 24) (name "Net-(D7-Pad3)")
      (node (ref D7) (pin 3))
      (node (ref P13) (pin 3)))
    (net (code 25) (name "Net-(D7-Pad2)")
      (node (ref P13) (pin 2))
      (node (ref D7) (pin 2)))
    (net (code 26) (name "Net-(D3-Pad1)")
      (node (ref U4) (pin 7))
      (node (ref P1) (pin 4))
      (node (ref D3) (pin 1))
      (node (ref P14) (pin 4))
      (node (ref JP1) (pin 1)))
    (net (code 27) (name "Net-(D3-Pad2)")
      (node (ref P14) (pin 5))
      (node (ref R9) (pin 1))
      (node (ref U4) (pin 6))
      (node (ref P1) (pin 5))
      (node (ref D3) (pin 2)))
    (net (code 28) (name /brdaddr0)
      (node (ref J1) (pin 2))
      (node (ref U7) (pin 34)))
    (net (code 29) (name /brdaddr1)
      (node (ref U7) (pin 37))
      (node (ref J1) (pin 4)))
    (net (code 30) (name /brdaddr2)
      (node (ref U7) (pin 38))
      (node (ref J1) (pin 6)))
    (net (code 31) (name "Net-(U7-Pad5)")
      (node (ref U7) (pin 5)))
    (net (code 32) (name +5V)
      (node (ref R6) (pin 1))
      (node (ref U2) (pin 3))
      (node (ref U3) (pin 3))
      (node (ref C8) (pin 1))
      (node (ref U1) (pin 4))
      (node (ref U4) (pin 3))
      (node (ref L1) (pin 1))
      (node (ref C4) (pin 1))
      (node (ref D4) (pin 1)))
    (net (code 33) (name "Net-(C3-Pad1)")
      (node (ref C3) (pin 1))
      (node (ref U3) (pin 4))
      (node (ref U3) (pin 2))
      (node (ref C7) (pin 2))
      (node (ref U8) (pin 3))
      (node (ref U8) (pin 2)))
    (net (code 34) (name "Net-(U7-Pad6)")
      (node (ref U7) (pin 6)))
    (net (code 35) (name "Net-(P12-Pad2)")
      (node (ref U7) (pin 31))
      (node (ref P12) (pin 2)))
    (net (code 36) (name "Net-(P12-Pad3)")
      (node (ref U7) (pin 30))
      (node (ref P12) (pin 3)))
    (net (code 37) (name "Net-(U7-Pad12)")
      (node (ref U7) (pin 12)))
    (net (code 38) (name /I12V)
      (node (ref R36) (pin 1))
      (node (ref U7) (pin 13))
      (node (ref C9) (pin 1)))
    (net (code 39) (name "Net-(U7-Pad14)")
      (node (ref U7) (pin 14)))
    (net (code 40) (name "Net-(U7-Pad15)")
      (node (ref U7) (pin 15)))
    (net (code 41) (name "Net-(U7-Pad17)")
      (node (ref U7) (pin 17)))
    (net (code 42) (name "Net-(U7-Pad28)")
      (node (ref U7) (pin 28)))
    (net (code 43) (name "Net-(U7-Pad27)")
      (node (ref U7) (pin 27)))
    (net (code 44) (name "Net-(U7-Pad26)")
      (node (ref U7) (pin 26)))
    (net (code 45) (name "Net-(U7-Pad40)")
      (node (ref U7) (pin 40)))
    (net (code 46) (name "Net-(U7-Pad4)")
      (node (ref U7) (pin 4)))
    (net (code 47) (name "Net-(U7-Pad3)")
      (node (ref U7) (pin 3)))
    (net (code 48) (name "Net-(U7-Pad2)")
      (node (ref U7) (pin 2)))
    (net (code 49) (name /V5)
      (node (ref D9) (pin 1))
      (node (ref U7) (pin 11))
      (node (ref R6) (pin 2))
      (node (ref R7) (pin 1)))
    (net (code 50) (name /3v3_sensors)
      (node (ref R1) (pin 1))
      (node (ref P4) (pin 3))
      (node (ref P9) (pin 3))
      (node (ref P8) (pin 3))
      (node (ref P7) (pin 3))
      (node (ref P6) (pin 3))
      (node (ref U8) (pin 6))
      (node (ref U8) (pin 7))
      (node (ref U8) (pin 8))
      (node (ref P5) (pin 3))
      (node (ref P2) (pin 3))
      (node (ref P3) (pin 3)))
    (net (code 51) (name /V3.3)
      (node (ref U7) (pin 16))
      (node (ref R2) (pin 1))
      (node (ref R1) (pin 2)))
    (net (code 52) (name /V12)
      (node (ref U7) (pin 10))
      (node (ref R3) (pin 2))
      (node (ref R4) (pin 1))
      (node (ref D8) (pin 1)))
    (net (code 53) (name "Net-(D7-Pad7)")
      (node (ref R34) (pin 1))
      (node (ref D7) (pin 7)))
    (net (code 54) (name "Net-(D7-Pad6)")
      (node (ref D7) (pin 6))
      (node (ref R35) (pin 1)))
    (net (code 55) (name "Net-(R32-Pad1)")
      (node (ref U5) (pin 3))
      (node (ref R32) (pin 1)))
    (net (code 56) (name "Net-(R33-Pad1)")
      (node (ref R33) (pin 1))
      (node (ref U6) (pin 3)))
    (net (code 57) (name /C3)
      (node (ref U6) (pin 12))
      (node (ref P5) (pin 2))
      (node (ref R17) (pin 1)))
    (net (code 58) (name /C0)
      (node (ref R11) (pin 1))
      (node (ref P2) (pin 2))
      (node (ref U6) (pin 13)))
    (net (code 59) (name /C1)
      (node (ref R13) (pin 1))
      (node (ref P3) (pin 2))
      (node (ref U6) (pin 14)))
    (net (code 60) (name /C2)
      (node (ref R15) (pin 1))
      (node (ref U6) (pin 15))
      (node (ref P4) (pin 2)))
    (net (code 61) (name /D4)
      (node (ref P6) (pin 1))
      (node (ref R18) (pin 1))
      (node (ref U5) (pin 1)))
    (net (code 62) (name /D6)
      (node (ref U5) (pin 2))
      (node (ref R22) (pin 1))
      (node (ref P8) (pin 1)))
    (net (code 63) (name /D7)
      (node (ref U5) (pin 4))
      (node (ref R24) (pin 1))
      (node (ref P9) (pin 1)))
    (net (code 64) (name /D5)
      (node (ref R20) (pin 1))
      (node (ref U5) (pin 5))
      (node (ref P7) (pin 1)))
    (net (code 65) (name /D3)
      (node (ref R16) (pin 1))
      (node (ref U5) (pin 12))
      (node (ref P5) (pin 1)))
    (net (code 66) (name /D0)
      (node (ref R10) (pin 1))
      (node (ref P2) (pin 1))
      (node (ref U5) (pin 13)))
    (net (code 67) (name /D1)
      (node (ref R12) (pin 1))
      (node (ref U5) (pin 14))
      (node (ref P3) (pin 1)))
    (net (code 68) (name /D2)
      (node (ref R14) (pin 1))
      (node (ref P4) (pin 1))
      (node (ref U5) (pin 15)))
    (net (code 69) (name /5Vusb)
      (node (ref D7) (pin 8))
      (node (ref D4) (pin 2)))
    (net (code 70) (name "Net-(U4-Pad5)")
      (node (ref U4) (pin 5)))
    (net (code 71) (name "Net-(U7-Pad1)")
      (node (ref U7) (pin 1)))
    (net (code 72) (name "Net-(U7-Pad41)")
      (node (ref U7) (pin 41)))
    (net (code 73) (name /~EN)
      (node (ref U7) (pin 25))
      (node (ref U6) (pin 6))
      (node (ref U5) (pin 6)))
    (net (code 74) (name /ADDR0)
      (node (ref U7) (pin 18))
      (node (ref U5) (pin 11))
      (node (ref U6) (pin 11)))
    (net (code 75) (name /BOOT0)
      (node (ref C6) (pin 1))
      (node (ref R27) (pin 1))
      (node (ref SW2) (pin 1))
      (node (ref U7) (pin 44)))
    (net (code 76) (name /ADDR1)
      (node (ref U5) (pin 10))
      (node (ref U6) (pin 10))
      (node (ref U7) (pin 19)))
    (net (code 77) (name /LED0)
      (node (ref D5) (pin 1))
      (node (ref U7) (pin 21)))
    (net (code 78) (name /NRST)
      (node (ref R28) (pin 1))
      (node (ref C5) (pin 1))
      (node (ref SW1) (pin 1))
      (node (ref U7) (pin 7)))
    (net (code 79) (name +3V3)
      (node (ref R18) (pin 2))
      (node (ref R19) (pin 2))
      (node (ref C2) (pin 1))
      (node (ref R17) (pin 2))
      (node (ref R26) (pin 2))
      (node (ref R16) (pin 2))
      (node (ref R14) (pin 2))
      (node (ref R15) (pin 2))
      (node (ref R11) (pin 2))
      (node (ref R23) (pin 2))
      (node (ref R10) (pin 2))
      (node (ref U2) (pin 2))
      (node (ref U7) (pin 9))
      (node (ref R12) (pin 2))
      (node (ref R13) (pin 2))
      (node (ref R20) (pin 2))
      (node (ref C11) (pin 2))
      (node (ref U7) (pin 24))
      (node (ref U7) (pin 48))
      (node (ref U7) (pin 36))
      (node (ref C14) (pin 2))
      (node (ref R22) (pin 2))
      (node (ref R21) (pin 2))
      (node (ref R29) (pin 2))
      (node (ref U6) (pin 16))
      (node (ref R24) (pin 2))
      (node (ref R25) (pin 2))
      (node (ref SW2) (pin 2))
      (node (ref D2) (pin 2))
      (node (ref C6) (pin 2))
      (node (ref R28) (pin 2))
      (node (ref R30) (pin 2))
      (node (ref U2) (pin 4))
      (node (ref U5) (pin 16))
      (node (ref C13) (pin 2))
      (node (ref C12) (pin 2)))
    (net (code 80) (name /ADDR2)
      (node (ref U7) (pin 20))
      (node (ref U5) (pin 9))
      (node (ref U6) (pin 9)))
    (net (code 81) (name /I2C1_SCL)
      (node (ref U7) (pin 42))
      (node (ref R33) (pin 2))
      (node (ref D11) (pin 1)))
    (net (code 82) (name "Net-(D1-Pad1)")
      (node (ref L1) (pin 2))
      (node (ref D1) (pin 1))
      (node (ref U1) (pin 2)))
    (net (code 83) (name "Net-(P1-Pad1)")
      (node (ref P14) (pin 3))
      (node (ref P14) (pin 2))
      (node (ref P14) (pin 1))
      (node (ref P1) (pin 2))
      (node (ref P1) (pin 1))
      (node (ref P1) (pin 3))
      (node (ref Q1) (pin 3)))
    (net (code 84) (name "Net-(P16-Pad1)")
      (node (ref P16) (pin 1)))
    (net (code 85) (name "Net-(P17-Pad1)")
      (node (ref P17) (pin 1)))
    (net (code 86) (name "Net-(P18-Pad1)")
      (node (ref P18) (pin 1)))
    (net (code 87) (name "Net-(P15-Pad1)")
      (node (ref P15) (pin 1)))
    (net (code 88) (name /I2C1_SDA)
      (node (ref R32) (pin 2))
      (node (ref D10) (pin 1))
      (node (ref U7) (pin 43)))))