## KiBoM PCB Bill of Materials

Source File | /Big/Data/00__Electronics/STM32/TSYS01/git/kicad/stm32/stm32.sch
BoM Date | 10 2018 21:51:15
Schematic Version |
Schematic Date |
KiCad Version | Eeschema 4.0.7
Component Groups | 38
Component Count (per PCB) | 92
Fitted Components (per PCB) | 92
Number of PCBs | 1
Total Component Count (for 1 PCBs) | 92

## Component Groups

Kicad Fields (default)

Generated Fields

User Fields

Empty Fields

| Description | Part | References | Value | Footprint | Quantity Per PCB | Datasheet | Manufacturer
--- | --- | --- | --- | --- | --- | --- | --- | ---
1 |  | C | C5 C6 C7 C8 C9 C11 C12 C13 C14 C15 | 0.1 | C_0603_1608Metric_Pad0.84x1.00mm_HandSolder | 10 |  |
2 |  | CP | C4 | 100u | CP_Radial_D8.0mm_P3.50mm | 1 |  |
3 |  | CP | C1 C2 C3 | 47u | CP_EIA-3216-18_Kemet-A_Pad1.53x1.40mm_HandSolder | 3 |  |
4 |  | D | D1 | 1n5822 | D_DO-201_P12.70mm_Horizontal | 1 |  |
5 |  | LED-RESCUE-stm32 | D2 | LED | LED_0805_2012Metric_Pad0.97x1.50mm_HandSolder | 1 |  |
6 |  | LED-RESCUE-stm32 | D5 | LED0 | LED_0805_2012Metric_Pad0.97x1.50mm_HandSolder | 1 |  |
7 |  | LED-RESCUE-stm32 | D6 | LED1 | LED_0805_2012Metric_Pad0.97x1.50mm_HandSolder | 1 |  |
8 |  | D_Schottky | D4 | MBRS130L | D_SMB_Handsoldering | 1 |  |
9 |  | D_Zener | D8 D9 D10 D11 | MM3Z3V6 | D_0805_2012Metric_Pad0.97x1.50mm_HandSolder | 4 |  |
10 |  | PESD1CAN | D3 | PESD1CAN | SOT-23 | 1 |  |
11 |  | USB6B1 | D7 | USB6B1 | SOIC-8_3.9x4.9mm_P1.27mm | 1 |  |
12 |  | CONN_02X03 | J1 | CONN_02X03 | PinHeader_2x03_P2.54mm_Vertical | 1 |  |
13 |  | Jumper_NO_Small | JP1 | Terminal | PinHeader_1x02_P2.54mm_Vertical | 1 |  |
14 |  | L | L1 | 100u | C_Rect_L9.0mm_W2.5mm_P7.50mm_MKT | 1 |  |
15 |  | CONN_01X01 | P15 P16 P17 P18 | Hole | Hole_3mm | 4 |  |
16 |  | CONN_01X08 | P1 P14 | RJ45-CAN_power | RJ45_8 | 2 |  |
17 |  | CONN_01X04 | P2 P3 P4 P5 P6 P7 P8 P9 | RJ9-sensor | RJ9-4P4C | 8 |  |
18 |  | CONN_01X03 | P12 | USART_BOOT | PinHeader_1x03_P2.54mm_Vertical | 1 |  |
19 |  | USB_A-RESCUE-stm32 | P13 | USB_A | USB_Mini-B_Lumber_2486_Horizontal | 1 |  |
20 |  | Q_PMOS_GSD | Q1 | AO3407 | SOT-23_Handsoldering | 1 |  |
21 |  | R | R26 R27 R28 R36 | 10k | R_0603_1608Metric_Pad0.84x1.00mm_HandSolder | 4 |  |
22 |  | R | R9 | 120 | R_0603_1608Metric_Pad0.84x1.00mm_HandSolder | 1 |  |
23 |  | R | R32 R33 R34 R35 | 22 | R_0603_1608Metric_Pad0.84x1.00mm_HandSolder | 4 |  |
24 |  | R | R3 | 220k | R_0603_1608Metric_Pad0.84x1.00mm_HandSolder | 1 |  |
25 |  | R | R31 | 2k 1% | R_0603_1608Metric_Pad0.84x1.00mm_HandSolder | 1 |  |
26 |  | R | R5 R29 R30 | 330 | R_0603_1608Metric_Pad0.84x1.00mm_HandSolder | 3 |  |
27 |  | R | R1 R2 R6 R7 | 47k | R_0603_1608Metric_Pad0.84x1.00mm_HandSolder | 4 |  |
28 |  | R | R8 R10 R11 R12 R13 R14 R15 R16 R17 R18 R19 R20 R21 R22 R23 R24 R25 | 4k7 | R_0603_1608Metric_Pad0.84x1.00mm_HandSolder | 17 |  |
29 |  | R | R4 | 56k | R_0603_1608Metric_Pad0.84x1.00mm_HandSolder | 1 |  |
30 |  | SW_Push | SW2 | Boot | SW_SPST_FSMSM | 1 |  |
31 |  | SW_Push | SW1 | Reset | SW_SPST_FSMSM | 1 |  |
32 |  | 74HC4051 | U5 U6 | 74HC4051 | SOIC-16_3.9x9.9mm_P1.27mm | 2 |  |
33 |  | LM1117-3.3-RESCUE-stm32 | U2 U3 | LM1117-3.3 | SOT-223 | 2 |  |
34 |  | LM2576HV | U1 | LM2576HV | TO-220-5_Vertical_StaggeredType2 | 1 |  | Texas Instruments
35 |  | MAX471-RESCUE-stm32 | U9 | MAX471 | SOIC-8_3.9x4.9mm_P1.27mm | 1 |  |
36 |  | MCP2551-I/SN | U4 | MCP2551-I/SN | SOIC-8_3.9x4.9mm_P1.27mm | 1 |  |
37 |  | STM32F042C6Tx | U7 | STM32F042C6Tx | LQFP-48_7x7mm_P0.5mm | 1 |  |
38 |  | TPS2051 | U8 | TPS2051 | SOIC-8_3.9x4.9mm_P1.27mm | 1 |  |