(export (version D)
  (design
    (source /home/eddy/Docs/SAO/BTA/MIRROR_CONTROL_termo/Project/kicad/RJ45_plate/RJ45_plate.sch)
    (date "Пн 06 авг 2018 17:42:20")
    (tool "Eeschema 4.0.7")
    (sheet (number 1) (name /) (tstamps /)
      (title_block
        (title)
        (company)
        (rev)
        (date)
        (source RJ45_plate.sch)
        (comment (number 1) (value ""))
        (comment (number 2) (value ""))
        (comment (number 3) (value ""))
        (comment (number 4) (value "")))))
  (components
    (comp (ref J2)
      (value RJ45)
      (footprint RJ45:RJ45)
      (libsource (lib conn) (part Conn_01x08))
      (sheetpath (names /) (tstamps /))
      (tstamp 5B67DE38))
    (comp (ref J3)
      (value RJ45)
      (footprint RJ45:RJ45)
      (libsource (lib conn) (part Conn_01x08))
      (sheetpath (names /) (tstamps /))
      (tstamp 5B67DF3D))
    (comp (ref J1)
      (value Conn_01x04)
      (footprint Connector_PinHeader_2.54mm.pretty:PinHeader_1x04_P2.54mm_Vertical)
      (libsource (lib conn) (part Conn_01x04))
      (sheetpath (names /) (tstamps /))
      (tstamp 5B67E004))
    (comp (ref F1)
      (value Fuse)
      (footprint RJ45:FUSE)
      (libsource (lib device) (part Fuse))
      (sheetpath (names /) (tstamps /))
      (tstamp 5B685A07)))
  (libparts
    (libpart (lib conn) (part Conn_01x04)
      (description "Generic connector, single row, 01x04")
      (docs ~)
      (footprints
        (fp Connector*:*_??x*mm*)
        (fp Connector*:*1x??x*mm*)
        (fp Pin?Header?Straight?1X*)
        (fp Pin?Header?Angled?1X*)
        (fp Socket?Strip?Straight?1X*)
        (fp Socket?Strip?Angled?1X*))
      (fields
        (field (name Reference) J)
        (field (name Value) Conn_01x04))
      (pins
        (pin (num 1) (name Pin_1) (type passive))
        (pin (num 2) (name Pin_2) (type passive))
        (pin (num 3) (name Pin_3) (type passive))
        (pin (num 4) (name Pin_4) (type passive))))
    (libpart (lib conn) (part Conn_01x08)
      (description "Generic connector, single row, 01x08")
      (docs ~)
      (footprints
        (fp Connector*:*_??x*mm*)
        (fp Connector*:*1x??x*mm*)
        (fp Pin?Header?Straight?1X*)
        (fp Pin?Header?Angled?1X*)
        (fp Socket?Strip?Straight?1X*)
        (fp Socket?Strip?Angled?1X*))
      (fields
        (field (name Reference) J)
        (field (name Value) Conn_01x08))
      (pins
        (pin (num 1) (name Pin_1) (type passive))
        (pin (num 2) (name Pin_2) (type passive))
        (pin (num 3) (name Pin_3) (type passive))
        (pin (num 4) (name Pin_4) (type passive))
        (pin (num 5) (name Pin_5) (type passive))
        (pin (num 6) (name Pin_6) (type passive))
        (pin (num 7) (name Pin_7) (type passive))
        (pin (num 8) (name Pin_8) (type passive))))
    (libpart (lib device) (part Fuse)
      (description "Fuse, generic")
      (footprints
        (fp *Fuse*))
      (fields
        (field (name Reference) F)
        (field (name Value) Fuse))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive)))))
  (libraries
    (library (logical conn)
      (uri /usr/share/kicad/library/conn.lib))
    (library (logical device)
      (uri /usr/share/kicad/library/device.lib)))
  (nets
    (net (code 1) (name "Net-(J1-Pad1)")
      (node (ref J2) (pin 8))
      (node (ref J3) (pin 7))
      (node (ref J3) (pin 8))
      (node (ref J2) (pin 7))
      (node (ref J2) (pin 6))
      (node (ref J1) (pin 1))
      (node (ref J3) (pin 6)))
    (net (code 2) (name "Net-(J1-Pad3)")
      (node (ref J1) (pin 3))
      (node (ref J2) (pin 4))
      (node (ref J3) (pin 4)))
    (net (code 3) (name "Net-(J1-Pad2)")
      (node (ref J3) (pin 5))
      (node (ref J1) (pin 2))
      (node (ref J2) (pin 5)))
    (net (code 4) (name "Net-(F1-Pad1)")
      (node (ref J2) (pin 3))
      (node (ref J2) (pin 1))
      (node (ref J3) (pin 3))
      (node (ref J3) (pin 2))
      (node (ref J3) (pin 1))
      (node (ref F1) (pin 1))
      (node (ref J2) (pin 2)))
    (net (code 5) (name "Net-(F1-Pad2)")
      (node (ref F1) (pin 2))
      (node (ref J1) (pin 4)))))