(export (version D)
  (design
    (source /home/eddy/Docs/SAO/BTA/MIRROR_CONTROL_termo/Project/termorez_NX3L4051/termorez.sch)
    (date "Вт 10 июл 2018 14:30:35")
    (tool "Eeschema 4.0.7")
    (sheet (number 1) (name /) (tstamps /)
      (title_block
        (title noname.sch)
        (company)
        (rev)
        (date "27 dec 2014")
        (source termorez.sch)
        (comment (number 1) (value ""))
        (comment (number 2) (value ""))
        (comment (number 3) (value ""))
        (comment (number 4) (value "")))))
  (components
    (comp (ref U4)
      (value AD7794/7795)
      (libsource (lib my_elements) (part AD7794/7795))
      (sheetpath (names /) (tstamps /))
      (tstamp 524D62C1))
    (comp (ref R4)
      (value "1k 0.1% (RT0805BRB071KL)")
      (footprint SM0805)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 53562118))
    (comp (ref C12)
      (value 47u)
      (footprint Capacitor_Tantalum_SMD.pretty:CP_EIA-3216-12_Kemet-S)
      (libsource (lib device) (part CP1))
      (sheetpath (names /) (tstamps /))
      (tstamp 5357750C))
    (comp (ref L1)
      (value BMB2A0300AN1)
      (libsource (lib termorez-cache) (part INDUCTOR_SMALL))
      (sheetpath (names /) (tstamps /))
      (tstamp 53577523))
    (comp (ref C9)
      (value 0.1u)
      (footprint Capacitor_SMD.pretty:C_0603_1608Metric_Pad0.99x1.00mm_HandSolder)
      (libsource (lib device) (part C))
      (sheetpath (names /) (tstamps /))
      (tstamp 53576FB6))
    (comp (ref C8)
      (value 0.1u)
      (footprint Capacitor_SMD.pretty:C_0603_1608Metric_Pad0.99x1.00mm_HandSolder)
      (libsource (lib device) (part C))
      (sheetpath (names /) (tstamps /))
      (tstamp 53576FC3))
    (comp (ref U5)
      (value LM1117-33)
      (footprint SOT-223)
      (libsource (lib termorez-rescue) (part LM317AEMP-RESCUE-termorez))
      (sheetpath (names /) (tstamps /))
      (tstamp 535787B7))
    (comp (ref R1)
      (value 10k)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 53579396))
    (comp (ref R2)
      (value 10k)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 535793A8))
    (comp (ref P1)
      (value conn1)
      (libsource (lib termorez-cache) (part CONN_8))
      (sheetpath (names /) (tstamps /))
      (tstamp 53579853))
    (comp (ref P6)
      (value 5V)
      (libsource (lib termorez-cache) (part CONN_2))
      (sheetpath (names /) (tstamps /))
      (tstamp 5357ABB4))
    (comp (ref P4)
      (value MCU)
      (libsource (lib termorez-cache) (part CONN_8))
      (sheetpath (names /) (tstamps /))
      (tstamp 5357BA72))
    (comp (ref R3)
      (value 47k)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 5357C8F8))
    (comp (ref P2)
      (value conn2a)
      (libsource (lib termorez-cache) (part CONN_8))
      (sheetpath (names /) (tstamps /))
      (tstamp 5475974D))
    (comp (ref P3)
      (value conn2b)
      (libsource (lib termorez-cache) (part CONN_8))
      (sheetpath (names /) (tstamps /))
      (tstamp 5475975B))
    (comp (ref DA1)
      (value NX3L4051-HX)
      (footprint HXQFN-16)
      (libsource (lib my_elements) (part NX3L4051-HX))
      (sheetpath (names /) (tstamps /))
      (tstamp 54759E36))
    (comp (ref DA3)
      (value NX3L4051-HX)
      (footprint HXQFN-16)
      (libsource (lib my_elements) (part NX3L4051-HX))
      (sheetpath (names /) (tstamps /))
      (tstamp 5475A2C7))
    (comp (ref DA2)
      (value NX3L4051-HX)
      (footprint HXQFN-16)
      (libsource (lib my_elements) (part NX3L4051-HX))
      (sheetpath (names /) (tstamps /))
      (tstamp 5475A2C1))
    (comp (ref C10)
      (value 1u)
      (libsource (lib device) (part C))
      (sheetpath (names /) (tstamps /))
      (tstamp 5357821E))
    (comp (ref R5)
      (value "1k 0.1% (RT0805BRB071KL)")
      (footprint SM0805)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 547C0DD9))
    (comp (ref R6)
      (value "1k 0.1% (RT0805BRB071KL)")
      (footprint SM0805)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 547C0DE4))
    (comp (ref R7)
      (value "1k 0.1% (RT0805BRB071KL)")
      (footprint SM0805)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 547C0DEA))
    (comp (ref R8)
      (value "1k 0.1% (RT0805BRB071KL)")
      (footprint SM0805)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 547C0DF0))
    (comp (ref X1)
      (value GND_CONNECTOR)
      (footprint GND_CONNECTOR)
      (libsource (lib my_elements) (part GND_CONNECTOR))
      (sheetpath (names /) (tstamps /))
      (tstamp 549EDA1E)))
  (libparts
    (libpart (lib my_elements) (part AD7794/7795)
      (footprints
        (fp TSSOP24)
        (fp SSOP24))
      (fields
        (field (name Reference) U)
        (field (name Value) AD7794/7795)
        (field (name Footprint) TSSOP24))
      (pins
        (pin (num 1) (name SCLK) (type passive))
        (pin (num 2) (name CLC) (type passive))
        (pin (num 3) (name !CS) (type passive))
        (pin (num 5) (name "AIN6(+)/P1") (type BiDi))
        (pin (num 6) (name "AIN6(-)/P2") (type BiDi))
        (pin (num 7) (name "AIN1(+)") (type input))
        (pin (num 8) (name "AIN1(-)") (type input))
        (pin (num 9) (name "AIN2(+)") (type input))
        (pin (num 10) (name "AIN2(-)") (type input))
        (pin (num 11) (name "AIN3(+)") (type input))
        (pin (num 12) (name "AIN3(-)") (type input))
        (pin (num 13) (name "REFIN1(+)") (type input))
        (pin (num 14) (name "REFIN1(-)") (type input))
        (pin (num 15) (name "AIN5(+)/IOUT2") (type input))
        (pin (num 16) (name "AIN5(-)/IOUT1") (type input))
        (pin (num 17) (name "AIN4(+)/REFIN2(+)") (type input))
        (pin (num 18) (name "AIN4(-)/REFIN2(-)") (type input))
        (pin (num 19) (name PSW) (type input))
        (pin (num 20) (name GND) (type power_in))
        (pin (num 21) (name AVDD) (type power_in))
        (pin (num 22) (name DVDD) (type power_in))
        (pin (num 23) (name DOUT/!RDY) (type passive))
        (pin (num 24) (name DIN) (type passive))))
    (libpart (lib device) (part C)
      (description "Unpolarized capacitor")
      (footprints
        (fp C_*))
      (fields
        (field (name Reference) C)
        (field (name Value) C))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib termorez-cache) (part CONN_2)
      (fields
        (field (name Reference) P)
        (field (name Value) CONN_2))
      (pins
        (pin (num 1) (name P1) (type passive))
        (pin (num 2) (name PM) (type passive))))
    (libpart (lib termorez-cache) (part CONN_8)
      (fields
        (field (name Reference) P)
        (field (name Value) CONN_8))
      (pins
        (pin (num 1) (name P1) (type passive))
        (pin (num 2) (name P2) (type passive))
        (pin (num 3) (name P3) (type passive))
        (pin (num 4) (name P4) (type passive))
        (pin (num 5) (name P5) (type passive))
        (pin (num 6) (name P6) (type passive))
        (pin (num 7) (name P7) (type passive))
        (pin (num 8) (name P8) (type passive))))
    (libpart (lib device) (part CP1)
      (description "Polarised capacitor")
      (footprints
        (fp CP_*))
      (fields
        (field (name Reference) C)
        (field (name Value) CP1))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib my_elements) (part GND_CONNECTOR)
      (footprints
        (fp GND_connector)
        (fp GND*))
      (fields
        (field (name Reference) X)
        (field (name Value) GND_CONNECTOR)
        (field (name Footprint) GND_connector))
      (pins
        (pin (num 1) (name GND1) (type passive))
        (pin (num 2) (name GND2) (type passive))))
    (libpart (lib termorez-cache) (part INDUCTOR_SMALL)
      (footprints
        (fp Choke_*)
        (fp *Coil*))
      (fields
        (field (name Reference) L)
        (field (name Value) INDUCTOR_SMALL))
      (pins
        (pin (num 1) (name 1) (type input))
        (pin (num 2) (name 2) (type input))))
    (libpart (lib termorez-rescue) (part LM317AEMP-RESCUE-termorez)
      (footprints
        (fp SOT*))
      (fields
        (field (name Reference) U)
        (field (name Value) LM317AEMP-RESCUE-termorez)
        (field (name Footprint) SOT-223))
      (pins
        (pin (num 1) (name ADJ) (type power_in))
        (pin (num 2) (name OUT) (type passive))
        (pin (num 3) (name IN) (type power_in))
        (pin (num 4) (name OUT) (type power_out))))
    (libpart (lib my_elements) (part NX3L4051-HX)
      (fields
        (field (name Reference) DA)
        (field (name Value) NX3L4051-HX)
        (field (name Footprint) HXQFN-16))
      (pins
        (pin (num 1) (name Z) (type BiDi))
        (pin (num 2) (name Y7) (type BiDi))
        (pin (num 3) (name Y5) (type BiDi))
        (pin (num 4) (name ~E) (type input))
        (pin (num 6) (name GND) (type power_in))
        (pin (num 7) (name S3) (type input))
        (pin (num 8) (name S2) (type input))
        (pin (num 9) (name S1) (type input))
        (pin (num 10) (name Y3) (type BiDi))
        (pin (num 11) (name Y0) (type BiDi))
        (pin (num 12) (name Y1) (type BiDi))
        (pin (num 13) (name Y2) (type BiDi))
        (pin (num 14) (name VCC) (type power_in))
        (pin (num 15) (name Y4) (type BiDi))
        (pin (num 16) (name Y6) (type BiDi))))
    (libpart (lib device) (part R)
      (description Resistor)
      (footprints
        (fp R_*)
        (fp R_*))
      (fields
        (field (name Reference) R)
        (field (name Value) R))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive)))))
  (libraries
    (library (logical termorez-rescue)
      (uri termorez-rescue.lib))
    (library (logical device)
      (uri /usr/share/kicad/library/device.lib))
    (library (logical my_elements)
      (uri my_elements.lib))
    (library (logical termorez-cache)
      (uri /home/eddy/Docs/SAO/BTA/MIRROR_CONTROL_termo/Project/termorez_NX3L4051/termorez-cache.lib)))
  (nets
    (net (code 1) (name "Net-(DA1-Pad1)")
      (node (ref U4) (pin 7))
      (node (ref U4) (pin 16))
      (node (ref DA1) (pin 1)))
    (net (code 2) (name +3V3)
      (node (ref L1) (pin 2))
      (node (ref C10) (pin 1))
      (node (ref U4) (pin 21)))
    (net (code 3) (name "Net-(C8-Pad1)")
      (node (ref C8) (pin 1))
      (node (ref U5) (pin 3))
      (node (ref P6) (pin 2)))
    (net (code 4) (name VDD)
      (node (ref U5) (pin 4))
      (node (ref C9) (pin 1))
      (node (ref L1) (pin 1))
      (node (ref DA2) (pin 14))
      (node (ref C12) (pin 1))
      (node (ref U5) (pin 2))
      (node (ref U4) (pin 22))
      (node (ref DA1) (pin 14))
      (node (ref DA3) (pin 14)))
    (net (code 5) (name "Net-(DA3-Pad1)")
      (node (ref DA3) (pin 1))
      (node (ref U4) (pin 13))
      (node (ref R4) (pin 1)))
    (net (code 6) (name "Net-(DA2-Pad1)")
      (node (ref U4) (pin 8))
      (node (ref U4) (pin 15))
      (node (ref DA2) (pin 1)))
    (net (code 7) (name DGND)
      (node (ref U4) (pin 2))
      (node (ref U4) (pin 3))
      (node (ref P4) (pin 5))
      (node (ref U5) (pin 1))
      (node (ref R3) (pin 2))
      (node (ref P6) (pin 1))
      (node (ref C12) (pin 2))
      (node (ref C8) (pin 2))
      (node (ref X1) (pin 1))
      (node (ref C9) (pin 2)))
    (net (code 8) (name "Net-(R1-Pad1)")
      (node (ref U4) (pin 5))
      (node (ref R1) (pin 1)))
    (net (code 9) (name "Net-(DA1-Pad2)")
      (node (ref DA1) (pin 2))
      (node (ref P1) (pin 8)))
    (net (code 10) (name AGND)
      (node (ref R1) (pin 2))
      (node (ref R2) (pin 2))
      (node (ref U4) (pin 14))
      (node (ref DA2) (pin 6))
      (node (ref C10) (pin 2))
      (node (ref U4) (pin 9))
      (node (ref U4) (pin 10))
      (node (ref U4) (pin 20))
      (node (ref U4) (pin 11))
      (node (ref U4) (pin 12))
      (node (ref X1) (pin 2))
      (node (ref U4) (pin 17))
      (node (ref U4) (pin 18))
      (node (ref U4) (pin 19))
      (node (ref DA3) (pin 6))
      (node (ref R8) (pin 2))
      (node (ref DA1) (pin 6)))
    (net (code 11) (name "Net-(R2-Pad1)")
      (node (ref R2) (pin 1))
      (node (ref U4) (pin 6)))
    (net (code 12) (name "Net-(DA2-Pad10)")
      (node (ref DA2) (pin 10))
      (node (ref P2) (pin 6)))
    (net (code 13) (name "Net-(DA2-Pad15)")
      (node (ref DA2) (pin 15))
      (node (ref P2) (pin 2)))
    (net (code 14) (name "Net-(DA2-Pad13)")
      (node (ref P2) (pin 3))
      (node (ref DA2) (pin 13)))
    (net (code 15) (name "Net-(DA2-Pad12)")
      (node (ref P2) (pin 4))
      (node (ref DA2) (pin 12)))
    (net (code 16) (name "Net-(DA2-Pad11)")
      (node (ref P2) (pin 5))
      (node (ref DA2) (pin 11)))
    (net (code 17) (name "Net-(DA2-Pad3)")
      (node (ref DA2) (pin 3))
      (node (ref P2) (pin 7)))
    (net (code 18) (name "Net-(DA2-Pad16)")
      (node (ref DA2) (pin 16))
      (node (ref P2) (pin 1)))
    (net (code 19) (name "Net-(DA2-Pad2)")
      (node (ref P2) (pin 8))
      (node (ref DA2) (pin 2)))
    (net (code 20) (name "Net-(DA3-Pad16)")
      (node (ref P3) (pin 1))
      (node (ref DA3) (pin 16)))
    (net (code 21) (name "Net-(DA1-Pad13)")
      (node (ref P1) (pin 3))
      (node (ref DA1) (pin 13)))
    (net (code 22) (name /EN)
      (node (ref DA1) (pin 4))
      (node (ref DA3) (pin 4))
      (node (ref R3) (pin 1))
      (node (ref DA2) (pin 4))
      (node (ref P4) (pin 4)))
    (net (code 23) (name "Net-(DA1-Pad11)")
      (node (ref P1) (pin 5))
      (node (ref DA1) (pin 11)))
    (net (code 24) (name "Net-(DA1-Pad12)")
      (node (ref P1) (pin 4))
      (node (ref DA1) (pin 12)))
    (net (code 25) (name "Net-(DA1-Pad15)")
      (node (ref DA1) (pin 15))
      (node (ref P1) (pin 2)))
    (net (code 26) (name "Net-(DA1-Pad10)")
      (node (ref DA1) (pin 10))
      (node (ref P1) (pin 6)))
    (net (code 27) (name "Net-(DA1-Pad3)")
      (node (ref DA1) (pin 3))
      (node (ref P1) (pin 7)))
    (net (code 28) (name "Net-(DA1-Pad16)")
      (node (ref DA1) (pin 16))
      (node (ref P1) (pin 1)))
    (net (code 29) (name "Net-(R6-Pad2)")
      (node (ref R6) (pin 2))
      (node (ref R7) (pin 2)))
    (net (code 30) (name "Net-(R5-Pad1)")
      (node (ref R5) (pin 1))
      (node (ref R6) (pin 1)))
    (net (code 31) (name "Net-(R4-Pad2)")
      (node (ref R5) (pin 2))
      (node (ref R4) (pin 2)))
    (net (code 32) (name "Net-(R7-Pad1)")
      (node (ref R7) (pin 1))
      (node (ref R8) (pin 1)))
    (net (code 33) (name "Net-(DA3-Pad3)")
      (node (ref P3) (pin 7))
      (node (ref DA3) (pin 3)))
    (net (code 34) (name "Net-(DA3-Pad15)")
      (node (ref P3) (pin 2))
      (node (ref DA3) (pin 15)))
    (net (code 35) (name "Net-(DA3-Pad11)")
      (node (ref P3) (pin 5))
      (node (ref DA3) (pin 11)))
    (net (code 36) (name "Net-(DA3-Pad12)")
      (node (ref DA3) (pin 12))
      (node (ref P3) (pin 4)))
    (net (code 37) (name "Net-(DA3-Pad10)")
      (node (ref DA3) (pin 10))
      (node (ref P3) (pin 6)))
    (net (code 38) (name "Net-(DA3-Pad13)")
      (node (ref P3) (pin 3))
      (node (ref DA3) (pin 13)))
    (net (code 39) (name "Net-(DA3-Pad2)")
      (node (ref DA3) (pin 2))
      (node (ref P3) (pin 8)))
    (net (code 40) (name /SC)
      (node (ref U4) (pin 1))
      (node (ref P4) (pin 8)))
    (net (code 41) (name /A2)
      (node (ref DA3) (pin 7))
      (node (ref P4) (pin 3))
      (node (ref DA2) (pin 7))
      (node (ref DA1) (pin 7)))
    (net (code 42) (name /A1)
      (node (ref DA1) (pin 8))
      (node (ref DA3) (pin 8))
      (node (ref DA2) (pin 8))
      (node (ref P4) (pin 2)))
    (net (code 43) (name /A0)
      (node (ref DA3) (pin 9))
      (node (ref DA2) (pin 9))
      (node (ref P4) (pin 1))
      (node (ref DA1) (pin 9)))
    (net (code 44) (name /SDO)
      (node (ref U4) (pin 24))
      (node (ref P4) (pin 7)))
    (net (code 45) (name /SDI)
      (node (ref U4) (pin 23))
      (node (ref P4) (pin 6)))))