(export (version D)
  (design
    (source /home/eddy/Docs/SAO/BTA/MIRROR_CONTROL_termo/Project/kicad/Sensors_tester_with_screen/stm32f042/stm32f042.sch)
    (date "Пн 15 июл 2019 17:19:38")
    (tool "Eeschema (6.0.0-rc1-dev-1613-ga55d9819b)")
    (sheet (number 1) (name /) (tstamps /)
      (title_block
        (title)
        (company)
        (rev)
        (date)
        (source stm32f042.sch)
        (comment (number 1) (value ""))
        (comment (number 2) (value ""))
        (comment (number 3) (value ""))
        (comment (number 4) (value "")))))
  (components
    (comp (ref R10)
      (value 10k)
      (footprint Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder)
      (libsource (lib stm32-rescue) (part R) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5D347863))
    (comp (ref C2)
      (value 0.1)
      (footprint Capacitor_SMD:C_0603_1608Metric_Pad1.05x0.95mm_HandSolder)
      (libsource (lib stm32-rescue) (part C) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 590D4150))
    (comp (ref C1)
      (value 0.1)
      (footprint Capacitor_SMD:C_0603_1608Metric_Pad1.05x0.95mm_HandSolder)
      (libsource (lib stm32-rescue) (part C) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5D4AE2B9))
    (comp (ref SW2)
      (value Boot)
      (footprint Buttons_Switches_SMD:SW_SPST_FSMSM)
      (libsource (lib Switch) (part SW_Push) (description "Push button switch, generic, two pins"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5D34785A))
    (comp (ref SW1)
      (value Reset)
      (footprint Buttons_Switches_SMD:SW_SPST_FSMSM)
      (libsource (lib Switch) (part SW_Push) (description "Push button switch, generic, two pins"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5D34785B))
    (comp (ref P1)
      (value USB_B)
      (footprint Connectors_USB:USB_B_OST_USB-B1HSxx_Horizontal)
      (libsource (lib stm32-rescue) (part USB_A-RESCUE-stm32) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CEABE76))
    (comp (ref R1)
      (value 22)
      (footprint Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder)
      (libsource (lib stm32-rescue) (part R) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CEABEA6))
    (comp (ref R2)
      (value 22)
      (footprint Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder)
      (libsource (lib stm32-rescue) (part R) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CEABEAC))
    (comp (ref U1)
      (value USBLC6-2SC6)
      (footprint TO_SOT_Packages_SMD:SOT-23-6_Handsoldering)
      (datasheet http://www2.st.com/resource/en/datasheet/CD00050750.pdf)
      (libsource (lib Power_Protection) (part USBLC6-2SC6) (description "Bidirectional ESD Protection Diode, SOT-23-6"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CED0250))
    (comp (ref D3)
      (value SS14)
      (footprint Diode_SMD:D_SMB_Handsoldering)
      (datasheet ~)
      (libsource (lib Device) (part D_Schottky) (description "Schottky diode"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5D89B9B8))
    (comp (ref J2)
      (value Conn)
      (footprint TerminalBlock_Phoenix:TerminalBlock_Phoenix_MKDS-1,5-2-5.08_1x02_P5.08mm_Horizontal)
      (datasheet ~)
      (libsource (lib Connector_Generic) (part Conn_01x02) (description "Generic connector, single row, 01x02, script generated (kicad-library-utils/schlib/autogen/connector/)"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5D2DE414))
    (comp (ref U2)
      (value STM32F042C6Tx)
      (footprint Package_QFP:LQFP-48_7x7mm_P0.5mm)
      (libsource (lib stm32-rescue) (part STM32F042C6Tx) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 58C42C0E))
    (comp (ref C3)
      (value 0.1)
      (footprint Capacitor_SMD:C_0603_1608Metric_Pad1.05x0.95mm_HandSolder)
      (libsource (lib stm32-rescue) (part C) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 58C42D39))
    (comp (ref C4)
      (value 0.1)
      (footprint Capacitor_SMD:C_0603_1608Metric_Pad1.05x0.95mm_HandSolder)
      (libsource (lib stm32-rescue) (part C) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5D6B4F1F))
    (comp (ref C5)
      (value 0.1)
      (footprint Capacitor_SMD:C_0603_1608Metric_Pad1.05x0.95mm_HandSolder)
      (libsource (lib stm32-rescue) (part C) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 59093675))
    (comp (ref C6)
      (value 0.1)
      (footprint Capacitor_SMD:C_0603_1608Metric_Pad1.05x0.95mm_HandSolder)
      (libsource (lib stm32-rescue) (part C) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5D6B4F23))
    (comp (ref P2)
      (value USART_BOOT)
      (footprint Connector_PinHeader_2.54mm:PinHeader_1x03_P2.54mm_Vertical)
      (libsource (lib stm32-rescue) (part CONN_01X03) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5D6B4F24))
    (comp (ref P3)
      (value Hole)
      (footprint my_footprints:Hole_3mm)
      (libsource (lib stm32-rescue) (part CONN_01X01) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 59143415))
    (comp (ref P4)
      (value Hole)
      (footprint my_footprints:Hole_3mm)
      (libsource (lib stm32-rescue) (part CONN_01X01) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5914456D))
    (comp (ref P5)
      (value Hole)
      (footprint my_footprints:Hole_3mm)
      (libsource (lib stm32-rescue) (part CONN_01X01) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5D6B4F29))
    (comp (ref P6)
      (value Hole)
      (footprint my_footprints:Hole_3mm)
      (libsource (lib stm32-rescue) (part CONN_01X01) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5D6B4F2A))
    (comp (ref J1)
      (value 4P4C)
      (footprint my_footprints:RJ9-4P4C)
      (datasheet ~)
      (libsource (lib Connector) (part 4P4C) (description "RJ connector, 4P4C (4 positions 4 connected), RJ9/RJ10/RJ22"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5D692FC5))
    (comp (ref J3)
      (value Conn)
      (footprint TerminalBlock_Phoenix:TerminalBlock_Phoenix_MKDS-1,5-2-5.08_1x02_P5.08mm_Horizontal)
      (datasheet ~)
      (libsource (lib Connector_Generic) (part Conn_01x02) (description "Generic connector, single row, 01x02, script generated (kicad-library-utils/schlib/autogen/connector/)"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5D6A6D23))
    (comp (ref U3)
      (value LM1117-3.3)
      (footprint TO_SOT_Packages_SMD:SOT-223)
      (libsource (lib stm32-rescue) (part LM1117-3.3-RESCUE-stm32) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 58C431FC))
    (comp (ref C7)
      (value 47u)
      (footprint Capacitor_Tantalum_SMD:CP_EIA-3216-18_Kemet-A_Pad1.58x1.35mm_HandSolder)
      (libsource (lib stm32-rescue) (part CP) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 58C454F6))
    (comp (ref D1)
      (value LED0)
      (footprint LED_SMD:LED_0805_2012Metric_Pad1.15x1.40mm_HandSolder)
      (libsource (lib stm32-rescue) (part LED-RESCUE-stm32) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5908EA64))
    (comp (ref R5)
      (value 330)
      (footprint Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder)
      (libsource (lib stm32-rescue) (part R) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5908EB17))
    (comp (ref D2)
      (value LED1)
      (footprint LED_SMD:LED_0805_2012Metric_Pad1.15x1.40mm_HandSolder)
      (libsource (lib stm32-rescue) (part LED-RESCUE-stm32) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5909AF9A))
    (comp (ref R6)
      (value 330)
      (footprint Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder)
      (libsource (lib stm32-rescue) (part R) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5909AFA0))
    (comp (ref D4)
      (value SS14)
      (footprint Diode_SMD:D_SMB_Handsoldering)
      (libsource (lib stm32-rescue) (part D_Schottky) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5A545B43))
    (comp (ref BT1)
      (value Battery_Cell)
      (footprint Battery:BatteryHolder_MPD_BH-18650-PC2)
      (datasheet ~)
      (libsource (lib Device) (part Battery_Cell) (description "Single-cell battery"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5D7DDF56))
    (comp (ref R8)
      (value 4k7)
      (footprint Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5D850AD1))
    (comp (ref R7)
      (value 4k7)
      (footprint Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5D85121F))
    (comp (ref R9)
      (value 22)
      (footprint Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5D86E056))
    (comp (ref Q1)
      (value AO3407)
      (footprint TO_SOT_Packages_SMD:SOT-23_Handsoldering)
      (datasheet ~)
      (libsource (lib Device) (part Q_PMOS_GSD) (description "P-MOSFET transistor, gate/source/drain"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5D886416))
    (comp (ref R11)
      (value 10k)
      (footprint Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder)
      (libsource (lib stm32-rescue) (part R) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5D89C1EC))
    (comp (ref R12)
      (value 510)
      (footprint Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5D89C918))
    (comp (ref SW3)
      (value Poweron)
      (footprint Button_Switch_THT:SW_PUSH_6mm_H13mm)
      (libsource (lib Switch) (part SW_Push) (description "Push button switch, generic, two pins"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5D8C5989))
    (comp (ref R4)
      (value 51k)
      (footprint Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder)
      (libsource (lib stm32-rescue) (part R) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5D93631F))
    (comp (ref R3)
      (value 51k)
      (footprint Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder)
      (libsource (lib stm32-rescue) (part R) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5D936816))
    (comp (ref J4)
      (value SPI_screen)
      (footprint Connector_PinSocket_2.54mm:PinSocket_1x07_P2.54mm_Vertical)
      (datasheet ~)
      (libsource (lib Connector) (part Conn_01x07_Female) (description "Generic connector, single row, 01x07, script generated (kicad-library-utils/schlib/autogen/connector/)"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5D96F1EC))
    (comp (ref C8)
      (value 0.1)
      (footprint Capacitor_SMD:C_0603_1608Metric_Pad1.05x0.95mm_HandSolder)
      (libsource (lib stm32-rescue) (part C) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5DA0ADC1)))
  (libparts
    (libpart (lib Connector) (part 4P4C)
      (aliases
        (alias RJ9)
        (alias RJ10)
        (alias RJ22))
      (description "RJ connector, 4P4C (4 positions 4 connected), RJ9/RJ10/RJ22")
      (docs ~)
      (footprints
        (fp 4P4C*)
        (fp RJ9*)
        (fp RJ10*)
        (fp RJ22*))
      (fields
        (field (name Reference) J)
        (field (name Value) 4P4C))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))
        (pin (num 3) (name ~) (type passive))
        (pin (num 4) (name ~) (type passive))))
    (libpart (lib Connector) (part Conn_01x07_Female)
      (description "Generic connector, single row, 01x07, script generated (kicad-library-utils/schlib/autogen/connector/)")
      (docs ~)
      (footprints
        (fp Connector*:*_1x??_*))
      (fields
        (field (name Reference) J)
        (field (name Value) Conn_01x07_Female))
      (pins
        (pin (num 1) (name Pin_1) (type passive))
        (pin (num 2) (name Pin_2) (type passive))
        (pin (num 3) (name Pin_3) (type passive))
        (pin (num 4) (name Pin_4) (type passive))
        (pin (num 5) (name Pin_5) (type passive))
        (pin (num 6) (name Pin_6) (type passive))
        (pin (num 7) (name Pin_7) (type passive))))
    (libpart (lib Connector_Generic) (part Conn_01x02)
      (description "Generic connector, single row, 01x02, script generated (kicad-library-utils/schlib/autogen/connector/)")
      (docs ~)
      (footprints
        (fp Connector*:*_1x??_*))
      (fields
        (field (name Reference) J)
        (field (name Value) Conn_01x02))
      (pins
        (pin (num 1) (name Pin_1) (type passive))
        (pin (num 2) (name Pin_2) (type passive))))
    (libpart (lib Device) (part Battery_Cell)
      (description "Single-cell battery")
      (docs ~)
      (fields
        (field (name Reference) BT)
        (field (name Value) Battery_Cell))
      (pins
        (pin (num 1) (name +) (type passive))
        (pin (num 2) (name -) (type passive))))
    (libpart (lib Device) (part D_Schottky)
      (description "Schottky diode")
      (docs ~)
      (footprints
        (fp TO-???*)
        (fp *_Diode_*)
        (fp *SingleDiode*)
        (fp D_*))
      (fields
        (field (name Reference) D)
        (field (name Value) D_Schottky))
      (pins
        (pin (num 1) (name K) (type passive))
        (pin (num 2) (name A) (type passive))))
    (libpart (lib Device) (part Q_PMOS_GSD)
      (description "P-MOSFET transistor, gate/source/drain")
      (docs ~)
      (fields
        (field (name Reference) Q)
        (field (name Value) Q_PMOS_GSD))
      (pins
        (pin (num 1) (name G) (type input))
        (pin (num 2) (name S) (type passive))
        (pin (num 3) (name D) (type passive))))
    (libpart (lib Device) (part R)
      (description Resistor)
      (docs ~)
      (footprints
        (fp R_*))
      (fields
        (field (name Reference) R)
        (field (name Value) R))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib Power_Protection) (part USBLC6-2SC6)
      (description "Bidirectional ESD Protection Diode, SOT-23-6")
      (docs http://www2.st.com/resource/en/datasheet/CD00050750.pdf)
      (footprints
        (fp SOT?23*))
      (fields
        (field (name Reference) U)
        (field (name Value) USBLC6-2SC6)
        (field (name Footprint) Package_TO_SOT_SMD:SOT-23-6))
      (pins
        (pin (num 1) (name IO1) (type passive))
        (pin (num 2) (name GND) (type passive))
        (pin (num 3) (name IO2) (type passive))
        (pin (num 4) (name IO2) (type passive))
        (pin (num 5) (name VBUS) (type passive))
        (pin (num 6) (name IO1) (type passive))))
    (libpart (lib Switch) (part SW_Push)
      (description "Push button switch, generic, two pins")
      (docs ~)
      (fields
        (field (name Reference) SW)
        (field (name Value) SW_Push))
      (pins
        (pin (num 1) (name 1) (type passive))
        (pin (num 2) (name 2) (type passive))))
    (libpart (lib stm32-rescue) (part C)
      (footprints
        (fp C_*))
      (fields
        (field (name Reference) C)
        (field (name Value) C))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib stm32-rescue) (part CONN_01X01)
      (footprints
        (fp Pin_Header_Straight_1X*)
        (fp Pin_Header_Angled_1X*)
        (fp Socket_Strip_Straight_1X*)
        (fp Socket_Strip_Angled_1X*))
      (fields
        (field (name Reference) J)
        (field (name Value) CONN_01X01))
      (pins
        (pin (num 1) (name P1) (type passive))))
    (libpart (lib stm32-rescue) (part CONN_01X03)
      (footprints
        (fp Pin_Header_Straight_1X*)
        (fp Pin_Header_Angled_1X*)
        (fp Socket_Strip_Straight_1X*)
        (fp Socket_Strip_Angled_1X*))
      (fields
        (field (name Reference) J)
        (field (name Value) CONN_01X03))
      (pins
        (pin (num 1) (name P1) (type passive))
        (pin (num 2) (name P2) (type passive))
        (pin (num 3) (name P3) (type passive))))
    (libpart (lib stm32-rescue) (part CP)
      (footprints
        (fp CP_*))
      (fields
        (field (name Reference) C)
        (field (name Value) CP))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib stm32-rescue) (part D_Schottky)
      (footprints
        (fp TO-???*)
        (fp *SingleDiode)
        (fp *_Diode_*)
        (fp *SingleDiode*)
        (fp D_*))
      (fields
        (field (name Reference) D)
        (field (name Value) D_Schottky))
      (pins
        (pin (num 1) (name K) (type passive))
        (pin (num 2) (name A) (type passive))))
    (libpart (lib stm32-rescue) (part LED-RESCUE-stm32)
      (footprints
        (fp LED*))
      (fields
        (field (name Reference) D)
        (field (name Value) LED-RESCUE-stm32))
      (pins
        (pin (num 1) (name K) (type passive))
        (pin (num 2) (name A) (type passive))))
    (libpart (lib stm32-rescue) (part LM1117-3.3-RESCUE-stm32)
      (footprints
        (fp SOT-223*)
        (fp TO-263*)
        (fp TO-252*))
      (fields
        (field (name Reference) U)
        (field (name Value) LM1117-3.3-RESCUE-stm32))
      (pins
        (pin (num 1) (name GND/ADJ) (type power_in))
        (pin (num 2) (name VO) (type passive))
        (pin (num 3) (name VI) (type power_in))
        (pin (num 4) (name VO) (type power_out))))
    (libpart (lib stm32-rescue) (part R)
      (footprints
        (fp R_*)
        (fp R_*))
      (fields
        (field (name Reference) R)
        (field (name Value) R))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib stm32-rescue) (part STM32F042C6Tx)
      (fields
        (field (name Reference) U)
        (field (name Value) STM32F042C6Tx)
        (field (name Footprint) LQFP48))
      (pins
        (pin (num 1) (name VBAT) (type power_in))
        (pin (num 2) (name PC13/RTC_OUT_ALARM/RTC_OUT_CALIB/RTC_TAMP1/RTC_TS/SYS_WKUP2) (type BiDi))
        (pin (num 3) (name PC14/RCC_OSC32_IN) (type BiDi))
        (pin (num 4) (name PC15/RCC_OSC32_OUT) (type BiDi))
        (pin (num 5) (name PF0/CRS_SYNC/I2C1_SDA/RCC_OSC_IN) (type input))
        (pin (num 6) (name PF1/I2C1_SCL/RCC_OSC_OUT) (type input))
        (pin (num 7) (name NRST) (type input))
        (pin (num 8) (name VSSA) (type power_in))
        (pin (num 9) (name VDDA) (type power_in))
        (pin (num 10) (name ADC_IN0/RTC_TAMP2/SYS_WKUP1/TIM2_CH1/TIM2_ETR/TSC_G1_IO1/USART2_CTS/PA0) (type BiDi))
        (pin (num 11) (name ADC_IN1/TIM2_CH2/TSC_G1_IO2/USART2_DE/USART2_RTS/PA1) (type BiDi))
        (pin (num 12) (name ADC_IN2/SYS_WKUP4/TIM2_CH3/TSC_G1_IO3/USART2_TX/PA2) (type BiDi))
        (pin (num 13) (name ADC_IN3/TIM2_CH4/TSC_G1_IO4/USART2_RX/PA3) (type BiDi))
        (pin (num 14) (name ADC_IN4/I2S1_WS/SPI1_NSS/TIM14_CH1/TSC_G2_IO1/USART2_CK/USB_OE/PA4) (type BiDi))
        (pin (num 15) (name ADC_IN5/CEC/I2S1_CK/SPI1_SCK/TIM2_CH1/TIM2_ETR/TSC_G2_IO2/PA5) (type BiDi))
        (pin (num 16) (name ADC_IN6/I2S1_MCK/SPI1_MISO/TIM16_CH1/TIM1_BKIN/TIM3_CH1/TSC_G2_IO3/PA6) (type BiDi))
        (pin (num 17) (name ADC_IN7/I2S1_SD/SPI1_MOSI/TIM14_CH1/TIM17_CH1/TIM1_CH1N/TIM3_CH2/TSC_G2_IO4/PA7) (type BiDi))
        (pin (num 18) (name PB0/ADC_IN8/TIM1_CH2N/TIM3_CH3/TSC_G3_IO2) (type BiDi))
        (pin (num 19) (name PB1/ADC_IN9/TIM14_CH1/TIM1_CH3N/TIM3_CH4/TSC_G3_IO3) (type BiDi))
        (pin (num 20) (name PB2/TSC_G3_IO4) (type BiDi))
        (pin (num 21) (name PB10/CEC/I2C1_SCL/SPI2_SCK/TIM2_CH3/TSC_SYNC) (type BiDi))
        (pin (num 22) (name PB11/I2C1_SDA/TIM2_CH4) (type BiDi))
        (pin (num 23) (name VSS) (type power_in))
        (pin (num 24) (name VDD) (type power_in))
        (pin (num 25) (name PB12/SPI2_NSS/TIM1_BKIN) (type BiDi))
        (pin (num 26) (name PB13/I2C1_SCL/SPI2_SCK/TIM1_CH1N) (type BiDi))
        (pin (num 27) (name PB14/I2C1_SDA/SPI2_MISO/TIM1_CH2N) (type BiDi))
        (pin (num 28) (name PB15/RTC_REFIN/SPI2_MOSI/SYS_WKUP7/TIM1_CH3N) (type BiDi))
        (pin (num 29) (name CRS_SYNC/RCC_MCO/TIM1_CH1/USART1_CK/PA8) (type BiDi))
        (pin (num 30) (name I2C1_SCL/TIM1_CH2/TSC_G4_IO1/USART1_TX/PA9) (type BiDi))
        (pin (num 31) (name I2C1_SDA/TIM17_BKIN/TIM1_CH3/TSC_G4_IO2/USART1_RX/PA10) (type BiDi))
        (pin (num 32) (name CAN_RX/I2C1_SCL/TIM1_CH4/TSC_G4_IO3/USART1_CTS/USB_DM/PA11) (type BiDi))
        (pin (num 33) (name CAN_TX/I2C1_SDA/TIM1_ETR/TSC_G4_IO4/USART1_DE/USART1_RTS/USB_DP/PA12) (type BiDi))
        (pin (num 34) (name IR_OUT/SYS_SWDIO/USB_OE/PA13) (type BiDi))
        (pin (num 35) (name VSS) (type power_in))
        (pin (num 36) (name VDDIO2) (type power_in))
        (pin (num 37) (name SYS_SWCLK/USART2_TX/PA14) (type BiDi))
        (pin (num 38) (name I2S1_WS/SPI1_NSS/TIM2_CH1/TIM2_ETR/USART2_RX/USB_OE/PA15) (type BiDi))
        (pin (num 39) (name PB3/I2S1_CK/SPI1_SCK/TIM2_CH2/TSC_G5_IO1) (type BiDi))
        (pin (num 40) (name PB4/I2S1_MCK/SPI1_MISO/TIM17_BKIN/TIM3_CH1/TSC_G5_IO2) (type BiDi))
        (pin (num 41) (name PB5/I2C1_SMBA/I2S1_SD/SPI1_MOSI/SYS_WKUP6/TIM16_BKIN/TIM3_CH2) (type BiDi))
        (pin (num 42) (name PB6/I2C1_SCL/TIM16_CH1N/TSC_G5_IO3/USART1_TX) (type BiDi))
        (pin (num 43) (name PB7/I2C1_SDA/TIM17_CH1N/TSC_G5_IO4/USART1_RX) (type BiDi))
        (pin (num 44) (name PF11) (type BiDi))
        (pin (num 45) (name PB8/CAN_RX/CEC/I2C1_SCL/TIM16_CH1/TSC_SYNC) (type BiDi))
        (pin (num 46) (name PB9/CAN_TX/I2C1_SDA/IR_OUT/SPI2_NSS/TIM17_CH1) (type BiDi))
        (pin (num 47) (name VSS) (type power_in))
        (pin (num 48) (name VDD) (type power_in))))
    (libpart (lib stm32-rescue) (part USB_A-RESCUE-stm32)
      (footprints
        (fp USB*))
      (fields
        (field (name Reference) P)
        (field (name Value) USB_A-RESCUE-stm32))
      (pins
        (pin (num 1) (name VBUS) (type power_in))
        (pin (num 2) (name D-) (type passive))
        (pin (num 3) (name D+) (type passive))
        (pin (num 4) (name GND) (type power_in))
        (pin (num 5) (name shield) (type passive)))))
  (libraries
    (library (logical Connector)
      (uri /usr/share/kicad/kicad-symbols//Connector.lib))
    (library (logical Connector_Generic)
      (uri /usr/share/kicad/kicad-symbols//Connector_Generic.lib))
    (library (logical Device)
      (uri /usr/share/kicad/kicad-symbols//Device.lib))
    (library (logical Power_Protection)
      (uri /usr/share/kicad/kicad-symbols//Power_Protection.lib))
    (library (logical Switch)
      (uri /usr/share/kicad/kicad-symbols//Switch.lib))
    (library (logical stm32-rescue)
      (uri /home/eddy/Docs/SAO/ELECTRONICS/STM32/F1-srcs/chronometer/kicad/chrono/stm32-rescue.lib)))
  (nets
    (net (code 1) (name "Net-(D1-Pad2)")
      (node (ref R5) (pin 1))
      (node (ref D1) (pin 2)))
    (net (code 2) (name +3V3)
      (node (ref C6) (pin 2))
      (node (ref U2) (pin 36))
      (node (ref U2) (pin 24))
      (node (ref U3) (pin 4))
      (node (ref J4) (pin 2))
      (node (ref R9) (pin 1))
      (node (ref U3) (pin 2))
      (node (ref SW2) (pin 2))
      (node (ref C2) (pin 2))
      (node (ref C7) (pin 1))
      (node (ref R5) (pin 2))
      (node (ref C4) (pin 2))
      (node (ref C5) (pin 2))
      (node (ref R6) (pin 2))
      (node (ref U2) (pin 9))
      (node (ref U2) (pin 48))
      (node (ref C3) (pin 2)))
    (net (code 3) (name "Net-(D2-Pad2)")
      (node (ref R6) (pin 1))
      (node (ref D2) (pin 2)))
    (net (code 4) (name /LED1)
      (node (ref D2) (pin 1))
      (node (ref U2) (pin 38)))
    (net (code 5) (name /LED0)
      (node (ref U2) (pin 37))
      (node (ref D1) (pin 1)))
    (net (code 6) (name "Net-(U2-Pad16)")
      (node (ref U2) (pin 16)))
    (net (code 7) (name /SCL)
      (node (ref U2) (pin 42))
      (node (ref J3) (pin 2))
      (node (ref J1) (pin 2))
      (node (ref R8) (pin 2)))
    (net (code 8) (name /SDA)
      (node (ref J1) (pin 1))
      (node (ref U2) (pin 43))
      (node (ref J2) (pin 1))
      (node (ref R7) (pin 2)))
    (net (code 9) (name "Net-(U2-Pad13)")
      (node (ref U2) (pin 13)))
    (net (code 10) (name "Net-(U2-Pad39)")
      (node (ref U2) (pin 39)))
    (net (code 11) (name "Net-(U2-Pad46)")
      (node (ref U2) (pin 46)))
    (net (code 12) (name "Net-(U2-Pad28)")
      (node (ref U2) (pin 28)))
    (net (code 13) (name GND)
      (node (ref R4) (pin 1))
      (node (ref J1) (pin 4))
      (node (ref U1) (pin 2))
      (node (ref BT1) (pin 2))
      (node (ref U2) (pin 35))
      (node (ref P2) (pin 1))
      (node (ref C6) (pin 1))
      (node (ref J4) (pin 1))
      (node (ref J3) (pin 1))
      (node (ref C8) (pin 2))
      (node (ref C5) (pin 1))
      (node (ref C4) (pin 1))
      (node (ref U2) (pin 47))
      (node (ref SW1) (pin 2))
      (node (ref U3) (pin 1))
      (node (ref C3) (pin 1))
      (node (ref U2) (pin 8))
      (node (ref C1) (pin 2))
      (node (ref R10) (pin 2))
      (node (ref U2) (pin 23))
      (node (ref C7) (pin 2))
      (node (ref P1) (pin 4))
      (node (ref P1) (pin 5)))
    (net (code 14) (name "Net-(BT1-Pad1)")
      (node (ref R11) (pin 1))
      (node (ref D4) (pin 1))
      (node (ref SW3) (pin 1))
      (node (ref BT1) (pin 1))
      (node (ref Q1) (pin 2)))
    (net (code 15) (name /USBDM)
      (node (ref U2) (pin 32))
      (node (ref R2) (pin 2)))
    (net (code 16) (name /USBDP)
      (node (ref R1) (pin 2))
      (node (ref U2) (pin 33)))
    (net (code 17) (name "Net-(U2-Pad29)")
      (node (ref U2) (pin 29)))
    (net (code 18) (name "Net-(U2-Pad34)")
      (node (ref U2) (pin 34)))
    (net (code 19) (name "Net-(U2-Pad12)")
      (node (ref U2) (pin 12)))
    (net (code 20) (name "Net-(P2-Pad3)")
      (node (ref P2) (pin 3))
      (node (ref U2) (pin 30)))
    (net (code 21) (name /D-C)
      (node (ref U2) (pin 19))
      (node (ref J4) (pin 6)))
    (net (code 22) (name /RST)
      (node (ref U2) (pin 18))
      (node (ref J4) (pin 5)))
    (net (code 23) (name /MOSI)
      (node (ref U2) (pin 17))
      (node (ref J4) (pin 4)))
    (net (code 24) (name /SCK)
      (node (ref U2) (pin 15))
      (node (ref J4) (pin 3)))
    (net (code 25) (name "Net-(U2-Pad26)")
      (node (ref U2) (pin 26)))
    (net (code 26) (name "Net-(U2-Pad10)")
      (node (ref U2) (pin 10)))
    (net (code 27) (name "Net-(U2-Pad25)")
      (node (ref U2) (pin 25)))
    (net (code 28) (name "Net-(U2-Pad22)")
      (node (ref U2) (pin 22)))
    (net (code 29) (name "Net-(U2-Pad21)")
      (node (ref U2) (pin 21)))
    (net (code 30) (name "Net-(U2-Pad14)")
      (node (ref U2) (pin 14)))
    (net (code 31) (name "Net-(U2-Pad41)")
      (node (ref U2) (pin 41)))
    (net (code 32) (name "Net-(U2-Pad40)")
      (node (ref U2) (pin 40)))
    (net (code 33) (name "Net-(U2-Pad45)")
      (node (ref U2) (pin 45)))
    (net (code 34) (name "Net-(Q1-Pad1)")
      (node (ref R12) (pin 1))
      (node (ref Q1) (pin 1)))
    (net (code 35) (name /5Vusb)
      (node (ref D4) (pin 2))
      (node (ref D3) (pin 1))
      (node (ref Q1) (pin 3))
      (node (ref SW3) (pin 2))
      (node (ref C8) (pin 1))
      (node (ref U3) (pin 3)))
    (net (code 36) (name "Net-(P2-Pad2)")
      (node (ref P2) (pin 2))
      (node (ref U2) (pin 31)))
    (net (code 37) (name "Net-(P1-Pad2)")
      (node (ref P1) (pin 2))
      (node (ref U1) (pin 4)))
    (net (code 38) (name /U5V)
      (node (ref D3) (pin 2))
      (node (ref U1) (pin 5))
      (node (ref R3) (pin 2))
      (node (ref P1) (pin 1)))
    (net (code 39) (name "Net-(R2-Pad1)")
      (node (ref R2) (pin 1))
      (node (ref U1) (pin 3)))
    (net (code 40) (name "Net-(R1-Pad1)")
      (node (ref U1) (pin 1))
      (node (ref R1) (pin 1)))
    (net (code 41) (name "Net-(P1-Pad3)")
      (node (ref U1) (pin 6))
      (node (ref P1) (pin 3)))
    (net (code 42) (name /CS)
      (node (ref J4) (pin 7))
      (node (ref U2) (pin 20)))
    (net (code 43) (name /POWERON)
      (node (ref U2) (pin 2))
      (node (ref R12) (pin 2))
      (node (ref R11) (pin 2)))
    (net (code 44) (name /USBON)
      (node (ref U2) (pin 11))
      (node (ref R3) (pin 1))
      (node (ref R4) (pin 2)))
    (net (code 45) (name "Net-(U2-Pad1)")
      (node (ref U2) (pin 1)))
    (net (code 46) (name /3V3Sensors)
      (node (ref R8) (pin 1))
      (node (ref R7) (pin 1))
      (node (ref R9) (pin 2))
      (node (ref J2) (pin 2))
      (node (ref J1) (pin 3)))
    (net (code 47) (name /BOOT0)
      (node (ref R10) (pin 1))
      (node (ref U2) (pin 44))
      (node (ref SW2) (pin 1))
      (node (ref C2) (pin 1)))
    (net (code 48) (name "Net-(P3-Pad1)")
      (node (ref P3) (pin 1)))
    (net (code 49) (name "Net-(P6-Pad1)")
      (node (ref P6) (pin 1)))
    (net (code 50) (name "Net-(P5-Pad1)")
      (node (ref P5) (pin 1)))
    (net (code 51) (name "Net-(P4-Pad1)")
      (node (ref P4) (pin 1)))
    (net (code 52) (name "Net-(U2-Pad5)")
      (node (ref U2) (pin 5)))
    (net (code 53) (name "Net-(U2-Pad6)")
      (node (ref U2) (pin 6)))
    (net (code 54) (name "Net-(U2-Pad3)")
      (node (ref U2) (pin 3)))
    (net (code 55) (name "Net-(U2-Pad4)")
      (node (ref U2) (pin 4)))
    (net (code 56) (name "Net-(U2-Pad27)")
      (node (ref U2) (pin 27)))
    (net (code 57) (name /NRST)
      (node (ref U2) (pin 7))
      (node (ref C1) (pin 1))
      (node (ref SW1) (pin 1)))))