(kicad_symbol_lib (version 20211014) (generator kicad_symbol_editor)
  (symbol "OPI-ZERO-XDEB" (pin_names (offset 1.016)) (in_bom yes) (on_board yes)
    (property "Reference" "X" (id 0) (at 2.54 5.08 0)
      (effects (font (size 1.4986 1.4986)) (justify left bottom))
    )
    (property "Value" "OPI-ZERO-XDEB" (id 1) (at 2.54 2.54 0)
      (effects (font (size 1.4986 1.4986)) (justify left bottom))
    )
    (property "Footprint" "opi-hat:OPIOHATDEB" (id 2) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "" (id 3) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "OPI-ZERO-XDEB_1_0"
      (polyline
        (pts
          (xy 0 0)
          (xy 53.34 0)
        )
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 0 35.56)
          (xy 0 0)
        )
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 0 35.56)
          (xy 53.34 35.56)
        )
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 0 55.88)
          (xy 0 35.56)
        )
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 53.34 0)
          (xy 53.34 35.56)
        )
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 53.34 35.56)
          (xy 53.34 55.88)
        )
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 53.34 55.88)
          (xy 0 55.88)
        )
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (text "1x13 pin header" (at 25.4 38.1 0)
        (effects (font (size 1.27 1.27)) (justify bottom))
      )
      (text "2x13 pin header" (at 25.4 22.86 900)
        (effects (font (size 1.27 1.27)) (justify bottom))
      )
      (pin power_in line (at 27.94 58.42 270) (length 2.54)
        (name "3V3" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 0 0))))
      )
      (pin bidirectional line (at 55.88 30.48 180) (length 2.54)
        (name "UART1_RX/PG07" (effects (font (size 1.27 1.27))))
        (number "10" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 55.88 22.86 180) (length 2.54)
        (name "UART5_RX/PA01" (effects (font (size 1.27 1.27))))
        (number "11" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 55.88 10.16 180) (length 2.54)
        (name "SIM_CLK/PA_EINT7/PA07" (effects (font (size 1.27 1.27))))
        (number "12" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 55.88 25.4 180) (length 2.54)
        (name "UART5_TX/PA00" (effects (font (size 1.27 1.27))))
        (number "13" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 25.4 -2.54 90) (length 2.54)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "14" (effects (font (size 0 0))))
      )
      (pin bidirectional line (at 55.88 17.78 180) (length 2.54)
        (name "UART2_CTS/PA03" (effects (font (size 1.27 1.27))))
        (number "15" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -2.54 22.86 0) (length 2.54)
        (name "PA19/TWI1_SDA" (effects (font (size 1.27 1.27))))
        (number "16" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 27.94 58.42 270) (length 2.54)
        (name "3V3" (effects (font (size 1.27 1.27))))
        (number "17" (effects (font (size 0 0))))
      )
      (pin bidirectional line (at -2.54 25.4 0) (length 2.54)
        (name "PA18/TWI1_SCL" (effects (font (size 1.27 1.27))))
        (number "18" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -2.54 12.7 0) (length 2.54)
        (name "PA15/SPI1_MOSI" (effects (font (size 1.27 1.27))))
        (number "19" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 22.86 58.42 270) (length 2.54)
        (name "5V" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 0 0))))
      )
      (pin power_in line (at 25.4 -2.54 90) (length 2.54)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "20" (effects (font (size 0 0))))
      )
      (pin bidirectional line (at -2.54 10.16 0) (length 2.54)
        (name "PA16/SPI1_MISO" (effects (font (size 1.27 1.27))))
        (number "21" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 55.88 20.32 180) (length 2.54)
        (name "UART2_RTS/PA02" (effects (font (size 1.27 1.27))))
        (number "22" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -2.54 15.24 0) (length 2.54)
        (name "PA14/SPI1_CLK" (effects (font (size 1.27 1.27))))
        (number "23" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -2.54 17.78 0) (length 2.54)
        (name "PA13/SPI1_CS" (effects (font (size 1.27 1.27))))
        (number "24" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 25.4 -2.54 90) (length 2.54)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "25" (effects (font (size 0 0))))
      )
      (pin bidirectional line (at 55.88 7.62 180) (length 2.54)
        (name "SIM_DET/PA_EINT10/PA10" (effects (font (size 1.27 1.27))))
        (number "26" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 22.86 58.42 270) (length 2.54)
        (name "5V" (effects (font (size 1.27 1.27))))
        (number "27" (effects (font (size 0 0))))
      )
      (pin power_in line (at 22.86 58.42 270) (length 2.54)
        (name "5V" (effects (font (size 1.27 1.27))))
        (number "27" (effects (font (size 0 0))))
      )
      (pin power_in line (at 25.4 -2.54 90) (length 2.54)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "28" (effects (font (size 0 0))))
      )
      (pin bidirectional line (at -2.54 48.26 0) (length 2.54)
        (name "USB-DM2" (effects (font (size 1.27 1.27))))
        (number "29" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -2.54 30.48 0) (length 2.54)
        (name "PA12/TWI0_SDA" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -2.54 45.72 0) (length 2.54)
        (name "USB-DP2" (effects (font (size 1.27 1.27))))
        (number "30" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -2.54 40.64 0) (length 2.54)
        (name "USB-DM3" (effects (font (size 1.27 1.27))))
        (number "31" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -2.54 38.1 0) (length 2.54)
        (name "USB-DP3" (effects (font (size 1.27 1.27))))
        (number "32" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 55.88 40.64 180) (length 2.54)
        (name "LINE_OUT-R" (effects (font (size 1.27 1.27))))
        (number "33" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 55.88 43.18 180) (length 2.54)
        (name "LINE_OUT-L" (effects (font (size 1.27 1.27))))
        (number "34" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 55.88 38.1 180) (length 2.54)
        (name "VIDEO_OUT" (effects (font (size 1.27 1.27))))
        (number "35" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 55.88 53.34 180) (length 2.54)
        (name "MIC_BIAS" (effects (font (size 1.27 1.27))))
        (number "36" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 55.88 50.8 180) (length 2.54)
        (name "MIC_IN-P" (effects (font (size 1.27 1.27))))
        (number "37" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 55.88 48.26 180) (length 2.54)
        (name "MIC_IN-N" (effects (font (size 1.27 1.27))))
        (number "38" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at -2.54 53.34 0) (length 2.54)
        (name "IR-RX" (effects (font (size 1.27 1.27))))
        (number "39" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 22.86 58.42 270) (length 2.54)
        (name "5V" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 0 0))))
      )
      (pin power_in line (at 22.86 58.42 270) (length 2.54)
        (name "5V" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 0 0))))
      )
      (pin bidirectional line (at -2.54 33.02 0) (length 2.54)
        (name "PA11/TWI0_SCL" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 25.4 -2.54 90) (length 2.54)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "6" (effects (font (size 0 0))))
      )
      (pin bidirectional line (at 55.88 12.7 180) (length 2.54)
        (name "PWM1/PA06" (effects (font (size 1.27 1.27))))
        (number "7" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 55.88 33.02 180) (length 2.54)
        (name "UART1_TX/PG06" (effects (font (size 1.27 1.27))))
        (number "8" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 25.4 -2.54 90) (length 2.54)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "9" (effects (font (size 0 0))))
      )
    )
  )
  (symbol "OPI-ZERO-XHAT" (pin_names (offset 1.016)) (in_bom yes) (on_board yes)
    (property "Reference" "X" (id 0) (at 2.54 5.08 0)
      (effects (font (size 1.4986 1.4986)) (justify left bottom))
    )
    (property "Value" "OPI-ZERO-XHAT" (id 1) (at 2.54 2.54 0)
      (effects (font (size 1.4986 1.4986)) (justify left bottom))
    )
    (property "Footprint" "opi-hat:OPIOHATDEB" (id 2) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "" (id 3) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "OPI-ZERO-XHAT_1_0"
      (polyline
        (pts
          (xy 0 0)
          (xy 53.34 0)
        )
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 0 35.56)
          (xy 0 0)
        )
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 0 35.56)
          (xy 53.34 35.56)
        )
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 0 55.88)
          (xy 0 35.56)
        )
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 53.34 0)
          (xy 53.34 35.56)
        )
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 53.34 35.56)
          (xy 53.34 55.88)
        )
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 53.34 55.88)
          (xy 0 55.88)
        )
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (text "1x13 pin header" (at 25.4 38.1 0)
        (effects (font (size 1.27 1.27)) (justify bottom))
      )
      (text "2x13 pin header" (at 25.4 22.86 900)
        (effects (font (size 1.27 1.27)) (justify bottom))
      )
      (pin power_in line (at 27.94 58.42 270) (length 2.54)
        (name "3V3" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 0 0))))
      )
      (pin bidirectional line (at 55.88 30.48 180) (length 2.54)
        (name "UART1_RX/PG07" (effects (font (size 1.27 1.27))))
        (number "10" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 55.88 22.86 180) (length 2.54)
        (name "UART2_RX/PA01" (effects (font (size 1.27 1.27))))
        (number "11" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 55.88 10.16 180) (length 2.54)
        (name "SIM_CLK/PA_EINT7/PA07" (effects (font (size 1.27 1.27))))
        (number "12" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 55.88 25.4 180) (length 2.54)
        (name "UART2_TX/PA00" (effects (font (size 1.27 1.27))))
        (number "13" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 25.4 -2.54 90) (length 2.54)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "14" (effects (font (size 0 0))))
      )
      (pin bidirectional line (at 55.88 17.78 180) (length 2.54)
        (name "UART2_CTS/PA03" (effects (font (size 1.27 1.27))))
        (number "15" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -2.54 22.86 0) (length 2.54)
        (name "PA19/TWI1_SDA" (effects (font (size 1.27 1.27))))
        (number "16" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 27.94 58.42 270) (length 2.54)
        (name "3V3" (effects (font (size 1.27 1.27))))
        (number "17" (effects (font (size 0 0))))
      )
      (pin bidirectional line (at -2.54 25.4 0) (length 2.54)
        (name "PA18/TWI1_SCL" (effects (font (size 1.27 1.27))))
        (number "18" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -2.54 12.7 0) (length 2.54)
        (name "PA15/SPI1_MOSI" (effects (font (size 1.27 1.27))))
        (number "19" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 22.86 58.42 270) (length 2.54)
        (name "5V" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 0 0))))
      )
      (pin power_in line (at 25.4 -2.54 90) (length 2.54)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "20" (effects (font (size 0 0))))
      )
      (pin bidirectional line (at -2.54 10.16 0) (length 2.54)
        (name "PA16/SPI1_MISO" (effects (font (size 1.27 1.27))))
        (number "21" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 55.88 20.32 180) (length 2.54)
        (name "UART2_RTS/PA02" (effects (font (size 1.27 1.27))))
        (number "22" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -2.54 15.24 0) (length 2.54)
        (name "PA14/SPI1_CLK" (effects (font (size 1.27 1.27))))
        (number "23" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -2.54 17.78 0) (length 2.54)
        (name "PA13/SPI1_CS" (effects (font (size 1.27 1.27))))
        (number "24" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 25.4 -2.54 90) (length 2.54)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "25" (effects (font (size 0 0))))
      )
      (pin bidirectional line (at 55.88 7.62 180) (length 2.54)
        (name "SIM_DET/PA_EINT10/PA10" (effects (font (size 1.27 1.27))))
        (number "26" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 22.86 58.42 270) (length 2.54)
        (name "5V" (effects (font (size 1.27 1.27))))
        (number "27" (effects (font (size 0 0))))
      )
      (pin power_in line (at 25.4 -2.54 90) (length 2.54)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "28" (effects (font (size 0 0))))
      )
      (pin bidirectional line (at -2.54 48.26 0) (length 2.54)
        (name "USB-DM2" (effects (font (size 1.27 1.27))))
        (number "29" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -2.54 30.48 0) (length 2.54)
        (name "PA12/TWI0_SDA" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -2.54 45.72 0) (length 2.54)
        (name "USB-DP2" (effects (font (size 1.27 1.27))))
        (number "30" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -2.54 40.64 0) (length 2.54)
        (name "USB-DM3" (effects (font (size 1.27 1.27))))
        (number "31" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -2.54 38.1 0) (length 2.54)
        (name "USB-DP3" (effects (font (size 1.27 1.27))))
        (number "32" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 55.88 40.64 180) (length 2.54)
        (name "LINE_OUT-R" (effects (font (size 1.27 1.27))))
        (number "33" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 55.88 43.18 180) (length 2.54)
        (name "LINE_OUT-L" (effects (font (size 1.27 1.27))))
        (number "34" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 55.88 38.1 180) (length 2.54)
        (name "VIDEO_OUT" (effects (font (size 1.27 1.27))))
        (number "35" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 55.88 53.34 180) (length 2.54)
        (name "MIC_BIAS" (effects (font (size 1.27 1.27))))
        (number "36" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 55.88 50.8 180) (length 2.54)
        (name "MIC_IN-P" (effects (font (size 1.27 1.27))))
        (number "37" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 55.88 48.26 180) (length 2.54)
        (name "MIC_IN-N" (effects (font (size 1.27 1.27))))
        (number "38" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at -2.54 53.34 0) (length 2.54)
        (name "IR-RX" (effects (font (size 1.27 1.27))))
        (number "39" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 22.86 58.42 270) (length 2.54)
        (name "5V" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 0 0))))
      )
      (pin bidirectional line (at -2.54 33.02 0) (length 2.54)
        (name "PA11/TWI0_SCL" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 25.4 -2.54 90) (length 2.54)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "6" (effects (font (size 0 0))))
      )
      (pin bidirectional line (at 55.88 12.7 180) (length 2.54)
        (name "PWM1/PA06" (effects (font (size 1.27 1.27))))
        (number "7" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 55.88 33.02 180) (length 2.54)
        (name "UART1_TX/PG06" (effects (font (size 1.27 1.27))))
        (number "8" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 25.4 -2.54 90) (length 2.54)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "9" (effects (font (size 0 0))))
      )
    )
  )
  (symbol "OPI-ZERO-XX" (pin_names (offset 1.016)) (in_bom yes) (on_board yes)
    (property "Reference" "X" (id 0) (at 2.54 5.08 0)
      (effects (font (size 1.4986 1.4986)) (justify left bottom))
    )
    (property "Value" "OPI-ZERO-XX" (id 1) (at 2.54 2.54 0)
      (effects (font (size 1.4986 1.4986)) (justify left bottom))
    )
    (property "Footprint" "opi-hat:OPIOHATDEB" (id 2) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "" (id 3) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "OPI-ZERO-XX_1_0"
      (polyline
        (pts
          (xy 0 0)
          (xy 53.34 0)
        )
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 0 35.56)
          (xy 0 0)
        )
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 0 35.56)
          (xy 53.34 35.56)
        )
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 0 55.88)
          (xy 0 35.56)
        )
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 53.34 0)
          (xy 53.34 35.56)
        )
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 53.34 35.56)
          (xy 53.34 55.88)
        )
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 53.34 55.88)
          (xy 0 55.88)
        )
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (text "1x13 pin header" (at 25.4 38.1 0)
        (effects (font (size 1.27 1.27)) (justify bottom))
      )
      (text "2x13 pin header" (at 25.4 22.86 900)
        (effects (font (size 1.27 1.27)) (justify bottom))
      )
      (pin power_in line (at 27.94 58.42 270) (length 2.54)
        (name "3V3" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 0 0))))
      )
      (pin bidirectional line (at 55.88 30.48 180) (length 2.54)
        (name "UART1_RX/PG07" (effects (font (size 1.27 1.27))))
        (number "10" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 55.88 22.86 180) (length 2.54)
        (name "UART2_RX/PA01" (effects (font (size 1.27 1.27))))
        (number "11" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 55.88 10.16 180) (length 2.54)
        (name "SIM_CLK/PA_EINT7/PA07" (effects (font (size 1.27 1.27))))
        (number "12" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 55.88 25.4 180) (length 2.54)
        (name "UART2_TX/PA00" (effects (font (size 1.27 1.27))))
        (number "13" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 25.4 -2.54 90) (length 2.54)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "14" (effects (font (size 0 0))))
      )
      (pin bidirectional line (at 55.88 17.78 180) (length 2.54)
        (name "UART2_CTS/PA03" (effects (font (size 1.27 1.27))))
        (number "15" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -2.54 22.86 0) (length 2.54)
        (name "PA19/TWI1_SDA" (effects (font (size 1.27 1.27))))
        (number "16" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 27.94 58.42 270) (length 2.54)
        (name "3V3" (effects (font (size 1.27 1.27))))
        (number "17" (effects (font (size 0 0))))
      )
      (pin bidirectional line (at -2.54 25.4 0) (length 2.54)
        (name "PA18/TWI1_SCL" (effects (font (size 1.27 1.27))))
        (number "18" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -2.54 12.7 0) (length 2.54)
        (name "PA15/SPI1_MOSI" (effects (font (size 1.27 1.27))))
        (number "19" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 22.86 58.42 270) (length 2.54)
        (name "5V" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 0 0))))
      )
      (pin power_in line (at 25.4 -2.54 90) (length 2.54)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "20" (effects (font (size 0 0))))
      )
      (pin bidirectional line (at -2.54 10.16 0) (length 2.54)
        (name "PA16/SPI1_MISO" (effects (font (size 1.27 1.27))))
        (number "21" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 55.88 20.32 180) (length 2.54)
        (name "UART2_RTS/PA02" (effects (font (size 1.27 1.27))))
        (number "22" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -2.54 15.24 0) (length 2.54)
        (name "PA14/SPI1_CLK" (effects (font (size 1.27 1.27))))
        (number "23" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -2.54 17.78 0) (length 2.54)
        (name "PA13/SPI1_CS" (effects (font (size 1.27 1.27))))
        (number "24" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 25.4 -2.54 90) (length 2.54)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "25" (effects (font (size 0 0))))
      )
      (pin bidirectional line (at 55.88 7.62 180) (length 2.54)
        (name "SIM_DET/PA_EINT10/PA10" (effects (font (size 1.27 1.27))))
        (number "26" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 22.86 58.42 270) (length 2.54)
        (name "5V" (effects (font (size 1.27 1.27))))
        (number "27" (effects (font (size 0 0))))
      )
      (pin power_in line (at 25.4 -2.54 90) (length 2.54)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "28" (effects (font (size 0 0))))
      )
      (pin bidirectional line (at -2.54 48.26 0) (length 2.54)
        (name "USB-DM2" (effects (font (size 1.27 1.27))))
        (number "29" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -2.54 30.48 0) (length 2.54)
        (name "PA12/TWI0_SDA" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -2.54 45.72 0) (length 2.54)
        (name "USB-DP2" (effects (font (size 1.27 1.27))))
        (number "30" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -2.54 40.64 0) (length 2.54)
        (name "USB-DM3" (effects (font (size 1.27 1.27))))
        (number "31" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -2.54 38.1 0) (length 2.54)
        (name "USB-DP3" (effects (font (size 1.27 1.27))))
        (number "32" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 55.88 40.64 180) (length 2.54)
        (name "LINE_OUT-R" (effects (font (size 1.27 1.27))))
        (number "33" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 55.88 43.18 180) (length 2.54)
        (name "LINE_OUT-L" (effects (font (size 1.27 1.27))))
        (number "34" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 55.88 38.1 180) (length 2.54)
        (name "VIDEO_OUT" (effects (font (size 1.27 1.27))))
        (number "35" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 55.88 53.34 180) (length 2.54)
        (name "MIC_BIAS" (effects (font (size 1.27 1.27))))
        (number "36" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 55.88 50.8 180) (length 2.54)
        (name "MIC_IN-P" (effects (font (size 1.27 1.27))))
        (number "37" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 55.88 48.26 180) (length 2.54)
        (name "MIC_IN-N" (effects (font (size 1.27 1.27))))
        (number "38" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at -2.54 53.34 0) (length 2.54)
        (name "IR-RX" (effects (font (size 1.27 1.27))))
        (number "39" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 22.86 58.42 270) (length 2.54)
        (name "5V" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 0 0))))
      )
      (pin bidirectional line (at -2.54 33.02 0) (length 2.54)
        (name "PA11/TWI0_SCL" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 25.4 -2.54 90) (length 2.54)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "6" (effects (font (size 0 0))))
      )
      (pin bidirectional line (at 55.88 12.7 180) (length 2.54)
        (name "PWM1/PA06" (effects (font (size 1.27 1.27))))
        (number "7" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 55.88 33.02 180) (length 2.54)
        (name "UART1_TX/PG06" (effects (font (size 1.27 1.27))))
        (number "8" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 25.4 -2.54 90) (length 2.54)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "9" (effects (font (size 0 0))))
      )
    )
  )
  (symbol "OPI-ZERO2-XDEB" (pin_names (offset 1.016)) (in_bom yes) (on_board yes)
    (property "Reference" "X" (id 0) (at 2.54 5.08 0)
      (effects (font (size 1.4986 1.4986)) (justify left bottom))
    )
    (property "Value" "OPI-ZERO2-XDEB" (id 1) (at 2.54 2.54 0)
      (effects (font (size 1.4986 1.4986)) (justify left bottom))
    )
    (property "Footprint" "opi-hat:OPIOHATDEB" (id 2) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "" (id 3) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "OPI-ZERO2-XDEB_1_0"
      (polyline
        (pts
          (xy 0 0)
          (xy 53.34 0)
        )
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 0 35.56)
          (xy 0 0)
        )
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 0 35.56)
          (xy 53.34 35.56)
        )
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 0 55.88)
          (xy 0 35.56)
        )
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 53.34 0)
          (xy 53.34 35.56)
        )
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 53.34 35.56)
          (xy 53.34 55.88)
        )
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 53.34 55.88)
          (xy 0 55.88)
        )
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (text "1x13 pin header" (at 25.4 38.1 0)
        (effects (font (size 1.27 1.27)) (justify bottom))
      )
      (text "2x13 pin header" (at 25.4 22.86 900)
        (effects (font (size 1.27 1.27)) (justify bottom))
      )
      (pin power_in line (at 27.94 58.42 270) (length 2.54)
        (name "3V3" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 0 0))))
      )
      (pin bidirectional line (at 55.88 30.48 180) (length 2.54)
        (name "UART5_RX/PG07" (effects (font (size 1.27 1.27))))
        (number "10" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 55.88 22.86 180) (length 2.54)
        (name "PC6" (effects (font (size 1.27 1.27))))
        (number "11" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 55.88 10.16 180) (length 2.54)
        (name "PC11" (effects (font (size 1.27 1.27))))
        (number "12" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 55.88 25.4 180) (length 2.54)
        (name "PC5" (effects (font (size 1.27 1.27))))
        (number "13" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 25.4 -2.54 90) (length 2.54)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "14" (effects (font (size 0 0))))
      )
      (pin bidirectional line (at 55.88 17.78 180) (length 2.54)
        (name "PC8" (effects (font (size 1.27 1.27))))
        (number "15" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 55.88 5.08 180) (length 2.54)
        (name "PC15" (effects (font (size 1.27 1.27))))
        (number "16" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 27.94 58.42 270) (length 2.54)
        (name "3V3" (effects (font (size 1.27 1.27))))
        (number "17" (effects (font (size 0 0))))
      )
      (pin bidirectional line (at 55.88 7.62 180) (length 2.54)
        (name "PC14" (effects (font (size 1.27 1.27))))
        (number "18" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -2.54 12.7 0) (length 2.54)
        (name "PH7/SPI1_MOSI" (effects (font (size 1.27 1.27))))
        (number "19" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 22.86 58.42 270) (length 2.54)
        (name "5V" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 0 0))))
      )
      (pin power_in line (at 25.4 -2.54 90) (length 2.54)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "20" (effects (font (size 0 0))))
      )
      (pin bidirectional line (at -2.54 10.16 0) (length 2.54)
        (name "PH8/SPI1_MISO" (effects (font (size 1.27 1.27))))
        (number "21" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 55.88 20.32 180) (length 2.54)
        (name "PC7" (effects (font (size 1.27 1.27))))
        (number "22" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -2.54 15.24 0) (length 2.54)
        (name "PH6/SPI1_CLK" (effects (font (size 1.27 1.27))))
        (number "23" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -2.54 17.78 0) (length 2.54)
        (name "PH9/SPI1_CS" (effects (font (size 1.27 1.27))))
        (number "24" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 25.4 -2.54 90) (length 2.54)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "25" (effects (font (size 0 0))))
      )
      (pin bidirectional line (at 55.88 12.7 180) (length 2.54)
        (name "PC10" (effects (font (size 1.27 1.27))))
        (number "26" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 22.86 58.42 270) (length 2.54)
        (name "5V" (effects (font (size 1.27 1.27))))
        (number "27" (effects (font (size 0 0))))
      )
      (pin power_in line (at 22.86 58.42 270) (length 2.54)
        (name "5V" (effects (font (size 1.27 1.27))))
        (number "27" (effects (font (size 0 0))))
      )
      (pin power_in line (at 25.4 -2.54 90) (length 2.54)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "28" (effects (font (size 0 0))))
      )
      (pin bidirectional line (at -2.54 48.26 0) (length 2.54)
        (name "USB-DM2" (effects (font (size 1.27 1.27))))
        (number "29" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -2.54 25.4 0) (length 2.54)
        (name "PH5/I2C3_SDA" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -2.54 45.72 0) (length 2.54)
        (name "USB-DP2" (effects (font (size 1.27 1.27))))
        (number "30" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -2.54 40.64 0) (length 2.54)
        (name "USB-DM3" (effects (font (size 1.27 1.27))))
        (number "31" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -2.54 38.1 0) (length 2.54)
        (name "USB-DP3" (effects (font (size 1.27 1.27))))
        (number "32" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 55.88 40.64 180) (length 2.54)
        (name "LINE_OUT-R" (effects (font (size 1.27 1.27))))
        (number "33" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 55.88 43.18 180) (length 2.54)
        (name "LINE_OUT-L" (effects (font (size 1.27 1.27))))
        (number "34" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 55.88 38.1 180) (length 2.54)
        (name "VIDEO_OUT" (effects (font (size 1.27 1.27))))
        (number "35" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 55.88 53.34 180) (length 2.54)
        (name "PC1" (effects (font (size 1.27 1.27))))
        (number "36" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 55.88 50.8 180) (length 2.54)
        (name "PI16" (effects (font (size 1.27 1.27))))
        (number "37" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 55.88 48.26 180) (length 2.54)
        (name "PI6" (effects (font (size 1.27 1.27))))
        (number "38" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at -2.54 53.34 0) (length 2.54)
        (name "IR-RX" (effects (font (size 1.27 1.27))))
        (number "39" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 22.86 58.42 270) (length 2.54)
        (name "5V" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 0 0))))
      )
      (pin power_in line (at 22.86 58.42 270) (length 2.54)
        (name "5V" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 0 0))))
      )
      (pin bidirectional line (at -2.54 27.94 0) (length 2.54)
        (name "PH4/I2C3_SCK" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 25.4 -2.54 90) (length 2.54)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "6" (effects (font (size 0 0))))
      )
      (pin bidirectional line (at 55.88 15.24 180) (length 2.54)
        (name "PC9" (effects (font (size 1.27 1.27))))
        (number "7" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 55.88 33.02 180) (length 2.54)
        (name "UART5_TX/PG06" (effects (font (size 1.27 1.27))))
        (number "8" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 25.4 -2.54 90) (length 2.54)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "9" (effects (font (size 0 0))))
      )
    )
  )
)
