(export (version D)
  (design
    (source /home/eddy/Docs/SAO/ELECTRONICS/STM32/kicad/termo-NX3L4051/termorez.sch)
    (date "Сб 27 дек 2014 18:53:47")
    (tool "eeschema (2013-feb-26)-stable"))
  (components
    (comp (ref U4)
      (value AD7794/7795)
      (libsource (lib my_elements) (part AD7794/7795))
      (sheetpath (names /) (tstamps /))
      (tstamp 524D62C1))
    (comp (ref R4)
      (value "1k 0.1% (RT0805BRB071KL)")
      (footprint SM0805)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 53562118))
    (comp (ref C12)
      (value 47u)
      (libsource (lib device) (part CP1))
      (sheetpath (names /) (tstamps /))
      (tstamp 5357750C))
    (comp (ref L1)
      (value BMB2A0300AN1)
      (libsource (lib device) (part INDUCTOR_SMALL))
      (sheetpath (names /) (tstamps /))
      (tstamp 53577523))
    (comp (ref C9)
      (value 0.1u)
      (libsource (lib device) (part C))
      (sheetpath (names /) (tstamps /))
      (tstamp 53576FB6))
    (comp (ref C8)
      (value 0.33u)
      (libsource (lib device) (part C))
      (sheetpath (names /) (tstamps /))
      (tstamp 53576FC3))
    (comp (ref U5)
      (value LM1117-33)
      (footprint SOT-223)
      (libsource (lib regul) (part LM317AEMP))
      (sheetpath (names /) (tstamps /))
      (tstamp 535787B7))
    (comp (ref R1)
      (value 10k)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 53579396))
    (comp (ref R2)
      (value 10k)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 535793A8))
    (comp (ref P1)
      (value "контакт 1")
      (libsource (lib conn) (part CONN_8))
      (sheetpath (names /) (tstamps /))
      (tstamp 53579853))
    (comp (ref P6)
      (value 5V)
      (libsource (lib conn) (part CONN_2))
      (sheetpath (names /) (tstamps /))
      (tstamp 5357ABB4))
    (comp (ref P4)
      (value MCU)
      (libsource (lib conn) (part CONN_8))
      (sheetpath (names /) (tstamps /))
      (tstamp 5357BA72))
    (comp (ref R3)
      (value 47k)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 5357C8F8))
    (comp (ref P2)
      (value "контакт 2a")
      (libsource (lib conn) (part CONN_8))
      (sheetpath (names /) (tstamps /))
      (tstamp 5475974D))
    (comp (ref P3)
      (value "контакт 2б")
      (libsource (lib conn) (part CONN_8))
      (sheetpath (names /) (tstamps /))
      (tstamp 5475975B))
    (comp (ref DA1)
      (value NX3L4051-HX)
      (footprint HXQFN-16)
      (libsource (lib my_elements) (part NX3L4051-HX))
      (sheetpath (names /) (tstamps /))
      (tstamp 54759E36))
    (comp (ref DA3)
      (value NX3L4051-HX)
      (footprint HXQFN-16)
      (libsource (lib my_elements) (part NX3L4051-HX))
      (sheetpath (names /) (tstamps /))
      (tstamp 5475A2C7))
    (comp (ref DA2)
      (value NX3L4051-HX)
      (footprint HXQFN-16)
      (libsource (lib my_elements) (part NX3L4051-HX))
      (sheetpath (names /) (tstamps /))
      (tstamp 5475A2C1))
    (comp (ref C10)
      (value 1u)
      (libsource (lib device) (part C))
      (sheetpath (names /) (tstamps /))
      (tstamp 5357821E))
    (comp (ref R5)
      (value "1k 0.1% (RT0805BRB071KL)")
      (footprint SM0805)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 547C0DD9))
    (comp (ref R6)
      (value "1k 0.1% (RT0805BRB071KL)")
      (footprint SM0805)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 547C0DE4))
    (comp (ref R7)
      (value "1k 0.1% (RT0805BRB071KL)")
      (footprint SM0805)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 547C0DEA))
    (comp (ref R8)
      (value "1k 0.1% (RT0805BRB071KL)")
      (footprint SM0805)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 547C0DF0))
    (comp (ref X1)
      (value GND_CONNECTOR)
      (footprint GND_CONNECTOR)
      (libsource (lib my_elements) (part GND_CONNECTOR))
      (sheetpath (names /) (tstamps /))
      (tstamp 549EDA1E)))
  (libparts
    (libpart (lib device) (part C)
      (description "Condensateur non polarise")
      (footprints
        (fp SM*)
        (fp C?)
        (fp C1-1))
      (fields
        (field (name Reference) C)
        (field (name Value) C)
        (field (name Footprint) ~)
        (field (name Datasheet) ~))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib device) (part CP1)
      (description "Condensateur polarise")
      (footprints
        (fp CP*)
        (fp SM*))
      (fields
        (field (name Reference) C)
        (field (name Value) CP1)
        (field (name Footprint) ~)
        (field (name Datasheet) ~))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib device) (part INDUCTOR_SMALL)
      (fields
        (field (name Reference) L)
        (field (name Value) INDUCTOR_SMALL)
        (field (name Footprint) ~)
        (field (name Datasheet) ~))
      (pins
        (pin (num 1) (name 1) (type input))
        (pin (num 2) (name 2) (type input))))
    (libpart (lib device) (part R)
      (description Resistance)
      (footprints
        (fp R?)
        (fp SM0603)
        (fp SM0805)
        (fp R?-*)
        (fp SM1206))
      (fields
        (field (name Reference) R)
        (field (name Value) R)
        (field (name Footprint) ~)
        (field (name Datasheet) ~))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib conn) (part CONN_2)
      (description "Symbole general de connecteur")
      (fields
        (field (name Reference) P)
        (field (name Value) CONN_2))
      (pins
        (pin (num 1) (name P1) (type passive))
        (pin (num 2) (name PM) (type passive))))
    (libpart (lib conn) (part CONN_8)
      (description "Symbole general de connecteur")
      (fields
        (field (name Reference) P)
        (field (name Value) CONN_8))
      (pins
        (pin (num 1) (name P1) (type passive))
        (pin (num 2) (name P2) (type passive))
        (pin (num 3) (name P3) (type passive))
        (pin (num 4) (name P4) (type passive))
        (pin (num 5) (name P5) (type passive))
        (pin (num 6) (name P6) (type passive))
        (pin (num 7) (name P7) (type passive))
        (pin (num 8) (name P8) (type passive))))
    (libpart (lib regul) (part LM317EMP)
      (description "LM317EMP, 1A 35V Adjustable Linear Regulator, SOT-223")
      (docs http://www.national.com/ds/LM/LM117.pdf)
      (footprints
        (fp SOT*))
      (fields
        (field (name Reference) U)
        (field (name Value) LM317EMP)
        (field (name Footprint) SOT-223))
      (pins
        (pin (num 1) (name ADJ) (type input))
        (pin (num 2) (name OUT) (type power_out))
        (pin (num 3) (name IN) (type input))))
    (libpart (lib my_elements) (part AD7794/7795)
      (footprints
        (fp TSSOP24)
        (fp SSOP24))
      (fields
        (field (name Reference) U)
        (field (name Value) AD7794/7795)
        (field (name Footprint) TSSOP24)
        (field (name Datasheet) ~))
      (pins
        (pin (num 1) (name SCLK) (type passive))
        (pin (num 2) (name CLC) (type passive))
        (pin (num 3) (name !CS) (type passive))
        (pin (num 5) (name "AIN6(+)/P1") (type BiDi))
        (pin (num 6) (name "AIN6(-)/P2") (type BiDi))
        (pin (num 7) (name "AIN1(+)") (type input))
        (pin (num 8) (name "AIN1(-)") (type input))
        (pin (num 9) (name "AIN2(+)") (type input))
        (pin (num 10) (name "AIN2(-)") (type input))
        (pin (num 11) (name "AIN3(+)") (type input))
        (pin (num 12) (name "AIN3(-)") (type input))
        (pin (num 13) (name "REFIN1(+)") (type input))
        (pin (num 14) (name "REFIN1(-)") (type input))
        (pin (num 15) (name "AIN5(+)/IOUT2") (type input))
        (pin (num 16) (name "AIN5(-)/IOUT1") (type input))
        (pin (num 17) (name "AIN4(+)/REFIN2(+)") (type input))
        (pin (num 18) (name "AIN4(-)/REFIN2(-)") (type input))
        (pin (num 19) (name PSW) (type input))
        (pin (num 20) (name GND) (type power_in))
        (pin (num 21) (name AVDD) (type power_in))
        (pin (num 22) (name DVDD) (type power_in))
        (pin (num 23) (name DOUT/!RDY) (type passive))
        (pin (num 24) (name DIN) (type passive))))
    (libpart (lib my_elements) (part NX3L4051-HX)
      (fields
        (field (name Reference) DA)
        (field (name Value) NX3L4051-HX)
        (field (name Footprint) HXQFN-16)
        (field (name Datasheet) ~))
      (pins
        (pin (num 1) (name Z) (type BiDi))
        (pin (num 2) (name Y7) (type BiDi))
        (pin (num 3) (name Y5) (type BiDi))
        (pin (num 4) (name ~E) (type input))
        (pin (num 6) (name GND) (type power_in))
        (pin (num 7) (name S3) (type input))
        (pin (num 8) (name S2) (type input))
        (pin (num 9) (name S1) (type input))
        (pin (num 10) (name Y3) (type BiDi))
        (pin (num 11) (name Y0) (type BiDi))
        (pin (num 12) (name Y1) (type BiDi))
        (pin (num 13) (name Y2) (type BiDi))
        (pin (num 14) (name VCC) (type power_in))
        (pin (num 15) (name Y4) (type BiDi))
        (pin (num 16) (name Y6) (type BiDi))))
    (libpart (lib my_elements) (part GND_CONNECTOR)
      (footprints
        (fp GND_connector)
        (fp GND*))
      (fields
        (field (name Reference) X)
        (field (name Value) GND_CONNECTOR)
        (field (name Footprint) GND_connector))
      (pins
        (pin (num 1) (name GND1) (type passive))
        (pin (num 2) (name GND2) (type passive)))))
  (libraries
    (library (logical device)
      (uri /usr/share/kicad/library/device.lib))
    (library (logical conn)
      (uri /usr/share/kicad/library/conn.lib))
    (library (logical regul)
      (uri /usr/share/kicad/library/regul.lib))
    (library (logical my_elements)
      (uri my_elements.lib)))
  (nets
    (net (code 1) (name "")
      (node (ref U4) (pin 16))
      (node (ref U4) (pin 7))
      (node (ref DA1) (pin 1)))
    (net (code 2) (name "")
      (node (ref P3) (pin 7))
      (node (ref DA3) (pin 16)))
    (net (code 3) (name AGND)
      (node (ref R2) (pin 2))
      (node (ref R8) (pin 2))
      (node (ref C10) (pin 2))
      (node (ref R1) (pin 2))
      (node (ref X1) (pin 2))
      (node (ref U4) (pin 20))
      (node (ref U4) (pin 11))
      (node (ref U4) (pin 19))
      (node (ref U4) (pin 12))
      (node (ref U4) (pin 10))
      (node (ref U4) (pin 9))
      (node (ref U4) (pin 14))
      (node (ref U4) (pin 17))
      (node (ref U4) (pin 18))
      (node (ref DA3) (pin 6))
      (node (ref DA2) (pin 6))
      (node (ref DA1) (pin 6)))
    (net (code 4) (name "")
      (node (ref P3) (pin 6))
      (node (ref DA3) (pin 3)))
    (net (code 5) (name "")
      (node (ref DA3) (pin 2))
      (node (ref P3) (pin 8)))
    (net (code 6) (name "")
      (node (ref P1) (pin 7))
      (node (ref DA1) (pin 16)))
    (net (code 7) (name "")
      (node (ref DA1) (pin 15))
      (node (ref P1) (pin 5)))
    (net (code 8) (name "")
      (node (ref P1) (pin 3))
      (node (ref DA1) (pin 13)))
    (net (code 9) (name "")
      (node (ref DA2) (pin 3))
      (node (ref P2) (pin 6)))
    (net (code 10) (name "")
      (node (ref DA2) (pin 13))
      (node (ref P2) (pin 3)))
    (net (code 11) (name "")
      (node (ref DA2) (pin 12))
      (node (ref P2) (pin 2)))
    (net (code 12) (name "")
      (node (ref DA2) (pin 11))
      (node (ref P2) (pin 1)))
    (net (code 13) (name "")
      (node (ref DA2) (pin 10))
      (node (ref P2) (pin 4)))
    (net (code 14) (name "")
      (node (ref DA1) (pin 12))
      (node (ref P1) (pin 2)))
    (net (code 15) (name "")
      (node (ref P2) (pin 8))
      (node (ref DA2) (pin 2)))
    (net (code 16) (name "")
      (node (ref P3) (pin 4))
      (node (ref DA3) (pin 10)))
    (net (code 17) (name "")
      (node (ref P3) (pin 3))
      (node (ref DA3) (pin 13)))
    (net (code 18) (name "")
      (node (ref P3) (pin 2))
      (node (ref DA3) (pin 12)))
    (net (code 19) (name "")
      (node (ref P3) (pin 1))
      (node (ref DA3) (pin 11)))
    (net (code 20) (name "")
      (node (ref P2) (pin 7))
      (node (ref DA2) (pin 16)))
    (net (code 21) (name "")
      (node (ref DA2) (pin 15))
      (node (ref P2) (pin 5)))
    (net (code 22) (name "")
      (node (ref DA3) (pin 15))
      (node (ref P3) (pin 5)))
    (net (code 23) (name GND)
      (node (ref C12) (pin 2))
      (node (ref U5) (pin 1))
      (node (ref P4) (pin 5))
      (node (ref C8) (pin 2))
      (node (ref C9) (pin 2))
      (node (ref U4) (pin 2))
      (node (ref U4) (pin 3))
      (node (ref X1) (pin 1))
      (node (ref R3) (pin 2))
      (node (ref P6) (pin 1)))
    (net (code 24) (name "")
      (node (ref P1) (pin 1))
      (node (ref DA1) (pin 11)))
    (net (code 25) (name "")
      (node (ref DA1) (pin 10))
      (node (ref P1) (pin 4)))
    (net (code 26) (name "")
      (node (ref P1) (pin 6))
      (node (ref DA1) (pin 3)))
    (net (code 27) (name "")
      (node (ref DA1) (pin 2))
      (node (ref P1) (pin 8)))
    (net (code 28) (name "")
      (node (ref R5) (pin 2))
      (node (ref R4) (pin 2)))
    (net (code 29) (name "")
      (node (ref R7) (pin 2))
      (node (ref R6) (pin 2)))
    (net (code 30) (name "")
      (node (ref R6) (pin 1))
      (node (ref R5) (pin 1)))
    (net (code 31) (name "")
      (node (ref R7) (pin 1))
      (node (ref R8) (pin 1)))
    (net (code 32) (name +3.3V)
      (node (ref U4) (pin 21))
      (node (ref C10) (pin 1))
      (node (ref L1) (pin 2)))
    (net (code 33) (name VDD)
      (node (ref C12) (pin 1))
      (node (ref C9) (pin 1))
      (node (ref L1) (pin 1))
      (node (ref U5) (pin 2))
      (node (ref DA2) (pin 14))
      (node (ref DA1) (pin 14))
      (node (ref DA3) (pin 14))
      (node (ref U4) (pin 22)))
    (net (code 34) (name /A1)
      (node (ref P4) (pin 3))
      (node (ref DA3) (pin 8))
      (node (ref DA1) (pin 8))
      (node (ref DA2) (pin 8)))
    (net (code 35) (name /A0)
      (node (ref P4) (pin 2))
      (node (ref DA1) (pin 9))
      (node (ref DA2) (pin 9))
      (node (ref DA3) (pin 9)))
    (net (code 36) (name /EN)
      (node (ref DA1) (pin 4))
      (node (ref R3) (pin 1))
      (node (ref DA2) (pin 4))
      (node (ref DA3) (pin 4))
      (node (ref P4) (pin 1)))
    (net (code 37) (name /A2)
      (node (ref DA1) (pin 7))
      (node (ref P4) (pin 4))
      (node (ref DA2) (pin 7))
      (node (ref DA3) (pin 7)))
    (net (code 38) (name "")
      (node (ref U4) (pin 13))
      (node (ref DA3) (pin 1))
      (node (ref R4) (pin 1)))
    (net (code 39) (name DVDD)
      (node (ref P6) (pin 2))
      (node (ref U5) (pin 3))
      (node (ref C8) (pin 1)))
    (net (code 40) (name "")
      (node (ref DA2) (pin 1))
      (node (ref U4) (pin 15))
      (node (ref U4) (pin 8)))
    (net (code 41) (name /SDO)
      (node (ref U4) (pin 24))
      (node (ref P4) (pin 7)))
    (net (code 42) (name /SDI)
      (node (ref P4) (pin 8))
      (node (ref U4) (pin 23)))
    (net (code 43) (name "")
      (node (ref R2) (pin 1))
      (node (ref U4) (pin 6)))
    (net (code 44) (name "")
      (node (ref U4) (pin 5))
      (node (ref R1) (pin 1)))
    (net (code 45) (name /SC)
      (node (ref U4) (pin 1))
      (node (ref P4) (pin 6)))))