(export (version D)
  (design
    (source /home/eddy/Docs/SAO/ELECTRONICS/STM32/kicad/termo/termorez.sch)
    (date "Чт 24 апр 2014 14:47:57")
    (tool "eeschema (2013-feb-26)-stable"))
  (components
    (comp (ref U4)
      (value AD7794/7795)
      (libsource (lib my_elements) (part AD7794/7795))
      (sheetpath (names /) (tstamps /))
      (tstamp 524D62C1))
    (comp (ref U1)
      (value ADG506A)
      (libsource (lib my_elements) (part ADG506A))
      (sheetpath (names /) (tstamps /))
      (tstamp 524D638F))
    (comp (ref U2)
      (value ADG506A)
      (libsource (lib my_elements) (part ADG506A))
      (sheetpath (names /) (tstamps /))
      (tstamp 524E4CE6))
    (comp (ref U3)
      (value ADG506A)
      (libsource (lib my_elements) (part ADG506A))
      (sheetpath (names /) (tstamps /))
      (tstamp 524E54D1))
    (comp (ref R4)
      (value "5.1k PREC!")
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 53562118))
    (comp (ref C1)
      (value 0.1u)
      (libsource (lib device) (part C))
      (sheetpath (names /) (tstamps /))
      (tstamp 53576CAA))
    (comp (ref C2)
      (value 0.1u)
      (libsource (lib device) (part C))
      (sheetpath (names /) (tstamps /))
      (tstamp 53576E16))
    (comp (ref C3)
      (value 0.1u)
      (libsource (lib device) (part C))
      (sheetpath (names /) (tstamps /))
      (tstamp 53576E2C))
    (comp (ref C4)
      (value 0.1u)
      (libsource (lib device) (part C))
      (sheetpath (names /) (tstamps /))
      (tstamp 53577203))
    (comp (ref C5)
      (value 10u)
      (libsource (lib device) (part C))
      (sheetpath (names /) (tstamps /))
      (tstamp 53577209))
    (comp (ref C6)
      (value 0.1u)
      (libsource (lib device) (part C))
      (sheetpath (names /) (tstamps /))
      (tstamp 535773CF))
    (comp (ref C7)
      (value 10u)
      (libsource (lib device) (part C))
      (sheetpath (names /) (tstamps /))
      (tstamp 535773D5))
    (comp (ref C11)
      (value 1u)
      (libsource (lib device) (part C))
      (sheetpath (names /) (tstamps /))
      (tstamp 535774FF))
    (comp (ref C12)
      (value 10u)
      (libsource (lib device) (part C))
      (sheetpath (names /) (tstamps /))
      (tstamp 5357750C))
    (comp (ref L1)
      (value BMB2A0300AN1)
      (libsource (lib device) (part INDUCTOR_SMALL))
      (sheetpath (names /) (tstamps /))
      (tstamp 53577523))
    (comp (ref C9)
      (value 0.1u)
      (libsource (lib device) (part C))
      (sheetpath (names /) (tstamps /))
      (tstamp 53576FB6))
    (comp (ref C8)
      (value 0.33u)
      (libsource (lib device) (part C))
      (sheetpath (names /) (tstamps /))
      (tstamp 53576FC3))
    (comp (ref JP2)
      (value "VDD ext")
      (libsource (lib device) (part JUMPER))
      (sheetpath (names /) (tstamps /))
      (tstamp 53576FD5))
    (comp (ref JP1)
      (value "VDD int")
      (libsource (lib device) (part JUMPER))
      (sheetpath (names /) (tstamps /))
      (tstamp 5357756C))
    (comp (ref L2)
      (value BMB2A0300AN1)
      (libsource (lib device) (part INDUCTOR_SMALL))
      (sheetpath (names /) (tstamps /))
      (tstamp 53577663))
    (comp (ref C13)
      (value 100u)
      (libsource (lib device) (part C))
      (sheetpath (names /) (tstamps /))
      (tstamp 53577669))
    (comp (ref C10)
      (value 1u)
      (libsource (lib device) (part C))
      (sheetpath (names /) (tstamps /))
      (tstamp 5357821E))
    (comp (ref U5)
      (value LM1117-05)
      (footprint SOT-223)
      (libsource (lib regul) (part LM317AEMP))
      (sheetpath (names /) (tstamps /))
      (tstamp 535787B7))
    (comp (ref R1)
      (value 10k)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 53579396))
    (comp (ref R2)
      (value 10k)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 535793A8))
    (comp (ref P1)
      (value "контакт 1")
      (libsource (lib my_elements) (part CONN_16))
      (sheetpath (names /) (tstamps /))
      (tstamp 53579853))
    (comp (ref P2)
      (value "контакт 2А")
      (libsource (lib my_elements) (part CONN_16))
      (sheetpath (names /) (tstamps /))
      (tstamp 5357A1B9))
    (comp (ref P3)
      (value "контакт 2Б")
      (libsource (lib my_elements) (part CONN_16))
      (sheetpath (names /) (tstamps /))
      (tstamp 5357A1CF))
    (comp (ref P5)
      (value 12V)
      (libsource (lib conn) (part CONN_2))
      (sheetpath (names /) (tstamps /))
      (tstamp 5357A978))
    (comp (ref P6)
      (value 5V)
      (libsource (lib conn) (part CONN_2))
      (sheetpath (names /) (tstamps /))
      (tstamp 5357ABB4))
    (comp (ref P4)
      (value MCU)
      (libsource (lib conn) (part CONN_8))
      (sheetpath (names /) (tstamps /))
      (tstamp 5357BA72))
    (comp (ref R3)
      (value 47k)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 5357C8F8)))
  (libparts
    (libpart (lib device) (part C)
      (description "Condensateur non polarise")
      (footprints
        (fp SM*)
        (fp C?)
        (fp C1-1))
      (fields
        (field (name Reference) C)
        (field (name Value) C)
        (field (name Footprint) ~)
        (field (name Datasheet) ~))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib device) (part INDUCTOR_SMALL)
      (fields
        (field (name Reference) L)
        (field (name Value) INDUCTOR_SMALL)
        (field (name Footprint) ~)
        (field (name Datasheet) ~))
      (pins
        (pin (num 1) (name 1) (type input))
        (pin (num 2) (name 2) (type input))))
    (libpart (lib device) (part JUMPER)
      (fields
        (field (name Reference) JP)
        (field (name Value) JUMPER)
        (field (name Footprint) ~)
        (field (name Datasheet) ~))
      (pins
        (pin (num 1) (name 1) (type passive))
        (pin (num 2) (name 2) (type passive))))
    (libpart (lib device) (part R)
      (description Resistance)
      (footprints
        (fp R?)
        (fp SM0603)
        (fp SM0805)
        (fp R?-*)
        (fp SM1206))
      (fields
        (field (name Reference) R)
        (field (name Value) R)
        (field (name Footprint) ~)
        (field (name Datasheet) ~))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib conn) (part CONN_2)
      (description "Symbole general de connecteur")
      (fields
        (field (name Reference) P)
        (field (name Value) CONN_2))
      (pins
        (pin (num 1) (name P1) (type passive))
        (pin (num 2) (name PM) (type passive))))
    (libpart (lib conn) (part CONN_8)
      (description "Symbole general de connecteur")
      (fields
        (field (name Reference) P)
        (field (name Value) CONN_8))
      (pins
        (pin (num 1) (name P1) (type passive))
        (pin (num 2) (name P2) (type passive))
        (pin (num 3) (name P3) (type passive))
        (pin (num 4) (name P4) (type passive))
        (pin (num 5) (name P5) (type passive))
        (pin (num 6) (name P6) (type passive))
        (pin (num 7) (name P7) (type passive))
        (pin (num 8) (name P8) (type passive))))
    (libpart (lib regul) (part LM317EMP)
      (description "LM317EMP, 1A 35V Adjustable Linear Regulator, SOT-223")
      (docs http://www.national.com/ds/LM/LM117.pdf)
      (footprints
        (fp SOT*))
      (fields
        (field (name Reference) U)
        (field (name Value) LM317EMP)
        (field (name Footprint) SOT-223))
      (pins
        (pin (num 1) (name ADJ) (type input))
        (pin (num 2) (name OUT) (type power_out))
        (pin (num 3) (name IN) (type input))))
    (libpart (lib my_elements) (part AD7794/7795)
      (footprints
        (fp TSSOP24)
        (fp SSOP24))
      (fields
        (field (name Reference) U)
        (field (name Value) AD7794/7795)
        (field (name Footprint) ~)
        (field (name Datasheet) ~))
      (pins
        (pin (num 1) (name SCLK) (type passive))
        (pin (num 2) (name CLC) (type passive))
        (pin (num 3) (name !CS) (type passive))
        (pin (num 5) (name "AIN6(+)/P1") (type BiDi))
        (pin (num 6) (name "AIN6(-)/P2") (type BiDi))
        (pin (num 7) (name "AIN1(+)") (type input))
        (pin (num 8) (name "AIN1(-)") (type input))
        (pin (num 9) (name "AIN2(+)") (type input))
        (pin (num 10) (name "AIN2(-)") (type input))
        (pin (num 11) (name "AIN3(+)") (type input))
        (pin (num 12) (name "AIN3(-)") (type input))
        (pin (num 13) (name "REFIN1(+)") (type input))
        (pin (num 14) (name "REFIN1(-)") (type input))
        (pin (num 15) (name "AIN5(+)/IOUT2") (type input))
        (pin (num 16) (name "AIN5(-)/IOUT1") (type input))
        (pin (num 17) (name "AIN4(+)/REFIN2(+)") (type input))
        (pin (num 18) (name "AIN4(-)/REFIN2(-)") (type input))
        (pin (num 19) (name PSW) (type input))
        (pin (num 20) (name GND) (type power_in))
        (pin (num 21) (name AVDD) (type power_in))
        (pin (num 22) (name DVDD) (type power_in))
        (pin (num 23) (name DOUT/!RDY) (type passive))
        (pin (num 24) (name DIN) (type passive))))
    (libpart (lib my_elements) (part ADG506A)
      (fields
        (field (name Reference) U)
        (field (name Value) ADG506A)
        (field (name Footprint) ~)
        (field (name Datasheet) ~))
      (pins
        (pin (num 1) (name VDD) (type power_in))
        (pin (num 4) (name S16) (type input))
        (pin (num 5) (name S15) (type input))
        (pin (num 6) (name S14) (type input))
        (pin (num 7) (name S13) (type input))
        (pin (num 8) (name S12) (type input))
        (pin (num 9) (name S11) (type input))
        (pin (num 10) (name S10) (type input))
        (pin (num 11) (name S9) (type input))
        (pin (num 12) (name GND) (type power_in))
        (pin (num 14) (name A3) (type passive))
        (pin (num 15) (name A2) (type passive))
        (pin (num 16) (name A1) (type passive))
        (pin (num 17) (name A0) (type passive))
        (pin (num 18) (name EN) (type passive))
        (pin (num 19) (name S1) (type input))
        (pin (num 20) (name S2) (type input))
        (pin (num 21) (name S3) (type input))
        (pin (num 22) (name S4) (type input))
        (pin (num 23) (name S5) (type input))
        (pin (num 24) (name S6) (type input))
        (pin (num 25) (name S7) (type input))
        (pin (num 26) (name S8) (type input))
        (pin (num 27) (name VSS) (type power_in))
        (pin (num 28) (name D) (type output))))
    (libpart (lib my_elements) (part CONN_16)
      (description "Symbole general de connexion")
      (fields
        (field (name Reference) P)
        (field (name Value) CONN_16)
        (field (name Footprint) ~)
        (field (name Datasheet) ~))
      (pins
        (pin (num 1) (name P1) (type passive))
        (pin (num 2) (name P2) (type passive))
        (pin (num 3) (name P3) (type passive))
        (pin (num 4) (name P4) (type passive))
        (pin (num 5) (name P5) (type passive))
        (pin (num 6) (name P6) (type passive))
        (pin (num 7) (name P7) (type passive))
        (pin (num 8) (name P8) (type passive))
        (pin (num 9) (name P9) (type passive))
        (pin (num 10) (name P10) (type passive))
        (pin (num 11) (name P11) (type passive))
        (pin (num 12) (name P12) (type passive))
        (pin (num 13) (name P13) (type passive))
        (pin (num 14) (name P14) (type passive))
        (pin (num 15) (name P15) (type passive))
        (pin (num 16) (name P16) (type passive)))))
  (libraries
    (library (logical device)
      (uri /usr/share/kicad/library/device.lib))
    (library (logical conn)
      (uri /usr/share/kicad/library/conn.lib))
    (library (logical regul)
      (uri /usr/share/kicad/library/regul.lib))
    (library (logical my_elements)
      (uri /home/eddy/kicad/my_elements.lib)))
  (nets
    (net (code 1) (name "")
      (node (ref P1) (pin 3))
      (node (ref U1) (pin 21)))
    (net (code 2) (name "")
      (node (ref P1) (pin 2))
      (node (ref U1) (pin 20)))
    (net (code 3) (name "")
      (node (ref P1) (pin 1))
      (node (ref U1) (pin 19)))
    (net (code 4) (name "")
      (node (ref U1) (pin 4))
      (node (ref P1) (pin 16)))
    (net (code 5) (name "")
      (node (ref U1) (pin 5))
      (node (ref P1) (pin 15)))
    (net (code 6) (name "")
      (node (ref U1) (pin 6))
      (node (ref P1) (pin 14)))
    (net (code 7) (name "")
      (node (ref U1) (pin 7))
      (node (ref P1) (pin 13)))
    (net (code 8) (name "")
      (node (ref U1) (pin 8))
      (node (ref P1) (pin 12)))
    (net (code 9) (name "")
      (node (ref U1) (pin 9))
      (node (ref P1) (pin 11)))
    (net (code 10) (name "")
      (node (ref P1) (pin 10))
      (node (ref U1) (pin 10)))
    (net (code 11) (name "")
      (node (ref U1) (pin 11))
      (node (ref P1) (pin 9)))
    (net (code 12) (name "")
      (node (ref P1) (pin 8))
      (node (ref U1) (pin 26)))
    (net (code 13) (name "")
      (node (ref P1) (pin 7))
      (node (ref U1) (pin 25)))
    (net (code 14) (name "")
      (node (ref P1) (pin 6))
      (node (ref U1) (pin 24)))
    (net (code 15) (name "")
      (node (ref U1) (pin 23))
      (node (ref P1) (pin 5)))
    (net (code 16) (name "")
      (node (ref P1) (pin 4))
      (node (ref U1) (pin 22)))
    (net (code 17) (name VDD)
      (node (ref C12) (pin 1))
      (node (ref JP1) (pin 2))
      (node (ref C6) (pin 1))
      (node (ref C7) (pin 1))
      (node (ref JP2) (pin 1))
      (node (ref U4) (pin 22)))
    (net (code 18) (name +5VA)
      (node (ref C5) (pin 1))
      (node (ref C10) (pin 1))
      (node (ref C4) (pin 1))
      (node (ref L1) (pin 2))
      (node (ref U4) (pin 21)))
    (net (code 19) (name "")
      (node (ref R2) (pin 1))
      (node (ref U4) (pin 6)))
    (net (code 20) (name "")
      (node (ref U2) (pin 21))
      (node (ref P2) (pin 3)))
    (net (code 21) (name "")
      (node (ref P2) (pin 2))
      (node (ref U2) (pin 20)))
    (net (code 22) (name "")
      (node (ref U2) (pin 19))
      (node (ref P2) (pin 1)))
    (net (code 23) (name "")
      (node (ref P2) (pin 16))
      (node (ref U2) (pin 4)))
    (net (code 24) (name "")
      (node (ref U2) (pin 5))
      (node (ref P2) (pin 15)))
    (net (code 25) (name "")
      (node (ref U2) (pin 6))
      (node (ref P2) (pin 14)))
    (net (code 26) (name "")
      (node (ref P2) (pin 13))
      (node (ref U2) (pin 7)))
    (net (code 27) (name "")
      (node (ref P2) (pin 12))
      (node (ref U2) (pin 8)))
    (net (code 28) (name "")
      (node (ref U2) (pin 9))
      (node (ref P2) (pin 11)))
    (net (code 29) (name "")
      (node (ref U2) (pin 10))
      (node (ref P2) (pin 10)))
    (net (code 30) (name "")
      (node (ref U2) (pin 11))
      (node (ref P2) (pin 9)))
    (net (code 31) (name "")
      (node (ref P2) (pin 8))
      (node (ref U2) (pin 26)))
    (net (code 32) (name "")
      (node (ref P2) (pin 7))
      (node (ref U2) (pin 25)))
    (net (code 33) (name "")
      (node (ref P2) (pin 6))
      (node (ref U2) (pin 24)))
    (net (code 34) (name "")
      (node (ref P2) (pin 5))
      (node (ref U2) (pin 23)))
    (net (code 35) (name "")
      (node (ref U2) (pin 22))
      (node (ref P2) (pin 4)))
    (net (code 36) (name "")
      (node (ref R1) (pin 1))
      (node (ref U4) (pin 5)))
    (net (code 37) (name "")
      (node (ref U4) (pin 13))
      (node (ref R4) (pin 1))
      (node (ref U3) (pin 28)))
    (net (code 38) (name GND)
      (node (ref U4) (pin 11))
      (node (ref U4) (pin 20))
      (node (ref U4) (pin 12))
      (node (ref U3) (pin 27))
      (node (ref U3) (pin 12))
      (node (ref U2) (pin 27))
      (node (ref U4) (pin 17))
      (node (ref R4) (pin 2))
      (node (ref U4) (pin 14))
      (node (ref U4) (pin 19))
      (node (ref U4) (pin 18))
      (node (ref C2) (pin 2))
      (node (ref C11) (pin 2))
      (node (ref C7) (pin 2))
      (node (ref C6) (pin 2))
      (node (ref C5) (pin 2))
      (node (ref C4) (pin 2))
      (node (ref C3) (pin 2))
      (node (ref C1) (pin 2))
      (node (ref C8) (pin 2))
      (node (ref C13) (pin 2))
      (node (ref C9) (pin 2))
      (node (ref U4) (pin 9))
      (node (ref U4) (pin 3))
      (node (ref U4) (pin 2))
      (node (ref U2) (pin 12))
      (node (ref U1) (pin 27))
      (node (ref U1) (pin 12))
      (node (ref U4) (pin 10))
      (node (ref C12) (pin 2))
      (node (ref P5) (pin 2))
      (node (ref R1) (pin 2))
      (node (ref R2) (pin 2))
      (node (ref P6) (pin 2))
      (node (ref R3) (pin 2))
      (node (ref U5) (pin 1))
      (node (ref C10) (pin 2)))
    (net (code 39) (name +12V)
      (node (ref C3) (pin 1))
      (node (ref U2) (pin 1))
      (node (ref C11) (pin 1))
      (node (ref U5) (pin 3))
      (node (ref L2) (pin 1))
      (node (ref C1) (pin 1))
      (node (ref C2) (pin 1))
      (node (ref C8) (pin 1))
      (node (ref U1) (pin 1))
      (node (ref U3) (pin 1)))
    (net (code 40) (name "")
      (node (ref U4) (pin 7))
      (node (ref U4) (pin 16))
      (node (ref U1) (pin 28)))
    (net (code 41) (name "")
      (node (ref U4) (pin 15))
      (node (ref U4) (pin 8))
      (node (ref U2) (pin 28)))
    (net (code 42) (name "")
      (node (ref JP1) (pin 1))
      (node (ref L1) (pin 1))
      (node (ref U5) (pin 2))
      (node (ref C9) (pin 1)))
    (net (code 43) (name /A3)
      (node (ref P4) (pin 5))
      (node (ref U3) (pin 14))
      (node (ref U1) (pin 14))
      (node (ref U2) (pin 14)))
    (net (code 44) (name /A2)
      (node (ref U3) (pin 15))
      (node (ref U1) (pin 15))
      (node (ref U2) (pin 15))
      (node (ref P4) (pin 4)))
    (net (code 45) (name /A1)
      (node (ref U3) (pin 16))
      (node (ref P4) (pin 3))
      (node (ref U1) (pin 16))
      (node (ref U2) (pin 16)))
    (net (code 46) (name /A0)
      (node (ref U2) (pin 17))
      (node (ref U3) (pin 17))
      (node (ref P4) (pin 2))
      (node (ref U1) (pin 17)))
    (net (code 47) (name /EN)
      (node (ref P4) (pin 1))
      (node (ref U3) (pin 18))
      (node (ref U1) (pin 18))
      (node (ref U2) (pin 18))
      (node (ref R3) (pin 1)))
    (net (code 48) (name "")
      (node (ref P3) (pin 3))
      (node (ref U3) (pin 21)))
    (net (code 49) (name "")
      (node (ref P3) (pin 2))
      (node (ref U3) (pin 20)))
    (net (code 50) (name "")
      (node (ref P3) (pin 1))
      (node (ref U3) (pin 19)))
    (net (code 51) (name "")
      (node (ref U3) (pin 4))
      (node (ref P3) (pin 16)))
    (net (code 52) (name "")
      (node (ref P3) (pin 15))
      (node (ref U3) (pin 5)))
    (net (code 53) (name "")
      (node (ref P3) (pin 14))
      (node (ref U3) (pin 6)))
    (net (code 54) (name "")
      (node (ref P3) (pin 13))
      (node (ref U3) (pin 7)))
    (net (code 55) (name "")
      (node (ref U3) (pin 8))
      (node (ref P3) (pin 12)))
    (net (code 56) (name "")
      (node (ref U3) (pin 9))
      (node (ref P3) (pin 11)))
    (net (code 57) (name "")
      (node (ref P3) (pin 10))
      (node (ref U3) (pin 10)))
    (net (code 58) (name "")
      (node (ref P3) (pin 9))
      (node (ref U3) (pin 11)))
    (net (code 59) (name "")
      (node (ref P3) (pin 8))
      (node (ref U3) (pin 26)))
    (net (code 60) (name "")
      (node (ref P3) (pin 7))
      (node (ref U3) (pin 25)))
    (net (code 61) (name "")
      (node (ref U3) (pin 24))
      (node (ref P3) (pin 6)))
    (net (code 62) (name "")
      (node (ref U3) (pin 23))
      (node (ref P3) (pin 5)))
    (net (code 63) (name "")
      (node (ref P3) (pin 4))
      (node (ref U3) (pin 22)))
    (net (code 64) (name DVDD)
      (node (ref JP2) (pin 2))
      (node (ref P6) (pin 1)))
    (net (code 65) (name /SDO)
      (node (ref U4) (pin 24))
      (node (ref P4) (pin 7)))
    (net (code 66) (name /SDI)
      (node (ref U4) (pin 23))
      (node (ref P4) (pin 8)))
    (net (code 67) (name +12Vex)
      (node (ref P5) (pin 1))
      (node (ref L2) (pin 2))
      (node (ref C13) (pin 1)))
    (net (code 68) (name /SC)
      (node (ref U4) (pin 1))
      (node (ref P4) (pin 6)))))