(export (version D)
  (design
    (source /home/eddy/Docs/SAO/ELECTRONICS/STM32/kicad/alltogether/LEDs_in_box.sch)
    (date "Пн 02 мар 2015 16:30:01")
    (tool "eeschema (2013-feb-26)-stable"))
  (components
    (comp (ref D1)
      (value LED)
      (libsource (lib device) (part LED))
      (sheetpath (names /) (tstamps /))
      (tstamp 54F40B18))
    (comp (ref D2)
      (value LED)
      (libsource (lib device) (part LED))
      (sheetpath (names /) (tstamps /))
      (tstamp 54F40B25))
    (comp (ref K1)
      (value CONN_3)
      (libsource (lib conn) (part CONN_3))
      (sheetpath (names /) (tstamps /))
      (tstamp 54F40B2D))
    (comp (ref R2)
      (value 330)
      (footprint SM0603)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 54F40B3C))
    (comp (ref R1)
      (value 330)
      (footprint SM0603)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 54F40B6D))
    (comp (ref D4)
      (value LED)
      (libsource (lib device) (part LED))
      (sheetpath (names /) (tstamps /))
      (tstamp 54F40BD8))
    (comp (ref D5)
      (value LED)
      (libsource (lib device) (part LED))
      (sheetpath (names /) (tstamps /))
      (tstamp 54F40BDE))
    (comp (ref K2)
      (value CONN_4)
      (libsource (lib conn) (part CONN_4))
      (sheetpath (names /) (tstamps /))
      (tstamp 54F40BE4))
    (comp (ref R5)
      (value 6.8k)
      (footprint SM1206)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 54F40BEA))
    (comp (ref R4)
      (value 2.2k)
      (footprint SM0603)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 54F40BF0))
    (comp (ref D3)
      (value LED)
      (libsource (lib device) (part LED))
      (sheetpath (names /) (tstamps /))
      (tstamp 54F40BFF))
    (comp (ref R3)
      (value 2.2k)
      (footprint SM0603)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 54F40C05))
    (comp (ref HOLE1)
      (value HOLE)
      (libsource (lib my_elements) (part HOLE))
      (sheetpath (names /) (tstamps /))
      (tstamp 54F40D0F))
    (comp (ref HOLE2)
      (value HOLE)
      (libsource (lib my_elements) (part HOLE))
      (sheetpath (names /) (tstamps /))
      (tstamp 54F40D1C))
    (comp (ref HOLE3)
      (value HOLE)
      (libsource (lib my_elements) (part HOLE))
      (sheetpath (names /) (tstamps /))
      (tstamp 54F40D22))
    (comp (ref HOLE4)
      (value HOLE)
      (libsource (lib my_elements) (part HOLE))
      (sheetpath (names /) (tstamps /))
      (tstamp 54F40D28)))
  (libparts
    (libpart (lib device) (part LED)
      (footprints
        (fp LED-3MM)
        (fp LED-5MM)
        (fp LED-10MM)
        (fp LED-0603)
        (fp LED-0805)
        (fp LED-1206)
        (fp LEDV))
      (fields
        (field (name Reference) D)
        (field (name Value) LED)
        (field (name Footprint) ~)
        (field (name Datasheet) ~))
      (pins
        (pin (num 1) (name A) (type passive))
        (pin (num 2) (name K) (type passive))))
    (libpart (lib device) (part R)
      (description Resistance)
      (footprints
        (fp R?)
        (fp SM0603)
        (fp SM0805)
        (fp R?-*)
        (fp SM1206))
      (fields
        (field (name Reference) R)
        (field (name Value) R)
        (field (name Footprint) ~)
        (field (name Datasheet) ~))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib conn) (part CONN_3)
      (description "Symbole general de connecteur")
      (fields
        (field (name Reference) K)
        (field (name Value) CONN_3))
      (pins
        (pin (num 1) (name P1) (type passive))
        (pin (num 2) (name PM) (type passive))
        (pin (num 3) (name P3) (type passive))))
    (libpart (lib conn) (part CONN_4)
      (description "Symbole general de connecteur")
      (fields
        (field (name Reference) P)
        (field (name Value) CONN_4))
      (pins
        (pin (num 1) (name P1) (type passive))
        (pin (num 2) (name P2) (type passive))
        (pin (num 3) (name P3) (type passive))
        (pin (num 4) (name P4) (type passive))))
    (libpart (lib my_elements) (part HOLE)
      (description "Simple hole")
      (footprints
        (fp hole*))
      (fields
        (field (name Reference) HOLE)
        (field (name Value) HOLE)
        (field (name Footprint) ~)
        (field (name Datasheet) ~))))
  (libraries
    (library (logical device)
      (uri /usr/share/kicad/library/device.lib))
    (library (logical conn)
      (uri /usr/share/kicad/library/conn.lib))
    (library (logical my_elements)
      (uri my_elements.lib)))
  (nets
    (net (code 1) (name "")
      (node (ref D3) (pin 1))
      (node (ref K2) (pin 1)))
    (net (code 2) (name "")
      (node (ref K2) (pin 3))
      (node (ref D4) (pin 1)))
    (net (code 3) (name "")
      (node (ref R5) (pin 2))
      (node (ref D5) (pin 2)))
    (net (code 4) (name "")
      (node (ref R4) (pin 1))
      (node (ref K2) (pin 4))
      (node (ref R5) (pin 1))
      (node (ref R3) (pin 1)))
    (net (code 5) (name "")
      (node (ref R4) (pin 2))
      (node (ref D4) (pin 2)))
    (net (code 6) (name "")
      (node (ref R3) (pin 2))
      (node (ref D3) (pin 2)))
    (net (code 7) (name "")
      (node (ref D5) (pin 1))
      (node (ref K2) (pin 2)))
    (net (code 8) (name "")
      (node (ref D1) (pin 1))
      (node (ref R1) (pin 2)))
    (net (code 9) (name "")
      (node (ref D1) (pin 2))
      (node (ref K1) (pin 1)))
    (net (code 10) (name "")
      (node (ref D2) (pin 2))
      (node (ref K1) (pin 2)))
    (net (code 11) (name "")
      (node (ref K1) (pin 3))
      (node (ref R2) (pin 1))
      (node (ref R1) (pin 1)))
    (net (code 12) (name "")
      (node (ref R2) (pin 2))
      (node (ref D2) (pin 1)))))