(export (version D)
  (design
    (source /home/eddy/Docs/SAO/ELECTRONICS/STM32/kicad/alltogether/ALL.sch)
    (date "Вс 30 ноя 2014 15:38:48")
    (tool "eeschema (2013-feb-26)-stable"))
  (components
    (comp (ref XP2)
      (value TRD)
      (footprint VASCH10x2)
      (libsource (lib conn) (part CONN_10X2))
      (sheetpath (names /) (tstamps /))
      (tstamp 53956EEF))
    (comp (ref DA5)
      (value RO-1224)
      (footprint SIP-4-RO)
      (libsource (lib my_elements) (part RO-XX))
      (sheetpath (names /) (tstamps /))
      (tstamp 53AC9E48))
    (comp (ref DA1)
      (value IPS5451)
      (footprint TO220-5)
      (libsource (lib my_elements) (part IPS5451))
      (sheetpath (names /) (tstamps /))
      (tstamp 53BC4F8D))
    (comp (ref R19)
      (value 4.7k)
      (footprint SM0603)
      (libsource (lib my_elements) (part R0603))
      (sheetpath (names /) (tstamps /))
      (tstamp 53BEC9FF))
    (comp (ref VD1)
      (value B120-E3)
      (footprint DO-214)
      (libsource (lib device) (part DIODESCH))
      (sheetpath (names /) (tstamps /))
      (tstamp 53CDDF73))
    (comp (ref XP7)
      (value Power)
      (footprint VASCH10x2)
      (libsource (lib conn) (part CONN_10X2))
      (sheetpath (names /) (tstamps /))
      (tstamp 53CA50BA))
    (comp (ref XP1)
      (value GPRM1-61)
      (footprint gprm1-61)
      (libsource (lib my_elements) (part GPRM1-61))
      (sheetpath (names /) (tstamps /))
      (tstamp 53DA1715))
    (comp (ref R44)
      (value 4.7k)
      (footprint SM0603)
      (libsource (lib my_elements) (part R0603))
      (sheetpath (names /) (tstamps /))
      (tstamp 546A5949))
    (comp (ref R43)
      (value 12k)
      (footprint SM0603)
      (libsource (lib my_elements) (part R0603))
      (sheetpath (names /) (tstamps /))
      (tstamp 546A5B54))
    (comp (ref DA3)
      (value RO-1205)
      (footprint SIP-4-RO)
      (libsource (lib my_elements) (part RO-XX))
      (sheetpath (names /) (tstamps /))
      (tstamp 5477C0AD))
    (comp (ref C19)
      (value 1u)
      (footprint SM0805)
      (libsource (lib device) (part C))
      (sheetpath (names /) (tstamps /))
      (tstamp 547DB437))
    (comp (ref P2)
      (value CONN_1)
      (libsource (lib conn) (part CONN_1))
      (sheetpath (names /) (tstamps /))
      (tstamp 5474762D))
    (comp (ref P1)
      (value CONN_1)
      (libsource (lib conn) (part CONN_1))
      (sheetpath (names /) (tstamps /))
      (tstamp 5474C8E5))
    (comp (ref HOLE1)
      (value 3mm)
      (libsource (lib my_elements) (part HOLE))
      (sheetpath (names /) (tstamps /))
      (tstamp 54770F82))
    (comp (ref HOLE3)
      (value 3mm)
      (libsource (lib my_elements) (part HOLE))
      (sheetpath (names /) (tstamps /))
      (tstamp 54774C57))
    (comp (ref HOLE5)
      (value 3mm)
      (libsource (lib my_elements) (part HOLE))
      (sheetpath (names /) (tstamps /))
      (tstamp 547759FC))
    (comp (ref HOLE2)
      (value 3mm)
      (libsource (lib my_elements) (part HOLE))
      (sheetpath (names /) (tstamps /))
      (tstamp 54775C06))
    (comp (ref HOLE4)
      (value 3mm)
      (libsource (lib my_elements) (part HOLE))
      (sheetpath (names /) (tstamps /))
      (tstamp 54775C0C))
    (comp (ref HOLE6)
      (value 3mm)
      (libsource (lib my_elements) (part HOLE))
      (sheetpath (names /) (tstamps /))
      (tstamp 54775C12))
    (comp (ref U1)
      (value LM7805CT)
      (footprint TO-220)
      (libsource (lib regul) (part LM7805CT))
      (sheetpath (names /) (tstamps /))
      (tstamp 547C3BA5))
    (comp (ref C3.1)
      (value 1n)
      (footprint SM0805)
      (libsource (lib device) (part C))
      (sheetpath (names "/Turret slits/") (tstamps /53A910B8/))
      (tstamp 50CECA5D))
    (comp (ref R6.1)
      (value 51k)
      (footprint SM0603)
      (libsource (lib device) (part R))
      (sheetpath (names "/Turret slits/") (tstamps /53A910B8/))
      (tstamp 50CECA5C))
    (comp (ref R5.1)
      (value 51k)
      (footprint SM0603)
      (libsource (lib device) (part R))
      (sheetpath (names "/Turret slits/") (tstamps /53A910B8/))
      (tstamp 50CEC791))
    (comp (ref C2.1)
      (value 1n)
      (footprint SM0805)
      (libsource (lib device) (part C))
      (sheetpath (names "/Turret slits/") (tstamps /53A910B8/))
      (tstamp 50CEC790))
    (comp (ref R2.1)
      (value 0.33)
      (footprint SM2010)
      (libsource (lib device) (part R))
      (sheetpath (names "/Turret slits/") (tstamps /53A910B8/))
      (tstamp 50CEB99A))
    (comp (ref R1.1)
      (value 0.33)
      (footprint SM2010)
      (libsource (lib device) (part R))
      (sheetpath (names "/Turret slits/") (tstamps /53A910B8/))
      (tstamp 50CEB97A))
    (comp (ref C1.1)
      (value 68n)
      (footprint SM0805)
      (libsource (lib device) (part C))
      (sheetpath (names "/Turret slits/") (tstamps /53A910B8/))
      (tstamp 50AF1E60))
    (comp (ref R3.1)
      (value 22k)
      (footprint SM0603)
      (libsource (lib device) (part R))
      (sheetpath (names "/Turret slits/") (tstamps /53A910B8/))
      (tstamp 50AF1C25))
    (comp (ref DD2.1)
      (value L6208N)
      (footprint DIP-24__300_ELL)
      (libsource (lib my_elements) (part L6208N))
      (sheetpath (names "/Turret slits/") (tstamps /53A910B8/))
      (tstamp 50AE2A4D))
    (comp (ref R4.1)
      (value 1.8k)
      (footprint SM0603)
      (libsource (lib device) (part R))
      (sheetpath (names "/Turret slits/") (tstamps /53A910B8/))
      (tstamp 534BB108))
    (comp (ref C17)
      (value 100n)
      (footprint SM0805)
      (libsource (lib device) (part C))
      (sheetpath (names "/STM32F103 module/") (tstamps /53973803/))
      (tstamp 53969846))
    (comp (ref C15)
      (value 100n)
      (footprint SM0805)
      (libsource (lib device) (part C))
      (sheetpath (names "/STM32F103 module/") (tstamps /53973803/))
      (tstamp 5396ADDE))
    (comp (ref C18)
      (value 100n)
      (footprint SM0805)
      (libsource (lib device) (part C))
      (sheetpath (names "/STM32F103 module/") (tstamps /53973803/))
      (tstamp 5396C0ED))
    (comp (ref C16)
      (value 100n)
      (footprint SM0805)
      (libsource (lib device) (part C))
      (sheetpath (names "/STM32F103 module/") (tstamps /53973803/))
      (tstamp 5396C789))
    (comp (ref C13)
      (value 10u)
      (footprint C2)
      (libsource (lib device) (part C))
      (sheetpath (names "/STM32F103 module/") (tstamps /53973803/))
      (tstamp 539751BC))
    (comp (ref C14)
      (value 100n)
      (footprint SM0805)
      (libsource (lib my_elements) (part C0805))
      (sheetpath (names "/STM32F103 module/") (tstamps /53973803/))
      (tstamp 53979DD9))
    (comp (ref DA6)
      (value LM1117MPX-3.3)
      (footprint SOT223)
      (libsource (lib my_elements) (part LM1117MPX-3.3))
      (sheetpath (names "/STM32F103 module/") (tstamps /53973803/))
      (tstamp 53996A85))
    (comp (ref C5)
      (value 10u)
      (footprint C2)
      (libsource (lib device) (part C))
      (sheetpath (names "/STM32F103 module/") (tstamps /53973803/))
      (tstamp 53997111))
    (comp (ref C6)
      (value 100u)
      (footprint C2)
      (libsource (lib device) (part C))
      (sheetpath (names "/STM32F103 module/") (tstamps /53973803/))
      (tstamp 53997130))
    (comp (ref C7)
      (value 100n)
      (footprint SM0805)
      (libsource (lib device) (part C))
      (sheetpath (names "/STM32F103 module/") (tstamps /53973803/))
      (tstamp 5399B7BA))
    (comp (ref SB1)
      (value RESET)
      (footprint SPST)
      (libsource (lib device) (part SW_PUSH))
      (sheetpath (names "/STM32F103 module/") (tstamps /53973803/))
      (tstamp 5399B811))
    (comp (ref R26)
      (value 10k)
      (footprint SM0603)
      (libsource (lib device) (part R))
      (sheetpath (names "/STM32F103 module/") (tstamps /53973803/))
      (tstamp 5399B99B))
    (comp (ref L1)
      (value BMB2A0300AN1)
      (footprint SM0805)
      (libsource (lib my_elements) (part BMB2A0300AN1))
      (sheetpath (names "/STM32F103 module/") (tstamps /53973803/))
      (tstamp 53973C3F))
    (comp (ref VD2)
      (value PWR)
      (footprint SM0603)
      (libsource (lib device) (part LED))
      (sheetpath (names "/STM32F103 module/") (tstamps /53973803/))
      (tstamp 5399C66D))
    (comp (ref R10)
      (value 510)
      (footprint SM0603)
      (libsource (lib device) (part R))
      (sheetpath (names "/STM32F103 module/") (tstamps /53973803/))
      (tstamp 5399C848))
    (comp (ref R11)
      (value 4.7k)
      (footprint SM0603)
      (libsource (lib device) (part R))
      (sheetpath (names "/STM32F103 module/") (tstamps /53973803/))
      (tstamp 53A38ACC))
    (comp (ref C9)
      (value 100n)
      (footprint SM0805)
      (libsource (lib device) (part C))
      (sheetpath (names "/STM32F103 module/") (tstamps /53973803/))
      (tstamp 53A79646))
    (comp (ref G1)
      (value 8MHz)
      (footprint hc49)
      (libsource (lib my_elements) (part QUARTZ))
      (sheetpath (names "/STM32F103 module/") (tstamps /53973803/))
      (tstamp 53B31F6E))
    (comp (ref C10)
      (value 27p)
      (footprint SM0805)
      (libsource (lib my_elements) (part C0805))
      (sheetpath (names "/STM32F103 module/") (tstamps /53973803/))
      (tstamp 53B31F74))
    (comp (ref C11)
      (value 27p)
      (footprint SM0805)
      (libsource (lib my_elements) (part C0805))
      (sheetpath (names "/STM32F103 module/") (tstamps /53973803/))
      (tstamp 53B31F7A))
    (comp (ref R12)
      (value 1M)
      (footprint SM0603)
      (libsource (lib my_elements) (part R0603))
      (sheetpath (names "/STM32F103 module/") (tstamps /53973803/))
      (tstamp 53B323F6))
    (comp (ref R13)
      (value 10k)
      (footprint SM0603)
      (libsource (lib my_elements) (part R0603))
      (sheetpath (names "/STM32F103 module/") (tstamps /53973803/))
      (tstamp 53B858E4))
    (comp (ref R14)
      (value 10k)
      (footprint SM0603)
      (libsource (lib my_elements) (part R0603))
      (sheetpath (names "/STM32F103 module/") (tstamps /53973803/))
      (tstamp 53B858EA))
    (comp (ref R15)
      (value 10k)
      (footprint SM0603)
      (libsource (lib my_elements) (part R0603))
      (sheetpath (names "/STM32F103 module/") (tstamps /53973803/))
      (tstamp 53B85A4F))
    (comp (ref R16)
      (value 10k)
      (footprint SM0603)
      (libsource (lib my_elements) (part R0603))
      (sheetpath (names "/STM32F103 module/") (tstamps /53973803/))
      (tstamp 53B85A5B))
    (comp (ref XP4)
      (value CONN_4)
      (footprint SIL-4)
      (libsource (lib conn) (part CONN_4))
      (sheetpath (names "/STM32F103 module/") (tstamps /53973803/))
      (tstamp 53A259E0))
    (comp (ref XP5)
      (value CONN_7)
      (footprint SIL-7)
      (libsource (lib conn) (part CONN_7))
      (sheetpath (names "/STM32F103 module/") (tstamps /53973803/))
      (tstamp 53A363AA))
    (comp (ref R18)
      (value 100k)
      (footprint SM0603)
      (libsource (lib my_elements) (part R0603))
      (sheetpath (names "/STM32F103 module/") (tstamps /53973803/))
      (tstamp 53A3D1C0))
    (comp (ref R17)
      (value 10k)
      (footprint SM0603)
      (libsource (lib my_elements) (part R0603))
      (sheetpath (names "/STM32F103 module/") (tstamps /53973803/))
      (tstamp 53A3D5DE))
    (comp (ref SB2)
      (value BOOT)
      (footprint SPST)
      (libsource (lib device) (part SW_PUSH))
      (sheetpath (names "/STM32F103 module/") (tstamps /53973803/))
      (tstamp 53A4246E))
    (comp (ref C8)
      (value 100n)
      (footprint SM0805)
      (libsource (lib device) (part C))
      (sheetpath (names "/STM32F103 module/") (tstamps /53973803/))
      (tstamp 53A44EC1))
    (comp (ref DD3)
      (value STM32F103)
      (footprint LQFP100_STM32)
      (libsource (lib STM32f103) (part STM32F103))
      (sheetpath (names "/STM32F103 module/") (tstamps /53973803/))
      (tstamp 53976A8B))
    (comp (ref XP3)
      (value CONN_7)
      (footprint SIL-7)
      (libsource (lib conn) (part CONN_7))
      (sheetpath (names "/STM32F103 module/") (tstamps /53973803/))
      (tstamp 53AD262A))
    (comp (ref R27)
      (value RT0805BRB071KL)
      (footprint SM0805)
      (libsource (lib my_elements) (part RT0805BRB071KL))
      (sheetpath (names "/STM32F103 module/") (tstamps /53973803/))
      (tstamp 53AF4804))
    (comp (ref R28)
      (value RT0805BRB071KL)
      (footprint SM0805)
      (libsource (lib my_elements) (part RT0805BRB071KL))
      (sheetpath (names "/STM32F103 module/") (tstamps /53973803/))
      (tstamp 53AF4838))
    (comp (ref R29)
      (value RT0805BRB071KL)
      (footprint SM0805)
      (libsource (lib my_elements) (part RT0805BRB071KL))
      (sheetpath (names "/STM32F103 module/") (tstamps /53973803/))
      (tstamp 53AF483E))
    (comp (ref R30)
      (value RT0805BRB071KL)
      (footprint SM0805)
      (libsource (lib my_elements) (part RT0805BRB071KL))
      (sheetpath (names "/STM32F103 module/") (tstamps /53973803/))
      (tstamp 53AF4844))
    (comp (ref R31)
      (value RT0805BRB071KL)
      (footprint SM0805)
      (libsource (lib my_elements) (part RT0805BRB071KL))
      (sheetpath (names "/STM32F103 module/") (tstamps /53973803/))
      (tstamp 53AF484A))
    (comp (ref R32)
      (value RT0805BRB071KL)
      (footprint SM0805)
      (libsource (lib my_elements) (part RT0805BRB071KL))
      (sheetpath (names "/STM32F103 module/") (tstamps /53973803/))
      (tstamp 53AF4850))
    (comp (ref R33)
      (value RT0805BRB071KL)
      (footprint SM0805)
      (libsource (lib my_elements) (part RT0805BRB071KL))
      (sheetpath (names "/STM32F103 module/") (tstamps /53973803/))
      (tstamp 53AF4856))
    (comp (ref R34)
      (value RT0805BRB071KL)
      (footprint SM0805)
      (libsource (lib my_elements) (part RT0805BRB071KL))
      (sheetpath (names "/STM32F103 module/") (tstamps /53973803/))
      (tstamp 53AF485C))
    (comp (ref R21)
      (value 15k)
      (footprint SM0603)
      (libsource (lib my_elements) (part R0603))
      (sheetpath (names "/STM32F103 module/") (tstamps /53973803/))
      (tstamp 53C435C5))
    (comp (ref R20)
      (value 15k)
      (footprint SM0603)
      (libsource (lib my_elements) (part R0603))
      (sheetpath (names "/STM32F103 module/") (tstamps /53973803/))
      (tstamp 53C435CB))
    (comp (ref R23)
      (value 10k)
      (footprint SM0603)
      (libsource (lib my_elements) (part R0603))
      (sheetpath (names "/STM32F103 module/") (tstamps /53973803/))
      (tstamp 53C4BB5E))
    (comp (ref R24)
      (value 10k)
      (footprint SM0603)
      (libsource (lib my_elements) (part R0603))
      (sheetpath (names "/STM32F103 module/") (tstamps /53973803/))
      (tstamp 53C4BB64))
    (comp (ref R22)
      (value 10k)
      (footprint SM0603)
      (libsource (lib my_elements) (part R0603))
      (sheetpath (names "/STM32F103 module/") (tstamps /53973803/))
      (tstamp 53C4BB71))
    (comp (ref R37)
      (value 10k)
      (footprint SM0603)
      (libsource (lib my_elements) (part R0603))
      (sheetpath (names "/STM32F103 module/") (tstamps /53973803/))
      (tstamp 53CF8387))
    (comp (ref R38)
      (value 10k)
      (footprint SM0603)
      (libsource (lib my_elements) (part R0603))
      (sheetpath (names "/STM32F103 module/") (tstamps /53973803/))
      (tstamp 53CF8EAC))
    (comp (ref R39)
      (value 10k)
      (footprint SM0603)
      (libsource (lib my_elements) (part R0603))
      (sheetpath (names "/STM32F103 module/") (tstamps /53973803/))
      (tstamp 53CFF43C))
    (comp (ref DA4)
      (value USBLC6-2)
      (footprint SOT23_6)
      (libsource (lib my_elements) (part USBLC6-2))
      (sheetpath (names "/STM32F103 module/USB input circuit/") (tstamps /53973803/53976CAB/))
      (tstamp 5395C045))
    (comp (ref VT1)
      (value DTA114Y)
      (footprint SOT323)
      (libsource (lib transistors) (part DTA114Y))
      (sheetpath (names "/STM32F103 module/USB input circuit/") (tstamps /53973803/53976CAB/))
      (tstamp 5395C059))
    (comp (ref R8)
      (value 15k)
      (footprint SM0603)
      (libsource (lib device) (part R))
      (sheetpath (names "/STM32F103 module/USB input circuit/") (tstamps /53973803/53976CAB/))
      (tstamp 5395CE71))
    (comp (ref R7)
      (value 22k)
      (footprint SM0603)
      (libsource (lib device) (part R))
      (sheetpath (names "/STM32F103 module/USB input circuit/") (tstamps /53973803/53976CAB/))
      (tstamp 5395CE96))
    (comp (ref R9)
      (value 1.5k)
      (footprint SM0603)
      (libsource (lib device) (part R))
      (sheetpath (names "/STM32F103 module/USB input circuit/") (tstamps /53973803/53976CAB/))
      (tstamp 5395D182))
    (comp (ref C12)
      (value 100n)
      (footprint SM0805)
      (libsource (lib device) (part C))
      (sheetpath (names "/STM32F103 module/USB input circuit/") (tstamps /53973803/53976CAB/))
      (tstamp 5395D7E9))
    (comp (ref R35)
      (value 22)
      (footprint SM0603)
      (libsource (lib device) (part R))
      (sheetpath (names "/STM32F103 module/USB input circuit/") (tstamps /53973803/53976CAB/))
      (tstamp 5395E223))
    (comp (ref R36)
      (value 22)
      (footprint SM0603)
      (libsource (lib device) (part R))
      (sheetpath (names "/STM32F103 module/USB input circuit/") (tstamps /53973803/53976CAB/))
      (tstamp 5395E230))
    (comp (ref VD3)
      (value B120-E3)
      (footprint DO-214)
      (libsource (lib device) (part DIODESCH))
      (sheetpath (names "/STM32F103 module/USB input circuit/") (tstamps /53973803/53976CAB/))
      (tstamp 539B75AF))
    (comp (ref CON1)
      (value USB-MICRO-B)
      (footprint MINI-B-USB)
      (libsource (lib my_elements) (part USB-MICRO-B))
      (sheetpath (names "/STM32F103 module/USB input circuit/") (tstamps /53973803/53976CAB/))
      (tstamp 53BE6988))
    (comp (ref XS1)
      (value DB9-F)
      (footprint DB9-F)
      (libsource (lib conn) (part DB9))
      (sheetpath (names "/STM32F103 module/RS-232 level converter/") (tstamps /53973803/53974779/))
      (tstamp 53975A15))
    (comp (ref DD1)
      (value ADM233L)
      (footprint DIP-20__300)
      (libsource (lib my_elements) (part ADM233L))
      (sheetpath (names "/STM32F103 module/RS-232 level converter/") (tstamps /53973803/53974779/))
      (tstamp 53A48DFB))
    (comp (ref XP6)
      (value DB9-M)
      (footprint DB9-M)
      (libsource (lib conn) (part DB9))
      (sheetpath (names "/STM32F103 module/RS-232 level converter/") (tstamps /53973803/53974779/))
      (tstamp 53AB4443))
    (comp (ref C3.2)
      (value 1n)
      (footprint SM0805)
      (libsource (lib device) (part C))
      (sheetpath (names "/Filters slit #1/") (tstamps /53A910B7/))
      (tstamp 50CECA5D))
    (comp (ref R6.2)
      (value 51k)
      (footprint SM0603)
      (libsource (lib device) (part R))
      (sheetpath (names "/Filters slit #1/") (tstamps /53A910B7/))
      (tstamp 50CECA5C))
    (comp (ref R5.2)
      (value 51k)
      (footprint SM0603)
      (libsource (lib device) (part R))
      (sheetpath (names "/Filters slit #1/") (tstamps /53A910B7/))
      (tstamp 50CEC791))
    (comp (ref C2.2)
      (value 1n)
      (footprint SM0805)
      (libsource (lib device) (part C))
      (sheetpath (names "/Filters slit #1/") (tstamps /53A910B7/))
      (tstamp 50CEC790))
    (comp (ref R2.2)
      (value 0.33)
      (footprint SM2010)
      (libsource (lib device) (part R))
      (sheetpath (names "/Filters slit #1/") (tstamps /53A910B7/))
      (tstamp 50CEB99A))
    (comp (ref R1.2)
      (value 0.33)
      (footprint SM2010)
      (libsource (lib device) (part R))
      (sheetpath (names "/Filters slit #1/") (tstamps /53A910B7/))
      (tstamp 50CEB97A))
    (comp (ref C1.2)
      (value 68n)
      (footprint SM0805)
      (libsource (lib device) (part C))
      (sheetpath (names "/Filters slit #1/") (tstamps /53A910B7/))
      (tstamp 50AF1E60))
    (comp (ref R3.2)
      (value 22k)
      (footprint SM0603)
      (libsource (lib device) (part R))
      (sheetpath (names "/Filters slit #1/") (tstamps /53A910B7/))
      (tstamp 50AF1C25))
    (comp (ref DD2.2)
      (value L6208N)
      (footprint DIP-24__300_ELL)
      (libsource (lib my_elements) (part L6208N))
      (sheetpath (names "/Filters slit #1/") (tstamps /53A910B7/))
      (tstamp 50AE2A4D))
    (comp (ref R4.2)
      (value 1.8k)
      (footprint SM0603)
      (libsource (lib device) (part R))
      (sheetpath (names "/Filters slit #1/") (tstamps /53A910B7/))
      (tstamp 534BB108))
    (comp (ref C3.3)
      (value 1n)
      (footprint SM0805)
      (libsource (lib device) (part C))
      (sheetpath (names "/Filters slit #2/") (tstamps /5391724D/))
      (tstamp 50CECA5D))
    (comp (ref R6.3)
      (value 51k)
      (footprint SM0603)
      (libsource (lib device) (part R))
      (sheetpath (names "/Filters slit #2/") (tstamps /5391724D/))
      (tstamp 50CECA5C))
    (comp (ref R5.3)
      (value 51k)
      (footprint SM0603)
      (libsource (lib device) (part R))
      (sheetpath (names "/Filters slit #2/") (tstamps /5391724D/))
      (tstamp 50CEC791))
    (comp (ref C2.3)
      (value 1n)
      (footprint SM0805)
      (libsource (lib device) (part C))
      (sheetpath (names "/Filters slit #2/") (tstamps /5391724D/))
      (tstamp 50CEC790))
    (comp (ref R2.3)
      (value 0.33)
      (footprint SM2010)
      (libsource (lib device) (part R))
      (sheetpath (names "/Filters slit #2/") (tstamps /5391724D/))
      (tstamp 50CEB99A))
    (comp (ref R1.3)
      (value 0.33)
      (footprint SM2010)
      (libsource (lib device) (part R))
      (sheetpath (names "/Filters slit #2/") (tstamps /5391724D/))
      (tstamp 50CEB97A))
    (comp (ref C1.3)
      (value 68n)
      (footprint SM0805)
      (libsource (lib device) (part C))
      (sheetpath (names "/Filters slit #2/") (tstamps /5391724D/))
      (tstamp 50AF1E60))
    (comp (ref R3.3)
      (value 22k)
      (footprint SM0603)
      (libsource (lib device) (part R))
      (sheetpath (names "/Filters slit #2/") (tstamps /5391724D/))
      (tstamp 50AF1C25))
    (comp (ref DD2.3)
      (value L6208N)
      (footprint DIP-24__300_ELL)
      (libsource (lib my_elements) (part L6208N))
      (sheetpath (names "/Filters slit #2/") (tstamps /5391724D/))
      (tstamp 50AE2A4D))
    (comp (ref R4.3)
      (value 1.8k)
      (footprint SM0603)
      (libsource (lib device) (part R))
      (sheetpath (names "/Filters slit #2/") (tstamps /5391724D/))
      (tstamp 534BB108))
    (comp (ref C3.4)
      (value 1n)
      (footprint SM0805)
      (libsource (lib device) (part C))
      (sheetpath (names "/Long stage/") (tstamps /53A910BA/))
      (tstamp 50CECA5D))
    (comp (ref R6.4)
      (value 51k)
      (footprint SM0603)
      (libsource (lib device) (part R))
      (sheetpath (names "/Long stage/") (tstamps /53A910BA/))
      (tstamp 50CECA5C))
    (comp (ref R5.4)
      (value 51k)
      (footprint SM0603)
      (libsource (lib device) (part R))
      (sheetpath (names "/Long stage/") (tstamps /53A910BA/))
      (tstamp 50CEC791))
    (comp (ref C2.4)
      (value 1n)
      (footprint SM0805)
      (libsource (lib device) (part C))
      (sheetpath (names "/Long stage/") (tstamps /53A910BA/))
      (tstamp 50CEC790))
    (comp (ref R2.4)
      (value 0.33)
      (footprint SM2010)
      (libsource (lib device) (part R))
      (sheetpath (names "/Long stage/") (tstamps /53A910BA/))
      (tstamp 50CEB99A))
    (comp (ref R1.4)
      (value 0.33)
      (footprint SM2010)
      (libsource (lib device) (part R))
      (sheetpath (names "/Long stage/") (tstamps /53A910BA/))
      (tstamp 50CEB97A))
    (comp (ref C1.4)
      (value 68n)
      (footprint SM0805)
      (libsource (lib device) (part C))
      (sheetpath (names "/Long stage/") (tstamps /53A910BA/))
      (tstamp 50AF1E60))
    (comp (ref R3.4)
      (value 22k)
      (footprint SM0603)
      (libsource (lib device) (part R))
      (sheetpath (names "/Long stage/") (tstamps /53A910BA/))
      (tstamp 50AF1C25))
    (comp (ref DD2.4)
      (value L6208N)
      (footprint DIP-24__300_ELL)
      (libsource (lib my_elements) (part L6208N))
      (sheetpath (names "/Long stage/") (tstamps /53A910BA/))
      (tstamp 50AE2A4D))
    (comp (ref R4.4)
      (value 1.8k)
      (footprint SM0603)
      (libsource (lib device) (part R))
      (sheetpath (names "/Long stage/") (tstamps /53A910BA/))
      (tstamp 534BB108))
    (comp (ref C3.5)
      (value 1n)
      (footprint SM0805)
      (libsource (lib device) (part C))
      (sheetpath (names "/Short stage/") (tstamps /53A910B9/))
      (tstamp 50CECA5D))
    (comp (ref R6.5)
      (value 51k)
      (footprint SM0603)
      (libsource (lib device) (part R))
      (sheetpath (names "/Short stage/") (tstamps /53A910B9/))
      (tstamp 50CECA5C))
    (comp (ref R5.5)
      (value 51k)
      (footprint SM0603)
      (libsource (lib device) (part R))
      (sheetpath (names "/Short stage/") (tstamps /53A910B9/))
      (tstamp 50CEC791))
    (comp (ref C2.5)
      (value 1n)
      (footprint SM0805)
      (libsource (lib device) (part C))
      (sheetpath (names "/Short stage/") (tstamps /53A910B9/))
      (tstamp 50CEC790))
    (comp (ref R2.5)
      (value 0.33)
      (footprint SM2010)
      (libsource (lib device) (part R))
      (sheetpath (names "/Short stage/") (tstamps /53A910B9/))
      (tstamp 50CEB99A))
    (comp (ref R1.5)
      (value 0.33)
      (footprint SM2010)
      (libsource (lib device) (part R))
      (sheetpath (names "/Short stage/") (tstamps /53A910B9/))
      (tstamp 50CEB97A))
    (comp (ref C1.5)
      (value 68n)
      (footprint SM0805)
      (libsource (lib device) (part C))
      (sheetpath (names "/Short stage/") (tstamps /53A910B9/))
      (tstamp 50AF1E60))
    (comp (ref R3.5)
      (value 22k)
      (footprint SM0603)
      (libsource (lib device) (part R))
      (sheetpath (names "/Short stage/") (tstamps /53A910B9/))
      (tstamp 50AF1C25))
    (comp (ref DD2.5)
      (value L6208N)
      (footprint DIP-24__300_ELL)
      (libsource (lib my_elements) (part L6208N))
      (sheetpath (names "/Short stage/") (tstamps /53A910B9/))
      (tstamp 50AE2A4D))
    (comp (ref R4.5)
      (value 1.8k)
      (footprint SM0603)
      (libsource (lib device) (part R))
      (sheetpath (names "/Short stage/") (tstamps /53A910B9/))
      (tstamp 534BB108))
    (comp (ref VT2.2)
      (value FQP30N06)
      (footprint TO220-3-vert)
      (libsource (lib my_elements) (part NTE2984))
      (sheetpath (names "/Power MOSFET module 1/") (tstamps /53A8FBFD/))
      (tstamp 53AF4F62))
    (comp (ref R40.2)
      (value 68)
      (footprint SM1206)
      (libsource (lib my_elements) (part R1206))
      (sheetpath (names "/Power MOSFET module 1/") (tstamps /53A8FBFD/))
      (tstamp 53C8FF70))
    (comp (ref VT2.1)
      (value FQP30N06)
      (footprint TO220-3-vert)
      (libsource (lib my_elements) (part NTE2984))
      (sheetpath (names "/Power MOSFET module 2/") (tstamps /53AA0E2D/))
      (tstamp 53AF4F62))
    (comp (ref R40.1)
      (value 68)
      (footprint SM1206)
      (libsource (lib my_elements) (part R1206))
      (sheetpath (names "/Power MOSFET module 2/") (tstamps /53AA0E2D/))
      (tstamp 53C8FF70))
    (comp (ref DA2)
      (value TLE5205)
      (footprint TO220-7-12)
      (libsource (lib my_elements) (part TLE5205))
      (sheetpath (names "/Shutter MOSFET/") (tstamps /53AE6F08/))
      (tstamp 53C09F3E))
    (comp (ref R25)
      (value "300 (II)")
      (footprint R7)
      (libsource (lib device) (part R))
      (sheetpath (names "/Shutter MOSFET/") (tstamps /53AE6F08/))
      (tstamp 53C10962))
    (comp (ref C4)
      (value "2200u, 40V")
      (footprint CP36V)
      (libsource (lib device) (part CP1))
      (sheetpath (names "/Shutter MOSFET/") (tstamps /53AE6F08/))
      (tstamp 53C10BBB))
    (comp (ref R42)
      (value 4.7k)
      (footprint SM0603)
      (libsource (lib my_elements) (part R0603))
      (sheetpath (names "/Shutter MOSFET/") (tstamps /53AE6F08/))
      (tstamp 5465870A))
    (comp (ref R41)
      (value 56k)
      (footprint SM0603)
      (libsource (lib my_elements) (part R0603))
      (sheetpath (names "/Shutter MOSFET/") (tstamps /53AE6F08/))
      (tstamp 54658717)))
  (libparts
    (libpart (lib device) (part C)
      (description "Condensateur non polarise")
      (footprints
        (fp SM*)
        (fp C?)
        (fp C1-1))
      (fields
        (field (name Reference) C)
        (field (name Value) C)
        (field (name Footprint) ~)
        (field (name Datasheet) ~))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib device) (part CP1)
      (description "Condensateur polarise")
      (footprints
        (fp CP*)
        (fp SM*))
      (fields
        (field (name Reference) C)
        (field (name Value) CP1)
        (field (name Footprint) ~)
        (field (name Datasheet) ~))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib device) (part DIODESCH)
      (description "Diode schottky")
      (footprints
        (fp D?)
        (fp S*))
      (fields
        (field (name Reference) D)
        (field (name Value) DIODESCH)
        (field (name Footprint) ~)
        (field (name Datasheet) ~))
      (pins
        (pin (num 1) (name A) (type passive))
        (pin (num 2) (name K) (type passive))))
    (libpart (lib device) (part LED)
      (footprints
        (fp LED-3MM)
        (fp LED-5MM)
        (fp LED-10MM)
        (fp LED-0603)
        (fp LED-0805)
        (fp LED-1206)
        (fp LEDV))
      (fields
        (field (name Reference) D)
        (field (name Value) LED)
        (field (name Footprint) ~)
        (field (name Datasheet) ~))
      (pins
        (pin (num 1) (name A) (type passive))
        (pin (num 2) (name K) (type passive))))
    (libpart (lib device) (part R)
      (description Resistance)
      (footprints
        (fp R?)
        (fp SM0603)
        (fp SM0805)
        (fp R?-*)
        (fp SM1206))
      (fields
        (field (name Reference) R)
        (field (name Value) R)
        (field (name Footprint) ~)
        (field (name Datasheet) ~))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib device) (part SW_PUSH)
      (description "Push Button")
      (fields
        (field (name Reference) SW)
        (field (name Value) SW_PUSH)
        (field (name Footprint) ~)
        (field (name Datasheet) ~))
      (pins
        (pin (num 1) (name 1) (type passive))
        (pin (num 2) (name 2) (type passive))))
    (libpart (lib transistors) (part DTA114Y)
      (description "DTA114Y, Digital Transistor, 10k/47k, SOT23")
      (footprints
        (fp SOT23*)
        (fp SC59*))
      (fields
        (field (name Reference) Q)
        (field (name Value) DTA114Y))
      (pins
        (pin (num 1) (name B) (type input))
        (pin (num 2) (name E) (type passive))
        (pin (num 3) (name C) (type passive))))
    (libpart (lib conn) (part CONN_1)
      (description "1 pin")
      (fields
        (field (name Reference) P)
        (field (name Value) CONN_1))
      (pins
        (pin (num 1) (name 1) (type passive))))
    (libpart (lib conn) (part CONN_10X2)
      (description "symbole general de connecteur")
      (fields
        (field (name Reference) P)
        (field (name Value) CONN_10X2))
      (pins
        (pin (num 1) (name P1) (type passive))
        (pin (num 2) (name P2) (type passive))
        (pin (num 3) (name P3) (type passive))
        (pin (num 4) (name P4) (type passive))
        (pin (num 5) (name P5) (type passive))
        (pin (num 6) (name P6) (type passive))
        (pin (num 7) (name P7) (type passive))
        (pin (num 8) (name P8) (type passive))
        (pin (num 9) (name P9) (type passive))
        (pin (num 10) (name P10) (type passive))
        (pin (num 11) (name P11) (type passive))
        (pin (num 12) (name P12) (type passive))
        (pin (num 13) (name P13) (type passive))
        (pin (num 14) (name P14) (type passive))
        (pin (num 15) (name P15) (type passive))
        (pin (num 16) (name P16) (type passive))
        (pin (num 17) (name P17) (type passive))
        (pin (num 18) (name P18) (type passive))
        (pin (num 19) (name P19) (type passive))
        (pin (num 20) (name P20) (type passive))))
    (libpart (lib conn) (part CONN_4)
      (description "Symbole general de connecteur")
      (fields
        (field (name Reference) P)
        (field (name Value) CONN_4))
      (pins
        (pin (num 1) (name P1) (type passive))
        (pin (num 2) (name P2) (type passive))
        (pin (num 3) (name P3) (type passive))
        (pin (num 4) (name P4) (type passive))))
    (libpart (lib conn) (part CONN_7)
      (description "Symbole general pour connexions")
      (fields
        (field (name Reference) P)
        (field (name Value) CONN_7))
      (pins
        (pin (num 1) (name P1) (type passive))
        (pin (num 2) (name P2) (type passive))
        (pin (num 3) (name P3) (type passive))
        (pin (num 4) (name P4) (type passive))
        (pin (num 5) (name P5) (type passive))
        (pin (num 6) (name P6) (type passive))
        (pin (num 7) (name P7) (type passive))))
    (libpart (lib conn) (part DB9)
      (footprints
        (fp DB9*))
      (fields
        (field (name Reference) J)
        (field (name Value) DB9))
      (pins
        (pin (num 1) (name 1) (type passive))
        (pin (num 2) (name 2) (type passive))
        (pin (num 3) (name 3) (type passive))
        (pin (num 4) (name 4) (type passive))
        (pin (num 5) (name 5) (type passive))
        (pin (num 6) (name P6) (type passive))
        (pin (num 7) (name P7) (type passive))
        (pin (num 8) (name P8) (type passive))
        (pin (num 9) (name P9) (type passive))))
    (libpart (lib regul) (part LM7805CT)
      (description "LM7805CT, Positive 1A 35V Linear Regulator, Fixed Output 5V, TO-220")
      (docs http://www.fairchildsemi.com/ds/LM/LM7805.pdf)
      (footprints
        (fp TO*))
      (fields
        (field (name Reference) U)
        (field (name Value) LM7805CT)
        (field (name Footprint) TO-220))
      (pins
        (pin (num 1) (name IN) (type input))
        (pin (num 2) (name GND) (type power_in))
        (pin (num 3) (name OUT) (type power_out))))
    (libpart (lib STM32f103) (part STM32f103)
      (footprints
        (fp QFP100))
      (fields
        (field (name Reference) U)
        (field (name Value) STM32f103)
        (field (name Footprint) ~)
        (field (name Datasheet) ~))
      (pins
        (pin (num 1) (name PE2/TRACECK) (type BiDi))
        (pin (num 2) (name PE3/TRACED0) (type BiDi))
        (pin (num 3) (name PE4/TRACED1) (type BiDi))
        (pin (num 4) (name PE5/TRACED2) (type BiDi))
        (pin (num 5) (name PE6/TRACED3) (type BiDi))
        (pin (num 6) (name VBAT) (type power_in))
        (pin (num 7) (name PC13/TAMPER-RTC) (type BiDi))
        (pin (num 8) (name PC14/OSC32IN) (type BiDi))
        (pin (num 9) (name PC15/OSC32OUT) (type BiDi))
        (pin (num 10) (name VSS5) (type power_in))
        (pin (num 11) (name VDD5) (type power_in))
        (pin (num 12) (name OSC_IN) (type input))
        (pin (num 13) (name OSC_OUT) (type output))
        (pin (num 14) (name NRST) (type BiDi))
        (pin (num 15) (name PC0/ADC12_IN10) (type BiDi))
        (pin (num 16) (name PC1/ADC12_IN11) (type BiDi))
        (pin (num 17) (name PC2/ADC12_IN12) (type BiDi))
        (pin (num 18) (name PC3/ADC12_IN13) (type BiDi))
        (pin (num 19) (name VSSA) (type power_in))
        (pin (num 20) (name VREF-) (type power_in))
        (pin (num 21) (name VREF+) (type power_in))
        (pin (num 22) (name VDDA) (type power_in))
        (pin (num 23) (name PA0/WKUP/USART2_CTS/ADC12_IN0/TIM2_CH1_ETR) (type BiDi))
        (pin (num 24) (name PA1/USART2_RTS/ADC12_IN1/TIM2_CH2) (type BiDi))
        (pin (num 25) (name PA2/USART2_TX/ADC12_IN2/TIM2_CH3) (type BiDi))
        (pin (num 26) (name PA3/USART2_RX/ADC12_IN3/TIM2_CH4) (type BiDi))
        (pin (num 27) (name VSS4) (type power_in))
        (pin (num 28) (name VDD4) (type power_in))
        (pin (num 29) (name PA4/SPI1_NSS/USART2_CK/ADC12_IN4) (type BiDi))
        (pin (num 30) (name PA5/SPI1_SCK/ADC12_IN5) (type BiDi))
        (pin (num 31) (name "PA6/SPI1_MISO/ADC12_IN6/TIM3_CH1(TIM1_BKIN)") (type BiDi))
        (pin (num 32) (name "PA7/SPI1_MOSI/ADC2_IN7/TIM3_CH2(TIM1_CH1N)") (type BiDi))
        (pin (num 33) (name PC4/ADC12_IN14) (type BiDi))
        (pin (num 34) (name PC5/ADC12_IN15) (type BiDi))
        (pin (num 35) (name "PB0/ADC12_IN8/TIM3_CH3(TIM1_CH2N)") (type BiDi))
        (pin (num 36) (name "PB1/ADC12_IN9/TIM3_CH4(TIM1_CH3N)") (type BiDi))
        (pin (num 37) (name PB2/BOOT1) (type BiDi))
        (pin (num 38) (name "PE7(TIM1_ETR)") (type BiDi))
        (pin (num 39) (name "PE8(TIM1_CH1N)") (type BiDi))
        (pin (num 40) (name "PE9(TIM1_CH1)") (type BiDi))
        (pin (num 41) (name "PE10(TIM1_CH2N)") (type BiDi))
        (pin (num 42) (name "PE11(TIM1_CH2)") (type BiDi))
        (pin (num 43) (name "PE12(TIM1_CH3N)") (type BiDi))
        (pin (num 44) (name "PE13(TIM1_CH3)") (type BiDi))
        (pin (num 45) (name "PE14(TIM1_CH4)") (type BiDi))
        (pin (num 46) (name "PE15(TIM1_BKIN)") (type BiDi))
        (pin (num 47) (name "PB10/I2C2_SCL/USART3_TX(TIM2_CH3)") (type BiDi))
        (pin (num 48) (name "PB11/I2C2_SDA/USART3_RX(TIM2_CH4)") (type BiDi))
        (pin (num 49) (name VSS1) (type power_in))
        (pin (num 50) (name VDD1) (type power_in))
        (pin (num 51) (name PB12/SPI2_NSS/I2C2_SMBAI/USART3_CK/TIM1_BKIN) (type BiDi))
        (pin (num 52) (name PB13/SPI2_SCK/USART3_CTS/TIM1_CH1N) (type BiDi))
        (pin (num 53) (name PB14/SPI2_MISO/USART3_RTS/TIM1_CH2N) (type BiDi))
        (pin (num 54) (name PB15/SPI2_MOSI/TIM1_CH3N) (type BiDi))
        (pin (num 55) (name "PD8(USART3_TX)") (type BiDi))
        (pin (num 56) (name "PD9(USART3_RX)") (type BiDi))
        (pin (num 57) (name "PD10(USART3_CK)") (type BiDi))
        (pin (num 58) (name "PD11(USART3_CTS)") (type BiDi))
        (pin (num 59) (name "PD12(TIM4_CH1/USART3_RTS)") (type BiDi))
        (pin (num 60) (name "PD13(TIM4_CH2)") (type BiDi))
        (pin (num 61) (name "PD14(TIM4_CH3)") (type BiDi))
        (pin (num 62) (name "PD15(TIM4_CH4)") (type BiDi))
        (pin (num 63) (name "PC6(TIM3_CH1)") (type BiDi))
        (pin (num 64) (name "PC7(TIM3_CH2)") (type BiDi))
        (pin (num 65) (name "PC8(TIM3_CH3)") (type BiDi))
        (pin (num 66) (name "PC9(TIM3_CH4)") (type BiDi))
        (pin (num 67) (name PA8/USART1_CK/TIM1_CH1/MCO) (type BiDi))
        (pin (num 68) (name PA9/USART1_TX/TIM1_CH2) (type BiDi))
        (pin (num 69) (name PA10/USART1_RX/TIM1_CH3) (type BiDi))
        (pin (num 70) (name PA11/USART1_CTS/CANRX/USBDM/TIM1_CH4) (type BiDi))
        (pin (num 71) (name PA12/USART1_RTS/CANTX/USBDP/TIM1_ETR) (type BiDi))
        (pin (num 72) (name "JTMS/SWDIO(PA13)") (type BiDi))
        (pin (num 73) (name NC) (type unspc))
        (pin (num 74) (name VSS2) (type power_in))
        (pin (num 75) (name VDD2) (type power_in))
        (pin (num 76) (name "JTCK/SWCLK(PA14)") (type BiDi))
        (pin (num 77) (name "JTDI(TIM2_CH1_ETR/PA15/SPI1_NSS)") (type BiDi))
        (pin (num 78) (name "PC10(USART3_TX)") (type BiDi))
        (pin (num 79) (name "PC11(USART3_RX)") (type BiDi))
        (pin (num 80) (name "PC12(USART3_CK)") (type BiDi))
        (pin (num 81) (name "PD0/OSC_IN(CANRX)") (type BiDi))
        (pin (num 82) (name "PD1/OSC_OUT(CANTX)") (type BiDi))
        (pin (num 83) (name PD2/TIM3_ETR) (type BiDi))
        (pin (num 84) (name "PD3(USART2_CTS)") (type BiDi))
        (pin (num 85) (name "PD4(USART2_RTS)") (type BiDi))
        (pin (num 86) (name "PD5(USART2_TX)") (type BiDi))
        (pin (num 87) (name "PD6(USART2_RX)") (type BiDi))
        (pin (num 88) (name "PD7(USART2_CK)") (type BiDi))
        (pin (num 89) (name "JTDO(TIM2_CH2/PB3/TRACESWO/SPI1_SCK)") (type BiDi))
        (pin (num 90) (name "JNTRST(TIM3_CH1/PB4/SPI1_MISO)") (type BiDi))
        (pin (num 91) (name "PB5/I2C1_SMBAI(TIM3_CH2/SPI1_MOSI)") (type BiDi))
        (pin (num 92) (name "PB6/I2C1_SCL/TIM4_CH1(USART1_TX)") (type BiDi))
        (pin (num 93) (name "PB7/I2C1_SDA/TIM4_CH2(USART1_RX)") (type BiDi))
        (pin (num 94) (name BOOT0) (type BiDi))
        (pin (num 95) (name "PB8/TIM4_CH3(I2C1_SCL/CANRX)") (type BiDi))
        (pin (num 96) (name "PB9/TIM4_CH4(I2C1_SDA/CANTX)") (type BiDi))
        (pin (num 97) (name PE0/TIM4_ETR) (type BiDi))
        (pin (num 98) (name PE1) (type BiDi))
        (pin (num 99) (name VSS3) (type power_in))
        (pin (num 100) (name VDD3) (type power_in))))
    (libpart (lib my_elements) (part ADM233L)
      (footprints
        (fp DIP-20*))
      (fields
        (field (name Reference) IC)
        (field (name Value) ADM233L)
        (field (name Footprint) DIP-20__300)
        (field (name Datasheet) ~))
      (pins
        (pin (num 1) (name T2_I) (type input))
        (pin (num 2) (name T1_I) (type input))
        (pin (num 3) (name R1_O) (type output))
        (pin (num 4) (name R1_I) (type input))
        (pin (num 5) (name T1_O) (type output))
        (pin (num 6) (name GND) (type power_in))
        (pin (num 7) (name VCC) (type power_in))
        (pin (num 8) (name C1+) (type passive))
        (pin (num 9) (name GND) (type power_in))
        (pin (num 10) (name C2-) (type passive))
        (pin (num 11) (name C2+) (type passive))
        (pin (num 12) (name intV-) (type passive))
        (pin (num 13) (name C1-) (type passive))
        (pin (num 14) (name intV+) (type passive))
        (pin (num 15) (name C2-) (type passive))
        (pin (num 16) (name C2-) (type passive))
        (pin (num 17) (name intV-) (type passive))
        (pin (num 18) (name T2_O) (type output))
        (pin (num 19) (name R2_I) (type output))
        (pin (num 20) (name R2_O) (type output))))
    (libpart (lib my_elements) (part BMB2A0300AN1)
      (footprints
        (fp SM0805))
      (fields
        (field (name Reference) L)
        (field (name Value) BMB2A0300AN1)
        (field (name Footprint) SM0805)
        (field (name Datasheet) ~))
      (pins
        (pin (num 1) (name 1) (type input))
        (pin (num 2) (name 2) (type input))))
    (libpart (lib my_elements) (part C0805)
      (footprints
        (fp SM0805))
      (fields
        (field (name Reference) C)
        (field (name Value) C0805)
        (field (name Footprint) SM0805)
        (field (name Datasheet) ~))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib my_elements) (part gprm1-61)
      (fields
        (field (name Reference) P)
        (field (name Value) gprm1-61)
        (field (name Footprint) gprm1-61)
        (field (name Datasheet) ~))
      (pins
        (pin (num 1-1) (name 1-1) (type passive))
        (pin (num 1-2) (name 1-2) (type passive))
        (pin (num 1-3) (name 1-3) (type passive))
        (pin (num 1-4) (name 1-4) (type passive))
        (pin (num 1-5) (name 1-5) (type passive))
        (pin (num 1-6) (name 1-6) (type passive))
        (pin (num 1-7) (name 1-7) (type passive))
        (pin (num 1-8) (name 1-8) (type passive))
        (pin (num 1-9) (name 1-9) (type passive))
        (pin (num 1-10) (name 1-10) (type passive))
        (pin (num 1-11) (name 1-11) (type passive))
        (pin (num 1-12) (name 1-12) (type passive))
        (pin (num 1-13) (name 1-13) (type passive))
        (pin (num 1-14) (name 1-14) (type passive))
        (pin (num 1-15) (name 1-15) (type passive))
        (pin (num 1-16) (name 1-16) (type passive))
        (pin (num 1-17) (name 1-17) (type passive))
        (pin (num 1-18) (name 1-18) (type passive))
        (pin (num 1-19) (name 1-19) (type passive))
        (pin (num 1-20) (name 1-20) (type passive))
        (pin (num 1-21) (name 1-21) (type passive))
        (pin (num 1-22) (name 1-22) (type passive))
        (pin (num 1-23) (name 1-23) (type passive))
        (pin (num 1-24) (name 1-24) (type passive))
        (pin (num 1-25) (name 1-25) (type passive))
        (pin (num 1-26) (name 1-26) (type passive))
        (pin (num 1-27) (name 1-27) (type passive))
        (pin (num 1-28) (name 1-28) (type passive))
        (pin (num 1-29) (name 1-29) (type passive))
        (pin (num 1-30) (name 1-30) (type passive))
        (pin (num 2-1) (name 2-1) (type passive))
        (pin (num 2-2) (name 2-2) (type passive))
        (pin (num 2-3) (name 2-3) (type passive))
        (pin (num 2-4) (name 2-4) (type passive))
        (pin (num 2-5) (name 2-5) (type passive))
        (pin (num 2-6) (name 2-6) (type passive))
        (pin (num 2-7) (name 2-7) (type passive))
        (pin (num 2-8) (name 2-8) (type passive))
        (pin (num 2-9) (name 2-9) (type passive))
        (pin (num 2-10) (name 2-10) (type passive))
        (pin (num 2-11) (name 2-11) (type passive))
        (pin (num 2-12) (name 2-12) (type passive))
        (pin (num 2-13) (name 2-13) (type passive))
        (pin (num 2-14) (name 2-14) (type passive))
        (pin (num 2-15) (name 2-15) (type passive))
        (pin (num 2-16) (name 2-16) (type passive))
        (pin (num 2-17) (name 2-17) (type passive))
        (pin (num 2-18) (name 2-18) (type passive))
        (pin (num 2-19) (name 2-19) (type passive))
        (pin (num 2-20) (name 2-20) (type passive))
        (pin (num 2-21) (name 2-21) (type passive))
        (pin (num 2-22) (name 2-22) (type passive))
        (pin (num 2-23) (name 2-23) (type passive))
        (pin (num 2-24) (name 2-24) (type passive))
        (pin (num 2-25) (name 2-25) (type passive))
        (pin (num 2-26) (name 2-26) (type passive))
        (pin (num 2-27) (name 2-27) (type passive))
        (pin (num 2-28) (name 2-28) (type passive))
        (pin (num 2-29) (name 2-29) (type passive))
        (pin (num 2-30) (name 2-30) (type passive))
        (pin (num 2-31) (name 2-31) (type passive))))
    (libpart (lib my_elements) (part HOLE)
      (description "Simple hole")
      (footprints
        (fp hole*))
      (fields
        (field (name Reference) HOLE)
        (field (name Value) HOLE)
        (field (name Footprint) ~)
        (field (name Datasheet) ~)))
    (libpart (lib my_elements) (part IPS5451)
      (footprints
        (fp TO-220)
        (fp SMD220))
      (fields
        (field (name Reference) U)
        (field (name Value) IPS5451)
        (field (name Footprint) TO220-4)
        (field (name Datasheet) ~))
      (pins
        (pin (num 1) (name GND) (type power_in))
        (pin (num 2) (name IN) (type input))
        (pin (num 3) (name VCC) (type power_in))
        (pin (num 4) (name DG) (type output))
        (pin (num 5) (name VOUT) (type power_out))))
    (libpart (lib my_elements) (part L6208N)
      (footprints
        (fp POWERDIP24)
        (fp DIP24*))
      (fields
        (field (name Reference) IC)
        (field (name Value) L6208N)
        (field (name Footprint) POWERDIP24)
        (field (name Datasheet) ~))
      (pins
        (pin (num 1) (name CLOCK) (type input))
        (pin (num 2) (name CW/CWW) (type input))
        (pin (num 3) (name SENSE_A) (type input))
        (pin (num 4) (name RCA) (type input))
        (pin (num 5) (name OUT1A) (type output))
        (pin (num 6) (name GND) (type power_in))
        (pin (num 7) (name GND@1) (type power_in))
        (pin (num 8) (name OUT1B) (type output))
        (pin (num 9) (name RCB) (type input))
        (pin (num 10) (name SENSE_B) (type input))
        (pin (num 11) (name VREF_B) (type input))
        (pin (num 12) (name HALF/FULL) (type input))
        (pin (num 13) (name CONTROL) (type input))
        (pin (num 14) (name EN) (type input))
        (pin (num 15) (name VBOOT) (type power_in))
        (pin (num 16) (name OUT2B) (type output))
        (pin (num 17) (name VS_B) (type power_in))
        (pin (num 18) (name GND@2) (type power_in))
        (pin (num 19) (name GND@3) (type power_in))
        (pin (num 20) (name VS_A) (type power_in))
        (pin (num 21) (name OUT2A) (type output))
        (pin (num 22) (name VCP) (type power_in))
        (pin (num 23) (name RESET) (type input))
        (pin (num 24) (name VREF_A) (type input))))
    (libpart (lib my_elements) (part LM1117MPX-3.3)
      (footprints
        (fp SOT223*))
      (fields
        (field (name Reference) U)
        (field (name Value) LM1117MPX-3.3)
        (field (name Footprint) SOT223)
        (field (name Datasheet) ~))
      (pins
        (pin (num 1) (name GND) (type power_in))
        (pin (num 2) (name OUT) (type power_out))
        (pin (num 3) (name IN) (type power_in))))
    (libpart (lib my_elements) (part NTE2984)
      (fields
        (field (name Reference) Q)
        (field (name Value) NTE2984)
        (field (name Footprint) TO220)
        (field (name Datasheet) ~))
      (pins
        (pin (num 1) (name G) (type input))
        (pin (num 2) (name D) (type passive))
        (pin (num 3) (name S) (type passive))))
    (libpart (lib my_elements) (part Quartz)
      (fields
        (field (name Reference) Q)
        (field (name Value) Quartz)
        (field (name Footprint) ~)
        (field (name Datasheet) ~))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib my_elements) (part R0603)
      (footprints
        (fp SM0603))
      (fields
        (field (name Reference) R)
        (field (name Value) R0603)
        (field (name Footprint) SM0603)
        (field (name Datasheet) ~))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib my_elements) (part R1206)
      (footprints
        (fp SM1206))
      (fields
        (field (name Reference) R)
        (field (name Value) R1206)
        (field (name Footprint) SM1206)
        (field (name Datasheet) ~))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib my_elements) (part RO-XX)
      (fields
        (field (name Reference) Q)
        (field (name Value) RO-XX)
        (field (name Footprint) SIP-4)
        (field (name Datasheet) ~))
      (pins
        (pin (num 1) (name -Vin) (type power_in))
        (pin (num 2) (name +Vin) (type power_in))
        (pin (num 3) (name -Vout) (type passive))
        (pin (num 4) (name +Vout) (type power_out))))
    (libpart (lib my_elements) (part RT0805BRB071KL)
      (footprints
        (fp SM0603)
        (fp SM0805))
      (fields
        (field (name Reference) R)
        (field (name Value) RT0805BRB071KL)
        (field (name Footprint) SM0805)
        (field (name Datasheet) ~))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib my_elements) (part TLE5205)
      (footprints
        (fp TO220*)
        (fp TO-220*))
      (fields
        (field (name Reference) U)
        (field (name Value) TLE5205)
        (field (name Footprint) ~)
        (field (name Datasheet) ~))
      (pins
        (pin (num 1) (name OUT1) (type power_out))
        (pin (num 2) (name EF) (type output))
        (pin (num 3) (name IN1) (type input))
        (pin (num 4) (name GND) (type power_in))
        (pin (num 5) (name IN2) (type input))
        (pin (num 6) (name Vs) (type power_in))
        (pin (num 7) (name OUT2) (type power_out))))
    (libpart (lib my_elements) (part USB-MICRO-B)
      (footprints
        (fp USB-Mini-B-Jack))
      (fields
        (field (name Reference) CON)
        (field (name Value) USB-MICRO-B)
        (field (name Footprint) MICRO-B-USB)
        (field (name Datasheet) ~))
      (pins
        (pin (num 1) (name VBUS) (type passive))
        (pin (num 2) (name D-) (type BiDi))
        (pin (num 3) (name D+) (type BiDi))
        (pin (num 4) (name ID) (type passive))
        (pin (num 5) (name GND) (type passive))
        (pin (num 6) (name SHELL1) (type passive))
        (pin (num 7) (name SHELL2) (type passive))
        (pin (num 8) (name SHELL3) (type passive))
        (pin (num 9) (name SHELL4) (type passive))))
    (libpart (lib my_elements) (part USBLC6-2)
      (footprints
        (fp SOT666*)
        (fp SOT23-6*))
      (fields
        (field (name Reference) U)
        (field (name Value) USBLC6-2)
        (field (name Footprint) SOT23_6)
        (field (name Datasheet) ~))
      (pins
        (pin (num 1) (name I/O1) (type passive))
        (pin (num 2) (name GND) (type power_in))
        (pin (num 3) (name I/O2) (type passive))
        (pin (num 4) (name I/O2) (type passive))
        (pin (num 5) (name VBUS) (type power_in))
        (pin (num 6) (name I/O1) (type passive)))))
  (libraries
    (library (logical device)
      (uri /usr/share/kicad/library/device.lib))
    (library (logical transistors)
      (uri /usr/share/kicad/library/transistors.lib))
    (library (logical conn)
      (uri /usr/share/kicad/library/conn.lib))
    (library (logical regul)
      (uri /usr/share/kicad/library/regul.lib))
    (library (logical STM32f103)
      (uri /home/eddy/kicad/STM32f103.lib))
    (library (logical my_elements)
      (uri my_elements.lib)))
  (nets
    (net (code 1) (name "/Power MOSFET module 2/GND_OUT")
      (node (ref XP7) (pin 19))
      (node (ref XP7) (pin 20))
      (node (ref VT2.1) (pin 2)))
    (net (code 2) (name "/Shutter MOSFET/OUT1")
      (node (ref XP7) (pin 4))
      (node (ref XP7) (pin 2))
      (node (ref XP7) (pin 1))
      (node (ref XP7) (pin 3))
      (node (ref DA2) (pin 1)))
    (net (code 3) (name "/Power MOSFET module 1/GND_OUT")
      (node (ref XP7) (pin 11))
      (node (ref XP7) (pin 12))
      (node (ref VT2.2) (pin 2)))
    (net (code 4) (name "/Filters slit #2/B*")
      (node (ref XP1) (pin 1-22))
      (node (ref DD2.3) (pin 8)))
    (net (code 5) (name "/Filters slit #2/B")
      (node (ref DD2.3) (pin 5))
      (node (ref XP1) (pin 1-21)))
    (net (code 6) (name "/Filters slit #1/B*")
      (node (ref DD2.2) (pin 8))
      (node (ref XP1) (pin 1-18)))
    (net (code 7) (name "/Filters slit #1/A*")
      (node (ref DD2.2) (pin 16))
      (node (ref XP1) (pin 1-16)))
    (net (code 8) (name "/Filters slit #1/A")
      (node (ref XP1) (pin 1-15))
      (node (ref DD2.2) (pin 21)))
    (net (code 9) (name "/Turret slits/B*")
      (node (ref XP1) (pin 1-14))
      (node (ref DD2.1) (pin 8)))
    (net (code 10) (name "/Turret slits/B")
      (node (ref DD2.1) (pin 5))
      (node (ref XP1) (pin 1-13)))
    (net (code 11) (name "/Turret slits/A*")
      (node (ref XP1) (pin 1-12))
      (node (ref DD2.1) (pin 16)))
    (net (code 12) (name "/Turret slits/A")
      (node (ref XP1) (pin 1-11))
      (node (ref DD2.1) (pin 21)))
    (net (code 13) (name "")
      (node (ref XP1) (pin 2-29)))
    (net (code 14) (name "")
      (node (ref XP1) (pin 2-24)))
    (net (code 15) (name "")
      (node (ref XP1) (pin 2-18)))
    (net (code 16) (name +5V)
      (node (ref R3.3) (pin 2))
      (node (ref XP1) (pin 1-2))
      (node (ref DD2.3) (pin 23))
      (node (ref DD2.3) (pin 13))
      (node (ref VD1) (pin 2))
      (node (ref R3.4) (pin 2))
      (node (ref DD2.4) (pin 23))
      (node (ref DD2.4) (pin 13))
      (node (ref R3.5) (pin 2))
      (node (ref DD2.5) (pin 13))
      (node (ref DD2.5) (pin 23))
      (node (ref DA4) (pin 5))
      (node (ref VD3) (pin 2))
      (node (ref C12) (pin 2))
      (node (ref DD1) (pin 7))
      (node (ref C5) (pin 1))
      (node (ref DA6) (pin 3))
      (node (ref R11) (pin 1))
      (node (ref DD2.1) (pin 23))
      (node (ref DD2.1) (pin 13))
      (node (ref R3.1) (pin 2))
      (node (ref DD2.2) (pin 13))
      (node (ref DD2.2) (pin 23))
      (node (ref R3.2) (pin 2))
      (node (ref DA3) (pin 4))
      (node (ref P2) (pin 1))
      (node (ref XP1) (pin 2-17))
      (node (ref U1) (pin 3))
      (node (ref C19) (pin 2)))
    (net (code 17) (name "")
      (node (ref VD1) (pin 1))
      (node (ref XP1) (pin 2-1)))
    (net (code 18) (name "")
      (node (ref XP7) (pin 9)))
    (net (code 19) (name "")
      (node (ref XP7) (pin 10)))
    (net (code 20) (name "/Long stage/A")
      (node (ref XP1) (pin 1-23))
      (node (ref DD2.4) (pin 21)))
    (net (code 21) (name "/Filters slit #1/SM_CLK")
      (node (ref DD2.3) (pin 1))
      (node (ref DD2.2) (pin 1))
      (node (ref DD2.1) (pin 1))
      (node (ref DD3) (pin 63)))
    (net (code 22) (name "/Filters slit #1/SM_DIR")
      (node (ref DD2.2) (pin 2))
      (node (ref DD3) (pin 98)))
    (net (code 23) (name "/Filters slit #1/SM_EN")
      (node (ref DD3) (pin 39))
      (node (ref DD2.2) (pin 14)))
    (net (code 24) (name "/Filters slit #1/+24V")
      (node (ref DD2.3) (pin 15))
      (node (ref DD2.4) (pin 15))
      (node (ref P1) (pin 1))
      (node (ref DD2.5) (pin 15))
      (node (ref DA5) (pin 4))
      (node (ref DD2.2) (pin 15))
      (node (ref DD2.1) (pin 15)))
    (net (code 25) (name "/Filters slit #2/SM_DIR")
      (node (ref DD2.3) (pin 2))
      (node (ref DD3) (pin 1)))
    (net (code 26) (name "/Filters slit #2/SM_EN")
      (node (ref DD3) (pin 40))
      (node (ref DD2.3) (pin 14)))
    (net (code 27) (name "/STM32F103 module/1-WIRE")
      (node (ref DD3) (pin 26))
      (node (ref DD3) (pin 25))
      (node (ref XP1) (pin 1-1))
      (node (ref R11) (pin 2)))
    (net (code 28) (name "/Short stage/B*")
      (node (ref XP1) (pin 1-30))
      (node (ref DD2.5) (pin 8)))
    (net (code 29) (name "/Short stage/B")
      (node (ref DD2.5) (pin 5))
      (node (ref XP1) (pin 1-29)))
    (net (code 30) (name "/Short stage/A*")
      (node (ref DD2.5) (pin 16))
      (node (ref XP1) (pin 1-28)))
    (net (code 31) (name "/Short stage/A")
      (node (ref DD2.5) (pin 21))
      (node (ref XP1) (pin 1-27)))
    (net (code 32) (name "/Long stage/B*")
      (node (ref XP1) (pin 1-26))
      (node (ref DD2.4) (pin 8)))
    (net (code 33) (name "/Long stage/B")
      (node (ref DD2.4) (pin 5))
      (node (ref XP1) (pin 1-25)))
    (net (code 34) (name "/Long stage/A*")
      (node (ref DD2.4) (pin 16))
      (node (ref XP1) (pin 1-24)))
    (net (code 35) (name "/Shutter MOSFET/EF")
      (node (ref DA2) (pin 2))
      (node (ref R22) (pin 2))
      (node (ref DD3) (pin 16)))
    (net (code 36) (name /POW_LOAD)
      (node (ref XP1) (pin 1-6))
      (node (ref XP1) (pin 1-5))
      (node (ref DA1) (pin 5)))
    (net (code 37) (name "")
      (node (ref R19) (pin 1))
      (node (ref DA1) (pin 2)))
    (net (code 38) (name "/STM32F103 module/POW3_FEEDBACK")
      (node (ref R20) (pin 1))
      (node (ref R21) (pin 2))
      (node (ref DA1) (pin 4)))
    (net (code 39) (name "/Shutter MOSFET/IN2")
      (node (ref R23) (pin 2))
      (node (ref DA2) (pin 5))
      (node (ref DD3) (pin 15)))
    (net (code 40) (name "/Shutter MOSFET/OUT2")
      (node (ref DA2) (pin 7))
      (node (ref XP7) (pin 7))
      (node (ref XP7) (pin 6))
      (node (ref XP7) (pin 5))
      (node (ref XP7) (pin 8)))
    (net (code 41) (name "/Shutter MOSFET/Sense")
      (node (ref R42) (pin 1))
      (node (ref R41) (pin 2))
      (node (ref DD3) (pin 24)))
    (net (code 42) (name "/STM32F103 module/U10")
      (node (ref DD3) (pin 23))
      (node (ref R44) (pin 1))
      (node (ref R43) (pin 2)))
    (net (code 43) (name "")
      (node (ref XP7) (pin 15)))
    (net (code 44) (name "")
      (node (ref XP7) (pin 16)))
    (net (code 45) (name "/Filters slit #1/+10V")
      (node (ref XP1) (pin 2-27))
      (node (ref XP1) (pin 2-25))
      (node (ref XP1) (pin 2-26))
      (node (ref XP7) (pin 14))
      (node (ref U1) (pin 1))
      (node (ref DD2.5) (pin 17))
      (node (ref DD2.4) (pin 20))
      (node (ref DD2.1) (pin 17))
      (node (ref DD2.3) (pin 20))
      (node (ref DD2.4) (pin 17))
      (node (ref XP1) (pin 2-28))
      (node (ref DD2.5) (pin 20))
      (node (ref XP7) (pin 13))
      (node (ref DD2.3) (pin 17))
      (node (ref DD2.2) (pin 20))
      (node (ref R43) (pin 1))
      (node (ref DD2.2) (pin 17))
      (node (ref DD2.1) (pin 20))
      (node (ref XP7) (pin 18))
      (node (ref XP7) (pin 17))
      (node (ref DA3) (pin 2))
      (node (ref DA5) (pin 2))
      (node (ref DA1) (pin 3)))
    (net (code 46) (name /EP0)
      (node (ref DD3) (pin 64))
      (node (ref R13) (pin 1))
      (node (ref XP1) (pin 2-15)))
    (net (code 47) (name /EP1)
      (node (ref XP1) (pin 2-14))
      (node (ref DD3) (pin 65))
      (node (ref R14) (pin 1)))
    (net (code 48) (name /EP2)
      (node (ref XP1) (pin 2-13))
      (node (ref DD3) (pin 66))
      (node (ref R15) (pin 1)))
    (net (code 49) (name /EP3)
      (node (ref XP1) (pin 2-12))
      (node (ref R16) (pin 1))
      (node (ref DD3) (pin 67)))
    (net (code 50) (name "/Shutter MOSFET/IN1")
      (node (ref R24) (pin 2))
      (node (ref DA2) (pin 3))
      (node (ref DD3) (pin 17)))
    (net (code 51) (name "/Power MOSFET module 1/ON")
      (node (ref DD3) (pin 44))
      (node (ref R37) (pin 1))
      (node (ref R40.2) (pin 1)))
    (net (code 52) (name "/Power MOSFET module 2/ON")
      (node (ref R38) (pin 1))
      (node (ref R40.1) (pin 1))
      (node (ref DD3) (pin 43)))
    (net (code 53) (name /POW3)
      (node (ref R39) (pin 1))
      (node (ref DD3) (pin 4))
      (node (ref R19) (pin 2)))
    (net (code 54) (name "/Turret slits/SM_DIR")
      (node (ref DD3) (pin 97))
      (node (ref DD2.1) (pin 2)))
    (net (code 55) (name "/Turret slits/SM_EN")
      (node (ref DD2.1) (pin 14))
      (node (ref DD3) (pin 38)))
    (net (code 56) (name /T1_4)
      (node (ref XP2) (pin 11))
      (node (ref DD3) (pin 32))
      (node (ref R30) (pin 2)))
    (net (code 57) (name /T1_0)
      (node (ref DD3) (pin 36))
      (node (ref R34) (pin 2))
      (node (ref XP2) (pin 3)))
    (net (code 58) (name /T1_1)
      (node (ref DD3) (pin 35))
      (node (ref R33) (pin 2))
      (node (ref XP2) (pin 5)))
    (net (code 59) (name /T1_2)
      (node (ref DD3) (pin 34))
      (node (ref R32) (pin 2))
      (node (ref XP2) (pin 7)))
    (net (code 60) (name /T1_3)
      (node (ref DD3) (pin 33))
      (node (ref R31) (pin 2))
      (node (ref XP2) (pin 9)))
    (net (code 61) (name /T1_5)
      (node (ref XP2) (pin 13))
      (node (ref R29) (pin 2))
      (node (ref DD3) (pin 31)))
    (net (code 62) (name /T1_6)
      (node (ref R28) (pin 2))
      (node (ref DD3) (pin 30))
      (node (ref XP2) (pin 15)))
    (net (code 63) (name /T1_7)
      (node (ref R27) (pin 2))
      (node (ref XP2) (pin 17))
      (node (ref DD3) (pin 29)))
    (net (code 64) (name GND)
      (node (ref C9) (pin 2))
      (node (ref R10) (pin 1))
      (node (ref XP1) (pin 2-20))
      (node (ref DA6) (pin 1))
      (node (ref C5) (pin 2))
      (node (ref SB1) (pin 1))
      (node (ref C7) (pin 2))
      (node (ref C6) (pin 2))
      (node (ref VT2.2) (pin 3))
      (node (ref C3.2) (pin 2))
      (node (ref R1.2) (pin 1))
      (node (ref R2.2) (pin 1))
      (node (ref C2.2) (pin 2))
      (node (ref R6.2) (pin 2))
      (node (ref R5.2) (pin 2))
      (node (ref R4.2) (pin 2))
      (node (ref DD3) (pin 74))
      (node (ref DD3) (pin 10))
      (node (ref DD3) (pin 20))
      (node (ref R17) (pin 2))
      (node (ref XP5) (pin 1))
      (node (ref R18) (pin 2))
      (node (ref XP4) (pin 4))
      (node (ref C3.4) (pin 2))
      (node (ref VT2.1) (pin 3))
      (node (ref R6.4) (pin 2))
      (node (ref DA2) (pin 4))
      (node (ref R42) (pin 2))
      (node (ref C4) (pin 2))
      (node (ref C1.4) (pin 2))
      (node (ref R1.4) (pin 1))
      (node (ref R2.4) (pin 1))
      (node (ref C2.4) (pin 2))
      (node (ref R5.4) (pin 2))
      (node (ref DD2.4) (pin 18))
      (node (ref R4.4) (pin 2))
      (node (ref DD2.4) (pin 19))
      (node (ref CON1) (pin 4))
      (node (ref C12) (pin 1))
      (node (ref CON1) (pin 5))
      (node (ref CON1) (pin 6))
      (node (ref CON1) (pin 7))
      (node (ref CON1) (pin 8))
      (node (ref CON1) (pin 9))
      (node (ref R7) (pin 2))
      (node (ref DA4) (pin 2))
      (node (ref XP6) (pin 5))
      (node (ref XS1) (pin 5))
      (node (ref DD1) (pin 6))
      (node (ref DD1) (pin 9))
      (node (ref R4.1) (pin 2))
      (node (ref DD2.1) (pin 19))
      (node (ref DD2.1) (pin 18))
      (node (ref C3.1) (pin 2))
      (node (ref DD2.1) (pin 7))
      (node (ref DD2.1) (pin 6))
      (node (ref DD2.2) (pin 12))
      (node (ref DD2.2) (pin 18))
      (node (ref DD2.2) (pin 19))
      (node (ref DD2.1) (pin 12))
      (node (ref C1.2) (pin 2))
      (node (ref DD2.2) (pin 6))
      (node (ref DD2.2) (pin 7))
      (node (ref R5.1) (pin 2))
      (node (ref C1.1) (pin 2))
      (node (ref R1.1) (pin 1))
      (node (ref C2.1) (pin 2))
      (node (ref R6.1) (pin 2))
      (node (ref R2.1) (pin 1))
      (node (ref C2.5) (pin 2))
      (node (ref R5.5) (pin 2))
      (node (ref R6.5) (pin 2))
      (node (ref DD2.5) (pin 12))
      (node (ref C3.5) (pin 2))
      (node (ref R2.5) (pin 1))
      (node (ref DD2.4) (pin 12))
      (node (ref DD2.4) (pin 7))
      (node (ref DD2.4) (pin 6))
      (node (ref C1.5) (pin 2))
      (node (ref R1.5) (pin 1))
      (node (ref DD2.5) (pin 7))
      (node (ref DD2.5) (pin 6))
      (node (ref DD2.5) (pin 18))
      (node (ref DD2.5) (pin 19))
      (node (ref R4.5) (pin 2))
      (node (ref C10) (pin 1))
      (node (ref DA1) (pin 1))
      (node (ref C1.3) (pin 2))
      (node (ref DA5) (pin 1))
      (node (ref DD2.3) (pin 7))
      (node (ref DD2.3) (pin 6))
      (node (ref C11) (pin 1))
      (node (ref DA3) (pin 3))
      (node (ref DA3) (pin 1))
      (node (ref DA5) (pin 3))
      (node (ref R5.3) (pin 2))
      (node (ref U1) (pin 2))
      (node (ref XP1) (pin 2-19))
      (node (ref C19) (pin 1))
      (node (ref C3.3) (pin 2))
      (node (ref R4.3) (pin 2))
      (node (ref R1.3) (pin 1))
      (node (ref R2.3) (pin 1))
      (node (ref C2.3) (pin 2))
      (node (ref R6.3) (pin 2))
      (node (ref R44) (pin 2))
      (node (ref XP1) (pin 1-4))
      (node (ref XP1) (pin 1-3))
      (node (ref XP3) (pin 1))
      (node (ref XP1) (pin 2-16))
      (node (ref C13) (pin 2))
      (node (ref DD2.3) (pin 12))
      (node (ref C14) (pin 2))
      (node (ref XP1) (pin 1-10))
      (node (ref XP1) (pin 2-22))
      (node (ref C15) (pin 1))
      (node (ref DD3) (pin 49))
      (node (ref DD3) (pin 19))
      (node (ref XP1) (pin 2-21))
      (node (ref DD3) (pin 99))
      (node (ref C17) (pin 1))
      (node (ref XP1) (pin 1-9))
      (node (ref XP2) (pin 12))
      (node (ref DD2.3) (pin 18))
      (node (ref XP2) (pin 1))
      (node (ref XP2) (pin 2))
      (node (ref XP2) (pin 4))
      (node (ref XP2) (pin 6))
      (node (ref XP2) (pin 8))
      (node (ref XP2) (pin 10))
      (node (ref XP2) (pin 20))
      (node (ref DD3) (pin 27))
      (node (ref XP2) (pin 14))
      (node (ref XP2) (pin 16))
      (node (ref R38) (pin 2))
      (node (ref R37) (pin 2))
      (node (ref DD2.3) (pin 19))
      (node (ref XP2) (pin 18))
      (node (ref XP1) (pin 2-23))
      (node (ref XP2) (pin 19))
      (node (ref R39) (pin 2))
      (node (ref C18) (pin 1))
      (node (ref XP1) (pin 1-8))
      (node (ref XP1) (pin 1-7))
      (node (ref C16) (pin 1)))
    (net (code 65) (name "/Shutter MOSFET/+36V")
      (node (ref R25) (pin 1))
      (node (ref XP1) (pin 2-30))
      (node (ref XP1) (pin 2-31)))
    (net (code 66) (name "/Filters slit #1/B")
      (node (ref XP1) (pin 1-17))
      (node (ref DD2.2) (pin 5)))
    (net (code 67) (name "/Filters slit #2/A")
      (node (ref XP1) (pin 1-19))
      (node (ref DD2.3) (pin 21)))
    (net (code 68) (name "/Filters slit #2/A*")
      (node (ref XP1) (pin 1-20))
      (node (ref DD2.3) (pin 16)))
    (net (code 69) (name "/Long stage/SM_CLK")
      (node (ref DD2.5) (pin 1))
      (node (ref DD2.4) (pin 1))
      (node (ref DD3) (pin 62)))
    (net (code 70) (name "")
      (node (ref DD2.3) (pin 4))
      (node (ref R6.3) (pin 1))
      (node (ref C3.3) (pin 1)))
    (net (code 71) (name "")
      (node (ref R5.3) (pin 1))
      (node (ref DD2.3) (pin 9))
      (node (ref C2.3) (pin 1)))
    (net (code 72) (name "")
      (node (ref R2.3) (pin 2))
      (node (ref DD2.3) (pin 3)))
    (net (code 73) (name "")
      (node (ref DD2.3) (pin 10))
      (node (ref R1.3) (pin 2)))
    (net (code 74) (name "")
      (node (ref DD2.3) (pin 24))
      (node (ref DD2.3) (pin 11))
      (node (ref R3.3) (pin 1))
      (node (ref C1.3) (pin 1))
      (node (ref R4.3) (pin 1)))
    (net (code 75) (name "")
      (node (ref DD2.3) (pin 22)))
    (net (code 76) (name "/STM32F103 module/RST")
      (node (ref SB1) (pin 2))
      (node (ref C7) (pin 1))
      (node (ref R26) (pin 1))
      (node (ref DD3) (pin 14)))
    (net (code 77) (name "")
      (node (ref DD3) (pin 51)))
    (net (code 78) (name "/STM32F103 module/USB input circuit/USB_DISC")
      (node (ref DD3) (pin 79))
      (node (ref VT1) (pin 1)))
    (net (code 79) (name "/STM32F103 module/USB input circuit/USB_DP")
      (node (ref R9) (pin 2))
      (node (ref R36) (pin 2))
      (node (ref DD3) (pin 71)))
    (net (code 80) (name "/STM32F103 module/USB input circuit/USB_DM")
      (node (ref R35) (pin 2))
      (node (ref DD3) (pin 70)))
    (net (code 81) (name "/STM32F103 module/BOOT")
      (node (ref DD3) (pin 94))
      (node (ref C8) (pin 1))
      (node (ref SB2) (pin 2))
      (node (ref R17) (pin 1)))
    (net (code 82) (name "")
      (node (ref DD3) (pin 18)))
    (net (code 83) (name "/STM32F103 module/RS-232 level converter/UART_RX")
      (node (ref DD3) (pin 48))
      (node (ref DD1) (pin 3)))
    (net (code 84) (name "/STM32F103 module/EXT1")
      (node (ref DD3) (pin 58))
      (node (ref XP5) (pin 3)))
    (net (code 85) (name "/STM32F103 module/USB input circuit/USB_POWER")
      (node (ref R8) (pin 1))
      (node (ref R7) (pin 1))
      (node (ref DD3) (pin 78)))
    (net (code 86) (name "")
      (node (ref DD3) (pin 77)))
    (net (code 87) (name "/STM32F103 module/SPI1_SCK")
      (node (ref XP3) (pin 2))
      (node (ref DD3) (pin 89)))
    (net (code 88) (name "")
      (node (ref DD3) (pin 45)))
    (net (code 89) (name "")
      (node (ref DD3) (pin 55)))
    (net (code 90) (name "/STM32F103 module/I2C_SCL/CANRX")
      (node (ref DD3) (pin 95))
      (node (ref XP3) (pin 5)))
    (net (code 91) (name "")
      (node (ref DD3) (pin 46)))
    (net (code 92) (name "")
      (node (ref DD3) (pin 56)))
    (net (code 93) (name "")
      (node (ref DD3) (pin 76)))
    (net (code 94) (name "/STM32F103 module/I2C_SDA/CANTX")
      (node (ref XP3) (pin 6))
      (node (ref DD3) (pin 96)))
    (net (code 95) (name "")
      (node (ref R18) (pin 1))
      (node (ref DD3) (pin 37)))
    (net (code 96) (name "/STM32F103 module/RS-232 level converter/UART_TX")
      (node (ref DD1) (pin 2))
      (node (ref DD3) (pin 47)))
    (net (code 97) (name "/STM32F103 module/EXT0")
      (node (ref DD3) (pin 57))
      (node (ref XP5) (pin 2)))
    (net (code 98) (name +3.3V)
      (node (ref DD3) (pin 28))
      (node (ref VT1) (pin 2))
      (node (ref XP3) (pin 7))
      (node (ref C8) (pin 2))
      (node (ref SB2) (pin 1))
      (node (ref R22) (pin 1))
      (node (ref R16) (pin 2))
      (node (ref R15) (pin 2))
      (node (ref R14) (pin 2))
      (node (ref R13) (pin 2))
      (node (ref DD3) (pin 50))
      (node (ref R24) (pin 1))
      (node (ref R23) (pin 1))
      (node (ref DD3) (pin 11))
      (node (ref R26) (pin 2))
      (node (ref C6) (pin 1))
      (node (ref DA6) (pin 2))
      (node (ref C17) (pin 2))
      (node (ref C16) (pin 2))
      (node (ref DD3) (pin 75))
      (node (ref L1) (pin 1))
      (node (ref DD3) (pin 100))
      (node (ref R20) (pin 2))
      (node (ref VD2) (pin 1))
      (node (ref C15) (pin 2))
      (node (ref C9) (pin 1))
      (node (ref C18) (pin 2)))
    (net (code 99) (name "/STM32F103 module/RS-232 level converter/UART_RX1")
      (node (ref DD3) (pin 69))
      (node (ref DD1) (pin 20))
      (node (ref XP5) (pin 6)))
    (net (code 100) (name "/STM32F103 module/RS-232 level converter/UART_TX1")
      (node (ref XP5) (pin 7))
      (node (ref DD3) (pin 68))
      (node (ref DD1) (pin 1)))
    (net (code 101) (name "")
      (node (ref R10) (pin 2))
      (node (ref VD2) (pin 2)))
    (net (code 102) (name "/STM32F103 module/EXT3")
      (node (ref DD3) (pin 60))
      (node (ref XP5) (pin 5)))
    (net (code 103) (name "/STM32F103 module/EXT2")
      (node (ref DD3) (pin 59))
      (node (ref XP5) (pin 4)))
    (net (code 104) (name "")
      (node (ref DD3) (pin 80)))
    (net (code 105) (name "")
      (node (ref R12) (pin 1))
      (node (ref G1) (pin 2))
      (node (ref C10) (pin 2))
      (node (ref DD3) (pin 12)))
    (net (code 106) (name "")
      (node (ref G1) (pin 1))
      (node (ref C11) (pin 2))
      (node (ref DD3) (pin 13))
      (node (ref R12) (pin 2)))
    (net (code 107) (name "/STM32F103 module/VDDA")
      (node (ref R31) (pin 1))
      (node (ref L1) (pin 2))
      (node (ref R30) (pin 1))
      (node (ref R29) (pin 1))
      (node (ref R28) (pin 1))
      (node (ref R27) (pin 1))
      (node (ref DD3) (pin 22))
      (node (ref R32) (pin 1))
      (node (ref C13) (pin 1))
      (node (ref DD3) (pin 21))
      (node (ref C14) (pin 1))
      (node (ref R33) (pin 1))
      (node (ref R34) (pin 1)))
    (net (code 108) (name "")
      (node (ref DD3) (pin 6)))
    (net (code 109) (name "")
      (node (ref DD3) (pin 73)))
    (net (code 110) (name "")
      (node (ref DD3) (pin 7)))
    (net (code 111) (name "")
      (node (ref DD3) (pin 61)))
    (net (code 112) (name "")
      (node (ref DD3) (pin 72)))
    (net (code 113) (name "/STM32F103 module/SPI1_MOSI")
      (node (ref DD3) (pin 91))
      (node (ref XP3) (pin 4)))
    (net (code 114) (name "/STM32F103 module/SPI2_SCK")
      (node (ref DD3) (pin 52))
      (node (ref XP4) (pin 3)))
    (net (code 115) (name "/STM32F103 module/SPI2_MISO")
      (node (ref DD3) (pin 53))
      (node (ref XP4) (pin 2)))
    (net (code 116) (name "/STM32F103 module/SPI2_MOSI")
      (node (ref XP4) (pin 1))
      (node (ref DD3) (pin 54)))
    (net (code 117) (name "/STM32F103 module/DG_FEEDBACK")
      (node (ref R21) (pin 1))
      (node (ref DD3) (pin 5)))
    (net (code 118) (name "")
      (node (ref DD3) (pin 8)))
    (net (code 119) (name "")
      (node (ref DD3) (pin 9)))
    (net (code 120) (name "/STM32F103 module/SPI1_MISO")
      (node (ref DD3) (pin 90))
      (node (ref XP3) (pin 3)))
    (net (code 121) (name "")
      (node (ref R40.2) (pin 2))
      (node (ref VT2.2) (pin 1)))
    (net (code 122) (name "")
      (node (ref C3.2) (pin 1))
      (node (ref R6.2) (pin 1))
      (node (ref DD2.2) (pin 4)))
    (net (code 123) (name "")
      (node (ref DD2.2) (pin 9))
      (node (ref C2.2) (pin 1))
      (node (ref R5.2) (pin 1)))
    (net (code 124) (name "")
      (node (ref R2.2) (pin 2))
      (node (ref DD2.2) (pin 3)))
    (net (code 125) (name "")
      (node (ref R1.2) (pin 2))
      (node (ref DD2.2) (pin 10)))
    (net (code 126) (name "")
      (node (ref C1.2) (pin 1))
      (node (ref DD2.2) (pin 24))
      (node (ref R3.2) (pin 1))
      (node (ref R4.2) (pin 1))
      (node (ref DD2.2) (pin 11)))
    (net (code 127) (name "")
      (node (ref DD2.2) (pin 22)))
    (net (code 128) (name "")
      (node (ref DD2.1) (pin 3))
      (node (ref R2.1) (pin 2)))
    (net (code 129) (name "")
      (node (ref R1.1) (pin 2))
      (node (ref DD2.1) (pin 10)))
    (net (code 130) (name "")
      (node (ref DD2.1) (pin 22)))
    (net (code 131) (name "")
      (node (ref R4.1) (pin 1))
      (node (ref C1.1) (pin 1))
      (node (ref DD2.1) (pin 11))
      (node (ref R3.1) (pin 1))
      (node (ref DD2.1) (pin 24)))
    (net (code 132) (name "")
      (node (ref DD2.1) (pin 4))
      (node (ref R6.1) (pin 1))
      (node (ref C3.1) (pin 1)))
    (net (code 133) (name "")
      (node (ref R5.1) (pin 1))
      (node (ref C2.1) (pin 1))
      (node (ref DD2.1) (pin 9)))
    (net (code 134) (name "")
      (node (ref DD2.5) (pin 10))
      (node (ref R1.5) (pin 2)))
    (net (code 135) (name "")
      (node (ref DD2.5) (pin 3))
      (node (ref R2.5) (pin 2)))
    (net (code 136) (name "")
      (node (ref R6.5) (pin 1))
      (node (ref C3.5) (pin 1))
      (node (ref DD2.5) (pin 4)))
    (net (code 137) (name "")
      (node (ref R3.5) (pin 1))
      (node (ref DD2.5) (pin 24))
      (node (ref R4.5) (pin 1))
      (node (ref C1.5) (pin 1))
      (node (ref DD2.5) (pin 11)))
    (net (code 138) (name "")
      (node (ref DD2.5) (pin 22)))
    (net (code 139) (name "")
      (node (ref DD2.5) (pin 9))
      (node (ref R5.5) (pin 1))
      (node (ref C2.5) (pin 1)))
    (net (code 140) (name "")
      (node (ref DD2.4) (pin 3))
      (node (ref R2.4) (pin 2)))
    (net (code 141) (name "")
      (node (ref DD2.4) (pin 9))
      (node (ref C2.4) (pin 1))
      (node (ref R5.4) (pin 1)))
    (net (code 142) (name "")
      (node (ref R1.4) (pin 2))
      (node (ref DD2.4) (pin 10)))
    (net (code 143) (name "")
      (node (ref DD2.4) (pin 22)))
    (net (code 144) (name "")
      (node (ref R4.4) (pin 1))
      (node (ref C1.4) (pin 1))
      (node (ref DD2.4) (pin 24))
      (node (ref DD2.4) (pin 11))
      (node (ref R3.4) (pin 1)))
    (net (code 145) (name "")
      (node (ref DD2.4) (pin 4))
      (node (ref C3.4) (pin 1))
      (node (ref R6.4) (pin 1)))
    (net (code 146) (name "")
      (node (ref VT2.1) (pin 1))
      (node (ref R40.1) (pin 2)))
    (net (code 147) (name "")
      (node (ref C4) (pin 1))
      (node (ref R25) (pin 2))
      (node (ref DA2) (pin 6))
      (node (ref R41) (pin 1)))
    (net (code 148) (name "")
      (node (ref XS1) (pin 2))
      (node (ref DD1) (pin 5)))
    (net (code 149) (name "")
      (node (ref DD1) (pin 8)))
    (net (code 150) (name "")
      (node (ref DD1) (pin 13)))
    (net (code 151) (name "")
      (node (ref DD1) (pin 14)))
    (net (code 152) (name "")
      (node (ref DD1) (pin 11))
      (node (ref DD1) (pin 15)))
    (net (code 153) (name "")
      (node (ref DD1) (pin 16))
      (node (ref DD1) (pin 10)))
    (net (code 154) (name "")
      (node (ref DD1) (pin 12))
      (node (ref DD1) (pin 17)))
    (net (code 155) (name "")
      (node (ref DD1) (pin 18))
      (node (ref XP6) (pin 3)))
    (net (code 156) (name "")
      (node (ref DD1) (pin 4))
      (node (ref XS1) (pin 3)))
    (net (code 157) (name "")
      (node (ref XS1) (pin 4)))
    (net (code 158) (name "")
      (node (ref XS1) (pin 6)))
    (net (code 159) (name "")
      (node (ref XS1) (pin 7)))
    (net (code 160) (name "")
      (node (ref XS1) (pin 8)))
    (net (code 161) (name "")
      (node (ref XS1) (pin 9)))
    (net (code 162) (name "")
      (node (ref XP6) (pin 9)))
    (net (code 163) (name "")
      (node (ref XP6) (pin 6)))
    (net (code 164) (name "")
      (node (ref XP6) (pin 8)))
    (net (code 165) (name "")
      (node (ref XP6) (pin 7)))
    (net (code 166) (name "")
      (node (ref XP6) (pin 4)))
    (net (code 167) (name "")
      (node (ref XP6) (pin 1)))
    (net (code 168) (name "")
      (node (ref XS1) (pin 1)))
    (net (code 169) (name "")
      (node (ref DD1) (pin 19))
      (node (ref XP6) (pin 2)))
    (net (code 170) (name "")
      (node (ref DA4) (pin 3))
      (node (ref CON1) (pin 3)))
    (net (code 171) (name "")
      (node (ref DA4) (pin 1))
      (node (ref CON1) (pin 2)))
    (net (code 172) (name "")
      (node (ref VT1) (pin 3))
      (node (ref R9) (pin 1)))
    (net (code 173) (name "")
      (node (ref R36) (pin 1))
      (node (ref DA4) (pin 4)))
    (net (code 174) (name "")
      (node (ref DA4) (pin 6))
      (node (ref R35) (pin 1)))
    (net (code 175) (name "")
      (node (ref CON1) (pin 1))
      (node (ref VD3) (pin 1))
      (node (ref R8) (pin 2)))
    (net (code 176) (name /Hall1)
      (node (ref DD3) (pin 82))
      (node (ref XP1) (pin 2-10)))
    (net (code 177) (name /Hall0)
      (node (ref DD3) (pin 81))
      (node (ref XP1) (pin 2-11)))
    (net (code 178) (name /Hall2)
      (node (ref XP1) (pin 2-9))
      (node (ref DD3) (pin 83)))
    (net (code 179) (name /Hall3)
      (node (ref DD3) (pin 84))
      (node (ref XP1) (pin 2-8)))
    (net (code 180) (name /Hall4)
      (node (ref XP1) (pin 2-7))
      (node (ref DD3) (pin 85)))
    (net (code 181) (name /Hall5)
      (node (ref XP1) (pin 2-6))
      (node (ref DD3) (pin 86)))
    (net (code 182) (name /Hall6)
      (node (ref XP1) (pin 2-5))
      (node (ref DD3) (pin 87)))
    (net (code 183) (name /Hall7)
      (node (ref XP1) (pin 2-4))
      (node (ref DD3) (pin 88)))
    (net (code 184) (name /Hall8)
      (node (ref DD3) (pin 92))
      (node (ref XP1) (pin 2-3)))
    (net (code 185) (name /Hall9)
      (node (ref DD3) (pin 93))
      (node (ref XP1) (pin 2-2)))
    (net (code 186) (name "/Long stage/SM_EN")
      (node (ref DD3) (pin 41))
      (node (ref DD2.4) (pin 14)))
    (net (code 187) (name "/Short stage/SM_EN")
      (node (ref DD3) (pin 42))
      (node (ref DD2.5) (pin 14)))
    (net (code 188) (name "/Long stage/SM_DIR")
      (node (ref DD2.4) (pin 2))
      (node (ref DD3) (pin 2)))
    (net (code 189) (name "/Short stage/SM_DIR")
      (node (ref DD3) (pin 3))
      (node (ref DD2.5) (pin 2)))))