(export (version D)
  (design
    (source /home/eddy/tmp/microdrill/schematics/MCU_module.sch)
    (date "Вс 16 ноя 2014 01:25:03")
    (tool "eeschema (2013-may-18)-stable"))
  (components
    (comp (ref DA1)
      (value L9110)
      (libsource (lib L9110) (part L9110))
      (sheetpath (names /) (tstamps /))
      (tstamp 53F0EE9F))
    (comp (ref DA2)
      (value L9110)
      (libsource (lib L9110) (part L9110))
      (sheetpath (names /) (tstamps /))
      (tstamp 53F0EF24))
    (comp (ref DA3)
      (value L9110)
      (libsource (lib L9110) (part L9110))
      (sheetpath (names /) (tstamps /))
      (tstamp 53F0EF3C))
    (comp (ref P3)
      (value Stepper)
      (libsource (lib conn) (part CONN_4))
      (sheetpath (names /) (tstamps /))
      (tstamp 53F0F09A))
    (comp (ref U2)
      (value LM1117MPX-3.3)
      (footprint SOT223)
      (libsource (lib LM1117) (part LM1117MPX-3.3))
      (sheetpath (names /) (tstamps /))
      (tstamp 53F0F811))
    (comp (ref C4)
      (value 0.1u)
      (footprint SM0603)
      (libsource (lib device) (part C))
      (sheetpath (names /) (tstamps /))
      (tstamp 53F0F83E))
    (comp (ref C5)
      (value 47u)
      (footprint SM1206)
      (libsource (lib device) (part CP1))
      (sheetpath (names /) (tstamps /))
      (tstamp 53F0F88C))
    (comp (ref K1)
      (value POWER)
      (libsource (lib conn) (part CONN_3))
      (sheetpath (names /) (tstamps /))
      (tstamp 53F0FD67))
    (comp (ref P4)
      (value Slide)
      (libsource (lib conn) (part CONN_2))
      (sheetpath (names /) (tstamps /))
      (tstamp 53F1169C))
    (comp (ref X1)
      (value STM8S105BOARD)
      (footprint devboard_pins-9-14)
      (libsource (lib stm8s105k4t6c) (part STM8S105BOARD))
      (sheetpath (names /) (tstamps /))
      (tstamp 54626F55))
    (comp (ref UP1)
      (value CONN_1)
      (libsource (lib conn) (part CONN_1))
      (sheetpath (names /) (tstamps /))
      (tstamp 54628F0D))
    (comp (ref DOWN1)
      (value CONN_1)
      (libsource (lib conn) (part CONN_1))
      (sheetpath (names /) (tstamps /))
      (tstamp 54628F38))
    (comp (ref BTN1)
      (value CONN_1)
      (libsource (lib conn) (part CONN_1))
      (sheetpath (names /) (tstamps /))
      (tstamp 54628F3E))
    (comp (ref BTN2)
      (value CONN_1)
      (libsource (lib conn) (part CONN_1))
      (sheetpath (names /) (tstamps /))
      (tstamp 54628FEC))
    (comp (ref POT1)
      (value CONN_1)
      (libsource (lib conn) (part CONN_1))
      (sheetpath (names /) (tstamps /))
      (tstamp 54628FF2))
    (comp (ref DRILL+1)
      (value CONN_1)
      (libsource (lib conn) (part CONN_1))
      (sheetpath (names /) (tstamps /))
      (tstamp 54629D60))
    (comp (ref DRILL-1)
      (value CONN_1)
      (libsource (lib conn) (part CONN_1))
      (sheetpath (names /) (tstamps /))
      (tstamp 54629E20))
    (comp (ref DRILLSW1)
      (value CONN_1)
      (libsource (lib conn) (part CONN_1))
      (sheetpath (names /) (tstamps /))
      (tstamp 5462B0E5))
    (comp (ref GND1)
      (value CONN_1)
      (libsource (lib conn) (part CONN_1))
      (sheetpath (names /) (tstamps /))
      (tstamp 5462B0EB))
    (comp (ref R5)
      (value 0.33R)
      (footprint SM2512)
      (libsource (lib device) (part R))
      (sheetpath (names "/Drill motor/") (tstamps /53EF036E/))
      (tstamp 53E67E8A))
    (comp (ref R4)
      (value 47k)
      (libsource (lib device) (part R))
      (sheetpath (names "/Drill motor/") (tstamps /53EF036E/))
      (tstamp 53E680EF))
    (comp (ref D3)
      (value DIODESCH)
      (libsource (lib device) (part DIODESCH))
      (sheetpath (names "/Drill motor/") (tstamps /53EF036E/))
      (tstamp 53E68EA1))
    (comp (ref VT1)
      (value S8205A)
      (footprint TSSOP-8)
      (libsource (lib s8205a) (part S8205A))
      (sheetpath (names "/Drill motor/") (tstamps /53EF036E/))
      (tstamp 53F123C0))
    (comp (ref C6)
      (value 0.1u)
      (footprint SM0603)
      (libsource (lib device) (part CP1))
      (sheetpath (names "/Drill motor/") (tstamps /53EF036E/))
      (tstamp 53F36070)))
  (libparts
    (libpart (lib device) (part C)
      (description "Condensateur non polarise")
      (footprints
        (fp SM*)
        (fp C?)
        (fp C1-1))
      (fields
        (field (name Reference) C)
        (field (name Value) C))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib device) (part CP1)
      (description "Condensateur polarise")
      (footprints
        (fp CP*)
        (fp SM*))
      (fields
        (field (name Reference) C)
        (field (name Value) CP1))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib device) (part DIODESCH)
      (description "Diode schottky")
      (footprints
        (fp D?)
        (fp S*))
      (fields
        (field (name Reference) D)
        (field (name Value) DIODESCH))
      (pins
        (pin (num 1) (name A) (type passive))
        (pin (num 2) (name K) (type passive))))
    (libpart (lib device) (part R)
      (description Resistance)
      (footprints
        (fp R?)
        (fp SM0603)
        (fp SM0805)
        (fp R?-*)
        (fp SM1206))
      (fields
        (field (name Reference) R)
        (field (name Value) R))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib conn) (part CONN_1)
      (description "1 pin")
      (fields
        (field (name Reference) P)
        (field (name Value) CONN_1))
      (pins
        (pin (num 1) (name 1) (type passive))))
    (libpart (lib conn) (part CONN_2)
      (description "Symbole general de connecteur")
      (fields
        (field (name Reference) P)
        (field (name Value) CONN_2))
      (pins
        (pin (num 1) (name P1) (type passive))
        (pin (num 2) (name PM) (type passive))))
    (libpart (lib conn) (part CONN_3)
      (description "Symbole general de connecteur")
      (fields
        (field (name Reference) K)
        (field (name Value) CONN_3))
      (pins
        (pin (num 1) (name P1) (type passive))
        (pin (num 2) (name PM) (type passive))
        (pin (num 3) (name P3) (type passive))))
    (libpart (lib conn) (part CONN_4)
      (description "Symbole general de connecteur")
      (fields
        (field (name Reference) P)
        (field (name Value) CONN_4))
      (pins
        (pin (num 1) (name P1) (type passive))
        (pin (num 2) (name P2) (type passive))
        (pin (num 3) (name P3) (type passive))
        (pin (num 4) (name P4) (type passive))))
    (libpart (lib L9110) (part L9110)
      (footprints
        (fp DIP8*)
        (fp DIP-8*)
        (fp SOP8*)
        (fp SOP-8*))
      (fields
        (field (name Reference) DA)
        (field (name Value) L9110)
        (field (name Footprint) ~)
        (field (name Datasheet) ~))
      (pins
        (pin (num 1) (name OA) (type output))
        (pin (num 2) (name VCC) (type power_in))
        (pin (num 3) (name VCC) (type power_in))
        (pin (num 4) (name OB) (type output))
        (pin (num 5) (name GND) (type power_in))
        (pin (num 6) (name IA) (type input))
        (pin (num 7) (name IB) (type input))
        (pin (num 8) (name GND) (type power_in))))
    (libpart (lib stm8s105k4t6c) (part stm8s105board)
      (footprints
        (fp stm8s105board))
      (fields
        (field (name Reference) X)
        (field (name Value) stm8s105board)
        (field (name Footprint) devboard_pins-9-14)
        (field (name Datasheet) ~))
      (pins
        (pin (num 1) (name "VDD(3.3-5v)") (type power_in))
        (pin (num 2) (name GND) (type power_in))
        (pin (num 3) (name NRST) (type input))
        (pin (num 4) (name OSCIN/PA1) (type 3state))
        (pin (num 5) (name OSCOUT/PA2) (type 3state))
        (pin (num 6) (name PF4/AIN12) (type 3state))
        (pin (num 7) (name PB5/AIN5[I2X_SDA]) (type 3state))
        (pin (num 8) (name PB4/AIN4[I2C_SCL]) (type 3state))
        (pin (num 9) (name PB3/AIN3[TIM1_ETR]) (type 3state))
        (pin (num 10) (name PB2/AIN2[TIM1_CH3N]) (type 3state))
        (pin (num 11) (name PB1/AIN1_[TIM1_CH2N]) (type 3state))
        (pin (num 12) (name PB0/AIN0_[TIM1_CH1N]) (type 3state))
        (pin (num 13) (name PE5/SPI_NSS) (type 3state))
        (pin (num 14) (name "PC1(HS)/TIM1_CH1") (type 3state))
        (pin (num 15) (name "PC2(HS)/TIM1_CH2") (type 3state))
        (pin (num 16) (name "PC3(HS)/TIM1_CH3") (type 3state))
        (pin (num 17) (name "PC4(HS)/TIM1_CH4") (type 3state))
        (pin (num 18) (name "PC5(HS)/SPI_SCK") (type 3state))
        (pin (num 19) (name "PC6(HS)/SPI_MOSI") (type 3state))
        (pin (num 20) (name "PC7(HS)/SPI_MISO") (type 3state))
        (pin (num 21) (name "PD0(HS)/TIM3_CH2[TIM1_BKIN][CLK_CCO]") (type 3state))
        (pin (num 22) (name "PD1(HS)/SWIM") (type 3state))
        (pin (num 23) (name "PD2(HS)/TIM3_CH1[TIM2_CH3]") (type 3state))
        (pin (num 24) (name "PD3(HS)/TIM2_CH2[ADC_ETR]") (type 3state))
        (pin (num 25) (name "PD4(HS)/TIM2_CH1[BEEP]") (type 3state))
        (pin (num 26) (name PD5/UART2_TX) (type 3state))
        (pin (num 27) (name PD6/UART2_RX) (type 3state))
        (pin (num 28) (name PD7/TLI[TIM1_CH4]) (type 3state))))
    (libpart (lib LM1117) (part LM1117MPX-3.3)
      (footprints
        (fp SOT223*))
      (fields
        (field (name Reference) U)
        (field (name Value) LM1117MPX-3.3)
        (field (name Footprint) SOT223)
        (field (name Datasheet) ~))
      (pins
        (pin (num 1) (name GND) (type power_in))
        (pin (num 2) (name OUT) (type power_out))
        (pin (num 3) (name IN) (type power_in))))
    (libpart (lib s8205a) (part S8205A)
      (footprints
        (fp TSSOP8*)
        (fp TSSOP-8*))
      (fields
        (field (name Reference) VT)
        (field (name Value) S8205A)
        (field (name Footprint) TSSOP-8)
        (field (name Datasheet) ~))
      (pins
        (pin (num 1) (name D) (type passive))
        (pin (num 2) (name S1) (type passive))
        (pin (num 3) (name S1) (type passive))
        (pin (num 4) (name G1) (type passive))
        (pin (num 5) (name G2) (type passive))
        (pin (num 6) (name S2) (type passive))
        (pin (num 7) (name S2) (type passive))
        (pin (num 8) (name D) (type passive)))))
  (libraries
    (library (logical device)
      (uri /usr/share/kicad/library/device.lib))
    (library (logical conn)
      (uri /usr/share/kicad/library/conn.lib))
    (library (logical L9110)
      (uri L9110.lib))
    (library (logical stm8s105k4t6c)
      (uri stm8s105k4t6c.lib))
    (library (logical LM1117)
      (uri LM1117.lib))
    (library (logical s8205a)
      (uri s8205a.lib)))
  (nets
    (net (code 1) (name /NRST)
      (node (ref X1) (pin 3)))
    (net (code 2) (name /PC5)
      (node (ref DRILLSW1) (pin 1))
      (node (ref X1) (pin 18)))
    (net (code 3) (name /OSC1IN)
      (node (ref X1) (pin 4)))
    (net (code 4) (name /OSC2IN)
      (node (ref X1) (pin 5)))
    (net (code 5) (name /PB5)
      (node (ref X1) (pin 7)))
    (net (code 6) (name /PB3)
      (node (ref X1) (pin 9))
      (node (ref DA2) (pin 7)))
    (net (code 7) (name /PD0)
      (node (ref X1) (pin 21)))
    (net (code 8) (name /SWIM/PD1)
      (node (ref X1) (pin 22)))
    (net (code 9) (name /PE5)
      (node (ref X1) (pin 13)))
    (net (code 10) (name "")
      (node (ref P3) (pin 2))
      (node (ref DA1) (pin 1)))
    (net (code 11) (name "")
      (node (ref DA1) (pin 4))
      (node (ref P3) (pin 1)))
    (net (code 12) (name "")
      (node (ref DA2) (pin 1))
      (node (ref P3) (pin 4)))
    (net (code 13) (name "")
      (node (ref DA2) (pin 4))
      (node (ref P3) (pin 3)))
    (net (code 14) (name "/Drill motor/PWM_in")
      (node (ref X1) (pin 14))
      (node (ref VT1) (pin 5))
      (node (ref VT1) (pin 4)))
    (net (code 15) (name +5V)
      (node (ref DA3) (pin 2))
      (node (ref DA3) (pin 3))
      (node (ref U2) (pin 3))
      (node (ref C4) (pin 1))
      (node (ref K1) (pin 2))
      (node (ref DA1) (pin 2))
      (node (ref DA1) (pin 3))
      (node (ref DA2) (pin 2))
      (node (ref DA2) (pin 3)))
    (net (code 16) (name "")
      (node (ref DA3) (pin 1))
      (node (ref P4) (pin 1)))
    (net (code 17) (name "")
      (node (ref DA3) (pin 4))
      (node (ref P4) (pin 2)))
    (net (code 18) (name /PD7)
      (node (ref X1) (pin 28)))
    (net (code 19) (name "/Drill motor/DRILL-")
      (node (ref VT1) (pin 8))
      (node (ref VT1) (pin 1))
      (node (ref D3) (pin 1))
      (node (ref DRILL-1) (pin 1)))
    (net (code 20) (name GND)
      (node (ref U2) (pin 1))
      (node (ref K1) (pin 1))
      (node (ref C5) (pin 2))
      (node (ref C4) (pin 2))
      (node (ref X1) (pin 2))
      (node (ref DA3) (pin 8))
      (node (ref GND1) (pin 1))
      (node (ref C6) (pin 2))
      (node (ref DA3) (pin 5))
      (node (ref R5) (pin 2))
      (node (ref DA2) (pin 8))
      (node (ref DA2) (pin 5))
      (node (ref DA1) (pin 8))
      (node (ref DA1) (pin 5)))
    (net (code 21) (name /PD4)
      (node (ref X1) (pin 25)))
    (net (code 22) (name /PC2)
      (node (ref X1) (pin 15)))
    (net (code 23) (name /PD6)
      (node (ref X1) (pin 27)))
    (net (code 24) (name /PD5)
      (node (ref X1) (pin 26)))
    (net (code 25) (name /PC4)
      (node (ref UP1) (pin 1))
      (node (ref X1) (pin 17)))
    (net (code 26) (name /PC3)
      (node (ref DOWN1) (pin 1))
      (node (ref X1) (pin 16)))
    (net (code 27) (name /PC6)
      (node (ref BTN1) (pin 1))
      (node (ref X1) (pin 19)))
    (net (code 28) (name /PC7)
      (node (ref X1) (pin 20))
      (node (ref BTN2) (pin 1)))
    (net (code 29) (name /PB4)
      (node (ref POT1) (pin 1))
      (node (ref X1) (pin 8)))
    (net (code 30) (name +12V)
      (node (ref D3) (pin 2))
      (node (ref DRILL+1) (pin 1))
      (node (ref K1) (pin 3)))
    (net (code 31) (name /PB1)
      (node (ref DA1) (pin 7))
      (node (ref X1) (pin 11)))
    (net (code 32) (name "/Drill motor/Sence")
      (node (ref X1) (pin 6))
      (node (ref R4) (pin 1))
      (node (ref C6) (pin 1)))
    (net (code 33) (name /PB0)
      (node (ref DA1) (pin 6))
      (node (ref X1) (pin 12)))
    (net (code 34) (name /PB2)
      (node (ref X1) (pin 10))
      (node (ref DA2) (pin 6)))
    (net (code 35) (name +3.3V)
      (node (ref X1) (pin 1))
      (node (ref U2) (pin 2))
      (node (ref C5) (pin 1)))
    (net (code 36) (name /PD3)
      (node (ref DA3) (pin 7))
      (node (ref X1) (pin 24)))
    (net (code 37) (name /PD2)
      (node (ref DA3) (pin 6))
      (node (ref X1) (pin 23)))
    (net (code 38) (name "")
      (node (ref VT1) (pin 6))
      (node (ref VT1) (pin 7))
      (node (ref R5) (pin 1))
      (node (ref VT1) (pin 2))
      (node (ref VT1) (pin 3))
      (node (ref R4) (pin 2)))))