Cmp-Mod V01 Created by CvPcb (2013-may-18)-stable date = Ср 12 ноя 2014 00:15:14

BeginCmp
TimeStamp = /54628F3E;
Reference = BTN1;
ValeurCmp = CONN_1;
IdModule  = PINTST;
EndCmp

BeginCmp
TimeStamp = /54628FEC;
Reference = BTN2;
ValeurCmp = CONN_1;
IdModule  = PINTST;
EndCmp

BeginCmp
TimeStamp = /53F0F83E;
Reference = C4;
ValeurCmp = 0.1u;
IdModule  = SM0603;
EndCmp

BeginCmp
TimeStamp = /53F0F88C;
Reference = C5;
ValeurCmp = 47u;
IdModule  = SM1206POL;
EndCmp

BeginCmp
TimeStamp = /53EF036E/53F36070;
Reference = C6;
ValeurCmp = 0.1u;
IdModule  = SM0603;
EndCmp

BeginCmp
TimeStamp = /53EF036E/53E68EA1;
Reference = D3;
ValeurCmp = DIODESCH;
IdModule  = D4;
EndCmp

BeginCmp
TimeStamp = /53F0EE9F;
Reference = DA1;
ValeurCmp = L9110;
IdModule  = so-8;
EndCmp

BeginCmp
TimeStamp = /53F0EF24;
Reference = DA2;
ValeurCmp = L9110;
IdModule  = so-8;
EndCmp

BeginCmp
TimeStamp = /53F0EF3C;
Reference = DA3;
ValeurCmp = L9110;
IdModule  = so-8;
EndCmp

BeginCmp
TimeStamp = /54628F38;
Reference = DOWN1;
ValeurCmp = CONN_1;
IdModule  = PINTST;
EndCmp

BeginCmp
TimeStamp = /54629D60;
Reference = DRILL+1;
ValeurCmp = CONN_1;
IdModule  = PINTST;
EndCmp

BeginCmp
TimeStamp = /54629E20;
Reference = DRILL-1;
ValeurCmp = CONN_1;
IdModule  = PINTST;
EndCmp

BeginCmp
TimeStamp = /5462B0E5;
Reference = DRILLSW1;
ValeurCmp = CONN_1;
IdModule  = PINTST;
EndCmp

BeginCmp
TimeStamp = /5462B0EB;
Reference = GND1;
ValeurCmp = CONN_1;
IdModule  = PINTST;
EndCmp

BeginCmp
TimeStamp = /53F0FD67;
Reference = K1;
ValeurCmp = POWER;
IdModule  = PIN_ARRAY_3X1;
EndCmp

BeginCmp
TimeStamp = /53F0F09A;
Reference = P3;
ValeurCmp = Stepper;
IdModule  = PIN_ARRAY_4x1;
EndCmp

BeginCmp
TimeStamp = /53F1169C;
Reference = P4;
ValeurCmp = Slide;
IdModule  = PIN_ARRAY_2X1;
EndCmp

BeginCmp
TimeStamp = /54628FF2;
Reference = POT1;
ValeurCmp = CONN_1;
IdModule  = PINTST;
EndCmp

BeginCmp
TimeStamp = /53EF036E/53E680EF;
Reference = R4;
ValeurCmp = 47k;
IdModule  = SM0603;
EndCmp

BeginCmp
TimeStamp = /53EF036E/53E67E8A;
Reference = R5;
ValeurCmp = 0.33R;
IdModule  = r_2512;
EndCmp

BeginCmp
TimeStamp = /53F0F811;
Reference = U2;
ValeurCmp = LM1117MPX-3.3;
IdModule  = SOT223;
EndCmp

BeginCmp
TimeStamp = /54628F0D;
Reference = UP1;
ValeurCmp = CONN_1;
IdModule  = PINTST;
EndCmp

BeginCmp
TimeStamp = /53EF036E/53F123C0;
Reference = VT1;
ValeurCmp = S8205A;
IdModule  = TSSOP-8;
EndCmp

BeginCmp
TimeStamp = /54626F55;
Reference = X1;
ValeurCmp = STM8S105BOARD;
IdModule  = devboard_pins-9-14;
EndCmp

EndListe
