(export (version D)
  (design
    (source /home/eddy/Docs/SAO/Zeiss-1000/Simple_photometer/kicad/hall.sch)
    (date "Пн 27 ноя 2017 15:06:03")
    (tool "Eeschema 4.0.7")
    (sheet (number 1) (name /) (tstamps /)
      (title_block
        (title)
        (company)
        (rev)
        (date)
        (source hall.sch)
        (comment (number 1) (value ""))
        (comment (number 2) (value ""))
        (comment (number 3) (value ""))
        (comment (number 4) (value "")))))
  (components
    (comp (ref P4)
      (value Hole)
      (footprint my_footprints:Hole_2mm)
      (libsource (lib conn) (part Conn_01x01))
      (sheetpath (names /) (tstamps /))
      (tstamp 59143415))
    (comp (ref P1)
      (value Hole)
      (footprint my_footprints:Hole_2mm)
      (libsource (lib conn) (part Conn_01x01))
      (sheetpath (names /) (tstamps /))
      (tstamp 591446F9))
    (comp (ref U1)
      (value A3212LH)
      (footprint TO_SOT_Packages_SMD.pretty:SOT-23W_Handsoldering)
      (libsource (lib a3212lh) (part A3212LH))
      (sheetpath (names /) (tstamps /))
      (tstamp 5A1C0A65))
    (comp (ref R1)
      (value 47k)
      (footprint Resistors_SMD.pretty:R_0805_HandSoldering)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 5A1C0C88))
    (comp (ref J1)
      (value Conn_01x05)
      (footprint my_footprints:SMD5pin)
      (libsource (lib conn) (part Conn_01x05))
      (sheetpath (names /) (tstamps /))
      (tstamp 5A1C0D39)))
  (libparts
    (libpart (lib a3212lh) (part A3212LH)
      (description "Linear Hall Effect Sensor, SOT-23W")
      (footprints
        (fp SOT*))
      (fields
        (field (name Reference) U)
        (field (name Value) A3212LH)
        (field (name Footprint) TO_SOT_Packages_SMD:SOT-23W))
      (pins
        (pin (num 1) (name VCC) (type power_in))
        (pin (num 2) (name Vout) (type output))
        (pin (num 3) (name GND) (type power_in))))
    (libpart (lib conn) (part Conn_01x01)
      (description "Generic connector, single row, 01x01")
      (docs ~)
      (footprints
        (fp Connector*:*_??x*mm*)
        (fp Connector*:*1x??x*mm*)
        (fp Pin?Header?Straight?1X*)
        (fp Pin?Header?Angled?1X*)
        (fp Socket?Strip?Straight?1X*)
        (fp Socket?Strip?Angled?1X*))
      (fields
        (field (name Reference) J)
        (field (name Value) Conn_01x01))
      (pins
        (pin (num 1) (name Pin_1) (type passive))))
    (libpart (lib conn) (part Conn_01x05)
      (description "Generic connector, single row, 01x05")
      (docs ~)
      (footprints
        (fp Connector*:*_??x*mm*)
        (fp Connector*:*1x??x*mm*)
        (fp Pin?Header?Straight?1X*)
        (fp Pin?Header?Angled?1X*)
        (fp Socket?Strip?Straight?1X*)
        (fp Socket?Strip?Angled?1X*))
      (fields
        (field (name Reference) J)
        (field (name Value) Conn_01x05))
      (pins
        (pin (num 1) (name Pin_1) (type passive))
        (pin (num 2) (name Pin_2) (type passive))
        (pin (num 3) (name Pin_3) (type passive))
        (pin (num 4) (name Pin_4) (type passive))
        (pin (num 5) (name Pin_5) (type passive))))
    (libpart (lib device) (part R)
      (description Resistor)
      (footprints
        (fp R_*)
        (fp R_*))
      (fields
        (field (name Reference) R)
        (field (name Value) R))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive)))))
  (libraries
    (library (logical device)
      (uri /usr/share/kicad/library/device.lib))
    (library (logical a3212lh)
      (uri a3212lh.lib))
    (library (logical conn)
      (uri /usr/share/kicad/library/conn.lib)))
  (nets
    (net (code 1) (name "Net-(P4-Pad1)")
      (node (ref P4) (pin 1)))
    (net (code 2) (name "Net-(J1-Pad5)")
      (node (ref R1) (pin 1))
      (node (ref J1) (pin 5)))
    (net (code 3) (name "Net-(P1-Pad1)")
      (node (ref P1) (pin 1)))
    (net (code 5) (name "Net-(J1-Pad1)")
      (node (ref U1) (pin 1))
      (node (ref J1) (pin 1)))
    (net (code 6) (name "Net-(J1-Pad2)")
      (node (ref J1) (pin 3))
      (node (ref J1) (pin 2))
      (node (ref U1) (pin 2)))
    (net (code 7) (name GND)
      (node (ref R1) (pin 2))
      (node (ref U1) (pin 3))
      (node (ref J1) (pin 4)))))