(export (version D)
  (design
    (source /home/eddy/Docs/SAO/Zeiss-1000/Simple_photometer/kicad/usbbrd.sch)
    (date "Пн 27 ноя 2017 15:52:58")
    (tool "Eeschema 4.0.7")
    (sheet (number 1) (name /) (tstamps /)
      (title_block
        (title)
        (company)
        (rev)
        (date)
        (source usbbrd.sch)
        (comment (number 1) (value ""))
        (comment (number 2) (value ""))
        (comment (number 3) (value ""))
        (comment (number 4) (value "")))))
  (components
    (comp (ref J1)
      (value USB_B)
      (footprint Connectors.pretty:USB_B)
      (libsource (lib conn) (part USB_B))
      (sheetpath (names /) (tstamps /))
      (tstamp 5A1C0904))
    (comp (ref J2)
      (value Conn_01x05)
      (footprint my_footprints:SMD5pin)
      (libsource (lib conn) (part Conn_01x05))
      (sheetpath (names /) (tstamps /))
      (tstamp 5A1C0988)))
  (libparts
    (libpart (lib conn) (part Conn_01x05)
      (description "Generic connector, single row, 01x05")
      (docs ~)
      (footprints
        (fp Connector*:*_??x*mm*)
        (fp Connector*:*1x??x*mm*)
        (fp Pin?Header?Straight?1X*)
        (fp Pin?Header?Angled?1X*)
        (fp Socket?Strip?Straight?1X*)
        (fp Socket?Strip?Angled?1X*))
      (fields
        (field (name Reference) J)
        (field (name Value) Conn_01x05))
      (pins
        (pin (num 1) (name Pin_1) (type passive))
        (pin (num 2) (name Pin_2) (type passive))
        (pin (num 3) (name Pin_3) (type passive))
        (pin (num 4) (name Pin_4) (type passive))
        (pin (num 5) (name Pin_5) (type passive))))
    (libpart (lib conn) (part USB_B)
      (description "USB Type B connector")
      (footprints
        (fp USB*))
      (fields
        (field (name Reference) J)
        (field (name Value) USB_B))
      (pins
        (pin (num 1) (name VBUS) (type power_out))
        (pin (num 2) (name D-) (type passive))
        (pin (num 3) (name D+) (type passive))
        (pin (num 4) (name GND) (type power_out))
        (pin (num 5) (name Shield) (type passive)))))
  (libraries
    (library (logical conn)
      (uri /usr/share/kicad/library/conn.lib)))
  (nets
    (net (code 1) (name "Net-(J1-Pad1)")
      (node (ref J2) (pin 4))
      (node (ref J1) (pin 1)))
    (net (code 2) (name "Net-(J1-Pad2)")
      (node (ref J1) (pin 2))
      (node (ref J2) (pin 2)))
    (net (code 3) (name "Net-(J1-Pad3)")
      (node (ref J2) (pin 1))
      (node (ref J1) (pin 3)))
    (net (code 4) (name "Net-(J1-Pad4)")
      (node (ref J2) (pin 5))
      (node (ref J1) (pin 4)))
    (net (code 5) (name "Net-(J2-Pad3)")
      (node (ref J2) (pin 3)))
    (net (code 6) (name "Net-(J1-Pad5)")
      (node (ref J1) (pin 5)))))