4727638037479213
Button_Switch_THT
KSA_Tactile_SPST
KSA http://www.ckswitches.com/media/1457/ksa_ksl.pdf
SWITCH SMD KSA SW
0
5
5
Button_Switch_THT
Nidec_Copal_SH-7010C
4-bit rotary coded switch, through-hole, https://www.nidec-copal-electronics.com/e/catalog/switch/sh-7000.pdf
rotary switch bcd
0
6
5
Button_Switch_THT
Push_E-Switch_KS01Q01
E-Switch KS01Q01 http://spec_sheets.e-switch.com/specs/29-KS01Q01.pdf
Push Button
0
4
4
Button_Switch_THT
SW_CW_GPTS203211B
SPST Off-On Pushbutton, 1A, 30V, CW Industries P/N GPTS203211B, http://switches-connectors-custom.cwind.com/Asset/GPTS203211BR2.pdf
SPST button switch Off-On
0
2
2
Button_Switch_THT
SW_CuK_JS202011AQN_DPDT_Angled
CuK sub miniature slide switch, JS series, DPDT, right angle, http://www.ckswitches.com/media/1422/js.pdf
switch DPDT
0
6
6
Button_Switch_THT
SW_CuK_JS202011CQN_DPDT_Straight
CuK sub miniature slide switch, JS series, DPDT, right angle, http://www.ckswitches.com/media/1422/js.pdf
switch DPDT
0
6
6
Button_Switch_THT
SW_CuK_OS102011MA1QN1_SPDT_Angled
CuK miniature slide switch, OS series, SPDT, right angle, http://www.ckswitches.com/media/1428/os.pdf
switch SPDT
0
5
3
Button_Switch_THT
SW_DIP_SPSTx01_Piano_10.8x4.1mm_W7.62mm_P2.54mm
1x-dip-switch SPST , Piano, row spacing 7.62 mm (300 mils), body size 10.8x4.1mm
DIP Switch SPST Piano 7.62mm 300mil
0
2
2
Button_Switch_THT
SW_DIP_SPSTx01_Slide_6.7x4.1mm_W7.62mm_P2.54mm_LowProfile
1x-dip-switch SPST , Slide, row spacing 7.62 mm (300 mils), body size 6.7x4.1mm (see e.g. https://www.ctscorp.com/wp-content/uploads/209-210.pdf), LowProfile
DIP Switch SPST Slide 7.62mm 300mil LowProfile
0
2
2
Button_Switch_THT
SW_DIP_SPSTx01_Slide_9.78x4.72mm_W7.62mm_P2.54mm
1x-dip-switch SPST , Slide, row spacing 7.62 mm (300 mils), body size 9.78x4.72mm (see e.g. https://www.ctscorp.com/wp-content/uploads/206-208.pdf)
DIP Switch SPST Slide 7.62mm 300mil
0
2
2
Button_Switch_THT
SW_DIP_SPSTx02_Piano_10.8x6.64mm_W7.62mm_P2.54mm
2x-dip-switch SPST , Piano, row spacing 7.62 mm (300 mils), body size 10.8x6.64mm
DIP Switch SPST Piano 7.62mm 300mil
0
4
4
Button_Switch_THT
SW_DIP_SPSTx02_Piano_CTS_Series194-2MSTN_W7.62mm_P2.54mm
2x-dip-switch SPST CTS_Series194-2MSTN, Piano, row spacing 7.62 mm (300 mils), body size  (see https://www.ctscorp.com/wp-content/uploads/194-195.pdf)
DIP Switch SPST Piano 7.62mm 300mil
0
4
4
Button_Switch_THT
SW_DIP_SPSTx02_Slide_6.7x6.64mm_W7.62mm_P2.54mm_LowProfile
2x-dip-switch SPST , Slide, row spacing 7.62 mm (300 mils), body size 6.7x6.64mm (see e.g. https://www.ctscorp.com/wp-content/uploads/209-210.pdf), LowProfile
DIP Switch SPST Slide 7.62mm 300mil LowProfile
0
4
4
Button_Switch_THT
SW_DIP_SPSTx02_Slide_9.78x7.26mm_W7.62mm_P2.54mm
2x-dip-switch SPST , Slide, row spacing 7.62 mm (300 mils), body size 9.78x7.26mm (see e.g. https://www.ctscorp.com/wp-content/uploads/206-208.pdf)
DIP Switch SPST Slide 7.62mm 300mil
0
4
4
Button_Switch_THT
SW_DIP_SPSTx03_Piano_10.8x9.18mm_W7.62mm_P2.54mm
3x-dip-switch SPST , Piano, row spacing 7.62 mm (300 mils), body size 10.8x9.18mm
DIP Switch SPST Piano 7.62mm 300mil
0
6
6
Button_Switch_THT
SW_DIP_SPSTx03_Piano_CTS_Series194-3MSTN_W7.62mm_P2.54mm
3x-dip-switch SPST CTS_Series194-3MSTN, Piano, row spacing 7.62 mm (300 mils), body size  (see https://www.ctscorp.com/wp-content/uploads/194-195.pdf)
DIP Switch SPST Piano 7.62mm 300mil
0
6
6
Button_Switch_THT
SW_DIP_SPSTx03_Slide_6.7x9.18mm_W7.62mm_P2.54mm_LowProfile
3x-dip-switch SPST , Slide, row spacing 7.62 mm (300 mils), body size 6.7x9.18mm (see e.g. https://www.ctscorp.com/wp-content/uploads/209-210.pdf), LowProfile
DIP Switch SPST Slide 7.62mm 300mil LowProfile
0
6
6
Button_Switch_THT
SW_DIP_SPSTx03_Slide_9.78x9.8mm_W7.62mm_P2.54mm
3x-dip-switch SPST , Slide, row spacing 7.62 mm (300 mils), body size 9.78x9.8mm (see e.g. https://www.ctscorp.com/wp-content/uploads/206-208.pdf)
DIP Switch SPST Slide 7.62mm 300mil
0
6
6
Button_Switch_THT
SW_DIP_SPSTx04_Piano_10.8x11.72mm_W7.62mm_P2.54mm
4x-dip-switch SPST , Piano, row spacing 7.62 mm (300 mils), body size 10.8x11.72mm
DIP Switch SPST Piano 7.62mm 300mil
0
8
8
Button_Switch_THT
SW_DIP_SPSTx04_Piano_CTS_Series194-4MSTN_W7.62mm_P2.54mm
4x-dip-switch SPST CTS_Series194-4MSTN, Piano, row spacing 7.62 mm (300 mils), body size  (see https://www.ctscorp.com/wp-content/uploads/194-195.pdf)
DIP Switch SPST Piano 7.62mm 300mil
0
8
8
Button_Switch_THT
SW_DIP_SPSTx04_Slide_6.7x11.72mm_W7.62mm_P2.54mm_LowProfile
4x-dip-switch SPST , Slide, row spacing 7.62 mm (300 mils), body size 6.7x11.72mm (see e.g. https://www.ctscorp.com/wp-content/uploads/209-210.pdf), LowProfile
DIP Switch SPST Slide 7.62mm 300mil LowProfile
0
8
8
Button_Switch_THT
SW_DIP_SPSTx04_Slide_9.78x12.34mm_W7.62mm_P2.54mm
4x-dip-switch SPST , Slide, row spacing 7.62 mm (300 mils), body size 9.78x12.34mm (see e.g. https://www.ctscorp.com/wp-content/uploads/206-208.pdf)
DIP Switch SPST Slide 7.62mm 300mil
0
8
8
Button_Switch_THT
SW_DIP_SPSTx05_Piano_10.8x14.26mm_W7.62mm_P2.54mm
5x-dip-switch SPST , Piano, row spacing 7.62 mm (300 mils), body size 10.8x14.26mm
DIP Switch SPST Piano 7.62mm 300mil
0
10
10
Button_Switch_THT
SW_DIP_SPSTx05_Piano_CTS_Series194-5MSTN_W7.62mm_P2.54mm
5x-dip-switch SPST CTS_Series194-5MSTN, Piano, row spacing 7.62 mm (300 mils), body size  (see https://www.ctscorp.com/wp-content/uploads/194-195.pdf)
DIP Switch SPST Piano 7.62mm 300mil
0
10
10
Button_Switch_THT
SW_DIP_SPSTx05_Slide_6.7x14.26mm_W7.62mm_P2.54mm_LowProfile
5x-dip-switch SPST , Slide, row spacing 7.62 mm (300 mils), body size 6.7x14.26mm (see e.g. https://www.ctscorp.com/wp-content/uploads/209-210.pdf), LowProfile
DIP Switch SPST Slide 7.62mm 300mil LowProfile
0
10
10
Button_Switch_THT
SW_DIP_SPSTx05_Slide_9.78x14.88mm_W7.62mm_P2.54mm
5x-dip-switch SPST , Slide, row spacing 7.62 mm (300 mils), body size 9.78x14.88mm (see e.g. https://www.ctscorp.com/wp-content/uploads/206-208.pdf)
DIP Switch SPST Slide 7.62mm 300mil
0
10
10
Button_Switch_THT
SW_DIP_SPSTx06_Piano_10.8x16.8mm_W7.62mm_P2.54mm
6x-dip-switch SPST , Piano, row spacing 7.62 mm (300 mils), body size 10.8x16.8mm
DIP Switch SPST Piano 7.62mm 300mil
0
12
12
Button_Switch_THT
SW_DIP_SPSTx06_Piano_CTS_Series194-6MSTN_W7.62mm_P2.54mm
6x-dip-switch SPST CTS_Series194-6MSTN, Piano, row spacing 7.62 mm (300 mils), body size  (see https://www.ctscorp.com/wp-content/uploads/194-195.pdf)
DIP Switch SPST Piano 7.62mm 300mil
0
12
12
Button_Switch_THT
SW_DIP_SPSTx06_Slide_6.7x16.8mm_W7.62mm_P2.54mm_LowProfile
6x-dip-switch SPST , Slide, row spacing 7.62 mm (300 mils), body size 6.7x16.8mm (see e.g. https://www.ctscorp.com/wp-content/uploads/209-210.pdf), LowProfile
DIP Switch SPST Slide 7.62mm 300mil LowProfile
0
12
12
Button_Switch_THT
SW_DIP_SPSTx06_Slide_9.78x17.42mm_W7.62mm_P2.54mm
6x-dip-switch SPST , Slide, row spacing 7.62 mm (300 mils), body size 9.78x17.42mm (see e.g. https://www.ctscorp.com/wp-content/uploads/206-208.pdf)
DIP Switch SPST Slide 7.62mm 300mil
0
12
12
Button_Switch_THT
SW_DIP_SPSTx07_Piano_10.8x19.34mm_W7.62mm_P2.54mm
7x-dip-switch SPST , Piano, row spacing 7.62 mm (300 mils), body size 10.8x19.34mm
DIP Switch SPST Piano 7.62mm 300mil
0
14
14
Button_Switch_THT
SW_DIP_SPSTx07_Piano_CTS_Series194-7MSTN_W7.62mm_P2.54mm
7x-dip-switch SPST CTS_Series194-7MSTN, Piano, row spacing 7.62 mm (300 mils), body size  (see https://www.ctscorp.com/wp-content/uploads/194-195.pdf)
DIP Switch SPST Piano 7.62mm 300mil
0
14
14
Button_Switch_THT
SW_DIP_SPSTx07_Slide_6.7x19.34mm_W7.62mm_P2.54mm_LowProfile
7x-dip-switch SPST , Slide, row spacing 7.62 mm (300 mils), body size 6.7x19.34mm (see e.g. https://www.ctscorp.com/wp-content/uploads/209-210.pdf), LowProfile
DIP Switch SPST Slide 7.62mm 300mil LowProfile
0
14
14
Button_Switch_THT
SW_DIP_SPSTx07_Slide_9.78x19.96mm_W7.62mm_P2.54mm
7x-dip-switch SPST , Slide, row spacing 7.62 mm (300 mils), body size 9.78x19.96mm (see e.g. https://www.ctscorp.com/wp-content/uploads/206-208.pdf)
DIP Switch SPST Slide 7.62mm 300mil
0
14
14
Button_Switch_THT
SW_DIP_SPSTx08_Piano_10.8x21.88mm_W7.62mm_P2.54mm
8x-dip-switch SPST , Piano, row spacing 7.62 mm (300 mils), body size 10.8x21.88mm
DIP Switch SPST Piano 7.62mm 300mil
0
16
16
Button_Switch_THT
SW_DIP_SPSTx08_Piano_CTS_Series194-8MSTN_W7.62mm_P2.54mm
8x-dip-switch SPST CTS_Series194-8MSTN, Piano, row spacing 7.62 mm (300 mils), body size  (see https://www.ctscorp.com/wp-content/uploads/194-195.pdf)
DIP Switch SPST Piano 7.62mm 300mil
0
16
16
Button_Switch_THT
SW_DIP_SPSTx08_Slide_6.7x21.88mm_W7.62mm_P2.54mm_LowProfile
8x-dip-switch SPST , Slide, row spacing 7.62 mm (300 mils), body size 6.7x21.88mm (see e.g. https://www.ctscorp.com/wp-content/uploads/209-210.pdf), LowProfile
DIP Switch SPST Slide 7.62mm 300mil LowProfile
0
16
16
Button_Switch_THT
SW_DIP_SPSTx08_Slide_9.78x22.5mm_W7.62mm_P2.54mm
8x-dip-switch SPST , Slide, row spacing 7.62 mm (300 mils), body size 9.78x22.5mm (see e.g. https://www.ctscorp.com/wp-content/uploads/206-208.pdf)
DIP Switch SPST Slide 7.62mm 300mil
0
16
16
Button_Switch_THT
SW_DIP_SPSTx09_Piano_10.8x24.42mm_W7.62mm_P2.54mm
9x-dip-switch SPST , Piano, row spacing 7.62 mm (300 mils), body size 10.8x24.42mm
DIP Switch SPST Piano 7.62mm 300mil
0
18
18
Button_Switch_THT
SW_DIP_SPSTx09_Piano_CTS_Series194-9MSTN_W7.62mm_P2.54mm
9x-dip-switch SPST CTS_Series194-9MSTN, Piano, row spacing 7.62 mm (300 mils), body size  (see https://www.ctscorp.com/wp-content/uploads/194-195.pdf)
DIP Switch SPST Piano 7.62mm 300mil
0
18
18
Button_Switch_THT
SW_DIP_SPSTx09_Slide_6.7x24.42mm_W7.62mm_P2.54mm_LowProfile
9x-dip-switch SPST , Slide, row spacing 7.62 mm (300 mils), body size 6.7x24.42mm (see e.g. https://www.ctscorp.com/wp-content/uploads/209-210.pdf), LowProfile
DIP Switch SPST Slide 7.62mm 300mil LowProfile
0
18
18
Button_Switch_THT
SW_DIP_SPSTx09_Slide_9.78x25.04mm_W7.62mm_P2.54mm
9x-dip-switch SPST , Slide, row spacing 7.62 mm (300 mils), body size 9.78x25.04mm (see e.g. https://www.ctscorp.com/wp-content/uploads/206-208.pdf)
DIP Switch SPST Slide 7.62mm 300mil
0
18
18
Button_Switch_THT
SW_DIP_SPSTx10_Piano_10.8x26.96mm_W7.62mm_P2.54mm
10x-dip-switch SPST , Piano, row spacing 7.62 mm (300 mils), body size 10.8x26.96mm
DIP Switch SPST Piano 7.62mm 300mil
0
20
20
Button_Switch_THT
SW_DIP_SPSTx10_Piano_CTS_Series194-10MSTN_W7.62mm_P2.54mm
10x-dip-switch SPST CTS_Series194-10MSTN, Piano, row spacing 7.62 mm (300 mils), body size  (see https://www.ctscorp.com/wp-content/uploads/194-195.pdf)
DIP Switch SPST Piano 7.62mm 300mil
0
20
20
Button_Switch_THT
SW_DIP_SPSTx10_Slide_6.7x26.96mm_W7.62mm_P2.54mm_LowProfile
10x-dip-switch SPST , Slide, row spacing 7.62 mm (300 mils), body size 6.7x26.96mm (see e.g. https://www.ctscorp.com/wp-content/uploads/209-210.pdf), LowProfile
DIP Switch SPST Slide 7.62mm 300mil LowProfile
0
20
20
Button_Switch_THT
SW_DIP_SPSTx10_Slide_9.78x27.58mm_W7.62mm_P2.54mm
10x-dip-switch SPST , Slide, row spacing 7.62 mm (300 mils), body size 9.78x27.58mm (see e.g. https://www.ctscorp.com/wp-content/uploads/206-208.pdf)
DIP Switch SPST Slide 7.62mm 300mil
0
20
20
Button_Switch_THT
SW_DIP_SPSTx11_Piano_10.8x29.5mm_W7.62mm_P2.54mm
11x-dip-switch SPST , Piano, row spacing 7.62 mm (300 mils), body size 10.8x29.5mm
DIP Switch SPST Piano 7.62mm 300mil
0
22
22
Button_Switch_THT
SW_DIP_SPSTx11_Piano_CTS_Series194-11MSTN_W7.62mm_P2.54mm
11x-dip-switch SPST CTS_Series194-11MSTN, Piano, row spacing 7.62 mm (300 mils), body size  (see https://www.ctscorp.com/wp-content/uploads/194-195.pdf)
DIP Switch SPST Piano 7.62mm 300mil
0
22
22
Button_Switch_THT
SW_DIP_SPSTx11_Slide_6.7x29.5mm_W7.62mm_P2.54mm_LowProfile
11x-dip-switch SPST , Slide, row spacing 7.62 mm (300 mils), body size 6.7x29.5mm (see e.g. https://www.ctscorp.com/wp-content/uploads/209-210.pdf), LowProfile
DIP Switch SPST Slide 7.62mm 300mil LowProfile
0
22
22
Button_Switch_THT
SW_DIP_SPSTx11_Slide_9.78x30.12mm_W7.62mm_P2.54mm
11x-dip-switch SPST , Slide, row spacing 7.62 mm (300 mils), body size 9.78x30.12mm (see e.g. https://www.ctscorp.com/wp-content/uploads/206-208.pdf)
DIP Switch SPST Slide 7.62mm 300mil
0
22
22
Button_Switch_THT
SW_DIP_SPSTx12_Piano_10.8x32.04mm_W7.62mm_P2.54mm
12x-dip-switch SPST , Piano, row spacing 7.62 mm (300 mils), body size 10.8x32.04mm
DIP Switch SPST Piano 7.62mm 300mil
0
24
24
Button_Switch_THT
SW_DIP_SPSTx12_Piano_CTS_Series194-12MSTN_W7.62mm_P2.54mm
12x-dip-switch SPST CTS_Series194-12MSTN, Piano, row spacing 7.62 mm (300 mils), body size  (see https://www.ctscorp.com/wp-content/uploads/194-195.pdf)
DIP Switch SPST Piano 7.62mm 300mil
0
24
24
Button_Switch_THT
SW_DIP_SPSTx12_Slide_6.7x32.04mm_W7.62mm_P2.54mm_LowProfile
12x-dip-switch SPST , Slide, row spacing 7.62 mm (300 mils), body size 6.7x32.04mm (see e.g. https://www.ctscorp.com/wp-content/uploads/209-210.pdf), LowProfile
DIP Switch SPST Slide 7.62mm 300mil LowProfile
0
24
24
Button_Switch_THT
SW_DIP_SPSTx12_Slide_9.78x32.66mm_W7.62mm_P2.54mm
12x-dip-switch SPST , Slide, row spacing 7.62 mm (300 mils), body size 9.78x32.66mm (see e.g. https://www.ctscorp.com/wp-content/uploads/206-208.pdf)
DIP Switch SPST Slide 7.62mm 300mil
0
24
24
Button_Switch_THT
SW_E-Switch_EG1224_SPDT_Angled
E-Switch slide switch, EG series, SPDT, right angle, http://spec_sheets.e-switch.com/specs/P040042.pdf
switch SPDT
0
7
3
Button_Switch_THT
SW_E-Switch_EG1271_DPDT
E-Switch sub miniature slide switch, EG series, DPDT, http://spec_sheets.e-switch.com/specs/P040047.pdf
switch DPDT
0
6
6
Button_Switch_THT
SW_E-Switch_EG2219_DPDT_Angled
E-Switch slide switch, EG series, DPDT, right angle, http://spec_sheets.e-switch.com/specs/P040170.pdf
switch DPDT
0
10
6
Button_Switch_THT
SW_Lever_1P2T_NKK_GW12LxH
Switch, single pole double throw, right angle, http://www.nkkswitches.com/pdf/GW.pdf
switch single-pole double-throw spdt ON-ON horizontal
0
5
3
Button_Switch_THT
SW_MEC_5GTH9
MEC 5G single pole normally-open tactile switch https://cdn.sos.sk/productdata/80/f6/aabf7be6/5gth9358222.pdf
switch normally-open pushbutton push-button
0
4
2
Button_Switch_THT
SW_NKK_BB15AH
https://www.nkkswitches.com/pdf/Bpushbuttons-1.pdf
Pushbutton Right-angle
0
5
3
Button_Switch_THT
SW_NKK_G1xJP
Switch NKK G1xJP http://www.nkkswitches.com/pdf/gwillum.pdf
SWITCH TOGGLE ILLUM SPDT NKK
0
6
6
Button_Switch_THT
SW_NKK_GW12LJP
Switch, single pole double throw, illuminated paddle, http://www.nkkswitches.com/pdf/gwillum.pdf
switch single-pole double-throw spdt ON-ON illuminated LED
0
6
6
Button_Switch_THT
SW_PUSH-12mm
SW PUSH 12mm https://www.e-switch.com/system/asset/product_line/data_sheet/143/TL1100.pdf
tact sw push 12mm
0
4
2
Button_Switch_THT
SW_PUSH-12mm_Wuerth-430476085716
SW PUSH 12mm http://katalog.we-online.de/em/datasheet/430476085716.pdf
tact sw push 12mm
0
4
2
Button_Switch_THT
SW_PUSH_6mm
https://www.omron.com/ecb/products/pdf/en-b3f.pdf
tact sw push 6mm
0
4
2
Button_Switch_THT
SW_PUSH_6mm_H4.3mm
tactile push button, 6x6mm e.g. PHAP33xx series, height=4.3mm
tact sw push 6mm
0
4
2
Button_Switch_THT
SW_PUSH_6mm_H5mm
tactile push button, 6x6mm e.g. PHAP33xx series, height=5mm
tact sw push 6mm
0
4
2
Button_Switch_THT
SW_PUSH_6mm_H7.3mm
tactile push button, 6x6mm e.g. PHAP33xx series, height=7.3mm
tact sw push 6mm
0
4
2
Button_Switch_THT
SW_PUSH_6mm_H8.5mm
tactile push button, 6x6mm e.g. PHAP33xx series, height=8.5mm
tact sw push 6mm
0
4
2
Button_Switch_THT
SW_PUSH_6mm_H8mm
tactile push button, 6x6mm e.g. PHAP33xx series, height=8mm
tact sw push 6mm
0
4
2
Button_Switch_THT
SW_PUSH_6mm_H9.5mm
tactile push button, 6x6mm e.g. PHAP33xx series, height=9.5mm
tact sw push 6mm
0
4
2
Button_Switch_THT
SW_PUSH_6mm_H13mm
tactile push button, 6x6mm e.g. PHAP33xx series, height=13mm
tact sw push 6mm
0
4
2
Button_Switch_THT
SW_PUSH_E-Switch_FS5700DP_DPDT
FS5700 series pushbutton footswitch, DPDT, https://www.e-switch.com/system/asset/product_line/data_sheet/226/FS5700.pdf
switch DPDT footswitch
0
6
6
Button_Switch_THT
SW_PUSH_LCD_E3_SAxxxx
Switch with LCD screen E3 SAxxxx
switch normally-open pushbutton push-button LCD
0
6
6
Button_Switch_THT
SW_PUSH_LCD_E3_SAxxxx_SocketPins
Switch with LCD screen E3 SAxxxx
switch normally-open pushbutton push-button LCD
0
6
6
Button_Switch_THT
SW_Push_1P1T_NO_LED_E-Switch_TL1250
illuminated right angle tact switch https://www.e-switch.com/system/asset/product_line/data_sheet/148/TL1250.pdf
led push switch right angle
0
6
4
Button_Switch_THT
SW_Push_1P2T_Vertical_E-Switch_800UDP8P1A1M6
 right angle SPDT push button https://www.e-switch.com/system/asset/product_line/data_sheet/210/800U.pdf
IP67 ultra-miniture horizontal
0
5
3
Button_Switch_THT
SW_Push_2P2T_Vertical_E-Switch_800UDP8P1A1M6
 right angle DPDT push button https://www.e-switch.com/system/asset/product_line/data_sheet/210/800U.pdf
IP67 ultra-miniture horizontal
0
8
6
Button_Switch_THT
SW_Slide_1P2T_CK_OS102011MS2Q
CuK miniature slide switch, OS series, SPDT, https://www.ckswitches.com/media/1428/os.pdf
switch SPDT
0
5
3
Button_Switch_THT
SW_TH_Tactile_Omron_B3F-10xx
SW_TH_Tactile_Omron_B3F-10xx_https://www.omron.com/ecb/products/pdf/en-b3f.pdf
Omron B3F-10xx
0
4
4
Button_Switch_THT
SW_Tactile_SKHH_Angled
tactile switch 6mm ALPS SKHH right angle http://www.alps.com/prod/info/E/HTML/Tact/SnapIn/SKHH/SKHHLUA010.html
tactile switch 6mm ALPS SKHH right angle
0
4
2
Button_Switch_THT
SW_Tactile_SPST_Angled_PTS645Vx31-2LFS
tactile switch SPST right angle, PTS645VL31-2 LFS
tactile switch SPST angled PTS645VL31-2 LFS C&K Button
0
4
2
Button_Switch_THT
SW_Tactile_SPST_Angled_PTS645Vx39-2LFS
tactile switch SPST right angle, PTS645VL39-2 LFS
tactile switch SPST angled PTS645VL39-2 LFS C&K Button
0
4
2
Button_Switch_THT
SW_Tactile_SPST_Angled_PTS645Vx58-2LFS
tactile switch SPST right angle, PTS645VL58-2 LFS
tactile switch SPST angled PTS645VL58-2 LFS C&K Button
0
4
2
Button_Switch_THT
SW_Tactile_SPST_Angled_PTS645Vx83-2LFS
tactile switch SPST right angle, PTS645VL83-2 LFS
tactile switch SPST angled PTS645VL83-2 LFS C&K Button
0
4
2
Button_Switch_THT
SW_Tactile_Straight_KSA0Axx1LFTR
SW PUSH SMALL http://www.ckswitches.com/media/1457/ksa_ksl.pdf
SW PUSH SMALL Tactile C&K
0
4
2
Button_Switch_THT
SW_Tactile_Straight_KSL0Axx1LFTR
SW PUSH SMALL http://www.ckswitches.com/media/1457/ksa_ksl.pdf
SW PUSH SMALL Tactile C&K
0
4
2
Buttons_Switches_SMD
Nidec_Copal_SH-7010A
4-bit rotary coded switch, J-hook, https://www.nidec-copal-electronics.com/e/catalog/switch/sh-7000.pdf
rotary switch bcd
0
6
5
Buttons_Switches_SMD
Nidec_Copal_SH-7010B
4-bit rotary coded switch, gull wing, https://www.nidec-copal-electronics.com/e/catalog/switch/sh-7000.pdf
rotary switch bcd
0
6
5
Buttons_Switches_SMD
Nidec_Copal_SH-7040B
4-bit rotary coded switch, gull wing, Gray code, https://www.nidec-copal-electronics.com/e/catalog/switch/sh-7000.pdf
rotary switch bcd
0
5
5
Buttons_Switches_SMD
Panasonic_EVQPUJ_EVQPUA
http://industrial.panasonic.com/cdbs/www-data/pdf/ATV0000/ATV0000CE5.pdf
SMD SMT SPST EVQPUJ EVQPUA
0
4
2
Buttons_Switches_SMD
Panasonic_EVQPUK_EVQPUB
http://industrial.panasonic.com/cdbs/www-data/pdf/ATV0000/ATV0000CE5.pdf
SMD SMT SPST EVQPUK EVQPUB
0
4
2
Buttons_Switches_SMD
Panasonic_EVQPUL_EVQPUC
http://industrial.panasonic.com/cdbs/www-data/pdf/ATV0000/ATV0000CE5.pdf
SMD SMT SPST EVQPUL EVQPUC
0
4
2
Buttons_Switches_SMD
Panasonic_EVQPUM_EVQPUD
http://industrial.panasonic.com/cdbs/www-data/pdf/ATV0000/ATV0000CE5.pdf
SMD SMT SPST EVQPUM EVQPUD
0
4
2
Buttons_Switches_SMD
SW_DIP_SPSTx01_Slide_6.7x4.1mm_W6.73mm_P2.54mm_LowProfile_JPin
SMD 1x-dip-switch SPST , Slide, row spacing 6.73 mm (264 mils), body size 6.7x4.1mm (see e.g. https://www.ctscorp.com/wp-content/uploads/219.pdf), SMD, LowProfile, JPin
SMD DIP Switch SPST Slide 6.73mm 264mil SMD LowProfile JPin
0
2
2
Buttons_Switches_SMD
SW_DIP_SPSTx01_Slide_6.7x4.1mm_W8.61mm_P2.54mm_LowProfile
SMD 1x-dip-switch SPST , Slide, row spacing 8.61 mm (338 mils), body size 6.7x4.1mm (see e.g. https://www.ctscorp.com/wp-content/uploads/219.pdf), SMD, LowProfile
SMD DIP Switch SPST Slide 8.61mm 338mil SMD LowProfile
0
2
2
Buttons_Switches_SMD
SW_DIP_SPSTx01_Slide_9.78x4.72mm_W8.61mm_P2.54mm
SMD 1x-dip-switch SPST , Slide, row spacing 8.61 mm (338 mils), body size 9.78x4.72mm (see e.g. https://www.ctscorp.com/wp-content/uploads/204.pdf), SMD
SMD DIP Switch SPST Slide 8.61mm 338mil SMD
0
2
2
Buttons_Switches_SMD
SW_DIP_SPSTx01_Slide_Copal_CHS-01A_W5.08mm_P1.27mm_JPin
SMD 1x-dip-switch SPST Copal_CHS-01A, Slide, row spacing 5.08 mm (200 mils), body size  (see http://www.nidec-copal-electronics.com/e/catalog/switch/chs.pdf), SMD, JPin
SMD DIP Switch SPST Slide 5.08mm 200mil SMD JPin
0
2
2
Buttons_Switches_SMD
SW_DIP_SPSTx01_Slide_Copal_CHS-01B_W7.62mm_P1.27mm
SMD 1x-dip-switch SPST Copal_CHS-01B, Slide, row spacing 7.62 mm (300 mils), body size  (see http://www.nidec-copal-electronics.com/e/catalog/switch/chs.pdf), SMD
SMD DIP Switch SPST Slide 7.62mm 300mil SMD
0
2
2
Buttons_Switches_SMD
SW_DIP_SPSTx01_Slide_Copal_CVS-01xB_W5.9mm_P1mm
SMD 1x-dip-switch SPST Copal_CVS-01xB, Slide, row spacing 5.9 mm (232 mils), body size  (see http://www.nidec-copal-electronics.com/e/catalog/switch/cvs.pdf)
SMD DIP Switch SPST Slide 5.9mm 232mil
0
6
3
Buttons_Switches_SMD
SW_DIP_SPSTx01_Slide_Omron_A6S-110x_W8.9mm_P2.54mm
SMD 1x-dip-switch SPST Omron_A6S-110x, Slide, row spacing 8.9 mm (350 mils), body size  (see http://omronfs.omron.com/en_US/ecb/products/pdf/en-a6s.pdf)
SMD DIP Switch SPST Slide 8.9mm 350mil
0
2
2
Buttons_Switches_SMD
SW_DIP_SPSTx02_Slide_6.7x6.64mm_W6.73mm_P2.54mm_LowProfile_JPin
SMD 2x-dip-switch SPST , Slide, row spacing 6.73 mm (264 mils), body size 6.7x6.64mm (see e.g. https://www.ctscorp.com/wp-content/uploads/219.pdf), SMD, LowProfile, JPin
SMD DIP Switch SPST Slide 6.73mm 264mil SMD LowProfile JPin
0
4
4
Buttons_Switches_SMD
SW_DIP_SPSTx02_Slide_6.7x6.64mm_W8.61mm_P2.54mm_LowProfile
SMD 2x-dip-switch SPST , Slide, row spacing 8.61 mm (338 mils), body size 6.7x6.64mm (see e.g. https://www.ctscorp.com/wp-content/uploads/219.pdf), SMD, LowProfile
SMD DIP Switch SPST Slide 8.61mm 338mil SMD LowProfile
0
4
4
Buttons_Switches_SMD
SW_DIP_SPSTx02_Slide_9.78x7.26mm_W8.61mm_P2.54mm
SMD 2x-dip-switch SPST , Slide, row spacing 8.61 mm (338 mils), body size 9.78x7.26mm (see e.g. https://www.ctscorp.com/wp-content/uploads/204.pdf), SMD
SMD DIP Switch SPST Slide 8.61mm 338mil SMD
0
4
4
Buttons_Switches_SMD
SW_DIP_SPSTx02_Slide_Copal_CHS-02A_W5.08mm_P1.27mm_JPin
SMD 2x-dip-switch SPST Copal_CHS-02A, Slide, row spacing 5.08 mm (200 mils), body size  (see http://www.nidec-copal-electronics.com/e/catalog/switch/chs.pdf), SMD, JPin
SMD DIP Switch SPST Slide 5.08mm 200mil SMD JPin
0
4
4
Buttons_Switches_SMD
SW_DIP_SPSTx02_Slide_Copal_CHS-02B_W7.62mm_P1.27mm
SMD 2x-dip-switch SPST Copal_CHS-02B, Slide, row spacing 7.62 mm (300 mils), body size  (see http://www.nidec-copal-electronics.com/e/catalog/switch/chs.pdf), SMD
SMD DIP Switch SPST Slide 7.62mm 300mil SMD
0
4
4
Buttons_Switches_SMD
SW_DIP_SPSTx02_Slide_Copal_CVS-02xB_W5.9mm_P1mm
SMD 2x-dip-switch SPST Copal_CVS-02xB, Slide, row spacing 5.9 mm (232 mils), body size  (see http://www.nidec-copal-electronics.com/e/catalog/switch/cvs.pdf)
SMD DIP Switch SPST Slide 5.9mm 232mil
0
8
5
Buttons_Switches_SMD
SW_DIP_SPSTx02_Slide_KingTek_DSHP02TJ_W5.25mm_P1.27mm_JPin
SMD 2x-dip-switch SPST KingTek_DSHP02TJ, Slide, row spacing 5.25 mm (206 mils), body size  (see http://www.kingtek.net.cn/pic/201601201446313350.pdf), JPin
SMD DIP Switch SPST Slide 5.25mm 206mil JPin
0
4
4
Buttons_Switches_SMD
SW_DIP_SPSTx02_Slide_KingTek_DSHP02TS_W7.62mm_P1.27mm
SMD 2x-dip-switch SPST KingTek_DSHP02TS, Slide, row spacing 7.62 mm (300 mils), body size  (see http://www.kingtek.net.cn/pic/201601201417455112.pdf)
SMD DIP Switch SPST Slide 7.62mm 300mil
0
4
4
Buttons_Switches_SMD
SW_DIP_SPSTx02_Slide_Omron_A6H-2101_W6.15mm_P1.27mm
SMD 2x-dip-switch SPST Omron_A6H-2101, Slide, row spacing 6.15 mm (242 mils), body size  (see https://www.omron.com/ecb/products/pdf/en-a6h.pdf)
SMD DIP Switch SPST Slide 6.15mm 242mil
0
4
4
Buttons_Switches_SMD
SW_DIP_SPSTx02_Slide_Omron_A6S-210x_W8.9mm_P2.54mm
SMD 2x-dip-switch SPST Omron_A6S-210x, Slide, row spacing 8.9 mm (350 mils), body size  (see http://omronfs.omron.com/en_US/ecb/products/pdf/en-a6s.pdf)
SMD DIP Switch SPST Slide 8.9mm 350mil
0
4
4
Buttons_Switches_SMD
SW_DIP_SPSTx03_Slide_6.7x9.18mm_W6.73mm_P2.54mm_LowProfile_JPin
SMD 3x-dip-switch SPST , Slide, row spacing 6.73 mm (264 mils), body size 6.7x9.18mm (see e.g. https://www.ctscorp.com/wp-content/uploads/219.pdf), SMD, LowProfile, JPin
SMD DIP Switch SPST Slide 6.73mm 264mil SMD LowProfile JPin
0
6
6
Buttons_Switches_SMD
SW_DIP_SPSTx03_Slide_6.7x9.18mm_W8.61mm_P2.54mm_LowProfile
SMD 3x-dip-switch SPST , Slide, row spacing 8.61 mm (338 mils), body size 6.7x9.18mm (see e.g. https://www.ctscorp.com/wp-content/uploads/219.pdf), SMD, LowProfile
SMD DIP Switch SPST Slide 8.61mm 338mil SMD LowProfile
0
6
6
Buttons_Switches_SMD
SW_DIP_SPSTx03_Slide_9.78x9.8mm_W8.61mm_P2.54mm
SMD 3x-dip-switch SPST , Slide, row spacing 8.61 mm (338 mils), body size 9.78x9.8mm (see e.g. https://www.ctscorp.com/wp-content/uploads/204.pdf), SMD
SMD DIP Switch SPST Slide 8.61mm 338mil SMD
0
6
6
Buttons_Switches_SMD
SW_DIP_SPSTx03_Slide_Copal_CVS-03xB_W5.9mm_P1mm
SMD 3x-dip-switch SPST Copal_CVS-03xB, Slide, row spacing 5.9 mm (232 mils), body size  (see http://www.nidec-copal-electronics.com/e/catalog/switch/cvs.pdf)
SMD DIP Switch SPST Slide 5.9mm 232mil
0
10
7
Buttons_Switches_SMD
SW_DIP_SPSTx03_Slide_KingTek_DSHP03TJ_W5.25mm_P1.27mm_JPin
SMD 3x-dip-switch SPST KingTek_DSHP03TJ, Slide, row spacing 5.25 mm (206 mils), body size  (see http://www.kingtek.net.cn/pic/201601201446313350.pdf), JPin
SMD DIP Switch SPST Slide 5.25mm 206mil JPin
0
6
6
Buttons_Switches_SMD
SW_DIP_SPSTx03_Slide_KingTek_DSHP03TS_W7.62mm_P1.27mm
SMD 3x-dip-switch SPST KingTek_DSHP03TS, Slide, row spacing 7.62 mm (300 mils), body size  (see http://www.kingtek.net.cn/pic/201601201417455112.pdf)
SMD DIP Switch SPST Slide 7.62mm 300mil
0
6
6
Buttons_Switches_SMD
SW_DIP_SPSTx03_Slide_Omron_A6S-310x_W8.9mm_P2.54mm
SMD 3x-dip-switch SPST Omron_A6S-310x, Slide, row spacing 8.9 mm (350 mils), body size  (see http://omronfs.omron.com/en_US/ecb/products/pdf/en-a6s.pdf)
SMD DIP Switch SPST Slide 8.9mm 350mil
0
6
6
Buttons_Switches_SMD
SW_DIP_SPSTx04_Slide_6.7x11.72mm_W6.73mm_P2.54mm_LowProfile_JPin
SMD 4x-dip-switch SPST , Slide, row spacing 6.73 mm (264 mils), body size 6.7x11.72mm (see e.g. https://www.ctscorp.com/wp-content/uploads/219.pdf), SMD, LowProfile, JPin
SMD DIP Switch SPST Slide 6.73mm 264mil SMD LowProfile JPin
0
8
8
Buttons_Switches_SMD
SW_DIP_SPSTx04_Slide_6.7x11.72mm_W8.61mm_P2.54mm_LowProfile
SMD 4x-dip-switch SPST , Slide, row spacing 8.61 mm (338 mils), body size 6.7x11.72mm (see e.g. https://www.ctscorp.com/wp-content/uploads/219.pdf), SMD, LowProfile
SMD DIP Switch SPST Slide 8.61mm 338mil SMD LowProfile
0
8
8
Buttons_Switches_SMD
SW_DIP_SPSTx04_Slide_9.78x12.34mm_W8.61mm_P2.54mm
SMD 4x-dip-switch SPST , Slide, row spacing 8.61 mm (338 mils), body size 9.78x12.34mm (see e.g. https://www.ctscorp.com/wp-content/uploads/204.pdf), SMD
SMD DIP Switch SPST Slide 8.61mm 338mil SMD
0
8
8
Buttons_Switches_SMD
SW_DIP_SPSTx04_Slide_Copal_CHS-04A_W5.08mm_P1.27mm_JPin
SMD 4x-dip-switch SPST Copal_CHS-04A, Slide, row spacing 5.08 mm (200 mils), body size  (see http://www.nidec-copal-electronics.com/e/catalog/switch/chs.pdf), SMD, JPin
SMD DIP Switch SPST Slide 5.08mm 200mil SMD JPin
0
8
8
Buttons_Switches_SMD
SW_DIP_SPSTx04_Slide_Copal_CHS-04B_W7.62mm_P1.27mm
SMD 4x-dip-switch SPST Copal_CHS-04B, Slide, row spacing 7.62 mm (300 mils), body size  (see http://www.nidec-copal-electronics.com/e/catalog/switch/chs.pdf), SMD
SMD DIP Switch SPST Slide 7.62mm 300mil SMD
0
8
8
Buttons_Switches_SMD
SW_DIP_SPSTx04_Slide_Copal_CVS-04xB_W5.9mm_P1mm
SMD 4x-dip-switch SPST Copal_CVS-04xB, Slide, row spacing 5.9 mm (232 mils), body size  (see http://www.nidec-copal-electronics.com/e/catalog/switch/cvs.pdf)
SMD DIP Switch SPST Slide 5.9mm 232mil
0
12
9
Buttons_Switches_SMD
SW_DIP_SPSTx04_Slide_KingTek_DSHP04TJ_W5.25mm_P1.27mm_JPin
SMD 4x-dip-switch SPST KingTek_DSHP04TJ, Slide, row spacing 5.25 mm (206 mils), body size  (see http://www.kingtek.net.cn/pic/201601201446313350.pdf), JPin
SMD DIP Switch SPST Slide 5.25mm 206mil JPin
0
8
8
Buttons_Switches_SMD
SW_DIP_SPSTx04_Slide_KingTek_DSHP04TS_W7.62mm_P1.27mm
SMD 4x-dip-switch SPST KingTek_DSHP04TS, Slide, row spacing 7.62 mm (300 mils), body size  (see http://www.kingtek.net.cn/pic/201601201417455112.pdf)
SMD DIP Switch SPST Slide 7.62mm 300mil
0
8
8
Buttons_Switches_SMD
SW_DIP_SPSTx04_Slide_Omron_A6H-4101_W6.15mm_P1.27mm
SMD 4x-dip-switch SPST Omron_A6H-4101, Slide, row spacing 6.15 mm (242 mils), body size  (see https://www.omron.com/ecb/products/pdf/en-a6h.pdf)
SMD DIP Switch SPST Slide 6.15mm 242mil
0
8
8
Buttons_Switches_SMD
SW_DIP_SPSTx04_Slide_Omron_A6S-410x_W8.9mm_P2.54mm
SMD 4x-dip-switch SPST Omron_A6S-410x, Slide, row spacing 8.9 mm (350 mils), body size  (see http://omronfs.omron.com/en_US/ecb/products/pdf/en-a6s.pdf)
SMD DIP Switch SPST Slide 8.9mm 350mil
0
8
8
Buttons_Switches_SMD
SW_DIP_SPSTx05_Slide_6.7x14.26mm_W6.73mm_P2.54mm_LowProfile_JPin
SMD 5x-dip-switch SPST , Slide, row spacing 6.73 mm (264 mils), body size 6.7x14.26mm (see e.g. https://www.ctscorp.com/wp-content/uploads/219.pdf), SMD, LowProfile, JPin
SMD DIP Switch SPST Slide 6.73mm 264mil SMD LowProfile JPin
0
10
10
Buttons_Switches_SMD
SW_DIP_SPSTx05_Slide_6.7x14.26mm_W8.61mm_P2.54mm_LowProfile
SMD 5x-dip-switch SPST , Slide, row spacing 8.61 mm (338 mils), body size 6.7x14.26mm (see e.g. https://www.ctscorp.com/wp-content/uploads/219.pdf), SMD, LowProfile
SMD DIP Switch SPST Slide 8.61mm 338mil SMD LowProfile
0
10
10
Buttons_Switches_SMD
SW_DIP_SPSTx05_Slide_9.78x14.88mm_W8.61mm_P2.54mm
SMD 5x-dip-switch SPST , Slide, row spacing 8.61 mm (338 mils), body size 9.78x14.88mm (see e.g. https://www.ctscorp.com/wp-content/uploads/204.pdf), SMD
SMD DIP Switch SPST Slide 8.61mm 338mil SMD
0
10
10
Buttons_Switches_SMD
SW_DIP_SPSTx05_Slide_KingTek_DSHP05TJ_W5.25mm_P1.27mm_JPin
SMD 5x-dip-switch SPST KingTek_DSHP05TJ, Slide, row spacing 5.25 mm (206 mils), body size  (see http://www.kingtek.net.cn/pic/201601201446313350.pdf), JPin
SMD DIP Switch SPST Slide 5.25mm 206mil JPin
0
10
10
Buttons_Switches_SMD
SW_DIP_SPSTx05_Slide_KingTek_DSHP05TS_W7.62mm_P1.27mm
SMD 5x-dip-switch SPST KingTek_DSHP05TS, Slide, row spacing 7.62 mm (300 mils), body size  (see http://www.kingtek.net.cn/pic/201601201417455112.pdf)
SMD DIP Switch SPST Slide 7.62mm 300mil
0
10
10
Buttons_Switches_SMD
SW_DIP_SPSTx05_Slide_Omron_A6S-510x_W8.9mm_P2.54mm
SMD 5x-dip-switch SPST Omron_A6S-510x, Slide, row spacing 8.9 mm (350 mils), body size  (see http://omronfs.omron.com/en_US/ecb/products/pdf/en-a6s.pdf)
SMD DIP Switch SPST Slide 8.9mm 350mil
0
10
10
Buttons_Switches_SMD
SW_DIP_SPSTx06_Slide_6.7x16.8mm_W6.73mm_P2.54mm_LowProfile_JPin
SMD 6x-dip-switch SPST , Slide, row spacing 6.73 mm (264 mils), body size 6.7x16.8mm (see e.g. https://www.ctscorp.com/wp-content/uploads/219.pdf), SMD, LowProfile, JPin
SMD DIP Switch SPST Slide 6.73mm 264mil SMD LowProfile JPin
0
12
12
Buttons_Switches_SMD
SW_DIP_SPSTx06_Slide_6.7x16.8mm_W8.61mm_P2.54mm_LowProfile
SMD 6x-dip-switch SPST , Slide, row spacing 8.61 mm (338 mils), body size 6.7x16.8mm (see e.g. https://www.ctscorp.com/wp-content/uploads/219.pdf), SMD, LowProfile
SMD DIP Switch SPST Slide 8.61mm 338mil SMD LowProfile
0
12
12
Buttons_Switches_SMD
SW_DIP_SPSTx06_Slide_9.78x17.42mm_W8.61mm_P2.54mm
SMD 6x-dip-switch SPST , Slide, row spacing 8.61 mm (338 mils), body size 9.78x17.42mm (see e.g. https://www.ctscorp.com/wp-content/uploads/204.pdf), SMD
SMD DIP Switch SPST Slide 8.61mm 338mil SMD
0
12
12
Buttons_Switches_SMD
SW_DIP_SPSTx06_Slide_Copal_CHS-06A_W5.08mm_P1.27mm_JPin
SMD 6x-dip-switch SPST Copal_CHS-06A, Slide, row spacing 5.08 mm (200 mils), body size  (see http://www.nidec-copal-electronics.com/e/catalog/switch/chs.pdf), SMD, JPin
SMD DIP Switch SPST Slide 5.08mm 200mil SMD JPin
0
12
12
Buttons_Switches_SMD
SW_DIP_SPSTx06_Slide_Copal_CHS-06B_W7.62mm_P1.27mm
SMD 6x-dip-switch SPST Copal_CHS-06B, Slide, row spacing 7.62 mm (300 mils), body size  (see http://www.nidec-copal-electronics.com/e/catalog/switch/chs.pdf), SMD
SMD DIP Switch SPST Slide 7.62mm 300mil SMD
0
12
12
Buttons_Switches_SMD
SW_DIP_SPSTx06_Slide_KingTek_DSHP06TJ_W5.25mm_P1.27mm_JPin
SMD 6x-dip-switch SPST KingTek_DSHP06TJ, Slide, row spacing 5.25 mm (206 mils), body size  (see http://www.kingtek.net.cn/pic/201601201446313350.pdf), JPin
SMD DIP Switch SPST Slide 5.25mm 206mil JPin
0
12
12
Buttons_Switches_SMD
SW_DIP_SPSTx06_Slide_KingTek_DSHP06TS_W7.62mm_P1.27mm
SMD 6x-dip-switch SPST KingTek_DSHP06TS, Slide, row spacing 7.62 mm (300 mils), body size  (see http://www.kingtek.net.cn/pic/201601201417455112.pdf)
SMD DIP Switch SPST Slide 7.62mm 300mil
0
12
12
Buttons_Switches_SMD
SW_DIP_SPSTx06_Slide_Omron_A6H-6101_W6.15mm_P1.27mm
SMD 6x-dip-switch SPST Omron_A6H-6101, Slide, row spacing 6.15 mm (242 mils), body size  (see https://www.omron.com/ecb/products/pdf/en-a6h.pdf)
SMD DIP Switch SPST Slide 6.15mm 242mil
0
12
12
Buttons_Switches_SMD
SW_DIP_SPSTx06_Slide_Omron_A6S-610x_W8.9mm_P2.54mm
SMD 6x-dip-switch SPST Omron_A6S-610x, Slide, row spacing 8.9 mm (350 mils), body size  (see http://omronfs.omron.com/en_US/ecb/products/pdf/en-a6s.pdf)
SMD DIP Switch SPST Slide 8.9mm 350mil
0
12
12
Buttons_Switches_SMD
SW_DIP_SPSTx07_Slide_6.7x19.34mm_W6.73mm_P2.54mm_LowProfile_JPin
SMD 7x-dip-switch SPST , Slide, row spacing 6.73 mm (264 mils), body size 6.7x19.34mm (see e.g. https://www.ctscorp.com/wp-content/uploads/219.pdf), SMD, LowProfile, JPin
SMD DIP Switch SPST Slide 6.73mm 264mil SMD LowProfile JPin
0
14
14
Buttons_Switches_SMD
SW_DIP_SPSTx07_Slide_6.7x19.34mm_W8.61mm_P2.54mm_LowProfile
SMD 7x-dip-switch SPST , Slide, row spacing 8.61 mm (338 mils), body size 6.7x19.34mm (see e.g. https://www.ctscorp.com/wp-content/uploads/219.pdf), SMD, LowProfile
SMD DIP Switch SPST Slide 8.61mm 338mil SMD LowProfile
0
14
14
Buttons_Switches_SMD
SW_DIP_SPSTx07_Slide_9.78x19.96mm_W8.61mm_P2.54mm
SMD 7x-dip-switch SPST , Slide, row spacing 8.61 mm (338 mils), body size 9.78x19.96mm (see e.g. https://www.ctscorp.com/wp-content/uploads/204.pdf), SMD
SMD DIP Switch SPST Slide 8.61mm 338mil SMD
0
14
14
Buttons_Switches_SMD
SW_DIP_SPSTx07_Slide_KingTek_DSHP07TJ_W5.25mm_P1.27mm_JPin
SMD 7x-dip-switch SPST KingTek_DSHP07TJ, Slide, row spacing 5.25 mm (206 mils), body size  (see http://www.kingtek.net.cn/pic/201601201446313350.pdf), JPin
SMD DIP Switch SPST Slide 5.25mm 206mil JPin
0
14
14
Buttons_Switches_SMD
SW_DIP_SPSTx07_Slide_KingTek_DSHP07TS_W7.62mm_P1.27mm
SMD 7x-dip-switch SPST KingTek_DSHP07TS, Slide, row spacing 7.62 mm (300 mils), body size  (see http://www.kingtek.net.cn/pic/201601201417455112.pdf)
SMD DIP Switch SPST Slide 7.62mm 300mil
0
14
14
Buttons_Switches_SMD
SW_DIP_SPSTx07_Slide_Omron_A6S-710x_W8.9mm_P2.54mm
SMD 7x-dip-switch SPST Omron_A6S-710x, Slide, row spacing 8.9 mm (350 mils), body size  (see http://omronfs.omron.com/en_US/ecb/products/pdf/en-a6s.pdf)
SMD DIP Switch SPST Slide 8.9mm 350mil
0
14
14
Buttons_Switches_SMD
SW_DIP_SPSTx08_Slide_6.7x21.88mm_W6.73mm_P2.54mm_LowProfile_JPin
SMD 8x-dip-switch SPST , Slide, row spacing 6.73 mm (264 mils), body size 6.7x21.88mm (see e.g. https://www.ctscorp.com/wp-content/uploads/219.pdf), SMD, LowProfile, JPin
SMD DIP Switch SPST Slide 6.73mm 264mil SMD LowProfile JPin
0
16
16
Buttons_Switches_SMD
SW_DIP_SPSTx08_Slide_6.7x21.88mm_W8.61mm_P2.54mm_LowProfile
SMD 8x-dip-switch SPST , Slide, row spacing 8.61 mm (338 mils), body size 6.7x21.88mm (see e.g. https://www.ctscorp.com/wp-content/uploads/219.pdf), SMD, LowProfile
SMD DIP Switch SPST Slide 8.61mm 338mil SMD LowProfile
0
16
16
Buttons_Switches_SMD
SW_DIP_SPSTx08_Slide_9.78x22.5mm_W8.61mm_P2.54mm
SMD 8x-dip-switch SPST , Slide, row spacing 8.61 mm (338 mils), body size 9.78x22.5mm (see e.g. https://www.ctscorp.com/wp-content/uploads/204.pdf), SMD
SMD DIP Switch SPST Slide 8.61mm 338mil SMD
0
16
16
Buttons_Switches_SMD
SW_DIP_SPSTx08_Slide_Copal_CHS-08A_W5.08mm_P1.27mm_JPin
SMD 8x-dip-switch SPST Copal_CHS-08A, Slide, row spacing 5.08 mm (200 mils), body size  (see http://www.nidec-copal-electronics.com/e/catalog/switch/chs.pdf), SMD, JPin
SMD DIP Switch SPST Slide 5.08mm 200mil SMD JPin
0
16
16
Buttons_Switches_SMD
SW_DIP_SPSTx08_Slide_Copal_CHS-08B_W7.62mm_P1.27mm
SMD 8x-dip-switch SPST Copal_CHS-08B, Slide, row spacing 7.62 mm (300 mils), body size  (see http://www.nidec-copal-electronics.com/e/catalog/switch/chs.pdf), SMD
SMD DIP Switch SPST Slide 7.62mm 300mil SMD
0
16
16
Buttons_Switches_SMD
SW_DIP_SPSTx08_Slide_Copal_CVS-08xB_W5.9mm_P1mm
SMD 8x-dip-switch SPST Copal_CVS-08xB, Slide, row spacing 5.9 mm (232 mils), body size  (see http://www.nidec-copal-electronics.com/e/catalog/switch/cvs.pdf)
SMD DIP Switch SPST Slide 5.9mm 232mil
0
20
17
Buttons_Switches_SMD
SW_DIP_SPSTx08_Slide_KingTek_DSHP08TJ_W5.25mm_P1.27mm_JPin
SMD 8x-dip-switch SPST KingTek_DSHP08TJ, Slide, row spacing 5.25 mm (206 mils), body size  (see http://www.kingtek.net.cn/pic/201601201446313350.pdf), JPin
SMD DIP Switch SPST Slide 5.25mm 206mil JPin
0
16
16
Buttons_Switches_SMD
SW_DIP_SPSTx08_Slide_KingTek_DSHP08TS_W7.62mm_P1.27mm
SMD 8x-dip-switch SPST KingTek_DSHP08TS, Slide, row spacing 7.62 mm (300 mils), body size  (see http://www.kingtek.net.cn/pic/201601201417455112.pdf)
SMD DIP Switch SPST Slide 7.62mm 300mil
0
16
16
Buttons_Switches_SMD
SW_DIP_SPSTx08_Slide_Omron_A6H-8101_W6.15mm_P1.27mm
SMD 8x-dip-switch SPST Omron_A6H-8101, Slide, row spacing 6.15 mm (242 mils), body size  (see https://www.omron.com/ecb/products/pdf/en-a6h.pdf)
SMD DIP Switch SPST Slide 6.15mm 242mil
0
16
16
Buttons_Switches_SMD
SW_DIP_SPSTx08_Slide_Omron_A6S-810x_W8.9mm_P2.54mm
SMD 8x-dip-switch SPST Omron_A6S-810x, Slide, row spacing 8.9 mm (350 mils), body size  (see http://omronfs.omron.com/en_US/ecb/products/pdf/en-a6s.pdf)
SMD DIP Switch SPST Slide 8.9mm 350mil
0
16
16
Buttons_Switches_SMD
SW_DIP_SPSTx09_Slide_6.7x24.42mm_W6.73mm_P2.54mm_LowProfile_JPin
SMD 9x-dip-switch SPST , Slide, row spacing 6.73 mm (264 mils), body size 6.7x24.42mm (see e.g. https://www.ctscorp.com/wp-content/uploads/219.pdf), SMD, LowProfile, JPin
SMD DIP Switch SPST Slide 6.73mm 264mil SMD LowProfile JPin
0
18
18
Buttons_Switches_SMD
SW_DIP_SPSTx09_Slide_6.7x24.42mm_W8.61mm_P2.54mm_LowProfile
SMD 9x-dip-switch SPST , Slide, row spacing 8.61 mm (338 mils), body size 6.7x24.42mm (see e.g. https://www.ctscorp.com/wp-content/uploads/219.pdf), SMD, LowProfile
SMD DIP Switch SPST Slide 8.61mm 338mil SMD LowProfile
0
18
18
Buttons_Switches_SMD
SW_DIP_SPSTx09_Slide_9.78x25.04mm_W8.61mm_P2.54mm
SMD 9x-dip-switch SPST , Slide, row spacing 8.61 mm (338 mils), body size 9.78x25.04mm (see e.g. https://www.ctscorp.com/wp-content/uploads/204.pdf), SMD
SMD DIP Switch SPST Slide 8.61mm 338mil SMD
0
18
18
Buttons_Switches_SMD
SW_DIP_SPSTx09_Slide_KingTek_DSHP09TJ_W5.25mm_P1.27mm_JPin
SMD 9x-dip-switch SPST KingTek_DSHP09TJ, Slide, row spacing 5.25 mm (206 mils), body size  (see http://www.kingtek.net.cn/pic/201601201446313350.pdf), JPin
SMD DIP Switch SPST Slide 5.25mm 206mil JPin
0
18
18
Buttons_Switches_SMD
SW_DIP_SPSTx09_Slide_KingTek_DSHP09TS_W7.62mm_P1.27mm
SMD 9x-dip-switch SPST KingTek_DSHP09TS, Slide, row spacing 7.62 mm (300 mils), body size  (see http://www.kingtek.net.cn/pic/201601201417455112.pdf)
SMD DIP Switch SPST Slide 7.62mm 300mil
0
18
18
Buttons_Switches_SMD
SW_DIP_SPSTx09_Slide_Omron_A6S-910x_W8.9mm_P2.54mm
SMD 9x-dip-switch SPST Omron_A6S-910x, Slide, row spacing 8.9 mm (350 mils), body size  (see http://omronfs.omron.com/en_US/ecb/products/pdf/en-a6s.pdf)
SMD DIP Switch SPST Slide 8.9mm 350mil
0
18
18
Buttons_Switches_SMD
SW_DIP_SPSTx10_Slide_6.7x26.96mm_W6.73mm_P2.54mm_LowProfile_JPin
SMD 10x-dip-switch SPST , Slide, row spacing 6.73 mm (264 mils), body size 6.7x26.96mm (see e.g. https://www.ctscorp.com/wp-content/uploads/219.pdf), SMD, LowProfile, JPin
SMD DIP Switch SPST Slide 6.73mm 264mil SMD LowProfile JPin
0
20
20
Buttons_Switches_SMD
SW_DIP_SPSTx10_Slide_6.7x26.96mm_W8.61mm_P2.54mm_LowProfile
SMD 10x-dip-switch SPST , Slide, row spacing 8.61 mm (338 mils), body size 6.7x26.96mm (see e.g. https://www.ctscorp.com/wp-content/uploads/219.pdf), SMD, LowProfile
SMD DIP Switch SPST Slide 8.61mm 338mil SMD LowProfile
0
20
20
Buttons_Switches_SMD
SW_DIP_SPSTx10_Slide_9.78x27.58mm_W8.61mm_P2.54mm
SMD 10x-dip-switch SPST , Slide, row spacing 8.61 mm (338 mils), body size 9.78x27.58mm (see e.g. https://www.ctscorp.com/wp-content/uploads/204.pdf), SMD
SMD DIP Switch SPST Slide 8.61mm 338mil SMD
0
20
20
Buttons_Switches_SMD
SW_DIP_SPSTx10_Slide_Copal_CHS-10A_W5.08mm_P1.27mm_JPin
SMD 10x-dip-switch SPST Copal_CHS-10A, Slide, row spacing 5.08 mm (200 mils), body size  (see http://www.nidec-copal-electronics.com/e/catalog/switch/chs.pdf), SMD, JPin
SMD DIP Switch SPST Slide 5.08mm 200mil SMD JPin
0
20
20
Buttons_Switches_SMD
SW_DIP_SPSTx10_Slide_Copal_CHS-10B_W7.62mm_P1.27mm
SMD 10x-dip-switch SPST Copal_CHS-10B, Slide, row spacing 7.62 mm (300 mils), body size  (see http://www.nidec-copal-electronics.com/e/catalog/switch/chs.pdf), SMD
SMD DIP Switch SPST Slide 7.62mm 300mil SMD
0
20
20
Buttons_Switches_SMD
SW_DIP_SPSTx10_Slide_KingTek_DSHP10TJ_W5.25mm_P1.27mm_JPin
SMD 10x-dip-switch SPST KingTek_DSHP10TJ, Slide, row spacing 5.25 mm (206 mils), body size  (see http://www.kingtek.net.cn/pic/201601201446313350.pdf), JPin
SMD DIP Switch SPST Slide 5.25mm 206mil JPin
0
20
20
Buttons_Switches_SMD
SW_DIP_SPSTx10_Slide_KingTek_DSHP10TS_W7.62mm_P1.27mm
SMD 10x-dip-switch SPST KingTek_DSHP10TS, Slide, row spacing 7.62 mm (300 mils), body size  (see http://www.kingtek.net.cn/pic/201601201417455112.pdf)
SMD DIP Switch SPST Slide 7.62mm 300mil
0
20
20
Buttons_Switches_SMD
SW_DIP_SPSTx10_Slide_Omron_A6H-10101_W6.15mm_P1.27mm
SMD 10x-dip-switch SPST Omron_A6H-10101, Slide, row spacing 6.15 mm (242 mils), body size  (see https://www.omron.com/ecb/products/pdf/en-a6h.pdf)
SMD DIP Switch SPST Slide 6.15mm 242mil
0
20
20
Buttons_Switches_SMD
SW_DIP_SPSTx10_Slide_Omron_A6S-1010x_W8.9mm_P2.54mm
SMD 10x-dip-switch SPST Omron_A6S-1010x, Slide, row spacing 8.9 mm (350 mils), body size  (see http://omronfs.omron.com/en_US/ecb/products/pdf/en-a6s.pdf)
SMD DIP Switch SPST Slide 8.9mm 350mil
0
20
20
Buttons_Switches_SMD
SW_DIP_SPSTx11_Slide_6.7x29.5mm_W6.73mm_P2.54mm_LowProfile_JPin
SMD 11x-dip-switch SPST , Slide, row spacing 6.73 mm (264 mils), body size 6.7x29.5mm (see e.g. https://www.ctscorp.com/wp-content/uploads/219.pdf), SMD, LowProfile, JPin
SMD DIP Switch SPST Slide 6.73mm 264mil SMD LowProfile JPin
0
22
22
Buttons_Switches_SMD
SW_DIP_SPSTx11_Slide_6.7x29.5mm_W8.61mm_P2.54mm_LowProfile
SMD 11x-dip-switch SPST , Slide, row spacing 8.61 mm (338 mils), body size 6.7x29.5mm (see e.g. https://www.ctscorp.com/wp-content/uploads/219.pdf), SMD, LowProfile
SMD DIP Switch SPST Slide 8.61mm 338mil SMD LowProfile
0
22
22
Buttons_Switches_SMD
SW_DIP_SPSTx11_Slide_9.78x30.12mm_W8.61mm_P2.54mm
SMD 11x-dip-switch SPST , Slide, row spacing 8.61 mm (338 mils), body size 9.78x30.12mm (see e.g. https://www.ctscorp.com/wp-content/uploads/204.pdf), SMD
SMD DIP Switch SPST Slide 8.61mm 338mil SMD
0
22
22
Buttons_Switches_SMD
SW_DIP_SPSTx12_Slide_6.7x32.04mm_W6.73mm_P2.54mm_LowProfile_JPin
SMD 12x-dip-switch SPST , Slide, row spacing 6.73 mm (264 mils), body size 6.7x32.04mm (see e.g. https://www.ctscorp.com/wp-content/uploads/219.pdf), SMD, LowProfile, JPin
SMD DIP Switch SPST Slide 6.73mm 264mil SMD LowProfile JPin
0
24
24
Buttons_Switches_SMD
SW_DIP_SPSTx12_Slide_6.7x32.04mm_W8.61mm_P2.54mm_LowProfile
SMD 12x-dip-switch SPST , Slide, row spacing 8.61 mm (338 mils), body size 6.7x32.04mm (see e.g. https://www.ctscorp.com/wp-content/uploads/219.pdf), SMD, LowProfile
SMD DIP Switch SPST Slide 8.61mm 338mil SMD LowProfile
0
24
24
Buttons_Switches_SMD
SW_DIP_SPSTx12_Slide_9.78x32.66mm_W8.61mm_P2.54mm
SMD 12x-dip-switch SPST , Slide, row spacing 8.61 mm (338 mils), body size 9.78x32.66mm (see e.g. https://www.ctscorp.com/wp-content/uploads/204.pdf), SMD
SMD DIP Switch SPST Slide 8.61mm 338mil SMD
0
24
24
Buttons_Switches_SMD
SW_MEC_5GSH9
MEC 5G single pole normally-open tactile switch
switch normally-open pushbutton push-button
0
4
4
Buttons_Switches_SMD
SW_Push_1P1T-MP_NO_Horizontal_Alps_SKRTLAE010
Side push button (https://www.alps.com/prod/info/E/PDF/Tact/SurfaceMount/SKRT/SKRT.pdf)
push horizontal SPST 1P1T
0
5
3
Buttons_Switches_SMD
SW_Push_1P1T-SH_NO_CK_KMR2xxG
CK components KMR2 tactile switch with ground pin http://www.ckswitches.com/media/1479/kmr2.pdf
tactile switch kmr2
0
5
3
Buttons_Switches_SMD
SW_Push_1P1T_NO_6x6mm_H9.5mm
tactile push button, 6x6mm e.g. PTS645xx series, height=9.5mm
tact sw push 6mm smd
0
4
2
Buttons_Switches_SMD
SW_Push_1P1T_NO_CK_KMR2
CK components KMR2 tactile switch http://www.ckswitches.com/media/1479/kmr2.pdf
tactile switch kmr2
0
4
2
Buttons_Switches_SMD
SW_Push_1P1T_NO_CK_KSC6xxJ
CK components KSC6 tactile switch https://www.ckswitches.com/media/1972/ksc6.pdf
tactile switch ksc6
0
4
2
Buttons_Switches_SMD
SW_Push_1P1T_NO_CK_KSC7xxJ
CK components KSC7 tactile switch https://www.ckswitches.com/media/1973/ksc7.pdf
tactile switch ksc7
0
4
2
Buttons_Switches_SMD
SW_Push_1P1T_NO_CK_PTS125Sx43PSMTR
C&K Switches 1P1T SMD PTS125 Series 12mm Tact Switch with Pegs, https://www.ckswitches.com/media/1462/pts125.pdf
Button Tactile Switch SPST 1P1T
0
4
2
Buttons_Switches_SMD
SW_Push_1P1T_NO_Vertical_Wuerth_434133025816
https://katalog.we-online.com/em/datasheet/434133025816.pdf
tactile switch Wurth Wuerth
0
4
2
Buttons_Switches_SMD
SW_Push_SPST_NO_Alps_SKRK
http://www.alps.com/prod/info/E/HTML/Tact/SurfaceMount/SKRK/SKRKAHE020.html
SMD SMT button
0
2
2
Buttons_Switches_SMD
SW_SP3T_PCM13
Ultraminiature Surface Mount Slide Switch, right-angle, https://www.ckswitches.com/media/1424/pcm.pdf

0
8
4
Buttons_Switches_SMD
SW_SPDT_CK-JS102011SAQN
Sub-miniature slide switch, right-angle, http://www.ckswitches.com/media/1422/js.pdf
switch spdt
0
3
3
Buttons_Switches_SMD
SW_SPDT_PCM12
Ultraminiature Surface Mount Slide Switch, right-angle, https://www.ckswitches.com/media/1424/pcm.pdf

0
7
3
Buttons_Switches_SMD
SW_SPST_B3S-1000
Surface Mount Tactile Switch for High-Density Packaging
Tactile Switch
0
4
2
Buttons_Switches_SMD
SW_SPST_B3S-1100
Surface Mount Tactile Switch for High-Density Packaging with Ground Terminal
Tactile Switch
0
5
3
Buttons_Switches_SMD
SW_SPST_B3SL-1002P
Middle Stroke Tactile Switch, B3SL
Middle Stroke Tactile Switch
0
4
2
Buttons_Switches_SMD
SW_SPST_B3SL-1022P
Middle Stroke Tactile Switch, B3SL
Middle Stroke Tactile Switch
0
4
2
Buttons_Switches_SMD
SW_SPST_B3U-1000P
Ultra-small-sized Tactile Switch with High Contact Reliability, Top-actuated Model, without Ground Terminal, without Boss
Tactile Switch
0
2
2
Buttons_Switches_SMD
SW_SPST_B3U-1000P-B
Ultra-small-sized Tactile Switch with High Contact Reliability, Top-actuated Model, without Ground Terminal, with Boss
Tactile Switch
0
2
2
Buttons_Switches_SMD
SW_SPST_B3U-1100P
Ultra-small-sized Tactile Switch with High Contact Reliability, Top-actuated Model, with Ground Terminal, without Boss
Tactile Switch
0
3
3
Buttons_Switches_SMD
SW_SPST_B3U-1100P-B
Ultra-small-sized Tactile Switch with High Contact Reliability, Top-actuated Model, with Ground Terminal, with Boss
Tactile Switch
0
3
3
Buttons_Switches_SMD
SW_SPST_B3U-3000P
Ultra-small-sized Tactile Switch with High Contact Reliability, Side-actuated Model, without Ground Terminal, without Boss
Tactile Switch
0
2
2
Buttons_Switches_SMD
SW_SPST_B3U-3000P-B
Ultra-small-sized Tactile Switch with High Contact Reliability, Side-actuated Model, without Ground Terminal, with Boss
Tactile Switch
0
2
2
Buttons_Switches_SMD
SW_SPST_B3U-3100P
Ultra-small-sized Tactile Switch with High Contact Reliability, Side-actuated Model, with Ground Terminal, without Boss
Tactile Switch
0
3
3
Buttons_Switches_SMD
SW_SPST_B3U-3100P-B
Ultra-small-sized Tactile Switch with High Contact Reliability, Side-actuated Model, with Ground Terminal, with Boss
Tactile Switch
0
3
3
Buttons_Switches_SMD
SW_SPST_CK_KXT3
https://www.ckswitches.com/media/1465/kxt3.pdf
Switch SPST KXT3
0
2
2
Buttons_Switches_SMD
SW_SPST_CK_RS282G05A3
https://www.mouser.com/ds/2/60/RS-282G05A-SM_RT-1159762.pdf
SPST button tactile switch
0
2
2
Buttons_Switches_SMD
SW_SPST_EVPBF
Light Touch Switch

0
4
2
Buttons_Switches_SMD
SW_SPST_EVQP0
Light Touch Switch, https://industrial.panasonic.com/cdbs/www-data/pdf/ATK0000/ATK0000CE28.pdf

0
4
2
Buttons_Switches_SMD
SW_SPST_EVQP2
Light Touch Switch

0
4
2
Buttons_Switches_SMD
SW_SPST_EVQP7A
Light Touch Switch,https://industrial.panasonic.com/cdbs/www-data/pdf/ATK0000/ATK0000CE20.pdf

0
4
2
Buttons_Switches_SMD
SW_SPST_EVQP7C
Light Touch Switch

0
4
2
Buttons_Switches_SMD
SW_SPST_EVQPE1
Light Touch Switch, https://industrial.panasonic.com/cdbs/www-data/pdf/ATK0000/ATK0000CE7.pdf

0
2
2
Buttons_Switches_SMD
SW_SPST_EVQQ2
Light Touch Switch, https://industrial.panasonic.com/cdbs/www-data/pdf/ATK0000/ATK0000CE28.pdf

0
4
2
Buttons_Switches_SMD
SW_SPST_FSMSM
http://www.te.com/commerce/DocumentDelivery/DDEController?Action=srchrtrv&DocNm=1437566-3&DocType=Customer+Drawing&DocLang=English
SPST button tactile switch
0
2
2
Buttons_Switches_SMD
SW_SPST_PTS645
C&K Components SPST SMD PTS645 Series 6mm Tact Switch
SPST Button Switch
0
4
2
Buttons_Switches_SMD
SW_SPST_PTS810
C&K Components, PTS 810 Series, Microminiature SMT Top Actuated, http://www.ckswitches.com/media/1476/pts810.pdf
SPST Button Switch
0
4
2
Buttons_Switches_SMD
SW_SPST_Panasonic_EVQPL_3PL_5PL_PT_A08
Light Touch Switch, http://industrial.panasonic.com/cdbs/www-data/pdf/ATK0000/ATK0000CE3.pdf
SMD SMT SPST EVQPL EVQPT
0
6
3
Buttons_Switches_SMD
SW_SPST_Panasonic_EVQPL_3PL_5PL_PT_A15
Light Touch Switch, http://industrial.panasonic.com/cdbs/www-data/pdf/ATK0000/ATK0000CE3.pdf
SMD SMT SPST EVQPL EVQPT
0
6
3
Buttons_Switches_SMD
SW_SPST_REED_CT05-XXXX-G1
Coto Technologies SPST Reed Switch CT05-XXXX-G1
Coto Reed SPST Switch
0
2
2
Buttons_Switches_SMD
SW_SPST_REED_CT05-XXXX-J1
Coto Technologies SPST Reed Switch CT05-XXXX-J1
Coto Reed SPST Switch
0
2
2
Buttons_Switches_SMD
SW_SPST_REED_CT10-XXXX-G1
Coto Technologies SPST Reed Switch CT10-XXXX-G1
Coto Reed SPST Switch
0
2
2
Buttons_Switches_SMD
SW_SPST_REED_CT10-XXXX-G2
Coto Technologies SPST Reed Switch CT10-XXXX-G2
Coto Reed SPST Switch
0
2
2
Buttons_Switches_SMD
SW_SPST_REED_CT10-XXXX-G4
Coto Technologies SPST Reed Switch CT10-XXXX-G4
Coto Reed SPST Switch
0
2
2
Buttons_Switches_SMD
SW_SPST_SKQG_WithStem
ALPS 5.2mm Square Low-profile Type (Surface Mount) SKQG Series, With stem, http://www.alps.com/prod/info/E/HTML/Tact/SurfaceMount/SKQG/SKQGAFE010.html
SPST Button Switch
0
4
2
Buttons_Switches_SMD
SW_SPST_SKQG_WithoutStem
ALPS 5.2mm Square Low-profile Type (Surface Mount) SKQG Series, Without stem, http://www.alps.com/prod/info/E/HTML/Tact/SurfaceMount/SKQG/SKQGAEE010.html
SPST Button Switch
0
4
2
Buttons_Switches_SMD
SW_SPST_TL3305A
https://www.e-switch.com/system/asset/product_line/data_sheet/213/TL3305.pdf
TL3305 Series Tact Switch
0
4
2
Buttons_Switches_SMD
SW_SPST_TL3305B
https://www.e-switch.com/system/asset/product_line/data_sheet/213/TL3305.pdf
TL3305 Series Tact Switch
0
4
2
Buttons_Switches_SMD
SW_SPST_TL3305C
https://www.e-switch.com/system/asset/product_line/data_sheet/213/TL3305.pdf
TL3305 Series Tact Switch
0
4
2
Buttons_Switches_SMD
SW_SPST_TL3342
Low-profile SMD Tactile Switch, https://www.e-switch.com/system/asset/product_line/data_sheet/165/TL3342.pdf
SPST Tactile Switch
0
4
2
Buzzer_Beeper
Buzzer_12x9.5RM7.6
Generic Buzzer, D12mm height 9.5mm with RM7.6mm
buzzer
0
2
2
Buzzer_Beeper
Buzzer_15x7.5RM7.6
Generic Buzzer, D15mm height 7.5mm with RM7.6mm
buzzer
0
2
2
Buzzer_Beeper
Buzzer_CUI_CPT-9019S-SMT
https://www.cui.com/product/resource/cpt-9019s-smt.pdf
buzzer piezo
0
2
2
Buzzer_Beeper
Buzzer_D14mm_H7mm_P10mm
Generic Buzzer, D14mm height 7mm with pitch 10mm
buzzer
0
2
2
Buzzer_Beeper
Buzzer_Mallory_AST1109MLTRQ
Mallory low-profile piezo buzzer, https://www.mspindy.com/specifications/AST1109MLTRQ.pdf
buzzer piezo
0
2
2
Buzzer_Beeper
Buzzer_Murata_PKMCS0909E4000-R1
Murata Buzzer http://www.murata.com/en-us/api/pdfdownloadapi?cate=&partno=PKMCS0909E4000-R1
Murata Buzzer Beeper
0
2
2
Buzzer_Beeper
Buzzer_TDK_PS1240P02BT_D12.2mm_H6.5mm
Buzzer, D12.2mm height 6.5mm, https://product.tdk.com/info/en/catalog/datasheets/piezoelectronic_buzzer_ps_en.pdf
buzzer
0
2
2
Buzzer_Beeper
MagneticBuzzer_CUI_CST-931RP-A
CST-931RP-A, http://www.cui.com/product/resource/cst-931rp-a.pdf
CST-931RP-A
0
2
2
Buzzer_Beeper
MagneticBuzzer_Kingstate_KCG0601
Buzzer, Elektromagnetic Beeper, Summer,
Kingstate KCG0601 
0
2
2
Buzzer_Beeper
MagneticBuzzer_Kobitone_254-EMB84Q-RO
MagneticBuzzer Kobitone 254-EMB84Q-RO https://www.mouser.es/datasheet/2/209/KT-400385-1171904.pdf
MagneticBuzzer Kobitone 254-EMB84Q-RO
0
3
3
Buzzer_Beeper
MagneticBuzzer_PUI_AT-0927-TT-6-R
Buzzer Magnetic 9mm AT-0927-TT-6-R, http://www.puiaudio.com/pdf/AT-0927-TT-6-R.pdf
Buzzer Magnetic 9mm AT-0927-TT-6-R
0
2
2
Buzzer_Beeper
MagneticBuzzer_ProSignal_ABI-009-RC
Buzzer, Elektromagnetic Beeper, Summer, 6V-DC,
Pro Signal ABI-009-RC 
0
2
2
Buzzer_Beeper
MagneticBuzzer_ProSignal_ABI-010-RC
Buzzer, Elektromagnetic Beeper, Summer, 12V-DC,
Pro Signal ABI-010-RC 
0
2
2
Buzzer_Beeper
MagneticBuzzer_ProSignal_ABT-410-RC
Buzzer, Elektromagnetic Beeper, Summer, 1,5V-DC,
Pro Signal ABT-410-RC 
0
2
2
Buzzer_Beeper
MagneticBuzzer_ProjectsUnlimited_AI-4228-TWT-R
Buzzer, Elektromagnetic Beeper, Summer, 3-28V-DC, https://www.kynix.com/uploadfiles/pdf/AI-4228-TWT-R.pdf
Projects Unlimited AI-4228-TWT-R 
0
2
2
Buzzer_Beeper
MagneticBuzzer_StarMicronics_HMB-06_HMB-12
Buzzer, Elektromagnetic Beeper, Summer,
Star Micronics HMB-06 HMB-12
0
2
2
Buzzer_Beeper
PUIAudio_SMT_0825_S_4_R
SMD 8540, http://www.puiaudio.com/product-detail.aspx?partnumber=SMT-0825-S-4-R
SMD 8540
0
4
4
Capacitor_SMD
CP_Elec_3x5.3
SMT capacitor, aluminium electrolytic, 3x5.3, Cornell Dubilier Electronics 
Capacitor Electrolytic
0
2
2
Capacitor_SMD
CP_Elec_3x5.4
SMD capacitor, aluminum electrolytic, Nichicon, 3.0x5.4mm
capacitor electrolytic
0
2
2
Capacitor_SMD
CP_Elec_4x3
SMD capacitor, aluminum electrolytic, Nichicon, 4.0x3mm
capacitor electrolytic
0
2
2
Capacitor_SMD
CP_Elec_4x3.9
SMD capacitor, aluminum electrolytic, Nichicon, 4.0x3.9mm
capacitor electrolytic
0
2
2
Capacitor_SMD
CP_Elec_4x4.5
SMD capacitor, aluminum electrolytic, Nichicon, 4.0x4.5mm
capacitor electrolytic
0
2
2
Capacitor_SMD
CP_Elec_4x5.3
SMD capacitor, aluminum electrolytic, Vishay, 4.0x5.3mm
capacitor electrolytic
0
2
2
Capacitor_SMD
CP_Elec_4x5.4
SMD capacitor, aluminum electrolytic, Panasonic A5 / Nichicon, 4.0x5.4mm
capacitor electrolytic
0
2
2
Capacitor_SMD
CP_Elec_4x5.7
SMD capacitor, aluminum electrolytic, United Chemi-Con, 4.0x5.7mm
capacitor electrolytic
0
2
2
Capacitor_SMD
CP_Elec_4x5.8
SMD capacitor, aluminum electrolytic, Panasonic, 4.0x5.8mm
capacitor electrolytic
0
2
2
Capacitor_SMD
CP_Elec_5x3
SMD capacitor, aluminum electrolytic, Nichicon, 5.0x3.0mm
capacitor electrolytic
0
2
2
Capacitor_SMD
CP_Elec_5x3.9
SMD capacitor, aluminum electrolytic, Nichicon, 5.0x3.9mm
capacitor electrolytic
0
2
2
Capacitor_SMD
CP_Elec_5x4.4
SMD capacitor, aluminum electrolytic, Panasonic B45, 5.0x4.4mm
capacitor electrolytic
0
2
2
Capacitor_SMD
CP_Elec_5x4.5
SMD capacitor, aluminum electrolytic, Nichicon, 5.0x4.5mm
capacitor electrolytic
0
2
2
Capacitor_SMD
CP_Elec_5x5.3
SMD capacitor, aluminum electrolytic, Nichicon, 5.0x5.3mm
capacitor electrolytic
0
2
2
Capacitor_SMD
CP_Elec_5x5.4
SMD capacitor, aluminum electrolytic, Nichicon, 5.0x5.4mm
capacitor electrolytic
0
2
2
Capacitor_SMD
CP_Elec_5x5.7
SMD capacitor, aluminum electrolytic, United Chemi-Con, 5.0x5.7mm
capacitor electrolytic
0
2
2
Capacitor_SMD
CP_Elec_5x5.8
SMD capacitor, aluminum electrolytic, Panasonic, 5.0x5.8mm
capacitor electrolytic
0
2
2
Capacitor_SMD
CP_Elec_5x5.9
SMD capacitor, aluminum electrolytic, Panasonic B6, 5.0x5.9mm
capacitor electrolytic
0
2
2
Capacitor_SMD
CP_Elec_6.3x3
SMD capacitor, aluminum electrolytic, Nichicon, 6.3x3.0mm
capacitor electrolytic
0
2
2
Capacitor_SMD
CP_Elec_6.3x3.9
SMD capacitor, aluminum electrolytic, Nichicon, 6.3x3.9mm
capacitor electrolytic
0
2
2
Capacitor_SMD
CP_Elec_6.3x4.5
SMD capacitor, aluminum electrolytic, Nichicon, 6.3x4.5mm
capacitor electrolytic
0
2
2
Capacitor_SMD
CP_Elec_6.3x4.9
SMD capacitor, aluminum electrolytic, Panasonic C5, 6.3x4.9mm
capacitor electrolytic
0
2
2
Capacitor_SMD
CP_Elec_6.3x5.2
SMD capacitor, aluminum electrolytic, United Chemi-Con, 6.3x5.2mm
capacitor electrolytic
0
2
2
Capacitor_SMD
CP_Elec_6.3x5.3
SMD capacitor, aluminum electrolytic, Cornell Dubilier, 6.3x5.3mm
capacitor electrolytic
0
2
2
Capacitor_SMD
CP_Elec_6.3x5.4
SMD capacitor, aluminum electrolytic, Panasonic C55, 6.3x5.4mm
capacitor electrolytic
0
2
2
Capacitor_SMD
CP_Elec_6.3x5.4_Nichicon
SMD capacitor, aluminum electrolytic, Nichicon, 6.3x5.4mm
capacitor electrolytic
0
2
2
Capacitor_SMD
CP_Elec_6.3x5.7
SMD capacitor, aluminum electrolytic, United Chemi-Con, 6.3x5.7mm
capacitor electrolytic
0
2
2
Capacitor_SMD
CP_Elec_6.3x5.8
SMD capacitor, aluminum electrolytic, Nichicon, 6.3x5.8mm
capacitor electrolytic
0
2
2
Capacitor_SMD
CP_Elec_6.3x5.9
SMD capacitor, aluminum electrolytic, Panasonic C6, 6.3x5.9mm
capacitor electrolytic
0
2
2
Capacitor_SMD
CP_Elec_6.3x7.7
SMD capacitor, aluminum electrolytic, Nichicon, 6.3x7.7mm
capacitor electrolytic
0
2
2
Capacitor_SMD
CP_Elec_6.3x9.9
SMD capacitor, aluminum electrolytic, Panasonic C10, 6.3x9.9mm
capacitor electrolytic
0
2
2
Capacitor_SMD
CP_Elec_8x5.4
SMD capacitor, aluminum electrolytic, Nichicon, 8.0x5.4mm
capacitor electrolytic
0
2
2
Capacitor_SMD
CP_Elec_8x6.2
SMD capacitor, aluminum electrolytic, Nichicon, 8.0x6.2mm
capacitor electrolytic
0
2
2
Capacitor_SMD
CP_Elec_8x6.5
SMD capacitor, aluminum electrolytic, Rubycon, 8.0x6.5mm
capacitor electrolytic
0
2
2
Capacitor_SMD
CP_Elec_8x6.7
SMD capacitor, aluminum electrolytic, United Chemi-Con, 8.0x6.7mm
capacitor electrolytic
0
2
2
Capacitor_SMD
CP_Elec_8x6.9
SMD capacitor, aluminum electrolytic, Panasonic E7, 8.0x6.9mm
capacitor electrolytic
0
2
2
Capacitor_SMD
CP_Elec_8x10
SMD capacitor, aluminum electrolytic, Nichicon, 8.0x10mm
capacitor electrolytic
0
2
2
Capacitor_SMD
CP_Elec_8x10.5
SMD capacitor, aluminum electrolytic, Vishay 0810, 8.0x10.5mm, http://www.vishay.com/docs/28395/150crz.pdf
capacitor electrolytic
0
2
2
Capacitor_SMD
CP_Elec_8x11.9
SMD capacitor, aluminum electrolytic, Panasonic E12, 8.0x11.9mm
capacitor electrolytic
0
2
2
Capacitor_SMD
CP_Elec_10x7.7
SMD capacitor, aluminum electrolytic, Nichicon, 10.0x7.7mm
capacitor electrolytic
0
2
2
Capacitor_SMD
CP_Elec_10x7.9
SMD capacitor, aluminum electrolytic, Panasonic F8, 10.0x7.9mm
capacitor electrolytic
0
2
2
Capacitor_SMD
CP_Elec_10x10
SMD capacitor, aluminum electrolytic, Nichicon, 10.0x10.0mm
capacitor electrolytic
0
2
2
Capacitor_SMD
CP_Elec_10x10.5
SMD capacitor, aluminum electrolytic, Vishay 1010, 10.0x10.5mm, http://www.vishay.com/docs/28395/150crz.pdf
capacitor electrolytic
0
2
2
Capacitor_SMD
CP_Elec_10x12.5
SMD capacitor, aluminum electrolytic, Vishay 1012, 10.0x12.5mm, http://www.vishay.com/docs/28395/150crz.pdf
capacitor electrolytic
0
2
2
Capacitor_SMD
CP_Elec_10x12.6
SMD capacitor, aluminum electrolytic, Panasonic F12, 10.0x12.6mm
capacitor electrolytic
0
2
2
Capacitor_SMD
CP_Elec_10x14.3
SMD capacitor, aluminum electrolytic, Vishay 1014, 10.0x14.3mm, http://www.vishay.com/docs/28395/150crz.pdf
capacitor electrolytic
0
2
2
Capacitor_SMD
CP_Elec_16x17.5
SMD capacitor, aluminum electrolytic, Vishay 1616, 16.0x17.5mm, http://www.vishay.com/docs/28395/150crz.pdf
capacitor electrolytic
0
2
2
Capacitor_SMD
CP_Elec_16x22
SMD capacitor, aluminum electrolytic, Vishay 1621, 16.0x22.0mm, http://www.vishay.com/docs/28395/150crz.pdf
capacitor electrolytic
0
2
2
Capacitor_SMD
CP_Elec_18x17.5
SMD capacitor, aluminum electrolytic, Vishay 1816, 18.0x17.5mm, http://www.vishay.com/docs/28395/150crz.pdf
capacitor electrolytic
0
2
2
Capacitor_SMD
CP_Elec_18x22
SMD capacitor, aluminum electrolytic, Vishay 1821, 18.0x22.0mm, http://www.vishay.com/docs/28395/150crz.pdf
capacitor electrolytic
0
2
2
Capacitor_SMD
C_0201_0603Metric
Capacitor SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), generated with kicad-footprint-generator
capacitor
0
4
2
Capacitor_SMD
C_0402_1005Metric
Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator
capacitor
0
2
2
Capacitor_SMD
C_0603_1608Metric
Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator
capacitor
0
2
2
Capacitor_SMD
C_0603_1608Metric_Pad1.05x0.95mm_HandSolder
Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator
capacitor handsolder
0
2
2
Capacitor_SMD
C_0805_2012Metric
Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator
capacitor
0
2
2
Capacitor_SMD
C_0805_2012Metric_Pad1.15x1.40mm_HandSolder
Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator
capacitor handsolder
0
2
2
Capacitor_SMD
C_01005_0402Metric
Capacitor SMD 01005 (0402 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.vishay.com/docs/20056/crcw01005e3.pdf), generated with kicad-footprint-generator
capacitor
0
4
2
Capacitor_SMD
C_1206_3216Metric
Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator
capacitor
0
2
2
Capacitor_SMD
C_1206_3216Metric_Pad1.42x1.75mm_HandSolder
Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator
capacitor handsolder
0
2
2
Capacitor_SMD
C_1210_3225Metric
Capacitor SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator
capacitor
0
2
2
Capacitor_SMD
C_1210_3225Metric_Pad1.42x2.65mm_HandSolder
Capacitor SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator
capacitor handsolder
0
2
2
Capacitor_SMD
C_1806_4516Metric
Capacitor SMD 1806 (4516 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://www.modelithics.com/models/Vendor/MuRata/BLM41P.pdf), generated with kicad-footprint-generator
capacitor
0
2
2
Capacitor_SMD
C_1806_4516Metric_Pad1.57x1.80mm_HandSolder
Capacitor SMD 1806 (4516 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://www.modelithics.com/models/Vendor/MuRata/BLM41P.pdf), generated with kicad-footprint-generator
capacitor handsolder
0
2
2
Capacitor_SMD
C_1812_4532Metric
Capacitor SMD 1812 (4532 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://www.nikhef.nl/pub/departments/mt/projects/detectorR_D/dtddice/ERJ2G.pdf), generated with kicad-footprint-generator
capacitor
0
2
2
Capacitor_SMD
C_1812_4532Metric_Pad1.30x3.40mm_HandSolder
Capacitor SMD 1812 (4532 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://www.nikhef.nl/pub/departments/mt/projects/detectorR_D/dtddice/ERJ2G.pdf), generated with kicad-footprint-generator
capacitor handsolder
0
2
2
Capacitor_SMD
C_1825_4564Metric
Capacitor SMD 1825 (4564 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size from: http://datasheets.avx.com/AVX-HV_MLCC.pdf), generated with kicad-footprint-generator
capacitor
0
2
2
Capacitor_SMD
C_1825_4564Metric_Pad1.88x6.70mm_HandSolder
Capacitor SMD 1825 (4564 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size from: http://datasheets.avx.com/AVX-HV_MLCC.pdf), generated with kicad-footprint-generator
capacitor handsolder
0
2
2
Capacitor_SMD
C_2010_5025Metric
Capacitor SMD 2010 (5025 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator
capacitor
0
2
2
Capacitor_SMD
C_2010_5025Metric_Pad1.52x2.65mm_HandSolder
Capacitor SMD 2010 (5025 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator
capacitor handsolder
0
2
2
Capacitor_SMD
C_2220_5650Metric
Capacitor SMD 2220 (5650 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size from: http://datasheets.avx.com/AVX-HV_MLCC.pdf), generated with kicad-footprint-generator
capacitor
0
2
2
Capacitor_SMD
C_2220_5650Metric_Pad1.97x5.40mm_HandSolder
Capacitor SMD 2220 (5650 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size from: http://datasheets.avx.com/AVX-HV_MLCC.pdf), generated with kicad-footprint-generator
capacitor handsolder
0
2
2
Capacitor_SMD
C_2225_5664Metric
Capacitor SMD 2225 (5664 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size from: http://datasheets.avx.com/AVX-HV_MLCC.pdf), generated with kicad-footprint-generator
capacitor
0
2
2
Capacitor_SMD
C_2225_5664Metric_Pad1.80x6.60mm_HandSolder
Capacitor SMD 2225 (5664 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size from: http://datasheets.avx.com/AVX-HV_MLCC.pdf), generated with kicad-footprint-generator
capacitor handsolder
0
2
2
Capacitor_SMD
C_2512_6332Metric
Capacitor SMD 2512 (6332 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator
capacitor
0
2
2
Capacitor_SMD
C_2512_6332Metric_Pad1.52x3.35mm_HandSolder
Capacitor SMD 2512 (6332 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator
capacitor handsolder
0
2
2
Capacitor_SMD
C_2816_7142Metric
Capacitor SMD 2816 (7142 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size from: https://www.vishay.com/docs/30100/wsl.pdf), generated with kicad-footprint-generator
capacitor
0
2
2
Capacitor_SMD
C_2816_7142Metric_Pad3.20x4.45mm_HandSolder
Capacitor SMD 2816 (7142 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size from: https://www.vishay.com/docs/30100/wsl.pdf), generated with kicad-footprint-generator
capacitor handsolder
0
2
2
Capacitor_SMD
C_3640_9110Metric
Capacitor SMD 3640 (9110 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size from: http://datasheets.avx.com/AVX-HV_MLCC.pdf), generated with kicad-footprint-generator
capacitor
0
2
2
Capacitor_SMD
C_3640_9110Metric_Pad2.10x10.45mm_HandSolder
Capacitor SMD 3640 (9110 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size from: http://datasheets.avx.com/AVX-HV_MLCC.pdf), generated with kicad-footprint-generator
capacitor handsolder
0
2
2
Capacitor_SMD
C_Elec_3x5.4
SMD capacitor, aluminum electrolytic nonpolar, 3.0x5.4mm
capacitor electrolyic nonpolar
0
2
2
Capacitor_SMD
C_Elec_4x5.4
SMD capacitor, aluminum electrolytic nonpolar, 4.0x5.4mm
capacitor electrolyic nonpolar
0
2
2
Capacitor_SMD
C_Elec_4x5.8
SMD capacitor, aluminum electrolytic nonpolar, 4.0x5.8mm
capacitor electrolyic nonpolar
0
2
2
Capacitor_SMD
C_Elec_5x5.4
SMD capacitor, aluminum electrolytic nonpolar, 5.0x5.4mm
capacitor electrolyic nonpolar
0
2
2
Capacitor_SMD
C_Elec_5x5.8
SMD capacitor, aluminum electrolytic nonpolar, 5.0x5.8mm
capacitor electrolyic nonpolar
0
2
2
Capacitor_SMD
C_Elec_6.3x5.4
SMD capacitor, aluminum electrolytic nonpolar, 6.3x5.4mm
capacitor electrolyic nonpolar
0
2
2
Capacitor_SMD
C_Elec_6.3x5.8
SMD capacitor, aluminum electrolytic nonpolar, 6.3x5.8mm
capacitor electrolyic nonpolar
0
2
2
Capacitor_SMD
C_Elec_6.3x7.7
SMD capacitor, aluminum electrolytic nonpolar, 6.3x7.7mm
capacitor electrolyic nonpolar
0
2
2
Capacitor_SMD
C_Elec_8x5.4
SMD capacitor, aluminum electrolytic nonpolar, 8.0x5.4mm
capacitor electrolyic nonpolar
0
2
2
Capacitor_SMD
C_Elec_8x6.2
SMD capacitor, aluminum electrolytic nonpolar, 8.0x6.2mm
capacitor electrolyic nonpolar
0
2
2
Capacitor_SMD
C_Elec_8x10.2
SMD capacitor, aluminum electrolytic nonpolar, 8.0x10.2mm
capacitor electrolyic nonpolar
0
2
2
Capacitor_SMD
C_Elec_10x10.2
SMD capacitor, aluminum electrolytic nonpolar, 10.0x10.2mm
capacitor electrolyic nonpolar
0
2
2
Capacitor_SMD
C_Trimmer_Murata_TZB4-A
trimmer capacitor SMD horizontal, http://www.murata.com/~/media/webrenewal/support/library/catalog/products/capacitor/trimmer/t13e.ashx?la=en-gb
 Murata TZB4 TZB4-A
0
2
2
Capacitor_SMD
C_Trimmer_Murata_TZB4-B
trimmer capacitor SMD horizontal, http://www.murata.com/~/media/webrenewal/support/library/catalog/products/capacitor/trimmer/t13e.ashx?la=en-gb
 Murata TZB4 TZB4-A
0
2
2
Capacitor_SMD
C_Trimmer_Murata_TZC3
trimmer capacitor SMD horizontal, http://www.murata.com/~/media/webrenewal/support/library/catalog/products/capacitor/trimmer/t13e.ashx?la=en-gb
 Murata TZC3
0
2
2
Capacitor_SMD
C_Trimmer_Murata_TZR1
trimmer capacitor SMD horizontal, http://www.murata.com/~/media/webrenewal/support/library/catalog/products/capacitor/trimmer/t13e.ashx?la=en-gb
 Murata TZR1
0
2
2
Capacitor_SMD
C_Trimmer_Murata_TZW4
trimmer capacitor SMD horizontal, http://www.murata.com/~/media/webrenewal/support/library/catalog/products/capacitor/trimmer/t13e.ashx?la=en-gb
 Murata TZW4
0
2
2
Capacitor_SMD
C_Trimmer_Murata_TZY2
trimmer capacitor SMD horizontal, http://www.murata.com/~/media/webrenewal/support/library/catalog/products/capacitor/trimmer/t13e.ashx?la=en-gb
 Murata TZY2
0
2
2
Capacitor_SMD
C_Trimmer_Sprague-Goodman_SGC3
trimmer capacitor SMD horizontal, http://media.wix.com/ugd/d86717_38d9821e12823a7aa9cef38c6c2a73cc.pdf
 Sprague Goodman SGC3
0
2
2
Capacitor_SMD
C_Trimmer_Voltronics_JN
trimmer capacitor SMD horizontal, http://www.knowlescapacitors.com/File%20Library/Voltronics/English/GlobalNavigation/Products/Trimmer%20Capacitors/CerChipTrimCap.pdf
 Voltronics JN
0
2
2
Capacitor_SMD
C_Trimmer_Voltronics_JQ
trimmer capacitor SMD horizontal, http://www.knowlescapacitors.com/File%20Library/Voltronics/English/GlobalNavigation/Products/Trimmer%20Capacitors/CerChipTrimCap.pdf
 Voltronics JQ
0
2
2
Capacitor_SMD
C_Trimmer_Voltronics_JR
trimmer capacitor SMD horizontal, http://www.knowlescapacitors.com/File%20Library/Voltronics/English/GlobalNavigation/Products/Trimmer%20Capacitors/CerChipTrimCap.pdf
 Voltronics JR
0
2
2
Capacitor_SMD
C_Trimmer_Voltronics_JV
trimmer capacitor SMD horizontal, http://www.knowlescapacitors.com/File%20Library/Voltronics/English/GlobalNavigation/Products/Trimmer%20Capacitors/CerChipTrimCap.pdf
 Voltronics JV
0
2
2
Capacitor_SMD
C_Trimmer_Voltronics_JZ
trimmer capacitor SMD horizontal, http://www.knowlescapacitors.com/File%20Library/Voltronics/English/GlobalNavigation/Products/Trimmer%20Capacitors/CerChipTrimCap.pdf
 Voltronics JR
0
2
2
Capacitor_THT
CP_Axial_L10.0mm_D4.5mm_P15.00mm_Horizontal
CP, Axial series, Axial, Horizontal, pin pitch=15mm, , length*diameter=10*4.5mm^2, Electrolytic Capacitor, , http://www.vishay.com/docs/28325/021asm.pdf
CP Axial series Axial Horizontal pin pitch 15mm  length 10mm diameter 4.5mm Electrolytic Capacitor
0
2
2
Capacitor_THT
CP_Axial_L10.0mm_D6.0mm_P15.00mm_Horizontal
CP, Axial series, Axial, Horizontal, pin pitch=15mm, , length*diameter=10*6mm^2, Electrolytic Capacitor, , http://www.vishay.com/docs/28325/021asm.pdf
CP Axial series Axial Horizontal pin pitch 15mm  length 10mm diameter 6mm Electrolytic Capacitor
0
2
2
Capacitor_THT
CP_Axial_L11.0mm_D5.0mm_P18.00mm_Horizontal
CP, Axial series, Axial, Horizontal, pin pitch=18mm, , length*diameter=11*5mm^2, Electrolytic Capacitor
CP Axial series Axial Horizontal pin pitch 18mm  length 11mm diameter 5mm Electrolytic Capacitor
0
2
2
Capacitor_THT
CP_Axial_L11.0mm_D6.0mm_P18.00mm_Horizontal
CP, Axial series, Axial, Horizontal, pin pitch=18mm, , length*diameter=11*6mm^2, Electrolytic Capacitor
CP Axial series Axial Horizontal pin pitch 18mm  length 11mm diameter 6mm Electrolytic Capacitor
0
2
2
Capacitor_THT
CP_Axial_L11.0mm_D8.0mm_P15.00mm_Horizontal
CP, Axial series, Axial, Horizontal, pin pitch=15mm, , length*diameter=11*8mm^2, Electrolytic Capacitor, , http://www.vishay.com/docs/28325/021asm.pdf
CP Axial series Axial Horizontal pin pitch 15mm  length 11mm diameter 8mm Electrolytic Capacitor
0
2
2
Capacitor_THT
CP_Axial_L18.0mm_D6.5mm_P25.00mm_Horizontal
CP, Axial series, Axial, Horizontal, pin pitch=25mm, , length*diameter=18*6.5mm^2, Electrolytic Capacitor, , http://www.vishay.com/docs/28325/021asm.pdf
CP Axial series Axial Horizontal pin pitch 25mm  length 18mm diameter 6.5mm Electrolytic Capacitor
0
2
2
Capacitor_THT
CP_Axial_L18.0mm_D8.0mm_P25.00mm_Horizontal
CP, Axial series, Axial, Horizontal, pin pitch=25mm, , length*diameter=18*8mm^2, Electrolytic Capacitor, , http://www.vishay.com/docs/28325/021asm.pdf
CP Axial series Axial Horizontal pin pitch 25mm  length 18mm diameter 8mm Electrolytic Capacitor
0
2
2
Capacitor_THT
CP_Axial_L18.0mm_D10.0mm_P25.00mm_Horizontal
CP, Axial series, Axial, Horizontal, pin pitch=25mm, , length*diameter=18*10mm^2, Electrolytic Capacitor, , http://www.vishay.com/docs/28325/021asm.pdf
CP Axial series Axial Horizontal pin pitch 25mm  length 18mm diameter 10mm Electrolytic Capacitor
0
2
2
Capacitor_THT
CP_Axial_L20.0mm_D10.0mm_P26.00mm_Horizontal
CP, Axial series, Axial, Horizontal, pin pitch=26mm, , length*diameter=20*10mm^2, Electrolytic Capacitor, , http://www.kemet.com/Lists/ProductCatalog/Attachments/424/KEM_AC102.pdf
CP Axial series Axial Horizontal pin pitch 26mm  length 20mm diameter 10mm Electrolytic Capacitor
0
2
2
Capacitor_THT
CP_Axial_L20.0mm_D13.0mm_P26.00mm_Horizontal
CP, Axial series, Axial, Horizontal, pin pitch=26mm, , length*diameter=20*13mm^2, Electrolytic Capacitor, , http://www.kemet.com/Lists/ProductCatalog/Attachments/424/KEM_AC102.pdf
CP Axial series Axial Horizontal pin pitch 26mm  length 20mm diameter 13mm Electrolytic Capacitor
0
2
2
Capacitor_THT
CP_Axial_L21.0mm_D8.0mm_P28.00mm_Horizontal
CP, Axial series, Axial, Horizontal, pin pitch=28mm, , length*diameter=21*8mm^2, Electrolytic Capacitor
CP Axial series Axial Horizontal pin pitch 28mm  length 21mm diameter 8mm Electrolytic Capacitor
0
2
2
Capacitor_THT
CP_Axial_L25.0mm_D10.0mm_P30.00mm_Horizontal
CP, Axial series, Axial, Horizontal, pin pitch=30mm, , length*diameter=25*10mm^2, Electrolytic Capacitor, , http://www.vishay.com/docs/28325/021asm.pdf
CP Axial series Axial Horizontal pin pitch 30mm  length 25mm diameter 10mm Electrolytic Capacitor
0
2
2
Capacitor_THT
CP_Axial_L26.5mm_D20.0mm_P33.00mm_Horizontal
CP, Axial series, Axial, Horizontal, pin pitch=33mm, , length*diameter=26.5*20mm^2, Electrolytic Capacitor, , http://www.kemet.com/Lists/ProductCatalog/Attachments/424/KEM_AC102.pdf
CP Axial series Axial Horizontal pin pitch 33mm  length 26.5mm diameter 20mm Electrolytic Capacitor
0
2
2
Capacitor_THT
CP_Axial_L29.0mm_D10.0mm_P35.00mm_Horizontal
CP, Axial series, Axial, Horizontal, pin pitch=35mm, , length*diameter=29*10mm^2, Electrolytic Capacitor, , http://www.kemet.com/Lists/ProductCatalog/Attachments/424/KEM_AC102.pdf
CP Axial series Axial Horizontal pin pitch 35mm  length 29mm diameter 10mm Electrolytic Capacitor
0
2
2
Capacitor_THT
CP_Axial_L29.0mm_D13.0mm_P35.00mm_Horizontal
CP, Axial series, Axial, Horizontal, pin pitch=35mm, , length*diameter=29*13mm^2, Electrolytic Capacitor, , http://www.kemet.com/Lists/ProductCatalog/Attachments/424/KEM_AC102.pdf
CP Axial series Axial Horizontal pin pitch 35mm  length 29mm diameter 13mm Electrolytic Capacitor
0
2
2
Capacitor_THT
CP_Axial_L29.0mm_D16.0mm_P35.00mm_Horizontal
CP, Axial series, Axial, Horizontal, pin pitch=35mm, , length*diameter=29*16mm^2, Electrolytic Capacitor, , http://www.kemet.com/Lists/ProductCatalog/Attachments/424/KEM_AC102.pdf
CP Axial series Axial Horizontal pin pitch 35mm  length 29mm diameter 16mm Electrolytic Capacitor
0
2
2
Capacitor_THT
CP_Axial_L29.0mm_D20.0mm_P35.00mm_Horizontal
CP, Axial series, Axial, Horizontal, pin pitch=35mm, , length*diameter=29*20mm^2, Electrolytic Capacitor, , http://www.kemet.com/Lists/ProductCatalog/Attachments/424/KEM_AC102.pdf
CP Axial series Axial Horizontal pin pitch 35mm  length 29mm diameter 20mm Electrolytic Capacitor
0
2
2
Capacitor_THT
CP_Axial_L30.0mm_D10.0mm_P35.00mm_Horizontal
CP, Axial series, Axial, Horizontal, pin pitch=35mm, , length*diameter=30*10mm^2, Electrolytic Capacitor, , http://www.vishay.com/docs/28325/021asm.pdf
CP Axial series Axial Horizontal pin pitch 35mm  length 30mm diameter 10mm Electrolytic Capacitor
0
2
2
Capacitor_THT
CP_Axial_L30.0mm_D12.5mm_P35.00mm_Horizontal
CP, Axial series, Axial, Horizontal, pin pitch=35mm, , length*diameter=30*12.5mm^2, Electrolytic Capacitor, , http://www.vishay.com/docs/28325/021asm.pdf
CP Axial series Axial Horizontal pin pitch 35mm  length 30mm diameter 12.5mm Electrolytic Capacitor
0
2
2
Capacitor_THT
CP_Axial_L30.0mm_D15.0mm_P35.00mm_Horizontal
CP, Axial series, Axial, Horizontal, pin pitch=35mm, , length*diameter=30*15mm^2, Electrolytic Capacitor, , http://www.vishay.com/docs/28325/021asm.pdf
CP Axial series Axial Horizontal pin pitch 35mm  length 30mm diameter 15mm Electrolytic Capacitor
0
2
2
Capacitor_THT
CP_Axial_L30.0mm_D18.0mm_P35.00mm_Horizontal
CP, Axial series, Axial, Horizontal, pin pitch=35mm, , length*diameter=30*18mm^2, Electrolytic Capacitor, , http://www.vishay.com/docs/28325/021asm.pdf
CP Axial series Axial Horizontal pin pitch 35mm  length 30mm diameter 18mm Electrolytic Capacitor
0
2
2
Capacitor_THT
CP_Axial_L34.5mm_D20.0mm_P41.00mm_Horizontal
CP, Axial series, Axial, Horizontal, pin pitch=41mm, , length*diameter=34.5*20mm^2, Electrolytic Capacitor, , http://www.kemet.com/Lists/ProductCatalog/Attachments/424/KEM_AC102.pdf
CP Axial series Axial Horizontal pin pitch 41mm  length 34.5mm diameter 20mm Electrolytic Capacitor
0
2
2
Capacitor_THT
CP_Axial_L37.0mm_D13.0mm_P43.00mm_Horizontal
CP, Axial series, Axial, Horizontal, pin pitch=43mm, , length*diameter=37*13mm^2, Electrolytic Capacitor, , http://www.kemet.com/Lists/ProductCatalog/Attachments/424/KEM_AC102.pdf
CP Axial series Axial Horizontal pin pitch 43mm  length 37mm diameter 13mm Electrolytic Capacitor
0
2
2
Capacitor_THT
CP_Axial_L37.0mm_D16.0mm_P43.00mm_Horizontal
CP, Axial series, Axial, Horizontal, pin pitch=43mm, , length*diameter=37*16mm^2, Electrolytic Capacitor, , http://www.kemet.com/Lists/ProductCatalog/Attachments/424/KEM_AC102.pdf
CP Axial series Axial Horizontal pin pitch 43mm  length 37mm diameter 16mm Electrolytic Capacitor
0
2
2
Capacitor_THT
CP_Axial_L37.0mm_D20.0mm_P43.00mm_Horizontal
CP, Axial series, Axial, Horizontal, pin pitch=43mm, , length*diameter=37*20mm^2, Electrolytic Capacitor, , http://www.kemet.com/Lists/ProductCatalog/Attachments/424/KEM_AC102.pdf
CP Axial series Axial Horizontal pin pitch 43mm  length 37mm diameter 20mm Electrolytic Capacitor
0
2
2
Capacitor_THT
CP_Axial_L38.0mm_D18.0mm_P44.00mm_Horizontal
CP, Axial series, Axial, Horizontal, pin pitch=44mm, , length*diameter=38*18mm^2, Electrolytic Capacitor, , http://www.vishay.com/docs/28325/021asm.pdf
CP Axial series Axial Horizontal pin pitch 44mm  length 38mm diameter 18mm Electrolytic Capacitor
0
2
2
Capacitor_THT
CP_Axial_L38.0mm_D21.0mm_P44.00mm_Horizontal
CP, Axial series, Axial, Horizontal, pin pitch=44mm, , length*diameter=38*21mm^2, Electrolytic Capacitor, , http://www.vishay.com/docs/28325/021asm.pdf
CP Axial series Axial Horizontal pin pitch 44mm  length 38mm diameter 21mm Electrolytic Capacitor
0
2
2
Capacitor_THT
CP_Axial_L40.0mm_D16.0mm_P48.00mm_Horizontal
CP, Axial series, Axial, Horizontal, pin pitch=48mm, , length*diameter=40*16mm^2, Electrolytic Capacitor
CP Axial series Axial Horizontal pin pitch 48mm  length 40mm diameter 16mm Electrolytic Capacitor
0
2
2
Capacitor_THT
CP_Axial_L42.0mm_D23.0mm_P45.00mm_Horizontal
CP, Axial series, Axial, Horizontal, pin pitch=45mm, , length*diameter=42*23.0mm^2, Electrolytic Capacitor, , http://www.vishay.com/docs/42037/53d.pdf
CP Axial series Axial Horizontal pin pitch 45mm  length 42mm diameter 23.0mm Electrolytic Capacitor
0
2
2
Capacitor_THT
CP_Axial_L42.0mm_D26.0mm_P45.00mm_Horizontal
CP, Axial series, Axial, Horizontal, pin pitch=45mm, , length*diameter=42*26mm^2, Electrolytic Capacitor, , http://www.vishay.com/docs/42037/53d.pdf
CP Axial series Axial Horizontal pin pitch 45mm  length 42mm diameter 26mm Electrolytic Capacitor
0
2
2
Capacitor_THT
CP_Axial_L42.0mm_D29.0mm_P45.00mm_Horizontal
CP, Axial series, Axial, Horizontal, pin pitch=45mm, , length*diameter=42*29.0mm^2, Electrolytic Capacitor, , http://www.vishay.com/docs/42037/53d.pdf
CP Axial series Axial Horizontal pin pitch 45mm  length 42mm diameter 29.0mm Electrolytic Capacitor
0
2
2
Capacitor_THT
CP_Axial_L42.0mm_D32.0mm_P45.00mm_Horizontal
CP, Axial series, Axial, Horizontal, pin pitch=45mm, , length*diameter=42*32.0mm^2, Electrolytic Capacitor, , http://www.vishay.com/docs/42037/53d.pdf
CP Axial series Axial Horizontal pin pitch 45mm  length 42mm diameter 32.0mm Electrolytic Capacitor
0
2
2
Capacitor_THT
CP_Axial_L42.0mm_D35.0mm_P45.00mm_Horizontal
CP, Axial series, Axial, Horizontal, pin pitch=45mm, , length*diameter=42*35.0mm^2, Electrolytic Capacitor, , http://www.vishay.com/docs/42037/53d.pdf
CP Axial series Axial Horizontal pin pitch 45mm  length 42mm diameter 35.0mm Electrolytic Capacitor
0
2
2
Capacitor_THT
CP_Axial_L42.5mm_D20.0mm_P49.00mm_Horizontal
CP, Axial series, Axial, Horizontal, pin pitch=49mm, , length*diameter=42.5*20mm^2, Electrolytic Capacitor
CP Axial series Axial Horizontal pin pitch 49mm  length 42.5mm diameter 20mm Electrolytic Capacitor
0
2
2
Capacitor_THT
CP_Axial_L46.0mm_D20.0mm_P52.00mm_Horizontal
CP, Axial series, Axial, Horizontal, pin pitch=52mm, , length*diameter=46*20mm^2, Electrolytic Capacitor
CP Axial series Axial Horizontal pin pitch 52mm  length 46mm diameter 20mm Electrolytic Capacitor
0
2
2
Capacitor_THT
CP_Axial_L55.0mm_D23.0mm_P60.00mm_Horizontal
CP, Axial series, Axial, Horizontal, pin pitch=60mm, , length*diameter=55*23.0mm^2, Electrolytic Capacitor, , http://www.vishay.com/docs/42037/53d.pdf
CP Axial series Axial Horizontal pin pitch 60mm  length 55mm diameter 23.0mm Electrolytic Capacitor
0
2
2
Capacitor_THT
CP_Axial_L55.0mm_D26.0mm_P60.00mm_Horizontal
CP, Axial series, Axial, Horizontal, pin pitch=60mm, , length*diameter=55*26mm^2, Electrolytic Capacitor, , http://www.vishay.com/docs/42037/53d.pdf
CP Axial series Axial Horizontal pin pitch 60mm  length 55mm diameter 26mm Electrolytic Capacitor
0
2
2
Capacitor_THT
CP_Axial_L55.0mm_D29.0mm_P60.00mm_Horizontal
CP, Axial series, Axial, Horizontal, pin pitch=60mm, , length*diameter=55*29.0mm^2, Electrolytic Capacitor, , http://www.vishay.com/docs/42037/53d.pdf
CP Axial series Axial Horizontal pin pitch 60mm  length 55mm diameter 29.0mm Electrolytic Capacitor
0
2
2
Capacitor_THT
CP_Axial_L55.0mm_D32.0mm_P60.00mm_Horizontal
CP, Axial series, Axial, Horizontal, pin pitch=60mm, , length*diameter=55*32.0mm^2, Electrolytic Capacitor, , http://www.vishay.com/docs/42037/53d.pdf
CP Axial series Axial Horizontal pin pitch 60mm  length 55mm diameter 32.0mm Electrolytic Capacitor
0
2
2
Capacitor_THT
CP_Axial_L55.0mm_D35.0mm_P60.00mm_Horizontal
CP, Axial series, Axial, Horizontal, pin pitch=60mm, , length*diameter=55*35.0mm^2, Electrolytic Capacitor, , http://www.vishay.com/docs/42037/53d.pdf
CP Axial series Axial Horizontal pin pitch 60mm  length 55mm diameter 35.0mm Electrolytic Capacitor
0
2
2
Capacitor_THT
CP_Axial_L67.0mm_D23.0mm_P75.00mm_Horizontal
CP, Axial series, Axial, Horizontal, pin pitch=75mm, , length*diameter=67*23.0mm^2, Electrolytic Capacitor, , http://www.vishay.com/docs/42037/53d.pdf
CP Axial series Axial Horizontal pin pitch 75mm  length 67mm diameter 23.0mm Electrolytic Capacitor
0
2
2
Capacitor_THT
CP_Axial_L67.0mm_D26.0mm_P75.00mm_Horizontal
CP, Axial series, Axial, Horizontal, pin pitch=75mm, , length*diameter=67*26mm^2, Electrolytic Capacitor, , http://www.vishay.com/docs/42037/53d.pdf
CP Axial series Axial Horizontal pin pitch 75mm  length 67mm diameter 26mm Electrolytic Capacitor
0
2
2
Capacitor_THT
CP_Axial_L67.0mm_D29.0mm_P75.00mm_Horizontal
CP, Axial series, Axial, Horizontal, pin pitch=75mm, , length*diameter=67*29.0mm^2, Electrolytic Capacitor, , http://www.vishay.com/docs/42037/53d.pdf
CP Axial series Axial Horizontal pin pitch 75mm  length 67mm diameter 29.0mm Electrolytic Capacitor
0
2
2
Capacitor_THT
CP_Axial_L67.0mm_D32.0mm_P75.00mm_Horizontal
CP, Axial series, Axial, Horizontal, pin pitch=75mm, , length*diameter=67*32.0mm^2, Electrolytic Capacitor, , http://www.vishay.com/docs/42037/53d.pdf
CP Axial series Axial Horizontal pin pitch 75mm  length 67mm diameter 32.0mm Electrolytic Capacitor
0
2
2
Capacitor_THT
CP_Axial_L67.0mm_D35.0mm_P75.00mm_Horizontal
CP, Axial series, Axial, Horizontal, pin pitch=75mm, , length*diameter=67*35.0mm^2, Electrolytic Capacitor, , http://www.vishay.com/docs/42037/53d.pdf
CP Axial series Axial Horizontal pin pitch 75mm  length 67mm diameter 35.0mm Electrolytic Capacitor
0
2
2
Capacitor_THT
CP_Axial_L80.0mm_D23.0mm_P85.00mm_Horizontal
CP, Axial series, Axial, Horizontal, pin pitch=85mm, , length*diameter=80*23.0mm^2, Electrolytic Capacitor, , http://www.vishay.com/docs/42037/53d.pdf
CP Axial series Axial Horizontal pin pitch 85mm  length 80mm diameter 23.0mm Electrolytic Capacitor
0
2
2
Capacitor_THT
CP_Axial_L80.0mm_D26.0mm_P85.00mm_Horizontal
CP, Axial series, Axial, Horizontal, pin pitch=85mm, , length*diameter=80*26mm^2, Electrolytic Capacitor, , http://www.vishay.com/docs/42037/53d.pdf
CP Axial series Axial Horizontal pin pitch 85mm  length 80mm diameter 26mm Electrolytic Capacitor
0
2
2
Capacitor_THT
CP_Axial_L80.0mm_D29.0mm_P85.00mm_Horizontal
CP, Axial series, Axial, Horizontal, pin pitch=85mm, , length*diameter=80*29.0mm^2, Electrolytic Capacitor, , http://www.vishay.com/docs/42037/53d.pdf
CP Axial series Axial Horizontal pin pitch 85mm  length 80mm diameter 29.0mm Electrolytic Capacitor
0
2
2
Capacitor_THT
CP_Axial_L80.0mm_D32.0mm_P85.00mm_Horizontal
CP, Axial series, Axial, Horizontal, pin pitch=85mm, , length*diameter=80*32.0mm^2, Electrolytic Capacitor, , http://www.vishay.com/docs/42037/53d.pdf
CP Axial series Axial Horizontal pin pitch 85mm  length 80mm diameter 32.0mm Electrolytic Capacitor
0
2
2
Capacitor_THT
CP_Axial_L80.0mm_D35.0mm_P85.00mm_Horizontal
CP, Axial series, Axial, Horizontal, pin pitch=85mm, , length*diameter=80*35.0mm^2, Electrolytic Capacitor, , http://www.vishay.com/docs/42037/53d.pdf
CP Axial series Axial Horizontal pin pitch 85mm  length 80mm diameter 35.0mm Electrolytic Capacitor
0
2
2
Capacitor_THT
CP_Axial_L93.0mm_D23.0mm_P100.00mm_Horizontal
CP, Axial series, Axial, Horizontal, pin pitch=100mm, , length*diameter=93*23.0mm^2, Electrolytic Capacitor, , http://www.vishay.com/docs/42037/53d.pdf
CP Axial series Axial Horizontal pin pitch 100mm  length 93mm diameter 23.0mm Electrolytic Capacitor
0
2
2
Capacitor_THT
CP_Axial_L93.0mm_D26.0mm_P100.00mm_Horizontal
CP, Axial series, Axial, Horizontal, pin pitch=100mm, , length*diameter=93*26mm^2, Electrolytic Capacitor, , http://www.vishay.com/docs/42037/53d.pdf
CP Axial series Axial Horizontal pin pitch 100mm  length 93mm diameter 26mm Electrolytic Capacitor
0
2
2
Capacitor_THT
CP_Axial_L93.0mm_D29.0mm_P100.00mm_Horizontal
CP, Axial series, Axial, Horizontal, pin pitch=100mm, , length*diameter=93*29.0mm^2, Electrolytic Capacitor, , http://www.vishay.com/docs/42037/53d.pdf
CP Axial series Axial Horizontal pin pitch 100mm  length 93mm diameter 29.0mm Electrolytic Capacitor
0
2
2
Capacitor_THT
CP_Axial_L93.0mm_D32.0mm_P100.00mm_Horizontal
CP, Axial series, Axial, Horizontal, pin pitch=100mm, , length*diameter=93*32.0mm^2, Electrolytic Capacitor, , http://www.vishay.com/docs/42037/53d.pdf
CP Axial series Axial Horizontal pin pitch 100mm  length 93mm diameter 32.0mm Electrolytic Capacitor
0
2
2
Capacitor_THT
CP_Axial_L93.0mm_D35.0mm_P100.00mm_Horizontal
CP, Axial series, Axial, Horizontal, pin pitch=100mm, , length*diameter=93*35.0mm^2, Electrolytic Capacitor, , http://www.vishay.com/docs/42037/53d.pdf
CP Axial series Axial Horizontal pin pitch 100mm  length 93mm diameter 35.0mm Electrolytic Capacitor
0
2
2
Capacitor_THT
CP_Radial_D4.0mm_P1.50mm
CP, Radial series, Radial, pin pitch=1.50mm, , diameter=4mm, Electrolytic Capacitor
CP Radial series Radial pin pitch 1.50mm  diameter 4mm Electrolytic Capacitor
0
2
2
Capacitor_THT
CP_Radial_D4.0mm_P2.00mm
CP, Radial series, Radial, pin pitch=2.00mm, , diameter=4mm, Electrolytic Capacitor
CP Radial series Radial pin pitch 2.00mm  diameter 4mm Electrolytic Capacitor
0
2
2
Capacitor_THT
CP_Radial_D5.0mm_P2.00mm
CP, Radial series, Radial, pin pitch=2.00mm, , diameter=5mm, Electrolytic Capacitor
CP Radial series Radial pin pitch 2.00mm  diameter 5mm Electrolytic Capacitor
0
2
2
Capacitor_THT
CP_Radial_D5.0mm_P2.50mm
CP, Radial series, Radial, pin pitch=2.50mm, , diameter=5mm, Electrolytic Capacitor
CP Radial series Radial pin pitch 2.50mm  diameter 5mm Electrolytic Capacitor
0
2
2
Capacitor_THT
CP_Radial_D6.3mm_P2.50mm
CP, Radial series, Radial, pin pitch=2.50mm, , diameter=6.3mm, Electrolytic Capacitor
CP Radial series Radial pin pitch 2.50mm  diameter 6.3mm Electrolytic Capacitor
0
2
2
Capacitor_THT
CP_Radial_D7.5mm_P2.50mm
CP, Radial series, Radial, pin pitch=2.50mm, , diameter=7.5mm, Electrolytic Capacitor
CP Radial series Radial pin pitch 2.50mm  diameter 7.5mm Electrolytic Capacitor
0
2
2
Capacitor_THT
CP_Radial_D8.0mm_P2.50mm
CP, Radial series, Radial, pin pitch=2.50mm, , diameter=8mm, Electrolytic Capacitor
CP Radial series Radial pin pitch 2.50mm  diameter 8mm Electrolytic Capacitor
0
2
2
Capacitor_THT
CP_Radial_D8.0mm_P3.50mm
CP, Radial series, Radial, pin pitch=3.50mm, , diameter=8mm, Electrolytic Capacitor
CP Radial series Radial pin pitch 3.50mm  diameter 8mm Electrolytic Capacitor
0
2
2
Capacitor_THT
CP_Radial_D8.0mm_P3.80mm
CP, Radial series, Radial, pin pitch=3.80mm, , diameter=8mm, Electrolytic Capacitor
CP Radial series Radial pin pitch 3.80mm  diameter 8mm Electrolytic Capacitor
0
2
2
Capacitor_THT
CP_Radial_D8.0mm_P5.00mm
CP, Radial series, Radial, pin pitch=5.00mm, , diameter=8mm, Electrolytic Capacitor
CP Radial series Radial pin pitch 5.00mm  diameter 8mm Electrolytic Capacitor
0
2
2
Capacitor_THT
CP_Radial_D10.0mm_P2.50mm
CP, Radial series, Radial, pin pitch=2.50mm, , diameter=10mm, Electrolytic Capacitor
CP Radial series Radial pin pitch 2.50mm  diameter 10mm Electrolytic Capacitor
0
2
2
Capacitor_THT
CP_Radial_D10.0mm_P2.50mm_P5.00mm
CP, Radial series, Radial, pin pitch=2.50mm 5.00mm, , diameter=10mm, Electrolytic Capacitor
CP Radial series Radial pin pitch 2.50mm 5.00mm  diameter 10mm Electrolytic Capacitor
0
4
2
Capacitor_THT
CP_Radial_D10.0mm_P3.50mm
CP, Radial series, Radial, pin pitch=3.50mm, , diameter=10mm, Electrolytic Capacitor
CP Radial series Radial pin pitch 3.50mm  diameter 10mm Electrolytic Capacitor
0
2
2
Capacitor_THT
CP_Radial_D10.0mm_P3.80mm
CP, Radial series, Radial, pin pitch=3.80mm, , diameter=10mm, Electrolytic Capacitor
CP Radial series Radial pin pitch 3.80mm  diameter 10mm Electrolytic Capacitor
0
2
2
Capacitor_THT
CP_Radial_D10.0mm_P5.00mm
CP, Radial series, Radial, pin pitch=5.00mm, , diameter=10mm, Electrolytic Capacitor
CP Radial series Radial pin pitch 5.00mm  diameter 10mm Electrolytic Capacitor
0
2
2
Capacitor_THT
CP_Radial_D10.0mm_P5.00mm_P7.50mm
CP, Radial series, Radial, pin pitch=5.00mm 7.50mm, , diameter=10mm, Electrolytic Capacitor
CP Radial series Radial pin pitch 5.00mm 7.50mm  diameter 10mm Electrolytic Capacitor
0
4
2
Capacitor_THT
CP_Radial_D10.0mm_P7.50mm
CP, Radial series, Radial, pin pitch=7.50mm, , diameter=10mm, Electrolytic Capacitor
CP Radial series Radial pin pitch 7.50mm  diameter 10mm Electrolytic Capacitor
0
2
2
Capacitor_THT
CP_Radial_D12.5mm_P2.50mm
CP, Radial series, Radial, pin pitch=2.50mm, , diameter=12.5mm, Electrolytic Capacitor
CP Radial series Radial pin pitch 2.50mm  diameter 12.5mm Electrolytic Capacitor
0
2
2
Capacitor_THT
CP_Radial_D12.5mm_P5.00mm
CP, Radial series, Radial, pin pitch=5.00mm, , diameter=12.5mm, Electrolytic Capacitor
CP Radial series Radial pin pitch 5.00mm  diameter 12.5mm Electrolytic Capacitor
0
2
2
Capacitor_THT
CP_Radial_D12.5mm_P7.50mm
CP, Radial series, Radial, pin pitch=7.50mm, , diameter=12.5mm, Electrolytic Capacitor
CP Radial series Radial pin pitch 7.50mm  diameter 12.5mm Electrolytic Capacitor
0
2
2
Capacitor_THT
CP_Radial_D13.0mm_P2.50mm
CP, Radial series, Radial, pin pitch=2.50mm, , diameter=13mm, Electrolytic Capacitor
CP Radial series Radial pin pitch 2.50mm  diameter 13mm Electrolytic Capacitor
0
2
2
Capacitor_THT
CP_Radial_D13.0mm_P5.00mm
CP, Radial series, Radial, pin pitch=5.00mm, , diameter=13mm, Electrolytic Capacitor
CP Radial series Radial pin pitch 5.00mm  diameter 13mm Electrolytic Capacitor
0
2
2
Capacitor_THT
CP_Radial_D13.0mm_P7.50mm
CP, Radial series, Radial, pin pitch=7.50mm, , diameter=13mm, Electrolytic Capacitor
CP Radial series Radial pin pitch 7.50mm  diameter 13mm Electrolytic Capacitor
0
2
2
Capacitor_THT
CP_Radial_D14.0mm_P5.00mm
CP, Radial series, Radial, pin pitch=5.00mm, , diameter=14mm, Electrolytic Capacitor
CP Radial series Radial pin pitch 5.00mm  diameter 14mm Electrolytic Capacitor
0
2
2
Capacitor_THT
CP_Radial_D14.0mm_P7.50mm
CP, Radial series, Radial, pin pitch=7.50mm, , diameter=14mm, Electrolytic Capacitor
CP Radial series Radial pin pitch 7.50mm  diameter 14mm Electrolytic Capacitor
0
2
2
Capacitor_THT
CP_Radial_D16.0mm_P7.50mm
CP, Radial series, Radial, pin pitch=7.50mm, , diameter=16mm, Electrolytic Capacitor
CP Radial series Radial pin pitch 7.50mm  diameter 16mm Electrolytic Capacitor
0
2
2
Capacitor_THT
CP_Radial_D17.0mm_P7.50mm
CP, Radial series, Radial, pin pitch=7.50mm, , diameter=17mm, Electrolytic Capacitor
CP Radial series Radial pin pitch 7.50mm  diameter 17mm Electrolytic Capacitor
0
2
2
Capacitor_THT
CP_Radial_D18.0mm_P7.50mm
CP, Radial series, Radial, pin pitch=7.50mm, , diameter=18mm, Electrolytic Capacitor
CP Radial series Radial pin pitch 7.50mm  diameter 18mm Electrolytic Capacitor
0
2
2
Capacitor_THT
CP_Radial_D22.0mm_P10.00mm_3pin_SnapIn
CP, Radial series, Radial, pin pitch=10.00mm, , diameter=22mm, Electrolytic Capacitor, , http://www.vishay.com/docs/28342/058059pll-si.pdf
CP Radial series Radial pin pitch 10.00mm  diameter 22mm Electrolytic Capacitor
0
3
2
Capacitor_THT
CP_Radial_D22.0mm_P10.00mm_SnapIn
CP, Radial series, Radial, pin pitch=10.00mm, , diameter=22mm, Electrolytic Capacitor, , http://www.vishay.com/docs/28342/058059pll-si.pdf
CP Radial series Radial pin pitch 10.00mm  diameter 22mm Electrolytic Capacitor
0
2
2
Capacitor_THT
CP_Radial_D24.0mm_P10.00mm_3pin_SnapIn
CP, Radial series, Radial, pin pitch=10.00mm, , diameter=24mm, Electrolytic Capacitor, , http://www.vishay.com/docs/28342/058059pll-si.pdf
CP Radial series Radial pin pitch 10.00mm  diameter 24mm Electrolytic Capacitor
0
3
2
Capacitor_THT
CP_Radial_D24.0mm_P10.00mm_SnapIn
CP, Radial series, Radial, pin pitch=10.00mm, , diameter=24mm, Electrolytic Capacitor, , http://www.vishay.com/docs/28342/058059pll-si.pdf
CP Radial series Radial pin pitch 10.00mm  diameter 24mm Electrolytic Capacitor
0
2
2
Capacitor_THT
CP_Radial_D25.0mm_P10.00mm_3pin_SnapIn
CP, Radial series, Radial, pin pitch=10.00mm, , diameter=25mm, Electrolytic Capacitor, , http://www.vishay.com/docs/28342/058059pll-si.pdf
CP Radial series Radial pin pitch 10.00mm  diameter 25mm Electrolytic Capacitor
0
3
2
Capacitor_THT
CP_Radial_D25.0mm_P10.00mm_SnapIn
CP, Radial series, Radial, pin pitch=10.00mm, , diameter=25mm, Electrolytic Capacitor, , http://www.vishay.com/docs/28342/058059pll-si.pdf
CP Radial series Radial pin pitch 10.00mm  diameter 25mm Electrolytic Capacitor
0
2
2
Capacitor_THT
CP_Radial_D26.0mm_P10.00mm_3pin_SnapIn
CP, Radial series, Radial, pin pitch=10.00mm, , diameter=26mm, Electrolytic Capacitor, , http://www.vishay.com/docs/28342/058059pll-si.pdf
CP Radial series Radial pin pitch 10.00mm  diameter 26mm Electrolytic Capacitor
0
3
2
Capacitor_THT
CP_Radial_D26.0mm_P10.00mm_SnapIn
CP, Radial series, Radial, pin pitch=10.00mm, , diameter=26mm, Electrolytic Capacitor, , http://www.vishay.com/docs/28342/058059pll-si.pdf
CP Radial series Radial pin pitch 10.00mm  diameter 26mm Electrolytic Capacitor
0
2
2
Capacitor_THT
CP_Radial_D30.0mm_P10.00mm_3pin_SnapIn
CP, Radial series, Radial, pin pitch=10.00mm, , diameter=30mm, Electrolytic Capacitor, , http://www.vishay.com/docs/28342/058059pll-si.pdf
CP Radial series Radial pin pitch 10.00mm  diameter 30mm Electrolytic Capacitor
0
3
2
Capacitor_THT
CP_Radial_D30.0mm_P10.00mm_SnapIn
CP, Radial series, Radial, pin pitch=10.00mm, , diameter=30mm, Electrolytic Capacitor, , http://www.vishay.com/docs/28342/058059pll-si.pdf
CP Radial series Radial pin pitch 10.00mm  diameter 30mm Electrolytic Capacitor
0
2
2
Capacitor_THT
CP_Radial_D35.0mm_P10.00mm_3pin_SnapIn
CP, Radial series, Radial, pin pitch=10.00mm, , diameter=35mm, Electrolytic Capacitor, , http://www.vishay.com/docs/28342/058059pll-si.pdf
CP Radial series Radial pin pitch 10.00mm  diameter 35mm Electrolytic Capacitor
0
3
2
Capacitor_THT
CP_Radial_D35.0mm_P10.00mm_SnapIn
CP, Radial series, Radial, pin pitch=10.00mm, , diameter=35mm, Electrolytic Capacitor, , http://www.vishay.com/docs/28342/058059pll-si.pdf
CP Radial series Radial pin pitch 10.00mm  diameter 35mm Electrolytic Capacitor
0
2
2
Capacitor_THT
CP_Radial_D40.0mm_P10.00mm_3pin_SnapIn
CP, Radial series, Radial, pin pitch=10.00mm, , diameter=40mm, Electrolytic Capacitor, , http://www.vishay.com/docs/28342/058059pll-si.pdf
CP Radial series Radial pin pitch 10.00mm  diameter 40mm Electrolytic Capacitor
0
3
2
Capacitor_THT
CP_Radial_D40.0mm_P10.00mm_SnapIn
CP, Radial series, Radial, pin pitch=10.00mm, , diameter=40mm, Electrolytic Capacitor, , http://www.vishay.com/docs/28342/058059pll-si.pdf
CP Radial series Radial pin pitch 10.00mm  diameter 40mm Electrolytic Capacitor
0
2
2
Capacitor_THT
CP_Radial_Tantal_D4.5mm_P2.50mm
CP, Radial_Tantal series, Radial, pin pitch=2.50mm, , diameter=4.5mm, Tantal Electrolytic Capacitor, http://cdn-reichelt.de/documents/datenblatt/B300/TANTAL-TB-Serie%23.pdf
CP Radial_Tantal series Radial pin pitch 2.50mm  diameter 4.5mm Tantal Electrolytic Capacitor
0
2
2
Capacitor_THT
CP_Radial_Tantal_D4.5mm_P5.00mm
CP, Radial_Tantal series, Radial, pin pitch=5.00mm, , diameter=4.5mm, Tantal Electrolytic Capacitor, http://cdn-reichelt.de/documents/datenblatt/B300/TANTAL-TB-Serie%23.pdf
CP Radial_Tantal series Radial pin pitch 5.00mm  diameter 4.5mm Tantal Electrolytic Capacitor
0
2
2
Capacitor_THT
CP_Radial_Tantal_D5.0mm_P2.50mm
CP, Radial_Tantal series, Radial, pin pitch=2.50mm, , diameter=5.0mm, Tantal Electrolytic Capacitor, http://cdn-reichelt.de/documents/datenblatt/B300/TANTAL-TB-Serie%23.pdf
CP Radial_Tantal series Radial pin pitch 2.50mm  diameter 5.0mm Tantal Electrolytic Capacitor
0
2
2
Capacitor_THT
CP_Radial_Tantal_D5.0mm_P5.00mm
CP, Radial_Tantal series, Radial, pin pitch=5.00mm, , diameter=5.0mm, Tantal Electrolytic Capacitor, http://cdn-reichelt.de/documents/datenblatt/B300/TANTAL-TB-Serie%23.pdf
CP Radial_Tantal series Radial pin pitch 5.00mm  diameter 5.0mm Tantal Electrolytic Capacitor
0
2
2
Capacitor_THT
CP_Radial_Tantal_D5.5mm_P2.50mm
CP, Radial_Tantal series, Radial, pin pitch=2.50mm, , diameter=5.5mm, Tantal Electrolytic Capacitor, http://cdn-reichelt.de/documents/datenblatt/B300/TANTAL-TB-Serie%23.pdf
CP Radial_Tantal series Radial pin pitch 2.50mm  diameter 5.5mm Tantal Electrolytic Capacitor
0
2
2
Capacitor_THT
CP_Radial_Tantal_D5.5mm_P5.00mm
CP, Radial_Tantal series, Radial, pin pitch=5.00mm, , diameter=5.5mm, Tantal Electrolytic Capacitor, http://cdn-reichelt.de/documents/datenblatt/B300/TANTAL-TB-Serie%23.pdf
CP Radial_Tantal series Radial pin pitch 5.00mm  diameter 5.5mm Tantal Electrolytic Capacitor
0
2
2
Capacitor_THT
CP_Radial_Tantal_D6.0mm_P2.50mm
CP, Radial_Tantal series, Radial, pin pitch=2.50mm, , diameter=6.0mm, Tantal Electrolytic Capacitor, http://cdn-reichelt.de/documents/datenblatt/B300/TANTAL-TB-Serie%23.pdf
CP Radial_Tantal series Radial pin pitch 2.50mm  diameter 6.0mm Tantal Electrolytic Capacitor
0
2
2
Capacitor_THT
CP_Radial_Tantal_D6.0mm_P5.00mm
CP, Radial_Tantal series, Radial, pin pitch=5.00mm, , diameter=6.0mm, Tantal Electrolytic Capacitor, http://cdn-reichelt.de/documents/datenblatt/B300/TANTAL-TB-Serie%23.pdf
CP Radial_Tantal series Radial pin pitch 5.00mm  diameter 6.0mm Tantal Electrolytic Capacitor
0
2
2
Capacitor_THT
CP_Radial_Tantal_D7.0mm_P2.50mm
CP, Radial_Tantal series, Radial, pin pitch=2.50mm, , diameter=7.0mm, Tantal Electrolytic Capacitor, http://cdn-reichelt.de/documents/datenblatt/B300/TANTAL-TB-Serie%23.pdf
CP Radial_Tantal series Radial pin pitch 2.50mm  diameter 7.0mm Tantal Electrolytic Capacitor
0
2
2
Capacitor_THT
CP_Radial_Tantal_D7.0mm_P5.00mm
CP, Radial_Tantal series, Radial, pin pitch=5.00mm, , diameter=7.0mm, Tantal Electrolytic Capacitor, http://cdn-reichelt.de/documents/datenblatt/B300/TANTAL-TB-Serie%23.pdf
CP Radial_Tantal series Radial pin pitch 5.00mm  diameter 7.0mm Tantal Electrolytic Capacitor
0
2
2
Capacitor_THT
CP_Radial_Tantal_D8.0mm_P2.50mm
CP, Radial_Tantal series, Radial, pin pitch=2.50mm, , diameter=8.0mm, Tantal Electrolytic Capacitor, http://cdn-reichelt.de/documents/datenblatt/B300/TANTAL-TB-Serie%23.pdf
CP Radial_Tantal series Radial pin pitch 2.50mm  diameter 8.0mm Tantal Electrolytic Capacitor
0
2
2
Capacitor_THT
CP_Radial_Tantal_D8.0mm_P5.00mm
CP, Radial_Tantal series, Radial, pin pitch=5.00mm, , diameter=8.0mm, Tantal Electrolytic Capacitor, http://cdn-reichelt.de/documents/datenblatt/B300/TANTAL-TB-Serie%23.pdf
CP Radial_Tantal series Radial pin pitch 5.00mm  diameter 8.0mm Tantal Electrolytic Capacitor
0
2
2
Capacitor_THT
CP_Radial_Tantal_D9.0mm_P2.50mm
CP, Radial_Tantal series, Radial, pin pitch=2.50mm, , diameter=9.0mm, Tantal Electrolytic Capacitor, http://cdn-reichelt.de/documents/datenblatt/B300/TANTAL-TB-Serie%23.pdf
CP Radial_Tantal series Radial pin pitch 2.50mm  diameter 9.0mm Tantal Electrolytic Capacitor
0
2
2
Capacitor_THT
CP_Radial_Tantal_D9.0mm_P5.00mm
CP, Radial_Tantal series, Radial, pin pitch=5.00mm, , diameter=9.0mm, Tantal Electrolytic Capacitor, http://cdn-reichelt.de/documents/datenblatt/B300/TANTAL-TB-Serie%23.pdf
CP Radial_Tantal series Radial pin pitch 5.00mm  diameter 9.0mm Tantal Electrolytic Capacitor
0
2
2
Capacitor_THT
CP_Radial_Tantal_D10.5mm_P2.50mm
CP, Radial_Tantal series, Radial, pin pitch=2.50mm, , diameter=10.5mm, Tantal Electrolytic Capacitor, http://cdn-reichelt.de/documents/datenblatt/B300/TANTAL-TB-Serie%23.pdf
CP Radial_Tantal series Radial pin pitch 2.50mm  diameter 10.5mm Tantal Electrolytic Capacitor
0
2
2
Capacitor_THT
CP_Radial_Tantal_D10.5mm_P5.00mm
CP, Radial_Tantal series, Radial, pin pitch=5.00mm, , diameter=10.5mm, Tantal Electrolytic Capacitor, http://cdn-reichelt.de/documents/datenblatt/B300/TANTAL-TB-Serie%23.pdf
CP Radial_Tantal series Radial pin pitch 5.00mm  diameter 10.5mm Tantal Electrolytic Capacitor
0
2
2
Capacitor_THT
C_Axial_L3.8mm_D2.6mm_P7.50mm_Horizontal
C, Axial series, Axial, Horizontal, pin pitch=7.5mm, , length*diameter=3.8*2.6mm^2, http://www.vishay.com/docs/45231/arseries.pdf
C Axial series Axial Horizontal pin pitch 7.5mm  length 3.8mm diameter 2.6mm
0
2
2
Capacitor_THT
C_Axial_L3.8mm_D2.6mm_P10.00mm_Horizontal
C, Axial series, Axial, Horizontal, pin pitch=10mm, , length*diameter=3.8*2.6mm^2, http://www.vishay.com/docs/45231/arseries.pdf
C Axial series Axial Horizontal pin pitch 10mm  length 3.8mm diameter 2.6mm
0
2
2
Capacitor_THT
C_Axial_L3.8mm_D2.6mm_P12.50mm_Horizontal
C, Axial series, Axial, Horizontal, pin pitch=12.5mm, , length*diameter=3.8*2.6mm^2, http://www.vishay.com/docs/45231/arseries.pdf
C Axial series Axial Horizontal pin pitch 12.5mm  length 3.8mm diameter 2.6mm
0
2
2
Capacitor_THT
C_Axial_L3.8mm_D2.6mm_P15.00mm_Horizontal
C, Axial series, Axial, Horizontal, pin pitch=15mm, , length*diameter=3.8*2.6mm^2, http://www.vishay.com/docs/45231/arseries.pdf
C Axial series Axial Horizontal pin pitch 15mm  length 3.8mm diameter 2.6mm
0
2
2
Capacitor_THT
C_Axial_L5.1mm_D3.1mm_P7.50mm_Horizontal
C, Axial series, Axial, Horizontal, pin pitch=7.5mm, , length*diameter=5.1*3.1mm^2, http://www.vishay.com/docs/45231/arseries.pdf
C Axial series Axial Horizontal pin pitch 7.5mm  length 5.1mm diameter 3.1mm
0
2
2
Capacitor_THT
C_Axial_L5.1mm_D3.1mm_P10.00mm_Horizontal
C, Axial series, Axial, Horizontal, pin pitch=10mm, , length*diameter=5.1*3.1mm^2, http://www.vishay.com/docs/45231/arseries.pdf
C Axial series Axial Horizontal pin pitch 10mm  length 5.1mm diameter 3.1mm
0
2
2
Capacitor_THT
C_Axial_L5.1mm_D3.1mm_P12.50mm_Horizontal
C, Axial series, Axial, Horizontal, pin pitch=12.5mm, , length*diameter=5.1*3.1mm^2, http://www.vishay.com/docs/45231/arseries.pdf
C Axial series Axial Horizontal pin pitch 12.5mm  length 5.1mm diameter 3.1mm
0
2
2
Capacitor_THT
C_Axial_L5.1mm_D3.1mm_P15.00mm_Horizontal
C, Axial series, Axial, Horizontal, pin pitch=15mm, , length*diameter=5.1*3.1mm^2, http://www.vishay.com/docs/45231/arseries.pdf
C Axial series Axial Horizontal pin pitch 15mm  length 5.1mm diameter 3.1mm
0
2
2
Capacitor_THT
C_Axial_L12.0mm_D6.5mm_P15.00mm_Horizontal
C, Axial series, Axial, Horizontal, pin pitch=15mm, , length*diameter=12*6.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B300/STYROFLEX.pdf
C Axial series Axial Horizontal pin pitch 15mm  length 12mm diameter 6.5mm
0
2
2
Capacitor_THT
C_Axial_L12.0mm_D6.5mm_P20.00mm_Horizontal
C, Axial series, Axial, Horizontal, pin pitch=20mm, , length*diameter=12*6.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B300/STYROFLEX.pdf
C Axial series Axial Horizontal pin pitch 20mm  length 12mm diameter 6.5mm
0
2
2
Capacitor_THT
C_Axial_L12.0mm_D7.5mm_P15.00mm_Horizontal
C, Axial series, Axial, Horizontal, pin pitch=15mm, , length*diameter=12*7.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B300/STYROFLEX.pdf
C Axial series Axial Horizontal pin pitch 15mm  length 12mm diameter 7.5mm
0
2
2
Capacitor_THT
C_Axial_L12.0mm_D7.5mm_P20.00mm_Horizontal
C, Axial series, Axial, Horizontal, pin pitch=20mm, , length*diameter=12*7.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B300/STYROFLEX.pdf
C Axial series Axial Horizontal pin pitch 20mm  length 12mm diameter 7.5mm
0
2
2
Capacitor_THT
C_Axial_L12.0mm_D8.5mm_P15.00mm_Horizontal
C, Axial series, Axial, Horizontal, pin pitch=15mm, , length*diameter=12*8.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B300/STYROFLEX.pdf
C Axial series Axial Horizontal pin pitch 15mm  length 12mm diameter 8.5mm
0
2
2
Capacitor_THT
C_Axial_L12.0mm_D8.5mm_P20.00mm_Horizontal
C, Axial series, Axial, Horizontal, pin pitch=20mm, , length*diameter=12*8.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B300/STYROFLEX.pdf
C Axial series Axial Horizontal pin pitch 20mm  length 12mm diameter 8.5mm
0
2
2
Capacitor_THT
C_Axial_L12.0mm_D9.5mm_P15.00mm_Horizontal
C, Axial series, Axial, Horizontal, pin pitch=15mm, , length*diameter=12*9.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B300/STYROFLEX.pdf
C Axial series Axial Horizontal pin pitch 15mm  length 12mm diameter 9.5mm
0
2
2
Capacitor_THT
C_Axial_L12.0mm_D9.5mm_P20.00mm_Horizontal
C, Axial series, Axial, Horizontal, pin pitch=20mm, , length*diameter=12*9.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B300/STYROFLEX.pdf
C Axial series Axial Horizontal pin pitch 20mm  length 12mm diameter 9.5mm
0
2
2
Capacitor_THT
C_Axial_L12.0mm_D10.5mm_P15.00mm_Horizontal
C, Axial series, Axial, Horizontal, pin pitch=15mm, , length*diameter=12*10.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B300/STYROFLEX.pdf
C Axial series Axial Horizontal pin pitch 15mm  length 12mm diameter 10.5mm
0
2
2
Capacitor_THT
C_Axial_L12.0mm_D10.5mm_P20.00mm_Horizontal
C, Axial series, Axial, Horizontal, pin pitch=20mm, , length*diameter=12*10.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B300/STYROFLEX.pdf
C Axial series Axial Horizontal pin pitch 20mm  length 12mm diameter 10.5mm
0
2
2
Capacitor_THT
C_Axial_L17.0mm_D6.5mm_P20.00mm_Horizontal
C, Axial series, Axial, Horizontal, pin pitch=20mm, , length*diameter=17*6.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B300/STYROFLEX.pdf
C Axial series Axial Horizontal pin pitch 20mm  length 17mm diameter 6.5mm
0
2
2
Capacitor_THT
C_Axial_L17.0mm_D6.5mm_P25.00mm_Horizontal
C, Axial series, Axial, Horizontal, pin pitch=25mm, , length*diameter=17*6.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B300/STYROFLEX.pdf
C Axial series Axial Horizontal pin pitch 25mm  length 17mm diameter 6.5mm
0
2
2
Capacitor_THT
C_Axial_L17.0mm_D7.0mm_P20.00mm_Horizontal
C, Axial series, Axial, Horizontal, pin pitch=20mm, , length*diameter=17*7.0mm^2, http://cdn-reichelt.de/documents/datenblatt/B300/STYROFLEX.pdf
C Axial series Axial Horizontal pin pitch 20mm  length 17mm diameter 7.0mm
0
2
2
Capacitor_THT
C_Axial_L17.0mm_D7.0mm_P25.00mm_Horizontal
C, Axial series, Axial, Horizontal, pin pitch=25mm, , length*diameter=17*7.0mm^2, http://cdn-reichelt.de/documents/datenblatt/B300/STYROFLEX.pdf
C Axial series Axial Horizontal pin pitch 25mm  length 17mm diameter 7.0mm
0
2
2
Capacitor_THT
C_Axial_L19.0mm_D7.5mm_P25.00mm_Horizontal
C, Axial series, Axial, Horizontal, pin pitch=25mm, , length*diameter=19*7.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B300/STYROFLEX.pdf
C Axial series Axial Horizontal pin pitch 25mm  length 19mm diameter 7.5mm
0
2
2
Capacitor_THT
C_Axial_L19.0mm_D8.0mm_P25.00mm_Horizontal
C, Axial series, Axial, Horizontal, pin pitch=25mm, , length*diameter=19*8.0mm^2, http://cdn-reichelt.de/documents/datenblatt/B300/STYROFLEX.pdf
C Axial series Axial Horizontal pin pitch 25mm  length 19mm diameter 8.0mm
0
2
2
Capacitor_THT
C_Axial_L19.0mm_D9.0mm_P25.00mm_Horizontal
C, Axial series, Axial, Horizontal, pin pitch=25mm, , length*diameter=19*9mm^2, http://cdn-reichelt.de/documents/datenblatt/B300/STYROFLEX.pdf
C Axial series Axial Horizontal pin pitch 25mm  length 19mm diameter 9mm
0
2
2
Capacitor_THT
C_Axial_L19.0mm_D9.5mm_P25.00mm_Horizontal
C, Axial series, Axial, Horizontal, pin pitch=25mm, , length*diameter=19*9.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B300/STYROFLEX.pdf
C Axial series Axial Horizontal pin pitch 25mm  length 19mm diameter 9.5mm
0
2
2
Capacitor_THT
C_Axial_L22.0mm_D9.5mm_P27.50mm_Horizontal
C, Axial series, Axial, Horizontal, pin pitch=27.5mm, , length*diameter=22*9.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B300/STYROFLEX.pdf
C Axial series Axial Horizontal pin pitch 27.5mm  length 22mm diameter 9.5mm
0
2
2
Capacitor_THT
C_Axial_L22.0mm_D10.5mm_P27.50mm_Horizontal
C, Axial series, Axial, Horizontal, pin pitch=27.5mm, , length*diameter=22*10.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B300/STYROFLEX.pdf
C Axial series Axial Horizontal pin pitch 27.5mm  length 22mm diameter 10.5mm
0
2
2
Capacitor_THT
C_Disc_D3.0mm_W1.6mm_P2.50mm
C, Disc series, Radial, pin pitch=2.50mm, , diameter*width=3.0*1.6mm^2, Capacitor, http://www.vishay.com/docs/45233/krseries.pdf
C Disc series Radial pin pitch 2.50mm  diameter 3.0mm width 1.6mm Capacitor
0
2
2
Capacitor_THT
C_Disc_D3.0mm_W2.0mm_P2.50mm
C, Disc series, Radial, pin pitch=2.50mm, , diameter*width=3*2mm^2, Capacitor
C Disc series Radial pin pitch 2.50mm  diameter 3mm width 2mm Capacitor
0
2
2
Capacitor_THT
C_Disc_D3.4mm_W2.1mm_P2.50mm
C, Disc series, Radial, pin pitch=2.50mm, , diameter*width=3.4*2.1mm^2, Capacitor, http://www.vishay.com/docs/45233/krseries.pdf
C Disc series Radial pin pitch 2.50mm  diameter 3.4mm width 2.1mm Capacitor
0
2
2
Capacitor_THT
C_Disc_D3.8mm_W2.6mm_P2.50mm
C, Disc series, Radial, pin pitch=2.50mm, , diameter*width=3.8*2.6mm^2, Capacitor, http://www.vishay.com/docs/45233/krseries.pdf
C Disc series Radial pin pitch 2.50mm  diameter 3.8mm width 2.6mm Capacitor
0
2
2
Capacitor_THT
C_Disc_D4.3mm_W1.9mm_P5.00mm
C, Disc series, Radial, pin pitch=5.00mm, , diameter*width=4.3*1.9mm^2, Capacitor, http://www.vishay.com/docs/45233/krseries.pdf
C Disc series Radial pin pitch 5.00mm  diameter 4.3mm width 1.9mm Capacitor
0
2
2
Capacitor_THT
C_Disc_D4.7mm_W2.5mm_P5.00mm
C, Disc series, Radial, pin pitch=5.00mm, , diameter*width=4.7*2.5mm^2, Capacitor, http://www.vishay.com/docs/45233/krseries.pdf
C Disc series Radial pin pitch 5.00mm  diameter 4.7mm width 2.5mm Capacitor
0
2
2
Capacitor_THT
C_Disc_D5.0mm_W2.5mm_P2.50mm
C, Disc series, Radial, pin pitch=2.50mm, , diameter*width=5*2.5mm^2, Capacitor, http://cdn-reichelt.de/documents/datenblatt/B300/DS_KERKO_TC.pdf
C Disc series Radial pin pitch 2.50mm  diameter 5mm width 2.5mm Capacitor
0
2
2
Capacitor_THT
C_Disc_D5.0mm_W2.5mm_P5.00mm
C, Disc series, Radial, pin pitch=5.00mm, , diameter*width=5*2.5mm^2, Capacitor, http://cdn-reichelt.de/documents/datenblatt/B300/DS_KERKO_TC.pdf
C Disc series Radial pin pitch 5.00mm  diameter 5mm width 2.5mm Capacitor
0
2
2
Capacitor_THT
C_Disc_D5.1mm_W3.2mm_P5.00mm
C, Disc series, Radial, pin pitch=5.00mm, , diameter*width=5.1*3.2mm^2, Capacitor, http://www.vishay.com/docs/45233/krseries.pdf
C Disc series Radial pin pitch 5.00mm  diameter 5.1mm width 3.2mm Capacitor
0
2
2
Capacitor_THT
C_Disc_D6.0mm_W2.5mm_P5.00mm
C, Disc series, Radial, pin pitch=5.00mm, , diameter*width=6*2.5mm^2, Capacitor, http://cdn-reichelt.de/documents/datenblatt/B300/DS_KERKO_TC.pdf
C Disc series Radial pin pitch 5.00mm  diameter 6mm width 2.5mm Capacitor
0
2
2
Capacitor_THT
C_Disc_D6.0mm_W4.4mm_P5.00mm
C, Disc series, Radial, pin pitch=5.00mm, , diameter*width=6*4.4mm^2, Capacitor
C Disc series Radial pin pitch 5.00mm  diameter 6mm width 4.4mm Capacitor
0
2
2
Capacitor_THT
C_Disc_D7.0mm_W2.5mm_P5.00mm
C, Disc series, Radial, pin pitch=5.00mm, , diameter*width=7*2.5mm^2, Capacitor, http://cdn-reichelt.de/documents/datenblatt/B300/DS_KERKO_TC.pdf
C Disc series Radial pin pitch 5.00mm  diameter 7mm width 2.5mm Capacitor
0
2
2
Capacitor_THT
C_Disc_D7.5mm_W2.5mm_P5.00mm
C, Disc series, Radial, pin pitch=5.00mm, , diameter*width=7.5*2.5mm^2, Capacitor, http://www.vishay.com/docs/28535/vy2series.pdf
C Disc series Radial pin pitch 5.00mm  diameter 7.5mm width 2.5mm Capacitor
0
2
2
Capacitor_THT
C_Disc_D7.5mm_W4.4mm_P5.00mm
C, Disc series, Radial, pin pitch=5.00mm, , diameter*width=7.5*4.4mm^2, Capacitor
C Disc series Radial pin pitch 5.00mm  diameter 7.5mm width 4.4mm Capacitor
0
2
2
Capacitor_THT
C_Disc_D7.5mm_W5.0mm_P5.00mm
C, Disc series, Radial, pin pitch=5.00mm, , diameter*width=7.5*5.0mm^2, Capacitor, http://www.vishay.com/docs/28535/vy2series.pdf
C Disc series Radial pin pitch 5.00mm  diameter 7.5mm width 5.0mm Capacitor
0
2
2
Capacitor_THT
C_Disc_D7.5mm_W5.0mm_P7.50mm
C, Disc series, Radial, pin pitch=7.50mm, , diameter*width=7.5*5.0mm^2, Capacitor, http://www.vishay.com/docs/28535/vy2series.pdf
C Disc series Radial pin pitch 7.50mm  diameter 7.5mm width 5.0mm Capacitor
0
2
2
Capacitor_THT
C_Disc_D7.5mm_W5.0mm_P10.00mm
C, Disc series, Radial, pin pitch=10.00mm, , diameter*width=7.5*5.0mm^2, Capacitor, http://www.vishay.com/docs/28535/vy2series.pdf
C Disc series Radial pin pitch 10.00mm  diameter 7.5mm width 5.0mm Capacitor
0
2
2
Capacitor_THT
C_Disc_D8.0mm_W2.5mm_P5.00mm
C, Disc series, Radial, pin pitch=5.00mm, , diameter*width=8*2.5mm^2, Capacitor, http://cdn-reichelt.de/documents/datenblatt/B300/DS_KERKO_TC.pdf
C Disc series Radial pin pitch 5.00mm  diameter 8mm width 2.5mm Capacitor
0
2
2
Capacitor_THT
C_Disc_D8.0mm_W5.0mm_P5.00mm
C, Disc series, Radial, pin pitch=5.00mm, , diameter*width=8*5.0mm^2, Capacitor, http://www.vishay.com/docs/28535/vy2series.pdf
C Disc series Radial pin pitch 5.00mm  diameter 8mm width 5.0mm Capacitor
0
2
2
Capacitor_THT
C_Disc_D8.0mm_W5.0mm_P7.50mm
C, Disc series, Radial, pin pitch=7.50mm, , diameter*width=8*5.0mm^2, Capacitor, http://www.vishay.com/docs/28535/vy2series.pdf
C Disc series Radial pin pitch 7.50mm  diameter 8mm width 5.0mm Capacitor
0
2
2
Capacitor_THT
C_Disc_D8.0mm_W5.0mm_P10.00mm
C, Disc series, Radial, pin pitch=10.00mm, , diameter*width=8*5.0mm^2, Capacitor, http://www.vishay.com/docs/28535/vy2series.pdf
C Disc series Radial pin pitch 10.00mm  diameter 8mm width 5.0mm Capacitor
0
2
2
Capacitor_THT
C_Disc_D9.0mm_W2.5mm_P5.00mm
C, Disc series, Radial, pin pitch=5.00mm, , diameter*width=9*2.5mm^2, Capacitor, http://cdn-reichelt.de/documents/datenblatt/B300/DS_KERKO_TC.pdf
C Disc series Radial pin pitch 5.00mm  diameter 9mm width 2.5mm Capacitor
0
2
2
Capacitor_THT
C_Disc_D9.0mm_W5.0mm_P5.00mm
C, Disc series, Radial, pin pitch=5.00mm, , diameter*width=9*5.0mm^2, Capacitor, http://www.vishay.com/docs/28535/vy2series.pdf
C Disc series Radial pin pitch 5.00mm  diameter 9mm width 5.0mm Capacitor
0
2
2
Capacitor_THT
C_Disc_D9.0mm_W5.0mm_P7.50mm
C, Disc series, Radial, pin pitch=7.50mm, , diameter*width=9*5.0mm^2, Capacitor, http://www.vishay.com/docs/28535/vy2series.pdf
C Disc series Radial pin pitch 7.50mm  diameter 9mm width 5.0mm Capacitor
0
2
2
Capacitor_THT
C_Disc_D9.0mm_W5.0mm_P10.00mm
C, Disc series, Radial, pin pitch=10.00mm, , diameter*width=9*5.0mm^2, Capacitor, http://www.vishay.com/docs/28535/vy2series.pdf
C Disc series Radial pin pitch 10.00mm  diameter 9mm width 5.0mm Capacitor
0
2
2
Capacitor_THT
C_Disc_D10.0mm_W2.5mm_P5.00mm
C, Disc series, Radial, pin pitch=5.00mm, , diameter*width=10*2.5mm^2, Capacitor, http://cdn-reichelt.de/documents/datenblatt/B300/DS_KERKO_TC.pdf
C Disc series Radial pin pitch 5.00mm  diameter 10mm width 2.5mm Capacitor
0
2
2
Capacitor_THT
C_Disc_D10.5mm_W5.0mm_P5.00mm
C, Disc series, Radial, pin pitch=5.00mm, , diameter*width=10.5*5.0mm^2, Capacitor, http://www.vishay.com/docs/28535/vy2series.pdf
C Disc series Radial pin pitch 5.00mm  diameter 10.5mm width 5.0mm Capacitor
0
2
2
Capacitor_THT
C_Disc_D10.5mm_W5.0mm_P7.50mm
C, Disc series, Radial, pin pitch=7.50mm, , diameter*width=10.5*5.0mm^2, Capacitor, http://www.vishay.com/docs/28535/vy2series.pdf
C Disc series Radial pin pitch 7.50mm  diameter 10.5mm width 5.0mm Capacitor
0
2
2
Capacitor_THT
C_Disc_D10.5mm_W5.0mm_P10.00mm
C, Disc series, Radial, pin pitch=10.00mm, , diameter*width=10.5*5.0mm^2, Capacitor, http://www.vishay.com/docs/28535/vy2series.pdf
C Disc series Radial pin pitch 10.00mm  diameter 10.5mm width 5.0mm Capacitor
0
2
2
Capacitor_THT
C_Disc_D11.0mm_W5.0mm_P5.00mm
C, Disc series, Radial, pin pitch=5.00mm, , diameter*width=11*5.0mm^2, Capacitor, http://www.vishay.com/docs/28535/vy2series.pdf
C Disc series Radial pin pitch 5.00mm  diameter 11mm width 5.0mm Capacitor
0
2
2
Capacitor_THT
C_Disc_D11.0mm_W5.0mm_P7.50mm
C, Disc series, Radial, pin pitch=7.50mm, , diameter*width=11*5.0mm^2, Capacitor, http://www.vishay.com/docs/28535/vy2series.pdf
C Disc series Radial pin pitch 7.50mm  diameter 11mm width 5.0mm Capacitor
0
2
2
Capacitor_THT
C_Disc_D11.0mm_W5.0mm_P10.00mm
C, Disc series, Radial, pin pitch=10.00mm, , diameter*width=11*5.0mm^2, Capacitor, http://www.vishay.com/docs/28535/vy2series.pdf
C Disc series Radial pin pitch 10.00mm  diameter 11mm width 5.0mm Capacitor
0
2
2
Capacitor_THT
C_Disc_D12.0mm_W4.4mm_P7.75mm
C, Disc series, Radial, pin pitch=7.75mm, , diameter*width=12*4.4mm^2, Capacitor
C Disc series Radial pin pitch 7.75mm  diameter 12mm width 4.4mm Capacitor
0
2
2
Capacitor_THT
C_Disc_D12.5mm_W5.0mm_P7.50mm
C, Disc series, Radial, pin pitch=7.50mm, , diameter*width=12.5*5.0mm^2, Capacitor, http://www.vishay.com/docs/28535/vy2series.pdf
C Disc series Radial pin pitch 7.50mm  diameter 12.5mm width 5.0mm Capacitor
0
2
2
Capacitor_THT
C_Disc_D12.5mm_W5.0mm_P10.00mm
C, Disc series, Radial, pin pitch=10.00mm, , diameter*width=12.5*5.0mm^2, Capacitor, http://www.vishay.com/docs/28535/vy2series.pdf
C Disc series Radial pin pitch 10.00mm  diameter 12.5mm width 5.0mm Capacitor
0
2
2
Capacitor_THT
C_Disc_D14.5mm_W5.0mm_P7.50mm
C, Disc series, Radial, pin pitch=7.50mm, , diameter*width=14.5*5.0mm^2, Capacitor, http://www.vishay.com/docs/28535/vy2series.pdf
C Disc series Radial pin pitch 7.50mm  diameter 14.5mm width 5.0mm Capacitor
0
2
2
Capacitor_THT
C_Disc_D14.5mm_W5.0mm_P10.00mm
C, Disc series, Radial, pin pitch=10.00mm, , diameter*width=14.5*5.0mm^2, Capacitor, http://www.vishay.com/docs/28535/vy2series.pdf
C Disc series Radial pin pitch 10.00mm  diameter 14.5mm width 5.0mm Capacitor
0
2
2
Capacitor_THT
C_Disc_D16.0mm_W5.0mm_P7.50mm
C, Disc series, Radial, pin pitch=7.50mm, , diameter*width=16.0*5.0mm^2, Capacitor, http://www.vishay.com/docs/28535/vy2series.pdf
C Disc series Radial pin pitch 7.50mm  diameter 16.0mm width 5.0mm Capacitor
0
2
2
Capacitor_THT
C_Disc_D16.0mm_W5.0mm_P10.00mm
C, Disc series, Radial, pin pitch=10.00mm, , diameter*width=16.0*5.0mm^2, Capacitor, http://www.vishay.com/docs/28535/vy2series.pdf
C Disc series Radial pin pitch 10.00mm  diameter 16.0mm width 5.0mm Capacitor
0
2
2
Capacitor_THT
C_Radial_D4.0mm_H5.0mm_P1.50mm
C, Radial series, Radial, pin pitch=1.50mm, diameter=4mm, height=5mm, Non-Polar Electrolytic Capacitor
C Radial series Radial pin pitch 1.50mm diameter 4mm height 5mm Non-Polar Electrolytic Capacitor
0
2
2
Capacitor_THT
C_Radial_D4.0mm_H7.0mm_P1.50mm
C, Radial series, Radial, pin pitch=1.50mm, diameter=4mm, height=7mm, Non-Polar Electrolytic Capacitor
C Radial series Radial pin pitch 1.50mm diameter 4mm height 7mm Non-Polar Electrolytic Capacitor
0
2
2
Capacitor_THT
C_Radial_D5.0mm_H5.0mm_P2.00mm
C, Radial series, Radial, pin pitch=2.00mm, diameter=5mm, height=5mm, Non-Polar Electrolytic Capacitor
C Radial series Radial pin pitch 2.00mm diameter 5mm height 5mm Non-Polar Electrolytic Capacitor
0
2
2
Capacitor_THT
C_Radial_D5.0mm_H7.0mm_P2.00mm
C, Radial series, Radial, pin pitch=2.00mm, diameter=5mm, height=7mm, Non-Polar Electrolytic Capacitor
C Radial series Radial pin pitch 2.00mm diameter 5mm height 7mm Non-Polar Electrolytic Capacitor
0
2
2
Capacitor_THT
C_Radial_D5.0mm_H11.0mm_P2.00mm
C, Radial series, Radial, pin pitch=2.00mm, diameter=5mm, height=11mm, Non-Polar Electrolytic Capacitor
C Radial series Radial pin pitch 2.00mm diameter 5mm height 11mm Non-Polar Electrolytic Capacitor
0
2
2
Capacitor_THT
C_Radial_D6.3mm_H5.0mm_P2.50mm
C, Radial series, Radial, pin pitch=2.50mm, diameter=6.3mm, height=5mm, Non-Polar Electrolytic Capacitor
C Radial series Radial pin pitch 2.50mm diameter 6.3mm height 5mm Non-Polar Electrolytic Capacitor
0
2
2
Capacitor_THT
C_Radial_D6.3mm_H7.0mm_P2.50mm
C, Radial series, Radial, pin pitch=2.50mm, diameter=6.3mm, height=7mm, Non-Polar Electrolytic Capacitor
C Radial series Radial pin pitch 2.50mm diameter 6.3mm height 7mm Non-Polar Electrolytic Capacitor
0
2
2
Capacitor_THT
C_Radial_D6.3mm_H11.0mm_P2.50mm
C, Radial series, Radial, pin pitch=2.50mm, diameter=6.3mm, height=11mm, Non-Polar Electrolytic Capacitor
C Radial series Radial pin pitch 2.50mm diameter 6.3mm height 11mm Non-Polar Electrolytic Capacitor
0
2
2
Capacitor_THT
C_Radial_D8.0mm_H7.0mm_P3.50mm
C, Radial series, Radial, pin pitch=3.50mm, diameter=8mm, height=7mm, Non-Polar Electrolytic Capacitor
C Radial series Radial pin pitch 3.50mm diameter 8mm height 7mm Non-Polar Electrolytic Capacitor
0
2
2
Capacitor_THT
C_Radial_D8.0mm_H11.5mm_P3.50mm
C, Radial series, Radial, pin pitch=3.50mm, diameter=8mm, height=11.5mm, Non-Polar Electrolytic Capacitor
C Radial series Radial pin pitch 3.50mm diameter 8mm height 11.5mm Non-Polar Electrolytic Capacitor
0
2
2
Capacitor_THT
C_Radial_D10.0mm_H12.5mm_P5.00mm
C, Radial series, Radial, pin pitch=5.00mm, diameter=10mm, height=12.5mm, Non-Polar Electrolytic Capacitor
C Radial series Radial pin pitch 5.00mm diameter 10mm height 12.5mm Non-Polar Electrolytic Capacitor
0
2
2
Capacitor_THT
C_Radial_D10.0mm_H16.0mm_P5.00mm
C, Radial series, Radial, pin pitch=5.00mm, diameter=10mm, height=16mm, Non-Polar Electrolytic Capacitor
C Radial series Radial pin pitch 5.00mm diameter 10mm height 16mm Non-Polar Electrolytic Capacitor
0
2
2
Capacitor_THT
C_Radial_D10.0mm_H20.0mm_P5.00mm
C, Radial series, Radial, pin pitch=5.00mm, diameter=10mm, height=20mm, Non-Polar Electrolytic Capacitor
C Radial series Radial pin pitch 5.00mm diameter 10mm height 20mm Non-Polar Electrolytic Capacitor
0
2
2
Capacitor_THT
C_Radial_D12.5mm_H20.0mm_P5.00mm
C, Radial series, Radial, pin pitch=5.00mm, diameter=12.5mm, height=20mm, Non-Polar Electrolytic Capacitor
C Radial series Radial pin pitch 5.00mm diameter 12.5mm height 20mm Non-Polar Electrolytic Capacitor
0
2
2
Capacitor_THT
C_Radial_D12.5mm_H25.0mm_P5.00mm
C, Radial series, Radial, pin pitch=5.00mm, diameter=12.5mm, height=25mm, Non-Polar Electrolytic Capacitor
C Radial series Radial pin pitch 5.00mm diameter 12.5mm height 25mm Non-Polar Electrolytic Capacitor
0
2
2
Capacitor_THT
C_Radial_D16.0mm_H25.0mm_P7.50mm
C, Radial series, Radial, pin pitch=7.50mm, diameter=16mm, height=25mm, Non-Polar Electrolytic Capacitor
C Radial series Radial pin pitch 7.50mm diameter 16mm height 25mm Non-Polar Electrolytic Capacitor
0
2
2
Capacitor_THT
C_Radial_D16.0mm_H31.5mm_P7.50mm
C, Radial series, Radial, pin pitch=7.50mm, diameter=16mm, height=31.5mm, Non-Polar Electrolytic Capacitor
C Radial series Radial pin pitch 7.50mm diameter 16mm height 31.5mm Non-Polar Electrolytic Capacitor
0
2
2
Capacitor_THT
C_Radial_D18.0mm_H35.5mm_P7.50mm
C, Radial series, Radial, pin pitch=7.50mm, diameter=18mm, height=35.5mm, Non-Polar Electrolytic Capacitor
C Radial series Radial pin pitch 7.50mm diameter 18mm height 35.5mm Non-Polar Electrolytic Capacitor
0
2
2
Capacitor_THT
C_Rect_L4.0mm_W2.5mm_P2.50mm
C, Rect series, Radial, pin pitch=2.50mm, , length*width=4*2.5mm^2, Capacitor
C Rect series Radial pin pitch 2.50mm  length 4mm width 2.5mm Capacitor
0
2
2
Capacitor_THT
C_Rect_L4.6mm_W2.0mm_P2.50mm_MKS02_FKP02
C, Rect series, Radial, pin pitch=2.50mm, , length*width=4.6*2mm^2, Capacitor, http://www.wima.de/DE/WIMA_MKS_02.pdf
C Rect series Radial pin pitch 2.50mm  length 4.6mm width 2mm Capacitor
0
2
2
Capacitor_THT
C_Rect_L4.6mm_W3.0mm_P2.50mm_MKS02_FKP02
C, Rect series, Radial, pin pitch=2.50mm, , length*width=4.6*3.0mm^2, Capacitor, http://www.wima.de/DE/WIMA_MKS_02.pdf
C Rect series Radial pin pitch 2.50mm  length 4.6mm width 3.0mm Capacitor
0
2
2
Capacitor_THT
C_Rect_L4.6mm_W3.8mm_P2.50mm_MKS02_FKP02
C, Rect series, Radial, pin pitch=2.50mm, , length*width=4.6*3.8mm^2, Capacitor, http://www.wima.de/DE/WIMA_MKS_02.pdf
C Rect series Radial pin pitch 2.50mm  length 4.6mm width 3.8mm Capacitor
0
2
2
Capacitor_THT
C_Rect_L4.6mm_W4.6mm_P2.50mm_MKS02_FKP02
C, Rect series, Radial, pin pitch=2.50mm, , length*width=4.6*4.6mm^2, Capacitor, http://www.wima.de/DE/WIMA_MKS_02.pdf
C Rect series Radial pin pitch 2.50mm  length 4.6mm width 4.6mm Capacitor
0
2
2
Capacitor_THT
C_Rect_L4.6mm_W5.5mm_P2.50mm_MKS02_FKP02
C, Rect series, Radial, pin pitch=2.50mm, , length*width=4.6*5.5mm^2, Capacitor, http://www.wima.de/DE/WIMA_MKS_02.pdf
C Rect series Radial pin pitch 2.50mm  length 4.6mm width 5.5mm Capacitor
0
2
2
Capacitor_THT
C_Rect_L7.0mm_W2.0mm_P5.00mm
C, Rect series, Radial, pin pitch=5.00mm, , length*width=7*2mm^2, Capacitor
C Rect series Radial pin pitch 5.00mm  length 7mm width 2mm Capacitor
0
2
2
Capacitor_THT
C_Rect_L7.0mm_W2.5mm_P5.00mm
C, Rect series, Radial, pin pitch=5.00mm, , length*width=7*2.5mm^2, Capacitor
C Rect series Radial pin pitch 5.00mm  length 7mm width 2.5mm Capacitor
0
2
2
Capacitor_THT
C_Rect_L7.0mm_W3.5mm_P2.50mm_P5.00mm
C, Rect series, Radial, pin pitch=2.50mm 5.00mm, , length*width=7*3.5mm^2, Capacitor
C Rect series Radial pin pitch 2.50mm 5.00mm  length 7mm width 3.5mm Capacitor
0
4
2
Capacitor_THT
C_Rect_L7.0mm_W3.5mm_P5.00mm
C, Rect series, Radial, pin pitch=5.00mm, , length*width=7*3.5mm^2, Capacitor
C Rect series Radial pin pitch 5.00mm  length 7mm width 3.5mm Capacitor
0
2
2
Capacitor_THT
C_Rect_L7.0mm_W4.5mm_P5.00mm
C, Rect series, Radial, pin pitch=5.00mm, , length*width=7*4.5mm^2, Capacitor
C Rect series Radial pin pitch 5.00mm  length 7mm width 4.5mm Capacitor
0
2
2
Capacitor_THT
C_Rect_L7.0mm_W6.0mm_P5.00mm
C, Rect series, Radial, pin pitch=5.00mm, , length*width=7*6mm^2, Capacitor
C Rect series Radial pin pitch 5.00mm  length 7mm width 6mm Capacitor
0
2
2
Capacitor_THT
C_Rect_L7.0mm_W6.5mm_P5.00mm
C, Rect series, Radial, pin pitch=5.00mm, , length*width=7*6.5mm^2, Capacitor
C Rect series Radial pin pitch 5.00mm  length 7mm width 6.5mm Capacitor
0
2
2
Capacitor_THT
C_Rect_L7.2mm_W2.5mm_P5.00mm_FKS2_FKP2_MKS2_MKP2
C, Rect series, Radial, pin pitch=5.00mm, , length*width=7.2*2.5mm^2, Capacitor, http://www.wima.com/EN/WIMA_FKS_2.pdf
C Rect series Radial pin pitch 5.00mm  length 7.2mm width 2.5mm Capacitor
0
2
2
Capacitor_THT
C_Rect_L7.2mm_W3.0mm_P5.00mm_FKS2_FKP2_MKS2_MKP2
C, Rect series, Radial, pin pitch=5.00mm, , length*width=7.2*3.0mm^2, Capacitor, http://www.wima.com/EN/WIMA_FKS_2.pdf
C Rect series Radial pin pitch 5.00mm  length 7.2mm width 3.0mm Capacitor
0
2
2
Capacitor_THT
C_Rect_L7.2mm_W3.5mm_P5.00mm_FKS2_FKP2_MKS2_MKP2
C, Rect series, Radial, pin pitch=5.00mm, , length*width=7.2*3.5mm^2, Capacitor, http://www.wima.com/EN/WIMA_FKS_2.pdf
C Rect series Radial pin pitch 5.00mm  length 7.2mm width 3.5mm Capacitor
0
2
2
Capacitor_THT
C_Rect_L7.2mm_W4.5mm_P5.00mm_FKS2_FKP2_MKS2_MKP2
C, Rect series, Radial, pin pitch=5.00mm, , length*width=7.2*4.5mm^2, Capacitor, http://www.wima.com/EN/WIMA_FKS_2.pdf
C Rect series Radial pin pitch 5.00mm  length 7.2mm width 4.5mm Capacitor
0
2
2
Capacitor_THT
C_Rect_L7.2mm_W5.5mm_P5.00mm_FKS2_FKP2_MKS2_MKP2
C, Rect series, Radial, pin pitch=5.00mm, , length*width=7.2*5.5mm^2, Capacitor, http://www.wima.com/EN/WIMA_FKS_2.pdf
C Rect series Radial pin pitch 5.00mm  length 7.2mm width 5.5mm Capacitor
0
2
2
Capacitor_THT
C_Rect_L7.2mm_W7.2mm_P5.00mm_FKS2_FKP2_MKS2_MKP2
C, Rect series, Radial, pin pitch=5.00mm, , length*width=7.2*7.2mm^2, Capacitor, http://www.wima.com/EN/WIMA_FKS_2.pdf
C Rect series Radial pin pitch 5.00mm  length 7.2mm width 7.2mm Capacitor
0
2
2
Capacitor_THT
C_Rect_L7.2mm_W8.5mm_P5.00mm_FKP2_FKP2_MKS2_MKP2
C, Rect series, Radial, pin pitch=5.00mm, , length*width=7.2*8.5mm^2, Capacitor, http://www.wima.com/EN/WIMA_FKS_2.pdf
C Rect series Radial pin pitch 5.00mm  length 7.2mm width 8.5mm Capacitor
0
2
2
Capacitor_THT
C_Rect_L7.2mm_W11.0mm_P5.00mm_FKS2_FKP2_MKS2_MKP2
C, Rect series, Radial, pin pitch=5.00mm, , length*width=7.2*11mm^2, Capacitor, http://www.wima.com/EN/WIMA_FKS_2.pdf
C Rect series Radial pin pitch 5.00mm  length 7.2mm width 11mm Capacitor
0
2
2
Capacitor_THT
C_Rect_L7.5mm_W6.5mm_P5.00mm
C, Rect series, Radial, pin pitch=5.00mm, , length*width=7.5*6.5mm^2, Capacitor
C Rect series Radial pin pitch 5.00mm  length 7.5mm width 6.5mm Capacitor
0
2
2
Capacitor_THT
C_Rect_L9.0mm_W2.5mm_P7.50mm_MKT
C, Rect series, Radial, pin pitch=7.50mm, , length*width=9*2.5mm^2, Capacitor, https://en.tdk.eu/inf/20/20/db/fc_2009/MKT_B32560_564.pdf
C Rect series Radial pin pitch 7.50mm  length 9mm width 2.5mm Capacitor
0
2
2
Capacitor_THT
C_Rect_L9.0mm_W2.6mm_P7.50mm_MKT
C, Rect series, Radial, pin pitch=7.50mm, , length*width=9*2.6mm^2, Capacitor, https://en.tdk.eu/inf/20/20/db/fc_2009/MKT_B32560_564.pdf
C Rect series Radial pin pitch 7.50mm  length 9mm width 2.6mm Capacitor
0
2
2
Capacitor_THT
C_Rect_L9.0mm_W2.7mm_P7.50mm_MKT
C, Rect series, Radial, pin pitch=7.50mm, , length*width=9*2.7mm^2, Capacitor, https://en.tdk.eu/inf/20/20/db/fc_2009/MKT_B32560_564.pdf
C Rect series Radial pin pitch 7.50mm  length 9mm width 2.7mm Capacitor
0
2
2
Capacitor_THT
C_Rect_L9.0mm_W3.2mm_P7.50mm_MKT
C, Rect series, Radial, pin pitch=7.50mm, , length*width=9*3.2mm^2, Capacitor, https://en.tdk.eu/inf/20/20/db/fc_2009/MKT_B32560_564.pdf
C Rect series Radial pin pitch 7.50mm  length 9mm width 3.2mm Capacitor
0
2
2
Capacitor_THT
C_Rect_L9.0mm_W3.3mm_P7.50mm_MKT
C, Rect series, Radial, pin pitch=7.50mm, , length*width=9*3.3mm^2, Capacitor, https://en.tdk.eu/inf/20/20/db/fc_2009/MKT_B32560_564.pdf
C Rect series Radial pin pitch 7.50mm  length 9mm width 3.3mm Capacitor
0
2
2
Capacitor_THT
C_Rect_L9.0mm_W3.4mm_P7.50mm_MKT
C, Rect series, Radial, pin pitch=7.50mm, , length*width=9*3.4mm^2, Capacitor, https://en.tdk.eu/inf/20/20/db/fc_2009/MKT_B32560_564.pdf
C Rect series Radial pin pitch 7.50mm  length 9mm width 3.4mm Capacitor
0
2
2
Capacitor_THT
C_Rect_L9.0mm_W3.6mm_P7.50mm_MKT
C, Rect series, Radial, pin pitch=7.50mm, , length*width=9*3.6mm^2, Capacitor, https://en.tdk.eu/inf/20/20/db/fc_2009/MKT_B32560_564.pdf
C Rect series Radial pin pitch 7.50mm  length 9mm width 3.6mm Capacitor
0
2
2
Capacitor_THT
C_Rect_L9.0mm_W3.8mm_P7.50mm_MKT
C, Rect series, Radial, pin pitch=7.50mm, , length*width=9*3.8mm^2, Capacitor, https://en.tdk.eu/inf/20/20/db/fc_2009/MKT_B32560_564.pdf
C Rect series Radial pin pitch 7.50mm  length 9mm width 3.8mm Capacitor
0
2
2
Capacitor_THT
C_Rect_L9.0mm_W3.9mm_P7.50mm_MKT
C, Rect series, Radial, pin pitch=7.50mm, , length*width=9*3.9mm^2, Capacitor, https://en.tdk.eu/inf/20/20/db/fc_2009/MKT_B32560_564.pdf
C Rect series Radial pin pitch 7.50mm  length 9mm width 3.9mm Capacitor
0
2
2
Capacitor_THT
C_Rect_L9.0mm_W4.0mm_P7.50mm_MKT
C, Rect series, Radial, pin pitch=7.50mm, , length*width=9*4.0mm^2, Capacitor, https://en.tdk.eu/inf/20/20/db/fc_2009/MKT_B32560_564.pdf
C Rect series Radial pin pitch 7.50mm  length 9mm width 4.0mm Capacitor
0
2
2
Capacitor_THT
C_Rect_L9.0mm_W4.2mm_P7.50mm_MKT
C, Rect series, Radial, pin pitch=7.50mm, , length*width=9*4.2mm^2, Capacitor, https://en.tdk.eu/inf/20/20/db/fc_2009/MKT_B32560_564.pdf
C Rect series Radial pin pitch 7.50mm  length 9mm width 4.2mm Capacitor
0
2
2
Capacitor_THT
C_Rect_L9.0mm_W4.9mm_P7.50mm_MKT
C, Rect series, Radial, pin pitch=7.50mm, , length*width=9*4.9mm^2, Capacitor, https://en.tdk.eu/inf/20/20/db/fc_2009/MKT_B32560_564.pdf
C Rect series Radial pin pitch 7.50mm  length 9mm width 4.9mm Capacitor
0
2
2
Capacitor_THT
C_Rect_L9.0mm_W5.1mm_P7.50mm_MKT
C, Rect series, Radial, pin pitch=7.50mm, , length*width=9*5.1mm^2, Capacitor, https://en.tdk.eu/inf/20/20/db/fc_2009/MKT_B32560_564.pdf
C Rect series Radial pin pitch 7.50mm  length 9mm width 5.1mm Capacitor
0
2
2
Capacitor_THT
C_Rect_L9.0mm_W5.7mm_P7.50mm_MKT
C, Rect series, Radial, pin pitch=7.50mm, , length*width=9*5.7mm^2, Capacitor, https://en.tdk.eu/inf/20/20/db/fc_2009/MKT_B32560_564.pdf
C Rect series Radial pin pitch 7.50mm  length 9mm width 5.7mm Capacitor
0
2
2
Capacitor_THT
C_Rect_L9.0mm_W6.4mm_P7.50mm_MKT
C, Rect series, Radial, pin pitch=7.50mm, , length*width=9*6.4mm^2, Capacitor, https://en.tdk.eu/inf/20/20/db/fc_2009/MKT_B32560_564.pdf
C Rect series Radial pin pitch 7.50mm  length 9mm width 6.4mm Capacitor
0
2
2
Capacitor_THT
C_Rect_L9.0mm_W6.7mm_P7.50mm_MKT
C, Rect series, Radial, pin pitch=7.50mm, , length*width=9*6.7mm^2, Capacitor, https://en.tdk.eu/inf/20/20/db/fc_2009/MKT_B32560_564.pdf
C Rect series Radial pin pitch 7.50mm  length 9mm width 6.7mm Capacitor
0
2
2
Capacitor_THT
C_Rect_L9.0mm_W7.7mm_P7.50mm_MKT
C, Rect series, Radial, pin pitch=7.50mm, , length*width=9*7.7mm^2, Capacitor, https://en.tdk.eu/inf/20/20/db/fc_2009/MKT_B32560_564.pdf
C Rect series Radial pin pitch 7.50mm  length 9mm width 7.7mm Capacitor
0
2
2
Capacitor_THT
C_Rect_L9.0mm_W8.5mm_P7.50mm_MKT
C, Rect series, Radial, pin pitch=7.50mm, , length*width=9*8.5mm^2, Capacitor, https://en.tdk.eu/inf/20/20/db/fc_2009/MKT_B32560_564.pdf
C Rect series Radial pin pitch 7.50mm  length 9mm width 8.5mm Capacitor
0
2
2
Capacitor_THT
C_Rect_L9.0mm_W9.5mm_P7.50mm_MKT
C, Rect series, Radial, pin pitch=7.50mm, , length*width=9*9.5mm^2, Capacitor, https://en.tdk.eu/inf/20/20/db/fc_2009/MKT_B32560_564.pdf
C Rect series Radial pin pitch 7.50mm  length 9mm width 9.5mm Capacitor
0
2
2
Capacitor_THT
C_Rect_L9.0mm_W9.8mm_P7.50mm_MKT
C, Rect series, Radial, pin pitch=7.50mm, , length*width=9*9.8mm^2, Capacitor, https://en.tdk.eu/inf/20/20/db/fc_2009/MKT_B32560_564.pdf
C Rect series Radial pin pitch 7.50mm  length 9mm width 9.8mm Capacitor
0
2
2
Capacitor_THT
C_Rect_L10.0mm_W2.5mm_P7.50mm_MKS4
C, Rect series, Radial, pin pitch=7.50mm, , length*width=10*2.5mm^2, Capacitor, http://www.wima.com/EN/WIMA_MKS_4.pdf
C Rect series Radial pin pitch 7.50mm  length 10mm width 2.5mm Capacitor
0
2
2
Capacitor_THT
C_Rect_L10.0mm_W3.0mm_P7.50mm_FKS3_FKP3
C, Rect series, Radial, pin pitch=7.50mm, , length*width=10*3mm^2, Capacitor, http://www.wima.com/EN/WIMA_FKS_3.pdf
C Rect series Radial pin pitch 7.50mm  length 10mm width 3mm Capacitor
0
2
2
Capacitor_THT
C_Rect_L10.0mm_W3.0mm_P7.50mm_MKS4
C, Rect series, Radial, pin pitch=7.50mm, , length*width=10*3.0mm^2, Capacitor, http://www.wima.com/EN/WIMA_MKS_4.pdf
C Rect series Radial pin pitch 7.50mm  length 10mm width 3.0mm Capacitor
0
2
2
Capacitor_THT
C_Rect_L10.0mm_W4.0mm_P7.50mm_FKS3_FKP3
C, Rect series, Radial, pin pitch=7.50mm, , length*width=10*4mm^2, Capacitor, http://www.wima.com/EN/WIMA_FKS_3.pdf
C Rect series Radial pin pitch 7.50mm  length 10mm width 4mm Capacitor
0
2
2
Capacitor_THT
C_Rect_L10.0mm_W4.0mm_P7.50mm_MKS4
C, Rect series, Radial, pin pitch=7.50mm, , length*width=10*4.0mm^2, Capacitor, http://www.wima.com/EN/WIMA_MKS_4.pdf
C Rect series Radial pin pitch 7.50mm  length 10mm width 4.0mm Capacitor
0
2
2
Capacitor_THT
C_Rect_L10.0mm_W5.0mm_P5.00mm_P7.50mm
C, Rect series, Radial, pin pitch=5.00mm 7.50mm, , length*width=10*5mm^2, Capacitor
C Rect series Radial pin pitch 5.00mm 7.50mm  length 10mm width 5mm Capacitor
0
4
2
Capacitor_THT
C_Rect_L10.3mm_W4.5mm_P7.50mm_MKS4
C, Rect series, Radial, pin pitch=7.50mm, , length*width=10.3*4.5mm^2, Capacitor, http://www.wima.com/EN/WIMA_MKS_4.pdf
C Rect series Radial pin pitch 7.50mm  length 10.3mm width 4.5mm Capacitor
0
2
2
Capacitor_THT
C_Rect_L10.3mm_W5.0mm_P7.50mm_MKS4
C, Rect series, Radial, pin pitch=7.50mm, , length*width=10.3*5mm^2, Capacitor, http://www.wima.com/EN/WIMA_MKS_4.pdf
C Rect series Radial pin pitch 7.50mm  length 10.3mm width 5mm Capacitor
0
2
2
Capacitor_THT
C_Rect_L10.3mm_W5.7mm_P7.50mm_MKS4
C, Rect series, Radial, pin pitch=7.50mm, , length*width=10.3*5.7mm^2, Capacitor, http://www.wima.com/EN/WIMA_MKS_4.pdf
C Rect series Radial pin pitch 7.50mm  length 10.3mm width 5.7mm Capacitor
0
2
2
Capacitor_THT
C_Rect_L10.3mm_W7.2mm_P7.50mm_MKS4
C, Rect series, Radial, pin pitch=7.50mm, , length*width=10.3*7.2mm^2, Capacitor, http://www.wima.com/EN/WIMA_MKS_4.pdf
C Rect series Radial pin pitch 7.50mm  length 10.3mm width 7.2mm Capacitor
0
2
2
Capacitor_THT
C_Rect_L11.0mm_W2.8mm_P10.00mm_MKT
C, Rect series, Radial, pin pitch=10.00mm, , length*width=11.0*2.8mm^2, Capacitor, https://en.tdk.eu/inf/20/20/db/fc_2009/MKT_B32560_564.pdf
C Rect series Radial pin pitch 10.00mm  length 11.0mm width 2.8mm Capacitor
0
2
2
Capacitor_THT
C_Rect_L11.0mm_W3.4mm_P10.00mm_MKT
C, Rect series, Radial, pin pitch=10.00mm, , length*width=11.0*3.4mm^2, Capacitor, https://en.tdk.eu/inf/20/20/db/fc_2009/MKT_B32560_564.pdf
C Rect series Radial pin pitch 10.00mm  length 11.0mm width 3.4mm Capacitor
0
2
2
Capacitor_THT
C_Rect_L11.0mm_W3.5mm_P10.00mm_MKT
C, Rect series, Radial, pin pitch=10.00mm, , length*width=11.0*3.5mm^2, Capacitor, https://en.tdk.eu/inf/20/20/db/fc_2009/MKT_B32560_564.pdf
C Rect series Radial pin pitch 10.00mm  length 11.0mm width 3.5mm Capacitor
0
2
2
Capacitor_THT
C_Rect_L11.0mm_W4.2mm_P10.00mm_MKT
C, Rect series, Radial, pin pitch=10.00mm, , length*width=11.0*4.2mm^2, Capacitor, https://en.tdk.eu/inf/20/20/db/fc_2009/MKT_B32560_564.pdf
C Rect series Radial pin pitch 10.00mm  length 11.0mm width 4.2mm Capacitor
0
2
2
Capacitor_THT
C_Rect_L11.0mm_W4.3mm_P10.00mm_MKT
C, Rect series, Radial, pin pitch=10.00mm, , length*width=11.0*4.3mm^2, Capacitor, https://en.tdk.eu/inf/20/20/db/fc_2009/MKT_B32560_564.pdf
C Rect series Radial pin pitch 10.00mm  length 11.0mm width 4.3mm Capacitor
0
2
2
Capacitor_THT
C_Rect_L11.0mm_W5.1mm_P10.00mm_MKT
C, Rect series, Radial, pin pitch=10.00mm, , length*width=11.0*5.1mm^2, Capacitor, https://en.tdk.eu/inf/20/20/db/fc_2009/MKT_B32560_564.pdf
C Rect series Radial pin pitch 10.00mm  length 11.0mm width 5.1mm Capacitor
0
2
2
Capacitor_THT
C_Rect_L11.0mm_W5.3mm_P10.00mm_MKT
C, Rect series, Radial, pin pitch=10.00mm, , length*width=11.0*5.3mm^2, Capacitor, https://en.tdk.eu/inf/20/20/db/fc_2009/MKT_B32560_564.pdf
C Rect series Radial pin pitch 10.00mm  length 11.0mm width 5.3mm Capacitor
0
2
2
Capacitor_THT
C_Rect_L11.0mm_W6.3mm_P10.00mm_MKT
C, Rect series, Radial, pin pitch=10.00mm, , length*width=11.0*6.3mm^2, Capacitor, https://en.tdk.eu/inf/20/20/db/fc_2009/MKT_B32560_564.pdf
C Rect series Radial pin pitch 10.00mm  length 11.0mm width 6.3mm Capacitor
0
2
2
Capacitor_THT
C_Rect_L11.0mm_W6.4mm_P10.00mm_MKT
C, Rect series, Radial, pin pitch=10.00mm, , length*width=11.0*6.4mm^2, Capacitor, https://en.tdk.eu/inf/20/20/db/fc_2009/MKT_B32560_564.pdf
C Rect series Radial pin pitch 10.00mm  length 11.0mm width 6.4mm Capacitor
0
2
2
Capacitor_THT
C_Rect_L11.0mm_W7.3mm_P10.00mm_MKT
C, Rect series, Radial, pin pitch=10.00mm, , length*width=11.0*7.3mm^2, Capacitor, https://en.tdk.eu/inf/20/20/db/fc_2009/MKT_B32560_564.pdf
C Rect series Radial pin pitch 10.00mm  length 11.0mm width 7.3mm Capacitor
0
2
2
Capacitor_THT
C_Rect_L11.0mm_W8.8mm_P10.00mm_MKT
C, Rect series, Radial, pin pitch=10.00mm, , length*width=11.0*8.8mm^2, Capacitor, https://en.tdk.eu/inf/20/20/db/fc_2009/MKT_B32560_564.pdf
C Rect series Radial pin pitch 10.00mm  length 11.0mm width 8.8mm Capacitor
0
2
2
Capacitor_THT
C_Rect_L11.5mm_W2.0mm_P10.00mm_MKT
C, Rect series, Radial, pin pitch=10.00mm, , length*width=11.5*2mm^2, Capacitor, https://en.tdk.eu/inf/20/20/db/fc_2009/MKT_B32560_564.pdf
C Rect series Radial pin pitch 10.00mm  length 11.5mm width 2mm Capacitor
0
2
2
Capacitor_THT
C_Rect_L11.5mm_W2.6mm_P10.00mm_MKT
C, Rect series, Radial, pin pitch=10.00mm, , length*width=11.5*2.6mm^2, Capacitor, https://en.tdk.eu/inf/20/20/db/fc_2009/MKT_B32560_564.pdf
C Rect series Radial pin pitch 10.00mm  length 11.5mm width 2.6mm Capacitor
0
2
2
Capacitor_THT
C_Rect_L11.5mm_W2.8mm_P10.00mm_MKT
C, Rect series, Radial, pin pitch=10.00mm, , length*width=11.5*2.8mm^2, Capacitor, https://en.tdk.eu/inf/20/20/db/fc_2009/MKT_B32560_564.pdf
C Rect series Radial pin pitch 10.00mm  length 11.5mm width 2.8mm Capacitor
0
2
2
Capacitor_THT
C_Rect_L11.5mm_W3.2mm_P10.00mm_MKT
C, Rect series, Radial, pin pitch=10.00mm, , length*width=11.5*3.2mm^2, Capacitor, https://en.tdk.eu/inf/20/20/db/fc_2009/MKT_B32560_564.pdf
C Rect series Radial pin pitch 10.00mm  length 11.5mm width 3.2mm Capacitor
0
2
2
Capacitor_THT
C_Rect_L11.5mm_W3.5mm_P10.00mm_MKT
C, Rect series, Radial, pin pitch=10.00mm, , length*width=11.5*3.5mm^2, Capacitor, https://en.tdk.eu/inf/20/20/db/fc_2009/MKT_B32560_564.pdf
C Rect series Radial pin pitch 10.00mm  length 11.5mm width 3.5mm Capacitor
0
2
2
Capacitor_THT
C_Rect_L11.5mm_W3.6mm_P10.00mm_MKT
C, Rect series, Radial, pin pitch=10.00mm, , length*width=11.5*3.6mm^2, Capacitor, https://en.tdk.eu/inf/20/20/db/fc_2009/MKT_B32560_564.pdf
C Rect series Radial pin pitch 10.00mm  length 11.5mm width 3.6mm Capacitor
0
2
2
Capacitor_THT
C_Rect_L11.5mm_W4.0mm_P10.00mm_MKT
C, Rect series, Radial, pin pitch=10.00mm, , length*width=11.5*4.0mm^2, Capacitor, https://en.tdk.eu/inf/20/20/db/fc_2009/MKT_B32560_564.pdf
C Rect series Radial pin pitch 10.00mm  length 11.5mm width 4.0mm Capacitor
0
2
2
Capacitor_THT
C_Rect_L11.5mm_W4.3mm_P10.00mm_MKT
C, Rect series, Radial, pin pitch=10.00mm, , length*width=11.5*4.3mm^2, Capacitor, https://en.tdk.eu/inf/20/20/db/fc_2009/MKT_B32560_564.pdf
C Rect series Radial pin pitch 10.00mm  length 11.5mm width 4.3mm Capacitor
0
2
2
Capacitor_THT
C_Rect_L11.5mm_W4.5mm_P10.00mm_MKT
C, Rect series, Radial, pin pitch=10.00mm, , length*width=11.5*4.5mm^2, Capacitor, https://en.tdk.eu/inf/20/20/db/fc_2009/MKT_B32560_564.pdf
C Rect series Radial pin pitch 10.00mm  length 11.5mm width 4.5mm Capacitor
0
2
2
Capacitor_THT
C_Rect_L11.5mm_W5.0mm_P10.00mm_MKT
C, Rect series, Radial, pin pitch=10.00mm, , length*width=11.5*5mm^2, Capacitor, https://en.tdk.eu/inf/20/20/db/fc_2009/MKT_B32560_564.pdf
C Rect series Radial pin pitch 10.00mm  length 11.5mm width 5mm Capacitor
0
2
2
Capacitor_THT
C_Rect_L11.5mm_W5.1mm_P10.00mm_MKT
C, Rect series, Radial, pin pitch=10.00mm, , length*width=11.5*5.1mm^2, Capacitor, https://en.tdk.eu/inf/20/20/db/fc_2009/MKT_B32560_564.pdf
C Rect series Radial pin pitch 10.00mm  length 11.5mm width 5.1mm Capacitor
0
2
2
Capacitor_THT
C_Rect_L11.5mm_W5.2mm_P10.00mm_MKT
C, Rect series, Radial, pin pitch=10.00mm, , length*width=11.5*5.2mm^2, Capacitor, https://en.tdk.eu/inf/20/20/db/fc_2009/MKT_B32560_564.pdf
C Rect series Radial pin pitch 10.00mm  length 11.5mm width 5.2mm Capacitor
0
2
2
Capacitor_THT
C_Rect_L11.5mm_W5.6mm_P10.00mm_MKT
C, Rect series, Radial, pin pitch=10.00mm, , length*width=11.5*5.6mm^2, Capacitor, https://en.tdk.eu/inf/20/20/db/fc_2009/MKT_B32560_564.pdf
C Rect series Radial pin pitch 10.00mm  length 11.5mm width 5.6mm Capacitor
0
2
2
Capacitor_THT
C_Rect_L11.5mm_W6.4mm_P10.00mm_MKT
C, Rect series, Radial, pin pitch=10.00mm, , length*width=11.5*6.4mm^2, Capacitor, https://en.tdk.eu/inf/20/20/db/fc_2009/MKT_B32560_564.pdf
C Rect series Radial pin pitch 10.00mm  length 11.5mm width 6.4mm Capacitor
0
2
2
Capacitor_THT
C_Rect_L11.5mm_W6.6mm_P10.00mm_MKT
C, Rect series, Radial, pin pitch=10.00mm, , length*width=11.5*6.6mm^2, Capacitor, https://en.tdk.eu/inf/20/20/db/fc_2009/MKT_B32560_564.pdf
C Rect series Radial pin pitch 10.00mm  length 11.5mm width 6.6mm Capacitor
0
2
2
Capacitor_THT
C_Rect_L11.5mm_W6.9mm_P10.00mm_MKT
C, Rect series, Radial, pin pitch=10.00mm, , length*width=11.5*6.9mm^2, Capacitor, https://en.tdk.eu/inf/20/20/db/fc_2009/MKT_B32560_564.pdf
C Rect series Radial pin pitch 10.00mm  length 11.5mm width 6.9mm Capacitor
0
2
2
Capacitor_THT
C_Rect_L11.5mm_W7.3mm_P10.00mm_MKT
C, Rect series, Radial, pin pitch=10.00mm, , length*width=11.5*7.3mm^2, Capacitor, https://en.tdk.eu/inf/20/20/db/fc_2009/MKT_B32560_564.pdf
C Rect series Radial pin pitch 10.00mm  length 11.5mm width 7.3mm Capacitor
0
2
2
Capacitor_THT
C_Rect_L11.5mm_W7.5mm_P10.00mm_MKT
C, Rect series, Radial, pin pitch=10.00mm, , length*width=11.5*7.5mm^2, Capacitor, https://en.tdk.eu/inf/20/20/db/fc_2009/MKT_B32560_564.pdf
C Rect series Radial pin pitch 10.00mm  length 11.5mm width 7.5mm Capacitor
0
2
2
Capacitor_THT
C_Rect_L11.5mm_W7.8mm_P10.00mm_MKT
C, Rect series, Radial, pin pitch=10.00mm, , length*width=11.5*7.8mm^2, Capacitor, https://en.tdk.eu/inf/20/20/db/fc_2009/MKT_B32560_564.pdf
C Rect series Radial pin pitch 10.00mm  length 11.5mm width 7.8mm Capacitor
0
2
2
Capacitor_THT
C_Rect_L11.5mm_W8.0mm_P10.00mm_MKT
C, Rect series, Radial, pin pitch=10.00mm, , length*width=11.5*8.0mm^2, Capacitor, https://en.tdk.eu/inf/20/20/db/fc_2009/MKT_B32560_564.pdf
C Rect series Radial pin pitch 10.00mm  length 11.5mm width 8.0mm Capacitor
0
2
2
Capacitor_THT
C_Rect_L11.5mm_W8.8mm_P10.00mm_MKT
C, Rect series, Radial, pin pitch=10.00mm, , length*width=11.5*8.8mm^2, Capacitor, https://en.tdk.eu/inf/20/20/db/fc_2009/MKT_B32560_564.pdf
C Rect series Radial pin pitch 10.00mm  length 11.5mm width 8.8mm Capacitor
0
2
2
Capacitor_THT
C_Rect_L11.5mm_W9.5mm_P10.00mm_MKT
C, Rect series, Radial, pin pitch=10.00mm, , length*width=11.5*9.5mm^2, Capacitor, https://en.tdk.eu/inf/20/20/db/fc_2009/MKT_B32560_564.pdf
C Rect series Radial pin pitch 10.00mm  length 11.5mm width 9.5mm Capacitor
0
2
2
Capacitor_THT
C_Rect_L11.5mm_W9.8mm_P10.00mm_MKT
C, Rect series, Radial, pin pitch=10.00mm, , length*width=11.5*9.8mm^2, Capacitor, https://en.tdk.eu/inf/20/20/db/fc_2009/MKT_B32560_564.pdf
C Rect series Radial pin pitch 10.00mm  length 11.5mm width 9.8mm Capacitor
0
2
2
Capacitor_THT
C_Rect_L13.0mm_W3.0mm_P10.00mm_FKS3_FKP3_MKS4
C, Rect series, Radial, pin pitch=10.00mm, , length*width=13*3mm^2, Capacitor, http://www.wima.com/EN/WIMA_FKS_3.pdf, http://www.wima.com/EN/WIMA_MKS_4.pdf
C Rect series Radial pin pitch 10.00mm  length 13mm width 3mm Capacitor
0
2
2
Capacitor_THT
C_Rect_L13.0mm_W4.0mm_P10.00mm_FKS3_FKP3_MKS4
C, Rect series, Radial, pin pitch=10.00mm, , length*width=13*4mm^2, Capacitor, http://www.wima.com/EN/WIMA_FKS_3.pdf, http://www.wima.com/EN/WIMA_MKS_4.pdf
C Rect series Radial pin pitch 10.00mm  length 13mm width 4mm Capacitor
0
2
2
Capacitor_THT
C_Rect_L13.0mm_W5.0mm_P10.00mm_FKS3_FKP3_MKS4
C, Rect series, Radial, pin pitch=10.00mm, , length*width=13*5mm^2, Capacitor, http://www.wima.com/EN/WIMA_FKS_3.pdf, http://www.wima.com/EN/WIMA_MKS_4.pdf
C Rect series Radial pin pitch 10.00mm  length 13mm width 5mm Capacitor
0
2
2
Capacitor_THT
C_Rect_L13.0mm_W6.0mm_P10.00mm_FKS3_FKP3_MKS4
C, Rect series, Radial, pin pitch=10.00mm, , length*width=13*6mm^2, Capacitor, http://www.wima.com/EN/WIMA_FKS_3.pdf, http://www.wima.com/EN/WIMA_MKS_4.pdf
C Rect series Radial pin pitch 10.00mm  length 13mm width 6mm Capacitor
0
2
2
Capacitor_THT
C_Rect_L13.0mm_W6.5mm_P7.50mm_P10.00mm
C, Rect series, Radial, pin pitch=7.50mm 10.00mm, , length*width=13*6.5mm^2, Capacitor
C Rect series Radial pin pitch 7.50mm 10.00mm  length 13mm width 6.5mm Capacitor
0
4
2
Capacitor_THT
C_Rect_L13.0mm_W8.0mm_P10.00mm_FKS3_FKP3_MKS4
C, Rect series, Radial, pin pitch=10.00mm, , length*width=13*8mm^2, Capacitor, http://www.wima.com/EN/WIMA_FKS_3.pdf, http://www.wima.com/EN/WIMA_MKS_4.pdf
C Rect series Radial pin pitch 10.00mm  length 13mm width 8mm Capacitor
0
2
2
Capacitor_THT
C_Rect_L13.5mm_W4.0mm_P10.00mm_FKS3_FKP3_MKS4
C, Rect series, Radial, pin pitch=10.00mm, , length*width=13.5*4mm^2, Capacitor, http://www.wima.com/EN/WIMA_FKS_3.pdf, http://www.wima.com/EN/WIMA_MKS_4.pdf
C Rect series Radial pin pitch 10.00mm  length 13.5mm width 4mm Capacitor
0
2
2
Capacitor_THT
C_Rect_L13.5mm_W5.0mm_P10.00mm_FKS3_FKP3_MKS4
C, Rect series, Radial, pin pitch=10.00mm, , length*width=13.5*5mm^2, Capacitor, http://www.wima.com/EN/WIMA_FKS_3.pdf, http://www.wima.com/EN/WIMA_MKS_4.pdf
C Rect series Radial pin pitch 10.00mm  length 13.5mm width 5mm Capacitor
0
2
2
Capacitor_THT
C_Rect_L16.5mm_W4.7mm_P15.00mm_MKT
C, Rect series, Radial, pin pitch=15.00mm, , length*width=16.5*4.7mm^2, Capacitor, https://en.tdk.eu/inf/20/20/db/fc_2009/MKT_B32560_564.pdf
C Rect series Radial pin pitch 15.00mm  length 16.5mm width 4.7mm Capacitor
0
2
2
Capacitor_THT
C_Rect_L16.5mm_W4.9mm_P15.00mm_MKT
C, Rect series, Radial, pin pitch=15.00mm, , length*width=16.5*4.9mm^2, Capacitor, https://en.tdk.eu/inf/20/20/db/fc_2009/MKT_B32560_564.pdf
C Rect series Radial pin pitch 15.00mm  length 16.5mm width 4.9mm Capacitor
0
2
2
Capacitor_THT
C_Rect_L16.5mm_W5.0mm_P15.00mm_MKT
C, Rect series, Radial, pin pitch=15.00mm, , length*width=16.5*5mm^2, Capacitor, https://en.tdk.eu/inf/20/20/db/fc_2009/MKT_B32560_564.pdf
C Rect series Radial pin pitch 15.00mm  length 16.5mm width 5mm Capacitor
0
2
2
Capacitor_THT
C_Rect_L16.5mm_W6.0mm_P15.00mm_MKT
C, Rect series, Radial, pin pitch=15.00mm, , length*width=16.5*6mm^2, Capacitor, https://en.tdk.eu/inf/20/20/db/fc_2009/MKT_B32560_564.pdf
C Rect series Radial pin pitch 15.00mm  length 16.5mm width 6mm Capacitor
0
2
2
Capacitor_THT
C_Rect_L16.5mm_W7.0mm_P15.00mm_MKT
C, Rect series, Radial, pin pitch=15.00mm, , length*width=16.5*7mm^2, Capacitor, https://en.tdk.eu/inf/20/20/db/fc_2009/MKT_B32560_564.pdf
C Rect series Radial pin pitch 15.00mm  length 16.5mm width 7mm Capacitor
0
2
2
Capacitor_THT
C_Rect_L16.5mm_W7.3mm_P15.00mm_MKT
C, Rect series, Radial, pin pitch=15.00mm, , length*width=16.5*7.3mm^2, Capacitor, https://en.tdk.eu/inf/20/20/db/fc_2009/MKT_B32560_564.pdf
C Rect series Radial pin pitch 15.00mm  length 16.5mm width 7.3mm Capacitor
0
2
2
Capacitor_THT
C_Rect_L16.5mm_W8.7mm_P15.00mm_MKT
C, Rect series, Radial, pin pitch=15.00mm, , length*width=16.5*8.7mm^2, Capacitor, https://en.tdk.eu/inf/20/20/db/fc_2009/MKT_B32560_564.pdf
C Rect series Radial pin pitch 15.00mm  length 16.5mm width 8.7mm Capacitor
0
2
2
Capacitor_THT
C_Rect_L16.5mm_W8.9mm_P15.00mm_MKT
C, Rect series, Radial, pin pitch=15.00mm, , length*width=16.5*8.9mm^2, Capacitor, https://en.tdk.eu/inf/20/20/db/fc_2009/MKT_B32560_564.pdf
C Rect series Radial pin pitch 15.00mm  length 16.5mm width 8.9mm Capacitor
0
2
2
Capacitor_THT
C_Rect_L16.5mm_W9.0mm_P15.00mm_MKT
C, Rect series, Radial, pin pitch=15.00mm, , length*width=16.5*9mm^2, Capacitor, https://en.tdk.eu/inf/20/20/db/fc_2009/MKT_B32560_564.pdf
C Rect series Radial pin pitch 15.00mm  length 16.5mm width 9mm Capacitor
0
2
2
Capacitor_THT
C_Rect_L16.5mm_W9.2mm_P15.00mm_MKT
C, Rect series, Radial, pin pitch=15.00mm, , length*width=16.5*9.2mm^2, Capacitor, https://en.tdk.eu/inf/20/20/db/fc_2009/MKT_B32560_564.pdf
C Rect series Radial pin pitch 15.00mm  length 16.5mm width 9.2mm Capacitor
0
2
2
Capacitor_THT
C_Rect_L16.5mm_W10.7mm_P15.00mm_MKT
C, Rect series, Radial, pin pitch=15.00mm, , length*width=16.5*10.7mm^2, Capacitor, https://en.tdk.eu/inf/20/20/db/fc_2009/MKT_B32560_564.pdf
C Rect series Radial pin pitch 15.00mm  length 16.5mm width 10.7mm Capacitor
0
2
2
Capacitor_THT
C_Rect_L16.5mm_W10.9mm_P15.00mm_MKT
C, Rect series, Radial, pin pitch=15.00mm, , length*width=16.5*10.9mm^2, Capacitor, https://en.tdk.eu/inf/20/20/db/fc_2009/MKT_B32560_564.pdf
C Rect series Radial pin pitch 15.00mm  length 16.5mm width 10.9mm Capacitor
0
2
2
Capacitor_THT
C_Rect_L16.5mm_W11.2mm_P15.00mm_MKT
C, Rect series, Radial, pin pitch=15.00mm, , length*width=16.5*11.2mm^2, Capacitor, https://en.tdk.eu/inf/20/20/db/fc_2009/MKT_B32560_564.pdf
C Rect series Radial pin pitch 15.00mm  length 16.5mm width 11.2mm Capacitor
0
2
2
Capacitor_THT
C_Rect_L16.5mm_W11.8mm_P15.00mm_MKT
C, Rect series, Radial, pin pitch=15.00mm, , length*width=16.5*11.8mm^2, Capacitor, https://en.tdk.eu/inf/20/20/db/fc_2009/MKT_B32560_564.pdf
C Rect series Radial pin pitch 15.00mm  length 16.5mm width 11.8mm Capacitor
0
2
2
Capacitor_THT
C_Rect_L16.5mm_W13.5mm_P15.00mm_MKT
C, Rect series, Radial, pin pitch=15.00mm, , length*width=16.5*13.5mm^2, Capacitor, https://en.tdk.eu/inf/20/20/db/fc_2009/MKT_B32560_564.pdf
C Rect series Radial pin pitch 15.00mm  length 16.5mm width 13.5mm Capacitor
0
2
2
Capacitor_THT
C_Rect_L16.5mm_W13.7mm_P15.00mm_MKT
C, Rect series, Radial, pin pitch=15.00mm, , length*width=16.5*13.7mm^2, Capacitor, https://en.tdk.eu/inf/20/20/db/fc_2009/MKT_B32560_564.pdf
C Rect series Radial pin pitch 15.00mm  length 16.5mm width 13.7mm Capacitor
0
2
2
Capacitor_THT
C_Rect_L16.5mm_W13.9mm_P15.00mm_MKT
C, Rect series, Radial, pin pitch=15.00mm, , length*width=16.5*13.9mm^2, Capacitor, https://en.tdk.eu/inf/20/20/db/fc_2009/MKT_B32560_564.pdf
C Rect series Radial pin pitch 15.00mm  length 16.5mm width 13.9mm Capacitor
0
2
2
Capacitor_THT
C_Rect_L18.0mm_W5.0mm_P15.00mm_FKS3_FKP3
C, Rect series, Radial, pin pitch=15.00mm, , length*width=18*5mm^2, Capacitor, http://www.wima.com/EN/WIMA_FKS_3.pdf
C Rect series Radial pin pitch 15.00mm  length 18mm width 5mm Capacitor
0
2
2
Capacitor_THT
C_Rect_L18.0mm_W6.0mm_P15.00mm_FKS3_FKP3
C, Rect series, Radial, pin pitch=15.00mm, , length*width=18*6mm^2, Capacitor, http://www.wima.com/EN/WIMA_FKS_3.pdf
C Rect series Radial pin pitch 15.00mm  length 18mm width 6mm Capacitor
0
2
2
Capacitor_THT
C_Rect_L18.0mm_W7.0mm_P15.00mm_FKS3_FKP3
C, Rect series, Radial, pin pitch=15.00mm, , length*width=18*7mm^2, Capacitor, http://www.wima.com/EN/WIMA_FKS_3.pdf
C Rect series Radial pin pitch 15.00mm  length 18mm width 7mm Capacitor
0
2
2
Capacitor_THT
C_Rect_L18.0mm_W8.0mm_P15.00mm_FKS3_FKP3
C, Rect series, Radial, pin pitch=15.00mm, , length*width=18*8mm^2, Capacitor, http://www.wima.com/EN/WIMA_FKS_3.pdf
C Rect series Radial pin pitch 15.00mm  length 18mm width 8mm Capacitor
0
2
2
Capacitor_THT
C_Rect_L18.0mm_W9.0mm_P15.00mm_FKS3_FKP3
C, Rect series, Radial, pin pitch=15.00mm, , length*width=18*9mm^2, Capacitor, http://www.wima.com/EN/WIMA_FKS_3.pdf
C Rect series Radial pin pitch 15.00mm  length 18mm width 9mm Capacitor
0
2
2
Capacitor_THT
C_Rect_L18.0mm_W11.0mm_P15.00mm_FKS3_FKP3
C, Rect series, Radial, pin pitch=15.00mm, , length*width=18*11mm^2, Capacitor, http://www.wima.com/EN/WIMA_FKS_3.pdf
C Rect series Radial pin pitch 15.00mm  length 18mm width 11mm Capacitor
0
2
2
Capacitor_THT
C_Rect_L19.0mm_W5.0mm_P15.00mm_MKS4
C, Rect series, Radial, pin pitch=15.00mm, , length*width=19*5mm^2, Capacitor, http://www.wima.com/EN/WIMA_MKS_4.pdf
C Rect series Radial pin pitch 15.00mm  length 19mm width 5mm Capacitor
0
2
2
Capacitor_THT
C_Rect_L19.0mm_W6.0mm_P15.00mm_MKS4
C, Rect series, Radial, pin pitch=15.00mm, , length*width=19*6mm^2, Capacitor, http://www.wima.com/EN/WIMA_MKS_4.pdf
C Rect series Radial pin pitch 15.00mm  length 19mm width 6mm Capacitor
0
2
2
Capacitor_THT
C_Rect_L19.0mm_W7.0mm_P15.00mm_MKS4
C, Rect series, Radial, pin pitch=15.00mm, , length*width=19*7mm^2, Capacitor, http://www.wima.com/EN/WIMA_MKS_4.pdf
C Rect series Radial pin pitch 15.00mm  length 19mm width 7mm Capacitor
0
2
2
Capacitor_THT
C_Rect_L19.0mm_W8.0mm_P15.00mm_MKS4
C, Rect series, Radial, pin pitch=15.00mm, , length*width=19*8mm^2, Capacitor, http://www.wima.com/EN/WIMA_MKS_4.pdf
C Rect series Radial pin pitch 15.00mm  length 19mm width 8mm Capacitor
0
2
2
Capacitor_THT
C_Rect_L19.0mm_W9.0mm_P15.00mm_MKS4
C, Rect series, Radial, pin pitch=15.00mm, , length*width=19*9mm^2, Capacitor, http://www.wima.com/EN/WIMA_MKS_4.pdf
C Rect series Radial pin pitch 15.00mm  length 19mm width 9mm Capacitor
0
2
2
Capacitor_THT
C_Rect_L19.0mm_W11.0mm_P15.00mm_MKS4
C, Rect series, Radial, pin pitch=15.00mm, , length*width=19*11mm^2, Capacitor, http://www.wima.com/EN/WIMA_MKS_4.pdf
C Rect series Radial pin pitch 15.00mm  length 19mm width 11mm Capacitor
0
2
2
Capacitor_THT
C_Rect_L24.0mm_W7.0mm_P22.50mm_MKT
C, Rect series, Radial, pin pitch=22.50mm, , length*width=24*7mm^2, Capacitor, https://en.tdk.eu/inf/20/20/db/fc_2009/MKT_B32560_564.pdf
C Rect series Radial pin pitch 22.50mm  length 24mm width 7mm Capacitor
0
2
2
Capacitor_THT
C_Rect_L24.0mm_W8.3mm_P22.50mm_MKT
C, Rect series, Radial, pin pitch=22.50mm, , length*width=24*8.3mm^2, Capacitor, https://en.tdk.eu/inf/20/20/db/fc_2009/MKT_B32560_564.pdf
C Rect series Radial pin pitch 22.50mm  length 24mm width 8.3mm Capacitor
0
2
2
Capacitor_THT
C_Rect_L24.0mm_W8.6mm_P22.50mm_MKT
C, Rect series, Radial, pin pitch=22.50mm, , length*width=24*8.6mm^2, Capacitor, https://en.tdk.eu/inf/20/20/db/fc_2009/MKT_B32560_564.pdf
C Rect series Radial pin pitch 22.50mm  length 24mm width 8.6mm Capacitor
0
2
2
Capacitor_THT
C_Rect_L24.0mm_W10.1mm_P22.50mm_MKT
C, Rect series, Radial, pin pitch=22.50mm, , length*width=24*10.1mm^2, Capacitor, https://en.tdk.eu/inf/20/20/db/fc_2009/MKT_B32560_564.pdf
C Rect series Radial pin pitch 22.50mm  length 24mm width 10.1mm Capacitor
0
2
2
Capacitor_THT
C_Rect_L24.0mm_W10.3mm_P22.50mm_MKT
C, Rect series, Radial, pin pitch=22.50mm, , length*width=24*10.3mm^2, Capacitor, https://en.tdk.eu/inf/20/20/db/fc_2009/MKT_B32560_564.pdf
C Rect series Radial pin pitch 22.50mm  length 24mm width 10.3mm Capacitor
0
2
2
Capacitor_THT
C_Rect_L24.0mm_W10.9mm_P22.50mm_MKT
C, Rect series, Radial, pin pitch=22.50mm, , length*width=24*10.9mm^2, Capacitor, https://en.tdk.eu/inf/20/20/db/fc_2009/MKT_B32560_564.pdf
C Rect series Radial pin pitch 22.50mm  length 24mm width 10.9mm Capacitor
0
2
2
Capacitor_THT
C_Rect_L24.0mm_W12.2mm_P22.50mm_MKT
C, Rect series, Radial, pin pitch=22.50mm, , length*width=24*12.2mm^2, Capacitor, https://en.tdk.eu/inf/20/20/db/fc_2009/MKT_B32560_564.pdf
C Rect series Radial pin pitch 22.50mm  length 24mm width 12.2mm Capacitor
0
2
2
Capacitor_THT
C_Rect_L24.0mm_W12.6mm_P22.50mm_MKT
C, Rect series, Radial, pin pitch=22.50mm, , length*width=24*12.6mm^2, Capacitor, https://en.tdk.eu/inf/20/20/db/fc_2009/MKT_B32560_564.pdf
C Rect series Radial pin pitch 22.50mm  length 24mm width 12.6mm Capacitor
0
2
2
Capacitor_THT
C_Rect_L24.0mm_W12.8mm_P22.50mm_MKT
C, Rect series, Radial, pin pitch=22.50mm, , length*width=24*12.8mm^2, Capacitor, https://en.tdk.eu/inf/20/20/db/fc_2009/MKT_B32560_564.pdf
C Rect series Radial pin pitch 22.50mm  length 24mm width 12.8mm Capacitor
0
2
2
Capacitor_THT
C_Rect_L26.5mm_W5.0mm_P22.50mm_MKS4
C, Rect series, Radial, pin pitch=22.50mm, , length*width=26.5*5mm^2, Capacitor, http://www.wima.com/EN/WIMA_MKS_4.pdf
C Rect series Radial pin pitch 22.50mm  length 26.5mm width 5mm Capacitor
0
2
2
Capacitor_THT
C_Rect_L26.5mm_W6.0mm_P22.50mm_MKS4
C, Rect series, Radial, pin pitch=22.50mm, , length*width=26.5*6mm^2, Capacitor, http://www.wima.com/EN/WIMA_MKS_4.pdf
C Rect series Radial pin pitch 22.50mm  length 26.5mm width 6mm Capacitor
0
2
2
Capacitor_THT
C_Rect_L26.5mm_W7.0mm_P22.50mm_MKS4
C, Rect series, Radial, pin pitch=22.50mm, , length*width=26.5*7mm^2, Capacitor, http://www.wima.com/EN/WIMA_MKS_4.pdf
C Rect series Radial pin pitch 22.50mm  length 26.5mm width 7mm Capacitor
0
2
2
Capacitor_THT
C_Rect_L26.5mm_W8.5mm_P22.50mm_MKS4
C, Rect series, Radial, pin pitch=22.50mm, , length*width=26.5*8.5mm^2, Capacitor, http://www.wima.com/EN/WIMA_MKS_4.pdf
C Rect series Radial pin pitch 22.50mm  length 26.5mm width 8.5mm Capacitor
0
2
2
Capacitor_THT
C_Rect_L26.5mm_W10.5mm_P22.50mm_MKS4
C, Rect series, Radial, pin pitch=22.50mm, , length*width=26.5*10.5mm^2, Capacitor, http://www.wima.com/EN/WIMA_MKS_4.pdf
C Rect series Radial pin pitch 22.50mm  length 26.5mm width 10.5mm Capacitor
0
2
2
Capacitor_THT
C_Rect_L26.5mm_W11.5mm_P22.50mm_MKS4
C, Rect series, Radial, pin pitch=22.50mm, , length*width=26.5*11.5mm^2, Capacitor, http://www.wima.com/EN/WIMA_MKS_4.pdf
C Rect series Radial pin pitch 22.50mm  length 26.5mm width 11.5mm Capacitor
0
2
2
Capacitor_THT
C_Rect_L27.0mm_W9.0mm_P22.00mm
C, Rect series, Radial, pin pitch=22.00mm, , length*width=27*9mm^2, Capacitor
C Rect series Radial pin pitch 22.00mm  length 27mm width 9mm Capacitor
0
2
2
Capacitor_THT
C_Rect_L27.0mm_W9.0mm_P23.00mm
C, Rect series, Radial, pin pitch=23.00mm, , length*width=27*9mm^2, Capacitor
C Rect series Radial pin pitch 23.00mm  length 27mm width 9mm Capacitor
0
2
2
Capacitor_THT
C_Rect_L27.0mm_W11.0mm_P22.00mm
C, Rect series, Radial, pin pitch=22.00mm, , length*width=27*11mm^2, Capacitor
C Rect series Radial pin pitch 22.00mm  length 27mm width 11mm Capacitor
0
2
2
Capacitor_THT
C_Rect_L28.0mm_W8.0mm_P22.50mm_MKS4
C, Rect series, Radial, pin pitch=22.50mm, , length*width=28*8mm^2, Capacitor, http://www.wima.com/EN/WIMA_MKS_4.pdf
C Rect series Radial pin pitch 22.50mm  length 28mm width 8mm Capacitor
0
2
2
Capacitor_THT
C_Rect_L28.0mm_W10.0mm_P22.50mm_MKS4
C, Rect series, Radial, pin pitch=22.50mm, , length*width=28*10mm^2, Capacitor, http://www.wima.com/EN/WIMA_MKS_4.pdf
C Rect series Radial pin pitch 22.50mm  length 28mm width 10mm Capacitor
0
2
2
Capacitor_THT
C_Rect_L28.0mm_W12.0mm_P22.50mm_MKS4
C, Rect series, Radial, pin pitch=22.50mm, , length*width=28*12mm^2, Capacitor, http://www.wima.com/EN/WIMA_MKS_4.pdf
C Rect series Radial pin pitch 22.50mm  length 28mm width 12mm Capacitor
0
2
2
Capacitor_THT
C_Rect_L29.0mm_W7.6mm_P27.50mm_MKT
C, Rect series, Radial, pin pitch=27.50mm, , length*width=29*7.6mm^2, Capacitor, https://en.tdk.eu/inf/20/20/db/fc_2009/MKT_B32560_564.pdf
C Rect series Radial pin pitch 27.50mm  length 29mm width 7.6mm Capacitor
0
2
2
Capacitor_THT
C_Rect_L29.0mm_W7.8mm_P27.50mm_MKT
C, Rect series, Radial, pin pitch=27.50mm, , length*width=29*7.8mm^2, Capacitor, https://en.tdk.eu/inf/20/20/db/fc_2009/MKT_B32560_564.pdf
C Rect series Radial pin pitch 27.50mm  length 29mm width 7.8mm Capacitor
0
2
2
Capacitor_THT
C_Rect_L29.0mm_W7.9mm_P27.50mm_MKT
C, Rect series, Radial, pin pitch=27.50mm, , length*width=29*7.9mm^2, Capacitor, https://en.tdk.eu/inf/20/20/db/fc_2009/MKT_B32560_564.pdf
C Rect series Radial pin pitch 27.50mm  length 29mm width 7.9mm Capacitor
0
2
2
Capacitor_THT
C_Rect_L29.0mm_W9.1mm_P27.50mm_MKT
C, Rect series, Radial, pin pitch=27.50mm, , length*width=29*9.1mm^2, Capacitor, https://en.tdk.eu/inf/20/20/db/fc_2009/MKT_B32560_564.pdf
C Rect series Radial pin pitch 27.50mm  length 29mm width 9.1mm Capacitor
0
2
2
Capacitor_THT
C_Rect_L29.0mm_W9.6mm_P27.50mm_MKT
C, Rect series, Radial, pin pitch=27.50mm, , length*width=29*9.6mm^2, Capacitor, https://en.tdk.eu/inf/20/20/db/fc_2009/MKT_B32560_564.pdf
C Rect series Radial pin pitch 27.50mm  length 29mm width 9.6mm Capacitor
0
2
2
Capacitor_THT
C_Rect_L29.0mm_W11.0mm_P27.50mm_MKT
C, Rect series, Radial, pin pitch=27.50mm, , length*width=29*11mm^2, Capacitor, https://en.tdk.eu/inf/20/20/db/fc_2009/MKT_B32560_564.pdf
C Rect series Radial pin pitch 27.50mm  length 29mm width 11mm Capacitor
0
2
2
Capacitor_THT
C_Rect_L29.0mm_W11.9mm_P27.50mm_MKT
C, Rect series, Radial, pin pitch=27.50mm, , length*width=29*11.9mm^2, Capacitor, https://en.tdk.eu/inf/20/20/db/fc_2009/MKT_B32560_564.pdf
C Rect series Radial pin pitch 27.50mm  length 29mm width 11.9mm Capacitor
0
2
2
Capacitor_THT
C_Rect_L29.0mm_W12.2mm_P27.50mm_MKT
C, Rect series, Radial, pin pitch=27.50mm, , length*width=29*12.2mm^2, Capacitor, https://en.tdk.eu/inf/20/20/db/fc_2009/MKT_B32560_564.pdf
C Rect series Radial pin pitch 27.50mm  length 29mm width 12.2mm Capacitor
0
2
2
Capacitor_THT
C_Rect_L29.0mm_W13.0mm_P27.50mm_MKT
C, Rect series, Radial, pin pitch=27.50mm, , length*width=29*13mm^2, Capacitor, https://en.tdk.eu/inf/20/20/db/fc_2009/MKT_B32560_564.pdf
C Rect series Radial pin pitch 27.50mm  length 29mm width 13mm Capacitor
0
2
2
Capacitor_THT
C_Rect_L29.0mm_W13.8mm_P27.50mm_MKT
C, Rect series, Radial, pin pitch=27.50mm, , length*width=29*13.8mm^2, Capacitor, https://en.tdk.eu/inf/20/20/db/fc_2009/MKT_B32560_564.pdf
C Rect series Radial pin pitch 27.50mm  length 29mm width 13.8mm Capacitor
0
2
2
Capacitor_THT
C_Rect_L29.0mm_W14.2mm_P27.50mm_MKT
C, Rect series, Radial, pin pitch=27.50mm, , length*width=29*14.2mm^2, Capacitor, https://en.tdk.eu/inf/20/20/db/fc_2009/MKT_B32560_564.pdf
C Rect series Radial pin pitch 27.50mm  length 29mm width 14.2mm Capacitor
0
2
2
Capacitor_THT
C_Rect_L29.0mm_W16.0mm_P27.50mm_MKT
C, Rect series, Radial, pin pitch=27.50mm, , length*width=29*16mm^2, Capacitor, https://en.tdk.eu/inf/20/20/db/fc_2009/MKT_B32560_564.pdf
C Rect series Radial pin pitch 27.50mm  length 29mm width 16mm Capacitor
0
2
2
Capacitor_THT
C_Rect_L31.5mm_W9.0mm_P27.50mm_MKS4
C, Rect series, Radial, pin pitch=27.50mm, , length*width=31.5*9mm^2, Capacitor, http://www.wima.com/EN/WIMA_MKS_4.pdf
C Rect series Radial pin pitch 27.50mm  length 31.5mm width 9mm Capacitor
0
2
2
Capacitor_THT
C_Rect_L31.5mm_W11.0mm_P27.50mm_MKS4
C, Rect series, Radial, pin pitch=27.50mm, , length*width=31.5*11mm^2, Capacitor, http://www.wima.com/EN/WIMA_MKS_4.pdf
C Rect series Radial pin pitch 27.50mm  length 31.5mm width 11mm Capacitor
0
2
2
Capacitor_THT
C_Rect_L31.5mm_W13.0mm_P27.50mm_MKS4
C, Rect series, Radial, pin pitch=27.50mm, , length*width=31.5*13mm^2, Capacitor, http://www.wima.com/EN/WIMA_MKS_4.pdf
C Rect series Radial pin pitch 27.50mm  length 31.5mm width 13mm Capacitor
0
2
2
Capacitor_THT
C_Rect_L31.5mm_W15.0mm_P27.50mm_MKS4
C, Rect series, Radial, pin pitch=27.50mm, , length*width=31.5*15mm^2, Capacitor, http://www.wima.com/EN/WIMA_MKS_4.pdf
C Rect series Radial pin pitch 27.50mm  length 31.5mm width 15mm Capacitor
0
2
2
Capacitor_THT
C_Rect_L31.5mm_W17.0mm_P27.50mm_MKS4
C, Rect series, Radial, pin pitch=27.50mm, , length*width=31.5*17mm^2, Capacitor, http://www.wima.com/EN/WIMA_MKS_4.pdf
C Rect series Radial pin pitch 27.50mm  length 31.5mm width 17mm Capacitor
0
2
2
Capacitor_THT
C_Rect_L31.5mm_W20.0mm_P27.50mm_MKS4
C, Rect series, Radial, pin pitch=27.50mm, , length*width=31.5*20mm^2, Capacitor, http://www.wima.com/EN/WIMA_MKS_4.pdf
C Rect series Radial pin pitch 27.50mm  length 31.5mm width 20mm Capacitor
0
2
2
Capacitor_THT
C_Rect_L32.0mm_W15.0mm_P27.00mm
C, Rect series, Radial, pin pitch=27.00mm, , length*width=32*15mm^2, Capacitor
C Rect series Radial pin pitch 27.00mm  length 32mm width 15mm Capacitor
0
2
2
Capacitor_THT
C_Rect_L33.0mm_W13.0mm_P27.50mm_MKS4
C, Rect series, Radial, pin pitch=27.50mm, , length*width=33*13mm^2, Capacitor, http://www.wima.com/EN/WIMA_MKS_4.pdf
C Rect series Radial pin pitch 27.50mm  length 33mm width 13mm Capacitor
0
2
2
Capacitor_THT
C_Rect_L33.0mm_W15.0mm_P27.50mm_MKS4
C, Rect series, Radial, pin pitch=27.50mm, , length*width=33*15mm^2, Capacitor, http://www.wima.com/EN/WIMA_MKS_4.pdf
C Rect series Radial pin pitch 27.50mm  length 33mm width 15mm Capacitor
0
2
2
Capacitor_THT
C_Rect_L33.0mm_W20.0mm_P27.50mm_MKS4
C, Rect series, Radial, pin pitch=27.50mm, , length*width=33*20mm^2, Capacitor, http://www.wima.com/EN/WIMA_MKS_4.pdf
C Rect series Radial pin pitch 27.50mm  length 33mm width 20mm Capacitor
0
2
2
Capacitor_THT
C_Rect_L41.5mm_W9.0mm_P37.50mm_MKS4
C, Rect series, Radial, pin pitch=37.50mm, , length*width=41.5*9mm^2, Capacitor, http://www.wima.com/EN/WIMA_MKS_4.pdf
C Rect series Radial pin pitch 37.50mm  length 41.5mm width 9mm Capacitor
0
2
2
Capacitor_THT
C_Rect_L41.5mm_W11.0mm_P37.50mm_MKS4
C, Rect series, Radial, pin pitch=37.50mm, , length*width=41.5*11mm^2, Capacitor, http://www.wima.com/EN/WIMA_MKS_4.pdf
C Rect series Radial pin pitch 37.50mm  length 41.5mm width 11mm Capacitor
0
2
2
Capacitor_THT
C_Rect_L41.5mm_W13.0mm_P37.50mm_MKS4
C, Rect series, Radial, pin pitch=37.50mm, , length*width=41.5*13mm^2, Capacitor, http://www.wima.com/EN/WIMA_MKS_4.pdf
C Rect series Radial pin pitch 37.50mm  length 41.5mm width 13mm Capacitor
0
2
2
Capacitor_THT
C_Rect_L41.5mm_W15.0mm_P37.50mm_MKS4
C, Rect series, Radial, pin pitch=37.50mm, , length*width=41.5*15mm^2, Capacitor, http://www.wima.com/EN/WIMA_MKS_4.pdf
C Rect series Radial pin pitch 37.50mm  length 41.5mm width 15mm Capacitor
0
2
2
Capacitor_THT
C_Rect_L41.5mm_W17.0mm_P37.50mm_MKS4
C, Rect series, Radial, pin pitch=37.50mm, , length*width=41.5*17mm^2, Capacitor, http://www.wima.com/EN/WIMA_MKS_4.pdf
C Rect series Radial pin pitch 37.50mm  length 41.5mm width 17mm Capacitor
0
2
2
Capacitor_THT
C_Rect_L41.5mm_W19.0mm_P37.50mm_MKS4
C, Rect series, Radial, pin pitch=37.50mm, , length*width=41.5*19mm^2, Capacitor, http://www.wima.com/EN/WIMA_MKS_4.pdf
C Rect series Radial pin pitch 37.50mm  length 41.5mm width 19mm Capacitor
0
2
2
Capacitor_THT
C_Rect_L41.5mm_W20.0mm_P37.50mm_MKS4
C, Rect series, Radial, pin pitch=37.50mm, , length*width=41.5*20mm^2, Capacitor, http://www.wima.com/EN/WIMA_MKS_4.pdf
C Rect series Radial pin pitch 37.50mm  length 41.5mm width 20mm Capacitor
0
2
2
Capacitor_THT
C_Rect_L41.5mm_W24.0mm_P37.50mm_MKS4
C, Rect series, Radial, pin pitch=37.50mm, , length*width=41.5*24mm^2, Capacitor, http://www.wima.com/EN/WIMA_MKS_4.pdf
C Rect series Radial pin pitch 37.50mm  length 41.5mm width 24mm Capacitor
0
2
2
Capacitor_THT
C_Rect_L41.5mm_W31.0mm_P37.50mm_MKS4
C, Rect series, Radial, pin pitch=37.50mm, , length*width=41.5*31mm^2, Capacitor, http://www.wima.com/EN/WIMA_MKS_4.pdf
C Rect series Radial pin pitch 37.50mm  length 41.5mm width 31mm Capacitor
0
2
2
Capacitor_THT
C_Rect_L41.5mm_W35.0mm_P37.50mm_MKS4
C, Rect series, Radial, pin pitch=37.50mm, , length*width=41.5*35mm^2, Capacitor, http://www.wima.com/EN/WIMA_MKS_4.pdf
C Rect series Radial pin pitch 37.50mm  length 41.5mm width 35mm Capacitor
0
2
2
Capacitor_THT
C_Rect_L41.5mm_W40.0mm_P37.50mm_MKS4
C, Rect series, Radial, pin pitch=37.50mm, , length*width=41.5*40mm^2, Capacitor, http://www.wima.com/EN/WIMA_MKS_4.pdf
C Rect series Radial pin pitch 37.50mm  length 41.5mm width 40mm Capacitor
0
2
2
Capacitor_Tantalum_SMD
CP_EIA-1608-08_AVX-J
Tantalum Capacitor SMD AVX-J (1608-08 Metric), IPC_7351 nominal, (Body size from: https://www.vishay.com/docs/48064/_t58_vmn_pt0471_1601.pdf), generated with kicad-footprint-generator
capacitor tantalum
0
2
2
Capacitor_Tantalum_SMD
CP_EIA-1608-08_AVX-J_Pad1.25x1.05mm_HandSolder
Tantalum Capacitor SMD AVX-J (1608-08 Metric), IPC_7351 nominal, (Body size from: https://www.vishay.com/docs/48064/_t58_vmn_pt0471_1601.pdf), generated with kicad-footprint-generator
capacitor tantalum
0
2
2
Capacitor_Tantalum_SMD
CP_EIA-1608-10_AVX-L
Tantalum Capacitor SMD AVX-L (1608-10 Metric), IPC_7351 nominal, (Body size from: https://www.vishay.com/docs/48064/_t58_vmn_pt0471_1601.pdf), generated with kicad-footprint-generator
capacitor tantalum
0
2
2
Capacitor_Tantalum_SMD
CP_EIA-1608-10_AVX-L_Pad1.25x1.05mm_HandSolder
Tantalum Capacitor SMD AVX-L (1608-10 Metric), IPC_7351 nominal, (Body size from: https://www.vishay.com/docs/48064/_t58_vmn_pt0471_1601.pdf), generated with kicad-footprint-generator
capacitor tantalum
0
2
2
Capacitor_Tantalum_SMD
CP_EIA-2012-12_Kemet-R
Tantalum Capacitor SMD Kemet-R (2012-12 Metric), IPC_7351 nominal, (Body size from: https://www.vishay.com/docs/40182/tmch.pdf), generated with kicad-footprint-generator
capacitor tantalum
0
2
2
Capacitor_Tantalum_SMD
CP_EIA-2012-12_Kemet-R_Pad1.30x1.05mm_HandSolder
Tantalum Capacitor SMD Kemet-R (2012-12 Metric), IPC_7351 nominal, (Body size from: https://www.vishay.com/docs/40182/tmch.pdf), generated with kicad-footprint-generator
capacitor tantalum
0
2
2
Capacitor_Tantalum_SMD
CP_EIA-2012-15_AVX-P
Tantalum Capacitor SMD AVX-P (2012-15 Metric), IPC_7351 nominal, (Body size from: https://www.vishay.com/docs/40182/tmch.pdf), generated with kicad-footprint-generator
capacitor tantalum
0
2
2
Capacitor_Tantalum_SMD
CP_EIA-2012-15_AVX-P_Pad1.30x1.05mm_HandSolder
Tantalum Capacitor SMD AVX-P (2012-15 Metric), IPC_7351 nominal, (Body size from: https://www.vishay.com/docs/40182/tmch.pdf), generated with kicad-footprint-generator
capacitor tantalum
0
2
2
Capacitor_Tantalum_SMD
CP_EIA-3216-10_Kemet-I
Tantalum Capacitor SMD Kemet-I (3216-10 Metric), IPC_7351 nominal, (Body size from: http://www.kemet.com/Lists/ProductCatalog/Attachments/253/KEM_TC101_STD.pdf), generated with kicad-footprint-generator
capacitor tantalum
0
2
2
Capacitor_Tantalum_SMD
CP_EIA-3216-10_Kemet-I_Pad1.58x1.35mm_HandSolder
Tantalum Capacitor SMD Kemet-I (3216-10 Metric), IPC_7351 nominal, (Body size from: http://www.kemet.com/Lists/ProductCatalog/Attachments/253/KEM_TC101_STD.pdf), generated with kicad-footprint-generator
capacitor tantalum
0
2
2
Capacitor_Tantalum_SMD
CP_EIA-3216-12_Kemet-S
Tantalum Capacitor SMD Kemet-S (3216-12 Metric), IPC_7351 nominal, (Body size from: http://www.kemet.com/Lists/ProductCatalog/Attachments/253/KEM_TC101_STD.pdf), generated with kicad-footprint-generator
capacitor tantalum
0
2
2
Capacitor_Tantalum_SMD
CP_EIA-3216-12_Kemet-S_Pad1.58x1.35mm_HandSolder
Tantalum Capacitor SMD Kemet-S (3216-12 Metric), IPC_7351 nominal, (Body size from: http://www.kemet.com/Lists/ProductCatalog/Attachments/253/KEM_TC101_STD.pdf), generated with kicad-footprint-generator
capacitor tantalum
0
2
2
Capacitor_Tantalum_SMD
CP_EIA-3216-18_Kemet-A
Tantalum Capacitor SMD Kemet-A (3216-18 Metric), IPC_7351 nominal, (Body size from: http://www.kemet.com/Lists/ProductCatalog/Attachments/253/KEM_TC101_STD.pdf), generated with kicad-footprint-generator
capacitor tantalum
0
2
2
Capacitor_Tantalum_SMD
CP_EIA-3216-18_Kemet-A_Pad1.58x1.35mm_HandSolder
Tantalum Capacitor SMD Kemet-A (3216-18 Metric), IPC_7351 nominal, (Body size from: http://www.kemet.com/Lists/ProductCatalog/Attachments/253/KEM_TC101_STD.pdf), generated with kicad-footprint-generator
capacitor tantalum
0
2
2
Capacitor_Tantalum_SMD
CP_EIA-3528-12_Kemet-T
Tantalum Capacitor SMD Kemet-T (3528-12 Metric), IPC_7351 nominal, (Body size from: http://www.kemet.com/Lists/ProductCatalog/Attachments/253/KEM_TC101_STD.pdf), generated with kicad-footprint-generator
capacitor tantalum
0
2
2
Capacitor_Tantalum_SMD
CP_EIA-3528-12_Kemet-T_Pad1.50x2.35mm_HandSolder
Tantalum Capacitor SMD Kemet-T (3528-12 Metric), IPC_7351 nominal, (Body size from: http://www.kemet.com/Lists/ProductCatalog/Attachments/253/KEM_TC101_STD.pdf), generated with kicad-footprint-generator
capacitor tantalum
0
2
2
Capacitor_Tantalum_SMD
CP_EIA-3528-15_AVX-H
Tantalum Capacitor SMD AVX-H (3528-15 Metric), IPC_7351 nominal, (Body size from: http://www.kemet.com/Lists/ProductCatalog/Attachments/253/KEM_TC101_STD.pdf), generated with kicad-footprint-generator
capacitor tantalum
0
2
2
Capacitor_Tantalum_SMD
CP_EIA-3528-15_AVX-H_Pad1.50x2.35mm_HandSolder
Tantalum Capacitor SMD AVX-H (3528-15 Metric), IPC_7351 nominal, (Body size from: http://www.kemet.com/Lists/ProductCatalog/Attachments/253/KEM_TC101_STD.pdf), generated with kicad-footprint-generator
capacitor tantalum
0
2
2
Capacitor_Tantalum_SMD
CP_EIA-3528-21_Kemet-B
Tantalum Capacitor SMD Kemet-B (3528-21 Metric), IPC_7351 nominal, (Body size from: http://www.kemet.com/Lists/ProductCatalog/Attachments/253/KEM_TC101_STD.pdf), generated with kicad-footprint-generator
capacitor tantalum
0
2
2
Capacitor_Tantalum_SMD
CP_EIA-3528-21_Kemet-B_Pad1.50x2.35mm_HandSolder
Tantalum Capacitor SMD Kemet-B (3528-21 Metric), IPC_7351 nominal, (Body size from: http://www.kemet.com/Lists/ProductCatalog/Attachments/253/KEM_TC101_STD.pdf), generated with kicad-footprint-generator
capacitor tantalum
0
2
2
Capacitor_Tantalum_SMD
CP_EIA-6032-15_Kemet-U
Tantalum Capacitor SMD Kemet-U (6032-15 Metric), IPC_7351 nominal, (Body size from: http://www.kemet.com/Lists/ProductCatalog/Attachments/253/KEM_TC101_STD.pdf), generated with kicad-footprint-generator
capacitor tantalum
0
2
2
Capacitor_Tantalum_SMD
CP_EIA-6032-15_Kemet-U_Pad2.25x2.35mm_HandSolder
Tantalum Capacitor SMD Kemet-U (6032-15 Metric), IPC_7351 nominal, (Body size from: http://www.kemet.com/Lists/ProductCatalog/Attachments/253/KEM_TC101_STD.pdf), generated with kicad-footprint-generator
capacitor tantalum
0
2
2
Capacitor_Tantalum_SMD
CP_EIA-6032-20_AVX-F
Tantalum Capacitor SMD AVX-F (6032-20 Metric), IPC_7351 nominal, (Body size from: http://www.kemet.com/Lists/ProductCatalog/Attachments/253/KEM_TC101_STD.pdf), generated with kicad-footprint-generator
capacitor tantalum
0
2
2
Capacitor_Tantalum_SMD
CP_EIA-6032-20_AVX-F_Pad2.25x2.35mm_HandSolder
Tantalum Capacitor SMD AVX-F (6032-20 Metric), IPC_7351 nominal, (Body size from: http://www.kemet.com/Lists/ProductCatalog/Attachments/253/KEM_TC101_STD.pdf), generated with kicad-footprint-generator
capacitor tantalum
0
2
2
Capacitor_Tantalum_SMD
CP_EIA-6032-28_Kemet-C
Tantalum Capacitor SMD Kemet-C (6032-28 Metric), IPC_7351 nominal, (Body size from: http://www.kemet.com/Lists/ProductCatalog/Attachments/253/KEM_TC101_STD.pdf), generated with kicad-footprint-generator
capacitor tantalum
0
2
2
Capacitor_Tantalum_SMD
CP_EIA-6032-28_Kemet-C_Pad2.25x2.35mm_HandSolder
Tantalum Capacitor SMD Kemet-C (6032-28 Metric), IPC_7351 nominal, (Body size from: http://www.kemet.com/Lists/ProductCatalog/Attachments/253/KEM_TC101_STD.pdf), generated with kicad-footprint-generator
capacitor tantalum
0
2
2
Capacitor_Tantalum_SMD
CP_EIA-7132-20_AVX-U
Tantalum Capacitor SMD AVX-U (7132-20 Metric), IPC_7351 nominal, (Body size from: http://datasheets.avx.com/F72-F75.pdf), generated with kicad-footprint-generator
capacitor tantalum
0
2
2
Capacitor_Tantalum_SMD
CP_EIA-7132-20_AVX-U_Pad2.72x3.50mm_HandSolder
Tantalum Capacitor SMD AVX-U (7132-20 Metric), IPC_7351 nominal, (Body size from: http://datasheets.avx.com/F72-F75.pdf), generated with kicad-footprint-generator
capacitor tantalum
0
2
2
Capacitor_Tantalum_SMD
CP_EIA-7132-28_AVX-C
Tantalum Capacitor SMD AVX-C (7132-28 Metric), IPC_7351 nominal, (Body size from: http://datasheets.avx.com/F72-F75.pdf), generated with kicad-footprint-generator
capacitor tantalum
0
2
2
Capacitor_Tantalum_SMD
CP_EIA-7132-28_AVX-C_Pad2.72x3.50mm_HandSolder
Tantalum Capacitor SMD AVX-C (7132-28 Metric), IPC_7351 nominal, (Body size from: http://datasheets.avx.com/F72-F75.pdf), generated with kicad-footprint-generator
capacitor tantalum
0
2
2
Capacitor_Tantalum_SMD
CP_EIA-7260-15_AVX-R
Tantalum Capacitor SMD AVX-R (7260-15 Metric), IPC_7351 nominal, (Body size from: http://datasheets.avx.com/F72-F75.pdf), generated with kicad-footprint-generator
capacitor tantalum
0
2
2
Capacitor_Tantalum_SMD
CP_EIA-7260-15_AVX-R_Pad2.68x6.30mm_HandSolder
Tantalum Capacitor SMD AVX-R (7260-15 Metric), IPC_7351 nominal, (Body size from: http://datasheets.avx.com/F72-F75.pdf), generated with kicad-footprint-generator
capacitor tantalum
0
2
2
Capacitor_Tantalum_SMD
CP_EIA-7260-20_AVX-M
Tantalum Capacitor SMD AVX-M (7260-20 Metric), IPC_7351 nominal, (Body size from: http://datasheets.avx.com/F72-F75.pdf), generated with kicad-footprint-generator
capacitor tantalum
0
2
2
Capacitor_Tantalum_SMD
CP_EIA-7260-20_AVX-M_Pad2.68x6.30mm_HandSolder
Tantalum Capacitor SMD AVX-M (7260-20 Metric), IPC_7351 nominal, (Body size from: http://datasheets.avx.com/F72-F75.pdf), generated with kicad-footprint-generator
capacitor tantalum
0
2
2
Capacitor_Tantalum_SMD
CP_EIA-7260-28_AVX-M
Tantalum Capacitor SMD AVX-M (7260-28 Metric), IPC_7351 nominal, (Body size from: http://datasheets.avx.com/F72-F75.pdf), generated with kicad-footprint-generator
capacitor tantalum
0
2
2
Capacitor_Tantalum_SMD
CP_EIA-7260-28_AVX-M_Pad2.68x6.30mm_HandSolder
Tantalum Capacitor SMD AVX-M (7260-28 Metric), IPC_7351 nominal, (Body size from: http://datasheets.avx.com/F72-F75.pdf), generated with kicad-footprint-generator
capacitor tantalum
0
2
2
Capacitor_Tantalum_SMD
CP_EIA-7260-38_AVX-R
Tantalum Capacitor SMD AVX-R (7260-38 Metric), IPC_7351 nominal, (Body size from: http://datasheets.avx.com/F72-F75.pdf), generated with kicad-footprint-generator
capacitor tantalum
0
2
2
Capacitor_Tantalum_SMD
CP_EIA-7260-38_AVX-R_Pad2.68x6.30mm_HandSolder
Tantalum Capacitor SMD AVX-R (7260-38 Metric), IPC_7351 nominal, (Body size from: http://datasheets.avx.com/F72-F75.pdf), generated with kicad-footprint-generator
capacitor tantalum
0
2
2
Capacitor_Tantalum_SMD
CP_EIA-7343-15_Kemet-W
Tantalum Capacitor SMD Kemet-W (7343-15 Metric), IPC_7351 nominal, (Body size from: http://www.kemet.com/Lists/ProductCatalog/Attachments/253/KEM_TC101_STD.pdf), generated with kicad-footprint-generator
capacitor tantalum
0
2
2
Capacitor_Tantalum_SMD
CP_EIA-7343-15_Kemet-W_Pad2.25x2.55mm_HandSolder
Tantalum Capacitor SMD Kemet-W (7343-15 Metric), IPC_7351 nominal, (Body size from: http://www.kemet.com/Lists/ProductCatalog/Attachments/253/KEM_TC101_STD.pdf), generated with kicad-footprint-generator
capacitor tantalum
0
2
2
Capacitor_Tantalum_SMD
CP_EIA-7343-20_Kemet-V
Tantalum Capacitor SMD Kemet-V (7343-20 Metric), IPC_7351 nominal, (Body size from: http://www.kemet.com/Lists/ProductCatalog/Attachments/253/KEM_TC101_STD.pdf), generated with kicad-footprint-generator
capacitor tantalum
0
2
2
Capacitor_Tantalum_SMD
CP_EIA-7343-20_Kemet-V_Pad2.25x2.55mm_HandSolder
Tantalum Capacitor SMD Kemet-V (7343-20 Metric), IPC_7351 nominal, (Body size from: http://www.kemet.com/Lists/ProductCatalog/Attachments/253/KEM_TC101_STD.pdf), generated with kicad-footprint-generator
capacitor tantalum
0
2
2
Capacitor_Tantalum_SMD
CP_EIA-7343-30_AVX-N
Tantalum Capacitor SMD AVX-N (7343-30 Metric), IPC_7351 nominal, (Body size from: http://www.kemet.com/Lists/ProductCatalog/Attachments/253/KEM_TC101_STD.pdf), generated with kicad-footprint-generator
capacitor tantalum
0
2
2
Capacitor_Tantalum_SMD
CP_EIA-7343-30_AVX-N_Pad2.25x2.55mm_HandSolder
Tantalum Capacitor SMD AVX-N (7343-30 Metric), IPC_7351 nominal, (Body size from: http://www.kemet.com/Lists/ProductCatalog/Attachments/253/KEM_TC101_STD.pdf), generated with kicad-footprint-generator
capacitor tantalum
0
2
2
Capacitor_Tantalum_SMD
CP_EIA-7343-31_Kemet-D
Tantalum Capacitor SMD Kemet-D (7343-31 Metric), IPC_7351 nominal, (Body size from: http://www.kemet.com/Lists/ProductCatalog/Attachments/253/KEM_TC101_STD.pdf), generated with kicad-footprint-generator
capacitor tantalum
0
2
2
Capacitor_Tantalum_SMD
CP_EIA-7343-31_Kemet-D_Pad2.25x2.55mm_HandSolder
Tantalum Capacitor SMD Kemet-D (7343-31 Metric), IPC_7351 nominal, (Body size from: http://www.kemet.com/Lists/ProductCatalog/Attachments/253/KEM_TC101_STD.pdf), generated with kicad-footprint-generator
capacitor tantalum
0
2
2
Capacitor_Tantalum_SMD
CP_EIA-7343-40_Kemet-Y
Tantalum Capacitor SMD Kemet-Y (7343-40 Metric), IPC_7351 nominal, (Body size from: http://www.kemet.com/Lists/ProductCatalog/Attachments/253/KEM_TC101_STD.pdf), generated with kicad-footprint-generator
capacitor tantalum
0
2
2
Capacitor_Tantalum_SMD
CP_EIA-7343-40_Kemet-Y_Pad2.25x2.55mm_HandSolder
Tantalum Capacitor SMD Kemet-Y (7343-40 Metric), IPC_7351 nominal, (Body size from: http://www.kemet.com/Lists/ProductCatalog/Attachments/253/KEM_TC101_STD.pdf), generated with kicad-footprint-generator
capacitor tantalum
0
2
2
Capacitor_Tantalum_SMD
CP_EIA-7343-43_Kemet-X
Tantalum Capacitor SMD Kemet-X (7343-43 Metric), IPC_7351 nominal, (Body size from: http://www.kemet.com/Lists/ProductCatalog/Attachments/253/KEM_TC101_STD.pdf), generated with kicad-footprint-generator
capacitor tantalum
0
2
2
Capacitor_Tantalum_SMD
CP_EIA-7343-43_Kemet-X_Pad2.25x2.55mm_HandSolder
Tantalum Capacitor SMD Kemet-X (7343-43 Metric), IPC_7351 nominal, (Body size from: http://www.kemet.com/Lists/ProductCatalog/Attachments/253/KEM_TC101_STD.pdf), generated with kicad-footprint-generator
capacitor tantalum
0
2
2
Capacitor_Tantalum_SMD
CP_EIA-7360-38_Kemet-E
Tantalum Capacitor SMD Kemet-E (7360-38 Metric), IPC_7351 nominal, (Body size from: http://www.kemet.com/Lists/ProductCatalog/Attachments/253/KEM_TC101_STD.pdf), generated with kicad-footprint-generator
capacitor tantalum
0
2
2
Capacitor_Tantalum_SMD
CP_EIA-7360-38_Kemet-E_Pad2.25x4.25mm_HandSolder
Tantalum Capacitor SMD Kemet-E (7360-38 Metric), IPC_7351 nominal, (Body size from: http://www.kemet.com/Lists/ProductCatalog/Attachments/253/KEM_TC101_STD.pdf), generated with kicad-footprint-generator
capacitor tantalum
0
2
2
Capacitor_Tantalum_SMD
CP_EIA-7361-38_AVX-V
Tantalum Capacitor SMD AVX-V (7361-38 Metric), IPC_7351 nominal, (Body size from: http://datasheets.avx.com/NOS.pdf), generated with kicad-footprint-generator
capacitor tantalum
0
2
2
Capacitor_Tantalum_SMD
CP_EIA-7361-38_AVX-V_Pad2.18x3.30mm_HandSolder
Tantalum Capacitor SMD AVX-V (7361-38 Metric), IPC_7351 nominal, (Body size from: http://datasheets.avx.com/NOS.pdf), generated with kicad-footprint-generator
capacitor tantalum
0
2
2
Capacitor_Tantalum_SMD
CP_EIA-7361-438_AVX-U
Tantalum Capacitor SMD AVX-U (7361-438 Metric), IPC_7351 nominal, (Body size from: http://datasheets.avx.com/NOS.pdf), generated with kicad-footprint-generator
capacitor tantalum
0
2
2
Capacitor_Tantalum_SMD
CP_EIA-7361-438_AVX-U_Pad2.18x3.30mm_HandSolder
Tantalum Capacitor SMD AVX-U (7361-438 Metric), IPC_7351 nominal, (Body size from: http://datasheets.avx.com/NOS.pdf), generated with kicad-footprint-generator
capacitor tantalum
0
2
2
Connector_IDC
IDC-Header_2x03_P2.54mm_Horizontal
Through hole angled IDC box header, 2x03, 2.54mm pitch, double rows
Through hole IDC box header THT 2x03 2.54mm double row
0
6
6
Connector_IDC
IDC-Header_2x03_P2.54mm_Vertical
Through hole straight IDC box header, 2x03, 2.54mm pitch, double rows
Through hole IDC box header THT 2x03 2.54mm double row
0
6
6
Connector_IDC
IDC-Header_2x04_P2.54mm_Horizontal
Through hole angled IDC box header, 2x04, 2.54mm pitch, double rows
Through hole IDC box header THT 2x04 2.54mm double row
0
8
8
Connector_IDC
IDC-Header_2x04_P2.54mm_Vertical
Through hole straight IDC box header, 2x04, 2.54mm pitch, double rows
Through hole IDC box header THT 2x04 2.54mm double row
0
8
8
Connector_IDC
IDC-Header_2x05_P2.54mm_Horizontal
Through hole angled IDC box header, 2x05, 2.54mm pitch, double rows
Through hole IDC box header THT 2x05 2.54mm double row
0
10
10
Connector_IDC
IDC-Header_2x05_P2.54mm_Horizontal_Lock
Connector IDC Locked, 10 contacts, compatible header: PANCON HE10 (Series 50, (https://www.reboul.fr/storage/00003af6.pdf)
connector idc locked
0
12
10
Connector_IDC
IDC-Header_2x05_P2.54mm_Vertical
Through hole straight IDC box header, 2x05, 2.54mm pitch, double rows
Through hole IDC box header THT 2x05 2.54mm double row
0
10
10
Connector_IDC
IDC-Header_2x05_P2.54mm_Vertical_Lock
Connector IDC Locked, 10 contacts, compatible header: PANCON HE10 (Series 50, (https://www.reboul.fr/storage/00003af6.pdf)
connector idc locked
0
12
10
Connector_IDC
IDC-Header_2x06_P2.54mm_Horizontal
Through hole angled IDC box header, 2x06, 2.54mm pitch, double rows
Through hole IDC box header THT 2x06 2.54mm double row
0
12
12
Connector_IDC
IDC-Header_2x06_P2.54mm_Vertical
Through hole straight IDC box header, 2x06, 2.54mm pitch, double rows
Through hole IDC box header THT 2x06 2.54mm double row
0
12
12
Connector_IDC
IDC-Header_2x07_P2.54mm_Horizontal
Through hole angled IDC box header, 2x07, 2.54mm pitch, double rows
Through hole IDC box header THT 2x07 2.54mm double row
0
14
14
Connector_IDC
IDC-Header_2x07_P2.54mm_Horizontal_Lock
Connector IDC Locked, 10 contacts, compatible header: PANCON HE10 (Series 50, (https://www.reboul.fr/storage/00003af6.pdf)
connector idc locked
0
16
14
Connector_IDC
IDC-Header_2x07_P2.54mm_Vertical
Through hole straight IDC box header, 2x07, 2.54mm pitch, double rows
Through hole IDC box header THT 2x07 2.54mm double row
0
14
14
Connector_IDC
IDC-Header_2x07_P2.54mm_Vertical_Lock
Connector IDC Locked, 10 contacts, compatible header: PANCON HE10 (Series 50, (https://www.reboul.fr/storage/00003af6.pdf)
connector idc locked
0
16
14
Connector_IDC
IDC-Header_2x08_P2.54mm_Horizontal
Through hole angled IDC box header, 2x08, 2.54mm pitch, double rows
Through hole IDC box header THT 2x08 2.54mm double row
0
16
16
Connector_IDC
IDC-Header_2x08_P2.54mm_Horizontal_Lock
Connector IDC Locked, 10 contacts, compatible header: PANCON HE10 (Series 50, (https://www.reboul.fr/storage/00003af6.pdf)
connector idc locked
0
18
16
Connector_IDC
IDC-Header_2x08_P2.54mm_Vertical
Through hole straight IDC box header, 2x08, 2.54mm pitch, double rows
Through hole IDC box header THT 2x08 2.54mm double row
0
16
16
Connector_IDC
IDC-Header_2x08_P2.54mm_Vertical_Lock
Connector IDC Locked, 10 contacts, compatible header: PANCON HE10 (Series 50, (https://www.reboul.fr/storage/00003af6.pdf)
connector idc locked
0
18
16
Connector_IDC
IDC-Header_2x10_P2.54mm_Horizontal
Through hole angled IDC box header, 2x10, 2.54mm pitch, double rows
Through hole IDC box header THT 2x10 2.54mm double row
0
20
20
Connector_IDC
IDC-Header_2x10_P2.54mm_Horizontal_Lock
Connector IDC Locked, 10 contacts, compatible header: PANCON HE10 (Series 50, (https://www.reboul.fr/storage/00003af6.pdf)
connector idc locked
0
22
20
Connector_IDC
IDC-Header_2x10_P2.54mm_Vertical
Through hole straight IDC box header, 2x10, 2.54mm pitch, double rows
Through hole IDC box header THT 2x10 2.54mm double row
0
20
20
Connector_IDC
IDC-Header_2x10_P2.54mm_Vertical_Lock
Connector IDC Locked, 10 contacts, compatible header: PANCON HE10 (Series 50, (https://www.reboul.fr/storage/00003af6.pdf)
connector idc locked
0
22
20
Connector_IDC
IDC-Header_2x13_P2.54mm_Horizontal
Through hole angled IDC box header, 2x13, 2.54mm pitch, double rows
Through hole IDC box header THT 2x13 2.54mm double row
0
26
26
Connector_IDC
IDC-Header_2x13_P2.54mm_Horizontal_Lock
Connector IDC Locked, 10 contacts, compatible header: PANCON HE10 (Series 50, (https://www.reboul.fr/storage/00003af6.pdf)
connector idc locked
0
28
26
Connector_IDC
IDC-Header_2x13_P2.54mm_Vertical
Through hole straight IDC box header, 2x13, 2.54mm pitch, double rows
Through hole IDC box header THT 2x13 2.54mm double row
0
26
26
Connector_IDC
IDC-Header_2x13_P2.54mm_Vertical_Lock
Connector IDC Locked, 10 contacts, compatible header: PANCON HE10 (Series 50, (https://www.reboul.fr/storage/00003af6.pdf)
connector idc locked
0
28
26
Connector_IDC
IDC-Header_2x15_P2.54mm_Horizontal
Through hole angled IDC box header, 2x15, 2.54mm pitch, double rows
Through hole IDC box header THT 2x15 2.54mm double row
0
30
30
Connector_IDC
IDC-Header_2x15_P2.54mm_Vertical
Through hole straight IDC box header, 2x15, 2.54mm pitch, double rows
Through hole IDC box header THT 2x15 2.54mm double row
0
30
30
Connector_IDC
IDC-Header_2x17_P2.54mm_Horizontal
Through hole angled IDC box header, 2x17, 2.54mm pitch, double rows
Through hole IDC box header THT 2x17 2.54mm double row
0
34
34
Connector_IDC
IDC-Header_2x17_P2.54mm_Horizontal_Lock
Connector IDC Locked, 10 contacts, compatible header: PANCON HE10 (Series 50, (https://www.reboul.fr/storage/00003af6.pdf)
connector idc locked
0
36
34
Connector_IDC
IDC-Header_2x17_P2.54mm_Vertical
Through hole straight IDC box header, 2x17, 2.54mm pitch, double rows
Through hole IDC box header THT 2x17 2.54mm double row
0
34
34
Connector_IDC
IDC-Header_2x17_P2.54mm_Vertical_Lock
Connector IDC Locked, 10 contacts, compatible header: PANCON HE10 (Series 50, (https://www.reboul.fr/storage/00003af6.pdf)
connector idc locked
0
36
34
Connector_IDC
IDC-Header_2x20_P2.54mm_Horizontal
Through hole angled IDC box header, 2x20, 2.54mm pitch, double rows
Through hole IDC box header THT 2x20 2.54mm double row
0
40
40
Connector_IDC
IDC-Header_2x20_P2.54mm_Horizontal_Lock
Connector IDC Locked, 10 contacts, compatible header: PANCON HE10 (Series 50, (https://www.reboul.fr/storage/00003af6.pdf)
connector idc locked
0
42
41
Connector_IDC
IDC-Header_2x20_P2.54mm_Vertical
Through hole straight IDC box header, 2x20, 2.54mm pitch, double rows
Through hole IDC box header THT 2x20 2.54mm double row
0
40
40
Connector_IDC
IDC-Header_2x20_P2.54mm_Vertical_Lock
Connector IDC Locked, 10 contacts, compatible header: PANCON HE10 (Series 50, (https://www.reboul.fr/storage/00003af6.pdf)
connector idc locked
0
42
40
Connector_IDC
IDC-Header_2x25_P2.54mm_Horizontal
Through hole angled IDC box header, 2x25, 2.54mm pitch, double rows
Through hole IDC box header THT 2x25 2.54mm double row
0
50
50
Connector_IDC
IDC-Header_2x25_P2.54mm_Vertical
Through hole straight IDC box header, 2x25, 2.54mm pitch, double rows
Through hole IDC box header THT 2x25 2.54mm double row
0
50
50
Connector_IDC
IDC-Header_2x25_P2.54mm_Vertical_Lock
Connector IDC Locked, 10 contacts, compatible header: PANCON HE10 (Series 50, (https://www.reboul.fr/storage/00003af6.pdf)
connector idc locked
0
52
50
Connector_IDC
IDC-Header_2x30_P2.54mm_Horizontal
Through hole angled IDC box header, 2x30, 2.54mm pitch, double rows
Through hole IDC box header THT 2x30 2.54mm double row
0
60
60
Connector_IDC
IDC-Header_2x30_P2.54mm_Vertical
Through hole straight IDC box header, 2x30, 2.54mm pitch, double rows
Through hole IDC box header THT 2x30 2.54mm double row
0
60
60
Connector_IDC
IDC-Header_2x30_P2.54mm_Vertical_Lock
Connector IDC Locked, 10 contacts, compatible header: PANCON HE10 (Series 50, (https://www.reboul.fr/storage/00003af6.pdf)
connector idc locked
0
62
60
Connector_IDC
IDC-Header_2x32_P2.54mm_Horizontal
Through hole angled IDC box header, 2x32, 2.54mm pitch, double rows
Through hole IDC box header THT 2x32 2.54mm double row
0
64
64
Connector_IDC
IDC-Header_2x32_P2.54mm_Vertical
Through hole straight IDC box header, 2x32, 2.54mm pitch, double rows
Through hole IDC box header THT 2x32 2.54mm double row
0
64
64
Connector_IDC
IDC-Header_2x32_P2.54mm_Vertical_Lock
Connector IDC Locked, 10 contacts, compatible header: PANCON HE10 (Series 50, (https://www.reboul.fr/storage/00003af6.pdf)
connector idc locked
0
66
64
Connector_PinHeader_2.54mm
PinHeader_1x01_P2.54mm_Horizontal
Through hole angled pin header, 1x01, 2.54mm pitch, 6mm pin length, single row
Through hole angled pin header THT 1x01 2.54mm single row
0
1
1
Connector_PinHeader_2.54mm
PinHeader_1x01_P2.54mm_Vertical
Through hole straight pin header, 1x01, 2.54mm pitch, single row
Through hole pin header THT 1x01 2.54mm single row
0
1
1
Connector_PinHeader_2.54mm
PinHeader_1x02_P2.54mm_Horizontal
Through hole angled pin header, 1x02, 2.54mm pitch, 6mm pin length, single row
Through hole angled pin header THT 1x02 2.54mm single row
0
2
2
Connector_PinHeader_2.54mm
PinHeader_1x02_P2.54mm_Vertical
Through hole straight pin header, 1x02, 2.54mm pitch, single row
Through hole pin header THT 1x02 2.54mm single row
0
2
2
Connector_PinHeader_2.54mm
PinHeader_1x02_P2.54mm_Vertical_SMD_Pin1Left
surface-mounted straight pin header, 1x02, 2.54mm pitch, single row, style 1 (pin 1 left)
Surface mounted pin header SMD 1x02 2.54mm single row style1 pin1 left
0
2
2
Connector_PinHeader_2.54mm
PinHeader_1x02_P2.54mm_Vertical_SMD_Pin1Right
surface-mounted straight pin header, 1x02, 2.54mm pitch, single row, style 2 (pin 1 right)
Surface mounted pin header SMD 1x02 2.54mm single row style2 pin1 right
0
2
2
Connector_PinHeader_2.54mm
PinHeader_1x03_P2.54mm_Horizontal
Through hole angled pin header, 1x03, 2.54mm pitch, 6mm pin length, single row
Through hole angled pin header THT 1x03 2.54mm single row
0
3
3
Connector_PinHeader_2.54mm
PinHeader_1x03_P2.54mm_Vertical
Through hole straight pin header, 1x03, 2.54mm pitch, single row
Through hole pin header THT 1x03 2.54mm single row
0
3
3
Connector_PinHeader_2.54mm
PinHeader_1x03_P2.54mm_Vertical_SMD_Pin1Left
surface-mounted straight pin header, 1x03, 2.54mm pitch, single row, style 1 (pin 1 left)
Surface mounted pin header SMD 1x03 2.54mm single row style1 pin1 left
0
3
3
Connector_PinHeader_2.54mm
PinHeader_1x03_P2.54mm_Vertical_SMD_Pin1Right
surface-mounted straight pin header, 1x03, 2.54mm pitch, single row, style 2 (pin 1 right)
Surface mounted pin header SMD 1x03 2.54mm single row style2 pin1 right
0
3
3
Connector_PinHeader_2.54mm
PinHeader_1x04_P2.54mm_Horizontal
Through hole angled pin header, 1x04, 2.54mm pitch, 6mm pin length, single row
Through hole angled pin header THT 1x04 2.54mm single row
0
4
4
Connector_PinHeader_2.54mm
PinHeader_1x04_P2.54mm_Vertical
Through hole straight pin header, 1x04, 2.54mm pitch, single row
Through hole pin header THT 1x04 2.54mm single row
0
4
4
Connector_PinHeader_2.54mm
PinHeader_1x04_P2.54mm_Vertical_SMD_Pin1Left
surface-mounted straight pin header, 1x04, 2.54mm pitch, single row, style 1 (pin 1 left)
Surface mounted pin header SMD 1x04 2.54mm single row style1 pin1 left
0
4
4
Connector_PinHeader_2.54mm
PinHeader_1x04_P2.54mm_Vertical_SMD_Pin1Right
surface-mounted straight pin header, 1x04, 2.54mm pitch, single row, style 2 (pin 1 right)
Surface mounted pin header SMD 1x04 2.54mm single row style2 pin1 right
0
4
4
Connector_PinHeader_2.54mm
PinHeader_1x05_P2.54mm_Horizontal
Through hole angled pin header, 1x05, 2.54mm pitch, 6mm pin length, single row
Through hole angled pin header THT 1x05 2.54mm single row
0
5
5
Connector_PinHeader_2.54mm
PinHeader_1x05_P2.54mm_Vertical
Through hole straight pin header, 1x05, 2.54mm pitch, single row
Through hole pin header THT 1x05 2.54mm single row
0
5
5
Connector_PinHeader_2.54mm
PinHeader_1x05_P2.54mm_Vertical_SMD_Pin1Left
surface-mounted straight pin header, 1x05, 2.54mm pitch, single row, style 1 (pin 1 left)
Surface mounted pin header SMD 1x05 2.54mm single row style1 pin1 left
0
5
5
Connector_PinHeader_2.54mm
PinHeader_1x05_P2.54mm_Vertical_SMD_Pin1Right
surface-mounted straight pin header, 1x05, 2.54mm pitch, single row, style 2 (pin 1 right)
Surface mounted pin header SMD 1x05 2.54mm single row style2 pin1 right
0
5
5
Connector_PinHeader_2.54mm
PinHeader_1x06_P2.54mm_Horizontal
Through hole angled pin header, 1x06, 2.54mm pitch, 6mm pin length, single row
Through hole angled pin header THT 1x06 2.54mm single row
0
6
6
Connector_PinHeader_2.54mm
PinHeader_1x06_P2.54mm_Vertical
Through hole straight pin header, 1x06, 2.54mm pitch, single row
Through hole pin header THT 1x06 2.54mm single row
0
6
6
Connector_PinHeader_2.54mm
PinHeader_1x06_P2.54mm_Vertical_SMD_Pin1Left
surface-mounted straight pin header, 1x06, 2.54mm pitch, single row, style 1 (pin 1 left)
Surface mounted pin header SMD 1x06 2.54mm single row style1 pin1 left
0
6
6
Connector_PinHeader_2.54mm
PinHeader_1x06_P2.54mm_Vertical_SMD_Pin1Right
surface-mounted straight pin header, 1x06, 2.54mm pitch, single row, style 2 (pin 1 right)
Surface mounted pin header SMD 1x06 2.54mm single row style2 pin1 right
0
6
6
Connector_PinHeader_2.54mm
PinHeader_1x07_P2.54mm_Horizontal
Through hole angled pin header, 1x07, 2.54mm pitch, 6mm pin length, single row
Through hole angled pin header THT 1x07 2.54mm single row
0
7
7
Connector_PinHeader_2.54mm
PinHeader_1x07_P2.54mm_Vertical
Through hole straight pin header, 1x07, 2.54mm pitch, single row
Through hole pin header THT 1x07 2.54mm single row
0
7
7
Connector_PinHeader_2.54mm
PinHeader_1x07_P2.54mm_Vertical_SMD_Pin1Left
surface-mounted straight pin header, 1x07, 2.54mm pitch, single row, style 1 (pin 1 left)
Surface mounted pin header SMD 1x07 2.54mm single row style1 pin1 left
0
7
7
Connector_PinHeader_2.54mm
PinHeader_1x07_P2.54mm_Vertical_SMD_Pin1Right
surface-mounted straight pin header, 1x07, 2.54mm pitch, single row, style 2 (pin 1 right)
Surface mounted pin header SMD 1x07 2.54mm single row style2 pin1 right
0
7
7
Connector_PinHeader_2.54mm
PinHeader_1x08_P2.54mm_Horizontal
Through hole angled pin header, 1x08, 2.54mm pitch, 6mm pin length, single row
Through hole angled pin header THT 1x08 2.54mm single row
0
8
8
Connector_PinHeader_2.54mm
PinHeader_1x08_P2.54mm_Vertical
Through hole straight pin header, 1x08, 2.54mm pitch, single row
Through hole pin header THT 1x08 2.54mm single row
0
8
8
Connector_PinHeader_2.54mm
PinHeader_1x08_P2.54mm_Vertical_SMD_Pin1Left
surface-mounted straight pin header, 1x08, 2.54mm pitch, single row, style 1 (pin 1 left)
Surface mounted pin header SMD 1x08 2.54mm single row style1 pin1 left
0
8
8
Connector_PinHeader_2.54mm
PinHeader_1x08_P2.54mm_Vertical_SMD_Pin1Right
surface-mounted straight pin header, 1x08, 2.54mm pitch, single row, style 2 (pin 1 right)
Surface mounted pin header SMD 1x08 2.54mm single row style2 pin1 right
0
8
8
Connector_PinHeader_2.54mm
PinHeader_1x09_P2.54mm_Horizontal
Through hole angled pin header, 1x09, 2.54mm pitch, 6mm pin length, single row
Through hole angled pin header THT 1x09 2.54mm single row
0
9
9
Connector_PinHeader_2.54mm
PinHeader_1x09_P2.54mm_Vertical
Through hole straight pin header, 1x09, 2.54mm pitch, single row
Through hole pin header THT 1x09 2.54mm single row
0
9
9
Connector_PinHeader_2.54mm
PinHeader_1x09_P2.54mm_Vertical_SMD_Pin1Left
surface-mounted straight pin header, 1x09, 2.54mm pitch, single row, style 1 (pin 1 left)
Surface mounted pin header SMD 1x09 2.54mm single row style1 pin1 left
0
9
9
Connector_PinHeader_2.54mm
PinHeader_1x09_P2.54mm_Vertical_SMD_Pin1Right
surface-mounted straight pin header, 1x09, 2.54mm pitch, single row, style 2 (pin 1 right)
Surface mounted pin header SMD 1x09 2.54mm single row style2 pin1 right
0
9
9
Connector_PinHeader_2.54mm
PinHeader_1x10_P2.54mm_Horizontal
Through hole angled pin header, 1x10, 2.54mm pitch, 6mm pin length, single row
Through hole angled pin header THT 1x10 2.54mm single row
0
10
10
Connector_PinHeader_2.54mm
PinHeader_1x10_P2.54mm_Vertical
Through hole straight pin header, 1x10, 2.54mm pitch, single row
Through hole pin header THT 1x10 2.54mm single row
0
10
10
Connector_PinHeader_2.54mm
PinHeader_1x10_P2.54mm_Vertical_SMD_Pin1Left
surface-mounted straight pin header, 1x10, 2.54mm pitch, single row, style 1 (pin 1 left)
Surface mounted pin header SMD 1x10 2.54mm single row style1 pin1 left
0
10
10
Connector_PinHeader_2.54mm
PinHeader_1x10_P2.54mm_Vertical_SMD_Pin1Right
surface-mounted straight pin header, 1x10, 2.54mm pitch, single row, style 2 (pin 1 right)
Surface mounted pin header SMD 1x10 2.54mm single row style2 pin1 right
0
10
10
Connector_PinHeader_2.54mm
PinHeader_1x11_P2.54mm_Horizontal
Through hole angled pin header, 1x11, 2.54mm pitch, 6mm pin length, single row
Through hole angled pin header THT 1x11 2.54mm single row
0
11
11
Connector_PinHeader_2.54mm
PinHeader_1x11_P2.54mm_Vertical
Through hole straight pin header, 1x11, 2.54mm pitch, single row
Through hole pin header THT 1x11 2.54mm single row
0
11
11
Connector_PinHeader_2.54mm
PinHeader_1x11_P2.54mm_Vertical_SMD_Pin1Left
surface-mounted straight pin header, 1x11, 2.54mm pitch, single row, style 1 (pin 1 left)
Surface mounted pin header SMD 1x11 2.54mm single row style1 pin1 left
0
11
11
Connector_PinHeader_2.54mm
PinHeader_1x11_P2.54mm_Vertical_SMD_Pin1Right
surface-mounted straight pin header, 1x11, 2.54mm pitch, single row, style 2 (pin 1 right)
Surface mounted pin header SMD 1x11 2.54mm single row style2 pin1 right
0
11
11
Connector_PinHeader_2.54mm
PinHeader_1x12_P2.54mm_Horizontal
Through hole angled pin header, 1x12, 2.54mm pitch, 6mm pin length, single row
Through hole angled pin header THT 1x12 2.54mm single row
0
12
12
Connector_PinHeader_2.54mm
PinHeader_1x12_P2.54mm_Vertical
Through hole straight pin header, 1x12, 2.54mm pitch, single row
Through hole pin header THT 1x12 2.54mm single row
0
12
12
Connector_PinHeader_2.54mm
PinHeader_1x12_P2.54mm_Vertical_SMD_Pin1Left
surface-mounted straight pin header, 1x12, 2.54mm pitch, single row, style 1 (pin 1 left)
Surface mounted pin header SMD 1x12 2.54mm single row style1 pin1 left
0
12
12
Connector_PinHeader_2.54mm
PinHeader_1x12_P2.54mm_Vertical_SMD_Pin1Right
surface-mounted straight pin header, 1x12, 2.54mm pitch, single row, style 2 (pin 1 right)
Surface mounted pin header SMD 1x12 2.54mm single row style2 pin1 right
0
12
12
Connector_PinHeader_2.54mm
PinHeader_1x13_P2.54mm_Horizontal
Through hole angled pin header, 1x13, 2.54mm pitch, 6mm pin length, single row
Through hole angled pin header THT 1x13 2.54mm single row
0
13
13
Connector_PinHeader_2.54mm
PinHeader_1x13_P2.54mm_Vertical
Through hole straight pin header, 1x13, 2.54mm pitch, single row
Through hole pin header THT 1x13 2.54mm single row
0
13
13
Connector_PinHeader_2.54mm
PinHeader_1x13_P2.54mm_Vertical_SMD_Pin1Left
surface-mounted straight pin header, 1x13, 2.54mm pitch, single row, style 1 (pin 1 left)
Surface mounted pin header SMD 1x13 2.54mm single row style1 pin1 left
0
13
13
Connector_PinHeader_2.54mm
PinHeader_1x13_P2.54mm_Vertical_SMD_Pin1Right
surface-mounted straight pin header, 1x13, 2.54mm pitch, single row, style 2 (pin 1 right)
Surface mounted pin header SMD 1x13 2.54mm single row style2 pin1 right
0
13
13
Connector_PinHeader_2.54mm
PinHeader_1x14_P2.54mm_Horizontal
Through hole angled pin header, 1x14, 2.54mm pitch, 6mm pin length, single row
Through hole angled pin header THT 1x14 2.54mm single row
0
14
14
Connector_PinHeader_2.54mm
PinHeader_1x14_P2.54mm_Vertical
Through hole straight pin header, 1x14, 2.54mm pitch, single row
Through hole pin header THT 1x14 2.54mm single row
0
14
14
Connector_PinHeader_2.54mm
PinHeader_1x14_P2.54mm_Vertical_SMD_Pin1Left
surface-mounted straight pin header, 1x14, 2.54mm pitch, single row, style 1 (pin 1 left)
Surface mounted pin header SMD 1x14 2.54mm single row style1 pin1 left
0
14
14
Connector_PinHeader_2.54mm
PinHeader_1x14_P2.54mm_Vertical_SMD_Pin1Right
surface-mounted straight pin header, 1x14, 2.54mm pitch, single row, style 2 (pin 1 right)
Surface mounted pin header SMD 1x14 2.54mm single row style2 pin1 right
0
14
14
Connector_PinHeader_2.54mm
PinHeader_1x15_P2.54mm_Horizontal
Through hole angled pin header, 1x15, 2.54mm pitch, 6mm pin length, single row
Through hole angled pin header THT 1x15 2.54mm single row
0
15
15
Connector_PinHeader_2.54mm
PinHeader_1x15_P2.54mm_Vertical
Through hole straight pin header, 1x15, 2.54mm pitch, single row
Through hole pin header THT 1x15 2.54mm single row
0
15
15
Connector_PinHeader_2.54mm
PinHeader_1x15_P2.54mm_Vertical_SMD_Pin1Left
surface-mounted straight pin header, 1x15, 2.54mm pitch, single row, style 1 (pin 1 left)
Surface mounted pin header SMD 1x15 2.54mm single row style1 pin1 left
0
15
15
Connector_PinHeader_2.54mm
PinHeader_1x15_P2.54mm_Vertical_SMD_Pin1Right
surface-mounted straight pin header, 1x15, 2.54mm pitch, single row, style 2 (pin 1 right)
Surface mounted pin header SMD 1x15 2.54mm single row style2 pin1 right
0
15
15
Connector_PinHeader_2.54mm
PinHeader_1x16_P2.54mm_Horizontal
Through hole angled pin header, 1x16, 2.54mm pitch, 6mm pin length, single row
Through hole angled pin header THT 1x16 2.54mm single row
0
16
16
Connector_PinHeader_2.54mm
PinHeader_1x16_P2.54mm_Vertical
Through hole straight pin header, 1x16, 2.54mm pitch, single row
Through hole pin header THT 1x16 2.54mm single row
0
16
16
Connector_PinHeader_2.54mm
PinHeader_1x16_P2.54mm_Vertical_SMD_Pin1Left
surface-mounted straight pin header, 1x16, 2.54mm pitch, single row, style 1 (pin 1 left)
Surface mounted pin header SMD 1x16 2.54mm single row style1 pin1 left
0
16
16
Connector_PinHeader_2.54mm
PinHeader_1x16_P2.54mm_Vertical_SMD_Pin1Right
surface-mounted straight pin header, 1x16, 2.54mm pitch, single row, style 2 (pin 1 right)
Surface mounted pin header SMD 1x16 2.54mm single row style2 pin1 right
0
16
16
Connector_PinHeader_2.54mm
PinHeader_1x17_P2.54mm_Horizontal
Through hole angled pin header, 1x17, 2.54mm pitch, 6mm pin length, single row
Through hole angled pin header THT 1x17 2.54mm single row
0
17
17
Connector_PinHeader_2.54mm
PinHeader_1x17_P2.54mm_Vertical
Through hole straight pin header, 1x17, 2.54mm pitch, single row
Through hole pin header THT 1x17 2.54mm single row
0
17
17
Connector_PinHeader_2.54mm
PinHeader_1x17_P2.54mm_Vertical_SMD_Pin1Left
surface-mounted straight pin header, 1x17, 2.54mm pitch, single row, style 1 (pin 1 left)
Surface mounted pin header SMD 1x17 2.54mm single row style1 pin1 left
0
17
17
Connector_PinHeader_2.54mm
PinHeader_1x17_P2.54mm_Vertical_SMD_Pin1Right
surface-mounted straight pin header, 1x17, 2.54mm pitch, single row, style 2 (pin 1 right)
Surface mounted pin header SMD 1x17 2.54mm single row style2 pin1 right
0
17
17
Connector_PinHeader_2.54mm
PinHeader_1x18_P2.54mm_Horizontal
Through hole angled pin header, 1x18, 2.54mm pitch, 6mm pin length, single row
Through hole angled pin header THT 1x18 2.54mm single row
0
18
18
Connector_PinHeader_2.54mm
PinHeader_1x18_P2.54mm_Vertical
Through hole straight pin header, 1x18, 2.54mm pitch, single row
Through hole pin header THT 1x18 2.54mm single row
0
18
18
Connector_PinHeader_2.54mm
PinHeader_1x18_P2.54mm_Vertical_SMD_Pin1Left
surface-mounted straight pin header, 1x18, 2.54mm pitch, single row, style 1 (pin 1 left)
Surface mounted pin header SMD 1x18 2.54mm single row style1 pin1 left
0
18
18
Connector_PinHeader_2.54mm
PinHeader_1x18_P2.54mm_Vertical_SMD_Pin1Right
surface-mounted straight pin header, 1x18, 2.54mm pitch, single row, style 2 (pin 1 right)
Surface mounted pin header SMD 1x18 2.54mm single row style2 pin1 right
0
18
18
Connector_PinHeader_2.54mm
PinHeader_1x19_P2.54mm_Horizontal
Through hole angled pin header, 1x19, 2.54mm pitch, 6mm pin length, single row
Through hole angled pin header THT 1x19 2.54mm single row
0
19
19
Connector_PinHeader_2.54mm
PinHeader_1x19_P2.54mm_Vertical
Through hole straight pin header, 1x19, 2.54mm pitch, single row
Through hole pin header THT 1x19 2.54mm single row
0
19
19
Connector_PinHeader_2.54mm
PinHeader_1x19_P2.54mm_Vertical_SMD_Pin1Left
surface-mounted straight pin header, 1x19, 2.54mm pitch, single row, style 1 (pin 1 left)
Surface mounted pin header SMD 1x19 2.54mm single row style1 pin1 left
0
19
19
Connector_PinHeader_2.54mm
PinHeader_1x19_P2.54mm_Vertical_SMD_Pin1Right
surface-mounted straight pin header, 1x19, 2.54mm pitch, single row, style 2 (pin 1 right)
Surface mounted pin header SMD 1x19 2.54mm single row style2 pin1 right
0
19
19
Connector_PinHeader_2.54mm
PinHeader_1x20_P2.54mm_Horizontal
Through hole angled pin header, 1x20, 2.54mm pitch, 6mm pin length, single row
Through hole angled pin header THT 1x20 2.54mm single row
0
20
20
Connector_PinHeader_2.54mm
PinHeader_1x20_P2.54mm_Vertical
Through hole straight pin header, 1x20, 2.54mm pitch, single row
Through hole pin header THT 1x20 2.54mm single row
0
20
20
Connector_PinHeader_2.54mm
PinHeader_1x20_P2.54mm_Vertical_SMD_Pin1Left
surface-mounted straight pin header, 1x20, 2.54mm pitch, single row, style 1 (pin 1 left)
Surface mounted pin header SMD 1x20 2.54mm single row style1 pin1 left
0
20
20
Connector_PinHeader_2.54mm
PinHeader_1x20_P2.54mm_Vertical_SMD_Pin1Right
surface-mounted straight pin header, 1x20, 2.54mm pitch, single row, style 2 (pin 1 right)
Surface mounted pin header SMD 1x20 2.54mm single row style2 pin1 right
0
20
20
Connector_PinHeader_2.54mm
PinHeader_1x21_P2.54mm_Horizontal
Through hole angled pin header, 1x21, 2.54mm pitch, 6mm pin length, single row
Through hole angled pin header THT 1x21 2.54mm single row
0
21
21
Connector_PinHeader_2.54mm
PinHeader_1x21_P2.54mm_Vertical
Through hole straight pin header, 1x21, 2.54mm pitch, single row
Through hole pin header THT 1x21 2.54mm single row
0
21
21
Connector_PinHeader_2.54mm
PinHeader_1x21_P2.54mm_Vertical_SMD_Pin1Left
surface-mounted straight pin header, 1x21, 2.54mm pitch, single row, style 1 (pin 1 left)
Surface mounted pin header SMD 1x21 2.54mm single row style1 pin1 left
0
21
21
Connector_PinHeader_2.54mm
PinHeader_1x21_P2.54mm_Vertical_SMD_Pin1Right
surface-mounted straight pin header, 1x21, 2.54mm pitch, single row, style 2 (pin 1 right)
Surface mounted pin header SMD 1x21 2.54mm single row style2 pin1 right
0
21
21
Connector_PinHeader_2.54mm
PinHeader_1x22_P2.54mm_Horizontal
Through hole angled pin header, 1x22, 2.54mm pitch, 6mm pin length, single row
Through hole angled pin header THT 1x22 2.54mm single row
0
22
22
Connector_PinHeader_2.54mm
PinHeader_1x22_P2.54mm_Vertical
Through hole straight pin header, 1x22, 2.54mm pitch, single row
Through hole pin header THT 1x22 2.54mm single row
0
22
22
Connector_PinHeader_2.54mm
PinHeader_1x22_P2.54mm_Vertical_SMD_Pin1Left
surface-mounted straight pin header, 1x22, 2.54mm pitch, single row, style 1 (pin 1 left)
Surface mounted pin header SMD 1x22 2.54mm single row style1 pin1 left
0
22
22
Connector_PinHeader_2.54mm
PinHeader_1x22_P2.54mm_Vertical_SMD_Pin1Right
surface-mounted straight pin header, 1x22, 2.54mm pitch, single row, style 2 (pin 1 right)
Surface mounted pin header SMD 1x22 2.54mm single row style2 pin1 right
0
22
22
Connector_PinHeader_2.54mm
PinHeader_1x23_P2.54mm_Horizontal
Through hole angled pin header, 1x23, 2.54mm pitch, 6mm pin length, single row
Through hole angled pin header THT 1x23 2.54mm single row
0
23
23
Connector_PinHeader_2.54mm
PinHeader_1x23_P2.54mm_Vertical
Through hole straight pin header, 1x23, 2.54mm pitch, single row
Through hole pin header THT 1x23 2.54mm single row
0
23
23
Connector_PinHeader_2.54mm
PinHeader_1x23_P2.54mm_Vertical_SMD_Pin1Left
surface-mounted straight pin header, 1x23, 2.54mm pitch, single row, style 1 (pin 1 left)
Surface mounted pin header SMD 1x23 2.54mm single row style1 pin1 left
0
23
23
Connector_PinHeader_2.54mm
PinHeader_1x23_P2.54mm_Vertical_SMD_Pin1Right
surface-mounted straight pin header, 1x23, 2.54mm pitch, single row, style 2 (pin 1 right)
Surface mounted pin header SMD 1x23 2.54mm single row style2 pin1 right
0
23
23
Connector_PinHeader_2.54mm
PinHeader_1x24_P2.54mm_Horizontal
Through hole angled pin header, 1x24, 2.54mm pitch, 6mm pin length, single row
Through hole angled pin header THT 1x24 2.54mm single row
0
24
24
Connector_PinHeader_2.54mm
PinHeader_1x24_P2.54mm_Vertical
Through hole straight pin header, 1x24, 2.54mm pitch, single row
Through hole pin header THT 1x24 2.54mm single row
0
24
24
Connector_PinHeader_2.54mm
PinHeader_1x24_P2.54mm_Vertical_SMD_Pin1Left
surface-mounted straight pin header, 1x24, 2.54mm pitch, single row, style 1 (pin 1 left)
Surface mounted pin header SMD 1x24 2.54mm single row style1 pin1 left
0
24
24
Connector_PinHeader_2.54mm
PinHeader_1x24_P2.54mm_Vertical_SMD_Pin1Right
surface-mounted straight pin header, 1x24, 2.54mm pitch, single row, style 2 (pin 1 right)
Surface mounted pin header SMD 1x24 2.54mm single row style2 pin1 right
0
24
24
Connector_PinHeader_2.54mm
PinHeader_1x25_P2.54mm_Horizontal
Through hole angled pin header, 1x25, 2.54mm pitch, 6mm pin length, single row
Through hole angled pin header THT 1x25 2.54mm single row
0
25
25
Connector_PinHeader_2.54mm
PinHeader_1x25_P2.54mm_Vertical
Through hole straight pin header, 1x25, 2.54mm pitch, single row
Through hole pin header THT 1x25 2.54mm single row
0
25
25
Connector_PinHeader_2.54mm
PinHeader_1x25_P2.54mm_Vertical_SMD_Pin1Left
surface-mounted straight pin header, 1x25, 2.54mm pitch, single row, style 1 (pin 1 left)
Surface mounted pin header SMD 1x25 2.54mm single row style1 pin1 left
0
25
25
Connector_PinHeader_2.54mm
PinHeader_1x25_P2.54mm_Vertical_SMD_Pin1Right
surface-mounted straight pin header, 1x25, 2.54mm pitch, single row, style 2 (pin 1 right)
Surface mounted pin header SMD 1x25 2.54mm single row style2 pin1 right
0
25
25
Connector_PinHeader_2.54mm
PinHeader_1x26_P2.54mm_Horizontal
Through hole angled pin header, 1x26, 2.54mm pitch, 6mm pin length, single row
Through hole angled pin header THT 1x26 2.54mm single row
0
26
26
Connector_PinHeader_2.54mm
PinHeader_1x26_P2.54mm_Vertical
Through hole straight pin header, 1x26, 2.54mm pitch, single row
Through hole pin header THT 1x26 2.54mm single row
0
26
26
Connector_PinHeader_2.54mm
PinHeader_1x26_P2.54mm_Vertical_SMD_Pin1Left
surface-mounted straight pin header, 1x26, 2.54mm pitch, single row, style 1 (pin 1 left)
Surface mounted pin header SMD 1x26 2.54mm single row style1 pin1 left
0
26
26
Connector_PinHeader_2.54mm
PinHeader_1x26_P2.54mm_Vertical_SMD_Pin1Right
surface-mounted straight pin header, 1x26, 2.54mm pitch, single row, style 2 (pin 1 right)
Surface mounted pin header SMD 1x26 2.54mm single row style2 pin1 right
0
26
26
Connector_PinHeader_2.54mm
PinHeader_1x27_P2.54mm_Horizontal
Through hole angled pin header, 1x27, 2.54mm pitch, 6mm pin length, single row
Through hole angled pin header THT 1x27 2.54mm single row
0
27
27
Connector_PinHeader_2.54mm
PinHeader_1x27_P2.54mm_Vertical
Through hole straight pin header, 1x27, 2.54mm pitch, single row
Through hole pin header THT 1x27 2.54mm single row
0
27
27
Connector_PinHeader_2.54mm
PinHeader_1x27_P2.54mm_Vertical_SMD_Pin1Left
surface-mounted straight pin header, 1x27, 2.54mm pitch, single row, style 1 (pin 1 left)
Surface mounted pin header SMD 1x27 2.54mm single row style1 pin1 left
0
27
27
Connector_PinHeader_2.54mm
PinHeader_1x27_P2.54mm_Vertical_SMD_Pin1Right
surface-mounted straight pin header, 1x27, 2.54mm pitch, single row, style 2 (pin 1 right)
Surface mounted pin header SMD 1x27 2.54mm single row style2 pin1 right
0
27
27
Connector_PinHeader_2.54mm
PinHeader_1x28_P2.54mm_Horizontal
Through hole angled pin header, 1x28, 2.54mm pitch, 6mm pin length, single row
Through hole angled pin header THT 1x28 2.54mm single row
0
28
28
Connector_PinHeader_2.54mm
PinHeader_1x28_P2.54mm_Vertical
Through hole straight pin header, 1x28, 2.54mm pitch, single row
Through hole pin header THT 1x28 2.54mm single row
0
28
28
Connector_PinHeader_2.54mm
PinHeader_1x28_P2.54mm_Vertical_SMD_Pin1Left
surface-mounted straight pin header, 1x28, 2.54mm pitch, single row, style 1 (pin 1 left)
Surface mounted pin header SMD 1x28 2.54mm single row style1 pin1 left
0
28
28
Connector_PinHeader_2.54mm
PinHeader_1x28_P2.54mm_Vertical_SMD_Pin1Right
surface-mounted straight pin header, 1x28, 2.54mm pitch, single row, style 2 (pin 1 right)
Surface mounted pin header SMD 1x28 2.54mm single row style2 pin1 right
0
28
28
Connector_PinHeader_2.54mm
PinHeader_1x29_P2.54mm_Horizontal
Through hole angled pin header, 1x29, 2.54mm pitch, 6mm pin length, single row
Through hole angled pin header THT 1x29 2.54mm single row
0
29
29
Connector_PinHeader_2.54mm
PinHeader_1x29_P2.54mm_Vertical
Through hole straight pin header, 1x29, 2.54mm pitch, single row
Through hole pin header THT 1x29 2.54mm single row
0
29
29
Connector_PinHeader_2.54mm
PinHeader_1x29_P2.54mm_Vertical_SMD_Pin1Left
surface-mounted straight pin header, 1x29, 2.54mm pitch, single row, style 1 (pin 1 left)
Surface mounted pin header SMD 1x29 2.54mm single row style1 pin1 left
0
29
29
Connector_PinHeader_2.54mm
PinHeader_1x29_P2.54mm_Vertical_SMD_Pin1Right
surface-mounted straight pin header, 1x29, 2.54mm pitch, single row, style 2 (pin 1 right)
Surface mounted pin header SMD 1x29 2.54mm single row style2 pin1 right
0
29
29
Connector_PinHeader_2.54mm
PinHeader_1x30_P2.54mm_Horizontal
Through hole angled pin header, 1x30, 2.54mm pitch, 6mm pin length, single row
Through hole angled pin header THT 1x30 2.54mm single row
0
30
30
Connector_PinHeader_2.54mm
PinHeader_1x30_P2.54mm_Vertical
Through hole straight pin header, 1x30, 2.54mm pitch, single row
Through hole pin header THT 1x30 2.54mm single row
0
30
30
Connector_PinHeader_2.54mm
PinHeader_1x30_P2.54mm_Vertical_SMD_Pin1Left
surface-mounted straight pin header, 1x30, 2.54mm pitch, single row, style 1 (pin 1 left)
Surface mounted pin header SMD 1x30 2.54mm single row style1 pin1 left
0
30
30
Connector_PinHeader_2.54mm
PinHeader_1x30_P2.54mm_Vertical_SMD_Pin1Right
surface-mounted straight pin header, 1x30, 2.54mm pitch, single row, style 2 (pin 1 right)
Surface mounted pin header SMD 1x30 2.54mm single row style2 pin1 right
0
30
30
Connector_PinHeader_2.54mm
PinHeader_1x31_P2.54mm_Horizontal
Through hole angled pin header, 1x31, 2.54mm pitch, 6mm pin length, single row
Through hole angled pin header THT 1x31 2.54mm single row
0
31
31
Connector_PinHeader_2.54mm
PinHeader_1x31_P2.54mm_Vertical
Through hole straight pin header, 1x31, 2.54mm pitch, single row
Through hole pin header THT 1x31 2.54mm single row
0
31
31
Connector_PinHeader_2.54mm
PinHeader_1x31_P2.54mm_Vertical_SMD_Pin1Left
surface-mounted straight pin header, 1x31, 2.54mm pitch, single row, style 1 (pin 1 left)
Surface mounted pin header SMD 1x31 2.54mm single row style1 pin1 left
0
31
31
Connector_PinHeader_2.54mm
PinHeader_1x31_P2.54mm_Vertical_SMD_Pin1Right
surface-mounted straight pin header, 1x31, 2.54mm pitch, single row, style 2 (pin 1 right)
Surface mounted pin header SMD 1x31 2.54mm single row style2 pin1 right
0
31
31
Connector_PinHeader_2.54mm
PinHeader_1x32_P2.54mm_Horizontal
Through hole angled pin header, 1x32, 2.54mm pitch, 6mm pin length, single row
Through hole angled pin header THT 1x32 2.54mm single row
0
32
32
Connector_PinHeader_2.54mm
PinHeader_1x32_P2.54mm_Vertical
Through hole straight pin header, 1x32, 2.54mm pitch, single row
Through hole pin header THT 1x32 2.54mm single row
0
32
32
Connector_PinHeader_2.54mm
PinHeader_1x32_P2.54mm_Vertical_SMD_Pin1Left
surface-mounted straight pin header, 1x32, 2.54mm pitch, single row, style 1 (pin 1 left)
Surface mounted pin header SMD 1x32 2.54mm single row style1 pin1 left
0
32
32
Connector_PinHeader_2.54mm
PinHeader_1x32_P2.54mm_Vertical_SMD_Pin1Right
surface-mounted straight pin header, 1x32, 2.54mm pitch, single row, style 2 (pin 1 right)
Surface mounted pin header SMD 1x32 2.54mm single row style2 pin1 right
0
32
32
Connector_PinHeader_2.54mm
PinHeader_1x33_P2.54mm_Horizontal
Through hole angled pin header, 1x33, 2.54mm pitch, 6mm pin length, single row
Through hole angled pin header THT 1x33 2.54mm single row
0
33
33
Connector_PinHeader_2.54mm
PinHeader_1x33_P2.54mm_Vertical
Through hole straight pin header, 1x33, 2.54mm pitch, single row
Through hole pin header THT 1x33 2.54mm single row
0
33
33
Connector_PinHeader_2.54mm
PinHeader_1x33_P2.54mm_Vertical_SMD_Pin1Left
surface-mounted straight pin header, 1x33, 2.54mm pitch, single row, style 1 (pin 1 left)
Surface mounted pin header SMD 1x33 2.54mm single row style1 pin1 left
0
33
33
Connector_PinHeader_2.54mm
PinHeader_1x33_P2.54mm_Vertical_SMD_Pin1Right
surface-mounted straight pin header, 1x33, 2.54mm pitch, single row, style 2 (pin 1 right)
Surface mounted pin header SMD 1x33 2.54mm single row style2 pin1 right
0
33
33
Connector_PinHeader_2.54mm
PinHeader_1x34_P2.54mm_Horizontal
Through hole angled pin header, 1x34, 2.54mm pitch, 6mm pin length, single row
Through hole angled pin header THT 1x34 2.54mm single row
0
34
34
Connector_PinHeader_2.54mm
PinHeader_1x34_P2.54mm_Vertical
Through hole straight pin header, 1x34, 2.54mm pitch, single row
Through hole pin header THT 1x34 2.54mm single row
0
34
34
Connector_PinHeader_2.54mm
PinHeader_1x34_P2.54mm_Vertical_SMD_Pin1Left
surface-mounted straight pin header, 1x34, 2.54mm pitch, single row, style 1 (pin 1 left)
Surface mounted pin header SMD 1x34 2.54mm single row style1 pin1 left
0
34
34
Connector_PinHeader_2.54mm
PinHeader_1x34_P2.54mm_Vertical_SMD_Pin1Right
surface-mounted straight pin header, 1x34, 2.54mm pitch, single row, style 2 (pin 1 right)
Surface mounted pin header SMD 1x34 2.54mm single row style2 pin1 right
0
34
34
Connector_PinHeader_2.54mm
PinHeader_1x35_P2.54mm_Horizontal
Through hole angled pin header, 1x35, 2.54mm pitch, 6mm pin length, single row
Through hole angled pin header THT 1x35 2.54mm single row
0
35
35
Connector_PinHeader_2.54mm
PinHeader_1x35_P2.54mm_Vertical
Through hole straight pin header, 1x35, 2.54mm pitch, single row
Through hole pin header THT 1x35 2.54mm single row
0
35
35
Connector_PinHeader_2.54mm
PinHeader_1x35_P2.54mm_Vertical_SMD_Pin1Left
surface-mounted straight pin header, 1x35, 2.54mm pitch, single row, style 1 (pin 1 left)
Surface mounted pin header SMD 1x35 2.54mm single row style1 pin1 left
0
35
35
Connector_PinHeader_2.54mm
PinHeader_1x35_P2.54mm_Vertical_SMD_Pin1Right
surface-mounted straight pin header, 1x35, 2.54mm pitch, single row, style 2 (pin 1 right)
Surface mounted pin header SMD 1x35 2.54mm single row style2 pin1 right
0
35
35
Connector_PinHeader_2.54mm
PinHeader_1x36_P2.54mm_Horizontal
Through hole angled pin header, 1x36, 2.54mm pitch, 6mm pin length, single row
Through hole angled pin header THT 1x36 2.54mm single row
0
36
36
Connector_PinHeader_2.54mm
PinHeader_1x36_P2.54mm_Vertical
Through hole straight pin header, 1x36, 2.54mm pitch, single row
Through hole pin header THT 1x36 2.54mm single row
0
36
36
Connector_PinHeader_2.54mm
PinHeader_1x36_P2.54mm_Vertical_SMD_Pin1Left
surface-mounted straight pin header, 1x36, 2.54mm pitch, single row, style 1 (pin 1 left)
Surface mounted pin header SMD 1x36 2.54mm single row style1 pin1 left
0
36
36
Connector_PinHeader_2.54mm
PinHeader_1x36_P2.54mm_Vertical_SMD_Pin1Right
surface-mounted straight pin header, 1x36, 2.54mm pitch, single row, style 2 (pin 1 right)
Surface mounted pin header SMD 1x36 2.54mm single row style2 pin1 right
0
36
36
Connector_PinHeader_2.54mm
PinHeader_1x37_P2.54mm_Horizontal
Through hole angled pin header, 1x37, 2.54mm pitch, 6mm pin length, single row
Through hole angled pin header THT 1x37 2.54mm single row
0
37
37
Connector_PinHeader_2.54mm
PinHeader_1x37_P2.54mm_Vertical
Through hole straight pin header, 1x37, 2.54mm pitch, single row
Through hole pin header THT 1x37 2.54mm single row
0
37
37
Connector_PinHeader_2.54mm
PinHeader_1x37_P2.54mm_Vertical_SMD_Pin1Left
surface-mounted straight pin header, 1x37, 2.54mm pitch, single row, style 1 (pin 1 left)
Surface mounted pin header SMD 1x37 2.54mm single row style1 pin1 left
0
37
37
Connector_PinHeader_2.54mm
PinHeader_1x37_P2.54mm_Vertical_SMD_Pin1Right
surface-mounted straight pin header, 1x37, 2.54mm pitch, single row, style 2 (pin 1 right)
Surface mounted pin header SMD 1x37 2.54mm single row style2 pin1 right
0
37
37
Connector_PinHeader_2.54mm
PinHeader_1x38_P2.54mm_Horizontal
Through hole angled pin header, 1x38, 2.54mm pitch, 6mm pin length, single row
Through hole angled pin header THT 1x38 2.54mm single row
0
38
38
Connector_PinHeader_2.54mm
PinHeader_1x38_P2.54mm_Vertical
Through hole straight pin header, 1x38, 2.54mm pitch, single row
Through hole pin header THT 1x38 2.54mm single row
0
38
38
Connector_PinHeader_2.54mm
PinHeader_1x38_P2.54mm_Vertical_SMD_Pin1Left
surface-mounted straight pin header, 1x38, 2.54mm pitch, single row, style 1 (pin 1 left)
Surface mounted pin header SMD 1x38 2.54mm single row style1 pin1 left
0
38
38
Connector_PinHeader_2.54mm
PinHeader_1x38_P2.54mm_Vertical_SMD_Pin1Right
surface-mounted straight pin header, 1x38, 2.54mm pitch, single row, style 2 (pin 1 right)
Surface mounted pin header SMD 1x38 2.54mm single row style2 pin1 right
0
38
38
Connector_PinHeader_2.54mm
PinHeader_1x39_P2.54mm_Horizontal
Through hole angled pin header, 1x39, 2.54mm pitch, 6mm pin length, single row
Through hole angled pin header THT 1x39 2.54mm single row
0
39
39
Connector_PinHeader_2.54mm
PinHeader_1x39_P2.54mm_Vertical
Through hole straight pin header, 1x39, 2.54mm pitch, single row
Through hole pin header THT 1x39 2.54mm single row
0
39
39
Connector_PinHeader_2.54mm
PinHeader_1x39_P2.54mm_Vertical_SMD_Pin1Left
surface-mounted straight pin header, 1x39, 2.54mm pitch, single row, style 1 (pin 1 left)
Surface mounted pin header SMD 1x39 2.54mm single row style1 pin1 left
0
39
39
Connector_PinHeader_2.54mm
PinHeader_1x39_P2.54mm_Vertical_SMD_Pin1Right
surface-mounted straight pin header, 1x39, 2.54mm pitch, single row, style 2 (pin 1 right)
Surface mounted pin header SMD 1x39 2.54mm single row style2 pin1 right
0
39
39
Connector_PinHeader_2.54mm
PinHeader_1x40_P2.54mm_Horizontal
Through hole angled pin header, 1x40, 2.54mm pitch, 6mm pin length, single row
Through hole angled pin header THT 1x40 2.54mm single row
0
40
40
Connector_PinHeader_2.54mm
PinHeader_1x40_P2.54mm_Vertical
Through hole straight pin header, 1x40, 2.54mm pitch, single row
Through hole pin header THT 1x40 2.54mm single row
0
40
40
Connector_PinHeader_2.54mm
PinHeader_1x40_P2.54mm_Vertical_SMD_Pin1Left
surface-mounted straight pin header, 1x40, 2.54mm pitch, single row, style 1 (pin 1 left)
Surface mounted pin header SMD 1x40 2.54mm single row style1 pin1 left
0
40
40
Connector_PinHeader_2.54mm
PinHeader_1x40_P2.54mm_Vertical_SMD_Pin1Right
surface-mounted straight pin header, 1x40, 2.54mm pitch, single row, style 2 (pin 1 right)
Surface mounted pin header SMD 1x40 2.54mm single row style2 pin1 right
0
40
40
Connector_PinHeader_2.54mm
PinHeader_2x01_P2.54mm_Horizontal
Through hole angled pin header, 2x01, 2.54mm pitch, 6mm pin length, double rows
Through hole angled pin header THT 2x01 2.54mm double row
0
2
2
Connector_PinHeader_2.54mm
PinHeader_2x01_P2.54mm_Vertical
Through hole straight pin header, 2x01, 2.54mm pitch, double rows
Through hole pin header THT 2x01 2.54mm double row
0
2
2
Connector_PinHeader_2.54mm
PinHeader_2x01_P2.54mm_Vertical_SMD
surface-mounted straight pin header, 2x01, 2.54mm pitch, double rows
Surface mounted pin header SMD 2x01 2.54mm double row
0
2
2
Connector_PinHeader_2.54mm
PinHeader_2x02_P2.54mm_Horizontal
Through hole angled pin header, 2x02, 2.54mm pitch, 6mm pin length, double rows
Through hole angled pin header THT 2x02 2.54mm double row
0
4
4
Connector_PinHeader_2.54mm
PinHeader_2x02_P2.54mm_Vertical
Through hole straight pin header, 2x02, 2.54mm pitch, double rows
Through hole pin header THT 2x02 2.54mm double row
0
4
4
Connector_PinHeader_2.54mm
PinHeader_2x02_P2.54mm_Vertical_SMD
surface-mounted straight pin header, 2x02, 2.54mm pitch, double rows
Surface mounted pin header SMD 2x02 2.54mm double row
0
4
4
Connector_PinHeader_2.54mm
PinHeader_2x03_P2.54mm_Horizontal
Through hole angled pin header, 2x03, 2.54mm pitch, 6mm pin length, double rows
Through hole angled pin header THT 2x03 2.54mm double row
0
6
6
Connector_PinHeader_2.54mm
PinHeader_2x03_P2.54mm_Vertical
Through hole straight pin header, 2x03, 2.54mm pitch, double rows
Through hole pin header THT 2x03 2.54mm double row
0
6
6
Connector_PinHeader_2.54mm
PinHeader_2x03_P2.54mm_Vertical_SMD
surface-mounted straight pin header, 2x03, 2.54mm pitch, double rows
Surface mounted pin header SMD 2x03 2.54mm double row
0
6
6
Connector_PinHeader_2.54mm
PinHeader_2x04_P2.54mm_Horizontal
Through hole angled pin header, 2x04, 2.54mm pitch, 6mm pin length, double rows
Through hole angled pin header THT 2x04 2.54mm double row
0
8
8
Connector_PinHeader_2.54mm
PinHeader_2x04_P2.54mm_Vertical
Through hole straight pin header, 2x04, 2.54mm pitch, double rows
Through hole pin header THT 2x04 2.54mm double row
0
8
8
Connector_PinHeader_2.54mm
PinHeader_2x04_P2.54mm_Vertical_SMD
surface-mounted straight pin header, 2x04, 2.54mm pitch, double rows
Surface mounted pin header SMD 2x04 2.54mm double row
0
8
8
Connector_PinHeader_2.54mm
PinHeader_2x05_P2.54mm_Horizontal
Through hole angled pin header, 2x05, 2.54mm pitch, 6mm pin length, double rows
Through hole angled pin header THT 2x05 2.54mm double row
0
10
10
Connector_PinHeader_2.54mm
PinHeader_2x05_P2.54mm_Vertical
Through hole straight pin header, 2x05, 2.54mm pitch, double rows
Through hole pin header THT 2x05 2.54mm double row
0
10
10
Connector_PinHeader_2.54mm
PinHeader_2x05_P2.54mm_Vertical_SMD
surface-mounted straight pin header, 2x05, 2.54mm pitch, double rows
Surface mounted pin header SMD 2x05 2.54mm double row
0
10
10
Connector_PinHeader_2.54mm
PinHeader_2x06_P2.54mm_Horizontal
Through hole angled pin header, 2x06, 2.54mm pitch, 6mm pin length, double rows
Through hole angled pin header THT 2x06 2.54mm double row
0
12
12
Connector_PinHeader_2.54mm
PinHeader_2x06_P2.54mm_Vertical
Through hole straight pin header, 2x06, 2.54mm pitch, double rows
Through hole pin header THT 2x06 2.54mm double row
0
12
12
Connector_PinHeader_2.54mm
PinHeader_2x06_P2.54mm_Vertical_SMD
surface-mounted straight pin header, 2x06, 2.54mm pitch, double rows
Surface mounted pin header SMD 2x06 2.54mm double row
0
12
12
Connector_PinHeader_2.54mm
PinHeader_2x07_P2.54mm_Horizontal
Through hole angled pin header, 2x07, 2.54mm pitch, 6mm pin length, double rows
Through hole angled pin header THT 2x07 2.54mm double row
0
14
14
Connector_PinHeader_2.54mm
PinHeader_2x07_P2.54mm_Vertical
Through hole straight pin header, 2x07, 2.54mm pitch, double rows
Through hole pin header THT 2x07 2.54mm double row
0
14
14
Connector_PinHeader_2.54mm
PinHeader_2x07_P2.54mm_Vertical_SMD
surface-mounted straight pin header, 2x07, 2.54mm pitch, double rows
Surface mounted pin header SMD 2x07 2.54mm double row
0
14
14
Connector_PinHeader_2.54mm
PinHeader_2x08_P2.54mm_Horizontal
Through hole angled pin header, 2x08, 2.54mm pitch, 6mm pin length, double rows
Through hole angled pin header THT 2x08 2.54mm double row
0
16
16
Connector_PinHeader_2.54mm
PinHeader_2x08_P2.54mm_Vertical
Through hole straight pin header, 2x08, 2.54mm pitch, double rows
Through hole pin header THT 2x08 2.54mm double row
0
16
16
Connector_PinHeader_2.54mm
PinHeader_2x08_P2.54mm_Vertical_SMD
surface-mounted straight pin header, 2x08, 2.54mm pitch, double rows
Surface mounted pin header SMD 2x08 2.54mm double row
0
16
16
Connector_PinHeader_2.54mm
PinHeader_2x09_P2.54mm_Horizontal
Through hole angled pin header, 2x09, 2.54mm pitch, 6mm pin length, double rows
Through hole angled pin header THT 2x09 2.54mm double row
0
18
18
Connector_PinHeader_2.54mm
PinHeader_2x09_P2.54mm_Vertical
Through hole straight pin header, 2x09, 2.54mm pitch, double rows
Through hole pin header THT 2x09 2.54mm double row
0
18
18
Connector_PinHeader_2.54mm
PinHeader_2x09_P2.54mm_Vertical_SMD
surface-mounted straight pin header, 2x09, 2.54mm pitch, double rows
Surface mounted pin header SMD 2x09 2.54mm double row
0
18
18
Connector_PinHeader_2.54mm
PinHeader_2x10_P2.54mm_Horizontal
Through hole angled pin header, 2x10, 2.54mm pitch, 6mm pin length, double rows
Through hole angled pin header THT 2x10 2.54mm double row
0
20
20
Connector_PinHeader_2.54mm
PinHeader_2x10_P2.54mm_Vertical
Through hole straight pin header, 2x10, 2.54mm pitch, double rows
Through hole pin header THT 2x10 2.54mm double row
0
20
20
Connector_PinHeader_2.54mm
PinHeader_2x10_P2.54mm_Vertical_SMD
surface-mounted straight pin header, 2x10, 2.54mm pitch, double rows
Surface mounted pin header SMD 2x10 2.54mm double row
0
20
20
Connector_PinHeader_2.54mm
PinHeader_2x11_P2.54mm_Horizontal
Through hole angled pin header, 2x11, 2.54mm pitch, 6mm pin length, double rows
Through hole angled pin header THT 2x11 2.54mm double row
0
22
22
Connector_PinHeader_2.54mm
PinHeader_2x11_P2.54mm_Vertical
Through hole straight pin header, 2x11, 2.54mm pitch, double rows
Through hole pin header THT 2x11 2.54mm double row
0
22
22
Connector_PinHeader_2.54mm
PinHeader_2x11_P2.54mm_Vertical_SMD
surface-mounted straight pin header, 2x11, 2.54mm pitch, double rows
Surface mounted pin header SMD 2x11 2.54mm double row
0
22
22
Connector_PinHeader_2.54mm
PinHeader_2x12_P2.54mm_Horizontal
Through hole angled pin header, 2x12, 2.54mm pitch, 6mm pin length, double rows
Through hole angled pin header THT 2x12 2.54mm double row
0
24
24
Connector_PinHeader_2.54mm
PinHeader_2x12_P2.54mm_Vertical
Through hole straight pin header, 2x12, 2.54mm pitch, double rows
Through hole pin header THT 2x12 2.54mm double row
0
24
24
Connector_PinHeader_2.54mm
PinHeader_2x12_P2.54mm_Vertical_SMD
surface-mounted straight pin header, 2x12, 2.54mm pitch, double rows
Surface mounted pin header SMD 2x12 2.54mm double row
0
24
24
Connector_PinHeader_2.54mm
PinHeader_2x13_P2.54mm_Horizontal
Through hole angled pin header, 2x13, 2.54mm pitch, 6mm pin length, double rows
Through hole angled pin header THT 2x13 2.54mm double row
0
26
26
Connector_PinHeader_2.54mm
PinHeader_2x13_P2.54mm_Vertical
Through hole straight pin header, 2x13, 2.54mm pitch, double rows
Through hole pin header THT 2x13 2.54mm double row
0
26
26
Connector_PinHeader_2.54mm
PinHeader_2x13_P2.54mm_Vertical_SMD
surface-mounted straight pin header, 2x13, 2.54mm pitch, double rows
Surface mounted pin header SMD 2x13 2.54mm double row
0
26
26
Connector_PinHeader_2.54mm
PinHeader_2x14_P2.54mm_Horizontal
Through hole angled pin header, 2x14, 2.54mm pitch, 6mm pin length, double rows
Through hole angled pin header THT 2x14 2.54mm double row
0
28
28
Connector_PinHeader_2.54mm
PinHeader_2x14_P2.54mm_Vertical
Through hole straight pin header, 2x14, 2.54mm pitch, double rows
Through hole pin header THT 2x14 2.54mm double row
0
28
28
Connector_PinHeader_2.54mm
PinHeader_2x14_P2.54mm_Vertical_SMD
surface-mounted straight pin header, 2x14, 2.54mm pitch, double rows
Surface mounted pin header SMD 2x14 2.54mm double row
0
28
28
Connector_PinHeader_2.54mm
PinHeader_2x15_P2.54mm_Horizontal
Through hole angled pin header, 2x15, 2.54mm pitch, 6mm pin length, double rows
Through hole angled pin header THT 2x15 2.54mm double row
0
30
30
Connector_PinHeader_2.54mm
PinHeader_2x15_P2.54mm_Vertical
Through hole straight pin header, 2x15, 2.54mm pitch, double rows
Through hole pin header THT 2x15 2.54mm double row
0
30
30
Connector_PinHeader_2.54mm
PinHeader_2x15_P2.54mm_Vertical_SMD
surface-mounted straight pin header, 2x15, 2.54mm pitch, double rows
Surface mounted pin header SMD 2x15 2.54mm double row
0
30
30
Connector_PinHeader_2.54mm
PinHeader_2x16_P2.54mm_Horizontal
Through hole angled pin header, 2x16, 2.54mm pitch, 6mm pin length, double rows
Through hole angled pin header THT 2x16 2.54mm double row
0
32
32
Connector_PinHeader_2.54mm
PinHeader_2x16_P2.54mm_Vertical
Through hole straight pin header, 2x16, 2.54mm pitch, double rows
Through hole pin header THT 2x16 2.54mm double row
0
32
32
Connector_PinHeader_2.54mm
PinHeader_2x16_P2.54mm_Vertical_SMD
surface-mounted straight pin header, 2x16, 2.54mm pitch, double rows
Surface mounted pin header SMD 2x16 2.54mm double row
0
32
32
Connector_PinHeader_2.54mm
PinHeader_2x17_P2.54mm_Horizontal
Through hole angled pin header, 2x17, 2.54mm pitch, 6mm pin length, double rows
Through hole angled pin header THT 2x17 2.54mm double row
0
34
34
Connector_PinHeader_2.54mm
PinHeader_2x17_P2.54mm_Vertical
Through hole straight pin header, 2x17, 2.54mm pitch, double rows
Through hole pin header THT 2x17 2.54mm double row
0
34
34
Connector_PinHeader_2.54mm
PinHeader_2x17_P2.54mm_Vertical_SMD
surface-mounted straight pin header, 2x17, 2.54mm pitch, double rows
Surface mounted pin header SMD 2x17 2.54mm double row
0
34
34
Connector_PinHeader_2.54mm
PinHeader_2x18_P2.54mm_Horizontal
Through hole angled pin header, 2x18, 2.54mm pitch, 6mm pin length, double rows
Through hole angled pin header THT 2x18 2.54mm double row
0
36
36
Connector_PinHeader_2.54mm
PinHeader_2x18_P2.54mm_Vertical
Through hole straight pin header, 2x18, 2.54mm pitch, double rows
Through hole pin header THT 2x18 2.54mm double row
0
36
36
Connector_PinHeader_2.54mm
PinHeader_2x18_P2.54mm_Vertical_SMD
surface-mounted straight pin header, 2x18, 2.54mm pitch, double rows
Surface mounted pin header SMD 2x18 2.54mm double row
0
36
36
Connector_PinHeader_2.54mm
PinHeader_2x19_P2.54mm_Horizontal
Through hole angled pin header, 2x19, 2.54mm pitch, 6mm pin length, double rows
Through hole angled pin header THT 2x19 2.54mm double row
0
38
38
Connector_PinHeader_2.54mm
PinHeader_2x19_P2.54mm_Vertical
Through hole straight pin header, 2x19, 2.54mm pitch, double rows
Through hole pin header THT 2x19 2.54mm double row
0
38
38
Connector_PinHeader_2.54mm
PinHeader_2x19_P2.54mm_Vertical_SMD
surface-mounted straight pin header, 2x19, 2.54mm pitch, double rows
Surface mounted pin header SMD 2x19 2.54mm double row
0
38
38
Connector_PinHeader_2.54mm
PinHeader_2x20_P2.54mm_Horizontal
Through hole angled pin header, 2x20, 2.54mm pitch, 6mm pin length, double rows
Through hole angled pin header THT 2x20 2.54mm double row
0
40
40
Connector_PinHeader_2.54mm
PinHeader_2x20_P2.54mm_Vertical
Through hole straight pin header, 2x20, 2.54mm pitch, double rows
Through hole pin header THT 2x20 2.54mm double row
0
40
40
Connector_PinHeader_2.54mm
PinHeader_2x20_P2.54mm_Vertical_SMD
surface-mounted straight pin header, 2x20, 2.54mm pitch, double rows
Surface mounted pin header SMD 2x20 2.54mm double row
0
40
40
Connector_PinHeader_2.54mm
PinHeader_2x21_P2.54mm_Horizontal
Through hole angled pin header, 2x21, 2.54mm pitch, 6mm pin length, double rows
Through hole angled pin header THT 2x21 2.54mm double row
0
42
42
Connector_PinHeader_2.54mm
PinHeader_2x21_P2.54mm_Vertical
Through hole straight pin header, 2x21, 2.54mm pitch, double rows
Through hole pin header THT 2x21 2.54mm double row
0
42
42
Connector_PinHeader_2.54mm
PinHeader_2x21_P2.54mm_Vertical_SMD
surface-mounted straight pin header, 2x21, 2.54mm pitch, double rows
Surface mounted pin header SMD 2x21 2.54mm double row
0
42
42
Connector_PinHeader_2.54mm
PinHeader_2x22_P2.54mm_Horizontal
Through hole angled pin header, 2x22, 2.54mm pitch, 6mm pin length, double rows
Through hole angled pin header THT 2x22 2.54mm double row
0
44
44
Connector_PinHeader_2.54mm
PinHeader_2x22_P2.54mm_Vertical
Through hole straight pin header, 2x22, 2.54mm pitch, double rows
Through hole pin header THT 2x22 2.54mm double row
0
44
44
Connector_PinHeader_2.54mm
PinHeader_2x22_P2.54mm_Vertical_SMD
surface-mounted straight pin header, 2x22, 2.54mm pitch, double rows
Surface mounted pin header SMD 2x22 2.54mm double row
0
44
44
Connector_PinHeader_2.54mm
PinHeader_2x23_P2.54mm_Horizontal
Through hole angled pin header, 2x23, 2.54mm pitch, 6mm pin length, double rows
Through hole angled pin header THT 2x23 2.54mm double row
0
46
46
Connector_PinHeader_2.54mm
PinHeader_2x23_P2.54mm_Vertical
Through hole straight pin header, 2x23, 2.54mm pitch, double rows
Through hole pin header THT 2x23 2.54mm double row
0
46
46
Connector_PinHeader_2.54mm
PinHeader_2x23_P2.54mm_Vertical_SMD
surface-mounted straight pin header, 2x23, 2.54mm pitch, double rows
Surface mounted pin header SMD 2x23 2.54mm double row
0
46
46
Connector_PinHeader_2.54mm
PinHeader_2x24_P2.54mm_Horizontal
Through hole angled pin header, 2x24, 2.54mm pitch, 6mm pin length, double rows
Through hole angled pin header THT 2x24 2.54mm double row
0
48
48
Connector_PinHeader_2.54mm
PinHeader_2x24_P2.54mm_Vertical
Through hole straight pin header, 2x24, 2.54mm pitch, double rows
Through hole pin header THT 2x24 2.54mm double row
0
48
48
Connector_PinHeader_2.54mm
PinHeader_2x24_P2.54mm_Vertical_SMD
surface-mounted straight pin header, 2x24, 2.54mm pitch, double rows
Surface mounted pin header SMD 2x24 2.54mm double row
0
48
48
Connector_PinHeader_2.54mm
PinHeader_2x25_P2.54mm_Horizontal
Through hole angled pin header, 2x25, 2.54mm pitch, 6mm pin length, double rows
Through hole angled pin header THT 2x25 2.54mm double row
0
50
50
Connector_PinHeader_2.54mm
PinHeader_2x25_P2.54mm_Vertical
Through hole straight pin header, 2x25, 2.54mm pitch, double rows
Through hole pin header THT 2x25 2.54mm double row
0
50
50
Connector_PinHeader_2.54mm
PinHeader_2x25_P2.54mm_Vertical_SMD
surface-mounted straight pin header, 2x25, 2.54mm pitch, double rows
Surface mounted pin header SMD 2x25 2.54mm double row
0
50
50
Connector_PinHeader_2.54mm
PinHeader_2x26_P2.54mm_Horizontal
Through hole angled pin header, 2x26, 2.54mm pitch, 6mm pin length, double rows
Through hole angled pin header THT 2x26 2.54mm double row
0
52
52
Connector_PinHeader_2.54mm
PinHeader_2x26_P2.54mm_Vertical
Through hole straight pin header, 2x26, 2.54mm pitch, double rows
Through hole pin header THT 2x26 2.54mm double row
0
52
52
Connector_PinHeader_2.54mm
PinHeader_2x26_P2.54mm_Vertical_SMD
surface-mounted straight pin header, 2x26, 2.54mm pitch, double rows
Surface mounted pin header SMD 2x26 2.54mm double row
0
52
52
Connector_PinHeader_2.54mm
PinHeader_2x27_P2.54mm_Horizontal
Through hole angled pin header, 2x27, 2.54mm pitch, 6mm pin length, double rows
Through hole angled pin header THT 2x27 2.54mm double row
0
54
54
Connector_PinHeader_2.54mm
PinHeader_2x27_P2.54mm_Vertical
Through hole straight pin header, 2x27, 2.54mm pitch, double rows
Through hole pin header THT 2x27 2.54mm double row
0
54
54
Connector_PinHeader_2.54mm
PinHeader_2x27_P2.54mm_Vertical_SMD
surface-mounted straight pin header, 2x27, 2.54mm pitch, double rows
Surface mounted pin header SMD 2x27 2.54mm double row
0
54
54
Connector_PinHeader_2.54mm
PinHeader_2x28_P2.54mm_Horizontal
Through hole angled pin header, 2x28, 2.54mm pitch, 6mm pin length, double rows
Through hole angled pin header THT 2x28 2.54mm double row
0
56
56
Connector_PinHeader_2.54mm
PinHeader_2x28_P2.54mm_Vertical
Through hole straight pin header, 2x28, 2.54mm pitch, double rows
Through hole pin header THT 2x28 2.54mm double row
0
56
56
Connector_PinHeader_2.54mm
PinHeader_2x28_P2.54mm_Vertical_SMD
surface-mounted straight pin header, 2x28, 2.54mm pitch, double rows
Surface mounted pin header SMD 2x28 2.54mm double row
0
56
56
Connector_PinHeader_2.54mm
PinHeader_2x29_P2.54mm_Horizontal
Through hole angled pin header, 2x29, 2.54mm pitch, 6mm pin length, double rows
Through hole angled pin header THT 2x29 2.54mm double row
0
58
58
Connector_PinHeader_2.54mm
PinHeader_2x29_P2.54mm_Vertical
Through hole straight pin header, 2x29, 2.54mm pitch, double rows
Through hole pin header THT 2x29 2.54mm double row
0
58
58
Connector_PinHeader_2.54mm
PinHeader_2x29_P2.54mm_Vertical_SMD
surface-mounted straight pin header, 2x29, 2.54mm pitch, double rows
Surface mounted pin header SMD 2x29 2.54mm double row
0
58
58
Connector_PinHeader_2.54mm
PinHeader_2x30_P2.54mm_Horizontal
Through hole angled pin header, 2x30, 2.54mm pitch, 6mm pin length, double rows
Through hole angled pin header THT 2x30 2.54mm double row
0
60
60
Connector_PinHeader_2.54mm
PinHeader_2x30_P2.54mm_Vertical
Through hole straight pin header, 2x30, 2.54mm pitch, double rows
Through hole pin header THT 2x30 2.54mm double row
0
60
60
Connector_PinHeader_2.54mm
PinHeader_2x30_P2.54mm_Vertical_SMD
surface-mounted straight pin header, 2x30, 2.54mm pitch, double rows
Surface mounted pin header SMD 2x30 2.54mm double row
0
60
60
Connector_PinHeader_2.54mm
PinHeader_2x31_P2.54mm_Horizontal
Through hole angled pin header, 2x31, 2.54mm pitch, 6mm pin length, double rows
Through hole angled pin header THT 2x31 2.54mm double row
0
62
62
Connector_PinHeader_2.54mm
PinHeader_2x31_P2.54mm_Vertical
Through hole straight pin header, 2x31, 2.54mm pitch, double rows
Through hole pin header THT 2x31 2.54mm double row
0
62
62
Connector_PinHeader_2.54mm
PinHeader_2x31_P2.54mm_Vertical_SMD
surface-mounted straight pin header, 2x31, 2.54mm pitch, double rows
Surface mounted pin header SMD 2x31 2.54mm double row
0
62
62
Connector_PinHeader_2.54mm
PinHeader_2x32_P2.54mm_Horizontal
Through hole angled pin header, 2x32, 2.54mm pitch, 6mm pin length, double rows
Through hole angled pin header THT 2x32 2.54mm double row
0
64
64
Connector_PinHeader_2.54mm
PinHeader_2x32_P2.54mm_Vertical
Through hole straight pin header, 2x32, 2.54mm pitch, double rows
Through hole pin header THT 2x32 2.54mm double row
0
64
64
Connector_PinHeader_2.54mm
PinHeader_2x32_P2.54mm_Vertical_SMD
surface-mounted straight pin header, 2x32, 2.54mm pitch, double rows
Surface mounted pin header SMD 2x32 2.54mm double row
0
64
64
Connector_PinHeader_2.54mm
PinHeader_2x33_P2.54mm_Horizontal
Through hole angled pin header, 2x33, 2.54mm pitch, 6mm pin length, double rows
Through hole angled pin header THT 2x33 2.54mm double row
0
66
66
Connector_PinHeader_2.54mm
PinHeader_2x33_P2.54mm_Vertical
Through hole straight pin header, 2x33, 2.54mm pitch, double rows
Through hole pin header THT 2x33 2.54mm double row
0
66
66
Connector_PinHeader_2.54mm
PinHeader_2x33_P2.54mm_Vertical_SMD
surface-mounted straight pin header, 2x33, 2.54mm pitch, double rows
Surface mounted pin header SMD 2x33 2.54mm double row
0
66
66
Connector_PinHeader_2.54mm
PinHeader_2x34_P2.54mm_Horizontal
Through hole angled pin header, 2x34, 2.54mm pitch, 6mm pin length, double rows
Through hole angled pin header THT 2x34 2.54mm double row
0
68
68
Connector_PinHeader_2.54mm
PinHeader_2x34_P2.54mm_Vertical
Through hole straight pin header, 2x34, 2.54mm pitch, double rows
Through hole pin header THT 2x34 2.54mm double row
0
68
68
Connector_PinHeader_2.54mm
PinHeader_2x34_P2.54mm_Vertical_SMD
surface-mounted straight pin header, 2x34, 2.54mm pitch, double rows
Surface mounted pin header SMD 2x34 2.54mm double row
0
68
68
Connector_PinHeader_2.54mm
PinHeader_2x35_P2.54mm_Horizontal
Through hole angled pin header, 2x35, 2.54mm pitch, 6mm pin length, double rows
Through hole angled pin header THT 2x35 2.54mm double row
0
70
70
Connector_PinHeader_2.54mm
PinHeader_2x35_P2.54mm_Vertical
Through hole straight pin header, 2x35, 2.54mm pitch, double rows
Through hole pin header THT 2x35 2.54mm double row
0
70
70
Connector_PinHeader_2.54mm
PinHeader_2x35_P2.54mm_Vertical_SMD
surface-mounted straight pin header, 2x35, 2.54mm pitch, double rows
Surface mounted pin header SMD 2x35 2.54mm double row
0
70
70
Connector_PinHeader_2.54mm
PinHeader_2x36_P2.54mm_Horizontal
Through hole angled pin header, 2x36, 2.54mm pitch, 6mm pin length, double rows
Through hole angled pin header THT 2x36 2.54mm double row
0
72
72
Connector_PinHeader_2.54mm
PinHeader_2x36_P2.54mm_Vertical
Through hole straight pin header, 2x36, 2.54mm pitch, double rows
Through hole pin header THT 2x36 2.54mm double row
0
72
72
Connector_PinHeader_2.54mm
PinHeader_2x36_P2.54mm_Vertical_SMD
surface-mounted straight pin header, 2x36, 2.54mm pitch, double rows
Surface mounted pin header SMD 2x36 2.54mm double row
0
72
72
Connector_PinHeader_2.54mm
PinHeader_2x37_P2.54mm_Horizontal
Through hole angled pin header, 2x37, 2.54mm pitch, 6mm pin length, double rows
Through hole angled pin header THT 2x37 2.54mm double row
0
74
74
Connector_PinHeader_2.54mm
PinHeader_2x37_P2.54mm_Vertical
Through hole straight pin header, 2x37, 2.54mm pitch, double rows
Through hole pin header THT 2x37 2.54mm double row
0
74
74
Connector_PinHeader_2.54mm
PinHeader_2x37_P2.54mm_Vertical_SMD
surface-mounted straight pin header, 2x37, 2.54mm pitch, double rows
Surface mounted pin header SMD 2x37 2.54mm double row
0
74
74
Connector_PinHeader_2.54mm
PinHeader_2x38_P2.54mm_Horizontal
Through hole angled pin header, 2x38, 2.54mm pitch, 6mm pin length, double rows
Through hole angled pin header THT 2x38 2.54mm double row
0
76
76
Connector_PinHeader_2.54mm
PinHeader_2x38_P2.54mm_Vertical
Through hole straight pin header, 2x38, 2.54mm pitch, double rows
Through hole pin header THT 2x38 2.54mm double row
0
76
76
Connector_PinHeader_2.54mm
PinHeader_2x38_P2.54mm_Vertical_SMD
surface-mounted straight pin header, 2x38, 2.54mm pitch, double rows
Surface mounted pin header SMD 2x38 2.54mm double row
0
76
76
Connector_PinHeader_2.54mm
PinHeader_2x39_P2.54mm_Horizontal
Through hole angled pin header, 2x39, 2.54mm pitch, 6mm pin length, double rows
Through hole angled pin header THT 2x39 2.54mm double row
0
78
78
Connector_PinHeader_2.54mm
PinHeader_2x39_P2.54mm_Vertical
Through hole straight pin header, 2x39, 2.54mm pitch, double rows
Through hole pin header THT 2x39 2.54mm double row
0
78
78
Connector_PinHeader_2.54mm
PinHeader_2x39_P2.54mm_Vertical_SMD
surface-mounted straight pin header, 2x39, 2.54mm pitch, double rows
Surface mounted pin header SMD 2x39 2.54mm double row
0
78
78
Connector_PinHeader_2.54mm
PinHeader_2x40_P2.54mm_Horizontal
Through hole angled pin header, 2x40, 2.54mm pitch, 6mm pin length, double rows
Through hole angled pin header THT 2x40 2.54mm double row
0
80
80
Connector_PinHeader_2.54mm
PinHeader_2x40_P2.54mm_Vertical
Through hole straight pin header, 2x40, 2.54mm pitch, double rows
Through hole pin header THT 2x40 2.54mm double row
0
80
80
Connector_PinHeader_2.54mm
PinHeader_2x40_P2.54mm_Vertical_SMD
surface-mounted straight pin header, 2x40, 2.54mm pitch, double rows
Surface mounted pin header SMD 2x40 2.54mm double row
0
80
80
Connector_PinSocket_2.54mm
PinSocket_1x01_P2.54mm_Horizontal
Through hole angled socket strip, 1x01, 2.54mm pitch, 8.51mm socket length, single row (from Kicad 4.0.7), script generated
Through hole angled socket strip THT 1x01 2.54mm single row
0
1
1
Connector_PinSocket_2.54mm
PinSocket_1x01_P2.54mm_Vertical
Through hole straight socket strip, 1x01, 2.54mm pitch, single row (from Kicad 4.0.7), script generated
Through hole socket strip THT 1x01 2.54mm single row
0
1
1
Connector_PinSocket_2.54mm
PinSocket_1x02_P2.54mm_Horizontal
Through hole angled socket strip, 1x02, 2.54mm pitch, 8.51mm socket length, single row (from Kicad 4.0.7), script generated
Through hole angled socket strip THT 1x02 2.54mm single row
0
2
2
Connector_PinSocket_2.54mm
PinSocket_1x02_P2.54mm_Vertical
Through hole straight socket strip, 1x02, 2.54mm pitch, single row (from Kicad 4.0.7), script generated
Through hole socket strip THT 1x02 2.54mm single row
0
2
2
Connector_PinSocket_2.54mm
PinSocket_1x02_P2.54mm_Vertical_SMD_Pin1Left
surface-mounted straight socket strip, 1x02, 2.54mm pitch, single row, style 1 (pin 1 left) (https://cdn.harwin.com/pdfs/M20-786.pdf), script generated
Surface mounted socket strip SMD 1x02 2.54mm single row style1 pin1 left
0
2
2
Connector_PinSocket_2.54mm
PinSocket_1x02_P2.54mm_Vertical_SMD_Pin1Right
surface-mounted straight socket strip, 1x02, 2.54mm pitch, single row, style 2 (pin 1 right) (https://cdn.harwin.com/pdfs/M20-786.pdf), script generated
Surface mounted socket strip SMD 1x02 2.54mm single row style2 pin1 right
0
2
2
Connector_PinSocket_2.54mm
PinSocket_1x03_P2.54mm_Horizontal
Through hole angled socket strip, 1x03, 2.54mm pitch, 8.51mm socket length, single row (from Kicad 4.0.7), script generated
Through hole angled socket strip THT 1x03 2.54mm single row
0
3
3
Connector_PinSocket_2.54mm
PinSocket_1x03_P2.54mm_Vertical
Through hole straight socket strip, 1x03, 2.54mm pitch, single row (from Kicad 4.0.7), script generated
Through hole socket strip THT 1x03 2.54mm single row
0
3
3
Connector_PinSocket_2.54mm
PinSocket_1x03_P2.54mm_Vertical_SMD_Pin1Left
surface-mounted straight socket strip, 1x03, 2.54mm pitch, single row, style 1 (pin 1 left) (https://cdn.harwin.com/pdfs/M20-786.pdf), script generated
Surface mounted socket strip SMD 1x03 2.54mm single row style1 pin1 left
0
3
3
Connector_PinSocket_2.54mm
PinSocket_1x03_P2.54mm_Vertical_SMD_Pin1Right
surface-mounted straight socket strip, 1x03, 2.54mm pitch, single row, style 2 (pin 1 right) (https://cdn.harwin.com/pdfs/M20-786.pdf), script generated
Surface mounted socket strip SMD 1x03 2.54mm single row style2 pin1 right
0
3
3
Connector_PinSocket_2.54mm
PinSocket_1x04_P2.54mm_Horizontal
Through hole angled socket strip, 1x04, 2.54mm pitch, 8.51mm socket length, single row (from Kicad 4.0.7), script generated
Through hole angled socket strip THT 1x04 2.54mm single row
0
4
4
Connector_PinSocket_2.54mm
PinSocket_1x04_P2.54mm_Vertical
Through hole straight socket strip, 1x04, 2.54mm pitch, single row (from Kicad 4.0.7), script generated
Through hole socket strip THT 1x04 2.54mm single row
0
4
4
Connector_PinSocket_2.54mm
PinSocket_1x04_P2.54mm_Vertical_SMD_Pin1Left
surface-mounted straight socket strip, 1x04, 2.54mm pitch, single row, style 1 (pin 1 left) (https://cdn.harwin.com/pdfs/M20-786.pdf), script generated
Surface mounted socket strip SMD 1x04 2.54mm single row style1 pin1 left
0
4
4
Connector_PinSocket_2.54mm
PinSocket_1x04_P2.54mm_Vertical_SMD_Pin1Right
surface-mounted straight socket strip, 1x04, 2.54mm pitch, single row, style 2 (pin 1 right) (https://cdn.harwin.com/pdfs/M20-786.pdf), script generated
Surface mounted socket strip SMD 1x04 2.54mm single row style2 pin1 right
0
4
4
Connector_PinSocket_2.54mm
PinSocket_1x05_P2.54mm_Horizontal
Through hole angled socket strip, 1x05, 2.54mm pitch, 8.51mm socket length, single row (from Kicad 4.0.7), script generated
Through hole angled socket strip THT 1x05 2.54mm single row
0
5
5
Connector_PinSocket_2.54mm
PinSocket_1x05_P2.54mm_Vertical
Through hole straight socket strip, 1x05, 2.54mm pitch, single row (from Kicad 4.0.7), script generated
Through hole socket strip THT 1x05 2.54mm single row
0
5
5
Connector_PinSocket_2.54mm
PinSocket_1x05_P2.54mm_Vertical_SMD_Pin1Left
surface-mounted straight socket strip, 1x05, 2.54mm pitch, single row, style 1 (pin 1 left) (https://cdn.harwin.com/pdfs/M20-786.pdf), script generated
Surface mounted socket strip SMD 1x05 2.54mm single row style1 pin1 left
0
5
5
Connector_PinSocket_2.54mm
PinSocket_1x05_P2.54mm_Vertical_SMD_Pin1Right
surface-mounted straight socket strip, 1x05, 2.54mm pitch, single row, style 2 (pin 1 right) (https://cdn.harwin.com/pdfs/M20-786.pdf), script generated
Surface mounted socket strip SMD 1x05 2.54mm single row style2 pin1 right
0
5
5
Connector_PinSocket_2.54mm
PinSocket_1x06_P2.54mm_Horizontal
Through hole angled socket strip, 1x06, 2.54mm pitch, 8.51mm socket length, single row (from Kicad 4.0.7), script generated
Through hole angled socket strip THT 1x06 2.54mm single row
0
6
6
Connector_PinSocket_2.54mm
PinSocket_1x06_P2.54mm_Vertical
Through hole straight socket strip, 1x06, 2.54mm pitch, single row (from Kicad 4.0.7), script generated
Through hole socket strip THT 1x06 2.54mm single row
0
6
6
Connector_PinSocket_2.54mm
PinSocket_1x06_P2.54mm_Vertical_SMD_Pin1Left
surface-mounted straight socket strip, 1x06, 2.54mm pitch, single row, style 1 (pin 1 left) (https://cdn.harwin.com/pdfs/M20-786.pdf), script generated
Surface mounted socket strip SMD 1x06 2.54mm single row style1 pin1 left
0
6
6
Connector_PinSocket_2.54mm
PinSocket_1x06_P2.54mm_Vertical_SMD_Pin1Right
surface-mounted straight socket strip, 1x06, 2.54mm pitch, single row, style 2 (pin 1 right) (https://cdn.harwin.com/pdfs/M20-786.pdf), script generated
Surface mounted socket strip SMD 1x06 2.54mm single row style2 pin1 right
0
6
6
Connector_PinSocket_2.54mm
PinSocket_1x07_P2.54mm_Horizontal
Through hole angled socket strip, 1x07, 2.54mm pitch, 8.51mm socket length, single row (from Kicad 4.0.7), script generated
Through hole angled socket strip THT 1x07 2.54mm single row
0
7
7
Connector_PinSocket_2.54mm
PinSocket_1x07_P2.54mm_Vertical
Through hole straight socket strip, 1x07, 2.54mm pitch, single row (from Kicad 4.0.7), script generated
Through hole socket strip THT 1x07 2.54mm single row
0
7
7
Connector_PinSocket_2.54mm
PinSocket_1x07_P2.54mm_Vertical_SMD_Pin1Left
surface-mounted straight socket strip, 1x07, 2.54mm pitch, single row, style 1 (pin 1 left) (https://cdn.harwin.com/pdfs/M20-786.pdf), script generated
Surface mounted socket strip SMD 1x07 2.54mm single row style1 pin1 left
0
7
7
Connector_PinSocket_2.54mm
PinSocket_1x07_P2.54mm_Vertical_SMD_Pin1Right
surface-mounted straight socket strip, 1x07, 2.54mm pitch, single row, style 2 (pin 1 right) (https://cdn.harwin.com/pdfs/M20-786.pdf), script generated
Surface mounted socket strip SMD 1x07 2.54mm single row style2 pin1 right
0
7
7
Connector_PinSocket_2.54mm
PinSocket_1x08_P2.54mm_Horizontal
Through hole angled socket strip, 1x08, 2.54mm pitch, 8.51mm socket length, single row (from Kicad 4.0.7), script generated
Through hole angled socket strip THT 1x08 2.54mm single row
0
8
8
Connector_PinSocket_2.54mm
PinSocket_1x08_P2.54mm_Vertical
Through hole straight socket strip, 1x08, 2.54mm pitch, single row (from Kicad 4.0.7), script generated
Through hole socket strip THT 1x08 2.54mm single row
0
8
8
Connector_PinSocket_2.54mm
PinSocket_1x08_P2.54mm_Vertical_SMD_Pin1Left
surface-mounted straight socket strip, 1x08, 2.54mm pitch, single row, style 1 (pin 1 left) (https://cdn.harwin.com/pdfs/M20-786.pdf), script generated
Surface mounted socket strip SMD 1x08 2.54mm single row style1 pin1 left
0
8
8
Connector_PinSocket_2.54mm
PinSocket_1x08_P2.54mm_Vertical_SMD_Pin1Right
surface-mounted straight socket strip, 1x08, 2.54mm pitch, single row, style 2 (pin 1 right) (https://cdn.harwin.com/pdfs/M20-786.pdf), script generated
Surface mounted socket strip SMD 1x08 2.54mm single row style2 pin1 right
0
8
8
Connector_PinSocket_2.54mm
PinSocket_1x09_P2.54mm_Horizontal
Through hole angled socket strip, 1x09, 2.54mm pitch, 8.51mm socket length, single row (from Kicad 4.0.7), script generated
Through hole angled socket strip THT 1x09 2.54mm single row
0
9
9
Connector_PinSocket_2.54mm
PinSocket_1x09_P2.54mm_Vertical
Through hole straight socket strip, 1x09, 2.54mm pitch, single row (from Kicad 4.0.7), script generated
Through hole socket strip THT 1x09 2.54mm single row
0
9
9
Connector_PinSocket_2.54mm
PinSocket_1x09_P2.54mm_Vertical_SMD_Pin1Left
surface-mounted straight socket strip, 1x09, 2.54mm pitch, single row, style 1 (pin 1 left) (https://cdn.harwin.com/pdfs/M20-786.pdf), script generated
Surface mounted socket strip SMD 1x09 2.54mm single row style1 pin1 left
0
9
9
Connector_PinSocket_2.54mm
PinSocket_1x09_P2.54mm_Vertical_SMD_Pin1Right
surface-mounted straight socket strip, 1x09, 2.54mm pitch, single row, style 2 (pin 1 right) (https://cdn.harwin.com/pdfs/M20-786.pdf), script generated
Surface mounted socket strip SMD 1x09 2.54mm single row style2 pin1 right
0
9
9
Connector_PinSocket_2.54mm
PinSocket_1x10_P2.54mm_Horizontal
Through hole angled socket strip, 1x10, 2.54mm pitch, 8.51mm socket length, single row (from Kicad 4.0.7), script generated
Through hole angled socket strip THT 1x10 2.54mm single row
0
10
10
Connector_PinSocket_2.54mm
PinSocket_1x10_P2.54mm_Vertical
Through hole straight socket strip, 1x10, 2.54mm pitch, single row (from Kicad 4.0.7), script generated
Through hole socket strip THT 1x10 2.54mm single row
0
10
10
Connector_PinSocket_2.54mm
PinSocket_1x10_P2.54mm_Vertical_SMD_Pin1Left
surface-mounted straight socket strip, 1x10, 2.54mm pitch, single row, style 1 (pin 1 left) (https://cdn.harwin.com/pdfs/M20-786.pdf), script generated
Surface mounted socket strip SMD 1x10 2.54mm single row style1 pin1 left
0
10
10
Connector_PinSocket_2.54mm
PinSocket_1x10_P2.54mm_Vertical_SMD_Pin1Right
surface-mounted straight socket strip, 1x10, 2.54mm pitch, single row, style 2 (pin 1 right) (https://cdn.harwin.com/pdfs/M20-786.pdf), script generated
Surface mounted socket strip SMD 1x10 2.54mm single row style2 pin1 right
0
10
10
Connector_PinSocket_2.54mm
PinSocket_1x11_P2.54mm_Horizontal
Through hole angled socket strip, 1x11, 2.54mm pitch, 8.51mm socket length, single row (from Kicad 4.0.7), script generated
Through hole angled socket strip THT 1x11 2.54mm single row
0
11
11
Connector_PinSocket_2.54mm
PinSocket_1x11_P2.54mm_Vertical
Through hole straight socket strip, 1x11, 2.54mm pitch, single row (from Kicad 4.0.7), script generated
Through hole socket strip THT 1x11 2.54mm single row
0
11
11
Connector_PinSocket_2.54mm
PinSocket_1x11_P2.54mm_Vertical_SMD_Pin1Left
surface-mounted straight socket strip, 1x11, 2.54mm pitch, single row, style 1 (pin 1 left) (https://cdn.harwin.com/pdfs/M20-786.pdf), script generated
Surface mounted socket strip SMD 1x11 2.54mm single row style1 pin1 left
0
11
11
Connector_PinSocket_2.54mm
PinSocket_1x11_P2.54mm_Vertical_SMD_Pin1Right
surface-mounted straight socket strip, 1x11, 2.54mm pitch, single row, style 2 (pin 1 right) (https://cdn.harwin.com/pdfs/M20-786.pdf), script generated
Surface mounted socket strip SMD 1x11 2.54mm single row style2 pin1 right
0
11
11
Connector_PinSocket_2.54mm
PinSocket_1x12_P2.54mm_Horizontal
Through hole angled socket strip, 1x12, 2.54mm pitch, 8.51mm socket length, single row (from Kicad 4.0.7), script generated
Through hole angled socket strip THT 1x12 2.54mm single row
0
12
12
Connector_PinSocket_2.54mm
PinSocket_1x12_P2.54mm_Vertical
Through hole straight socket strip, 1x12, 2.54mm pitch, single row (from Kicad 4.0.7), script generated
Through hole socket strip THT 1x12 2.54mm single row
0
12
12
Connector_PinSocket_2.54mm
PinSocket_1x12_P2.54mm_Vertical_SMD_Pin1Left
surface-mounted straight socket strip, 1x12, 2.54mm pitch, single row, style 1 (pin 1 left) (https://cdn.harwin.com/pdfs/M20-786.pdf), script generated
Surface mounted socket strip SMD 1x12 2.54mm single row style1 pin1 left
0
12
12
Connector_PinSocket_2.54mm
PinSocket_1x12_P2.54mm_Vertical_SMD_Pin1Right
surface-mounted straight socket strip, 1x12, 2.54mm pitch, single row, style 2 (pin 1 right) (https://cdn.harwin.com/pdfs/M20-786.pdf), script generated
Surface mounted socket strip SMD 1x12 2.54mm single row style2 pin1 right
0
12
12
Connector_PinSocket_2.54mm
PinSocket_1x13_P2.54mm_Horizontal
Through hole angled socket strip, 1x13, 2.54mm pitch, 8.51mm socket length, single row (from Kicad 4.0.7), script generated
Through hole angled socket strip THT 1x13 2.54mm single row
0
13
13
Connector_PinSocket_2.54mm
PinSocket_1x13_P2.54mm_Vertical
Through hole straight socket strip, 1x13, 2.54mm pitch, single row (from Kicad 4.0.7), script generated
Through hole socket strip THT 1x13 2.54mm single row
0
13
13
Connector_PinSocket_2.54mm
PinSocket_1x13_P2.54mm_Vertical_SMD_Pin1Left
surface-mounted straight socket strip, 1x13, 2.54mm pitch, single row, style 1 (pin 1 left) (https://cdn.harwin.com/pdfs/M20-786.pdf), script generated
Surface mounted socket strip SMD 1x13 2.54mm single row style1 pin1 left
0
13
13
Connector_PinSocket_2.54mm
PinSocket_1x13_P2.54mm_Vertical_SMD_Pin1Right
surface-mounted straight socket strip, 1x13, 2.54mm pitch, single row, style 2 (pin 1 right) (https://cdn.harwin.com/pdfs/M20-786.pdf), script generated
Surface mounted socket strip SMD 1x13 2.54mm single row style2 pin1 right
0
13
13
Connector_PinSocket_2.54mm
PinSocket_1x14_P2.54mm_Horizontal
Through hole angled socket strip, 1x14, 2.54mm pitch, 8.51mm socket length, single row (from Kicad 4.0.7), script generated
Through hole angled socket strip THT 1x14 2.54mm single row
0
14
14
Connector_PinSocket_2.54mm
PinSocket_1x14_P2.54mm_Vertical
Through hole straight socket strip, 1x14, 2.54mm pitch, single row (from Kicad 4.0.7), script generated
Through hole socket strip THT 1x14 2.54mm single row
0
14
14
Connector_PinSocket_2.54mm
PinSocket_1x14_P2.54mm_Vertical_SMD_Pin1Left
surface-mounted straight socket strip, 1x14, 2.54mm pitch, single row, style 1 (pin 1 left) (https://cdn.harwin.com/pdfs/M20-786.pdf), script generated
Surface mounted socket strip SMD 1x14 2.54mm single row style1 pin1 left
0
14
14
Connector_PinSocket_2.54mm
PinSocket_1x14_P2.54mm_Vertical_SMD_Pin1Right
surface-mounted straight socket strip, 1x14, 2.54mm pitch, single row, style 2 (pin 1 right) (https://cdn.harwin.com/pdfs/M20-786.pdf), script generated
Surface mounted socket strip SMD 1x14 2.54mm single row style2 pin1 right
0
14
14
Connector_PinSocket_2.54mm
PinSocket_1x15_P2.54mm_Horizontal
Through hole angled socket strip, 1x15, 2.54mm pitch, 8.51mm socket length, single row (from Kicad 4.0.7), script generated
Through hole angled socket strip THT 1x15 2.54mm single row
0
15
15
Connector_PinSocket_2.54mm
PinSocket_1x15_P2.54mm_Vertical
Through hole straight socket strip, 1x15, 2.54mm pitch, single row (from Kicad 4.0.7), script generated
Through hole socket strip THT 1x15 2.54mm single row
0
15
15
Connector_PinSocket_2.54mm
PinSocket_1x15_P2.54mm_Vertical_SMD_Pin1Left
surface-mounted straight socket strip, 1x15, 2.54mm pitch, single row, style 1 (pin 1 left) (https://cdn.harwin.com/pdfs/M20-786.pdf), script generated
Surface mounted socket strip SMD 1x15 2.54mm single row style1 pin1 left
0
15
15
Connector_PinSocket_2.54mm
PinSocket_1x15_P2.54mm_Vertical_SMD_Pin1Right
surface-mounted straight socket strip, 1x15, 2.54mm pitch, single row, style 2 (pin 1 right) (https://cdn.harwin.com/pdfs/M20-786.pdf), script generated
Surface mounted socket strip SMD 1x15 2.54mm single row style2 pin1 right
0
15
15
Connector_PinSocket_2.54mm
PinSocket_1x16_P2.54mm_Horizontal
Through hole angled socket strip, 1x16, 2.54mm pitch, 8.51mm socket length, single row (from Kicad 4.0.7), script generated
Through hole angled socket strip THT 1x16 2.54mm single row
0
16
16
Connector_PinSocket_2.54mm
PinSocket_1x16_P2.54mm_Vertical
Through hole straight socket strip, 1x16, 2.54mm pitch, single row (from Kicad 4.0.7), script generated
Through hole socket strip THT 1x16 2.54mm single row
0
16
16
Connector_PinSocket_2.54mm
PinSocket_1x16_P2.54mm_Vertical_SMD_Pin1Left
surface-mounted straight socket strip, 1x16, 2.54mm pitch, single row, style 1 (pin 1 left) (https://cdn.harwin.com/pdfs/M20-786.pdf), script generated
Surface mounted socket strip SMD 1x16 2.54mm single row style1 pin1 left
0
16
16
Connector_PinSocket_2.54mm
PinSocket_1x16_P2.54mm_Vertical_SMD_Pin1Right
surface-mounted straight socket strip, 1x16, 2.54mm pitch, single row, style 2 (pin 1 right) (https://cdn.harwin.com/pdfs/M20-786.pdf), script generated
Surface mounted socket strip SMD 1x16 2.54mm single row style2 pin1 right
0
16
16
Connector_PinSocket_2.54mm
PinSocket_1x17_P2.54mm_Horizontal
Through hole angled socket strip, 1x17, 2.54mm pitch, 8.51mm socket length, single row (from Kicad 4.0.7), script generated
Through hole angled socket strip THT 1x17 2.54mm single row
0
17
17
Connector_PinSocket_2.54mm
PinSocket_1x17_P2.54mm_Vertical
Through hole straight socket strip, 1x17, 2.54mm pitch, single row (from Kicad 4.0.7), script generated
Through hole socket strip THT 1x17 2.54mm single row
0
17
17
Connector_PinSocket_2.54mm
PinSocket_1x17_P2.54mm_Vertical_SMD_Pin1Left
surface-mounted straight socket strip, 1x17, 2.54mm pitch, single row, style 1 (pin 1 left) (https://cdn.harwin.com/pdfs/M20-786.pdf), script generated
Surface mounted socket strip SMD 1x17 2.54mm single row style1 pin1 left
0
17
17
Connector_PinSocket_2.54mm
PinSocket_1x17_P2.54mm_Vertical_SMD_Pin1Right
surface-mounted straight socket strip, 1x17, 2.54mm pitch, single row, style 2 (pin 1 right) (https://cdn.harwin.com/pdfs/M20-786.pdf), script generated
Surface mounted socket strip SMD 1x17 2.54mm single row style2 pin1 right
0
17
17
Connector_PinSocket_2.54mm
PinSocket_1x18_P2.54mm_Horizontal
Through hole angled socket strip, 1x18, 2.54mm pitch, 8.51mm socket length, single row (from Kicad 4.0.7), script generated
Through hole angled socket strip THT 1x18 2.54mm single row
0
18
18
Connector_PinSocket_2.54mm
PinSocket_1x18_P2.54mm_Vertical
Through hole straight socket strip, 1x18, 2.54mm pitch, single row (from Kicad 4.0.7), script generated
Through hole socket strip THT 1x18 2.54mm single row
0
18
18
Connector_PinSocket_2.54mm
PinSocket_1x18_P2.54mm_Vertical_SMD_Pin1Left
surface-mounted straight socket strip, 1x18, 2.54mm pitch, single row, style 1 (pin 1 left) (https://cdn.harwin.com/pdfs/M20-786.pdf), script generated
Surface mounted socket strip SMD 1x18 2.54mm single row style1 pin1 left
0
18
18
Connector_PinSocket_2.54mm
PinSocket_1x18_P2.54mm_Vertical_SMD_Pin1Right
surface-mounted straight socket strip, 1x18, 2.54mm pitch, single row, style 2 (pin 1 right) (https://cdn.harwin.com/pdfs/M20-786.pdf), script generated
Surface mounted socket strip SMD 1x18 2.54mm single row style2 pin1 right
0
18
18
Connector_PinSocket_2.54mm
PinSocket_1x19_P2.54mm_Horizontal
Through hole angled socket strip, 1x19, 2.54mm pitch, 8.51mm socket length, single row (from Kicad 4.0.7), script generated
Through hole angled socket strip THT 1x19 2.54mm single row
0
19
19
Connector_PinSocket_2.54mm
PinSocket_1x19_P2.54mm_Vertical
Through hole straight socket strip, 1x19, 2.54mm pitch, single row (from Kicad 4.0.7), script generated
Through hole socket strip THT 1x19 2.54mm single row
0
19
19
Connector_PinSocket_2.54mm
PinSocket_1x19_P2.54mm_Vertical_SMD_Pin1Left
surface-mounted straight socket strip, 1x19, 2.54mm pitch, single row, style 1 (pin 1 left) (https://cdn.harwin.com/pdfs/M20-786.pdf), script generated
Surface mounted socket strip SMD 1x19 2.54mm single row style1 pin1 left
0
19
19
Connector_PinSocket_2.54mm
PinSocket_1x19_P2.54mm_Vertical_SMD_Pin1Right
surface-mounted straight socket strip, 1x19, 2.54mm pitch, single row, style 2 (pin 1 right) (https://cdn.harwin.com/pdfs/M20-786.pdf), script generated
Surface mounted socket strip SMD 1x19 2.54mm single row style2 pin1 right
0
19
19
Connector_PinSocket_2.54mm
PinSocket_1x20_P2.54mm_Horizontal
Through hole angled socket strip, 1x20, 2.54mm pitch, 8.51mm socket length, single row (from Kicad 4.0.7), script generated
Through hole angled socket strip THT 1x20 2.54mm single row
0
20
20
Connector_PinSocket_2.54mm
PinSocket_1x20_P2.54mm_Vertical
Through hole straight socket strip, 1x20, 2.54mm pitch, single row (from Kicad 4.0.7), script generated
Through hole socket strip THT 1x20 2.54mm single row
0
20
20
Connector_PinSocket_2.54mm
PinSocket_1x20_P2.54mm_Vertical_SMD_Pin1Left
surface-mounted straight socket strip, 1x20, 2.54mm pitch, single row, style 1 (pin 1 left) (https://cdn.harwin.com/pdfs/M20-786.pdf), script generated
Surface mounted socket strip SMD 1x20 2.54mm single row style1 pin1 left
0
20
20
Connector_PinSocket_2.54mm
PinSocket_1x20_P2.54mm_Vertical_SMD_Pin1Right
surface-mounted straight socket strip, 1x20, 2.54mm pitch, single row, style 2 (pin 1 right) (https://cdn.harwin.com/pdfs/M20-786.pdf), script generated
Surface mounted socket strip SMD 1x20 2.54mm single row style2 pin1 right
0
20
20
Connector_PinSocket_2.54mm
PinSocket_1x21_P2.54mm_Horizontal
Through hole angled socket strip, 1x21, 2.54mm pitch, 8.51mm socket length, single row (from Kicad 4.0.7), script generated
Through hole angled socket strip THT 1x21 2.54mm single row
0
21
21
Connector_PinSocket_2.54mm
PinSocket_1x21_P2.54mm_Vertical
Through hole straight socket strip, 1x21, 2.54mm pitch, single row (from Kicad 4.0.7), script generated
Through hole socket strip THT 1x21 2.54mm single row
0
21
21
Connector_PinSocket_2.54mm
PinSocket_1x21_P2.54mm_Vertical_SMD_Pin1Left
surface-mounted straight socket strip, 1x21, 2.54mm pitch, single row, style 1 (pin 1 left) (https://cdn.harwin.com/pdfs/M20-786.pdf), script generated
Surface mounted socket strip SMD 1x21 2.54mm single row style1 pin1 left
0
21
21
Connector_PinSocket_2.54mm
PinSocket_1x21_P2.54mm_Vertical_SMD_Pin1Right
surface-mounted straight socket strip, 1x21, 2.54mm pitch, single row, style 2 (pin 1 right) (https://cdn.harwin.com/pdfs/M20-786.pdf), script generated
Surface mounted socket strip SMD 1x21 2.54mm single row style2 pin1 right
0
21
21
Connector_PinSocket_2.54mm
PinSocket_1x22_P2.54mm_Horizontal
Through hole angled socket strip, 1x22, 2.54mm pitch, 8.51mm socket length, single row (from Kicad 4.0.7), script generated
Through hole angled socket strip THT 1x22 2.54mm single row
0
22
22
Connector_PinSocket_2.54mm
PinSocket_1x22_P2.54mm_Vertical
Through hole straight socket strip, 1x22, 2.54mm pitch, single row (from Kicad 4.0.7), script generated
Through hole socket strip THT 1x22 2.54mm single row
0
22
22
Connector_PinSocket_2.54mm
PinSocket_1x22_P2.54mm_Vertical_SMD_Pin1Left
surface-mounted straight socket strip, 1x22, 2.54mm pitch, single row, style 1 (pin 1 left) (https://cdn.harwin.com/pdfs/M20-786.pdf), script generated
Surface mounted socket strip SMD 1x22 2.54mm single row style1 pin1 left
0
22
22
Connector_PinSocket_2.54mm
PinSocket_1x22_P2.54mm_Vertical_SMD_Pin1Right
surface-mounted straight socket strip, 1x22, 2.54mm pitch, single row, style 2 (pin 1 right) (https://cdn.harwin.com/pdfs/M20-786.pdf), script generated
Surface mounted socket strip SMD 1x22 2.54mm single row style2 pin1 right
0
22
22
Connector_PinSocket_2.54mm
PinSocket_1x23_P2.54mm_Horizontal
Through hole angled socket strip, 1x23, 2.54mm pitch, 8.51mm socket length, single row (from Kicad 4.0.7), script generated
Through hole angled socket strip THT 1x23 2.54mm single row
0
23
23
Connector_PinSocket_2.54mm
PinSocket_1x23_P2.54mm_Vertical
Through hole straight socket strip, 1x23, 2.54mm pitch, single row (from Kicad 4.0.7), script generated
Through hole socket strip THT 1x23 2.54mm single row
0
23
23
Connector_PinSocket_2.54mm
PinSocket_1x23_P2.54mm_Vertical_SMD_Pin1Left
surface-mounted straight socket strip, 1x23, 2.54mm pitch, single row, style 1 (pin 1 left) (https://cdn.harwin.com/pdfs/M20-786.pdf), script generated
Surface mounted socket strip SMD 1x23 2.54mm single row style1 pin1 left
0
23
23
Connector_PinSocket_2.54mm
PinSocket_1x23_P2.54mm_Vertical_SMD_Pin1Right
surface-mounted straight socket strip, 1x23, 2.54mm pitch, single row, style 2 (pin 1 right) (https://cdn.harwin.com/pdfs/M20-786.pdf), script generated
Surface mounted socket strip SMD 1x23 2.54mm single row style2 pin1 right
0
23
23
Connector_PinSocket_2.54mm
PinSocket_1x24_P2.54mm_Horizontal
Through hole angled socket strip, 1x24, 2.54mm pitch, 8.51mm socket length, single row (from Kicad 4.0.7), script generated
Through hole angled socket strip THT 1x24 2.54mm single row
0
24
24
Connector_PinSocket_2.54mm
PinSocket_1x24_P2.54mm_Vertical
Through hole straight socket strip, 1x24, 2.54mm pitch, single row (from Kicad 4.0.7), script generated
Through hole socket strip THT 1x24 2.54mm single row
0
24
24
Connector_PinSocket_2.54mm
PinSocket_1x24_P2.54mm_Vertical_SMD_Pin1Left
surface-mounted straight socket strip, 1x24, 2.54mm pitch, single row, style 1 (pin 1 left) (https://cdn.harwin.com/pdfs/M20-786.pdf), script generated
Surface mounted socket strip SMD 1x24 2.54mm single row style1 pin1 left
0
24
24
Connector_PinSocket_2.54mm
PinSocket_1x24_P2.54mm_Vertical_SMD_Pin1Right
surface-mounted straight socket strip, 1x24, 2.54mm pitch, single row, style 2 (pin 1 right) (https://cdn.harwin.com/pdfs/M20-786.pdf), script generated
Surface mounted socket strip SMD 1x24 2.54mm single row style2 pin1 right
0
24
24
Connector_PinSocket_2.54mm
PinSocket_1x25_P2.54mm_Horizontal
Through hole angled socket strip, 1x25, 2.54mm pitch, 8.51mm socket length, single row (from Kicad 4.0.7), script generated
Through hole angled socket strip THT 1x25 2.54mm single row
0
25
25
Connector_PinSocket_2.54mm
PinSocket_1x25_P2.54mm_Vertical
Through hole straight socket strip, 1x25, 2.54mm pitch, single row (from Kicad 4.0.7), script generated
Through hole socket strip THT 1x25 2.54mm single row
0
25
25
Connector_PinSocket_2.54mm
PinSocket_1x25_P2.54mm_Vertical_SMD_Pin1Left
surface-mounted straight socket strip, 1x25, 2.54mm pitch, single row, style 1 (pin 1 left) (https://cdn.harwin.com/pdfs/M20-786.pdf), script generated
Surface mounted socket strip SMD 1x25 2.54mm single row style1 pin1 left
0
25
25
Connector_PinSocket_2.54mm
PinSocket_1x25_P2.54mm_Vertical_SMD_Pin1Right
surface-mounted straight socket strip, 1x25, 2.54mm pitch, single row, style 2 (pin 1 right) (https://cdn.harwin.com/pdfs/M20-786.pdf), script generated
Surface mounted socket strip SMD 1x25 2.54mm single row style2 pin1 right
0
25
25
Connector_PinSocket_2.54mm
PinSocket_1x26_P2.54mm_Horizontal
Through hole angled socket strip, 1x26, 2.54mm pitch, 8.51mm socket length, single row (from Kicad 4.0.7), script generated
Through hole angled socket strip THT 1x26 2.54mm single row
0
26
26
Connector_PinSocket_2.54mm
PinSocket_1x26_P2.54mm_Vertical
Through hole straight socket strip, 1x26, 2.54mm pitch, single row (from Kicad 4.0.7), script generated
Through hole socket strip THT 1x26 2.54mm single row
0
26
26
Connector_PinSocket_2.54mm
PinSocket_1x26_P2.54mm_Vertical_SMD_Pin1Left
surface-mounted straight socket strip, 1x26, 2.54mm pitch, single row, style 1 (pin 1 left) (https://cdn.harwin.com/pdfs/M20-786.pdf), script generated
Surface mounted socket strip SMD 1x26 2.54mm single row style1 pin1 left
0
26
26
Connector_PinSocket_2.54mm
PinSocket_1x26_P2.54mm_Vertical_SMD_Pin1Right
surface-mounted straight socket strip, 1x26, 2.54mm pitch, single row, style 2 (pin 1 right) (https://cdn.harwin.com/pdfs/M20-786.pdf), script generated
Surface mounted socket strip SMD 1x26 2.54mm single row style2 pin1 right
0
26
26
Connector_PinSocket_2.54mm
PinSocket_1x27_P2.54mm_Horizontal
Through hole angled socket strip, 1x27, 2.54mm pitch, 8.51mm socket length, single row (from Kicad 4.0.7), script generated
Through hole angled socket strip THT 1x27 2.54mm single row
0
27
27
Connector_PinSocket_2.54mm
PinSocket_1x27_P2.54mm_Vertical
Through hole straight socket strip, 1x27, 2.54mm pitch, single row (from Kicad 4.0.7), script generated
Through hole socket strip THT 1x27 2.54mm single row
0
27
27
Connector_PinSocket_2.54mm
PinSocket_1x27_P2.54mm_Vertical_SMD_Pin1Left
surface-mounted straight socket strip, 1x27, 2.54mm pitch, single row, style 1 (pin 1 left) (https://cdn.harwin.com/pdfs/M20-786.pdf), script generated
Surface mounted socket strip SMD 1x27 2.54mm single row style1 pin1 left
0
27
27
Connector_PinSocket_2.54mm
PinSocket_1x27_P2.54mm_Vertical_SMD_Pin1Right
surface-mounted straight socket strip, 1x27, 2.54mm pitch, single row, style 2 (pin 1 right) (https://cdn.harwin.com/pdfs/M20-786.pdf), script generated
Surface mounted socket strip SMD 1x27 2.54mm single row style2 pin1 right
0
27
27
Connector_PinSocket_2.54mm
PinSocket_1x28_P2.54mm_Horizontal
Through hole angled socket strip, 1x28, 2.54mm pitch, 8.51mm socket length, single row (from Kicad 4.0.7), script generated
Through hole angled socket strip THT 1x28 2.54mm single row
0
28
28
Connector_PinSocket_2.54mm
PinSocket_1x28_P2.54mm_Vertical
Through hole straight socket strip, 1x28, 2.54mm pitch, single row (from Kicad 4.0.7), script generated
Through hole socket strip THT 1x28 2.54mm single row
0
28
28
Connector_PinSocket_2.54mm
PinSocket_1x28_P2.54mm_Vertical_SMD_Pin1Left
surface-mounted straight socket strip, 1x28, 2.54mm pitch, single row, style 1 (pin 1 left) (https://cdn.harwin.com/pdfs/M20-786.pdf), script generated
Surface mounted socket strip SMD 1x28 2.54mm single row style1 pin1 left
0
28
28
Connector_PinSocket_2.54mm
PinSocket_1x28_P2.54mm_Vertical_SMD_Pin1Right
surface-mounted straight socket strip, 1x28, 2.54mm pitch, single row, style 2 (pin 1 right) (https://cdn.harwin.com/pdfs/M20-786.pdf), script generated
Surface mounted socket strip SMD 1x28 2.54mm single row style2 pin1 right
0
28
28
Connector_PinSocket_2.54mm
PinSocket_1x29_P2.54mm_Horizontal
Through hole angled socket strip, 1x29, 2.54mm pitch, 8.51mm socket length, single row (from Kicad 4.0.7), script generated
Through hole angled socket strip THT 1x29 2.54mm single row
0
29
29
Connector_PinSocket_2.54mm
PinSocket_1x29_P2.54mm_Vertical
Through hole straight socket strip, 1x29, 2.54mm pitch, single row (from Kicad 4.0.7), script generated
Through hole socket strip THT 1x29 2.54mm single row
0
29
29
Connector_PinSocket_2.54mm
PinSocket_1x29_P2.54mm_Vertical_SMD_Pin1Left
surface-mounted straight socket strip, 1x29, 2.54mm pitch, single row, style 1 (pin 1 left) (https://cdn.harwin.com/pdfs/M20-786.pdf), script generated
Surface mounted socket strip SMD 1x29 2.54mm single row style1 pin1 left
0
29
29
Connector_PinSocket_2.54mm
PinSocket_1x29_P2.54mm_Vertical_SMD_Pin1Right
surface-mounted straight socket strip, 1x29, 2.54mm pitch, single row, style 2 (pin 1 right) (https://cdn.harwin.com/pdfs/M20-786.pdf), script generated
Surface mounted socket strip SMD 1x29 2.54mm single row style2 pin1 right
0
29
29
Connector_PinSocket_2.54mm
PinSocket_1x30_P2.54mm_Horizontal
Through hole angled socket strip, 1x30, 2.54mm pitch, 8.51mm socket length, single row (from Kicad 4.0.7), script generated
Through hole angled socket strip THT 1x30 2.54mm single row
0
30
30
Connector_PinSocket_2.54mm
PinSocket_1x30_P2.54mm_Vertical
Through hole straight socket strip, 1x30, 2.54mm pitch, single row (from Kicad 4.0.7), script generated
Through hole socket strip THT 1x30 2.54mm single row
0
30
30
Connector_PinSocket_2.54mm
PinSocket_1x30_P2.54mm_Vertical_SMD_Pin1Left
surface-mounted straight socket strip, 1x30, 2.54mm pitch, single row, style 1 (pin 1 left) (https://cdn.harwin.com/pdfs/M20-786.pdf), script generated
Surface mounted socket strip SMD 1x30 2.54mm single row style1 pin1 left
0
30
30
Connector_PinSocket_2.54mm
PinSocket_1x30_P2.54mm_Vertical_SMD_Pin1Right
surface-mounted straight socket strip, 1x30, 2.54mm pitch, single row, style 2 (pin 1 right) (https://cdn.harwin.com/pdfs/M20-786.pdf), script generated
Surface mounted socket strip SMD 1x30 2.54mm single row style2 pin1 right
0
30
30
Connector_PinSocket_2.54mm
PinSocket_1x31_P2.54mm_Horizontal
Through hole angled socket strip, 1x31, 2.54mm pitch, 8.51mm socket length, single row (from Kicad 4.0.7), script generated
Through hole angled socket strip THT 1x31 2.54mm single row
0
31
31
Connector_PinSocket_2.54mm
PinSocket_1x31_P2.54mm_Vertical
Through hole straight socket strip, 1x31, 2.54mm pitch, single row (from Kicad 4.0.7), script generated
Through hole socket strip THT 1x31 2.54mm single row
0
31
31
Connector_PinSocket_2.54mm
PinSocket_1x31_P2.54mm_Vertical_SMD_Pin1Left
surface-mounted straight socket strip, 1x31, 2.54mm pitch, single row, style 1 (pin 1 left) (https://cdn.harwin.com/pdfs/M20-786.pdf), script generated
Surface mounted socket strip SMD 1x31 2.54mm single row style1 pin1 left
0
31
31
Connector_PinSocket_2.54mm
PinSocket_1x31_P2.54mm_Vertical_SMD_Pin1Right
surface-mounted straight socket strip, 1x31, 2.54mm pitch, single row, style 2 (pin 1 right) (https://cdn.harwin.com/pdfs/M20-786.pdf), script generated
Surface mounted socket strip SMD 1x31 2.54mm single row style2 pin1 right
0
31
31
Connector_PinSocket_2.54mm
PinSocket_1x32_P2.54mm_Horizontal
Through hole angled socket strip, 1x32, 2.54mm pitch, 8.51mm socket length, single row (from Kicad 4.0.7), script generated
Through hole angled socket strip THT 1x32 2.54mm single row
0
32
32
Connector_PinSocket_2.54mm
PinSocket_1x32_P2.54mm_Vertical
Through hole straight socket strip, 1x32, 2.54mm pitch, single row (from Kicad 4.0.7), script generated
Through hole socket strip THT 1x32 2.54mm single row
0
32
32
Connector_PinSocket_2.54mm
PinSocket_1x32_P2.54mm_Vertical_SMD_Pin1Left
surface-mounted straight socket strip, 1x32, 2.54mm pitch, single row, style 1 (pin 1 left) (https://cdn.harwin.com/pdfs/M20-786.pdf), script generated
Surface mounted socket strip SMD 1x32 2.54mm single row style1 pin1 left
0
32
32
Connector_PinSocket_2.54mm
PinSocket_1x32_P2.54mm_Vertical_SMD_Pin1Right
surface-mounted straight socket strip, 1x32, 2.54mm pitch, single row, style 2 (pin 1 right) (https://cdn.harwin.com/pdfs/M20-786.pdf), script generated
Surface mounted socket strip SMD 1x32 2.54mm single row style2 pin1 right
0
32
32
Connector_PinSocket_2.54mm
PinSocket_1x33_P2.54mm_Horizontal
Through hole angled socket strip, 1x33, 2.54mm pitch, 8.51mm socket length, single row (from Kicad 4.0.7), script generated
Through hole angled socket strip THT 1x33 2.54mm single row
0
33
33
Connector_PinSocket_2.54mm
PinSocket_1x33_P2.54mm_Vertical
Through hole straight socket strip, 1x33, 2.54mm pitch, single row (from Kicad 4.0.7), script generated
Through hole socket strip THT 1x33 2.54mm single row
0
33
33
Connector_PinSocket_2.54mm
PinSocket_1x33_P2.54mm_Vertical_SMD_Pin1Left
surface-mounted straight socket strip, 1x33, 2.54mm pitch, single row, style 1 (pin 1 left) (https://cdn.harwin.com/pdfs/M20-786.pdf), script generated
Surface mounted socket strip SMD 1x33 2.54mm single row style1 pin1 left
0
33
33
Connector_PinSocket_2.54mm
PinSocket_1x33_P2.54mm_Vertical_SMD_Pin1Right
surface-mounted straight socket strip, 1x33, 2.54mm pitch, single row, style 2 (pin 1 right) (https://cdn.harwin.com/pdfs/M20-786.pdf), script generated
Surface mounted socket strip SMD 1x33 2.54mm single row style2 pin1 right
0
33
33
Connector_PinSocket_2.54mm
PinSocket_1x34_P2.54mm_Horizontal
Through hole angled socket strip, 1x34, 2.54mm pitch, 8.51mm socket length, single row (from Kicad 4.0.7), script generated
Through hole angled socket strip THT 1x34 2.54mm single row
0
34
34
Connector_PinSocket_2.54mm
PinSocket_1x34_P2.54mm_Vertical
Through hole straight socket strip, 1x34, 2.54mm pitch, single row (from Kicad 4.0.7), script generated
Through hole socket strip THT 1x34 2.54mm single row
0
34
34
Connector_PinSocket_2.54mm
PinSocket_1x34_P2.54mm_Vertical_SMD_Pin1Left
surface-mounted straight socket strip, 1x34, 2.54mm pitch, single row, style 1 (pin 1 left) (https://cdn.harwin.com/pdfs/M20-786.pdf), script generated
Surface mounted socket strip SMD 1x34 2.54mm single row style1 pin1 left
0
34
34
Connector_PinSocket_2.54mm
PinSocket_1x34_P2.54mm_Vertical_SMD_Pin1Right
surface-mounted straight socket strip, 1x34, 2.54mm pitch, single row, style 2 (pin 1 right) (https://cdn.harwin.com/pdfs/M20-786.pdf), script generated
Surface mounted socket strip SMD 1x34 2.54mm single row style2 pin1 right
0
34
34
Connector_PinSocket_2.54mm
PinSocket_1x35_P2.54mm_Horizontal
Through hole angled socket strip, 1x35, 2.54mm pitch, 8.51mm socket length, single row (from Kicad 4.0.7), script generated
Through hole angled socket strip THT 1x35 2.54mm single row
0
35
35
Connector_PinSocket_2.54mm
PinSocket_1x35_P2.54mm_Vertical
Through hole straight socket strip, 1x35, 2.54mm pitch, single row (from Kicad 4.0.7), script generated
Through hole socket strip THT 1x35 2.54mm single row
0
35
35
Connector_PinSocket_2.54mm
PinSocket_1x35_P2.54mm_Vertical_SMD_Pin1Left
surface-mounted straight socket strip, 1x35, 2.54mm pitch, single row, style 1 (pin 1 left) (https://cdn.harwin.com/pdfs/M20-786.pdf), script generated
Surface mounted socket strip SMD 1x35 2.54mm single row style1 pin1 left
0
35
35
Connector_PinSocket_2.54mm
PinSocket_1x35_P2.54mm_Vertical_SMD_Pin1Right
surface-mounted straight socket strip, 1x35, 2.54mm pitch, single row, style 2 (pin 1 right) (https://cdn.harwin.com/pdfs/M20-786.pdf), script generated
Surface mounted socket strip SMD 1x35 2.54mm single row style2 pin1 right
0
35
35
Connector_PinSocket_2.54mm
PinSocket_1x36_P2.54mm_Horizontal
Through hole angled socket strip, 1x36, 2.54mm pitch, 8.51mm socket length, single row (from Kicad 4.0.7), script generated
Through hole angled socket strip THT 1x36 2.54mm single row
0
36
36
Connector_PinSocket_2.54mm
PinSocket_1x36_P2.54mm_Vertical
Through hole straight socket strip, 1x36, 2.54mm pitch, single row (from Kicad 4.0.7), script generated
Through hole socket strip THT 1x36 2.54mm single row
0
36
36
Connector_PinSocket_2.54mm
PinSocket_1x36_P2.54mm_Vertical_SMD_Pin1Left
surface-mounted straight socket strip, 1x36, 2.54mm pitch, single row, style 1 (pin 1 left) (https://cdn.harwin.com/pdfs/M20-786.pdf), script generated
Surface mounted socket strip SMD 1x36 2.54mm single row style1 pin1 left
0
36
36
Connector_PinSocket_2.54mm
PinSocket_1x36_P2.54mm_Vertical_SMD_Pin1Right
surface-mounted straight socket strip, 1x36, 2.54mm pitch, single row, style 2 (pin 1 right) (https://cdn.harwin.com/pdfs/M20-786.pdf), script generated
Surface mounted socket strip SMD 1x36 2.54mm single row style2 pin1 right
0
36
36
Connector_PinSocket_2.54mm
PinSocket_1x37_P2.54mm_Horizontal
Through hole angled socket strip, 1x37, 2.54mm pitch, 8.51mm socket length, single row (from Kicad 4.0.7), script generated
Through hole angled socket strip THT 1x37 2.54mm single row
0
37
37
Connector_PinSocket_2.54mm
PinSocket_1x37_P2.54mm_Vertical
Through hole straight socket strip, 1x37, 2.54mm pitch, single row (from Kicad 4.0.7), script generated
Through hole socket strip THT 1x37 2.54mm single row
0
37
37
Connector_PinSocket_2.54mm
PinSocket_1x37_P2.54mm_Vertical_SMD_Pin1Left
surface-mounted straight socket strip, 1x37, 2.54mm pitch, single row, style 1 (pin 1 left) (https://cdn.harwin.com/pdfs/M20-786.pdf), script generated
Surface mounted socket strip SMD 1x37 2.54mm single row style1 pin1 left
0
37
37
Connector_PinSocket_2.54mm
PinSocket_1x37_P2.54mm_Vertical_SMD_Pin1Right
surface-mounted straight socket strip, 1x37, 2.54mm pitch, single row, style 2 (pin 1 right) (https://cdn.harwin.com/pdfs/M20-786.pdf), script generated
Surface mounted socket strip SMD 1x37 2.54mm single row style2 pin1 right
0
37
37
Connector_PinSocket_2.54mm
PinSocket_1x38_P2.54mm_Horizontal
Through hole angled socket strip, 1x38, 2.54mm pitch, 8.51mm socket length, single row (from Kicad 4.0.7), script generated
Through hole angled socket strip THT 1x38 2.54mm single row
0
38
38
Connector_PinSocket_2.54mm
PinSocket_1x38_P2.54mm_Vertical
Through hole straight socket strip, 1x38, 2.54mm pitch, single row (from Kicad 4.0.7), script generated
Through hole socket strip THT 1x38 2.54mm single row
0
38
38
Connector_PinSocket_2.54mm
PinSocket_1x38_P2.54mm_Vertical_SMD_Pin1Left
surface-mounted straight socket strip, 1x38, 2.54mm pitch, single row, style 1 (pin 1 left) (https://cdn.harwin.com/pdfs/M20-786.pdf), script generated
Surface mounted socket strip SMD 1x38 2.54mm single row style1 pin1 left
0
38
38
Connector_PinSocket_2.54mm
PinSocket_1x38_P2.54mm_Vertical_SMD_Pin1Right
surface-mounted straight socket strip, 1x38, 2.54mm pitch, single row, style 2 (pin 1 right) (https://cdn.harwin.com/pdfs/M20-786.pdf), script generated
Surface mounted socket strip SMD 1x38 2.54mm single row style2 pin1 right
0
38
38
Connector_PinSocket_2.54mm
PinSocket_1x39_P2.54mm_Horizontal
Through hole angled socket strip, 1x39, 2.54mm pitch, 8.51mm socket length, single row (from Kicad 4.0.7), script generated
Through hole angled socket strip THT 1x39 2.54mm single row
0
39
39
Connector_PinSocket_2.54mm
PinSocket_1x39_P2.54mm_Vertical
Through hole straight socket strip, 1x39, 2.54mm pitch, single row (from Kicad 4.0.7), script generated
Through hole socket strip THT 1x39 2.54mm single row
0
39
39
Connector_PinSocket_2.54mm
PinSocket_1x39_P2.54mm_Vertical_SMD_Pin1Left
surface-mounted straight socket strip, 1x39, 2.54mm pitch, single row, style 1 (pin 1 left) (https://cdn.harwin.com/pdfs/M20-786.pdf), script generated
Surface mounted socket strip SMD 1x39 2.54mm single row style1 pin1 left
0
39
39
Connector_PinSocket_2.54mm
PinSocket_1x39_P2.54mm_Vertical_SMD_Pin1Right
surface-mounted straight socket strip, 1x39, 2.54mm pitch, single row, style 2 (pin 1 right) (https://cdn.harwin.com/pdfs/M20-786.pdf), script generated
Surface mounted socket strip SMD 1x39 2.54mm single row style2 pin1 right
0
39
39
Connector_PinSocket_2.54mm
PinSocket_1x40_P2.54mm_Horizontal
Through hole angled socket strip, 1x40, 2.54mm pitch, 8.51mm socket length, single row (from Kicad 4.0.7), script generated
Through hole angled socket strip THT 1x40 2.54mm single row
0
40
40
Connector_PinSocket_2.54mm
PinSocket_1x40_P2.54mm_Vertical
Through hole straight socket strip, 1x40, 2.54mm pitch, single row (from Kicad 4.0.7), script generated
Through hole socket strip THT 1x40 2.54mm single row
0
40
40
Connector_PinSocket_2.54mm
PinSocket_1x40_P2.54mm_Vertical_SMD_Pin1Left
surface-mounted straight socket strip, 1x40, 2.54mm pitch, single row, style 1 (pin 1 left) (https://cdn.harwin.com/pdfs/M20-786.pdf), script generated
Surface mounted socket strip SMD 1x40 2.54mm single row style1 pin1 left
0
40
40
Connector_PinSocket_2.54mm
PinSocket_1x40_P2.54mm_Vertical_SMD_Pin1Right
surface-mounted straight socket strip, 1x40, 2.54mm pitch, single row, style 2 (pin 1 right) (https://cdn.harwin.com/pdfs/M20-786.pdf), script generated
Surface mounted socket strip SMD 1x40 2.54mm single row style2 pin1 right
0
40
40
Connector_PinSocket_2.54mm
PinSocket_2x01_P2.54mm_Horizontal
Through hole angled socket strip, 2x01, 2.54mm pitch, 8.51mm socket length, double cols (from Kicad 4.0.7), script generated
Through hole angled socket strip THT 2x01 2.54mm double row
0
2
2
Connector_PinSocket_2.54mm
PinSocket_2x01_P2.54mm_Vertical
Through hole straight socket strip, 2x01, 2.54mm pitch, double cols (from Kicad 4.0.7), script generated
Through hole socket strip THT 2x01 2.54mm double row
0
2
2
Connector_PinSocket_2.54mm
PinSocket_2x01_P2.54mm_Vertical_SMD
surface-mounted straight socket strip, 2x01, 2.54mm pitch, double cols (from Kicad 4.0.7), script generated
Surface mounted socket strip SMD 2x01 2.54mm double row
0
2
2
Connector_PinSocket_2.54mm
PinSocket_2x02_P2.54mm_Horizontal
Through hole angled socket strip, 2x02, 2.54mm pitch, 8.51mm socket length, double cols (from Kicad 4.0.7), script generated
Through hole angled socket strip THT 2x02 2.54mm double row
0
4
4
Connector_PinSocket_2.54mm
PinSocket_2x02_P2.54mm_Vertical
Through hole straight socket strip, 2x02, 2.54mm pitch, double cols (from Kicad 4.0.7), script generated
Through hole socket strip THT 2x02 2.54mm double row
0
4
4
Connector_PinSocket_2.54mm
PinSocket_2x02_P2.54mm_Vertical_SMD
surface-mounted straight socket strip, 2x02, 2.54mm pitch, double cols (from Kicad 4.0.7), script generated
Surface mounted socket strip SMD 2x02 2.54mm double row
0
4
4
Connector_PinSocket_2.54mm
PinSocket_2x03_P2.54mm_Horizontal
Through hole angled socket strip, 2x03, 2.54mm pitch, 8.51mm socket length, double cols (from Kicad 4.0.7), script generated
Through hole angled socket strip THT 2x03 2.54mm double row
0
6
6
Connector_PinSocket_2.54mm
PinSocket_2x03_P2.54mm_Vertical
Through hole straight socket strip, 2x03, 2.54mm pitch, double cols (from Kicad 4.0.7), script generated
Through hole socket strip THT 2x03 2.54mm double row
0
6
6
Connector_PinSocket_2.54mm
PinSocket_2x03_P2.54mm_Vertical_SMD
surface-mounted straight socket strip, 2x03, 2.54mm pitch, double cols (from Kicad 4.0.7), script generated
Surface mounted socket strip SMD 2x03 2.54mm double row
0
6
6
Connector_PinSocket_2.54mm
PinSocket_2x04_P2.54mm_Horizontal
Through hole angled socket strip, 2x04, 2.54mm pitch, 8.51mm socket length, double cols (from Kicad 4.0.7), script generated
Through hole angled socket strip THT 2x04 2.54mm double row
0
8
8
Connector_PinSocket_2.54mm
PinSocket_2x04_P2.54mm_Vertical
Through hole straight socket strip, 2x04, 2.54mm pitch, double cols (from Kicad 4.0.7), script generated
Through hole socket strip THT 2x04 2.54mm double row
0
8
8
Connector_PinSocket_2.54mm
PinSocket_2x04_P2.54mm_Vertical_SMD
surface-mounted straight socket strip, 2x04, 2.54mm pitch, double cols (from Kicad 4.0.7), script generated
Surface mounted socket strip SMD 2x04 2.54mm double row
0
8
8
Connector_PinSocket_2.54mm
PinSocket_2x05_P2.54mm_Horizontal
Through hole angled socket strip, 2x05, 2.54mm pitch, 8.51mm socket length, double cols (from Kicad 4.0.7), script generated
Through hole angled socket strip THT 2x05 2.54mm double row
0
10
10
Connector_PinSocket_2.54mm
PinSocket_2x05_P2.54mm_Vertical
Through hole straight socket strip, 2x05, 2.54mm pitch, double cols (from Kicad 4.0.7), script generated
Through hole socket strip THT 2x05 2.54mm double row
0
10
10
Connector_PinSocket_2.54mm
PinSocket_2x05_P2.54mm_Vertical_SMD
surface-mounted straight socket strip, 2x05, 2.54mm pitch, double cols (from Kicad 4.0.7), script generated
Surface mounted socket strip SMD 2x05 2.54mm double row
0
10
10
Connector_PinSocket_2.54mm
PinSocket_2x06_P2.54mm_Horizontal
Through hole angled socket strip, 2x06, 2.54mm pitch, 8.51mm socket length, double cols (from Kicad 4.0.7), script generated
Through hole angled socket strip THT 2x06 2.54mm double row
0
12
12
Connector_PinSocket_2.54mm
PinSocket_2x06_P2.54mm_Vertical
Through hole straight socket strip, 2x06, 2.54mm pitch, double cols (from Kicad 4.0.7), script generated
Through hole socket strip THT 2x06 2.54mm double row
0
12
12
Connector_PinSocket_2.54mm
PinSocket_2x06_P2.54mm_Vertical_SMD
surface-mounted straight socket strip, 2x06, 2.54mm pitch, double cols (from Kicad 4.0.7), script generated
Surface mounted socket strip SMD 2x06 2.54mm double row
0
12
12
Connector_PinSocket_2.54mm
PinSocket_2x07_P2.54mm_Horizontal
Through hole angled socket strip, 2x07, 2.54mm pitch, 8.51mm socket length, double cols (from Kicad 4.0.7), script generated
Through hole angled socket strip THT 2x07 2.54mm double row
0
14
14
Connector_PinSocket_2.54mm
PinSocket_2x07_P2.54mm_Vertical
Through hole straight socket strip, 2x07, 2.54mm pitch, double cols (from Kicad 4.0.7), script generated
Through hole socket strip THT 2x07 2.54mm double row
0
14
14
Connector_PinSocket_2.54mm
PinSocket_2x07_P2.54mm_Vertical_SMD
surface-mounted straight socket strip, 2x07, 2.54mm pitch, double cols (from Kicad 4.0.7), script generated
Surface mounted socket strip SMD 2x07 2.54mm double row
0
14
14
Connector_PinSocket_2.54mm
PinSocket_2x08_P2.54mm_Horizontal
Through hole angled socket strip, 2x08, 2.54mm pitch, 8.51mm socket length, double cols (from Kicad 4.0.7), script generated
Through hole angled socket strip THT 2x08 2.54mm double row
0
16
16
Connector_PinSocket_2.54mm
PinSocket_2x08_P2.54mm_Vertical
Through hole straight socket strip, 2x08, 2.54mm pitch, double cols (from Kicad 4.0.7), script generated
Through hole socket strip THT 2x08 2.54mm double row
0
16
16
Connector_PinSocket_2.54mm
PinSocket_2x08_P2.54mm_Vertical_SMD
surface-mounted straight socket strip, 2x08, 2.54mm pitch, double cols (from Kicad 4.0.7), script generated
Surface mounted socket strip SMD 2x08 2.54mm double row
0
16
16
Connector_PinSocket_2.54mm
PinSocket_2x09_P2.54mm_Horizontal
Through hole angled socket strip, 2x09, 2.54mm pitch, 8.51mm socket length, double cols (from Kicad 4.0.7), script generated
Through hole angled socket strip THT 2x09 2.54mm double row
0
18
18
Connector_PinSocket_2.54mm
PinSocket_2x09_P2.54mm_Vertical
Through hole straight socket strip, 2x09, 2.54mm pitch, double cols (from Kicad 4.0.7), script generated
Through hole socket strip THT 2x09 2.54mm double row
0
18
18
Connector_PinSocket_2.54mm
PinSocket_2x09_P2.54mm_Vertical_SMD
surface-mounted straight socket strip, 2x09, 2.54mm pitch, double cols (from Kicad 4.0.7), script generated
Surface mounted socket strip SMD 2x09 2.54mm double row
0
18
18
Connector_PinSocket_2.54mm
PinSocket_2x10_P2.54mm_Horizontal
Through hole angled socket strip, 2x10, 2.54mm pitch, 8.51mm socket length, double cols (from Kicad 4.0.7), script generated
Through hole angled socket strip THT 2x10 2.54mm double row
0
20
20
Connector_PinSocket_2.54mm
PinSocket_2x10_P2.54mm_Vertical
Through hole straight socket strip, 2x10, 2.54mm pitch, double cols (from Kicad 4.0.7), script generated
Through hole socket strip THT 2x10 2.54mm double row
0
20
20
Connector_PinSocket_2.54mm
PinSocket_2x10_P2.54mm_Vertical_SMD
surface-mounted straight socket strip, 2x10, 2.54mm pitch, double cols (from Kicad 4.0.7), script generated
Surface mounted socket strip SMD 2x10 2.54mm double row
0
20
20
Connector_PinSocket_2.54mm
PinSocket_2x11_P2.54mm_Horizontal
Through hole angled socket strip, 2x11, 2.54mm pitch, 8.51mm socket length, double cols (from Kicad 4.0.7), script generated
Through hole angled socket strip THT 2x11 2.54mm double row
0
22
22
Connector_PinSocket_2.54mm
PinSocket_2x11_P2.54mm_Vertical
Through hole straight socket strip, 2x11, 2.54mm pitch, double cols (from Kicad 4.0.7), script generated
Through hole socket strip THT 2x11 2.54mm double row
0
22
22
Connector_PinSocket_2.54mm
PinSocket_2x11_P2.54mm_Vertical_SMD
surface-mounted straight socket strip, 2x11, 2.54mm pitch, double cols (from Kicad 4.0.7), script generated
Surface mounted socket strip SMD 2x11 2.54mm double row
0
22
22
Connector_PinSocket_2.54mm
PinSocket_2x12_P2.54mm_Horizontal
Through hole angled socket strip, 2x12, 2.54mm pitch, 8.51mm socket length, double cols (from Kicad 4.0.7), script generated
Through hole angled socket strip THT 2x12 2.54mm double row
0
24
24
Connector_PinSocket_2.54mm
PinSocket_2x12_P2.54mm_Vertical
Through hole straight socket strip, 2x12, 2.54mm pitch, double cols (from Kicad 4.0.7), script generated
Through hole socket strip THT 2x12 2.54mm double row
0
24
24
Connector_PinSocket_2.54mm
PinSocket_2x12_P2.54mm_Vertical_SMD
surface-mounted straight socket strip, 2x12, 2.54mm pitch, double cols (from Kicad 4.0.7), script generated
Surface mounted socket strip SMD 2x12 2.54mm double row
0
24
24
Connector_PinSocket_2.54mm
PinSocket_2x13_P2.54mm_Horizontal
Through hole angled socket strip, 2x13, 2.54mm pitch, 8.51mm socket length, double cols (from Kicad 4.0.7), script generated
Through hole angled socket strip THT 2x13 2.54mm double row
0
26
26
Connector_PinSocket_2.54mm
PinSocket_2x13_P2.54mm_Vertical
Through hole straight socket strip, 2x13, 2.54mm pitch, double cols (from Kicad 4.0.7), script generated
Through hole socket strip THT 2x13 2.54mm double row
0
26
26
Connector_PinSocket_2.54mm
PinSocket_2x13_P2.54mm_Vertical_SMD
surface-mounted straight socket strip, 2x13, 2.54mm pitch, double cols (from Kicad 4.0.7), script generated
Surface mounted socket strip SMD 2x13 2.54mm double row
0
26
26
Connector_PinSocket_2.54mm
PinSocket_2x14_P2.54mm_Horizontal
Through hole angled socket strip, 2x14, 2.54mm pitch, 8.51mm socket length, double cols (from Kicad 4.0.7), script generated
Through hole angled socket strip THT 2x14 2.54mm double row
0
28
28
Connector_PinSocket_2.54mm
PinSocket_2x14_P2.54mm_Vertical
Through hole straight socket strip, 2x14, 2.54mm pitch, double cols (from Kicad 4.0.7), script generated
Through hole socket strip THT 2x14 2.54mm double row
0
28
28
Connector_PinSocket_2.54mm
PinSocket_2x14_P2.54mm_Vertical_SMD
surface-mounted straight socket strip, 2x14, 2.54mm pitch, double cols (from Kicad 4.0.7), script generated
Surface mounted socket strip SMD 2x14 2.54mm double row
0
28
28
Connector_PinSocket_2.54mm
PinSocket_2x15_P2.54mm_Horizontal
Through hole angled socket strip, 2x15, 2.54mm pitch, 8.51mm socket length, double cols (from Kicad 4.0.7), script generated
Through hole angled socket strip THT 2x15 2.54mm double row
0
30
30
Connector_PinSocket_2.54mm
PinSocket_2x15_P2.54mm_Vertical
Through hole straight socket strip, 2x15, 2.54mm pitch, double cols (from Kicad 4.0.7), script generated
Through hole socket strip THT 2x15 2.54mm double row
0
30
30
Connector_PinSocket_2.54mm
PinSocket_2x15_P2.54mm_Vertical_SMD
surface-mounted straight socket strip, 2x15, 2.54mm pitch, double cols (from Kicad 4.0.7), script generated
Surface mounted socket strip SMD 2x15 2.54mm double row
0
30
30
Connector_PinSocket_2.54mm
PinSocket_2x16_P2.54mm_Horizontal
Through hole angled socket strip, 2x16, 2.54mm pitch, 8.51mm socket length, double cols (from Kicad 4.0.7), script generated
Through hole angled socket strip THT 2x16 2.54mm double row
0
32
32
Connector_PinSocket_2.54mm
PinSocket_2x16_P2.54mm_Vertical
Through hole straight socket strip, 2x16, 2.54mm pitch, double cols (from Kicad 4.0.7), script generated
Through hole socket strip THT 2x16 2.54mm double row
0
32
32
Connector_PinSocket_2.54mm
PinSocket_2x16_P2.54mm_Vertical_SMD
surface-mounted straight socket strip, 2x16, 2.54mm pitch, double cols (from Kicad 4.0.7), script generated
Surface mounted socket strip SMD 2x16 2.54mm double row
0
32
32
Connector_PinSocket_2.54mm
PinSocket_2x17_P2.54mm_Horizontal
Through hole angled socket strip, 2x17, 2.54mm pitch, 8.51mm socket length, double cols (from Kicad 4.0.7), script generated
Through hole angled socket strip THT 2x17 2.54mm double row
0
34
34
Connector_PinSocket_2.54mm
PinSocket_2x17_P2.54mm_Vertical
Through hole straight socket strip, 2x17, 2.54mm pitch, double cols (from Kicad 4.0.7), script generated
Through hole socket strip THT 2x17 2.54mm double row
0
34
34
Connector_PinSocket_2.54mm
PinSocket_2x17_P2.54mm_Vertical_SMD
surface-mounted straight socket strip, 2x17, 2.54mm pitch, double cols (from Kicad 4.0.7), script generated
Surface mounted socket strip SMD 2x17 2.54mm double row
0
34
34
Connector_PinSocket_2.54mm
PinSocket_2x18_P2.54mm_Horizontal
Through hole angled socket strip, 2x18, 2.54mm pitch, 8.51mm socket length, double cols (from Kicad 4.0.7), script generated
Through hole angled socket strip THT 2x18 2.54mm double row
0
36
36
Connector_PinSocket_2.54mm
PinSocket_2x18_P2.54mm_Vertical
Through hole straight socket strip, 2x18, 2.54mm pitch, double cols (from Kicad 4.0.7), script generated
Through hole socket strip THT 2x18 2.54mm double row
0
36
36
Connector_PinSocket_2.54mm
PinSocket_2x18_P2.54mm_Vertical_SMD
surface-mounted straight socket strip, 2x18, 2.54mm pitch, double cols (from Kicad 4.0.7), script generated
Surface mounted socket strip SMD 2x18 2.54mm double row
0
36
36
Connector_PinSocket_2.54mm
PinSocket_2x19_P2.54mm_Horizontal
Through hole angled socket strip, 2x19, 2.54mm pitch, 8.51mm socket length, double cols (from Kicad 4.0.7), script generated
Through hole angled socket strip THT 2x19 2.54mm double row
0
38
38
Connector_PinSocket_2.54mm
PinSocket_2x19_P2.54mm_Vertical
Through hole straight socket strip, 2x19, 2.54mm pitch, double cols (from Kicad 4.0.7), script generated
Through hole socket strip THT 2x19 2.54mm double row
0
38
38
Connector_PinSocket_2.54mm
PinSocket_2x19_P2.54mm_Vertical_SMD
surface-mounted straight socket strip, 2x19, 2.54mm pitch, double cols (from Kicad 4.0.7), script generated
Surface mounted socket strip SMD 2x19 2.54mm double row
0
38
38
Connector_PinSocket_2.54mm
PinSocket_2x20_P2.54mm_Horizontal
Through hole angled socket strip, 2x20, 2.54mm pitch, 8.51mm socket length, double cols (from Kicad 4.0.7), script generated
Through hole angled socket strip THT 2x20 2.54mm double row
0
40
40
Connector_PinSocket_2.54mm
PinSocket_2x20_P2.54mm_Vertical
Through hole straight socket strip, 2x20, 2.54mm pitch, double cols (from Kicad 4.0.7), script generated
Through hole socket strip THT 2x20 2.54mm double row
0
40
40
Connector_PinSocket_2.54mm
PinSocket_2x20_P2.54mm_Vertical_SMD
surface-mounted straight socket strip, 2x20, 2.54mm pitch, double cols (from Kicad 4.0.7), script generated
Surface mounted socket strip SMD 2x20 2.54mm double row
0
40
40
Connector_PinSocket_2.54mm
PinSocket_2x21_P2.54mm_Horizontal
Through hole angled socket strip, 2x21, 2.54mm pitch, 8.51mm socket length, double cols (from Kicad 4.0.7), script generated
Through hole angled socket strip THT 2x21 2.54mm double row
0
42
42
Connector_PinSocket_2.54mm
PinSocket_2x21_P2.54mm_Vertical
Through hole straight socket strip, 2x21, 2.54mm pitch, double cols (from Kicad 4.0.7), script generated
Through hole socket strip THT 2x21 2.54mm double row
0
42
42
Connector_PinSocket_2.54mm
PinSocket_2x21_P2.54mm_Vertical_SMD
surface-mounted straight socket strip, 2x21, 2.54mm pitch, double cols (from Kicad 4.0.7), script generated
Surface mounted socket strip SMD 2x21 2.54mm double row
0
42
42
Connector_PinSocket_2.54mm
PinSocket_2x22_P2.54mm_Horizontal
Through hole angled socket strip, 2x22, 2.54mm pitch, 8.51mm socket length, double cols (from Kicad 4.0.7), script generated
Through hole angled socket strip THT 2x22 2.54mm double row
0
44
44
Connector_PinSocket_2.54mm
PinSocket_2x22_P2.54mm_Vertical
Through hole straight socket strip, 2x22, 2.54mm pitch, double cols (from Kicad 4.0.7), script generated
Through hole socket strip THT 2x22 2.54mm double row
0
44
44
Connector_PinSocket_2.54mm
PinSocket_2x22_P2.54mm_Vertical_SMD
surface-mounted straight socket strip, 2x22, 2.54mm pitch, double cols (from Kicad 4.0.7), script generated
Surface mounted socket strip SMD 2x22 2.54mm double row
0
44
44
Connector_PinSocket_2.54mm
PinSocket_2x23_P2.54mm_Horizontal
Through hole angled socket strip, 2x23, 2.54mm pitch, 8.51mm socket length, double cols (from Kicad 4.0.7), script generated
Through hole angled socket strip THT 2x23 2.54mm double row
0
46
46
Connector_PinSocket_2.54mm
PinSocket_2x23_P2.54mm_Vertical
Through hole straight socket strip, 2x23, 2.54mm pitch, double cols (from Kicad 4.0.7), script generated
Through hole socket strip THT 2x23 2.54mm double row
0
46
46
Connector_PinSocket_2.54mm
PinSocket_2x23_P2.54mm_Vertical_SMD
surface-mounted straight socket strip, 2x23, 2.54mm pitch, double cols (from Kicad 4.0.7), script generated
Surface mounted socket strip SMD 2x23 2.54mm double row
0
46
46
Connector_PinSocket_2.54mm
PinSocket_2x24_P2.54mm_Horizontal
Through hole angled socket strip, 2x24, 2.54mm pitch, 8.51mm socket length, double cols (from Kicad 4.0.7), script generated
Through hole angled socket strip THT 2x24 2.54mm double row
0
48
48
Connector_PinSocket_2.54mm
PinSocket_2x24_P2.54mm_Vertical
Through hole straight socket strip, 2x24, 2.54mm pitch, double cols (from Kicad 4.0.7), script generated
Through hole socket strip THT 2x24 2.54mm double row
0
48
48
Connector_PinSocket_2.54mm
PinSocket_2x24_P2.54mm_Vertical_SMD
surface-mounted straight socket strip, 2x24, 2.54mm pitch, double cols (from Kicad 4.0.7), script generated
Surface mounted socket strip SMD 2x24 2.54mm double row
0
48
48
Connector_PinSocket_2.54mm
PinSocket_2x25_P2.54mm_Horizontal
Through hole angled socket strip, 2x25, 2.54mm pitch, 8.51mm socket length, double cols (from Kicad 4.0.7), script generated
Through hole angled socket strip THT 2x25 2.54mm double row
0
50
50
Connector_PinSocket_2.54mm
PinSocket_2x25_P2.54mm_Vertical
Through hole straight socket strip, 2x25, 2.54mm pitch, double cols (from Kicad 4.0.7), script generated
Through hole socket strip THT 2x25 2.54mm double row
0
50
50
Connector_PinSocket_2.54mm
PinSocket_2x25_P2.54mm_Vertical_SMD
surface-mounted straight socket strip, 2x25, 2.54mm pitch, double cols (from Kicad 4.0.7), script generated
Surface mounted socket strip SMD 2x25 2.54mm double row
0
50
50
Connector_PinSocket_2.54mm
PinSocket_2x26_P2.54mm_Horizontal
Through hole angled socket strip, 2x26, 2.54mm pitch, 8.51mm socket length, double cols (from Kicad 4.0.7), script generated
Through hole angled socket strip THT 2x26 2.54mm double row
0
52
52
Connector_PinSocket_2.54mm
PinSocket_2x26_P2.54mm_Vertical
Through hole straight socket strip, 2x26, 2.54mm pitch, double cols (from Kicad 4.0.7), script generated
Through hole socket strip THT 2x26 2.54mm double row
0
52
52
Connector_PinSocket_2.54mm
PinSocket_2x26_P2.54mm_Vertical_SMD
surface-mounted straight socket strip, 2x26, 2.54mm pitch, double cols (from Kicad 4.0.7), script generated
Surface mounted socket strip SMD 2x26 2.54mm double row
0
52
52
Connector_PinSocket_2.54mm
PinSocket_2x27_P2.54mm_Horizontal
Through hole angled socket strip, 2x27, 2.54mm pitch, 8.51mm socket length, double cols (from Kicad 4.0.7), script generated
Through hole angled socket strip THT 2x27 2.54mm double row
0
54
54
Connector_PinSocket_2.54mm
PinSocket_2x27_P2.54mm_Vertical
Through hole straight socket strip, 2x27, 2.54mm pitch, double cols (from Kicad 4.0.7), script generated
Through hole socket strip THT 2x27 2.54mm double row
0
54
54
Connector_PinSocket_2.54mm
PinSocket_2x27_P2.54mm_Vertical_SMD
surface-mounted straight socket strip, 2x27, 2.54mm pitch, double cols (from Kicad 4.0.7), script generated
Surface mounted socket strip SMD 2x27 2.54mm double row
0
54
54
Connector_PinSocket_2.54mm
PinSocket_2x28_P2.54mm_Horizontal
Through hole angled socket strip, 2x28, 2.54mm pitch, 8.51mm socket length, double cols (from Kicad 4.0.7), script generated
Through hole angled socket strip THT 2x28 2.54mm double row
0
56
56
Connector_PinSocket_2.54mm
PinSocket_2x28_P2.54mm_Vertical
Through hole straight socket strip, 2x28, 2.54mm pitch, double cols (from Kicad 4.0.7), script generated
Through hole socket strip THT 2x28 2.54mm double row
0
56
56
Connector_PinSocket_2.54mm
PinSocket_2x28_P2.54mm_Vertical_SMD
surface-mounted straight socket strip, 2x28, 2.54mm pitch, double cols (from Kicad 4.0.7), script generated
Surface mounted socket strip SMD 2x28 2.54mm double row
0
56
56
Connector_PinSocket_2.54mm
PinSocket_2x29_P2.54mm_Horizontal
Through hole angled socket strip, 2x29, 2.54mm pitch, 8.51mm socket length, double cols (from Kicad 4.0.7), script generated
Through hole angled socket strip THT 2x29 2.54mm double row
0
58
58
Connector_PinSocket_2.54mm
PinSocket_2x29_P2.54mm_Vertical
Through hole straight socket strip, 2x29, 2.54mm pitch, double cols (from Kicad 4.0.7), script generated
Through hole socket strip THT 2x29 2.54mm double row
0
58
58
Connector_PinSocket_2.54mm
PinSocket_2x29_P2.54mm_Vertical_SMD
surface-mounted straight socket strip, 2x29, 2.54mm pitch, double cols (from Kicad 4.0.7), script generated
Surface mounted socket strip SMD 2x29 2.54mm double row
0
58
58
Connector_PinSocket_2.54mm
PinSocket_2x30_P2.54mm_Horizontal
Through hole angled socket strip, 2x30, 2.54mm pitch, 8.51mm socket length, double cols (from Kicad 4.0.7), script generated
Through hole angled socket strip THT 2x30 2.54mm double row
0
60
60
Connector_PinSocket_2.54mm
PinSocket_2x30_P2.54mm_Vertical
Through hole straight socket strip, 2x30, 2.54mm pitch, double cols (from Kicad 4.0.7), script generated
Through hole socket strip THT 2x30 2.54mm double row
0
60
60
Connector_PinSocket_2.54mm
PinSocket_2x30_P2.54mm_Vertical_SMD
surface-mounted straight socket strip, 2x30, 2.54mm pitch, double cols (from Kicad 4.0.7), script generated
Surface mounted socket strip SMD 2x30 2.54mm double row
0
60
60
Connector_PinSocket_2.54mm
PinSocket_2x31_P2.54mm_Horizontal
Through hole angled socket strip, 2x31, 2.54mm pitch, 8.51mm socket length, double cols (from Kicad 4.0.7), script generated
Through hole angled socket strip THT 2x31 2.54mm double row
0
62
62
Connector_PinSocket_2.54mm
PinSocket_2x31_P2.54mm_Vertical
Through hole straight socket strip, 2x31, 2.54mm pitch, double cols (from Kicad 4.0.7), script generated
Through hole socket strip THT 2x31 2.54mm double row
0
62
62
Connector_PinSocket_2.54mm
PinSocket_2x31_P2.54mm_Vertical_SMD
surface-mounted straight socket strip, 2x31, 2.54mm pitch, double cols (from Kicad 4.0.7), script generated
Surface mounted socket strip SMD 2x31 2.54mm double row
0
62
62
Connector_PinSocket_2.54mm
PinSocket_2x32_P2.54mm_Horizontal
Through hole angled socket strip, 2x32, 2.54mm pitch, 8.51mm socket length, double cols (from Kicad 4.0.7), script generated
Through hole angled socket strip THT 2x32 2.54mm double row
0
64
64
Connector_PinSocket_2.54mm
PinSocket_2x32_P2.54mm_Vertical
Through hole straight socket strip, 2x32, 2.54mm pitch, double cols (from Kicad 4.0.7), script generated
Through hole socket strip THT 2x32 2.54mm double row
0
64
64
Connector_PinSocket_2.54mm
PinSocket_2x32_P2.54mm_Vertical_SMD
surface-mounted straight socket strip, 2x32, 2.54mm pitch, double cols (from Kicad 4.0.7), script generated
Surface mounted socket strip SMD 2x32 2.54mm double row
0
64
64
Connector_PinSocket_2.54mm
PinSocket_2x33_P2.54mm_Horizontal
Through hole angled socket strip, 2x33, 2.54mm pitch, 8.51mm socket length, double cols (from Kicad 4.0.7), script generated
Through hole angled socket strip THT 2x33 2.54mm double row
0
66
66
Connector_PinSocket_2.54mm
PinSocket_2x33_P2.54mm_Vertical
Through hole straight socket strip, 2x33, 2.54mm pitch, double cols (from Kicad 4.0.7), script generated
Through hole socket strip THT 2x33 2.54mm double row
0
66
66
Connector_PinSocket_2.54mm
PinSocket_2x33_P2.54mm_Vertical_SMD
surface-mounted straight socket strip, 2x33, 2.54mm pitch, double cols (from Kicad 4.0.7), script generated
Surface mounted socket strip SMD 2x33 2.54mm double row
0
66
66
Connector_PinSocket_2.54mm
PinSocket_2x34_P2.54mm_Horizontal
Through hole angled socket strip, 2x34, 2.54mm pitch, 8.51mm socket length, double cols (from Kicad 4.0.7), script generated
Through hole angled socket strip THT 2x34 2.54mm double row
0
68
68
Connector_PinSocket_2.54mm
PinSocket_2x34_P2.54mm_Vertical
Through hole straight socket strip, 2x34, 2.54mm pitch, double cols (from Kicad 4.0.7), script generated
Through hole socket strip THT 2x34 2.54mm double row
0
68
68
Connector_PinSocket_2.54mm
PinSocket_2x34_P2.54mm_Vertical_SMD
surface-mounted straight socket strip, 2x34, 2.54mm pitch, double cols (from Kicad 4.0.7), script generated
Surface mounted socket strip SMD 2x34 2.54mm double row
0
68
68
Connector_PinSocket_2.54mm
PinSocket_2x35_P2.54mm_Horizontal
Through hole angled socket strip, 2x35, 2.54mm pitch, 8.51mm socket length, double cols (from Kicad 4.0.7), script generated
Through hole angled socket strip THT 2x35 2.54mm double row
0
70
70
Connector_PinSocket_2.54mm
PinSocket_2x35_P2.54mm_Vertical
Through hole straight socket strip, 2x35, 2.54mm pitch, double cols (from Kicad 4.0.7), script generated
Through hole socket strip THT 2x35 2.54mm double row
0
70
70
Connector_PinSocket_2.54mm
PinSocket_2x35_P2.54mm_Vertical_SMD
surface-mounted straight socket strip, 2x35, 2.54mm pitch, double cols (from Kicad 4.0.7), script generated
Surface mounted socket strip SMD 2x35 2.54mm double row
0
70
70
Connector_PinSocket_2.54mm
PinSocket_2x36_P2.54mm_Horizontal
Through hole angled socket strip, 2x36, 2.54mm pitch, 8.51mm socket length, double cols (from Kicad 4.0.7), script generated
Through hole angled socket strip THT 2x36 2.54mm double row
0
72
72
Connector_PinSocket_2.54mm
PinSocket_2x36_P2.54mm_Vertical
Through hole straight socket strip, 2x36, 2.54mm pitch, double cols (from Kicad 4.0.7), script generated
Through hole socket strip THT 2x36 2.54mm double row
0
72
72
Connector_PinSocket_2.54mm
PinSocket_2x36_P2.54mm_Vertical_SMD
surface-mounted straight socket strip, 2x36, 2.54mm pitch, double cols (from Kicad 4.0.7), script generated
Surface mounted socket strip SMD 2x36 2.54mm double row
0
72
72
Connector_PinSocket_2.54mm
PinSocket_2x37_P2.54mm_Horizontal
Through hole angled socket strip, 2x37, 2.54mm pitch, 8.51mm socket length, double cols (from Kicad 4.0.7), script generated
Through hole angled socket strip THT 2x37 2.54mm double row
0
74
74
Connector_PinSocket_2.54mm
PinSocket_2x37_P2.54mm_Vertical
Through hole straight socket strip, 2x37, 2.54mm pitch, double cols (from Kicad 4.0.7), script generated
Through hole socket strip THT 2x37 2.54mm double row
0
74
74
Connector_PinSocket_2.54mm
PinSocket_2x37_P2.54mm_Vertical_SMD
surface-mounted straight socket strip, 2x37, 2.54mm pitch, double cols (from Kicad 4.0.7), script generated
Surface mounted socket strip SMD 2x37 2.54mm double row
0
74
74
Connector_PinSocket_2.54mm
PinSocket_2x38_P2.54mm_Horizontal
Through hole angled socket strip, 2x38, 2.54mm pitch, 8.51mm socket length, double cols (from Kicad 4.0.7), script generated
Through hole angled socket strip THT 2x38 2.54mm double row
0
76
76
Connector_PinSocket_2.54mm
PinSocket_2x38_P2.54mm_Vertical
Through hole straight socket strip, 2x38, 2.54mm pitch, double cols (from Kicad 4.0.7), script generated
Through hole socket strip THT 2x38 2.54mm double row
0
76
76
Connector_PinSocket_2.54mm
PinSocket_2x38_P2.54mm_Vertical_SMD
surface-mounted straight socket strip, 2x38, 2.54mm pitch, double cols (from Kicad 4.0.7), script generated
Surface mounted socket strip SMD 2x38 2.54mm double row
0
76
76
Connector_PinSocket_2.54mm
PinSocket_2x39_P2.54mm_Horizontal
Through hole angled socket strip, 2x39, 2.54mm pitch, 8.51mm socket length, double cols (from Kicad 4.0.7), script generated
Through hole angled socket strip THT 2x39 2.54mm double row
0
78
78
Connector_PinSocket_2.54mm
PinSocket_2x39_P2.54mm_Vertical
Through hole straight socket strip, 2x39, 2.54mm pitch, double cols (from Kicad 4.0.7), script generated
Through hole socket strip THT 2x39 2.54mm double row
0
78
78
Connector_PinSocket_2.54mm
PinSocket_2x39_P2.54mm_Vertical_SMD
surface-mounted straight socket strip, 2x39, 2.54mm pitch, double cols (from Kicad 4.0.7), script generated
Surface mounted socket strip SMD 2x39 2.54mm double row
0
78
78
Connector_PinSocket_2.54mm
PinSocket_2x40_P2.54mm_Horizontal
Through hole angled socket strip, 2x40, 2.54mm pitch, 8.51mm socket length, double cols (from Kicad 4.0.7), script generated
Through hole angled socket strip THT 2x40 2.54mm double row
0
80
80
Connector_PinSocket_2.54mm
PinSocket_2x40_P2.54mm_Vertical
Through hole straight socket strip, 2x40, 2.54mm pitch, double cols (from Kicad 4.0.7), script generated
Through hole socket strip THT 2x40 2.54mm double row
0
80
80
Connector_PinSocket_2.54mm
PinSocket_2x40_P2.54mm_Vertical_SMD
surface-mounted straight socket strip, 2x40, 2.54mm pitch, double cols (from Kicad 4.0.7), script generated
Surface mounted socket strip SMD 2x40 2.54mm double row
0
80
80
Connectors
Banana_Jack_1Pin
Single banana socket, footprint - 6mm drill
banana socket
0
1
1
Connectors
Banana_Jack_2Pin
Dual banana socket, footprint - 2 x 6mm drills
banana socket
0
2
2
Connectors
Banana_Jack_3Pin
Triple banana socket, footprint - 3 x 6mm drills
banana socket
0
3
3
Connectors
CUI_PD-30
3 pin connector, PD-30, http://www.cui.com/product/resource/pd-30.pdf
connector 3-pin PD-30 power DIN
0
4
4
Connectors
CalTest_CT3151
Right-angle standard banana jack, http://www.caltestelectronics.com/images/attachments/P315100rH_drawing.pdf
banana jack horizontal
0
4
1
Connectors
Connector_SFP_and_Cage
https://www.te.com/commerce/DocumentDelivery/DDEController?Action=srchrtrv&DocNm=2227302&DocType=Customer+Drawing&DocLang=English
SFP+ SFP
0
40
21
Connectors
DTF13-12Px
http://www.te.com/usa-en/product-DTF13-12PA-G003.html
DEUTSCH DT header 12 pin 
0
12
12
Connectors
FanPinHeader_1x03_P2.54mm_Vertical
3-pin CPU fan Through hole pin header, see http://www.formfactors.org/developer%5Cspecs%5Crev1_2_public.pdf
pin header 3-pin CPU fan
0
3
3
Connectors
FanPinHeader_1x04_P2.54mm_Vertical
4-pin CPU fan Through hole pin header, e.g. for Wieson part number 2366C888-007 Molex 47053-1000, Foxconn HF27040-M1, Tyco 1470947-1 or equivalent, see http://www.formfactors.org/developer%5Cspecs%5Crev1_2_public.pdf
pin header 4-pin CPU fan
0
4
4
Connectors
GB042-34S-H10
http://www.lsmtron.com/pdf/Connector&Antenna_catalog.PDF
34pin SMD connector 
0
34
34
Connectors
IHI_B6A-PCB-45_Vertical
https://lugsdirect.com/PDF_Webprint/B6A-PCB-45-XX(-X).pdf
connector IHI B6A-PCB-45
0
49
1
Connectors
JWT_A3963_1x02_P3.96mm_Vertical
JWT A3963, 3.96mm pitch Pin head connector (http://www.jwt.com.tw/pro_pdf/A3963.pdf)
connector JWT A3963 pinhead
0
2
2
Connectors
NS-Tech_Grove_1x04_P2mm_Vertical
https://statics3.seeedstudio.com/images/opl/datasheet/3470130P1.pdf
Grove-1x04
0
4
4
Connectors
Tag-Connect_TC2030-IDC-FP_2x03_P1.27mm_Vertical
Tag-Connect programming header; http://www.tag-connect.com/Materials/TC2030-IDC.pdf
tag connect programming header pogo pins
0
6
6
Connectors
Tag-Connect_TC2030-IDC-NL_2x03_P1.27mm_Vertical
Tag-Connect programming header; http://www.tag-connect.com/Materials/TC2030-IDC-NL.pdf
tag connect programming header pogo pins
0
6
6
Connectors
Tag-Connect_TC2050-IDC-FP_2x05_P1.27mm_Vertical
Tag-Connect programming header; http://www.tag-connect.com/Materials/TC2050-IDC-430%20Datasheet.pdf
tag connect programming header pogo pins
0
10
10
Connectors
Tag-Connect_TC2050-IDC-NL_2x05_P1.27mm_Vertical
Tag-Connect programming header; http://www.tag-connect.com/Materials/TC2050-IDC-NL%20Datasheet.pdf
tag connect programming header pogo pins
0
10
10
Connectors
Tag-Connect_TC2070-IDC-FP_2x07_P1.27mm_Vertical
Tag-Connect programming header; http://www.tag-connect.com/Materials/TC2070-IDC%20Datasheet.pdf
tag connect programming header pogo pins
0
14
14
Connectors_USB
USB3_A_Molex_48393-001
USB 3.0, type A, right angle (http://www.molex.com/pdm_docs/sd/483930003_sd.pdf)
USB 3.0 type A right angle
0
13
10
Connectors_USB
USB3_A_Plug_Wuerth_692112030100_Horizontal
USB type A Plug, Horizontal, http://katalog.we-online.de/em/datasheet/692112030100.pdf
usb A plug horizontal
0
11
10
Connectors_USB
USB_A_CNCTech_1001-011-01101_Horizontal
http://cnctech.us/pdfs/1001-011-01101.pdf
USB-A
0
6
5
Connectors_USB
USB_A_Molex_105057_Vertical
https://www.molex.com/pdm_docs/sd/1050570001_sd.pdf
USB A Vertical
0
7
5
Connectors_USB
USB_A_Stewart_SS-52100-001_Horizontal
USB A connector https://belfuse.com/resources/drawings/stewartconnector/dr-stw-ss-52100-001.pdf
USB_A Female Connector receptacle
0
6
5
Connectors_USB
USB_A_Wuerth_61400826021_Horizontal_Stacked
Stacked USB A connector http://katalog.we-online.de/em/datasheet/61400826021.pdf
Wuerth stacked USB_A
0
12
9
Connectors_USB
USB_B_Amphenol_MUSB-D511_Vertical_Rugged
A,phenol MUSB_D511, USB B female connector, straight, rugged, https://www.amphenolcanada.com/ProductSearch/drawings/AC/MUSBD511XX.pdf
USB_B_MUSB_Straight female connector straight rugged MUSB D511
0
6
5
Connectors_USB
USB_B_OST_USB-B1HSxx_Horizontal
USB B receptacle, Horizontal, through-hole, http://www.on-shore.com/wp-content/uploads/2015/09/usb-b1hsxx.pdf
USB-B receptacle horizontal through-hole
0
6
5
Connectors_USB
USB_B_TE_5787834_Vertical
http://www.mouser.com/ds/2/418/NG_CD_5787834_A4-669110.pdf
USB_B USB B vertical female connector
0
6
5
Connectors_USB
USB_C_Plug_JAE_DX07P024AJ1
Universal Serial Bus (USB) Shielded I/O Plug, Type C, Right Angle, Surface Mount, https://www.jae.com/en/searchfilter/?topics_keyword=DX07P024AJ1&mainItemSelect=1
USB Type-C Plug Edge Mount
0
30
25
Connectors_USB
USB_C_Plug_Molex_105444
Universal Serial Bus (USB) Shielded I/O Plug, Type C, Right Angle, Surface Mount, http://www.molex.com/pdm_docs/sd/1054440001_sd.pdf
USB Type-C Plug Edge Mount
0
24
23
Connectors_USB
USB_C_Receptacle_Amphenol_12401548E4-2A
USB TYPE C, RA RCPT PCB, Hybrid, https://www.amphenolcanada.com/StockAvailabilityPrice.aspx?From=&PartNum=12401548E4%7e2A
USB C Type-C Receptacle Hybrid
0
28
25
Connectors_USB
USB_C_Receptacle_Amphenol_12401548E4-2A_CircularHoles
USB TYPE C, RA RCPT PCB, Hybrid, https://www.amphenolcanada.com/StockAvailabilityPrice.aspx?From=&PartNum=12401548E4%7e2A
USB C Type-C Receptacle Hybrid
0
28
25
Connectors_USB
USB_C_Receptacle_Amphenol_12401610E4-2A
USB TYPE C, RA RCPT PCB, SMT, https://www.amphenolcanada.com/StockAvailabilityPrice.aspx?From=&PartNum=12401610E4%7e2A
USB C Type-C Receptacle SMD
0
28
25
Connectors_USB
USB_C_Receptacle_Amphenol_12401610E4-2A_CircularHoles
USB TYPE C, RA RCPT PCB, SMT, https://www.amphenolcanada.com/StockAvailabilityPrice.aspx?From=&PartNum=12401610E4%7e2A
USB C Type-C Receptacle SMD
0
28
25
Connectors_USB
USB_C_Receptacle_GCT_USB4085
USB 2.0 Type C Receptacle, https://gct.co/Files/Drawings/USB4085.pdf
USB Type-C Receptacle Through-hole Right angle
0
20
17
Connectors_USB
USB_C_Receptacle_HRO_TYPE-C-31-M-12
USB Type-C receptacle for USB 2.0 and PD, http://www.krhro.com/uploads/soft/180320/1-1P320120243.pdf
usb usb-c 2.0 pd
0
20
17
Connectors_USB
USB_C_Receptacle_JAE_DX07S024WJ1R350
http://www.jae.com/z-en/pdf_download_exec.cfm?param=SJ117219.pdf
USB C Type-C Receptacle SMD
0
30
25
Connectors_USB
USB_C_Receptacle_JAE_DX07S024WJ3R400
USB TYPE C, VERT RCPT PCB, SMT, http://www.jae.com/z-en/pdf_download_exec.cfm?param=SJ117928.pdf
USB C Type-C Receptacle SMD
0
28
25
Connectors_USB
USB_C_Receptacle_Palconn_UTC16-G
http://www.palpilot.com/wp-content/uploads/2017/05/UTC027-GKN-OR-Rev-A.pdf
USB C Type-C Receptacle USB2.0
0
20
17
Connectors_USB
USB_C_Receptacle_XKB_U262-16XN-4BVC11
USB Type C, right-angle, SMT, https://datasheet.lcsc.com/szlcsc/1811141824_XKB-Enterprise-U262-161N-4BVC11_C319148.pdf
USB C Type-C Receptacle SMD
0
20
17
Connectors_USB
USB_Micro-AB_Molex_47590-0001
Micro USB AB receptable, right-angle inverted (https://www.molex.com/pdm_docs/sd/475900001_sd.pdf)
Micro AB USB SMD
0
14
6
Connectors_USB
USB_Micro-B_Amphenol_10103594-0001LF_Horizontal
Micro USB Type B 10103594-0001LF, http://cdn.amphenol-icc.com/media/wysiwyg/files/drawing/10103594.pdf
USB USB_B USB_micro USB_OTG
0
17
6
Connectors_USB
USB_Micro-B_GCT_USB3076-30-A
GCT Micro USB https://gct.co/files/drawings/usb3076.pdf
Micro-USB SMD Typ-B GCT
0
11
6
Connectors_USB
USB_Micro-B_Molex-105017-0001
http://www.molex.com/pdm_docs/sd/1050170001_sd.pdf
Micro-USB SMD Typ-B
0
13
6
Connectors_USB
USB_Micro-B_Molex-105133-0001
Molex Vertical Micro USB Typ-B (http://www.molex.com/pdm_docs/sd/1051330001_sd.pdf)
Micro-USB SMD Typ-B Vertical
0
8
6
Connectors_USB
USB_Micro-B_Molex-105133-0031
Molex Vertical Micro USB Typ-B (http://www.molex.com/pdm_docs/sd/1051330031_sd.pdf)
Micro-USB SMD Typ-B Vertical
0
8
6
Connectors_USB
USB_Micro-B_Molex_47346-0001
Micro USB B receptable with flange, bottom-mount, SMD, right-angle (http://www.molex.com/pdm_docs/sd/473460001_sd.pdf)
Micro B USB SMD
0
11
6
Connectors_USB
USB_Micro-B_Wuerth_614105150721_Vertical
USB Micro-B receptacle, through-hole, vertical, http://katalog.we-online.de/em/datasheet/614105150721.pdf
usb micro receptacle vertical
0
7
6
Connectors_USB
USB_Micro-B_Wuerth_614105150721_Vertical_CircularHoles
USB Micro-B receptacle, through-hole, vertical, http://katalog.we-online.de/em/datasheet/614105150721.pdf
usb micro receptacle vertical
0
7
6
Connectors_USB
USB_Micro-B_Wuerth_629105150521
USB Micro-B receptacle, http://www.mouser.com/ds/2/445/629105150521-469306.pdf
usb micro receptacle
0
9
6
Connectors_USB
USB_Micro-B_Wuerth_629105150521_CircularHoles
USB Micro-B receptacle, http://www.mouser.com/ds/2/445/629105150521-469306.pdf
usb micro receptacle
0
9
6
Connectors_USB
USB_Mini-B_AdamTech_MUSB-B5-S-VT-TSMT-1_SMD_Vertical
http://www.adam-tech.com/upload/MUSB-B5-S-VT-TSMT-1.pdf
USB Mini-B
0
7
6
Connectors_USB
USB_Mini-B_Lumberg_2486_01_Horizontal
USB Mini-B 5-pin SMD connector, http://downloads.lumberg.com/datenblaetter/en/2486_01.pdf
USB USB_B USB_Mini connector
0
9
6
Connectors_USB
USB_Mini-B_Tensility_54-00023_Vertical
http://www.tensility.com/pdffiles/54-00023.pdf
usb mini receptacle vertical
0
7
6
Connectors_USB
USB_Mini-B_Tensility_54-00023_Vertical_CircularHoles
http://www.tensility.com/pdffiles/54-00023.pdf
usb mini receptacle vertical
0
7
6
Connectors_USB
USB_Mini-B_Wuerth_65100516121_Horizontal
Mini USB 2.0 Type B SMT Horizontal 5 Contacts (https://katalog.we-online.de/em/datasheet/65100516121.pdf)
Mini USB 2.0 Type B
0
9
6
Diode_SMD
D_0201_0603Metric
Diode SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), generated with kicad-footprint-generator
diode
0
4
2
Diode_SMD
D_0402_1005Metric
Diode SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator
diode
0
2
2
Diode_SMD
D_0603_1608Metric
Diode SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator
diode
0
2
2
Diode_SMD
D_0603_1608Metric_Castellated
Diode SMD 0603 (1608 Metric), castellated end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator
diode castellated
0
2
2
Diode_SMD
D_0603_1608Metric_Pad1.05x0.95mm_HandSolder
Diode SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator
diode handsolder
0
2
2
Diode_SMD
D_0805_2012Metric
Diode SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator
diode
0
2
2
Diode_SMD
D_0805_2012Metric_Castellated
Diode SMD 0805 (2012 Metric), castellated end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator
diode castellated
0
2
2
Diode_SMD
D_0805_2012Metric_Pad1.15x1.40mm_HandSolder
Diode SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator
diode handsolder
0
2
2
Diode_SMD
D_01005_0402Metric
Diode SMD 01005 (0402 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.vishay.com/docs/20056/crcw01005e3.pdf), generated with kicad-footprint-generator
diode
0
4
2
Diode_SMD
D_1206_3216Metric
Diode SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator
diode
0
2
2
Diode_SMD
D_1206_3216Metric_Castellated
Diode SMD 1206 (3216 Metric), castellated end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator
diode castellated
0
2
2
Diode_SMD
D_1206_3216Metric_Pad1.42x1.75mm_HandSolder
Diode SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator
diode handsolder
0
2
2
Diode_SMD
D_1210_3225Metric
Diode SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator
diode
0
2
2
Diode_SMD
D_1210_3225Metric_Castellated
Diode SMD 1210 (3225 Metric), castellated end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator
diode castellated
0
2
2
Diode_SMD
D_1210_3225Metric_Pad1.42x2.65mm_HandSolder
Diode SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator
diode handsolder
0
2
2
Diode_SMD
D_1806_4516Metric
Diode SMD 1806 (4516 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://www.modelithics.com/models/Vendor/MuRata/BLM41P.pdf), generated with kicad-footprint-generator
diode
0
2
2
Diode_SMD
D_1806_4516Metric_Castellated
Diode SMD 1806 (4516 Metric), castellated end terminal, IPC_7351 nominal, (Body size source: https://www.modelithics.com/models/Vendor/MuRata/BLM41P.pdf), generated with kicad-footprint-generator
diode castellated
0
2
2
Diode_SMD
D_1806_4516Metric_Pad1.57x1.80mm_HandSolder
Diode SMD 1806 (4516 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://www.modelithics.com/models/Vendor/MuRata/BLM41P.pdf), generated with kicad-footprint-generator
diode handsolder
0
2
2
Diode_SMD
D_1812_4532Metric
Diode SMD 1812 (4532 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://www.nikhef.nl/pub/departments/mt/projects/detectorR_D/dtddice/ERJ2G.pdf), generated with kicad-footprint-generator
diode
0
2
2
Diode_SMD
D_1812_4532Metric_Castellated
Diode SMD 1812 (4532 Metric), castellated end terminal, IPC_7351 nominal, (Body size source: https://www.nikhef.nl/pub/departments/mt/projects/detectorR_D/dtddice/ERJ2G.pdf), generated with kicad-footprint-generator
diode castellated
0
2
2
Diode_SMD
D_1812_4532Metric_Pad1.30x3.40mm_HandSolder
Diode SMD 1812 (4532 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://www.nikhef.nl/pub/departments/mt/projects/detectorR_D/dtddice/ERJ2G.pdf), generated with kicad-footprint-generator
diode handsolder
0
2
2
Diode_SMD
D_2010_5025Metric
Diode SMD 2010 (5025 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator
diode
0
2
2
Diode_SMD
D_2010_5025Metric_Castellated
Diode SMD 2010 (5025 Metric), castellated end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator
diode castellated
0
2
2
Diode_SMD
D_2010_5025Metric_Pad1.52x2.65mm_HandSolder
Diode SMD 2010 (5025 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator
diode handsolder
0
2
2
Diode_SMD
D_2114_3652Metric
Diode SMD 2114 (3652 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size from: http://datasheets.avx.com/schottky.pdf), generated with kicad-footprint-generator
diode
0
2
2
Diode_SMD
D_2114_3652Metric_Castellated
Diode SMD 2114 (3652 Metric), castellated end terminal, IPC_7351 nominal, (Body size from: http://datasheets.avx.com/schottky.pdf), generated with kicad-footprint-generator
diode castellated
0
2
2
Diode_SMD
D_2114_3652Metric_Pad1.85x3.75mm_HandSolder
Diode SMD 2114 (3652 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size from: http://datasheets.avx.com/schottky.pdf), generated with kicad-footprint-generator
diode handsolder
0
2
2
Diode_SMD
D_2512_6332Metric
Diode SMD 2512 (6332 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator
diode
0
2
2
Diode_SMD
D_2512_6332Metric_Castellated
Diode SMD 2512 (6332 Metric), castellated end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator
diode castellated
0
2
2
Diode_SMD
D_2512_6332Metric_Pad1.52x3.35mm_HandSolder
Diode SMD 2512 (6332 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator
diode handsolder
0
2
2
Diode_SMD
D_2816_7142Metric
Diode SMD 2816 (7142 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size from: https://www.vishay.com/docs/30100/wsl.pdf), generated with kicad-footprint-generator
diode
0
2
2
Diode_SMD
D_2816_7142Metric_Castellated
Diode SMD 2816 (7142 Metric), castellated end terminal, IPC_7351 nominal, (Body size from: https://www.vishay.com/docs/30100/wsl.pdf), generated with kicad-footprint-generator
diode castellated
0
2
2
Diode_SMD
D_2816_7142Metric_Pad3.20x4.45mm_HandSolder
Diode SMD 2816 (7142 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size from: https://www.vishay.com/docs/30100/wsl.pdf), generated with kicad-footprint-generator
diode handsolder
0
2
2
Diode_SMD
D_3220_8050Metric
Diode SMD 3220 (8050 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size from: http://datasheets.avx.com/schottky.pdf), generated with kicad-footprint-generator
diode
0
2
2
Diode_SMD
D_3220_8050Metric_Castellated
Diode SMD 3220 (8050 Metric), castellated end terminal, IPC_7351 nominal, (Body size from: http://datasheets.avx.com/schottky.pdf), generated with kicad-footprint-generator
diode castellated
0
2
2
Diode_SMD
D_3220_8050Metric_Pad2.65x5.15mm_HandSolder
Diode SMD 3220 (8050 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size from: http://datasheets.avx.com/schottky.pdf), generated with kicad-footprint-generator
diode handsolder
0
2
2
Diode_SMD
D_MELF
Diode, MELF,,
Diode MELF 
0
2
2
Diode_SMD
D_MELF-RM10_Universal_Handsoldering
Diode, Universal, MELF, RM10, Handsoldering, SMD, Thruhole,
Diode Universal MELF RM10 Handsoldering SMD Thruhole 
0
2
2
Diode_SMD
D_MELF_Handsoldering
Diode MELF Handsoldering
Diode MELF Handsoldering
0
2
2
Diode_SMD
D_MicroMELF
Diode, MicroMELF, Reflow Soldering, http://www.vishay.com/docs/85597/bzm55.pdf
MicroMELF Diode
0
2
2
Diode_SMD
D_MicroMELF_Handsoldering
Diode, MicroMELF, Hand Soldering, http://www.vishay.com/docs/85597/bzm55.pdf
MicroMELF Diode
0
2
2
Diode_SMD
D_MiniMELF
Diode Mini-MELF
Diode Mini-MELF
0
2
2
Diode_SMD
D_MiniMELF_Handsoldering
Diode Mini-MELF Handsoldering
Diode Mini-MELF Handsoldering
0
2
2
Diode_SMD
D_PowerDI-5
PowerDI,Diode,Vishay,https://www.diodes.com/assets/Package-Files/PowerDI5.pdf
PowerDI diode vishay
0
3
2
Diode_SMD
D_PowerDI-123
http://www.diodes.com/_files/datasheets/ds30497.pdf
PowerDI diode vishay
0
2
2
Diode_SMD
D_Powermite2_AK
Microsemi Powermite 2 SMD power package (https://www.microsemi.com/packaging-information/partpackage/details?pid=5341)
PowerMite2
0
2
2
Diode_SMD
D_Powermite2_KA
Microsemi Powermite 2 SMD power package (https://www.microsemi.com/packaging-information/partpackage/details?pid=5341)
PowerMite2
0
2
2
Diode_SMD
D_Powermite3
Microsemi Powermite 3 SMD power package (https://www.microsemi.com/packaging-information/partpackage/details?pid=5340)
PowerMite3
0
3
3
Diode_SMD
D_Powermite_AK
Microsemi Powermite SMD power package (https://www.microsemi.com/packaging-information/partpackage/details?pid=5339, https://www.onsemi.com/pub/Collateral/457-04.PDF)
Powermite
0
2
2
Diode_SMD
D_Powermite_KA
Microsemi Powermite SMD power package (https://www.microsemi.com/packaging-information/partpackage/details?pid=5339, https://www.onsemi.com/pub/Collateral/457-04.PDF)
Powermite
0
2
2
Diode_SMD
D_QFN_3.3x3.3mm_P0.65mm
QFN, diode, 3.3x3.3x1mm (https://www.wolfspeed.com/media/downloads/846/C3D1P7060Q.pdf)
diode qfn 3.3
0
3
2
Diode_SMD
D_SC-80
JEITA SC-80
SC-80
0
2
2
Diode_SMD
D_SC-80_HandSoldering
JEITA SC-80
SC-80
0
2
2
Diode_SMD
D_SMA
Diode SMA (DO-214AC)
Diode SMA (DO-214AC)
0
2
2
Diode_SMD
D_SMA-SMB_Universal_Handsoldering
Diode, Universal, SMA (DO-214AC) or SMB (DO-214AA), Handsoldering,
Diode Universal SMA (DO-214AC) SMB (DO-214AA) Handsoldering 
0
2
2
Diode_SMD
D_SMA_Handsoldering
Diode SMA (DO-214AC) Handsoldering
Diode SMA (DO-214AC) Handsoldering
0
2
2
Diode_SMD
D_SMB
Diode SMB (DO-214AA)
Diode SMB (DO-214AA)
0
2
2
Diode_SMD
D_SMB-SMC_Universal_Handsoldering
Diode, Universal, SMB(DO-214AA) or SMC (DO-214AB), Handsoldering,
Diode Universal SMB(DO-214AA) SMC (DO-214AB) Handsoldering 
0
2
2
Diode_SMD
D_SMB_Handsoldering
Diode SMB (DO-214AA) Handsoldering
Diode SMB (DO-214AA) Handsoldering
0
2
2
Diode_SMD
D_SMB_Modified
Diode SMB (DO-214AA) Modified (http://www.littelfuse.com/~/media/electronics/datasheets/sidactors/littelfuse_sidactor_battrax_positive_negative_modified_do_214_datasheet.pdf.pdf)
Diode SMB (DO-214AA)
0
3
3
Diode_SMD
D_SMC
Diode SMC (DO-214AB)
Diode SMC (DO-214AB)
0
2
2
Diode_SMD
D_SMC-RM10_Universal_Handsoldering
Diode, Universal, SMC (DO-214AB), RM10, Handsoldering, SMD, Thruhole
Diode Universal SMC (DO-214AB) RM10 Handsoldering SMD Thruhole
0
2
2
Diode_SMD
D_SMC_Handsoldering
Diode SMC (DO-214AB) Handsoldering
Diode SMC (DO-214AB) Handsoldering
0
2
2
Diode_SMD
D_SMF
Diode SMF (DO-219AB), http://www.vishay.com/docs/95572/smf_do-219ab.pdf
Diode SMF (DO-214AB)
0
2
2
Diode_SMD
D_SOD-110
SOD-110
SOD-110
0
2
2
Diode_SMD
D_SOD-123
SOD-123
SOD-123
0
2
2
Diode_SMD
D_SOD-123F
D_SOD-123F
D_SOD-123F
0
2
2
Diode_SMD
D_SOD-128
D_SOD-128 (CFP5 SlimSMAW), https://assets.nexperia.com/documents/outline-drawing/SOD128.pdf
D_SOD-128
0
2
2
Diode_SMD
D_SOD-323
SOD-323
SOD-323
0
2
2
Diode_SMD
D_SOD-323F
SOD-323F http://www.nxp.com/documents/outline_drawing/SOD323F.pdf
SOD-323F
0
2
2
Diode_SMD
D_SOD-323_HandSoldering
SOD-323
SOD-323
0
2
2
Diode_SMD
D_SOD-523
http://www.diodes.com/datasheets/ap02001.pdf p.144
Diode SOD523
0
2
2
Diode_SMD
D_SOD-923
https://www.onsemi.com/pub/Collateral/ESD9B-D.PDF#page=4
Diode SOD923
0
2
2
Diode_SMD
D_SOT-23_ANK
SOT-23, Single Diode
SOT-23
0
3
2
Diode_SMD
D_SOT-23_NKA
SOT-23, Single Diode
SOT-23
0
3
2
Diode_SMD
D_TUMD2
ROHM - TUMD2
TUMD2
0
2
2
Diode_SMD
Diode_Bridge_Bourns_CD-DF4xxS
8.1x10.5mm, 4A, single phase bridge rectifier, https://www.bourns.com/docs/Product-Datasheets/CD-DF4xxSL.pdf
Surface Mount Bridge Rectifier Diode
0
4
4
Diode_SMD
Diode_Bridge_Diotec_ABS
SMD diode bridge ABS (Diotec), see https://diotec.com/tl_files/diotec/files/pdf/datasheets/abs2.pdf
ABS MBLS
0
4
4
Diode_SMD
Diode_Bridge_Diotec_MicroDil_3.0x3.0x1.8mm
SMD package Diotec Diotec MicroDil, body 3.0x3.0x1.8mm (e.g. diode bridge), see https://diotec.com/tl_files/diotec/files/pdf/datasheets/mys40.pdf
Diotec MicroDil diode bridge
0
4
4
Diode_SMD
Diode_Bridge_Diotec_SO-DIL-Slim
SMD diode bridge Diotec SO-DIL Slim, see https://diotec.com/tl_files/diotec/files/pdf/datasheets/b40fs.pdf
DFS SO-DIL Slim
0
4
4
Diode_SMD
Diode_Bridge_Vishay_DFS
SMD diode bridge DFS, see http://www.vishay.com/docs/88854/padlayouts.pdf
DFS
0
4
4
Diode_SMD
Diode_Bridge_Vishay_DFSFlat
SMD diode bridge Low Profile DFS "Flat", see http://www.vishay.com/docs/88874/dfl15005.pdf
DFS
0
4
4
Diode_SMD
Diode_Bridge_Vishay_MBLS
SMD diode bridge MBLS, see http://www.vishay.com/docs/89959/mbl104s.pdf http://www.vishay.com/docs/88854/padlayouts.pdf
DFS
0
4
4
Diode_SMD
Littelfuse_PolyZen-LS
http://m.littelfuse.com/~/media/electronics/datasheets/polyzen_devices/littelfuse_polyzen_standard_polyzen_catalog_datasheet.pdf.pdf
Diode Polymer Protected Zener Diode Littelfuse LS
0
3
3
Diode_THT
D_5KPW_P7.62mm_Vertical_AnodeUp
Diode, 5KPW series, Axial, Vertical, pin pitch=7.62mm, , length*diameter=9*8mm^2, , http://www.diodes.com/_files/packages/8686949.gif
Diode 5KPW series Axial Vertical pin pitch 7.62mm  length 9mm diameter 8mm
0
2
2
Diode_THT
D_5KPW_P7.62mm_Vertical_KathodeUp
Diode, 5KPW series, Axial, Vertical, pin pitch=7.62mm, , length*diameter=9*8mm^2, , http://www.diodes.com/_files/packages/8686949.gif
Diode 5KPW series Axial Vertical pin pitch 7.62mm  length 9mm diameter 8mm
0
2
2
Diode_THT
D_5KPW_P12.70mm_Horizontal
Diode, 5KPW series, Axial, Horizontal, pin pitch=12.7mm, , length*diameter=9*8mm^2, , http://www.diodes.com/_files/packages/8686949.gif
Diode 5KPW series Axial Horizontal pin pitch 12.7mm  length 9mm diameter 8mm
0
2
2
Diode_THT
D_5KP_P7.62mm_Vertical_AnodeUp
Diode, 5KP series, Axial, Vertical, pin pitch=7.62mm, , length*diameter=7.62*9.53mm^2, , http://www.diodes.com/_files/packages/8686949.gif
Diode 5KP series Axial Vertical pin pitch 7.62mm  length 7.62mm diameter 9.53mm
0
2
2
Diode_THT
D_5KP_P7.62mm_Vertical_KathodeUp
Diode, 5KP series, Axial, Vertical, pin pitch=7.62mm, , length*diameter=7.62*9.53mm^2, , http://www.diodes.com/_files/packages/8686949.gif
Diode 5KP series Axial Vertical pin pitch 7.62mm  length 7.62mm diameter 9.53mm
0
2
2
Diode_THT
D_5KP_P10.16mm_Horizontal
Diode, 5KP series, Axial, Horizontal, pin pitch=10.16mm, , length*diameter=7.62*9.53mm^2, , http://www.diodes.com/_files/packages/8686949.gif
Diode 5KP series Axial Horizontal pin pitch 10.16mm  length 7.62mm diameter 9.53mm
0
2
2
Diode_THT
D_5KP_P12.70mm_Horizontal
Diode, 5KP series, Axial, Horizontal, pin pitch=12.7mm, , length*diameter=7.62*9.53mm^2, , http://www.diodes.com/_files/packages/8686949.gif
Diode 5KP series Axial Horizontal pin pitch 12.7mm  length 7.62mm diameter 9.53mm
0
2
2
Diode_THT
D_5W_P5.08mm_Vertical_AnodeUp
Diode, 5W series, Axial, Vertical, pin pitch=5.08mm, , length*diameter=8.9*3.7mm^2, , http://www.diodes.com/_files/packages/8686949.gif
Diode 5W series Axial Vertical pin pitch 5.08mm  length 8.9mm diameter 3.7mm
0
2
2
Diode_THT
D_5W_P5.08mm_Vertical_KathodeUp
Diode, 5W series, Axial, Vertical, pin pitch=5.08mm, , length*diameter=8.9*3.7mm^2, , http://www.diodes.com/_files/packages/8686949.gif
Diode 5W series Axial Vertical pin pitch 5.08mm  length 8.9mm diameter 3.7mm
0
2
2
Diode_THT
D_5W_P10.16mm_Horizontal
Diode, 5W series, Axial, Horizontal, pin pitch=10.16mm, , length*diameter=8.9*3.7mm^2, , http://www.diodes.com/_files/packages/8686949.gif
Diode 5W series Axial Horizontal pin pitch 10.16mm  length 8.9mm diameter 3.7mm
0
2
2
Diode_THT
D_5W_P12.70mm_Horizontal
Diode, 5W series, Axial, Horizontal, pin pitch=12.7mm, , length*diameter=8.9*3.7mm^2, , http://www.diodes.com/_files/packages/8686949.gif
Diode 5W series Axial Horizontal pin pitch 12.7mm  length 8.9mm diameter 3.7mm
0
2
2
Diode_THT
D_A-405_P2.54mm_Vertical_AnodeUp
Diode, A-405 series, Axial, Vertical, pin pitch=2.54mm, , length*diameter=5.2*2.7mm^2, , http://www.diodes.com/_files/packages/A-405.pdf
Diode A-405 series Axial Vertical pin pitch 2.54mm  length 5.2mm diameter 2.7mm
0
2
2
Diode_THT
D_A-405_P2.54mm_Vertical_KathodeUp
Diode, A-405 series, Axial, Vertical, pin pitch=2.54mm, , length*diameter=5.2*2.7mm^2, , http://www.diodes.com/_files/packages/A-405.pdf
Diode A-405 series Axial Vertical pin pitch 2.54mm  length 5.2mm diameter 2.7mm
0
2
2
Diode_THT
D_A-405_P5.08mm_Vertical_AnodeUp
Diode, A-405 series, Axial, Vertical, pin pitch=5.08mm, , length*diameter=5.2*2.7mm^2, , http://www.diodes.com/_files/packages/A-405.pdf
Diode A-405 series Axial Vertical pin pitch 5.08mm  length 5.2mm diameter 2.7mm
0
2
2
Diode_THT
D_A-405_P5.08mm_Vertical_KathodeUp
Diode, A-405 series, Axial, Vertical, pin pitch=5.08mm, , length*diameter=5.2*2.7mm^2, , http://www.diodes.com/_files/packages/A-405.pdf
Diode A-405 series Axial Vertical pin pitch 5.08mm  length 5.2mm diameter 2.7mm
0
2
2
Diode_THT
D_A-405_P7.62mm_Horizontal
Diode, A-405 series, Axial, Horizontal, pin pitch=7.62mm, , length*diameter=5.2*2.7mm^2, , http://www.diodes.com/_files/packages/A-405.pdf
Diode A-405 series Axial Horizontal pin pitch 7.62mm  length 5.2mm diameter 2.7mm
0
2
2
Diode_THT
D_A-405_P10.16mm_Horizontal
Diode, A-405 series, Axial, Horizontal, pin pitch=10.16mm, , length*diameter=5.2*2.7mm^2, , http://www.diodes.com/_files/packages/A-405.pdf
Diode A-405 series Axial Horizontal pin pitch 10.16mm  length 5.2mm diameter 2.7mm
0
2
2
Diode_THT
D_A-405_P12.70mm_Horizontal
Diode, A-405 series, Axial, Horizontal, pin pitch=12.7mm, , length*diameter=5.2*2.7mm^2, , http://www.diodes.com/_files/packages/A-405.pdf
Diode A-405 series Axial Horizontal pin pitch 12.7mm  length 5.2mm diameter 2.7mm
0
2
2
Diode_THT
D_DO-15_P2.54mm_Vertical_AnodeUp
Diode, DO-15 series, Axial, Vertical, pin pitch=2.54mm, , length*diameter=7.6*3.6mm^2, , http://www.diodes.com/_files/packages/DO-15.pdf
Diode DO-15 series Axial Vertical pin pitch 2.54mm  length 7.6mm diameter 3.6mm
0
2
2
Diode_THT
D_DO-15_P2.54mm_Vertical_KathodeUp
Diode, DO-15 series, Axial, Vertical, pin pitch=2.54mm, , length*diameter=7.6*3.6mm^2, , http://www.diodes.com/_files/packages/DO-15.pdf
Diode DO-15 series Axial Vertical pin pitch 2.54mm  length 7.6mm diameter 3.6mm
0
2
2
Diode_THT
D_DO-15_P3.81mm_Vertical_AnodeUp
Diode, DO-15 series, Axial, Vertical, pin pitch=3.81mm, , length*diameter=7.6*3.6mm^2, , http://www.diodes.com/_files/packages/DO-15.pdf
Diode DO-15 series Axial Vertical pin pitch 3.81mm  length 7.6mm diameter 3.6mm
0
2
2
Diode_THT
D_DO-15_P3.81mm_Vertical_KathodeUp
Diode, DO-15 series, Axial, Vertical, pin pitch=3.81mm, , length*diameter=7.6*3.6mm^2, , http://www.diodes.com/_files/packages/DO-15.pdf
Diode DO-15 series Axial Vertical pin pitch 3.81mm  length 7.6mm diameter 3.6mm
0
2
2
Diode_THT
D_DO-15_P5.08mm_Vertical_AnodeUp
Diode, DO-15 series, Axial, Vertical, pin pitch=5.08mm, , length*diameter=7.6*3.6mm^2, , http://www.diodes.com/_files/packages/DO-15.pdf
Diode DO-15 series Axial Vertical pin pitch 5.08mm  length 7.6mm diameter 3.6mm
0
2
2
Diode_THT
D_DO-15_P5.08mm_Vertical_KathodeUp
Diode, DO-15 series, Axial, Vertical, pin pitch=5.08mm, , length*diameter=7.6*3.6mm^2, , http://www.diodes.com/_files/packages/DO-15.pdf
Diode DO-15 series Axial Vertical pin pitch 5.08mm  length 7.6mm diameter 3.6mm
0
2
2
Diode_THT
D_DO-15_P10.16mm_Horizontal
Diode, DO-15 series, Axial, Horizontal, pin pitch=10.16mm, , length*diameter=7.6*3.6mm^2, , http://www.diodes.com/_files/packages/DO-15.pdf
Diode DO-15 series Axial Horizontal pin pitch 10.16mm  length 7.6mm diameter 3.6mm
0
2
2
Diode_THT
D_DO-15_P12.70mm_Horizontal
Diode, DO-15 series, Axial, Horizontal, pin pitch=12.7mm, , length*diameter=7.6*3.6mm^2, , http://www.diodes.com/_files/packages/DO-15.pdf
Diode DO-15 series Axial Horizontal pin pitch 12.7mm  length 7.6mm diameter 3.6mm
0
2
2
Diode_THT
D_DO-15_P15.24mm_Horizontal
Diode, DO-15 series, Axial, Horizontal, pin pitch=15.24mm, , length*diameter=7.6*3.6mm^2, , http://www.diodes.com/_files/packages/DO-15.pdf
Diode DO-15 series Axial Horizontal pin pitch 15.24mm  length 7.6mm diameter 3.6mm
0
2
2
Diode_THT
D_DO-27_P5.08mm_Vertical_AnodeUp
Diode, DO-27 series, Axial, Vertical, pin pitch=5.08mm, , length*diameter=9.52*5.33mm^2, , http://www.slottechforum.com/slotinfo/Techstuff/CD2%20Diodes%20and%20Transistors/Cases/Diode%20DO-27.jpg
Diode DO-27 series Axial Vertical pin pitch 5.08mm  length 9.52mm diameter 5.33mm
0
2
2
Diode_THT
D_DO-27_P5.08mm_Vertical_KathodeUp
Diode, DO-27 series, Axial, Vertical, pin pitch=5.08mm, , length*diameter=9.52*5.33mm^2, , http://www.slottechforum.com/slotinfo/Techstuff/CD2%20Diodes%20and%20Transistors/Cases/Diode%20DO-27.jpg
Diode DO-27 series Axial Vertical pin pitch 5.08mm  length 9.52mm diameter 5.33mm
0
2
2
Diode_THT
D_DO-27_P12.70mm_Horizontal
Diode, DO-27 series, Axial, Horizontal, pin pitch=12.7mm, , length*diameter=9.52*5.33mm^2, , http://www.slottechforum.com/slotinfo/Techstuff/CD2%20Diodes%20and%20Transistors/Cases/Diode%20DO-27.jpg
Diode DO-27 series Axial Horizontal pin pitch 12.7mm  length 9.52mm diameter 5.33mm
0
2
2
Diode_THT
D_DO-27_P15.24mm_Horizontal
Diode, DO-27 series, Axial, Horizontal, pin pitch=15.24mm, , length*diameter=9.52*5.33mm^2, , http://www.slottechforum.com/slotinfo/Techstuff/CD2%20Diodes%20and%20Transistors/Cases/Diode%20DO-27.jpg
Diode DO-27 series Axial Horizontal pin pitch 15.24mm  length 9.52mm diameter 5.33mm
0
2
2
Diode_THT
D_DO-34_SOD68_P2.54mm_Vertical_AnodeUp
Diode, DO-34_SOD68 series, Axial, Vertical, pin pitch=2.54mm, , length*diameter=3.04*1.6mm^2, , https://www.nxp.com/docs/en/data-sheet/KTY83_SER.pdf
Diode DO-34_SOD68 series Axial Vertical pin pitch 2.54mm  length 3.04mm diameter 1.6mm
0
2
2
Diode_THT
D_DO-34_SOD68_P2.54mm_Vertical_KathodeUp
Diode, DO-34_SOD68 series, Axial, Vertical, pin pitch=2.54mm, , length*diameter=3.04*1.6mm^2, , https://www.nxp.com/docs/en/data-sheet/KTY83_SER.pdf
Diode DO-34_SOD68 series Axial Vertical pin pitch 2.54mm  length 3.04mm diameter 1.6mm
0
2
2
Diode_THT
D_DO-34_SOD68_P5.08mm_Vertical_AnodeUp
Diode, DO-34_SOD68 series, Axial, Vertical, pin pitch=5.08mm, , length*diameter=3.04*1.6mm^2, , https://www.nxp.com/docs/en/data-sheet/KTY83_SER.pdf
Diode DO-34_SOD68 series Axial Vertical pin pitch 5.08mm  length 3.04mm diameter 1.6mm
0
2
2
Diode_THT
D_DO-34_SOD68_P5.08mm_Vertical_KathodeUp
Diode, DO-34_SOD68 series, Axial, Vertical, pin pitch=5.08mm, , length*diameter=3.04*1.6mm^2, , https://www.nxp.com/docs/en/data-sheet/KTY83_SER.pdf
Diode DO-34_SOD68 series Axial Vertical pin pitch 5.08mm  length 3.04mm diameter 1.6mm
0
2
2
Diode_THT
D_DO-34_SOD68_P7.62mm_Horizontal
Diode, DO-34_SOD68 series, Axial, Horizontal, pin pitch=7.62mm, , length*diameter=3.04*1.6mm^2, , https://www.nxp.com/docs/en/data-sheet/KTY83_SER.pdf
Diode DO-34_SOD68 series Axial Horizontal pin pitch 7.62mm  length 3.04mm diameter 1.6mm
0
2
2
Diode_THT
D_DO-34_SOD68_P10.16mm_Horizontal
Diode, DO-34_SOD68 series, Axial, Horizontal, pin pitch=10.16mm, , length*diameter=3.04*1.6mm^2, , https://www.nxp.com/docs/en/data-sheet/KTY83_SER.pdf
Diode DO-34_SOD68 series Axial Horizontal pin pitch 10.16mm  length 3.04mm diameter 1.6mm
0
2
2
Diode_THT
D_DO-34_SOD68_P12.70mm_Horizontal
Diode, DO-34_SOD68 series, Axial, Horizontal, pin pitch=12.7mm, , length*diameter=3.04*1.6mm^2, , https://www.nxp.com/docs/en/data-sheet/KTY83_SER.pdf
Diode DO-34_SOD68 series Axial Horizontal pin pitch 12.7mm  length 3.04mm diameter 1.6mm
0
2
2
Diode_THT
D_DO-35_SOD27_P2.54mm_Vertical_AnodeUp
Diode, DO-35_SOD27 series, Axial, Vertical, pin pitch=2.54mm, , length*diameter=4*2mm^2, , http://www.diodes.com/_files/packages/DO-35.pdf
Diode DO-35_SOD27 series Axial Vertical pin pitch 2.54mm  length 4mm diameter 2mm
0
2
2
Diode_THT
D_DO-35_SOD27_P2.54mm_Vertical_KathodeUp
Diode, DO-35_SOD27 series, Axial, Vertical, pin pitch=2.54mm, , length*diameter=4*2mm^2, , http://www.diodes.com/_files/packages/DO-35.pdf
Diode DO-35_SOD27 series Axial Vertical pin pitch 2.54mm  length 4mm diameter 2mm
0
2
2
Diode_THT
D_DO-35_SOD27_P3.81mm_Vertical_AnodeUp
Diode, DO-35_SOD27 series, Axial, Vertical, pin pitch=3.81mm, , length*diameter=4*2mm^2, , http://www.diodes.com/_files/packages/DO-35.pdf
Diode DO-35_SOD27 series Axial Vertical pin pitch 3.81mm  length 4mm diameter 2mm
0
2
2
Diode_THT
D_DO-35_SOD27_P3.81mm_Vertical_KathodeUp
Diode, DO-35_SOD27 series, Axial, Vertical, pin pitch=3.81mm, , length*diameter=4*2mm^2, , http://www.diodes.com/_files/packages/DO-35.pdf
Diode DO-35_SOD27 series Axial Vertical pin pitch 3.81mm  length 4mm diameter 2mm
0
2
2
Diode_THT
D_DO-35_SOD27_P5.08mm_Vertical_AnodeUp
Diode, DO-35_SOD27 series, Axial, Vertical, pin pitch=5.08mm, , length*diameter=4*2mm^2, , http://www.diodes.com/_files/packages/DO-35.pdf
Diode DO-35_SOD27 series Axial Vertical pin pitch 5.08mm  length 4mm diameter 2mm
0
2
2
Diode_THT
D_DO-35_SOD27_P5.08mm_Vertical_KathodeUp
Diode, DO-35_SOD27 series, Axial, Vertical, pin pitch=5.08mm, , length*diameter=4*2mm^2, , http://www.diodes.com/_files/packages/DO-35.pdf
Diode DO-35_SOD27 series Axial Vertical pin pitch 5.08mm  length 4mm diameter 2mm
0
2
2
Diode_THT
D_DO-35_SOD27_P7.62mm_Horizontal
Diode, DO-35_SOD27 series, Axial, Horizontal, pin pitch=7.62mm, , length*diameter=4*2mm^2, , http://www.diodes.com/_files/packages/DO-35.pdf
Diode DO-35_SOD27 series Axial Horizontal pin pitch 7.62mm  length 4mm diameter 2mm
0
2
2
Diode_THT
D_DO-35_SOD27_P10.16mm_Horizontal
Diode, DO-35_SOD27 series, Axial, Horizontal, pin pitch=10.16mm, , length*diameter=4*2mm^2, , http://www.diodes.com/_files/packages/DO-35.pdf
Diode DO-35_SOD27 series Axial Horizontal pin pitch 10.16mm  length 4mm diameter 2mm
0
2
2
Diode_THT
D_DO-35_SOD27_P12.70mm_Horizontal
Diode, DO-35_SOD27 series, Axial, Horizontal, pin pitch=12.7mm, , length*diameter=4*2mm^2, , http://www.diodes.com/_files/packages/DO-35.pdf
Diode DO-35_SOD27 series Axial Horizontal pin pitch 12.7mm  length 4mm diameter 2mm
0
2
2
Diode_THT
D_DO-41_SOD81_P2.54mm_Vertical_AnodeUp
Diode, DO-41_SOD81 series, Axial, Vertical, pin pitch=2.54mm, , length*diameter=5.2*2.7mm^2, , http://www.diodes.com/_files/packages/DO-41%20(Plastic).pdf
Diode DO-41_SOD81 series Axial Vertical pin pitch 2.54mm  length 5.2mm diameter 2.7mm
0
2
2
Diode_THT
D_DO-41_SOD81_P2.54mm_Vertical_KathodeUp
Diode, DO-41_SOD81 series, Axial, Vertical, pin pitch=2.54mm, , length*diameter=5.2*2.7mm^2, , http://www.diodes.com/_files/packages/DO-41%20(Plastic).pdf
Diode DO-41_SOD81 series Axial Vertical pin pitch 2.54mm  length 5.2mm diameter 2.7mm
0
2
2
Diode_THT
D_DO-41_SOD81_P3.81mm_Vertical_AnodeUp
Diode, DO-41_SOD81 series, Axial, Vertical, pin pitch=3.81mm, , length*diameter=5.2*2.7mm^2, , https://www.diodes.com/assets/Package-Files/DO-41-Plastic.pdf
Diode DO-41_SOD81 series Axial Vertical pin pitch 3.81mm  length 5.2mm diameter 2.7mm
0
2
2
Diode_THT
D_DO-41_SOD81_P3.81mm_Vertical_KathodeUp
Diode, DO-41_SOD81 series, Axial, Vertical, pin pitch=3.81mm, , length*diameter=5.2*2.7mm^2, , https://www.diodes.com/assets/Package-Files/DO-41-Plastic.pdf
Diode DO-41_SOD81 series Axial Vertical pin pitch 3.81mm  length 5.2mm diameter 2.7mm
0
2
2
Diode_THT
D_DO-41_SOD81_P5.08mm_Vertical_AnodeUp
Diode, DO-41_SOD81 series, Axial, Vertical, pin pitch=5.08mm, , length*diameter=5.2*2.7mm^2, , http://www.diodes.com/_files/packages/DO-41%20(Plastic).pdf
Diode DO-41_SOD81 series Axial Vertical pin pitch 5.08mm  length 5.2mm diameter 2.7mm
0
2
2
Diode_THT
D_DO-41_SOD81_P5.08mm_Vertical_KathodeUp
Diode, DO-41_SOD81 series, Axial, Vertical, pin pitch=5.08mm, , length*diameter=5.2*2.7mm^2, , http://www.diodes.com/_files/packages/DO-41%20(Plastic).pdf
Diode DO-41_SOD81 series Axial Vertical pin pitch 5.08mm  length 5.2mm diameter 2.7mm
0
2
2
Diode_THT
D_DO-41_SOD81_P7.62mm_Horizontal
Diode, DO-41_SOD81 series, Axial, Horizontal, pin pitch=7.62mm, , length*diameter=5.2*2.7mm^2, , http://www.diodes.com/_files/packages/DO-41%20(Plastic).pdf
Diode DO-41_SOD81 series Axial Horizontal pin pitch 7.62mm  length 5.2mm diameter 2.7mm
0
2
2
Diode_THT
D_DO-41_SOD81_P10.16mm_Horizontal
Diode, DO-41_SOD81 series, Axial, Horizontal, pin pitch=10.16mm, , length*diameter=5.2*2.7mm^2, , http://www.diodes.com/_files/packages/DO-41%20(Plastic).pdf
Diode DO-41_SOD81 series Axial Horizontal pin pitch 10.16mm  length 5.2mm diameter 2.7mm
0
2
2
Diode_THT
D_DO-41_SOD81_P12.70mm_Horizontal
Diode, DO-41_SOD81 series, Axial, Horizontal, pin pitch=12.7mm, , length*diameter=5.2*2.7mm^2, , http://www.diodes.com/_files/packages/DO-41%20(Plastic).pdf
Diode DO-41_SOD81 series Axial Horizontal pin pitch 12.7mm  length 5.2mm diameter 2.7mm
0
2
2
Diode_THT
D_DO-201AD_P3.81mm_Vertical_AnodeUp
Diode, DO-201AD series, Axial, Vertical, pin pitch=3.81mm, , length*diameter=9.5*5.2mm^2, , http://www.diodes.com/_files/packages/DO-201AD.pdf
Diode DO-201AD series Axial Vertical pin pitch 3.81mm  length 9.5mm diameter 5.2mm
0
2
2
Diode_THT
D_DO-201AD_P3.81mm_Vertical_KathodeUp
Diode, DO-201AD series, Axial, Vertical, pin pitch=3.81mm, , length*diameter=9.5*5.2mm^2, , http://www.diodes.com/_files/packages/DO-201AD.pdf
Diode DO-201AD series Axial Vertical pin pitch 3.81mm  length 9.5mm diameter 5.2mm
0
2
2
Diode_THT
D_DO-201AD_P5.08mm_Vertical_AnodeUp
Diode, DO-201AD series, Axial, Vertical, pin pitch=5.08mm, , length*diameter=9.5*5.2mm^2, , http://www.diodes.com/_files/packages/DO-201AD.pdf
Diode DO-201AD series Axial Vertical pin pitch 5.08mm  length 9.5mm diameter 5.2mm
0
2
2
Diode_THT
D_DO-201AD_P5.08mm_Vertical_KathodeUp
Diode, DO-201AD series, Axial, Vertical, pin pitch=5.08mm, , length*diameter=9.5*5.2mm^2, , http://www.diodes.com/_files/packages/DO-201AD.pdf
Diode DO-201AD series Axial Vertical pin pitch 5.08mm  length 9.5mm diameter 5.2mm
0
2
2
Diode_THT
D_DO-201AD_P12.70mm_Horizontal
Diode, DO-201AD series, Axial, Horizontal, pin pitch=12.7mm, , length*diameter=9.5*5.2mm^2, , http://www.diodes.com/_files/packages/DO-201AD.pdf
Diode DO-201AD series Axial Horizontal pin pitch 12.7mm  length 9.5mm diameter 5.2mm
0
2
2
Diode_THT
D_DO-201AD_P15.24mm_Horizontal
Diode, DO-201AD series, Axial, Horizontal, pin pitch=15.24mm, , length*diameter=9.5*5.2mm^2, , http://www.diodes.com/_files/packages/DO-201AD.pdf
Diode DO-201AD series Axial Horizontal pin pitch 15.24mm  length 9.5mm diameter 5.2mm
0
2
2
Diode_THT
D_DO-201AE_P3.81mm_Vertical_AnodeUp
Diode, DO-201AE series, Axial, Vertical, pin pitch=3.81mm, , length*diameter=9*5.3mm^2, , http://www.farnell.com/datasheets/529758.pdf
Diode DO-201AE series Axial Vertical pin pitch 3.81mm  length 9mm diameter 5.3mm
0
2
2
Diode_THT
D_DO-201AE_P3.81mm_Vertical_KathodeUp
Diode, DO-201AE series, Axial, Vertical, pin pitch=3.81mm, , length*diameter=9*5.3mm^2, , http://www.farnell.com/datasheets/529758.pdf
Diode DO-201AE series Axial Vertical pin pitch 3.81mm  length 9mm diameter 5.3mm
0
2
2
Diode_THT
D_DO-201AE_P5.08mm_Vertical_AnodeUp
Diode, DO-201AE series, Axial, Vertical, pin pitch=5.08mm, , length*diameter=9*5.3mm^2, , http://www.farnell.com/datasheets/529758.pdf
Diode DO-201AE series Axial Vertical pin pitch 5.08mm  length 9mm diameter 5.3mm
0
2
2
Diode_THT
D_DO-201AE_P5.08mm_Vertical_KathodeUp
Diode, DO-201AE series, Axial, Vertical, pin pitch=5.08mm, , length*diameter=9*5.3mm^2, , http://www.farnell.com/datasheets/529758.pdf
Diode DO-201AE series Axial Vertical pin pitch 5.08mm  length 9mm diameter 5.3mm
0
2
2
Diode_THT
D_DO-201AE_P12.70mm_Horizontal
Diode, DO-201AE series, Axial, Horizontal, pin pitch=12.7mm, , length*diameter=9*5.3mm^2, , http://www.farnell.com/datasheets/529758.pdf
Diode DO-201AE series Axial Horizontal pin pitch 12.7mm  length 9mm diameter 5.3mm
0
2
2
Diode_THT
D_DO-201AE_P15.24mm_Horizontal
Diode, DO-201AE series, Axial, Horizontal, pin pitch=15.24mm, , length*diameter=9*5.3mm^2, , http://www.farnell.com/datasheets/529758.pdf
Diode DO-201AE series Axial Horizontal pin pitch 15.24mm  length 9mm diameter 5.3mm
0
2
2
Diode_THT
D_DO-201_P3.81mm_Vertical_AnodeUp
Diode, DO-201 series, Axial, Vertical, pin pitch=3.81mm, , length*diameter=9.53*5.21mm^2, , http://www.diodes.com/_files/packages/DO-201.pdf
Diode DO-201 series Axial Vertical pin pitch 3.81mm  length 9.53mm diameter 5.21mm
0
2
2
Diode_THT
D_DO-201_P3.81mm_Vertical_KathodeUp
Diode, DO-201 series, Axial, Vertical, pin pitch=3.81mm, , length*diameter=9.53*5.21mm^2, , http://www.diodes.com/_files/packages/DO-201.pdf
Diode DO-201 series Axial Vertical pin pitch 3.81mm  length 9.53mm diameter 5.21mm
0
2
2
Diode_THT
D_DO-201_P5.08mm_Vertical_AnodeUp
Diode, DO-201 series, Axial, Vertical, pin pitch=5.08mm, , length*diameter=9.53*5.21mm^2, , http://www.diodes.com/_files/packages/DO-201.pdf
Diode DO-201 series Axial Vertical pin pitch 5.08mm  length 9.53mm diameter 5.21mm
0
2
2
Diode_THT
D_DO-201_P5.08mm_Vertical_KathodeUp
Diode, DO-201 series, Axial, Vertical, pin pitch=5.08mm, , length*diameter=9.53*5.21mm^2, , http://www.diodes.com/_files/packages/DO-201.pdf
Diode DO-201 series Axial Vertical pin pitch 5.08mm  length 9.53mm diameter 5.21mm
0
2
2
Diode_THT
D_DO-201_P12.70mm_Horizontal
Diode, DO-201 series, Axial, Horizontal, pin pitch=12.7mm, , length*diameter=9.53*5.21mm^2, , http://www.diodes.com/_files/packages/DO-201.pdf
Diode DO-201 series Axial Horizontal pin pitch 12.7mm  length 9.53mm diameter 5.21mm
0
2
2
Diode_THT
D_DO-201_P15.24mm_Horizontal
Diode, DO-201 series, Axial, Horizontal, pin pitch=15.24mm, , length*diameter=9.53*5.21mm^2, , http://www.diodes.com/_files/packages/DO-201.pdf
Diode DO-201 series Axial Horizontal pin pitch 15.24mm  length 9.53mm diameter 5.21mm
0
2
2
Diode_THT
D_P600_R-6_P7.62mm_Vertical_AnodeUp
Diode, P600_R-6 series, Axial, Vertical, pin pitch=7.62mm, , length*diameter=9.1*9.1mm^2, , http://www.vishay.com/docs/88692/p600a.pdf, http://www.diodes.com/_files/packages/R-6.pdf
Diode P600_R-6 series Axial Vertical pin pitch 7.62mm  length 9.1mm diameter 9.1mm
0
2
2
Diode_THT
D_P600_R-6_P7.62mm_Vertical_KathodeUp
Diode, P600_R-6 series, Axial, Vertical, pin pitch=7.62mm, , length*diameter=9.1*9.1mm^2, , http://www.vishay.com/docs/88692/p600a.pdf, http://www.diodes.com/_files/packages/R-6.pdf
Diode P600_R-6 series Axial Vertical pin pitch 7.62mm  length 9.1mm diameter 9.1mm
0
2
2
Diode_THT
D_P600_R-6_P12.70mm_Horizontal
Diode, P600_R-6 series, Axial, Horizontal, pin pitch=12.7mm, , length*diameter=9.1*9.1mm^2, , http://www.vishay.com/docs/88692/p600a.pdf, http://www.diodes.com/_files/packages/R-6.pdf
Diode P600_R-6 series Axial Horizontal pin pitch 12.7mm  length 9.1mm diameter 9.1mm
0
2
2
Diode_THT
D_P600_R-6_P20.00mm_Horizontal
Diode, P600_R-6 series, Axial, Horizontal, pin pitch=20mm, , length*diameter=9.1*9.1mm^2, , http://www.vishay.com/docs/88692/p600a.pdf, http://www.diodes.com/_files/packages/R-6.pdf
Diode P600_R-6 series Axial Horizontal pin pitch 20mm  length 9.1mm diameter 9.1mm
0
2
2
Diode_THT
D_T-1_P2.54mm_Vertical_AnodeUp
Diode, T-1 series, Axial, Vertical, pin pitch=2.54mm, , length*diameter=3.2*2.6mm^2, , http://www.diodes.com/_files/packages/T-1.pdf
Diode T-1 series Axial Vertical pin pitch 2.54mm  length 3.2mm diameter 2.6mm
0
2
2
Diode_THT
D_T-1_P2.54mm_Vertical_KathodeUp
Diode, T-1 series, Axial, Vertical, pin pitch=2.54mm, , length*diameter=3.2*2.6mm^2, , http://www.diodes.com/_files/packages/T-1.pdf
Diode T-1 series Axial Vertical pin pitch 2.54mm  length 3.2mm diameter 2.6mm
0
2
2
Diode_THT
D_T-1_P5.08mm_Horizontal
Diode, T-1 series, Axial, Horizontal, pin pitch=5.08mm, , length*diameter=3.2*2.6mm^2, , http://www.diodes.com/_files/packages/T-1.pdf
Diode T-1 series Axial Horizontal pin pitch 5.08mm  length 3.2mm diameter 2.6mm
0
2
2
Diode_THT
D_T-1_P10.16mm_Horizontal
Diode, T-1 series, Axial, Horizontal, pin pitch=10.16mm, , length*diameter=3.2*2.6mm^2, , http://www.diodes.com/_files/packages/T-1.pdf
Diode T-1 series Axial Horizontal pin pitch 10.16mm  length 3.2mm diameter 2.6mm
0
2
2
Diode_THT
D_T-1_P12.70mm_Horizontal
Diode, T-1 series, Axial, Horizontal, pin pitch=12.7mm, , length*diameter=3.2*2.6mm^2, , http://www.diodes.com/_files/packages/T-1.pdf
Diode T-1 series Axial Horizontal pin pitch 12.7mm  length 3.2mm diameter 2.6mm
0
2
2
Diode_THT
Diode_Bridge_15.1x15.1x6.3mm_P10.9mm
Single phase bridge rectifier case 15.1x15.1mm, pitch 10.9mm, see https://diotec.com/tl_files/diotec/files/pdf/datasheets/pb1000.pdf
Diode Bridge PB10xxS
0
4
4
Diode_THT
Diode_Bridge_15.2x15.2x6.3mm_P10.9mm
Single phase bridge rectifier case 15.2x15.2mm, pitch 10.9mm, see https://diotec.com/tl_files/diotec/files/pdf/datasheets/kbpc600.pdf
Diode Bridge KBPC6xx
0
4
4
Diode_THT
Diode_Bridge_15.7x15.7x6.3mm_P10.8mm
Single phase bridge rectifier case 15.7x15.7
Diode Bridge
0
4
4
Diode_THT
Diode_Bridge_16.7x16.7x6.3mm_P10.8mm
Single phase bridge rectifier case 16.7x16.7
Diode Bridge
0
4
4
Diode_THT
Diode_Bridge_19.0x3.5x10.0mm_P5.0mm
Vishay GBU rectifier package, 5.08mm pitch, see http://www.vishay.com/docs/88606/g3sba20.pdf
Vishay GBU rectifier diode bridge
0
4
4
Diode_THT
Diode_Bridge_19.0x19.0x6.8mm_P12.7mm
Single phase bridge rectifier case 19x19mm, pitch 12.7mm, see https://diotec.com/tl_files/diotec/files/pdf/datasheets/pb1000.pdf
Diode Bridge PB10xx
0
4
4
Diode_THT
Diode_Bridge_28.6x28.6x7.3mm_P18.0mm_P11.6mm
Single phase bridge rectifier case 28.6x28.6mm, pitch 18.0mm & 11.6mm, see https://diotec.com/tl_files/diotec/files/pdf/datasheets/kbpc1500fw.pdf
Diode Bridge KBPCxxxxWP
0
4
4
Diode_THT
Diode_Bridge_32.0x5.6x17.0mm_P10.0mm_P7.5mm
Diotec 32x5.6x17mm rectifier package, 7.5mm/10mm pitch, see https://diotec.com/tl_files/diotec/files/pdf/datasheets/b40c3700.pdf
Diotec rectifier diode bridge
0
4
4
Diode_THT
Diode_Bridge_DIP-4_W5.08mm_P2.54mm
4-lead dip package for diode bridges, row spacing 5.08mm, pin-spacing 2.54mm, see http://www.vishay.com/docs/88898/b2m.pdf
DIL DIP PDIP 5.08mm 2.54
0
4
4
Diode_THT
Diode_Bridge_DIP-4_W7.62mm_P5.08mm
4-lead dip package for diode bridges, row spacing 7.62 mm (300 mils), see http://cdn-reichelt.de/documents/datenblatt/A400/HDBL101G_20SERIES-TSC.pdf
DIL DIP PDIP 5.08mm 7.62mm 300mil
0
4
4
Diode_THT
Diode_Bridge_Round_D8.9mm
4-lead round diode bridge package, diameter 8.9mm, pin pitch 5.08mm, see http://cdn-reichelt.de/documents/datenblatt/A400/W005M-W10M_SEP.PDF
diode bridge 8.9mm 8.85mm WOB pitch 5.08mm
0
4
4
Diode_THT
Diode_Bridge_Round_D9.0mm
4-lead round diode bridge package, diameter 9.0mm, pin pitch 5.0mm, see https://diotec.com/tl_files/diotec/files/pdf/datasheets/b40r.pdf
diode bridge 9.0mm 8.85mm WOB pitch 5.0mm
0
4
4
Diode_THT
Diode_Bridge_Round_D9.8mm
4-lead round diode bridge package, diameter 9.8mm, pin pitch 5.08mm, see http://www.vishay.com/docs/88769/woo5g.pdf
diode bridge 9.8mm WOG pitch 5.08mm
0
4
4
Diode_THT
Diode_Bridge_Vishay_GBL
Vishay GBL rectifier package, 5.08mm pitch, see http://www.vishay.com/docs/88609/gbl005.pdf
Vishay GBL rectifier diode bridge
0
4
4
Diode_THT
Diode_Bridge_Vishay_GBU
Vishay GBU rectifier package, 5.08mm pitch, see http://www.vishay.com/docs/88606/g3sba20.pdf
Vishay GBU rectifier diode bridge
0
4
4
Diode_THT
Diode_Bridge_Vishay_KBL
Vishay KBL rectifier package, 5.08mm pitch, see http://www.vishay.com/docs/88655/kbl005.pdf
Vishay KBL rectifier diode bridge
0
4
4
Diode_THT
Diode_Bridge_Vishay_KBPC1
Single phase bridge rectifier case KBPC1, see http://www.vishay.com/docs/93585/vs-kbpc1series.pdf
Diode Bridge
0
4
4
Diode_THT
Diode_Bridge_Vishay_KBPC6
Single phase bridge rectifier case KBPC6, see http://www.vishay.com/docs/93585/vs-kbpc1series.pdf
Diode Bridge
0
4
4
Diode_THT
Diode_Bridge_Vishay_KBU
Vishay KBU rectifier package, 5.08mm pitch, see http://www.vishay.com/docs/88656/kbu4.pdf
Vishay KBU rectifier diode bridge
0
4
4
Jumper
SolderJumper-2_P1.3mm_Bridged2Bar_Pad1.0x1.5mm
SMD Solder Jumper, 1x1.5mm Pads, 0.3mm gap, bridged with 2 copper strips
solder jumper open
0
2
2
Jumper
SolderJumper-2_P1.3mm_Bridged2Bar_RoundedPad1.0x1.5mm
SMD Solder Jumper, 1x1.5mm, rounded Pads, 0.3mm gap, bridged with 2 copper strips
solder jumper open
0
2
2
Jumper
SolderJumper-2_P1.3mm_Bridged_Pad1.0x1.5mm
SMD Solder Jumper, 1x1.5mm Pads, 0.3mm gap, bridged with 1 copper strip
solder jumper open
0
2
2
Jumper
SolderJumper-2_P1.3mm_Bridged_RoundedPad1.0x1.5mm
SMD Solder Jumper, 1x1.5mm, rounded Pads, 0.3mm gap, bridged with 1 copper strip
solder jumper open
0
2
2
Jumper
SolderJumper-2_P1.3mm_Open_Pad1.0x1.5mm
SMD Solder Jumper, 1x1.5mm Pads, 0.3mm gap, open
solder jumper open
0
2
2
Jumper
SolderJumper-2_P1.3mm_Open_RoundedPad1.0x1.5mm
SMD Solder Jumper, 1x1.5mm, rounded Pads, 0.3mm gap, open
solder jumper open
0
2
2
Jumper
SolderJumper-2_P1.3mm_Open_TrianglePad1.0x1.5mm
SMD Solder Jumper, 1x1.5mm Triangular Pads, 0.3mm gap, open
solder jumper open
0
2
2
Jumper
SolderJumper-3_P1.3mm_Bridged2Bar12_Pad1.0x1.5mm
SMD Solder 3-pad Jumper, 1x1.5mm Pads, 0.3mm gap, pads 1-2 Bridged2Bar with 2 copper strip
solder jumper open
0
3
3
Jumper
SolderJumper-3_P1.3mm_Bridged2Bar12_Pad1.0x1.5mm_NumberLabels
SMD Solder Jumper, 1x1.5mm Pads, 0.3mm gap, pads 1-2 Bridged2Bar with 2 copper strip, labeled with numbers
solder jumper open
0
3
3
Jumper
SolderJumper-3_P1.3mm_Bridged2Bar12_RoundedPad1.0x1.5mm
SMD Solder 3-pad Jumper, 1x1.5mm rounded Pads, 0.3mm gap, pads 1-2 Bridged2Bar with 2 copper strip
solder jumper open
0
3
3
Jumper
SolderJumper-3_P1.3mm_Bridged2Bar12_RoundedPad1.0x1.5mm_NumberLabels
SMD Solder 3-pad Jumper, 1x1.5mm rounded Pads, 0.3mm gap, pads 1-2 Bridged2Bar with 2 copper strip, labeled with numbers
solder jumper open
0
3
3
Jumper
SolderJumper-3_P1.3mm_Bridged12_Pad1.0x1.5mm
SMD Solder 3-pad Jumper, 1x1.5mm Pads, 0.3mm gap, pads 1-2 bridged with 1 copper strip
solder jumper open
0
3
3
Jumper
SolderJumper-3_P1.3mm_Bridged12_Pad1.0x1.5mm_NumberLabels
SMD Solder Jumper, 1x1.5mm Pads, 0.3mm gap, pads 1-2 bridged with 1 copper strip, labeled with numbers
solder jumper open
0
3
3
Jumper
SolderJumper-3_P1.3mm_Bridged12_RoundedPad1.0x1.5mm
SMD Solder 3-pad Jumper, 1x1.5mm rounded Pads, 0.3mm gap, pads 1-2 bridged with 1 copper strip
solder jumper open
0
3
3
Jumper
SolderJumper-3_P1.3mm_Bridged12_RoundedPad1.0x1.5mm_NumberLabels
SMD Solder 3-pad Jumper, 1x1.5mm rounded Pads, 0.3mm gap, pads 1-2 bridged with 1 copper strip, labeled with numbers
solder jumper open
0
3
3
Jumper
SolderJumper-3_P1.3mm_Open_Pad1.0x1.5mm
SMD Solder 3-pad Jumper, 1x1.5mm Pads, 0.3mm gap, open
solder jumper open
0
3
3
Jumper
SolderJumper-3_P1.3mm_Open_Pad1.0x1.5mm_NumberLabels
SMD Solder Jumper, 1x1.5mm Pads, 0.3mm gap, open, labeled with numbers
solder jumper open
0
3
3
Jumper
SolderJumper-3_P1.3mm_Open_RoundedPad1.0x1.5mm
SMD Solder 3-pad Jumper, 1x1.5mm rounded Pads, 0.3mm gap, open
solder jumper open
0
3
3
Jumper
SolderJumper-3_P1.3mm_Open_RoundedPad1.0x1.5mm_NumberLabels
SMD Solder 3-pad Jumper, 1x1.5mm rounded Pads, 0.3mm gap, open, labeled with numbers
solder jumper open
0
3
3
Jumper
SolderJumper-3_P2.0mm_Open_TrianglePad1.0x1.5mm
SMD Solder Jumper, 1x1.5mm Triangular Pads, 0.3mm gap, open
solder jumper open
0
5
3
Jumper
SolderJumper-3_P2.0mm_Open_TrianglePad1.0x1.5mm_NumberLabels
SMD Solder Jumper, 1x1.5mm Triangular Pads, 0.3mm gap, open, labeled with numbers
solder jumper open
0
5
3
LED_SMD
LED-APA102-2020
http://www.led-color.com/upload/201604/APA102-2020%20SMD%20LED.pdf
LED RGB SPI
0
8
6
LED_SMD
LED-L1T2_LUMILEDS
http://www.lumileds.com/uploads/438/DS133-pdf
LUMILEDS LUXEON TX L1T2 LED
0
3
3
LED_SMD
LED_1W_3W_R8
https://www.gme.cz/data/attachments/dsh.518-234.1.pdf
LED 1W 3W 5W
0
3
3
LED_SMD
LED_0201_0603Metric
LED SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), generated with kicad-footprint-generator
LED
0
4
2
LED_SMD
LED_0402_1005Metric
LED SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator
LED
0
2
2
LED_SMD
LED_0603_1608Metric
LED SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator
diode
0
2
2
LED_SMD
LED_0603_1608Metric_Castellated
LED SMD 0603 (1608 Metric), castellated end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator
LED castellated
0
2
2
LED_SMD
LED_0603_1608Metric_Pad1.05x0.95mm_HandSolder
LED SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator
LED handsolder
0
2
2
LED_SMD
LED_0805_2012Metric
LED SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator
diode
0
2
2
LED_SMD
LED_0805_2012Metric_Castellated
LED SMD 0805 (2012 Metric), castellated end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator
LED castellated
0
2
2
LED_SMD
LED_0805_2012Metric_Pad1.15x1.40mm_HandSolder
LED SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator
LED handsolder
0
2
2
LED_SMD
LED_01005_0402Metric
LED SMD 01005 (0402 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.vishay.com/docs/20056/crcw01005e3.pdf), generated with kicad-footprint-generator
LED
0
4
2
LED_SMD
LED_1206_3216Metric
LED SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator
diode
0
2
2
LED_SMD
LED_1206_3216Metric_Castellated
LED SMD 1206 (3216 Metric), castellated end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator
LED castellated
0
2
2
LED_SMD
LED_1206_3216Metric_Pad1.42x1.75mm_HandSolder
LED SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator
LED handsolder
0
2
2
LED_SMD
LED_1206_3216Metric_ReverseMount_Hole1.8x2.4mm
LED SMD 1206 (3216 Metric), reverse mount, square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator
diode reverse
0
2
2
LED_SMD
LED_1210_3225Metric
LED SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator
diode
0
2
2
LED_SMD
LED_1210_3225Metric_Castellated
LED SMD 1210 (3225 Metric), castellated end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator
LED castellated
0
2
2
LED_SMD
LED_1210_3225Metric_Pad1.42x2.65mm_HandSolder
LED SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator
LED handsolder
0
2
2
LED_SMD
LED_1806_4516Metric
LED SMD 1806 (4516 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://www.modelithics.com/models/Vendor/MuRata/BLM41P.pdf), generated with kicad-footprint-generator
diode
0
2
2
LED_SMD
LED_1806_4516Metric_Castellated
LED SMD 1806 (4516 Metric), castellated end terminal, IPC_7351 nominal, (Body size source: https://www.modelithics.com/models/Vendor/MuRata/BLM41P.pdf), generated with kicad-footprint-generator
LED castellated
0
2
2
LED_SMD
LED_1806_4516Metric_Pad1.57x1.80mm_HandSolder
LED SMD 1806 (4516 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://www.modelithics.com/models/Vendor/MuRata/BLM41P.pdf), generated with kicad-footprint-generator
LED handsolder
0
2
2
LED_SMD
LED_1812_4532Metric
LED SMD 1812 (4532 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://www.nikhef.nl/pub/departments/mt/projects/detectorR_D/dtddice/ERJ2G.pdf), generated with kicad-footprint-generator
diode
0
2
2
LED_SMD
LED_1812_4532Metric_Castellated
LED SMD 1812 (4532 Metric), castellated end terminal, IPC_7351 nominal, (Body size source: https://www.nikhef.nl/pub/departments/mt/projects/detectorR_D/dtddice/ERJ2G.pdf), generated with kicad-footprint-generator
LED castellated
0
2
2
LED_SMD
LED_1812_4532Metric_Pad1.30x3.40mm_HandSolder
LED SMD 1812 (4532 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://www.nikhef.nl/pub/departments/mt/projects/detectorR_D/dtddice/ERJ2G.pdf), generated with kicad-footprint-generator
LED handsolder
0
2
2
LED_SMD
LED_2010_5025Metric
LED SMD 2010 (5025 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator
diode
0
2
2
LED_SMD
LED_2010_5025Metric_Castellated
LED SMD 2010 (5025 Metric), castellated end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator
LED castellated
0
2
2
LED_SMD
LED_2010_5025Metric_Pad1.52x2.65mm_HandSolder
LED SMD 2010 (5025 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator
LED handsolder
0
2
2
LED_SMD
LED_2512_6332Metric
LED SMD 2512 (6332 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator
diode
0
2
2
LED_SMD
LED_2512_6332Metric_Castellated
LED SMD 2512 (6332 Metric), castellated end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator
LED castellated
0
2
2
LED_SMD
LED_2512_6332Metric_Pad1.52x3.35mm_HandSolder
LED SMD 2512 (6332 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator
LED handsolder
0
2
2
LED_SMD
LED_2816_7142Metric
LED SMD 2816 (7142 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size from: https://www.vishay.com/docs/30100/wsl.pdf), generated with kicad-footprint-generator
diode
0
2
2
LED_SMD
LED_2816_7142Metric_Castellated
LED SMD 2816 (7142 Metric), castellated end terminal, IPC_7351 nominal, (Body size from: https://www.vishay.com/docs/30100/wsl.pdf), generated with kicad-footprint-generator
LED castellated
0
2
2
LED_SMD
LED_2816_7142Metric_Pad3.20x4.45mm_HandSolder
LED SMD 2816 (7142 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size from: https://www.vishay.com/docs/30100/wsl.pdf), generated with kicad-footprint-generator
LED handsolder
0
2
2
LED_SMD
LED_Avago_PLCC4_3.2x2.8mm_CW
https://docs.broadcom.com/docs/AV02-4186EN
LED Avago PLCC-4 ASMB-MTB0-0A3A2
0
4
4
LED_SMD
LED_Avago_PLCC6_3x2.8mm
https://docs.broadcom.com/docs/AV02-3793EN
LED Avago PLCC-6 ASMT-YTB7-0AA02
0
6
6
LED_SMD
LED_Cree-PLCC4_2x2mm_CW
2.0mm x 2.0mm PLCC4 LED, http://www.cree.com/~/media/Files/Cree/LED-Components-and-Modules/HB/Data-Sheets/CLMVBFKA.pdf
LED Cree PLCC-4
0
4
4
LED_SMD
LED_Cree-PLCC4_3.2x2.8mm_CCW
3.2mm x 2.8mm PLCC4 LED, http://www.cree.com/led-components/media/documents/CLV1AFKB(874).pdf
LED Cree PLCC-4
0
4
4
LED_SMD
LED_Cree-PLCC4_5x5mm_CW
5.0mm x 5.0mm PLCC4 LED
LED Cree PLCC-4
0
4
4
LED_SMD
LED_Cree-PLCC6_4.7x1.5mm
4.7mm x 1.5mm PLCC6 LED, http://www.cree.com/led-components/media/documents/1381-QLS6AFKW.pdf
LED Cree PLCC-6
0
6
6
LED_SMD
LED_Cree-XB
http://www.cree.com/~/media/Files/Cree/LED-Components-and-Modules/XLamp/Data-and-Binning/XLampXBD.pdf
LED Cree XB
0
5
3
LED_SMD
LED_Cree-XH
http://www.cree.com/~/media/Files/Cree/LED-Components-and-Modules/XLamp/Data-and-Binning/ds-XHB.pdf
LED Cree XH
0
8
2
LED_SMD
LED_Cree-XHP35
http://www.cree.com/~/media/Files/Cree/LED-Components-and-Modules/XLamp/Data-and-Binning/ds--XHP35.pdf
LED Cree XHP35
0
6
3
LED_SMD
LED_Cree-XHP50_6V
Cree XHP50, 6V footprint, http://www.cree.com/~/media/Files/Cree/LED%20Components%20and%20Modules/XLamp/Data%20and%20Binning/ds%20XHP50.pdf
LED Cree XHP50
0
17
3
LED_SMD
LED_Cree-XHP50_12V
Cree XHP50, 12V footprint, http://www.cree.com/~/media/Files/Cree/LED%20Components%20and%20Modules/XLamp/Data%20and%20Binning/ds%20XHP50.pdf
LED XHP50 Cree
0
15
3
LED_SMD
LED_Cree-XHP70_6V
Cree XHP70 LED, 6V version, http://www.cree.com/~/media/Files/Cree/LED%20Components%20and%20Modules/XLamp/Data%20and%20Binning/ds%20XHP70.pdf
LED Cree XHP70
0
17
3
LED_SMD
LED_Cree-XHP70_12V
Cree XHP70 LED, 12V version, http://www.cree.com/~/media/Files/Cree/LED%20Components%20and%20Modules/XLamp/Data%20and%20Binning/ds%20XHP70.pdf
LED Cree XHP70
0
15
3
LED_SMD
LED_Cree-XP
LED Cree-XP http://www.cree.com/~/media/Files/Cree/LED-Components-and-Modules/XLamp/Data-and-Binning/XLampXPE2.pdf
LED Cree XP
0
6
3
LED_SMD
LED_Cree-XP-G
LED Cree-XP-G http://www.cree.com/~/media/Files/Cree/LED%20Components%20and%20Modules/XLamp/Data%20and%20Binning/XLampXPG.pdf
LED Cree XP-G
0
6
3
LED_SMD
LED_Cree-XQ
LED Cree-XQ http://www.cree.com/~/media/Files/Cree/LED-Components-and-Modules/XLamp/Data-and-Binning/ds-XQB.pdf
LED Cree XQ
0
2
2
LED_SMD
LED_Cree-XQ_HandSoldering
LED Cree-XQ handsoldering pads http://www.cree.com/~/media/Files/Cree/LED-Components-and-Modules/XLamp/Data-and-Binning/ds-XQB.pdf
LED Cree XQ
0
2
2
LED_SMD
LED_Dialight_591
LED SMD 3mm Right Angle series (http://www.dialightsignalsandcomponents.com/Assets/Drawings/2D_Drawings_DrawingDetailedSpec/C17354.pdf)
LED Dialight 591
0
2
2
LED_SMD
LED_Inolux_IN-PI554FCH_PLCC4_5.0x5.0mm_P3.2mm
http://www.inolux-corp.com/datasheet/SMDLED/Addressable%20LED/IN-PI554FCH.pdf
RGB LED NeoPixel addressable
0
4
4
LED_SMD
LED_Kingbright_AAA3528ESGCT
Kingbright, dual LED, 3.5 x 2.8 mm Surface Mount LED Lamp (http://www.kingbrightusa.com/images/catalog/SPEC/AAA3528ESGCT.pdf)
dual led smd
0
4
4
LED_SMD
LED_Kingbright_APFA3010_3x1.5mm_Horizontal
LED RGB, APFA3010, http://www.kingbrightusa.com/images/catalog/SPEC/APFA3010LSEEZGKQBKC.pdf
LED RGB APFA3010 KINGBRIGHT 3x1.5mm
0
4
4
LED_SMD
LED_LiteOn_LTST-C19HE1WT
LiteOn RGB LED; https://optoelectronics.liteon.com/upload/download/DS22-2008-0044/LTST-C19HE1WT.pdf
LED RGB Chip SMD
0
4
4
LED_SMD
LED_LiteOn_LTST-S326
http://optoelectronics.liteon.com/upload/download/DS22-2000-287/LTST-S326KGJRKT.PDF
LED SMD right angle  CCA
0
3
3
LED_SMD
LED_Osram_Lx_P47F_D2mm_ReverseMount
OSRAM, reverse-mount LED, SMD, 2mm diameter, http://www.farnell.com/datasheets/2711587.pdf
LED ReverseMount Reverse
0
4
2
LED_SMD
LED_PLCC-2
LED PLCC-2 SMD package
LED PLCC-2 SMD
0
2
2
LED_SMD
LED_PLCC_2835
https://www.luckylight.cn/media/component/data-sheet/R2835BC-B2M-M10.pdf
LED
0
2
2
LED_SMD
LED_PLCC_2835_Handsoldering
https://www.luckylight.cn/media/component/data-sheet/R2835BC-B2M-M10.pdf
LED
0
2
2
LED_SMD
LED_RGB_1210
RGB LED 3.2x2.7mm http://www.avagotech.com/docs/AV02-0610EN
LED 3227
0
4
4
LED_SMD
LED_RGB_5050-6
http://cdn.sparkfun.com/datasheets/Components/LED/5060BRG4.pdf
RGB LED 5050-6
0
6
6
LED_SMD
LED_RGB_Cree-PLCC-6_6x5mm_P2.1mm
http://www.farnell.com/datasheets/2003905.pdf
LED RGB PLCC-6 CLP6C-FBK
0
6
6
LED_SMD
LED_RGB_Getian_GT-P6PRGB4303
https://www.gme.sk/img/cache/doc/518/177/vykonova-led-getian-gt-p6prgb4303-datasheet-1.pdf
LED RGB 
0
7
7
LED_SMD
LED_RGB_PLCC-6
RGB LED PLCC-6
RGB LED PLCC-6
0
6
6
LED_SMD
LED_ROHM_SMLVN6
https://www.rohm.com/datasheet/SMLVN6RGB1U
LED ROHM SMLVN6
0
6
6
LED_SMD
LED_SK6805_PLCC4_2.4x2.7mm_P1.3mm
https://cdn-shop.adafruit.com/product-files/3484/3484_Datasheet.pdf
LED RGB NeoPixel Nano
0
4
4
LED_SMD
LED_SK6812MINI_PLCC4_3.5x3.5mm_P1.75mm
https://cdn-shop.adafruit.com/product-files/2686/SK6812MINI_REV.01-1-2.pdf
LED RGB NeoPixel Mini
0
4
4
LED_SMD
LED_SK6812_EC15_1.5x1.5mm
http://www.newstar-ledstrip.com/product/20181119172602110.pdf
LED RGB NeoPixel
0
4
4
LED_SMD
LED_SK6812_PLCC4_5.0x5.0mm_P3.2mm
https://cdn-shop.adafruit.com/product-files/1138/SK6812+LED+datasheet+.pdf
LED RGB NeoPixel
0
4
4
LED_SMD
LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm
https://cdn-shop.adafruit.com/datasheets/WS2812B.pdf
LED RGB NeoPixel
0
4
4
LED_SMD
LED_WS2812_PLCC6_5.0x5.0mm_P1.6mm
https://cdn-shop.adafruit.com/datasheets/WS2812.pdf
LED RGB NeoPixel
0
6
6
LED_SMD
LED_Yuji_5730
LED,Yuji,5730,https://cdn.shopify.com/s/files/1/0344/6401/files/YJWJ014-1.1_YJ-BC-5730L-G02.pdf
LED Yuji 5730
0
3
2
LED_SMD
LED_miniPLCC_2315
https://docs.broadcom.com/cs/Satellite?blobcol=urldata&blobheader=application%2Fpdf&blobheadername1=Content-Disposition&blobheadername2=Content-Type&blobheadername3=MDT-Type&blobheadervalue1=attachment%3Bfilename%3DAV02-2205EN_DS_ASMT-TxBM_2014-05-09.pdf&blobheadervalue2=application%2Fx-download&blobheadervalue3=abinary%253B%2Bcharset%253DUTF-8&blobkey=id&blobnocache=true&blobtable=MungoBlobs&blobwhere=1430858274704&ssbinary=true
LED
0
2
2
LED_SMD
LED_miniPLCC_2315_Handsoldering
https://docs.broadcom.com/cs/Satellite?blobcol=urldata&blobheader=application%2Fpdf&blobheadername1=Content-Disposition&blobheadername2=Content-Type&blobheadername3=MDT-Type&blobheadervalue1=attachment%3Bfilename%3DAV02-2205EN_DS_ASMT-TxBM_2014-05-09.pdf&blobheadervalue2=application%2Fx-download&blobheadervalue3=abinary%253B%2Bcharset%253DUTF-8&blobkey=id&blobnocache=true&blobtable=MungoBlobs&blobwhere=1430858274704&ssbinary=true
LED
0
2
2
LED_THT
LED_BL-FL7680RGB
'Piranha' RGB LED, through hole, common anode, 7.62x7.62mm, BGRA pin order, https://cdn-shop.adafruit.com/datasheets/BL-FL7680RGB.pdf
RGB LED Piranha Super-Flux BetLux
0
4
4
LED_THT
LED_D1.8mm_W1.8mm_H2.4mm_Horizontal_O1.27mm_Z1.6mm
LED, ,  diameter 1.8mm size 1.8x2.4mm^2 z-position of LED center 1.6mm, 2 pins
LED   diameter 1.8mm size 1.8x2.4mm^2 z-position of LED center 1.6mm 2 pins
0
2
2
LED_THT
LED_D1.8mm_W1.8mm_H2.4mm_Horizontal_O1.27mm_Z4.9mm
LED, ,  diameter 1.8mm size 1.8x2.4mm^2 z-position of LED center 1.6mm, 2 pins,  diameter 1.8mm size 1.8x2.4mm^2 z-position of LED center 1.6mm, 2 pins,  diameter 1.8mm size 1.8x2.4mm^2 z-position of LED center 1.6mm, 2 pins,  diameter 1.8mm size 1.8x2.4mm^2 z-position of LED center 4.9mm, 2 pins
LED   diameter 1.8mm size 1.8x2.4mm^2 z-position of LED center 1.6mm 2 pins  diameter 1.8mm size 1.8x2.4mm^2 z-position of LED center 1.6mm 2 pins  diameter 1.8mm size 1.8x2.4mm^2 z-position of LED center 1.6mm 2 pins  diameter 1.8mm size 1.8x2.4mm^2 z-position of LED center 4.9mm 2 pins
0
2
2
LED_THT
LED_D1.8mm_W1.8mm_H2.4mm_Horizontal_O1.27mm_Z8.2mm
LED, ,  diameter 1.8mm size 1.8x2.4mm^2 z-position of LED center 1.6mm, 2 pins,  diameter 1.8mm size 1.8x2.4mm^2 z-position of LED center 1.6mm, 2 pins,  diameter 1.8mm size 1.8x2.4mm^2 z-position of LED center 1.6mm, 2 pins,  diameter 1.8mm size 1.8x2.4mm^2 z-position of LED center 4.9mm, 2 pins,  diameter 1.8mm size 1.8x2.4mm^2 z-position of LED center 4.9mm, 2 pins,  diameter 1.8mm size 1.8x2.4mm^2 z-position of LED center 4.9mm, 2 pins,  diameter 1.8mm size 1.8x2.4mm^2 z-position of LED center 8.2mm, 2 pins
LED   diameter 1.8mm size 1.8x2.4mm^2 z-position of LED center 1.6mm 2 pins  diameter 1.8mm size 1.8x2.4mm^2 z-position of LED center 1.6mm 2 pins  diameter 1.8mm size 1.8x2.4mm^2 z-position of LED center 1.6mm 2 pins  diameter 1.8mm size 1.8x2.4mm^2 z-position of LED center 4.9mm 2 pins  diameter 1.8mm size 1.8x2.4mm^2 z-position of LED center 4.9mm 2 pins  diameter 1.8mm size 1.8x2.4mm^2 z-position of LED center 4.9mm 2 pins  diameter 1.8mm size 1.8x2.4mm^2 z-position of LED center 8.2mm 2 pins
0
2
2
LED_THT
LED_D1.8mm_W1.8mm_H2.4mm_Horizontal_O3.81mm_Z1.6mm
LED, ,  diameter 1.8mm size 1.8x2.4mm^2 z-position of LED center 1.6mm, 2 pins,  diameter 1.8mm size 1.8x2.4mm^2 z-position of LED center 1.6mm, 2 pins
LED   diameter 1.8mm size 1.8x2.4mm^2 z-position of LED center 1.6mm 2 pins  diameter 1.8mm size 1.8x2.4mm^2 z-position of LED center 1.6mm 2 pins
0
2
2
LED_THT
LED_D1.8mm_W1.8mm_H2.4mm_Horizontal_O3.81mm_Z4.9mm
LED, ,  diameter 1.8mm size 1.8x2.4mm^2 z-position of LED center 1.6mm, 2 pins,  diameter 1.8mm size 1.8x2.4mm^2 z-position of LED center 1.6mm, 2 pins,  diameter 1.8mm size 1.8x2.4mm^2 z-position of LED center 1.6mm, 2 pins,  diameter 1.8mm size 1.8x2.4mm^2 z-position of LED center 4.9mm, 2 pins,  diameter 1.8mm size 1.8x2.4mm^2 z-position of LED center 4.9mm, 2 pins
LED   diameter 1.8mm size 1.8x2.4mm^2 z-position of LED center 1.6mm 2 pins  diameter 1.8mm size 1.8x2.4mm^2 z-position of LED center 1.6mm 2 pins  diameter 1.8mm size 1.8x2.4mm^2 z-position of LED center 1.6mm 2 pins  diameter 1.8mm size 1.8x2.4mm^2 z-position of LED center 4.9mm 2 pins  diameter 1.8mm size 1.8x2.4mm^2 z-position of LED center 4.9mm 2 pins
0
2
2
LED_THT
LED_D1.8mm_W1.8mm_H2.4mm_Horizontal_O3.81mm_Z8.2mm
LED, ,  diameter 1.8mm size 1.8x2.4mm^2 z-position of LED center 1.6mm, 2 pins,  diameter 1.8mm size 1.8x2.4mm^2 z-position of LED center 1.6mm, 2 pins,  diameter 1.8mm size 1.8x2.4mm^2 z-position of LED center 1.6mm, 2 pins,  diameter 1.8mm size 1.8x2.4mm^2 z-position of LED center 4.9mm, 2 pins,  diameter 1.8mm size 1.8x2.4mm^2 z-position of LED center 4.9mm, 2 pins,  diameter 1.8mm size 1.8x2.4mm^2 z-position of LED center 4.9mm, 2 pins,  diameter 1.8mm size 1.8x2.4mm^2 z-position of LED center 8.2mm, 2 pins,  diameter 1.8mm size 1.8x2.4mm^2 z-position of LED center 8.2mm, 2 pins
LED   diameter 1.8mm size 1.8x2.4mm^2 z-position of LED center 1.6mm 2 pins  diameter 1.8mm size 1.8x2.4mm^2 z-position of LED center 1.6mm 2 pins  diameter 1.8mm size 1.8x2.4mm^2 z-position of LED center 1.6mm 2 pins  diameter 1.8mm size 1.8x2.4mm^2 z-position of LED center 4.9mm 2 pins  diameter 1.8mm size 1.8x2.4mm^2 z-position of LED center 4.9mm 2 pins  diameter 1.8mm size 1.8x2.4mm^2 z-position of LED center 4.9mm 2 pins  diameter 1.8mm size 1.8x2.4mm^2 z-position of LED center 8.2mm 2 pins  diameter 1.8mm size 1.8x2.4mm^2 z-position of LED center 8.2mm 2 pins
0
2
2
LED_THT
LED_D1.8mm_W1.8mm_H2.4mm_Horizontal_O6.35mm_Z1.6mm
LED, ,  diameter 1.8mm size 1.8x2.4mm^2 z-position of LED center 1.6mm, 2 pins,  diameter 1.8mm size 1.8x2.4mm^2 z-position of LED center 1.6mm, 2 pins,  diameter 1.8mm size 1.8x2.4mm^2 z-position of LED center 1.6mm, 2 pins
LED   diameter 1.8mm size 1.8x2.4mm^2 z-position of LED center 1.6mm 2 pins  diameter 1.8mm size 1.8x2.4mm^2 z-position of LED center 1.6mm 2 pins  diameter 1.8mm size 1.8x2.4mm^2 z-position of LED center 1.6mm 2 pins
0
2
2
LED_THT
LED_D1.8mm_W1.8mm_H2.4mm_Horizontal_O6.35mm_Z4.9mm
LED, ,  diameter 1.8mm size 1.8x2.4mm^2 z-position of LED center 1.6mm, 2 pins,  diameter 1.8mm size 1.8x2.4mm^2 z-position of LED center 1.6mm, 2 pins,  diameter 1.8mm size 1.8x2.4mm^2 z-position of LED center 1.6mm, 2 pins,  diameter 1.8mm size 1.8x2.4mm^2 z-position of LED center 4.9mm, 2 pins,  diameter 1.8mm size 1.8x2.4mm^2 z-position of LED center 4.9mm, 2 pins,  diameter 1.8mm size 1.8x2.4mm^2 z-position of LED center 4.9mm, 2 pins
LED   diameter 1.8mm size 1.8x2.4mm^2 z-position of LED center 1.6mm 2 pins  diameter 1.8mm size 1.8x2.4mm^2 z-position of LED center 1.6mm 2 pins  diameter 1.8mm size 1.8x2.4mm^2 z-position of LED center 1.6mm 2 pins  diameter 1.8mm size 1.8x2.4mm^2 z-position of LED center 4.9mm 2 pins  diameter 1.8mm size 1.8x2.4mm^2 z-position of LED center 4.9mm 2 pins  diameter 1.8mm size 1.8x2.4mm^2 z-position of LED center 4.9mm 2 pins
0
2
2
LED_THT
LED_D1.8mm_W1.8mm_H2.4mm_Horizontal_O6.35mm_Z8.2mm
LED, ,  diameter 1.8mm size 1.8x2.4mm^2 z-position of LED center 1.6mm, 2 pins,  diameter 1.8mm size 1.8x2.4mm^2 z-position of LED center 1.6mm, 2 pins,  diameter 1.8mm size 1.8x2.4mm^2 z-position of LED center 1.6mm, 2 pins,  diameter 1.8mm size 1.8x2.4mm^2 z-position of LED center 4.9mm, 2 pins,  diameter 1.8mm size 1.8x2.4mm^2 z-position of LED center 4.9mm, 2 pins,  diameter 1.8mm size 1.8x2.4mm^2 z-position of LED center 4.9mm, 2 pins,  diameter 1.8mm size 1.8x2.4mm^2 z-position of LED center 8.2mm, 2 pins,  diameter 1.8mm size 1.8x2.4mm^2 z-position of LED center 8.2mm, 2 pins,  diameter 1.8mm size 1.8x2.4mm^2 z-position of LED center 8.2mm, 2 pins
LED   diameter 1.8mm size 1.8x2.4mm^2 z-position of LED center 1.6mm 2 pins  diameter 1.8mm size 1.8x2.4mm^2 z-position of LED center 1.6mm 2 pins  diameter 1.8mm size 1.8x2.4mm^2 z-position of LED center 1.6mm 2 pins  diameter 1.8mm size 1.8x2.4mm^2 z-position of LED center 4.9mm 2 pins  diameter 1.8mm size 1.8x2.4mm^2 z-position of LED center 4.9mm 2 pins  diameter 1.8mm size 1.8x2.4mm^2 z-position of LED center 4.9mm 2 pins  diameter 1.8mm size 1.8x2.4mm^2 z-position of LED center 8.2mm 2 pins  diameter 1.8mm size 1.8x2.4mm^2 z-position of LED center 8.2mm 2 pins  diameter 1.8mm size 1.8x2.4mm^2 z-position of LED center 8.2mm 2 pins
0
2
2
LED_THT
LED_D1.8mm_W3.3mm_H2.4mm
LED, Round,  Rectangular size 3.3x2.4mm^2 diameter 1.8mm, 2 pins
LED Round  Rectangular size 3.3x2.4mm^2 diameter 1.8mm 2 pins
0
2
2
LED_THT
LED_D2.0mm_W4.0mm_H2.8mm_FlatTop
LED, Round, FlatTop,  Rectangular size 4.0x2.8mm^2 diameter 2.0mm, 2 pins, http://www.kingbright.com/attachments/file/psearch/000/00/00/L-1034IDT(Ver.9A).pdf
LED Round FlatTop  Rectangular size 4.0x2.8mm^2 diameter 2.0mm 2 pins
0
2
2
LED_THT
LED_D2.0mm_W4.8mm_H2.5mm_FlatTop
LED, Round, FlatTop,  Rectangular size 4.8x2.5mm^2 diameter 2.0mm, 2 pins, http://www.kingbright.com/attachments/file/psearch/000/00/00/L-13GD(Ver.11B).pdf
LED Round FlatTop  Rectangular size 4.8x2.5mm^2 diameter 2.0mm 2 pins
0
2
2
LED_THT
LED_D3.0mm
LED, diameter 3.0mm, 2 pins
LED diameter 3.0mm 2 pins
0
2
2
LED_THT
LED_D3.0mm-3
LED, diameter 3.0mm, 2 pins, diameter 3.0mm, 3 pins, http://www.kingbright.com/attachments/file/psearch/000/00/00/L-3VSURKCGKC(Ver.8A).pdf
LED diameter 3.0mm 2 pins diameter 3.0mm 3 pins
0
3
3
LED_THT
LED_D3.0mm_Clear
IR-LED, diameter 3.0mm, 2 pins, color: clear
IR infrared LED diameter 3.0mm 2 pins clear
0
2
2
LED_THT
LED_D3.0mm_FlatTop
LED, Round, FlatTop, diameter 3.0mm, 2 pins, http://www.kingbright.com/attachments/file/psearch/000/00/00/L-47XEC(Ver.9A).pdf
LED Round FlatTop diameter 3.0mm 2 pins
0
2
2
LED_THT
LED_D3.0mm_Horizontal_O1.27mm_Z2.0mm
LED, diameter 3.0mm z-position of LED center 2.0mm, 2 pins
LED diameter 3.0mm z-position of LED center 2.0mm 2 pins
0
2
2
LED_THT
LED_D3.0mm_Horizontal_O1.27mm_Z2.0mm_Clear
LED, diameter 3.0mm z-position of LED center 2.0mm, 2 pins
LED diameter 3.0mm z-position of LED center 2.0mm 2 pins
0
2
2
LED_THT
LED_D3.0mm_Horizontal_O1.27mm_Z2.0mm_IRBlack
LED, diameter 3.0mm z-position of LED center 2.0mm, 2 pins
LED diameter 3.0mm z-position of LED center 2.0mm 2 pins
0
2
2
LED_THT
LED_D3.0mm_Horizontal_O1.27mm_Z2.0mm_IRGrey
LED, diameter 3.0mm z-position of LED center 2.0mm, 2 pins
LED diameter 3.0mm z-position of LED center 2.0mm 2 pins
0
2
2
LED_THT
LED_D3.0mm_Horizontal_O1.27mm_Z6.0mm
LED, diameter 3.0mm z-position of LED center 2.0mm, 2 pins, diameter 3.0mm z-position of LED center 2.0mm, 2 pins, diameter 3.0mm z-position of LED center 2.0mm, 2 pins, diameter 3.0mm z-position of LED center 6.0mm, 2 pins
LED diameter 3.0mm z-position of LED center 2.0mm 2 pins diameter 3.0mm z-position of LED center 2.0mm 2 pins diameter 3.0mm z-position of LED center 2.0mm 2 pins diameter 3.0mm z-position of LED center 6.0mm 2 pins
0
2
2
LED_THT
LED_D3.0mm_Horizontal_O1.27mm_Z10.0mm
LED, diameter 3.0mm z-position of LED center 2.0mm, 2 pins, diameter 3.0mm z-position of LED center 2.0mm, 2 pins, diameter 3.0mm z-position of LED center 2.0mm, 2 pins, diameter 3.0mm z-position of LED center 6.0mm, 2 pins, diameter 3.0mm z-position of LED center 6.0mm, 2 pins, diameter 3.0mm z-position of LED center 6.0mm, 2 pins, diameter 3.0mm z-position of LED center 10.0mm, 2 pins
LED diameter 3.0mm z-position of LED center 2.0mm 2 pins diameter 3.0mm z-position of LED center 2.0mm 2 pins diameter 3.0mm z-position of LED center 2.0mm 2 pins diameter 3.0mm z-position of LED center 6.0mm 2 pins diameter 3.0mm z-position of LED center 6.0mm 2 pins diameter 3.0mm z-position of LED center 6.0mm 2 pins diameter 3.0mm z-position of LED center 10.0mm 2 pins
0
2
2
LED_THT
LED_D3.0mm_Horizontal_O3.81mm_Z2.0mm
LED, diameter 3.0mm z-position of LED center 2.0mm, 2 pins, diameter 3.0mm z-position of LED center 2.0mm, 2 pins
LED diameter 3.0mm z-position of LED center 2.0mm 2 pins diameter 3.0mm z-position of LED center 2.0mm 2 pins
0
2
2
LED_THT
LED_D3.0mm_Horizontal_O3.81mm_Z6.0mm
LED, diameter 3.0mm z-position of LED center 2.0mm, 2 pins, diameter 3.0mm z-position of LED center 2.0mm, 2 pins, diameter 3.0mm z-position of LED center 2.0mm, 2 pins, diameter 3.0mm z-position of LED center 6.0mm, 2 pins, diameter 3.0mm z-position of LED center 6.0mm, 2 pins
LED diameter 3.0mm z-position of LED center 2.0mm 2 pins diameter 3.0mm z-position of LED center 2.0mm 2 pins diameter 3.0mm z-position of LED center 2.0mm 2 pins diameter 3.0mm z-position of LED center 6.0mm 2 pins diameter 3.0mm z-position of LED center 6.0mm 2 pins
0
2
2
LED_THT
LED_D3.0mm_Horizontal_O3.81mm_Z10.0mm
LED, diameter 3.0mm z-position of LED center 2.0mm, 2 pins, diameter 3.0mm z-position of LED center 2.0mm, 2 pins, diameter 3.0mm z-position of LED center 2.0mm, 2 pins, diameter 3.0mm z-position of LED center 6.0mm, 2 pins, diameter 3.0mm z-position of LED center 6.0mm, 2 pins, diameter 3.0mm z-position of LED center 6.0mm, 2 pins, diameter 3.0mm z-position of LED center 10.0mm, 2 pins, diameter 3.0mm z-position of LED center 10.0mm, 2 pins
LED diameter 3.0mm z-position of LED center 2.0mm 2 pins diameter 3.0mm z-position of LED center 2.0mm 2 pins diameter 3.0mm z-position of LED center 2.0mm 2 pins diameter 3.0mm z-position of LED center 6.0mm 2 pins diameter 3.0mm z-position of LED center 6.0mm 2 pins diameter 3.0mm z-position of LED center 6.0mm 2 pins diameter 3.0mm z-position of LED center 10.0mm 2 pins diameter 3.0mm z-position of LED center 10.0mm 2 pins
0
2
2
LED_THT
LED_D3.0mm_Horizontal_O6.35mm_Z2.0mm
LED, diameter 3.0mm z-position of LED center 2.0mm, 2 pins, diameter 3.0mm z-position of LED center 2.0mm, 2 pins, diameter 3.0mm z-position of LED center 2.0mm, 2 pins
LED diameter 3.0mm z-position of LED center 2.0mm 2 pins diameter 3.0mm z-position of LED center 2.0mm 2 pins diameter 3.0mm z-position of LED center 2.0mm 2 pins
0
2
2
LED_THT
LED_D3.0mm_Horizontal_O6.35mm_Z6.0mm
LED, diameter 3.0mm z-position of LED center 2.0mm, 2 pins, diameter 3.0mm z-position of LED center 2.0mm, 2 pins, diameter 3.0mm z-position of LED center 2.0mm, 2 pins, diameter 3.0mm z-position of LED center 6.0mm, 2 pins, diameter 3.0mm z-position of LED center 6.0mm, 2 pins, diameter 3.0mm z-position of LED center 6.0mm, 2 pins
LED diameter 3.0mm z-position of LED center 2.0mm 2 pins diameter 3.0mm z-position of LED center 2.0mm 2 pins diameter 3.0mm z-position of LED center 2.0mm 2 pins diameter 3.0mm z-position of LED center 6.0mm 2 pins diameter 3.0mm z-position of LED center 6.0mm 2 pins diameter 3.0mm z-position of LED center 6.0mm 2 pins
0
2
2
LED_THT
LED_D3.0mm_Horizontal_O6.35mm_Z10.0mm
LED, diameter 3.0mm z-position of LED center 2.0mm, 2 pins, diameter 3.0mm z-position of LED center 2.0mm, 2 pins, diameter 3.0mm z-position of LED center 2.0mm, 2 pins, diameter 3.0mm z-position of LED center 6.0mm, 2 pins, diameter 3.0mm z-position of LED center 6.0mm, 2 pins, diameter 3.0mm z-position of LED center 6.0mm, 2 pins, diameter 3.0mm z-position of LED center 10.0mm, 2 pins, diameter 3.0mm z-position of LED center 10.0mm, 2 pins, diameter 3.0mm z-position of LED center 10.0mm, 2 pins
LED diameter 3.0mm z-position of LED center 2.0mm 2 pins diameter 3.0mm z-position of LED center 2.0mm 2 pins diameter 3.0mm z-position of LED center 2.0mm 2 pins diameter 3.0mm z-position of LED center 6.0mm 2 pins diameter 3.0mm z-position of LED center 6.0mm 2 pins diameter 3.0mm z-position of LED center 6.0mm 2 pins diameter 3.0mm z-position of LED center 10.0mm 2 pins diameter 3.0mm z-position of LED center 10.0mm 2 pins diameter 3.0mm z-position of LED center 10.0mm 2 pins
0
2
2
LED_THT
LED_D3.0mm_IRBlack
IR-ED, diameter 3.0mm, 2 pins, color: black
IR infrared LED diameter 3.0mm 2 pins black
0
2
2
LED_THT
LED_D3.0mm_IRGrey
IR-LED, diameter 3.0mm, 2 pins, color: grey
IR infrared LED diameter 3.0mm 2 pins grey
0
2
2
LED_THT
LED_D4.0mm
LED, diameter 4.0mm, 2 pins, http://www.kingbright.com/attachments/file/psearch/000/00/00/L-43GD(Ver.12B).pdf
LED diameter 4.0mm 2 pins
0
2
2
LED_THT
LED_D5.0mm
LED, diameter 5.0mm, 2 pins, http://cdn-reichelt.de/documents/datenblatt/A500/LL-504BC2E-009.pdf
LED diameter 5.0mm 2 pins
0
2
2
LED_THT
LED_D5.0mm-3
LED, diameter 5.0mm, 2 pins, diameter 5.0mm, 3 pins, http://www.kingbright.com/attachments/file/psearch/000/00/00/L-59EGC(Ver.17A).pdf
LED diameter 5.0mm 2 pins diameter 5.0mm 3 pins
0
3
3
LED_THT
LED_D5.0mm-3_Horizontal_O3.81mm_Z3.0mm
LED, diameter 5.0mm z-position of LED center 3.0mm, 3 pins, diameter 5.0mm z-position of LED center 3.0mm, 2 pins
LED diameter 5.0mm z-position of LED center 3.0mm 3 pins diameter 5.0mm z-position of LED center 3.0mm 2 pins
0
3
3
LED_THT
LED_D5.0mm-4_RGB
LED, diameter 5.0mm, 2 pins, diameter 5.0mm, 3 pins, diameter 5.0mm, 4 pins, http://www.kingbright.com/attachments/file/psearch/000/00/00/L-154A4SUREQBFZGEW(Ver.9A).pdf
LED diameter 5.0mm 2 pins diameter 5.0mm 3 pins diameter 5.0mm 4 pins RGB RGBLED
0
4
4
LED_THT
LED_D5.0mm-4_RGB_Staggered_Pins
LED, diameter 5.0mm, 2 pins, diameter 5.0mm, 3 pins, diameter 5.0mm, 4 pins, http://www.kingbright.com/attachments/file/psearch/000/00/00/L-154A4SUREQBFZGEW(Ver.9A).pdf
LED diameter 5.0mm 2 pins diameter 5.0mm 3 pins diameter 5.0mm 4 pins RGB RGBLED
0
4
4
LED_THT
LED_D5.0mm-4_RGB_Wide_Pins
LED, diameter 5.0mm, 2 pins, diameter 5.0mm, 3 pins, diameter 5.0mm, 4 pins, http://www.kingbright.com/attachments/file/psearch/000/00/00/L-154A4SUREQBFZGEW(Ver.9A).pdf
LED diameter 5.0mm 2 pins diameter 5.0mm 3 pins diameter 5.0mm 4 pins RGB RGBLED
0
4
4
LED_THT
LED_D5.0mm_Clear
LED, diameter 5.0mm, 2 pins, http://cdn-reichelt.de/documents/datenblatt/A500/LL-504BC2E-009.pdf
LED diameter 5.0mm 2 pins
0
2
2
LED_THT
LED_D5.0mm_FlatTop
LED, Round, FlatTop, diameter 5.0mm, 2 pins, http://www.kingbright.com/attachments/file/psearch/000/00/00/L-483GDT(Ver.15B).pdf
LED Round FlatTop diameter 5.0mm 2 pins
0
2
2
LED_THT
LED_D5.0mm_Horizontal_O1.27mm_Z3.0mm
LED, diameter 5.0mm z-position of LED center 3.0mm, 2 pins
LED diameter 5.0mm z-position of LED center 3.0mm 2 pins
0
2
2
LED_THT
LED_D5.0mm_Horizontal_O1.27mm_Z3.0mm_Clear
LED, diameter 5.0mm z-position of LED center 3.0mm, 2 pins
LED diameter 5.0mm z-position of LED center 3.0mm 2 pins
0
2
2
LED_THT
LED_D5.0mm_Horizontal_O1.27mm_Z3.0mm_IRBlack
LED, diameter 5.0mm z-position of LED center 3.0mm, 2 pins
LED diameter 5.0mm z-position of LED center 3.0mm 2 pins
0
2
2
LED_THT
LED_D5.0mm_Horizontal_O1.27mm_Z3.0mm_IRGrey
LED, diameter 5.0mm z-position of LED center 3.0mm, 2 pins
LED diameter 5.0mm z-position of LED center 3.0mm 2 pins
0
2
2
LED_THT
LED_D5.0mm_Horizontal_O1.27mm_Z9.0mm
LED, diameter 5.0mm z-position of LED center 3.0mm, 2 pins, diameter 5.0mm z-position of LED center 3.0mm, 2 pins, diameter 5.0mm z-position of LED center 3.0mm, 2 pins, diameter 5.0mm z-position of LED center 9.0mm, 2 pins
LED diameter 5.0mm z-position of LED center 3.0mm 2 pins diameter 5.0mm z-position of LED center 3.0mm 2 pins diameter 5.0mm z-position of LED center 3.0mm 2 pins diameter 5.0mm z-position of LED center 9.0mm 2 pins
0
2
2
LED_THT
LED_D5.0mm_Horizontal_O1.27mm_Z15.0mm
LED, diameter 5.0mm z-position of LED center 3.0mm, 2 pins, diameter 5.0mm z-position of LED center 3.0mm, 2 pins, diameter 5.0mm z-position of LED center 3.0mm, 2 pins, diameter 5.0mm z-position of LED center 9.0mm, 2 pins, diameter 5.0mm z-position of LED center 9.0mm, 2 pins, diameter 5.0mm z-position of LED center 9.0mm, 2 pins, diameter 5.0mm z-position of LED center 15.0mm, 2 pins
LED diameter 5.0mm z-position of LED center 3.0mm 2 pins diameter 5.0mm z-position of LED center 3.0mm 2 pins diameter 5.0mm z-position of LED center 3.0mm 2 pins diameter 5.0mm z-position of LED center 9.0mm 2 pins diameter 5.0mm z-position of LED center 9.0mm 2 pins diameter 5.0mm z-position of LED center 9.0mm 2 pins diameter 5.0mm z-position of LED center 15.0mm 2 pins
0
2
2
LED_THT
LED_D5.0mm_Horizontal_O3.81mm_Z3.0mm
LED, diameter 5.0mm z-position of LED center 3.0mm, 2 pins, diameter 5.0mm z-position of LED center 3.0mm, 2 pins
LED diameter 5.0mm z-position of LED center 3.0mm 2 pins diameter 5.0mm z-position of LED center 3.0mm 2 pins
0
2
2
LED_THT
LED_D5.0mm_Horizontal_O3.81mm_Z9.0mm
LED, diameter 5.0mm z-position of LED center 3.0mm, 2 pins, diameter 5.0mm z-position of LED center 3.0mm, 2 pins, diameter 5.0mm z-position of LED center 3.0mm, 2 pins, diameter 5.0mm z-position of LED center 9.0mm, 2 pins, diameter 5.0mm z-position of LED center 9.0mm, 2 pins
LED diameter 5.0mm z-position of LED center 3.0mm 2 pins diameter 5.0mm z-position of LED center 3.0mm 2 pins diameter 5.0mm z-position of LED center 3.0mm 2 pins diameter 5.0mm z-position of LED center 9.0mm 2 pins diameter 5.0mm z-position of LED center 9.0mm 2 pins
0
2
2
LED_THT
LED_D5.0mm_Horizontal_O3.81mm_Z15.0mm
LED, diameter 5.0mm z-position of LED center 3.0mm, 2 pins, diameter 5.0mm z-position of LED center 3.0mm, 2 pins, diameter 5.0mm z-position of LED center 3.0mm, 2 pins, diameter 5.0mm z-position of LED center 9.0mm, 2 pins, diameter 5.0mm z-position of LED center 9.0mm, 2 pins, diameter 5.0mm z-position of LED center 9.0mm, 2 pins, diameter 5.0mm z-position of LED center 15.0mm, 2 pins, diameter 5.0mm z-position of LED center 15.0mm, 2 pins
LED diameter 5.0mm z-position of LED center 3.0mm 2 pins diameter 5.0mm z-position of LED center 3.0mm 2 pins diameter 5.0mm z-position of LED center 3.0mm 2 pins diameter 5.0mm z-position of LED center 9.0mm 2 pins diameter 5.0mm z-position of LED center 9.0mm 2 pins diameter 5.0mm z-position of LED center 9.0mm 2 pins diameter 5.0mm z-position of LED center 15.0mm 2 pins diameter 5.0mm z-position of LED center 15.0mm 2 pins
0
2
2
LED_THT
LED_D5.0mm_Horizontal_O6.35mm_Z3.0mm
LED, diameter 5.0mm z-position of LED center 3.0mm, 2 pins, diameter 5.0mm z-position of LED center 3.0mm, 2 pins, diameter 5.0mm z-position of LED center 3.0mm, 2 pins
LED diameter 5.0mm z-position of LED center 3.0mm 2 pins diameter 5.0mm z-position of LED center 3.0mm 2 pins diameter 5.0mm z-position of LED center 3.0mm 2 pins
0
2
2
LED_THT
LED_D5.0mm_Horizontal_O6.35mm_Z9.0mm
LED, diameter 5.0mm z-position of LED center 3.0mm, 2 pins, diameter 5.0mm z-position of LED center 3.0mm, 2 pins, diameter 5.0mm z-position of LED center 3.0mm, 2 pins, diameter 5.0mm z-position of LED center 9.0mm, 2 pins, diameter 5.0mm z-position of LED center 9.0mm, 2 pins, diameter 5.0mm z-position of LED center 9.0mm, 2 pins
LED diameter 5.0mm z-position of LED center 3.0mm 2 pins diameter 5.0mm z-position of LED center 3.0mm 2 pins diameter 5.0mm z-position of LED center 3.0mm 2 pins diameter 5.0mm z-position of LED center 9.0mm 2 pins diameter 5.0mm z-position of LED center 9.0mm 2 pins diameter 5.0mm z-position of LED center 9.0mm 2 pins
0
2
2
LED_THT
LED_D5.0mm_Horizontal_O6.35mm_Z15.0mm
LED, diameter 5.0mm z-position of LED center 3.0mm, 2 pins, diameter 5.0mm z-position of LED center 3.0mm, 2 pins, diameter 5.0mm z-position of LED center 3.0mm, 2 pins, diameter 5.0mm z-position of LED center 9.0mm, 2 pins, diameter 5.0mm z-position of LED center 9.0mm, 2 pins, diameter 5.0mm z-position of LED center 9.0mm, 2 pins, diameter 5.0mm z-position of LED center 15.0mm, 2 pins, diameter 5.0mm z-position of LED center 15.0mm, 2 pins, diameter 5.0mm z-position of LED center 15.0mm, 2 pins
LED diameter 5.0mm z-position of LED center 3.0mm 2 pins diameter 5.0mm z-position of LED center 3.0mm 2 pins diameter 5.0mm z-position of LED center 3.0mm 2 pins diameter 5.0mm z-position of LED center 9.0mm 2 pins diameter 5.0mm z-position of LED center 9.0mm 2 pins diameter 5.0mm z-position of LED center 9.0mm 2 pins diameter 5.0mm z-position of LED center 15.0mm 2 pins diameter 5.0mm z-position of LED center 15.0mm 2 pins diameter 5.0mm z-position of LED center 15.0mm 2 pins
0
2
2
LED_THT
LED_D5.0mm_IRBlack
LED, diameter 5.0mm, 2 pins, http://cdn-reichelt.de/documents/datenblatt/A500/LL-504BC2E-009.pdf
LED diameter 5.0mm 2 pins
0
2
2
LED_THT
LED_D5.0mm_IRGrey
LED, diameter 5.0mm, 2 pins, http://cdn-reichelt.de/documents/datenblatt/A500/LL-504BC2E-009.pdf
LED diameter 5.0mm 2 pins
0
2
2
LED_THT
LED_D8.0mm
LED, diameter 8.0mm, 2 pins, http://cdn-reichelt.de/documents/datenblatt/A500/LED8MMGE_LED8MMGN_LED8MMRT%23KIN.pdf
LED diameter 8.0mm 2 pins
0
2
2
LED_THT
LED_D8.0mm-3
LED, diameter 8.0mm, 2 pins, diameter 8.0mm, 3 pins
LED diameter 8.0mm 2 pins diameter 8.0mm 3 pins
0
3
3
LED_THT
LED_D10.0mm
LED, diameter 10.0mm, 2 pins, http://cdn-reichelt.de/documents/datenblatt/A500/LED10-4500RT%23KIN.pdf
LED diameter 10.0mm 2 pins
0
2
2
LED_THT
LED_D10.0mm-3
LED, diameter 10.0mm, 2 pins, diameter 10.0mm, 3 pins, http://www.kingbright.com/attachments/file/psearch/000/00/00/L-819EGW(Ver.14A).pdf
LED diameter 10.0mm 2 pins diameter 10.0mm 3 pins
0
3
3
LED_THT
LED_D20.0mm
LED, diameter 20.0mm, 2 pins, http://cdn-reichelt.de/documents/datenblatt/A500/DLC2-6GD%28V6%29.pdf
LED diameter 20.0mm 2 pins
0
2
2
LED_THT
LED_Oval_W5.2mm_H3.8mm
LED_Oval, Oval,  Oval size 5.2x3.8mm^2, 2 pins, http://www.kingbright.com/attachments/file/psearch/000/00/00/L-5603QBC-D(Ver.12B).pdf
LED_Oval Oval  Oval size 5.2x3.8mm^2 2 pins
0
2
2
LED_THT
LED_Rectangular_W3.0mm_H2.0mm
LED_Rectangular, Rectangular,  Rectangular size 3.0x2.0mm^2, 2 pins, http://www.kingbright.com/attachments/file/psearch/000/00/00/L-169XCGDK(Ver.9B).pdf
LED_Rectangular Rectangular  Rectangular size 3.0x2.0mm^2 2 pins
0
2
2
LED_THT
LED_Rectangular_W3.9mm_H1.8mm
LED_Rectangular, Rectangular,  Rectangular size 3.9x1.8mm^2, 2 pins, http://www.kingbright.com/attachments/file/psearch/000/00/00/L-2774GD(Ver.7B).pdf
LED_Rectangular Rectangular  Rectangular size 3.9x1.8mm^2 2 pins
0
2
2
LED_THT
LED_Rectangular_W3.9mm_H1.8mm_FlatTop
LED_Rectangular, Rectangular,  Rectangular size 3.9x1.8mm^2, 2 pins, http://www.kingbright.com/attachments/file/psearch/000/00/00/L-2774GD(Ver.7B).pdf
LED_Rectangular Rectangular  Rectangular size 3.9x1.8mm^2 2 pins
0
2
2
LED_THT
LED_Rectangular_W3.9mm_H1.9mm
LED_Rectangular, Rectangular,  Rectangular size 3.9x1.9mm^2, 2 pins, http://www.kingbright.com/attachments/file/psearch/000/00/00/L-144GDT(Ver.14B).pdf
LED_Rectangular Rectangular  Rectangular size 3.9x1.9mm^2 2 pins
0
2
2
LED_THT
LED_Rectangular_W5.0mm_H2.0mm
LED_Rectangular, Rectangular,  Rectangular size 5.0x2.0mm^2, 2 pins, http://www.kingbright.com/attachments/file/psearch/000/00/00/L-169XCGDK(Ver.9B).pdf
LED_Rectangular Rectangular  Rectangular size 5.0x2.0mm^2 2 pins
0
2
2
LED_THT
LED_Rectangular_W5.0mm_H2.0mm-3Pins
LED_Rectangular, Rectangular,  Rectangular size 5.0x2.0mm^2, 3 pins, http://www.kingbright.com/attachments/file/psearch/000/00/00/L-169XCGDK(Ver.9B).pdf
LED_Rectangular Rectangular  Rectangular size 5.0x2.0mm^2 3 pins
0
3
3
LED_THT
LED_Rectangular_W5.0mm_H2.0mm_Horizontal_O1.27mm_Z1.0mm
LED_Rectangular, Rectangular,  Rectangular size 5.0x2.0mm^2 z-position of LED center 1.0mm, 2 pins
LED_Rectangular Rectangular  Rectangular size 5.0x2.0mm^2 z-position of LED center 1.0mm 2 pins
0
2
2
LED_THT
LED_Rectangular_W5.0mm_H2.0mm_Horizontal_O1.27mm_Z3.0mm
LED_Rectangular, Rectangular,  Rectangular size 5.0x2.0mm^2 z-position of LED center 1.0mm, 2 pins,  Rectangular size 5.0x2.0mm^2 z-position of LED center 1.0mm, 2 pins,  Rectangular size 5.0x2.0mm^2 z-position of LED center 1.0mm, 2 pins,  Rectangular size 5.0x2.0mm^2 z-position of LED center 3.0mm, 2 pins
LED_Rectangular Rectangular  Rectangular size 5.0x2.0mm^2 z-position of LED center 1.0mm 2 pins  Rectangular size 5.0x2.0mm^2 z-position of LED center 1.0mm 2 pins  Rectangular size 5.0x2.0mm^2 z-position of LED center 1.0mm 2 pins  Rectangular size 5.0x2.0mm^2 z-position of LED center 3.0mm 2 pins
0
2
2
LED_THT
LED_Rectangular_W5.0mm_H2.0mm_Horizontal_O1.27mm_Z5.0mm
LED_Rectangular, Rectangular,  Rectangular size 5.0x2.0mm^2 z-position of LED center 1.0mm, 2 pins,  Rectangular size 5.0x2.0mm^2 z-position of LED center 1.0mm, 2 pins,  Rectangular size 5.0x2.0mm^2 z-position of LED center 1.0mm, 2 pins,  Rectangular size 5.0x2.0mm^2 z-position of LED center 3.0mm, 2 pins,  Rectangular size 5.0x2.0mm^2 z-position of LED center 3.0mm, 2 pins,  Rectangular size 5.0x2.0mm^2 z-position of LED center 3.0mm, 2 pins,  Rectangular size 5.0x2.0mm^2 z-position of LED center 5.0mm, 2 pins
LED_Rectangular Rectangular  Rectangular size 5.0x2.0mm^2 z-position of LED center 1.0mm 2 pins  Rectangular size 5.0x2.0mm^2 z-position of LED center 1.0mm 2 pins  Rectangular size 5.0x2.0mm^2 z-position of LED center 1.0mm 2 pins  Rectangular size 5.0x2.0mm^2 z-position of LED center 3.0mm 2 pins  Rectangular size 5.0x2.0mm^2 z-position of LED center 3.0mm 2 pins  Rectangular size 5.0x2.0mm^2 z-position of LED center 3.0mm 2 pins  Rectangular size 5.0x2.0mm^2 z-position of LED center 5.0mm 2 pins
0
2
2
LED_THT
LED_Rectangular_W5.0mm_H2.0mm_Horizontal_O3.81mm_Z1.0mm
LED_Rectangular, Rectangular,  Rectangular size 5.0x2.0mm^2 z-position of LED center 1.0mm, 2 pins,  Rectangular size 5.0x2.0mm^2 z-position of LED center 1.0mm, 2 pins
LED_Rectangular Rectangular  Rectangular size 5.0x2.0mm^2 z-position of LED center 1.0mm 2 pins  Rectangular size 5.0x2.0mm^2 z-position of LED center 1.0mm 2 pins
0
2
2
LED_THT
LED_Rectangular_W5.0mm_H2.0mm_Horizontal_O3.81mm_Z3.0mm
LED_Rectangular, Rectangular,  Rectangular size 5.0x2.0mm^2 z-position of LED center 1.0mm, 2 pins,  Rectangular size 5.0x2.0mm^2 z-position of LED center 1.0mm, 2 pins,  Rectangular size 5.0x2.0mm^2 z-position of LED center 1.0mm, 2 pins,  Rectangular size 5.0x2.0mm^2 z-position of LED center 3.0mm, 2 pins,  Rectangular size 5.0x2.0mm^2 z-position of LED center 3.0mm, 2 pins
LED_Rectangular Rectangular  Rectangular size 5.0x2.0mm^2 z-position of LED center 1.0mm 2 pins  Rectangular size 5.0x2.0mm^2 z-position of LED center 1.0mm 2 pins  Rectangular size 5.0x2.0mm^2 z-position of LED center 1.0mm 2 pins  Rectangular size 5.0x2.0mm^2 z-position of LED center 3.0mm 2 pins  Rectangular size 5.0x2.0mm^2 z-position of LED center 3.0mm 2 pins
0
2
2
LED_THT
LED_Rectangular_W5.0mm_H2.0mm_Horizontal_O3.81mm_Z5.0mm
LED_Rectangular, Rectangular,  Rectangular size 5.0x2.0mm^2 z-position of LED center 1.0mm, 2 pins,  Rectangular size 5.0x2.0mm^2 z-position of LED center 1.0mm, 2 pins,  Rectangular size 5.0x2.0mm^2 z-position of LED center 1.0mm, 2 pins,  Rectangular size 5.0x2.0mm^2 z-position of LED center 3.0mm, 2 pins,  Rectangular size 5.0x2.0mm^2 z-position of LED center 3.0mm, 2 pins,  Rectangular size 5.0x2.0mm^2 z-position of LED center 3.0mm, 2 pins,  Rectangular size 5.0x2.0mm^2 z-position of LED center 5.0mm, 2 pins,  Rectangular size 5.0x2.0mm^2 z-position of LED center 5.0mm, 2 pins
LED_Rectangular Rectangular  Rectangular size 5.0x2.0mm^2 z-position of LED center 1.0mm 2 pins  Rectangular size 5.0x2.0mm^2 z-position of LED center 1.0mm 2 pins  Rectangular size 5.0x2.0mm^2 z-position of LED center 1.0mm 2 pins  Rectangular size 5.0x2.0mm^2 z-position of LED center 3.0mm 2 pins  Rectangular size 5.0x2.0mm^2 z-position of LED center 3.0mm 2 pins  Rectangular size 5.0x2.0mm^2 z-position of LED center 3.0mm 2 pins  Rectangular size 5.0x2.0mm^2 z-position of LED center 5.0mm 2 pins  Rectangular size 5.0x2.0mm^2 z-position of LED center 5.0mm 2 pins
0
2
2
LED_THT
LED_Rectangular_W5.0mm_H2.0mm_Horizontal_O6.35mm_Z1.0mm
LED_Rectangular, Rectangular,  Rectangular size 5.0x2.0mm^2 z-position of LED center 1.0mm, 2 pins,  Rectangular size 5.0x2.0mm^2 z-position of LED center 1.0mm, 2 pins,  Rectangular size 5.0x2.0mm^2 z-position of LED center 1.0mm, 2 pins
LED_Rectangular Rectangular  Rectangular size 5.0x2.0mm^2 z-position of LED center 1.0mm 2 pins  Rectangular size 5.0x2.0mm^2 z-position of LED center 1.0mm 2 pins  Rectangular size 5.0x2.0mm^2 z-position of LED center 1.0mm 2 pins
0
2
2
LED_THT
LED_Rectangular_W5.0mm_H2.0mm_Horizontal_O6.35mm_Z3.0mm
LED_Rectangular, Rectangular,  Rectangular size 5.0x2.0mm^2 z-position of LED center 1.0mm, 2 pins,  Rectangular size 5.0x2.0mm^2 z-position of LED center 1.0mm, 2 pins,  Rectangular size 5.0x2.0mm^2 z-position of LED center 1.0mm, 2 pins,  Rectangular size 5.0x2.0mm^2 z-position of LED center 3.0mm, 2 pins,  Rectangular size 5.0x2.0mm^2 z-position of LED center 3.0mm, 2 pins,  Rectangular size 5.0x2.0mm^2 z-position of LED center 3.0mm, 2 pins
LED_Rectangular Rectangular  Rectangular size 5.0x2.0mm^2 z-position of LED center 1.0mm 2 pins  Rectangular size 5.0x2.0mm^2 z-position of LED center 1.0mm 2 pins  Rectangular size 5.0x2.0mm^2 z-position of LED center 1.0mm 2 pins  Rectangular size 5.0x2.0mm^2 z-position of LED center 3.0mm 2 pins  Rectangular size 5.0x2.0mm^2 z-position of LED center 3.0mm 2 pins  Rectangular size 5.0x2.0mm^2 z-position of LED center 3.0mm 2 pins
0
2
2
LED_THT
LED_Rectangular_W5.0mm_H2.0mm_Horizontal_O6.35mm_Z5.0mm
LED_Rectangular, Rectangular,  Rectangular size 5.0x2.0mm^2 z-position of LED center 1.0mm, 2 pins,  Rectangular size 5.0x2.0mm^2 z-position of LED center 1.0mm, 2 pins,  Rectangular size 5.0x2.0mm^2 z-position of LED center 1.0mm, 2 pins,  Rectangular size 5.0x2.0mm^2 z-position of LED center 3.0mm, 2 pins,  Rectangular size 5.0x2.0mm^2 z-position of LED center 3.0mm, 2 pins,  Rectangular size 5.0x2.0mm^2 z-position of LED center 3.0mm, 2 pins,  Rectangular size 5.0x2.0mm^2 z-position of LED center 5.0mm, 2 pins,  Rectangular size 5.0x2.0mm^2 z-position of LED center 5.0mm, 2 pins,  Rectangular size 5.0x2.0mm^2 z-position of LED center 5.0mm, 2 pins
LED_Rectangular Rectangular  Rectangular size 5.0x2.0mm^2 z-position of LED center 1.0mm 2 pins  Rectangular size 5.0x2.0mm^2 z-position of LED center 1.0mm 2 pins  Rectangular size 5.0x2.0mm^2 z-position of LED center 1.0mm 2 pins  Rectangular size 5.0x2.0mm^2 z-position of LED center 3.0mm 2 pins  Rectangular size 5.0x2.0mm^2 z-position of LED center 3.0mm 2 pins  Rectangular size 5.0x2.0mm^2 z-position of LED center 3.0mm 2 pins  Rectangular size 5.0x2.0mm^2 z-position of LED center 5.0mm 2 pins  Rectangular size 5.0x2.0mm^2 z-position of LED center 5.0mm 2 pins  Rectangular size 5.0x2.0mm^2 z-position of LED center 5.0mm 2 pins
0
2
2
LED_THT
LED_Rectangular_W5.0mm_H5.0mm
LED_Rectangular, Rectangular,  Rectangular size 5.0x5.0mm^2, 2 pins, http://www.kingbright.com/attachments/file/psearch/000/00/00/L-169XCGDK(Ver.9B).pdf
LED_Rectangular Rectangular  Rectangular size 5.0x5.0mm^2 2 pins
0
2
2
LED_THT
LED_Rectangular_W7.62mm_H4.55mm_P5.08mm_R3
Datasheet can be found at https://www.gme.cz/data/attachments/dsh.511-795.1.pdf
LED automotive super flux 7.62mm
0
4
2
LED_THT
LED_SideEmitter_Rectangular_W4.5mm_H1.6mm
LED_SideEmitter_Rectangular, Rectangular, SideEmitter,  Rectangular size 4.5x1.6mm^2, 2 pins, http://cdn-reichelt.de/documents/datenblatt/A500/LED15MMGE_LED15MMGN%23KIN.pdf
LED_SideEmitter_Rectangular Rectangular SideEmitter  Rectangular size 4.5x1.6mm^2 2 pins
0
2
2
LED_THT
LED_VCCLite_5381H1_6.35x6.35mm
Red 5381 Series LED VCCLite https://vcclite.com/wp-content/uploads/wpallimport/files/files/5381Series.pdf http://static.vcclite.com/pdf/Mounting%20Hole%20Pattern%202.pdf
Red 5381 Series LED
0
2
2
LED_THT
LED_VCCLite_5381H3_6.35x6.35mm
Amber 5381 Series LED VCCLite https://vcclite.com/wp-content/uploads/wpallimport/files/files/5381Series.pdf http://static.vcclite.com/pdf/Mounting%20Hole%20Pattern%202.pdf
Amber 5381 Series LED
0
2
2
LED_THT
LED_VCCLite_5381H5_6.35x6.35mm
Green 5381 Series LED VCCLite https://vcclite.com/wp-content/uploads/wpallimport/files/files/5381Series.pdf http://static.vcclite.com/pdf/Mounting%20Hole%20Pattern%202.pdf
Green 5381 Series LED
0
2
2
LED_THT
LED_VCCLite_5381H7_6.35x6.35mm
Yellow 5381 Series LED VCCLite https://vcclite.com/wp-content/uploads/wpallimport/files/files/5381Series.pdf http://static.vcclite.com/pdf/Mounting%20Hole%20Pattern%202.pdf
Yellow 5381 Series LED
0
2
2
MountingHole
MountingHole_2.1mm
Mounting Hole 2.1mm, no annular
mounting hole 2.1mm no annular
0
0
0
MountingHole
MountingHole_2.2mm_M2
Mounting Hole 2.2mm, no annular, M2
mounting hole 2.2mm no annular m2
0
0
0
MountingHole
MountingHole_2.2mm_M2_DIN965
Mounting Hole 2.2mm, no annular, M2, DIN965
mounting hole 2.2mm no annular m2 din965
0
0
0
MountingHole
MountingHole_2.2mm_M2_DIN965_Pad
Mounting Hole 2.2mm, M2, DIN965
mounting hole 2.2mm m2 din965
0
1
1
MountingHole
MountingHole_2.2mm_M2_ISO7380
Mounting Hole 2.2mm, no annular, M2, ISO7380
mounting hole 2.2mm no annular m2 iso7380
0
0
0
MountingHole
MountingHole_2.2mm_M2_ISO7380_Pad
Mounting Hole 2.2mm, M2, ISO7380
mounting hole 2.2mm m2 iso7380
0
1
1
MountingHole
MountingHole_2.2mm_M2_ISO14580
Mounting Hole 2.2mm, no annular, M2, ISO14580
mounting hole 2.2mm no annular m2 iso14580
0
0
0
MountingHole
MountingHole_2.2mm_M2_ISO14580_Pad
Mounting Hole 2.2mm, M2, ISO14580
mounting hole 2.2mm m2 iso14580
0
1
1
MountingHole
MountingHole_2.2mm_M2_Pad
Mounting Hole 2.2mm, M2
mounting hole 2.2mm m2
0
1
1
MountingHole
MountingHole_2.2mm_M2_Pad_Via
Mounting Hole 2.2mm, M2
mounting hole 2.2mm m2
0
9
1
MountingHole
MountingHole_2.5mm
Mounting Hole 2.5mm, no annular
mounting hole 2.5mm no annular
0
0
0
MountingHole
MountingHole_2.5mm_Pad
Mounting Hole 2.5mm
mounting hole 2.5mm
0
1
1
MountingHole
MountingHole_2.5mm_Pad_Via
Mounting Hole 2.5mm
mounting hole 2.5mm
0
9
1
MountingHole
MountingHole_2.7mm
Mounting Hole 2.7mm, no annular
mounting hole 2.7mm no annular
0
0
0
MountingHole
MountingHole_2.7mm_M2.5
Mounting Hole 2.7mm, no annular, M2.5
mounting hole 2.7mm no annular m2.5
0
0
0
MountingHole
MountingHole_2.7mm_M2.5_DIN965
Mounting Hole 2.7mm, no annular, M2.5, DIN965
mounting hole 2.7mm no annular m2.5 din965
0
0
0
MountingHole
MountingHole_2.7mm_M2.5_DIN965_Pad
Mounting Hole 2.7mm, M2.5, DIN965
mounting hole 2.7mm m2.5 din965
0
1
1
MountingHole
MountingHole_2.7mm_M2.5_ISO7380
Mounting Hole 2.7mm, no annular, M2.5, ISO7380
mounting hole 2.7mm no annular m2.5 iso7380
0
0
0
MountingHole
MountingHole_2.7mm_M2.5_ISO7380_Pad
Mounting Hole 2.7mm, M2.5, ISO7380
mounting hole 2.7mm m2.5 iso7380
0
1
1
MountingHole
MountingHole_2.7mm_M2.5_ISO14580
Mounting Hole 2.7mm, no annular, M2.5, ISO14580
mounting hole 2.7mm no annular m2.5 iso14580
0
0
0
MountingHole
MountingHole_2.7mm_M2.5_ISO14580_Pad
Mounting Hole 2.7mm, M2.5, ISO14580
mounting hole 2.7mm m2.5 iso14580
0
1
1
MountingHole
MountingHole_2.7mm_M2.5_Pad
Mounting Hole 2.7mm, M2.5
mounting hole 2.7mm m2.5
0
1
1
MountingHole
MountingHole_2.7mm_M2.5_Pad_Via
Mounting Hole 2.7mm
mounting hole 2.7mm
0
9
1
MountingHole
MountingHole_2.7mm_Pad
Mounting Hole 2.7mm
mounting hole 2.7mm
0
1
1
MountingHole
MountingHole_2.7mm_Pad_Via
Mounting Hole 2.7mm
mounting hole 2.7mm
0
9
1
MountingHole
MountingHole_2mm
Mounting Hole 2mm, no annular
mounting hole 2mm no annular
0
0
0
MountingHole
MountingHole_3.2mm_M3
Mounting Hole 3.2mm, no annular, M3
mounting hole 3.2mm no annular m3
0
0
0
MountingHole
MountingHole_3.2mm_M3_DIN965
Mounting Hole 3.2mm, no annular, M3, DIN965
mounting hole 3.2mm no annular m3 din965
0
0
0
MountingHole
MountingHole_3.2mm_M3_DIN965_Pad
Mounting Hole 3.2mm, M3, DIN965
mounting hole 3.2mm m3 din965
0
1
1
MountingHole
MountingHole_3.2mm_M3_ISO7380
Mounting Hole 3.2mm, no annular, M3, ISO7380
mounting hole 3.2mm no annular m3 iso7380
0
0
0
MountingHole
MountingHole_3.2mm_M3_ISO7380_Pad
Mounting Hole 3.2mm, M3, ISO7380
mounting hole 3.2mm m3 iso7380
0
1
1
MountingHole
MountingHole_3.2mm_M3_ISO14580
Mounting Hole 3.2mm, no annular, M3, ISO14580
mounting hole 3.2mm no annular m3 iso14580
0
0
0
MountingHole
MountingHole_3.2mm_M3_ISO14580_Pad
Mounting Hole 3.2mm, M3, ISO14580
mounting hole 3.2mm m3 iso14580
0
1
1
MountingHole
MountingHole_3.2mm_M3_Pad
Mounting Hole 3.2mm, M3
mounting hole 3.2mm m3
0
1
1
MountingHole
MountingHole_3.2mm_M3_Pad_Via
Mounting Hole 3.2mm, M3
mounting hole 3.2mm m3
0
9
1
MountingHole
MountingHole_3.5mm
Mounting Hole 3.5mm, no annular
mounting hole 3.5mm no annular
0
0
0
MountingHole
MountingHole_3.5mm_Pad
Mounting Hole 3.5mm
mounting hole 3.5mm
0
1
1
MountingHole
MountingHole_3.5mm_Pad_Via
Mounting Hole 3.5mm
mounting hole 3.5mm
0
9
1
MountingHole
MountingHole_3.7mm
Mounting Hole 3.7mm, no annular
mounting hole 3.7mm no annular
0
0
0
MountingHole
MountingHole_3.7mm_Pad
Mounting Hole 3.7mm
mounting hole 3.7mm
0
1
1
MountingHole
MountingHole_3.7mm_Pad_Via
Mounting Hole 3.7mm
mounting hole 3.7mm
0
9
1
MountingHole
MountingHole_3mm
Mounting Hole 3mm, no annular
mounting hole 3mm no annular
0
0
0
MountingHole
MountingHole_3mm_Pad
Mounting Hole 3mm
mounting hole 3mm
0
1
1
MountingHole
MountingHole_3mm_Pad_Via
Mounting Hole 3mm
mounting hole 3mm
0
9
1
MountingHole
MountingHole_4.3mm_M4
Mounting Hole 4.3mm, no annular, M4
mounting hole 4.3mm no annular m4
0
0
0
MountingHole
MountingHole_4.3mm_M4_DIN965
Mounting Hole 4.3mm, no annular, M4, DIN965
mounting hole 4.3mm no annular m4 din965
0
0
0
MountingHole
MountingHole_4.3mm_M4_DIN965_Pad
Mounting Hole 4.3mm, M4, DIN965
mounting hole 4.3mm m4 din965
0
1
1
MountingHole
MountingHole_4.3mm_M4_ISO7380
Mounting Hole 4.3mm, no annular, M4, ISO7380
mounting hole 4.3mm no annular m4 iso7380
0
0
0
MountingHole
MountingHole_4.3mm_M4_ISO7380_Pad
Mounting Hole 4.3mm, M4, ISO7380
mounting hole 4.3mm m4 iso7380
0
1
1
MountingHole
MountingHole_4.3mm_M4_ISO14580
Mounting Hole 4.3mm, no annular, M4, ISO14580
mounting hole 4.3mm no annular m4 iso14580
0
0
0
MountingHole
MountingHole_4.3mm_M4_ISO14580_Pad
Mounting Hole 4.3mm, M4, ISO14580
mounting hole 4.3mm m4 iso14580
0
1
1
MountingHole
MountingHole_4.3mm_M4_Pad
Mounting Hole 4.3mm, M4
mounting hole 4.3mm m4
0
1
1
MountingHole
MountingHole_4.3mm_M4_Pad_Via
Mounting Hole 4.3mm, M4
mounting hole 4.3mm m4
0
9
1
MountingHole
MountingHole_4.3x6.2mm_M4_Pad
Mounting Hole 4.3x6.2mm, M4
mounting hole 4.3x6.2mm m4
0
1
1
MountingHole
MountingHole_4.3x6.2mm_M4_Pad_Via
Mounting Hole 4.3x6.2mm, M4
mounting hole 4.3x6.2mm m4
0
17
1
MountingHole
MountingHole_4.5mm
Mounting Hole 4.5mm, no annular
mounting hole 4.5mm no annular
0
0
0
MountingHole
MountingHole_4.5mm_Pad
Mounting Hole 4.5mm
mounting hole 4.5mm
0
1
1
MountingHole
MountingHole_4.5mm_Pad_Via
Mounting Hole 4.5mm
mounting hole 4.5mm
0
9
1
MountingHole
MountingHole_4mm
Mounting Hole 4mm, no annular
mounting hole 4mm no annular
0
0
0
MountingHole
MountingHole_4mm_Pad
Mounting Hole 4mm
mounting hole 4mm
0
1
1
MountingHole
MountingHole_4mm_Pad_Via
Mounting Hole 4mm
mounting hole 4mm
0
9
1
MountingHole
MountingHole_5.3mm_M5
Mounting Hole 5.3mm, no annular, M5
mounting hole 5.3mm no annular m5
0
0
0
MountingHole
MountingHole_5.3mm_M5_DIN965
Mounting Hole 5.3mm, no annular, M5, DIN965
mounting hole 5.3mm no annular m5 din965
0
0
0
MountingHole
MountingHole_5.3mm_M5_DIN965_Pad
Mounting Hole 5.3mm, M5, DIN965
mounting hole 5.3mm m5 din965
0
1
1
MountingHole
MountingHole_5.3mm_M5_ISO7380
Mounting Hole 5.3mm, no annular, M5, ISO7380
mounting hole 5.3mm no annular m5 iso7380
0
0
0
MountingHole
MountingHole_5.3mm_M5_ISO7380_Pad
Mounting Hole 5.3mm, M5, ISO7380
mounting hole 5.3mm m5 iso7380
0
1
1
MountingHole
MountingHole_5.3mm_M5_ISO14580
Mounting Hole 5.3mm, no annular, M5, ISO14580
mounting hole 5.3mm no annular m5 iso14580
0
0
0
MountingHole
MountingHole_5.3mm_M5_ISO14580_Pad
Mounting Hole 5.3mm, M5, ISO14580
mounting hole 5.3mm m5 iso14580
0
1
1
MountingHole
MountingHole_5.3mm_M5_Pad
Mounting Hole 5.3mm, M5
mounting hole 5.3mm m5
0
1
1
MountingHole
MountingHole_5.3mm_M5_Pad_Via
Mounting Hole 5.3mm, M5
mounting hole 5.3mm m5
0
9
1
MountingHole
MountingHole_5.5mm
Mounting Hole 5.5mm, no annular
mounting hole 5.5mm no annular
0
0
0
MountingHole
MountingHole_5.5mm_Pad
Mounting Hole 5.5mm
mounting hole 5.5mm
0
1
1
MountingHole
MountingHole_5.5mm_Pad_Via
Mounting Hole 5.5mm
mounting hole 5.5mm
0
9
1
MountingHole
MountingHole_5mm
Mounting Hole 5mm, no annular
mounting hole 5mm no annular
0
0
0
MountingHole
MountingHole_5mm_Pad
Mounting Hole 5mm
mounting hole 5mm
0
1
1
MountingHole
MountingHole_5mm_Pad_Via
Mounting Hole 5mm
mounting hole 5mm
0
9
1
MountingHole
MountingHole_6.4mm_M6
Mounting Hole 6.4mm, no annular, M6
mounting hole 6.4mm no annular m6
0
0
0
MountingHole
MountingHole_6.4mm_M6_DIN965
Mounting Hole 6.4mm, no annular, M6, DIN965
mounting hole 6.4mm no annular m6 din965
0
0
0
MountingHole
MountingHole_6.4mm_M6_DIN965_Pad
Mounting Hole 6.4mm, M6, DIN965
mounting hole 6.4mm m6 din965
0
1
1
MountingHole
MountingHole_6.4mm_M6_ISO7380
Mounting Hole 6.4mm, no annular, M6, ISO7380
mounting hole 6.4mm no annular m6 iso7380
0
0
0
MountingHole
MountingHole_6.4mm_M6_ISO7380_Pad
Mounting Hole 6.4mm, M6, ISO7380
mounting hole 6.4mm m6 iso7380
0
1
1
MountingHole
MountingHole_6.4mm_M6_ISO14580
Mounting Hole 6.4mm, no annular, M6, ISO14580
mounting hole 6.4mm no annular m6 iso14580
0
0
0
MountingHole
MountingHole_6.4mm_M6_ISO14580_Pad
Mounting Hole 6.4mm, M6, ISO14580
mounting hole 6.4mm m6 iso14580
0
1
1
MountingHole
MountingHole_6.4mm_M6_Pad
Mounting Hole 6.4mm, M6
mounting hole 6.4mm m6
0
1
1
MountingHole
MountingHole_6.4mm_M6_Pad_Via
Mounting Hole 6.4mm, M6
mounting hole 6.4mm m6
0
9
1
MountingHole
MountingHole_6.5mm
Mounting Hole 6.5mm, no annular
mounting hole 6.5mm no annular
0
0
0
MountingHole
MountingHole_6.5mm_Pad
Mounting Hole 6.5mm
mounting hole 6.5mm
0
1
1
MountingHole
MountingHole_6.5mm_Pad_Via
Mounting Hole 6.5mm
mounting hole 6.5mm
0
9
1
MountingHole
MountingHole_6mm
Mounting Hole 6mm, no annular
mounting hole 6mm no annular
0
0
0
MountingHole
MountingHole_6mm_Pad
Mounting Hole 6mm
mounting hole 6mm
0
1
1
MountingHole
MountingHole_6mm_Pad_Via
Mounting Hole 6mm
mounting hole 6mm
0
9
1
MountingHole
MountingHole_8.4mm_M8
Mounting Hole 8.4mm, no annular, M8
mounting hole 8.4mm no annular m8
0
0
0
MountingHole
MountingHole_8.4mm_M8_Pad
Mounting Hole 8.4mm, M8
mounting hole 8.4mm m8
0
1
1
MountingHole
MountingHole_8.4mm_M8_Pad_Via
Mounting Hole 8.4mm, M8
mounting hole 8.4mm m8
0
9
1
Package_DIP
DIP-4_W7.62mm
4-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils)
THT DIP DIL PDIP 2.54mm 7.62mm 300mil
0
4
4
Package_DIP
DIP-4_W7.62mm_LongPads
4-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils), LongPads
THT DIP DIL PDIP 2.54mm 7.62mm 300mil LongPads
0
4
4
Package_DIP
DIP-4_W7.62mm_SMDSocket_SmallPads
4-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils), SMDSocket, SmallPads
THT DIP DIL PDIP 2.54mm 7.62mm 300mil SMDSocket SmallPads
0
4
4
Package_DIP
DIP-4_W7.62mm_Socket
4-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils), Socket
THT DIP DIL PDIP 2.54mm 7.62mm 300mil Socket
0
4
4
Package_DIP
DIP-4_W7.62mm_Socket_LongPads
4-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils), Socket, LongPads
THT DIP DIL PDIP 2.54mm 7.62mm 300mil Socket LongPads
0
4
4
Package_DIP
DIP-4_W8.89mm_SMDSocket_LongPads
4-lead though-hole mounted DIP package, row spacing 8.89 mm (350 mils), SMDSocket, LongPads
THT DIP DIL PDIP 2.54mm 8.89mm 350mil SMDSocket LongPads
0
4
4
Package_DIP
DIP-4_W10.16mm
4-lead though-hole mounted DIP package, row spacing 10.16 mm (400 mils)
THT DIP DIL PDIP 2.54mm 10.16mm 400mil
0
4
4
Package_DIP
DIP-4_W10.16mm_LongPads
4-lead though-hole mounted DIP package, row spacing 10.16 mm (400 mils), LongPads
THT DIP DIL PDIP 2.54mm 10.16mm 400mil LongPads
0
4
4
Package_DIP
DIP-5-6_W7.62mm
5-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils)
THT DIP DIL PDIP 2.54mm 7.62mm 300mil
0
5
5
Package_DIP
DIP-5-6_W7.62mm_LongPads
5-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils), LongPads
THT DIP DIL PDIP 2.54mm 7.62mm 300mil LongPads
0
5
5
Package_DIP
DIP-5-6_W7.62mm_SMDSocket_SmallPads
5-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils), SMDSocket, SmallPads
THT DIP DIL PDIP 2.54mm 7.62mm 300mil SMDSocket SmallPads
0
5
5
Package_DIP
DIP-5-6_W7.62mm_Socket
5-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils), Socket
THT DIP DIL PDIP 2.54mm 7.62mm 300mil Socket
0
5
5
Package_DIP
DIP-5-6_W7.62mm_Socket_LongPads
5-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils), Socket, LongPads
THT DIP DIL PDIP 2.54mm 7.62mm 300mil Socket LongPads
0
5
5
Package_DIP
DIP-5-6_W8.89mm_SMDSocket_LongPads
5-lead though-hole mounted DIP package, row spacing 8.89 mm (350 mils), SMDSocket, LongPads
THT DIP DIL PDIP 2.54mm 8.89mm 350mil SMDSocket LongPads
0
5
5
Package_DIP
DIP-5-6_W10.16mm
5-lead though-hole mounted DIP package, row spacing 10.16 mm (400 mils)
THT DIP DIL PDIP 2.54mm 10.16mm 400mil
0
5
5
Package_DIP
DIP-5-6_W10.16mm_LongPads
5-lead though-hole mounted DIP package, row spacing 10.16 mm (400 mils), LongPads
THT DIP DIL PDIP 2.54mm 10.16mm 400mil LongPads
0
5
5
Package_DIP
DIP-6_W7.62mm
6-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils)
THT DIP DIL PDIP 2.54mm 7.62mm 300mil
0
6
6
Package_DIP
DIP-6_W7.62mm_LongPads
6-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils), LongPads
THT DIP DIL PDIP 2.54mm 7.62mm 300mil LongPads
0
6
6
Package_DIP
DIP-6_W7.62mm_SMDSocket_SmallPads
6-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils), SMDSocket, SmallPads
THT DIP DIL PDIP 2.54mm 7.62mm 300mil SMDSocket SmallPads
0
6
6
Package_DIP
DIP-6_W7.62mm_Socket
6-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils), Socket
THT DIP DIL PDIP 2.54mm 7.62mm 300mil Socket
0
6
6
Package_DIP
DIP-6_W7.62mm_Socket_LongPads
6-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils), Socket, LongPads
THT DIP DIL PDIP 2.54mm 7.62mm 300mil Socket LongPads
0
6
6
Package_DIP
DIP-6_W8.89mm_SMDSocket_LongPads
6-lead though-hole mounted DIP package, row spacing 8.89 mm (350 mils), SMDSocket, LongPads
THT DIP DIL PDIP 2.54mm 8.89mm 350mil SMDSocket LongPads
0
6
6
Package_DIP
DIP-6_W10.16mm
6-lead though-hole mounted DIP package, row spacing 10.16 mm (400 mils)
THT DIP DIL PDIP 2.54mm 10.16mm 400mil
0
6
6
Package_DIP
DIP-6_W10.16mm_LongPads
6-lead though-hole mounted DIP package, row spacing 10.16 mm (400 mils), LongPads
THT DIP DIL PDIP 2.54mm 10.16mm 400mil LongPads
0
6
6
Package_DIP
DIP-8-16_W7.62mm
16-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils)
THT DIP DIL PDIP 2.54mm 7.62mm 300mil
0
8
8
Package_DIP
DIP-8-16_W7.62mm_Socket
16-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils), Socket
THT DIP DIL PDIP 2.54mm 7.62mm 300mil Socket
0
8
8
Package_DIP
DIP-8-16_W7.62mm_Socket_LongPads
16-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils), Socket, LongPads
THT DIP DIL PDIP 2.54mm 7.62mm 300mil Socket LongPads
0
8
8
Package_DIP
DIP-8-N6_W7.62mm
8-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils), missing pin 6
THT DIP DIL PDIP 2.54mm 7.62mm 300mil
0
7
7
Package_DIP
DIP-8-N7_W7.62mm
8-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils), missing pin 7
THT DIP DIL PDIP 2.54mm 7.62mm 300mil
0
7
7
Package_DIP
DIP-8_W7.62mm
8-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils)
THT DIP DIL PDIP 2.54mm 7.62mm 300mil
0
8
8
Package_DIP
DIP-8_W7.62mm_LongPads
8-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils), LongPads
THT DIP DIL PDIP 2.54mm 7.62mm 300mil LongPads
0
8
8
Package_DIP
DIP-8_W7.62mm_SMDSocket_SmallPads
8-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils), SMDSocket, SmallPads
THT DIP DIL PDIP 2.54mm 7.62mm 300mil SMDSocket SmallPads
0
8
8
Package_DIP
DIP-8_W7.62mm_Socket
8-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils), Socket
THT DIP DIL PDIP 2.54mm 7.62mm 300mil Socket
0
8
8
Package_DIP
DIP-8_W7.62mm_Socket_LongPads
8-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils), Socket, LongPads
THT DIP DIL PDIP 2.54mm 7.62mm 300mil Socket LongPads
0
8
8
Package_DIP
DIP-8_W8.89mm_SMDSocket_LongPads
8-lead though-hole mounted DIP package, row spacing 8.89 mm (350 mils), SMDSocket, LongPads
THT DIP DIL PDIP 2.54mm 8.89mm 350mil SMDSocket LongPads
0
8
8
Package_DIP
DIP-8_W10.16mm
8-lead though-hole mounted DIP package, row spacing 10.16 mm (400 mils)
THT DIP DIL PDIP 2.54mm 10.16mm 400mil
0
8
8
Package_DIP
DIP-8_W10.16mm_LongPads
8-lead though-hole mounted DIP package, row spacing 10.16 mm (400 mils), LongPads
THT DIP DIL PDIP 2.54mm 10.16mm 400mil LongPads
0
8
8
Package_DIP
DIP-10_W7.62mm
10-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils)
THT DIP DIL PDIP 2.54mm 7.62mm 300mil
0
10
10
Package_DIP
DIP-10_W7.62mm_LongPads
10-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils), LongPads
THT DIP DIL PDIP 2.54mm 7.62mm 300mil LongPads
0
10
10
Package_DIP
DIP-10_W7.62mm_SMDSocket_SmallPads
10-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils), SMDSocket, SmallPads
THT DIP DIL PDIP 2.54mm 7.62mm 300mil SMDSocket SmallPads
0
10
10
Package_DIP
DIP-10_W7.62mm_Socket
10-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils), Socket
THT DIP DIL PDIP 2.54mm 7.62mm 300mil Socket
0
10
10
Package_DIP
DIP-10_W7.62mm_Socket_LongPads
10-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils), Socket, LongPads
THT DIP DIL PDIP 2.54mm 7.62mm 300mil Socket LongPads
0
10
10
Package_DIP
DIP-10_W8.89mm_SMDSocket_LongPads
10-lead though-hole mounted DIP package, row spacing 8.89 mm (350 mils), SMDSocket, LongPads
THT DIP DIL PDIP 2.54mm 8.89mm 350mil SMDSocket LongPads
0
10
10
Package_DIP
DIP-10_W10.16mm
10-lead though-hole mounted DIP package, row spacing 10.16 mm (400 mils)
THT DIP DIL PDIP 2.54mm 10.16mm 400mil
0
10
10
Package_DIP
DIP-10_W10.16mm_LongPads
10-lead though-hole mounted DIP package, row spacing 10.16 mm (400 mils), LongPads
THT DIP DIL PDIP 2.54mm 10.16mm 400mil LongPads
0
10
10
Package_DIP
DIP-12_W7.62mm
12-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils)
THT DIP DIL PDIP 2.54mm 7.62mm 300mil
0
12
12
Package_DIP
DIP-12_W7.62mm_LongPads
12-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils), LongPads
THT DIP DIL PDIP 2.54mm 7.62mm 300mil LongPads
0
12
12
Package_DIP
DIP-12_W7.62mm_SMDSocket_SmallPads
12-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils), SMDSocket, SmallPads
THT DIP DIL PDIP 2.54mm 7.62mm 300mil SMDSocket SmallPads
0
12
12
Package_DIP
DIP-12_W7.62mm_Socket
12-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils), Socket
THT DIP DIL PDIP 2.54mm 7.62mm 300mil Socket
0
12
12
Package_DIP
DIP-12_W7.62mm_Socket_LongPads
12-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils), Socket, LongPads
THT DIP DIL PDIP 2.54mm 7.62mm 300mil Socket LongPads
0
12
12
Package_DIP
DIP-12_W8.89mm_SMDSocket_LongPads
12-lead though-hole mounted DIP package, row spacing 8.89 mm (350 mils), SMDSocket, LongPads
THT DIP DIL PDIP 2.54mm 8.89mm 350mil SMDSocket LongPads
0
12
12
Package_DIP
DIP-12_W10.16mm
12-lead though-hole mounted DIP package, row spacing 10.16 mm (400 mils)
THT DIP DIL PDIP 2.54mm 10.16mm 400mil
0
12
12
Package_DIP
DIP-12_W10.16mm_LongPads
12-lead though-hole mounted DIP package, row spacing 10.16 mm (400 mils), LongPads
THT DIP DIL PDIP 2.54mm 10.16mm 400mil LongPads
0
12
12
Package_DIP
DIP-14_W7.62mm
14-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils)
THT DIP DIL PDIP 2.54mm 7.62mm 300mil
0
14
14
Package_DIP
DIP-14_W7.62mm_LongPads
14-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils), LongPads
THT DIP DIL PDIP 2.54mm 7.62mm 300mil LongPads
0
14
14
Package_DIP
DIP-14_W7.62mm_SMDSocket_SmallPads
14-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils), SMDSocket, SmallPads
THT DIP DIL PDIP 2.54mm 7.62mm 300mil SMDSocket SmallPads
0
14
14
Package_DIP
DIP-14_W7.62mm_Socket
14-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils), Socket
THT DIP DIL PDIP 2.54mm 7.62mm 300mil Socket
0
14
14
Package_DIP
DIP-14_W7.62mm_Socket_LongPads
14-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils), Socket, LongPads
THT DIP DIL PDIP 2.54mm 7.62mm 300mil Socket LongPads
0
14
14
Package_DIP
DIP-14_W8.89mm_SMDSocket_LongPads
14-lead though-hole mounted DIP package, row spacing 8.89 mm (350 mils), SMDSocket, LongPads
THT DIP DIL PDIP 2.54mm 8.89mm 350mil SMDSocket LongPads
0
14
14
Package_DIP
DIP-14_W10.16mm
14-lead though-hole mounted DIP package, row spacing 10.16 mm (400 mils)
THT DIP DIL PDIP 2.54mm 10.16mm 400mil
0
14
14
Package_DIP
DIP-14_W10.16mm_LongPads
14-lead though-hole mounted DIP package, row spacing 10.16 mm (400 mils), LongPads
THT DIP DIL PDIP 2.54mm 10.16mm 400mil LongPads
0
14
14
Package_DIP
DIP-16_W7.62mm
16-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils)
THT DIP DIL PDIP 2.54mm 7.62mm 300mil
0
16
16
Package_DIP
DIP-16_W7.62mm_LongPads
16-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils), LongPads
THT DIP DIL PDIP 2.54mm 7.62mm 300mil LongPads
0
16
16
Package_DIP
DIP-16_W7.62mm_SMDSocket_SmallPads
16-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils), SMDSocket, SmallPads
THT DIP DIL PDIP 2.54mm 7.62mm 300mil SMDSocket SmallPads
0
16
16
Package_DIP
DIP-16_W7.62mm_Socket
16-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils), Socket
THT DIP DIL PDIP 2.54mm 7.62mm 300mil Socket
0
16
16
Package_DIP
DIP-16_W7.62mm_Socket_LongPads
16-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils), Socket, LongPads
THT DIP DIL PDIP 2.54mm 7.62mm 300mil Socket LongPads
0
16
16
Package_DIP
DIP-16_W8.89mm_SMDSocket_LongPads
16-lead though-hole mounted DIP package, row spacing 8.89 mm (350 mils), SMDSocket, LongPads
THT DIP DIL PDIP 2.54mm 8.89mm 350mil SMDSocket LongPads
0
16
16
Package_DIP
DIP-16_W10.16mm
16-lead though-hole mounted DIP package, row spacing 10.16 mm (400 mils)
THT DIP DIL PDIP 2.54mm 10.16mm 400mil
0
16
16
Package_DIP
DIP-16_W10.16mm_LongPads
16-lead though-hole mounted DIP package, row spacing 10.16 mm (400 mils), LongPads
THT DIP DIL PDIP 2.54mm 10.16mm 400mil LongPads
0
16
16
Package_DIP
DIP-18_W7.62mm
18-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils)
THT DIP DIL PDIP 2.54mm 7.62mm 300mil
0
18
18
Package_DIP
DIP-18_W7.62mm_LongPads
18-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils), LongPads
THT DIP DIL PDIP 2.54mm 7.62mm 300mil LongPads
0
18
18
Package_DIP
DIP-18_W7.62mm_SMDSocket_SmallPads
18-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils), SMDSocket, SmallPads
THT DIP DIL PDIP 2.54mm 7.62mm 300mil SMDSocket SmallPads
0
18
18
Package_DIP
DIP-18_W7.62mm_Socket
18-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils), Socket
THT DIP DIL PDIP 2.54mm 7.62mm 300mil Socket
0
18
18
Package_DIP
DIP-18_W7.62mm_Socket_LongPads
18-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils), Socket, LongPads
THT DIP DIL PDIP 2.54mm 7.62mm 300mil Socket LongPads
0
18
18
Package_DIP
DIP-18_W8.89mm_SMDSocket_LongPads
18-lead though-hole mounted DIP package, row spacing 8.89 mm (350 mils), SMDSocket, LongPads
THT DIP DIL PDIP 2.54mm 8.89mm 350mil SMDSocket LongPads
0
18
18
Package_DIP
DIP-20_W7.62mm
20-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils)
THT DIP DIL PDIP 2.54mm 7.62mm 300mil
0
20
20
Package_DIP
DIP-20_W7.62mm_LongPads
20-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils), LongPads
THT DIP DIL PDIP 2.54mm 7.62mm 300mil LongPads
0
20
20
Package_DIP
DIP-20_W7.62mm_SMDSocket_SmallPads
20-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils), SMDSocket, SmallPads
THT DIP DIL PDIP 2.54mm 7.62mm 300mil SMDSocket SmallPads
0
20
20
Package_DIP
DIP-20_W7.62mm_Socket
20-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils), Socket
THT DIP DIL PDIP 2.54mm 7.62mm 300mil Socket
0
20
20
Package_DIP
DIP-20_W7.62mm_Socket_LongPads
20-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils), Socket, LongPads
THT DIP DIL PDIP 2.54mm 7.62mm 300mil Socket LongPads
0
20
20
Package_DIP
DIP-20_W8.89mm_SMDSocket_LongPads
20-lead though-hole mounted DIP package, row spacing 8.89 mm (350 mils), SMDSocket, LongPads
THT DIP DIL PDIP 2.54mm 8.89mm 350mil SMDSocket LongPads
0
20
20
Package_DIP
DIP-22_W7.62mm
22-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils)
THT DIP DIL PDIP 2.54mm 7.62mm 300mil
0
22
22
Package_DIP
DIP-22_W7.62mm_LongPads
22-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils), LongPads
THT DIP DIL PDIP 2.54mm 7.62mm 300mil LongPads
0
22
22
Package_DIP
DIP-22_W7.62mm_SMDSocket_SmallPads
22-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils), SMDSocket, SmallPads
THT DIP DIL PDIP 2.54mm 7.62mm 300mil SMDSocket SmallPads
0
22
22
Package_DIP
DIP-22_W7.62mm_Socket
22-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils), Socket
THT DIP DIL PDIP 2.54mm 7.62mm 300mil Socket
0
22
22
Package_DIP
DIP-22_W7.62mm_Socket_LongPads
22-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils), Socket, LongPads
THT DIP DIL PDIP 2.54mm 7.62mm 300mil Socket LongPads
0
22
22
Package_DIP
DIP-22_W8.89mm_SMDSocket_LongPads
22-lead though-hole mounted DIP package, row spacing 8.89 mm (350 mils), SMDSocket, LongPads
THT DIP DIL PDIP 2.54mm 8.89mm 350mil SMDSocket LongPads
0
22
22
Package_DIP
DIP-22_W10.16mm
22-lead though-hole mounted DIP package, row spacing 10.16 mm (400 mils)
THT DIP DIL PDIP 2.54mm 10.16mm 400mil
0
22
22
Package_DIP
DIP-22_W10.16mm_LongPads
22-lead though-hole mounted DIP package, row spacing 10.16 mm (400 mils), LongPads
THT DIP DIL PDIP 2.54mm 10.16mm 400mil LongPads
0
22
22
Package_DIP
DIP-22_W10.16mm_SMDSocket_SmallPads
22-lead though-hole mounted DIP package, row spacing 10.16 mm (400 mils), SMDSocket, SmallPads
THT DIP DIL PDIP 2.54mm 10.16mm 400mil SMDSocket SmallPads
0
22
22
Package_DIP
DIP-22_W10.16mm_Socket
22-lead though-hole mounted DIP package, row spacing 10.16 mm (400 mils), Socket
THT DIP DIL PDIP 2.54mm 10.16mm 400mil Socket
0
22
22
Package_DIP
DIP-22_W10.16mm_Socket_LongPads
22-lead though-hole mounted DIP package, row spacing 10.16 mm (400 mils), Socket, LongPads
THT DIP DIL PDIP 2.54mm 10.16mm 400mil Socket LongPads
0
22
22
Package_DIP
DIP-22_W11.43mm_SMDSocket_LongPads
22-lead though-hole mounted DIP package, row spacing 11.43 mm (450 mils), SMDSocket, LongPads
THT DIP DIL PDIP 2.54mm 11.43mm 450mil SMDSocket LongPads
0
22
22
Package_DIP
DIP-24_W7.62mm
24-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils)
THT DIP DIL PDIP 2.54mm 7.62mm 300mil
0
24
24
Package_DIP
DIP-24_W7.62mm_LongPads
24-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils), LongPads
THT DIP DIL PDIP 2.54mm 7.62mm 300mil LongPads
0
24
24
Package_DIP
DIP-24_W7.62mm_SMDSocket_SmallPads
24-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils), SMDSocket, SmallPads
THT DIP DIL PDIP 2.54mm 7.62mm 300mil SMDSocket SmallPads
0
24
24
Package_DIP
DIP-24_W7.62mm_Socket
24-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils), Socket
THT DIP DIL PDIP 2.54mm 7.62mm 300mil Socket
0
24
24
Package_DIP
DIP-24_W7.62mm_Socket_LongPads
24-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils), Socket, LongPads
THT DIP DIL PDIP 2.54mm 7.62mm 300mil Socket LongPads
0
24
24
Package_DIP
DIP-24_W8.89mm_SMDSocket_LongPads
24-lead though-hole mounted DIP package, row spacing 8.89 mm (350 mils), SMDSocket, LongPads
THT DIP DIL PDIP 2.54mm 8.89mm 350mil SMDSocket LongPads
0
24
24
Package_DIP
DIP-24_W10.16mm
24-lead though-hole mounted DIP package, row spacing 10.16 mm (400 mils)
THT DIP DIL PDIP 2.54mm 10.16mm 400mil
0
24
24
Package_DIP
DIP-24_W10.16mm_LongPads
24-lead though-hole mounted DIP package, row spacing 10.16 mm (400 mils), LongPads
THT DIP DIL PDIP 2.54mm 10.16mm 400mil LongPads
0
24
24
Package_DIP
DIP-24_W10.16mm_SMDSocket_SmallPads
24-lead though-hole mounted DIP package, row spacing 10.16 mm (400 mils), SMDSocket, SmallPads
THT DIP DIL PDIP 2.54mm 10.16mm 400mil SMDSocket SmallPads
0
24
24
Package_DIP
DIP-24_W10.16mm_Socket
24-lead though-hole mounted DIP package, row spacing 10.16 mm (400 mils), Socket
THT DIP DIL PDIP 2.54mm 10.16mm 400mil Socket
0
24
24
Package_DIP
DIP-24_W10.16mm_Socket_LongPads
24-lead though-hole mounted DIP package, row spacing 10.16 mm (400 mils), Socket, LongPads
THT DIP DIL PDIP 2.54mm 10.16mm 400mil Socket LongPads
0
24
24
Package_DIP
DIP-24_W11.43mm_SMDSocket_LongPads
24-lead though-hole mounted DIP package, row spacing 11.43 mm (450 mils), SMDSocket, LongPads
THT DIP DIL PDIP 2.54mm 11.43mm 450mil SMDSocket LongPads
0
24
24
Package_DIP
DIP-24_W15.24mm
24-lead though-hole mounted DIP package, row spacing 15.24 mm (600 mils)
THT DIP DIL PDIP 2.54mm 15.24mm 600mil
0
24
24
Package_DIP
DIP-24_W15.24mm_LongPads
24-lead though-hole mounted DIP package, row spacing 15.24 mm (600 mils), LongPads
THT DIP DIL PDIP 2.54mm 15.24mm 600mil LongPads
0
24
24
Package_DIP
DIP-24_W15.24mm_SMDSocket_SmallPads
24-lead though-hole mounted DIP package, row spacing 15.24 mm (600 mils), SMDSocket, SmallPads
THT DIP DIL PDIP 2.54mm 15.24mm 600mil SMDSocket SmallPads
0
24
24
Package_DIP
DIP-24_W15.24mm_Socket
24-lead though-hole mounted DIP package, row spacing 15.24 mm (600 mils), Socket
THT DIP DIL PDIP 2.54mm 15.24mm 600mil Socket
0
24
24
Package_DIP
DIP-24_W15.24mm_Socket_LongPads
24-lead though-hole mounted DIP package, row spacing 15.24 mm (600 mils), Socket, LongPads
THT DIP DIL PDIP 2.54mm 15.24mm 600mil Socket LongPads
0
24
24
Package_DIP
DIP-24_W16.51mm_SMDSocket_LongPads
24-lead though-hole mounted DIP package, row spacing 16.51 mm (650 mils), SMDSocket, LongPads
THT DIP DIL PDIP 2.54mm 16.51mm 650mil SMDSocket LongPads
0
24
24
Package_DIP
DIP-28_W7.62mm
28-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils)
THT DIP DIL PDIP 2.54mm 7.62mm 300mil
0
28
28
Package_DIP
DIP-28_W7.62mm_LongPads
28-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils), LongPads
THT DIP DIL PDIP 2.54mm 7.62mm 300mil LongPads
0
28
28
Package_DIP
DIP-28_W7.62mm_SMDSocket_SmallPads
28-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils), SMDSocket, SmallPads
THT DIP DIL PDIP 2.54mm 7.62mm 300mil SMDSocket SmallPads
0
28
28
Package_DIP
DIP-28_W7.62mm_Socket
28-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils), Socket
THT DIP DIL PDIP 2.54mm 7.62mm 300mil Socket
0
28
28
Package_DIP
DIP-28_W7.62mm_Socket_LongPads
28-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils), Socket, LongPads
THT DIP DIL PDIP 2.54mm 7.62mm 300mil Socket LongPads
0
28
28
Package_DIP
DIP-28_W8.89mm_SMDSocket_LongPads
28-lead though-hole mounted DIP package, row spacing 8.89 mm (350 mils), SMDSocket, LongPads
THT DIP DIL PDIP 2.54mm 8.89mm 350mil SMDSocket LongPads
0
28
28
Package_DIP
DIP-28_W15.24mm
28-lead though-hole mounted DIP package, row spacing 15.24 mm (600 mils)
THT DIP DIL PDIP 2.54mm 15.24mm 600mil
0
28
28
Package_DIP
DIP-28_W15.24mm_LongPads
28-lead though-hole mounted DIP package, row spacing 15.24 mm (600 mils), LongPads
THT DIP DIL PDIP 2.54mm 15.24mm 600mil LongPads
0
28
28
Package_DIP
DIP-28_W15.24mm_SMDSocket_SmallPads
28-lead though-hole mounted DIP package, row spacing 15.24 mm (600 mils), SMDSocket, SmallPads
THT DIP DIL PDIP 2.54mm 15.24mm 600mil SMDSocket SmallPads
0
28
28
Package_DIP
DIP-28_W15.24mm_Socket
28-lead though-hole mounted DIP package, row spacing 15.24 mm (600 mils), Socket
THT DIP DIL PDIP 2.54mm 15.24mm 600mil Socket
0
28
28
Package_DIP
DIP-28_W15.24mm_Socket_LongPads
28-lead though-hole mounted DIP package, row spacing 15.24 mm (600 mils), Socket, LongPads
THT DIP DIL PDIP 2.54mm 15.24mm 600mil Socket LongPads
0
28
28
Package_DIP
DIP-28_W16.51mm_SMDSocket_LongPads
28-lead though-hole mounted DIP package, row spacing 16.51 mm (650 mils), SMDSocket, LongPads
THT DIP DIL PDIP 2.54mm 16.51mm 650mil SMDSocket LongPads
0
28
28
Package_DIP
DIP-32_W7.62mm
32-lead dip package, row spacing 7.62 mm (300 mils)
DIL DIP PDIP 2.54mm 7.62mm 300mil
0
32
32
Package_DIP
DIP-32_W15.24mm
32-lead though-hole mounted DIP package, row spacing 15.24 mm (600 mils)
THT DIP DIL PDIP 2.54mm 15.24mm 600mil
0
32
32
Package_DIP
DIP-32_W15.24mm_LongPads
32-lead though-hole mounted DIP package, row spacing 15.24 mm (600 mils), LongPads
THT DIP DIL PDIP 2.54mm 15.24mm 600mil LongPads
0
32
32
Package_DIP
DIP-32_W15.24mm_SMDSocket_SmallPads
32-lead though-hole mounted DIP package, row spacing 15.24 mm (600 mils), SMDSocket, SmallPads
THT DIP DIL PDIP 2.54mm 15.24mm 600mil SMDSocket SmallPads
0
32
32
Package_DIP
DIP-32_W15.24mm_Socket
32-lead though-hole mounted DIP package, row spacing 15.24 mm (600 mils), Socket
THT DIP DIL PDIP 2.54mm 15.24mm 600mil Socket
0
32
32
Package_DIP
DIP-32_W15.24mm_Socket_LongPads
32-lead though-hole mounted DIP package, row spacing 15.24 mm (600 mils), Socket, LongPads
THT DIP DIL PDIP 2.54mm 15.24mm 600mil Socket LongPads
0
32
32
Package_DIP
DIP-32_W16.51mm_SMDSocket_LongPads
32-lead though-hole mounted DIP package, row spacing 16.51 mm (650 mils), SMDSocket, LongPads
THT DIP DIL PDIP 2.54mm 16.51mm 650mil SMDSocket LongPads
0
32
32
Package_DIP
DIP-40_W15.24mm
40-lead though-hole mounted DIP package, row spacing 15.24 mm (600 mils)
THT DIP DIL PDIP 2.54mm 15.24mm 600mil
0
40
40
Package_DIP
DIP-40_W15.24mm_LongPads
40-lead though-hole mounted DIP package, row spacing 15.24 mm (600 mils), LongPads
THT DIP DIL PDIP 2.54mm 15.24mm 600mil LongPads
0
40
40
Package_DIP
DIP-40_W15.24mm_SMDSocket_SmallPads
40-lead though-hole mounted DIP package, row spacing 15.24 mm (600 mils), SMDSocket, SmallPads
THT DIP DIL PDIP 2.54mm 15.24mm 600mil SMDSocket SmallPads
0
40
40
Package_DIP
DIP-40_W15.24mm_Socket
40-lead though-hole mounted DIP package, row spacing 15.24 mm (600 mils), Socket
THT DIP DIL PDIP 2.54mm 15.24mm 600mil Socket
0
40
40
Package_DIP
DIP-40_W15.24mm_Socket_LongPads
40-lead though-hole mounted DIP package, row spacing 15.24 mm (600 mils), Socket, LongPads
THT DIP DIL PDIP 2.54mm 15.24mm 600mil Socket LongPads
0
40
40
Package_DIP
DIP-40_W16.51mm_SMDSocket_LongPads
40-lead though-hole mounted DIP package, row spacing 16.51 mm (650 mils), SMDSocket, LongPads
THT DIP DIL PDIP 2.54mm 16.51mm 650mil SMDSocket LongPads
0
40
40
Package_DIP
DIP-40_W25.4mm
40-lead though-hole mounted DIP package, row spacing 25.4 mm (1000 mils)
THT DIP DIL PDIP 2.54mm 25.4mm 1000mil
0
40
40
Package_DIP
DIP-40_W25.4mm_LongPads
40-lead though-hole mounted DIP package, row spacing 25.4 mm (1000 mils), LongPads
THT DIP DIL PDIP 2.54mm 25.4mm 1000mil LongPads
0
40
40
Package_DIP
DIP-40_W25.4mm_SMDSocket_SmallPads
40-lead though-hole mounted DIP package, row spacing 25.4 mm (1000 mils), SMDSocket, SmallPads
THT DIP DIL PDIP 2.54mm 25.4mm 1000mil SMDSocket SmallPads
0
40
40
Package_DIP
DIP-40_W25.4mm_Socket
40-lead though-hole mounted DIP package, row spacing 25.4 mm (1000 mils), Socket
THT DIP DIL PDIP 2.54mm 25.4mm 1000mil Socket
0
40
40
Package_DIP
DIP-40_W25.4mm_Socket_LongPads
40-lead though-hole mounted DIP package, row spacing 25.4 mm (1000 mils), Socket, LongPads
THT DIP DIL PDIP 2.54mm 25.4mm 1000mil Socket LongPads
0
40
40
Package_DIP
DIP-40_W26.67mm_SMDSocket_LongPads
40-lead though-hole mounted DIP package, row spacing 26.67 mm (1050 mils), SMDSocket, LongPads
THT DIP DIL PDIP 2.54mm 26.669999999999998mm 1050mil SMDSocket LongPads
0
40
40
Package_DIP
DIP-42_W15.24mm
42-lead though-hole mounted DIP package, row spacing 15.24 mm (600 mils)
THT DIP DIL PDIP 2.54mm 15.24mm 600mil
0
42
42
Package_DIP
DIP-42_W15.24mm_LongPads
42-lead though-hole mounted DIP package, row spacing 15.24 mm (600 mils), LongPads
THT DIP DIL PDIP 2.54mm 15.24mm 600mil LongPads
0
42
42
Package_DIP
DIP-42_W15.24mm_SMDSocket_SmallPads
42-lead though-hole mounted DIP package, row spacing 15.24 mm (600 mils), SMDSocket, SmallPads
THT DIP DIL PDIP 2.54mm 15.24mm 600mil SMDSocket SmallPads
0
42
42
Package_DIP
DIP-42_W15.24mm_Socket
42-lead though-hole mounted DIP package, row spacing 15.24 mm (600 mils), Socket
THT DIP DIL PDIP 2.54mm 15.24mm 600mil Socket
0
42
42
Package_DIP
DIP-42_W15.24mm_Socket_LongPads
42-lead though-hole mounted DIP package, row spacing 15.24 mm (600 mils), Socket, LongPads
THT DIP DIL PDIP 2.54mm 15.24mm 600mil Socket LongPads
0
42
42
Package_DIP
DIP-42_W16.51mm_SMDSocket_LongPads
42-lead though-hole mounted DIP package, row spacing 16.51 mm (650 mils), SMDSocket, LongPads
THT DIP DIL PDIP 2.54mm 16.51mm 650mil SMDSocket LongPads
0
42
42
Package_DIP
DIP-48_W15.24mm
48-lead though-hole mounted DIP package, row spacing 15.24 mm (600 mils)
THT DIP DIL PDIP 2.54mm 15.24mm 600mil
0
48
48
Package_DIP
DIP-48_W15.24mm_LongPads
48-lead though-hole mounted DIP package, row spacing 15.24 mm (600 mils), LongPads
THT DIP DIL PDIP 2.54mm 15.24mm 600mil LongPads
0
48
48
Package_DIP
DIP-48_W15.24mm_SMDSocket_SmallPads
48-lead though-hole mounted DIP package, row spacing 15.24 mm (600 mils), SMDSocket, SmallPads
THT DIP DIL PDIP 2.54mm 15.24mm 600mil SMDSocket SmallPads
0
48
48
Package_DIP
DIP-48_W15.24mm_Socket
48-lead though-hole mounted DIP package, row spacing 15.24 mm (600 mils), Socket
THT DIP DIL PDIP 2.54mm 15.24mm 600mil Socket
0
48
48
Package_DIP
DIP-48_W15.24mm_Socket_LongPads
48-lead though-hole mounted DIP package, row spacing 15.24 mm (600 mils), Socket, LongPads
THT DIP DIL PDIP 2.54mm 15.24mm 600mil Socket LongPads
0
48
48
Package_DIP
DIP-48_W16.51mm_SMDSocket_LongPads
48-lead though-hole mounted DIP package, row spacing 16.51 mm (650 mils), SMDSocket, LongPads
THT DIP DIL PDIP 2.54mm 16.51mm 650mil SMDSocket LongPads
0
48
48
Package_DIP
DIP-64_W15.24mm
64-lead though-hole mounted DIP package, row spacing 15.24 mm (600 mils)
THT DIP DIL PDIP 2.54mm 15.24mm 600mil
0
64
64
Package_DIP
DIP-64_W15.24mm_LongPads
64-lead though-hole mounted DIP package, row spacing 15.24 mm (600 mils), LongPads
THT DIP DIL PDIP 2.54mm 15.24mm 600mil LongPads
0
64
64
Package_DIP
DIP-64_W15.24mm_SMDSocket_SmallPads
64-lead though-hole mounted DIP package, row spacing 15.24 mm (600 mils), SMDSocket, SmallPads
THT DIP DIL PDIP 2.54mm 15.24mm 600mil SMDSocket SmallPads
0
64
64
Package_DIP
DIP-64_W15.24mm_Socket
64-lead though-hole mounted DIP package, row spacing 15.24 mm (600 mils), Socket
THT DIP DIL PDIP 2.54mm 15.24mm 600mil Socket
0
64
64
Package_DIP
DIP-64_W15.24mm_Socket_LongPads
64-lead though-hole mounted DIP package, row spacing 15.24 mm (600 mils), Socket, LongPads
THT DIP DIL PDIP 2.54mm 15.24mm 600mil Socket LongPads
0
64
64
Package_DIP
DIP-64_W16.51mm_SMDSocket_LongPads
64-lead though-hole mounted DIP package, row spacing 16.51 mm (650 mils), SMDSocket, LongPads
THT DIP DIL PDIP 2.54mm 16.51mm 650mil SMDSocket LongPads
0
64
64
Package_DIP
DIP-64_W22.86mm
64-lead though-hole mounted DIP package, row spacing 22.86 mm (900 mils)
THT DIP DIL PDIP 2.54mm 22.86mm 900mil
0
64
64
Package_DIP
DIP-64_W22.86mm_LongPads
64-lead though-hole mounted DIP package, row spacing 22.86 mm (900 mils), LongPads
THT DIP DIL PDIP 2.54mm 22.86mm 900mil LongPads
0
64
64
Package_DIP
DIP-64_W22.86mm_SMDSocket_SmallPads
64-lead though-hole mounted DIP package, row spacing 22.86 mm (900 mils), SMDSocket, SmallPads
THT DIP DIL PDIP 2.54mm 22.86mm 900mil SMDSocket SmallPads
0
64
64
Package_DIP
DIP-64_W22.86mm_Socket
64-lead though-hole mounted DIP package, row spacing 22.86 mm (900 mils), Socket
THT DIP DIL PDIP 2.54mm 22.86mm 900mil Socket
0
64
64
Package_DIP
DIP-64_W22.86mm_Socket_LongPads
64-lead though-hole mounted DIP package, row spacing 22.86 mm (900 mils), Socket, LongPads
THT DIP DIL PDIP 2.54mm 22.86mm 900mil Socket LongPads
0
64
64
Package_DIP
DIP-64_W24.13mm_SMDSocket_LongPads
64-lead though-hole mounted DIP package, row spacing 24.13 mm (950 mils), SMDSocket, LongPads
THT DIP DIL PDIP 2.54mm 24.13mm 950mil SMDSocket LongPads
0
64
64
Package_DIP
DIP-64_W25.4mm
64-lead though-hole mounted DIP package, row spacing 25.4 mm (1000 mils)
THT DIP DIL PDIP 2.54mm 25.4mm 1000mil
0
64
64
Package_DIP
DIP-64_W25.4mm_LongPads
64-lead though-hole mounted DIP package, row spacing 25.4 mm (1000 mils), LongPads
THT DIP DIL PDIP 2.54mm 25.4mm 1000mil LongPads
0
64
64
Package_DIP
DIP-64_W25.4mm_SMDSocket_SmallPads
64-lead though-hole mounted DIP package, row spacing 25.4 mm (1000 mils), SMDSocket, SmallPads
THT DIP DIL PDIP 2.54mm 25.4mm 1000mil SMDSocket SmallPads
0
64
64
Package_DIP
DIP-64_W25.4mm_Socket
64-lead though-hole mounted DIP package, row spacing 25.4 mm (1000 mils), Socket
THT DIP DIL PDIP 2.54mm 25.4mm 1000mil Socket
0
64
64
Package_DIP
DIP-64_W25.4mm_Socket_LongPads
64-lead though-hole mounted DIP package, row spacing 25.4 mm (1000 mils), Socket, LongPads
THT DIP DIL PDIP 2.54mm 25.4mm 1000mil Socket LongPads
0
64
64
Package_DIP
DIP-64_W26.67mm_SMDSocket_LongPads
64-lead though-hole mounted DIP package, row spacing 26.67 mm (1050 mils), SMDSocket, LongPads
THT DIP DIL PDIP 2.54mm 26.669999999999998mm 1050mil SMDSocket LongPads
0
64
64
Package_DIP
Fairchild_LSOP-8
8-Lead, 300\" Wide, Surface Mount Package (https://www.fairchildsemi.com/package-drawings/ML/MLSOP08A.pdf)
LSOP 2.54mm 300mil
0
8
8
Package_DIP
PowerIntegrations_PDIP-8B
Power Integrations variant of 8-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils), LongPads, see https://www.power.com/sites/default/files/product-docs/lnk520.pdf
THT DIP DIL PDIP 2.54mm 7.62mm 300mil LongPads
0
7
7
Package_DIP
PowerIntegrations_PDIP-8C
Power Integrations variant of 8-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils), LongPads, see https://ac-dc.power.com/sites/default/files/product-docs/tinyswitch-iii_family_datasheet.pdf
THT DIP DIL PDIP 2.54mm 7.62mm 300mil LongPads
0
7
7
Package_DIP
PowerIntegrations_SDIP-10C
PowerIntegrations variant of 10-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils), LongPads, see https://www.power.com/sites/default/files/product-docs/tophx_family_datasheet.pdf
THT DIP DIL PDIP 2.54mm 7.62mm 300mil LongPads
0
9
9
Package_DIP
PowerIntegrations_SMD-8
PowerIntegrations variant of 8-lead surface-mounted (SMD) DIP package, row spacing 7.62 mm (300 mils), see https://www.power.com/sites/default/files/product-docs/lnk520.pdf
SMD DIP DIL PDIP SMDIP 2.54mm 7.62mm 300mil
0
8
8
Package_DIP
PowerIntegrations_SMD-8B
PowerIntegrations variant of 8-lead surface-mounted (SMD) DIP package, row spacing 7.62 mm (300 mils), see https://www.power.com/sites/default/files/product-docs/lnk520.pdf
SMD DIP DIL PDIP SMDIP 2.54mm 7.62mm 300mil
0
7
7
Package_DIP
PowerIntegrations_SMD-8C
PowerIntegrations variant of 8-lead surface-mounted (SMD) DIP package, row spacing 7.62 mm (300 mils), see https://ac-dc.power.com/sites/default/files/product-docs/tinyswitch-iii_family_datasheet.pdf
SMD DIP DIL PDIP SMDIP 2.54mm 7.62mm 300mil
0
7
7
Package_DIP
PowerIntegrations_eDIP-12B
Power Integrations eDIP-12B, see https://www.power.com/sites/default/files/product-docs/linkswitch-pl_family_datasheet.pdf
THT DIP DIL PDIP 2.54mm 7.62mm 300mil
0
11
11
Package_DIP
SMDIP-4_W7.62mm
4-lead surface-mounted (SMD) DIP package, row spacing 7.62 mm (300 mils)
SMD DIP DIL PDIP SMDIP 2.54mm 7.62mm 300mil
0
4
4
Package_DIP
SMDIP-4_W9.53mm
4-lead surface-mounted (SMD) DIP package, row spacing 9.53 mm (375 mils)
SMD DIP DIL PDIP SMDIP 2.54mm 9.53mm 375mil
0
4
4
Package_DIP
SMDIP-4_W9.53mm_Clearance8mm
4-lead surface-mounted (SMD) DIP package, row spacing 9.53 mm (375 mils), Clearance8mm
SMD DIP DIL PDIP SMDIP 2.54mm 9.53mm 375mil Clearance8mm
0
4
4
Package_DIP
SMDIP-4_W11.48mm
4-lead surface-mounted (SMD) DIP package, row spacing 11.48 mm (451 mils)
SMD DIP DIL PDIP SMDIP 2.54mm 11.48mm 451mil
0
4
4
Package_DIP
SMDIP-6_W7.62mm
6-lead surface-mounted (SMD) DIP package, row spacing 7.62 mm (300 mils)
SMD DIP DIL PDIP SMDIP 2.54mm 7.62mm 300mil
0
6
6
Package_DIP
SMDIP-6_W9.53mm
6-lead surface-mounted (SMD) DIP package, row spacing 9.53 mm (375 mils)
SMD DIP DIL PDIP SMDIP 2.54mm 9.53mm 375mil
0
6
6
Package_DIP
SMDIP-6_W9.53mm_Clearance8mm
6-lead surface-mounted (SMD) DIP package, row spacing 9.53 mm (375 mils), Clearance8mm
SMD DIP DIL PDIP SMDIP 2.54mm 9.53mm 375mil Clearance8mm
0
6
6
Package_DIP
SMDIP-6_W11.48mm
6-lead surface-mounted (SMD) DIP package, row spacing 11.48 mm (451 mils)
SMD DIP DIL PDIP SMDIP 2.54mm 11.48mm 451mil
0
6
6
Package_DIP
SMDIP-8_W7.62mm
8-lead surface-mounted (SMD) DIP package, row spacing 7.62 mm (300 mils)
SMD DIP DIL PDIP SMDIP 2.54mm 7.62mm 300mil
0
8
8
Package_DIP
SMDIP-8_W9.53mm
8-lead surface-mounted (SMD) DIP package, row spacing 9.53 mm (375 mils)
SMD DIP DIL PDIP SMDIP 2.54mm 9.53mm 375mil
0
8
8
Package_DIP
SMDIP-8_W9.53mm_Clearance8mm
8-lead surface-mounted (SMD) DIP package, row spacing 9.53 mm (375 mils), Clearance8mm
SMD DIP DIL PDIP SMDIP 2.54mm 9.53mm 375mil Clearance8mm
0
8
8
Package_DIP
SMDIP-8_W11.48mm
8-lead surface-mounted (SMD) DIP package, row spacing 11.48 mm (451 mils)
SMD DIP DIL PDIP SMDIP 2.54mm 11.48mm 451mil
0
8
8
Package_DIP
SMDIP-10_W7.62mm
10-lead surface-mounted (SMD) DIP package, row spacing 7.62 mm (300 mils)
SMD DIP DIL PDIP SMDIP 2.54mm 7.62mm 300mil
0
10
10
Package_DIP
SMDIP-10_W9.53mm
10-lead surface-mounted (SMD) DIP package, row spacing 9.53 mm (375 mils)
SMD DIP DIL PDIP SMDIP 2.54mm 9.53mm 375mil
0
10
10
Package_DIP
SMDIP-10_W9.53mm_Clearance8mm
10-lead surface-mounted (SMD) DIP package, row spacing 9.53 mm (375 mils), Clearance8mm
SMD DIP DIL PDIP SMDIP 2.54mm 9.53mm 375mil Clearance8mm
0
10
10
Package_DIP
SMDIP-10_W11.48mm
10-lead surface-mounted (SMD) DIP package, row spacing 11.48 mm (451 mils)
SMD DIP DIL PDIP SMDIP 2.54mm 11.48mm 451mil
0
10
10
Package_DIP
SMDIP-12_W7.62mm
12-lead surface-mounted (SMD) DIP package, row spacing 7.62 mm (300 mils)
SMD DIP DIL PDIP SMDIP 2.54mm 7.62mm 300mil
0
12
12
Package_DIP
SMDIP-12_W9.53mm
12-lead surface-mounted (SMD) DIP package, row spacing 9.53 mm (375 mils)
SMD DIP DIL PDIP SMDIP 2.54mm 9.53mm 375mil
0
12
12
Package_DIP
SMDIP-12_W9.53mm_Clearance8mm
12-lead surface-mounted (SMD) DIP package, row spacing 9.53 mm (375 mils), Clearance8mm
SMD DIP DIL PDIP SMDIP 2.54mm 9.53mm 375mil Clearance8mm
0
12
12
Package_DIP
SMDIP-12_W11.48mm
12-lead surface-mounted (SMD) DIP package, row spacing 11.48 mm (451 mils)
SMD DIP DIL PDIP SMDIP 2.54mm 11.48mm 451mil
0
12
12
Package_DIP
SMDIP-14_W7.62mm
14-lead surface-mounted (SMD) DIP package, row spacing 7.62 mm (300 mils)
SMD DIP DIL PDIP SMDIP 2.54mm 7.62mm 300mil
0
14
14
Package_DIP
SMDIP-14_W9.53mm
14-lead surface-mounted (SMD) DIP package, row spacing 9.53 mm (375 mils)
SMD DIP DIL PDIP SMDIP 2.54mm 9.53mm 375mil
0
14
14
Package_DIP
SMDIP-14_W9.53mm_Clearance8mm
14-lead surface-mounted (SMD) DIP package, row spacing 9.53 mm (375 mils), Clearance8mm
SMD DIP DIL PDIP SMDIP 2.54mm 9.53mm 375mil Clearance8mm
0
14
14
Package_DIP
SMDIP-14_W11.48mm
14-lead surface-mounted (SMD) DIP package, row spacing 11.48 mm (451 mils)
SMD DIP DIL PDIP SMDIP 2.54mm 11.48mm 451mil
0
14
14
Package_DIP
SMDIP-16_W7.62mm
16-lead surface-mounted (SMD) DIP package, row spacing 7.62 mm (300 mils)
SMD DIP DIL PDIP SMDIP 2.54mm 7.62mm 300mil
0
16
16
Package_DIP
SMDIP-16_W9.53mm
16-lead surface-mounted (SMD) DIP package, row spacing 9.53 mm (375 mils)
SMD DIP DIL PDIP SMDIP 2.54mm 9.53mm 375mil
0
16
16
Package_DIP
SMDIP-16_W9.53mm_Clearance8mm
16-lead surface-mounted (SMD) DIP package, row spacing 9.53 mm (375 mils), Clearance8mm
SMD DIP DIL PDIP SMDIP 2.54mm 9.53mm 375mil Clearance8mm
0
16
16
Package_DIP
SMDIP-16_W11.48mm
16-lead surface-mounted (SMD) DIP package, row spacing 11.48 mm (451 mils)
SMD DIP DIL PDIP SMDIP 2.54mm 11.48mm 451mil
0
16
16
Package_DIP
SMDIP-18_W7.62mm
18-lead surface-mounted (SMD) DIP package, row spacing 7.62 mm (300 mils)
SMD DIP DIL PDIP SMDIP 2.54mm 7.62mm 300mil
0
18
18
Package_DIP
SMDIP-18_W9.53mm
18-lead surface-mounted (SMD) DIP package, row spacing 9.53 mm (375 mils)
SMD DIP DIL PDIP SMDIP 2.54mm 9.53mm 375mil
0
18
18
Package_DIP
SMDIP-18_W9.53mm_Clearance8mm
18-lead surface-mounted (SMD) DIP package, row spacing 9.53 mm (375 mils), Clearance8mm
SMD DIP DIL PDIP SMDIP 2.54mm 9.53mm 375mil Clearance8mm
0
18
18
Package_DIP
SMDIP-18_W11.48mm
18-lead surface-mounted (SMD) DIP package, row spacing 11.48 mm (451 mils)
SMD DIP DIL PDIP SMDIP 2.54mm 11.48mm 451mil
0
18
18
Package_DIP
SMDIP-20_W7.62mm
20-lead surface-mounted (SMD) DIP package, row spacing 7.62 mm (300 mils)
SMD DIP DIL PDIP SMDIP 2.54mm 7.62mm 300mil
0
20
20
Package_DIP
SMDIP-20_W9.53mm
20-lead surface-mounted (SMD) DIP package, row spacing 9.53 mm (375 mils)
SMD DIP DIL PDIP SMDIP 2.54mm 9.53mm 375mil
0
20
20
Package_DIP
SMDIP-20_W9.53mm_Clearance8mm
20-lead surface-mounted (SMD) DIP package, row spacing 9.53 mm (375 mils), Clearance8mm
SMD DIP DIL PDIP SMDIP 2.54mm 9.53mm 375mil Clearance8mm
0
20
20
Package_DIP
SMDIP-20_W11.48mm
20-lead surface-mounted (SMD) DIP package, row spacing 11.48 mm (451 mils)
SMD DIP DIL PDIP SMDIP 2.54mm 11.48mm 451mil
0
20
20
Package_DIP
SMDIP-22_W7.62mm
22-lead surface-mounted (SMD) DIP package, row spacing 7.62 mm (300 mils)
SMD DIP DIL PDIP SMDIP 2.54mm 7.62mm 300mil
0
22
22
Package_DIP
SMDIP-22_W9.53mm
22-lead surface-mounted (SMD) DIP package, row spacing 9.53 mm (375 mils)
SMD DIP DIL PDIP SMDIP 2.54mm 9.53mm 375mil
0
22
22
Package_DIP
SMDIP-22_W9.53mm_Clearance8mm
22-lead surface-mounted (SMD) DIP package, row spacing 9.53 mm (375 mils), Clearance8mm
SMD DIP DIL PDIP SMDIP 2.54mm 9.53mm 375mil Clearance8mm
0
22
22
Package_DIP
SMDIP-22_W11.48mm
22-lead surface-mounted (SMD) DIP package, row spacing 11.48 mm (451 mils)
SMD DIP DIL PDIP SMDIP 2.54mm 11.48mm 451mil
0
22
22
Package_DIP
SMDIP-24_W7.62mm
24-lead surface-mounted (SMD) DIP package, row spacing 7.62 mm (300 mils)
SMD DIP DIL PDIP SMDIP 2.54mm 7.62mm 300mil
0
24
24
Package_DIP
SMDIP-24_W9.53mm
24-lead surface-mounted (SMD) DIP package, row spacing 9.53 mm (375 mils)
SMD DIP DIL PDIP SMDIP 2.54mm 9.53mm 375mil
0
24
24
Package_DIP
SMDIP-24_W11.48mm
24-lead surface-mounted (SMD) DIP package, row spacing 11.48 mm (451 mils)
SMD DIP DIL PDIP SMDIP 2.54mm 11.48mm 451mil
0
24
24
Package_DIP
SMDIP-24_W15.24mm
24-lead surface-mounted (SMD) DIP package, row spacing 15.24 mm (600 mils)
SMD DIP DIL PDIP SMDIP 2.54mm 15.24mm 600mil
0
24
24
Package_DIP
SMDIP-28_W15.24mm
28-lead surface-mounted (SMD) DIP package, row spacing 15.24 mm (600 mils)
SMD DIP DIL PDIP SMDIP 2.54mm 15.24mm 600mil
0
28
28
Package_DIP
SMDIP-32_W7.62mm
32-lead surface-mounted (SMD) DIP package, row spacing 7.62 mm (300 mils)
SMD DIP DIL PDIP SMDIP 2.54mm 7.62mm 300mil
0
32
32
Package_DIP
SMDIP-32_W9.53mm
32-lead surface-mounted (SMD) DIP package, row spacing 9.53 mm (375 mils)
SMD DIP DIL PDIP SMDIP 2.54mm 9.53mm 375mil
0
32
32
Package_DIP
SMDIP-32_W11.48mm
32-lead surface-mounted (SMD) DIP package, row spacing 11.48 mm (451 mils)
SMD DIP DIL PDIP SMDIP 2.54mm 11.48mm 451mil
0
32
32
Package_DIP
SMDIP-32_W15.24mm
32-lead surface-mounted (SMD) DIP package, row spacing 15.24 mm (600 mils)
SMD DIP DIL PDIP SMDIP 2.54mm 15.24mm 600mil
0
32
32
Package_DIP
SMDIP-40_W15.24mm
40-lead surface-mounted (SMD) DIP package, row spacing 15.24 mm (600 mils)
SMD DIP DIL PDIP SMDIP 2.54mm 15.24mm 600mil
0
40
40
Package_DIP
SMDIP-40_W25.24mm
40-lead surface-mounted (SMD) DIP package, row spacing 25.24 mm (993 mils)
SMD DIP DIL PDIP SMDIP 2.54mm 25.24mm 993mil
0
40
40
Package_DIP
SMDIP-42_W15.24mm
42-lead surface-mounted (SMD) DIP package, row spacing 15.24 mm (600 mils)
SMD DIP DIL PDIP SMDIP 2.54mm 15.24mm 600mil
0
42
42
Package_DIP
SMDIP-48_W15.24mm
48-lead surface-mounted (SMD) DIP package, row spacing 15.24 mm (600 mils)
SMD DIP DIL PDIP SMDIP 2.54mm 15.24mm 600mil
0
48
48
Package_DIP
SMDIP-64_W15.24mm
64-lead surface-mounted (SMD) DIP package, row spacing 15.24 mm (600 mils)
SMD DIP DIL PDIP SMDIP 2.54mm 15.24mm 600mil
0
64
64
Package_DIP
Toshiba_11-7A9
Toshiba 11-7A9 package, like 6-lead dip package with missing pin 5, row spacing 7.62 mm (300 mils), https://toshiba.semicon-storage.com/info/docget.jsp?did=1421&prodName=TLP3021(S)
Toshiba 11-7A9 DIL DIP PDIP 2.54mm 7.62mm 300mil
0
5
5
Package_DIP
Vishay_HVM-DIP-3_W7.62mm
3-lead though-hole mounted high-volatge DIP package (based on standard DIP-4), row spacing 7.62 mm (300 mils), see https://www.vishay.com/docs/91361/hexdip.pdf
THT DIP DIL PDIP 2.54mm 7.62mm 300mil Vishay HVMDIP HEXDIP
0
4
3
Package_QFP
EQFP-144-1EP_20x20mm_P0.5mm_EP4x4mm
EQFP, 144 Pin (https://www.intel.com/content/dam/www/programmable/us/en/pdfs/literature/packaging/04r00482-02.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py
EQFP QFP
0
154
145
Package_QFP
EQFP-144-1EP_20x20mm_P0.5mm_EP4x4mm_ThermalVias
EQFP, 144 Pin (https://www.intel.com/content/dam/www/programmable/us/en/pdfs/literature/packaging/04r00482-02.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py
EQFP QFP
0
171
145
Package_QFP
EQFP-144-1EP_20x20mm_P0.5mm_EP5x5mm
EQFP, 144 Pin (https://www.intel.com/content/dam/www/programmable/us/en/pdfs/literature/packaging/04r00476-02.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py
EQFP QFP
0
161
145
Package_QFP
EQFP-144-1EP_20x20mm_P0.5mm_EP5x5mm_ThermalVias
EQFP, 144 Pin (https://www.intel.com/content/dam/www/programmable/us/en/pdfs/literature/packaging/04r00476-02.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py
EQFP QFP
0
187
145
Package_QFP
EQFP-144-1EP_20x20mm_P0.5mm_EP6.61x5.615mm
EQFP, 144 Pin (https://www.intel.com/content/dam/www/programmable/us/en/pdfs/literature/packaging/04r00485-02.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py
EQFP QFP
0
165
145
Package_QFP
EQFP-144-1EP_20x20mm_P0.5mm_EP6.61x5.615mm_ThermalVias
EQFP, 144 Pin (https://www.intel.com/content/dam/www/programmable/us/en/pdfs/literature/packaging/04r00485-02.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py
EQFP QFP
0
196
145
Package_QFP
EQFP-144-1EP_20x20mm_P0.5mm_EP7.2x6.35mm
EQFP, 144 Pin (https://www.intel.com/content/dam/www/programmable/us/en/pdfs/literature/packaging/04r00487-01.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py
EQFP QFP
0
175
145
Package_QFP
EQFP-144-1EP_20x20mm_P0.5mm_EP7.2x6.35mm_ThermalVias
EQFP, 144 Pin (https://www.intel.com/content/dam/www/programmable/us/en/pdfs/literature/packaging/04r00487-01.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py
EQFP QFP
0
218
145
Package_QFP
EQFP-144-1EP_20x20mm_P0.5mm_EP8.93x8.7mm
EQFP, 144 Pin (https://www.intel.com/content/dam/www/programmable/us/en/pdfs/literature/packaging/04r00479-02.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py
EQFP QFP
0
194
145
Package_QFP
EQFP-144-1EP_20x20mm_P0.5mm_EP8.93x8.7mm_ThermalVias
EQFP, 144 Pin (https://www.intel.com/content/dam/www/programmable/us/en/pdfs/literature/packaging/04r00479-02.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py
EQFP QFP
0
259
145
Package_QFP
HTQFP-64-1EP_10x10mm_P0.5mm_EP8x8mm
64-Lead Plastic Thin Quad Flatpack (PT) - 10x10x1 mm Body, 2.00 mm Footprint [HTQFP] thermal pad
HTQFP-64 Pitch 0.5 
0
69
65
Package_QFP
HTQFP-64-1EP_10x10mm_P0.5mm_EP8x8mm_Mask4.4x4.4mm_ThermalVias
64-Lead Plastic Thin Quad Flatpack (PT) - 10x10x1 mm Body, 2.00 mm Footprint [HTQFP] thermal pad
HTQFP-64 Pitch 0.5 
0
135
65
Package_QFP
LQFP-32_5x5mm_P0.5mm
LQFP, 32 Pin (https://www.nxp.com/docs/en/package-information/SOT401-1.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py
LQFP QFP
0
32
32
Package_QFP
LQFP-32_7x7mm_P0.8mm
LQFP, 32 Pin (https://www.nxp.com/docs/en/package-information/SOT358-1.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py
LQFP QFP
0
32
32
Package_QFP
LQFP-36_7x7mm_P0.65mm
LQFP, 36 Pin (https://www.onsemi.com/pub/Collateral/561AV.PDF), generated with kicad-footprint-generator ipc_gullwing_generator.py
LQFP QFP
0
36
36
Package_QFP
LQFP-44_10x10mm_P0.8mm
LQFP, 44 Pin (https://www.nxp.com/files-static/shared/doc/package_info/98ASS23225W.pdf?&fsrch=1), generated with kicad-footprint-generator ipc_gullwing_generator.py
LQFP QFP
0
44
44
Package_QFP
LQFP-48-1EP_7x7mm_P0.5mm_EP3.6x3.6mm
LQFP, 48 Pin (http://www.analog.com/media/en/technical-documentation/data-sheets/LTC7810.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py
LQFP QFP
0
58
49
Package_QFP
LQFP-48-1EP_7x7mm_P0.5mm_EP3.6x3.6mm_ThermalVias
LQFP, 48 Pin (http://www.analog.com/media/en/technical-documentation/data-sheets/LTC7810.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py
LQFP QFP
0
75
49
Package_QFP
LQFP-48_7x7mm_P0.5mm
LQFP, 48 Pin (https://www.analog.com/media/en/technical-documentation/data-sheets/ltc2358-16.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py
LQFP QFP
0
48
48
Package_QFP
LQFP-52-1EP_10x10mm_P0.65mm_EP4.8x4.8mm
LQFP, 52 Pin (https://www.onsemi.com/pub/Collateral/848H-01.PDF), generated with kicad-footprint-generator ipc_gullwing_generator.py
LQFP QFP
0
62
53
Package_QFP
LQFP-52-1EP_10x10mm_P0.65mm_EP4.8x4.8mm_ThermalVias
LQFP, 52 Pin (https://www.onsemi.com/pub/Collateral/848H-01.PDF), generated with kicad-footprint-generator ipc_gullwing_generator.py
LQFP QFP
0
95
53
Package_QFP
LQFP-52_10x10mm_P0.65mm
LQFP, 52 Pin (https://www.nxp.com/docs/en/package-information/98ARL10526D.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py
LQFP QFP
0
52
52
Package_QFP
LQFP-52_14x14mm_P1mm
LQFP, 52 Pin (http://www.holtek.com/documents/10179/116711/HT1632Cv170.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py
LQFP QFP
0
52
52
Package_QFP
LQFP-64-1EP_10x10mm_P0.5mm_EP5x5mm
LQFP, 64 Pin (https://www.analog.com/media/en/technical-documentation/data-sheets/adv7611.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py
LQFP QFP
0
90
65
Package_QFP
LQFP-64-1EP_10x10mm_P0.5mm_EP5x5mm_ThermalVias
LQFP, 64 Pin (https://www.analog.com/media/en/technical-documentation/data-sheets/adv7611.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py
LQFP QFP
0
107
65
Package_QFP
LQFP-64-1EP_10x10mm_P0.5mm_EP6.5x6.5mm
LQFP, 64 Pin (https://www.nxp.com/files-static/shared/doc/package_info/98ARH98426A.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py
LQFP QFP
0
90
65
Package_QFP
LQFP-64-1EP_10x10mm_P0.5mm_EP6.5x6.5mm_ThermalVias
LQFP, 64 Pin (https://www.nxp.com/files-static/shared/doc/package_info/98ARH98426A.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py
LQFP QFP
0
127
65
Package_QFP
LQFP-64_7x7mm_P0.4mm
LQFP, 64 Pin (https://www.nxp.com/docs/en/package-information/SOT414-1.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py
LQFP QFP
0
64
64
Package_QFP
LQFP-64_10x10mm_P0.5mm
LQFP, 64 Pin (https://www.analog.com/media/en/technical-documentation/data-sheets/ad7606_7606-6_7606-4.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py
LQFP QFP
0
64
64
Package_QFP
LQFP-64_14x14mm_P0.8mm
LQFP, 64 Pin (https://www.nxp.com/docs/en/package-information/SOT791-1.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py
LQFP QFP
0
64
64
Package_QFP
LQFP-80_10x10mm_P0.4mm
LQFP, 80 Pin (https://www.renesas.com/eu/en/package-image/pdf/outdrawing/q80.10x10.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py
LQFP QFP
0
80
80
Package_QFP
LQFP-80_12x12mm_P0.5mm
LQFP, 80 Pin (https://www.nxp.com/docs/en/package-information/SOT315-1.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py
LQFP QFP
0
80
80
Package_QFP
LQFP-80_14x14mm_P0.65mm
LQFP, 80 Pin (https://www.analog.com/media/en/technical-documentation/data-sheets/AD9852.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py
LQFP QFP
0
80
80
Package_QFP
LQFP-100_14x14mm_P0.5mm
LQFP, 100 Pin (https://www.nxp.com/docs/en/package-information/SOT407-1.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py
LQFP QFP
0
100
100
Package_QFP
LQFP-128_14x14mm_P0.4mm
LQFP, 128 Pin (https://www.renesas.com/eu/en/package-image/pdf/outdrawing/q128.14x14.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py
LQFP QFP
0
128
128
Package_QFP
LQFP-128_14x20mm_P0.5mm
LQFP, 128 Pin (https://www.nxp.com/docs/en/package-information/SOT425-1.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py
LQFP QFP
0
128
128
Package_QFP
LQFP-144_20x20mm_P0.5mm
LQFP, 144 Pin (http://ww1.microchip.com/downloads/en/PackagingSpec/00000049BQ.pdf#page=425), generated with kicad-footprint-generator ipc_gullwing_generator.py
LQFP QFP
0
144
144
Package_QFP
LQFP-160_24x24mm_P0.5mm
LQFP, 160 Pin (https://www.nxp.com/docs/en/package-information/SOT435-1.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py
LQFP QFP
0
160
160
Package_QFP
LQFP-176_20x20mm_P0.4mm
LQFP, 176 Pin (https://www.onsemi.com/pub/Collateral/566DB.PDF), generated with kicad-footprint-generator ipc_gullwing_generator.py
LQFP QFP
0
176
176
Package_QFP
LQFP-176_24x24mm_P0.5mm
LQFP, 176 Pin (https://www.st.com/resource/en/datasheet/stm32f207vg.pdf#page=163), generated with kicad-footprint-generator ipc_gullwing_generator.py
LQFP QFP
0
176
176
Package_QFP
LQFP-208_28x28mm_P0.5mm
LQFP, 208 Pin (https://www.nxp.com/docs/en/package-information/SOT459-1.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py
LQFP QFP
0
208
208
Package_QFP
LQFP-216_24x24mm_P0.4mm
LQFP, 216 Pin (https://www.onsemi.com/pub/Collateral/561BE.PDF), generated with kicad-footprint-generator ipc_gullwing_generator.py
LQFP QFP
0
216
216
Package_QFP
MQFP-44_10x10mm_P0.8mm
MQFP, 44 Pin (https://www.analog.com/media/en/technical-documentation/data-sheets/ad7722.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py
MQFP QFP
0
44
44
Package_QFP
PQFP-44_10x10mm_P0.8mm
44-Lead Plastic Quad Flatpack - 10x10x2.5mm Body (http://www.onsemi.com/pub/Collateral/122BK.PDF)
PQFP 0.8
0
44
44
Package_QFP
PQFP-80_14x20mm_P0.8mm
PQFP80 14x20 / QIP80E CASE 122BS (see ON Semiconductor 122BS.PDF)
QFP 0.8
0
80
80
Package_QFP
PQFP-100_14x20mm_P0.65mm
PQFP, 100 Pin (http://www.microsemi.com/index.php?option=com_docman&task=doc_download&gid=131095), generated with kicad-footprint-generator ipc_gullwing_generator.py
PQFP QFP
0
100
100
Package_QFP
PQFP-112_20x20mm_P0.65mm
PQFP, 112 pins, 20mm sq body, 0.65mm pitch (http://cache.freescale.com/files/shared/doc/package_info/98ASS23330W.pdf, http://www.nxp.com/docs/en/application-note/AN4388.pdf)
PQFP 112
0
112
112
Package_QFP
PQFP-132_24x24mm_P0.635mm
PQFP, 132 pins, 24mm sq body, 0.635mm pitch (https://www.intel.com/content/dam/www/public/us/en/documents/packaging-databooks/packaging-chapter-02-databook.pdf, http://www.nxp.com/docs/en/application-note/AN4388.pdf)
PQFP 132
0
132
132
Package_QFP
PQFP-132_24x24mm_P0.635mm_i386
PQFP, 132 pins, 24mm sq body, 0.635mm pitch, Intel 386EX (https://www.intel.com/content/dam/www/public/us/en/documents/packaging-databooks/packaging-chapter-02-databook.pdf, http://www.nxp.com/docs/en/application-note/AN4388.pdf)
PQFP 132 Intel 386EX
0
132
132
Package_QFP
PQFP-144_28x28mm_P0.65mm
PQFP, 144 Pin (http://www.microsemi.com/index.php?option=com_docman&task=doc_download&gid=131095), generated with kicad-footprint-generator ipc_gullwing_generator.py
PQFP QFP
0
144
144
Package_QFP
PQFP-160_28x28mm_P0.65mm
PQFP, 160 Pin (http://www.microsemi.com/index.php?option=com_docman&task=doc_download&gid=131095), generated with kicad-footprint-generator ipc_gullwing_generator.py
PQFP QFP
0
160
160
Package_QFP
PQFP-208_28x28mm_P0.5mm
PQFP, 208 Pin (http://www.microsemi.com/index.php?option=com_docman&task=doc_download&gid=131095), generated with kicad-footprint-generator ipc_gullwing_generator.py
PQFP QFP
0
208
208
Package_QFP
PQFP-240_32.1x32.1mm_P0.5mm
PQFP, 240 Pin (http://www.microsemi.com/index.php?option=com_docman&task=doc_download&gid=131095), generated with kicad-footprint-generator ipc_gullwing_generator.py
PQFP QFP
0
240
240
Package_QFP
PQFP-256_28x28mm_P0.4mm
PQFP256 28x28 / QFP256J CASE 122BX (see ON Semiconductor 122BX.PDF)
QFP 0.4
0
256
256
Package_QFP
TQFP-32_7x7mm_P0.8mm
32-Lead Plastic Thin Quad Flatpack (PT) - 7x7x1.0 mm Body, 2.00 mm [TQFP] (see Microchip Packaging Specification 00000049BS.pdf)
QFP 0.8
0
32
32
Package_QFP
TQFP-44-1EP_10x10mm_P0.8mm_EP4.5x4.5mm
44-Lead Plastic Thin Quad Flatpack (MW) - 10x10x1.0 mm Body [TQFP] With 4.5x4.5 mm Exposed Pad (see Microchip Packaging Specification 00000049BS.pdf)
QFP 0.8
0
54
45
Package_QFP
TQFP-44_10x10mm_P0.8mm
44-Lead Plastic Thin Quad Flatpack (PT) - 10x10x1.0 mm Body [TQFP] (see Microchip Packaging Specification 00000049BS.pdf)
QFP 0.8
0
44
44
Package_QFP
TQFP-48-1EP_7x7mm_P0.5mm_EP3.5x3.5mm
48-Lead Thin Quad Flatpack (PT) - 7x7x1.0 mm Body [TQFP] With Exposed Pad (see Microchip Packaging Specification 00000049BS.pdf)
QFP 0.5
0
53
49
Package_QFP
TQFP-48-1EP_7x7mm_P0.5mm_EP5x5mm
TQFP, 48 Pin (https://www.trinamic.com/fileadmin/assets/Products/ICs_Documents/TMC2100_datasheet_Rev1.08.pdf (page 45)), generated with kicad-footprint-generator ipc_gullwing_generator.py
TQFP QFP
0
65
49
Package_QFP
TQFP-48-1EP_7x7mm_P0.5mm_EP5x5mm_ThermalVias
TQFP, 48 Pin (https://www.trinamic.com/fileadmin/assets/Products/ICs_Documents/TMC2100_datasheet_Rev1.08.pdf (page 45)), generated with kicad-footprint-generator ipc_gullwing_generator.py
TQFP QFP
0
91
49
Package_QFP
TQFP-48_7x7mm_P0.5mm
48 LEAD TQFP 7x7mm (see MICREL TQFP7x7-48LD-PL-1.pdf)
QFP 0.5
0
48
48
Package_QFP
TQFP-52-1EP_10x10mm_P0.65mm_EP6.5x6.5mm
TQFP, 52 Pin (http://www.analog.com/media/en/package-pcb-resources/package/pkg_pdf/tqfp_edsv/sv_52_1.pdf), generated with kicad-footprint-generator ipc_qfp_generator.py
TQFP QFP
0
78
53
Package_QFP
TQFP-52-1EP_10x10mm_P0.65mm_EP6.5x6.5mm_ThermalVias
TQFP, 52 Pin (http://www.analog.com/media/en/package-pcb-resources/package/pkg_pdf/tqfp_edsv/sv_52_1.pdf), generated with kicad-footprint-generator ipc_qfp_generator.py
TQFP QFP
0
79
53
Package_QFP
TQFP-64-1EP_10x10mm_P0.5mm_EP8x8mm
64-Lead Plastic Thin Quad Flatpack (PT) - 10x10x1 mm Body, 2.00 mm Footprint [TQFP] thermal pad
QFP 0.5 
0
90
65
Package_QFP
TQFP-64_7x7mm_P0.4mm
TQFP64 7x7, 0.4P CASE 932BH (see ON Semiconductor 932BH.PDF)
QFP 0.4
0
64
64
Package_QFP
TQFP-64_10x10mm_P0.5mm
TQFP, 64 Pin (http://www.microsemi.com/index.php?option=com_docman&task=doc_download&gid=131095), generated with kicad-footprint-generator ipc_gullwing_generator.py
TQFP QFP
0
64
64
Package_QFP
TQFP-64_14x14mm_P0.8mm
64-Lead Plastic Thin Quad Flatpack (PF) - 14x14x1 mm Body, 2.00 mm [TQFP] (see Microchip Packaging Specification 00000049BS.pdf)
QFP 0.8
0
64
64
Package_QFP
TQFP-80-1EP_14x14mm_P0.65mm_EP9.5x9.5mm
80-Lead Plastic Thin Quad Flatpack (PF) - 14x14mm body, 9.5mm sq thermal pad (http://www.analog.com/media/en/technical-documentation/data-sheets/AD9852.pdf)
QFP 0.65
0
85
81
Package_QFP
TQFP-80_12x12mm_P0.5mm
80-Lead Plastic Thin Quad Flatpack (PT) - 12x12x1 mm Body, 2.00 mm [TQFP] (see Microchip Packaging Specification 00000049BS.pdf)
QFP 0.5
0
80
80
Package_QFP
TQFP-80_14x14mm_P0.65mm
80-Lead Plastic Thin Quad Flatpack (PF) - 14x14x1 mm Body, 2.00 mm [TQFP] (see Microchip Packaging Specification 00000049BS.pdf)
QFP 0.65
0
80
80
Package_QFP
TQFP-100-1EP_14x14mm_P0.5mm_EP5x5mm
TQFP, 100 Pin (https://www.analog.com/media/en/package-pcb-resources/package/pkg_pdf/tqfp_edsv/sv_100_4.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py
TQFP QFP
0
117
101
Package_QFP
TQFP-100-1EP_14x14mm_P0.5mm_EP5x5mm_ThermalVias
TQFP, 100 Pin (https://www.analog.com/media/en/package-pcb-resources/package/pkg_pdf/tqfp_edsv/sv_100_4.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py
TQFP QFP
0
143
101
Package_QFP
TQFP-100_12x12mm_P0.4mm
100-Lead Plastic Thin Quad Flatpack (PT) - 12x12x1 mm Body, 2.00 mm [TQFP] (see Microchip Packaging Specification 00000049BS.pdf)
QFP 0.4
0
100
100
Package_QFP
TQFP-100_14x14mm_P0.5mm
TQFP, 100 Pin (http://www.microsemi.com/index.php?option=com_docman&task=doc_download&gid=131095), generated with kicad-footprint-generator ipc_gullwing_generator.py
TQFP QFP
0
100
100
Package_QFP
TQFP-120_14x14mm_P0.4mm
TQFP120 14x14 / TQFP120 CASE 932AZ (see ON Semiconductor 932AZ.PDF)
QFP 0.4
0
120
120
Package_QFP
TQFP-128_14x14mm_P0.4mm
TQFP128 14x14 / TQFP128 CASE 932BB (see ON Semiconductor 932BB.PDF)
QFP 0.4
0
128
128
Package_QFP
TQFP-144_16x16mm_P0.4mm
144-Lead Plastic Thin Quad Flatpack (PH) - 16x16x1 mm Body, 2.00 mm Footprint [TQFP] (see Microchip Packaging Specification 00000049BS.pdf)
QFP 0.4
0
144
144
Package_QFP
TQFP-144_20x20mm_P0.5mm
TQFP, 144 Pin (http://www.microsemi.com/index.php?option=com_docman&task=doc_download&gid=131095), generated with kicad-footprint-generator ipc_gullwing_generator.py
TQFP QFP
0
144
144
Package_QFP
TQFP-176_24x24mm_P0.5mm
TQFP, 176 Pin (http://www.microsemi.com/index.php?option=com_docman&task=doc_download&gid=131095), generated with kicad-footprint-generator ipc_gullwing_generator.py
TQFP QFP
0
176
176
Package_QFP
VQFP-80_14x14mm_P0.65mm
VQFP, 80 Pin (http://www.microsemi.com/index.php?option=com_docman&task=doc_download&gid=131095), generated with kicad-footprint-generator ipc_gullwing_generator.py
VQFP QFP
0
80
80
Package_QFP
VQFP-100_14x14mm_P0.5mm
VQFP, 100 Pin (http://www.microsemi.com/index.php?option=com_docman&task=doc_download&gid=131095), generated with kicad-footprint-generator ipc_gullwing_generator.py
VQFP QFP
0
100
100
Package_QFP
VQFP-128_14x14mm_P0.4mm
VQFP, 128 Pin (http://www.microsemi.com/index.php?option=com_docman&task=doc_download&gid=131095), generated with kicad-footprint-generator ipc_gullwing_generator.py
VQFP QFP
0
128
128
Package_QFP
VQFP-176_20x20mm_P0.4mm
VQFP, 176 Pin (http://www.microsemi.com/index.php?option=com_docman&task=doc_download&gid=131095), generated with kicad-footprint-generator ipc_gullwing_generator.py
VQFP QFP
0
176
176
Package_SO
Diodes_PSOP-8
8-Lead Plastic PSOP, Exposed Die Pad (see https://www.diodes.com/assets/Datasheets/AP2204.pdf)
SSOP 0.50 exposed pad
0
12
9
Package_SO
Diodes_SO-8EP
8-Lead Plastic SO, Exposed Die Pad (see https://www.diodes.com/assets/Package-Files/SO-8EP.pdf)
SO exposed pad
0
9
9
Package_SO
ETSSOP-20-1EP_4.4x6.5mm_P0.65mm_EP3x4.2mm
20-Lead Plastic Thin Shrink Small Outline (ST)-4.4 mm Body with Exposed Pad [eTSSOP] (see Microchip Packaging Specification 00000049BS.pdf)
SSOP 0.65
0
27
21
Package_SO
HSOP-8-1EP_3.9x4.9mm_P1.27mm_EP2.41x3.1mm
HSOP, 8 Pin (https://www.st.com/resource/en/datasheet/l5973d.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py
HSOP SO
0
13
9
Package_SO
HSOP-8-1EP_3.9x4.9mm_P1.27mm_EP2.41x3.1mm_ThermalVias
HSOP, 8 Pin (https://www.st.com/resource/en/datasheet/l5973d.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py
HSOP SO
0
20
9
Package_SO
HSOP-20-1EP_11.0x15.9mm_P1.27mm_SlugDown
HSOP 11.0x15.9mm Pitch 1.27mm Slug Down (PowerSO-20) [JEDEC MO-166] (http://www.st.com/resource/en/datasheet/tda7266d.pdf, www.st.com/resource/en/application_note/cd00003801.pdf)
HSOP 11.0 x 15.9mm Pitch 1.27mm
0
23
21
Package_SO
HSOP-20-1EP_11.0x15.9mm_P1.27mm_SlugDown_ThermalVias
HSOP 11.0x15.9mm Pitch 1.27mm Slug Down Thermal Vias (PowerSO-20) [JEDEC MO-166] (http://www.st.com/resource/en/datasheet/tda7266d.pdf, www.st.com/resource/en/application_note/cd00003801.pdf)
HSOP 11.0 x 15.9mm Pitch 1.27mm
0
45
21
Package_SO
HSOP-20-1EP_11.0x15.9mm_P1.27mm_SlugUp
HSOP 11.0x15.9mm Pitch 1.27mm Slug Up (PowerSO-20) [JEDEC MO-166] (http://www.st.com/resource/en/datasheet/tda7266d.pdf, www.st.com/resource/en/application_note/cd00003801.pdf)
HSOP 11.0 x 15.9mm Pitch 1.27mm
0
20
20
Package_SO
HSOP-36-1EP_11.0x15.9mm_P0.65mm_SlugDown
HSOP 11.0x15.9mm Pitch 0.65mm Slug Down (PowerSO-36) [JEDEC MO-166] (http://www.st.com/resource/en/datasheet/vn808cm-32-e.pdf, http://www.st.com/resource/en/application_note/cd00003801.pdf)
HSOP 11.0 x 15.9mm Pitch 0.65mm
0
39
37
Package_SO
HSOP-36-1EP_11.0x15.9mm_P0.65mm_SlugDown_ThermalVias
HSOP 11.0x15.9mm Pitch 0.65mm Slug Down Thermal Vias (PowerSO-36) [JEDEC MO-166] (http://www.st.com/resource/en/datasheet/vn808cm-32-e.pdf, http://www.st.com/resource/en/application_note/cd00003801.pdf)
HSOP 11.0 x 15.9mm Pitch 0.65mm
0
61
37
Package_SO
HSOP-36-1EP_11.0x15.9mm_P0.65mm_SlugUp
HSOP 11.0x15.9mm Pitch 0.65mm Slug Up (PowerSO-36) [JEDEC MO-166] (http://www.st.com/resource/en/datasheet/vn808cm-32-e.pdf, http://www.st.com/resource/en/application_note/cd00003801.pdf)
HSOP 11.0 x 15.9mm Pitch 0.65mm
0
36
36
Package_SO
HTSOP-8-1EP_3.9x4.9mm_P1.27mm_EP2.4x3.2mm
HTSOP, 8 Pin (https://media.digikey.com/pdf/Data%20Sheets/Rohm%20PDFs/BD9G341EFJ.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py
HTSOP SO
0
13
9
Package_SO
HTSOP-8-1EP_3.9x4.9mm_P1.27mm_EP2.4x3.2mm_ThermalVias
HTSOP, 8 Pin (https://media.digikey.com/pdf/Data%20Sheets/Rohm%20PDFs/BD9G341EFJ.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py
HTSOP SO
0
20
9
Package_SO
HTSSOP-16-1EP_4.4x5mm_P0.65mm_EP3.4x5mm
16-Lead Plastic HTSSOP (4.4x5x1.2mm); Thermal pad; (http://www.ti.com/lit/ds/symlink/drv8833.pdf)
SSOP 0.65
0
29
17
Package_SO
HTSSOP-16-1EP_4.4x5mm_P0.65mm_EP3.4x5mm_Mask2.46x2.31mm
HTSSOP, 16 Pin (http://www.analog.com/media/en/technical-documentation/data-sheets/LTC7810.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py
HTSSOP SO
0
20
17
Package_SO
HTSSOP-16-1EP_4.4x5mm_P0.65mm_EP3.4x5mm_Mask2.46x2.31mm_ThermalVias
HTSSOP, 16 Pin (http://www.analog.com/media/en/technical-documentation/data-sheets/LTC7810.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py
HTSSOP SO
0
27
17
Package_SO
HTSSOP-16-1EP_4.4x5mm_P0.65mm_EP3.4x5mm_Mask3x3mm_ThermalVias
16-Lead Plastic HTSSOP (4.4x5x1.2mm); Thermal pad with vias; (http://www.ti.com/lit/ds/symlink/drv8800.pdf)
SSOP 0.65
0
46
17
Package_SO
HTSSOP-16-1EP_4.4x5mm_P0.65mm_EP3x3mm
HTSSOP, 16 Pin (https://www.st.com/resource/en/datasheet/stp08cp05.pdf#page=20), generated with kicad-footprint-generator ipc_gullwing_generator.py
HTSSOP SO
0
21
17
Package_SO
HTSSOP-20-1EP_4.4x6.5mm_P0.65mm_EP3.4x6.5mm
20-Lead Plastic Thin Shrink Small Outline (ST)-4.4 mm Body [HTSSOP], with thermal pad with vias
HTSSOP 0.65
0
29
21
Package_SO
HTSSOP-20-1EP_4.4x6.5mm_P0.65mm_EP3.4x6.5mm_Mask2.4x3.7mm
HTSSOP, 20 Pin (http://www.ti.com/lit/ds/symlink/bq24006.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py
HTSSOP SO
0
24
21
Package_SO
HTSSOP-20-1EP_4.4x6.5mm_P0.65mm_EP3.4x6.5mm_Mask2.75x3.43mm
HTSSOP, 20 Pin (http://www.ti.com/lit/ds/symlink/tlc5971.pdf#page=37&zoom=160,-90,3), generated with kicad-footprint-generator ipc_gullwing_generator.py
HTSSOP SO
0
26
21
Package_SO
HTSSOP-20-1EP_4.4x6.5mm_P0.65mm_EP3.4x6.5mm_Mask2.75x3.43mm_ThermalVias
HTSSOP, 20 Pin (http://www.ti.com/lit/ds/symlink/tlc5971.pdf#page=37&zoom=160,-90,3), generated with kicad-footprint-generator ipc_gullwing_generator.py
HTSSOP SO
0
42
21
Package_SO
HTSSOP-20-1EP_4.4x6.5mm_P0.65mm_EP3.4x6.5mm_Mask2.75x3.43mm_ThermalVias_HandSolder
HTSSOP, 20 Pin (http://www.ti.com/lit/ds/symlink/tlc5971.pdf#page=37&zoom=160,-90,3), generated with kicad-footprint-generator ipc_gullwing_generator.py
HTSSOP SO
0
42
21
Package_SO
HTSSOP-20-1EP_4.4x6.5mm_P0.65mm_EP3.4x6.5mm_ThermalVias
20-Lead Plastic Thin Shrink Small Outline (ST)-4.4 mm Body [HTSSOP], with thermal pad with vias
HTSSOP 0.65
0
45
21
Package_SO
HTSSOP-24-1EP_4.4x7.8mm_P0.65mm_EP3.2x5mm
HTSSOP, 24 Pin (https://www.st.com/resource/en/datasheet/stp16cp05.pdf#page=25), generated with kicad-footprint-generator ipc_gullwing_generator.py
HTSSOP SO
0
31
25
Package_SO
HTSSOP-24-1EP_4.4x7.8mm_P0.65mm_EP3.4x7.8mm_Mask2.4x4.68mm
HTSSOP, 24 Pin (http://www.ti.com/lit/ds/symlink/tps703.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py
HTSSOP SO
0
28
25
Package_SO
HTSSOP-24-1EP_4.4x7.8mm_P0.65mm_EP3.4x7.8mm_Mask2.4x4.68mm_ThermalVias
HTSSOP, 24 Pin (http://www.ti.com/lit/ds/symlink/tps703.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py
HTSSOP SO
0
47
25
Package_SO
HTSSOP-28-1EP_4.4x9.7mm_P0.65mm_EP2.85x5.4mm
HTSSOP, 28 Pin (https://pdfserv.maximintegrated.com/package_dwgs/21-0108.PDF), generated with kicad-footprint-generator ipc_gullwing_generator.py
HTSSOP SO
0
30
29
Package_SO
HTSSOP-28-1EP_4.4x9.7mm_P0.65mm_EP2.85x5.4mm_ThermalVias
HTSSOP, 28 Pin (https://pdfserv.maximintegrated.com/package_dwgs/21-0108.PDF), generated with kicad-footprint-generator ipc_gullwing_generator.py
HTSSOP SO
0
41
29
Package_SO
HTSSOP-28-1EP_4.4x9.7mm_P0.65mm_EP3.4x9.5mm
HTSSOP28: plastic thin shrink small outline package; 28 leads; body width 4.4 mm; thermal pad
TSSOP HTSSOP 0.65 thermal pad
0
39
29
Package_SO
HTSSOP-28-1EP_4.4x9.7mm_P0.65mm_EP3.4x9.5mm_Mask2.4x6.17mm
HTSSOP28: plastic thin shrink small outline package; 28 leads; body width 4.4 mm; thermal pad
TSSOP HTSSOP 0.65 thermal pad
0
40
29
Package_SO
HTSSOP-28-1EP_4.4x9.7mm_P0.65mm_EP3.4x9.5mm_Mask2.4x6.17mm_ThermalVias
HTSSOP28: plastic thin shrink small outline package; 28 leads; body width 4.4 mm; thermal pad
TSSOP HTSSOP 0.65 thermal pad
0
55
29
Package_SO
HTSSOP-28-1EP_4.4x9.7mm_P0.65mm_EP3.4x9.5mm_ThermalVias
HTSSOP28: plastic thin shrink small outline package; 28 leads; body width 4.4 mm; thermal pad
TSSOP HTSSOP 0.65 thermal pad
0
58
29
Package_SO
HTSSOP-32-1EP_6.1x11mm_P0.65mm_EP5.2x11mm_Mask4.11x4.36mm
HTSSOP32: plastic thin shrink small outline package; 32 leads; body width 6.1 mm; lead pitch 0.65 mm (see NXP SSOP-TSSOP-VSO-REFLOW.pdf and sot487-1_po.pdf)
SSOP 0.65 PowerPAD
0
43
33
Package_SO
HTSSOP-32-1EP_6.1x11mm_P0.65mm_EP5.2x11mm_Mask4.11x4.36mm_ThermalVias
HTSSOP32: plastic thin shrink small outline package; 32 leads; body width 6.1 mm; lead pitch 0.65 mm (see NXP SSOP-TSSOP-VSO-REFLOW.pdf and sot487-1_po.pdf)
SSOP 0.65 PowerPAD
0
83
33
Package_SO
HTSSOP-38-1EP_6.1x12.5mm_P0.65mm_EP5.2x12.5mm_Mask3.39x6.35mm
HTSSOP, 38 Pin (http://www.ti.com/lit/ds/symlink/tlc5951.pdf#page=47&zoom=140,-67,15), generated with kicad-footprint-generator ipc_gullwing_generator.py
HTSSOP SO
0
46
39
Package_SO
HTSSOP-38-1EP_6.1x12.5mm_P0.65mm_EP5.2x12.5mm_Mask3.39x6.35mm_ThermalVias
HTSSOP, 38 Pin (http://www.ti.com/lit/ds/symlink/tlc5951.pdf#page=47&zoom=140,-67,15), generated with kicad-footprint-generator ipc_gullwing_generator.py
HTSSOP SO
0
87
39
Package_SO
HTSSOP-56-1EP_6.1x14mm_P0.5mm_EP3.61x6.35mm
HTSSOP56: plastic thin shrink small outline package http://www.ti.com/lit/ds/symlink/drv8301.pdf
HTSSOP 0.5
0
72
57
Package_SO
Infineon_PG-DSO-8-27_3.9x4.9mm_EP2.65x3mm
Infineon  PG-DSO, 8 Pin (https://www.infineon.com/cms/en/product/packages/PG-DSO/PG-DSO-8-27), generated with kicad-footprint-generator ipc_gullwing_generator.py
Infineon PG-DSO SO
0
13
9
Package_SO
Infineon_PG-DSO-8-27_3.9x4.9mm_EP2.65x3mm_ThermalVias
Infineon  PG-DSO, 8 Pin (https://www.infineon.com/cms/en/product/packages/PG-DSO/PG-DSO-8-27), generated with kicad-footprint-generator ipc_gullwing_generator.py
Infineon PG-DSO SO
0
23
9
Package_SO
Infineon_PG-DSO-8-43
Infineon_PG-DSO-8-43
DSO DSO-8 SOIC SOIC-8
0
12
9
Package_SO
Infineon_PG-DSO-12-9
Infineon PG-DSO 12 pin, exposed pad: 4.5x8.1mm, with thermal vias (https://www.infineon.com/cms/en/product/packages/PG-DSO/PG-DSO-12-9/)
PG-DSO
0
23
13
Package_SO
Infineon_PG-DSO-12-9_ThermalVias
Infineon PG-DSO 12 pin, exposed pad: 4.5x8.1mm, with thermal vias (https://www.infineon.com/cms/en/product/packages/PG-DSO/PG-DSO-12-9/)
PG-DSO
0
42
13
Package_SO
Infineon_PG-DSO-12-11
Infineon PG-DSO 12 pin, exposed pad: 4.5x8.1mm, with thermal vias (https://www.infineon.com/cms/en/product/packages/PG-DSO/PG-DSO-12-11/)
PG-DSO
0
23
13
Package_SO
Infineon_PG-DSO-12-11_ThermalVias
Infineon PG-DSO 12 pin, exposed pad: 4.5x8.1mm, with thermal vias (https://www.infineon.com/cms/en/product/packages/PG-DSO/PG-DSO-12-11/)
PG-DSO
0
42
13
Package_SO
Infineon_PG-DSO-20-30
Infineon SO package 20pin, exposed pad 4.5x7mm (https://www.infineon.com/cms/en/product/packages/PG-DSO/PG-DSO-20-71/)
DSO-20
0
31
21
Package_SO
Infineon_PG-DSO-20-30_ThermalVias
Infineon SO package 20pin, exposed pad 4.5x7mm (https://www.infineon.com/cms/en/product/packages/PG-DSO/PG-DSO-20-71/)
DSO-20
0
45
21
Package_SO
Infineon_PG-DSO-20-32
Infineon SO package 20pin without exposed pad (https://www.infineon.com/cms/en/product/packages/PG-DSO/PG-DSO-20-32/)
DSO-20
0
20
20
Package_SO
Infineon_PG-TSDSO-14-22
Infineon_PG-TSDSO-14-22
Infineon TSDSO 14-22 
0
17
15
Package_SO
Linear_MSOP-12-16-1EP_3x4mm_P0.5mm
12-Lead Plastic Micro Small Outline Package (MS) [MSOP], variant of MSOP-16 (see http://cds.linear.com/docs/en/datasheet/3630fd.pdf)
SSOP 0.5
0
15
13
Package_SO
Linear_MSOP-12-16_3x4mm_P0.5mm
12-Lead Plastic Micro Small Outline Package (MS) [MSOP], variant of MSOP-16 (see https://www.analog.com/media/en/technical-documentation/data-sheets/3748fb.pdf)
SSOP 0.5
0
12
12
Package_SO
MFSOP6-4_4.4x3.6mm_P1.27mm
https://toshiba.semicon-storage.com/ap-en/design-support/package/detail.4pin%20MFSOP6.html
MFSOP 4 pin SMD
0
4
4
Package_SO
MFSOP6-5_4.4x3.6mm_P1.27mm
https://toshiba.semicon-storage.com/ap-en/design-support/package/detail.5pin%20MFSOP6.html
MFSOP 4 pin SMD
0
5
5
Package_SO
MSOP-8-1EP_3x3mm_P0.65mm_EP1.68x1.88mm
MSOP, 8 Pin (https://www.analog.com/media/en/technical-documentation/data-sheets/4440fb.pdf#page=13), generated with kicad-footprint-generator ipc_gullwing_generator.py
MSOP SO
0
13
9
Package_SO
MSOP-8-1EP_3x3mm_P0.65mm_EP1.68x1.88mm_ThermalVias
MSOP, 8 Pin (https://www.analog.com/media/en/technical-documentation/data-sheets/4440fb.pdf#page=13), generated with kicad-footprint-generator ipc_gullwing_generator.py
MSOP SO
0
18
9
Package_SO
MSOP-8-1EP_3x3mm_P0.65mm_EP1.73x1.85mm
MSOP, 8 Pin (http://www.ti.com/lit/ds/symlink/lm25085.pdf#page=32), generated with kicad-footprint-generator ipc_gullwing_generator.py
MSOP SO
0
13
9
Package_SO
MSOP-8-1EP_3x3mm_P0.65mm_EP1.73x1.85mm_ThermalVias
MSOP, 8 Pin (http://www.ti.com/lit/ds/symlink/lm25085.pdf#page=32), generated with kicad-footprint-generator ipc_gullwing_generator.py
MSOP SO
0
18
9
Package_SO
MSOP-8-1EP_3x3mm_P0.65mm_EP1.95x2.15mm
MSOP, 8 Pin (http://www.st.com/resource/en/datasheet/pm8834.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py
MSOP SO
0
13
9
Package_SO
MSOP-8-1EP_3x3mm_P0.65mm_EP1.95x2.15mm_ThermalVias
MSOP, 8 Pin (http://www.st.com/resource/en/datasheet/pm8834.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py
MSOP SO
0
18
9
Package_SO
MSOP-8-1EP_3x3mm_P0.65mm_EP2.5x3mm_Mask1.73x2.36mm
MSOP, 8 Pin (http://ww1.microchip.com/downloads/en/DeviceDoc/mic5355_6.pdf#page=15), generated with kicad-footprint-generator ipc_gullwing_generator.py
MSOP SO
0
14
9
Package_SO
MSOP-8-1EP_3x3mm_P0.65mm_EP2.5x3mm_Mask1.73x2.36mm_ThermalVias
MSOP, 8 Pin (http://ww1.microchip.com/downloads/en/DeviceDoc/mic5355_6.pdf#page=15), generated with kicad-footprint-generator ipc_gullwing_generator.py
MSOP SO
0
19
9
Package_SO
MSOP-8_3x3mm_P0.65mm
MSOP, 8 Pin (https://www.jedec.org/system/files/docs/mo-187F.pdf variant AA), generated with kicad-footprint-generator ipc_gullwing_generator.py
MSOP SO
0
8
8
Package_SO
MSOP-10-1EP_3x3mm_P0.5mm_EP1.68x1.88mm
MSOP, 10 Pin (https://www.analog.com/media/en/technical-documentation/data-sheets/3805fg.pdf#page=18), generated with kicad-footprint-generator ipc_gullwing_generator.py
MSOP SO
0
15
11
Package_SO
MSOP-10-1EP_3x3mm_P0.5mm_EP1.68x1.88mm_ThermalVias
MSOP, 10 Pin (https://www.analog.com/media/en/technical-documentation/data-sheets/3805fg.pdf#page=18), generated with kicad-footprint-generator ipc_gullwing_generator.py
MSOP SO
0
20
11
Package_SO
MSOP-10-1EP_3x3mm_P0.5mm_EP1.73x1.98mm
MSOP, 10 Pin (www.allegromicro.com/~/media/Files/Datasheets/A4952-3-Datasheet.ashx?la=en#page=10), generated with kicad-footprint-generator ipc_gullwing_generator.py
MSOP SO
0
15
11
Package_SO
MSOP-10-1EP_3x3mm_P0.5mm_EP1.73x1.98mm_ThermalVias
MSOP, 10 Pin (www.allegromicro.com/~/media/Files/Datasheets/A4952-3-Datasheet.ashx?la=en#page=10), generated with kicad-footprint-generator ipc_gullwing_generator.py
MSOP SO
0
20
11
Package_SO
MSOP-10_3x3mm_P0.5mm
10-Lead Plastic Micro Small Outline Package (MS) [MSOP] (see Microchip Packaging Specification 00000049BS.pdf)
SSOP 0.5
0
10
10
Package_SO
MSOP-12-1EP_3x4mm_P0.65mm_EP1.65x2.85mm
MSOP, 12 Pin (https://www.analog.com/media/en/technical-documentation/data-sheets/3652fe.pdf#page=24), generated with kicad-footprint-generator ipc_gullwing_generator.py
MSOP SO
0
17
13
Package_SO
MSOP-12-1EP_3x4mm_P0.65mm_EP1.65x2.85mm_ThermalVias
MSOP, 12 Pin (https://www.analog.com/media/en/technical-documentation/data-sheets/3652fe.pdf#page=24), generated with kicad-footprint-generator ipc_gullwing_generator.py
MSOP SO
0
24
13
Package_SO
MSOP-12-16-1EP_3x4mm_P0.5mm_EP1.65x2.85mm
10-Lead Plastic Micro Small Outline Package (MS) [MSOP] (see Microchip Packaging Specification 00000049BS.pdf)
SSOP 0.5
0
19
13
Package_SO
MSOP-12-16-1EP_3x4mm_P0.5mm_EP1.65x2.85mm_ThermalVias
10-Lead Plastic Micro Small Outline Package (MS) [MSOP] (see Microchip Packaging Specification 00000049BS.pdf)
SSOP 0.5
0
25
13
Package_SO
MSOP-12-16_3x4mm_P0.5mm
10-Lead Plastic Micro Small Outline Package (MS) [MSOP] (see Microchip Packaging Specification 00000049BS.pdf)
SSOP 0.5
0
12
12
Package_SO
MSOP-12_3x4mm_P0.65mm
MSOP, 12 Pin (https://www.analog.com/media/en/technical-documentation/data-sheets/6957fb.pdf#page=36), generated with kicad-footprint-generator ipc_gullwing_generator.py
MSOP SO
0
12
12
Package_SO
MSOP-16-1EP_3x4.039mm_P0.5mm_EP1.651x2.845mm
MSOP, 16 Pin (https://www.analog.com/media/en/package-pcb-resources/package/pkg_pdf/ltc-legacy-msop/05081667_F_MSE16.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py
MSOP SO
0
21
17
Package_SO
MSOP-16-1EP_3x4.039mm_P0.5mm_EP1.651x2.845mm_ThermalVias
MSOP, 16 Pin (https://www.analog.com/media/en/package-pcb-resources/package/pkg_pdf/ltc-legacy-msop/05081667_F_MSE16.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py
MSOP SO
0
28
17
Package_SO
MSOP-16-1EP_3x4mm_P0.5mm_EP1.65x2.85mm
MSOP, 16 Pin (http://cds.linear.com/docs/en/datasheet/37551fd.pdf#page=23), generated with kicad-footprint-generator ipc_gullwing_generator.py
MSOP SO
0
21
17
Package_SO
MSOP-16-1EP_3x4mm_P0.5mm_EP1.65x2.85mm_ThermalVias
MSOP, 16 Pin (http://cds.linear.com/docs/en/datasheet/37551fd.pdf#page=23), generated with kicad-footprint-generator ipc_gullwing_generator.py
MSOP SO
0
28
17
Package_SO
MSOP-16_3x4.039mm_P0.5mm
MSOP, 16 Pin (http://www.analog.com/media/en/package-pcb-resources/package/pkg_pdf/ltc-legacy-msop/05081669_A_MS16.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py
MSOP SO
0
16
16
Package_SO
MSOP-16_3x4mm_P0.5mm
MSOP, 16 Pin (https://www.analog.com/media/en/technical-documentation/data-sheets/436412f.pdf#page=22), generated with kicad-footprint-generator ipc_gullwing_generator.py
MSOP SO
0
16
16
Package_SO
OnSemi_Micro8
ON Semiconductor Micro8 (Case846A-02): https://www.onsemi.com/pub/Collateral/846A-02.PDF
micro8
0
8
8
Package_SO
PSOP-44_16.9x27.17mm_P1.27mm
PSOP44: plastic thin shrink small outline package; 44 leads; body width 16.90 mm
PSOP 1.27
0
44
44
Package_SO
PowerIntegrations_SO-8
Power-Integrations variant of 8-Lead Plastic Small Outline (SN) - Narrow, 3.90 mm Body [SOIC], see https://ac-dc.power.com/sites/default/files/product-docs/senzero_family_datasheet.pdf
SOIC 1.27
0
8
8
Package_SO
PowerIntegrations_SO-8B
Power-Integrations variant of 8-Lead Plastic Small Outline (SN) - Narrow, 3.90 mm Body [SOIC], see https://www.mouser.com/ds/2/328/linkswitch-pl_family_datasheet-12517.pdf
SOIC 1.27
0
7
7
Package_SO
PowerIntegrations_SO-8C
Power-Integrations variant of 8-Lead Plastic Small Outline (SN) - Narrow, 3.90 mm Body [SOIC], see https://www.mouser.com/ds/2/328/linkswitch-pl_family_datasheet-12517.pdf
SOIC 1.27
0
7
7
Package_SO
PowerIntegrations_eSOP-12B
eSOP-12B SMT Flat Package with Heatsink Tab, see https://ac-dc.power.com/sites/default/files/product-docs/topswitch-jx_family_datasheet.pdf
Power Integrations K Package
0
12
12
Package_SO
PowerPAK_SO-8_Dual
PowerPAK SO-8 Dual (https://www.vishay.com/docs/71655/powerpak.pdf, https://www.vishay.com/docs/72600/72600.pdf)
PowerPAK SO-8 Dual
0
10
6
Package_SO
PowerPAK_SO-8_Single
PowerPAK SO-8 Single (https://www.vishay.com/docs/71655/powerpak.pdf, https://www.vishay.com/docs/72599/72599.pdf)
PowerPAK SO-8 Single
0
9
5
Package_SO
QSOP-16_3.9x4.9mm_P0.635mm
16-Lead Plastic Shrink Small Outline Narrow Body (QR)-.150" Body [QSOP] (see Microchip Packaging Specification 00000049BS.pdf)
SSOP 0.635
0
16
16
Package_SO
QSOP-20_3.9x8.7mm_P0.635mm
20-Lead Plastic Shrink Small Outline Narrow Body (http://www.analog.com/media/en/technical-documentation/data-sheets/ADuM7640_7641_7642_7643.pdf)
QSOP 0.635
0
20
20
Package_SO
QSOP-24_3.9x8.7mm_P0.635mm
24-Lead Plastic Shrink Small Outline Narrow Body (QR)-.150" Body [QSOP] (see Microchip Packaging Specification 00000049CH.pdf)
QSOP 0.635
0
24
24
Package_SO
SC-74-6_1.5x2.9mm_P0.95mm
SC-74, 6 Pin (https://www.nxp.com/docs/en/package-information/SOT457.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py
SC-74 SO
0
6
6
Package_SO
SO-4_4.4x2.3mm_P1.27mm
4-Lead Plastic Small Outline (SO), see http://datasheet.octopart.com/OPIA403BTRE-Optek-datasheet-5328560.pdf
SO SOIC 1.27
0
4
4
Package_SO
SO-4_4.4x3.6mm_P2.54mm
4-Lead Plastic Small Outline (SO), see https://www.elpro.org/de/index.php?controller=attachment&id_attachment=339
SO SOIC 2.54
0
4
4
Package_SO
SO-4_4.4x3.9mm_P2.54mm
SO, 4 Pin (https://toshiba.semicon-storage.com/info/docget.jsp?did=10047&prodName=TLP3123), generated with kicad-footprint-generator ipc_gullwing_generator.py
SO SO
0
4
4
Package_SO
SO-4_4.4x4.3mm_P2.54mm
4-Lead Plastic Small Outline (SO), see https://docs.broadcom.com/docs/AV02-0173EN
SO SOIC 2.54
0
4
4
Package_SO
SO-4_7.6x3.6mm_P2.54mm
4-Lead Plastic Small Outline (SO) (http://www.everlight.com/file/ProductFile/201407061745083848.pdf)
SO SOIC 2.54
0
4
4
Package_SO
SO-5_4.4x3.6mm_P1.27mm
5-Lead Plastic Small Outline (SO), see https://docs.broadcom.com/cs/Satellite?blobcol=urldata&blobheader=application%2Fpdf&blobheadername1=Content-Disposition&blobheadername2=Content-Type&blobheadername3=MDT-Type&blobheadervalue1=attachment%3Bfilename%3DIPD-Selection-Guide_AV00-0254EN_030617.pdf&blobheadervalue2=application%2Fx-download&blobheadervalue3=abinary%253B%2Bcharset%253DUTF-8&blobkey=id&blobnocache=true&blobtable=MungoBlobs&blobwhere=1430884105675&ssbinary=true
SO SOIC 1.27
0
5
5
Package_SO
SO-6L_10x3.84mm_P1.27mm
6-pin plasic small outline 7,5mm long https://toshiba.semicon-storage.com/info/docget.jsp?did=53548&prodName=TLP2770
SO-6L
0
6
6
Package_SO
SO-6_4.4x3.6mm_P1.27mm
6-Lead Plastic Small Outline (SO), see https://docs.broadcom.com/cs/Satellite?blobcol=urldata&blobheader=application%2Fpdf&blobheadername1=Content-Disposition&blobheadername2=Content-Type&blobheadername3=MDT-Type&blobheadervalue1=attachment%3Bfilename%3DIPD-Selection-Guide_AV00-0254EN_030617.pdf&blobheadervalue2=application%2Fx-download&blobheadervalue3=abinary%253B%2Bcharset%253DUTF-8&blobkey=id&blobnocache=true&blobtable=MungoBlobs&blobwhere=1430884105675&ssbinary=true
SO SOIC 1.27
0
6
6
Package_SO
SO-8_3.9x4.9mm_P1.27mm
SO, 8 Pin (https://www.nxp.com/docs/en/data-sheet/PCF8523.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py
SO SO
0
8
8
Package_SO
SO-8_5.3x6.2mm_P1.27mm
8-Lead Plastic Small Outline, 5.3x6.2mm Body (http://www.ti.com.cn/cn/lit/ds/symlink/tl7705a.pdf)
SOIC 1.27
0
8
8
Package_SO
SO-20-1EP_7.52x12.825mm_P1.27mm_EP6.045x12.09mm_Mask3.56x4.47mm
SO, 20 Pin (http://www.ti.com/lit/ds/symlink/opa569.pdf, http://www.ti.com/lit/an/slma004b/slma004b.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py
SO SO
0
23
21
Package_SO
SO-20-1EP_7.52x12.825mm_P1.27mm_EP6.045x12.09mm_Mask3.56x4.47mm_ThermalVias
SO, 20 Pin (http://www.ti.com/lit/ds/symlink/opa569.pdf, http://www.ti.com/lit/an/slma004b/slma004b.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py
SO SO
0
51
21
Package_SO
SO-20_12.8x7.5mm_P1.27mm
SO-20, 12.8x7.5mm, https://www.nxp.com/docs/en/data-sheet/SA605.pdf
S0-20 
0
20
20
Package_SO
SOIC-4_4.55x2.6mm_P1.27mm
SOIC, 4 Pin (https://toshiba.semicon-storage.com/info/docget.jsp?did=12884&prodName=TLP291), generated with kicad-footprint-generator ipc_gullwing_generator.py
SOIC SO
0
4
4
Package_SO
SOIC-4_4.55x3.7mm_P2.54mm
SOIC, 6 Pin (https://toshiba.semicon-storage.com/info/docget.jsp?did=11791&prodName=TLP185), generated with kicad-footprint-generator ipc_gullwing_generator.py
SOIC SO
0
4
4
Package_SO
SOIC-8-1EP_3.9x4.9mm_P1.27mm_EP2.29x3mm
SOIC, 8 Pin (https://www.analog.com/media/en/technical-documentation/data-sheets/ada4898-1_4898-2.pdf#page=29), generated with kicad-footprint-generator ipc_gullwing_generator.py
SOIC SO
0
13
9
Package_SO
SOIC-8-1EP_3.9x4.9mm_P1.27mm_EP2.29x3mm_ThermalVias
SOIC, 8 Pin (https://www.analog.com/media/en/technical-documentation/data-sheets/ada4898-1_4898-2.pdf#page=29), generated with kicad-footprint-generator ipc_gullwing_generator.py
SOIC SO
0
20
9
Package_SO
SOIC-8-1EP_3.9x4.9mm_P1.27mm_EP2.41x3.3mm
SOIC, 8 Pin (http://www.allegromicro.com/~/media/Files/Datasheets/A4950-Datasheet.ashx#page=8), generated with kicad-footprint-generator ipc_gullwing_generator.py
SOIC SO
0
13
9
Package_SO
SOIC-8-1EP_3.9x4.9mm_P1.27mm_EP2.41x3.3mm_ThermalVias
SOIC, 8 Pin (http://www.allegromicro.com/~/media/Files/Datasheets/A4950-Datasheet.ashx#page=8), generated with kicad-footprint-generator ipc_gullwing_generator.py
SOIC SO
0
20
9
Package_SO
SOIC-8-1EP_3.9x4.9mm_P1.27mm_EP2.41x3.81mm
SOIC, 8 Pin (https://www.analog.com/media/en/technical-documentation/data-sheets/ada4898-1_4898-2.pdf#page=29), generated with kicad-footprint-generator ipc_gullwing_generator.py
SOIC SO
0
13
9
Package_SO
SOIC-8-1EP_3.9x4.9mm_P1.27mm_EP2.41x3.81mm_ThermalVias
SOIC, 8 Pin (https://www.analog.com/media/en/technical-documentation/data-sheets/ada4898-1_4898-2.pdf#page=29), generated with kicad-footprint-generator ipc_gullwing_generator.py
SOIC SO
0
20
9
Package_SO
SOIC-8-1EP_3.9x4.9mm_P1.27mm_EP2.95x4.9mm_Mask2.71x3.4mm
SOIC, 8 Pin (http://www.ti.com/lit/ds/symlink/lm5017.pdf#page=31), generated with kicad-footprint-generator ipc_gullwing_generator.py
SOIC SO
0
14
9
Package_SO
SOIC-8-1EP_3.9x4.9mm_P1.27mm_EP2.95x4.9mm_Mask2.71x3.4mm_ThermalVias
SOIC, 8 Pin (http://www.ti.com/lit/ds/symlink/lm5017.pdf#page=31), generated with kicad-footprint-generator ipc_gullwing_generator.py
SOIC SO
0
23
9
Package_SO
SOIC-8-1EP_3.9x4.9mm_P1.27mm_EP2.514x3.2mm
SOIC, 8 Pin (https://www.renesas.com/eu/en/www/doc/datasheet/hip2100.pdf#page=13), generated with kicad-footprint-generator ipc_gullwing_generator.py
SOIC SO
0
13
9
Package_SO
SOIC-8-1EP_3.9x4.9mm_P1.27mm_EP2.514x3.2mm_ThermalVias
SOIC, 8 Pin (https://www.renesas.com/eu/en/www/doc/datasheet/hip2100.pdf#page=13), generated with kicad-footprint-generator ipc_gullwing_generator.py
SOIC SO
0
20
9
Package_SO
SOIC-8-N7_3.9x4.9mm_P1.27mm
8-Lead Plastic Small Outline (SN) - Narrow, 3.90 mm Body [SOIC], pin 7 removed (Microchip Packaging Specification 00000049BS.pdf, http://www.onsemi.com/pub/Collateral/NCP1207B.PDF)
SOIC 1.27
0
7
7
Package_SO
SOIC-8_3.9x4.9mm_P1.27mm
SOIC, 8 Pin (JEDEC MS-012AA, https://www.analog.com/media/en/package-pcb-resources/package/pkg_pdf/soic_narrow-r/r_8.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py
SOIC SO
0
8
8
Package_SO
SOIC-8_5.23x5.23mm_P1.27mm
SOIC, 8 Pin (http://www.winbond.com/resource-files/w25q32jv%20revg%2003272018%20plus.pdf#page=68), generated with kicad-footprint-generator ipc_gullwing_generator.py
SOIC SO
0
8
8
Package_SO
SOIC-8_5.275x5.275mm_P1.27mm
SOIC, 8 Pin (http://ww1.microchip.com/downloads/en/DeviceDoc/20005045C.pdf#page=23), generated with kicad-footprint-generator ipc_gullwing_generator.py
SOIC SO
0
8
8
Package_SO
SOIC-8_7.5x5.85mm_P1.27mm
SOIC, 8 Pin (http://www.ti.com/lit/ml/mpds382b/mpds382b.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py
SOIC SO
0
8
8
Package_SO
SOIC-14W_7.5x9mm_P1.27mm
SOIC, 14 Pin (JEDEC MS-013AF, https://www.analog.com/media/en/package-pcb-resources/package/54614177245586rw_14.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py
SOIC SO
0
14
14
Package_SO
SOIC-14_3.9x8.7mm_P1.27mm
SOIC, 14 Pin (JEDEC MS-012AB, https://www.analog.com/media/en/package-pcb-resources/package/pkg_pdf/soic_narrow-r/r_14.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py
SOIC SO
0
14
14
Package_SO
SOIC-16W-12_7.5x10.3mm_P1.27mm
SOIC-16 With 12 Pin Placed - Wide, 7.50 mm Body [SOIC] (https://docs.broadcom.com/docs/AV02-0169EN)
SOIC 1.27 16 12 Wide
0
12
12
Package_SO
SOIC-16W_5.3x10.2mm_P1.27mm
16-Lead Plastic Small Outline (SO) - Wide, 5.3 mm Body (http://www.ti.com/lit/ml/msop002a/msop002a.pdf)
SOIC 1.27
0
16
16
Package_SO
SOIC-16W_7.5x10.3mm_P1.27mm
SOIC, 16 Pin (JEDEC MS-013AA, https://www.analog.com/media/en/package-pcb-resources/package/pkg_pdf/soic_wide-rw/rw_16.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py
SOIC SO
0
16
16
Package_SO
SOIC-16W_7.5x12.8mm_P1.27mm
SOIC, 16 Pin (https://www.analog.com/media/en/package-pcb-resources/package/pkg_pdf/ri_soic_ic/ri_16_1.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py
SOIC SO
0
16
16
Package_SO
SOIC-16_3.9x9.9mm_P1.27mm
SOIC, 16 Pin (JEDEC MS-012AC, https://www.analog.com/media/en/package-pcb-resources/package/pkg_pdf/soic_narrow-r/r_16.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py
SOIC SO
0
16
16
Package_SO
SOIC-16_4.55x10.3mm_P1.27mm
SOIC, 16 Pin (https://toshiba.semicon-storage.com/info/docget.jsp?did=12858&prodName=TLP291-4), generated with kicad-footprint-generator ipc_gullwing_generator.py
SOIC SO
0
16
16
Package_SO
SOIC-18W_7.5x11.6mm_P1.27mm
SOIC, 18 Pin (JEDEC MS-013AB, https://www.analog.com/media/en/package-pcb-resources/package/33254132129439rw_18.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py
SOIC SO
0
18
18
Package_SO
SOIC-20W_7.5x12.8mm_P1.27mm
SOIC, 20 Pin (JEDEC MS-013AC, https://www.analog.com/media/en/package-pcb-resources/package/233848rw_20.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py
SOIC SO
0
20
20
Package_SO
SOIC-24W_7.5x15.4mm_P1.27mm
SOIC, 24 Pin (JEDEC MS-013AD, https://www.analog.com/media/en/package-pcb-resources/package/pkg_pdf/soic_wide-rw/RW_24.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py
SOIC SO
0
24
24
Package_SO
SOIC-28W_7.5x17.9mm_P1.27mm
SOIC, 28 Pin (JEDEC MS-013AE, https://www.analog.com/media/en/package-pcb-resources/package/35833120341221rw_28.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py
SOIC SO
0
28
28
Package_SO
SOIC-28W_7.5x18.7mm_P1.27mm
SOIC, 28 Pin (https://www.akm.com/akm/en/file/datasheet/AK5394AVS.pdf#page=23), generated with kicad-footprint-generator ipc_gullwing_generator.py
SOIC SO
0
28
28
Package_SO
SOIJ-8_5.3x5.3mm_P1.27mm
8-Lead Plastic Small Outline (SM) - Medium, 5.28 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)
SOIC 1.27
0
8
8
Package_SO
SOJ-36_10.16x23.49mm_P1.27mm
SOJ, 36 Pin (http://www.issi.com/WW/pdf/61-64C5128AL.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py
SOJ SO
0
36
36
Package_SO
SOP-4_3.8x4.1mm_P2.54mm
SOP, 4 Pin (http://www.ixysic.com/home/pdfs.nsf/www/CPC1017N.pdf/$file/CPC1017N.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py
SOP SO
0
4
4
Package_SO
SOP-4_4.4x2.6mm_P1.27mm
SOP, 4 Pin (http://www.vishay.com/docs/83510/tcmt1100.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py
SOP SO
0
4
4
Package_SO
SOP-8-1EP_4.57x4.57mm_P1.27mm_EP4.57x4.45mm
SOP, 8 Pin (https://ww2.minicircuits.com/case_style/XX112.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py
SOP SO
0
13
9
Package_SO
SOP-8-1EP_4.57x4.57mm_P1.27mm_EP4.57x4.45mm_ThermalVias
SOP, 8 Pin (https://ww2.minicircuits.com/case_style/XX112.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py
SOP SO
0
20
9
Package_SO
SOP-8_3.9x4.9mm_P1.27mm
SOP, 8 Pin (http://www.macronix.com/Lists/Datasheet/Attachments/7534/MX25R3235F,%20Wide%20Range,%2032Mb,%20v1.6.pdf#page=79), generated with kicad-footprint-generator ipc_gullwing_generator.py
SOP SO
0
8
8
Package_SO
SOP-8_3.76x4.96mm_P1.27mm
SOP, 8 Pin (https://ww2.minicircuits.com/case_style/XX211.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py
SOP SO
0
8
8
Package_SO
SOP-8_5.28x5.23mm_P1.27mm
SOP, 8 Pin (http://www.macronix.com/Lists/Datasheet/Attachments/7534/MX25R3235F,%20Wide%20Range,%2032Mb,%20v1.6.pdf#page=80), generated with kicad-footprint-generator ipc_gullwing_generator.py
SOP SO
0
8
8
Package_SO
SOP-8_6.62x9.15mm_P2.54mm
SOP, 8 Pin (http://www.ti.com/lit/ds/symlink/iso1050.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py
SOP SO
0
8
8
Package_SO
SOP-16_4.4x10.4mm_P1.27mm
16-Lead Plastic Small Outline http://www.vishay.com/docs/49633/sg2098.pdf
SOP 1.27
0
16
16
Package_SO
SOP-16_4.55x10.3mm_P1.27mm
SOP, 16 Pin (https://toshiba.semicon-storage.com/info/docget.jsp?did=12855&prodName=TLP290-4), generated with kicad-footprint-generator ipc_gullwing_generator.py
SOP SO
0
16
16
Package_SO
SOP-18_7x12.5mm_P1.27mm
SOP, 18 Pin (https://toshiba.semicon-storage.com/info/docget.jsp?did=30523), generated with kicad-footprint-generator ipc_gullwing_generator.py
SOP SO
0
18
18
Package_SO
SOP-24_7.5x15.4mm_P1.27mm
SOP, 24 Pin (http://www.issi.com/WW/pdf/31FL3218.pdf#page=14), generated with kicad-footprint-generator ipc_gullwing_generator.py
SOP SO
0
24
24
Package_SO
SSO-4_6.7x5.1mm_P2.54mm_Clearance8mm
4-Lead Plastic Stretched Small Outline (SSO/Stretched SO), see https://www.vishay.com/docs/84299/vor1142b4.pdf
SSO Stretched SO SOIC 2.54
0
4
4
Package_SO
SSO-6_6.8x4.6mm_P1.27mm_Clearance7mm
8-Lead Plastic Stretched Small Outline (SSO/Stretched SO), see https://docs.broadcom.com/cs/Satellite?blobcol=urldata&blobheader=application%2Fpdf&blobheadername1=Content-Disposition&blobheadername2=Content-Type&blobheadername3=MDT-Type&blobheadervalue1=attachment%3Bfilename%3DIPD-Selection-Guide_AV00-0254EN_030617.pdf&blobheadervalue2=application%2Fx-download&blobheadervalue3=abinary%253B%2Bcharset%253DUTF-8&blobkey=id&blobnocache=true&blobtable=MungoBlobs&blobwhere=1430884105675&ssbinary=true
SSO Stretched SO SOIC 1.27
0
6
6
Package_SO
SSO-6_6.8x4.6mm_P1.27mm_Clearance8mm
8-Lead Plastic Stretched Small Outline (SSO/Stretched SO), see https://docs.broadcom.com/cs/Satellite?blobcol=urldata&blobheader=application%2Fpdf&blobheadername1=Content-Disposition&blobheadername2=Content-Type&blobheadername3=MDT-Type&blobheadervalue1=attachment%3Bfilename%3DIPD-Selection-Guide_AV00-0254EN_030617.pdf&blobheadervalue2=application%2Fx-download&blobheadervalue3=abinary%253B%2Bcharset%253DUTF-8&blobkey=id&blobnocache=true&blobtable=MungoBlobs&blobwhere=1430884105675&ssbinary=true
SSO Stretched SO SOIC 1.27
0
6
6
Package_SO
SSO-8_6.7x9.8mm_P2.54mm_Clearance8mm
8-Lead Plastic Stretched Small Outline (SSO/Stretched SO), see https://www.vishay.com/docs/83831/lh1533ab.pdf
SSO Stretched SO SOIC Pitch 2.54
0
8
8
Package_SO
SSO-8_6.8x5.9mm_P1.27mm_Clearance7mm
8-Lead Plastic Stretched Small Outline (SSO/Stretched SO), see https://docs.broadcom.com/cs/Satellite?blobcol=urldata&blobheader=application%2Fpdf&blobheadername1=Content-Disposition&blobheadername2=Content-Type&blobheadername3=MDT-Type&blobheadervalue1=attachment%3Bfilename%3DIPD-Selection-Guide_AV00-0254EN_030617.pdf&blobheadervalue2=application%2Fx-download&blobheadervalue3=abinary%253B%2Bcharset%253DUTF-8&blobkey=id&blobnocache=true&blobtable=MungoBlobs&blobwhere=1430884105675&ssbinary=true
SSO Stretched SO SOIC Pitch 1.27
0
8
8
Package_SO
SSO-8_6.8x5.9mm_P1.27mm_Clearance8mm
8-Lead Plastic Stretched Small Outline (SSO/Stretched SO), see https://docs.broadcom.com/cs/Satellite?blobcol=urldata&blobheader=application%2Fpdf&blobheadername1=Content-Disposition&blobheadername2=Content-Type&blobheadername3=MDT-Type&blobheadervalue1=attachment%3Bfilename%3DIPD-Selection-Guide_AV00-0254EN_030617.pdf&blobheadervalue2=application%2Fx-download&blobheadervalue3=abinary%253B%2Bcharset%253DUTF-8&blobkey=id&blobnocache=true&blobtable=MungoBlobs&blobwhere=1430884105675&ssbinary=true
SSO Stretched SO SOIC Pitch 1.27
0
8
8
Package_SO
SSO-8_9.6x6.3mm_P1.27mm_Clearance10.5mm
8-Lead Plastic Stretched Small Outline (SSO/Stretched SO), see https://docs.broadcom.com/cs/Satellite?blobcol=urldata&blobheader=application%2Fpdf&blobheadername1=Content-Disposition&blobheadername2=Content-Type&blobheadername3=MDT-Type&blobheadervalue1=attachment%3Bfilename%3DIPD-Selection-Guide_AV00-0254EN_030617.pdf&blobheadervalue2=application%2Fx-download&blobheadervalue3=abinary%253B%2Bcharset%253DUTF-8&blobkey=id&blobnocache=true&blobtable=MungoBlobs&blobwhere=1430884105675&ssbinary=true
SSO Stretched SO SOIC Pitch 1.27
0
8
8
Package_SO
SSO-8_13.6x6.3mm_P1.27mm_Clearance14.2mm
8-Lead Plastic Stretched Small Outline (SSO/Stretched SO), see https://docs.broadcom.com/cs/Satellite?blobcol=urldata&blobheader=application%2Fpdf&blobheadername1=Content-Disposition&blobheadername2=Content-Type&blobheadername3=MDT-Type&blobheadervalue1=attachment%3Bfilename%3DIPD-Selection-Guide_AV00-0254EN_030617.pdf&blobheadervalue2=application%2Fx-download&blobheadervalue3=abinary%253B%2Bcharset%253DUTF-8&blobkey=id&blobnocache=true&blobtable=MungoBlobs&blobwhere=1430884105675&ssbinary=true
SSO Stretched SO SOIC Pitch 1.27
0
8
8
Package_SO
SSOP-8_2.95x2.8mm_P0.65mm
SSOP-8 2.9 x2.8mm Pitch 0.65mm
SSOP-8 2.95x2.8mm Pitch 0.65mm
0
8
8
Package_SO
SSOP-8_3.9x5.05mm_P1.27mm
SSOP, 8 Pin (http://www.fujitsu.com/downloads/MICRO/fsa/pdf/products/memory/fram/MB85RS16-DS501-00014-6v0-E.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py
SSOP SO
0
8
8
Package_SO
SSOP-8_3.95x5.21x3.27mm_P1.27mm
SSOP-8 3.95x5.21x3.27mm Pitch 1.27mm
SSOP-8 3.95x5.21x3.27mm 1.27mm
0
8
8
Package_SO
SSOP-8_5.25x5.24mm_P1.27mm
SSOP, 8 Pin (http://www.fujitsu.com/ca/en/Images/MB85RS2MT-DS501-00023-1v0-E.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py
SSOP SO
0
8
8
Package_SO
SSOP-10_3.9x4.9mm_P1.00mm
10-Lead SSOP, 3.9 x 4.9mm body, 1.00mm pitch (http://www.st.com/resource/en/datasheet/viper01.pdf)
SSOP 3.9 4.9 1.00
0
10
10
Package_SO
SSOP-14_5.3x6.2mm_P0.65mm
SSOP14: plastic shrink small outline package; 14 leads; body width 5.3 mm; (see NXP SSOP-TSSOP-VSO-REFLOW.pdf and sot337-1_po.pdf)
SSOP 0.65
0
14
14
Package_SO
SSOP-16_3.9x4.9mm_P0.635mm
SSOP16: plastic shrink small outline package; 16 leads; body width 3.9 mm; lead pitch 0.635; (see NXP SSOP-TSSOP-VSO-REFLOW.pdf and sot519-1_po.pdf)
SSOP 0.635
0
16
16
Package_SO
SSOP-16_4.4x5.2mm_P0.65mm
SSOP16: plastic shrink small outline package; 16 leads; body width 4.4 mm; (see NXP SSOP-TSSOP-VSO-REFLOW.pdf and sot369-1_po.pdf)
SSOP 0.65
0
16
16
Package_SO
SSOP-16_5.3x6.2mm_P0.65mm
SSOP16: plastic shrink small outline package; 16 leads; body width 5.3 mm; (see NXP SSOP-TSSOP-VSO-REFLOW.pdf and sot338-1_po.pdf)
SSOP 0.65
0
16
16
Package_SO
SSOP-18_4.4x6.5mm_P0.65mm
SSOP18: plastic shrink small outline package; 18 leads; body width 4.4 mm (http://toshiba.semicon-storage.com/info/docget.jsp?did=30523&prodName=TBD62783APG)
SSOP 0.65
0
18
18
Package_SO
SSOP-20_3.9x8.7mm_P0.635mm
SSOP20: plastic shrink small outline package; 24 leads; body width 3.9 mm; lead pitch 0.635; (see http://www.ftdichip.com/Support/Documents/DataSheets/ICs/DS_FT231X.pdf)
SSOP 0.635
0
20
20
Package_SO
SSOP-20_4.4x6.5mm_P0.65mm
SSOP20: plastic shrink small outline package; 20 leads; body width 4.4 mm; (see NXP SSOP-TSSOP-VSO-REFLOW.pdf and sot266-1_po.pdf)
SSOP 0.65
0
20
20
Package_SO
SSOP-20_5.3x7.2mm_P0.65mm
SSOP, 20 Pin (http://ww1.microchip.com/downloads/en/DeviceDoc/40001800C.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py
SSOP SO
0
20
20
Package_SO
SSOP-24_3.9x8.7mm_P0.635mm
SSOP24: plastic shrink small outline package; 24 leads; body width 3.9 mm; lead pitch 0.635; (see NXP SSOP-TSSOP-VSO-REFLOW.pdf and sot556-1_po.pdf)
SSOP 0.635
0
24
24
Package_SO
SSOP-24_5.3x8.2mm_P0.65mm
24-Lead Plastic Shrink Small Outline (SS)-5.30 mm Body [SSOP] (see Microchip Packaging Specification 00000049BS.pdf)
SSOP 0.65
0
24
24
Package_SO
SSOP-28_3.9x9.9mm_P0.635mm
SSOP28: plastic shrink small outline package; 28 leads; body width 3.9 mm; lead pitch 0.635; (see http://cds.linear.com/docs/en/datasheet/38901fb.pdf)
SSOP 0.635
0
28
28
Package_SO
SSOP-28_5.3x10.2mm_P0.65mm
28-Lead Plastic Shrink Small Outline (SS)-5.30 mm Body [SSOP] (see Microchip Packaging Specification 00000049BS.pdf)
SSOP 0.65
0
28
28
Package_SO
SSOP-32_11.305x20.495mm_P1.27mm
SSOP, 32 Pin (http://www.issi.com/WW/pdf/61-64C5128AL.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py
SSOP SO
0
32
32
Package_SO
SSOP-44_5.3x12.8mm_P0.5mm
44-Lead Plastic Shrink Small Outline (SS)-5.30 mm Body [SSOP] (http://cds.linear.com/docs/en/datasheet/680313fa.pdf)
SSOP 0.5
0
44
44
Package_SO
SSOP-48_7.5x15.9mm_P0.635mm
SSOP48: plastic shrink small outline package; 48 leads; body width 7.5 mm; (see NXP SSOP-TSSOP-VSO-REFLOW.pdf and sot370-1_po.pdf)
SSOP 0.635
0
48
48
Package_SO
SSOP-56_7.5x18.5mm_P0.635mm
SSOP56: plastic shrink small outline package; 56 leads; body width 7.5 mm; (see NXP SSOP-TSSOP-VSO-REFLOW.pdf and sot371-1_po.pdf)
SSOP 0.635
0
56
56
Package_SO
STC_SOP-16_3.9x9.9mm_P1.27mm
STC  SOP, 16 Pin (https://www.stcmicro.com/datasheet/STC15F2K60S2-en.pdf#page=156), generated with kicad-footprint-generator ipc_gullwing_generator.py
STC SOP SO
0
16
16
Package_SO
ST_MultiPowerSO-30
MultiPowerSO-30 3EP 16.0x17.2mm Pitch 1mm (http://www.st.com/resource/en/datasheet/vnh2sp30-e.pdf)
MultiPowerSO-30 3EP 16.0x17.2mm Pitch 1mm
0
33
33
Package_SO
ST_PowerSSO-24_SlugDown
ST PowerSSO-24 1EP 7.5x10.3mm Pitch 0.8mm [JEDEC MO-271] (http://www.st.com/resource/en/datasheet/tda7266p.pdf, http://freedatasheets.com/downloads/Technical%20Note%20Powersso24%20TN0054.pdf)
ST PowerSSO-24 1EP 7.5x10.3mm Pitch 0.8mm
0
25
25
Package_SO
ST_PowerSSO-24_SlugDown_ThermalVias
ST PowerSSO-24 1EP 7.5x10.3mm Pitch 0.8mm [JEDEC MO-271] (http://www.st.com/resource/en/datasheet/tda7266p.pdf, http://freedatasheets.com/downloads/Technical%20Note%20Powersso24%20TN0054.pdf)
ST PowerSSO-24 1EP 7.5x10.3mm Pitch 0.8mm
0
38
25
Package_SO
ST_PowerSSO-24_SlugUp
ST PowerSSO-24 1EP 7.5x10.3mm Pitch 0.8mm [JEDEC MO-271] (http://www.st.com/resource/en/datasheet/tda7266p.pdf, http://freedatasheets.com/downloads/Technical%20Note%20Powersso24%20TN0054.pdf)
ST PowerSSO-24 1EP 7.5x10.3mm Pitch 0.8mm
0
24
24
Package_SO
ST_PowerSSO-36_SlugDown
ST PowerSSO-36 1EP 7.5x10.3mm Pitch 0.8mm [JEDEC MO-271] (http://www.st.com/resource/en/datasheet/tda7492p.pdf, http://freedatasheets.com/downloads/Technical%20Note%20Powersso24%20TN0054.pdf)
ST PowerSSO-36 1EP 7.5x10.3mm Pitch 0.8mm
0
37
37
Package_SO
ST_PowerSSO-36_SlugDown_ThermalVias
ST PowerSSO-36 1EP 7.5x10.3mm Pitch 0.8mm [JEDEC MO-271] (http://www.st.com/resource/en/datasheet/tda7492p.pdf, http://freedatasheets.com/downloads/Technical%20Note%20Powersso24%20TN0054.pdf)
ST PowerSSO-36 1EP 7.5x10.3mm Pitch 0.8mm
0
50
37
Package_SO
ST_PowerSSO-36_SlugUp
ST PowerSSO-36 1EP 7.5x10.3mm Pitch 0.8mm [JEDEC MO-271] (http://www.st.com/resource/en/datasheet/tda7492p.pdf, http://freedatasheets.com/downloads/Technical%20Note%20Powersso24%20TN0054.pdf)
ST PowerSSO-36 1EP 7.5x10.3mm Pitch 0.8mm
0
36
36
Package_SO
TI_SO-PowerPAD-8
8-Lead Plastic PSOP, Exposed Die Pad (TI DDA0008B, see http://www.ti.com/lit/ds/symlink/lm3404.pdf)
SSOP 0.50 exposed pad
0
12
9
Package_SO
TI_SO-PowerPAD-8_ThermalVias
8-pin HTSOP package with 1.27mm pin pitch, compatible with SOIC-8, 3.9x4.9mm² body, exposed pad, thermal vias with large copper area, as proposed in http://www.ti.com/lit/ds/symlink/tps5430.pdf
HTSOP 1.27
0
19
9
Package_SO
TSOP-5_1.65x3.05mm_P0.95mm
TSOP-5 package (comparable to TSOT-23), https://www.vishay.com/docs/71200/71200.pdf
Jedec MO-193C TSOP-5L
0
5
5
Package_SO
TSOP-6_1.65x3.05mm_P0.95mm
TSOP-6 package (comparable to TSOT-23), https://www.vishay.com/docs/71200/71200.pdf
Jedec MO-193C TSOP-6L
0
6
6
Package_SO
TSOP-I-28_11.8x8mm_P0.55mm
TSOP I, 28 pins, 18.8x8mm body, 0.55mm pitch, IPC-calculated pads (http://ww1.microchip.com/downloads/en/devicedoc/doc0807.pdf)
TSOP I 28 pins
0
28
28
Package_SO
TSOP-I-32_11.8x8mm_P0.5mm
TSOP-I, 32 Pin (http://www.issi.com/WW/pdf/61-64C5128AL.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py
TSOP-I SO
0
32
32
Package_SO
TSOP-I-32_18.4x8mm_P0.5mm
TSOP I, 32 pins, 18.4x8mm body (https://www.micron.com/~/media/documents/products/technical-note/nor-flash/tn1225_land_pad_design.pdf, http://www.fujitsu.com/downloads/MICRO/fma/pdfmcu/f32pm25.pdf)
TSOP I 32
0
32
32
Package_SO
TSOP-I-32_18.4x8mm_P0.5mm_Reverse
TSOP I, 32 pins, 18.4x8mm body (http://www.futurlec.com/Datasheet/Memory/628128.pdf), reverse mount
TSOP I 32 reverse
0
32
32
Package_SO
TSOP-I-48_18.4x12mm_P0.5mm
TSOP I, 32 pins, 18.4x8mm body (https://www.micron.com/~/media/documents/products/technical-note/nor-flash/tn1225_land_pad_design.pdf)
TSOP I 32
0
48
48
Package_SO
TSOP-I-56_18.4x14mm_P0.5mm
TSOP I, 32 pins, 18.4x8mm body (https://www.micron.com/~/media/documents/products/technical-note/nor-flash/tn1225_land_pad_design.pdf)
TSOP I 32
0
56
56
Package_SO
TSOP-II-32_21.0x10.2mm_P1.27mm
32-lead plastic TSOP; Type II
TSOP-II 32
0
32
32
Package_SO
TSOP-II-44_10.16x18.41mm_P0.8mm
TSOP-II, 44 Pin (http://www.issi.com/WW/pdf/61-64C5128AL.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py
TSOP-II SO
0
44
44
Package_SO
TSOP-II-54_22.2x10.16mm_P0.8mm
54-lead TSOP typ II package
TSOPII TSOP2
0
54
54
Package_SO
TSSOP-8_3x3mm_P0.65mm
TSSOP8: plastic thin shrink small outline package; 8 leads; body width 3 mm; (see NXP SSOP-TSSOP-VSO-REFLOW.pdf and sot505-1_po.pdf)
SSOP 0.65
0
8
8
Package_SO
TSSOP-8_4.4x3mm_P0.65mm
8-Lead Plastic Thin Shrink Small Outline (ST)-4.4 mm Body [TSSOP] (see Microchip Packaging Specification 00000049BS.pdf)
SSOP 0.65
0
8
8
Package_SO
TSSOP-10_3x3mm_P0.5mm
TSSOP10: plastic thin shrink small outline package; 10 leads; body width 3 mm; (see NXP SSOP-TSSOP-VSO-REFLOW.pdf and sot552-1_po.pdf)
SSOP 0.5
0
10
10
Package_SO
TSSOP-14-1EP_4.4x5mm_P0.65mm
14-Lead Plastic Thin Shrink Small Outline (ST)-4.4 mm Body [TSSOP] with exposed pad (http://cds.linear.com/docs/en/datasheet/34301fa.pdf)
SSOP 0.65 exposed pad
0
18
15
Package_SO
TSSOP-14_4.4x5mm_P0.65mm
14-Lead Plastic Thin Shrink Small Outline (ST)-4.4 mm Body [TSSOP] (see Microchip Packaging Specification 00000049BS.pdf)
SSOP 0.65
0
14
14
Package_SO
TSSOP-16-1EP_4.4x5mm_P0.65mm
FE Package; 16-Lead Plastic TSSOP (4.4mm); Exposed Pad Variation BB; (see Linear Technology 1956f.pdf)
SSOP 0.65
0
24
17
Package_SO
TSSOP-16_4.4x5mm_P0.65mm
16-Lead Plastic Thin Shrink Small Outline (ST)-4.4 mm Body [TSSOP] (see Microchip Packaging Specification 00000049BS.pdf)
SSOP 0.65
0
16
16
Package_SO
TSSOP-20_4.4x6.5mm_P0.65mm
20-Lead Plastic Thin Shrink Small Outline (ST)-4.4 mm Body [TSSOP] (see Microchip Packaging Specification 00000049BS.pdf)
SSOP 0.65
0
20
20
Package_SO
TSSOP-24_4.4x7.8mm_P0.65mm
TSSOP24: plastic thin shrink small outline package; 24 leads; body width 4.4 mm; (see NXP SSOP-TSSOP-VSO-REFLOW.pdf and sot355-1_po.pdf)
SSOP 0.65
0
24
24
Package_SO
TSSOP-28-1EP_4.4x9.7mm_P0.65mm
TSSOP28: plastic thin shrink small outline package; 28 leads; body width 4.4 mm; Exposed Pad Variation; (see NXP SSOP-TSSOP-VSO-REFLOW.pdf and sot361-1_po.pdf)
SSOP 0.65
0
36
29
Package_SO
TSSOP-28_4.4x9.7mm_P0.65mm
TSSOP28: plastic thin shrink small outline package; 28 leads; body width 4.4 mm; (see NXP SSOP-TSSOP-VSO-REFLOW.pdf and sot361-1_po.pdf)
SSOP 0.65
0
28
28
Package_SO
TSSOP-30_4.4x7.8mm_P0.5mm
TSSOP30: plastic thin shrink small outline package; 30 leads; body width 4.4 mm (http://www.ti.com/lit/ds/symlink/bq78350.pdf)
SSOP 0.5
0
30
30
Package_SO
TSSOP-32_6.1x11mm_P0.65mm
TSSOP32: plastic thin shrink small outline package; 32 leads; body width 6.1 mm; lead pitch 0.65 mm (see NXP SSOP-TSSOP-VSO-REFLOW.pdf and sot487-1_po.pdf)
SSOP 0.65
0
32
32
Package_SO
TSSOP-38_4.4x9.7mm_P0.5mm
TSSOP38: plastic thin shrink small outline package; 38 leads; body width 4.4 mm (see NXP SSOP-TSSOP-VSO-REFLOW.pdf and sot510-1_po.pdf)
SSOP 0.5
0
38
38
Package_SO
TSSOP-38_6.1x12.5mm_P0.65mm
TSSOP38: plastic thin shrink small outline package; 38 leads; body width 6.1 mm (http://www.ti.com/lit/ds/symlink/msp430g2744.pdf)
SSOP 0.65
0
38
38
Package_SO
TSSOP-44_4.4x11.2mm_P0.5mm
TSSOP44: plastic thin shrink small outline package; 44 leads; body width 4.4 mm (see NXP SSOP-TSSOP-VSO-REFLOW.pdf and sot510-1_po.pdf)
SSOP 0.5
0
44
44
Package_SO
TSSOP-48_6.1x12.5mm_P0.5mm
TSSOP48: plastic thin shrink small outline package; 48 leads; body width 6.1 mm (see NXP SSOP-TSSOP-VSO-REFLOW.pdf and sot362-1_po.pdf)
SSOP 0.5
0
48
48
Package_SO
TSSOP-56_6.1x14mm_P0.5mm
TSSOP56: plastic thin shrink small outline package; 56 leads; body width 6.1 mm (see NXP SSOP-TSSOP-VSO-REFLOW.pdf and sot364-1_po.pdf)
SSOP 0.5
0
56
56
Package_SO
Texas_HSOP-8-1EP_3.9x4.9mm_P1.27mm
Texas Instruments HSOP 9, 1.27mm pitch, 3.9x4.9mm body, exposed pad, DDA0008J (http://www.ti.com/lit/ds/symlink/tps5430.pdf)
HSOP 1.27
0
11
9
Package_SO
Texas_HSOP-8-1EP_3.9x4.9mm_P1.27mm_ThermalVias
Texas Instruments HSOP 9, 1.27mm pitch, 3.9x4.9mm body, exposed pad, thermal vias, DDA0008J (http://www.ti.com/lit/ds/symlink/tps5430.pdf)
HSOP 1.27
0
20
9
Package_SO
Texas_HTSOP-8-1EP_3.9x4.9mm_P1.27mm_EP2.95x4.9mm_Mask2.4x3.1mm_ThermalVias
8-pin HTSOP package with 1.27mm pin pitch, compatible with SOIC-8, 3.9x4.9mm body, exposed pad, thermal vias, http://www.ti.com/lit/ds/symlink/drv8870.pdf
HTSOP 1.27
0
18
9
Package_SO
Texas_PWP0020A
20-Pin Thermally Enhanced Thin Shrink Small-Outline Package, Body 4.4x6.5x1.1mm, Pad 3.0x4.2mm, Texas Instruments (see http://www.ti.com/lit/ds/symlink/lm5118.pdf)
PWP HTSSOP 0.65mm
0
25
21
Package_SO
Texas_R-PDSO-G8_EP2.95x4.9mm_Mask2.4x3.1mm
HSOIC, 8 Pin (http://www.ti.com/lit/ds/symlink/lmr14030.pdf#page=28, http://www.ti.com/lit/ml/msoi002j/msoi002j.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py
HSOIC SO
0
16
9
Package_SO
Texas_R-PDSO-G8_EP2.95x4.9mm_Mask2.4x3.1mm_ThermalVias
HSOIC, 8 Pin (http://www.ti.com/lit/ds/symlink/lmr14030.pdf#page=28, http://www.ti.com/lit/ml/msoi002j/msoi002j.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py
HSOIC SO
0
23
9
Package_SO
Texas_R-PDSO-N5
Plastic Small outline http://www.ti.com/lit/ml/mpds158c/mpds158c.pdf
SOT23 R-PDSO-N5
0
5
5
Package_SO
VSO-40_7.6x15.4mm_P0.762mm
VSO40: plastic very small outline package; 40 leads (see NXP SSOP-TSSOP-VSO-REFLOW.pdf and sot158-1_po.pdf)
SSOP 0.762
0
40
40
Package_SO
VSO-56_11.1x21.5mm_P0.75mm
VSO56: plastic very small outline package; 56 leads (see NXP SSOP-TSSOP-VSO-REFLOW.pdf and sot190-1_po.pdf)
SSOP 0.75
0
56
56
Package_SO
VSSOP-8_2.3x2mm_P0.5mm
VSSOP-8 2.3x2mm Pitch 0.5mm
VSSOP-8 2.3x2mm Pitch 0.5mm
0
8
8
Package_SO
VSSOP-8_2.4x2.1mm_P0.5mm
http://www.ti.com/lit/ml/mpds050d/mpds050d.pdf
VSSOP DCU R-PDSO-G8 Pitch0.5mm
0
8
8
Package_SO
VSSOP-8_3.0x3.0mm_P0.65mm
VSSOP-8 3.0 x 3.0, http://www.ti.com/lit/ds/symlink/lm75b.pdf
VSSOP-8 3.0 x 3.0
0
8
8
Package_SO
VSSOP-10_3x3mm_P0.5mm
VSSOP, 10 Pin (http://www.ti.com/lit/ds/symlink/ads1115.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py
VSSOP SO
0
10
10
Package_SO
Vishay_PowerPAK_1212-8_Dual
PowerPAK 1212-8 Dual (https://www.vishay.com/docs/71656/ppak12128.pdf, https://www.vishay.com/docs/72598/72598.pdf)
Vishay_PowerPAK_1212-8_Dual
0
6
6
Package_SO
Vishay_PowerPAK_1212-8_Single
PowerPAK 1212-8 Single (https://www.vishay.com/docs/71656/ppak12128.pdf, https://www.vishay.com/docs/72597/72597.pdf)
Vishay PowerPAK 1212-8 Single
0
5
5
Package_SO
Zetex_SM8
Zetex,  SMD, 8 pin package (http://datasheet.octopart.com/ZDT6758TA-Zetex-datasheet-68057.pdf)
Zetex SM8
0
8
8
Resistor_SMD
R_0201_0603Metric
Resistor SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), generated with kicad-footprint-generator
resistor
0
4
2
Resistor_SMD
R_0402_1005Metric
Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator
resistor
0
2
2
Resistor_SMD
R_0603_1608Metric
Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator
resistor
0
2
2
Resistor_SMD
R_0603_1608Metric_Pad1.05x0.95mm_HandSolder
Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator
resistor handsolder
0
2
2
Resistor_SMD
R_0612_1632Metric
Resistor SMD 0612 (1632 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://www.vishay.com/docs/20019/rcwe.pdf), generated with kicad-footprint-generator
resistor
0
2
2
Resistor_SMD
R_0612_1632Metric_Pad1.18x3.40mm_HandSolder
Resistor SMD 0612 (1632 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://www.vishay.com/docs/20019/rcwe.pdf), generated with kicad-footprint-generator
resistor handsolder
0
2
2
Resistor_SMD
R_0805_2012Metric
Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator
resistor
0
2
2
Resistor_SMD
R_0805_2012Metric_Pad1.15x1.40mm_HandSolder
Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator
resistor handsolder
0
2
2
Resistor_SMD
R_0815_2038Metric
Resistor SMD 0815 (2038 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.yageo.com/documents/recent/PYu-PRPFPH_521_RoHS_L_0.pdf), generated with kicad-footprint-generator
resistor
0
2
2
Resistor_SMD
R_0815_2038Metric_Pad1.53x4.00mm_HandSolder
Resistor SMD 0815 (2038 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.yageo.com/documents/recent/PYu-PRPFPH_521_RoHS_L_0.pdf), generated with kicad-footprint-generator
resistor handsolder
0
2
2
Resistor_SMD
R_01005_0402Metric
Resistor SMD 01005 (0402 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.vishay.com/docs/20056/crcw01005e3.pdf), generated with kicad-footprint-generator
resistor
0
4
2
Resistor_SMD
R_1020_2550Metric
Resistor SMD 1020 (2550 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://www.vishay.com/docs/20019/rcwe.pdf), generated with kicad-footprint-generator
resistor
0
2
2
Resistor_SMD
R_1020_2550Metric_Pad1.33x5.20mm_HandSolder
Resistor SMD 1020 (2550 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://www.vishay.com/docs/20019/rcwe.pdf), generated with kicad-footprint-generator
resistor handsolder
0
2
2
Resistor_SMD
R_1206_3216Metric
Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator
resistor
0
2
2
Resistor_SMD
R_1206_3216Metric_Pad1.42x1.75mm_HandSolder
Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator
resistor handsolder
0
2
2
Resistor_SMD
R_1210_3225Metric
Resistor SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator
resistor
0
2
2
Resistor_SMD
R_1210_3225Metric_Pad1.42x2.65mm_HandSolder
Resistor SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator
resistor handsolder
0
2
2
Resistor_SMD
R_1218_3246Metric
Resistor SMD 1218 (3246 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://www.vishay.com/docs/20035/dcrcwe3.pdf), generated with kicad-footprint-generator
resistor
0
2
2
Resistor_SMD
R_1218_3246Metric_Pad1.22x4.75mm_HandSolder
Resistor SMD 1218 (3246 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://www.vishay.com/docs/20035/dcrcwe3.pdf), generated with kicad-footprint-generator
resistor handsolder
0
2
2
Resistor_SMD
R_1806_4516Metric
Resistor SMD 1806 (4516 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://www.modelithics.com/models/Vendor/MuRata/BLM41P.pdf), generated with kicad-footprint-generator
resistor
0
2
2
Resistor_SMD
R_1806_4516Metric_Pad1.57x1.80mm_HandSolder
Resistor SMD 1806 (4516 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://www.modelithics.com/models/Vendor/MuRata/BLM41P.pdf), generated with kicad-footprint-generator
resistor handsolder
0
2
2
Resistor_SMD
R_1812_4532Metric
Resistor SMD 1812 (4532 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://www.nikhef.nl/pub/departments/mt/projects/detectorR_D/dtddice/ERJ2G.pdf), generated with kicad-footprint-generator
resistor
0
2
2
Resistor_SMD
R_1812_4532Metric_Pad1.30x3.40mm_HandSolder
Resistor SMD 1812 (4532 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://www.nikhef.nl/pub/departments/mt/projects/detectorR_D/dtddice/ERJ2G.pdf), generated with kicad-footprint-generator
resistor handsolder
0
2
2
Resistor_SMD
R_2010_5025Metric
Resistor SMD 2010 (5025 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator
resistor
0
2
2
Resistor_SMD
R_2010_5025Metric_Pad1.52x2.65mm_HandSolder
Resistor SMD 2010 (5025 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator
resistor handsolder
0
2
2
Resistor_SMD
R_2512_6332Metric
Resistor SMD 2512 (6332 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator
resistor
0
2
2
Resistor_SMD
R_2512_6332Metric_Pad1.52x3.35mm_HandSolder
Resistor SMD 2512 (6332 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator
resistor handsolder
0
2
2
Resistor_SMD
R_2816_7142Metric
Resistor SMD 2816 (7142 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size from: https://www.vishay.com/docs/30100/wsl.pdf), generated with kicad-footprint-generator
resistor
0
2
2
Resistor_SMD
R_2816_7142Metric_Pad3.20x4.45mm_HandSolder
Resistor SMD 2816 (7142 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size from: https://www.vishay.com/docs/30100/wsl.pdf), generated with kicad-footprint-generator
resistor handsolder
0
2
2
Resistor_SMD
R_4020_10251Metric
Resistor SMD 4020 (10251 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://datasheet.octopart.com/HVC0603T5004FET-Ohmite-datasheet-26699797.pdf), generated with kicad-footprint-generator
resistor
0
2
2
Resistor_SMD
R_4020_10251Metric_Pad1.65x5.30mm_HandSolder
Resistor SMD 4020 (10251 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://datasheet.octopart.com/HVC0603T5004FET-Ohmite-datasheet-26699797.pdf), generated with kicad-footprint-generator
resistor handsolder
0
2
2
Resistor_SMD
R_Array_Concave_2x0603
Thick Film Chip Resistor Array, Wave soldering, Vishay CRA06P (see cra06p.pdf)
resistor array
0
4
4
Resistor_SMD
R_Array_Concave_4x0402
Thick Film Chip Resistor Array, Wave soldering, Vishay CRA04P (see cra04p.pdf)
resistor array
0
8
8
Resistor_SMD
R_Array_Concave_4x0603
Thick Film Chip Resistor Array, Wave soldering, Vishay CRA06P (see cra06p.pdf)
resistor array
0
8
8
Resistor_SMD
R_Array_Convex_2x0402
Chip Resistor Network, ROHM MNR02 (see mnr_g.pdf)
resistor array
0
4
4
Resistor_SMD
R_Array_Convex_2x0603
Chip Resistor Network, ROHM MNR12 (see mnr_g.pdf)
resistor array
0
4
4
Resistor_SMD
R_Array_Convex_2x0606
Precision Thin Film Chip Resistor Array, VISHAY (see http://www.vishay.com/docs/28770/acasat.pdf)
resistor array
0
4
4
Resistor_SMD
R_Array_Convex_2x1206
Chip Resistor Network, ROHM MNR32 (see mnr_g.pdf)
resistor array
0
4
4
Resistor_SMD
R_Array_Convex_4x0402
Chip Resistor Network, ROHM MNR04 (see mnr_g.pdf)
resistor array
0
8
8
Resistor_SMD
R_Array_Convex_4x0603
Chip Resistor Network, ROHM MNR14 (see mnr_g.pdf)
resistor array
0
8
8
Resistor_SMD
R_Array_Convex_4x0612
Precision Thin Film Chip Resistor Array, VISHAY (see http://www.vishay.com/docs/28770/acasat.pdf)
resistor array
0
8
8
Resistor_SMD
R_Array_Convex_4x1206
Chip Resistor Network, ROHM MNR34 (see mnr_g.pdf)
resistor array
0
8
8
Resistor_SMD
R_Array_Convex_5x0603
Chip Resistor Network, ROHM MNR15 (see mnr_g.pdf)
resistor array
0
10
10
Resistor_SMD
R_Array_Convex_5x1206
Chip Resistor Network, ROHM MNR35 (see mnr_g.pdf)
resistor array
0
10
10
Resistor_SMD
R_Array_Convex_8x0602
Chip Resistor Network, ROHM MNR18 (see mnr_g.pdf)
resistor array
0
16
16
Resistor_SMD
R_Cat16-2
SMT resistor net, Bourns CAT16 series, 2 way
SMT resistor net Bourns CAT16 series 2 way
0
4
4
Resistor_SMD
R_Cat16-4
SMT resistor net, Bourns CAT16 series, 4 way
SMT resistor net Bourns CAT16 series 4 way
0
8
8
Resistor_SMD
R_Cat16-8
SMT resistor net, Bourns CAT16 series, 8 way
SMT resistor net Bourns CAT16 series 8 way
0
16
16
Resistor_SMD
R_MELF_MMB-0207
Resistor, MELF, MMB-0207, http://www.vishay.com/docs/28713/melfprof.pdf
MELF Resistor
0
2
2
Resistor_SMD
R_MicroMELF_MMU-0102
Resistor, MicroMELF, MMU-0102, http://www.vishay.com/docs/28713/melfprof.pdf
MicroMELF Resistor
0
2
2
Resistor_SMD
R_MiniMELF_MMA-0204
Resistor, MiniMELF, MMA-0204, http://www.vishay.com/docs/28713/melfprof.pdf
MiniMELF Resistor
0
2
2
Resistor_SMD
R_Shunt_Ohmite_LVK12
4 contact shunt resistor
shunt resistor 4 contacts
0
4
4
Resistor_SMD
R_Shunt_Ohmite_LVK20
4 contacts shunt resistor, https://www.ohmite.com/assets/docs/res_lvk.pdf
4 contacts resistor smd
0
4
4
Resistor_SMD
R_Shunt_Ohmite_LVK24
4 contacts shunt resistor,https://www.ohmite.com/assets/docs/res_lvk.pdf
4 contacts resistor smd
0
4
4
Resistor_SMD
R_Shunt_Ohmite_LVK25
4 contacts shunt resistor,https://www.ohmite.com/assets/docs/res_lvk.pdf
4 contacts resistor smd
0
4
4
Resistor_SMD
R_Shunt_Vishay_WSK2512_6332Metric_T1.19mm
Shunt Resistor SMD 2512 (6332 Metric), 2.6mm thick, Vishay WKS2512, Terminal length (T) 1.19mm, 5 to 200 milli Ohm (http://http://www.vishay.com/docs/30108/wsk.pdf)
resistor shunt WSK2512
0
4
4
Resistor_SMD
R_Shunt_Vishay_WSK2512_6332Metric_T2.21mm
Shunt Resistor SMD 2512 (6332 Metric), 2.6mm thick, Vishay WKS2512, Terminal length (T) 2.21mm, 1 to 4.9 milli Ohm (http://http://www.vishay.com/docs/30108/wsk.pdf)
resistor shunt WSK2512
0
4
4
Resistor_SMD
R_Shunt_Vishay_WSK2512_6332Metric_T2.66mm
Shunt Resistor SMD 2512 (6332 Metric), 2.6mm thick, Vishay WKS2512, Terminal length (T) 2.66mm, 0.5 to 0.99 milli Ohm (http://http://www.vishay.com/docs/30108/wsk.pdf)
resistor shunt WSK2512
0
4
4
Resistor_SMD
R_Shunt_Vishay_WSKW0612
https://www.vishay.com/docs/30332/wskw0612.pdf
4-Terminal SMD Shunt
0
4
4
Resistor_SMD
R_Shunt_Vishay_WSR2_WSR3
Power Metal Strip Resistors 0.005 to 0.2, https://www.vishay.com/docs/30101/wsr.pdf
SMD Shunt Resistor
0
2
2
Resistor_SMD
R_Shunt_Vishay_WSR2_WSR3_KelvinConnection
Power Metal Strip Resistors 0.005 to 0.2, https://www.vishay.com/docs/30101/wsr.pdf
SMD Shunt Resistor
0
4
2
Resistor_THT
R_Array_SIP4
4-pin Resistor SIP pack
R
0
4
4
Resistor_THT
R_Array_SIP5
5-pin Resistor SIP pack
R
0
5
5
Resistor_THT
R_Array_SIP6
6-pin Resistor SIP pack
R
0
6
6
Resistor_THT
R_Array_SIP7
7-pin Resistor SIP pack
R
0
7
7
Resistor_THT
R_Array_SIP8
8-pin Resistor SIP pack
R
0
8
8
Resistor_THT
R_Array_SIP9
9-pin Resistor SIP pack
R
0
9
9
Resistor_THT
R_Array_SIP10
10-pin Resistor SIP pack
R
0
10
10
Resistor_THT
R_Array_SIP11
11-pin Resistor SIP pack
R
0
11
11
Resistor_THT
R_Array_SIP12
12-pin Resistor SIP pack
R
0
12
12
Resistor_THT
R_Array_SIP13
13-pin Resistor SIP pack
R
0
13
13
Resistor_THT
R_Array_SIP14
14-pin Resistor SIP pack
R
0
14
14
Resistor_THT
R_Axial_DIN0204_L3.6mm_D1.6mm_P1.90mm_Vertical
Resistor, Axial_DIN0204 series, Axial, Vertical, pin pitch=1.9mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf
Resistor Axial_DIN0204 series Axial Vertical pin pitch 1.9mm 0.167W length 3.6mm diameter 1.6mm
0
2
2
Resistor_THT
R_Axial_DIN0204_L3.6mm_D1.6mm_P2.54mm_Vertical
Resistor, Axial_DIN0204 series, Axial, Vertical, pin pitch=2.54mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf
Resistor Axial_DIN0204 series Axial Vertical pin pitch 2.54mm 0.167W length 3.6mm diameter 1.6mm
0
2
2
Resistor_THT
R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal
Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=5.08mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf
Resistor Axial_DIN0204 series Axial Horizontal pin pitch 5.08mm 0.167W length 3.6mm diameter 1.6mm
0
2
2
Resistor_THT
R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Vertical
Resistor, Axial_DIN0204 series, Axial, Vertical, pin pitch=5.08mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf
Resistor Axial_DIN0204 series Axial Vertical pin pitch 5.08mm 0.167W length 3.6mm diameter 1.6mm
0
2
2
Resistor_THT
R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal
Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=7.62mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf
Resistor Axial_DIN0204 series Axial Horizontal pin pitch 7.62mm 0.167W length 3.6mm diameter 1.6mm
0
2
2
Resistor_THT
R_Axial_DIN0207_L6.3mm_D2.5mm_P2.54mm_Vertical
Resistor, Axial_DIN0207 series, Axial, Vertical, pin pitch=2.54mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf
Resistor Axial_DIN0207 series Axial Vertical pin pitch 2.54mm 0.25W = 1/4W length 6.3mm diameter 2.5mm
0
2
2
Resistor_THT
R_Axial_DIN0207_L6.3mm_D2.5mm_P5.08mm_Vertical
Resistor, Axial_DIN0207 series, Axial, Vertical, pin pitch=5.08mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf
Resistor Axial_DIN0207 series Axial Vertical pin pitch 5.08mm 0.25W = 1/4W length 6.3mm diameter 2.5mm
0
2
2
Resistor_THT
R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal
Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf
Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm
0
2
2
Resistor_THT
R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal
Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf
Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm
0
2
2
Resistor_THT
R_Axial_DIN0207_L6.3mm_D2.5mm_P15.24mm_Horizontal
Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=15.24mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf
Resistor Axial_DIN0207 series Axial Horizontal pin pitch 15.24mm 0.25W = 1/4W length 6.3mm diameter 2.5mm
0
2
2
Resistor_THT
R_Axial_DIN0309_L9.0mm_D3.2mm_P2.54mm_Vertical
Resistor, Axial_DIN0309 series, Axial, Vertical, pin pitch=2.54mm, 0.5W = 1/2W, length*diameter=9*3.2mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf
Resistor Axial_DIN0309 series Axial Vertical pin pitch 2.54mm 0.5W = 1/2W length 9mm diameter 3.2mm
0
2
2
Resistor_THT
R_Axial_DIN0309_L9.0mm_D3.2mm_P5.08mm_Vertical
Resistor, Axial_DIN0309 series, Axial, Vertical, pin pitch=5.08mm, 0.5W = 1/2W, length*diameter=9*3.2mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf
Resistor Axial_DIN0309 series Axial Vertical pin pitch 5.08mm 0.5W = 1/2W length 9mm diameter 3.2mm
0
2
2
Resistor_THT
R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal
Resistor, Axial_DIN0309 series, Axial, Horizontal, pin pitch=12.7mm, 0.5W = 1/2W, length*diameter=9*3.2mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf
Resistor Axial_DIN0309 series Axial Horizontal pin pitch 12.7mm 0.5W = 1/2W length 9mm diameter 3.2mm
0
2
2
Resistor_THT
R_Axial_DIN0309_L9.0mm_D3.2mm_P15.24mm_Horizontal
Resistor, Axial_DIN0309 series, Axial, Horizontal, pin pitch=15.24mm, 0.5W = 1/2W, length*diameter=9*3.2mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf
Resistor Axial_DIN0309 series Axial Horizontal pin pitch 15.24mm 0.5W = 1/2W length 9mm diameter 3.2mm
0
2
2
Resistor_THT
R_Axial_DIN0309_L9.0mm_D3.2mm_P20.32mm_Horizontal
Resistor, Axial_DIN0309 series, Axial, Horizontal, pin pitch=20.32mm, 0.5W = 1/2W, length*diameter=9*3.2mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf
Resistor Axial_DIN0309 series Axial Horizontal pin pitch 20.32mm 0.5W = 1/2W length 9mm diameter 3.2mm
0
2
2
Resistor_THT
R_Axial_DIN0309_L9.0mm_D3.2mm_P25.40mm_Horizontal
Resistor, Axial_DIN0309 series, Axial, Horizontal, pin pitch=25.4mm, 0.5W = 1/2W, length*diameter=9*3.2mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf
Resistor Axial_DIN0309 series Axial Horizontal pin pitch 25.4mm 0.5W = 1/2W length 9mm diameter 3.2mm
0
2
2
Resistor_THT
R_Axial_DIN0411_L9.9mm_D3.6mm_P5.08mm_Vertical
Resistor, Axial_DIN0411 series, Axial, Vertical, pin pitch=5.08mm, 1W, length*diameter=9.9*3.6mm^2
Resistor Axial_DIN0411 series Axial Vertical pin pitch 5.08mm 1W length 9.9mm diameter 3.6mm
0
2
2
Resistor_THT
R_Axial_DIN0411_L9.9mm_D3.6mm_P7.62mm_Vertical
Resistor, Axial_DIN0411 series, Axial, Vertical, pin pitch=7.62mm, 1W, length*diameter=9.9*3.6mm^2
Resistor Axial_DIN0411 series Axial Vertical pin pitch 7.62mm 1W length 9.9mm diameter 3.6mm
0
2
2
Resistor_THT
R_Axial_DIN0411_L9.9mm_D3.6mm_P12.70mm_Horizontal
Resistor, Axial_DIN0411 series, Axial, Horizontal, pin pitch=12.7mm, 1W, length*diameter=9.9*3.6mm^2
Resistor Axial_DIN0411 series Axial Horizontal pin pitch 12.7mm 1W length 9.9mm diameter 3.6mm
0
2
2
Resistor_THT
R_Axial_DIN0411_L9.9mm_D3.6mm_P15.24mm_Horizontal
Resistor, Axial_DIN0411 series, Axial, Horizontal, pin pitch=15.24mm, 1W, length*diameter=9.9*3.6mm^2
Resistor Axial_DIN0411 series Axial Horizontal pin pitch 15.24mm 1W length 9.9mm diameter 3.6mm
0
2
2
Resistor_THT
R_Axial_DIN0411_L9.9mm_D3.6mm_P20.32mm_Horizontal
Resistor, Axial_DIN0411 series, Axial, Horizontal, pin pitch=20.32mm, 1W, length*diameter=9.9*3.6mm^2
Resistor Axial_DIN0411 series Axial Horizontal pin pitch 20.32mm 1W length 9.9mm diameter 3.6mm
0
2
2
Resistor_THT
R_Axial_DIN0411_L9.9mm_D3.6mm_P25.40mm_Horizontal
Resistor, Axial_DIN0411 series, Axial, Horizontal, pin pitch=25.4mm, 1W, length*diameter=9.9*3.6mm^2
Resistor Axial_DIN0411 series Axial Horizontal pin pitch 25.4mm 1W length 9.9mm diameter 3.6mm
0
2
2
Resistor_THT
R_Axial_DIN0414_L11.9mm_D4.5mm_P5.08mm_Vertical
Resistor, Axial_DIN0414 series, Axial, Vertical, pin pitch=5.08mm, 2W, length*diameter=11.9*4.5mm^2, http://www.vishay.com/docs/20128/wkxwrx.pdf
Resistor Axial_DIN0414 series Axial Vertical pin pitch 5.08mm 2W length 11.9mm diameter 4.5mm
0
2
2
Resistor_THT
R_Axial_DIN0414_L11.9mm_D4.5mm_P7.62mm_Vertical
Resistor, Axial_DIN0414 series, Axial, Vertical, pin pitch=7.62mm, 2W, length*diameter=11.9*4.5mm^2, http://www.vishay.com/docs/20128/wkxwrx.pdf
Resistor Axial_DIN0414 series Axial Vertical pin pitch 7.62mm 2W length 11.9mm diameter 4.5mm
0
2
2
Resistor_THT
R_Axial_DIN0414_L11.9mm_D4.5mm_P15.24mm_Horizontal
Resistor, Axial_DIN0414 series, Axial, Horizontal, pin pitch=15.24mm, 2W, length*diameter=11.9*4.5mm^2, http://www.vishay.com/docs/20128/wkxwrx.pdf
Resistor Axial_DIN0414 series Axial Horizontal pin pitch 15.24mm 2W length 11.9mm diameter 4.5mm
0
2
2
Resistor_THT
R_Axial_DIN0414_L11.9mm_D4.5mm_P20.32mm_Horizontal
Resistor, Axial_DIN0414 series, Axial, Horizontal, pin pitch=20.32mm, 2W, length*diameter=11.9*4.5mm^2, http://www.vishay.com/docs/20128/wkxwrx.pdf
Resistor Axial_DIN0414 series Axial Horizontal pin pitch 20.32mm 2W length 11.9mm diameter 4.5mm
0
2
2
Resistor_THT
R_Axial_DIN0414_L11.9mm_D4.5mm_P25.40mm_Horizontal
Resistor, Axial_DIN0414 series, Axial, Horizontal, pin pitch=25.4mm, 2W, length*diameter=11.9*4.5mm^2, http://www.vishay.com/docs/20128/wkxwrx.pdf
Resistor Axial_DIN0414 series Axial Horizontal pin pitch 25.4mm 2W length 11.9mm diameter 4.5mm
0
2
2
Resistor_THT
R_Axial_DIN0516_L15.5mm_D5.0mm_P5.08mm_Vertical
Resistor, Axial_DIN0516 series, Axial, Vertical, pin pitch=5.08mm, 2W, length*diameter=15.5*5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf
Resistor Axial_DIN0516 series Axial Vertical pin pitch 5.08mm 2W length 15.5mm diameter 5mm
0
2
2
Resistor_THT
R_Axial_DIN0516_L15.5mm_D5.0mm_P7.62mm_Vertical
Resistor, Axial_DIN0516 series, Axial, Vertical, pin pitch=7.62mm, 2W, length*diameter=15.5*5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf
Resistor Axial_DIN0516 series Axial Vertical pin pitch 7.62mm 2W length 15.5mm diameter 5mm
0
2
2
Resistor_THT
R_Axial_DIN0516_L15.5mm_D5.0mm_P20.32mm_Horizontal
Resistor, Axial_DIN0516 series, Axial, Horizontal, pin pitch=20.32mm, 2W, length*diameter=15.5*5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf
Resistor Axial_DIN0516 series Axial Horizontal pin pitch 20.32mm 2W length 15.5mm diameter 5mm
0
2
2
Resistor_THT
R_Axial_DIN0516_L15.5mm_D5.0mm_P25.40mm_Horizontal
Resistor, Axial_DIN0516 series, Axial, Horizontal, pin pitch=25.4mm, 2W, length*diameter=15.5*5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf
Resistor Axial_DIN0516 series Axial Horizontal pin pitch 25.4mm 2W length 15.5mm diameter 5mm
0
2
2
Resistor_THT
R_Axial_DIN0516_L15.5mm_D5.0mm_P30.48mm_Horizontal
Resistor, Axial_DIN0516 series, Axial, Horizontal, pin pitch=30.48mm, 2W, length*diameter=15.5*5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf
Resistor Axial_DIN0516 series Axial Horizontal pin pitch 30.48mm 2W length 15.5mm diameter 5mm
0
2
2
Resistor_THT
R_Axial_DIN0614_L14.3mm_D5.7mm_P5.08mm_Vertical
Resistor, Axial_DIN0614 series, Axial, Vertical, pin pitch=5.08mm, 1.5W, length*diameter=14.3*5.7mm^2
Resistor Axial_DIN0614 series Axial Vertical pin pitch 5.08mm 1.5W length 14.3mm diameter 5.7mm
0
2
2
Resistor_THT
R_Axial_DIN0614_L14.3mm_D5.7mm_P7.62mm_Vertical
Resistor, Axial_DIN0614 series, Axial, Vertical, pin pitch=7.62mm, 1.5W, length*diameter=14.3*5.7mm^2
Resistor Axial_DIN0614 series Axial Vertical pin pitch 7.62mm 1.5W length 14.3mm diameter 5.7mm
0
2
2
Resistor_THT
R_Axial_DIN0614_L14.3mm_D5.7mm_P15.24mm_Horizontal
Resistor, Axial_DIN0614 series, Axial, Horizontal, pin pitch=15.24mm, 1.5W, length*diameter=14.3*5.7mm^2
Resistor Axial_DIN0614 series Axial Horizontal pin pitch 15.24mm 1.5W length 14.3mm diameter 5.7mm
0
2
2
Resistor_THT
R_Axial_DIN0614_L14.3mm_D5.7mm_P20.32mm_Horizontal
Resistor, Axial_DIN0614 series, Axial, Horizontal, pin pitch=20.32mm, 1.5W, length*diameter=14.3*5.7mm^2
Resistor Axial_DIN0614 series Axial Horizontal pin pitch 20.32mm 1.5W length 14.3mm diameter 5.7mm
0
2
2
Resistor_THT
R_Axial_DIN0614_L14.3mm_D5.7mm_P25.40mm_Horizontal
Resistor, Axial_DIN0614 series, Axial, Horizontal, pin pitch=25.4mm, 1.5W, length*diameter=14.3*5.7mm^2
Resistor Axial_DIN0614 series Axial Horizontal pin pitch 25.4mm 1.5W length 14.3mm diameter 5.7mm
0
2
2
Resistor_THT
R_Axial_DIN0617_L17.0mm_D6.0mm_P5.08mm_Vertical
Resistor, Axial_DIN0617 series, Axial, Vertical, pin pitch=5.08mm, 2W, length*diameter=17*6mm^2, http://www.vishay.com/docs/20128/wkxwrx.pdf
Resistor Axial_DIN0617 series Axial Vertical pin pitch 5.08mm 2W length 17mm diameter 6mm
0
2
2
Resistor_THT
R_Axial_DIN0617_L17.0mm_D6.0mm_P7.62mm_Vertical
Resistor, Axial_DIN0617 series, Axial, Vertical, pin pitch=7.62mm, 2W, length*diameter=17*6mm^2, http://www.vishay.com/docs/20128/wkxwrx.pdf
Resistor Axial_DIN0617 series Axial Vertical pin pitch 7.62mm 2W length 17mm diameter 6mm
0
2
2
Resistor_THT
R_Axial_DIN0617_L17.0mm_D6.0mm_P20.32mm_Horizontal
Resistor, Axial_DIN0617 series, Axial, Horizontal, pin pitch=20.32mm, 2W, length*diameter=17*6mm^2, http://www.vishay.com/docs/20128/wkxwrx.pdf
Resistor Axial_DIN0617 series Axial Horizontal pin pitch 20.32mm 2W length 17mm diameter 6mm
0
2
2
Resistor_THT
R_Axial_DIN0617_L17.0mm_D6.0mm_P25.40mm_Horizontal
Resistor, Axial_DIN0617 series, Axial, Horizontal, pin pitch=25.4mm, 2W, length*diameter=17*6mm^2, http://www.vishay.com/docs/20128/wkxwrx.pdf
Resistor Axial_DIN0617 series Axial Horizontal pin pitch 25.4mm 2W length 17mm diameter 6mm
0
2
2
Resistor_THT
R_Axial_DIN0617_L17.0mm_D6.0mm_P30.48mm_Horizontal
Resistor, Axial_DIN0617 series, Axial, Horizontal, pin pitch=30.48mm, 2W, length*diameter=17*6mm^2, http://www.vishay.com/docs/20128/wkxwrx.pdf
Resistor Axial_DIN0617 series Axial Horizontal pin pitch 30.48mm 2W length 17mm diameter 6mm
0
2
2
Resistor_THT
R_Axial_DIN0918_L18.0mm_D9.0mm_P7.62mm_Vertical
Resistor, Axial_DIN0918 series, Axial, Vertical, pin pitch=7.62mm, 4W, length*diameter=18*9mm^2
Resistor Axial_DIN0918 series Axial Vertical pin pitch 7.62mm 4W length 18mm diameter 9mm
0
2
2
Resistor_THT
R_Axial_DIN0918_L18.0mm_D9.0mm_P22.86mm_Horizontal
Resistor, Axial_DIN0918 series, Axial, Horizontal, pin pitch=22.86mm, 4W, length*diameter=18*9mm^2
Resistor Axial_DIN0918 series Axial Horizontal pin pitch 22.86mm 4W length 18mm diameter 9mm
0
2
2
Resistor_THT
R_Axial_DIN0918_L18.0mm_D9.0mm_P25.40mm_Horizontal
Resistor, Axial_DIN0918 series, Axial, Horizontal, pin pitch=25.4mm, 4W, length*diameter=18*9mm^2
Resistor Axial_DIN0918 series Axial Horizontal pin pitch 25.4mm 4W length 18mm diameter 9mm
0
2
2
Resistor_THT
R_Axial_DIN0918_L18.0mm_D9.0mm_P30.48mm_Horizontal
Resistor, Axial_DIN0918 series, Axial, Horizontal, pin pitch=30.48mm, 4W, length*diameter=18*9mm^2
Resistor Axial_DIN0918 series Axial Horizontal pin pitch 30.48mm 4W length 18mm diameter 9mm
0
2
2
Resistor_THT
R_Axial_DIN0922_L20.0mm_D9.0mm_P7.62mm_Vertical
Resistor, Axial_DIN0922 series, Axial, Vertical, pin pitch=7.62mm, 5W, length*diameter=20*9mm^2, http://www.vishay.com/docs/20128/wkxwrx.pdf
Resistor Axial_DIN0922 series Axial Vertical pin pitch 7.62mm 5W length 20mm diameter 9mm
0
2
2
Resistor_THT
R_Axial_DIN0922_L20.0mm_D9.0mm_P25.40mm_Horizontal
Resistor, Axial_DIN0922 series, Axial, Horizontal, pin pitch=25.4mm, 5W, length*diameter=20*9mm^2, http://www.vishay.com/docs/20128/wkxwrx.pdf
Resistor Axial_DIN0922 series Axial Horizontal pin pitch 25.4mm 5W length 20mm diameter 9mm
0
2
2
Resistor_THT
R_Axial_DIN0922_L20.0mm_D9.0mm_P30.48mm_Horizontal
Resistor, Axial_DIN0922 series, Axial, Horizontal, pin pitch=30.48mm, 5W, length*diameter=20*9mm^2, http://www.vishay.com/docs/20128/wkxwrx.pdf
Resistor Axial_DIN0922 series Axial Horizontal pin pitch 30.48mm 5W length 20mm diameter 9mm
0
2
2
Resistor_THT
R_Axial_Power_L20.0mm_W6.4mm_P5.08mm_Vertical
Resistor, Axial_Power series, Axial, Vertical, pin pitch=5.08mm, 4W, length*width*height=20*6.4*6.4mm^3, http://cdn-reichelt.de/documents/datenblatt/B400/5WAXIAL_9WAXIAL_11WAXIAL_17WAXIAL%23YAG.pdf
Resistor Axial_Power series Axial Vertical pin pitch 5.08mm 4W length 20mm width 6.4mm height 6.4mm
0
2
2
Resistor_THT
R_Axial_Power_L20.0mm_W6.4mm_P7.62mm_Vertical
Resistor, Axial_Power series, Axial, Vertical, pin pitch=7.62mm, 4W, length*width*height=20*6.4*6.4mm^3, http://cdn-reichelt.de/documents/datenblatt/B400/5WAXIAL_9WAXIAL_11WAXIAL_17WAXIAL%23YAG.pdf
Resistor Axial_Power series Axial Vertical pin pitch 7.62mm 4W length 20mm width 6.4mm height 6.4mm
0
2
2
Resistor_THT
R_Axial_Power_L20.0mm_W6.4mm_P22.40mm
Resistor, Axial_Power series, Box, pin pitch=22.4mm, 4W, length*width*height=20*6.4*6.4mm^3, http://cdn-reichelt.de/documents/datenblatt/B400/5WAXIAL_9WAXIAL_11WAXIAL_17WAXIAL%23YAG.pdf
Resistor Axial_Power series Box pin pitch 22.4mm 4W length 20mm width 6.4mm height 6.4mm
0
2
2
Resistor_THT
R_Axial_Power_L20.0mm_W6.4mm_P25.40mm
Resistor, Axial_Power series, Box, pin pitch=25.4mm, 4W, length*width*height=20*6.4*6.4mm^3, http://cdn-reichelt.de/documents/datenblatt/B400/5WAXIAL_9WAXIAL_11WAXIAL_17WAXIAL%23YAG.pdf
Resistor Axial_Power series Box pin pitch 25.4mm 4W length 20mm width 6.4mm height 6.4mm
0
2
2
Resistor_THT
R_Axial_Power_L20.0mm_W6.4mm_P30.48mm
Resistor, Axial_Power series, Box, pin pitch=30.48mm, 4W, length*width*height=20*6.4*6.4mm^3, http://cdn-reichelt.de/documents/datenblatt/B400/5WAXIAL_9WAXIAL_11WAXIAL_17WAXIAL%23YAG.pdf
Resistor Axial_Power series Box pin pitch 30.48mm 4W length 20mm width 6.4mm height 6.4mm
0
2
2
Resistor_THT
R_Axial_Power_L25.0mm_W6.4mm_P27.94mm
Resistor, Axial_Power series, Box, pin pitch=27.94mm, 5W, length*width*height=25*6.4*6.4mm^3, http://cdn-reichelt.de/documents/datenblatt/B400/5WAXIAL_9WAXIAL_11WAXIAL_17WAXIAL%23YAG.pdf
Resistor Axial_Power series Box pin pitch 27.94mm 5W length 25mm width 6.4mm height 6.4mm
0
2
2
Resistor_THT
R_Axial_Power_L25.0mm_W6.4mm_P30.48mm
Resistor, Axial_Power series, Box, pin pitch=30.48mm, 5W, length*width*height=25*6.4*6.4mm^3, http://cdn-reichelt.de/documents/datenblatt/B400/5WAXIAL_9WAXIAL_11WAXIAL_17WAXIAL%23YAG.pdf
Resistor Axial_Power series Box pin pitch 30.48mm 5W length 25mm width 6.4mm height 6.4mm
0
2
2
Resistor_THT
R_Axial_Power_L25.0mm_W9.0mm_P7.62mm_Vertical
Resistor, Axial_Power series, Axial, Vertical, pin pitch=7.62mm, 7W, length*width*height=25*9*9mm^3, http://cdn-reichelt.de/documents/datenblatt/B400/5WAXIAL_9WAXIAL_11WAXIAL_17WAXIAL%23YAG.pdf
Resistor Axial_Power series Axial Vertical pin pitch 7.62mm 7W length 25mm width 9mm height 9mm
0
2
2
Resistor_THT
R_Axial_Power_L25.0mm_W9.0mm_P10.16mm_Vertical
Resistor, Axial_Power series, Axial, Vertical, pin pitch=10.16mm, 7W, length*width*height=25*9*9mm^3, http://cdn-reichelt.de/documents/datenblatt/B400/5WAXIAL_9WAXIAL_11WAXIAL_17WAXIAL%23YAG.pdf
Resistor Axial_Power series Axial Vertical pin pitch 10.16mm 7W length 25mm width 9mm height 9mm
0
2
2
Resistor_THT
R_Axial_Power_L25.0mm_W9.0mm_P27.94mm
Resistor, Axial_Power series, Box, pin pitch=27.94mm, 7W, length*width*height=25*9*9mm^3, http://cdn-reichelt.de/documents/datenblatt/B400/5WAXIAL_9WAXIAL_11WAXIAL_17WAXIAL%23YAG.pdf
Resistor Axial_Power series Box pin pitch 27.94mm 7W length 25mm width 9mm height 9mm
0
2
2
Resistor_THT
R_Axial_Power_L25.0mm_W9.0mm_P30.48mm
Resistor, Axial_Power series, Box, pin pitch=30.48mm, 7W, length*width*height=25*9*9mm^3, http://cdn-reichelt.de/documents/datenblatt/B400/5WAXIAL_9WAXIAL_11WAXIAL_17WAXIAL%23YAG.pdf
Resistor Axial_Power series Box pin pitch 30.48mm 7W length 25mm width 9mm height 9mm
0
2
2
Resistor_THT
R_Axial_Power_L38.0mm_W6.4mm_P40.64mm
Resistor, Axial_Power series, Box, pin pitch=40.64mm, 7W, length*width*height=38*6.4*6.4mm^3, http://cdn-reichelt.de/documents/datenblatt/B400/5WAXIAL_9WAXIAL_11WAXIAL_17WAXIAL%23YAG.pdf
Resistor Axial_Power series Box pin pitch 40.64mm 7W length 38mm width 6.4mm height 6.4mm
0
2
2
Resistor_THT
R_Axial_Power_L38.0mm_W6.4mm_P45.72mm
Resistor, Axial_Power series, Box, pin pitch=45.72mm, 7W, length*width*height=38*6.4*6.4mm^3, http://cdn-reichelt.de/documents/datenblatt/B400/5WAXIAL_9WAXIAL_11WAXIAL_17WAXIAL%23YAG.pdf
Resistor Axial_Power series Box pin pitch 45.72mm 7W length 38mm width 6.4mm height 6.4mm
0
2
2
Resistor_THT
R_Axial_Power_L38.0mm_W9.0mm_P40.64mm
Resistor, Axial_Power series, Box, pin pitch=40.64mm, 9W, length*width*height=38*9*9mm^3, http://cdn-reichelt.de/documents/datenblatt/B400/5WAXIAL_9WAXIAL_11WAXIAL_17WAXIAL%23YAG.pdf
Resistor Axial_Power series Box pin pitch 40.64mm 9W length 38mm width 9mm height 9mm
0
2
2
Resistor_THT
R_Axial_Power_L38.0mm_W9.0mm_P45.72mm
Resistor, Axial_Power series, Box, pin pitch=45.72mm, 9W, length*width*height=38*9*9mm^3, http://cdn-reichelt.de/documents/datenblatt/B400/5WAXIAL_9WAXIAL_11WAXIAL_17WAXIAL%23YAG.pdf
Resistor Axial_Power series Box pin pitch 45.72mm 9W length 38mm width 9mm height 9mm
0
2
2
Resistor_THT
R_Axial_Power_L48.0mm_W12.5mm_P7.62mm_Vertical
Resistor, Axial_Power series, Axial, Vertical, pin pitch=7.62mm, 15W, length*width*height=48*12.5*12.5mm^3, http://cdn-reichelt.de/documents/datenblatt/B400/5WAXIAL_9WAXIAL_11WAXIAL_17WAXIAL%23YAG.pdf
Resistor Axial_Power series Axial Vertical pin pitch 7.62mm 15W length 48mm width 12.5mm height 12.5mm
0
2
2
Resistor_THT
R_Axial_Power_L48.0mm_W12.5mm_P10.16mm_Vertical
Resistor, Axial_Power series, Axial, Vertical, pin pitch=10.16mm, 15W, length*width*height=48*12.5*12.5mm^3, http://cdn-reichelt.de/documents/datenblatt/B400/5WAXIAL_9WAXIAL_11WAXIAL_17WAXIAL%23YAG.pdf
Resistor Axial_Power series Axial Vertical pin pitch 10.16mm 15W length 48mm width 12.5mm height 12.5mm
0
2
2
Resistor_THT
R_Axial_Power_L48.0mm_W12.5mm_P55.88mm
Resistor, Axial_Power series, Box, pin pitch=55.88mm, 15W, length*width*height=48*12.5*12.5mm^3, http://cdn-reichelt.de/documents/datenblatt/B400/5WAXIAL_9WAXIAL_11WAXIAL_17WAXIAL%23YAG.pdf
Resistor Axial_Power series Box pin pitch 55.88mm 15W length 48mm width 12.5mm height 12.5mm
0
2
2
Resistor_THT
R_Axial_Power_L48.0mm_W12.5mm_P60.96mm
Resistor, Axial_Power series, Box, pin pitch=60.96mm, 15W, length*width*height=48*12.5*12.5mm^3, http://cdn-reichelt.de/documents/datenblatt/B400/5WAXIAL_9WAXIAL_11WAXIAL_17WAXIAL%23YAG.pdf
Resistor Axial_Power series Box pin pitch 60.96mm 15W length 48mm width 12.5mm height 12.5mm
0
2
2
Resistor_THT
R_Axial_Power_L50.0mm_W9.0mm_P55.88mm
Resistor, Axial_Power series, Box, pin pitch=55.88mm, 11W, length*width*height=50*9*9mm^3, http://cdn-reichelt.de/documents/datenblatt/B400/5WAXIAL_9WAXIAL_11WAXIAL_17WAXIAL%23YAG.pdf
Resistor Axial_Power series Box pin pitch 55.88mm 11W length 50mm width 9mm height 9mm
0
2
2
Resistor_THT
R_Axial_Power_L50.0mm_W9.0mm_P60.96mm
Resistor, Axial_Power series, Box, pin pitch=60.96mm, 11W, length*width*height=50*9*9mm^3, http://cdn-reichelt.de/documents/datenblatt/B400/5WAXIAL_9WAXIAL_11WAXIAL_17WAXIAL%23YAG.pdf
Resistor Axial_Power series Box pin pitch 60.96mm 11W length 50mm width 9mm height 9mm
0
2
2
Resistor_THT
R_Axial_Power_L60.0mm_W14.0mm_P10.16mm_Vertical
Resistor, Axial_Power series, Axial, Vertical, pin pitch=10.16mm, 25W, length*width*height=60*14*14mm^3, http://cdn-reichelt.de/documents/datenblatt/B400/5WAXIAL_9WAXIAL_11WAXIAL_17WAXIAL%23YAG.pdf
Resistor Axial_Power series Axial Vertical pin pitch 10.16mm 25W length 60mm width 14mm height 14mm
0
2
2
Resistor_THT
R_Axial_Power_L60.0mm_W14.0mm_P66.04mm
Resistor, Axial_Power series, Box, pin pitch=66.04mm, 25W, length*width*height=60*14*14mm^3, http://cdn-reichelt.de/documents/datenblatt/B400/5WAXIAL_9WAXIAL_11WAXIAL_17WAXIAL%23YAG.pdf
Resistor Axial_Power series Box pin pitch 66.04mm 25W length 60mm width 14mm height 14mm
0
2
2
Resistor_THT
R_Axial_Power_L60.0mm_W14.0mm_P71.12mm
Resistor, Axial_Power series, Box, pin pitch=71.12mm, 25W, length*width*height=60*14*14mm^3, http://cdn-reichelt.de/documents/datenblatt/B400/5WAXIAL_9WAXIAL_11WAXIAL_17WAXIAL%23YAG.pdf
Resistor Axial_Power series Box pin pitch 71.12mm 25W length 60mm width 14mm height 14mm
0
2
2
Resistor_THT
R_Axial_Power_L75.0mm_W9.0mm_P81.28mm
Resistor, Axial_Power series, Box, pin pitch=81.28mm, 17W, length*width*height=75*9*9mm^3, http://cdn-reichelt.de/documents/datenblatt/B400/5WAXIAL_9WAXIAL_11WAXIAL_17WAXIAL%23YAG.pdf
Resistor Axial_Power series Box pin pitch 81.28mm 17W length 75mm width 9mm height 9mm
0
2
2
Resistor_THT
R_Axial_Power_L75.0mm_W9.0mm_P86.36mm
Resistor, Axial_Power series, Box, pin pitch=86.36mm, 17W, length*width*height=75*9*9mm^3, http://cdn-reichelt.de/documents/datenblatt/B400/5WAXIAL_9WAXIAL_11WAXIAL_17WAXIAL%23YAG.pdf
Resistor Axial_Power series Box pin pitch 86.36mm 17W length 75mm width 9mm height 9mm
0
2
2
Resistor_THT
R_Axial_Shunt_L22.2mm_W8.0mm_PS14.30mm_P25.40mm
Resistor, Axial_Shunt series, Box, pin pitch=25.4mm, 3W, length*width*height=22.2*8*8mm^3, shunt pin pitch = 14.30mm, http://www.vishay.com/docs/30217/cpsl.pdf
Resistor Axial_Shunt series Box pin pitch 25.4mm 3W length 22.2mm width 8mm height 8mm shunt pin pitch 14.30mm
0
4
4
Resistor_THT
R_Axial_Shunt_L22.2mm_W9.5mm_PS14.30mm_P25.40mm
Resistor, Axial_Shunt series, Box, pin pitch=25.4mm, 5W, length*width*height=22.2*9.5*9.5mm^3, shunt pin pitch = 14.30mm, http://www.vishay.com/docs/30217/cpsl.pdf
Resistor Axial_Shunt series Box pin pitch 25.4mm 5W length 22.2mm width 9.5mm height 9.5mm shunt pin pitch 14.30mm
0
4
4
Resistor_THT
R_Axial_Shunt_L35.3mm_W9.5mm_PS25.40mm_P38.10mm
Resistor, Axial_Shunt series, Box, pin pitch=38.1mm, 7W, length*width*height=35.3*9.5*9.5mm^3, shunt pin pitch = 25.40mm, http://www.vishay.com/docs/30217/cpsl.pdf
Resistor Axial_Shunt series Box pin pitch 38.1mm 7W length 35.3mm width 9.5mm height 9.5mm shunt pin pitch 25.40mm
0
4
4
Resistor_THT
R_Axial_Shunt_L47.6mm_W9.5mm_PS34.93mm_P50.80mm
Resistor, Axial_Shunt series, Box, pin pitch=50.8mm, 10W, length*width*height=47.6*9.5*9.5mm^3, shunt pin pitch = 34.93mm, http://www.vishay.com/docs/30217/cpsl.pdf
Resistor Axial_Shunt series Box pin pitch 50.8mm 10W length 47.6mm width 9.5mm height 9.5mm shunt pin pitch 34.93mm
0
4
4
Resistor_THT
R_Axial_Shunt_L47.6mm_W12.7mm_PS34.93mm_P50.80mm
Resistor, Axial_Shunt series, Box, pin pitch=50.8mm, 15W, length*width*height=47.6*12.7*12.7mm^3, shunt pin pitch = 34.93mm, http://www.vishay.com/docs/30217/cpsl.pdf
Resistor Axial_Shunt series Box pin pitch 50.8mm 15W length 47.6mm width 12.7mm height 12.7mm shunt pin pitch 34.93mm
0
4
4
Resistor_THT
R_Bare_Metal_Element_L12.4mm_W4.8mm_P11.40mm
Resistor, Bare_Metal_Element series, Bare Metal Strip/Wire, Horizontal, pin pitch=11.4mm, 1W, length*width=12.4*4.8mm^2, https://www.bourns.com/pdfs/PWR4412-2S.pdf
Resistor Bare_Metal_Element series Bare Metal Strip Wire Horizontal pin pitch 11.4mm 1W length 12.4mm width 4.8mm 
0
2
2
Resistor_THT
R_Bare_Metal_Element_L16.3mm_W4.8mm_P15.30mm
Resistor, Bare_Metal_Element series, Bare Metal Strip/Wire, Horizontal, pin pitch=15.3mm, 3W, length*width=16.3*4.8mm^2, https://www.bourns.com/pdfs/PWR4412-2S.pdf
Resistor Bare_Metal_Element series Bare Metal Strip Wire Horizontal pin pitch 15.3mm 3W length 16.3mm width 4.8mm 
0
2
2
Resistor_THT
R_Bare_Metal_Element_L21.3mm_W4.8mm_P20.30mm
Resistor, Bare_Metal_Element series, Bare Metal Strip/Wire, Horizontal, pin pitch=20.3mm, 5W, length*width=21.3*4.8mm^2, https://www.bourns.com/pdfs/PWR4412-2S.pdf
Resistor Bare_Metal_Element series Bare Metal Strip Wire Horizontal pin pitch 20.3mm 5W length 21.3mm width 4.8mm 
0
2
2
Resistor_THT
R_Box_L8.4mm_W2.5mm_P5.08mm
Resistor, Box series, Radial, pin pitch=5.08mm, 0.5W = 1/2W, length*width=8.38*2.54mm^2, http://www.vishay.com/docs/60051/cns020.pdf
Resistor Box series Radial pin pitch 5.08mm 0.5W = 1/2W length 8.38mm width 2.54mm
0
2
2
Resistor_THT
R_Box_L13.0mm_W4.0mm_P9.00mm
Resistor, Box series, Radial, pin pitch=9.00mm, 2W, length*width=13.0*4.0mm^2, http://www.produktinfo.conrad.com/datenblaetter/425000-449999/443860-da-01-de-METALLBAND_WIDERSTAND_0_1_OHM_5W_5Pr.pdf
Resistor Box series Radial pin pitch 9.00mm 2W length 13.0mm width 4.0mm
0
2
2
Resistor_THT
R_Box_L14.0mm_W5.0mm_P9.00mm
Resistor, Box series, Radial, pin pitch=9.00mm, 5W, length*width=14.0*5.0mm^2, http://www.produktinfo.conrad.com/datenblaetter/425000-449999/443860-da-01-de-METALLBAND_WIDERSTAND_0_1_OHM_5W_5Pr.pdf
Resistor Box series Radial pin pitch 9.00mm 5W length 14.0mm width 5.0mm
0
2
2
Resistor_THT
R_Box_L26.0mm_W5.0mm_P20.00mm
Resistor, Box series, Radial, pin pitch=20.00mm, 10W, length*width=26.0*5.0mm^2, http://www.produktinfo.conrad.com/datenblaetter/425000-449999/443860-da-01-de-METALLBAND_WIDERSTAND_0_1_OHM_5W_5Pr.pdf
Resistor Box series Radial pin pitch 20.00mm 10W length 26.0mm width 5.0mm
0
2
2
Resistor_THT
R_Radial_Power_L7.0mm_W8.0mm_Px2.40mm_Py2.30mm
Resistor, Radial_Power series, Radial, pin pitch=2.40*2.30mm^2, 7W, length*width=7*8mm^2, http://www.vitrohm.com/content/files/vitrohm_series_kv_-_201601.pdf
Resistor Radial_Power series Radial pin pitch 2.40*2.30mm^2 7W length 7mm width 8mm
0
2
2
Resistor_THT
R_Radial_Power_L9.0mm_W10.0mm_Px2.70mm_Py2.30mm
Resistor, Radial_Power series, Radial, pin pitch=2.70*2.30mm^2, 17W, length*width=9*10mm^2, http://www.vitrohm.com/content/files/vitrohm_series_kv_-_201601.pdf
Resistor Radial_Power series Radial pin pitch 2.70*2.30mm^2 17W length 9mm width 10mm
0
2
2
Resistor_THT
R_Radial_Power_L11.0mm_W7.0mm_P5.00mm
Resistor, Radial_Power series, Radial, pin pitch=5.00mm, 2W, length*width=11.0*7.0mm^2, http://www.vishay.com/docs/30218/cpcx.pdf
Resistor Radial_Power series Radial pin pitch 5.00mm 2W length 11.0mm width 7.0mm
0
2
2
Resistor_THT
R_Radial_Power_L12.0mm_W8.0mm_P5.00mm
Resistor, Radial_Power series, Radial, pin pitch=5.00mm, 3W, length*width=12.0*8.0mm^2, http://www.vishay.com/docs/30218/cpcx.pdf
Resistor Radial_Power series Radial pin pitch 5.00mm 3W length 12.0mm width 8.0mm
0
2
2
Resistor_THT
R_Radial_Power_L13.0mm_W9.0mm_P5.00mm
Resistor, Radial_Power series, Radial, pin pitch=5.00mm, 7W, length*width=13.0*9.0mm^2, http://www.vishay.com/docs/30218/cpcx.pdf
Resistor Radial_Power series Radial pin pitch 5.00mm 7W length 13.0mm width 9.0mm
0
2
2
Resistor_THT
R_Radial_Power_L16.1mm_W9.0mm_P7.37mm
Resistor, Radial_Power series, Radial, pin pitch=7.37mm, 10W, length*width=16.1*9mm^2, http://www.vishay.com/docs/30218/cpcx.pdf
Resistor Radial_Power series Radial pin pitch 7.37mm 10W length 16.1mm width 9mm
0
2
2
TO_SOT_Packages_SMD
ATPAK-2
ATPAK SMD package, http://www.onsemi.com/pub/Collateral/ENA2192-D.PDF
ATPAK 
0
7
3
TO_SOT_Packages_SMD
Analog_KS-4
Analog Devices KS-4, http://www.analog.com/media/en/package-pcb-resources/package/pkg_pdf/sc70ks/ks_4.pdf
Analog Devices KS-4 (like EIAJ SC-82)
0
4
4
TO_SOT_Packages_SMD
Diodes_SOT-553
Diodes SOT-553, https://www.diodes.com/assets/Package-Files/SOT553.pdf
SOT-553
0
5
5
TO_SOT_Packages_SMD
HVSOF5
HVSOF5, http://rohmfs.rohm.com/en/techdata_basic/ic/package/hvsof5_1-e.pdf, http://rohmfs.rohm.com/en/products/databook/datasheet/ic/sensor/hall/bu52001gul-e.pdf
HVSOF5
0
5
5
TO_SOT_Packages_SMD
HVSOF6
HVSOF6, http://rohmfs.rohm.com/en/techdata_basic/ic/package/hvsof6_1-e.pdf, http://rohmfs.rohm.com/en/products/databook/datasheet/ic/audio_video/video_amplifier/bh76106hfv-e.pdf
HVSOF6
0
7
7
TO_SOT_Packages_SMD
Infineon_PG-HDSOP-10-1
Infineon PG-HDSOP-10-1 (DDPAK), 20.96x6.5x2.3mm, slug up (https://www.infineon.com/cms/en/product/packages/PG-HDSOP/PG-HDSOP-10-1/)
hdsop 10 ddpak
0
10
10
TO_SOT_Packages_SMD
Infineon_PG-HSOF-8-1
Infineon HSOF-8-1 power mosfet http://www.infineon.com/cms/en/product/packages/PG-HSOF/PG-HSOF-8-1/
mosfet hsof
0
54
3
TO_SOT_Packages_SMD
Infineon_PG-HSOF-8-1_ThermalVias
HSOF-8-1 power mosfet http://www.infineon.com/cms/en/product/packages/PG-HSOF/PG-HSOF-8-1/
mosfet hsof thermal vias
0
57
3
TO_SOT_Packages_SMD
Infineon_PG-TO-220-7Lead_TabPin8
Infineon PG-TO-220-7, Tab as Pin 8, see e.g. https://www.infineon.com/dgdl/Infineon-BTS50055-1TMC-DS-v01_00-EN.pdf?fileId=5546d4625a888733015aa9b0007235e9
Infineon PG-TO-220-7
0
12
8
TO_SOT_Packages_SMD
LFPAK33
LFPAK33 SOT-1210 https://assets.nexperia.com/documents/outline-drawing/SOT1210.pdf
LFPAK33 SOT-1210
0
17
5
TO_SOT_Packages_SMD
LFPAK56
LFPAK56 https://assets.nexperia.com/documents/outline-drawing/SOT669.pdf
LFPAK56 SOT-669 Power-SO8
0
18
5
TO_SOT_Packages_SMD
OnSemi_ECH8
On Semiconductor ECH8, https://www.onsemi.com/pub/Collateral/318BF.PDF
ECH8 SOT28-FL SOT-28-FL
0
8
8
TO_SOT_Packages_SMD
PQFN_8x8
Low Profile 8x8mm PQFN, Dual Cool 88, https://www.onsemi.com/pub/Collateral/FDMT80080DC-D.pdf
pqfn vdfn mosfet
0
9
3
TO_SOT_Packages_SMD
PowerMacro_M234_NoHole
TO-50-4 Power Macro Package Style M234
TO-50-4 Power Macro Package Style M234
0
4
4
TO_SOT_Packages_SMD
PowerMacro_M234_WithHole
TO-50-4 Power Macro Package Style M234
TO-50-4 Power Macro Package Style M234
0
4
4
TO_SOT_Packages_SMD
Rohm_HRP7
Rohm HRP7 SMD package, http://rohmfs.rohm.com/en/techdata_basic/ic/package/hrp7_1-e.pdf, http://rohmfs.rohm.com/en/products/databook/datasheet/ic/motor/dc/bd621x-e.pdf
Rohm HRP7 SMD
0
69
7
TO_SOT_Packages_SMD
SC-59
SC-59, https://lib.chipdip.ru/images/import_diod/original/SOT-23_SC-59.jpg
SC-59
0
3
3
TO_SOT_Packages_SMD
SC-59_Handsoldering
SC-59, hand-soldering varaint, https://lib.chipdip.ru/images/import_diod/original/SOT-23_SC-59.jpg
SC-59 hand-soldering
0
3
3
TO_SOT_Packages_SMD
SC-70-8
SC70-8
SC70-8
0
8
8
TO_SOT_Packages_SMD
SC-70-8_Handsoldering
SC70-8, Handsoldering
SC70-8 Handsoldering
0
8
8
TO_SOT_Packages_SMD
SC-82AA
SC-82AA
SC-82AA
0
4
4
TO_SOT_Packages_SMD
SC-82AA_Handsoldering
SC-82AA
SC-82AA
0
4
4
TO_SOT_Packages_SMD
SC-82AB
SC-82AB
SC-82AB
0
4
4
TO_SOT_Packages_SMD
SC-82AB_Handsoldering
SC-82AB
SC-82AB
0
4
4
TO_SOT_Packages_SMD
SOT-23
SOT-23, Standard
SOT-23
0
3
3
TO_SOT_Packages_SMD
SOT-23-5
5-pin SOT23 package
SOT-23-5
0
5
5
TO_SOT_Packages_SMD
SOT-23-5_HandSoldering
5-pin SOT23 package
SOT-23-5 hand-soldering
0
5
5
TO_SOT_Packages_SMD
SOT-23-6
6-pin SOT-23 package
SOT-23-6
0
6
6
TO_SOT_Packages_SMD
SOT-23-6_Handsoldering
6-pin SOT-23 package, Handsoldering
SOT-23-6 Handsoldering
0
6
6
TO_SOT_Packages_SMD
SOT-23-8
8-pin SOT-23 package, http://www.analog.com/media/en/package-pcb-resources/package/pkg_pdf/sot-23rj/rj_8.pdf
SOT-23-8
0
8
8
TO_SOT_Packages_SMD
SOT-23-8_Handsoldering
8-pin SOT-23 package, Handsoldering, http://www.analog.com/media/en/package-pcb-resources/package/pkg_pdf/sot-23rj/rj_8.pdf
SOT-23-8 Handsoldering
0
8
8
TO_SOT_Packages_SMD
SOT-23W
SOT-23W http://www.allegromicro.com/~/media/Files/Datasheets/A112x-Datasheet.ashx?la=en&hash=7BC461E058CC246E0BAB62433B2F1ECA104CA9D3
SOT-23W
0
3
3
TO_SOT_Packages_SMD
SOT-23W_Handsoldering
SOT-23W http://www.allegromicro.com/~/media/Files/Datasheets/A112x-Datasheet.ashx?la=en&hash=7BC461E058CC246E0BAB62433B2F1ECA104CA9D3
SOT-23W for handsoldering
0
3
3
TO_SOT_Packages_SMD
SOT-23_Handsoldering
SOT-23, Handsoldering
SOT-23
0
3
3
TO_SOT_Packages_SMD
SOT-89-3
SOT-89-3, http://ww1.microchip.com/downloads/en/DeviceDoc/3L_SOT-89_MB_C04-029C.pdf
SOT-89-3
0
3
3
TO_SOT_Packages_SMD
SOT-89-3_Handsoldering
SOT-89-3 Handsoldering
SOT-89-3 Handsoldering
0
3
3
TO_SOT_Packages_SMD
SOT-89-5
SOT-89-5, http://www.e-devices.ricoh.co.jp/en/products/product_power/pkg/sot-89-5.pdf
SOT-89-5
0
5
5
TO_SOT_Packages_SMD
SOT-89-5_Handsoldering
SOT-89-5, http://www.e-devices.ricoh.co.jp/en/products/product_power/pkg/sot-89-5.pdf
SOT-89-5
0
5
5
TO_SOT_Packages_SMD
SOT-143
SOT-143
SOT-143
0
4
4
TO_SOT_Packages_SMD
SOT-143R_Reverse
SOT-143R Reverse
SOT-143R Reverse
0
4
4
TO_SOT_Packages_SMD
SOT-143R_Reverse_Handsoldering
SOT-143R Reverse Handsoldering
SOT-143 Reverse Handsoldering
0
4
4
TO_SOT_Packages_SMD
SOT-143_Handsoldering
SOT-143 Handsoldering
SOT-143 Handsoldering
0
4
4
TO_SOT_Packages_SMD
SOT-223
module CMS SOT223 4 pins
CMS SOT
0
4
4
TO_SOT_Packages_SMD
SOT-223-3_TabPin2
module CMS SOT223 4 pins
CMS SOT
0
4
3
TO_SOT_Packages_SMD
SOT-223-5
module CMS SOT223 5 pins, http://ww1.microchip.com/downloads/en/DeviceDoc/51751a.pdf
CMS SOT
0
5
5
TO_SOT_Packages_SMD
SOT-223-6
module CMS SOT223 6 pins, http://www.ti.com/lit/ds/symlink/tps737.pdf
CMS SOT
0
6
6
TO_SOT_Packages_SMD
SOT-223-6_TabPin3
module CMS SOT223 6 pins, http://www.ti.com/lit/ds/symlink/tps737.pdf
CMS SOT
0
6
5
TO_SOT_Packages_SMD
SOT-223-8
module CMS SOT223 8 pins, https://www.diodes.com/assets/Datasheets/ZXSBMR16PT8.pdf
CMS SOT
0
8
8
TO_SOT_Packages_SMD
SOT-323_SC-70
SOT-323, SC-70
SOT-323 SC-70
0
3
3
TO_SOT_Packages_SMD
SOT-323_SC-70_Handsoldering
SOT-323, SC-70 Handsoldering
SOT-323 SC-70 Handsoldering
0
3
3
TO_SOT_Packages_SMD
SOT-343_SC-70-4
SOT-343, SC-70-4
SOT-343 SC-70-4
0
4
4
TO_SOT_Packages_SMD
SOT-343_SC-70-4_Handsoldering
SOT-343, SC-70-4, Handsoldering
SOT-343 SC-70-4 Handsoldering
0
4
4
TO_SOT_Packages_SMD
SOT-353_SC-70-5
SOT-353, SC-70-5
SOT-353 SC-70-5
0
5
5
TO_SOT_Packages_SMD
SOT-353_SC-70-5_Handsoldering
SOT-353, SC-70-5, Handsoldering
SOT-353 SC-70-5 Handsoldering
0
5
5
TO_SOT_Packages_SMD
SOT-363_SC-70-6
SOT-363, SC-70-6
SOT-363 SC-70-6
0
6
6
TO_SOT_Packages_SMD
SOT-363_SC-70-6_Handsoldering
SOT-363, SC-70-6, Handsoldering
SOT-363 SC-70-6 Handsoldering
0
6
6
TO_SOT_Packages_SMD
SOT-383F
8-pin SOT-383F, http://www.mouser.com/ds/2/80/CPDVR085V0C-HF-RevB-10783.pdf
SOT-383F
0
9
9
TO_SOT_Packages_SMD
SOT-383FL
8-pin SOT-383FL package, http://www.onsemi.com/pub_link/Collateral/ENA2267-D.PDF
SOT-383FL
0
8
8
TO_SOT_Packages_SMD
SOT-416
SOT-416, https://www.nxp.com/docs/en/package-information/SOT416.pdf
SOT-416
0
3
3
TO_SOT_Packages_SMD
SOT-523
SOT523, https://www.diodes.com/assets/Package-Files/SOT523.pdf
SOT-523
0
3
3
TO_SOT_Packages_SMD
SOT-543
SOT-543 4 lead surface package
SOT-543 SC-107A EMD4
0
4
4
TO_SOT_Packages_SMD
SOT-553
SOT553
SOT-553
0
5
5
TO_SOT_Packages_SMD
SOT-563
SOT563
SOT-563
0
6
6
TO_SOT_Packages_SMD
SOT-665
SOT665
SOT-665
0
5
5
TO_SOT_Packages_SMD
SOT-666
SOT666
SOT-666
0
6
6
TO_SOT_Packages_SMD
SOT-723
http://toshiba.semicon-storage.com/info/docget.jsp?did=5879&prodName=RN1104MFV
sot 723
0
3
3
TO_SOT_Packages_SMD
SOT-883
SOT-883, https://assets.nexperia.com/documents/outline-drawing/SOT883.pdf
SOT-883
0
3
3
TO_SOT_Packages_SMD
SOT-886
SOT-886
SOT-886
0
6
6
TO_SOT_Packages_SMD
SOT-963
SOT 963 6 pins package 1x0.8mm pitch 0.35mm
SOT 963 6 pins package 1x0.8mm pitch 0.35mm
0
6
6
TO_SOT_Packages_SMD
SOT-1123
SOT-1123 small outline transistor (see http://www.onsemi.com/pub/Collateral/NST3906F3-D.PDF)
SOT-1123 transistor
0
3
3
TO_SOT_Packages_SMD
SOT-1333-1
SOT-1333-1 
SOT-1333-1 
0
9
9
TO_SOT_Packages_SMD
SOT-1334-1
SOT-1334-1
SOT-1334-1
0
14
14
TO_SOT_Packages_SMD
SuperSOT-3
3-pin SuperSOT package https://www.fairchildsemi.com/package-drawings/MA/MA03B.pdf
SuperSOT-3 SSOT-3
0
3
3
TO_SOT_Packages_SMD
SuperSOT-6
6-pin SuperSOT package http://www.mouser.com/ds/2/149/FMB5551-889214.pdf
SuperSOT-6 SSOT-6
0
6
6
TO_SOT_Packages_SMD
SuperSOT-8
8-pin SuperSOT package, http://www.icbank.com/icbank_data/semi_package/ssot8_dim.pdf
SuperSOT-8 SSOT-8
0
8
8
TO_SOT_Packages_SMD
TDSON-8-1
Power MOSFET package, TDSON-8-1, 5.15x5.9mm (https://www.infineon.com/cms/en/product/packages/PG-TDSON/PG-TDSON-8-1/)
tdson 
0
14
5
TO_SOT_Packages_SMD
TO-50-3_LongPad-NoHole_Housing
TO-50-3 Macro T Package Style M236
TO-50-3 Macro T Package Style M236
0
3
3
TO_SOT_Packages_SMD
TO-50-3_LongPad-WithHole_Housing
TO-50-3 Macro T Package Style M236
TO-50-3 Macro T Package Style M236
0
3
3
TO_SOT_Packages_SMD
TO-50-3_ShortPad-NoHole_Housing
TO-50-3 Macro T Package Style M236
TO-50-3 Macro T Package Style M236
0
3
3
TO_SOT_Packages_SMD
TO-50-3_ShortPad-WithHole_Housing
TO-50-3 Macro T Package Style M236
TO-50-3 Macro T Package Style M236
0
3
3
TO_SOT_Packages_SMD
TO-50-4_LongPad-NoHole_Housing
TO-50-4 Macro X Package Style M238
TO-50-4 Macro X Package Style M238
0
4
4
TO_SOT_Packages_SMD
TO-50-4_LongPad-WithHole_Housing
TO-50-4 Macro X Package Style M238
TO-50-4 Macro X Package Style M238
0
4
4
TO_SOT_Packages_SMD
TO-50-4_ShortPad-NoHole_Housing
TO-50-4 Macro X Package Style M238
TO-50-4 Macro X Package Style M238
0
4
4
TO_SOT_Packages_SMD
TO-50-4_ShortPad-WithHole_Housing
TO-50-4 Macro X Package Style M238
TO-50-4 Macro X Package Style M238
0
4
4
TO_SOT_Packages_SMD
TO-252-2
TO-252 / DPAK SMD package, http://www.infineon.com/cms/en/product/packages/PG-TO252/PG-TO252-3-1/
DPAK TO-252 DPAK-3 TO-252-3 SOT-428
0
7
3
TO_SOT_Packages_SMD
TO-252-2_TabPin1
TO-252-2, tab to pin 1 https://www.wolfspeed.com/media/downloads/87/CSD01060.pdf
TO-252-2 diode
0
7
2
TO_SOT_Packages_SMD
TO-252-3_TabPin2
TO-252 / DPAK SMD package, http://www.infineon.com/cms/en/product/packages/PG-TO252/PG-TO252-3-1/
DPAK TO-252 DPAK-3 TO-252-3 SOT-428
0
8
3
TO_SOT_Packages_SMD
TO-252-3_TabPin4
TO-252 / DPAK SMD package, http://www.infineon.com/cms/en/product/packages/PG-TO252/PG-TO252-3-1/
DPAK TO-252 DPAK-3 TO-252-3 SOT-428
0
8
4
TO_SOT_Packages_SMD
TO-252-4
TO-252 / DPAK SMD package, http://www.infineon.com/cms/en/product/packages/PG-TO252/PG-TO252-5-11/
DPAK TO-252 DPAK-5 TO-252-5
0
9
5
TO_SOT_Packages_SMD
TO-252-5_TabPin3
TO-252 / DPAK SMD package, http://www.infineon.com/cms/en/product/packages/PG-TO252/PG-TO252-5-11/
DPAK TO-252 DPAK-5 TO-252-5
0
10
5
TO_SOT_Packages_SMD
TO-252-5_TabPin6
TO-252 / DPAK SMD package, http://www.infineon.com/cms/en/product/packages/PG-TO252/PG-TO252-5-11/
DPAK TO-252 DPAK-5 TO-252-5
0
10
6
TO_SOT_Packages_SMD
TO-263-2
TO-263 / D2PAK / DDPAK SMD package, http://www.infineon.com/cms/en/product/packages/PG-TO263/PG-TO263-3-1/
D2PAK DDPAK TO-263 D2PAK-3 TO-263-3 SOT-404
0
7
3
TO_SOT_Packages_SMD
TO-263-2_TabPin1
TO-263 / D2PAK / DDPAK SMD package, tab to pin 1, https://www.wolfspeed.com/media/downloads/137/C3D06060G.pdf
D2PAK DDPAK TO-263 D2PAK-3 TO-263-3 SOT-404 diode
0
7
2
TO_SOT_Packages_SMD
TO-263-3_TabPin2
TO-263 / D2PAK / DDPAK SMD package, http://www.infineon.com/cms/en/product/packages/PG-TO263/PG-TO263-3-1/
D2PAK DDPAK TO-263 D2PAK-3 TO-263-3 SOT-404
0
8
3
TO_SOT_Packages_SMD
TO-263-3_TabPin4
TO-263 / D2PAK / DDPAK SMD package, http://www.infineon.com/cms/en/product/packages/PG-TO263/PG-TO263-3-1/
D2PAK DDPAK TO-263 D2PAK-3 TO-263-3 SOT-404
0
8
4
TO_SOT_Packages_SMD
TO-263-4
TO-263 / D2PAK / DDPAK SMD package, http://www.infineon.com/cms/en/product/packages/PG-TO263/PG-TO263-5-1/
D2PAK DDPAK TO-263 D2PAK-5 TO-263-5 SOT-426
0
9
5
TO_SOT_Packages_SMD
TO-263-5_TabPin3
TO-263 / D2PAK / DDPAK SMD package, http://www.infineon.com/cms/en/product/packages/PG-TO263/PG-TO263-5-1/
D2PAK DDPAK TO-263 D2PAK-5 TO-263-5 SOT-426
0
10
5
TO_SOT_Packages_SMD
TO-263-5_TabPin6
TO-263 / D2PAK / DDPAK SMD package, http://www.infineon.com/cms/en/product/packages/PG-TO263/PG-TO263-5-1/
D2PAK DDPAK TO-263 D2PAK-5 TO-263-5 SOT-426
0
10
6
TO_SOT_Packages_SMD
TO-263-6
TO-263 / D2PAK / DDPAK SMD package, http://www.infineon.com/cms/en/product/packages/PG-TO263/PG-TO263-7-1/
D2PAK DDPAK TO-263 D2PAK-7 TO-263-7 SOT-427
0
11
7
TO_SOT_Packages_SMD
TO-263-7_TabPin4
TO-263 / D2PAK / DDPAK SMD package, http://www.infineon.com/cms/en/product/packages/PG-TO263/PG-TO263-7-1/
D2PAK DDPAK TO-263 D2PAK-7 TO-263-7 SOT-427
0
12
7
TO_SOT_Packages_SMD
TO-263-7_TabPin8
TO-263 / D2PAK / DDPAK SMD package, http://www.infineon.com/cms/en/product/packages/PG-TO263/PG-TO263-7-1/
D2PAK DDPAK TO-263 D2PAK-7 TO-263-7 SOT-427
0
12
8
TO_SOT_Packages_SMD
TO-263-9_TabPin5
TO-263 / D2PAK / DDPAK SMD package, http://www.ti.com/lit/ds/symlink/lm4755.pdf
D2PAK DDPAK TO-263 D2PAK-9 TO-263-9
0
14
9
TO_SOT_Packages_SMD
TO-263-9_TabPin10
TO-263 / D2PAK / DDPAK SMD package, http://www.ti.com/lit/ds/symlink/lm4755.pdf
D2PAK DDPAK TO-263 D2PAK-9 TO-263-9
0
14
10
TO_SOT_Packages_SMD
TO-268-2
TO-268/D3PAK SMD package, http://www.icbank.com/icbank_data/semi_package/to268aa_dim.pdf
D3PAK TO-268 D3PAK-3 TO-268-3
0
7
3
TO_SOT_Packages_SMD
TO-269AA
SMD package TO-269AA (e.g. diode bridge), see http://www.vishay.com/docs/88854/padlayouts.pdf
TO-269AA MBS diode bridge
0
4
4
TO_SOT_Packages_SMD
TO-277A
Thermal enhanced ultra thin SMD package; 3 leads; body: 4.3x6.1x0.43mm, https://www.vishay.com/docs/95570/to-277asmpc.pdf
TO-277A SMPC
0
12
3
TO_SOT_Packages_SMD
TO-277B
TO-227B https://media.digikey.com/pdf/Data%20Sheets/Littelfuse%20PDFs/DST2050S.pdf
TO-277B
0
9
3
TO_SOT_Packages_SMD
TSOT-23
3-pin TSOT23 package, http://www.analog.com.tw/pdf/All_In_One.pdf
TSOT-23
0
3
3
TO_SOT_Packages_SMD
TSOT-23-5
5-pin TSOT23 package, http://cds.linear.com/docs/en/packaging/SOT_5_05-08-1635.pdf
TSOT-23-5
0
5
5
TO_SOT_Packages_SMD
TSOT-23-5_HandSoldering
5-pin TSOT23 package, http://cds.linear.com/docs/en/packaging/SOT_5_05-08-1635.pdf
TSOT-23-5 Hand-soldering
0
5
5
TO_SOT_Packages_SMD
TSOT-23-6
6-pin TSOT23 package, http://cds.linear.com/docs/en/packaging/SOT_6_05-08-1636.pdf
TSOT-23-6 MK06A TSOT-6
0
6
6
TO_SOT_Packages_SMD
TSOT-23-6_HandSoldering
6-pin TSOT23 package, http://cds.linear.com/docs/en/packaging/SOT_6_05-08-1636.pdf
TSOT-23-6 MK06A TSOT-6 Hand-soldering
0
6
6
TO_SOT_Packages_SMD
TSOT-23-8
8-pin TSOT23 package, http://cds.linear.com/docs/en/packaging/SOT_8_05-08-1637.pdf
TSOT-23-8
0
8
8
TO_SOT_Packages_SMD
TSOT-23-8_HandSoldering
8-pin TSOT23 package, http://cds.linear.com/docs/en/packaging/SOT_8_05-08-1637.pdf
TSOT-23-8 Hand-soldering
0
8
8
TO_SOT_Packages_SMD
TSOT-23_HandSoldering
5-pin TSOT23 package, http://cds.linear.com/docs/en/packaging/SOT_5_05-08-1635.pdf
TSOT-23 Hand-soldering
0
3
3
TO_SOT_Packages_SMD
Texas_DRT-3
Texas Instrument DRT-3 1x0.8mm Pitch 0.7mm http://www.ti.com/lit/ds/symlink/tpd2eusb30.pdf
DRT-3 1x0.8mm Pitch 0.7mm
0
3
3
TO_SOT_Packages_SMD
Texas_NDY0011A
TO-PMOD-11 11-pin switching regulator package, http://www.ti.com/lit/ml/mmsf025/mmsf025.pdf
Texas TO-PMOD NDY00011A
0
12
12
TO_SOT_Packages_SMD
Texas_R-PDSO-G6
R-PDSO-G6, http://www.ti.com/lit/ds/slis144b/slis144b.pdf
R-PDSO-G6 SC-70-6
0
6
6
TO_SOT_Packages_SMD
VSOF5
VSOF5
VSOF5
0
5
5
TO_SOT_Packages_SMD
Vishay_PowerPAK_SC70-6L_Dual
Vishay PowerPAK SC70 dual transistor package http://www.vishay.com/docs/70487/70487.pdf
powerpak sc70 sc-70 dual
0
8
6
TO_SOT_Packages_SMD
Vishay_PowerPAK_SC70-6L_Single
Vishay PowerPAK SC70 single transistor package http://www.vishay.com/docs/70486/70486.pdf
powerpak sc70 sc-70
0
6
3
TO_SOT_Packages_THT
Fairchild_TO-220F-6L
Fairchild TO-220F-6L, http://www.mouser.com/ds/2/149/FSL136MRT-113334.pdf
Fairchild TO-220F-6L
0
6
6
TO_SOT_Packages_THT
Heraeus_TO-92-2
TO-92 2-pin variant by Heraeus, drill 0.75mm (http://www.produktinfo.conrad.com/datenblaetter/175000-199999/181293-da-01-de-TO92_Temperatursensor_PT1000_32209225.pdf)
to-92 
0
2
2
TO_SOT_Packages_THT
NEC_Molded_7x4x9mm
Molded Japan Transistor Package 7x4x9mm^3, http://rtellason.com/transdata/2sb734.pdf
Japan transistor
0
3
3
TO_SOT_Packages_THT
PowerIntegrations_TO-220-7C
Non Isolated Modified TO-220 7pin Package, see http://www.farnell.com/datasheets/5793.pdf
Power Integration Y Package
0
6
6
TO_SOT_Packages_THT
SIPAK-1EP_Horizontal_TabDown
SIPAK, Horizontal, RM 2.286mm
SIPAK Horizontal RM 2.286mm
0
4
4
TO_SOT_Packages_THT
SIPAK_Vertical
SIPAK, Vertical, RM 2.286mm
SIPAK Vertical RM 2.286mm
0
3
3
TO_SOT_Packages_THT
SOD-70_P2.54mm
Plastic near cylindrical package Sod-70 see: https://www.nxp.com/docs/en/data-sheet/KTY81_SER.pdf  [StepUp generated footprint]
Sod-70
0
2
2
TO_SOT_Packages_THT
SOD-70_P5.08mm
Plastic near cylindrical package Sod-70 see: https://www.nxp.com/docs/en/data-sheet/KTY81_SER.pdf  [StepUp generated footprint]
Sod-70
0
2
2
TO_SOT_Packages_THT
SOT-227
SOT-227 / SOT-227B / ISOTOP, M4 mounting screws (https://www.vishay.com/docs/95423/sot227g2.pdf, https://www.vishay.com/docs/95793/vs-fc420sa10.pdf)
sot 227 isotop
0
8
4
TO_SOT_Packages_THT
TO-3
Transistor TO-3
TR TO-3 TO3 TO-204
0
4
3
TO_SOT_Packages_THT
TO-3P-3_Horizontal_TabDown
TO-3P-3, Horizontal, RM 5.45mm, , see https://toshiba.semicon-storage.com/ap-en/design-support/package/detail.TO-3P(N).html
TO-3P-3 Horizontal RM 5.45mm 
0
3
3
TO_SOT_Packages_THT
TO-3P-3_Horizontal_TabUp
TO-3P-3, Horizontal, RM 5.45mm, , see https://toshiba.semicon-storage.com/ap-en/design-support/package/detail.TO-3P(N).html
TO-3P-3 Horizontal RM 5.45mm 
0
3
3
TO_SOT_Packages_THT
TO-3P-3_Vertical
TO-3P-3, Vertical, RM 5.45mm, , see https://toshiba.semicon-storage.com/ap-en/design-support/package/detail.TO-3P(N).html
TO-3P-3 Vertical RM 5.45mm 
0
3
3
TO_SOT_Packages_THT
TO-3PB-3_Horizontal_TabDown
TO-3PB-3, Horizontal, RM 5.45mm, , see http://www.onsemi.com/pub/Collateral/340AC.PDF
TO-3PB-3 Horizontal RM 5.45mm 
0
3
3
TO_SOT_Packages_THT
TO-3PB-3_Horizontal_TabUp
TO-3PB-3, Horizontal, RM 5.45mm, , see http://www.onsemi.com/pub/Collateral/340AC.PDF
TO-3PB-3 Horizontal RM 5.45mm 
0
3
3
TO_SOT_Packages_THT
TO-3PB-3_Vertical
TO-3PB-3, Vertical, RM 5.45mm, , see http://www.onsemi.com/pub/Collateral/340AC.PDF
TO-3PB-3 Vertical RM 5.45mm 
0
3
3
TO_SOT_Packages_THT
TO-5-2
TO-5-2
TO-5-2
0
2
2
TO_SOT_Packages_THT
TO-5-2_Window
TO-5-2_Window, Window
TO-5-2_Window Window
0
2
2
TO_SOT_Packages_THT
TO-5-3
TO-5-3
TO-5-3
0
3
3
TO_SOT_Packages_THT
TO-5-3_Window
TO-5-3_Window, Window
TO-5-3_Window Window
0
3
3
TO_SOT_Packages_THT
TO-5-4
TO-5-4
TO-5-4
0
4
4
TO_SOT_Packages_THT
TO-5-4_Window
TO-5-4_Window, Window
TO-5-4_Window Window
0
4
4
TO_SOT_Packages_THT
TO-5-6
TO-5-6
TO-5-6
0
6
6
TO_SOT_Packages_THT
TO-5-6_Window
TO-5-6_Window, Window
TO-5-6_Window Window
0
6
6
TO_SOT_Packages_THT
TO-5-8
TO-5-8
TO-5-8
0
8
8
TO_SOT_Packages_THT
TO-5-8_PD5.08
TO-5-8_PD5.08
TO-5-8_PD5.08
0
8
8
TO_SOT_Packages_THT
TO-5-8_PD5.08_Window
TO-5-8_PD5.08_Window, Window
TO-5-8_PD5.08_Window Window
0
8
8
TO_SOT_Packages_THT
TO-5-8_Window
TO-5-8_Window, Window
TO-5-8_Window Window
0
8
8
TO_SOT_Packages_THT
TO-5-10
TO-5-10
TO-5-10
0
10
10
TO_SOT_Packages_THT
TO-5-10_Window
TO-5-10_Window, Window
TO-5-10_Window Window
0
10
10
TO_SOT_Packages_THT
TO-8-2
TO-8-2
TO-8-2
0
2
2
TO_SOT_Packages_THT
TO-8-2_Window
TO-8-2_Window, Window
TO-8-2_Window Window
0
2
2
TO_SOT_Packages_THT
TO-8-3
TO-8-3
TO-8-3
0
3
3
TO_SOT_Packages_THT
TO-8-3_Window
TO-8-3_Window, Window
TO-8-3_Window Window
0
3
3
TO_SOT_Packages_THT
TO-11-2
TO-11-2
TO-11-2
0
2
2
TO_SOT_Packages_THT
TO-11-2_Window
TO-11-2_Window, Window
TO-11-2_Window Window
0
2
2
TO_SOT_Packages_THT
TO-11-3
TO-11-3
TO-11-3
0
3
3
TO_SOT_Packages_THT
TO-11-3_Window
TO-11-3_Window, Window
TO-11-3_Window Window
0
3
3
TO_SOT_Packages_THT
TO-12-4
TO-12-4
TO-12-4
0
4
4
TO_SOT_Packages_THT
TO-12-4_Window
TO-12-4_Window, Window
TO-12-4_Window Window
0
4
4
TO_SOT_Packages_THT
TO-17-4
TO-17-4
TO-17-4
0
4
4
TO_SOT_Packages_THT
TO-17-4_Window
TO-17-4_Window, Window
TO-17-4_Window Window
0
4
4
TO_SOT_Packages_THT
TO-18-2
TO-18-2
TO-18-2
0
2
2
TO_SOT_Packages_THT
TO-18-2_Lens
TO-18-2_Lens, Lens
TO-18-2_Lens Lens
0
2
2
TO_SOT_Packages_THT
TO-18-2_Window
TO-18-2_Window, Window
TO-18-2_Window Window
0
2
2
TO_SOT_Packages_THT
TO-18-3
TO-18-3
TO-18-3
0
3
3
TO_SOT_Packages_THT
TO-18-3_Lens
TO-18-3_Lens, Lens
TO-18-3_Lens Lens
0
3
3
TO_SOT_Packages_THT
TO-18-3_Window
TO-18-3_Window, Window
TO-18-3_Window Window
0
3
3
TO_SOT_Packages_THT
TO-18-4
TO-18-4
TO-18-4
0
4
4
TO_SOT_Packages_THT
TO-18-4_Lens
TO-18-4_Lens, Lens
TO-18-4_Lens Lens
0
4
4
TO_SOT_Packages_THT
TO-18-4_Window
TO-18-4_Window, Window
TO-18-4_Window Window
0
4
4
TO_SOT_Packages_THT
TO-33-4
TO-33-4
TO-33-4
0
4
4
TO_SOT_Packages_THT
TO-33-4_Window
TO-33-4_Window, Window
TO-33-4_Window Window
0
4
4
TO_SOT_Packages_THT
TO-38-2
TO-38-2
TO-38-2
0
2
2
TO_SOT_Packages_THT
TO-38-2_Window
TO-38-2_Window, Window
TO-38-2_Window Window
0
2
2
TO_SOT_Packages_THT
TO-38-3
TO-38-3
TO-38-3
0
3
3
TO_SOT_Packages_THT
TO-38-3_Window
TO-38-3_Window, Window
TO-38-3_Window Window
0
3
3
TO_SOT_Packages_THT
TO-39-2
TO-39-2
TO-39-2
0
2
2
TO_SOT_Packages_THT
TO-39-2_Window
TO-39-2_Window, Window
TO-39-2_Window Window
0
2
2
TO_SOT_Packages_THT
TO-39-3
TO-39-3
TO-39-3
0
3
3
TO_SOT_Packages_THT
TO-39-3_Window
TO-39-3_Window, Window
TO-39-3_Window Window
0
3
3
TO_SOT_Packages_THT
TO-39-4
TO-39-4
TO-39-4
0
4
4
TO_SOT_Packages_THT
TO-39-4_Window
TO-39-4_Window, Window
TO-39-4_Window Window
0
4
4
TO_SOT_Packages_THT
TO-39-6
TO-39-6
TO-39-6
0
6
6
TO_SOT_Packages_THT
TO-39-6_Window
TO-39-6_Window, Window
TO-39-6_Window Window
0
6
6
TO_SOT_Packages_THT
TO-39-8
TO-39-8
TO-39-8
0
8
8
TO_SOT_Packages_THT
TO-39-8_Window
TO-39-8_Window, Window
TO-39-8_Window Window
0
8
8
TO_SOT_Packages_THT
TO-39-10
TO-39-10
TO-39-10
0
10
10
TO_SOT_Packages_THT
TO-39-10_Window
TO-39-10_Window, Window
TO-39-10_Window Window
0
10
10
TO_SOT_Packages_THT
TO-46-2
TO-46-2
TO-46-2
0
2
2
TO_SOT_Packages_THT
TO-46-2_Pin2Center
TO-46-2, Pin2 at center of package, Thorlabs photodiodes
TO-46-2 Thorlabs
0
2
2
TO_SOT_Packages_THT
TO-46-2_Pin2Center_Window
TO-46-2, Pin2 at center of package, Thorlabs photodiodes
TO-46-2 Thorlabs
0
2
2
TO_SOT_Packages_THT
TO-46-2_Window
TO-46-2_Window, Window
TO-46-2_Window Window
0
2
2
TO_SOT_Packages_THT
TO-46-3
TO-46-3
TO-46-3
0
3
3
TO_SOT_Packages_THT
TO-46-3_Pin2Center
TO-46-3, Pin2 at center of package, Thorlabs photodiodes, https://www.thorlabs.de/drawings/374b6862eb3b5a04-9360B5F6-5056-2306-D912111C06C3F830/FDGA05-SpecSheet.pdf
TO-46-3 Thorlabs
0
3
3
TO_SOT_Packages_THT
TO-46-3_Pin2Center_Window
TO-46-3, Pin2 at center of package, Thorlabs photodiodes, https://www.thorlabs.de/drawings/374b6862eb3b5a04-9360B5F6-5056-2306-D912111C06C3F830/FDGA05-SpecSheet.pdf
TO-46-3 Thorlabs
0
3
3
TO_SOT_Packages_THT
TO-46-3_Window
TO-46-3_Window, Window
TO-46-3_Window Window
0
3
3
TO_SOT_Packages_THT
TO-46-4
TO-46-4
TO-46-4
0
4
4
TO_SOT_Packages_THT
TO-46-4_Window
TO-46-4_Window, Window
TO-46-4_Window Window
0
4
4
TO_SOT_Packages_THT
TO-52-2
TO-52-2
TO-52-2
0
2
2
TO_SOT_Packages_THT
TO-52-2_Window
TO-52-2_Window, Window
TO-52-2_Window Window
0
2
2
TO_SOT_Packages_THT
TO-52-3
TO-52-3
TO-52-3
0
3
3
TO_SOT_Packages_THT
TO-52-3_Window
TO-52-3_Window, Window
TO-52-3_Window Window
0
3
3
TO_SOT_Packages_THT
TO-72-4
TO-72-4
TO-72-4
0
4
4
TO_SOT_Packages_THT
TO-72-4_Window
TO-72-4_Window, Window
TO-72-4_Window Window
0
4
4
TO_SOT_Packages_THT
TO-75-6
TO-75-6
TO-75-6
0
6
6
TO_SOT_Packages_THT
TO-75-6_Window
TO-75-6_Window, Window
TO-75-6_Window Window
0
6
6
TO_SOT_Packages_THT
TO-78-6
TO-78-6
TO-78-6
0
6
6
TO_SOT_Packages_THT
TO-78-6_Window
TO-78-6_Window, Window
TO-78-6_Window Window
0
6
6
TO_SOT_Packages_THT
TO-78-8
TO-78-8
TO-78-8
0
8
8
TO_SOT_Packages_THT
TO-78-8_Window
TO-78-8_Window, Window
TO-78-8_Window Window
0
8
8
TO_SOT_Packages_THT
TO-78-10
TO-78-10
TO-78-10
0
10
10
TO_SOT_Packages_THT
TO-78-10_Window
TO-78-10_Window, Window
TO-78-10_Window Window
0
10
10
TO_SOT_Packages_THT
TO-92
TO-92 leads molded, narrow, drill 0.75mm (see NXP sot054_po.pdf)
to-92 sc-43 sc-43a sot54 PA33 transistor
0
3
3
TO_SOT_Packages_THT
TO-92-2
TO-92 2-pin leads in-line, narrow, oval pads, drill 0.75mm (see NXP sot054_po.pdf)
to-92 sc-43 sc-43a sot54 PA33 diode SOD70
0
2
2
TO_SOT_Packages_THT
TO-92-2_Horizontal1
2-pin TO-92 horizontal, leads molded, narrow, drill 0.75mm (see NXP sot054_po.pdf)
to-92 sc-43 sc-43a sot54 PA33 temperature sensor diode
0
2
2
TO_SOT_Packages_THT
TO-92-2_Horizontal2
2-pin TO-92 horizontal, leads molded, narrow, drill 0.75mm (see NXP sot054_po.pdf)
to-92 sc-43 sc-43a sot54 PA33 temperature sensor diode
0
2
2
TO_SOT_Packages_THT
TO-92-2_W4.0mm_Horizontal_FlatSideDown
TO-92 horizontal, leads in-line, narrow, oval pads, drill 0.75mm (see NXP sot054_po.pdf)
to-92 sc-43 sc-43a sot54 PA33 transistor
0
2
2
TO_SOT_Packages_THT
TO-92-2_W4.0mm_Horizontal_FlatSideUp
TO-92 horizontal, leads in-line, narrow, oval pads, drill 0.75mm (see NXP sot054_po.pdf)
to-92 sc-43 sc-43a sot54 PA33 transistor
0
2
2
TO_SOT_Packages_THT
TO-92-2_Wide
TO-92 2-pin leads in-line, wide, drill 0.75mm
to-92 sc-43 sc-43a sot54 PA33 diode SOD70
0
2
2
TO_SOT_Packages_THT
TO-92Flat
TO-92Flat package, often used for hall sensors, drill 0.75mm (see e.g. http://www.ti.com/lit/ds/symlink/drv5023.pdf)
to-92Flat hall sensor
0
3
3
TO_SOT_Packages_THT
TO-92L
TO-92L leads in-line (large body variant of TO-92), also known as TO-226, wide, drill 0.75mm (see https://www.diodes.com/assets/Package-Files/TO92L.pdf and http://www.ti.com/lit/an/snoa059/snoa059.pdf)
TO-92L Molded Narrow transistor
0
3
3
TO_SOT_Packages_THT
TO-92L_HandSolder
TO-92L leads in-line (large body variant of TO-92), also known as TO-226, wide, drill 0.75mm, hand-soldering variant with enlarged pads (see https://www.diodes.com/assets/Package-Files/TO92L.pdf and http://www.ti.com/lit/an/snoa059/snoa059.pdf)
to-92 sc-43 sc-43a sot54 PA33 transistor
0
3
3
TO_SOT_Packages_THT
TO-92L_Inline
TO-92L leads in-line (large body variant of TO-92), also known as TO-226, wide, drill 0.75mm (see https://www.diodes.com/assets/Package-Files/TO92L.pdf and http://www.ti.com/lit/an/snoa059/snoa059.pdf)
TO-92L Inline Wide transistor
0
3
3
TO_SOT_Packages_THT
TO-92L_Inline_Wide
TO-92L leads in-line (large body variant of TO-92), also known as TO-226, wide, drill 0.75mm (see https://www.diodes.com/assets/Package-Files/TO92L.pdf and http://www.ti.com/lit/an/snoa059/snoa059.pdf)
TO-92L Inline Wide transistor
0
3
3
TO_SOT_Packages_THT
TO-92L_Wide
TO-92L leads in-line (large body variant of TO-92), also known as TO-226, wide, drill 0.75mm (see https://www.diodes.com/assets/Package-Files/TO92L.pdf and http://www.ti.com/lit/an/snoa059/snoa059.pdf)
TO-92L Molded Wide transistor
0
3
3
TO_SOT_Packages_THT
TO-92Mini-2
TO-92Mini package, drill 0.6mm (https://media.digikey.com/pdf/Data%20Sheets/Infineon%20PDFs/KT,KTY.pdf)
to-92Mini transistor 
0
2
2
TO_SOT_Packages_THT
TO-92S
TO-92S package, drill 0.75mm (https://www.diodes.com/assets/Package-Files/TO92S%20(Type%20B).pdf)
to-92S transistor
0
3
3
TO_SOT_Packages_THT
TO-92S-2
TO-92S package, 2-pin, drill 0.75mm (https://www.diodes.com/assets/Package-Files/TO92S%20(Type%20B).pdf)
to-92S transistor
0
2
2
TO_SOT_Packages_THT
TO-92S_Wide
TO-92S_Wide package, drill 0.75mm (https://www.diodes.com/assets/Package-Files/TO92S%20(Type%20B).pdf)
TO-92S_Wide transistor
0
3
3
TO_SOT_Packages_THT
TO-92_HandSolder
TO-92 leads molded, narrow, drill 0.75mm, handsoldering variant with enlarged pads (see NXP sot054_po.pdf)
to-92 sc-43 sc-43a sot54 PA33 transistor
0
3
3
TO_SOT_Packages_THT
TO-92_Horizontal1
TO-92 horizontal, leads molded, narrow, drill 0.75mm (see NXP sot054_po.pdf)
to-92 sc-43 sc-43a sot54 PA33 transistor
0
3
3
TO_SOT_Packages_THT
TO-92_Horizontal2
TO-92 horizontal, leads molded, narrow, drill 0.75mm (see NXP sot054_po.pdf)
to-92 sc-43 sc-43a sot54 PA33 transistor
0
3
3
TO_SOT_Packages_THT
TO-92_Inline
TO-92 leads in-line, narrow, oval pads, drill 0.75mm (see NXP sot054_po.pdf)
to-92 sc-43 sc-43a sot54 PA33 transistor
0
3
3
TO_SOT_Packages_THT
TO-92_Inline_Horizontal1
TO-92 horizontal, leads in-line, narrow, oval pads, drill 0.75mm (see NXP sot054_po.pdf)
to-92 sc-43 sc-43a sot54 PA33 transistor
0
3
3
TO_SOT_Packages_THT
TO-92_Inline_Horizontal2
TO-92 horizontal, leads in-line, narrow, oval pads, drill 0.75mm (see NXP sot054_po.pdf)
to-92 sc-43 sc-43a sot54 PA33 transistor
0
3
3
TO_SOT_Packages_THT
TO-92_Inline_W4.0mm_Horizontal_FlatSideDown
TO-92 horizontal, leads in-line, narrow, oval pads, drill 0.75mm (see NXP sot054_po.pdf)
to-92 sc-43 sc-43a sot54 PA33 transistor
0
3
3
TO_SOT_Packages_THT
TO-92_Inline_W4.0mm_Horizontal_FlatSideUp
TO-92 horizontal, leads in-line, narrow, oval pads, drill 0.75mm (see NXP sot054_po.pdf)
to-92 sc-43 sc-43a sot54 PA33 transistor
0
3
3
TO_SOT_Packages_THT
TO-92_Inline_Wide
TO-92 leads in-line, wide, drill 0.75mm (see NXP sot054_po.pdf)
to-92 sc-43 sc-43a sot54 PA33 transistor
0
3
3
TO_SOT_Packages_THT
TO-92_W4.0mm_StaggerEven_Horizontal_FlatSideDown
TO-92 horizontal, leads molded, narrow, drill 0.75mm (see NXP sot054_po.pdf)
to-92 sc-43 sc-43a sot54 PA33 transistor
0
3
3
TO_SOT_Packages_THT
TO-92_W4.0mm_StaggerEven_Horizontal_FlatSideUp
TO-92 horizontal, leads molded, narrow, drill 0.75mm (see NXP sot054_po.pdf)
to-92 sc-43 sc-43a sot54 PA33 transistor
0
3
3
TO_SOT_Packages_THT
TO-92_Wide
TO-92 leads molded, wide, drill 0.75mm (see NXP sot054_po.pdf)
to-92 sc-43 sc-43a sot54 PA33 transistor
0
3
3
TO_SOT_Packages_THT
TO-99-6
TO-99-6
TO-99-6
0
6
6
TO_SOT_Packages_THT
TO-99-6_Window
TO-99-6_Window, Window
TO-99-6_Window Window
0
6
6
TO_SOT_Packages_THT
TO-99-8
TO-99-8
TO-99-8
0
8
8
TO_SOT_Packages_THT
TO-99-8_Window
TO-99-8_Window, Window
TO-99-8_Window Window
0
8
8
TO_SOT_Packages_THT
TO-100-10
TO-100-10
TO-100-10
0
10
10
TO_SOT_Packages_THT
TO-100-10_Window
TO-100-10_Window, Window
TO-100-10_Window Window
0
10
10
TO_SOT_Packages_THT
TO-126-2_Horizontal_TabDown
TO-126-2, Horizontal, RM 5.08mm, see https://www.diodes.com/assets/Package-Files/TO126.pdf
TO-126-2 Horizontal RM 5.08mm
0
2
2
TO_SOT_Packages_THT
TO-126-2_Horizontal_TabUp
TO-126-2, Horizontal, RM 5.08mm, see https://www.diodes.com/assets/Package-Files/TO126.pdf
TO-126-2 Horizontal RM 5.08mm
0
2
2
TO_SOT_Packages_THT
TO-126-2_Vertical
TO-126-2, Vertical, RM 5.08mm, see https://www.diodes.com/assets/Package-Files/TO126.pdf
TO-126-2 Vertical RM 5.08mm
0
2
2
TO_SOT_Packages_THT
TO-126-3_Horizontal_TabDown
TO-126-3, Horizontal, RM 2.54mm, see https://www.diodes.com/assets/Package-Files/TO126.pdf
TO-126-3 Horizontal RM 2.54mm
0
3
3
TO_SOT_Packages_THT
TO-126-3_Horizontal_TabUp
TO-126-3, Horizontal, RM 2.54mm, see https://www.diodes.com/assets/Package-Files/TO126.pdf
TO-126-3 Horizontal RM 2.54mm
0
3
3
TO_SOT_Packages_THT
TO-126-3_Vertical
TO-126-3, Vertical, RM 2.54mm, see https://www.diodes.com/assets/Package-Files/TO126.pdf
TO-126-3 Vertical RM 2.54mm
0
3
3
TO_SOT_Packages_THT
TO-218-2_Horizontal_TabDown
TO-218-2, Horizontal, RM 10.95mm, SOT-93, see https://www.vishay.com/docs/95214/fto218.pdf
TO-218-2 Horizontal RM 10.95mm SOT-93
0
2
2
TO_SOT_Packages_THT
TO-218-2_Horizontal_TabUp
TO-218-2, Horizontal, RM 10.95mm, SOT-93, see https://www.vishay.com/docs/95214/fto218.pdf
TO-218-2 Horizontal RM 10.95mm SOT-93
0
2
2
TO_SOT_Packages_THT
TO-218-2_Vertical
TO-218-2, Vertical, RM 10.95mm, SOT-93, see https://www.vishay.com/docs/95214/fto218.pdf
TO-218-2 Vertical RM 10.95mm SOT-93
0
2
2
TO_SOT_Packages_THT
TO-218-3_Horizontal_TabDown
TO-218-3, Horizontal, RM 5.475mm, SOT-93, see https://www.vishay.com/docs/95214/fto218.pdf
TO-218-3 Horizontal RM 5.475mm SOT-93
0
3
3
TO_SOT_Packages_THT
TO-218-3_Horizontal_TabUp
TO-218-3, Horizontal, RM 5.475mm, SOT-93, see https://www.vishay.com/docs/95214/fto218.pdf
TO-218-3 Horizontal RM 5.475mm SOT-93
0
3
3
TO_SOT_Packages_THT
TO-218-3_Vertical
TO-218-3, Vertical, RM 5.475mm, SOT-93, see https://www.vishay.com/docs/95214/fto218.pdf
TO-218-3 Vertical RM 5.475mm SOT-93
0
3
3
TO_SOT_Packages_THT
TO-220-2_Horizontal_TabDown
TO-220-2, Horizontal, RM 5.08mm, see https://www.centralsemi.com/PDFS/CASE/TO-220-2PD.PDF
TO-220-2 Horizontal RM 5.08mm
0
2
2
TO_SOT_Packages_THT
TO-220-2_Horizontal_TabUp
TO-220-2, Horizontal, RM 5.08mm, see https://www.centralsemi.com/PDFS/CASE/TO-220-2PD.PDF
TO-220-2 Horizontal RM 5.08mm
0
2
2
TO_SOT_Packages_THT
TO-220-2_Vertical
TO-220-2, Vertical, RM 5.08mm, see https://www.centralsemi.com/PDFS/CASE/TO-220-2PD.PDF
TO-220-2 Vertical RM 5.08mm
0
2
2
TO_SOT_Packages_THT
TO-220-3_Horizontal_TabDown
TO-220-3, Horizontal, RM 2.54mm, see https://www.vishay.com/docs/66542/to-220-1.pdf
TO-220-3 Horizontal RM 2.54mm
0
3
3
TO_SOT_Packages_THT
TO-220-3_Horizontal_TabUp
TO-220-3, Horizontal, RM 2.54mm, see https://www.vishay.com/docs/66542/to-220-1.pdf
TO-220-3 Horizontal RM 2.54mm
0
3
3
TO_SOT_Packages_THT
TO-220-3_Vertical
TO-220-3, Vertical, RM 2.54mm, see https://www.vishay.com/docs/66542/to-220-1.pdf
TO-220-3 Vertical RM 2.54mm
0
3
3
TO_SOT_Packages_THT
TO-220-4_Horizontal_TabDown
TO-220-4, Horizontal, RM 2.54mm
TO-220-4 Horizontal RM 2.54mm
0
4
4
TO_SOT_Packages_THT
TO-220-4_Horizontal_TabUp
TO-220-4, Horizontal, RM 2.54mm
TO-220-4 Horizontal RM 2.54mm
0
4
4
TO_SOT_Packages_THT
TO-220-4_P5.08x2.54mm_StaggerEven_Lead3.8mm_Vertical
TO-220-4, Vertical, RM 2.54mm, staggered type-2
TO-220-4 Vertical RM 2.54mm staggered type-2
0
4
4
TO_SOT_Packages_THT
TO-220-4_P5.08x2.54mm_StaggerEven_Lead5.84mm_TabDown
TO-220-4, Horizontal, RM 2.54mm, staggered type-2
TO-220-4 Horizontal RM 2.54mm staggered type-2
0
4
4
TO_SOT_Packages_THT
TO-220-4_P5.08x2.54mm_StaggerOdd_Lead3.8mm_Vertical
TO-220-4, Vertical, RM 2.54mm, staggered type-1
TO-220-4 Vertical RM 2.54mm staggered type-1
0
4
4
TO_SOT_Packages_THT
TO-220-4_P5.08x2.54mm_StaggerOdd_Lead5.84mm_TabDown
TO-220-4, Horizontal, RM 2.54mm, staggered type-1
TO-220-4 Horizontal RM 2.54mm staggered type-1
0
4
4
TO_SOT_Packages_THT
TO-220-4_Vertical
TO-220-4, Vertical, RM 2.54mm
TO-220-4 Vertical RM 2.54mm
0
4
4
TO_SOT_Packages_THT
TO-220-5_Horizontal_TabDown
TO-220-5, Horizontal, RM 1.7mm, Pentawatt, Multiwatt-5, see http://www.analog.com/media/en/package-pcb-resources/package/pkg_pdf/ltc-legacy-to-220/to-220_5_05-08-1421_straight_lead.pdf
TO-220-5 Horizontal RM 1.7mm Pentawatt Multiwatt-5
0
5
5
TO_SOT_Packages_THT
TO-220-5_Horizontal_TabUp
TO-220-5, Horizontal, RM 1.7mm, Pentawatt, Multiwatt-5, see http://www.analog.com/media/en/package-pcb-resources/package/pkg_pdf/ltc-legacy-to-220/to-220_5_05-08-1421_straight_lead.pdf
TO-220-5 Horizontal RM 1.7mm Pentawatt Multiwatt-5
0
5
5
TO_SOT_Packages_THT
TO-220-5_P3.4x3.7mm_StaggerEven_Lead3.8mm_Vertical
TO-220-5, Vertical, RM 1.7mm, Pentawatt, Multiwatt-5, staggered type-2, see http://www.analog.com/media/en/package-pcb-resources/package/pkg_pdf/ltc-legacy-to-220/to-220_5_05-08-1421.pdf?domain=www.linear.com, https://www.diodes.com/assets/Package-Files/TO220-5.pdf
TO-220-5 Vertical RM 1.7mm Pentawatt Multiwatt-5 staggered type-2
0
5
5
TO_SOT_Packages_THT
TO-220-5_P3.4x3.7mm_StaggerOdd_Lead3.8mm_Vertical
TO-220-5, Vertical, RM 1.7mm, Pentawatt, Multiwatt-5, staggered type-1, see http://www.analog.com/media/en/package-pcb-resources/package/pkg_pdf/ltc-legacy-to-220/to-220_5_05-08-1421.pdf?domain=www.linear.com, https://www.diodes.com/assets/Package-Files/TO220-5.pdf
TO-220-5 Vertical RM 1.7mm Pentawatt Multiwatt-5 staggered type-1
0
5
5
TO_SOT_Packages_THT
TO-220-5_P3.4x3.8mm_StaggerEven_Lead7.13mm_TabDown
TO-220-5, Horizontal, RM 1.7mm, Pentawatt, Multiwatt-5, staggered type-2, see http://www.analog.com/media/en/package-pcb-resources/package/pkg_pdf/ltc-legacy-to-220/to-220_5_05-08-1421.pdf?domain=www.linear.com, https://www.diodes.com/assets/Package-Files/TO220-5.pdf
TO-220-5 Horizontal RM 1.7mm Pentawatt Multiwatt-5 staggered type-2
0
5
5
TO_SOT_Packages_THT
TO-220-5_P3.4x3.8mm_StaggerOdd_Lead7.13mm_TabDown
TO-220-5, Horizontal, RM 1.7mm, Pentawatt, Multiwatt-5, staggered type-1, see http://www.analog.com/media/en/package-pcb-resources/package/pkg_pdf/ltc-legacy-to-220/to-220_5_05-08-1421.pdf?domain=www.linear.com, https://www.diodes.com/assets/Package-Files/TO220-5.pdf
TO-220-5 Horizontal RM 1.7mm Pentawatt Multiwatt-5 staggered type-1
0
5
5
TO_SOT_Packages_THT
TO-220-5_Vertical
TO-220-5, Vertical, RM 1.7mm, Pentawatt, Multiwatt-5, see http://www.analog.com/media/en/package-pcb-resources/package/pkg_pdf/ltc-legacy-to-220/to-220_5_05-08-1421_straight_lead.pdf
TO-220-5 Vertical RM 1.7mm Pentawatt Multiwatt-5
0
5
5
TO_SOT_Packages_THT
TO-220-7_P2.54x3.7mm_StaggerEven_Lead3.8mm_Vertical
TO-220-7, Vertical, RM 1.27mm, Multiwatt-7, staggered type-2
TO-220-7 Vertical RM 1.27mm Multiwatt-7 staggered type-2
0
7
7
TO_SOT_Packages_THT
TO-220-7_P2.54x3.7mm_StaggerOdd_Lead3.8mm_Vertical
TO-220-7, Vertical, RM 1.27mm, Multiwatt-7, staggered type-1
TO-220-7 Vertical RM 1.27mm Multiwatt-7 staggered type-1
0
7
7
TO_SOT_Packages_THT
TO-220-7_P2.54x3.8mm_StaggerEven_Lead5.85mm_TabDown
TO-220-7, Horizontal, RM 1.27mm, Multiwatt-7, staggered type-2
TO-220-7 Horizontal RM 1.27mm Multiwatt-7 staggered type-2
0
7
7
TO_SOT_Packages_THT
TO-220-7_P2.54x3.8mm_StaggerOdd_Lead5.85mm_TabDown
TO-220-7, Horizontal, RM 1.27mm, Multiwatt-7, staggered type-1
TO-220-7 Horizontal RM 1.27mm Multiwatt-7 staggered type-1
0
7
7
TO_SOT_Packages_THT
TO-220-8_Vertical
TO-220-8 (Multiwatt8), Vertical, 2.54mm Pitch (http://www.st.com/resource/en/datasheet/tda7264.pdf)
TO-220-9 Vertical 2.54mm Pitch Multiwatt 8
0
8
8
TO_SOT_Packages_THT
TO-220-9_P1.94x3.7mm_StaggerEven_Lead3.8mm_Vertical
TO-220-9, Vertical, RM 0.97mm, Multiwatt-9, staggered type-2
TO-220-9 Vertical RM 0.97mm Multiwatt-9 staggered type-2
0
9
9
TO_SOT_Packages_THT
TO-220-9_P1.94x3.7mm_StaggerOdd_Lead3.8mm_Vertical
TO-220-9, Vertical, RM 0.97mm, Multiwatt-9, staggered type-1
TO-220-9 Vertical RM 0.97mm Multiwatt-9 staggered type-1
0
9
9
TO_SOT_Packages_THT
TO-220-9_P1.94x3.8mm_StaggerEven_Lead5.85mm_TabDown
TO-220-9, Horizontal, RM 0.97mm, Multiwatt-9, staggered type-2
TO-220-9 Horizontal RM 0.97mm Multiwatt-9 staggered type-2
0
9
9
TO_SOT_Packages_THT
TO-220-9_P1.94x3.8mm_StaggerOdd_Lead5.85mm_TabDown
TO-220-9, Horizontal, RM 0.97mm, Multiwatt-9, staggered type-1
TO-220-9 Horizontal RM 0.97mm Multiwatt-9 staggered type-1
0
9
9
TO_SOT_Packages_THT
TO-220-11_P3.4x2.54mm_StaggerEven_Lead5.84mm_TabDown
TO-220-11, Horizontal, RM 1.7mm, staggered type-2, see http://www.st.com/resource/en/datasheet/tda7391lv.pdf
TO-220-11 Horizontal RM 1.7mm staggered type-2
0
11
11
TO_SOT_Packages_THT
TO-220-11_P3.4x2.54mm_StaggerOdd_Lead5.84mm_TabDown
TO-220-11, Horizontal, RM 1.7mm, staggered type-1, see http://www.st.com/resource/en/datasheet/tda7391lv.pdf
TO-220-11 Horizontal RM 1.7mm staggered type-1
0
11
11
TO_SOT_Packages_THT
TO-220-11_P3.4x5.08mm_StaggerEven_Lead4.58mm_Vertical
TO-220-11, Vertical, RM 1.7mm, staggered type-2, see http://www.st.com/resource/en/datasheet/tda7391lv.pdf
TO-220-11 Vertical RM 1.7mm staggered type-2
0
11
11
TO_SOT_Packages_THT
TO-220-11_P3.4x5.08mm_StaggerOdd_Lead4.85mm_Vertical
TO-220-11, Vertical, RM 1.7mm, staggered type-1, see http://www.st.com/resource/en/datasheet/tda7391lv.pdf
TO-220-11 Vertical RM 1.7mm staggered type-1
0
11
11
TO_SOT_Packages_THT
TO-220-11_P3.4x5.08mm_StaggerOdd_Lead8.45mm_TabDown
TO-220-11, Horizontal, RM 1.7mm, staggered type-1, see http://www.ti.com/lit/ds/symlink/lmd18200.pdf
TO-220-11 Horizontal RM 1.7mm staggered type-1
0
11
11
TO_SOT_Packages_THT
TO-220-15_P2.54x2.54mm_StaggerEven_Lead4.58mm_Vertical
TO-220-15, Vertical, RM 1.27mm, staggered type-2, see http://www.st.com/resource/en/datasheet/l298.pdf
TO-220-15 Vertical RM 1.27mm staggered type-2
0
15
15
TO_SOT_Packages_THT
TO-220-15_P2.54x2.54mm_StaggerEven_Lead5.84mm_TabDown
TO-220-15, Horizontal, RM 1.27mm, staggered type-2, see http://www.st.com/resource/en/datasheet/l298.pdf
TO-220-15 Horizontal RM 1.27mm staggered type-2
0
15
15
TO_SOT_Packages_THT
TO-220-15_P2.54x2.54mm_StaggerOdd_Lead4.58mm_Vertical
TO-220-15, Vertical, RM 1.27mm, staggered type-1, see http://www.st.com/resource/en/datasheet/l298.pdf
TO-220-15 Vertical RM 1.27mm staggered type-1
0
15
15
TO_SOT_Packages_THT
TO-220-15_P2.54x2.54mm_StaggerOdd_Lead5.84mm_TabDown
TO-220-15, Horizontal, RM 1.27mm, staggered type-1, see http://www.st.com/resource/en/datasheet/l298.pdf
TO-220-15 Horizontal RM 1.27mm staggered type-1
0
15
15
TO_SOT_Packages_THT
TO-220F-2_Horizontal_TabDown
TO-220F-2, Horizontal, RM 5.08mm, see http://www.onsemi.com/pub/Collateral/FFPF10F150S-D.pdf
TO-220F-2 Horizontal RM 5.08mm
0
2
2
TO_SOT_Packages_THT
TO-220F-2_Horizontal_TabUp
TO-220F-2, Horizontal, RM 5.08mm, see http://www.onsemi.com/pub/Collateral/FFPF10F150S-D.pdf
TO-220F-2 Horizontal RM 5.08mm
0
2
2
TO_SOT_Packages_THT
TO-220F-2_Vertical
TO-220F-2, Vertical, RM 5.08mm, see http://www.onsemi.com/pub/Collateral/FFPF10F150S-D.pdf
TO-220F-2 Vertical RM 5.08mm
0
2
2
TO_SOT_Packages_THT
TO-220F-3_Horizontal_TabDown
TO-220F-3, Horizontal, RM 2.54mm, see http://www.st.com/resource/en/datasheet/stp20nm60.pdf
TO-220F-3 Horizontal RM 2.54mm
0
3
3
TO_SOT_Packages_THT
TO-220F-3_Horizontal_TabUp
TO-220F-3, Horizontal, RM 2.54mm, see http://www.st.com/resource/en/datasheet/stp20nm60.pdf
TO-220F-3 Horizontal RM 2.54mm
0
3
3
TO_SOT_Packages_THT
TO-220F-3_Vertical
TO-220F-3, Vertical, RM 2.54mm, see http://www.st.com/resource/en/datasheet/stp20nm60.pdf
TO-220F-3 Vertical RM 2.54mm
0
3
3
TO_SOT_Packages_THT
TO-220F-4_Horizontal_TabDown
TO-220F-4, Horizontal, RM 2.54mm, see https://www.njr.com/semicon/PDF/package/TO-220F-4_E.pdf
TO-220F-4 Horizontal RM 2.54mm
0
4
4
TO_SOT_Packages_THT
TO-220F-4_Horizontal_TabUp
TO-220F-4, Horizontal, RM 2.54mm, see https://www.njr.com/semicon/PDF/package/TO-220F-4_E.pdf
TO-220F-4 Horizontal RM 2.54mm
0
4
4
TO_SOT_Packages_THT
TO-220F-4_P5.08x2.05mm_StaggerEven_Lead1.85mm_Vertical
TO-220F-4, Vertical, RM 2.54mm, staggered type-2, see https://www.njr.com/semicon/PDF/package/TO-220F-4_E.pdf
TO-220F-4 Vertical RM 2.54mm staggered type-2
0
4
4
TO_SOT_Packages_THT
TO-220F-4_P5.08x2.05mm_StaggerOdd_Lead1.85mm_Vertical
TO-220F-4, Vertical, RM 2.54mm, staggered type-1, see https://www.njr.com/semicon/PDF/package/TO-220F-4_E.pdf
TO-220F-4 Vertical RM 2.54mm staggered type-1
0
4
4
TO_SOT_Packages_THT
TO-220F-4_P5.08x3.7mm_StaggerEven_Lead3.5mm_Vertical
TO-220F-4, Vertical, RM 2.54mm, staggered type-2, see https://www.njr.com/semicon/PDF/package/TO-220F-4_E.pdf
TO-220F-4 Vertical RM 2.54mm staggered type-2
0
4
4
TO_SOT_Packages_THT
TO-220F-4_P5.08x3.7mm_StaggerOdd_Lead3.5mm_Vertical
TO-220F-4, Vertical, RM 2.54mm, staggered type-1, see https://www.njr.com/semicon/PDF/package/TO-220F-4_E.pdf
TO-220F-4 Vertical RM 2.54mm staggered type-1
0
4
4
TO_SOT_Packages_THT
TO-220F-4_Vertical
TO-220F-4, Vertical, RM 2.54mm, see https://www.njr.com/semicon/PDF/package/TO-220F-4_E.pdf
TO-220F-4 Vertical RM 2.54mm
0
4
4
TO_SOT_Packages_THT
TO-220F-5_Horizontal_TabDown
TO-220F-5, Horizontal, RM 1.7mm, PentawattF-, MultiwattF-5
TO-220F-5 Horizontal RM 1.7mm PentawattF- MultiwattF-5
0
5
5
TO_SOT_Packages_THT
TO-220F-5_Horizontal_TabUp
TO-220F-5, Horizontal, RM 1.7mm, PentawattF-, MultiwattF-5
TO-220F-5 Horizontal RM 1.7mm PentawattF- MultiwattF-5
0
5
5
TO_SOT_Packages_THT
TO-220F-5_P3.4x2.06mm_StaggerEven_Lead1.86mm_Vertical
TO-220F-5, Vertical, RM 1.7mm, PentawattF-, MultiwattF-5, staggered type-2
TO-220F-5 Vertical RM 1.7mm PentawattF- MultiwattF-5 staggered type-2
0
5
5
TO_SOT_Packages_THT
TO-220F-5_P3.4x2.06mm_StaggerOdd_Lead1.86mm_Vertical
TO-220F-5, Vertical, RM 1.7mm, PentawattF-, MultiwattF-5, staggered type-1
TO-220F-5 Vertical RM 1.7mm PentawattF- MultiwattF-5 staggered type-1
0
5
5
TO_SOT_Packages_THT
TO-220F-5_P3.4x3.7mm_StaggerEven_Lead3.5mm_Vertical
TO-220F-5, Vertical, RM 1.7mm, PentawattF-, MultiwattF-5, staggered type-2
TO-220F-5 Vertical RM 1.7mm PentawattF- MultiwattF-5 staggered type-2
0
5
5
TO_SOT_Packages_THT
TO-220F-5_P3.4x3.7mm_StaggerOdd_Lead3.5mm_Vertical
TO-220F-5, Vertical, RM 1.7mm, PentawattF-, MultiwattF-5, staggered type-1
TO-220F-5 Vertical RM 1.7mm PentawattF- MultiwattF-5 staggered type-1
0
5
5
TO_SOT_Packages_THT
TO-220F-5_Vertical
TO-220F-5, Vertical, RM 1.7mm, PentawattF-, MultiwattF-5
TO-220F-5 Vertical RM 1.7mm PentawattF- MultiwattF-5
0
5
5
TO_SOT_Packages_THT
TO-220F-7_P2.54x3.7mm_StaggerEven_Lead3.5mm_Vertical
TO-220F-7, Vertical, RM 1.27mm, staggered type-2
TO-220F-7 Vertical RM 1.27mm staggered type-2
0
7
7
TO_SOT_Packages_THT
TO-220F-7_P2.54x3.7mm_StaggerOdd_Lead3.5mm_Vertical
TO-220F-7, Vertical, RM 1.27mm, staggered type-1
TO-220F-7 Vertical RM 1.27mm staggered type-1
0
7
7
TO_SOT_Packages_THT
TO-220F-9_P1.8x3.7mm_StaggerEven_Lead3.5mm_Vertical
TO-220F-9, Vertical, RM 0.9mm, staggered type-2
TO-220F-9 Vertical RM 0.9mm staggered type-2
0
9
9
TO_SOT_Packages_THT
TO-220F-9_P1.8x3.7mm_StaggerOdd_Lead3.5mm_Vertical
TO-220F-9, Vertical, RM 0.9mm, staggered type-1
TO-220F-9 Vertical RM 0.9mm staggered type-1
0
9
9
TO_SOT_Packages_THT
TO-220F-11_P3.4x5.08mm_StaggerEven_Lead5.08mm_Vertical
TO-220F-11, Vertical, RM 1.7mm, MultiwattF-11, staggered type-2, see http://www.ti.com/lit/ds/symlink/lm3886.pdf
TO-220F-11 Vertical RM 1.7mm MultiwattF-11 staggered type-2
0
11
11
TO_SOT_Packages_THT
TO-220F-11_P3.4x5.08mm_StaggerOdd_Lead5.08mm_Vertical
TO-220F-11, Vertical, RM 1.7mm, MultiwattF-11, staggered type-1, see http://www.ti.com/lit/ds/symlink/lm3886.pdf
TO-220F-11 Vertical RM 1.7mm MultiwattF-11 staggered type-1
0
11
11
TO_SOT_Packages_THT
TO-220F-15_P2.54x5.08mm_StaggerEven_Lead5.08mm_Vertical
TO-220F-15, Vertical, RM 1.27mm, MultiwattF-15, staggered type-2
TO-220F-15 Vertical RM 1.27mm MultiwattF-15 staggered type-2
0
15
15
TO_SOT_Packages_THT
TO-220F-15_P2.54x5.08mm_StaggerOdd_Lead5.08mm_Vertical
TO-220F-15, Vertical, RM 1.27mm, MultiwattF-15, staggered type-1
TO-220F-15 Vertical RM 1.27mm MultiwattF-15 staggered type-1
0
15
15
TO_SOT_Packages_THT
TO-247-2_Horizontal_TabDown
TO-247-2, Horizontal, RM 10.9mm, see https://toshiba.semicon-storage.com/us/product/mosfet/to-247-4l.html
TO-247-2 Horizontal RM 10.9mm
0
2
2
TO_SOT_Packages_THT
TO-247-2_Horizontal_TabUp
TO-247-2, Horizontal, RM 10.9mm, see https://toshiba.semicon-storage.com/us/product/mosfet/to-247-4l.html
TO-247-2 Horizontal RM 10.9mm
0
2
2
TO_SOT_Packages_THT
TO-247-2_Vertical
TO-247-2, Vertical, RM 10.9mm, see https://toshiba.semicon-storage.com/us/product/mosfet/to-247-4l.html
TO-247-2 Vertical RM 10.9mm
0
2
2
TO_SOT_Packages_THT
TO-247-3_Horizontal_TabDown
TO-247-3, Horizontal, RM 5.45mm, see https://toshiba.semicon-storage.com/us/product/mosfet/to-247-4l.html
TO-247-3 Horizontal RM 5.45mm
0
3
3
TO_SOT_Packages_THT
TO-247-3_Horizontal_TabUp
TO-247-3, Horizontal, RM 5.45mm, see https://toshiba.semicon-storage.com/us/product/mosfet/to-247-4l.html
TO-247-3 Horizontal RM 5.45mm
0
3
3
TO_SOT_Packages_THT
TO-247-3_Vertical
TO-247-3, Vertical, RM 5.45mm, see https://toshiba.semicon-storage.com/us/product/mosfet/to-247-4l.html
TO-247-3 Vertical RM 5.45mm
0
3
3
TO_SOT_Packages_THT
TO-247-4_Horizontal_TabDown
TO-247-4, Horizontal, RM 2.54mm, see https://toshiba.semicon-storage.com/us/product/mosfet/to-247-4l.html
TO-247-4 Horizontal RM 2.54mm
0
4
4
TO_SOT_Packages_THT
TO-247-4_Horizontal_TabUp
TO-247-4, Horizontal, RM 2.54mm, see https://toshiba.semicon-storage.com/us/product/mosfet/to-247-4l.html
TO-247-4 Horizontal RM 2.54mm
0
4
4
TO_SOT_Packages_THT
TO-247-4_Vertical
TO-247-4, Vertical, RM 2.54mm, see https://toshiba.semicon-storage.com/us/product/mosfet/to-247-4l.html
TO-247-4 Vertical RM 2.54mm
0
4
4
TO_SOT_Packages_THT
TO-247-5_Horizontal_TabDown
TO-247-5, Horizontal, RM 2.54mm, see http://ww1.microchip.com/downloads/en/DeviceDoc/20005685A.pdf
TO-247-5 Horizontal RM 2.54mm
0
5
5
TO_SOT_Packages_THT
TO-247-5_Horizontal_TabUp
TO-247-5, Horizontal, RM 2.54mm, see http://ww1.microchip.com/downloads/en/DeviceDoc/20005685A.pdf
TO-247-5 Horizontal RM 2.54mm
0
5
5
TO_SOT_Packages_THT
TO-247-5_Vertical
TO-247-5, Vertical, RM 2.54mm, see http://ww1.microchip.com/downloads/en/DeviceDoc/20005685A.pdf
TO-247-5 Vertical RM 2.54mm
0
5
5
TO_SOT_Packages_THT
TO-251-2-1EP_Horizontal_TabDown
TO-251-2, Horizontal, RM 4.58mm, IPAK, see https://www.diodes.com/assets/Package-Files/TO251.pdf
TO-251-2 Horizontal RM 4.58mm IPAK
0
3
3
TO_SOT_Packages_THT
TO-251-2_Vertical
TO-251-2, Vertical, RM 4.58mm, IPAK, see https://www.diodes.com/assets/Package-Files/TO251.pdf
TO-251-2 Vertical RM 4.58mm IPAK
0
2
2
TO_SOT_Packages_THT
TO-251-3-1EP_Horizontal_TabDown
TO-251-3, Horizontal, RM 2.29mm, IPAK, see https://www.diodes.com/assets/Package-Files/TO251.pdf
TO-251-3 Horizontal RM 2.29mm IPAK
0
4
4
TO_SOT_Packages_THT
TO-251-3_Vertical
TO-251-3, Vertical, RM 2.29mm, IPAK, see https://www.diodes.com/assets/Package-Files/TO251.pdf
TO-251-3 Vertical RM 2.29mm IPAK
0
3
3
TO_SOT_Packages_THT
TO-262-3-1EP_Horizontal_TabDown
TO-262-3, Horizontal, RM 2.54mm, IIPAK, I2PAK, see http://www.onsemi.com/pub/Collateral/EN8586-D.PDF
TO-262-3 Horizontal RM 2.54mm IIPAK I2PAK
0
4
4
TO_SOT_Packages_THT
TO-262-3_Vertical
TO-262-3, Vertical, RM 2.54mm, IIPAK, I2PAK, see http://www.onsemi.com/pub/Collateral/EN8586-D.PDF
TO-262-3 Vertical RM 2.54mm IIPAK I2PAK
0
3
3
TO_SOT_Packages_THT
TO-262-5-1EP_Horizontal_TabDown
TO-262-5, Horizontal, RM 1.7mm, IIPAK, I2PAK, see http://pdf.datasheetcatalog.com/datasheet/irf/iris4011.pdf
TO-262-5 Horizontal RM 1.7mm IIPAK I2PAK
0
6
6
TO_SOT_Packages_THT
TO-262-5_Vertical
TO-262-5, Vertical, RM 1.7mm, IIPAK, I2PAK, see http://pdf.datasheetcatalog.com/datasheet/irf/iris4011.pdf
TO-262-5 Vertical RM 1.7mm IIPAK I2PAK
0
5
5
TO_SOT_Packages_THT
TO-264-2_Horizontal_TabDown
TO-264-2, Horizontal, RM 10.9mm, see https://www.fairchildsemi.com/package-drawings/TO/TO264A03.pdf
TO-264-2 Horizontal RM 10.9mm
0
2
2
TO_SOT_Packages_THT
TO-264-2_Horizontal_TabUp
TO-264-2, Horizontal, RM 10.9mm, see https://www.fairchildsemi.com/package-drawings/TO/TO264A03.pdf
TO-264-2 Horizontal RM 10.9mm
0
2
2
TO_SOT_Packages_THT
TO-264-2_Vertical
TO-264-2, Vertical, RM 10.9mm, see https://www.fairchildsemi.com/package-drawings/TO/TO264A03.pdf
TO-264-2 Vertical RM 10.9mm
0
2
2
TO_SOT_Packages_THT
TO-264-3_Horizontal_TabDown
TO-264-3, Horizontal, RM 5.45mm, see https://www.fairchildsemi.com/package-drawings/TO/TO264A03.pdf
TO-264-3 Horizontal RM 5.45mm
0
3
3
TO_SOT_Packages_THT
TO-264-3_Horizontal_TabUp
TO-264-3, Horizontal, RM 5.45mm, see https://www.fairchildsemi.com/package-drawings/TO/TO264A03.pdf
TO-264-3 Horizontal RM 5.45mm
0
3
3
TO_SOT_Packages_THT
TO-264-3_Vertical
TO-264-3, Vertical, RM 5.45mm, see https://www.fairchildsemi.com/package-drawings/TO/TO264A03.pdf
TO-264-3 Vertical RM 5.45mm
0
3
3
TO_SOT_Packages_THT
TO-264-5_Horizontal_TabDown
TO-264-5, Horizontal, RM 3.81mm, see https://www.onsemi.com/pub/Collateral/NJL3281D-D.PDF
TO-264-5 Horizontal RM 3.81mm
0
5
5
TO_SOT_Packages_THT
TO-264-5_Horizontal_TabUp
TO-264-5, Horizontal, RM 3.81mm, see https://www.onsemi.com/pub/Collateral/NJL3281D-D.PDF
TO-264-5 Horizontal RM 3.81mm
0
5
5
TO_SOT_Packages_THT
TO-264-5_Vertical
TO-264-5, Vertical, RM 3.81mm, see https://www.onsemi.com/pub/Collateral/NJL3281D-D.PDF
TO-264-5 Vertical RM 3.81mm
0
5
5
TerminalBlock_Phoenix
TerminalBlock_Phoenix_MKDS-1,5-2-5.08_1x02_P5.08mm_Horizontal
Terminal Block Phoenix MKDS-1,5-2-5.08, 2 pins, pitch 5.08mm, size 10.2x9.8mm^2, drill diamater 1.3mm, pad diameter 2.6mm, see http://www.farnell.com/datasheets/100425.pdf, script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_Phoenix
THT Terminal Block Phoenix MKDS-1,5-2-5.08 pitch 5.08mm size 10.2x9.8mm^2 drill 1.3mm pad 2.6mm
0
2
2
TerminalBlock_Phoenix
TerminalBlock_Phoenix_MKDS-1,5-2_1x02_P5.00mm_Horizontal
Terminal Block Phoenix MKDS-1,5-2, 2 pins, pitch 5mm, size 10x9.8mm^2, drill diamater 1.3mm, pad diameter 2.6mm, see http://www.farnell.com/datasheets/100425.pdf, script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_Phoenix
THT Terminal Block Phoenix MKDS-1,5-2 pitch 5mm size 10x9.8mm^2 drill 1.3mm pad 2.6mm
0
2
2
TerminalBlock_Phoenix
TerminalBlock_Phoenix_MKDS-1,5-3-5.08_1x03_P5.08mm_Horizontal
Terminal Block Phoenix MKDS-1,5-3-5.08, 3 pins, pitch 5.08mm, size 15.2x9.8mm^2, drill diamater 1.3mm, pad diameter 2.6mm, see http://www.farnell.com/datasheets/100425.pdf, script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_Phoenix
THT Terminal Block Phoenix MKDS-1,5-3-5.08 pitch 5.08mm size 15.2x9.8mm^2 drill 1.3mm pad 2.6mm
0
3
3
TerminalBlock_Phoenix
TerminalBlock_Phoenix_MKDS-1,5-3_1x03_P5.00mm_Horizontal
Terminal Block Phoenix MKDS-1,5-3, 3 pins, pitch 5mm, size 15x9.8mm^2, drill diamater 1.3mm, pad diameter 2.6mm, see http://www.farnell.com/datasheets/100425.pdf, script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_Phoenix
THT Terminal Block Phoenix MKDS-1,5-3 pitch 5mm size 15x9.8mm^2 drill 1.3mm pad 2.6mm
0
3
3
TerminalBlock_Phoenix
TerminalBlock_Phoenix_MKDS-1,5-4-5.08_1x04_P5.08mm_Horizontal
Terminal Block Phoenix MKDS-1,5-4-5.08, 4 pins, pitch 5.08mm, size 20.3x9.8mm^2, drill diamater 1.3mm, pad diameter 2.6mm, see http://www.farnell.com/datasheets/100425.pdf, script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_Phoenix
THT Terminal Block Phoenix MKDS-1,5-4-5.08 pitch 5.08mm size 20.3x9.8mm^2 drill 1.3mm pad 2.6mm
0
4
4
TerminalBlock_Phoenix
TerminalBlock_Phoenix_MKDS-1,5-4_1x04_P5.00mm_Horizontal
Terminal Block Phoenix MKDS-1,5-4, 4 pins, pitch 5mm, size 20x9.8mm^2, drill diamater 1.3mm, pad diameter 2.6mm, see http://www.farnell.com/datasheets/100425.pdf, script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_Phoenix
THT Terminal Block Phoenix MKDS-1,5-4 pitch 5mm size 20x9.8mm^2 drill 1.3mm pad 2.6mm
0
4
4
TerminalBlock_Phoenix
TerminalBlock_Phoenix_MKDS-1,5-5-5.08_1x05_P5.08mm_Horizontal
Terminal Block Phoenix MKDS-1,5-5-5.08, 5 pins, pitch 5.08mm, size 25.4x9.8mm^2, drill diamater 1.3mm, pad diameter 2.6mm, see http://www.farnell.com/datasheets/100425.pdf, script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_Phoenix
THT Terminal Block Phoenix MKDS-1,5-5-5.08 pitch 5.08mm size 25.4x9.8mm^2 drill 1.3mm pad 2.6mm
0
5
5
TerminalBlock_Phoenix
TerminalBlock_Phoenix_MKDS-1,5-5_1x05_P5.00mm_Horizontal
Terminal Block Phoenix MKDS-1,5-5, 5 pins, pitch 5mm, size 25x9.8mm^2, drill diamater 1.3mm, pad diameter 2.6mm, see http://www.farnell.com/datasheets/100425.pdf, script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_Phoenix
THT Terminal Block Phoenix MKDS-1,5-5 pitch 5mm size 25x9.8mm^2 drill 1.3mm pad 2.6mm
0
5
5
TerminalBlock_Phoenix
TerminalBlock_Phoenix_MKDS-1,5-6-5.08_1x06_P5.08mm_Horizontal
Terminal Block Phoenix MKDS-1,5-6-5.08, 6 pins, pitch 5.08mm, size 30.5x9.8mm^2, drill diamater 1.3mm, pad diameter 2.6mm, see http://www.farnell.com/datasheets/100425.pdf, script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_Phoenix
THT Terminal Block Phoenix MKDS-1,5-6-5.08 pitch 5.08mm size 30.5x9.8mm^2 drill 1.3mm pad 2.6mm
0
6
6
TerminalBlock_Phoenix
TerminalBlock_Phoenix_MKDS-1,5-6_1x06_P5.00mm_Horizontal
Terminal Block Phoenix MKDS-1,5-6, 6 pins, pitch 5mm, size 30x9.8mm^2, drill diamater 1.3mm, pad diameter 2.6mm, see http://www.farnell.com/datasheets/100425.pdf, script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_Phoenix
THT Terminal Block Phoenix MKDS-1,5-6 pitch 5mm size 30x9.8mm^2 drill 1.3mm pad 2.6mm
0
6
6
TerminalBlock_Phoenix
TerminalBlock_Phoenix_MKDS-1,5-7-5.08_1x07_P5.08mm_Horizontal
Terminal Block Phoenix MKDS-1,5-7-5.08, 7 pins, pitch 5.08mm, size 35.6x9.8mm^2, drill diamater 1.3mm, pad diameter 2.6mm, see http://www.farnell.com/datasheets/100425.pdf, script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_Phoenix
THT Terminal Block Phoenix MKDS-1,5-7-5.08 pitch 5.08mm size 35.6x9.8mm^2 drill 1.3mm pad 2.6mm
0
7
7
TerminalBlock_Phoenix
TerminalBlock_Phoenix_MKDS-1,5-7_1x07_P5.00mm_Horizontal
Terminal Block Phoenix MKDS-1,5-7, 7 pins, pitch 5mm, size 35x9.8mm^2, drill diamater 1.3mm, pad diameter 2.6mm, see http://www.farnell.com/datasheets/100425.pdf, script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_Phoenix
THT Terminal Block Phoenix MKDS-1,5-7 pitch 5mm size 35x9.8mm^2 drill 1.3mm pad 2.6mm
0
7
7
TerminalBlock_Phoenix
TerminalBlock_Phoenix_MKDS-1,5-8-5.08_1x08_P5.08mm_Horizontal
Terminal Block Phoenix MKDS-1,5-8-5.08, 8 pins, pitch 5.08mm, size 40.6x9.8mm^2, drill diamater 1.3mm, pad diameter 2.6mm, see http://www.farnell.com/datasheets/100425.pdf, script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_Phoenix
THT Terminal Block Phoenix MKDS-1,5-8-5.08 pitch 5.08mm size 40.6x9.8mm^2 drill 1.3mm pad 2.6mm
0
8
8
TerminalBlock_Phoenix
TerminalBlock_Phoenix_MKDS-1,5-8_1x08_P5.00mm_Horizontal
Terminal Block Phoenix MKDS-1,5-8, 8 pins, pitch 5mm, size 40x9.8mm^2, drill diamater 1.3mm, pad diameter 2.6mm, see http://www.farnell.com/datasheets/100425.pdf, script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_Phoenix
THT Terminal Block Phoenix MKDS-1,5-8 pitch 5mm size 40x9.8mm^2 drill 1.3mm pad 2.6mm
0
8
8
TerminalBlock_Phoenix
TerminalBlock_Phoenix_MKDS-1,5-9-5.08_1x09_P5.08mm_Horizontal
Terminal Block Phoenix MKDS-1,5-9-5.08, 9 pins, pitch 5.08mm, size 45.7x9.8mm^2, drill diamater 1.3mm, pad diameter 2.6mm, see http://www.farnell.com/datasheets/100425.pdf, script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_Phoenix
THT Terminal Block Phoenix MKDS-1,5-9-5.08 pitch 5.08mm size 45.7x9.8mm^2 drill 1.3mm pad 2.6mm
0
9
9
TerminalBlock_Phoenix
TerminalBlock_Phoenix_MKDS-1,5-9_1x09_P5.00mm_Horizontal
Terminal Block Phoenix MKDS-1,5-9, 9 pins, pitch 5mm, size 45x9.8mm^2, drill diamater 1.3mm, pad diameter 2.6mm, see http://www.farnell.com/datasheets/100425.pdf, script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_Phoenix
THT Terminal Block Phoenix MKDS-1,5-9 pitch 5mm size 45x9.8mm^2 drill 1.3mm pad 2.6mm
0
9
9
TerminalBlock_Phoenix
TerminalBlock_Phoenix_MKDS-1,5-10-5.08_1x10_P5.08mm_Horizontal
Terminal Block Phoenix MKDS-1,5-10-5.08, 10 pins, pitch 5.08mm, size 50.8x9.8mm^2, drill diamater 1.3mm, pad diameter 2.6mm, see http://www.farnell.com/datasheets/100425.pdf, script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_Phoenix
THT Terminal Block Phoenix MKDS-1,5-10-5.08 pitch 5.08mm size 50.8x9.8mm^2 drill 1.3mm pad 2.6mm
0
10
10
TerminalBlock_Phoenix
TerminalBlock_Phoenix_MKDS-1,5-10_1x10_P5.00mm_Horizontal
Terminal Block Phoenix MKDS-1,5-10, 10 pins, pitch 5mm, size 50x9.8mm^2, drill diamater 1.3mm, pad diameter 2.6mm, see http://www.farnell.com/datasheets/100425.pdf, script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_Phoenix
THT Terminal Block Phoenix MKDS-1,5-10 pitch 5mm size 50x9.8mm^2 drill 1.3mm pad 2.6mm
0
10
10
TerminalBlock_Phoenix
TerminalBlock_Phoenix_MKDS-1,5-11-5.08_1x11_P5.08mm_Horizontal
Terminal Block Phoenix MKDS-1,5-11-5.08, 11 pins, pitch 5.08mm, size 55.9x9.8mm^2, drill diamater 1.3mm, pad diameter 2.6mm, see http://www.farnell.com/datasheets/100425.pdf, script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_Phoenix
THT Terminal Block Phoenix MKDS-1,5-11-5.08 pitch 5.08mm size 55.9x9.8mm^2 drill 1.3mm pad 2.6mm
0
11
11
TerminalBlock_Phoenix
TerminalBlock_Phoenix_MKDS-1,5-11_1x11_P5.00mm_Horizontal
Terminal Block Phoenix MKDS-1,5-11, 11 pins, pitch 5mm, size 55x9.8mm^2, drill diamater 1.3mm, pad diameter 2.6mm, see http://www.farnell.com/datasheets/100425.pdf, script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_Phoenix
THT Terminal Block Phoenix MKDS-1,5-11 pitch 5mm size 55x9.8mm^2 drill 1.3mm pad 2.6mm
0
11
11
TerminalBlock_Phoenix
TerminalBlock_Phoenix_MKDS-1,5-12-5.08_1x12_P5.08mm_Horizontal
Terminal Block Phoenix MKDS-1,5-12-5.08, 12 pins, pitch 5.08mm, size 61x9.8mm^2, drill diamater 1.3mm, pad diameter 2.6mm, see http://www.farnell.com/datasheets/100425.pdf, script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_Phoenix
THT Terminal Block Phoenix MKDS-1,5-12-5.08 pitch 5.08mm size 61x9.8mm^2 drill 1.3mm pad 2.6mm
0
12
12
TerminalBlock_Phoenix
TerminalBlock_Phoenix_MKDS-1,5-12_1x12_P5.00mm_Horizontal
Terminal Block Phoenix MKDS-1,5-12, 12 pins, pitch 5mm, size 60x9.8mm^2, drill diamater 1.3mm, pad diameter 2.6mm, see http://www.farnell.com/datasheets/100425.pdf, script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_Phoenix
THT Terminal Block Phoenix MKDS-1,5-12 pitch 5mm size 60x9.8mm^2 drill 1.3mm pad 2.6mm
0
12
12
TerminalBlock_Phoenix
TerminalBlock_Phoenix_MKDS-1,5-13-5.08_1x13_P5.08mm_Horizontal
Terminal Block Phoenix MKDS-1,5-13-5.08, 13 pins, pitch 5.08mm, size 66x9.8mm^2, drill diamater 1.3mm, pad diameter 2.6mm, see http://www.farnell.com/datasheets/100425.pdf, script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_Phoenix
THT Terminal Block Phoenix MKDS-1,5-13-5.08 pitch 5.08mm size 66x9.8mm^2 drill 1.3mm pad 2.6mm
0
13
13
TerminalBlock_Phoenix
TerminalBlock_Phoenix_MKDS-1,5-13_1x13_P5.00mm_Horizontal
Terminal Block Phoenix MKDS-1,5-13, 13 pins, pitch 5mm, size 65x9.8mm^2, drill diamater 1.3mm, pad diameter 2.6mm, see http://www.farnell.com/datasheets/100425.pdf, script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_Phoenix
THT Terminal Block Phoenix MKDS-1,5-13 pitch 5mm size 65x9.8mm^2 drill 1.3mm pad 2.6mm
0
13
13
TerminalBlock_Phoenix
TerminalBlock_Phoenix_MKDS-1,5-14-5.08_1x14_P5.08mm_Horizontal
Terminal Block Phoenix MKDS-1,5-14-5.08, 14 pins, pitch 5.08mm, size 71.1x9.8mm^2, drill diamater 1.3mm, pad diameter 2.6mm, see http://www.farnell.com/datasheets/100425.pdf, script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_Phoenix
THT Terminal Block Phoenix MKDS-1,5-14-5.08 pitch 5.08mm size 71.1x9.8mm^2 drill 1.3mm pad 2.6mm
0
14
14
TerminalBlock_Phoenix
TerminalBlock_Phoenix_MKDS-1,5-14_1x14_P5.00mm_Horizontal
Terminal Block Phoenix MKDS-1,5-14, 14 pins, pitch 5mm, size 70x9.8mm^2, drill diamater 1.3mm, pad diameter 2.6mm, see http://www.farnell.com/datasheets/100425.pdf, script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_Phoenix
THT Terminal Block Phoenix MKDS-1,5-14 pitch 5mm size 70x9.8mm^2 drill 1.3mm pad 2.6mm
0
14
14
TerminalBlock_Phoenix
TerminalBlock_Phoenix_MKDS-1,5-15-5.08_1x15_P5.08mm_Horizontal
Terminal Block Phoenix MKDS-1,5-15-5.08, 15 pins, pitch 5.08mm, size 76.2x9.8mm^2, drill diamater 1.3mm, pad diameter 2.6mm, see http://www.farnell.com/datasheets/100425.pdf, script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_Phoenix
THT Terminal Block Phoenix MKDS-1,5-15-5.08 pitch 5.08mm size 76.2x9.8mm^2 drill 1.3mm pad 2.6mm
0
15
15
TerminalBlock_Phoenix
TerminalBlock_Phoenix_MKDS-1,5-15_1x15_P5.00mm_Horizontal
Terminal Block Phoenix MKDS-1,5-15, 15 pins, pitch 5mm, size 75x9.8mm^2, drill diamater 1.3mm, pad diameter 2.6mm, see http://www.farnell.com/datasheets/100425.pdf, script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_Phoenix
THT Terminal Block Phoenix MKDS-1,5-15 pitch 5mm size 75x9.8mm^2 drill 1.3mm pad 2.6mm
0
15
15
TerminalBlock_Phoenix
TerminalBlock_Phoenix_MKDS-1,5-16-5.08_1x16_P5.08mm_Horizontal
Terminal Block Phoenix MKDS-1,5-16-5.08, 16 pins, pitch 5.08mm, size 81.3x9.8mm^2, drill diamater 1.3mm, pad diameter 2.6mm, see http://www.farnell.com/datasheets/100425.pdf, script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_Phoenix
THT Terminal Block Phoenix MKDS-1,5-16-5.08 pitch 5.08mm size 81.3x9.8mm^2 drill 1.3mm pad 2.6mm
0
16
16
TerminalBlock_Phoenix
TerminalBlock_Phoenix_MKDS-1,5-16_1x16_P5.00mm_Horizontal
Terminal Block Phoenix MKDS-1,5-16, 16 pins, pitch 5mm, size 80x9.8mm^2, drill diamater 1.3mm, pad diameter 2.6mm, see http://www.farnell.com/datasheets/100425.pdf, script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_Phoenix
THT Terminal Block Phoenix MKDS-1,5-16 pitch 5mm size 80x9.8mm^2 drill 1.3mm pad 2.6mm
0
16
16
TerminalBlock_Phoenix
TerminalBlock_Phoenix_MKDS-3-2-5.08_1x02_P5.08mm_Horizontal
Terminal Block Phoenix MKDS-3-2-5.08, 2 pins, pitch 5.08mm, size 10.2x11.2mm^2, drill diamater 1.3mm, pad diameter 2.6mm, see http://www.farnell.com/datasheets/2138224.pdf, script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_Phoenix
THT Terminal Block Phoenix MKDS-3-2-5.08 pitch 5.08mm size 10.2x11.2mm^2 drill 1.3mm pad 2.6mm
0
2
2
TerminalBlock_Phoenix
TerminalBlock_Phoenix_MKDS-3-3-5.08_1x03_P5.08mm_Horizontal
Terminal Block Phoenix MKDS-3-3-5.08, 3 pins, pitch 5.08mm, size 15.2x11.2mm^2, drill diamater 1.3mm, pad diameter 2.6mm, see http://www.farnell.com/datasheets/2138224.pdf, script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_Phoenix
THT Terminal Block Phoenix MKDS-3-3-5.08 pitch 5.08mm size 15.2x11.2mm^2 drill 1.3mm pad 2.6mm
0
3
3
TerminalBlock_Phoenix
TerminalBlock_Phoenix_MKDS-3-4-5.08_1x04_P5.08mm_Horizontal
Terminal Block Phoenix MKDS-3-4-5.08, 4 pins, pitch 5.08mm, size 20.3x11.2mm^2, drill diamater 1.3mm, pad diameter 2.6mm, see http://www.farnell.com/datasheets/2138224.pdf, script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_Phoenix
THT Terminal Block Phoenix MKDS-3-4-5.08 pitch 5.08mm size 20.3x11.2mm^2 drill 1.3mm pad 2.6mm
0
4
4
TerminalBlock_Phoenix
TerminalBlock_Phoenix_MKDS-3-5-5.08_1x05_P5.08mm_Horizontal
Terminal Block Phoenix MKDS-3-5-5.08, 5 pins, pitch 5.08mm, size 25.4x11.2mm^2, drill diamater 1.3mm, pad diameter 2.6mm, see http://www.farnell.com/datasheets/2138224.pdf, script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_Phoenix
THT Terminal Block Phoenix MKDS-3-5-5.08 pitch 5.08mm size 25.4x11.2mm^2 drill 1.3mm pad 2.6mm
0
5
5
TerminalBlock_Phoenix
TerminalBlock_Phoenix_MKDS-3-6-5.08_1x06_P5.08mm_Horizontal
Terminal Block Phoenix MKDS-3-6-5.08, 6 pins, pitch 5.08mm, size 30.5x11.2mm^2, drill diamater 1.3mm, pad diameter 2.6mm, see http://www.farnell.com/datasheets/2138224.pdf, script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_Phoenix
THT Terminal Block Phoenix MKDS-3-6-5.08 pitch 5.08mm size 30.5x11.2mm^2 drill 1.3mm pad 2.6mm
0
6
6
TerminalBlock_Phoenix
TerminalBlock_Phoenix_MKDS-3-7-5.08_1x07_P5.08mm_Horizontal
Terminal Block Phoenix MKDS-3-7-5.08, 7 pins, pitch 5.08mm, size 35.6x11.2mm^2, drill diamater 1.3mm, pad diameter 2.6mm, see http://www.farnell.com/datasheets/2138224.pdf, script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_Phoenix
THT Terminal Block Phoenix MKDS-3-7-5.08 pitch 5.08mm size 35.6x11.2mm^2 drill 1.3mm pad 2.6mm
0
7
7
TerminalBlock_Phoenix
TerminalBlock_Phoenix_MKDS-3-8-5.08_1x08_P5.08mm_Horizontal
Terminal Block Phoenix MKDS-3-8-5.08, 8 pins, pitch 5.08mm, size 40.6x11.2mm^2, drill diamater 1.3mm, pad diameter 2.6mm, see http://www.farnell.com/datasheets/2138224.pdf, script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_Phoenix
THT Terminal Block Phoenix MKDS-3-8-5.08 pitch 5.08mm size 40.6x11.2mm^2 drill 1.3mm pad 2.6mm
0
8
8
TerminalBlock_Phoenix
TerminalBlock_Phoenix_MKDS-3-9-5.08_1x09_P5.08mm_Horizontal
Terminal Block Phoenix MKDS-3-9-5.08, 9 pins, pitch 5.08mm, size 45.7x11.2mm^2, drill diamater 1.3mm, pad diameter 2.6mm, see http://www.farnell.com/datasheets/2138224.pdf, script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_Phoenix
THT Terminal Block Phoenix MKDS-3-9-5.08 pitch 5.08mm size 45.7x11.2mm^2 drill 1.3mm pad 2.6mm
0
9
9
TerminalBlock_Phoenix
TerminalBlock_Phoenix_MKDS-3-10-5.08_1x10_P5.08mm_Horizontal
Terminal Block Phoenix MKDS-3-10-5.08, 10 pins, pitch 5.08mm, size 50.8x11.2mm^2, drill diamater 1.3mm, pad diameter 2.6mm, see http://www.farnell.com/datasheets/2138224.pdf, script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_Phoenix
THT Terminal Block Phoenix MKDS-3-10-5.08 pitch 5.08mm size 50.8x11.2mm^2 drill 1.3mm pad 2.6mm
0
10
10
TerminalBlock_Phoenix
TerminalBlock_Phoenix_MKDS-3-11-5.08_1x11_P5.08mm_Horizontal
Terminal Block Phoenix MKDS-3-11-5.08, 11 pins, pitch 5.08mm, size 55.9x11.2mm^2, drill diamater 1.3mm, pad diameter 2.6mm, see http://www.farnell.com/datasheets/2138224.pdf, script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_Phoenix
THT Terminal Block Phoenix MKDS-3-11-5.08 pitch 5.08mm size 55.9x11.2mm^2 drill 1.3mm pad 2.6mm
0
11
11
TerminalBlock_Phoenix
TerminalBlock_Phoenix_MKDS-3-12-5.08_1x12_P5.08mm_Horizontal
Terminal Block Phoenix MKDS-3-12-5.08, 12 pins, pitch 5.08mm, size 61x11.2mm^2, drill diamater 1.3mm, pad diameter 2.6mm, see http://www.farnell.com/datasheets/2138224.pdf, script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_Phoenix
THT Terminal Block Phoenix MKDS-3-12-5.08 pitch 5.08mm size 61x11.2mm^2 drill 1.3mm pad 2.6mm
0
12
12
TerminalBlock_Phoenix
TerminalBlock_Phoenix_MKDS-3-13-5.08_1x13_P5.08mm_Horizontal
Terminal Block Phoenix MKDS-3-13-5.08, 13 pins, pitch 5.08mm, size 66x11.2mm^2, drill diamater 1.3mm, pad diameter 2.6mm, see http://www.farnell.com/datasheets/2138224.pdf, script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_Phoenix
THT Terminal Block Phoenix MKDS-3-13-5.08 pitch 5.08mm size 66x11.2mm^2 drill 1.3mm pad 2.6mm
0
13
13
TerminalBlock_Phoenix
TerminalBlock_Phoenix_MKDS-3-14-5.08_1x14_P5.08mm_Horizontal
Terminal Block Phoenix MKDS-3-14-5.08, 14 pins, pitch 5.08mm, size 71.1x11.2mm^2, drill diamater 1.3mm, pad diameter 2.6mm, see http://www.farnell.com/datasheets/2138224.pdf, script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_Phoenix
THT Terminal Block Phoenix MKDS-3-14-5.08 pitch 5.08mm size 71.1x11.2mm^2 drill 1.3mm pad 2.6mm
0
14
14
TerminalBlock_Phoenix
TerminalBlock_Phoenix_MKDS-3-15-5.08_1x15_P5.08mm_Horizontal
Terminal Block Phoenix MKDS-3-15-5.08, 15 pins, pitch 5.08mm, size 76.2x11.2mm^2, drill diamater 1.3mm, pad diameter 2.6mm, see http://www.farnell.com/datasheets/2138224.pdf, script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_Phoenix
THT Terminal Block Phoenix MKDS-3-15-5.08 pitch 5.08mm size 76.2x11.2mm^2 drill 1.3mm pad 2.6mm
0
15
15
TerminalBlock_Phoenix
TerminalBlock_Phoenix_MKDS-3-16-5.08_1x16_P5.08mm_Horizontal
Terminal Block Phoenix MKDS-3-16-5.08, 16 pins, pitch 5.08mm, size 81.3x11.2mm^2, drill diamater 1.3mm, pad diameter 2.6mm, see http://www.farnell.com/datasheets/2138224.pdf, script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_Phoenix
THT Terminal Block Phoenix MKDS-3-16-5.08 pitch 5.08mm size 81.3x11.2mm^2 drill 1.3mm pad 2.6mm
0
16
16
TerminalBlock_Phoenix
TerminalBlock_Phoenix_MPT-0,5-2-2.54_1x02_P2.54mm_Horizontal
Terminal Block Phoenix MPT-0,5-2-2.54, 2 pins, pitch 2.54mm, size 5.54x6.2mm^2, drill diamater 1.1mm, pad diameter 2.2mm, see http://www.mouser.com/ds/2/324/ItemDetail_1725656-920552.pdf, script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_Phoenix
THT Terminal Block Phoenix MPT-0,5-2-2.54 pitch 2.54mm size 5.54x6.2mm^2 drill 1.1mm pad 2.2mm
0
2
2
TerminalBlock_Phoenix
TerminalBlock_Phoenix_MPT-0,5-3-2.54_1x03_P2.54mm_Horizontal
Terminal Block Phoenix MPT-0,5-3-2.54, 3 pins, pitch 2.54mm, size 8.08x6.2mm^2, drill diamater 1.1mm, pad diameter 2.2mm, see http://www.mouser.com/ds/2/324/ItemDetail_1725656-920552.pdf, script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_Phoenix
THT Terminal Block Phoenix MPT-0,5-3-2.54 pitch 2.54mm size 8.08x6.2mm^2 drill 1.1mm pad 2.2mm
0
3
3
TerminalBlock_Phoenix
TerminalBlock_Phoenix_MPT-0,5-4-2.54_1x04_P2.54mm_Horizontal
Terminal Block Phoenix MPT-0,5-4-2.54, 4 pins, pitch 2.54mm, size 10.6x6.2mm^2, drill diamater 1.1mm, pad diameter 2.2mm, see http://www.mouser.com/ds/2/324/ItemDetail_1725672-916605.pdf, script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_Phoenix
THT Terminal Block Phoenix MPT-0,5-4-2.54 pitch 2.54mm size 10.6x6.2mm^2 drill 1.1mm pad 2.2mm
0
4
4
TerminalBlock_Phoenix
TerminalBlock_Phoenix_MPT-0,5-5-2.54_1x05_P2.54mm_Horizontal
Terminal Block Phoenix MPT-0,5-5-2.54, 5 pins, pitch 2.54mm, size 13.2x6.2mm^2, drill diamater 1.1mm, pad diameter 2.2mm, see http://www.mouser.com/ds/2/324/ItemDetail_1725672-916605.pdf, script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_Phoenix
THT Terminal Block Phoenix MPT-0,5-5-2.54 pitch 2.54mm size 13.2x6.2mm^2 drill 1.1mm pad 2.2mm
0
5
5
TerminalBlock_Phoenix
TerminalBlock_Phoenix_MPT-0,5-6-2.54_1x06_P2.54mm_Horizontal
Terminal Block Phoenix MPT-0,5-6-2.54, 6 pins, pitch 2.54mm, size 15.7x6.2mm^2, drill diamater 1.1mm, pad diameter 2.2mm, see http://www.mouser.com/ds/2/324/ItemDetail_1725672-916605.pdf, script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_Phoenix
THT Terminal Block Phoenix MPT-0,5-6-2.54 pitch 2.54mm size 15.7x6.2mm^2 drill 1.1mm pad 2.2mm
0
6
6
TerminalBlock_Phoenix
TerminalBlock_Phoenix_MPT-0,5-7-2.54_1x07_P2.54mm_Horizontal
Terminal Block Phoenix MPT-0,5-7-2.54, 7 pins, pitch 2.54mm, size 18.2x6.2mm^2, drill diamater 1.1mm, pad diameter 2.2mm, see http://www.mouser.com/ds/2/324/ItemDetail_1725672-916605.pdf, script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_Phoenix
THT Terminal Block Phoenix MPT-0,5-7-2.54 pitch 2.54mm size 18.2x6.2mm^2 drill 1.1mm pad 2.2mm
0
7
7
TerminalBlock_Phoenix
TerminalBlock_Phoenix_MPT-0,5-8-2.54_1x08_P2.54mm_Horizontal
Terminal Block Phoenix MPT-0,5-8-2.54, 8 pins, pitch 2.54mm, size 20.8x6.2mm^2, drill diamater 1.1mm, pad diameter 2.2mm, see http://www.mouser.com/ds/2/324/ItemDetail_1725672-916605.pdf, script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_Phoenix
THT Terminal Block Phoenix MPT-0,5-8-2.54 pitch 2.54mm size 20.8x6.2mm^2 drill 1.1mm pad 2.2mm
0
8
8
TerminalBlock_Phoenix
TerminalBlock_Phoenix_MPT-0,5-9-2.54_1x09_P2.54mm_Horizontal
Terminal Block Phoenix MPT-0,5-9-2.54, 9 pins, pitch 2.54mm, size 23.3x6.2mm^2, drill diamater 1.1mm, pad diameter 2.2mm, see http://www.mouser.com/ds/2/324/ItemDetail_1725672-916605.pdf, script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_Phoenix
THT Terminal Block Phoenix MPT-0,5-9-2.54 pitch 2.54mm size 23.3x6.2mm^2 drill 1.1mm pad 2.2mm
0
9
9
TerminalBlock_Phoenix
TerminalBlock_Phoenix_MPT-0,5-10-2.54_1x10_P2.54mm_Horizontal
Terminal Block Phoenix MPT-0,5-10-2.54, 10 pins, pitch 2.54mm, size 25.9x6.2mm^2, drill diamater 1.1mm, pad diameter 2.2mm, see http://www.mouser.com/ds/2/324/ItemDetail_1725672-916605.pdf, script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_Phoenix
THT Terminal Block Phoenix MPT-0,5-10-2.54 pitch 2.54mm size 25.9x6.2mm^2 drill 1.1mm pad 2.2mm
0
10
10
TerminalBlock_Phoenix
TerminalBlock_Phoenix_MPT-0,5-11-2.54_1x11_P2.54mm_Horizontal
Terminal Block Phoenix MPT-0,5-11-2.54, 11 pins, pitch 2.54mm, size 28.4x6.2mm^2, drill diamater 1.1mm, pad diameter 2.2mm, see http://www.mouser.com/ds/2/324/ItemDetail_1725672-916605.pdf, script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_Phoenix
THT Terminal Block Phoenix MPT-0,5-11-2.54 pitch 2.54mm size 28.4x6.2mm^2 drill 1.1mm pad 2.2mm
0
11
11
TerminalBlock_Phoenix
TerminalBlock_Phoenix_MPT-0,5-12-2.54_1x12_P2.54mm_Horizontal
Terminal Block Phoenix MPT-0,5-12-2.54, 12 pins, pitch 2.54mm, size 30.9x6.2mm^2, drill diamater 1.1mm, pad diameter 2.2mm, see http://www.mouser.com/ds/2/324/ItemDetail_1725672-916605.pdf, script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_Phoenix
THT Terminal Block Phoenix MPT-0,5-12-2.54 pitch 2.54mm size 30.9x6.2mm^2 drill 1.1mm pad 2.2mm
0
12
12
TerminalBlock_Phoenix
TerminalBlock_Phoenix_PT-1,5-2-3.5-H_1x02_P3.50mm_Horizontal
Terminal Block Phoenix PT-1,5-2-3.5-H, 2 pins, pitch 3.5mm, size 7x7.6mm^2, drill diamater 1.2mm, pad diameter 2.4mm, see , script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_Phoenix
THT Terminal Block Phoenix PT-1,5-2-3.5-H pitch 3.5mm size 7x7.6mm^2 drill 1.2mm pad 2.4mm
0
2
2
TerminalBlock_Phoenix
TerminalBlock_Phoenix_PT-1,5-2-5.0-H_1x02_P5.00mm_Horizontal
Terminal Block Phoenix PT-1,5-2-5.0-H, 2 pins, pitch 5mm, size 10x9mm^2, drill diamater 1.3mm, pad diameter 2.6mm, see http://www.mouser.com/ds/2/324/ItemDetail_1935161-922578.pdf, script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_Phoenix
THT Terminal Block Phoenix PT-1,5-2-5.0-H pitch 5mm size 10x9mm^2 drill 1.3mm pad 2.6mm
0
2
2
TerminalBlock_Phoenix
TerminalBlock_Phoenix_PT-1,5-3-3.5-H_1x03_P3.50mm_Horizontal
Terminal Block Phoenix PT-1,5-3-3.5-H, 3 pins, pitch 3.5mm, size 10.5x7.6mm^2, drill diamater 1.2mm, pad diameter 2.4mm, see , script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_Phoenix
THT Terminal Block Phoenix PT-1,5-3-3.5-H pitch 3.5mm size 10.5x7.6mm^2 drill 1.2mm pad 2.4mm
0
3
3
TerminalBlock_Phoenix
TerminalBlock_Phoenix_PT-1,5-3-5.0-H_1x03_P5.00mm_Horizontal
Terminal Block Phoenix PT-1,5-3-5.0-H, 3 pins, pitch 5mm, size 15x9mm^2, drill diamater 1.3mm, pad diameter 2.6mm, see http://www.mouser.com/ds/2/324/ItemDetail_1935161-922578.pdf, script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_Phoenix
THT Terminal Block Phoenix PT-1,5-3-5.0-H pitch 5mm size 15x9mm^2 drill 1.3mm pad 2.6mm
0
3
3
TerminalBlock_Phoenix
TerminalBlock_Phoenix_PT-1,5-4-3.5-H_1x04_P3.50mm_Horizontal
Terminal Block Phoenix PT-1,5-4-3.5-H, 4 pins, pitch 3.5mm, size 14x7.6mm^2, drill diamater 1.2mm, pad diameter 2.4mm, see , script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_Phoenix
THT Terminal Block Phoenix PT-1,5-4-3.5-H pitch 3.5mm size 14x7.6mm^2 drill 1.2mm pad 2.4mm
0
4
4
TerminalBlock_Phoenix
TerminalBlock_Phoenix_PT-1,5-4-5.0-H_1x04_P5.00mm_Horizontal
Terminal Block Phoenix PT-1,5-4-5.0-H, 4 pins, pitch 5mm, size 20x9mm^2, drill diamater 1.3mm, pad diameter 2.6mm, see http://www.mouser.com/ds/2/324/ItemDetail_1935161-922578.pdf, script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_Phoenix
THT Terminal Block Phoenix PT-1,5-4-5.0-H pitch 5mm size 20x9mm^2 drill 1.3mm pad 2.6mm
0
4
4
TerminalBlock_Phoenix
TerminalBlock_Phoenix_PT-1,5-5-3.5-H_1x05_P3.50mm_Horizontal
Terminal Block Phoenix PT-1,5-5-3.5-H, 5 pins, pitch 3.5mm, size 17.5x7.6mm^2, drill diamater 1.2mm, pad diameter 2.4mm, see , script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_Phoenix
THT Terminal Block Phoenix PT-1,5-5-3.5-H pitch 3.5mm size 17.5x7.6mm^2 drill 1.2mm pad 2.4mm
0
5
5
TerminalBlock_Phoenix
TerminalBlock_Phoenix_PT-1,5-5-5.0-H_1x05_P5.00mm_Horizontal
Terminal Block Phoenix PT-1,5-5-5.0-H, 5 pins, pitch 5mm, size 25x9mm^2, drill diamater 1.3mm, pad diameter 2.6mm, see http://www.mouser.com/ds/2/324/ItemDetail_1935161-922578.pdf, script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_Phoenix
THT Terminal Block Phoenix PT-1,5-5-5.0-H pitch 5mm size 25x9mm^2 drill 1.3mm pad 2.6mm
0
5
5
TerminalBlock_Phoenix
TerminalBlock_Phoenix_PT-1,5-6-3.5-H_1x06_P3.50mm_Horizontal
Terminal Block Phoenix PT-1,5-6-3.5-H, 6 pins, pitch 3.5mm, size 21x7.6mm^2, drill diamater 1.2mm, pad diameter 2.4mm, see , script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_Phoenix
THT Terminal Block Phoenix PT-1,5-6-3.5-H pitch 3.5mm size 21x7.6mm^2 drill 1.2mm pad 2.4mm
0
6
6
TerminalBlock_Phoenix
TerminalBlock_Phoenix_PT-1,5-6-5.0-H_1x06_P5.00mm_Horizontal
Terminal Block Phoenix PT-1,5-6-5.0-H, 6 pins, pitch 5mm, size 30x9mm^2, drill diamater 1.3mm, pad diameter 2.6mm, see http://www.mouser.com/ds/2/324/ItemDetail_1935161-922578.pdf, script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_Phoenix
THT Terminal Block Phoenix PT-1,5-6-5.0-H pitch 5mm size 30x9mm^2 drill 1.3mm pad 2.6mm
0
6
6
TerminalBlock_Phoenix
TerminalBlock_Phoenix_PT-1,5-7-3.5-H_1x07_P3.50mm_Horizontal
Terminal Block Phoenix PT-1,5-7-3.5-H, 7 pins, pitch 3.5mm, size 24.5x7.6mm^2, drill diamater 1.2mm, pad diameter 2.4mm, see , script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_Phoenix
THT Terminal Block Phoenix PT-1,5-7-3.5-H pitch 3.5mm size 24.5x7.6mm^2 drill 1.2mm pad 2.4mm
0
7
7
TerminalBlock_Phoenix
TerminalBlock_Phoenix_PT-1,5-7-5.0-H_1x07_P5.00mm_Horizontal
Terminal Block Phoenix PT-1,5-7-5.0-H, 7 pins, pitch 5mm, size 35x9mm^2, drill diamater 1.3mm, pad diameter 2.6mm, see http://www.mouser.com/ds/2/324/ItemDetail_1935161-922578.pdf, script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_Phoenix
THT Terminal Block Phoenix PT-1,5-7-5.0-H pitch 5mm size 35x9mm^2 drill 1.3mm pad 2.6mm
0
7
7
TerminalBlock_Phoenix
TerminalBlock_Phoenix_PT-1,5-8-3.5-H_1x08_P3.50mm_Horizontal
Terminal Block Phoenix PT-1,5-8-3.5-H, 8 pins, pitch 3.5mm, size 28x7.6mm^2, drill diamater 1.2mm, pad diameter 2.4mm, see , script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_Phoenix
THT Terminal Block Phoenix PT-1,5-8-3.5-H pitch 3.5mm size 28x7.6mm^2 drill 1.2mm pad 2.4mm
0
8
8
TerminalBlock_Phoenix
TerminalBlock_Phoenix_PT-1,5-8-5.0-H_1x08_P5.00mm_Horizontal
Terminal Block Phoenix PT-1,5-8-5.0-H, 8 pins, pitch 5mm, size 40x9mm^2, drill diamater 1.3mm, pad diameter 2.6mm, see http://www.mouser.com/ds/2/324/ItemDetail_1935161-922578.pdf, script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_Phoenix
THT Terminal Block Phoenix PT-1,5-8-5.0-H pitch 5mm size 40x9mm^2 drill 1.3mm pad 2.6mm
0
8
8
TerminalBlock_Phoenix
TerminalBlock_Phoenix_PT-1,5-9-3.5-H_1x09_P3.50mm_Horizontal
Terminal Block Phoenix PT-1,5-9-3.5-H, 9 pins, pitch 3.5mm, size 31.5x7.6mm^2, drill diamater 1.2mm, pad diameter 2.4mm, see , script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_Phoenix
THT Terminal Block Phoenix PT-1,5-9-3.5-H pitch 3.5mm size 31.5x7.6mm^2 drill 1.2mm pad 2.4mm
0
9
9
TerminalBlock_Phoenix
TerminalBlock_Phoenix_PT-1,5-9-5.0-H_1x09_P5.00mm_Horizontal
Terminal Block Phoenix PT-1,5-9-5.0-H, 9 pins, pitch 5mm, size 45x9mm^2, drill diamater 1.3mm, pad diameter 2.6mm, see http://www.mouser.com/ds/2/324/ItemDetail_1935161-922578.pdf, script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_Phoenix
THT Terminal Block Phoenix PT-1,5-9-5.0-H pitch 5mm size 45x9mm^2 drill 1.3mm pad 2.6mm
0
9
9
TerminalBlock_Phoenix
TerminalBlock_Phoenix_PT-1,5-10-3.5-H_1x10_P3.50mm_Horizontal
Terminal Block Phoenix PT-1,5-10-3.5-H, 10 pins, pitch 3.5mm, size 35x7.6mm^2, drill diamater 1.2mm, pad diameter 2.4mm, see , script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_Phoenix
THT Terminal Block Phoenix PT-1,5-10-3.5-H pitch 3.5mm size 35x7.6mm^2 drill 1.2mm pad 2.4mm
0
10
10
TerminalBlock_Phoenix
TerminalBlock_Phoenix_PT-1,5-10-5.0-H_1x10_P5.00mm_Horizontal
Terminal Block Phoenix PT-1,5-10-5.0-H, 10 pins, pitch 5mm, size 50x9mm^2, drill diamater 1.3mm, pad diameter 2.6mm, see http://www.mouser.com/ds/2/324/ItemDetail_1935161-922578.pdf, script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_Phoenix
THT Terminal Block Phoenix PT-1,5-10-5.0-H pitch 5mm size 50x9mm^2 drill 1.3mm pad 2.6mm
0
10
10
TerminalBlock_Phoenix
TerminalBlock_Phoenix_PT-1,5-11-3.5-H_1x11_P3.50mm_Horizontal
Terminal Block Phoenix PT-1,5-11-3.5-H, 11 pins, pitch 3.5mm, size 38.5x7.6mm^2, drill diamater 1.2mm, pad diameter 2.4mm, see , script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_Phoenix
THT Terminal Block Phoenix PT-1,5-11-3.5-H pitch 3.5mm size 38.5x7.6mm^2 drill 1.2mm pad 2.4mm
0
11
11
TerminalBlock_Phoenix
TerminalBlock_Phoenix_PT-1,5-11-5.0-H_1x11_P5.00mm_Horizontal
Terminal Block Phoenix PT-1,5-11-5.0-H, 11 pins, pitch 5mm, size 55x9mm^2, drill diamater 1.3mm, pad diameter 2.6mm, see http://www.mouser.com/ds/2/324/ItemDetail_1935161-922578.pdf, script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_Phoenix
THT Terminal Block Phoenix PT-1,5-11-5.0-H pitch 5mm size 55x9mm^2 drill 1.3mm pad 2.6mm
0
11
11
TerminalBlock_Phoenix
TerminalBlock_Phoenix_PT-1,5-12-3.5-H_1x12_P3.50mm_Horizontal
Terminal Block Phoenix PT-1,5-12-3.5-H, 12 pins, pitch 3.5mm, size 42x7.6mm^2, drill diamater 1.2mm, pad diameter 2.4mm, see , script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_Phoenix
THT Terminal Block Phoenix PT-1,5-12-3.5-H pitch 3.5mm size 42x7.6mm^2 drill 1.2mm pad 2.4mm
0
12
12
TerminalBlock_Phoenix
TerminalBlock_Phoenix_PT-1,5-12-5.0-H_1x12_P5.00mm_Horizontal
Terminal Block Phoenix PT-1,5-12-5.0-H, 12 pins, pitch 5mm, size 60x9mm^2, drill diamater 1.3mm, pad diameter 2.6mm, see http://www.mouser.com/ds/2/324/ItemDetail_1935161-922578.pdf, script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_Phoenix
THT Terminal Block Phoenix PT-1,5-12-5.0-H pitch 5mm size 60x9mm^2 drill 1.3mm pad 2.6mm
0
12
12
TerminalBlock_Phoenix
TerminalBlock_Phoenix_PT-1,5-13-3.5-H_1x13_P3.50mm_Horizontal
Terminal Block Phoenix PT-1,5-13-3.5-H, 13 pins, pitch 3.5mm, size 45.5x7.6mm^2, drill diamater 1.2mm, pad diameter 2.4mm, see , script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_Phoenix
THT Terminal Block Phoenix PT-1,5-13-3.5-H pitch 3.5mm size 45.5x7.6mm^2 drill 1.2mm pad 2.4mm
0
13
13
TerminalBlock_Phoenix
TerminalBlock_Phoenix_PT-1,5-13-5.0-H_1x13_P5.00mm_Horizontal
Terminal Block Phoenix PT-1,5-13-5.0-H, 13 pins, pitch 5mm, size 65x9mm^2, drill diamater 1.3mm, pad diameter 2.6mm, see http://www.mouser.com/ds/2/324/ItemDetail_1935161-922578.pdf, script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_Phoenix
THT Terminal Block Phoenix PT-1,5-13-5.0-H pitch 5mm size 65x9mm^2 drill 1.3mm pad 2.6mm
0
13
13
TerminalBlock_Phoenix
TerminalBlock_Phoenix_PT-1,5-14-3.5-H_1x14_P3.50mm_Horizontal
Terminal Block Phoenix PT-1,5-14-3.5-H, 14 pins, pitch 3.5mm, size 49x7.6mm^2, drill diamater 1.2mm, pad diameter 2.4mm, see , script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_Phoenix
THT Terminal Block Phoenix PT-1,5-14-3.5-H pitch 3.5mm size 49x7.6mm^2 drill 1.2mm pad 2.4mm
0
14
14
TerminalBlock_Phoenix
TerminalBlock_Phoenix_PT-1,5-14-5.0-H_1x14_P5.00mm_Horizontal
Terminal Block Phoenix PT-1,5-14-5.0-H, 14 pins, pitch 5mm, size 70x9mm^2, drill diamater 1.3mm, pad diameter 2.6mm, see http://www.mouser.com/ds/2/324/ItemDetail_1935161-922578.pdf, script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_Phoenix
THT Terminal Block Phoenix PT-1,5-14-5.0-H pitch 5mm size 70x9mm^2 drill 1.3mm pad 2.6mm
0
14
14
TerminalBlock_Phoenix
TerminalBlock_Phoenix_PT-1,5-15-3.5-H_1x15_P3.50mm_Horizontal
Terminal Block Phoenix PT-1,5-15-3.5-H, 15 pins, pitch 3.5mm, size 52.5x7.6mm^2, drill diamater 1.2mm, pad diameter 2.4mm, see , script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_Phoenix
THT Terminal Block Phoenix PT-1,5-15-3.5-H pitch 3.5mm size 52.5x7.6mm^2 drill 1.2mm pad 2.4mm
0
15
15
TerminalBlock_Phoenix
TerminalBlock_Phoenix_PT-1,5-15-5.0-H_1x15_P5.00mm_Horizontal
Terminal Block Phoenix PT-1,5-15-5.0-H, 15 pins, pitch 5mm, size 75x9mm^2, drill diamater 1.3mm, pad diameter 2.6mm, see http://www.mouser.com/ds/2/324/ItemDetail_1935161-922578.pdf, script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_Phoenix
THT Terminal Block Phoenix PT-1,5-15-5.0-H pitch 5mm size 75x9mm^2 drill 1.3mm pad 2.6mm
0
15
15
TerminalBlock_Phoenix
TerminalBlock_Phoenix_PT-1,5-16-3.5-H_1x16_P3.50mm_Horizontal
Terminal Block Phoenix PT-1,5-16-3.5-H, 16 pins, pitch 3.5mm, size 56x7.6mm^2, drill diamater 1.2mm, pad diameter 2.4mm, see , script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_Phoenix
THT Terminal Block Phoenix PT-1,5-16-3.5-H pitch 3.5mm size 56x7.6mm^2 drill 1.2mm pad 2.4mm
0
16
16
TerminalBlock_Phoenix
TerminalBlock_Phoenix_PT-1,5-16-5.0-H_1x16_P5.00mm_Horizontal
Terminal Block Phoenix PT-1,5-16-5.0-H, 16 pins, pitch 5mm, size 80x9mm^2, drill diamater 1.3mm, pad diameter 2.6mm, see http://www.mouser.com/ds/2/324/ItemDetail_1935161-922578.pdf, script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_Phoenix
THT Terminal Block Phoenix PT-1,5-16-5.0-H pitch 5mm size 80x9mm^2 drill 1.3mm pad 2.6mm
0
16
16
TerminalBlock_Phoenix
TerminalBlock_Phoenix_PTSM-0,5-2-2,5-V-SMD_1x02-1MP_P2.50mm_Vertical
PhoenixContact PTSM0,5 2 2,5mm vertical SMD spring clamp terminal block connector http://www.phoenixcontact.com/us/products/1814702/pdf
PhoenixContact PTSM0.5 2 2.5mm vertical SMD spring clamp terminal block connector 
0
4
3
TerminalBlock_Phoenix
TerminalBlock_Phoenix_PTSM-0,5-2-2.5-H-THR_1x02_P2.50mm_Horizontal
Terminal Block Phoenix PTSM-0,5-2-2.5-H-THR, 2 pins, pitch 2.5mm, size 7.2x10mm^2, drill diamater 1.2mm, pad diameter 3mm, see http://www.produktinfo.conrad.com/datenblaetter/550000-574999/556441-da-01-de-LEITERPLATTENKL__PTSM_0_5__8_2_5_H_THR.pdf, script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_Phoenix
THT Terminal Block Phoenix PTSM-0,5-2-2.5-H-THR pitch 2.5mm size 7.2x10mm^2 drill 1.2mm pad 3mm
0
4
2
TerminalBlock_Phoenix
TerminalBlock_Phoenix_PTSM-0,5-2-2.5-V-THR_1x02_P2.50mm_Vertical
Terminal Block Phoenix PTSM-0,5-2-2.5-V-THR, vertical (cable from top), 2 pins, pitch 2.5mm, size 5.5x5mm^2, drill diamater 1.2mm, pad diameter 2mm, see http://www.produktinfo.conrad.com/datenblaetter/550000-574999/556444-da-01-de-LEITERPLATTENKL__PTSM_0_5__4_2_5_V_THR.pdf, script-generated with , script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_Phoenix
THT Terminal Block Phoenix PTSM-0,5-2-2.5-V-THR vertical pitch 2.5mm size 5.5x5mm^2 drill 1.2mm pad 2mm
0
4
2
TerminalBlock_Phoenix
TerminalBlock_Phoenix_PTSM-0,5-2-HV-2.5-SMD_1x02-1MP_P2.50mm_Vertical
PhoenixContact PTSM0,5 2 HV 2,5mm vertical SMD spring clamp terminal block connector http://www.phoenixcontact.com/us/products/1778696/pdf
2.5mm vertical SMD spring clamp terminal block connector 
0
4
3
TerminalBlock_Phoenix
TerminalBlock_Phoenix_PTSM-0,5-3-2,5-V-SMD_1x03-1MP_P2.50mm_Vertical
PhoenixContact PTSM0,5 3 2,5mm vertical SMD spring clamp terminal block connector http://www.phoenixcontact.com/us/products/1814715/pdf
PhoenixContact PTSM0.5 3 2.5mm vertical SMD spring clamp terminal block connector 
0
5
4
TerminalBlock_Phoenix
TerminalBlock_Phoenix_PTSM-0,5-3-2.5-H-THR_1x03_P2.50mm_Horizontal
Terminal Block Phoenix PTSM-0,5-3-2.5-H-THR, 3 pins, pitch 2.5mm, size 9.7x10mm^2, drill diamater 1.2mm, pad diameter 3mm, see http://www.produktinfo.conrad.com/datenblaetter/550000-574999/556441-da-01-de-LEITERPLATTENKL__PTSM_0_5__8_2_5_H_THR.pdf, script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_Phoenix
THT Terminal Block Phoenix PTSM-0,5-3-2.5-H-THR pitch 2.5mm size 9.7x10mm^2 drill 1.2mm pad 3mm
0
6
3
TerminalBlock_Phoenix
TerminalBlock_Phoenix_PTSM-0,5-3-2.5-V-THR_1x03_P2.50mm_Vertical
Terminal Block Phoenix PTSM-0,5-3-2.5-V-THR, vertical (cable from top), 3 pins, pitch 2.5mm, size 8x5mm^2, drill diamater 1.2mm, pad diameter 2mm, see http://www.produktinfo.conrad.com/datenblaetter/550000-574999/556444-da-01-de-LEITERPLATTENKL__PTSM_0_5__4_2_5_V_THR.pdf, script-generated with , script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_Phoenix
THT Terminal Block Phoenix PTSM-0,5-3-2.5-V-THR vertical pitch 2.5mm size 8x5mm^2 drill 1.2mm pad 2mm
0
6
3
TerminalBlock_Phoenix
TerminalBlock_Phoenix_PTSM-0,5-3-HV-2.5-SMD_1x03-1MP_P2.50mm_Vertical
PhoenixContact PTSM0,5 3 HV 2,5mm vertical SMD spring clamp terminal block connector http://www.phoenixcontact.com/us/products/1778706/pdf
2.5mm vertical SMD spring clamp terminal block connector 
0
5
4
TerminalBlock_Phoenix
TerminalBlock_Phoenix_PTSM-0,5-4-2,5-V-SMD_1x04-1MP_P2.50mm_Vertical
PhoenixContact PTSM0,5 4 2,5mm vertical SMD spring clamp terminal block connector http://www.phoenixcontact.com/us/products/1814728/pdf
PhoenixContact PTSM0.5 4 2.5mm vertical SMD spring clamp terminal block connector 
0
6
5
TerminalBlock_Phoenix
TerminalBlock_Phoenix_PTSM-0,5-4-2.5-H-THR_1x04_P2.50mm_Horizontal
Terminal Block Phoenix PTSM-0,5-4-2.5-H-THR, 4 pins, pitch 2.5mm, size 12.2x10mm^2, drill diamater 1.2mm, pad diameter 3mm, see http://www.produktinfo.conrad.com/datenblaetter/550000-574999/556441-da-01-de-LEITERPLATTENKL__PTSM_0_5__8_2_5_H_THR.pdf, script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_Phoenix
THT Terminal Block Phoenix PTSM-0,5-4-2.5-H-THR pitch 2.5mm size 12.2x10mm^2 drill 1.2mm pad 3mm
0
8
4
TerminalBlock_Phoenix
TerminalBlock_Phoenix_PTSM-0,5-4-2.5-V-THR_1x04_P2.50mm_Vertical
Terminal Block Phoenix PTSM-0,5-4-2.5-V-THR, vertical (cable from top), 4 pins, pitch 2.5mm, size 10.5x5mm^2, drill diamater 1.2mm, pad diameter 2mm, see http://www.produktinfo.conrad.com/datenblaetter/550000-574999/556444-da-01-de-LEITERPLATTENKL__PTSM_0_5__4_2_5_V_THR.pdf, script-generated with , script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_Phoenix
THT Terminal Block Phoenix PTSM-0,5-4-2.5-V-THR vertical pitch 2.5mm size 10.5x5mm^2 drill 1.2mm pad 2mm
0
8
4
TerminalBlock_Phoenix
TerminalBlock_Phoenix_PTSM-0,5-4-HV-2.5-SMD_1x04-1MP_P2.50mm_Vertical
PhoenixContact PTSM0,5 4 HV 2,5mm vertical SMD spring clamp terminal block connector http://www.phoenixcontact.com/us/products/1778719/pdf
2.5mm vertical SMD spring clamp terminal block connector 
0
4
3
TerminalBlock_Phoenix
TerminalBlock_Phoenix_PTSM-0,5-5-2,5-V-SMD_1x05-1MP_P2.50mm_Vertical
PhoenixContact PTSM0,5 5 2,5mm vertical SMD spring clamp terminal block connector http://www.phoenixcontact.com/us/products/1814731/pdf
PhoenixContact PTSM0.5 5 2.5mm vertical SMD spring clamp terminal block connector 
0
7
6
TerminalBlock_Phoenix
TerminalBlock_Phoenix_PTSM-0,5-5-2.5-H-THR_1x05_P2.50mm_Horizontal
Terminal Block Phoenix PTSM-0,5-5-2.5-H-THR, 5 pins, pitch 2.5mm, size 14.7x10mm^2, drill diamater 1.2mm, pad diameter 3mm, see http://www.produktinfo.conrad.com/datenblaetter/550000-574999/556441-da-01-de-LEITERPLATTENKL__PTSM_0_5__8_2_5_H_THR.pdf, script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_Phoenix
THT Terminal Block Phoenix PTSM-0,5-5-2.5-H-THR pitch 2.5mm size 14.7x10mm^2 drill 1.2mm pad 3mm
0
10
5
TerminalBlock_Phoenix
TerminalBlock_Phoenix_PTSM-0,5-5-2.5-V-THR_1x05_P2.50mm_Vertical
Terminal Block Phoenix PTSM-0,5-5-2.5-V-THR, vertical (cable from top), 5 pins, pitch 2.5mm, size 13x5mm^2, drill diamater 1.2mm, pad diameter 2mm, see http://www.produktinfo.conrad.com/datenblaetter/550000-574999/556444-da-01-de-LEITERPLATTENKL__PTSM_0_5__4_2_5_V_THR.pdf, script-generated with , script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_Phoenix
THT Terminal Block Phoenix PTSM-0,5-5-2.5-V-THR vertical pitch 2.5mm size 13x5mm^2 drill 1.2mm pad 2mm
0
10
5
TerminalBlock_Phoenix
TerminalBlock_Phoenix_PTSM-0,5-5-HV-2.5-SMD_1x05-1MP_P2.50mm_Vertical
PhoenixContact PTSM0,5 5 HV 2,5mm vertical SMD spring clamp terminal block connector http://www.phoenixcontact.com/us/products/1778722/pdf
2.5mm vertical SMD spring clamp terminal block connector 
0
7
6
TerminalBlock_Phoenix
TerminalBlock_Phoenix_PTSM-0,5-6-2,5-V-SMD_1x06-1MP_P2.50mm_Vertical
PhoenixContact PTSM0,5 6 2,5mm vertical SMD spring clamp terminal block connector http://www.phoenixcontact.com/us/products/1814744/pdf
PhoenixContact PTSM0.5 6 2.5mm vertical SMD spring clamp terminal block connector 
0
8
7
TerminalBlock_Phoenix
TerminalBlock_Phoenix_PTSM-0,5-6-2.5-H-THR_1x06_P2.50mm_Horizontal
Terminal Block Phoenix PTSM-0,5-6-2.5-H-THR, 6 pins, pitch 2.5mm, size 17.2x10mm^2, drill diamater 1.2mm, pad diameter 3mm, see http://www.produktinfo.conrad.com/datenblaetter/550000-574999/556441-da-01-de-LEITERPLATTENKL__PTSM_0_5__8_2_5_H_THR.pdf, script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_Phoenix
THT Terminal Block Phoenix PTSM-0,5-6-2.5-H-THR pitch 2.5mm size 17.2x10mm^2 drill 1.2mm pad 3mm
0
12
6
TerminalBlock_Phoenix
TerminalBlock_Phoenix_PTSM-0,5-6-2.5-V-THR_1x06_P2.50mm_Vertical
Terminal Block Phoenix PTSM-0,5-6-2.5-V-THR, vertical (cable from top), 6 pins, pitch 2.5mm, size 15.5x5mm^2, drill diamater 1.2mm, pad diameter 2mm, see http://www.produktinfo.conrad.com/datenblaetter/550000-574999/556444-da-01-de-LEITERPLATTENKL__PTSM_0_5__4_2_5_V_THR.pdf, script-generated with , script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_Phoenix
THT Terminal Block Phoenix PTSM-0,5-6-2.5-V-THR vertical pitch 2.5mm size 15.5x5mm^2 drill 1.2mm pad 2mm
0
12
6
TerminalBlock_Phoenix
TerminalBlock_Phoenix_PTSM-0,5-6-HV-2.5-SMD_1x06-1MP_P2.50mm_Vertical
PhoenixContact PTSM0,5 6 HV 2,5mm vertical SMD spring clamp terminal block connector http://www.phoenixcontact.com/us/products/1778735/pdf
2.5mm vertical SMD spring clamp terminal block connector 
0
8
7
TerminalBlock_Phoenix
TerminalBlock_Phoenix_PTSM-0,5-7-2,5-V-SMD_1x07-1MP_P2.50mm_Vertical
PhoenixContact PTSM0,5 7 2,5mm vertical SMD spring clamp terminal block connector http://www.phoenixcontact.com/us/products/1814757/pdf
PhoenixContact PTSM0.5 7 2.5mm vertical SMD spring clamp terminal block connector 
0
9
8
TerminalBlock_Phoenix
TerminalBlock_Phoenix_PTSM-0,5-7-2.5-H-THR_1x07_P2.50mm_Horizontal
Terminal Block Phoenix PTSM-0,5-7-2.5-H-THR, 7 pins, pitch 2.5mm, size 19.7x10mm^2, drill diamater 1.2mm, pad diameter 3mm, see http://www.produktinfo.conrad.com/datenblaetter/550000-574999/556441-da-01-de-LEITERPLATTENKL__PTSM_0_5__8_2_5_H_THR.pdf, script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_Phoenix
THT Terminal Block Phoenix PTSM-0,5-7-2.5-H-THR pitch 2.5mm size 19.7x10mm^2 drill 1.2mm pad 3mm
0
14
7
TerminalBlock_Phoenix
TerminalBlock_Phoenix_PTSM-0,5-7-2.5-V-THR_1x07_P2.50mm_Vertical
Terminal Block Phoenix PTSM-0,5-7-2.5-V-THR, vertical (cable from top), 7 pins, pitch 2.5mm, size 18x5mm^2, drill diamater 1.2mm, pad diameter 2mm, see http://www.produktinfo.conrad.com/datenblaetter/550000-574999/556444-da-01-de-LEITERPLATTENKL__PTSM_0_5__4_2_5_V_THR.pdf, script-generated with , script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_Phoenix
THT Terminal Block Phoenix PTSM-0,5-7-2.5-V-THR vertical pitch 2.5mm size 18x5mm^2 drill 1.2mm pad 2mm
0
14
7
TerminalBlock_Phoenix
TerminalBlock_Phoenix_PTSM-0,5-7-HV-2.5-SMD_1x07-1MP_P2.50mm_Vertical
PhoenixContact PTSM0,5 7 HV 2,5mm vertical SMD spring clamp terminal block connector http://www.phoenixcontact.com/us/products/1778748/pdf
2.5mm vertical SMD spring clamp terminal block connector 
0
9
8
TerminalBlock_Phoenix
TerminalBlock_Phoenix_PTSM-0,5-8-2,5-V-SMD_1x08-1MP_P2.50mm_Vertical
PhoenixContact PTSM0,5 8 2,5mm vertical SMD spring clamp terminal block connector http://www.phoenixcontact.com/us/products/1814760/pdf
PhoenixContact PTSM0.5 8 2.5mm vertical SMD spring clamp terminal block connector 
0
10
9
TerminalBlock_Phoenix
TerminalBlock_Phoenix_PTSM-0,5-8-2.5-H-THR_1x08_P2.50mm_Horizontal
Terminal Block Phoenix PTSM-0,5-8-2.5-H-THR, 8 pins, pitch 2.5mm, size 22.2x10mm^2, drill diamater 1.2mm, pad diameter 3mm, see http://www.produktinfo.conrad.com/datenblaetter/550000-574999/556441-da-01-de-LEITERPLATTENKL__PTSM_0_5__8_2_5_H_THR.pdf, script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_Phoenix
THT Terminal Block Phoenix PTSM-0,5-8-2.5-H-THR pitch 2.5mm size 22.2x10mm^2 drill 1.2mm pad 3mm
0
16
8
TerminalBlock_Phoenix
TerminalBlock_Phoenix_PTSM-0,5-8-2.5-V-THR_1x08_P2.50mm_Vertical
Terminal Block Phoenix PTSM-0,5-8-2.5-V-THR, vertical (cable from top), 8 pins, pitch 2.5mm, size 20.5x5mm^2, drill diamater 1.2mm, pad diameter 2mm, see http://www.produktinfo.conrad.com/datenblaetter/550000-574999/556444-da-01-de-LEITERPLATTENKL__PTSM_0_5__4_2_5_V_THR.pdf, script-generated with , script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_Phoenix
THT Terminal Block Phoenix PTSM-0,5-8-2.5-V-THR vertical pitch 2.5mm size 20.5x5mm^2 drill 1.2mm pad 2mm
0
16
8
TerminalBlock_Phoenix
TerminalBlock_Phoenix_PTSM-0,5-8-HV-2.5-SMD_1x08-1MP_P2.50mm_Vertical
PhoenixContact PTSM0,5 8 HV 2,5mm vertical SMD spring clamp terminal block connector http://www.phoenixcontact.com/us/products/1778751/pdf
2.5mm vertical SMD spring clamp terminal block connector 
0
10
9
my_footprints
B0x0xS


0
4
4
my_footprints
Hole_3mm


0
1
1
