(kicad_symbol_lib (version 20220914) (generator kicad_symbol_editor)
  (symbol "ZXCT1009" (in_bom yes) (on_board yes)
    (property "Reference" "U" (at 0 5.08 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "ZXCT1009" (at 0 -5.08 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "Package_TO_SOT_SMD:SOT-23_Handsoldering" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "High side current sensor 1mA/100mV" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "ZXCT1009_0_0"
      (text "" (at 0 -6.35 0)
        (effects (font (size 1.27 1.27)))
      )
    )
    (symbol "ZXCT1009_0_1"
      (rectangle (start -3.81 3.81) (end 3.81 -3.81)
        (stroke (width 0) (type default))
        (fill (type none))
      )
    )
    (symbol "ZXCT1009_1_1"
      (pin passive line (at -8.89 2.54 0) (length 5.08)
        (name "-" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at -8.89 -2.54 0) (length 5.08)
        (name "+" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 8.89 0 180) (length 5.08)
        (name "sense" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
    )
  )
)
