(export (version D)
  (design
    (source /home/eddy/Yandex.Disk/Projects/stm32samples/F0-nolib/Socket_fans/kicad/stm32.sch)
    (date "Пн 02 ноя 2020 23:57:15")
    (tool "Eeschema 5.1.6")
    (sheet (number 1) (name /) (tstamps /)
      (title_block
        (title)
        (company)
        (rev)
        (date)
        (source stm32.sch)
        (comment (number 1) (value ""))
        (comment (number 2) (value ""))
        (comment (number 3) (value ""))
        (comment (number 4) (value "")))))
  (components
    (comp (ref C15)
      (value 0.1)
      (footprint Capacitor_SMD:C_0603_1608Metric_Pad1.05x0.95mm_HandSolder)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /) (tstamps /))
      (tstamp 58C42D39))
    (comp (ref U1)
      (value LM1117-3.3)
      (footprint Package_TO_SOT_SMD:SOT-223-3_TabPin2)
      (libsource (lib Regulator_Linear) (part LM1117-3.3) (description "800mA Low-Dropout Linear Regulator, 3.3V fixed output, TO-220/TO-252/TO-263/SOT-223"))
      (sheetpath (names /) (tstamps /))
      (tstamp 58C431FC))
    (comp (ref C17)
      (value 0.1)
      (footprint Capacitor_SMD:C_0603_1608Metric_Pad1.05x0.95mm_HandSolder)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /) (tstamps /))
      (tstamp 590935EA))
    (comp (ref C19)
      (value 0.1)
      (footprint Capacitor_SMD:C_0603_1608Metric_Pad1.05x0.95mm_HandSolder)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /) (tstamps /))
      (tstamp 59093675))
    (comp (ref R27)
      (value 1k)
      (footprint Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 590A6DDA))
    (comp (ref R28)
      (value 4.7k)
      (footprint Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 590A6F68))
    (comp (ref R29)
      (value 4.7k)
      (footprint Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 590A6F6E))
    (comp (ref P5)
      (value Hole)
      (footprint MountingHole:MountingHole_3.2mm_M3)
      (libsource (lib Connector_Generic) (part Conn_01x01) (description "Generic connector, single row, 01x01, script generated (kicad-library-utils/schlib/autogen/connector/)"))
      (sheetpath (names /) (tstamps /))
      (tstamp 59143415))
    (comp (ref P4)
      (value Hole)
      (footprint MountingHole:MountingHole_3.2mm_M3)
      (libsource (lib Connector_Generic) (part Conn_01x01) (description "Generic connector, single row, 01x01, script generated (kicad-library-utils/schlib/autogen/connector/)"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5914456D))
    (comp (ref P2)
      (value Hole)
      (footprint MountingHole:MountingHole_3.2mm_M3)
      (libsource (lib Connector_Generic) (part Conn_01x01) (description "Generic connector, single row, 01x01, script generated (kicad-library-utils/schlib/autogen/connector/)"))
      (sheetpath (names /) (tstamps /))
      (tstamp 591446F3))
    (comp (ref P3)
      (value Hole)
      (footprint MountingHole:MountingHole_3.2mm_M3)
      (libsource (lib Connector_Generic) (part Conn_01x01) (description "Generic connector, single row, 01x01, script generated (kicad-library-utils/schlib/autogen/connector/)"))
      (sheetpath (names /) (tstamps /))
      (tstamp 591446F9))
    (comp (ref D7)
      (value MM3Z4V3)
      (footprint Diode_SMD:D_0805_2012Metric_Pad1.15x1.40mm_HandSolder)
      (libsource (lib Device) (part D_Zener) (description "Zener diode"))
      (sheetpath (names /) (tstamps /))
      (tstamp 59684468))
    (comp (ref R30)
      (value 22)
      (footprint Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5968E385))
    (comp (ref R31)
      (value 22)
      (footprint Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5968E83B))
    (comp (ref D1)
      (value 1N5819)
      (footprint Diode_SMD:D_SOD-323_HandSoldering)
      (libsource (lib Device) (part D_Schottky) (description "Schottky diode"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E615086))
    (comp (ref C6)
      (value 0.1)
      (footprint Capacitor_SMD:C_0603_1608Metric_Pad1.05x0.95mm_HandSolder)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E7836BE))
    (comp (ref C7)
      (value "47uF, 10V")
      (footprint Capacitor_Tantalum_SMD:CP_EIA-6032-28_Kemet-C_Pad2.25x2.35mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part CP) (description "Polarized capacitor"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E794E88))
    (comp (ref R22)
      (value 47k)
      (footprint Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 590D30C8))
    (comp (ref R23)
      (value 22)
      (footprint Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5EA6930E))
    (comp (ref C18)
      (value 0.1)
      (footprint Capacitor_SMD:C_0603_1608Metric_Pad1.05x0.95mm_HandSolder)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E417130))
    (comp (ref C16)
      (value 0.1)
      (footprint Capacitor_SMD:C_0603_1608Metric_Pad1.05x0.95mm_HandSolder)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E42F960))
    (comp (ref C20)
      (value 0.1)
      (footprint Capacitor_SMD:C_0603_1608Metric_Pad1.05x0.95mm_HandSolder)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /) (tstamps /))
      (tstamp 590A8102))
    (comp (ref R1)
      (value 10k)
      (footprint Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5ED7FE5E))
    (comp (ref D3)
      (value MM3Z7V5)
      (footprint Diode_SMD:D_0805_2012Metric_Pad1.15x1.40mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part D_Zener) (description "Zener diode"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5ED78D2C))
    (comp (ref Q1)
      (value AO3401)
      (footprint Package_TO_SOT_SMD:SOT-23_Handsoldering)
      (libsource (lib Device) (part Q_PMOS_GSD) (description "P-MOSFET transistor, gate/source/drain"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5910E2F2))
    (comp (ref J1)
      (value 12VIN)
      (footprint TerminalBlock_Phoenix:TerminalBlock_Phoenix_MKDS-1,5-2_1x02_P5.00mm_Horizontal)
      (libsource (lib stm32-rescue) (part Conn_01x02-Chiller_control-rescue) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5A170C1F))
    (comp (ref R14)
      (value 10k)
      (footprint Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder)
      (libsource (lib stm32-rescue) (part R-Chiller_control-rescue) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5BEEBD18))
    (comp (ref R11)
      (value 510)
      (footprint Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder)
      (libsource (lib stm32-rescue) (part R-Chiller_control-rescue) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5BEEBD1E))
    (comp (ref Q4)
      (value IRLML2502)
      (footprint Package_TO_SOT_SMD:SOT-23_Handsoldering)
      (libsource (lib stm32-rescue) (part Q_NMOS_GSD-Chiller_control-rescue) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5BEEB585))
    (comp (ref R12)
      (value 510)
      (footprint Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder)
      (libsource (lib stm32-rescue) (part R-Chiller_control-rescue) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5BEEB37B))
    (comp (ref R16)
      (value 10k)
      (footprint Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder)
      (libsource (lib stm32-rescue) (part R-Chiller_control-rescue) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5BEEB2E1))
    (comp (ref L1)
      (value "BMBA 0.1mH")
      (footprint Inductor_SMD:L_0805_2012Metric_Pad1.15x1.40mm_HandSolder)
      (libsource (lib stm32-rescue) (part L-Chiller_control-rescue) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5F7F79F1))
    (comp (ref U2)
      (value L7805)
      (footprint Package_TO_SOT_THT:TO-220-3_Vertical)
      (datasheet http://www.st.com/content/ccc/resource/technical/document/datasheet/41/4f/b3/b0/12/d4/47/88/CD00000444.pdf/files/CD00000444.pdf/jcr:content/translations/en.CD00000444.pdf)
      (libsource (lib Regulator_Linear) (part L7805) (description "Positive 1.5A 35V Linear Regulator, Fixed Output 5V, TO-220/TO-263/TO-252"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5F943ABE))
    (comp (ref C3)
      (value 0.1)
      (footprint Capacitor_SMD:C_0603_1608Metric_Pad1.05x0.95mm_HandSolder)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /) (tstamps /))
      (tstamp 596772D4))
    (comp (ref C8)
      (value 0.1)
      (footprint Capacitor_SMD:C_0603_1608Metric_Pad1.05x0.95mm_HandSolder)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5A586F5C))
    (comp (ref C9)
      (value "10uF, 10V")
      (footprint Capacitor_SMD:C_1206_3216Metric_Pad1.42x1.75mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E5E1875))
    (comp (ref C5)
      (value 0.1)
      (footprint Capacitor_SMD:C_0603_1608Metric_Pad1.05x0.95mm_HandSolder)
      (libsource (lib stm32-rescue) (part C-Chiller_control-rescue) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5FA122F0))
    (comp (ref R2)
      (value 10k)
      (footprint Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder)
      (libsource (lib stm32-rescue) (part R-Chiller_control-rescue) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5FA12E95))
    (comp (ref R9)
      (value "4k7, 1%")
      (footprint Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder)
      (libsource (lib stm32-rescue) (part R-Chiller_control-rescue) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5FA11765))
    (comp (ref R7)
      (value "4k7, 1%")
      (footprint Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder)
      (libsource (lib stm32-rescue) (part R-Chiller_control-rescue) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5FA113CB))
    (comp (ref R5)
      (value "4k7, 1%")
      (footprint Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder)
      (libsource (lib stm32-rescue) (part R-Chiller_control-rescue) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5FA110F3))
    (comp (ref R3)
      (value "4k7, 1%")
      (footprint Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder)
      (libsource (lib stm32-rescue) (part R-Chiller_control-rescue) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5BEF45BA))
    (comp (ref R4)
      (value 10k)
      (footprint Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder)
      (libsource (lib stm32-rescue) (part R-Chiller_control-rescue) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5FA5AE90))
    (comp (ref R6)
      (value 10k)
      (footprint Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder)
      (libsource (lib stm32-rescue) (part R-Chiller_control-rescue) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5FA5BA50))
    (comp (ref R8)
      (value 10k)
      (footprint Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder)
      (libsource (lib stm32-rescue) (part R-Chiller_control-rescue) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5FA5BCFF))
    (comp (ref C4)
      (value 0.1)
      (footprint Capacitor_SMD:C_0603_1608Metric_Pad1.05x0.95mm_HandSolder)
      (libsource (lib stm32-rescue) (part C-Chiller_control-rescue) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5FA120D2))
    (comp (ref C2)
      (value 0.1)
      (footprint Capacitor_SMD:C_0603_1608Metric_Pad1.05x0.95mm_HandSolder)
      (libsource (lib stm32-rescue) (part C-Chiller_control-rescue) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5FA11F4D))
    (comp (ref C1)
      (value 0.1)
      (footprint Capacitor_SMD:C_0603_1608Metric_Pad1.05x0.95mm_HandSolder)
      (libsource (lib stm32-rescue) (part C-Chiller_control-rescue) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C5D51AF))
    (comp (ref R26)
      (value 3.3k)
      (footprint Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 590A6DD4))
    (comp (ref R17)
      (value 10k)
      (footprint Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder)
      (libsource (lib stm32-rescue) (part R-Chiller_control-rescue) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5F4074BF))
    (comp (ref R15)
      (value 510)
      (footprint Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder)
      (libsource (lib stm32-rescue) (part R-Chiller_control-rescue) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5F4074C5))
    (comp (ref Q5)
      (value IRLML2502)
      (footprint Package_TO_SOT_SMD:SOT-23_Handsoldering)
      (libsource (lib stm32-rescue) (part Q_NMOS_GSD-Chiller_control-rescue) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5F4074CB))
    (comp (ref U4)
      (value USBLC6-2SC6)
      (footprint Package_TO_SOT_SMD:SOT-23-6)
      (datasheet http://www2.st.com/resource/en/datasheet/CD00050750.pdf)
      (libsource (lib Power_Protection) (part USBLC6-2SC6) (description "Bidirectional ESD Protection Diode, SOT-23-6"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5F40EDD5))
    (comp (ref D2)
      (value 1N5819)
      (footprint Diode_SMD:D_SOD-323_HandSoldering)
      (libsource (lib Device) (part D_Schottky) (description "Schottky diode"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5F44DDD5))
    (comp (ref J4)
      (value cooler3)
      (footprint Connector_JST:JST_EH_B2B-EH-A_1x02_P2.50mm_Vertical)
      (datasheet ~)
      (libsource (lib Connector) (part Conn_01x02_Male) (description "Generic connector, single row, 01x02, script generated (kicad-library-utils/schlib/autogen/connector/)"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5F4058DC))
    (comp (ref J6)
      (value FAN)
      (footprint Connector:FanPinHeader_1x04_P2.54mm_Vertical)
      (datasheet ~)
      (libsource (lib Connector) (part Conn_01x04_Male) (description "Generic connector, single row, 01x04, script generated (kicad-library-utils/schlib/autogen/connector/)"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5F424D72))
    (comp (ref J3)
      (value Buzzer)
      (footprint Connector_JST:JST_EH_B2B-EH-A_1x02_P2.50mm_Vertical)
      (datasheet ~)
      (libsource (lib Connector) (part Conn_01x02_Male) (description "Generic connector, single row, 01x02, script generated (kicad-library-utils/schlib/autogen/connector/)"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5F4397CD))
    (comp (ref D5)
      (value 1N5819)
      (footprint Diode_SMD:D_SOD-323_HandSoldering)
      (libsource (lib Device) (part D_Schottky) (description "Schottky diode"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5F48E038))
    (comp (ref R19)
      (value 510)
      (footprint Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder)
      (libsource (lib stm32-rescue) (part R-Chiller_control-rescue) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5F4CEB3C))
    (comp (ref R21)
      (value 510)
      (footprint Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder)
      (libsource (lib stm32-rescue) (part R-Chiller_control-rescue) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5F4CF586))
    (comp (ref D6)
      (value 1N5819)
      (footprint Diode_SMD:D_SOD-323_HandSoldering)
      (libsource (lib Device) (part D_Schottky) (description "Schottky diode"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5F4E7DE3))
    (comp (ref R13)
      (value 10k)
      (footprint Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder)
      (libsource (lib stm32-rescue) (part R-Chiller_control-rescue) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5F506974))
    (comp (ref R10)
      (value 510)
      (footprint Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder)
      (libsource (lib stm32-rescue) (part R-Chiller_control-rescue) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5F50697A))
    (comp (ref J5)
      (value FAN)
      (footprint Connector:FanPinHeader_1x04_P2.54mm_Vertical)
      (datasheet ~)
      (libsource (lib Connector) (part Conn_01x04_Male) (description "Generic connector, single row, 01x04, script generated (kicad-library-utils/schlib/autogen/connector/)"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5F5069A0))
    (comp (ref D4)
      (value 1N5819)
      (footprint Diode_SMD:D_SOD-323_HandSoldering)
      (libsource (lib Device) (part D_Schottky) (description "Schottky diode"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5F5069A8))
    (comp (ref R18)
      (value 510)
      (footprint Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder)
      (libsource (lib stm32-rescue) (part R-Chiller_control-rescue) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5F5069B5))
    (comp (ref R20)
      (value 510)
      (footprint Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder)
      (libsource (lib stm32-rescue) (part R-Chiller_control-rescue) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5F5069BB))
    (comp (ref SW1)
      (value SW_Push)
      (footprint Connector_PinSocket_2.54mm:PinSocket_1x02_P2.54mm_Vertical)
      (datasheet ~)
      (libsource (lib Switch) (part SW_Push) (description "Push button switch, generic, two pins"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5F40AE40))
    (comp (ref SW2)
      (value SW_Push)
      (footprint Connector_PinSocket_2.54mm:PinSocket_1x02_P2.54mm_Vertical)
      (datasheet ~)
      (libsource (lib Switch) (part SW_Push) (description "Push button switch, generic, two pins"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5F40BE17))
    (comp (ref R24)
      (value 510)
      (footprint Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder)
      (libsource (lib stm32-rescue) (part R-Chiller_control-rescue) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5F4227FB))
    (comp (ref C13)
      (value 0.1)
      (footprint Capacitor_SMD:C_0603_1608Metric_Pad1.05x0.95mm_HandSolder)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5F43976C))
    (comp (ref C14)
      (value 0.1)
      (footprint Capacitor_SMD:C_0603_1608Metric_Pad1.05x0.95mm_HandSolder)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5F43A352))
    (comp (ref R25)
      (value 510)
      (footprint Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder)
      (libsource (lib stm32-rescue) (part R-Chiller_control-rescue) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5F423117))
    (comp (ref P1)
      (value USB_A)
      (footprint Connector_USB:USB_B_OST_USB-B1HSxx_Horizontal)
      (libsource (lib Connector) (part USB_B) (description "USB Type B connector"))
      (sheetpath (names /) (tstamps /))
      (tstamp 58C433D0))
    (comp (ref J2)
      (value thermal)
      (footprint Connector_PinSocket_2.54mm:PinSocket_2x04_P2.54mm_Vertical)
      (datasheet ~)
      (libsource (lib Connector_Generic) (part Conn_02x04_Odd_Even) (description "Generic connector, double row, 02x04, odd/even pin numbering scheme (row 1 odd numbers, row 2 even numbers), script generated (kicad-library-utils/schlib/autogen/connector/)"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5F9F47CC))
    (comp (ref J7)
      (value Conn_01x02_Female)
      (footprint Connector_PinSocket_2.54mm:PinSocket_1x02_P2.54mm_Vertical)
      (datasheet ~)
      (libsource (lib Connector) (part Conn_01x02_Female) (description "Generic connector, single row, 01x02, script generated (kicad-library-utils/schlib/autogen/connector/)"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5F670F02))
    (comp (ref J10)
      (value Conn_01x02_Female)
      (footprint Connector_PinSocket_2.54mm:PinSocket_1x02_P2.54mm_Vertical)
      (datasheet ~)
      (libsource (lib Connector) (part Conn_01x02_Female) (description "Generic connector, single row, 01x02, script generated (kicad-library-utils/schlib/autogen/connector/)"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5F67196D))
    (comp (ref U3)
      (value STM32F072CBTx)
      (footprint Package_QFP:LQFP-48_7x7mm_P0.5mm)
      (datasheet http://www.st.com/st-web-ui/static/active/en/resource/technical/document/datasheet/DM00090510.pdf)
      (libsource (lib MCU_ST_STM32F0) (part STM32F072CBTx) (description "ARM Cortex-M0 MCU, 128KB flash, 16KB RAM, 48MHz, 2-3.6V, 37 GPIO, LQFP-48"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E89EA8D))
    (comp (ref J8)
      (value MKDS)
      (footprint TerminalBlock_Phoenix:TerminalBlock_Phoenix_MKDS-1,5-2_1x02_P5.00mm_Horizontal)
      (datasheet ~)
      (libsource (lib Connector) (part Conn_01x02_Female) (description "Generic connector, single row, 01x02, script generated (kicad-library-utils/schlib/autogen/connector/)"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5F6401DC))
    (comp (ref D9)
      (value 1N5819)
      (footprint Diode_SMD:D_SOD-323_HandSoldering)
      (libsource (lib Device) (part D_Schottky) (description "Schottky diode"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5F45888F))
    (comp (ref Q6)
      (value IRLML2502)
      (footprint Package_TO_SOT_SMD:SOT-23_Handsoldering)
      (libsource (lib stm32-rescue) (part Q_NMOS_GSD-socket-rescue) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5F458885))
    (comp (ref K1)
      (value SRD-12VDC)
      (footprint Relay_THT:Relay_SPDT_SANYOU_SRD_Series_Form_C)
      (libsource (lib stm32-rescue) (part G5LE-1-socket-rescue) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5F458873))
    (comp (ref R34)
      (value 10k)
      (footprint Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder)
      (libsource (lib stm32-rescue) (part R-socket-rescue) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5F45886D))
    (comp (ref R32)
      (value 510)
      (footprint Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder)
      (libsource (lib stm32-rescue) (part R-socket-rescue) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5F458865))
    (comp (ref C10)
      (value "47u, 25V")
      (footprint Capacitor_THT:CP_Radial_D8.0mm_P3.50mm)
      (datasheet ~)
      (libsource (lib Device) (part CP) (description "Polarized capacitor"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5F97B2AC))
    (comp (ref Q2)
      (value IRLML2502)
      (footprint Package_TO_SOT_SMD:SOT-23_Handsoldering)
      (libsource (lib stm32-rescue) (part Q_NMOS_GSD-Chiller_control-rescue) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5F506980))
    (comp (ref Q3)
      (value IRLML2502)
      (footprint Package_TO_SOT_SMD:SOT-23_Handsoldering)
      (libsource (lib stm32-rescue) (part Q_NMOS_GSD-Chiller_control-rescue) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5BEEBD24))
    (comp (ref D10)
      (value MM3Z3V6)
      (footprint Diode_SMD:D_0805_2012Metric_Pad1.15x1.40mm_HandSolder)
      (libsource (lib Device) (part D_Zener) (description "Zener diode"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5FA13F5D))
    (comp (ref D8)
      (value MM3Z3V6)
      (footprint Diode_SMD:D_0805_2012Metric_Pad1.15x1.40mm_HandSolder)
      (libsource (lib Device) (part D_Zener) (description "Zener diode"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5FA2A4CC)))
  (libparts
    (libpart (lib Connector) (part Conn_01x02_Female)
      (description "Generic connector, single row, 01x02, script generated (kicad-library-utils/schlib/autogen/connector/)")
      (docs ~)
      (footprints
        (fp Connector*:*_1x??_*))
      (fields
        (field (name Reference) J)
        (field (name Value) Conn_01x02_Female))
      (pins
        (pin (num 1) (name Pin_1) (type passive))
        (pin (num 2) (name Pin_2) (type passive))))
    (libpart (lib Connector) (part Conn_01x02_Male)
      (description "Generic connector, single row, 01x02, script generated (kicad-library-utils/schlib/autogen/connector/)")
      (docs ~)
      (footprints
        (fp Connector*:*_1x??_*))
      (fields
        (field (name Reference) J)
        (field (name Value) Conn_01x02_Male))
      (pins
        (pin (num 1) (name Pin_1) (type passive))
        (pin (num 2) (name Pin_2) (type passive))))
    (libpart (lib Connector) (part Conn_01x04_Male)
      (description "Generic connector, single row, 01x04, script generated (kicad-library-utils/schlib/autogen/connector/)")
      (docs ~)
      (footprints
        (fp Connector*:*_1x??_*))
      (fields
        (field (name Reference) J)
        (field (name Value) Conn_01x04_Male))
      (pins
        (pin (num 1) (name Pin_1) (type passive))
        (pin (num 2) (name Pin_2) (type passive))
        (pin (num 3) (name Pin_3) (type passive))
        (pin (num 4) (name Pin_4) (type passive))))
    (libpart (lib Connector) (part USB_B)
      (description "USB Type B connector")
      (docs " ~")
      (footprints
        (fp USB*))
      (fields
        (field (name Reference) J)
        (field (name Value) USB_B))
      (pins
        (pin (num 1) (name VBUS) (type power_out))
        (pin (num 2) (name D-) (type passive))
        (pin (num 3) (name D+) (type passive))
        (pin (num 4) (name GND) (type power_out))
        (pin (num 5) (name Shield) (type passive))))
    (libpart (lib Connector_Generic) (part Conn_01x01)
      (description "Generic connector, single row, 01x01, script generated (kicad-library-utils/schlib/autogen/connector/)")
      (docs ~)
      (footprints
        (fp Connector*:*))
      (fields
        (field (name Reference) J)
        (field (name Value) Conn_01x01))
      (pins
        (pin (num 1) (name Pin_1) (type passive))))
    (libpart (lib Connector_Generic) (part Conn_02x04_Odd_Even)
      (description "Generic connector, double row, 02x04, odd/even pin numbering scheme (row 1 odd numbers, row 2 even numbers), script generated (kicad-library-utils/schlib/autogen/connector/)")
      (docs ~)
      (footprints
        (fp Connector*:*_2x??_*))
      (fields
        (field (name Reference) J)
        (field (name Value) Conn_02x04_Odd_Even))
      (pins
        (pin (num 1) (name Pin_1) (type passive))
        (pin (num 2) (name Pin_2) (type passive))
        (pin (num 3) (name Pin_3) (type passive))
        (pin (num 4) (name Pin_4) (type passive))
        (pin (num 5) (name Pin_5) (type passive))
        (pin (num 6) (name Pin_6) (type passive))
        (pin (num 7) (name Pin_7) (type passive))
        (pin (num 8) (name Pin_8) (type passive))))
    (libpart (lib Device) (part C)
      (description "Unpolarized capacitor")
      (docs ~)
      (footprints
        (fp C_*))
      (fields
        (field (name Reference) C)
        (field (name Value) C))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib Device) (part CP)
      (description "Polarized capacitor")
      (docs ~)
      (footprints
        (fp CP_*))
      (fields
        (field (name Reference) C)
        (field (name Value) CP))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib Device) (part D_Schottky)
      (description "Schottky diode")
      (docs ~)
      (footprints
        (fp TO-???*)
        (fp *_Diode_*)
        (fp *SingleDiode*)
        (fp D_*))
      (fields
        (field (name Reference) D)
        (field (name Value) D_Schottky))
      (pins
        (pin (num 1) (name K) (type passive))
        (pin (num 2) (name A) (type passive))))
    (libpart (lib Device) (part D_Zener)
      (description "Zener diode")
      (docs ~)
      (footprints
        (fp TO-???*)
        (fp *_Diode_*)
        (fp *SingleDiode*)
        (fp D_*))
      (fields
        (field (name Reference) D)
        (field (name Value) D_Zener))
      (pins
        (pin (num 1) (name K) (type passive))
        (pin (num 2) (name A) (type passive))))
    (libpart (lib Device) (part Q_PMOS_GSD)
      (description "P-MOSFET transistor, gate/source/drain")
      (docs ~)
      (fields
        (field (name Reference) Q)
        (field (name Value) Q_PMOS_GSD))
      (pins
        (pin (num 1) (name G) (type input))
        (pin (num 2) (name S) (type passive))
        (pin (num 3) (name D) (type passive))))
    (libpart (lib Device) (part R)
      (description Resistor)
      (docs ~)
      (footprints
        (fp R_*))
      (fields
        (field (name Reference) R)
        (field (name Value) R))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib MCU_ST_STM32F0) (part STM32F072C8Tx)
      (aliases
        (alias STM32F072CBTx))
      (description "ARM Cortex-M0 MCU, 64KB flash, 16KB RAM, 48MHz, 2-3.6V, 37 GPIO, LQFP-48")
      (docs http://www.st.com/st-web-ui/static/active/en/resource/technical/document/datasheet/DM00090510.pdf)
      (footprints
        (fp LQFP*7x7mm*P0.5mm*))
      (fields
        (field (name Reference) U)
        (field (name Value) STM32F072C8Tx)
        (field (name Footprint) Package_QFP:LQFP-48_7x7mm_P0.5mm))
      (pins
        (pin (num 1) (name VBAT) (type power_in))
        (pin (num 2) (name PC13) (type BiDi))
        (pin (num 3) (name PC14) (type BiDi))
        (pin (num 4) (name PC15) (type BiDi))
        (pin (num 5) (name PF0) (type input))
        (pin (num 6) (name PF1) (type input))
        (pin (num 7) (name NRST) (type input))
        (pin (num 8) (name VSSA) (type power_in))
        (pin (num 9) (name VDDA) (type power_in))
        (pin (num 10) (name PA0) (type BiDi))
        (pin (num 11) (name PA1) (type BiDi))
        (pin (num 12) (name PA2) (type BiDi))
        (pin (num 13) (name PA3) (type BiDi))
        (pin (num 14) (name PA4) (type BiDi))
        (pin (num 15) (name PA5) (type BiDi))
        (pin (num 16) (name PA6) (type BiDi))
        (pin (num 17) (name PA7) (type BiDi))
        (pin (num 18) (name PB0) (type BiDi))
        (pin (num 19) (name PB1) (type BiDi))
        (pin (num 20) (name PB2) (type BiDi))
        (pin (num 21) (name PB10) (type BiDi))
        (pin (num 22) (name PB11) (type BiDi))
        (pin (num 23) (name VSS) (type power_in))
        (pin (num 24) (name VDD) (type power_in))
        (pin (num 25) (name PB12) (type BiDi))
        (pin (num 26) (name PB13) (type BiDi))
        (pin (num 27) (name PB14) (type BiDi))
        (pin (num 28) (name PB15) (type BiDi))
        (pin (num 29) (name PA8) (type BiDi))
        (pin (num 30) (name PA9) (type BiDi))
        (pin (num 31) (name PA10) (type BiDi))
        (pin (num 32) (name PA11) (type BiDi))
        (pin (num 33) (name PA12) (type BiDi))
        (pin (num 34) (name PA13) (type BiDi))
        (pin (num 35) (name VSS) (type power_in))
        (pin (num 36) (name VDDIO2) (type power_in))
        (pin (num 37) (name PA14) (type BiDi))
        (pin (num 38) (name PA15) (type BiDi))
        (pin (num 39) (name PB3) (type BiDi))
        (pin (num 40) (name PB4) (type BiDi))
        (pin (num 41) (name PB5) (type BiDi))
        (pin (num 42) (name PB6) (type BiDi))
        (pin (num 43) (name PB7) (type BiDi))
        (pin (num 44) (name BOOT0) (type input))
        (pin (num 45) (name PB8) (type BiDi))
        (pin (num 46) (name PB9) (type BiDi))
        (pin (num 47) (name VSS) (type power_in))
        (pin (num 48) (name VDD) (type power_in))))
    (libpart (lib Power_Protection) (part USBLC6-2SC6)
      (description "Bidirectional ESD Protection Diode, SOT-23-6")
      (docs http://www2.st.com/resource/en/datasheet/CD00050750.pdf)
      (footprints
        (fp SOT?23*))
      (fields
        (field (name Reference) U)
        (field (name Value) USBLC6-2SC6)
        (field (name Footprint) Package_TO_SOT_SMD:SOT-23-6))
      (pins
        (pin (num 1) (name IO1) (type passive))
        (pin (num 2) (name GND) (type passive))
        (pin (num 3) (name IO2) (type passive))
        (pin (num 4) (name IO2) (type passive))
        (pin (num 5) (name VBUS) (type passive))
        (pin (num 6) (name IO1) (type passive))))
    (libpart (lib Regulator_Linear) (part L7805)
      (aliases
        (alias L7806)
        (alias L7808)
        (alias L7885)
        (alias L7809)
        (alias L7812)
        (alias L7815)
        (alias L7818)
        (alias L7824))
      (description "Positive 1.5A 35V Linear Regulator, Fixed Output 5V, TO-220/TO-263/TO-252")
      (docs http://www.st.com/content/ccc/resource/technical/document/datasheet/41/4f/b3/b0/12/d4/47/88/CD00000444.pdf/files/CD00000444.pdf/jcr:content/translations/en.CD00000444.pdf)
      (footprints
        (fp TO?252*)
        (fp TO?263*)
        (fp TO?220*))
      (fields
        (field (name Reference) U)
        (field (name Value) L7805))
      (pins
        (pin (num 1) (name IN) (type power_in))
        (pin (num 2) (name GND) (type power_in))
        (pin (num 3) (name OUT) (type power_out))))
    (libpart (lib Regulator_Linear) (part LM1117-1.8)
      (aliases
        (alias LM1117-2.5)
        (alias LM1117-3.3)
        (alias LM1117-5.0)
        (alias TLV1117-15)
        (alias TLV1117-18)
        (alias TLV1117-25)
        (alias TLV1117-33)
        (alias TLV1117-50))
      (description "800mA Low-Dropout Linear Regulator, 1.8V fixed output, TO-220/TO-252/TO-263/SOT-223")
      (docs http://www.ti.com/lit/ds/symlink/lm1117.pdf)
      (footprints
        (fp SOT?223*)
        (fp TO?263*)
        (fp TO?252*)
        (fp TO?220*))
      (fields
        (field (name Reference) U)
        (field (name Value) LM1117-1.8))
      (pins
        (pin (num 1) (name GND) (type power_in))
        (pin (num 2) (name VO) (type power_out))
        (pin (num 3) (name VI) (type power_in))))
    (libpart (lib Switch) (part SW_Push)
      (description "Push button switch, generic, two pins")
      (docs ~)
      (fields
        (field (name Reference) SW)
        (field (name Value) SW_Push))
      (pins
        (pin (num 1) (name 1) (type passive))
        (pin (num 2) (name 2) (type passive))))
    (libpart (lib stm32-rescue) (part C-Chiller_control-rescue)
      (footprints
        (fp C_*))
      (fields
        (field (name Reference) C)
        (field (name Value) C-Chiller_control-rescue))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib stm32-rescue) (part Conn_01x02-Chiller_control-rescue)
      (footprints
        (fp Connector*:*_??x*mm*)
        (fp Connector*:*1x??x*mm*)
        (fp Pin?Header?Straight?1X*)
        (fp Pin?Header?Angled?1X*)
        (fp Socket?Strip?Straight?1X*)
        (fp Socket?Strip?Angled?1X*))
      (fields
        (field (name Reference) J)
        (field (name Value) Conn_01x02-Chiller_control-rescue))
      (pins
        (pin (num 1) (name Pin_1) (type passive))
        (pin (num 2) (name Pin_2) (type passive))))
    (libpart (lib stm32-rescue) (part G5LE-1-socket-rescue)
      (footprints
        (fp Relay*SPDT*Omron*G5LE?1*))
      (fields
        (field (name Reference) K)
        (field (name Value) G5LE-1-socket-rescue)
        (field (name Footprint) Relay_THT:Relay_SPDT_OMRON-G5LE-1))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))
        (pin (num 3) (name ~) (type passive))
        (pin (num 4) (name ~) (type passive))
        (pin (num 5) (name ~) (type passive))))
    (libpart (lib stm32-rescue) (part L-Chiller_control-rescue)
      (footprints
        (fp Choke_*)
        (fp *Coil*)
        (fp Inductor_*)
        (fp L_*))
      (fields
        (field (name Reference) L)
        (field (name Value) L-Chiller_control-rescue))
      (pins
        (pin (num 1) (name 1) (type passive))
        (pin (num 2) (name 2) (type passive))))
    (libpart (lib stm32-rescue) (part Q_NMOS_GSD-Chiller_control-rescue)
      (fields
        (field (name Reference) Q)
        (field (name Value) Q_NMOS_GSD-Chiller_control-rescue))
      (pins
        (pin (num 1) (name G) (type input))
        (pin (num 2) (name S) (type passive))
        (pin (num 3) (name D) (type passive))))
    (libpart (lib stm32-rescue) (part Q_NMOS_GSD-socket-rescue)
      (fields
        (field (name Reference) Q)
        (field (name Value) Q_NMOS_GSD-socket-rescue))
      (pins
        (pin (num 1) (name G) (type input))
        (pin (num 2) (name S) (type passive))
        (pin (num 3) (name D) (type passive))))
    (libpart (lib stm32-rescue) (part R-Chiller_control-rescue)
      (footprints
        (fp R_*)
        (fp R_*))
      (fields
        (field (name Reference) R)
        (field (name Value) R-Chiller_control-rescue))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib stm32-rescue) (part R-socket-rescue)
      (footprints
        (fp R_*)
        (fp R_*))
      (fields
        (field (name Reference) R)
        (field (name Value) R-socket-rescue))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive)))))
  (libraries
    (library (logical Connector)
      (uri /usr/share/kicad/library/Connector.lib))
    (library (logical Connector_Generic)
      (uri /usr/share/kicad/library/Connector_Generic.lib))
    (library (logical Device)
      (uri /usr/share/kicad/library/Device.lib))
    (library (logical MCU_ST_STM32F0)
      (uri /usr/share/kicad/library/MCU_ST_STM32F0.lib))
    (library (logical Power_Protection)
      (uri /usr/share/kicad/library/Power_Protection.lib))
    (library (logical Regulator_Linear)
      (uri /usr/share/kicad/library/Regulator_Linear.lib))
    (library (logical Switch)
      (uri /usr/share/kicad/library/Switch.lib))
    (library (logical stm32-rescue)
      (uri /home/eddy/Yandex.Disk/Projects/stm32samples/F0-nolib/Socket_fans/kicad/stm32-rescue.lib)))
  (nets
    (net (code 1) (name GND)
      (node (ref Q5) (pin 2))
      (node (ref R13) (pin 1))
      (node (ref R17) (pin 1))
      (node (ref R27) (pin 2))
      (node (ref R34) (pin 2))
      (node (ref C5) (pin 1))
      (node (ref Q4) (pin 2))
      (node (ref R16) (pin 1))
      (node (ref C20) (pin 2))
      (node (ref R1) (pin 2))
      (node (ref R29) (pin 2))
      (node (ref Q2) (pin 2))
      (node (ref D7) (pin 2))
      (node (ref C17) (pin 1))
      (node (ref Q3) (pin 2))
      (node (ref D10) (pin 2))
      (node (ref C19) (pin 1))
      (node (ref Q6) (pin 2))
      (node (ref D8) (pin 2))
      (node (ref C10) (pin 2))
      (node (ref C1) (pin 1))
      (node (ref C2) (pin 1))
      (node (ref C4) (pin 1))
      (node (ref U1) (pin 1))
      (node (ref C15) (pin 1))
      (node (ref C7) (pin 2))
      (node (ref C9) (pin 2))
      (node (ref C16) (pin 2))
      (node (ref C18) (pin 2))
      (node (ref R22) (pin 2))
      (node (ref U3) (pin 35))
      (node (ref U3) (pin 8))
      (node (ref U3) (pin 47))
      (node (ref P1) (pin 4))
      (node (ref U3) (pin 23))
      (node (ref C6) (pin 2))
      (node (ref C14) (pin 2))
      (node (ref R5) (pin 1))
      (node (ref R7) (pin 1))
      (node (ref J1) (pin 2))
      (node (ref R14) (pin 1))
      (node (ref P1) (pin 5))
      (node (ref U4) (pin 2))
      (node (ref C13) (pin 2))
      (node (ref SW2) (pin 1))
      (node (ref SW1) (pin 1))
      (node (ref R9) (pin 1))
      (node (ref J10) (pin 2))
      (node (ref R3) (pin 1))
      (node (ref C8) (pin 2))
      (node (ref U2) (pin 2))
      (node (ref C3) (pin 2)))
    (net (code 2) (name "Net-(C14-Pad1)")
      (node (ref C14) (pin 1))
      (node (ref SW2) (pin 2))
      (node (ref R25) (pin 2)))
    (net (code 3) (name /Btn0)
      (node (ref U3) (pin 27))
      (node (ref R24) (pin 1)))
    (net (code 4) (name "Net-(C13-Pad1)")
      (node (ref SW1) (pin 2))
      (node (ref R24) (pin 2))
      (node (ref C13) (pin 1)))
    (net (code 5) (name /Btn1)
      (node (ref U3) (pin 28))
      (node (ref R25) (pin 1)))
    (net (code 6) (name "Net-(U3-Pad45)")
      (node (ref U3) (pin 45)))
    (net (code 7) (name "Net-(D4-Pad2)")
      (node (ref Q2) (pin 3))
      (node (ref D4) (pin 2))
      (node (ref J5) (pin 1)))
    (net (code 8) (name "Net-(U3-Pad5)")
      (node (ref U3) (pin 5)))
    (net (code 9) (name "Net-(U3-Pad6)")
      (node (ref U3) (pin 6)))
    (net (code 10) (name "Net-(U3-Pad4)")
      (node (ref U3) (pin 4)))
    (net (code 11) (name "Net-(U3-Pad34)")
      (node (ref U3) (pin 34)))
    (net (code 12) (name "Net-(U3-Pad38)")
      (node (ref U3) (pin 38)))
    (net (code 13) (name "Net-(U3-Pad42)")
      (node (ref U3) (pin 42)))
    (net (code 14) (name "Net-(U3-Pad43)")
      (node (ref U3) (pin 43)))
    (net (code 15) (name "Net-(U3-Pad46)")
      (node (ref U3) (pin 46)))
    (net (code 16) (name "Net-(U3-Pad25)")
      (node (ref U3) (pin 25)))
    (net (code 17) (name "Net-(U3-Pad26)")
      (node (ref U3) (pin 26)))
    (net (code 18) (name "Net-(P5-Pad1)")
      (node (ref P5) (pin 1)))
    (net (code 19) (name "Net-(P4-Pad1)")
      (node (ref P4) (pin 1)))
    (net (code 20) (name "Net-(P2-Pad1)")
      (node (ref P2) (pin 1)))
    (net (code 21) (name "Net-(P3-Pad1)")
      (node (ref P3) (pin 1)))
    (net (code 22) (name "Net-(J2-Pad1)")
      (node (ref J2) (pin 1))
      (node (ref R8) (pin 1))
      (node (ref R9) (pin 2)))
    (net (code 23) (name "Net-(P1-Pad3)")
      (node (ref U4) (pin 6))
      (node (ref P1) (pin 3)))
    (net (code 24) (name "Net-(J2-Pad5)")
      (node (ref J2) (pin 5))
      (node (ref R4) (pin 1))
      (node (ref R5) (pin 2)))
    (net (code 25) (name "Net-(J2-Pad3)")
      (node (ref J2) (pin 3))
      (node (ref R7) (pin 2))
      (node (ref R6) (pin 1)))
    (net (code 26) (name "Net-(R30-Pad1)")
      (node (ref R30) (pin 1))
      (node (ref U4) (pin 3)))
    (net (code 27) (name "Net-(R31-Pad1)")
      (node (ref R31) (pin 1))
      (node (ref U4) (pin 1)))
    (net (code 28) (name /5Vusb)
      (node (ref P1) (pin 1))
      (node (ref U4) (pin 5))
      (node (ref D2) (pin 2)))
    (net (code 29) (name "Net-(P1-Pad2)")
      (node (ref U4) (pin 4))
      (node (ref P1) (pin 2)))
    (net (code 30) (name "Net-(J6-Pad3)")
      (node (ref R19) (pin 2))
      (node (ref J6) (pin 3)))
    (net (code 31) (name "Net-(J6-Pad4)")
      (node (ref J6) (pin 4))
      (node (ref R21) (pin 2)))
    (net (code 32) (name "Net-(D6-Pad2)")
      (node (ref D6) (pin 2))
      (node (ref Q5) (pin 3))
      (node (ref J4) (pin 2)))
    (net (code 33) (name "Net-(J3-Pad1)")
      (node (ref Q4) (pin 3))
      (node (ref J3) (pin 1)))
    (net (code 34) (name +12V)
      (node (ref R26) (pin 1))
      (node (ref D3) (pin 1))
      (node (ref C3) (pin 1))
      (node (ref U2) (pin 1))
      (node (ref Q1) (pin 2))
      (node (ref C10) (pin 1))
      (node (ref J3) (pin 2))
      (node (ref J5) (pin 2))
      (node (ref D4) (pin 1))
      (node (ref K1) (pin 2))
      (node (ref D9) (pin 1))
      (node (ref J6) (pin 2))
      (node (ref J4) (pin 1))
      (node (ref D5) (pin 1))
      (node (ref D6) (pin 1)))
    (net (code 35) (name "Net-(J5-Pad3)")
      (node (ref R18) (pin 2))
      (node (ref J5) (pin 3)))
    (net (code 36) (name "Net-(J5-Pad4)")
      (node (ref R20) (pin 2))
      (node (ref J5) (pin 4)))
    (net (code 37) (name /TIM1_CH2)
      (node (ref R20) (pin 1))
      (node (ref U3) (pin 30)))
    (net (code 38) (name "Net-(Q2-Pad1)")
      (node (ref R10) (pin 1))
      (node (ref Q2) (pin 1)))
    (net (code 39) (name "Net-(J8-Pad1)")
      (node (ref K1) (pin 1))
      (node (ref J8) (pin 1)))
    (net (code 40) (name "Net-(J8-Pad2)")
      (node (ref J8) (pin 2))
      (node (ref K1) (pin 3)))
    (net (code 41) (name "Net-(K1-Pad4)")
      (node (ref K1) (pin 4)))
    (net (code 42) (name "Net-(Q6-Pad1)")
      (node (ref R32) (pin 1))
      (node (ref Q6) (pin 1)))
    (net (code 43) (name "Net-(U3-Pad3)")
      (node (ref U3) (pin 3)))
    (net (code 44) (name "Net-(D9-Pad2)")
      (node (ref K1) (pin 5))
      (node (ref D9) (pin 2))
      (node (ref Q6) (pin 3)))
    (net (code 45) (name "Net-(Q3-Pad1)")
      (node (ref R11) (pin 1))
      (node (ref Q3) (pin 1)))
    (net (code 46) (name "Net-(D5-Pad2)")
      (node (ref Q3) (pin 3))
      (node (ref J6) (pin 1))
      (node (ref D5) (pin 2)))
    (net (code 47) (name /TIM3_CH1)
      (node (ref D10) (pin 1))
      (node (ref R19) (pin 1))
      (node (ref U3) (pin 16)))
    (net (code 48) (name /TIM14_CH1)
      (node (ref R18) (pin 1))
      (node (ref D8) (pin 1))
      (node (ref U3) (pin 17)))
    (net (code 49) (name "Net-(D3-Pad2)")
      (node (ref D3) (pin 2))
      (node (ref R1) (pin 1))
      (node (ref Q1) (pin 1)))
    (net (code 50) (name "Net-(J1-Pad1)")
      (node (ref J1) (pin 1))
      (node (ref Q1) (pin 3)))
    (net (code 51) (name /BOOT0)
      (node (ref J7) (pin 2))
      (node (ref R22) (pin 1))
      (node (ref U3) (pin 44)))
    (net (code 52) (name /ADC0)
      (node (ref U3) (pin 10))
      (node (ref R2) (pin 2))
      (node (ref C1) (pin 2)))
    (net (code 53) (name /ADC1)
      (node (ref C2) (pin 2))
      (node (ref U3) (pin 11))
      (node (ref R4) (pin 2)))
    (net (code 54) (name "Net-(R30-Pad2)")
      (node (ref R30) (pin 2))
      (node (ref U3) (pin 32)))
    (net (code 55) (name /Buzzer)
      (node (ref R12) (pin 2))
      (node (ref R16) (pin 2))
      (node (ref U3) (pin 37)))
    (net (code 56) (name "Net-(U3-Pad18)")
      (node (ref U3) (pin 18)))
    (net (code 57) (name "Net-(U3-Pad39)")
      (node (ref U3) (pin 39)))
    (net (code 58) (name "Net-(U3-Pad19)")
      (node (ref U3) (pin 19)))
    (net (code 59) (name "Net-(U3-Pad20)")
      (node (ref U3) (pin 20)))
    (net (code 60) (name "Net-(U3-Pad21)")
      (node (ref U3) (pin 21)))
    (net (code 61) (name "Net-(U3-Pad22)")
      (node (ref U3) (pin 22)))
    (net (code 62) (name /NRST)
      (node (ref J10) (pin 1))
      (node (ref U3) (pin 7)))
    (net (code 63) (name /Cooler1)
      (node (ref R13) (pin 2))
      (node (ref R10) (pin 2))
      (node (ref U3) (pin 41)))
    (net (code 64) (name /Relay)
      (node (ref R32) (pin 2))
      (node (ref U3) (pin 2))
      (node (ref R34) (pin 1)))
    (net (code 65) (name /ADC2)
      (node (ref C4) (pin 2))
      (node (ref U3) (pin 12))
      (node (ref R6) (pin 2)))
    (net (code 66) (name /ADC3)
      (node (ref U3) (pin 13))
      (node (ref R8) (pin 2))
      (node (ref C5) (pin 2)))
    (net (code 67) (name /AIN0)
      (node (ref R26) (pin 2))
      (node (ref D7) (pin 1))
      (node (ref U3) (pin 14))
      (node (ref R27) (pin 1))
      (node (ref C16) (pin 1)))
    (net (code 68) (name /AIN1)
      (node (ref C18) (pin 1))
      (node (ref U3) (pin 15))
      (node (ref R29) (pin 1))
      (node (ref R28) (pin 2)))
    (net (code 69) (name /TIM1_CH1)
      (node (ref U3) (pin 29))
      (node (ref R21) (pin 1)))
    (net (code 70) (name +3V3)
      (node (ref U1) (pin 2))
      (node (ref R23) (pin 2))
      (node (ref L1) (pin 1))
      (node (ref C7) (pin 1))
      (node (ref C15) (pin 2))
      (node (ref C6) (pin 1))
      (node (ref C19) (pin 2))
      (node (ref U3) (pin 36))
      (node (ref U3) (pin 48))
      (node (ref U3) (pin 24))
      (node (ref U3) (pin 1))
      (node (ref J2) (pin 4))
      (node (ref J2) (pin 6))
      (node (ref J2) (pin 8))
      (node (ref C17) (pin 2))
      (node (ref J2) (pin 2)))
    (net (code 71) (name "Net-(J7-Pad1)")
      (node (ref J7) (pin 1))
      (node (ref R23) (pin 1)))
    (net (code 72) (name /5Vin)
      (node (ref C9) (pin 1))
      (node (ref D1) (pin 2))
      (node (ref C8) (pin 1))
      (node (ref U2) (pin 3)))
    (net (code 73) (name /Cooler0)
      (node (ref R14) (pin 2))
      (node (ref U3) (pin 40))
      (node (ref R11) (pin 2)))
    (net (code 74) (name "Net-(Q4-Pad1)")
      (node (ref R12) (pin 1))
      (node (ref Q4) (pin 1)))
    (net (code 75) (name +5V)
      (node (ref D2) (pin 1))
      (node (ref D1) (pin 1))
      (node (ref U1) (pin 3))
      (node (ref R28) (pin 1)))
    (net (code 76) (name "Net-(C20-Pad1)")
      (node (ref C20) (pin 1))
      (node (ref L1) (pin 2))
      (node (ref U3) (pin 9)))
    (net (code 77) (name "Net-(R31-Pad2)")
      (node (ref U3) (pin 33))
      (node (ref R31) (pin 2)))
    (net (code 78) (name "Net-(J2-Pad7)")
      (node (ref R2) (pin 1))
      (node (ref R3) (pin 2))
      (node (ref J2) (pin 7)))
    (net (code 79) (name "Net-(Q5-Pad1)")
      (node (ref Q5) (pin 1))
      (node (ref R15) (pin 1)))
    (net (code 80) (name /TIM1_CH3)
      (node (ref R17) (pin 2))
      (node (ref U3) (pin 31))
      (node (ref R15) (pin 2)))))