0
Audio_Module
Reverb_BTDR-1H
Digital Reverberation Unit, http://www.belton.co.kr/inc/downfile.php?seq=17&file=pdf (footprint from http://www.uk-electronic.de/PDF/BTDR-1.pdf)
audio belton reverb
0
7
7
Audio_Module
Reverb_BTDR-1V
Digital Reverberation Unit, http://www.belton.co.kr/inc/downfile.php?seq=17&file=pdf (footprint from http://www.uk-electronic.de/PDF/BTDR-1.pdf)
audio belton reverb
0
7
7
Battery
BatteryHolder_Bulgin_BX0036_1xC
Bulgin Battery Holder, BX0036, Battery Type C (https://www.bulgin.com/products/pub/media/bulgin/data/Battery_holders.pdf)
Bulgin BX0036
0
2
2
Battery
BatteryHolder_ComfortableElectronic_CH273-2450_1x2450
Comfortable Electronic CR2450 battery holder, http://www.comf.com.tw/ProductDetail.asp?no=148
Comfortable Electronic CR2450
0
2
2
Battery
BatteryHolder_Eagle_12BH611-GR
https://eu.mouser.com/datasheet/2/209/EPD-200766-1274481.pdf
9V Battery Holder
0
2
2
Battery
BatteryHolder_Keystone_103_1x20mm
http://www.keyelco.com/product-pdf.cfm?p=719
Keystone type 103 battery holder
0
2
2
Battery
BatteryHolder_Keystone_104_1x23mm
http://www.keyelco.com/product-pdf.cfm?p=744
Keystone type 104 battery holder
0
2
2
Battery
BatteryHolder_Keystone_105_1x2430
http://www.keyelco.com/product-pdf.cfm?p=745
Keystone type 105 battery holder
0
2
2
Battery
BatteryHolder_Keystone_106_1x20mm
http://www.keyelco.com/product-pdf.cfm?p=720
Keystone type 106 battery holder
0
2
2
Battery
BatteryHolder_Keystone_107_1x23mm
http://www.keyelco.com/product-pdf.cfm?p=746
Keystone type 107 battery holder
0
2
2
Battery
BatteryHolder_Keystone_500
Keystone #500, CR1220 battery holder, http://www.keyelco.com/product-pdf.cfm?p=710
CR1220 battery holder
0
2
2
Battery
BatteryHolder_Keystone_1042_1x18650
Battery holder for 18650 cylindrical cells http://www.keyelco.com/product.cfm/product_id/918
18650 Keystone 1042 Li-ion
0
2
2
Battery
BatteryHolder_Keystone_1057_1x2032
SMT (Auto-In/Ultra-Low) Holder for 2032 Cell, 33.2 x 23.9mm, 2mm height above PCB, https://www.keyelco.com/userAssets/file/M65p4.pdf
Keystone type 1057 coin cell holder
0
2
2
Battery
BatteryHolder_Keystone_1058_1x2032
http://www.keyelco.com/product-pdf.cfm?p=14028
Keystone type 1058 coin cell retainer
0
2
2
Battery
BatteryHolder_Keystone_1060_1x2032
http://www.keyelco.com/product-pdf.cfm?p=726
CR2032 BR2032 BatteryHolder Battery
0
2
2
Battery
BatteryHolder_Keystone_2460_1xAA
https://www.keyelco.com/product-pdf.cfm?p=1025
AA battery cell holder
0
2
2
Battery
BatteryHolder_Keystone_2462_2xAA
2xAA cell battery holder, Keystone P/N 2462, https://www.keyelco.com/product-pdf.cfm?p=1027
AA battery cell holder
0
2
2
Battery
BatteryHolder_Keystone_2466_1xAAA
1xAAA Battery Holder, Keystone, Plastic Case, http://www.keyelco.com/product-pdf.cfm?p=1031
AAA battery holder Keystone
0
2
2
Battery
BatteryHolder_Keystone_2468_2xAAA
2xAAA cell battery holder, Keystone P/N 2468, http://www.keyelco.com/product-pdf.cfm?p=1033
AAA battery cell holder
0
2
2
Battery
BatteryHolder_Keystone_2479_3xAAA
Keystone Battery Holder, 2479, Battery Type 3xAAA (Script generated with StandardBox.py) (Keystone Battery Holder, 2479, Battery Type 3xAAA)
Keystone Battery Holder 2479 Battery Type 3xAAA
0
2
2
Battery
BatteryHolder_Keystone_2993
http://www.keyelco.com/product-pdf.cfm?p=776
Keystone type 2993 negative battery contact
0
1
1
Battery
BatteryHolder_Keystone_2998_1x6.8mm
www.keyelco.com/product-pdf.cfm?p=763
Keystone type 2998 battery holder
0
3
2
Battery
BatteryHolder_Keystone_3000_1x12mm
http://www.keyelco.com/product-pdf.cfm?p=777
Keystone type 3000 coin cell retainer
0
3
2
Battery
BatteryHolder_Keystone_3001_1x12mm
http://www.keyelco.com/product-pdf.cfm?p=778
Keystone type 3001 coin cell retainer
0
3
2
Battery
BatteryHolder_Keystone_3002_1x2032
https://www.tme.eu/it/Document/a823211ec201a9e209042d155fe22d2b/KEYS2996.pdf
BR2016 CR2016 DL2016 BR2020 CL2020 BR2025 CR2025 DL2025 DR2032 CR2032 DL2032
0
3
2
Battery
BatteryHolder_Keystone_3008_1x2450
http://www.keyelco.com/product-pdf.cfm?p=786
Keystone type 3008 coin cell retainer
0
3
2
Battery
BatteryHolder_Keystone_3009_1x2450
http://www.keyelco.com/product-pdf.cfm?p=787
Keystone type 3009 coin cell retainer
0
3
2
Battery
BatteryHolder_Keystone_3034_1x20mm
Keystone 3034 SMD battery holder for 2020, 2025 and 2032 coincell batteries. http://www.keyelco.com/product-pdf.cfm?p=798
Keystone type 3034 coin cell retainer
0
3
2
Battery
BatteryHolder_LINX_BAT-HLD-012-SMT
SMT battery holder for CR1216/1220/1225, https://linxtechnologies.com/wp/wp-content/uploads/bat-hld-012-smt.pdf
battery holder coin cell cr1216 cr1220 cr1225
0
3
2
Battery
BatteryHolder_MPD_BA9VPC_1xPP3
1xPP3 (9V) battery holder, Memory Protection Devices P/N BA9VPC, http://www.memoryprotectiondevices.com/datasheets/BA9VPC-datasheet.pdf
PP3 Battery Holder BA9VPC 9V
0
2
2
Battery
BatteryHolder_MPD_BC2AAPC_2xAA
2xAA cell battery holder, Memory Protection Devices P/N BC2AAPC, http://www.memoryprotectiondevices.com/datasheets/BC2AAPC-datasheet.pdf
AA battery cell holder
0
2
2
Battery
BatteryHolder_MPD_BC12AAPC_2xAA
2xAA cell battery holder, Memory Protection Devices P/N BC12AAPC, http://www.memoryprotectiondevices.com/datasheets/BC12AAPC-datasheet.pdf
AA battery cell holder
0
2
2
Battery
BatteryHolder_MPD_BC2003_1x2032
http://www.memoryprotectiondevices.com/datasheets/BC-2003-datasheet.pdf
BC2003 CR2032 2032 Battery Holder
0
3
2
Battery
BatteryHolder_MPD_BH-18650-PC2
18650 Battery Holder (http://www.memoryprotectiondevices.com/datasheets/BK-18650-PC2-datasheet.pdf)
18650 Battery Holder
0
2
2
Battery
BatteryHolder_Seiko_MS621F
Seiko MS621F, https://www.sii.co.jp/en/me/files/2014/02/file_EXTENDED_PRDCT_SPEC_75_FILE_11.jpg
Seiko MS621F
0
2
2
Battery
BatteryHolder_TruPower_BH-331P_3xAA
Keystone Battery Holder BH-331P Battery Type 3xAA (Script generated with StandardBox.py) (Keystone Battery Holder BH-331P Battery Type 3xAA)
Battery Holder BH-331P Battery Type 3xAA
0
2
2
Battery
Battery_CR1225
CR1225 battery
battery CR1225 coin cell
0
0
0
Battery
Battery_Panasonic_CR1025-VSK_Vertical_CircularHoles
Panasonic CR-1025/VSK battery
battery CR-1025 coin cell vertical
0
2
2
Battery
Battery_Panasonic_CR1220-VCN_Vertical_CircularHoles
Panasonic CR-1220/VCN battery, https://industrial.panasonic.com/cdbs/www-data/pdf2/AAA4000/AAA4000D140.PDF
battery CR-1220 coin cell vertical
0
2
2
Battery
Battery_Panasonic_CR1632-V1AN_Vertical_CircularHoles
Panasonic CR-1632-V1AN battery, https://industrial.panasonic.com/cdbs/www-data/pdf2/AAA4000/AAA4000D464.PDF
battery CR-1632 coin cell vertical
0
2
2
Battery
Battery_Panasonic_CR2025-V1AK_Vertical_CircularHoles
Panasonic CR-2025/V1AK battery,
battery CR-2025 coin cell vertical
0
2
2
Battery
Battery_Panasonic_CR2032-VS1N_Vertical_CircularHoles
Panasonic CR-2032/VS1N battery, https://industrial.panasonic.com/cdbs/www-data/pdf2/AAA4000/AAA4000D348.PDF
battery CR-2032 coin cell vertical
0
2
2
Battery
Battery_Panasonic_CR2354-VCN_Vertical_CircularHoles
Panasonic CR-2354/VCN battery, https://industrial.panasonic.com/cdbs/www-data/pdf2/AAA4000/AAA4000D486.PDF
battery CR-2354/VCN coin cell vertical
0
2
2
Battery
Battery_Panasonic_CR2450-VAN_Vertical_CircularHoles
Panasonic CR-2450/VAN battery, https://industrial.panasonic.com/cdbs/www-data/pdf2/AAA4000/AAA4000D492.PDF
battery CR-2450 coin cell
0
2
2
Battery
Battery_Panasonic_CR2477-VCN_Vertical_CircularHoles
Panasonic CR-2477/VCN battery, https://industrial.panasonic.com/cdbs/www-data/pdf2/AAA4000/AAA4000D502.PDF
battery CR-2477 coin cell vertical
0
2
2
Battery
Battery_Panasonic_CR3032-VCN_Vertical_CircularHoles
Panasonic CR-3032/VCN battery, https://industrial.panasonic.com/cdbs/www-data/pdf2/AAA4000/AAA4000D508.PDF
battery CR-3032 coin cell vertical
0
2
2
Button_Switch_SMD
Nidec_Copal_SH-7010A
4-bit rotary coded switch, J-hook, https://www.nidec-copal-electronics.com/e/catalog/switch/sh-7000.pdf
rotary switch bcd
0
6
5
Button_Switch_SMD
Nidec_Copal_SH-7010B
4-bit rotary coded switch, gull wing, https://www.nidec-copal-electronics.com/e/catalog/switch/sh-7000.pdf
rotary switch bcd
0
6
5
Button_Switch_SMD
Nidec_Copal_SH-7040B
4-bit rotary coded switch, gull wing, Gray code, https://www.nidec-copal-electronics.com/e/catalog/switch/sh-7000.pdf
rotary switch bcd
0
5
5
Button_Switch_SMD
Panasonic_EVQPUJ_EVQPUA
http://industrial.panasonic.com/cdbs/www-data/pdf/ATV0000/ATV0000CE5.pdf
SMD SMT SPST EVQPUJ EVQPUA
0
4
2
Button_Switch_SMD
Panasonic_EVQPUK_EVQPUB
http://industrial.panasonic.com/cdbs/www-data/pdf/ATV0000/ATV0000CE5.pdf
SMD SMT SPST EVQPUK EVQPUB
0
4
2
Button_Switch_SMD
Panasonic_EVQPUL_EVQPUC
http://industrial.panasonic.com/cdbs/www-data/pdf/ATV0000/ATV0000CE5.pdf
SMD SMT SPST EVQPUL EVQPUC
0
4
2
Button_Switch_SMD
Panasonic_EVQPUM_EVQPUD
http://industrial.panasonic.com/cdbs/www-data/pdf/ATV0000/ATV0000CE5.pdf
SMD SMT SPST EVQPUM EVQPUD
0
4
2
Button_Switch_SMD
SW_DIP_SPSTx01_Slide_6.7x4.1mm_W6.73mm_P2.54mm_LowProfile_JPin
SMD 1x-dip-switch SPST , Slide, row spacing 6.73 mm (264 mils), body size 6.7x4.1mm (see e.g. https://www.ctscorp.com/wp-content/uploads/219.pdf), SMD, LowProfile, JPin
SMD DIP Switch SPST Slide 6.73mm 264mil SMD LowProfile JPin
0
2
2
Button_Switch_SMD
SW_DIP_SPSTx01_Slide_6.7x4.1mm_W8.61mm_P2.54mm_LowProfile
SMD 1x-dip-switch SPST , Slide, row spacing 8.61 mm (338 mils), body size 6.7x4.1mm (see e.g. https://www.ctscorp.com/wp-content/uploads/219.pdf), SMD, LowProfile
SMD DIP Switch SPST Slide 8.61mm 338mil SMD LowProfile
0
2
2
Button_Switch_SMD
SW_DIP_SPSTx01_Slide_9.78x4.72mm_W8.61mm_P2.54mm
SMD 1x-dip-switch SPST , Slide, row spacing 8.61 mm (338 mils), body size 9.78x4.72mm (see e.g. https://www.ctscorp.com/wp-content/uploads/204.pdf), SMD
SMD DIP Switch SPST Slide 8.61mm 338mil SMD
0
2
2
Button_Switch_SMD
SW_DIP_SPSTx01_Slide_Copal_CHS-01A_W5.08mm_P1.27mm_JPin
SMD 1x-dip-switch SPST Copal_CHS-01A, Slide, row spacing 5.08 mm (200 mils), body size  (see http://www.nidec-copal-electronics.com/e/catalog/switch/chs.pdf), SMD, JPin
SMD DIP Switch SPST Slide 5.08mm 200mil SMD JPin
0
2
2
Button_Switch_SMD
SW_DIP_SPSTx01_Slide_Copal_CHS-01B_W7.62mm_P1.27mm
SMD 1x-dip-switch SPST Copal_CHS-01B, Slide, row spacing 7.62 mm (300 mils), body size  (see http://www.nidec-copal-electronics.com/e/catalog/switch/chs.pdf), SMD
SMD DIP Switch SPST Slide 7.62mm 300mil SMD
0
2
2
Button_Switch_SMD
SW_DIP_SPSTx01_Slide_Copal_CVS-01xB_W5.9mm_P1mm
SMD 1x-dip-switch SPST Copal_CVS-01xB, Slide, row spacing 5.9 mm (232 mils), body size  (see http://www.nidec-copal-electronics.com/e/catalog/switch/cvs.pdf)
SMD DIP Switch SPST Slide 5.9mm 232mil
0
6
3
Button_Switch_SMD
SW_DIP_SPSTx01_Slide_Omron_A6S-110x_W8.9mm_P2.54mm
SMD 1x-dip-switch SPST Omron_A6S-110x, Slide, row spacing 8.9 mm (350 mils), body size  (see http://omronfs.omron.com/en_US/ecb/products/pdf/en-a6s.pdf)
SMD DIP Switch SPST Slide 8.9mm 350mil
0
2
2
Button_Switch_SMD
SW_DIP_SPSTx02_Slide_6.7x6.64mm_W6.73mm_P2.54mm_LowProfile_JPin
SMD 2x-dip-switch SPST , Slide, row spacing 6.73 mm (264 mils), body size 6.7x6.64mm (see e.g. https://www.ctscorp.com/wp-content/uploads/219.pdf), SMD, LowProfile, JPin
SMD DIP Switch SPST Slide 6.73mm 264mil SMD LowProfile JPin
0
4
4
Button_Switch_SMD
SW_DIP_SPSTx02_Slide_6.7x6.64mm_W8.61mm_P2.54mm_LowProfile
SMD 2x-dip-switch SPST , Slide, row spacing 8.61 mm (338 mils), body size 6.7x6.64mm (see e.g. https://www.ctscorp.com/wp-content/uploads/219.pdf), SMD, LowProfile
SMD DIP Switch SPST Slide 8.61mm 338mil SMD LowProfile
0
4
4
Button_Switch_SMD
SW_DIP_SPSTx02_Slide_9.78x7.26mm_W8.61mm_P2.54mm
SMD 2x-dip-switch SPST , Slide, row spacing 8.61 mm (338 mils), body size 9.78x7.26mm (see e.g. https://www.ctscorp.com/wp-content/uploads/204.pdf), SMD
SMD DIP Switch SPST Slide 8.61mm 338mil SMD
0
4
4
Button_Switch_SMD
SW_DIP_SPSTx02_Slide_Copal_CHS-02A_W5.08mm_P1.27mm_JPin
SMD 2x-dip-switch SPST Copal_CHS-02A, Slide, row spacing 5.08 mm (200 mils), body size  (see http://www.nidec-copal-electronics.com/e/catalog/switch/chs.pdf), SMD, JPin
SMD DIP Switch SPST Slide 5.08mm 200mil SMD JPin
0
4
4
Button_Switch_SMD
SW_DIP_SPSTx02_Slide_Copal_CHS-02B_W7.62mm_P1.27mm
SMD 2x-dip-switch SPST Copal_CHS-02B, Slide, row spacing 7.62 mm (300 mils), body size  (see http://www.nidec-copal-electronics.com/e/catalog/switch/chs.pdf), SMD
SMD DIP Switch SPST Slide 7.62mm 300mil SMD
0
4
4
Button_Switch_SMD
SW_DIP_SPSTx02_Slide_Copal_CVS-02xB_W5.9mm_P1mm
SMD 2x-dip-switch SPST Copal_CVS-02xB, Slide, row spacing 5.9 mm (232 mils), body size  (see http://www.nidec-copal-electronics.com/e/catalog/switch/cvs.pdf)
SMD DIP Switch SPST Slide 5.9mm 232mil
0
8
5
Button_Switch_SMD
SW_DIP_SPSTx02_Slide_KingTek_DSHP02TJ_W5.25mm_P1.27mm_JPin
SMD 2x-dip-switch SPST KingTek_DSHP02TJ, Slide, row spacing 5.25 mm (206 mils), body size  (see http://www.kingtek.net.cn/pic/201601201446313350.pdf), JPin
SMD DIP Switch SPST Slide 5.25mm 206mil JPin
0
4
4
Button_Switch_SMD
SW_DIP_SPSTx02_Slide_KingTek_DSHP02TS_W7.62mm_P1.27mm
SMD 2x-dip-switch SPST KingTek_DSHP02TS, Slide, row spacing 7.62 mm (300 mils), body size  (see http://www.kingtek.net.cn/pic/201601201417455112.pdf)
SMD DIP Switch SPST Slide 7.62mm 300mil
0
4
4
Button_Switch_SMD
SW_DIP_SPSTx02_Slide_Omron_A6H-2101_W6.15mm_P1.27mm
SMD 2x-dip-switch SPST Omron_A6H-2101, Slide, row spacing 6.15 mm (242 mils), body size  (see https://www.omron.com/ecb/products/pdf/en-a6h.pdf)
SMD DIP Switch SPST Slide 6.15mm 242mil
0
4
4
Button_Switch_SMD
SW_DIP_SPSTx02_Slide_Omron_A6S-210x_W8.9mm_P2.54mm
SMD 2x-dip-switch SPST Omron_A6S-210x, Slide, row spacing 8.9 mm (350 mils), body size  (see http://omronfs.omron.com/en_US/ecb/products/pdf/en-a6s.pdf)
SMD DIP Switch SPST Slide 8.9mm 350mil
0
4
4
Button_Switch_SMD
SW_DIP_SPSTx03_Slide_6.7x9.18mm_W6.73mm_P2.54mm_LowProfile_JPin
SMD 3x-dip-switch SPST , Slide, row spacing 6.73 mm (264 mils), body size 6.7x9.18mm (see e.g. https://www.ctscorp.com/wp-content/uploads/219.pdf), SMD, LowProfile, JPin
SMD DIP Switch SPST Slide 6.73mm 264mil SMD LowProfile JPin
0
6
6
Button_Switch_SMD
SW_DIP_SPSTx03_Slide_6.7x9.18mm_W8.61mm_P2.54mm_LowProfile
SMD 3x-dip-switch SPST , Slide, row spacing 8.61 mm (338 mils), body size 6.7x9.18mm (see e.g. https://www.ctscorp.com/wp-content/uploads/219.pdf), SMD, LowProfile
SMD DIP Switch SPST Slide 8.61mm 338mil SMD LowProfile
0
6
6
Button_Switch_SMD
SW_DIP_SPSTx03_Slide_9.78x9.8mm_W8.61mm_P2.54mm
SMD 3x-dip-switch SPST , Slide, row spacing 8.61 mm (338 mils), body size 9.78x9.8mm (see e.g. https://www.ctscorp.com/wp-content/uploads/204.pdf), SMD
SMD DIP Switch SPST Slide 8.61mm 338mil SMD
0
6
6
Button_Switch_SMD
SW_DIP_SPSTx03_Slide_Copal_CVS-03xB_W5.9mm_P1mm
SMD 3x-dip-switch SPST Copal_CVS-03xB, Slide, row spacing 5.9 mm (232 mils), body size  (see http://www.nidec-copal-electronics.com/e/catalog/switch/cvs.pdf)
SMD DIP Switch SPST Slide 5.9mm 232mil
0
10
7
Button_Switch_SMD
SW_DIP_SPSTx03_Slide_KingTek_DSHP03TJ_W5.25mm_P1.27mm_JPin
SMD 3x-dip-switch SPST KingTek_DSHP03TJ, Slide, row spacing 5.25 mm (206 mils), body size  (see http://www.kingtek.net.cn/pic/201601201446313350.pdf), JPin
SMD DIP Switch SPST Slide 5.25mm 206mil JPin
0
6
6
Button_Switch_SMD
SW_DIP_SPSTx03_Slide_KingTek_DSHP03TS_W7.62mm_P1.27mm
SMD 3x-dip-switch SPST KingTek_DSHP03TS, Slide, row spacing 7.62 mm (300 mils), body size  (see http://www.kingtek.net.cn/pic/201601201417455112.pdf)
SMD DIP Switch SPST Slide 7.62mm 300mil
0
6
6
Button_Switch_SMD
SW_DIP_SPSTx03_Slide_Omron_A6S-310x_W8.9mm_P2.54mm
SMD 3x-dip-switch SPST Omron_A6S-310x, Slide, row spacing 8.9 mm (350 mils), body size  (see http://omronfs.omron.com/en_US/ecb/products/pdf/en-a6s.pdf)
SMD DIP Switch SPST Slide 8.9mm 350mil
0
6
6
Button_Switch_SMD
SW_DIP_SPSTx04_Slide_6.7x11.72mm_W6.73mm_P2.54mm_LowProfile_JPin
SMD 4x-dip-switch SPST , Slide, row spacing 6.73 mm (264 mils), body size 6.7x11.72mm (see e.g. https://www.ctscorp.com/wp-content/uploads/219.pdf), SMD, LowProfile, JPin
SMD DIP Switch SPST Slide 6.73mm 264mil SMD LowProfile JPin
0
8
8
Button_Switch_SMD
SW_DIP_SPSTx04_Slide_6.7x11.72mm_W8.61mm_P2.54mm_LowProfile
SMD 4x-dip-switch SPST , Slide, row spacing 8.61 mm (338 mils), body size 6.7x11.72mm (see e.g. https://www.ctscorp.com/wp-content/uploads/219.pdf), SMD, LowProfile
SMD DIP Switch SPST Slide 8.61mm 338mil SMD LowProfile
0
8
8
Button_Switch_SMD
SW_DIP_SPSTx04_Slide_9.78x12.34mm_W8.61mm_P2.54mm
SMD 4x-dip-switch SPST , Slide, row spacing 8.61 mm (338 mils), body size 9.78x12.34mm (see e.g. https://www.ctscorp.com/wp-content/uploads/204.pdf), SMD
SMD DIP Switch SPST Slide 8.61mm 338mil SMD
0
8
8
Button_Switch_SMD
SW_DIP_SPSTx04_Slide_Copal_CHS-04A_W5.08mm_P1.27mm_JPin
SMD 4x-dip-switch SPST Copal_CHS-04A, Slide, row spacing 5.08 mm (200 mils), body size  (see http://www.nidec-copal-electronics.com/e/catalog/switch/chs.pdf), SMD, JPin
SMD DIP Switch SPST Slide 5.08mm 200mil SMD JPin
0
8
8
Button_Switch_SMD
SW_DIP_SPSTx04_Slide_Copal_CHS-04B_W7.62mm_P1.27mm
SMD 4x-dip-switch SPST Copal_CHS-04B, Slide, row spacing 7.62 mm (300 mils), body size  (see http://www.nidec-copal-electronics.com/e/catalog/switch/chs.pdf), SMD
SMD DIP Switch SPST Slide 7.62mm 300mil SMD
0
8
8
Button_Switch_SMD
SW_DIP_SPSTx04_Slide_Copal_CVS-04xB_W5.9mm_P1mm
SMD 4x-dip-switch SPST Copal_CVS-04xB, Slide, row spacing 5.9 mm (232 mils), body size  (see http://www.nidec-copal-electronics.com/e/catalog/switch/cvs.pdf)
SMD DIP Switch SPST Slide 5.9mm 232mil
0
12
9
Button_Switch_SMD
SW_DIP_SPSTx04_Slide_KingTek_DSHP04TJ_W5.25mm_P1.27mm_JPin
SMD 4x-dip-switch SPST KingTek_DSHP04TJ, Slide, row spacing 5.25 mm (206 mils), body size  (see http://www.kingtek.net.cn/pic/201601201446313350.pdf), JPin
SMD DIP Switch SPST Slide 5.25mm 206mil JPin
0
8
8
Button_Switch_SMD
SW_DIP_SPSTx04_Slide_KingTek_DSHP04TS_W7.62mm_P1.27mm
SMD 4x-dip-switch SPST KingTek_DSHP04TS, Slide, row spacing 7.62 mm (300 mils), body size  (see http://www.kingtek.net.cn/pic/201601201417455112.pdf)
SMD DIP Switch SPST Slide 7.62mm 300mil
0
8
8
Button_Switch_SMD
SW_DIP_SPSTx04_Slide_Omron_A6H-4101_W6.15mm_P1.27mm
SMD 4x-dip-switch SPST Omron_A6H-4101, Slide, row spacing 6.15 mm (242 mils), body size  (see https://www.omron.com/ecb/products/pdf/en-a6h.pdf)
SMD DIP Switch SPST Slide 6.15mm 242mil
0
8
8
Button_Switch_SMD
SW_DIP_SPSTx04_Slide_Omron_A6S-410x_W8.9mm_P2.54mm
SMD 4x-dip-switch SPST Omron_A6S-410x, Slide, row spacing 8.9 mm (350 mils), body size  (see http://omronfs.omron.com/en_US/ecb/products/pdf/en-a6s.pdf)
SMD DIP Switch SPST Slide 8.9mm 350mil
0
8
8
Button_Switch_SMD
SW_DIP_SPSTx05_Slide_6.7x14.26mm_W6.73mm_P2.54mm_LowProfile_JPin
SMD 5x-dip-switch SPST , Slide, row spacing 6.73 mm (264 mils), body size 6.7x14.26mm (see e.g. https://www.ctscorp.com/wp-content/uploads/219.pdf), SMD, LowProfile, JPin
SMD DIP Switch SPST Slide 6.73mm 264mil SMD LowProfile JPin
0
10
10
Button_Switch_SMD
SW_DIP_SPSTx05_Slide_6.7x14.26mm_W8.61mm_P2.54mm_LowProfile
SMD 5x-dip-switch SPST , Slide, row spacing 8.61 mm (338 mils), body size 6.7x14.26mm (see e.g. https://www.ctscorp.com/wp-content/uploads/219.pdf), SMD, LowProfile
SMD DIP Switch SPST Slide 8.61mm 338mil SMD LowProfile
0
10
10
Button_Switch_SMD
SW_DIP_SPSTx05_Slide_9.78x14.88mm_W8.61mm_P2.54mm
SMD 5x-dip-switch SPST , Slide, row spacing 8.61 mm (338 mils), body size 9.78x14.88mm (see e.g. https://www.ctscorp.com/wp-content/uploads/204.pdf), SMD
SMD DIP Switch SPST Slide 8.61mm 338mil SMD
0
10
10
Button_Switch_SMD
SW_DIP_SPSTx05_Slide_KingTek_DSHP05TJ_W5.25mm_P1.27mm_JPin
SMD 5x-dip-switch SPST KingTek_DSHP05TJ, Slide, row spacing 5.25 mm (206 mils), body size  (see http://www.kingtek.net.cn/pic/201601201446313350.pdf), JPin
SMD DIP Switch SPST Slide 5.25mm 206mil JPin
0
10
10
Button_Switch_SMD
SW_DIP_SPSTx05_Slide_KingTek_DSHP05TS_W7.62mm_P1.27mm
SMD 5x-dip-switch SPST KingTek_DSHP05TS, Slide, row spacing 7.62 mm (300 mils), body size  (see http://www.kingtek.net.cn/pic/201601201417455112.pdf)
SMD DIP Switch SPST Slide 7.62mm 300mil
0
10
10
Button_Switch_SMD
SW_DIP_SPSTx05_Slide_Omron_A6S-510x_W8.9mm_P2.54mm
SMD 5x-dip-switch SPST Omron_A6S-510x, Slide, row spacing 8.9 mm (350 mils), body size  (see http://omronfs.omron.com/en_US/ecb/products/pdf/en-a6s.pdf)
SMD DIP Switch SPST Slide 8.9mm 350mil
0
10
10
Button_Switch_SMD
SW_DIP_SPSTx06_Slide_6.7x16.8mm_W6.73mm_P2.54mm_LowProfile_JPin
SMD 6x-dip-switch SPST , Slide, row spacing 6.73 mm (264 mils), body size 6.7x16.8mm (see e.g. https://www.ctscorp.com/wp-content/uploads/219.pdf), SMD, LowProfile, JPin
SMD DIP Switch SPST Slide 6.73mm 264mil SMD LowProfile JPin
0
12
12
Button_Switch_SMD
SW_DIP_SPSTx06_Slide_6.7x16.8mm_W8.61mm_P2.54mm_LowProfile
SMD 6x-dip-switch SPST , Slide, row spacing 8.61 mm (338 mils), body size 6.7x16.8mm (see e.g. https://www.ctscorp.com/wp-content/uploads/219.pdf), SMD, LowProfile
SMD DIP Switch SPST Slide 8.61mm 338mil SMD LowProfile
0
12
12
Button_Switch_SMD
SW_DIP_SPSTx06_Slide_9.78x17.42mm_W8.61mm_P2.54mm
SMD 6x-dip-switch SPST , Slide, row spacing 8.61 mm (338 mils), body size 9.78x17.42mm (see e.g. https://www.ctscorp.com/wp-content/uploads/204.pdf), SMD
SMD DIP Switch SPST Slide 8.61mm 338mil SMD
0
12
12
Button_Switch_SMD
SW_DIP_SPSTx06_Slide_Copal_CHS-06A_W5.08mm_P1.27mm_JPin
SMD 6x-dip-switch SPST Copal_CHS-06A, Slide, row spacing 5.08 mm (200 mils), body size  (see http://www.nidec-copal-electronics.com/e/catalog/switch/chs.pdf), SMD, JPin
SMD DIP Switch SPST Slide 5.08mm 200mil SMD JPin
0
12
12
Button_Switch_SMD
SW_DIP_SPSTx06_Slide_Copal_CHS-06B_W7.62mm_P1.27mm
SMD 6x-dip-switch SPST Copal_CHS-06B, Slide, row spacing 7.62 mm (300 mils), body size  (see http://www.nidec-copal-electronics.com/e/catalog/switch/chs.pdf), SMD
SMD DIP Switch SPST Slide 7.62mm 300mil SMD
0
12
12
Button_Switch_SMD
SW_DIP_SPSTx06_Slide_KingTek_DSHP06TJ_W5.25mm_P1.27mm_JPin
SMD 6x-dip-switch SPST KingTek_DSHP06TJ, Slide, row spacing 5.25 mm (206 mils), body size  (see http://www.kingtek.net.cn/pic/201601201446313350.pdf), JPin
SMD DIP Switch SPST Slide 5.25mm 206mil JPin
0
12
12
Button_Switch_SMD
SW_DIP_SPSTx06_Slide_KingTek_DSHP06TS_W7.62mm_P1.27mm
SMD 6x-dip-switch SPST KingTek_DSHP06TS, Slide, row spacing 7.62 mm (300 mils), body size  (see http://www.kingtek.net.cn/pic/201601201417455112.pdf)
SMD DIP Switch SPST Slide 7.62mm 300mil
0
12
12
Button_Switch_SMD
SW_DIP_SPSTx06_Slide_Omron_A6H-6101_W6.15mm_P1.27mm
SMD 6x-dip-switch SPST Omron_A6H-6101, Slide, row spacing 6.15 mm (242 mils), body size  (see https://www.omron.com/ecb/products/pdf/en-a6h.pdf)
SMD DIP Switch SPST Slide 6.15mm 242mil
0
12
12
Button_Switch_SMD
SW_DIP_SPSTx06_Slide_Omron_A6S-610x_W8.9mm_P2.54mm
SMD 6x-dip-switch SPST Omron_A6S-610x, Slide, row spacing 8.9 mm (350 mils), body size  (see http://omronfs.omron.com/en_US/ecb/products/pdf/en-a6s.pdf)
SMD DIP Switch SPST Slide 8.9mm 350mil
0
12
12
Button_Switch_SMD
SW_DIP_SPSTx07_Slide_6.7x19.34mm_W6.73mm_P2.54mm_LowProfile_JPin
SMD 7x-dip-switch SPST , Slide, row spacing 6.73 mm (264 mils), body size 6.7x19.34mm (see e.g. https://www.ctscorp.com/wp-content/uploads/219.pdf), SMD, LowProfile, JPin
SMD DIP Switch SPST Slide 6.73mm 264mil SMD LowProfile JPin
0
14
14
Button_Switch_SMD
SW_DIP_SPSTx07_Slide_6.7x19.34mm_W8.61mm_P2.54mm_LowProfile
SMD 7x-dip-switch SPST , Slide, row spacing 8.61 mm (338 mils), body size 6.7x19.34mm (see e.g. https://www.ctscorp.com/wp-content/uploads/219.pdf), SMD, LowProfile
SMD DIP Switch SPST Slide 8.61mm 338mil SMD LowProfile
0
14
14
Button_Switch_SMD
SW_DIP_SPSTx07_Slide_9.78x19.96mm_W8.61mm_P2.54mm
SMD 7x-dip-switch SPST , Slide, row spacing 8.61 mm (338 mils), body size 9.78x19.96mm (see e.g. https://www.ctscorp.com/wp-content/uploads/204.pdf), SMD
SMD DIP Switch SPST Slide 8.61mm 338mil SMD
0
14
14
Button_Switch_SMD
SW_DIP_SPSTx07_Slide_KingTek_DSHP07TJ_W5.25mm_P1.27mm_JPin
SMD 7x-dip-switch SPST KingTek_DSHP07TJ, Slide, row spacing 5.25 mm (206 mils), body size  (see http://www.kingtek.net.cn/pic/201601201446313350.pdf), JPin
SMD DIP Switch SPST Slide 5.25mm 206mil JPin
0
14
14
Button_Switch_SMD
SW_DIP_SPSTx07_Slide_KingTek_DSHP07TS_W7.62mm_P1.27mm
SMD 7x-dip-switch SPST KingTek_DSHP07TS, Slide, row spacing 7.62 mm (300 mils), body size  (see http://www.kingtek.net.cn/pic/201601201417455112.pdf)
SMD DIP Switch SPST Slide 7.62mm 300mil
0
14
14
Button_Switch_SMD
SW_DIP_SPSTx07_Slide_Omron_A6S-710x_W8.9mm_P2.54mm
SMD 7x-dip-switch SPST Omron_A6S-710x, Slide, row spacing 8.9 mm (350 mils), body size  (see http://omronfs.omron.com/en_US/ecb/products/pdf/en-a6s.pdf)
SMD DIP Switch SPST Slide 8.9mm 350mil
0
14
14
Button_Switch_SMD
SW_DIP_SPSTx08_Slide_6.7x21.88mm_W6.73mm_P2.54mm_LowProfile_JPin
SMD 8x-dip-switch SPST , Slide, row spacing 6.73 mm (264 mils), body size 6.7x21.88mm (see e.g. https://www.ctscorp.com/wp-content/uploads/219.pdf), SMD, LowProfile, JPin
SMD DIP Switch SPST Slide 6.73mm 264mil SMD LowProfile JPin
0
16
16
Button_Switch_SMD
SW_DIP_SPSTx08_Slide_6.7x21.88mm_W8.61mm_P2.54mm_LowProfile
SMD 8x-dip-switch SPST , Slide, row spacing 8.61 mm (338 mils), body size 6.7x21.88mm (see e.g. https://www.ctscorp.com/wp-content/uploads/219.pdf), SMD, LowProfile
SMD DIP Switch SPST Slide 8.61mm 338mil SMD LowProfile
0
16
16
Button_Switch_SMD
SW_DIP_SPSTx08_Slide_9.78x22.5mm_W8.61mm_P2.54mm
SMD 8x-dip-switch SPST , Slide, row spacing 8.61 mm (338 mils), body size 9.78x22.5mm (see e.g. https://www.ctscorp.com/wp-content/uploads/204.pdf), SMD
SMD DIP Switch SPST Slide 8.61mm 338mil SMD
0
16
16
Button_Switch_SMD
SW_DIP_SPSTx08_Slide_Copal_CHS-08A_W5.08mm_P1.27mm_JPin
SMD 8x-dip-switch SPST Copal_CHS-08A, Slide, row spacing 5.08 mm (200 mils), body size  (see http://www.nidec-copal-electronics.com/e/catalog/switch/chs.pdf), SMD, JPin
SMD DIP Switch SPST Slide 5.08mm 200mil SMD JPin
0
16
16
Button_Switch_SMD
SW_DIP_SPSTx08_Slide_Copal_CHS-08B_W7.62mm_P1.27mm
SMD 8x-dip-switch SPST Copal_CHS-08B, Slide, row spacing 7.62 mm (300 mils), body size  (see http://www.nidec-copal-electronics.com/e/catalog/switch/chs.pdf), SMD
SMD DIP Switch SPST Slide 7.62mm 300mil SMD
0
16
16
Button_Switch_SMD
SW_DIP_SPSTx08_Slide_Copal_CVS-08xB_W5.9mm_P1mm
SMD 8x-dip-switch SPST Copal_CVS-08xB, Slide, row spacing 5.9 mm (232 mils), body size  (see http://www.nidec-copal-electronics.com/e/catalog/switch/cvs.pdf)
SMD DIP Switch SPST Slide 5.9mm 232mil
0
20
17
Button_Switch_SMD
SW_DIP_SPSTx08_Slide_KingTek_DSHP08TJ_W5.25mm_P1.27mm_JPin
SMD 8x-dip-switch SPST KingTek_DSHP08TJ, Slide, row spacing 5.25 mm (206 mils), body size  (see http://www.kingtek.net.cn/pic/201601201446313350.pdf), JPin
SMD DIP Switch SPST Slide 5.25mm 206mil JPin
0
16
16
Button_Switch_SMD
SW_DIP_SPSTx08_Slide_KingTek_DSHP08TS_W7.62mm_P1.27mm
SMD 8x-dip-switch SPST KingTek_DSHP08TS, Slide, row spacing 7.62 mm (300 mils), body size  (see http://www.kingtek.net.cn/pic/201601201417455112.pdf)
SMD DIP Switch SPST Slide 7.62mm 300mil
0
16
16
Button_Switch_SMD
SW_DIP_SPSTx08_Slide_Omron_A6H-8101_W6.15mm_P1.27mm
SMD 8x-dip-switch SPST Omron_A6H-8101, Slide, row spacing 6.15 mm (242 mils), body size  (see https://www.omron.com/ecb/products/pdf/en-a6h.pdf)
SMD DIP Switch SPST Slide 6.15mm 242mil
0
16
16
Button_Switch_SMD
SW_DIP_SPSTx08_Slide_Omron_A6S-810x_W8.9mm_P2.54mm
SMD 8x-dip-switch SPST Omron_A6S-810x, Slide, row spacing 8.9 mm (350 mils), body size  (see http://omronfs.omron.com/en_US/ecb/products/pdf/en-a6s.pdf)
SMD DIP Switch SPST Slide 8.9mm 350mil
0
16
16
Button_Switch_SMD
SW_DIP_SPSTx09_Slide_6.7x24.42mm_W6.73mm_P2.54mm_LowProfile_JPin
SMD 9x-dip-switch SPST , Slide, row spacing 6.73 mm (264 mils), body size 6.7x24.42mm (see e.g. https://www.ctscorp.com/wp-content/uploads/219.pdf), SMD, LowProfile, JPin
SMD DIP Switch SPST Slide 6.73mm 264mil SMD LowProfile JPin
0
18
18
Button_Switch_SMD
SW_DIP_SPSTx09_Slide_6.7x24.42mm_W8.61mm_P2.54mm_LowProfile
SMD 9x-dip-switch SPST , Slide, row spacing 8.61 mm (338 mils), body size 6.7x24.42mm (see e.g. https://www.ctscorp.com/wp-content/uploads/219.pdf), SMD, LowProfile
SMD DIP Switch SPST Slide 8.61mm 338mil SMD LowProfile
0
18
18
Button_Switch_SMD
SW_DIP_SPSTx09_Slide_9.78x25.04mm_W8.61mm_P2.54mm
SMD 9x-dip-switch SPST , Slide, row spacing 8.61 mm (338 mils), body size 9.78x25.04mm (see e.g. https://www.ctscorp.com/wp-content/uploads/204.pdf), SMD
SMD DIP Switch SPST Slide 8.61mm 338mil SMD
0
18
18
Button_Switch_SMD
SW_DIP_SPSTx09_Slide_KingTek_DSHP09TJ_W5.25mm_P1.27mm_JPin
SMD 9x-dip-switch SPST KingTek_DSHP09TJ, Slide, row spacing 5.25 mm (206 mils), body size  (see http://www.kingtek.net.cn/pic/201601201446313350.pdf), JPin
SMD DIP Switch SPST Slide 5.25mm 206mil JPin
0
18
18
Button_Switch_SMD
SW_DIP_SPSTx09_Slide_KingTek_DSHP09TS_W7.62mm_P1.27mm
SMD 9x-dip-switch SPST KingTek_DSHP09TS, Slide, row spacing 7.62 mm (300 mils), body size  (see http://www.kingtek.net.cn/pic/201601201417455112.pdf)
SMD DIP Switch SPST Slide 7.62mm 300mil
0
18
18
Button_Switch_SMD
SW_DIP_SPSTx09_Slide_Omron_A6S-910x_W8.9mm_P2.54mm
SMD 9x-dip-switch SPST Omron_A6S-910x, Slide, row spacing 8.9 mm (350 mils), body size  (see http://omronfs.omron.com/en_US/ecb/products/pdf/en-a6s.pdf)
SMD DIP Switch SPST Slide 8.9mm 350mil
0
18
18
Button_Switch_SMD
SW_DIP_SPSTx10_Slide_6.7x26.96mm_W6.73mm_P2.54mm_LowProfile_JPin
SMD 10x-dip-switch SPST , Slide, row spacing 6.73 mm (264 mils), body size 6.7x26.96mm (see e.g. https://www.ctscorp.com/wp-content/uploads/219.pdf), SMD, LowProfile, JPin
SMD DIP Switch SPST Slide 6.73mm 264mil SMD LowProfile JPin
0
20
20
Button_Switch_SMD
SW_DIP_SPSTx10_Slide_6.7x26.96mm_W8.61mm_P2.54mm_LowProfile
SMD 10x-dip-switch SPST , Slide, row spacing 8.61 mm (338 mils), body size 6.7x26.96mm (see e.g. https://www.ctscorp.com/wp-content/uploads/219.pdf), SMD, LowProfile
SMD DIP Switch SPST Slide 8.61mm 338mil SMD LowProfile
0
20
20
Button_Switch_SMD
SW_DIP_SPSTx10_Slide_9.78x27.58mm_W8.61mm_P2.54mm
SMD 10x-dip-switch SPST , Slide, row spacing 8.61 mm (338 mils), body size 9.78x27.58mm (see e.g. https://www.ctscorp.com/wp-content/uploads/204.pdf), SMD
SMD DIP Switch SPST Slide 8.61mm 338mil SMD
0
20
20
Button_Switch_SMD
SW_DIP_SPSTx10_Slide_Copal_CHS-10A_W5.08mm_P1.27mm_JPin
SMD 10x-dip-switch SPST Copal_CHS-10A, Slide, row spacing 5.08 mm (200 mils), body size  (see http://www.nidec-copal-electronics.com/e/catalog/switch/chs.pdf), SMD, JPin
SMD DIP Switch SPST Slide 5.08mm 200mil SMD JPin
0
20
20
Button_Switch_SMD
SW_DIP_SPSTx10_Slide_Copal_CHS-10B_W7.62mm_P1.27mm
SMD 10x-dip-switch SPST Copal_CHS-10B, Slide, row spacing 7.62 mm (300 mils), body size  (see http://www.nidec-copal-electronics.com/e/catalog/switch/chs.pdf), SMD
SMD DIP Switch SPST Slide 7.62mm 300mil SMD
0
20
20
Button_Switch_SMD
SW_DIP_SPSTx10_Slide_KingTek_DSHP10TJ_W5.25mm_P1.27mm_JPin
SMD 10x-dip-switch SPST KingTek_DSHP10TJ, Slide, row spacing 5.25 mm (206 mils), body size  (see http://www.kingtek.net.cn/pic/201601201446313350.pdf), JPin
SMD DIP Switch SPST Slide 5.25mm 206mil JPin
0
20
20
Button_Switch_SMD
SW_DIP_SPSTx10_Slide_KingTek_DSHP10TS_W7.62mm_P1.27mm
SMD 10x-dip-switch SPST KingTek_DSHP10TS, Slide, row spacing 7.62 mm (300 mils), body size  (see http://www.kingtek.net.cn/pic/201601201417455112.pdf)
SMD DIP Switch SPST Slide 7.62mm 300mil
0
20
20
Button_Switch_SMD
SW_DIP_SPSTx10_Slide_Omron_A6H-10101_W6.15mm_P1.27mm
SMD 10x-dip-switch SPST Omron_A6H-10101, Slide, row spacing 6.15 mm (242 mils), body size  (see https://www.omron.com/ecb/products/pdf/en-a6h.pdf)
SMD DIP Switch SPST Slide 6.15mm 242mil
0
20
20
Button_Switch_SMD
SW_DIP_SPSTx10_Slide_Omron_A6S-1010x_W8.9mm_P2.54mm
SMD 10x-dip-switch SPST Omron_A6S-1010x, Slide, row spacing 8.9 mm (350 mils), body size  (see http://omronfs.omron.com/en_US/ecb/products/pdf/en-a6s.pdf)
SMD DIP Switch SPST Slide 8.9mm 350mil
0
20
20
Button_Switch_SMD
SW_DIP_SPSTx11_Slide_6.7x29.5mm_W6.73mm_P2.54mm_LowProfile_JPin
SMD 11x-dip-switch SPST , Slide, row spacing 6.73 mm (264 mils), body size 6.7x29.5mm (see e.g. https://www.ctscorp.com/wp-content/uploads/219.pdf), SMD, LowProfile, JPin
SMD DIP Switch SPST Slide 6.73mm 264mil SMD LowProfile JPin
0
22
22
Button_Switch_SMD
SW_DIP_SPSTx11_Slide_6.7x29.5mm_W8.61mm_P2.54mm_LowProfile
SMD 11x-dip-switch SPST , Slide, row spacing 8.61 mm (338 mils), body size 6.7x29.5mm (see e.g. https://www.ctscorp.com/wp-content/uploads/219.pdf), SMD, LowProfile
SMD DIP Switch SPST Slide 8.61mm 338mil SMD LowProfile
0
22
22
Button_Switch_SMD
SW_DIP_SPSTx11_Slide_9.78x30.12mm_W8.61mm_P2.54mm
SMD 11x-dip-switch SPST , Slide, row spacing 8.61 mm (338 mils), body size 9.78x30.12mm (see e.g. https://www.ctscorp.com/wp-content/uploads/204.pdf), SMD
SMD DIP Switch SPST Slide 8.61mm 338mil SMD
0
22
22
Button_Switch_SMD
SW_DIP_SPSTx12_Slide_6.7x32.04mm_W6.73mm_P2.54mm_LowProfile_JPin
SMD 12x-dip-switch SPST , Slide, row spacing 6.73 mm (264 mils), body size 6.7x32.04mm (see e.g. https://www.ctscorp.com/wp-content/uploads/219.pdf), SMD, LowProfile, JPin
SMD DIP Switch SPST Slide 6.73mm 264mil SMD LowProfile JPin
0
24
24
Button_Switch_SMD
SW_DIP_SPSTx12_Slide_6.7x32.04mm_W8.61mm_P2.54mm_LowProfile
SMD 12x-dip-switch SPST , Slide, row spacing 8.61 mm (338 mils), body size 6.7x32.04mm (see e.g. https://www.ctscorp.com/wp-content/uploads/219.pdf), SMD, LowProfile
SMD DIP Switch SPST Slide 8.61mm 338mil SMD LowProfile
0
24
24
Button_Switch_SMD
SW_DIP_SPSTx12_Slide_9.78x32.66mm_W8.61mm_P2.54mm
SMD 12x-dip-switch SPST , Slide, row spacing 8.61 mm (338 mils), body size 9.78x32.66mm (see e.g. https://www.ctscorp.com/wp-content/uploads/204.pdf), SMD
SMD DIP Switch SPST Slide 8.61mm 338mil SMD
0
24
24
Button_Switch_SMD
SW_DPDT_CK_JS202011JCQN
Sub-miniature slide switch, vertical, SMT J bend https://dznh3ojzb2azq.cloudfront.net/products/Slide/JS/documents/datasheet.pdf
switch DPDT SMT
0
6
6
Button_Switch_SMD
SW_MEC_5GSH9
MEC 5G single pole normally-open tactile switch
switch normally-open pushbutton push-button
0
4
4
Button_Switch_SMD
SW_Push_1P1T-MP_NO_Horizontal_Alps_SKRTLAE010
Side push button (https://www.alps.com/prod/info/E/PDF/Tact/SurfaceMount/SKRT/SKRT.pdf)
push horizontal SPST 1P1T
0
5
3
Button_Switch_SMD
SW_Push_1P1T-SH_NO_CK_KMR2xxG
CK components KMR2 tactile switch with ground pin http://www.ckswitches.com/media/1479/kmr2.pdf
tactile switch kmr2
0
5
3
Button_Switch_SMD
SW_Push_1P1T_NO_6x6mm_H9.5mm
tactile push button, 6x6mm e.g. PTS645xx series, height=9.5mm
tact sw push 6mm smd
0
4
2
Button_Switch_SMD
SW_Push_1P1T_NO_CK_KMR2
CK components KMR2 tactile switch http://www.ckswitches.com/media/1479/kmr2.pdf
tactile switch kmr2
0
4
2
Button_Switch_SMD
SW_Push_1P1T_NO_CK_KSC6xxJ
CK components KSC6 tactile switch https://www.ckswitches.com/media/1972/ksc6.pdf
tactile switch ksc6
0
4
2
Button_Switch_SMD
SW_Push_1P1T_NO_CK_KSC7xxJ
CK components KSC7 tactile switch https://www.ckswitches.com/media/1973/ksc7.pdf
tactile switch ksc7
0
4
2
Button_Switch_SMD
SW_Push_1P1T_NO_CK_PTS125Sx43PSMTR
C&K Switches 1P1T SMD PTS125 Series 12mm Tact Switch with Pegs, https://www.ckswitches.com/media/1462/pts125.pdf
Button Tactile Switch SPST 1P1T
0
4
2
Button_Switch_SMD
SW_Push_1P1T_NO_Vertical_Wuerth_434133025816
https://katalog.we-online.com/em/datasheet/434133025816.pdf
tactile switch Wurth Wuerth
0
4
2
Button_Switch_SMD
SW_Push_SPST_NO_Alps_SKRK
http://www.alps.com/prod/info/E/HTML/Tact/SurfaceMount/SKRK/SKRKAHE020.html
SMD SMT button
0
2
2
Button_Switch_SMD
SW_SP3T_PCM13
Ultraminiature Surface Mount Slide Switch, right-angle, https://www.ckswitches.com/media/1424/pcm.pdf

0
8
4
Button_Switch_SMD
SW_SPDT_CK-JS102011SAQN
Sub-miniature slide switch, right-angle, http://www.ckswitches.com/media/1422/js.pdf
switch spdt
0
3
3
Button_Switch_SMD
SW_SPDT_PCM12
Ultraminiature Surface Mount Slide Switch, right-angle, https://www.ckswitches.com/media/1424/pcm.pdf

0
7
3
Button_Switch_SMD
SW_SPST_B3S-1000
Surface Mount Tactile Switch for High-Density Packaging
Tactile Switch
0
4
2
Button_Switch_SMD
SW_SPST_B3S-1100
Surface Mount Tactile Switch for High-Density Packaging with Ground Terminal
Tactile Switch
0
5
3
Button_Switch_SMD
SW_SPST_B3SL-1002P
Middle Stroke Tactile Switch, B3SL
Middle Stroke Tactile Switch
0
4
2
Button_Switch_SMD
SW_SPST_B3SL-1022P
Middle Stroke Tactile Switch, B3SL
Middle Stroke Tactile Switch
0
4
2
Button_Switch_SMD
SW_SPST_B3U-1000P
Ultra-small-sized Tactile Switch with High Contact Reliability, Top-actuated Model, without Ground Terminal, without Boss
Tactile Switch
0
2
2
Button_Switch_SMD
SW_SPST_B3U-1000P-B
Ultra-small-sized Tactile Switch with High Contact Reliability, Top-actuated Model, without Ground Terminal, with Boss
Tactile Switch
0
2
2
Button_Switch_SMD
SW_SPST_B3U-1100P
Ultra-small-sized Tactile Switch with High Contact Reliability, Top-actuated Model, with Ground Terminal, without Boss
Tactile Switch
0
3
3
Button_Switch_SMD
SW_SPST_B3U-1100P-B
Ultra-small-sized Tactile Switch with High Contact Reliability, Top-actuated Model, with Ground Terminal, with Boss
Tactile Switch
0
3
3
Button_Switch_SMD
SW_SPST_B3U-3000P
Ultra-small-sized Tactile Switch with High Contact Reliability, Side-actuated Model, without Ground Terminal, without Boss
Tactile Switch
0
2
2
Button_Switch_SMD
SW_SPST_B3U-3000P-B
Ultra-small-sized Tactile Switch with High Contact Reliability, Side-actuated Model, without Ground Terminal, with Boss
Tactile Switch
0
2
2
Button_Switch_SMD
SW_SPST_B3U-3100P
Ultra-small-sized Tactile Switch with High Contact Reliability, Side-actuated Model, with Ground Terminal, without Boss
Tactile Switch
0
3
3
Button_Switch_SMD
SW_SPST_B3U-3100P-B
Ultra-small-sized Tactile Switch with High Contact Reliability, Side-actuated Model, with Ground Terminal, with Boss
Tactile Switch
0
3
3
Button_Switch_SMD
SW_SPST_CK_KXT3
https://www.ckswitches.com/media/1465/kxt3.pdf
Switch SPST KXT3
0
2
2
Button_Switch_SMD
SW_SPST_CK_RS282G05A3
https://www.mouser.com/ds/2/60/RS-282G05A-SM_RT-1159762.pdf
SPST button tactile switch
0
2
2
Button_Switch_SMD
SW_SPST_EVPBF
Light Touch Switch

0
4
2
Button_Switch_SMD
SW_SPST_EVQP0
Light Touch Switch, https://industrial.panasonic.com/cdbs/www-data/pdf/ATK0000/ATK0000CE28.pdf

0
4
2
Button_Switch_SMD
SW_SPST_EVQP2
Light Touch Switch, https://industrial.panasonic.com/cdbs/www-data/pdf/ATK0000/ATK0000C374.pdf
SMD SMT SPST EVQP2
0
4
2
Button_Switch_SMD
SW_SPST_EVQP7A
Light Touch Switch,https://industrial.panasonic.com/cdbs/www-data/pdf/ATK0000/ATK0000CE20.pdf

0
4
2
Button_Switch_SMD
SW_SPST_EVQP7C
Light Touch Switch

0
4
2
Button_Switch_SMD
SW_SPST_EVQPE1
Light Touch Switch, https://industrial.panasonic.com/cdbs/www-data/pdf/ATK0000/ATK0000CE7.pdf

0
2
2
Button_Switch_SMD
SW_SPST_EVQQ2
Light Touch Switch, https://industrial.panasonic.com/cdbs/www-data/pdf/ATK0000/ATK0000CE28.pdf

0
4
2
Button_Switch_SMD
SW_SPST_FSMSM
http://www.te.com/commerce/DocumentDelivery/DDEController?Action=srchrtrv&DocNm=1437566-3&DocType=Customer+Drawing&DocLang=English
SPST button tactile switch
0
2
2
Button_Switch_SMD
SW_SPST_Omron_B3FS-100xP
Surface Mount Tactile Switch for High-Density Mounting, 3.1mm height, https://omronfs.omron.com/en_US/ecb/products/pdf/en-b3fs.pdf
Tactile Switch
0
4
2
Button_Switch_SMD
SW_SPST_Omron_B3FS-101xP
Surface Mount Tactile Switch for High-Density Mounting, 4.3mm height, https://omronfs.omron.com/en_US/ecb/products/pdf/en-b3fs.pdf
Tactile Switch
0
4
2
Button_Switch_SMD
SW_SPST_Omron_B3FS-105xP
Surface Mount Tactile Switch for High-Density Mounting, 7.3mm height, https://omronfs.omron.com/en_US/ecb/products/pdf/en-b3fs.pdf
Tactile Switch
0
4
2
Button_Switch_SMD
SW_SPST_PTS645
C&K Components SPST SMD PTS645 Series 6mm Tact Switch
SPST Button Switch
0
4
2
Button_Switch_SMD
SW_SPST_PTS810
C&K Components, PTS 810 Series, Microminiature SMT Top Actuated, http://www.ckswitches.com/media/1476/pts810.pdf
SPST Button Switch
0
4
2
Button_Switch_SMD
SW_SPST_Panasonic_EVQPL_3PL_5PL_PT_A08
Light Touch Switch, http://industrial.panasonic.com/cdbs/www-data/pdf/ATK0000/ATK0000CE3.pdf
SMD SMT SPST EVQPL EVQPT
0
6
3
Button_Switch_SMD
SW_SPST_Panasonic_EVQPL_3PL_5PL_PT_A15
Light Touch Switch, http://industrial.panasonic.com/cdbs/www-data/pdf/ATK0000/ATK0000CE3.pdf
SMD SMT SPST EVQPL EVQPT
0
6
3
Button_Switch_SMD
SW_SPST_REED_CT05-XXXX-G1
Coto Technologies SPST Reed Switch CT05-XXXX-G1
Coto Reed SPST Switch
0
2
2
Button_Switch_SMD
SW_SPST_REED_CT05-XXXX-J1
Coto Technologies SPST Reed Switch CT05-XXXX-J1
Coto Reed SPST Switch
0
2
2
Button_Switch_SMD
SW_SPST_REED_CT10-XXXX-G1
Coto Technologies SPST Reed Switch CT10-XXXX-G1
Coto Reed SPST Switch
0
2
2
Button_Switch_SMD
SW_SPST_REED_CT10-XXXX-G2
Coto Technologies SPST Reed Switch CT10-XXXX-G2
Coto Reed SPST Switch
0
2
2
Button_Switch_SMD
SW_SPST_REED_CT10-XXXX-G4
Coto Technologies SPST Reed Switch CT10-XXXX-G4
Coto Reed SPST Switch
0
2
2
Button_Switch_SMD
SW_SPST_SKQG_WithStem
ALPS 5.2mm Square Low-profile Type (Surface Mount) SKQG Series, With stem, http://www.alps.com/prod/info/E/HTML/Tact/SurfaceMount/SKQG/SKQGAFE010.html
SPST Button Switch
0
4
2
Button_Switch_SMD
SW_SPST_SKQG_WithoutStem
ALPS 5.2mm Square Low-profile Type (Surface Mount) SKQG Series, Without stem, http://www.alps.com/prod/info/E/HTML/Tact/SurfaceMount/SKQG/SKQGAEE010.html
SPST Button Switch
0
4
2
Button_Switch_SMD
SW_SPST_TL3305A
https://www.e-switch.com/system/asset/product_line/data_sheet/213/TL3305.pdf
TL3305 Series Tact Switch
0
4
2
Button_Switch_SMD
SW_SPST_TL3305B
https://www.e-switch.com/system/asset/product_line/data_sheet/213/TL3305.pdf
TL3305 Series Tact Switch
0
4
2
Button_Switch_SMD
SW_SPST_TL3305C
https://www.e-switch.com/system/asset/product_line/data_sheet/213/TL3305.pdf
TL3305 Series Tact Switch
0
4
2
Button_Switch_SMD
SW_SPST_TL3342
Low-profile SMD Tactile Switch, https://www.e-switch.com/system/asset/product_line/data_sheet/165/TL3342.pdf
SPST Tactile Switch
0
4
2
Button_Switch_THT
KSA_Tactile_SPST
KSA http://www.ckswitches.com/media/1457/ksa_ksl.pdf
SWITCH SMD KSA SW
0
5
5
Button_Switch_THT
Nidec_Copal_SH-7010C
4-bit rotary coded switch, through-hole, https://www.nidec-copal-electronics.com/e/catalog/switch/sh-7000.pdf
rotary switch bcd
0
6
5
Button_Switch_THT
Push_E-Switch_KS01Q01
E-Switch KS01Q01 http://spec_sheets.e-switch.com/specs/29-KS01Q01.pdf
Push Button
0
4
4
Button_Switch_THT
SW_CW_GPTS203211B
SPST Off-On Pushbutton, 1A, 30V, CW Industries P/N GPTS203211B, http://switches-connectors-custom.cwind.com/Asset/GPTS203211BR2.pdf
SPST button switch Off-On
0
2
2
Button_Switch_THT
SW_CuK_JS202011AQN_DPDT_Angled
CuK sub miniature slide switch, JS series, DPDT, right angle, http://www.ckswitches.com/media/1422/js.pdf
switch DPDT
0
6
6
Button_Switch_THT
SW_CuK_JS202011CQN_DPDT_Straight
CuK sub miniature slide switch, JS series, DPDT, right angle, http://www.ckswitches.com/media/1422/js.pdf
switch DPDT
0
6
6
Button_Switch_THT
SW_CuK_OS102011MA1QN1_SPDT_Angled
CuK miniature slide switch, OS series, SPDT, right angle, http://www.ckswitches.com/media/1428/os.pdf
switch SPDT
0
5
3
Button_Switch_THT
SW_DIP_SPSTx01_Piano_10.8x4.1mm_W7.62mm_P2.54mm
1x-dip-switch SPST , Piano, row spacing 7.62 mm (300 mils), body size 10.8x4.1mm
DIP Switch SPST Piano 7.62mm 300mil
0
2
2
Button_Switch_THT
SW_DIP_SPSTx01_Slide_6.7x4.1mm_W7.62mm_P2.54mm_LowProfile
1x-dip-switch SPST , Slide, row spacing 7.62 mm (300 mils), body size 6.7x4.1mm (see e.g. https://www.ctscorp.com/wp-content/uploads/209-210.pdf), LowProfile
DIP Switch SPST Slide 7.62mm 300mil LowProfile
0
2
2
Button_Switch_THT
SW_DIP_SPSTx01_Slide_9.78x4.72mm_W7.62mm_P2.54mm
1x-dip-switch SPST , Slide, row spacing 7.62 mm (300 mils), body size 9.78x4.72mm (see e.g. https://www.ctscorp.com/wp-content/uploads/206-208.pdf)
DIP Switch SPST Slide 7.62mm 300mil
0
2
2
Button_Switch_THT
SW_DIP_SPSTx02_Piano_10.8x6.64mm_W7.62mm_P2.54mm
2x-dip-switch SPST , Piano, row spacing 7.62 mm (300 mils), body size 10.8x6.64mm
DIP Switch SPST Piano 7.62mm 300mil
0
4
4
Button_Switch_THT
SW_DIP_SPSTx02_Piano_CTS_Series194-2MSTN_W7.62mm_P2.54mm
2x-dip-switch SPST CTS_Series194-2MSTN, Piano, row spacing 7.62 mm (300 mils), body size  (see https://www.ctscorp.com/wp-content/uploads/194-195.pdf)
DIP Switch SPST Piano 7.62mm 300mil
0
4
4
Button_Switch_THT
SW_DIP_SPSTx02_Slide_6.7x6.64mm_W7.62mm_P2.54mm_LowProfile
2x-dip-switch SPST , Slide, row spacing 7.62 mm (300 mils), body size 6.7x6.64mm (see e.g. https://www.ctscorp.com/wp-content/uploads/209-210.pdf), LowProfile
DIP Switch SPST Slide 7.62mm 300mil LowProfile
0
4
4
Button_Switch_THT
SW_DIP_SPSTx02_Slide_9.78x7.26mm_W7.62mm_P2.54mm
2x-dip-switch SPST , Slide, row spacing 7.62 mm (300 mils), body size 9.78x7.26mm (see e.g. https://www.ctscorp.com/wp-content/uploads/206-208.pdf)
DIP Switch SPST Slide 7.62mm 300mil
0
4
4
Button_Switch_THT
SW_DIP_SPSTx03_Piano_10.8x9.18mm_W7.62mm_P2.54mm
3x-dip-switch SPST , Piano, row spacing 7.62 mm (300 mils), body size 10.8x9.18mm
DIP Switch SPST Piano 7.62mm 300mil
0
6
6
Button_Switch_THT
SW_DIP_SPSTx03_Piano_CTS_Series194-3MSTN_W7.62mm_P2.54mm
3x-dip-switch SPST CTS_Series194-3MSTN, Piano, row spacing 7.62 mm (300 mils), body size  (see https://www.ctscorp.com/wp-content/uploads/194-195.pdf)
DIP Switch SPST Piano 7.62mm 300mil
0
6
6
Button_Switch_THT
SW_DIP_SPSTx03_Slide_6.7x9.18mm_W7.62mm_P2.54mm_LowProfile
3x-dip-switch SPST , Slide, row spacing 7.62 mm (300 mils), body size 6.7x9.18mm (see e.g. https://www.ctscorp.com/wp-content/uploads/209-210.pdf), LowProfile
DIP Switch SPST Slide 7.62mm 300mil LowProfile
0
6
6
Button_Switch_THT
SW_DIP_SPSTx03_Slide_9.78x9.8mm_W7.62mm_P2.54mm
3x-dip-switch SPST , Slide, row spacing 7.62 mm (300 mils), body size 9.78x9.8mm (see e.g. https://www.ctscorp.com/wp-content/uploads/206-208.pdf)
DIP Switch SPST Slide 7.62mm 300mil
0
6
6
Button_Switch_THT
SW_DIP_SPSTx04_Piano_10.8x11.72mm_W7.62mm_P2.54mm
4x-dip-switch SPST , Piano, row spacing 7.62 mm (300 mils), body size 10.8x11.72mm
DIP Switch SPST Piano 7.62mm 300mil
0
8
8
Button_Switch_THT
SW_DIP_SPSTx04_Piano_CTS_Series194-4MSTN_W7.62mm_P2.54mm
4x-dip-switch SPST CTS_Series194-4MSTN, Piano, row spacing 7.62 mm (300 mils), body size  (see https://www.ctscorp.com/wp-content/uploads/194-195.pdf)
DIP Switch SPST Piano 7.62mm 300mil
0
8
8
Button_Switch_THT
SW_DIP_SPSTx04_Slide_6.7x11.72mm_W7.62mm_P2.54mm_LowProfile
4x-dip-switch SPST , Slide, row spacing 7.62 mm (300 mils), body size 6.7x11.72mm (see e.g. https://www.ctscorp.com/wp-content/uploads/209-210.pdf), LowProfile
DIP Switch SPST Slide 7.62mm 300mil LowProfile
0
8
8
Button_Switch_THT
SW_DIP_SPSTx04_Slide_9.78x12.34mm_W7.62mm_P2.54mm
4x-dip-switch SPST , Slide, row spacing 7.62 mm (300 mils), body size 9.78x12.34mm (see e.g. https://www.ctscorp.com/wp-content/uploads/206-208.pdf)
DIP Switch SPST Slide 7.62mm 300mil
0
8
8
Button_Switch_THT
SW_DIP_SPSTx05_Piano_10.8x14.26mm_W7.62mm_P2.54mm
5x-dip-switch SPST , Piano, row spacing 7.62 mm (300 mils), body size 10.8x14.26mm
DIP Switch SPST Piano 7.62mm 300mil
0
10
10
Button_Switch_THT
SW_DIP_SPSTx05_Piano_CTS_Series194-5MSTN_W7.62mm_P2.54mm
5x-dip-switch SPST CTS_Series194-5MSTN, Piano, row spacing 7.62 mm (300 mils), body size  (see https://www.ctscorp.com/wp-content/uploads/194-195.pdf)
DIP Switch SPST Piano 7.62mm 300mil
0
10
10
Button_Switch_THT
SW_DIP_SPSTx05_Slide_6.7x14.26mm_W7.62mm_P2.54mm_LowProfile
5x-dip-switch SPST , Slide, row spacing 7.62 mm (300 mils), body size 6.7x14.26mm (see e.g. https://www.ctscorp.com/wp-content/uploads/209-210.pdf), LowProfile
DIP Switch SPST Slide 7.62mm 300mil LowProfile
0
10
10
Button_Switch_THT
SW_DIP_SPSTx05_Slide_9.78x14.88mm_W7.62mm_P2.54mm
5x-dip-switch SPST , Slide, row spacing 7.62 mm (300 mils), body size 9.78x14.88mm (see e.g. https://www.ctscorp.com/wp-content/uploads/206-208.pdf)
DIP Switch SPST Slide 7.62mm 300mil
0
10
10
Button_Switch_THT
SW_DIP_SPSTx06_Piano_10.8x16.8mm_W7.62mm_P2.54mm
6x-dip-switch SPST , Piano, row spacing 7.62 mm (300 mils), body size 10.8x16.8mm
DIP Switch SPST Piano 7.62mm 300mil
0
12
12
Button_Switch_THT
SW_DIP_SPSTx06_Piano_CTS_Series194-6MSTN_W7.62mm_P2.54mm
6x-dip-switch SPST CTS_Series194-6MSTN, Piano, row spacing 7.62 mm (300 mils), body size  (see https://www.ctscorp.com/wp-content/uploads/194-195.pdf)
DIP Switch SPST Piano 7.62mm 300mil
0
12
12
Button_Switch_THT
SW_DIP_SPSTx06_Slide_6.7x16.8mm_W7.62mm_P2.54mm_LowProfile
6x-dip-switch SPST , Slide, row spacing 7.62 mm (300 mils), body size 6.7x16.8mm (see e.g. https://www.ctscorp.com/wp-content/uploads/209-210.pdf), LowProfile
DIP Switch SPST Slide 7.62mm 300mil LowProfile
0
12
12
Button_Switch_THT
SW_DIP_SPSTx06_Slide_9.78x17.42mm_W7.62mm_P2.54mm
6x-dip-switch SPST , Slide, row spacing 7.62 mm (300 mils), body size 9.78x17.42mm (see e.g. https://www.ctscorp.com/wp-content/uploads/206-208.pdf)
DIP Switch SPST Slide 7.62mm 300mil
0
12
12
Button_Switch_THT
SW_DIP_SPSTx07_Piano_10.8x19.34mm_W7.62mm_P2.54mm
7x-dip-switch SPST , Piano, row spacing 7.62 mm (300 mils), body size 10.8x19.34mm
DIP Switch SPST Piano 7.62mm 300mil
0
14
14
Button_Switch_THT
SW_DIP_SPSTx07_Piano_CTS_Series194-7MSTN_W7.62mm_P2.54mm
7x-dip-switch SPST CTS_Series194-7MSTN, Piano, row spacing 7.62 mm (300 mils), body size  (see https://www.ctscorp.com/wp-content/uploads/194-195.pdf)
DIP Switch SPST Piano 7.62mm 300mil
0
14
14
Button_Switch_THT
SW_DIP_SPSTx07_Slide_6.7x19.34mm_W7.62mm_P2.54mm_LowProfile
7x-dip-switch SPST , Slide, row spacing 7.62 mm (300 mils), body size 6.7x19.34mm (see e.g. https://www.ctscorp.com/wp-content/uploads/209-210.pdf), LowProfile
DIP Switch SPST Slide 7.62mm 300mil LowProfile
0
14
14
Button_Switch_THT
SW_DIP_SPSTx07_Slide_9.78x19.96mm_W7.62mm_P2.54mm
7x-dip-switch SPST , Slide, row spacing 7.62 mm (300 mils), body size 9.78x19.96mm (see e.g. https://www.ctscorp.com/wp-content/uploads/206-208.pdf)
DIP Switch SPST Slide 7.62mm 300mil
0
14
14
Button_Switch_THT
SW_DIP_SPSTx08_Piano_10.8x21.88mm_W7.62mm_P2.54mm
8x-dip-switch SPST , Piano, row spacing 7.62 mm (300 mils), body size 10.8x21.88mm
DIP Switch SPST Piano 7.62mm 300mil
0
16
16
Button_Switch_THT
SW_DIP_SPSTx08_Piano_CTS_Series194-8MSTN_W7.62mm_P2.54mm
8x-dip-switch SPST CTS_Series194-8MSTN, Piano, row spacing 7.62 mm (300 mils), body size  (see https://www.ctscorp.com/wp-content/uploads/194-195.pdf)
DIP Switch SPST Piano 7.62mm 300mil
0
16
16
Button_Switch_THT
SW_DIP_SPSTx08_Slide_6.7x21.88mm_W7.62mm_P2.54mm_LowProfile
8x-dip-switch SPST , Slide, row spacing 7.62 mm (300 mils), body size 6.7x21.88mm (see e.g. https://www.ctscorp.com/wp-content/uploads/209-210.pdf), LowProfile
DIP Switch SPST Slide 7.62mm 300mil LowProfile
0
16
16
Button_Switch_THT
SW_DIP_SPSTx08_Slide_9.78x22.5mm_W7.62mm_P2.54mm
8x-dip-switch SPST , Slide, row spacing 7.62 mm (300 mils), body size 9.78x22.5mm (see e.g. https://www.ctscorp.com/wp-content/uploads/206-208.pdf)
DIP Switch SPST Slide 7.62mm 300mil
0
16
16
Button_Switch_THT
SW_DIP_SPSTx09_Piano_10.8x24.42mm_W7.62mm_P2.54mm
9x-dip-switch SPST , Piano, row spacing 7.62 mm (300 mils), body size 10.8x24.42mm
DIP Switch SPST Piano 7.62mm 300mil
0
18
18
Button_Switch_THT
SW_DIP_SPSTx09_Piano_CTS_Series194-9MSTN_W7.62mm_P2.54mm
9x-dip-switch SPST CTS_Series194-9MSTN, Piano, row spacing 7.62 mm (300 mils), body size  (see https://www.ctscorp.com/wp-content/uploads/194-195.pdf)
DIP Switch SPST Piano 7.62mm 300mil
0
18
18
Button_Switch_THT
SW_DIP_SPSTx09_Slide_6.7x24.42mm_W7.62mm_P2.54mm_LowProfile
9x-dip-switch SPST , Slide, row spacing 7.62 mm (300 mils), body size 6.7x24.42mm (see e.g. https://www.ctscorp.com/wp-content/uploads/209-210.pdf), LowProfile
DIP Switch SPST Slide 7.62mm 300mil LowProfile
0
18
18
Button_Switch_THT
SW_DIP_SPSTx09_Slide_9.78x25.04mm_W7.62mm_P2.54mm
9x-dip-switch SPST , Slide, row spacing 7.62 mm (300 mils), body size 9.78x25.04mm (see e.g. https://www.ctscorp.com/wp-content/uploads/206-208.pdf)
DIP Switch SPST Slide 7.62mm 300mil
0
18
18
Button_Switch_THT
SW_DIP_SPSTx10_Piano_10.8x26.96mm_W7.62mm_P2.54mm
10x-dip-switch SPST , Piano, row spacing 7.62 mm (300 mils), body size 10.8x26.96mm
DIP Switch SPST Piano 7.62mm 300mil
0
20
20
Button_Switch_THT
SW_DIP_SPSTx10_Piano_CTS_Series194-10MSTN_W7.62mm_P2.54mm
10x-dip-switch SPST CTS_Series194-10MSTN, Piano, row spacing 7.62 mm (300 mils), body size  (see https://www.ctscorp.com/wp-content/uploads/194-195.pdf)
DIP Switch SPST Piano 7.62mm 300mil
0
20
20
Button_Switch_THT
SW_DIP_SPSTx10_Slide_6.7x26.96mm_W7.62mm_P2.54mm_LowProfile
10x-dip-switch SPST , Slide, row spacing 7.62 mm (300 mils), body size 6.7x26.96mm (see e.g. https://www.ctscorp.com/wp-content/uploads/209-210.pdf), LowProfile
DIP Switch SPST Slide 7.62mm 300mil LowProfile
0
20
20
Button_Switch_THT
SW_DIP_SPSTx10_Slide_9.78x27.58mm_W7.62mm_P2.54mm
10x-dip-switch SPST , Slide, row spacing 7.62 mm (300 mils), body size 9.78x27.58mm (see e.g. https://www.ctscorp.com/wp-content/uploads/206-208.pdf)
DIP Switch SPST Slide 7.62mm 300mil
0
20
20
Button_Switch_THT
SW_DIP_SPSTx11_Piano_10.8x29.5mm_W7.62mm_P2.54mm
11x-dip-switch SPST , Piano, row spacing 7.62 mm (300 mils), body size 10.8x29.5mm
DIP Switch SPST Piano 7.62mm 300mil
0
22
22
Button_Switch_THT
SW_DIP_SPSTx11_Piano_CTS_Series194-11MSTN_W7.62mm_P2.54mm
11x-dip-switch SPST CTS_Series194-11MSTN, Piano, row spacing 7.62 mm (300 mils), body size  (see https://www.ctscorp.com/wp-content/uploads/194-195.pdf)
DIP Switch SPST Piano 7.62mm 300mil
0
22
22
Button_Switch_THT
SW_DIP_SPSTx11_Slide_6.7x29.5mm_W7.62mm_P2.54mm_LowProfile
11x-dip-switch SPST , Slide, row spacing 7.62 mm (300 mils), body size 6.7x29.5mm (see e.g. https://www.ctscorp.com/wp-content/uploads/209-210.pdf), LowProfile
DIP Switch SPST Slide 7.62mm 300mil LowProfile
0
22
22
Button_Switch_THT
SW_DIP_SPSTx11_Slide_9.78x30.12mm_W7.62mm_P2.54mm
11x-dip-switch SPST , Slide, row spacing 7.62 mm (300 mils), body size 9.78x30.12mm (see e.g. https://www.ctscorp.com/wp-content/uploads/206-208.pdf)
DIP Switch SPST Slide 7.62mm 300mil
0
22
22
Button_Switch_THT
SW_DIP_SPSTx12_Piano_10.8x32.04mm_W7.62mm_P2.54mm
12x-dip-switch SPST , Piano, row spacing 7.62 mm (300 mils), body size 10.8x32.04mm
DIP Switch SPST Piano 7.62mm 300mil
0
24
24
Button_Switch_THT
SW_DIP_SPSTx12_Piano_CTS_Series194-12MSTN_W7.62mm_P2.54mm
12x-dip-switch SPST CTS_Series194-12MSTN, Piano, row spacing 7.62 mm (300 mils), body size  (see https://www.ctscorp.com/wp-content/uploads/194-195.pdf)
DIP Switch SPST Piano 7.62mm 300mil
0
24
24
Button_Switch_THT
SW_DIP_SPSTx12_Slide_6.7x32.04mm_W7.62mm_P2.54mm_LowProfile
12x-dip-switch SPST , Slide, row spacing 7.62 mm (300 mils), body size 6.7x32.04mm (see e.g. https://www.ctscorp.com/wp-content/uploads/209-210.pdf), LowProfile
DIP Switch SPST Slide 7.62mm 300mil LowProfile
0
24
24
Button_Switch_THT
SW_DIP_SPSTx12_Slide_9.78x32.66mm_W7.62mm_P2.54mm
12x-dip-switch SPST , Slide, row spacing 7.62 mm (300 mils), body size 9.78x32.66mm (see e.g. https://www.ctscorp.com/wp-content/uploads/206-208.pdf)
DIP Switch SPST Slide 7.62mm 300mil
0
24
24
Button_Switch_THT
SW_E-Switch_EG1224_SPDT_Angled
E-Switch slide switch, EG series, SPDT, right angle, http://spec_sheets.e-switch.com/specs/P040042.pdf
switch SPDT
0
7
3
Button_Switch_THT
SW_E-Switch_EG1271_DPDT
E-Switch sub miniature slide switch, EG series, DPDT, http://spec_sheets.e-switch.com/specs/P040047.pdf
switch DPDT
0
6
6
Button_Switch_THT
SW_E-Switch_EG2219_DPDT_Angled
E-Switch slide switch, EG series, DPDT, right angle, http://spec_sheets.e-switch.com/specs/P040170.pdf
switch DPDT
0
10
6
Button_Switch_THT
SW_Lever_1P2T_NKK_GW12LxH
Switch, single pole double throw, right angle, http://www.nkkswitches.com/pdf/GW.pdf
switch single-pole double-throw spdt ON-ON horizontal
0
5
3
Button_Switch_THT
SW_MEC_5GTH9
MEC 5G single pole normally-open tactile switch https://cdn.sos.sk/productdata/80/f6/aabf7be6/5gth9358222.pdf
switch normally-open pushbutton push-button
0
4
2
Button_Switch_THT
SW_NKK_BB15AH
https://www.nkkswitches.com/pdf/Bpushbuttons-1.pdf
Pushbutton Right-angle
0
5
3
Button_Switch_THT
SW_NKK_G1xJP
Switch NKK G1xJP http://www.nkkswitches.com/pdf/gwillum.pdf
SWITCH TOGGLE ILLUM SPDT NKK
0
6
6
Button_Switch_THT
SW_NKK_GW12LJP
Switch, single pole double throw, illuminated paddle, http://www.nkkswitches.com/pdf/gwillum.pdf
switch single-pole double-throw spdt ON-ON illuminated LED
0
6
6
Button_Switch_THT
SW_PUSH-12mm
SW PUSH 12mm https://www.e-switch.com/system/asset/product_line/data_sheet/143/TL1100.pdf
tact sw push 12mm
0
4
2
Button_Switch_THT
SW_PUSH-12mm_Wuerth-430476085716
SW PUSH 12mm http://katalog.we-online.de/em/datasheet/430476085716.pdf
tact sw push 12mm
0
4
2
Button_Switch_THT
SW_PUSH_6mm
https://www.omron.com/ecb/products/pdf/en-b3f.pdf
tact sw push 6mm
0
4
2
Button_Switch_THT
SW_PUSH_6mm_H4.3mm
tactile push button, 6x6mm e.g. PHAP33xx series, height=4.3mm
tact sw push 6mm
0
4
2
Button_Switch_THT
SW_PUSH_6mm_H5mm
tactile push button, 6x6mm e.g. PHAP33xx series, height=5mm
tact sw push 6mm
0
4
2
Button_Switch_THT
SW_PUSH_6mm_H7.3mm
tactile push button, 6x6mm e.g. PHAP33xx series, height=7.3mm
tact sw push 6mm
0
4
2
Button_Switch_THT
SW_PUSH_6mm_H8.5mm
tactile push button, 6x6mm e.g. PHAP33xx series, height=8.5mm
tact sw push 6mm
0
4
2
Button_Switch_THT
SW_PUSH_6mm_H8mm
tactile push button, 6x6mm e.g. PHAP33xx series, height=8mm
tact sw push 6mm
0
4
2
Button_Switch_THT
SW_PUSH_6mm_H9.5mm
tactile push button, 6x6mm e.g. PHAP33xx series, height=9.5mm
tact sw push 6mm
0
4
2
Button_Switch_THT
SW_PUSH_6mm_H13mm
tactile push button, 6x6mm e.g. PHAP33xx series, height=13mm
tact sw push 6mm
0
4
2
Button_Switch_THT
SW_PUSH_E-Switch_FS5700DP_DPDT
FS5700 series pushbutton footswitch, DPDT, https://www.e-switch.com/system/asset/product_line/data_sheet/226/FS5700.pdf
switch DPDT footswitch
0
6
6
Button_Switch_THT
SW_PUSH_LCD_E3_SAxxxx
Switch with LCD screen E3 SAxxxx
switch normally-open pushbutton push-button LCD
0
6
6
Button_Switch_THT
SW_PUSH_LCD_E3_SAxxxx_SocketPins
Switch with LCD screen E3 SAxxxx
switch normally-open pushbutton push-button LCD
0
6
6
Button_Switch_THT
SW_Push_1P1T_NO_LED_E-Switch_TL1250
illuminated right angle tact switch https://www.e-switch.com/system/asset/product_line/data_sheet/148/TL1250.pdf
led push switch right angle
0
6
4
Button_Switch_THT
SW_Push_1P2T_Vertical_E-Switch_800UDP8P1A1M6
 right angle SPDT push button https://www.e-switch.com/system/asset/product_line/data_sheet/210/800U.pdf
IP67 ultra-miniture horizontal
0
5
3
Button_Switch_THT
SW_Push_2P1T_Toggle_CK_PVA1xxH1xxxxxxV2
momentary / push-push button, h=17.5mm C&K PVA1 https://www.ckswitches.com/media/1343/pva.pdf
tact sw push PVA1 DPST
0
4
4
Button_Switch_THT
SW_Push_2P1T_Toggle_CK_PVA1xxH2xxxxxxV2
momentary / push-push button, h=23mm C&K PVA1 https://www.ckswitches.com/media/1343/pva.pdf
tact sw push PVA1 DPST
0
4
4
Button_Switch_THT
SW_Push_2P1T_Toggle_CK_PVA1xxH3xxxxxxV2
momentary / push-push button, h=20.5mm C&K PVA1 https://www.ckswitches.com/media/1343/pva.pdf
tact sw push PVA1 DPST
0
4
4
Button_Switch_THT
SW_Push_2P1T_Toggle_CK_PVA1xxH4xxxxxxV2
momentary / push-push button, h=15mm C&K PVA1 https://www.ckswitches.com/media/1343/pva.pdf
tact sw push PVA1 DPST
0
4
4
Button_Switch_THT
SW_Push_2P2T_Toggle_CK_PVA2OAH5xxxxxxV2
momentary / push-push button, h=13mm C&K PVA2 https://www.ckswitches.com/media/1343/pva.pdf
tact sw push PVA2 DPDT
0
6
6
Button_Switch_THT
SW_Push_2P2T_Toggle_CK_PVA2xxH1xxxxxxV2
momentary / push-push button, h=17.5mm C&K PVA2 https://www.ckswitches.com/media/1343/pva.pdf
tact sw push PVA2 DPDT
0
6
6
Button_Switch_THT
SW_Push_2P2T_Toggle_CK_PVA2xxH2xxxxxxV2
momentary / push-push button, h=23mm C&K PVA2 https://www.ckswitches.com/media/1343/pva.pdf
tact sw push PVA2 DPDT
0
6
6
Button_Switch_THT
SW_Push_2P2T_Toggle_CK_PVA2xxH3xxxxxxV2
momentary / push-push button, h=20.5mm C&K PVA2 https://www.ckswitches.com/media/1343/pva.pdf
tact sw push PVA2 DPDT
0
6
6
Button_Switch_THT
SW_Push_2P2T_Toggle_CK_PVA2xxH4xxxxxxV2
momentary / push-push button, h=15mm C&K PVA2 https://www.ckswitches.com/media/1343/pva.pdf
tact sw push PVA2 DPDT
0
6
6
Button_Switch_THT
SW_Push_2P2T_Vertical_E-Switch_800UDP8P1A1M6
 right angle DPDT push button https://www.e-switch.com/system/asset/product_line/data_sheet/210/800U.pdf
IP67 ultra-miniture horizontal
0
8
6
Button_Switch_THT
SW_Slide_1P2T_CK_OS102011MS2Q
CuK miniature slide switch, OS series, SPDT, https://www.ckswitches.com/media/1428/os.pdf
switch SPDT
0
5
3
Button_Switch_THT
SW_TH_Tactile_Omron_B3F-10xx
SW_TH_Tactile_Omron_B3F-10xx_https://www.omron.com/ecb/products/pdf/en-b3f.pdf
Omron B3F-10xx
0
4
2
Button_Switch_THT
SW_Tactile_SKHH_Angled
tactile switch 6mm ALPS SKHH right angle http://www.alps.com/prod/info/E/HTML/Tact/SnapIn/SKHH/SKHHLUA010.html
tactile switch 6mm ALPS SKHH right angle
0
4
2
Button_Switch_THT
SW_Tactile_SPST_Angled_PTS645Vx31-2LFS
tactile switch SPST right angle, PTS645VL31-2 LFS
tactile switch SPST angled PTS645VL31-2 LFS C&K Button
0
4
2
Button_Switch_THT
SW_Tactile_SPST_Angled_PTS645Vx39-2LFS
tactile switch SPST right angle, PTS645VL39-2 LFS
tactile switch SPST angled PTS645VL39-2 LFS C&K Button
0
4
2
Button_Switch_THT
SW_Tactile_SPST_Angled_PTS645Vx58-2LFS
tactile switch SPST right angle, PTS645VL58-2 LFS
tactile switch SPST angled PTS645VL58-2 LFS C&K Button
0
4
2
Button_Switch_THT
SW_Tactile_SPST_Angled_PTS645Vx83-2LFS
tactile switch SPST right angle, PTS645VL83-2 LFS
tactile switch SPST angled PTS645VL83-2 LFS C&K Button
0
4
2
Button_Switch_THT
SW_Tactile_Straight_KSA0Axx1LFTR
SW PUSH SMALL http://www.ckswitches.com/media/1457/ksa_ksl.pdf
SW PUSH SMALL Tactile C&K
0
4
2
Button_Switch_THT
SW_Tactile_Straight_KSL0Axx1LFTR
SW PUSH SMALL http://www.ckswitches.com/media/1457/ksa_ksl.pdf
SW PUSH SMALL Tactile C&K
0
4
2
Buzzer_Beeper
Buzzer_12x9.5RM7.6
Generic Buzzer, D12mm height 9.5mm with RM7.6mm
buzzer
0
2
2
Buzzer_Beeper
Buzzer_15x7.5RM7.6
Generic Buzzer, D15mm height 7.5mm with RM7.6mm
buzzer
0
2
2
Buzzer_Beeper
Buzzer_CUI_CPT-9019S-SMT
https://www.cui.com/product/resource/cpt-9019s-smt.pdf
buzzer piezo
0
2
2
Buzzer_Beeper
Buzzer_D14mm_H7mm_P10mm
Generic Buzzer, D14mm height 7mm with pitch 10mm
buzzer
0
2
2
Buzzer_Beeper
Buzzer_Mallory_AST1109MLTRQ
Mallory low-profile piezo buzzer, https://www.mspindy.com/specifications/AST1109MLTRQ.pdf
buzzer piezo
0
2
2
Buzzer_Beeper
Buzzer_Mallory_AST1240MLQ
Mallory low-profile piezo buzzer, https://www.mspindy.com/specifications/AST12140MLQ.pdf
piezo buzzer
0
2
2
Buzzer_Beeper
Buzzer_Murata_PKLCS1212E
Murata Buzzer https://www.murata.com/~/media/webrenewal/support/library/catalog/products/sound/p37e.ashx
Murata Buzzer Beeper
0
2
2
Buzzer_Beeper
Buzzer_Murata_PKMCS0909E
Murata Buzzer http://www.murata.com/en-us/api/pdfdownloadapi?cate=&partno=PKMCS0909E4000-R1
Murata Buzzer Beeper
0
2
2
Buzzer_Beeper
Buzzer_TDK_PS1240P02BT_D12.2mm_H6.5mm
Buzzer, D12.2mm height 6.5mm, https://product.tdk.com/info/en/catalog/datasheets/piezoelectronic_buzzer_ps_en.pdf
buzzer
0
2
2
Buzzer_Beeper
Indicator_PUI_AI-1440-TWT-24V-2-R
14mm Indicator, https://www.puiaudio.com/media/SpecSheet/AI-1440-TWT-24V-2-R.pdf
piezo buzzer self drive oscillator
0
2
2
Buzzer_Beeper
MagneticBuzzer_CUI_CMT-8504-100-SMT
magnetic transducer buzzer, 5V, SPL of 100 dB at 10 cm, https://www.cuidevices.com/product/resource/pdf/cmt-8504-100-smt-tr.pdf
CMT 8504
0
4
4
Buzzer_Beeper
MagneticBuzzer_CUI_CST-931RP-A
CST-931RP-A, http://www.cui.com/product/resource/cst-931rp-a.pdf
CST-931RP-A
0
2
2
Buzzer_Beeper
MagneticBuzzer_Kingstate_KCG0601
Buzzer, Elektromagnetic Beeper, Summer,
Kingstate KCG0601 
0
2
2
Buzzer_Beeper
MagneticBuzzer_Kobitone_254-EMB84Q-RO
MagneticBuzzer Kobitone 254-EMB84Q-RO https://www.mouser.es/datasheet/2/209/KT-400385-1171904.pdf
MagneticBuzzer Kobitone 254-EMB84Q-RO
0
3
3
Buzzer_Beeper
MagneticBuzzer_PUI_AT-0927-TT-6-R
Buzzer Magnetic 9mm AT-0927-TT-6-R, http://www.puiaudio.com/pdf/AT-0927-TT-6-R.pdf
Buzzer Magnetic 9mm AT-0927-TT-6-R
0
2
2
Buzzer_Beeper
MagneticBuzzer_ProSignal_ABI-009-RC
Buzzer, Elektromagnetic Beeper, Summer, 6V-DC,
Pro Signal ABI-009-RC 
0
2
2
Buzzer_Beeper
MagneticBuzzer_ProSignal_ABI-010-RC
Buzzer, Elektromagnetic Beeper, Summer, 12V-DC,
Pro Signal ABI-010-RC 
0
2
2
Buzzer_Beeper
MagneticBuzzer_ProSignal_ABT-410-RC
Buzzer, Elektromagnetic Beeper, Summer, 1,5V-DC,
Pro Signal ABT-410-RC 
0
2
2
Buzzer_Beeper
MagneticBuzzer_ProjectsUnlimited_AI-4228-TWT-R
Buzzer, Elektromagnetic Beeper, Summer, 3-28V-DC, https://www.kynix.com/uploadfiles/pdf/AI-4228-TWT-R.pdf
Projects Unlimited AI-4228-TWT-R 
0
2
2
Buzzer_Beeper
MagneticBuzzer_StarMicronics_HMB-06_HMB-12
Buzzer, Elektromagnetic Beeper, Summer,
Star Micronics HMB-06 HMB-12
0
2
2
Buzzer_Beeper
PUIAudio_SMT_0825_S_4_R
SMD 8540, http://www.puiaudio.com/product-detail.aspx?partnumber=SMT-0825-S-4-R
SMD 8540
0
4
4
Buzzer_Beeper
Speaker_CUI_CMR-1206S-67
Speaker, 30mW, 300-7000Hz, IP67 face, 12x6x2,25mm, https://www.cuidevices.com/product/resource/cmr-12062s-67.pdf
speaker CUI
0
2
2
Calibration_Scale
Gauge_10mm_Type1_CopperTop
Gauge, Massstab, 10mm, CopperTop, Type 1,
Gauge Massstab 10mm CopperTop Type 1
0
0
0
Calibration_Scale
Gauge_10mm_Type1_SilkScreenTop
Gauge, Massstab, 10mm, SilkScreenTop, Type 1,
Gauge Massstab 10mm SilkScreenTop Type 1
0
0
0
Calibration_Scale
Gauge_10mm_Type2_CopperTop
Gauge, Massstab, 10mm, CopperTop, Type 2,
Gauge Massstab 10mm CopperTop Type 2
0
0
0
Calibration_Scale
Gauge_10mm_Type2_SilkScreenTop
Gauge, Massstab, 10mm, SilkScreenTop, Type 2,
Gauge Massstab 10mm SilkScreenTop Type 2
0
0
0
Calibration_Scale
Gauge_10mm_Type3_CopperTop
Gauge, Massstab, 10mm, CopperTop, Type 3,
Gauge Massstab 10mm CopperTop Type 3
0
0
0
Calibration_Scale
Gauge_10mm_Type3_SilkScreenTop
Gauge, Massstab, 10mm, SilkScreenTop, Type 3,
Gauge Massstab 10mm SilkScreenTop Type 3
0
0
0
Calibration_Scale
Gauge_10mm_Type4_CopperTop
Gauge, Massstab, 10mm, CopperTop, Type 4,
Gauge Massstab 10mm CopperTop Type 4
0
0
0
Calibration_Scale
Gauge_10mm_Type4_SilkScreenTop
Gauge, Massstab, 10mm, SilkScreenTop, Type 4,
Gauge Massstab 10mm SilkScreenTop Type 4
0
0
0
Calibration_Scale
Gauge_10mm_Type5_CopperTop
Gauge, Massstab, 10mm, CopperTop, Type 5,
Gauge Massstab 10mm CopperTop Type 5
0
0
0
Calibration_Scale
Gauge_10mm_Type5_SilkScreenTop
Gauge, Massstab, 10mm, SilkScreenTop, Type 5,
Gauge Massstab 10mm SilkScreenTop Type 5
0
0
0
Calibration_Scale
Gauge_50mm_Type1_CopperTop
Gauge, Massstab, 50mm, CopperTop, Type 1,
Gauge Massstab 50mm CopperTop Type 1
0
0
0
Calibration_Scale
Gauge_50mm_Type1_SilkScreenTop
Gauge, Massstab, 50mm, SilkScreenTop, Type 1,
Gauge Massstab 50mm SilkScreenTop Type 1
0
0
0
Calibration_Scale
Gauge_50mm_Type2_CopperTop
Gauge, Massstab, 50mm, CopperTop, Type 2,
Gauge Massstab 50mm CopperTop Type 2
0
0
0
Calibration_Scale
Gauge_50mm_Type2_SilkScreenTop
Gauge, Massstab, 50mm, SilkScreenTop, Type 2,
Gauge Massstab 50mm SilkScreenTop Type 2
0
0
0
Calibration_Scale
Gauge_100mm_Grid_Type1_CopperTop
Gauge, Massstab, 100mm, Gitter, Grid, CopperTop, Type 1,
Gauge Massstab 100mm Gitter Grid CopperTop Type 1
0
0
0
Calibration_Scale
Gauge_100mm_Type1_CopperTop
Gauge, Massstab, 100mm, CopperTop, Type 1,
Gauge Massstab 100mm CopperTop Type 1
0
0
0
Calibration_Scale
Gauge_100mm_Type1_SilkScreenTop
Gauge, Massstab, 100mm, SilkScreenTop, Type 1,
Gauge Massstab 100mm SilkScreenTop Type 1
0
0
0
Calibration_Scale
Gauge_100mm_Type2_CopperTop
Gauge, Massstab, 100mm, CopperTop, Type 2,
Gauge Massstab 100mm  CopperTop Type 2
0
0
0
Calibration_Scale
Gauge_100mm_Type2_SilkScreenTop
Gauge, Massstab, 100mm, SilkScreenTop, Type 2,
Gauge Massstab 100mm SilkScreenTop Type 2
0
0
0
Capacitor_THT
CP_Axial_L10.0mm_D4.5mm_P15.00mm_Horizontal
CP, Axial series, Axial, Horizontal, pin pitch=15mm, , length*diameter=10*4.5mm^2, Electrolytic Capacitor, , http://www.vishay.com/docs/28325/021asm.pdf
CP Axial series Axial Horizontal pin pitch 15mm  length 10mm diameter 4.5mm Electrolytic Capacitor
0
2
2
Capacitor_THT
CP_Axial_L10.0mm_D6.0mm_P15.00mm_Horizontal
CP, Axial series, Axial, Horizontal, pin pitch=15mm, , length*diameter=10*6mm^2, Electrolytic Capacitor, , http://www.vishay.com/docs/28325/021asm.pdf
CP Axial series Axial Horizontal pin pitch 15mm  length 10mm diameter 6mm Electrolytic Capacitor
0
2
2
Capacitor_THT
CP_Axial_L11.0mm_D5.0mm_P18.00mm_Horizontal
CP, Axial series, Axial, Horizontal, pin pitch=18mm, , length*diameter=11*5mm^2, Electrolytic Capacitor
CP Axial series Axial Horizontal pin pitch 18mm  length 11mm diameter 5mm Electrolytic Capacitor
0
2
2
Capacitor_THT
CP_Axial_L11.0mm_D6.0mm_P18.00mm_Horizontal
CP, Axial series, Axial, Horizontal, pin pitch=18mm, , length*diameter=11*6mm^2, Electrolytic Capacitor
CP Axial series Axial Horizontal pin pitch 18mm  length 11mm diameter 6mm Electrolytic Capacitor
0
2
2
Capacitor_THT
CP_Axial_L11.0mm_D8.0mm_P15.00mm_Horizontal
CP, Axial series, Axial, Horizontal, pin pitch=15mm, , length*diameter=11*8mm^2, Electrolytic Capacitor, , http://www.vishay.com/docs/28325/021asm.pdf
CP Axial series Axial Horizontal pin pitch 15mm  length 11mm diameter 8mm Electrolytic Capacitor
0
2
2
Capacitor_THT
CP_Axial_L18.0mm_D6.5mm_P25.00mm_Horizontal
CP, Axial series, Axial, Horizontal, pin pitch=25mm, , length*diameter=18*6.5mm^2, Electrolytic Capacitor, , http://www.vishay.com/docs/28325/021asm.pdf
CP Axial series Axial Horizontal pin pitch 25mm  length 18mm diameter 6.5mm Electrolytic Capacitor
0
2
2
Capacitor_THT
CP_Axial_L18.0mm_D8.0mm_P25.00mm_Horizontal
CP, Axial series, Axial, Horizontal, pin pitch=25mm, , length*diameter=18*8mm^2, Electrolytic Capacitor, , http://www.vishay.com/docs/28325/021asm.pdf
CP Axial series Axial Horizontal pin pitch 25mm  length 18mm diameter 8mm Electrolytic Capacitor
0
2
2
Capacitor_THT
CP_Axial_L18.0mm_D10.0mm_P25.00mm_Horizontal
CP, Axial series, Axial, Horizontal, pin pitch=25mm, , length*diameter=18*10mm^2, Electrolytic Capacitor, , http://www.vishay.com/docs/28325/021asm.pdf
CP Axial series Axial Horizontal pin pitch 25mm  length 18mm diameter 10mm Electrolytic Capacitor
0
2
2
Capacitor_THT
CP_Axial_L20.0mm_D10.0mm_P26.00mm_Horizontal
CP, Axial series, Axial, Horizontal, pin pitch=26mm, , length*diameter=20*10mm^2, Electrolytic Capacitor, , http://www.kemet.com/Lists/ProductCatalog/Attachments/424/KEM_AC102.pdf
CP Axial series Axial Horizontal pin pitch 26mm  length 20mm diameter 10mm Electrolytic Capacitor
0
2
2
Capacitor_THT
CP_Axial_L20.0mm_D13.0mm_P26.00mm_Horizontal
CP, Axial series, Axial, Horizontal, pin pitch=26mm, , length*diameter=20*13mm^2, Electrolytic Capacitor, , http://www.kemet.com/Lists/ProductCatalog/Attachments/424/KEM_AC102.pdf
CP Axial series Axial Horizontal pin pitch 26mm  length 20mm diameter 13mm Electrolytic Capacitor
0
2
2
Capacitor_THT
CP_Axial_L21.0mm_D8.0mm_P28.00mm_Horizontal
CP, Axial series, Axial, Horizontal, pin pitch=28mm, , length*diameter=21*8mm^2, Electrolytic Capacitor
CP Axial series Axial Horizontal pin pitch 28mm  length 21mm diameter 8mm Electrolytic Capacitor
0
2
2
Capacitor_THT
CP_Axial_L25.0mm_D10.0mm_P30.00mm_Horizontal
CP, Axial series, Axial, Horizontal, pin pitch=30mm, , length*diameter=25*10mm^2, Electrolytic Capacitor, , http://www.vishay.com/docs/28325/021asm.pdf
CP Axial series Axial Horizontal pin pitch 30mm  length 25mm diameter 10mm Electrolytic Capacitor
0
2
2
Capacitor_THT
CP_Axial_L26.5mm_D20.0mm_P33.00mm_Horizontal
CP, Axial series, Axial, Horizontal, pin pitch=33mm, , length*diameter=26.5*20mm^2, Electrolytic Capacitor, , http://www.kemet.com/Lists/ProductCatalog/Attachments/424/KEM_AC102.pdf
CP Axial series Axial Horizontal pin pitch 33mm  length 26.5mm diameter 20mm Electrolytic Capacitor
0
2
2
Capacitor_THT
CP_Axial_L29.0mm_D10.0mm_P35.00mm_Horizontal
CP, Axial series, Axial, Horizontal, pin pitch=35mm, , length*diameter=29*10mm^2, Electrolytic Capacitor, , http://www.kemet.com/Lists/ProductCatalog/Attachments/424/KEM_AC102.pdf
CP Axial series Axial Horizontal pin pitch 35mm  length 29mm diameter 10mm Electrolytic Capacitor
0
2
2
Capacitor_THT
CP_Axial_L29.0mm_D13.0mm_P35.00mm_Horizontal
CP, Axial series, Axial, Horizontal, pin pitch=35mm, , length*diameter=29*13mm^2, Electrolytic Capacitor, , http://www.kemet.com/Lists/ProductCatalog/Attachments/424/KEM_AC102.pdf
CP Axial series Axial Horizontal pin pitch 35mm  length 29mm diameter 13mm Electrolytic Capacitor
0
2
2
Capacitor_THT
CP_Axial_L29.0mm_D16.0mm_P35.00mm_Horizontal
CP, Axial series, Axial, Horizontal, pin pitch=35mm, , length*diameter=29*16mm^2, Electrolytic Capacitor, , http://www.kemet.com/Lists/ProductCatalog/Attachments/424/KEM_AC102.pdf
CP Axial series Axial Horizontal pin pitch 35mm  length 29mm diameter 16mm Electrolytic Capacitor
0
2
2
Capacitor_THT
CP_Axial_L29.0mm_D20.0mm_P35.00mm_Horizontal
CP, Axial series, Axial, Horizontal, pin pitch=35mm, , length*diameter=29*20mm^2, Electrolytic Capacitor, , http://www.kemet.com/Lists/ProductCatalog/Attachments/424/KEM_AC102.pdf
CP Axial series Axial Horizontal pin pitch 35mm  length 29mm diameter 20mm Electrolytic Capacitor
0
2
2
Capacitor_THT
CP_Axial_L30.0mm_D10.0mm_P35.00mm_Horizontal
CP, Axial series, Axial, Horizontal, pin pitch=35mm, , length*diameter=30*10mm^2, Electrolytic Capacitor, , http://www.vishay.com/docs/28325/021asm.pdf
CP Axial series Axial Horizontal pin pitch 35mm  length 30mm diameter 10mm Electrolytic Capacitor
0
2
2
Capacitor_THT
CP_Axial_L30.0mm_D12.5mm_P35.00mm_Horizontal
CP, Axial series, Axial, Horizontal, pin pitch=35mm, , length*diameter=30*12.5mm^2, Electrolytic Capacitor, , http://www.vishay.com/docs/28325/021asm.pdf
CP Axial series Axial Horizontal pin pitch 35mm  length 30mm diameter 12.5mm Electrolytic Capacitor
0
2
2
Capacitor_THT
CP_Axial_L30.0mm_D15.0mm_P35.00mm_Horizontal
CP, Axial series, Axial, Horizontal, pin pitch=35mm, , length*diameter=30*15mm^2, Electrolytic Capacitor, , http://www.vishay.com/docs/28325/021asm.pdf
CP Axial series Axial Horizontal pin pitch 35mm  length 30mm diameter 15mm Electrolytic Capacitor
0
2
2
Capacitor_THT
CP_Axial_L30.0mm_D18.0mm_P35.00mm_Horizontal
CP, Axial series, Axial, Horizontal, pin pitch=35mm, , length*diameter=30*18mm^2, Electrolytic Capacitor, , http://www.vishay.com/docs/28325/021asm.pdf
CP Axial series Axial Horizontal pin pitch 35mm  length 30mm diameter 18mm Electrolytic Capacitor
0
2
2
Capacitor_THT
CP_Axial_L34.5mm_D20.0mm_P41.00mm_Horizontal
CP, Axial series, Axial, Horizontal, pin pitch=41mm, , length*diameter=34.5*20mm^2, Electrolytic Capacitor, , http://www.kemet.com/Lists/ProductCatalog/Attachments/424/KEM_AC102.pdf
CP Axial series Axial Horizontal pin pitch 41mm  length 34.5mm diameter 20mm Electrolytic Capacitor
0
2
2
Capacitor_THT
CP_Axial_L37.0mm_D13.0mm_P43.00mm_Horizontal
CP, Axial series, Axial, Horizontal, pin pitch=43mm, , length*diameter=37*13mm^2, Electrolytic Capacitor, , http://www.kemet.com/Lists/ProductCatalog/Attachments/424/KEM_AC102.pdf
CP Axial series Axial Horizontal pin pitch 43mm  length 37mm diameter 13mm Electrolytic Capacitor
0
2
2
Capacitor_THT
CP_Axial_L37.0mm_D16.0mm_P43.00mm_Horizontal
CP, Axial series, Axial, Horizontal, pin pitch=43mm, , length*diameter=37*16mm^2, Electrolytic Capacitor, , http://www.kemet.com/Lists/ProductCatalog/Attachments/424/KEM_AC102.pdf
CP Axial series Axial Horizontal pin pitch 43mm  length 37mm diameter 16mm Electrolytic Capacitor
0
2
2
Capacitor_THT
CP_Axial_L37.0mm_D20.0mm_P43.00mm_Horizontal
CP, Axial series, Axial, Horizontal, pin pitch=43mm, , length*diameter=37*20mm^2, Electrolytic Capacitor, , http://www.kemet.com/Lists/ProductCatalog/Attachments/424/KEM_AC102.pdf
CP Axial series Axial Horizontal pin pitch 43mm  length 37mm diameter 20mm Electrolytic Capacitor
0
2
2
Capacitor_THT
CP_Axial_L38.0mm_D18.0mm_P44.00mm_Horizontal
CP, Axial series, Axial, Horizontal, pin pitch=44mm, , length*diameter=38*18mm^2, Electrolytic Capacitor, , http://www.vishay.com/docs/28325/021asm.pdf
CP Axial series Axial Horizontal pin pitch 44mm  length 38mm diameter 18mm Electrolytic Capacitor
0
2
2
Capacitor_THT
CP_Axial_L38.0mm_D21.0mm_P44.00mm_Horizontal
CP, Axial series, Axial, Horizontal, pin pitch=44mm, , length*diameter=38*21mm^2, Electrolytic Capacitor, , http://www.vishay.com/docs/28325/021asm.pdf
CP Axial series Axial Horizontal pin pitch 44mm  length 38mm diameter 21mm Electrolytic Capacitor
0
2
2
Capacitor_THT
CP_Axial_L40.0mm_D16.0mm_P48.00mm_Horizontal
CP, Axial series, Axial, Horizontal, pin pitch=48mm, , length*diameter=40*16mm^2, Electrolytic Capacitor
CP Axial series Axial Horizontal pin pitch 48mm  length 40mm diameter 16mm Electrolytic Capacitor
0
2
2
Capacitor_THT
CP_Axial_L42.0mm_D23.0mm_P45.00mm_Horizontal
CP, Axial series, Axial, Horizontal, pin pitch=45mm, , length*diameter=42*23.0mm^2, Electrolytic Capacitor, , http://www.vishay.com/docs/42037/53d.pdf
CP Axial series Axial Horizontal pin pitch 45mm  length 42mm diameter 23.0mm Electrolytic Capacitor
0
2
2
Capacitor_THT
CP_Axial_L42.0mm_D26.0mm_P45.00mm_Horizontal
CP, Axial series, Axial, Horizontal, pin pitch=45mm, , length*diameter=42*26mm^2, Electrolytic Capacitor, , http://www.vishay.com/docs/42037/53d.pdf
CP Axial series Axial Horizontal pin pitch 45mm  length 42mm diameter 26mm Electrolytic Capacitor
0
2
2
Capacitor_THT
CP_Axial_L42.0mm_D29.0mm_P45.00mm_Horizontal
CP, Axial series, Axial, Horizontal, pin pitch=45mm, , length*diameter=42*29.0mm^2, Electrolytic Capacitor, , http://www.vishay.com/docs/42037/53d.pdf
CP Axial series Axial Horizontal pin pitch 45mm  length 42mm diameter 29.0mm Electrolytic Capacitor
0
2
2
Capacitor_THT
CP_Axial_L42.0mm_D32.0mm_P45.00mm_Horizontal
CP, Axial series, Axial, Horizontal, pin pitch=45mm, , length*diameter=42*32.0mm^2, Electrolytic Capacitor, , http://www.vishay.com/docs/42037/53d.pdf
CP Axial series Axial Horizontal pin pitch 45mm  length 42mm diameter 32.0mm Electrolytic Capacitor
0
2
2
Capacitor_THT
CP_Axial_L42.0mm_D35.0mm_P45.00mm_Horizontal
CP, Axial series, Axial, Horizontal, pin pitch=45mm, , length*diameter=42*35.0mm^2, Electrolytic Capacitor, , http://www.vishay.com/docs/42037/53d.pdf
CP Axial series Axial Horizontal pin pitch 45mm  length 42mm diameter 35.0mm Electrolytic Capacitor
0
2
2
Capacitor_THT
CP_Axial_L42.5mm_D20.0mm_P49.00mm_Horizontal
CP, Axial series, Axial, Horizontal, pin pitch=49mm, , length*diameter=42.5*20mm^2, Electrolytic Capacitor
CP Axial series Axial Horizontal pin pitch 49mm  length 42.5mm diameter 20mm Electrolytic Capacitor
0
2
2
Capacitor_THT
CP_Axial_L46.0mm_D20.0mm_P52.00mm_Horizontal
CP, Axial series, Axial, Horizontal, pin pitch=52mm, , length*diameter=46*20mm^2, Electrolytic Capacitor
CP Axial series Axial Horizontal pin pitch 52mm  length 46mm diameter 20mm Electrolytic Capacitor
0
2
2
Capacitor_THT
CP_Axial_L55.0mm_D23.0mm_P60.00mm_Horizontal
CP, Axial series, Axial, Horizontal, pin pitch=60mm, , length*diameter=55*23.0mm^2, Electrolytic Capacitor, , http://www.vishay.com/docs/42037/53d.pdf
CP Axial series Axial Horizontal pin pitch 60mm  length 55mm diameter 23.0mm Electrolytic Capacitor
0
2
2
Capacitor_THT
CP_Axial_L55.0mm_D26.0mm_P60.00mm_Horizontal
CP, Axial series, Axial, Horizontal, pin pitch=60mm, , length*diameter=55*26mm^2, Electrolytic Capacitor, , http://www.vishay.com/docs/42037/53d.pdf
CP Axial series Axial Horizontal pin pitch 60mm  length 55mm diameter 26mm Electrolytic Capacitor
0
2
2
Capacitor_THT
CP_Axial_L55.0mm_D29.0mm_P60.00mm_Horizontal
CP, Axial series, Axial, Horizontal, pin pitch=60mm, , length*diameter=55*29.0mm^2, Electrolytic Capacitor, , http://www.vishay.com/docs/42037/53d.pdf
CP Axial series Axial Horizontal pin pitch 60mm  length 55mm diameter 29.0mm Electrolytic Capacitor
0
2
2
Capacitor_THT
CP_Axial_L55.0mm_D32.0mm_P60.00mm_Horizontal
CP, Axial series, Axial, Horizontal, pin pitch=60mm, , length*diameter=55*32.0mm^2, Electrolytic Capacitor, , http://www.vishay.com/docs/42037/53d.pdf
CP Axial series Axial Horizontal pin pitch 60mm  length 55mm diameter 32.0mm Electrolytic Capacitor
0
2
2
Capacitor_THT
CP_Axial_L55.0mm_D35.0mm_P60.00mm_Horizontal
CP, Axial series, Axial, Horizontal, pin pitch=60mm, , length*diameter=55*35.0mm^2, Electrolytic Capacitor, , http://www.vishay.com/docs/42037/53d.pdf
CP Axial series Axial Horizontal pin pitch 60mm  length 55mm diameter 35.0mm Electrolytic Capacitor
0
2
2
Capacitor_THT
CP_Axial_L67.0mm_D23.0mm_P75.00mm_Horizontal
CP, Axial series, Axial, Horizontal, pin pitch=75mm, , length*diameter=67*23.0mm^2, Electrolytic Capacitor, , http://www.vishay.com/docs/42037/53d.pdf
CP Axial series Axial Horizontal pin pitch 75mm  length 67mm diameter 23.0mm Electrolytic Capacitor
0
2
2
Capacitor_THT
CP_Axial_L67.0mm_D26.0mm_P75.00mm_Horizontal
CP, Axial series, Axial, Horizontal, pin pitch=75mm, , length*diameter=67*26mm^2, Electrolytic Capacitor, , http://www.vishay.com/docs/42037/53d.pdf
CP Axial series Axial Horizontal pin pitch 75mm  length 67mm diameter 26mm Electrolytic Capacitor
0
2
2
Capacitor_THT
CP_Axial_L67.0mm_D29.0mm_P75.00mm_Horizontal
CP, Axial series, Axial, Horizontal, pin pitch=75mm, , length*diameter=67*29.0mm^2, Electrolytic Capacitor, , http://www.vishay.com/docs/42037/53d.pdf
CP Axial series Axial Horizontal pin pitch 75mm  length 67mm diameter 29.0mm Electrolytic Capacitor
0
2
2
Capacitor_THT
CP_Axial_L67.0mm_D32.0mm_P75.00mm_Horizontal
CP, Axial series, Axial, Horizontal, pin pitch=75mm, , length*diameter=67*32.0mm^2, Electrolytic Capacitor, , http://www.vishay.com/docs/42037/53d.pdf
CP Axial series Axial Horizontal pin pitch 75mm  length 67mm diameter 32.0mm Electrolytic Capacitor
0
2
2
Capacitor_THT
CP_Axial_L67.0mm_D35.0mm_P75.00mm_Horizontal
CP, Axial series, Axial, Horizontal, pin pitch=75mm, , length*diameter=67*35.0mm^2, Electrolytic Capacitor, , http://www.vishay.com/docs/42037/53d.pdf
CP Axial series Axial Horizontal pin pitch 75mm  length 67mm diameter 35.0mm Electrolytic Capacitor
0
2
2
Capacitor_THT
CP_Axial_L80.0mm_D23.0mm_P85.00mm_Horizontal
CP, Axial series, Axial, Horizontal, pin pitch=85mm, , length*diameter=80*23.0mm^2, Electrolytic Capacitor, , http://www.vishay.com/docs/42037/53d.pdf
CP Axial series Axial Horizontal pin pitch 85mm  length 80mm diameter 23.0mm Electrolytic Capacitor
0
2
2
Capacitor_THT
CP_Axial_L80.0mm_D26.0mm_P85.00mm_Horizontal
CP, Axial series, Axial, Horizontal, pin pitch=85mm, , length*diameter=80*26mm^2, Electrolytic Capacitor, , http://www.vishay.com/docs/42037/53d.pdf
CP Axial series Axial Horizontal pin pitch 85mm  length 80mm diameter 26mm Electrolytic Capacitor
0
2
2
Capacitor_THT
CP_Axial_L80.0mm_D29.0mm_P85.00mm_Horizontal
CP, Axial series, Axial, Horizontal, pin pitch=85mm, , length*diameter=80*29.0mm^2, Electrolytic Capacitor, , http://www.vishay.com/docs/42037/53d.pdf
CP Axial series Axial Horizontal pin pitch 85mm  length 80mm diameter 29.0mm Electrolytic Capacitor
0
2
2
Capacitor_THT
CP_Axial_L80.0mm_D32.0mm_P85.00mm_Horizontal
CP, Axial series, Axial, Horizontal, pin pitch=85mm, , length*diameter=80*32.0mm^2, Electrolytic Capacitor, , http://www.vishay.com/docs/42037/53d.pdf
CP Axial series Axial Horizontal pin pitch 85mm  length 80mm diameter 32.0mm Electrolytic Capacitor
0
2
2
Capacitor_THT
CP_Axial_L80.0mm_D35.0mm_P85.00mm_Horizontal
CP, Axial series, Axial, Horizontal, pin pitch=85mm, , length*diameter=80*35.0mm^2, Electrolytic Capacitor, , http://www.vishay.com/docs/42037/53d.pdf
CP Axial series Axial Horizontal pin pitch 85mm  length 80mm diameter 35.0mm Electrolytic Capacitor
0
2
2
Capacitor_THT
CP_Axial_L93.0mm_D23.0mm_P100.00mm_Horizontal
CP, Axial series, Axial, Horizontal, pin pitch=100mm, , length*diameter=93*23.0mm^2, Electrolytic Capacitor, , http://www.vishay.com/docs/42037/53d.pdf
CP Axial series Axial Horizontal pin pitch 100mm  length 93mm diameter 23.0mm Electrolytic Capacitor
0
2
2
Capacitor_THT
CP_Axial_L93.0mm_D26.0mm_P100.00mm_Horizontal
CP, Axial series, Axial, Horizontal, pin pitch=100mm, , length*diameter=93*26mm^2, Electrolytic Capacitor, , http://www.vishay.com/docs/42037/53d.pdf
CP Axial series Axial Horizontal pin pitch 100mm  length 93mm diameter 26mm Electrolytic Capacitor
0
2
2
Capacitor_THT
CP_Axial_L93.0mm_D29.0mm_P100.00mm_Horizontal
CP, Axial series, Axial, Horizontal, pin pitch=100mm, , length*diameter=93*29.0mm^2, Electrolytic Capacitor, , http://www.vishay.com/docs/42037/53d.pdf
CP Axial series Axial Horizontal pin pitch 100mm  length 93mm diameter 29.0mm Electrolytic Capacitor
0
2
2
Capacitor_THT
CP_Axial_L93.0mm_D32.0mm_P100.00mm_Horizontal
CP, Axial series, Axial, Horizontal, pin pitch=100mm, , length*diameter=93*32.0mm^2, Electrolytic Capacitor, , http://www.vishay.com/docs/42037/53d.pdf
CP Axial series Axial Horizontal pin pitch 100mm  length 93mm diameter 32.0mm Electrolytic Capacitor
0
2
2
Capacitor_THT
CP_Axial_L93.0mm_D35.0mm_P100.00mm_Horizontal
CP, Axial series, Axial, Horizontal, pin pitch=100mm, , length*diameter=93*35.0mm^2, Electrolytic Capacitor, , http://www.vishay.com/docs/42037/53d.pdf
CP Axial series Axial Horizontal pin pitch 100mm  length 93mm diameter 35.0mm Electrolytic Capacitor
0
2
2
Capacitor_THT
CP_Radial_D4.0mm_P1.50mm
CP, Radial series, Radial, pin pitch=1.50mm, , diameter=4mm, Electrolytic Capacitor
CP Radial series Radial pin pitch 1.50mm  diameter 4mm Electrolytic Capacitor
0
2
2
Capacitor_THT
CP_Radial_D4.0mm_P2.00mm
CP, Radial series, Radial, pin pitch=2.00mm, , diameter=4mm, Electrolytic Capacitor
CP Radial series Radial pin pitch 2.00mm  diameter 4mm Electrolytic Capacitor
0
2
2
Capacitor_THT
CP_Radial_D5.0mm_P2.00mm
CP, Radial series, Radial, pin pitch=2.00mm, , diameter=5mm, Electrolytic Capacitor
CP Radial series Radial pin pitch 2.00mm  diameter 5mm Electrolytic Capacitor
0
2
2
Capacitor_THT
CP_Radial_D5.0mm_P2.50mm
CP, Radial series, Radial, pin pitch=2.50mm, , diameter=5mm, Electrolytic Capacitor
CP Radial series Radial pin pitch 2.50mm  diameter 5mm Electrolytic Capacitor
0
2
2
Capacitor_THT
CP_Radial_D6.3mm_P2.50mm
CP, Radial series, Radial, pin pitch=2.50mm, , diameter=6.3mm, Electrolytic Capacitor
CP Radial series Radial pin pitch 2.50mm  diameter 6.3mm Electrolytic Capacitor
0
2
2
Capacitor_THT
CP_Radial_D7.5mm_P2.50mm
CP, Radial series, Radial, pin pitch=2.50mm, , diameter=7.5mm, Electrolytic Capacitor
CP Radial series Radial pin pitch 2.50mm  diameter 7.5mm Electrolytic Capacitor
0
2
2
Capacitor_THT
CP_Radial_D8.0mm_P2.50mm
CP, Radial series, Radial, pin pitch=2.50mm, , diameter=8mm, Electrolytic Capacitor
CP Radial series Radial pin pitch 2.50mm  diameter 8mm Electrolytic Capacitor
0
2
2
Capacitor_THT
CP_Radial_D8.0mm_P3.50mm
CP, Radial series, Radial, pin pitch=3.50mm, , diameter=8mm, Electrolytic Capacitor
CP Radial series Radial pin pitch 3.50mm  diameter 8mm Electrolytic Capacitor
0
2
2
Capacitor_THT
CP_Radial_D8.0mm_P3.80mm
CP, Radial series, Radial, pin pitch=3.80mm, , diameter=8mm, Electrolytic Capacitor
CP Radial series Radial pin pitch 3.80mm  diameter 8mm Electrolytic Capacitor
0
2
2
Capacitor_THT
CP_Radial_D8.0mm_P5.00mm
CP, Radial series, Radial, pin pitch=5.00mm, , diameter=8mm, Electrolytic Capacitor
CP Radial series Radial pin pitch 5.00mm  diameter 8mm Electrolytic Capacitor
0
2
2
Capacitor_THT
CP_Radial_D10.0mm_P2.50mm
CP, Radial series, Radial, pin pitch=2.50mm, , diameter=10mm, Electrolytic Capacitor
CP Radial series Radial pin pitch 2.50mm  diameter 10mm Electrolytic Capacitor
0
2
2
Capacitor_THT
CP_Radial_D10.0mm_P2.50mm_P5.00mm
CP, Radial series, Radial, pin pitch=2.50mm 5.00mm, , diameter=10mm, Electrolytic Capacitor
CP Radial series Radial pin pitch 2.50mm 5.00mm  diameter 10mm Electrolytic Capacitor
0
4
2
Capacitor_THT
CP_Radial_D10.0mm_P3.50mm
CP, Radial series, Radial, pin pitch=3.50mm, , diameter=10mm, Electrolytic Capacitor
CP Radial series Radial pin pitch 3.50mm  diameter 10mm Electrolytic Capacitor
0
2
2
Capacitor_THT
CP_Radial_D10.0mm_P3.80mm
CP, Radial series, Radial, pin pitch=3.80mm, , diameter=10mm, Electrolytic Capacitor
CP Radial series Radial pin pitch 3.80mm  diameter 10mm Electrolytic Capacitor
0
2
2
Capacitor_THT
CP_Radial_D10.0mm_P5.00mm
CP, Radial series, Radial, pin pitch=5.00mm, , diameter=10mm, Electrolytic Capacitor
CP Radial series Radial pin pitch 5.00mm  diameter 10mm Electrolytic Capacitor
0
2
2
Capacitor_THT
CP_Radial_D10.0mm_P5.00mm_P7.50mm
CP, Radial series, Radial, pin pitch=5.00mm 7.50mm, , diameter=10mm, Electrolytic Capacitor
CP Radial series Radial pin pitch 5.00mm 7.50mm  diameter 10mm Electrolytic Capacitor
0
4
2
Capacitor_THT
CP_Radial_D10.0mm_P7.50mm
CP, Radial series, Radial, pin pitch=7.50mm, , diameter=10mm, Electrolytic Capacitor
CP Radial series Radial pin pitch 7.50mm  diameter 10mm Electrolytic Capacitor
0
2
2
Capacitor_THT
CP_Radial_D12.5mm_P2.50mm
CP, Radial series, Radial, pin pitch=2.50mm, , diameter=12.5mm, Electrolytic Capacitor
CP Radial series Radial pin pitch 2.50mm  diameter 12.5mm Electrolytic Capacitor
0
2
2
Capacitor_THT
CP_Radial_D12.5mm_P5.00mm
CP, Radial series, Radial, pin pitch=5.00mm, , diameter=12.5mm, Electrolytic Capacitor
CP Radial series Radial pin pitch 5.00mm  diameter 12.5mm Electrolytic Capacitor
0
2
2
Capacitor_THT
CP_Radial_D12.5mm_P7.50mm
CP, Radial series, Radial, pin pitch=7.50mm, , diameter=12.5mm, Electrolytic Capacitor
CP Radial series Radial pin pitch 7.50mm  diameter 12.5mm Electrolytic Capacitor
0
2
2
Capacitor_THT
CP_Radial_D13.0mm_P2.50mm
CP, Radial series, Radial, pin pitch=2.50mm, , diameter=13mm, Electrolytic Capacitor
CP Radial series Radial pin pitch 2.50mm  diameter 13mm Electrolytic Capacitor
0
2
2
Capacitor_THT
CP_Radial_D13.0mm_P5.00mm
CP, Radial series, Radial, pin pitch=5.00mm, , diameter=13mm, Electrolytic Capacitor
CP Radial series Radial pin pitch 5.00mm  diameter 13mm Electrolytic Capacitor
0
2
2
Capacitor_THT
CP_Radial_D13.0mm_P7.50mm
CP, Radial series, Radial, pin pitch=7.50mm, , diameter=13mm, Electrolytic Capacitor
CP Radial series Radial pin pitch 7.50mm  diameter 13mm Electrolytic Capacitor
0
2
2
Capacitor_THT
CP_Radial_D14.0mm_P5.00mm
CP, Radial series, Radial, pin pitch=5.00mm, , diameter=14mm, Electrolytic Capacitor
CP Radial series Radial pin pitch 5.00mm  diameter 14mm Electrolytic Capacitor
0
2
2
Capacitor_THT
CP_Radial_D14.0mm_P7.50mm
CP, Radial series, Radial, pin pitch=7.50mm, , diameter=14mm, Electrolytic Capacitor
CP Radial series Radial pin pitch 7.50mm  diameter 14mm Electrolytic Capacitor
0
2
2
Capacitor_THT
CP_Radial_D16.0mm_P7.50mm
CP, Radial series, Radial, pin pitch=7.50mm, , diameter=16mm, Electrolytic Capacitor
CP Radial series Radial pin pitch 7.50mm  diameter 16mm Electrolytic Capacitor
0
2
2
Capacitor_THT
CP_Radial_D17.0mm_P7.50mm
CP, Radial series, Radial, pin pitch=7.50mm, , diameter=17mm, Electrolytic Capacitor
CP Radial series Radial pin pitch 7.50mm  diameter 17mm Electrolytic Capacitor
0
2
2
Capacitor_THT
CP_Radial_D18.0mm_P7.50mm
CP, Radial series, Radial, pin pitch=7.50mm, , diameter=18mm, Electrolytic Capacitor
CP Radial series Radial pin pitch 7.50mm  diameter 18mm Electrolytic Capacitor
0
2
2
Capacitor_THT
CP_Radial_D22.0mm_P10.00mm_3pin_SnapIn
CP, Radial series, Radial, pin pitch=10.00mm, diameter=22mm, height=40mm, Electrolytic Capacitor, , http://www.vishay.com/docs/28342/058059pll-si.pdf
CP Radial series Radial pin pitch 10.00mm diameter 22mm height 40mm Electrolytic Capacitor
0
3
2
Capacitor_THT
CP_Radial_D22.0mm_P10.00mm_SnapIn
CP, Radial series, Radial, pin pitch=10.00mm, , diameter=22mm, Electrolytic Capacitor, , http://www.vishay.com/docs/28342/058059pll-si.pdf
CP Radial series Radial pin pitch 10.00mm  diameter 22mm Electrolytic Capacitor
0
2
2
Capacitor_THT
CP_Radial_D24.0mm_P10.00mm_3pin_SnapIn
CP, Radial series, Radial, pin pitch=10.00mm, diameter=24mm, height=40mm, Electrolytic Capacitor, , http://www.vishay.com/docs/28342/058059pll-si.pdf
CP Radial series Radial pin pitch 10.00mm diameter 24mm height 40mm Electrolytic Capacitor
0
3
2
Capacitor_THT
CP_Radial_D24.0mm_P10.00mm_SnapIn
CP, Radial series, Radial, pin pitch=10.00mm, , diameter=24mm, Electrolytic Capacitor, , http://www.vishay.com/docs/28342/058059pll-si.pdf
CP Radial series Radial pin pitch 10.00mm  diameter 24mm Electrolytic Capacitor
0
2
2
Capacitor_THT
CP_Radial_D25.0mm_P10.00mm_3pin_SnapIn
CP, Radial series, Radial, pin pitch=10.00mm, diameter=25mm, height=45mm, Electrolytic Capacitor, , http://www.vishay.com/docs/28342/058059pll-si.pdf
CP Radial series Radial pin pitch 10.00mm diameter 25mm height 45mm Electrolytic Capacitor
0
3
2
Capacitor_THT
CP_Radial_D25.0mm_P10.00mm_SnapIn
CP, Radial series, Radial, pin pitch=10.00mm, , diameter=25mm, Electrolytic Capacitor, , http://www.vishay.com/docs/28342/058059pll-si.pdf
CP Radial series Radial pin pitch 10.00mm  diameter 25mm Electrolytic Capacitor
0
2
2
Capacitor_THT
CP_Radial_D26.0mm_P10.00mm_3pin_SnapIn
CP, Radial series, Radial, pin pitch=10.00mm, diameter=26mm, height=45mm, Electrolytic Capacitor, , http://www.vishay.com/docs/28342/058059pll-si.pdf
CP Radial series Radial pin pitch 10.00mm diameter 26mm height 45mm Electrolytic Capacitor
0
3
2
Capacitor_THT
CP_Radial_D26.0mm_P10.00mm_SnapIn
CP, Radial series, Radial, pin pitch=10.00mm, , diameter=26mm, Electrolytic Capacitor, , http://www.vishay.com/docs/28342/058059pll-si.pdf
CP Radial series Radial pin pitch 10.00mm  diameter 26mm Electrolytic Capacitor
0
2
2
Capacitor_THT
CP_Radial_D30.0mm_P10.00mm_3pin_SnapIn
CP, Radial series, Radial, pin pitch=10.00mm, diameter=30mm, height=45mm, Electrolytic Capacitor, , http://www.vishay.com/docs/28342/058059pll-si.pdf
CP Radial series Radial pin pitch 10.00mm diameter 30mm height 45mm Electrolytic Capacitor
0
3
2
Capacitor_THT
CP_Radial_D30.0mm_P10.00mm_SnapIn
CP, Radial series, Radial, pin pitch=10.00mm, , diameter=30mm, Electrolytic Capacitor, , http://www.vishay.com/docs/28342/058059pll-si.pdf
CP Radial series Radial pin pitch 10.00mm  diameter 30mm Electrolytic Capacitor
0
2
2
Capacitor_THT
CP_Radial_D35.0mm_P10.00mm_3pin_SnapIn
CP, Radial series, Radial, pin pitch=10.00mm, diameter=35mm, height=50mm, Electrolytic Capacitor, , http://www.vishay.com/docs/28342/058059pll-si.pdf
CP Radial series Radial pin pitch 10.00mm diameter 35mm height 50mm Electrolytic Capacitor
0
3
2
Capacitor_THT
CP_Radial_D35.0mm_P10.00mm_SnapIn
CP, Radial series, Radial, pin pitch=10.00mm, , diameter=35mm, Electrolytic Capacitor, , http://www.vishay.com/docs/28342/058059pll-si.pdf
CP Radial series Radial pin pitch 10.00mm  diameter 35mm Electrolytic Capacitor
0
2
2
Capacitor_THT
CP_Radial_D40.0mm_P10.00mm_3pin_SnapIn
CP, Radial series, Radial, pin pitch=10.00mm, diameter=40mm, height=50mm, Electrolytic Capacitor, , http://www.vishay.com/docs/28342/058059pll-si.pdf
CP Radial series Radial pin pitch 10.00mm diameter 40mm height 50mm Electrolytic Capacitor
0
3
2
Capacitor_THT
CP_Radial_D40.0mm_P10.00mm_SnapIn
CP, Radial series, Radial, pin pitch=10.00mm, , diameter=40mm, Electrolytic Capacitor, , http://www.vishay.com/docs/28342/058059pll-si.pdf
CP Radial series Radial pin pitch 10.00mm  diameter 40mm Electrolytic Capacitor
0
2
2
Capacitor_THT
CP_Radial_Tantal_D4.5mm_P2.50mm
CP, Radial_Tantal series, Radial, pin pitch=2.50mm, , diameter=4.5mm, Tantal Electrolytic Capacitor, http://cdn-reichelt.de/documents/datenblatt/B300/TANTAL-TB-Serie%23.pdf
CP Radial_Tantal series Radial pin pitch 2.50mm  diameter 4.5mm Tantal Electrolytic Capacitor
0
2
2
Capacitor_THT
CP_Radial_Tantal_D4.5mm_P5.00mm
CP, Radial_Tantal series, Radial, pin pitch=5.00mm, , diameter=4.5mm, Tantal Electrolytic Capacitor, http://cdn-reichelt.de/documents/datenblatt/B300/TANTAL-TB-Serie%23.pdf
CP Radial_Tantal series Radial pin pitch 5.00mm  diameter 4.5mm Tantal Electrolytic Capacitor
0
2
2
Capacitor_THT
CP_Radial_Tantal_D5.0mm_P2.50mm
CP, Radial_Tantal series, Radial, pin pitch=2.50mm, , diameter=5.0mm, Tantal Electrolytic Capacitor, http://cdn-reichelt.de/documents/datenblatt/B300/TANTAL-TB-Serie%23.pdf
CP Radial_Tantal series Radial pin pitch 2.50mm  diameter 5.0mm Tantal Electrolytic Capacitor
0
2
2
Capacitor_THT
CP_Radial_Tantal_D5.0mm_P5.00mm
CP, Radial_Tantal series, Radial, pin pitch=5.00mm, , diameter=5.0mm, Tantal Electrolytic Capacitor, http://cdn-reichelt.de/documents/datenblatt/B300/TANTAL-TB-Serie%23.pdf
CP Radial_Tantal series Radial pin pitch 5.00mm  diameter 5.0mm Tantal Electrolytic Capacitor
0
2
2
Capacitor_THT
CP_Radial_Tantal_D5.5mm_P2.50mm
CP, Radial_Tantal series, Radial, pin pitch=2.50mm, , diameter=5.5mm, Tantal Electrolytic Capacitor, http://cdn-reichelt.de/documents/datenblatt/B300/TANTAL-TB-Serie%23.pdf
CP Radial_Tantal series Radial pin pitch 2.50mm  diameter 5.5mm Tantal Electrolytic Capacitor
0
2
2
Capacitor_THT
CP_Radial_Tantal_D5.5mm_P5.00mm
CP, Radial_Tantal series, Radial, pin pitch=5.00mm, , diameter=5.5mm, Tantal Electrolytic Capacitor, http://cdn-reichelt.de/documents/datenblatt/B300/TANTAL-TB-Serie%23.pdf
CP Radial_Tantal series Radial pin pitch 5.00mm  diameter 5.5mm Tantal Electrolytic Capacitor
0
2
2
Capacitor_THT
CP_Radial_Tantal_D6.0mm_P2.50mm
CP, Radial_Tantal series, Radial, pin pitch=2.50mm, , diameter=6.0mm, Tantal Electrolytic Capacitor, http://cdn-reichelt.de/documents/datenblatt/B300/TANTAL-TB-Serie%23.pdf
CP Radial_Tantal series Radial pin pitch 2.50mm  diameter 6.0mm Tantal Electrolytic Capacitor
0
2
2
Capacitor_THT
CP_Radial_Tantal_D6.0mm_P5.00mm
CP, Radial_Tantal series, Radial, pin pitch=5.00mm, , diameter=6.0mm, Tantal Electrolytic Capacitor, http://cdn-reichelt.de/documents/datenblatt/B300/TANTAL-TB-Serie%23.pdf
CP Radial_Tantal series Radial pin pitch 5.00mm  diameter 6.0mm Tantal Electrolytic Capacitor
0
2
2
Capacitor_THT
CP_Radial_Tantal_D7.0mm_P2.50mm
CP, Radial_Tantal series, Radial, pin pitch=2.50mm, , diameter=7.0mm, Tantal Electrolytic Capacitor, http://cdn-reichelt.de/documents/datenblatt/B300/TANTAL-TB-Serie%23.pdf
CP Radial_Tantal series Radial pin pitch 2.50mm  diameter 7.0mm Tantal Electrolytic Capacitor
0
2
2
Capacitor_THT
CP_Radial_Tantal_D7.0mm_P5.00mm
CP, Radial_Tantal series, Radial, pin pitch=5.00mm, , diameter=7.0mm, Tantal Electrolytic Capacitor, http://cdn-reichelt.de/documents/datenblatt/B300/TANTAL-TB-Serie%23.pdf
CP Radial_Tantal series Radial pin pitch 5.00mm  diameter 7.0mm Tantal Electrolytic Capacitor
0
2
2
Capacitor_THT
CP_Radial_Tantal_D8.0mm_P2.50mm
CP, Radial_Tantal series, Radial, pin pitch=2.50mm, , diameter=8.0mm, Tantal Electrolytic Capacitor, http://cdn-reichelt.de/documents/datenblatt/B300/TANTAL-TB-Serie%23.pdf
CP Radial_Tantal series Radial pin pitch 2.50mm  diameter 8.0mm Tantal Electrolytic Capacitor
0
2
2
Capacitor_THT
CP_Radial_Tantal_D8.0mm_P5.00mm
CP, Radial_Tantal series, Radial, pin pitch=5.00mm, , diameter=8.0mm, Tantal Electrolytic Capacitor, http://cdn-reichelt.de/documents/datenblatt/B300/TANTAL-TB-Serie%23.pdf
CP Radial_Tantal series Radial pin pitch 5.00mm  diameter 8.0mm Tantal Electrolytic Capacitor
0
2
2
Capacitor_THT
CP_Radial_Tantal_D9.0mm_P2.50mm
CP, Radial_Tantal series, Radial, pin pitch=2.50mm, , diameter=9.0mm, Tantal Electrolytic Capacitor, http://cdn-reichelt.de/documents/datenblatt/B300/TANTAL-TB-Serie%23.pdf
CP Radial_Tantal series Radial pin pitch 2.50mm  diameter 9.0mm Tantal Electrolytic Capacitor
0
2
2
Capacitor_THT
CP_Radial_Tantal_D9.0mm_P5.00mm
CP, Radial_Tantal series, Radial, pin pitch=5.00mm, , diameter=9.0mm, Tantal Electrolytic Capacitor, http://cdn-reichelt.de/documents/datenblatt/B300/TANTAL-TB-Serie%23.pdf
CP Radial_Tantal series Radial pin pitch 5.00mm  diameter 9.0mm Tantal Electrolytic Capacitor
0
2
2
Capacitor_THT
CP_Radial_Tantal_D10.5mm_P2.50mm
CP, Radial_Tantal series, Radial, pin pitch=2.50mm, , diameter=10.5mm, Tantal Electrolytic Capacitor, http://cdn-reichelt.de/documents/datenblatt/B300/TANTAL-TB-Serie%23.pdf
CP Radial_Tantal series Radial pin pitch 2.50mm  diameter 10.5mm Tantal Electrolytic Capacitor
0
2
2
Capacitor_THT
CP_Radial_Tantal_D10.5mm_P5.00mm
CP, Radial_Tantal series, Radial, pin pitch=5.00mm, , diameter=10.5mm, Tantal Electrolytic Capacitor, http://cdn-reichelt.de/documents/datenblatt/B300/TANTAL-TB-Serie%23.pdf
CP Radial_Tantal series Radial pin pitch 5.00mm  diameter 10.5mm Tantal Electrolytic Capacitor
0
2
2
Capacitor_THT
C_Axial_L3.8mm_D2.6mm_P7.50mm_Horizontal
C, Axial series, Axial, Horizontal, pin pitch=7.5mm, , length*diameter=3.8*2.6mm^2, http://www.vishay.com/docs/45231/arseries.pdf
C Axial series Axial Horizontal pin pitch 7.5mm  length 3.8mm diameter 2.6mm
0
2
2
Capacitor_THT
C_Axial_L3.8mm_D2.6mm_P10.00mm_Horizontal
C, Axial series, Axial, Horizontal, pin pitch=10mm, , length*diameter=3.8*2.6mm^2, http://www.vishay.com/docs/45231/arseries.pdf
C Axial series Axial Horizontal pin pitch 10mm  length 3.8mm diameter 2.6mm
0
2
2
Capacitor_THT
C_Axial_L3.8mm_D2.6mm_P12.50mm_Horizontal
C, Axial series, Axial, Horizontal, pin pitch=12.5mm, , length*diameter=3.8*2.6mm^2, http://www.vishay.com/docs/45231/arseries.pdf
C Axial series Axial Horizontal pin pitch 12.5mm  length 3.8mm diameter 2.6mm
0
2
2
Capacitor_THT
C_Axial_L3.8mm_D2.6mm_P15.00mm_Horizontal
C, Axial series, Axial, Horizontal, pin pitch=15mm, , length*diameter=3.8*2.6mm^2, http://www.vishay.com/docs/45231/arseries.pdf
C Axial series Axial Horizontal pin pitch 15mm  length 3.8mm diameter 2.6mm
0
2
2
Capacitor_THT
C_Axial_L5.1mm_D3.1mm_P7.50mm_Horizontal
C, Axial series, Axial, Horizontal, pin pitch=7.5mm, , length*diameter=5.1*3.1mm^2, http://www.vishay.com/docs/45231/arseries.pdf
C Axial series Axial Horizontal pin pitch 7.5mm  length 5.1mm diameter 3.1mm
0
2
2
Capacitor_THT
C_Axial_L5.1mm_D3.1mm_P10.00mm_Horizontal
C, Axial series, Axial, Horizontal, pin pitch=10mm, , length*diameter=5.1*3.1mm^2, http://www.vishay.com/docs/45231/arseries.pdf
C Axial series Axial Horizontal pin pitch 10mm  length 5.1mm diameter 3.1mm
0
2
2
Capacitor_THT
C_Axial_L5.1mm_D3.1mm_P12.50mm_Horizontal
C, Axial series, Axial, Horizontal, pin pitch=12.5mm, , length*diameter=5.1*3.1mm^2, http://www.vishay.com/docs/45231/arseries.pdf
C Axial series Axial Horizontal pin pitch 12.5mm  length 5.1mm diameter 3.1mm
0
2
2
Capacitor_THT
C_Axial_L5.1mm_D3.1mm_P15.00mm_Horizontal
C, Axial series, Axial, Horizontal, pin pitch=15mm, , length*diameter=5.1*3.1mm^2, http://www.vishay.com/docs/45231/arseries.pdf
C Axial series Axial Horizontal pin pitch 15mm  length 5.1mm diameter 3.1mm
0
2
2
Capacitor_THT
C_Axial_L12.0mm_D6.5mm_P15.00mm_Horizontal
C, Axial series, Axial, Horizontal, pin pitch=15mm, , length*diameter=12*6.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B300/STYROFLEX.pdf
C Axial series Axial Horizontal pin pitch 15mm  length 12mm diameter 6.5mm
0
2
2
Capacitor_THT
C_Axial_L12.0mm_D6.5mm_P20.00mm_Horizontal
C, Axial series, Axial, Horizontal, pin pitch=20mm, , length*diameter=12*6.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B300/STYROFLEX.pdf
C Axial series Axial Horizontal pin pitch 20mm  length 12mm diameter 6.5mm
0
2
2
Capacitor_THT
C_Axial_L12.0mm_D7.5mm_P15.00mm_Horizontal
C, Axial series, Axial, Horizontal, pin pitch=15mm, , length*diameter=12*7.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B300/STYROFLEX.pdf
C Axial series Axial Horizontal pin pitch 15mm  length 12mm diameter 7.5mm
0
2
2
Capacitor_THT
C_Axial_L12.0mm_D7.5mm_P20.00mm_Horizontal
C, Axial series, Axial, Horizontal, pin pitch=20mm, , length*diameter=12*7.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B300/STYROFLEX.pdf
C Axial series Axial Horizontal pin pitch 20mm  length 12mm diameter 7.5mm
0
2
2
Capacitor_THT
C_Axial_L12.0mm_D8.5mm_P15.00mm_Horizontal
C, Axial series, Axial, Horizontal, pin pitch=15mm, , length*diameter=12*8.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B300/STYROFLEX.pdf
C Axial series Axial Horizontal pin pitch 15mm  length 12mm diameter 8.5mm
0
2
2
Capacitor_THT
C_Axial_L12.0mm_D8.5mm_P20.00mm_Horizontal
C, Axial series, Axial, Horizontal, pin pitch=20mm, , length*diameter=12*8.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B300/STYROFLEX.pdf
C Axial series Axial Horizontal pin pitch 20mm  length 12mm diameter 8.5mm
0
2
2
Capacitor_THT
C_Axial_L12.0mm_D9.5mm_P15.00mm_Horizontal
C, Axial series, Axial, Horizontal, pin pitch=15mm, , length*diameter=12*9.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B300/STYROFLEX.pdf
C Axial series Axial Horizontal pin pitch 15mm  length 12mm diameter 9.5mm
0
2
2
Capacitor_THT
C_Axial_L12.0mm_D9.5mm_P20.00mm_Horizontal
C, Axial series, Axial, Horizontal, pin pitch=20mm, , length*diameter=12*9.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B300/STYROFLEX.pdf
C Axial series Axial Horizontal pin pitch 20mm  length 12mm diameter 9.5mm
0
2
2
Capacitor_THT
C_Axial_L12.0mm_D10.5mm_P15.00mm_Horizontal
C, Axial series, Axial, Horizontal, pin pitch=15mm, , length*diameter=12*10.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B300/STYROFLEX.pdf
C Axial series Axial Horizontal pin pitch 15mm  length 12mm diameter 10.5mm
0
2
2
Capacitor_THT
C_Axial_L12.0mm_D10.5mm_P20.00mm_Horizontal
C, Axial series, Axial, Horizontal, pin pitch=20mm, , length*diameter=12*10.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B300/STYROFLEX.pdf
C Axial series Axial Horizontal pin pitch 20mm  length 12mm diameter 10.5mm
0
2
2
Capacitor_THT
C_Axial_L17.0mm_D6.5mm_P20.00mm_Horizontal
C, Axial series, Axial, Horizontal, pin pitch=20mm, , length*diameter=17*6.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B300/STYROFLEX.pdf
C Axial series Axial Horizontal pin pitch 20mm  length 17mm diameter 6.5mm
0
2
2
Capacitor_THT
C_Axial_L17.0mm_D6.5mm_P25.00mm_Horizontal
C, Axial series, Axial, Horizontal, pin pitch=25mm, , length*diameter=17*6.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B300/STYROFLEX.pdf
C Axial series Axial Horizontal pin pitch 25mm  length 17mm diameter 6.5mm
0
2
2
Capacitor_THT
C_Axial_L17.0mm_D7.0mm_P20.00mm_Horizontal
C, Axial series, Axial, Horizontal, pin pitch=20mm, , length*diameter=17*7.0mm^2, http://cdn-reichelt.de/documents/datenblatt/B300/STYROFLEX.pdf
C Axial series Axial Horizontal pin pitch 20mm  length 17mm diameter 7.0mm
0
2
2
Capacitor_THT
C_Axial_L17.0mm_D7.0mm_P25.00mm_Horizontal
C, Axial series, Axial, Horizontal, pin pitch=25mm, , length*diameter=17*7.0mm^2, http://cdn-reichelt.de/documents/datenblatt/B300/STYROFLEX.pdf
C Axial series Axial Horizontal pin pitch 25mm  length 17mm diameter 7.0mm
0
2
2
Capacitor_THT
C_Axial_L19.0mm_D7.5mm_P25.00mm_Horizontal
C, Axial series, Axial, Horizontal, pin pitch=25mm, , length*diameter=19*7.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B300/STYROFLEX.pdf
C Axial series Axial Horizontal pin pitch 25mm  length 19mm diameter 7.5mm
0
2
2
Capacitor_THT
C_Axial_L19.0mm_D8.0mm_P25.00mm_Horizontal
C, Axial series, Axial, Horizontal, pin pitch=25mm, , length*diameter=19*8.0mm^2, http://cdn-reichelt.de/documents/datenblatt/B300/STYROFLEX.pdf
C Axial series Axial Horizontal pin pitch 25mm  length 19mm diameter 8.0mm
0
2
2
Capacitor_THT
C_Axial_L19.0mm_D9.0mm_P25.00mm_Horizontal
C, Axial series, Axial, Horizontal, pin pitch=25mm, , length*diameter=19*9mm^2, http://cdn-reichelt.de/documents/datenblatt/B300/STYROFLEX.pdf
C Axial series Axial Horizontal pin pitch 25mm  length 19mm diameter 9mm
0
2
2
Capacitor_THT
C_Axial_L19.0mm_D9.5mm_P25.00mm_Horizontal
C, Axial series, Axial, Horizontal, pin pitch=25mm, , length*diameter=19*9.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B300/STYROFLEX.pdf
C Axial series Axial Horizontal pin pitch 25mm  length 19mm diameter 9.5mm
0
2
2
Capacitor_THT
C_Axial_L22.0mm_D9.5mm_P27.50mm_Horizontal
C, Axial series, Axial, Horizontal, pin pitch=27.5mm, , length*diameter=22*9.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B300/STYROFLEX.pdf
C Axial series Axial Horizontal pin pitch 27.5mm  length 22mm diameter 9.5mm
0
2
2
Capacitor_THT
C_Axial_L22.0mm_D10.5mm_P27.50mm_Horizontal
C, Axial series, Axial, Horizontal, pin pitch=27.5mm, , length*diameter=22*10.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B300/STYROFLEX.pdf
C Axial series Axial Horizontal pin pitch 27.5mm  length 22mm diameter 10.5mm
0
2
2
Capacitor_THT
C_Disc_D3.0mm_W1.6mm_P2.50mm
C, Disc series, Radial, pin pitch=2.50mm, , diameter*width=3.0*1.6mm^2, Capacitor, http://www.vishay.com/docs/45233/krseries.pdf
C Disc series Radial pin pitch 2.50mm  diameter 3.0mm width 1.6mm Capacitor
0
2
2
Capacitor_THT
C_Disc_D3.0mm_W2.0mm_P2.50mm
C, Disc series, Radial, pin pitch=2.50mm, , diameter*width=3*2mm^2, Capacitor
C Disc series Radial pin pitch 2.50mm  diameter 3mm width 2mm Capacitor
0
2
2
Capacitor_THT
C_Disc_D3.4mm_W2.1mm_P2.50mm
C, Disc series, Radial, pin pitch=2.50mm, , diameter*width=3.4*2.1mm^2, Capacitor, http://www.vishay.com/docs/45233/krseries.pdf
C Disc series Radial pin pitch 2.50mm  diameter 3.4mm width 2.1mm Capacitor
0
2
2
Capacitor_THT
C_Disc_D3.8mm_W2.6mm_P2.50mm
C, Disc series, Radial, pin pitch=2.50mm, , diameter*width=3.8*2.6mm^2, Capacitor, http://www.vishay.com/docs/45233/krseries.pdf
C Disc series Radial pin pitch 2.50mm  diameter 3.8mm width 2.6mm Capacitor
0
2
2
Capacitor_THT
C_Disc_D4.3mm_W1.9mm_P5.00mm
C, Disc series, Radial, pin pitch=5.00mm, , diameter*width=4.3*1.9mm^2, Capacitor, http://www.vishay.com/docs/45233/krseries.pdf
C Disc series Radial pin pitch 5.00mm  diameter 4.3mm width 1.9mm Capacitor
0
2
2
Capacitor_THT
C_Disc_D4.7mm_W2.5mm_P5.00mm
C, Disc series, Radial, pin pitch=5.00mm, , diameter*width=4.7*2.5mm^2, Capacitor, http://www.vishay.com/docs/45233/krseries.pdf
C Disc series Radial pin pitch 5.00mm  diameter 4.7mm width 2.5mm Capacitor
0
2
2
Capacitor_THT
C_Disc_D5.0mm_W2.5mm_P2.50mm
C, Disc series, Radial, pin pitch=2.50mm, , diameter*width=5*2.5mm^2, Capacitor, http://cdn-reichelt.de/documents/datenblatt/B300/DS_KERKO_TC.pdf
C Disc series Radial pin pitch 2.50mm  diameter 5mm width 2.5mm Capacitor
0
2
2
Capacitor_THT
C_Disc_D5.0mm_W2.5mm_P5.00mm
C, Disc series, Radial, pin pitch=5.00mm, , diameter*width=5*2.5mm^2, Capacitor, http://cdn-reichelt.de/documents/datenblatt/B300/DS_KERKO_TC.pdf
C Disc series Radial pin pitch 5.00mm  diameter 5mm width 2.5mm Capacitor
0
2
2
Capacitor_THT
C_Disc_D5.1mm_W3.2mm_P5.00mm
C, Disc series, Radial, pin pitch=5.00mm, , diameter*width=5.1*3.2mm^2, Capacitor, http://www.vishay.com/docs/45233/krseries.pdf
C Disc series Radial pin pitch 5.00mm  diameter 5.1mm width 3.2mm Capacitor
0
2
2
Capacitor_THT
C_Disc_D6.0mm_W2.5mm_P5.00mm
C, Disc series, Radial, pin pitch=5.00mm, , diameter*width=6*2.5mm^2, Capacitor, http://cdn-reichelt.de/documents/datenblatt/B300/DS_KERKO_TC.pdf
C Disc series Radial pin pitch 5.00mm  diameter 6mm width 2.5mm Capacitor
0
2
2
Capacitor_THT
C_Disc_D6.0mm_W4.4mm_P5.00mm
C, Disc series, Radial, pin pitch=5.00mm, , diameter*width=6*4.4mm^2, Capacitor
C Disc series Radial pin pitch 5.00mm  diameter 6mm width 4.4mm Capacitor
0
2
2
Capacitor_THT
C_Disc_D7.0mm_W2.5mm_P5.00mm
C, Disc series, Radial, pin pitch=5.00mm, , diameter*width=7*2.5mm^2, Capacitor, http://cdn-reichelt.de/documents/datenblatt/B300/DS_KERKO_TC.pdf
C Disc series Radial pin pitch 5.00mm  diameter 7mm width 2.5mm Capacitor
0
2
2
Capacitor_THT
C_Disc_D7.5mm_W2.5mm_P5.00mm
C, Disc series, Radial, pin pitch=5.00mm, , diameter*width=7.5*2.5mm^2, Capacitor, http://www.vishay.com/docs/28535/vy2series.pdf
C Disc series Radial pin pitch 5.00mm  diameter 7.5mm width 2.5mm Capacitor
0
2
2
Capacitor_THT
C_Disc_D7.5mm_W4.4mm_P5.00mm
C, Disc series, Radial, pin pitch=5.00mm, , diameter*width=7.5*4.4mm^2, Capacitor
C Disc series Radial pin pitch 5.00mm  diameter 7.5mm width 4.4mm Capacitor
0
2
2
Capacitor_THT
C_Disc_D7.5mm_W5.0mm_P5.00mm
C, Disc series, Radial, pin pitch=5.00mm, , diameter*width=7.5*5.0mm^2, Capacitor, http://www.vishay.com/docs/28535/vy2series.pdf
C Disc series Radial pin pitch 5.00mm  diameter 7.5mm width 5.0mm Capacitor
0
2
2
Capacitor_THT
C_Disc_D7.5mm_W5.0mm_P7.50mm
C, Disc series, Radial, pin pitch=7.50mm, , diameter*width=7.5*5.0mm^2, Capacitor, http://www.vishay.com/docs/28535/vy2series.pdf
C Disc series Radial pin pitch 7.50mm  diameter 7.5mm width 5.0mm Capacitor
0
2
2
Capacitor_THT
C_Disc_D7.5mm_W5.0mm_P10.00mm
C, Disc series, Radial, pin pitch=10.00mm, , diameter*width=7.5*5.0mm^2, Capacitor, http://www.vishay.com/docs/28535/vy2series.pdf
C Disc series Radial pin pitch 10.00mm  diameter 7.5mm width 5.0mm Capacitor
0
2
2
Capacitor_THT
C_Disc_D8.0mm_W2.5mm_P5.00mm
C, Disc series, Radial, pin pitch=5.00mm, , diameter*width=8*2.5mm^2, Capacitor, http://cdn-reichelt.de/documents/datenblatt/B300/DS_KERKO_TC.pdf
C Disc series Radial pin pitch 5.00mm  diameter 8mm width 2.5mm Capacitor
0
2
2
Capacitor_THT
C_Disc_D8.0mm_W5.0mm_P5.00mm
C, Disc series, Radial, pin pitch=5.00mm, , diameter*width=8*5.0mm^2, Capacitor, http://www.vishay.com/docs/28535/vy2series.pdf
C Disc series Radial pin pitch 5.00mm  diameter 8mm width 5.0mm Capacitor
0
2
2
Capacitor_THT
C_Disc_D8.0mm_W5.0mm_P7.50mm
C, Disc series, Radial, pin pitch=7.50mm, , diameter*width=8*5.0mm^2, Capacitor, http://www.vishay.com/docs/28535/vy2series.pdf
C Disc series Radial pin pitch 7.50mm  diameter 8mm width 5.0mm Capacitor
0
2
2
Capacitor_THT
C_Disc_D8.0mm_W5.0mm_P10.00mm
C, Disc series, Radial, pin pitch=10.00mm, , diameter*width=8*5.0mm^2, Capacitor, http://www.vishay.com/docs/28535/vy2series.pdf
C Disc series Radial pin pitch 10.00mm  diameter 8mm width 5.0mm Capacitor
0
2
2
Capacitor_THT
C_Disc_D9.0mm_W2.5mm_P5.00mm
C, Disc series, Radial, pin pitch=5.00mm, , diameter*width=9*2.5mm^2, Capacitor, http://cdn-reichelt.de/documents/datenblatt/B300/DS_KERKO_TC.pdf
C Disc series Radial pin pitch 5.00mm  diameter 9mm width 2.5mm Capacitor
0
2
2
Capacitor_THT
C_Disc_D9.0mm_W5.0mm_P5.00mm
C, Disc series, Radial, pin pitch=5.00mm, , diameter*width=9*5.0mm^2, Capacitor, http://www.vishay.com/docs/28535/vy2series.pdf
C Disc series Radial pin pitch 5.00mm  diameter 9mm width 5.0mm Capacitor
0
2
2
Capacitor_THT
C_Disc_D9.0mm_W5.0mm_P7.50mm
C, Disc series, Radial, pin pitch=7.50mm, , diameter*width=9*5.0mm^2, Capacitor, http://www.vishay.com/docs/28535/vy2series.pdf
C Disc series Radial pin pitch 7.50mm  diameter 9mm width 5.0mm Capacitor
0
2
2
Capacitor_THT
C_Disc_D9.0mm_W5.0mm_P10.00mm
C, Disc series, Radial, pin pitch=10.00mm, , diameter*width=9*5.0mm^2, Capacitor, http://www.vishay.com/docs/28535/vy2series.pdf
C Disc series Radial pin pitch 10.00mm  diameter 9mm width 5.0mm Capacitor
0
2
2
Capacitor_THT
C_Disc_D10.0mm_W2.5mm_P5.00mm
C, Disc series, Radial, pin pitch=5.00mm, , diameter*width=10*2.5mm^2, Capacitor, http://cdn-reichelt.de/documents/datenblatt/B300/DS_KERKO_TC.pdf
C Disc series Radial pin pitch 5.00mm  diameter 10mm width 2.5mm Capacitor
0
2
2
Capacitor_THT
C_Disc_D10.5mm_W5.0mm_P5.00mm
C, Disc series, Radial, pin pitch=5.00mm, , diameter*width=10.5*5.0mm^2, Capacitor, http://www.vishay.com/docs/28535/vy2series.pdf
C Disc series Radial pin pitch 5.00mm  diameter 10.5mm width 5.0mm Capacitor
0
2
2
Capacitor_THT
C_Disc_D10.5mm_W5.0mm_P7.50mm
C, Disc series, Radial, pin pitch=7.50mm, , diameter*width=10.5*5.0mm^2, Capacitor, http://www.vishay.com/docs/28535/vy2series.pdf
C Disc series Radial pin pitch 7.50mm  diameter 10.5mm width 5.0mm Capacitor
0
2
2
Capacitor_THT
C_Disc_D10.5mm_W5.0mm_P10.00mm
C, Disc series, Radial, pin pitch=10.00mm, , diameter*width=10.5*5.0mm^2, Capacitor, http://www.vishay.com/docs/28535/vy2series.pdf
C Disc series Radial pin pitch 10.00mm  diameter 10.5mm width 5.0mm Capacitor
0
2
2
Capacitor_THT
C_Disc_D11.0mm_W5.0mm_P5.00mm
C, Disc series, Radial, pin pitch=5.00mm, , diameter*width=11*5.0mm^2, Capacitor, http://www.vishay.com/docs/28535/vy2series.pdf
C Disc series Radial pin pitch 5.00mm  diameter 11mm width 5.0mm Capacitor
0
2
2
Capacitor_THT
C_Disc_D11.0mm_W5.0mm_P7.50mm
C, Disc series, Radial, pin pitch=7.50mm, , diameter*width=11*5.0mm^2, Capacitor, http://www.vishay.com/docs/28535/vy2series.pdf
C Disc series Radial pin pitch 7.50mm  diameter 11mm width 5.0mm Capacitor
0
2
2
Capacitor_THT
C_Disc_D11.0mm_W5.0mm_P10.00mm
C, Disc series, Radial, pin pitch=10.00mm, , diameter*width=11*5.0mm^2, Capacitor, http://www.vishay.com/docs/28535/vy2series.pdf
C Disc series Radial pin pitch 10.00mm  diameter 11mm width 5.0mm Capacitor
0
2
2
Capacitor_THT
C_Disc_D12.0mm_W4.4mm_P7.75mm
C, Disc series, Radial, pin pitch=7.75mm, , diameter*width=12*4.4mm^2, Capacitor
C Disc series Radial pin pitch 7.75mm  diameter 12mm width 4.4mm Capacitor
0
2
2
Capacitor_THT
C_Disc_D12.5mm_W5.0mm_P7.50mm
C, Disc series, Radial, pin pitch=7.50mm, , diameter*width=12.5*5.0mm^2, Capacitor, http://www.vishay.com/docs/28535/vy2series.pdf
C Disc series Radial pin pitch 7.50mm  diameter 12.5mm width 5.0mm Capacitor
0
2
2
Capacitor_THT
C_Disc_D12.5mm_W5.0mm_P10.00mm
C, Disc series, Radial, pin pitch=10.00mm, , diameter*width=12.5*5.0mm^2, Capacitor, http://www.vishay.com/docs/28535/vy2series.pdf
C Disc series Radial pin pitch 10.00mm  diameter 12.5mm width 5.0mm Capacitor
0
2
2
Capacitor_THT
C_Disc_D14.5mm_W5.0mm_P7.50mm
C, Disc series, Radial, pin pitch=7.50mm, , diameter*width=14.5*5.0mm^2, Capacitor, http://www.vishay.com/docs/28535/vy2series.pdf
C Disc series Radial pin pitch 7.50mm  diameter 14.5mm width 5.0mm Capacitor
0
2
2
Capacitor_THT
C_Disc_D14.5mm_W5.0mm_P10.00mm
C, Disc series, Radial, pin pitch=10.00mm, , diameter*width=14.5*5.0mm^2, Capacitor, http://www.vishay.com/docs/28535/vy2series.pdf
C Disc series Radial pin pitch 10.00mm  diameter 14.5mm width 5.0mm Capacitor
0
2
2
Capacitor_THT
C_Disc_D16.0mm_W5.0mm_P7.50mm
C, Disc series, Radial, pin pitch=7.50mm, , diameter*width=16.0*5.0mm^2, Capacitor, http://www.vishay.com/docs/28535/vy2series.pdf
C Disc series Radial pin pitch 7.50mm  diameter 16.0mm width 5.0mm Capacitor
0
2
2
Capacitor_THT
C_Disc_D16.0mm_W5.0mm_P10.00mm
C, Disc series, Radial, pin pitch=10.00mm, , diameter*width=16.0*5.0mm^2, Capacitor, http://www.vishay.com/docs/28535/vy2series.pdf
C Disc series Radial pin pitch 10.00mm  diameter 16.0mm width 5.0mm Capacitor
0
2
2
Capacitor_THT
C_Radial_D4.0mm_H5.0mm_P1.50mm
C, Radial series, Radial, pin pitch=1.50mm, diameter=4mm, height=5mm, Non-Polar Electrolytic Capacitor
C Radial series Radial pin pitch 1.50mm diameter 4mm height 5mm Non-Polar Electrolytic Capacitor
0
2
2
Capacitor_THT
C_Radial_D4.0mm_H7.0mm_P1.50mm
C, Radial series, Radial, pin pitch=1.50mm, diameter=4mm, height=7mm, Non-Polar Electrolytic Capacitor
C Radial series Radial pin pitch 1.50mm diameter 4mm height 7mm Non-Polar Electrolytic Capacitor
0
2
2
Capacitor_THT
C_Radial_D5.0mm_H5.0mm_P2.00mm
C, Radial series, Radial, pin pitch=2.00mm, diameter=5mm, height=5mm, Non-Polar Electrolytic Capacitor
C Radial series Radial pin pitch 2.00mm diameter 5mm height 5mm Non-Polar Electrolytic Capacitor
0
2
2
Capacitor_THT
C_Radial_D5.0mm_H7.0mm_P2.00mm
C, Radial series, Radial, pin pitch=2.00mm, diameter=5mm, height=7mm, Non-Polar Electrolytic Capacitor
C Radial series Radial pin pitch 2.00mm diameter 5mm height 7mm Non-Polar Electrolytic Capacitor
0
2
2
Capacitor_THT
C_Radial_D5.0mm_H11.0mm_P2.00mm
C, Radial series, Radial, pin pitch=2.00mm, diameter=5mm, height=11mm, Non-Polar Electrolytic Capacitor
C Radial series Radial pin pitch 2.00mm diameter 5mm height 11mm Non-Polar Electrolytic Capacitor
0
2
2
Capacitor_THT
C_Radial_D6.3mm_H5.0mm_P2.50mm
C, Radial series, Radial, pin pitch=2.50mm, diameter=6.3mm, height=5mm, Non-Polar Electrolytic Capacitor
C Radial series Radial pin pitch 2.50mm diameter 6.3mm height 5mm Non-Polar Electrolytic Capacitor
0
2
2
Capacitor_THT
C_Radial_D6.3mm_H7.0mm_P2.50mm
C, Radial series, Radial, pin pitch=2.50mm, diameter=6.3mm, height=7mm, Non-Polar Electrolytic Capacitor
C Radial series Radial pin pitch 2.50mm diameter 6.3mm height 7mm Non-Polar Electrolytic Capacitor
0
2
2
Capacitor_THT
C_Radial_D6.3mm_H11.0mm_P2.50mm
C, Radial series, Radial, pin pitch=2.50mm, diameter=6.3mm, height=11mm, Non-Polar Electrolytic Capacitor
C Radial series Radial pin pitch 2.50mm diameter 6.3mm height 11mm Non-Polar Electrolytic Capacitor
0
2
2
Capacitor_THT
C_Radial_D8.0mm_H7.0mm_P3.50mm
C, Radial series, Radial, pin pitch=3.50mm, diameter=8mm, height=7mm, Non-Polar Electrolytic Capacitor
C Radial series Radial pin pitch 3.50mm diameter 8mm height 7mm Non-Polar Electrolytic Capacitor
0
2
2
Capacitor_THT
C_Radial_D8.0mm_H11.5mm_P3.50mm
C, Radial series, Radial, pin pitch=3.50mm, diameter=8mm, height=11.5mm, Non-Polar Electrolytic Capacitor
C Radial series Radial pin pitch 3.50mm diameter 8mm height 11.5mm Non-Polar Electrolytic Capacitor
0
2
2
Capacitor_THT
C_Radial_D10.0mm_H12.5mm_P5.00mm
C, Radial series, Radial, pin pitch=5.00mm, diameter=10mm, height=12.5mm, Non-Polar Electrolytic Capacitor
C Radial series Radial pin pitch 5.00mm diameter 10mm height 12.5mm Non-Polar Electrolytic Capacitor
0
2
2
Capacitor_THT
C_Radial_D10.0mm_H16.0mm_P5.00mm
C, Radial series, Radial, pin pitch=5.00mm, diameter=10mm, height=16mm, Non-Polar Electrolytic Capacitor
C Radial series Radial pin pitch 5.00mm diameter 10mm height 16mm Non-Polar Electrolytic Capacitor
0
2
2
Capacitor_THT
C_Radial_D10.0mm_H20.0mm_P5.00mm
C, Radial series, Radial, pin pitch=5.00mm, diameter=10mm, height=20mm, Non-Polar Electrolytic Capacitor
C Radial series Radial pin pitch 5.00mm diameter 10mm height 20mm Non-Polar Electrolytic Capacitor
0
2
2
Capacitor_THT
C_Radial_D12.5mm_H20.0mm_P5.00mm
C, Radial series, Radial, pin pitch=5.00mm, diameter=12.5mm, height=20mm, Non-Polar Electrolytic Capacitor
C Radial series Radial pin pitch 5.00mm diameter 12.5mm height 20mm Non-Polar Electrolytic Capacitor
0
2
2
Capacitor_THT
C_Radial_D12.5mm_H25.0mm_P5.00mm
C, Radial series, Radial, pin pitch=5.00mm, diameter=12.5mm, height=25mm, Non-Polar Electrolytic Capacitor
C Radial series Radial pin pitch 5.00mm diameter 12.5mm height 25mm Non-Polar Electrolytic Capacitor
0
2
2
Capacitor_THT
C_Radial_D16.0mm_H25.0mm_P7.50mm
C, Radial series, Radial, pin pitch=7.50mm, diameter=16mm, height=25mm, Non-Polar Electrolytic Capacitor
C Radial series Radial pin pitch 7.50mm diameter 16mm height 25mm Non-Polar Electrolytic Capacitor
0
2
2
Capacitor_THT
C_Radial_D16.0mm_H31.5mm_P7.50mm
C, Radial series, Radial, pin pitch=7.50mm, diameter=16mm, height=31.5mm, Non-Polar Electrolytic Capacitor
C Radial series Radial pin pitch 7.50mm diameter 16mm height 31.5mm Non-Polar Electrolytic Capacitor
0
2
2
Capacitor_THT
C_Radial_D18.0mm_H35.5mm_P7.50mm
C, Radial series, Radial, pin pitch=7.50mm, diameter=18mm, height=35.5mm, Non-Polar Electrolytic Capacitor
C Radial series Radial pin pitch 7.50mm diameter 18mm height 35.5mm Non-Polar Electrolytic Capacitor
0
2
2
Capacitor_THT
C_Rect_L4.0mm_W2.5mm_P2.50mm
C, Rect series, Radial, pin pitch=2.50mm, , length*width=4*2.5mm^2, Capacitor
C Rect series Radial pin pitch 2.50mm  length 4mm width 2.5mm Capacitor
0
2
2
Capacitor_THT
C_Rect_L4.6mm_W2.0mm_P2.50mm_MKS02_FKP02
C, Rect series, Radial, pin pitch=2.50mm, , length*width=4.6*2mm^2, Capacitor, http://www.wima.de/DE/WIMA_MKS_02.pdf
C Rect series Radial pin pitch 2.50mm  length 4.6mm width 2mm Capacitor
0
2
2
Capacitor_THT
C_Rect_L4.6mm_W3.0mm_P2.50mm_MKS02_FKP02
C, Rect series, Radial, pin pitch=2.50mm, , length*width=4.6*3.0mm^2, Capacitor, http://www.wima.de/DE/WIMA_MKS_02.pdf
C Rect series Radial pin pitch 2.50mm  length 4.6mm width 3.0mm Capacitor
0
2
2
Capacitor_THT
C_Rect_L4.6mm_W3.8mm_P2.50mm_MKS02_FKP02
C, Rect series, Radial, pin pitch=2.50mm, , length*width=4.6*3.8mm^2, Capacitor, http://www.wima.de/DE/WIMA_MKS_02.pdf
C Rect series Radial pin pitch 2.50mm  length 4.6mm width 3.8mm Capacitor
0
2
2
Capacitor_THT
C_Rect_L4.6mm_W4.6mm_P2.50mm_MKS02_FKP02
C, Rect series, Radial, pin pitch=2.50mm, , length*width=4.6*4.6mm^2, Capacitor, http://www.wima.de/DE/WIMA_MKS_02.pdf
C Rect series Radial pin pitch 2.50mm  length 4.6mm width 4.6mm Capacitor
0
2
2
Capacitor_THT
C_Rect_L4.6mm_W5.5mm_P2.50mm_MKS02_FKP02
C, Rect series, Radial, pin pitch=2.50mm, , length*width=4.6*5.5mm^2, Capacitor, http://www.wima.de/DE/WIMA_MKS_02.pdf
C Rect series Radial pin pitch 2.50mm  length 4.6mm width 5.5mm Capacitor
0
2
2
Capacitor_THT
C_Rect_L7.0mm_W2.0mm_P5.00mm
C, Rect series, Radial, pin pitch=5.00mm, , length*width=7*2mm^2, Capacitor
C Rect series Radial pin pitch 5.00mm  length 7mm width 2mm Capacitor
0
2
2
Capacitor_THT
C_Rect_L7.0mm_W2.5mm_P5.00mm
C, Rect series, Radial, pin pitch=5.00mm, , length*width=7*2.5mm^2, Capacitor
C Rect series Radial pin pitch 5.00mm  length 7mm width 2.5mm Capacitor
0
2
2
Capacitor_THT
C_Rect_L7.0mm_W3.5mm_P2.50mm_P5.00mm
C, Rect series, Radial, pin pitch=2.50mm 5.00mm, , length*width=7*3.5mm^2, Capacitor
C Rect series Radial pin pitch 2.50mm 5.00mm  length 7mm width 3.5mm Capacitor
0
4
2
Capacitor_THT
C_Rect_L7.0mm_W3.5mm_P5.00mm
C, Rect series, Radial, pin pitch=5.00mm, , length*width=7*3.5mm^2, Capacitor
C Rect series Radial pin pitch 5.00mm  length 7mm width 3.5mm Capacitor
0
2
2
Capacitor_THT
C_Rect_L7.0mm_W4.5mm_P5.00mm
C, Rect series, Radial, pin pitch=5.00mm, , length*width=7*4.5mm^2, Capacitor
C Rect series Radial pin pitch 5.00mm  length 7mm width 4.5mm Capacitor
0
2
2
Capacitor_THT
C_Rect_L7.0mm_W6.0mm_P5.00mm
C, Rect series, Radial, pin pitch=5.00mm, , length*width=7*6mm^2, Capacitor
C Rect series Radial pin pitch 5.00mm  length 7mm width 6mm Capacitor
0
2
2
Capacitor_THT
C_Rect_L7.0mm_W6.5mm_P5.00mm
C, Rect series, Radial, pin pitch=5.00mm, , length*width=7*6.5mm^2, Capacitor
C Rect series Radial pin pitch 5.00mm  length 7mm width 6.5mm Capacitor
0
2
2
Capacitor_THT
C_Rect_L7.2mm_W2.5mm_P5.00mm_FKS2_FKP2_MKS2_MKP2
C, Rect series, Radial, pin pitch=5.00mm, , length*width=7.2*2.5mm^2, Capacitor, http://www.wima.com/EN/WIMA_FKS_2.pdf
C Rect series Radial pin pitch 5.00mm  length 7.2mm width 2.5mm Capacitor
0
2
2
Capacitor_THT
C_Rect_L7.2mm_W3.0mm_P5.00mm_FKS2_FKP2_MKS2_MKP2
C, Rect series, Radial, pin pitch=5.00mm, , length*width=7.2*3.0mm^2, Capacitor, http://www.wima.com/EN/WIMA_FKS_2.pdf
C Rect series Radial pin pitch 5.00mm  length 7.2mm width 3.0mm Capacitor
0
2
2
Capacitor_THT
C_Rect_L7.2mm_W3.5mm_P5.00mm_FKS2_FKP2_MKS2_MKP2
C, Rect series, Radial, pin pitch=5.00mm, , length*width=7.2*3.5mm^2, Capacitor, http://www.wima.com/EN/WIMA_FKS_2.pdf
C Rect series Radial pin pitch 5.00mm  length 7.2mm width 3.5mm Capacitor
0
2
2
Capacitor_THT
C_Rect_L7.2mm_W4.5mm_P5.00mm_FKS2_FKP2_MKS2_MKP2
C, Rect series, Radial, pin pitch=5.00mm, , length*width=7.2*4.5mm^2, Capacitor, http://www.wima.com/EN/WIMA_FKS_2.pdf
C Rect series Radial pin pitch 5.00mm  length 7.2mm width 4.5mm Capacitor
0
2
2
Capacitor_THT
C_Rect_L7.2mm_W5.5mm_P5.00mm_FKS2_FKP2_MKS2_MKP2
C, Rect series, Radial, pin pitch=5.00mm, , length*width=7.2*5.5mm^2, Capacitor, http://www.wima.com/EN/WIMA_FKS_2.pdf
C Rect series Radial pin pitch 5.00mm  length 7.2mm width 5.5mm Capacitor
0
2
2
Capacitor_THT
C_Rect_L7.2mm_W7.2mm_P5.00mm_FKS2_FKP2_MKS2_MKP2
C, Rect series, Radial, pin pitch=5.00mm, , length*width=7.2*7.2mm^2, Capacitor, http://www.wima.com/EN/WIMA_FKS_2.pdf
C Rect series Radial pin pitch 5.00mm  length 7.2mm width 7.2mm Capacitor
0
2
2
Capacitor_THT
C_Rect_L7.2mm_W8.5mm_P5.00mm_FKP2_FKP2_MKS2_MKP2
C, Rect series, Radial, pin pitch=5.00mm, , length*width=7.2*8.5mm^2, Capacitor, http://www.wima.com/EN/WIMA_FKS_2.pdf
C Rect series Radial pin pitch 5.00mm  length 7.2mm width 8.5mm Capacitor
0
2
2
Capacitor_THT
C_Rect_L7.2mm_W11.0mm_P5.00mm_FKS2_FKP2_MKS2_MKP2
C, Rect series, Radial, pin pitch=5.00mm, , length*width=7.2*11mm^2, Capacitor, http://www.wima.com/EN/WIMA_FKS_2.pdf
C Rect series Radial pin pitch 5.00mm  length 7.2mm width 11mm Capacitor
0
2
2
Capacitor_THT
C_Rect_L7.5mm_W6.5mm_P5.00mm
C, Rect series, Radial, pin pitch=5.00mm, , length*width=7.5*6.5mm^2, Capacitor
C Rect series Radial pin pitch 5.00mm  length 7.5mm width 6.5mm Capacitor
0
2
2
Capacitor_THT
C_Rect_L9.0mm_W2.5mm_P7.50mm_MKT
C, Rect series, Radial, pin pitch=7.50mm, , length*width=9*2.5mm^2, Capacitor, https://en.tdk.eu/inf/20/20/db/fc_2009/MKT_B32560_564.pdf
C Rect series Radial pin pitch 7.50mm  length 9mm width 2.5mm Capacitor
0
2
2
Capacitor_THT
C_Rect_L9.0mm_W2.6mm_P7.50mm_MKT
C, Rect series, Radial, pin pitch=7.50mm, , length*width=9*2.6mm^2, Capacitor, https://en.tdk.eu/inf/20/20/db/fc_2009/MKT_B32560_564.pdf
C Rect series Radial pin pitch 7.50mm  length 9mm width 2.6mm Capacitor
0
2
2
Capacitor_THT
C_Rect_L9.0mm_W2.7mm_P7.50mm_MKT
C, Rect series, Radial, pin pitch=7.50mm, , length*width=9*2.7mm^2, Capacitor, https://en.tdk.eu/inf/20/20/db/fc_2009/MKT_B32560_564.pdf
C Rect series Radial pin pitch 7.50mm  length 9mm width 2.7mm Capacitor
0
2
2
Capacitor_THT
C_Rect_L9.0mm_W3.2mm_P7.50mm_MKT
C, Rect series, Radial, pin pitch=7.50mm, , length*width=9*3.2mm^2, Capacitor, https://en.tdk.eu/inf/20/20/db/fc_2009/MKT_B32560_564.pdf
C Rect series Radial pin pitch 7.50mm  length 9mm width 3.2mm Capacitor
0
2
2
Capacitor_THT
C_Rect_L9.0mm_W3.3mm_P7.50mm_MKT
C, Rect series, Radial, pin pitch=7.50mm, , length*width=9*3.3mm^2, Capacitor, https://en.tdk.eu/inf/20/20/db/fc_2009/MKT_B32560_564.pdf
C Rect series Radial pin pitch 7.50mm  length 9mm width 3.3mm Capacitor
0
2
2
Capacitor_THT
C_Rect_L9.0mm_W3.4mm_P7.50mm_MKT
C, Rect series, Radial, pin pitch=7.50mm, , length*width=9*3.4mm^2, Capacitor, https://en.tdk.eu/inf/20/20/db/fc_2009/MKT_B32560_564.pdf
C Rect series Radial pin pitch 7.50mm  length 9mm width 3.4mm Capacitor
0
2
2
Capacitor_THT
C_Rect_L9.0mm_W3.6mm_P7.50mm_MKT
C, Rect series, Radial, pin pitch=7.50mm, , length*width=9*3.6mm^2, Capacitor, https://en.tdk.eu/inf/20/20/db/fc_2009/MKT_B32560_564.pdf
C Rect series Radial pin pitch 7.50mm  length 9mm width 3.6mm Capacitor
0
2
2
Capacitor_THT
C_Rect_L9.0mm_W3.8mm_P7.50mm_MKT
C, Rect series, Radial, pin pitch=7.50mm, , length*width=9*3.8mm^2, Capacitor, https://en.tdk.eu/inf/20/20/db/fc_2009/MKT_B32560_564.pdf
C Rect series Radial pin pitch 7.50mm  length 9mm width 3.8mm Capacitor
0
2
2
Capacitor_THT
C_Rect_L9.0mm_W3.9mm_P7.50mm_MKT
C, Rect series, Radial, pin pitch=7.50mm, , length*width=9*3.9mm^2, Capacitor, https://en.tdk.eu/inf/20/20/db/fc_2009/MKT_B32560_564.pdf
C Rect series Radial pin pitch 7.50mm  length 9mm width 3.9mm Capacitor
0
2
2
Capacitor_THT
C_Rect_L9.0mm_W4.0mm_P7.50mm_MKT
C, Rect series, Radial, pin pitch=7.50mm, , length*width=9*4.0mm^2, Capacitor, https://en.tdk.eu/inf/20/20/db/fc_2009/MKT_B32560_564.pdf
C Rect series Radial pin pitch 7.50mm  length 9mm width 4.0mm Capacitor
0
2
2
Capacitor_THT
C_Rect_L9.0mm_W4.2mm_P7.50mm_MKT
C, Rect series, Radial, pin pitch=7.50mm, , length*width=9*4.2mm^2, Capacitor, https://en.tdk.eu/inf/20/20/db/fc_2009/MKT_B32560_564.pdf
C Rect series Radial pin pitch 7.50mm  length 9mm width 4.2mm Capacitor
0
2
2
Capacitor_THT
C_Rect_L9.0mm_W4.9mm_P7.50mm_MKT
C, Rect series, Radial, pin pitch=7.50mm, , length*width=9*4.9mm^2, Capacitor, https://en.tdk.eu/inf/20/20/db/fc_2009/MKT_B32560_564.pdf
C Rect series Radial pin pitch 7.50mm  length 9mm width 4.9mm Capacitor
0
2
2
Capacitor_THT
C_Rect_L9.0mm_W5.1mm_P7.50mm_MKT
C, Rect series, Radial, pin pitch=7.50mm, , length*width=9*5.1mm^2, Capacitor, https://en.tdk.eu/inf/20/20/db/fc_2009/MKT_B32560_564.pdf
C Rect series Radial pin pitch 7.50mm  length 9mm width 5.1mm Capacitor
0
2
2
Capacitor_THT
C_Rect_L9.0mm_W5.7mm_P7.50mm_MKT
C, Rect series, Radial, pin pitch=7.50mm, , length*width=9*5.7mm^2, Capacitor, https://en.tdk.eu/inf/20/20/db/fc_2009/MKT_B32560_564.pdf
C Rect series Radial pin pitch 7.50mm  length 9mm width 5.7mm Capacitor
0
2
2
Capacitor_THT
C_Rect_L9.0mm_W6.4mm_P7.50mm_MKT
C, Rect series, Radial, pin pitch=7.50mm, , length*width=9*6.4mm^2, Capacitor, https://en.tdk.eu/inf/20/20/db/fc_2009/MKT_B32560_564.pdf
C Rect series Radial pin pitch 7.50mm  length 9mm width 6.4mm Capacitor
0
2
2
Capacitor_THT
C_Rect_L9.0mm_W6.7mm_P7.50mm_MKT
C, Rect series, Radial, pin pitch=7.50mm, , length*width=9*6.7mm^2, Capacitor, https://en.tdk.eu/inf/20/20/db/fc_2009/MKT_B32560_564.pdf
C Rect series Radial pin pitch 7.50mm  length 9mm width 6.7mm Capacitor
0
2
2
Capacitor_THT
C_Rect_L9.0mm_W7.7mm_P7.50mm_MKT
C, Rect series, Radial, pin pitch=7.50mm, , length*width=9*7.7mm^2, Capacitor, https://en.tdk.eu/inf/20/20/db/fc_2009/MKT_B32560_564.pdf
C Rect series Radial pin pitch 7.50mm  length 9mm width 7.7mm Capacitor
0
2
2
Capacitor_THT
C_Rect_L9.0mm_W8.5mm_P7.50mm_MKT
C, Rect series, Radial, pin pitch=7.50mm, , length*width=9*8.5mm^2, Capacitor, https://en.tdk.eu/inf/20/20/db/fc_2009/MKT_B32560_564.pdf
C Rect series Radial pin pitch 7.50mm  length 9mm width 8.5mm Capacitor
0
2
2
Capacitor_THT
C_Rect_L9.0mm_W9.5mm_P7.50mm_MKT
C, Rect series, Radial, pin pitch=7.50mm, , length*width=9*9.5mm^2, Capacitor, https://en.tdk.eu/inf/20/20/db/fc_2009/MKT_B32560_564.pdf
C Rect series Radial pin pitch 7.50mm  length 9mm width 9.5mm Capacitor
0
2
2
Capacitor_THT
C_Rect_L9.0mm_W9.8mm_P7.50mm_MKT
C, Rect series, Radial, pin pitch=7.50mm, , length*width=9*9.8mm^2, Capacitor, https://en.tdk.eu/inf/20/20/db/fc_2009/MKT_B32560_564.pdf
C Rect series Radial pin pitch 7.50mm  length 9mm width 9.8mm Capacitor
0
2
2
Capacitor_THT
C_Rect_L10.0mm_W2.5mm_P7.50mm_MKS4
C, Rect series, Radial, pin pitch=7.50mm, , length*width=10*2.5mm^2, Capacitor, http://www.wima.com/EN/WIMA_MKS_4.pdf
C Rect series Radial pin pitch 7.50mm  length 10mm width 2.5mm Capacitor
0
2
2
Capacitor_THT
C_Rect_L10.0mm_W3.0mm_P7.50mm_FKS3_FKP3
C, Rect series, Radial, pin pitch=7.50mm, , length*width=10*3mm^2, Capacitor, http://www.wima.com/EN/WIMA_FKS_3.pdf
C Rect series Radial pin pitch 7.50mm  length 10mm width 3mm Capacitor
0
2
2
Capacitor_THT
C_Rect_L10.0mm_W3.0mm_P7.50mm_MKS4
C, Rect series, Radial, pin pitch=7.50mm, , length*width=10*3.0mm^2, Capacitor, http://www.wima.com/EN/WIMA_MKS_4.pdf
C Rect series Radial pin pitch 7.50mm  length 10mm width 3.0mm Capacitor
0
2
2
Capacitor_THT
C_Rect_L10.0mm_W4.0mm_P7.50mm_FKS3_FKP3
C, Rect series, Radial, pin pitch=7.50mm, , length*width=10*4mm^2, Capacitor, http://www.wima.com/EN/WIMA_FKS_3.pdf
C Rect series Radial pin pitch 7.50mm  length 10mm width 4mm Capacitor
0
2
2
Capacitor_THT
C_Rect_L10.0mm_W4.0mm_P7.50mm_MKS4
C, Rect series, Radial, pin pitch=7.50mm, , length*width=10*4.0mm^2, Capacitor, http://www.wima.com/EN/WIMA_MKS_4.pdf
C Rect series Radial pin pitch 7.50mm  length 10mm width 4.0mm Capacitor
0
2
2
Capacitor_THT
C_Rect_L10.0mm_W5.0mm_P5.00mm_P7.50mm
C, Rect series, Radial, pin pitch=5.00mm 7.50mm, , length*width=10*5mm^2, Capacitor
C Rect series Radial pin pitch 5.00mm 7.50mm  length 10mm width 5mm Capacitor
0
4
2
Capacitor_THT
C_Rect_L10.3mm_W4.5mm_P7.50mm_MKS4
C, Rect series, Radial, pin pitch=7.50mm, , length*width=10.3*4.5mm^2, Capacitor, http://www.wima.com/EN/WIMA_MKS_4.pdf
C Rect series Radial pin pitch 7.50mm  length 10.3mm width 4.5mm Capacitor
0
2
2
Capacitor_THT
C_Rect_L10.3mm_W5.0mm_P7.50mm_MKS4
C, Rect series, Radial, pin pitch=7.50mm, , length*width=10.3*5mm^2, Capacitor, http://www.wima.com/EN/WIMA_MKS_4.pdf
C Rect series Radial pin pitch 7.50mm  length 10.3mm width 5mm Capacitor
0
2
2
Capacitor_THT
C_Rect_L10.3mm_W5.7mm_P7.50mm_MKS4
C, Rect series, Radial, pin pitch=7.50mm, , length*width=10.3*5.7mm^2, Capacitor, http://www.wima.com/EN/WIMA_MKS_4.pdf
C Rect series Radial pin pitch 7.50mm  length 10.3mm width 5.7mm Capacitor
0
2
2
Capacitor_THT
C_Rect_L10.3mm_W7.2mm_P7.50mm_MKS4
C, Rect series, Radial, pin pitch=7.50mm, , length*width=10.3*7.2mm^2, Capacitor, http://www.wima.com/EN/WIMA_MKS_4.pdf
C Rect series Radial pin pitch 7.50mm  length 10.3mm width 7.2mm Capacitor
0
2
2
Capacitor_THT
C_Rect_L11.0mm_W2.8mm_P10.00mm_MKT
C, Rect series, Radial, pin pitch=10.00mm, , length*width=11.0*2.8mm^2, Capacitor, https://en.tdk.eu/inf/20/20/db/fc_2009/MKT_B32560_564.pdf
C Rect series Radial pin pitch 10.00mm  length 11.0mm width 2.8mm Capacitor
0
2
2
Capacitor_THT
C_Rect_L11.0mm_W3.4mm_P10.00mm_MKT
C, Rect series, Radial, pin pitch=10.00mm, , length*width=11.0*3.4mm^2, Capacitor, https://en.tdk.eu/inf/20/20/db/fc_2009/MKT_B32560_564.pdf
C Rect series Radial pin pitch 10.00mm  length 11.0mm width 3.4mm Capacitor
0
2
2
Capacitor_THT
C_Rect_L11.0mm_W3.5mm_P10.00mm_MKT
C, Rect series, Radial, pin pitch=10.00mm, , length*width=11.0*3.5mm^2, Capacitor, https://en.tdk.eu/inf/20/20/db/fc_2009/MKT_B32560_564.pdf
C Rect series Radial pin pitch 10.00mm  length 11.0mm width 3.5mm Capacitor
0
2
2
Capacitor_THT
C_Rect_L11.0mm_W4.2mm_P10.00mm_MKT
C, Rect series, Radial, pin pitch=10.00mm, , length*width=11.0*4.2mm^2, Capacitor, https://en.tdk.eu/inf/20/20/db/fc_2009/MKT_B32560_564.pdf
C Rect series Radial pin pitch 10.00mm  length 11.0mm width 4.2mm Capacitor
0
2
2
Capacitor_THT
C_Rect_L11.0mm_W4.3mm_P10.00mm_MKT
C, Rect series, Radial, pin pitch=10.00mm, , length*width=11.0*4.3mm^2, Capacitor, https://en.tdk.eu/inf/20/20/db/fc_2009/MKT_B32560_564.pdf
C Rect series Radial pin pitch 10.00mm  length 11.0mm width 4.3mm Capacitor
0
2
2
Capacitor_THT
C_Rect_L11.0mm_W5.1mm_P10.00mm_MKT
C, Rect series, Radial, pin pitch=10.00mm, , length*width=11.0*5.1mm^2, Capacitor, https://en.tdk.eu/inf/20/20/db/fc_2009/MKT_B32560_564.pdf
C Rect series Radial pin pitch 10.00mm  length 11.0mm width 5.1mm Capacitor
0
2
2
Capacitor_THT
C_Rect_L11.0mm_W5.3mm_P10.00mm_MKT
C, Rect series, Radial, pin pitch=10.00mm, , length*width=11.0*5.3mm^2, Capacitor, https://en.tdk.eu/inf/20/20/db/fc_2009/MKT_B32560_564.pdf
C Rect series Radial pin pitch 10.00mm  length 11.0mm width 5.3mm Capacitor
0
2
2
Capacitor_THT
C_Rect_L11.0mm_W6.3mm_P10.00mm_MKT
C, Rect series, Radial, pin pitch=10.00mm, , length*width=11.0*6.3mm^2, Capacitor, https://en.tdk.eu/inf/20/20/db/fc_2009/MKT_B32560_564.pdf
C Rect series Radial pin pitch 10.00mm  length 11.0mm width 6.3mm Capacitor
0
2
2
Capacitor_THT
C_Rect_L11.0mm_W6.4mm_P10.00mm_MKT
C, Rect series, Radial, pin pitch=10.00mm, , length*width=11.0*6.4mm^2, Capacitor, https://en.tdk.eu/inf/20/20/db/fc_2009/MKT_B32560_564.pdf
C Rect series Radial pin pitch 10.00mm  length 11.0mm width 6.4mm Capacitor
0
2
2
Capacitor_THT
C_Rect_L11.0mm_W7.3mm_P10.00mm_MKT
C, Rect series, Radial, pin pitch=10.00mm, , length*width=11.0*7.3mm^2, Capacitor, https://en.tdk.eu/inf/20/20/db/fc_2009/MKT_B32560_564.pdf
C Rect series Radial pin pitch 10.00mm  length 11.0mm width 7.3mm Capacitor
0
2
2
Capacitor_THT
C_Rect_L11.0mm_W8.8mm_P10.00mm_MKT
C, Rect series, Radial, pin pitch=10.00mm, , length*width=11.0*8.8mm^2, Capacitor, https://en.tdk.eu/inf/20/20/db/fc_2009/MKT_B32560_564.pdf
C Rect series Radial pin pitch 10.00mm  length 11.0mm width 8.8mm Capacitor
0
2
2
Capacitor_THT
C_Rect_L11.5mm_W2.0mm_P10.00mm_MKT
C, Rect series, Radial, pin pitch=10.00mm, , length*width=11.5*2mm^2, Capacitor, https://en.tdk.eu/inf/20/20/db/fc_2009/MKT_B32560_564.pdf
C Rect series Radial pin pitch 10.00mm  length 11.5mm width 2mm Capacitor
0
2
2
Capacitor_THT
C_Rect_L11.5mm_W2.6mm_P10.00mm_MKT
C, Rect series, Radial, pin pitch=10.00mm, , length*width=11.5*2.6mm^2, Capacitor, https://en.tdk.eu/inf/20/20/db/fc_2009/MKT_B32560_564.pdf
C Rect series Radial pin pitch 10.00mm  length 11.5mm width 2.6mm Capacitor
0
2
2
Capacitor_THT
C_Rect_L11.5mm_W2.8mm_P10.00mm_MKT
C, Rect series, Radial, pin pitch=10.00mm, , length*width=11.5*2.8mm^2, Capacitor, https://en.tdk.eu/inf/20/20/db/fc_2009/MKT_B32560_564.pdf
C Rect series Radial pin pitch 10.00mm  length 11.5mm width 2.8mm Capacitor
0
2
2
Capacitor_THT
C_Rect_L11.5mm_W3.2mm_P10.00mm_MKT
C, Rect series, Radial, pin pitch=10.00mm, , length*width=11.5*3.2mm^2, Capacitor, https://en.tdk.eu/inf/20/20/db/fc_2009/MKT_B32560_564.pdf
C Rect series Radial pin pitch 10.00mm  length 11.5mm width 3.2mm Capacitor
0
2
2
Capacitor_THT
C_Rect_L11.5mm_W3.5mm_P10.00mm_MKT
C, Rect series, Radial, pin pitch=10.00mm, , length*width=11.5*3.5mm^2, Capacitor, https://en.tdk.eu/inf/20/20/db/fc_2009/MKT_B32560_564.pdf
C Rect series Radial pin pitch 10.00mm  length 11.5mm width 3.5mm Capacitor
0
2
2
Capacitor_THT
C_Rect_L11.5mm_W3.6mm_P10.00mm_MKT
C, Rect series, Radial, pin pitch=10.00mm, , length*width=11.5*3.6mm^2, Capacitor, https://en.tdk.eu/inf/20/20/db/fc_2009/MKT_B32560_564.pdf
C Rect series Radial pin pitch 10.00mm  length 11.5mm width 3.6mm Capacitor
0
2
2
Capacitor_THT
C_Rect_L11.5mm_W4.0mm_P10.00mm_MKT
C, Rect series, Radial, pin pitch=10.00mm, , length*width=11.5*4.0mm^2, Capacitor, https://en.tdk.eu/inf/20/20/db/fc_2009/MKT_B32560_564.pdf
C Rect series Radial pin pitch 10.00mm  length 11.5mm width 4.0mm Capacitor
0
2
2
Capacitor_THT
C_Rect_L11.5mm_W4.3mm_P10.00mm_MKT
C, Rect series, Radial, pin pitch=10.00mm, , length*width=11.5*4.3mm^2, Capacitor, https://en.tdk.eu/inf/20/20/db/fc_2009/MKT_B32560_564.pdf
C Rect series Radial pin pitch 10.00mm  length 11.5mm width 4.3mm Capacitor
0
2
2
Capacitor_THT
C_Rect_L11.5mm_W4.5mm_P10.00mm_MKT
C, Rect series, Radial, pin pitch=10.00mm, , length*width=11.5*4.5mm^2, Capacitor, https://en.tdk.eu/inf/20/20/db/fc_2009/MKT_B32560_564.pdf
C Rect series Radial pin pitch 10.00mm  length 11.5mm width 4.5mm Capacitor
0
2
2
Capacitor_THT
C_Rect_L11.5mm_W5.0mm_P10.00mm_MKT
C, Rect series, Radial, pin pitch=10.00mm, , length*width=11.5*5mm^2, Capacitor, https://en.tdk.eu/inf/20/20/db/fc_2009/MKT_B32560_564.pdf
C Rect series Radial pin pitch 10.00mm  length 11.5mm width 5mm Capacitor
0
2
2
Capacitor_THT
C_Rect_L11.5mm_W5.1mm_P10.00mm_MKT
C, Rect series, Radial, pin pitch=10.00mm, , length*width=11.5*5.1mm^2, Capacitor, https://en.tdk.eu/inf/20/20/db/fc_2009/MKT_B32560_564.pdf
C Rect series Radial pin pitch 10.00mm  length 11.5mm width 5.1mm Capacitor
0
2
2
Capacitor_THT
C_Rect_L11.5mm_W5.2mm_P10.00mm_MKT
C, Rect series, Radial, pin pitch=10.00mm, , length*width=11.5*5.2mm^2, Capacitor, https://en.tdk.eu/inf/20/20/db/fc_2009/MKT_B32560_564.pdf
C Rect series Radial pin pitch 10.00mm  length 11.5mm width 5.2mm Capacitor
0
2
2
Capacitor_THT
C_Rect_L11.5mm_W5.6mm_P10.00mm_MKT
C, Rect series, Radial, pin pitch=10.00mm, , length*width=11.5*5.6mm^2, Capacitor, https://en.tdk.eu/inf/20/20/db/fc_2009/MKT_B32560_564.pdf
C Rect series Radial pin pitch 10.00mm  length 11.5mm width 5.6mm Capacitor
0
2
2
Capacitor_THT
C_Rect_L11.5mm_W6.4mm_P10.00mm_MKT
C, Rect series, Radial, pin pitch=10.00mm, , length*width=11.5*6.4mm^2, Capacitor, https://en.tdk.eu/inf/20/20/db/fc_2009/MKT_B32560_564.pdf
C Rect series Radial pin pitch 10.00mm  length 11.5mm width 6.4mm Capacitor
0
2
2
Capacitor_THT
C_Rect_L11.5mm_W6.6mm_P10.00mm_MKT
C, Rect series, Radial, pin pitch=10.00mm, , length*width=11.5*6.6mm^2, Capacitor, https://en.tdk.eu/inf/20/20/db/fc_2009/MKT_B32560_564.pdf
C Rect series Radial pin pitch 10.00mm  length 11.5mm width 6.6mm Capacitor
0
2
2
Capacitor_THT
C_Rect_L11.5mm_W6.9mm_P10.00mm_MKT
C, Rect series, Radial, pin pitch=10.00mm, , length*width=11.5*6.9mm^2, Capacitor, https://en.tdk.eu/inf/20/20/db/fc_2009/MKT_B32560_564.pdf
C Rect series Radial pin pitch 10.00mm  length 11.5mm width 6.9mm Capacitor
0
2
2
Capacitor_THT
C_Rect_L11.5mm_W7.3mm_P10.00mm_MKT
C, Rect series, Radial, pin pitch=10.00mm, , length*width=11.5*7.3mm^2, Capacitor, https://en.tdk.eu/inf/20/20/db/fc_2009/MKT_B32560_564.pdf
C Rect series Radial pin pitch 10.00mm  length 11.5mm width 7.3mm Capacitor
0
2
2
Capacitor_THT
C_Rect_L11.5mm_W7.5mm_P10.00mm_MKT
C, Rect series, Radial, pin pitch=10.00mm, , length*width=11.5*7.5mm^2, Capacitor, https://en.tdk.eu/inf/20/20/db/fc_2009/MKT_B32560_564.pdf
C Rect series Radial pin pitch 10.00mm  length 11.5mm width 7.5mm Capacitor
0
2
2
Capacitor_THT
C_Rect_L11.5mm_W7.8mm_P10.00mm_MKT
C, Rect series, Radial, pin pitch=10.00mm, , length*width=11.5*7.8mm^2, Capacitor, https://en.tdk.eu/inf/20/20/db/fc_2009/MKT_B32560_564.pdf
C Rect series Radial pin pitch 10.00mm  length 11.5mm width 7.8mm Capacitor
0
2
2
Capacitor_THT
C_Rect_L11.5mm_W8.0mm_P10.00mm_MKT
C, Rect series, Radial, pin pitch=10.00mm, , length*width=11.5*8.0mm^2, Capacitor, https://en.tdk.eu/inf/20/20/db/fc_2009/MKT_B32560_564.pdf
C Rect series Radial pin pitch 10.00mm  length 11.5mm width 8.0mm Capacitor
0
2
2
Capacitor_THT
C_Rect_L11.5mm_W8.8mm_P10.00mm_MKT
C, Rect series, Radial, pin pitch=10.00mm, , length*width=11.5*8.8mm^2, Capacitor, https://en.tdk.eu/inf/20/20/db/fc_2009/MKT_B32560_564.pdf
C Rect series Radial pin pitch 10.00mm  length 11.5mm width 8.8mm Capacitor
0
2
2
Capacitor_THT
C_Rect_L11.5mm_W9.5mm_P10.00mm_MKT
C, Rect series, Radial, pin pitch=10.00mm, , length*width=11.5*9.5mm^2, Capacitor, https://en.tdk.eu/inf/20/20/db/fc_2009/MKT_B32560_564.pdf
C Rect series Radial pin pitch 10.00mm  length 11.5mm width 9.5mm Capacitor
0
2
2
Capacitor_THT
C_Rect_L11.5mm_W9.8mm_P10.00mm_MKT
C, Rect series, Radial, pin pitch=10.00mm, , length*width=11.5*9.8mm^2, Capacitor, https://en.tdk.eu/inf/20/20/db/fc_2009/MKT_B32560_564.pdf
C Rect series Radial pin pitch 10.00mm  length 11.5mm width 9.8mm Capacitor
0
2
2
Capacitor_THT
C_Rect_L13.0mm_W3.0mm_P10.00mm_FKS3_FKP3_MKS4
C, Rect series, Radial, pin pitch=10.00mm, , length*width=13*3mm^2, Capacitor, http://www.wima.com/EN/WIMA_FKS_3.pdf, http://www.wima.com/EN/WIMA_MKS_4.pdf
C Rect series Radial pin pitch 10.00mm  length 13mm width 3mm Capacitor
0
2
2
Capacitor_THT
C_Rect_L13.0mm_W4.0mm_P10.00mm_FKS3_FKP3_MKS4
C, Rect series, Radial, pin pitch=10.00mm, , length*width=13*4mm^2, Capacitor, http://www.wima.com/EN/WIMA_FKS_3.pdf, http://www.wima.com/EN/WIMA_MKS_4.pdf
C Rect series Radial pin pitch 10.00mm  length 13mm width 4mm Capacitor
0
2
2
Capacitor_THT
C_Rect_L13.0mm_W5.0mm_P10.00mm_FKS3_FKP3_MKS4
C, Rect series, Radial, pin pitch=10.00mm, , length*width=13*5mm^2, Capacitor, http://www.wima.com/EN/WIMA_FKS_3.pdf, http://www.wima.com/EN/WIMA_MKS_4.pdf
C Rect series Radial pin pitch 10.00mm  length 13mm width 5mm Capacitor
0
2
2
Capacitor_THT
C_Rect_L13.0mm_W6.0mm_P10.00mm_FKS3_FKP3_MKS4
C, Rect series, Radial, pin pitch=10.00mm, , length*width=13*6mm^2, Capacitor, http://www.wima.com/EN/WIMA_FKS_3.pdf, http://www.wima.com/EN/WIMA_MKS_4.pdf
C Rect series Radial pin pitch 10.00mm  length 13mm width 6mm Capacitor
0
2
2
Capacitor_THT
C_Rect_L13.0mm_W6.5mm_P7.50mm_P10.00mm
C, Rect series, Radial, pin pitch=7.50mm 10.00mm, , length*width=13*6.5mm^2, Capacitor
C Rect series Radial pin pitch 7.50mm 10.00mm  length 13mm width 6.5mm Capacitor
0
4
2
Capacitor_THT
C_Rect_L13.0mm_W8.0mm_P10.00mm_FKS3_FKP3_MKS4
C, Rect series, Radial, pin pitch=10.00mm, , length*width=13*8mm^2, Capacitor, http://www.wima.com/EN/WIMA_FKS_3.pdf, http://www.wima.com/EN/WIMA_MKS_4.pdf
C Rect series Radial pin pitch 10.00mm  length 13mm width 8mm Capacitor
0
2
2
Capacitor_THT
C_Rect_L13.5mm_W4.0mm_P10.00mm_FKS3_FKP3_MKS4
C, Rect series, Radial, pin pitch=10.00mm, , length*width=13.5*4mm^2, Capacitor, http://www.wima.com/EN/WIMA_FKS_3.pdf, http://www.wima.com/EN/WIMA_MKS_4.pdf
C Rect series Radial pin pitch 10.00mm  length 13.5mm width 4mm Capacitor
0
2
2
Capacitor_THT
C_Rect_L13.5mm_W5.0mm_P10.00mm_FKS3_FKP3_MKS4
C, Rect series, Radial, pin pitch=10.00mm, , length*width=13.5*5mm^2, Capacitor, http://www.wima.com/EN/WIMA_FKS_3.pdf, http://www.wima.com/EN/WIMA_MKS_4.pdf
C Rect series Radial pin pitch 10.00mm  length 13.5mm width 5mm Capacitor
0
2
2
Capacitor_THT
C_Rect_L16.5mm_W4.7mm_P15.00mm_MKT
C, Rect series, Radial, pin pitch=15.00mm, , length*width=16.5*4.7mm^2, Capacitor, https://en.tdk.eu/inf/20/20/db/fc_2009/MKT_B32560_564.pdf
C Rect series Radial pin pitch 15.00mm  length 16.5mm width 4.7mm Capacitor
0
2
2
Capacitor_THT
C_Rect_L16.5mm_W4.9mm_P15.00mm_MKT
C, Rect series, Radial, pin pitch=15.00mm, , length*width=16.5*4.9mm^2, Capacitor, https://en.tdk.eu/inf/20/20/db/fc_2009/MKT_B32560_564.pdf
C Rect series Radial pin pitch 15.00mm  length 16.5mm width 4.9mm Capacitor
0
2
2
Capacitor_THT
C_Rect_L16.5mm_W5.0mm_P15.00mm_MKT
C, Rect series, Radial, pin pitch=15.00mm, , length*width=16.5*5mm^2, Capacitor, https://en.tdk.eu/inf/20/20/db/fc_2009/MKT_B32560_564.pdf
C Rect series Radial pin pitch 15.00mm  length 16.5mm width 5mm Capacitor
0
2
2
Capacitor_THT
C_Rect_L16.5mm_W6.0mm_P15.00mm_MKT
C, Rect series, Radial, pin pitch=15.00mm, , length*width=16.5*6mm^2, Capacitor, https://en.tdk.eu/inf/20/20/db/fc_2009/MKT_B32560_564.pdf
C Rect series Radial pin pitch 15.00mm  length 16.5mm width 6mm Capacitor
0
2
2
Capacitor_THT
C_Rect_L16.5mm_W7.0mm_P15.00mm_MKT
C, Rect series, Radial, pin pitch=15.00mm, , length*width=16.5*7mm^2, Capacitor, https://en.tdk.eu/inf/20/20/db/fc_2009/MKT_B32560_564.pdf
C Rect series Radial pin pitch 15.00mm  length 16.5mm width 7mm Capacitor
0
2
2
Capacitor_THT
C_Rect_L16.5mm_W7.3mm_P15.00mm_MKT
C, Rect series, Radial, pin pitch=15.00mm, , length*width=16.5*7.3mm^2, Capacitor, https://en.tdk.eu/inf/20/20/db/fc_2009/MKT_B32560_564.pdf
C Rect series Radial pin pitch 15.00mm  length 16.5mm width 7.3mm Capacitor
0
2
2
Capacitor_THT
C_Rect_L16.5mm_W8.7mm_P15.00mm_MKT
C, Rect series, Radial, pin pitch=15.00mm, , length*width=16.5*8.7mm^2, Capacitor, https://en.tdk.eu/inf/20/20/db/fc_2009/MKT_B32560_564.pdf
C Rect series Radial pin pitch 15.00mm  length 16.5mm width 8.7mm Capacitor
0
2
2
Capacitor_THT
C_Rect_L16.5mm_W8.9mm_P15.00mm_MKT
C, Rect series, Radial, pin pitch=15.00mm, , length*width=16.5*8.9mm^2, Capacitor, https://en.tdk.eu/inf/20/20/db/fc_2009/MKT_B32560_564.pdf
C Rect series Radial pin pitch 15.00mm  length 16.5mm width 8.9mm Capacitor
0
2
2
Capacitor_THT
C_Rect_L16.5mm_W9.0mm_P15.00mm_MKT
C, Rect series, Radial, pin pitch=15.00mm, , length*width=16.5*9mm^2, Capacitor, https://en.tdk.eu/inf/20/20/db/fc_2009/MKT_B32560_564.pdf
C Rect series Radial pin pitch 15.00mm  length 16.5mm width 9mm Capacitor
0
2
2
Capacitor_THT
C_Rect_L16.5mm_W9.2mm_P15.00mm_MKT
C, Rect series, Radial, pin pitch=15.00mm, , length*width=16.5*9.2mm^2, Capacitor, https://en.tdk.eu/inf/20/20/db/fc_2009/MKT_B32560_564.pdf
C Rect series Radial pin pitch 15.00mm  length 16.5mm width 9.2mm Capacitor
0
2
2
Capacitor_THT
C_Rect_L16.5mm_W10.7mm_P15.00mm_MKT
C, Rect series, Radial, pin pitch=15.00mm, , length*width=16.5*10.7mm^2, Capacitor, https://en.tdk.eu/inf/20/20/db/fc_2009/MKT_B32560_564.pdf
C Rect series Radial pin pitch 15.00mm  length 16.5mm width 10.7mm Capacitor
0
2
2
Capacitor_THT
C_Rect_L16.5mm_W10.9mm_P15.00mm_MKT
C, Rect series, Radial, pin pitch=15.00mm, , length*width=16.5*10.9mm^2, Capacitor, https://en.tdk.eu/inf/20/20/db/fc_2009/MKT_B32560_564.pdf
C Rect series Radial pin pitch 15.00mm  length 16.5mm width 10.9mm Capacitor
0
2
2
Capacitor_THT
C_Rect_L16.5mm_W11.2mm_P15.00mm_MKT
C, Rect series, Radial, pin pitch=15.00mm, , length*width=16.5*11.2mm^2, Capacitor, https://en.tdk.eu/inf/20/20/db/fc_2009/MKT_B32560_564.pdf
C Rect series Radial pin pitch 15.00mm  length 16.5mm width 11.2mm Capacitor
0
2
2
Capacitor_THT
C_Rect_L16.5mm_W11.8mm_P15.00mm_MKT
C, Rect series, Radial, pin pitch=15.00mm, , length*width=16.5*11.8mm^2, Capacitor, https://en.tdk.eu/inf/20/20/db/fc_2009/MKT_B32560_564.pdf
C Rect series Radial pin pitch 15.00mm  length 16.5mm width 11.8mm Capacitor
0
2
2
Capacitor_THT
C_Rect_L16.5mm_W13.5mm_P15.00mm_MKT
C, Rect series, Radial, pin pitch=15.00mm, , length*width=16.5*13.5mm^2, Capacitor, https://en.tdk.eu/inf/20/20/db/fc_2009/MKT_B32560_564.pdf
C Rect series Radial pin pitch 15.00mm  length 16.5mm width 13.5mm Capacitor
0
2
2
Capacitor_THT
C_Rect_L16.5mm_W13.7mm_P15.00mm_MKT
C, Rect series, Radial, pin pitch=15.00mm, , length*width=16.5*13.7mm^2, Capacitor, https://en.tdk.eu/inf/20/20/db/fc_2009/MKT_B32560_564.pdf
C Rect series Radial pin pitch 15.00mm  length 16.5mm width 13.7mm Capacitor
0
2
2
Capacitor_THT
C_Rect_L16.5mm_W13.9mm_P15.00mm_MKT
C, Rect series, Radial, pin pitch=15.00mm, , length*width=16.5*13.9mm^2, Capacitor, https://en.tdk.eu/inf/20/20/db/fc_2009/MKT_B32560_564.pdf
C Rect series Radial pin pitch 15.00mm  length 16.5mm width 13.9mm Capacitor
0
2
2
Capacitor_THT
C_Rect_L18.0mm_W5.0mm_P15.00mm_FKS3_FKP3
C, Rect series, Radial, pin pitch=15.00mm, , length*width=18*5mm^2, Capacitor, http://www.wima.com/EN/WIMA_FKS_3.pdf
C Rect series Radial pin pitch 15.00mm  length 18mm width 5mm Capacitor
0
2
2
Capacitor_THT
C_Rect_L18.0mm_W6.0mm_P15.00mm_FKS3_FKP3
C, Rect series, Radial, pin pitch=15.00mm, , length*width=18*6mm^2, Capacitor, http://www.wima.com/EN/WIMA_FKS_3.pdf
C Rect series Radial pin pitch 15.00mm  length 18mm width 6mm Capacitor
0
2
2
Capacitor_THT
C_Rect_L18.0mm_W7.0mm_P15.00mm_FKS3_FKP3
C, Rect series, Radial, pin pitch=15.00mm, , length*width=18*7mm^2, Capacitor, http://www.wima.com/EN/WIMA_FKS_3.pdf
C Rect series Radial pin pitch 15.00mm  length 18mm width 7mm Capacitor
0
2
2
Capacitor_THT
C_Rect_L18.0mm_W8.0mm_P15.00mm_FKS3_FKP3
C, Rect series, Radial, pin pitch=15.00mm, , length*width=18*8mm^2, Capacitor, http://www.wima.com/EN/WIMA_FKS_3.pdf
C Rect series Radial pin pitch 15.00mm  length 18mm width 8mm Capacitor
0
2
2
Capacitor_THT
C_Rect_L18.0mm_W9.0mm_P15.00mm_FKS3_FKP3
C, Rect series, Radial, pin pitch=15.00mm, , length*width=18*9mm^2, Capacitor, http://www.wima.com/EN/WIMA_FKS_3.pdf
C Rect series Radial pin pitch 15.00mm  length 18mm width 9mm Capacitor
0
2
2
Capacitor_THT
C_Rect_L18.0mm_W11.0mm_P15.00mm_FKS3_FKP3
C, Rect series, Radial, pin pitch=15.00mm, , length*width=18*11mm^2, Capacitor, http://www.wima.com/EN/WIMA_FKS_3.pdf
C Rect series Radial pin pitch 15.00mm  length 18mm width 11mm Capacitor
0
2
2
Capacitor_THT
C_Rect_L19.0mm_W5.0mm_P15.00mm_MKS4
C, Rect series, Radial, pin pitch=15.00mm, , length*width=19*5mm^2, Capacitor, http://www.wima.com/EN/WIMA_MKS_4.pdf
C Rect series Radial pin pitch 15.00mm  length 19mm width 5mm Capacitor
0
2
2
Capacitor_THT
C_Rect_L19.0mm_W6.0mm_P15.00mm_MKS4
C, Rect series, Radial, pin pitch=15.00mm, , length*width=19*6mm^2, Capacitor, http://www.wima.com/EN/WIMA_MKS_4.pdf
C Rect series Radial pin pitch 15.00mm  length 19mm width 6mm Capacitor
0
2
2
Capacitor_THT
C_Rect_L19.0mm_W7.0mm_P15.00mm_MKS4
C, Rect series, Radial, pin pitch=15.00mm, , length*width=19*7mm^2, Capacitor, http://www.wima.com/EN/WIMA_MKS_4.pdf
C Rect series Radial pin pitch 15.00mm  length 19mm width 7mm Capacitor
0
2
2
Capacitor_THT
C_Rect_L19.0mm_W8.0mm_P15.00mm_MKS4
C, Rect series, Radial, pin pitch=15.00mm, , length*width=19*8mm^2, Capacitor, http://www.wima.com/EN/WIMA_MKS_4.pdf
C Rect series Radial pin pitch 15.00mm  length 19mm width 8mm Capacitor
0
2
2
Capacitor_THT
C_Rect_L19.0mm_W9.0mm_P15.00mm_MKS4
C, Rect series, Radial, pin pitch=15.00mm, , length*width=19*9mm^2, Capacitor, http://www.wima.com/EN/WIMA_MKS_4.pdf
C Rect series Radial pin pitch 15.00mm  length 19mm width 9mm Capacitor
0
2
2
Capacitor_THT
C_Rect_L19.0mm_W11.0mm_P15.00mm_MKS4
C, Rect series, Radial, pin pitch=15.00mm, , length*width=19*11mm^2, Capacitor, http://www.wima.com/EN/WIMA_MKS_4.pdf
C Rect series Radial pin pitch 15.00mm  length 19mm width 11mm Capacitor
0
2
2
Capacitor_THT
C_Rect_L24.0mm_W7.0mm_P22.50mm_MKT
C, Rect series, Radial, pin pitch=22.50mm, , length*width=24*7mm^2, Capacitor, https://en.tdk.eu/inf/20/20/db/fc_2009/MKT_B32560_564.pdf
C Rect series Radial pin pitch 22.50mm  length 24mm width 7mm Capacitor
0
2
2
Capacitor_THT
C_Rect_L24.0mm_W8.3mm_P22.50mm_MKT
C, Rect series, Radial, pin pitch=22.50mm, , length*width=24*8.3mm^2, Capacitor, https://en.tdk.eu/inf/20/20/db/fc_2009/MKT_B32560_564.pdf
C Rect series Radial pin pitch 22.50mm  length 24mm width 8.3mm Capacitor
0
2
2
Capacitor_THT
C_Rect_L24.0mm_W8.6mm_P22.50mm_MKT
C, Rect series, Radial, pin pitch=22.50mm, , length*width=24*8.6mm^2, Capacitor, https://en.tdk.eu/inf/20/20/db/fc_2009/MKT_B32560_564.pdf
C Rect series Radial pin pitch 22.50mm  length 24mm width 8.6mm Capacitor
0
2
2
Capacitor_THT
C_Rect_L24.0mm_W10.1mm_P22.50mm_MKT
C, Rect series, Radial, pin pitch=22.50mm, , length*width=24*10.1mm^2, Capacitor, https://en.tdk.eu/inf/20/20/db/fc_2009/MKT_B32560_564.pdf
C Rect series Radial pin pitch 22.50mm  length 24mm width 10.1mm Capacitor
0
2
2
Capacitor_THT
C_Rect_L24.0mm_W10.3mm_P22.50mm_MKT
C, Rect series, Radial, pin pitch=22.50mm, , length*width=24*10.3mm^2, Capacitor, https://en.tdk.eu/inf/20/20/db/fc_2009/MKT_B32560_564.pdf
C Rect series Radial pin pitch 22.50mm  length 24mm width 10.3mm Capacitor
0
2
2
Capacitor_THT
C_Rect_L24.0mm_W10.9mm_P22.50mm_MKT
C, Rect series, Radial, pin pitch=22.50mm, , length*width=24*10.9mm^2, Capacitor, https://en.tdk.eu/inf/20/20/db/fc_2009/MKT_B32560_564.pdf
C Rect series Radial pin pitch 22.50mm  length 24mm width 10.9mm Capacitor
0
2
2
Capacitor_THT
C_Rect_L24.0mm_W12.2mm_P22.50mm_MKT
C, Rect series, Radial, pin pitch=22.50mm, , length*width=24*12.2mm^2, Capacitor, https://en.tdk.eu/inf/20/20/db/fc_2009/MKT_B32560_564.pdf
C Rect series Radial pin pitch 22.50mm  length 24mm width 12.2mm Capacitor
0
2
2
Capacitor_THT
C_Rect_L24.0mm_W12.6mm_P22.50mm_MKT
C, Rect series, Radial, pin pitch=22.50mm, , length*width=24*12.6mm^2, Capacitor, https://en.tdk.eu/inf/20/20/db/fc_2009/MKT_B32560_564.pdf
C Rect series Radial pin pitch 22.50mm  length 24mm width 12.6mm Capacitor
0
2
2
Capacitor_THT
C_Rect_L24.0mm_W12.8mm_P22.50mm_MKT
C, Rect series, Radial, pin pitch=22.50mm, , length*width=24*12.8mm^2, Capacitor, https://en.tdk.eu/inf/20/20/db/fc_2009/MKT_B32560_564.pdf
C Rect series Radial pin pitch 22.50mm  length 24mm width 12.8mm Capacitor
0
2
2
Capacitor_THT
C_Rect_L26.5mm_W5.0mm_P22.50mm_MKS4
C, Rect series, Radial, pin pitch=22.50mm, , length*width=26.5*5mm^2, Capacitor, http://www.wima.com/EN/WIMA_MKS_4.pdf
C Rect series Radial pin pitch 22.50mm  length 26.5mm width 5mm Capacitor
0
2
2
Capacitor_THT
C_Rect_L26.5mm_W6.0mm_P22.50mm_MKS4
C, Rect series, Radial, pin pitch=22.50mm, , length*width=26.5*6mm^2, Capacitor, http://www.wima.com/EN/WIMA_MKS_4.pdf
C Rect series Radial pin pitch 22.50mm  length 26.5mm width 6mm Capacitor
0
2
2
Capacitor_THT
C_Rect_L26.5mm_W7.0mm_P22.50mm_MKS4
C, Rect series, Radial, pin pitch=22.50mm, , length*width=26.5*7mm^2, Capacitor, http://www.wima.com/EN/WIMA_MKS_4.pdf
C Rect series Radial pin pitch 22.50mm  length 26.5mm width 7mm Capacitor
0
2
2
Capacitor_THT
C_Rect_L26.5mm_W8.5mm_P22.50mm_MKS4
C, Rect series, Radial, pin pitch=22.50mm, , length*width=26.5*8.5mm^2, Capacitor, http://www.wima.com/EN/WIMA_MKS_4.pdf
C Rect series Radial pin pitch 22.50mm  length 26.5mm width 8.5mm Capacitor
0
2
2
Capacitor_THT
C_Rect_L26.5mm_W10.5mm_P22.50mm_MKS4
C, Rect series, Radial, pin pitch=22.50mm, , length*width=26.5*10.5mm^2, Capacitor, http://www.wima.com/EN/WIMA_MKS_4.pdf
C Rect series Radial pin pitch 22.50mm  length 26.5mm width 10.5mm Capacitor
0
2
2
Capacitor_THT
C_Rect_L26.5mm_W11.5mm_P22.50mm_MKS4
C, Rect series, Radial, pin pitch=22.50mm, , length*width=26.5*11.5mm^2, Capacitor, http://www.wima.com/EN/WIMA_MKS_4.pdf
C Rect series Radial pin pitch 22.50mm  length 26.5mm width 11.5mm Capacitor
0
2
2
Capacitor_THT
C_Rect_L27.0mm_W9.0mm_P22.00mm
C, Rect series, Radial, pin pitch=22.00mm, , length*width=27*9mm^2, Capacitor
C Rect series Radial pin pitch 22.00mm  length 27mm width 9mm Capacitor
0
2
2
Capacitor_THT
C_Rect_L27.0mm_W9.0mm_P23.00mm
C, Rect series, Radial, pin pitch=23.00mm, , length*width=27*9mm^2, Capacitor
C Rect series Radial pin pitch 23.00mm  length 27mm width 9mm Capacitor
0
2
2
Capacitor_THT
C_Rect_L27.0mm_W11.0mm_P22.00mm
C, Rect series, Radial, pin pitch=22.00mm, , length*width=27*11mm^2, Capacitor
C Rect series Radial pin pitch 22.00mm  length 27mm width 11mm Capacitor
0
2
2
Capacitor_THT
C_Rect_L28.0mm_W8.0mm_P22.50mm_MKS4
C, Rect series, Radial, pin pitch=22.50mm, , length*width=28*8mm^2, Capacitor, http://www.wima.com/EN/WIMA_MKS_4.pdf
C Rect series Radial pin pitch 22.50mm  length 28mm width 8mm Capacitor
0
2
2
Capacitor_THT
C_Rect_L28.0mm_W10.0mm_P22.50mm_MKS4
C, Rect series, Radial, pin pitch=22.50mm, , length*width=28*10mm^2, Capacitor, http://www.wima.com/EN/WIMA_MKS_4.pdf
C Rect series Radial pin pitch 22.50mm  length 28mm width 10mm Capacitor
0
2
2
Capacitor_THT
C_Rect_L28.0mm_W12.0mm_P22.50mm_MKS4
C, Rect series, Radial, pin pitch=22.50mm, , length*width=28*12mm^2, Capacitor, http://www.wima.com/EN/WIMA_MKS_4.pdf
C Rect series Radial pin pitch 22.50mm  length 28mm width 12mm Capacitor
0
2
2
Capacitor_THT
C_Rect_L29.0mm_W7.6mm_P27.50mm_MKT
C, Rect series, Radial, pin pitch=27.50mm, , length*width=29*7.6mm^2, Capacitor, https://en.tdk.eu/inf/20/20/db/fc_2009/MKT_B32560_564.pdf
C Rect series Radial pin pitch 27.50mm  length 29mm width 7.6mm Capacitor
0
2
2
Capacitor_THT
C_Rect_L29.0mm_W7.8mm_P27.50mm_MKT
C, Rect series, Radial, pin pitch=27.50mm, , length*width=29*7.8mm^2, Capacitor, https://en.tdk.eu/inf/20/20/db/fc_2009/MKT_B32560_564.pdf
C Rect series Radial pin pitch 27.50mm  length 29mm width 7.8mm Capacitor
0
2
2
Capacitor_THT
C_Rect_L29.0mm_W7.9mm_P27.50mm_MKT
C, Rect series, Radial, pin pitch=27.50mm, , length*width=29*7.9mm^2, Capacitor, https://en.tdk.eu/inf/20/20/db/fc_2009/MKT_B32560_564.pdf
C Rect series Radial pin pitch 27.50mm  length 29mm width 7.9mm Capacitor
0
2
2
Capacitor_THT
C_Rect_L29.0mm_W9.1mm_P27.50mm_MKT
C, Rect series, Radial, pin pitch=27.50mm, , length*width=29*9.1mm^2, Capacitor, https://en.tdk.eu/inf/20/20/db/fc_2009/MKT_B32560_564.pdf
C Rect series Radial pin pitch 27.50mm  length 29mm width 9.1mm Capacitor
0
2
2
Capacitor_THT
C_Rect_L29.0mm_W9.6mm_P27.50mm_MKT
C, Rect series, Radial, pin pitch=27.50mm, , length*width=29*9.6mm^2, Capacitor, https://en.tdk.eu/inf/20/20/db/fc_2009/MKT_B32560_564.pdf
C Rect series Radial pin pitch 27.50mm  length 29mm width 9.6mm Capacitor
0
2
2
Capacitor_THT
C_Rect_L29.0mm_W11.0mm_P27.50mm_MKT
C, Rect series, Radial, pin pitch=27.50mm, , length*width=29*11mm^2, Capacitor, https://en.tdk.eu/inf/20/20/db/fc_2009/MKT_B32560_564.pdf
C Rect series Radial pin pitch 27.50mm  length 29mm width 11mm Capacitor
0
2
2
Capacitor_THT
C_Rect_L29.0mm_W11.9mm_P27.50mm_MKT
C, Rect series, Radial, pin pitch=27.50mm, , length*width=29*11.9mm^2, Capacitor, https://en.tdk.eu/inf/20/20/db/fc_2009/MKT_B32560_564.pdf
C Rect series Radial pin pitch 27.50mm  length 29mm width 11.9mm Capacitor
0
2
2
Capacitor_THT
C_Rect_L29.0mm_W12.2mm_P27.50mm_MKT
C, Rect series, Radial, pin pitch=27.50mm, , length*width=29*12.2mm^2, Capacitor, https://en.tdk.eu/inf/20/20/db/fc_2009/MKT_B32560_564.pdf
C Rect series Radial pin pitch 27.50mm  length 29mm width 12.2mm Capacitor
0
2
2
Capacitor_THT
C_Rect_L29.0mm_W13.0mm_P27.50mm_MKT
C, Rect series, Radial, pin pitch=27.50mm, , length*width=29*13mm^2, Capacitor, https://en.tdk.eu/inf/20/20/db/fc_2009/MKT_B32560_564.pdf
C Rect series Radial pin pitch 27.50mm  length 29mm width 13mm Capacitor
0
2
2
Capacitor_THT
C_Rect_L29.0mm_W13.8mm_P27.50mm_MKT
C, Rect series, Radial, pin pitch=27.50mm, , length*width=29*13.8mm^2, Capacitor, https://en.tdk.eu/inf/20/20/db/fc_2009/MKT_B32560_564.pdf
C Rect series Radial pin pitch 27.50mm  length 29mm width 13.8mm Capacitor
0
2
2
Capacitor_THT
C_Rect_L29.0mm_W14.2mm_P27.50mm_MKT
C, Rect series, Radial, pin pitch=27.50mm, , length*width=29*14.2mm^2, Capacitor, https://en.tdk.eu/inf/20/20/db/fc_2009/MKT_B32560_564.pdf
C Rect series Radial pin pitch 27.50mm  length 29mm width 14.2mm Capacitor
0
2
2
Capacitor_THT
C_Rect_L29.0mm_W16.0mm_P27.50mm_MKT
C, Rect series, Radial, pin pitch=27.50mm, , length*width=29*16mm^2, Capacitor, https://en.tdk.eu/inf/20/20/db/fc_2009/MKT_B32560_564.pdf
C Rect series Radial pin pitch 27.50mm  length 29mm width 16mm Capacitor
0
2
2
Capacitor_THT
C_Rect_L31.5mm_W9.0mm_P27.50mm_MKS4
C, Rect series, Radial, pin pitch=27.50mm, , length*width=31.5*9mm^2, Capacitor, http://www.wima.com/EN/WIMA_MKS_4.pdf
C Rect series Radial pin pitch 27.50mm  length 31.5mm width 9mm Capacitor
0
2
2
Capacitor_THT
C_Rect_L31.5mm_W11.0mm_P27.50mm_MKS4
C, Rect series, Radial, pin pitch=27.50mm, , length*width=31.5*11mm^2, Capacitor, http://www.wima.com/EN/WIMA_MKS_4.pdf
C Rect series Radial pin pitch 27.50mm  length 31.5mm width 11mm Capacitor
0
2
2
Capacitor_THT
C_Rect_L31.5mm_W13.0mm_P27.50mm_MKS4
C, Rect series, Radial, pin pitch=27.50mm, , length*width=31.5*13mm^2, Capacitor, http://www.wima.com/EN/WIMA_MKS_4.pdf
C Rect series Radial pin pitch 27.50mm  length 31.5mm width 13mm Capacitor
0
2
2
Capacitor_THT
C_Rect_L31.5mm_W15.0mm_P27.50mm_MKS4
C, Rect series, Radial, pin pitch=27.50mm, , length*width=31.5*15mm^2, Capacitor, http://www.wima.com/EN/WIMA_MKS_4.pdf
C Rect series Radial pin pitch 27.50mm  length 31.5mm width 15mm Capacitor
0
2
2
Capacitor_THT
C_Rect_L31.5mm_W17.0mm_P27.50mm_MKS4
C, Rect series, Radial, pin pitch=27.50mm, , length*width=31.5*17mm^2, Capacitor, http://www.wima.com/EN/WIMA_MKS_4.pdf
C Rect series Radial pin pitch 27.50mm  length 31.5mm width 17mm Capacitor
0
2
2
Capacitor_THT
C_Rect_L31.5mm_W20.0mm_P27.50mm_MKS4
C, Rect series, Radial, pin pitch=27.50mm, , length*width=31.5*20mm^2, Capacitor, http://www.wima.com/EN/WIMA_MKS_4.pdf
C Rect series Radial pin pitch 27.50mm  length 31.5mm width 20mm Capacitor
0
2
2
Capacitor_THT
C_Rect_L32.0mm_W15.0mm_P27.00mm
C, Rect series, Radial, pin pitch=27.00mm, , length*width=32*15mm^2, Capacitor
C Rect series Radial pin pitch 27.00mm  length 32mm width 15mm Capacitor
0
2
2
Capacitor_THT
C_Rect_L33.0mm_W13.0mm_P27.50mm_MKS4
C, Rect series, Radial, pin pitch=27.50mm, , length*width=33*13mm^2, Capacitor, http://www.wima.com/EN/WIMA_MKS_4.pdf
C Rect series Radial pin pitch 27.50mm  length 33mm width 13mm Capacitor
0
2
2
Capacitor_THT
C_Rect_L33.0mm_W15.0mm_P27.50mm_MKS4
C, Rect series, Radial, pin pitch=27.50mm, , length*width=33*15mm^2, Capacitor, http://www.wima.com/EN/WIMA_MKS_4.pdf
C Rect series Radial pin pitch 27.50mm  length 33mm width 15mm Capacitor
0
2
2
Capacitor_THT
C_Rect_L33.0mm_W20.0mm_P27.50mm_MKS4
C, Rect series, Radial, pin pitch=27.50mm, , length*width=33*20mm^2, Capacitor, http://www.wima.com/EN/WIMA_MKS_4.pdf
C Rect series Radial pin pitch 27.50mm  length 33mm width 20mm Capacitor
0
2
2
Capacitor_THT
C_Rect_L41.5mm_W9.0mm_P37.50mm_MKS4
C, Rect series, Radial, pin pitch=37.50mm, , length*width=41.5*9mm^2, Capacitor, http://www.wima.com/EN/WIMA_MKS_4.pdf
C Rect series Radial pin pitch 37.50mm  length 41.5mm width 9mm Capacitor
0
2
2
Capacitor_THT
C_Rect_L41.5mm_W11.0mm_P37.50mm_MKS4
C, Rect series, Radial, pin pitch=37.50mm, , length*width=41.5*11mm^2, Capacitor, http://www.wima.com/EN/WIMA_MKS_4.pdf
C Rect series Radial pin pitch 37.50mm  length 41.5mm width 11mm Capacitor
0
2
2
Capacitor_THT
C_Rect_L41.5mm_W13.0mm_P37.50mm_MKS4
C, Rect series, Radial, pin pitch=37.50mm, , length*width=41.5*13mm^2, Capacitor, http://www.wima.com/EN/WIMA_MKS_4.pdf
C Rect series Radial pin pitch 37.50mm  length 41.5mm width 13mm Capacitor
0
2
2
Capacitor_THT
C_Rect_L41.5mm_W15.0mm_P37.50mm_MKS4
C, Rect series, Radial, pin pitch=37.50mm, , length*width=41.5*15mm^2, Capacitor, http://www.wima.com/EN/WIMA_MKS_4.pdf
C Rect series Radial pin pitch 37.50mm  length 41.5mm width 15mm Capacitor
0
2
2
Capacitor_THT
C_Rect_L41.5mm_W17.0mm_P37.50mm_MKS4
C, Rect series, Radial, pin pitch=37.50mm, , length*width=41.5*17mm^2, Capacitor, http://www.wima.com/EN/WIMA_MKS_4.pdf
C Rect series Radial pin pitch 37.50mm  length 41.5mm width 17mm Capacitor
0
2
2
Capacitor_THT
C_Rect_L41.5mm_W19.0mm_P37.50mm_MKS4
C, Rect series, Radial, pin pitch=37.50mm, , length*width=41.5*19mm^2, Capacitor, http://www.wima.com/EN/WIMA_MKS_4.pdf
C Rect series Radial pin pitch 37.50mm  length 41.5mm width 19mm Capacitor
0
2
2
Capacitor_THT
C_Rect_L41.5mm_W20.0mm_P37.50mm_MKS4
C, Rect series, Radial, pin pitch=37.50mm, , length*width=41.5*20mm^2, Capacitor, http://www.wima.com/EN/WIMA_MKS_4.pdf
C Rect series Radial pin pitch 37.50mm  length 41.5mm width 20mm Capacitor
0
2
2
Capacitor_THT
C_Rect_L41.5mm_W24.0mm_P37.50mm_MKS4
C, Rect series, Radial, pin pitch=37.50mm, , length*width=41.5*24mm^2, Capacitor, http://www.wima.com/EN/WIMA_MKS_4.pdf
C Rect series Radial pin pitch 37.50mm  length 41.5mm width 24mm Capacitor
0
2
2
Capacitor_THT
C_Rect_L41.5mm_W31.0mm_P37.50mm_MKS4
C, Rect series, Radial, pin pitch=37.50mm, , length*width=41.5*31mm^2, Capacitor, http://www.wima.com/EN/WIMA_MKS_4.pdf
C Rect series Radial pin pitch 37.50mm  length 41.5mm width 31mm Capacitor
0
2
2
Capacitor_THT
C_Rect_L41.5mm_W35.0mm_P37.50mm_MKS4
C, Rect series, Radial, pin pitch=37.50mm, , length*width=41.5*35mm^2, Capacitor, http://www.wima.com/EN/WIMA_MKS_4.pdf
C Rect series Radial pin pitch 37.50mm  length 41.5mm width 35mm Capacitor
0
2
2
Capacitor_THT
C_Rect_L41.5mm_W40.0mm_P37.50mm_MKS4
C, Rect series, Radial, pin pitch=37.50mm, , length*width=41.5*40mm^2, Capacitor, http://www.wima.com/EN/WIMA_MKS_4.pdf
C Rect series Radial pin pitch 37.50mm  length 41.5mm width 40mm Capacitor
0
2
2
Capacitor_THT
DX_5R5HxxxxU_D11.5mm_P10.00mm
CP, Radial series, Radial, pin pitch=10.00mm, diameter=11.5mm, Supercapacitor, http://www.elna.co.jp/en/capacitor/double_layer/catalog/pdf/dx_e.pdf
CP Radial series Radial pin pitch 10.00mm diameter 11.5mm supercapacitor
0
2
2
Capacitor_THT
DX_5R5VxxxxU_D11.5mm_P5.00mm
CP, Radial series, Radial, pin pitch=5.00mm, diameter=11.5mm, Supercapacitor, http://www.elna.co.jp/en/capacitor/double_layer/catalog/pdf/dx_e.pdf
CP Radial series Radial pin pitch 5.00mm diameter 11.5mm supercapacitor
0
2
2
Capacitor_THT
DX_5R5VxxxxU_D19.0mm_P5.00mm
CP, Radial series, Radial, pin pitch=5.00mm, diameter=19mm, Supercapacitor, http://www.elna.co.jp/en/capacitor/double_layer/catalog/pdf/dx_e.pdf
CP Radial series Radial pin pitch 5.00mm diameter 19mm supercapacitor
0
2
2
Capacitor_Tantalum_SMD
CP_EIA-1608-08_AVX-J
Tantalum Capacitor SMD AVX-J (1608-08 Metric), IPC_7351 nominal, (Body size from: https://www.vishay.com/docs/48064/_t58_vmn_pt0471_1601.pdf), generated with kicad-footprint-generator
capacitor tantalum
0
2
2
Capacitor_Tantalum_SMD
CP_EIA-1608-08_AVX-J_Pad1.25x1.05mm_HandSolder
Tantalum Capacitor SMD AVX-J (1608-08 Metric), IPC_7351 nominal, (Body size from: https://www.vishay.com/docs/48064/_t58_vmn_pt0471_1601.pdf), generated with kicad-footprint-generator
capacitor tantalum
0
2
2
Capacitor_Tantalum_SMD
CP_EIA-1608-10_AVX-L
Tantalum Capacitor SMD AVX-L (1608-10 Metric), IPC_7351 nominal, (Body size from: https://www.vishay.com/docs/48064/_t58_vmn_pt0471_1601.pdf), generated with kicad-footprint-generator
capacitor tantalum
0
2
2
Capacitor_Tantalum_SMD
CP_EIA-1608-10_AVX-L_Pad1.25x1.05mm_HandSolder
Tantalum Capacitor SMD AVX-L (1608-10 Metric), IPC_7351 nominal, (Body size from: https://www.vishay.com/docs/48064/_t58_vmn_pt0471_1601.pdf), generated with kicad-footprint-generator
capacitor tantalum
0
2
2
Capacitor_Tantalum_SMD
CP_EIA-2012-12_Kemet-R
Tantalum Capacitor SMD Kemet-R (2012-12 Metric), IPC_7351 nominal, (Body size from: https://www.vishay.com/docs/40182/tmch.pdf), generated with kicad-footprint-generator
capacitor tantalum
0
2
2
Capacitor_Tantalum_SMD
CP_EIA-2012-12_Kemet-R_Pad1.30x1.05mm_HandSolder
Tantalum Capacitor SMD Kemet-R (2012-12 Metric), IPC_7351 nominal, (Body size from: https://www.vishay.com/docs/40182/tmch.pdf), generated with kicad-footprint-generator
capacitor tantalum
0
2
2
Capacitor_Tantalum_SMD
CP_EIA-2012-15_AVX-P
Tantalum Capacitor SMD AVX-P (2012-15 Metric), IPC_7351 nominal, (Body size from: https://www.vishay.com/docs/40182/tmch.pdf), generated with kicad-footprint-generator
capacitor tantalum
0
2
2
Capacitor_Tantalum_SMD
CP_EIA-2012-15_AVX-P_Pad1.30x1.05mm_HandSolder
Tantalum Capacitor SMD AVX-P (2012-15 Metric), IPC_7351 nominal, (Body size from: https://www.vishay.com/docs/40182/tmch.pdf), generated with kicad-footprint-generator
capacitor tantalum
0
2
2
Capacitor_Tantalum_SMD
CP_EIA-3216-10_Kemet-I
Tantalum Capacitor SMD Kemet-I (3216-10 Metric), IPC_7351 nominal, (Body size from: http://www.kemet.com/Lists/ProductCatalog/Attachments/253/KEM_TC101_STD.pdf), generated with kicad-footprint-generator
capacitor tantalum
0
2
2
Capacitor_Tantalum_SMD
CP_EIA-3216-10_Kemet-I_Pad1.58x1.35mm_HandSolder
Tantalum Capacitor SMD Kemet-I (3216-10 Metric), IPC_7351 nominal, (Body size from: http://www.kemet.com/Lists/ProductCatalog/Attachments/253/KEM_TC101_STD.pdf), generated with kicad-footprint-generator
capacitor tantalum
0
2
2
Capacitor_Tantalum_SMD
CP_EIA-3216-12_Kemet-S
Tantalum Capacitor SMD Kemet-S (3216-12 Metric), IPC_7351 nominal, (Body size from: http://www.kemet.com/Lists/ProductCatalog/Attachments/253/KEM_TC101_STD.pdf), generated with kicad-footprint-generator
capacitor tantalum
0
2
2
Capacitor_Tantalum_SMD
CP_EIA-3216-12_Kemet-S_Pad1.58x1.35mm_HandSolder
Tantalum Capacitor SMD Kemet-S (3216-12 Metric), IPC_7351 nominal, (Body size from: http://www.kemet.com/Lists/ProductCatalog/Attachments/253/KEM_TC101_STD.pdf), generated with kicad-footprint-generator
capacitor tantalum
0
2
2
Capacitor_Tantalum_SMD
CP_EIA-3216-18_Kemet-A
Tantalum Capacitor SMD Kemet-A (3216-18 Metric), IPC_7351 nominal, (Body size from: http://www.kemet.com/Lists/ProductCatalog/Attachments/253/KEM_TC101_STD.pdf), generated with kicad-footprint-generator
capacitor tantalum
0
2
2
Capacitor_Tantalum_SMD
CP_EIA-3216-18_Kemet-A_Pad1.58x1.35mm_HandSolder
Tantalum Capacitor SMD Kemet-A (3216-18 Metric), IPC_7351 nominal, (Body size from: http://www.kemet.com/Lists/ProductCatalog/Attachments/253/KEM_TC101_STD.pdf), generated with kicad-footprint-generator
capacitor tantalum
0
2
2
Capacitor_Tantalum_SMD
CP_EIA-3528-12_Kemet-T
Tantalum Capacitor SMD Kemet-T (3528-12 Metric), IPC_7351 nominal, (Body size from: http://www.kemet.com/Lists/ProductCatalog/Attachments/253/KEM_TC101_STD.pdf), generated with kicad-footprint-generator
capacitor tantalum
0
2
2
Capacitor_Tantalum_SMD
CP_EIA-3528-12_Kemet-T_Pad1.50x2.35mm_HandSolder
Tantalum Capacitor SMD Kemet-T (3528-12 Metric), IPC_7351 nominal, (Body size from: http://www.kemet.com/Lists/ProductCatalog/Attachments/253/KEM_TC101_STD.pdf), generated with kicad-footprint-generator
capacitor tantalum
0
2
2
Capacitor_Tantalum_SMD
CP_EIA-3528-15_AVX-H
Tantalum Capacitor SMD AVX-H (3528-15 Metric), IPC_7351 nominal, (Body size from: http://www.kemet.com/Lists/ProductCatalog/Attachments/253/KEM_TC101_STD.pdf), generated with kicad-footprint-generator
capacitor tantalum
0
2
2
Capacitor_Tantalum_SMD
CP_EIA-3528-15_AVX-H_Pad1.50x2.35mm_HandSolder
Tantalum Capacitor SMD AVX-H (3528-15 Metric), IPC_7351 nominal, (Body size from: http://www.kemet.com/Lists/ProductCatalog/Attachments/253/KEM_TC101_STD.pdf), generated with kicad-footprint-generator
capacitor tantalum
0
2
2
Capacitor_Tantalum_SMD
CP_EIA-3528-21_Kemet-B
Tantalum Capacitor SMD Kemet-B (3528-21 Metric), IPC_7351 nominal, (Body size from: http://www.kemet.com/Lists/ProductCatalog/Attachments/253/KEM_TC101_STD.pdf), generated with kicad-footprint-generator
capacitor tantalum
0
2
2
Capacitor_Tantalum_SMD
CP_EIA-3528-21_Kemet-B_Pad1.50x2.35mm_HandSolder
Tantalum Capacitor SMD Kemet-B (3528-21 Metric), IPC_7351 nominal, (Body size from: http://www.kemet.com/Lists/ProductCatalog/Attachments/253/KEM_TC101_STD.pdf), generated with kicad-footprint-generator
capacitor tantalum
0
2
2
Capacitor_Tantalum_SMD
CP_EIA-6032-15_Kemet-U
Tantalum Capacitor SMD Kemet-U (6032-15 Metric), IPC_7351 nominal, (Body size from: http://www.kemet.com/Lists/ProductCatalog/Attachments/253/KEM_TC101_STD.pdf), generated with kicad-footprint-generator
capacitor tantalum
0
2
2
Capacitor_Tantalum_SMD
CP_EIA-6032-15_Kemet-U_Pad2.25x2.35mm_HandSolder
Tantalum Capacitor SMD Kemet-U (6032-15 Metric), IPC_7351 nominal, (Body size from: http://www.kemet.com/Lists/ProductCatalog/Attachments/253/KEM_TC101_STD.pdf), generated with kicad-footprint-generator
capacitor tantalum
0
2
2
Capacitor_Tantalum_SMD
CP_EIA-6032-20_AVX-F
Tantalum Capacitor SMD AVX-F (6032-20 Metric), IPC_7351 nominal, (Body size from: http://www.kemet.com/Lists/ProductCatalog/Attachments/253/KEM_TC101_STD.pdf), generated with kicad-footprint-generator
capacitor tantalum
0
2
2
Capacitor_Tantalum_SMD
CP_EIA-6032-20_AVX-F_Pad2.25x2.35mm_HandSolder
Tantalum Capacitor SMD AVX-F (6032-20 Metric), IPC_7351 nominal, (Body size from: http://www.kemet.com/Lists/ProductCatalog/Attachments/253/KEM_TC101_STD.pdf), generated with kicad-footprint-generator
capacitor tantalum
0
2
2
Capacitor_Tantalum_SMD
CP_EIA-6032-28_Kemet-C
Tantalum Capacitor SMD Kemet-C (6032-28 Metric), IPC_7351 nominal, (Body size from: http://www.kemet.com/Lists/ProductCatalog/Attachments/253/KEM_TC101_STD.pdf), generated with kicad-footprint-generator
capacitor tantalum
0
2
2
Capacitor_Tantalum_SMD
CP_EIA-6032-28_Kemet-C_Pad2.25x2.35mm_HandSolder
Tantalum Capacitor SMD Kemet-C (6032-28 Metric), IPC_7351 nominal, (Body size from: http://www.kemet.com/Lists/ProductCatalog/Attachments/253/KEM_TC101_STD.pdf), generated with kicad-footprint-generator
capacitor tantalum
0
2
2
Capacitor_Tantalum_SMD
CP_EIA-7132-20_AVX-U
Tantalum Capacitor SMD AVX-U (7132-20 Metric), IPC_7351 nominal, (Body size from: http://datasheets.avx.com/F72-F75.pdf), generated with kicad-footprint-generator
capacitor tantalum
0
2
2
Capacitor_Tantalum_SMD
CP_EIA-7132-20_AVX-U_Pad2.72x3.50mm_HandSolder
Tantalum Capacitor SMD AVX-U (7132-20 Metric), IPC_7351 nominal, (Body size from: http://datasheets.avx.com/F72-F75.pdf), generated with kicad-footprint-generator
capacitor tantalum
0
2
2
Capacitor_Tantalum_SMD
CP_EIA-7132-28_AVX-C
Tantalum Capacitor SMD AVX-C (7132-28 Metric), IPC_7351 nominal, (Body size from: http://datasheets.avx.com/F72-F75.pdf), generated with kicad-footprint-generator
capacitor tantalum
0
2
2
Capacitor_Tantalum_SMD
CP_EIA-7132-28_AVX-C_Pad2.72x3.50mm_HandSolder
Tantalum Capacitor SMD AVX-C (7132-28 Metric), IPC_7351 nominal, (Body size from: http://datasheets.avx.com/F72-F75.pdf), generated with kicad-footprint-generator
capacitor tantalum
0
2
2
Capacitor_Tantalum_SMD
CP_EIA-7260-15_AVX-R
Tantalum Capacitor SMD AVX-R (7260-15 Metric), IPC_7351 nominal, (Body size from: http://datasheets.avx.com/F72-F75.pdf), generated with kicad-footprint-generator
capacitor tantalum
0
2
2
Capacitor_Tantalum_SMD
CP_EIA-7260-15_AVX-R_Pad2.68x6.30mm_HandSolder
Tantalum Capacitor SMD AVX-R (7260-15 Metric), IPC_7351 nominal, (Body size from: http://datasheets.avx.com/F72-F75.pdf), generated with kicad-footprint-generator
capacitor tantalum
0
2
2
Capacitor_Tantalum_SMD
CP_EIA-7260-20_AVX-M
Tantalum Capacitor SMD AVX-M (7260-20 Metric), IPC_7351 nominal, (Body size from: http://datasheets.avx.com/F72-F75.pdf), generated with kicad-footprint-generator
capacitor tantalum
0
2
2
Capacitor_Tantalum_SMD
CP_EIA-7260-20_AVX-M_Pad2.68x6.30mm_HandSolder
Tantalum Capacitor SMD AVX-M (7260-20 Metric), IPC_7351 nominal, (Body size from: http://datasheets.avx.com/F72-F75.pdf), generated with kicad-footprint-generator
capacitor tantalum
0
2
2
Capacitor_Tantalum_SMD
CP_EIA-7260-28_AVX-M
Tantalum Capacitor SMD AVX-M (7260-28 Metric), IPC_7351 nominal, (Body size from: http://datasheets.avx.com/F72-F75.pdf), generated with kicad-footprint-generator
capacitor tantalum
0
2
2
Capacitor_Tantalum_SMD
CP_EIA-7260-28_AVX-M_Pad2.68x6.30mm_HandSolder
Tantalum Capacitor SMD AVX-M (7260-28 Metric), IPC_7351 nominal, (Body size from: http://datasheets.avx.com/F72-F75.pdf), generated with kicad-footprint-generator
capacitor tantalum
0
2
2
Capacitor_Tantalum_SMD
CP_EIA-7260-38_AVX-R
Tantalum Capacitor SMD AVX-R (7260-38 Metric), IPC_7351 nominal, (Body size from: http://datasheets.avx.com/F72-F75.pdf), generated with kicad-footprint-generator
capacitor tantalum
0
2
2
Capacitor_Tantalum_SMD
CP_EIA-7260-38_AVX-R_Pad2.68x6.30mm_HandSolder
Tantalum Capacitor SMD AVX-R (7260-38 Metric), IPC_7351 nominal, (Body size from: http://datasheets.avx.com/F72-F75.pdf), generated with kicad-footprint-generator
capacitor tantalum
0
2
2
Capacitor_Tantalum_SMD
CP_EIA-7343-15_Kemet-W
Tantalum Capacitor SMD Kemet-W (7343-15 Metric), IPC_7351 nominal, (Body size from: http://www.kemet.com/Lists/ProductCatalog/Attachments/253/KEM_TC101_STD.pdf), generated with kicad-footprint-generator
capacitor tantalum
0
2
2
Capacitor_Tantalum_SMD
CP_EIA-7343-15_Kemet-W_Pad2.25x2.55mm_HandSolder
Tantalum Capacitor SMD Kemet-W (7343-15 Metric), IPC_7351 nominal, (Body size from: http://www.kemet.com/Lists/ProductCatalog/Attachments/253/KEM_TC101_STD.pdf), generated with kicad-footprint-generator
capacitor tantalum
0
2
2
Capacitor_Tantalum_SMD
CP_EIA-7343-20_Kemet-V
Tantalum Capacitor SMD Kemet-V (7343-20 Metric), IPC_7351 nominal, (Body size from: http://www.kemet.com/Lists/ProductCatalog/Attachments/253/KEM_TC101_STD.pdf), generated with kicad-footprint-generator
capacitor tantalum
0
2
2
Capacitor_Tantalum_SMD
CP_EIA-7343-20_Kemet-V_Pad2.25x2.55mm_HandSolder
Tantalum Capacitor SMD Kemet-V (7343-20 Metric), IPC_7351 nominal, (Body size from: http://www.kemet.com/Lists/ProductCatalog/Attachments/253/KEM_TC101_STD.pdf), generated with kicad-footprint-generator
capacitor tantalum
0
2
2
Capacitor_Tantalum_SMD
CP_EIA-7343-30_AVX-N
Tantalum Capacitor SMD AVX-N (7343-30 Metric), IPC_7351 nominal, (Body size from: http://www.kemet.com/Lists/ProductCatalog/Attachments/253/KEM_TC101_STD.pdf), generated with kicad-footprint-generator
capacitor tantalum
0
2
2
Capacitor_Tantalum_SMD
CP_EIA-7343-30_AVX-N_Pad2.25x2.55mm_HandSolder
Tantalum Capacitor SMD AVX-N (7343-30 Metric), IPC_7351 nominal, (Body size from: http://www.kemet.com/Lists/ProductCatalog/Attachments/253/KEM_TC101_STD.pdf), generated with kicad-footprint-generator
capacitor tantalum
0
2
2
Capacitor_Tantalum_SMD
CP_EIA-7343-31_Kemet-D
Tantalum Capacitor SMD Kemet-D (7343-31 Metric), IPC_7351 nominal, (Body size from: http://www.kemet.com/Lists/ProductCatalog/Attachments/253/KEM_TC101_STD.pdf), generated with kicad-footprint-generator
capacitor tantalum
0
2
2
Capacitor_Tantalum_SMD
CP_EIA-7343-31_Kemet-D_Pad2.25x2.55mm_HandSolder
Tantalum Capacitor SMD Kemet-D (7343-31 Metric), IPC_7351 nominal, (Body size from: http://www.kemet.com/Lists/ProductCatalog/Attachments/253/KEM_TC101_STD.pdf), generated with kicad-footprint-generator
capacitor tantalum
0
2
2
Capacitor_Tantalum_SMD
CP_EIA-7343-40_Kemet-Y
Tantalum Capacitor SMD Kemet-Y (7343-40 Metric), IPC_7351 nominal, (Body size from: http://www.kemet.com/Lists/ProductCatalog/Attachments/253/KEM_TC101_STD.pdf), generated with kicad-footprint-generator
capacitor tantalum
0
2
2
Capacitor_Tantalum_SMD
CP_EIA-7343-40_Kemet-Y_Pad2.25x2.55mm_HandSolder
Tantalum Capacitor SMD Kemet-Y (7343-40 Metric), IPC_7351 nominal, (Body size from: http://www.kemet.com/Lists/ProductCatalog/Attachments/253/KEM_TC101_STD.pdf), generated with kicad-footprint-generator
capacitor tantalum
0
2
2
Capacitor_Tantalum_SMD
CP_EIA-7343-43_Kemet-X
Tantalum Capacitor SMD Kemet-X (7343-43 Metric), IPC_7351 nominal, (Body size from: http://www.kemet.com/Lists/ProductCatalog/Attachments/253/KEM_TC101_STD.pdf), generated with kicad-footprint-generator
capacitor tantalum
0
2
2
Capacitor_Tantalum_SMD
CP_EIA-7343-43_Kemet-X_Pad2.25x2.55mm_HandSolder
Tantalum Capacitor SMD Kemet-X (7343-43 Metric), IPC_7351 nominal, (Body size from: http://www.kemet.com/Lists/ProductCatalog/Attachments/253/KEM_TC101_STD.pdf), generated with kicad-footprint-generator
capacitor tantalum
0
2
2
Capacitor_Tantalum_SMD
CP_EIA-7360-38_Kemet-E
Tantalum Capacitor SMD Kemet-E (7360-38 Metric), IPC_7351 nominal, (Body size from: http://www.kemet.com/Lists/ProductCatalog/Attachments/253/KEM_TC101_STD.pdf), generated with kicad-footprint-generator
capacitor tantalum
0
2
2
Capacitor_Tantalum_SMD
CP_EIA-7360-38_Kemet-E_Pad2.25x4.25mm_HandSolder
Tantalum Capacitor SMD Kemet-E (7360-38 Metric), IPC_7351 nominal, (Body size from: http://www.kemet.com/Lists/ProductCatalog/Attachments/253/KEM_TC101_STD.pdf), generated with kicad-footprint-generator
capacitor tantalum
0
2
2
Capacitor_Tantalum_SMD
CP_EIA-7361-38_AVX-V
Tantalum Capacitor SMD AVX-V (7361-38 Metric), IPC_7351 nominal, (Body size from: http://datasheets.avx.com/NOS.pdf), generated with kicad-footprint-generator
capacitor tantalum
0
2
2
Capacitor_Tantalum_SMD
CP_EIA-7361-38_AVX-V_Pad2.18x3.30mm_HandSolder
Tantalum Capacitor SMD AVX-V (7361-38 Metric), IPC_7351 nominal, (Body size from: http://datasheets.avx.com/NOS.pdf), generated with kicad-footprint-generator
capacitor tantalum
0
2
2
Capacitor_Tantalum_SMD
CP_EIA-7361-438_AVX-U
Tantalum Capacitor SMD AVX-U (7361-438 Metric), IPC_7351 nominal, (Body size from: http://datasheets.avx.com/NOS.pdf), generated with kicad-footprint-generator
capacitor tantalum
0
2
2
Capacitor_Tantalum_SMD
CP_EIA-7361-438_AVX-U_Pad2.18x3.30mm_HandSolder
Tantalum Capacitor SMD AVX-U (7361-438 Metric), IPC_7351 nominal, (Body size from: http://datasheets.avx.com/NOS.pdf), generated with kicad-footprint-generator
capacitor tantalum
0
2
2
Connector
Banana_Jack_1Pin
Single banana socket, footprint - 6mm drill
banana socket
0
1
1
Connector
Banana_Jack_2Pin
Dual banana socket, footprint - 2 x 6mm drills
banana socket
0
2
2
Connector
Banana_Jack_3Pin
Triple banana socket, footprint - 3 x 6mm drills
banana socket
0
3
3
Connector
CUI_PD-30
3 pin connector, PD-30, http://www.cui.com/product/resource/pd-30.pdf
connector 3-pin PD-30 power DIN
0
4
4
Connector
CUI_PD-30S
3-pin nonstandard DIN connector, shielded, PD-30S, http://www.cui.com/product/resource/pd-30s.pdf
connector 3-pin PD-30S power DIN shielded
0
8
5
Connector
CUI_PD-30S_CircularHoles
3-pin nonstandard DIN connector, shielded, PD-30S, http://www.cui.com/product/resource/pd-30s.pdf
connector 3-pin PD-30S power DIN shielded
0
8
5
Connector
CalTest_CT3151
Right-angle standard banana jack, http://www.caltestelectronics.com/images/attachments/P315100rH_drawing.pdf
banana jack horizontal
0
4
1
Connector
Connector_SFP_and_Cage
https://www.te.com/commerce/DocumentDelivery/DDEController?Action=srchrtrv&DocNm=2227302&DocType=Customer+Drawing&DocLang=English
SFP+ SFP
0
40
21
Connector
DTF13-12Px
http://www.te.com/usa-en/product-DTF13-12PA-G003.html
DEUTSCH DT header 12 pin 
0
12
12
Connector
FanPinHeader_1x03_P2.54mm_Vertical
3-pin CPU fan Through hole pin header, see http://www.formfactors.org/developer%5Cspecs%5Crev1_2_public.pdf
pin header 3-pin CPU fan
0
3
3
Connector
FanPinHeader_1x04_P2.54mm_Vertical
4-pin CPU fan Through hole pin header, e.g. for Wieson part number 2366C888-007 Molex 47053-1000, Foxconn HF27040-M1, Tyco 1470947-1 or equivalent, see http://www.formfactors.org/developer%5Cspecs%5Crev1_2_public.pdf
pin header 4-pin CPU fan
0
4
4
Connector
GB042-34S-H10
http://www.lsmtron.com/pdf/Connector&Antenna_catalog.PDF
34pin SMD connector 
0
34
34
Connector
IHI_B6A-PCB-45_Vertical
https://lugsdirect.com/PDF_Webprint/B6A-PCB-45-XX(-X).pdf
connector IHI B6A-PCB-45
0
49
1
Connector
JWT_A3963_1x02_P3.96mm_Vertical
JWT A3963, 3.96mm pitch Pin head connector (http://www.jwt.com.tw/pro_pdf/A3963.pdf)
connector JWT A3963 pinhead
0
2
2
Connector
NS-Tech_Grove_1x04_P2mm_Vertical
https://statics3.seeedstudio.com/images/opl/datasheet/3470130P1.pdf
Grove-1x04
0
4
4
Connector
SpringContact_Harwin_S1941-46R
7.25mm SMT Multi-directional Spring Contact (T+R), https://cdn.harwin.com/pdfs/S1941R.pdf
spring contact emi emc shield
0
1
1
Connector
Tag-Connect_TC2030-IDC-FP_2x03_P1.27mm_Vertical
Tag-Connect programming header; http://www.tag-connect.com/Materials/TC2030-IDC.pdf
tag connect programming header pogo pins
0
6
6
Connector
Tag-Connect_TC2030-IDC-NL_2x03_P1.27mm_Vertical
Tag-Connect programming header; http://www.tag-connect.com/Materials/TC2030-IDC-NL.pdf
tag connect programming header pogo pins
0
6
6
Connector
Tag-Connect_TC2050-IDC-FP_2x05_P1.27mm_Vertical
Tag-Connect programming header; http://www.tag-connect.com/Materials/TC2050-IDC-430%20Datasheet.pdf
tag connect programming header pogo pins
0
10
10
Connector
Tag-Connect_TC2050-IDC-NL_2x05_P1.27mm_Vertical
Tag-Connect programming header; http://www.tag-connect.com/Materials/TC2050-IDC-NL%20Datasheet.pdf
tag connect programming header pogo pins
0
10
10
Connector
Tag-Connect_TC2050-IDC-NL_2x05_P1.27mm_Vertical_with_bottom_clip
Tag-Connect programming header with bottom courtyard for TC2050-NL Clip board ; https://www.tag-connect.com/wp-content/uploads/bsk-pdf-manager/TC2050-IDC-NL_Datasheet_8.pdf https://www.tag-connect.com/wp-content/uploads/bsk-pdf-manager/TC2050-CLIP_Datasheet_25.pdf
tag connect programming header pogo pins
0
10
10
Connector
Tag-Connect_TC2070-IDC-FP_2x07_P1.27mm_Vertical
Tag-Connect programming header; http://www.tag-connect.com/Materials/TC2070-IDC%20Datasheet.pdf
tag connect programming header pogo pins
0
14
14
Connector_AMASS
AMASS_MR30PW-FB_1x03_P3.50mm_Horizontal
Connector XT30 Horizontal PCB Female, https://www.tme.eu/en/Document/5e47640ba39fa492dbd4c0f4c8ae7b93/MR30PW%20SPEC.pdf
RC Connector XT30
0
5
3
Connector_AMASS
AMASS_MR30PW-M_1x03_P3.50mm_Horizontal
Connector XT30 Horizontal PCB Male, https://www.tme.eu/en/Document/5e47640ba39fa492dbd4c0f4c8ae7b93/MR30PW%20SPEC.pdf
RC Connector XT30
0
5
3
Connector_AMASS
AMASS_XT30PW-F_1x02_P2.50mm_Horizontal
Connector XT30 Horizontal PCB Female, https://www.tme.eu/en/Document/ce4077e36b79046da520ca73227e15de/XT30PW%20SPEC.pdf
RC Connector XT30
0
4
2
Connector_AMASS
AMASS_XT30PW-M_1x02_P2.50mm_Horizontal
Connector XT30 Horizontal PCB Male, https://www.tme.eu/en/Document/ce4077e36b79046da520ca73227e15de/XT30PW%20SPEC.pdf
RC Connector XT30
0
4
2
Connector_AMASS
AMASS_XT30U-F_1x02_P5.0mm_Vertical
Connector XT30 Vertical Cable Female, https://www.tme.eu/en/Document/3cbfa5cfa544d79584972dd5234a409e/XT30U%20SPEC.pdf
RC Connector XT30
0
2
2
Connector_AMASS
AMASS_XT30U-M_1x02_P5.0mm_Vertical
Connector XT30 Vertical Cable Male, https://www.tme.eu/en/Document/3cbfa5cfa544d79584972dd5234a409e/XT30U%20SPEC.pdf
RC Connector XT30
0
2
2
Connector_AMASS
AMASS_XT30UPB-F_1x02_P5.0mm_Vertical
Connector XT30 Vertical PCB Female, https://www.tme.eu/en/Document/4acc913878197f8c2e30d4b8cdc47230/XT30UPB%20SPEC.pdf
RC Connector XT30
0
2
2
Connector_AMASS
AMASS_XT30UPB-M_1x02_P5.0mm_Vertical
Connector XT30 Vertical PCB Male, https://www.tme.eu/en/Document/4acc913878197f8c2e30d4b8cdc47230/XT30UPB%20SPEC.pdf
RC Connector XT30
0
2
2
Connector_AMASS
AMASS_XT60-F_1x02_P7.20mm_Vertical
AMASS female XT60, through hole, vertical, https://www.tme.eu/Document/2d152ced3b7a446066e6c419d84bb460/XT60%20SPEC.pdf
XT60 female vertical
0
2
2
Connector_AMASS
AMASS_XT60-M_1x02_P7.20mm_Vertical
AMASS female XT60, through hole, vertical, https://www.tme.eu/Document/2d152ced3b7a446066e6c419d84bb460/XT60%20SPEC.pdf
XT60 female vertical
0
2
2
Connector_AMASS
AMASS_XT60IPW-M_1x03_P7.20mm_Horizontal
Connector XT60 Horizontal PCB Male, https://www.bto.pl/pdf/08988/XT60IPW-M3.pdf
RC Connector XT60
0
5
3
Connector_AMASS
AMASS_XT60PW-F_1x02_P7.20mm_Horizontal
Connector XT60 Horizontal PCB Female, https://www.tme.eu/en/Document/9b8d0c5eb7094295f3d3112c214d3ade/XT60PW%20SPEC.pdf
RC Connector XT60
0
4
2
Connector_AMASS
AMASS_XT60PW-M_1x02_P7.20mm_Horizontal
Connector XT60 Horizontal PCB Female, https://www.tme.eu/en/Document/9b8d0c5eb7094295f3d3112c214d3ade/XT60PW%20SPEC.pdf
RC Connector XT60
0
4
2
Connector_Amphenol
Amphenol_M8S-03PMMR-SF8001
M8 Male connector for panel, 90° PCB mount (https://www.amphenolltw.com/2012download/2D%20PDF/03_M%20Series%20Sensor%20Connectors/M8S-XXPMMR-SF8001.pdf)
three-pin M8
0
5
4
Connector_Audio
Jack_3.5mm_CUI_SJ-3523-SMT_Horizontal
3.5 mm, Stereo, Right Angle, Surface Mount (SMT), Audio Jack Connector (https://www.cui.com/product/resource/sj-352x-smt-series.pdf)
3.5mm audio cui horizontal jack stereo
0
3
3
Connector_Audio
Jack_3.5mm_CUI_SJ-3524-SMT_Horizontal
3.5 mm, Stereo, Right Angle, Surface Mount (SMT), Audio Jack Connector (https://www.cui.com/product/resource/sj-352x-smt-series.pdf)
3.5mm audio cui horizontal jack stereo
0
4
4
Connector_Audio
Jack_3.5mm_CUI_SJ1-3523N_Horizontal
TRS 3.5mm, horizontal, through-hole, https://www.cuidevices.com/product/resource/pdf/sj1-352xn.pdf
TRS audio jack stereo horizontal
0
3
3
Connector_Audio
Jack_3.5mm_CUI_SJ1-3524N_Horizontal
TRS 3.5mm, horizontal, through-hole, https://www.cuidevices.com/product/resource/pdf/sj1-352xn.pdf
TRS audio jack stereo horizontal
0
4
4
Connector_Audio
Jack_3.5mm_CUI_SJ1-3525N_Horizontal
TRS 3.5mm, horizontal, through-hole, https://www.cuidevices.com/product/resource/pdf/sj1-352xn.pdf
TRS audio jack stereo horizontal
0
5
5
Connector_Audio
Jack_3.5mm_CUI_SJ1-3533NG_Horizontal
TRS 3.5mm, horizontal, through-hole, https://www.cui.com/product/resource/sj1-353xng.pdf
TRS audio jack stereo horizontal
0
3
3
Connector_Audio
Jack_3.5mm_CUI_SJ1-3533NG_Horizontal_CircularHoles
TRS 3.5mm, horizontal, through-hole, , circular holeshttps://www.cui.com/product/resource/sj1-353xng.pdf
TRS audio jack stereo horizontal circular
0
3
3
Connector_Audio
Jack_3.5mm_CUI_SJ1-3535NG_Horizontal
TRS 3.5mm, horizontal, through-hole, with switch, https://www.cui.com/product/resource/sj1-353xng.pdf
TRS audio jack stereo horizontal
0
5
5
Connector_Audio
Jack_3.5mm_CUI_SJ1-3535NG_Horizontal_CircularHoles
TRS 3.5mm, horizontal, through-hole, with switch, circular holes, https://www.cui.com/product/resource/sj1-353xng.pdf
TRS audio jack stereo horizontal circular
0
5
5
Connector_Audio
Jack_3.5mm_CUI_SJ2-3593D-SMT_Horizontal
3.5 mm, Stereo, Right Angle, Surface Mount (SMT), Audio Jack Connector (https://www.cuidevices.com/product/resource/sj2-359x-smt.pdf)
3.5mm audio cui horizontal jack stereo
0
5
5
Connector_Audio
Jack_3.5mm_Ledino_KB3SPRS_Horizontal
https://www.reichelt.de/index.html?ACTION=7&LA=3&OPEN=0&INDEX=0&FILENAME=C160%252FKB3SPRS.pdf
jack stereo TRS
0
5
5
Connector_Audio
Jack_3.5mm_Lumberg_1503_07_Horizontal
TRS 3.5mm, horizontal, through-hole, https://downloads.lumberg.com/datenblaetter/en/1503_07.pdf
TRS audio jack horizontal
0
4
3
Connector_Audio
Jack_3.5mm_PJ311_Horizontal
PJ311 6pin SMD 3.5mm stereo headphones jack.
headphones jack plug stereo 3.5mm PJ311
0
6
6
Connector_Audio
Jack_3.5mm_PJ320D_Horizontal
Headphones with microphone connector, 3.5mm, 4 pins (http://www.qingpu-electronics.com/en/products/WQP-PJ320D-72.html)
3.5mm jack mic microphone phones headphones 4pins audio plug
0
4
4
Connector_Audio
Jack_3.5mm_PJ320E_Horizontal
Headphones with microphone connector, 3.5mm, 4 pins (http://www.qingpu-electronics.com/en/products/WQP-PJ320E-177.html)
3.5mm jack mic microphone phones headphones 4pins audio plug
0
5
4
Connector_Audio
Jack_3.5mm_PJ31060-I_Horizontal
PJ31060-I 6pin SMD 3.5mm headphones jack (http://www.china-bsun.com/Product48/1577.html)
headphones jack plug stereo 3.5mm PJ31060-I PJ31060
0
6
6
Connector_Audio
Jack_3.5mm_QingPu_WQP-PJ398SM_Vertical_CircularHoles
TRS 3.5mm, vertical, Thonkiconn, PCB mount, (http://www.qingpu-electronics.com/en/products/WQP-PJ398SM-362.html)
WQP-PJ398SM WQP-PJ301M-12 TRS 3.5mm mono vertical jack thonkiconn qingpu
0
3
3
Connector_Audio
Jack_3.5mm_Switronic_ST-005-G_horizontal
3.5mm horizontal headphones jack, http://akizukidenshi.com/download/ds/switronic/ST-005-G.pdf
Connector Audio Switronic ST-005-G
0
4
3
Connector_Audio
Jack_3.5mm_Technik_TWP-3002_Horizontal
3.5mm Horizontal Waterproof Stereo Headphones Jack, https://www.technik.com.hk/images/pdf_product/WP3002-PA66-A.pdf
audio jack stereo horizontal waterproof
0
7
4
Connector_Audio
Jack_6.35mm_Neutrik_NJ2FD-V_Vertical
6.35mm (1/4 in) Vertical Jack, Non-switching mono jack (T/S), https://www.neutrik.com/en/product/nj2fd-v
neutrik jack vertical
0
2
2
Connector_Audio
Jack_6.35mm_Neutrik_NJ3FD-V_Vertical
6.35mm (1/4 in) Vertical Jack, Non-switching stereo jack (T/R/S), https://www.neutrik.com/en/product/nj3fd-v
neutrik jack vertical
0
3
3
Connector_Audio
Jack_6.35mm_Neutrik_NJ5FD-V_Vertical
6.35mm (1/4 in) Vertical Jack, 2 x switching (normalling) stereo jack (T/TN/R/RN/S), https://www.neutrik.com/en/product/nj5fd-v
neutrik jack vertical
0
5
5
Connector_Audio
Jack_6.35mm_Neutrik_NJ6FD-V_Vertical
6.35mm (1/4 in) Vertical Jack, 3 x switching (normalling) stereo jack (T/TN/R/RN/S/SN), https://www.neutrik.com/en/product/nj6fd-v
neutrik jack vertical
0
6
6
Connector_Audio
Jack_6.35mm_Neutrik_NJ6TB-V_Vertical
6.35mm (1/4 in) Vertical Jack, 3 x switching (normalling) stereo jack  B-gauge type (T/TN/R/RN/S/SN), https://www.neutrik.com/en/product/nj6tb-v
neutrik jack vertical
0
6
6
Connector_Audio
Jack_6.35mm_Neutrik_NMJ4HCD2_Horizontal
M Series, 6.35mm (1/4in) mono jack, switched, with chrome ferrule and straight PCB pins, https://www.neutrik.com/en/product/nmj4hcd2
neutrik jack m
0
4
4
Connector_Audio
Jack_6.35mm_Neutrik_NMJ4HFD2_Horizontal
M Series, 6.35mm (1/4in) mono jack, switched, with full threaded nose and straight PCB pins, https://www.neutrik.com/en/product/nmj4hfd2
neutrik jack m
0
4
4
Connector_Audio
Jack_6.35mm_Neutrik_NMJ4HFD3_Horizontal
M Series, 6.35mm (1/4in) mono jack, switched, with a full threaded nose and offset PCB pins, https://www.neutrik.com/en/product/nmj4hfd3
neutrik jack m
0
4
4
Connector_Audio
Jack_6.35mm_Neutrik_NMJ4HHD2_Horizontal
M Series, 6.35mm (1/4in) mono jack, switched, with a half threaded nose and offset PCB pins, https://www.neutrik.com/en/product/nmj4hhd2
neutrik jack m
0
4
4
Connector_Audio
Jack_6.35mm_Neutrik_NMJ6HCD2_Horizontal
M Series, 6.35mm (1/4in) stereo jack, switched, with chrome ferrule and straight PCB pins, https://www.neutrik.com/en/product/nmj6hcd2
neutrik jack m
0
6
6
Connector_Audio
Jack_6.35mm_Neutrik_NMJ6HCD3_Horizontal
M Series, 6.35mm (1/4in) stereo jack, switched, with chrome ferrule and offset PCB pins, https://www.neutrik.com/en/product/nmj6hcd3
neutrik jack m
0
6
6
Connector_Audio
Jack_6.35mm_Neutrik_NMJ6HFD2-AU_Horizontal
M Series, 6.35mm (1/4in) stereo jack, switched, full threaded nose, straight PCB pins, gold plated contacts, https://www.neutrik.com/en/product/nmj6hfd2-au
neutrik jack m
0
6
6
Connector_Audio
Jack_6.35mm_Neutrik_NMJ6HFD2_Horizontal
M Series, 6.35mm (1/4in) stereo jack, switched, with full threaded nose and straight PCB pins, https://www.neutrik.com/en/product/nmj6hfd2
neutrik jack m
0
6
6
Connector_Audio
Jack_6.35mm_Neutrik_NMJ6HFD3_Horizontal
M Series, 6.35mm (1/4in) stereo jack, switched, with full threaded nose and offset PCB pins, https://www.neutrik.com/en/product/nmj6hfd3
neutrik jack m
0
6
6
Connector_Audio
Jack_6.35mm_Neutrik_NMJ6HFD4_Horizontal
M Series, 6.35mm (1/4in) stereo jack, switched, with full threaded nose and fishtail PCB pins, https://www.neutrik.com/en/product/nmj6hfd4
neutrik jack m
0
6
6
Connector_Audio
Jack_6.35mm_Neutrik_NMJ6HHD2_Horizontal
M Series, 6.35mm (1/4in) stereo jack, switched, with half threaded nose and offset PCB pins, https://www.neutrik.com/en/product/nmj6hhd2
neutrik jack m
0
6
6
Connector_Audio
Jack_6.35mm_Neutrik_NRJ3HF-1_Horizontal
Slim Jacks, 6.35mm (1/4in) stereo jack, unswitched, fully threaded nose, sleeve contact/front panel connection, https://www.neutrik.com/en/product/nrj3hf-1
neutrik jack slim
0
4
4
Connector_Audio
Jack_6.35mm_Neutrik_NRJ4HF-1_Horizontal
Slim Jacks, 6.35mm (1/4in) mono jack, switched, fully threaded nose, sleeve contact/front panel connection, https://www.neutrik.com/en/product/nrj4hf-1
neutrik jack slim
0
4
4
Connector_Audio
Jack_6.35mm_Neutrik_NRJ4HF_Horizontal
Slim Jacks, 6.35mm (1/4in) mono jack, switched, fully threaded nose, https://www.neutrik.com/en/product/nrj4hf
neutrik jack slim
0
4
4
Connector_Audio
Jack_6.35mm_Neutrik_NRJ4HH-1_Horizontal
Slim Jacks, 6.35mm (1/4in) mono jack, switched, half threaded nose, sleeve contact/front panel connection, https://www.neutrik.com/en/product/nrj4hh-1
neutrik jack slim
0
4
4
Connector_Audio
Jack_6.35mm_Neutrik_NRJ4HH_Horizontal
Slim Jacks, 6.35mm (1/4in) mono jack, switched, half threaded nose, https://www.neutrik.com/en/product/nrj4hh
neutrik jack slim
0
4
4
Connector_Audio
Jack_6.35mm_Neutrik_NRJ6HF-1-AU_Horizontal
Slim Jacks, 6.35mm (1/4in) stereo jack, switched, gold plated contacts, fully threaded nose, sleeve contact/front panel connection, https://www.neutrik.com/en/product/nrj6hf-1-au
neutrik jack slim
0
6
6
Connector_Audio
Jack_6.35mm_Neutrik_NRJ6HF-1_Horizontal
Slim Jacks, 6.35mm (1/4in) stereo jack, switched, fully threaded nose, sleeve contact/front panel connection, https://www.neutrik.com/en/product/nrj6hf-1
neutrik jack slim
0
6
6
Connector_Audio
Jack_6.35mm_Neutrik_NRJ6HF-AU_Horizontal
Slim Jacks, 6.35mm (1/4in) stereo jack, switched, gold plated contacts, fully threaded nose, https://www.neutrik.com/en/product/nrj6hf-au
neutrik jack slim
0
6
6
Connector_Audio
Jack_6.35mm_Neutrik_NRJ6HF_Horizontal
Slim Jacks, 6.35mm (1/4in) stereo jack, switched, fully threaded nose, https://www.neutrik.com/en/product/nrj6hf
neutrik jack slim
0
6
6
Connector_Audio
Jack_6.35mm_Neutrik_NRJ6HH-1_Horizontal
Slim Jacks, 6.35mm (1/4in) stereo jack, switched, half threaded nose, sleeve contact/front panel connection, https://www.neutrik.com/en/product/nrj6hh-1
neutrik jack slim
0
6
6
Connector_Audio
Jack_6.35mm_Neutrik_NRJ6HH-AU_Horizontal
Slim Jacks, 6.35mm (1/4in) stereo jack, switched, gold plated contacts, half threaded nose, https://www.neutrik.com/en/product/nrj6hh-au
neutrik jack slim
0
6
6
Connector_Audio
Jack_6.35mm_Neutrik_NRJ6HH_Horizontal
Slim Jacks, 6.35mm (1/4in) stereo jack, switched, half threaded nose, https://www.neutrik.com/en/product/nrj6hh
neutrik jack slim
0
6
6
Connector_Audio
Jack_6.35mm_Neutrik_NRJ6HM-1-AU_Horizontal
Slim Jacks, 6.35mm (1/4in) stereo jack, metal nose, gold plated contacts, efficient chassis ground connection, T+R+S normalling contact, https://www.neutrik.com/en/product/nrj6hm-1-au
neutrik jack slim
0
6
6
Connector_Audio
Jack_6.35mm_Neutrik_NRJ6HM-1-PRE_Horizontal
Slim Jacks, 6.35mm (1/4in) stereo jack, metal nose, efficient chassis ground connection, T+R normalling contact, https://www.neutrik.com/en/product/nrj6hm-1-pre
neutrik jack slim
0
6
5
Connector_Audio
Jack_6.35mm_Neutrik_NRJ6HM-1_Horizontal
Slim Jacks, 6.35mm (1/4in) stereo jack, metal nose with efficient chassis ground connection, T+R+S normalling contact, https://www.neutrik.com/en/product/nrj6hm-1
neutrik jack slim
0
6
6
Connector_Audio
Jack_6.35mm_Neutrik_NSJ8HC_Horizontal
Stacking Jacks, Mono dual jack, full nose, https://www.neutrik.com/en/product/nsj8hc
neutrik jack stacking
0
9
9
Connector_Audio
Jack_6.35mm_Neutrik_NSJ8HL_Horizontal
Stacking Jacks, Mono dual jack, quick fix nose, https://www.neutrik.com/en/product/nsj8hl
neutrik jack stacking
0
9
9
Connector_Audio
Jack_6.35mm_Neutrik_NSJ12HC_Horizontal
Stacking Jacks, Stereo dual jack, full nose, https://www.neutrik.com/en/product/nsj12hc
neutrik jack stacking
0
13
13
Connector_Audio
Jack_6.35mm_Neutrik_NSJ12HF-1_Horizontal
Stacking Jacks, Stereo dual jack, full threaded nose, https://www.neutrik.com/en/product/nsj12hf-1
neutrik jack stacking
0
13
13
Connector_Audio
Jack_6.35mm_Neutrik_NSJ12HH-1_Horizontal
Stacking Jacks, Stereo dual jack, half threaded nose, https://www.neutrik.com/en/product/nsj12hh-1
neutrik jack stacking
0
13
13
Connector_Audio
Jack_6.35mm_Neutrik_NSJ12HL_Horizontal
Stacking Jacks, Stereo dual jack, quick fix nose, https://www.neutrik.com/en/product/nsj12hl
neutrik jack stacking
0
13
13
Connector_Audio
Jack_XLR-6.35mm_Neutrik_NCJ5FI-H-0_Horizontal
Combo I series, 3 pole XLR female receptacle with 6.35mm (1/4in) mono jack without switching contact, horizontal PCB mount, https://www.neutrik.com/en/product/ncj5fi-h-0
neutrik jack combo i
0
6
6
Connector_Audio
Jack_XLR-6.35mm_Neutrik_NCJ5FI-H_Horizontal
Combo I series, 3 pole XLR female receptacle with 6.35mm (1/4in) mono jack without switching contact, horizontal PCB mount, retention spring, https://www.neutrik.com/en/product/ncj5fi-h
neutrik jack combo i
0
6
6
Connector_Audio
Jack_XLR-6.35mm_Neutrik_NCJ5FI-V-0_Vertical
Combo I series, 3 pole XLR female receptacle with 6.35mm (1/4in) mono jack without switching contact, vertical PCB mount, https://www.neutrik.com/en/product/ncj5fi-v-0
neutrik jack combo i
0
6
6
Connector_Audio
Jack_XLR-6.35mm_Neutrik_NCJ5FI-V_Vertical
Combo I series, 3 pole XLR female receptacle with 6.35mm (1/4in) mono jack without switching contact, vertical PCB mount, retention spring, https://www.neutrik.com/en/product/ncj5fi-v
neutrik jack combo i
0
6
6
Connector_Audio
Jack_XLR-6.35mm_Neutrik_NCJ6FA-H-0_Horizontal
Combo A series, 3 pole XLR female receptacle with 6.35mm (1/4in) stereo jack, horizontal PCB mount, retention spring, https://www.neutrik.com/en/product/ncj6fa-h-0
neutrik jack combo a
0
8
7
Connector_Audio
Jack_XLR-6.35mm_Neutrik_NCJ6FA-H-DA_Horizontal
Combo A series, 3 pole XLR female receptacle with 6.35mm (1/4in) stereo jack, horizontal PCB mount, asymmetric push, https://www.neutrik.com/en/product/ncj6fa-h-da
neutrik jack combo a
0
8
7
Connector_Audio
Jack_XLR-6.35mm_Neutrik_NCJ6FA-H_Horizontal
Combo A series, 3 pole XLR female receptacle with 6.35mm (1/4in) stereo jack, horizontal PCB mount, https://www.neutrik.com/en/product/ncj6fa-h
neutrik jack combo a
0
8
7
Connector_Audio
Jack_XLR-6.35mm_Neutrik_NCJ6FA-V-0_Vertical
Combo A series, 3 pole XLR female receptacle with 6.35mm (1/4in) stereo jack, vertical PCB mount, retention spring, https://www.neutrik.com/en/product/ncj6fa-v-0
neutrik jack combo a
0
8
7
Connector_Audio
Jack_XLR-6.35mm_Neutrik_NCJ6FA-V-DA_Vertical
Combo A series, 3 pole XLR female receptacle with 6.35mm (1/4in) stereo jack, vertical PCB mount, asymmetric push, https://www.neutrik.com/en/product/ncj6fa-v-da
neutrik jack combo a
0
8
7
Connector_Audio
Jack_XLR-6.35mm_Neutrik_NCJ6FA-V_Vertical
Combo A series, 3 pole XLR female receptacle with 6.35mm (1/4in) stereo jack, vertical PCB mount, https://www.neutrik.com/en/product/ncj6fa-v
neutrik jack combo a
0
8
7
Connector_Audio
Jack_XLR-6.35mm_Neutrik_NCJ6FI-H-0_Horizontal
Combo I series, 3 pole XLR female receptacle with 6.35mm (1/4in) stereo jack without switching contact, horizontal PCB mount, https://www.neutrik.com/en/product/ncj6fi-h-0
neutrik jack combo i
0
7
7
Connector_Audio
Jack_XLR-6.35mm_Neutrik_NCJ6FI-H_Horizontal
Combo I series, 3 pole XLR female receptacle with 6.35mm (1/4in) stereo jack without switching contact, horizontal PCB mount, retention spring, https://www.neutrik.com/en/product/ncj6fi-h
neutrik jack combo i
0
7
7
Connector_Audio
Jack_XLR-6.35mm_Neutrik_NCJ6FI-V-0_Vertical
Combo I series, 3 pole XLR female receptacle with 6.35mm (1/4in) stereo jack without switching contact, vertical PCB mount, https://www.neutrik.com/en/product/ncj6fi-v-0
neutrik jack combo i
0
7
7
Connector_Audio
Jack_XLR-6.35mm_Neutrik_NCJ6FI-V_Vertical
Combo I series, 3 pole XLR female receptacle with 6.35mm (1/4in) stereo jack without switching contact, vertical PCB mount, retention spring, https://www.neutrik.com/en/product/ncj6fi-v
neutrik jack combo i
0
7
7
Connector_Audio
Jack_XLR-6.35mm_Neutrik_NCJ9FI-H-0_Horizontal
Combo I series, 3 pole XLR female receptacle with 6.35mm (1/4in) switching stereo jack, horizontal PCB mount, https://www.neutrik.com/en/product/ncj9fi-h-0
neutrik jack combo i
0
10
10
Connector_Audio
Jack_XLR-6.35mm_Neutrik_NCJ9FI-H_Horizontal
Combo I series, 3 pole XLR female receptacle with 6.35mm (1/4in) switching stereo jack, horizontal PCB mount, retention spring, https://www.neutrik.com/en/product/ncj9fi-h
neutrik jack combo i
0
10
10
Connector_Audio
Jack_XLR-6.35mm_Neutrik_NCJ9FI-V-0_Vertical
Combo I series, 3 pole XLR female receptacle with 6.35mm (1/4in) switching stereo jack, vertical PCB mount, https://www.neutrik.com/en/product/ncj9fi-v-0
neutrik jack combo i
0
10
10
Connector_Audio
Jack_XLR-6.35mm_Neutrik_NCJ9FI-V_Vertical
Combo I series, 3 pole XLR female receptacle with 6.35mm (1/4in) switching stereo jack, vertical PCB mount, retention spring, https://www.neutrik.com/en/product/ncj9fi-v
neutrik jack combo i
0
10
10
Connector_Audio
Jack_XLR-6.35mm_Neutrik_NCJ10FI-H-0_Horizontal
Combo I series, 3 pole XLR female receptacle with 6.35mm (1/4in) switching stereo jack and switching ground contact, horizontal PCB mount, https://www.neutrik.com/en/product/ncj10fi-h-0
neutrik jack combo i
0
11
11
Connector_Audio
Jack_XLR-6.35mm_Neutrik_NCJ10FI-H_Horizontal
Combo I series, 3 pole XLR female receptacle with 6.35mm (1/4in) switching stereo jack and switching ground contact, horizontal PCB mount, retention spring, https://www.neutrik.com/en/product/ncj10fi-h
neutrik jack combo i
0
11
11
Connector_Audio
Jack_XLR-6.35mm_Neutrik_NCJ10FI-V-0_Vertical
Combo I series, 3 pole XLR female receptacle with 6.35mm (1/4in) switching stereo jack and switching ground contact, vertical PCB mount, https://www.neutrik.com/en/product/ncj10fi-v-0
neutrik jack combo i
0
11
11
Connector_Audio
Jack_XLR-6.35mm_Neutrik_NCJ10FI-V_Vertical
Combo I series, 3 pole XLR female receptacle with 6.35mm (1/4in) switching stereo jack and switching ground contact, vertical PCB mount, retention spring, https://www.neutrik.com/en/product/ncj10fi-v
neutrik jack combo i
0
11
11
Connector_Audio
Jack_XLR_Neutrik_NC3FAAH-0_Horizontal
AA Series, 3 pole female XLR receptacle, grounding: without ground/shell contact, horizontal PCB mount, retention spring instead of latch, https://www.neutrik.com/en/product/nc3faah-0
neutrik xlr aa
0
3
3
Connector_Audio
Jack_XLR_Neutrik_NC3FAAH1-0_Horizontal
AA Series, 3 pole female XLR receptacle, grounding: mating connector shell to pin1 and front panel, horizontal PCB mount, retention spring instead of latch, https://www.neutrik.com/en/product/nc3faah1-0
neutrik xlr aa
0
3
3
Connector_Audio
Jack_XLR_Neutrik_NC3FAAH1-DA_Horizontal
AA Series, 3 pole female XLR receptacle, grounding: mating connector shell to pin1 and front panel, horizontal PCB mount, asymmetric push, https://www.neutrik.com/en/product/nc3faah1-da
neutrik xlr aa
0
3
3
Connector_Audio
Jack_XLR_Neutrik_NC3FAAH1_Horizontal
AA Series, 3 pole female XLR receptacle, grounding: mating connector shell to pin1 and front panel, horizontal PCB mount, https://www.neutrik.com/en/product/nc3faah1
neutrik xlr aa
0
3
3
Connector_Audio
Jack_XLR_Neutrik_NC3FAAH2-0_Horizontal
AA Series, 3 pole female XLR receptacle, grounding: separate ground contact to mating connector shell and front panel, horizontal PCB mount, retention spring instead of latch, https://www.neutrik.com/en/product/nc3faah2-0
neutrik xlr aa
0
4
4
Connector_Audio
Jack_XLR_Neutrik_NC3FAAH2_Horizontal
AA Series, 3 pole female XLR receptacle, grounding: separate ground contact to mating connector shell and front panel, horizontal PCB mount, https://www.neutrik.com/en/product/nc3faah2
neutrik xlr aa
0
4
4
Connector_Audio
Jack_XLR_Neutrik_NC3FAAH_Horizontal
AA Series, 3 pole female XLR receptacle, grounding: without ground/shell contact, horizontal PCB mount, https://www.neutrik.com/en/product/nc3faah
neutrik xlr aa
0
3
3
Connector_Audio
Jack_XLR_Neutrik_NC3FAAV-0_Vertical
AA Series, 3 pole female receptacle, grounding: without ground/shell contact, vertical PCB mount, retention spring instead of latch, https://www.neutrik.com/en/product/nc3faav-0
neutrik xlr aa
0
3
3
Connector_Audio
Jack_XLR_Neutrik_NC3FAAV1-0_Vertical
AA Series, 3 pole female receptacle, grounding: mating connector shell to pin1 and front panel, vertical PCB mount, retention spring instead of latch, https://www.neutrik.com/en/product/nc3faav1-0
neutrik xlr aa
0
3
3
Connector_Audio
Jack_XLR_Neutrik_NC3FAAV1-DA_Vertical
AA Series, 3 pole female receptacle, grounding: mating connector shell to pin1 and front panel, vertical PCB mount, asymmetric push, https://www.neutrik.com/en/product/nc3faav1-da
neutrik xlr aa
0
3
3
Connector_Audio
Jack_XLR_Neutrik_NC3FAAV1_Vertical
AA Series, 3 pole female receptacle, grounding: mating connector shell to pin1 and front panel, vertical PCB mount, https://www.neutrik.com/en/product/nc3faav1
neutrik xlr aa
0
3
3
Connector_Audio
Jack_XLR_Neutrik_NC3FAAV2-0_Vertical
AA Series, 3 pole female receptacle, grounding: separate ground contact to mating connector shell and front panel, vertical PCB mount, retention spring instead of latch, https://www.neutrik.com/en/product/nc3faav2-0
neutrik xlr aa
0
4
4
Connector_Audio
Jack_XLR_Neutrik_NC3FAAV2_Vertical
AA Series, 3 pole female receptacle, grounding: separate ground contact to mating connector shell and front panel, vertical PCB mount, https://www.neutrik.com/en/product/nc3faav2
neutrik xlr aa
0
4
4
Connector_Audio
Jack_XLR_Neutrik_NC3FAAV_Vertical
AA Series, 3 pole female receptacle, grounding: without ground/shell contact, vertical PCB mount, https://www.neutrik.com/en/product/nc3faav
neutrik xlr aa
0
3
3
Connector_Audio
Jack_XLR_Neutrik_NC3FAH-0_Horizontal
A Series, 3 pole female XLR receptacle, grounding: without ground/shell contact, horizontal PCB mount, retention spring instead of latch, https://www.neutrik.com/en/product/nc3fah-0
neutrik xlr a
0
3
3
Connector_Audio
Jack_XLR_Neutrik_NC3FAH1-0_Horizontal
A Series, 3 pole female XLR receptacle, grounding: mating connector shell to pin1 and front panel, horizontal PCB mount, retention spring instead of latch, https://www.neutrik.com/en/product/nc3fah1-0
neutrik xlr a
0
3
3
Connector_Audio
Jack_XLR_Neutrik_NC3FAH1-DA_Horizontal
A Series, 3 pole female XLR receptacle, grounding: mating connector shell to pin1 and front panel, horizontal PCB mount, asymmetric push, https://www.neutrik.com/en/product/nc3fah1-da
neutrik xlr a
0
3
3
Connector_Audio
Jack_XLR_Neutrik_NC3FAH1_Horizontal
A Series, 3 pole female XLR receptacle, grounding: mating connector shell to pin1 and front panel, horizontal PCB mount, https://www.neutrik.com/en/product/nc3fah1
neutrik xlr a
0
3
3
Connector_Audio
Jack_XLR_Neutrik_NC3FAH2-0_Horizontal
A Series, 3 pole female XLR receptacle, grounding: separate ground contact to mating connector shell and front panel, horizontal PCB mount, retention spring instead of latch, https://www.neutrik.com/en/product/nc3fah2-0
neutrik xlr a
0
4
4
Connector_Audio
Jack_XLR_Neutrik_NC3FAH2-DA_Horizontal
A Series, 3 pole female XLR receptacle, grounding: separate ground contact to mating connector shell and front panel, horizontal PCB mount, asymmetric push, https://www.neutrik.com/en/product/nc3fah2-da
neutrik xlr a
0
4
4
Connector_Audio
Jack_XLR_Neutrik_NC3FAH2_Horizontal
A Series, 3 pole female XLR receptacle, grounding: separate ground contact to mating connector shell and front panel, horizontal PCB mount, https://www.neutrik.com/en/product/nc3fah2
neutrik xlr a
0
4
4
Connector_Audio
Jack_XLR_Neutrik_NC3FAHL-0_Horizontal
A Series, 3 pole female XLR receptacle, grounding: without ground/shell contact, lateral left PCB mount, retention spring instead of latch, https://www.neutrik.com/en/product/nc3fahl-0
neutrik xlr a
0
3
3
Connector_Audio
Jack_XLR_Neutrik_NC3FAHL1-0_Horizontal
A Series, 3 pole female XLR receptacle, grounding: mating connector shell to pin1 and front panel, lateral left PCB mount, retention spring instead of latch, https://www.neutrik.com/en/product/nc3fahl1-0
neutrik xlr a
0
3
3
Connector_Audio
Jack_XLR_Neutrik_NC3FAHL1_Horizontal
A Series, 3 pole female XLR receptacle, grounding: mating connector shell to pin1 and front panel, lateral left PCB mount, https://www.neutrik.com/en/product/nc3fahl1
neutrik xlr a
0
3
3
Connector_Audio
Jack_XLR_Neutrik_NC3FAHR-0_Horizontal
A Series, 3 pole female XLR receptacle, grounding: without ground / shell contact, lateral right PCB mount, retention spring instead of latch, https://www.neutrik.com/en/product/nc3fahr-0
neutrik xlr a
0
3
3
Connector_Audio
Jack_XLR_Neutrik_NC3FAHR1-0_Horizontal
A Series, 3 pole female XLR receptacle, grounding: mating connector shell to pin1 and front panel, lateral right PCB mount, retention spring instead of latch, https://www.neutrik.com/en/product/nc3fahr1-0
neutrik xlr a
0
3
3
Connector_Audio
Jack_XLR_Neutrik_NC3FAHR1_Horizontal
A Series, 3 pole female XLR receptacle, grounding: mating connector shell to pin1 and front panel, lateral right PCB mount, https://www.neutrik.com/en/product/nc3fahr1
neutrik xlr a
0
3
3
Connector_Audio
Jack_XLR_Neutrik_NC3FAHR2-0_Horizontal
A Series, 3 pole female XLR receptacle, grounding: separate ground contact to mating connector shell and front panel, lateral right PCB mount, retention spring instead of latch, https://www.neutrik.com/en/product/nc3fahr2-0
neutrik xlr a
0
4
4
Connector_Audio
Jack_XLR_Neutrik_NC3FAHR2_Horizontal
A Series, 3 pole female XLR receptacle, grounding: separate ground contact to mating connector shell and front panel, lateral right PCB mount, https://www.neutrik.com/en/product/nc3fahr2
neutrik xlr a
0
4
4
Connector_Audio
Jack_XLR_Neutrik_NC3FAH_Horizontal
A Series, 3 pole female XLR receptacle, grounding: without ground/shell contact, horizontal PCB mount, https://www.neutrik.com/en/product/nc3fah
neutrik xlr a
0
3
3
Connector_Audio
Jack_XLR_Neutrik_NC3FAV-0_Vertical
A Series, 3 pole female XLR receptacle, grounding: without ground / shell contact, vertical PCB mount, retention spring instead of latch, https://www.neutrik.com/en/product/nc3fav-0
neutrik xlr a
0
3
3
Connector_Audio
Jack_XLR_Neutrik_NC3FAV1-0_Vertical
A Series, 3 pole female XLR receptacle, grounding: mating connector shell to pin1 and front panel, vertical PCB mount, retention spring instead of latch, https://www.neutrik.com/en/product/nc3fav1-0
neutrik xlr a
0
3
3
Connector_Audio
Jack_XLR_Neutrik_NC3FAV1-DA_Vertical
A Series, 3 pole female XLR receptacle, grounding: mating connector shell to pin1 and front panel, vertical PCB mount, asymmetric push, https://www.neutrik.com/en/product/nc3fav1-da
neutrik xlr a
0
3
3
Connector_Audio
Jack_XLR_Neutrik_NC3FAV1_Vertical
A Series, 3 pole female XLR receptacle, grounding: mating connector shell to pin1 and front panel, vertical PCB mount, https://www.neutrik.com/en/product/nc3fav1
neutrik xlr a
0
3
3
Connector_Audio
Jack_XLR_Neutrik_NC3FAV2-0_Vertical
A Series, 3 pole female XLR receptacle, grounding: separate ground contact to mating connector shell and front panel, vertical PCB mount, retention spring instead of latch, https://www.neutrik.com/en/product/nc3fav2-0
neutrik xlr a
0
4
4
Connector_Audio
Jack_XLR_Neutrik_NC3FAV2-DA_Vertical
A Series, 3 pole female XLR receptacle, grounding: separate ground contact to mating connector shell and front panel, vertical PCB mount, asymmetric push, https://www.neutrik.com/en/product/nc3fav2-da
neutrik xlr a
0
4
4
Connector_Audio
Jack_XLR_Neutrik_NC3FAV2_Vertical
A Series, 3 pole female XLR receptacle, grounding: separate ground contact to mating connector shell and front panel, vertical PCB mount, https://www.neutrik.com/en/product/nc3fav2
neutrik xlr a
0
4
4
Connector_Audio
Jack_XLR_Neutrik_NC3FAV_Vertical
A Series, 3 pole female XLR receptacle, grounding: without ground / shell contact, vertical PCB mount, https://www.neutrik.com/en/product/nc3fav
neutrik xlr a
0
3
3
Connector_Audio
Jack_XLR_Neutrik_NC3FBH1-B_Horizontal
B Series, 3 pole female XLR receptacle, grounding: mating connector shell to pin1 and front panel, horizontal PCB mount, black chrome shell, https://www.neutrik.com/en/product/nc3fbh1-b
neutrik xlr b
0
3
3
Connector_Audio
Jack_XLR_Neutrik_NC3FBH1-DA_Horizontal
B Series, 3 pole female XLR receptacle, grounding: mating connector shell to pin1 and front panel, horizontal PCB mount, asymmetric push, https://www.neutrik.com/en/product/nc3fbh1-da
neutrik xlr b
0
3
3
Connector_Audio
Jack_XLR_Neutrik_NC3FBH1-E_Horizontal
B Series, 3 pole female XLR receptacle, grounding: mating connector shell to pin1 and front panel, horizontal PCB mount, additional ground contacts, https://www.neutrik.com/en/product/nc3fbh1-e
neutrik xlr b
0
3
3
Connector_Audio
Jack_XLR_Neutrik_NC3FBH1_Horizontal
B Series, 3 pole female XLR receptacle, grounding: mating connector shell to pin1 and front panel, horizontal PCB mount, https://www.neutrik.com/en/product/nc3fbh1
neutrik xlr b
0
3
3
Connector_Audio
Jack_XLR_Neutrik_NC3FBH2-B_Horizontal
B Series, 3 pole female XLR receptacle, grounding: separate ground contact to mating connector shell and front panel, horizontal PCB mount, black chrome shell, https://www.neutrik.com/en/product/nc3fbh2-b
neutrik xlr b
0
4
4
Connector_Audio
Jack_XLR_Neutrik_NC3FBH2-DA_Horizontal
B Series, 3 pole female XLR receptacle, grounding: separate ground contact to mating connector shell and front panel, horizontal PCB mount, asymmetric push, https://www.neutrik.com/en/product/nc3fbh2-da
neutrik xlr b
0
4
4
Connector_Audio
Jack_XLR_Neutrik_NC3FBH2-E_Horizontal
B Series, 3 pole female XLR receptacle, grounding: separate ground contact to mating connector shell and front panel, horizontal PCB mount, additional ground contacts, https://www.neutrik.com/en/product/nc3fbh2-e
neutrik xlr b
0
4
4
Connector_Audio
Jack_XLR_Neutrik_NC3FBH2_Horizontal
B Series, 3 pole female XLR receptacle, grounding: separate ground contact to mating connector shell and front panel, horizontal PCB mount, https://www.neutrik.com/en/product/nc3fbh2
neutrik xlr b
0
4
4
Connector_Audio
Jack_XLR_Neutrik_NC3FBHL1_Horizontal
B Series, 3 pole female XLR receptacle, grounding: mating connector shell to pin1 and front panel, lateral left PCB mount, https://www.neutrik.com/en/product/nc3fbhl1
neutrik xlr b
0
3
3
Connector_Audio
Jack_XLR_Neutrik_NC3FBV1-0_Vertical
B Series, 3 pole female XLR receptacle, grounding: mating connector shell to pin1 and front panel, vertical PCB mount, retention spring, no latch, https://www.neutrik.com/en/product/nc3fbv1-0
neutrik xlr b
0
3
3
Connector_Audio
Jack_XLR_Neutrik_NC3FBV1-B_Vertical
B Series, 3 pole female XLR receptacle, grounding: mating connector shell to pin1 and front panel, vertical PCB mount, black chrome shell, https://www.neutrik.com/en/product/nc3fbv1-b
neutrik xlr b
0
3
3
Connector_Audio
Jack_XLR_Neutrik_NC3FBV1-DA_Vertical
B Series, 3 pole female XLR receptacle, grounding: mating connector shell to pin1 and front panel, vertical PCB mount, asymmetric push, https://www.neutrik.com/en/product/nc3fbv1-da
neutrik xlr b
0
3
3
Connector_Audio
Jack_XLR_Neutrik_NC3FBV1_Vertical
B Series, 3 pole female XLR receptacle, grounding: mating connector shell to pin1 and front panel, vertical PCB mount, https://www.neutrik.com/en/product/nc3fbv1
neutrik xlr b
0
3
3
Connector_Audio
Jack_XLR_Neutrik_NC3FBV2-B_Vertical
B Series, 3 pole female XLR receptacle, grounding: separate ground contact to mating connector shell and front panel, vertical PCB mount, black chrome shell, https://www.neutrik.com/en/product/nc3fbv2-b
neutrik xlr b
0
4
4
Connector_Audio
Jack_XLR_Neutrik_NC3FBV2-DA_Vertical
B Series, 3 pole female XLR receptacle, grounding: separate ground contact to mating connector shell and front panel, vertical PCB mount, asymmetric push, https://www.neutrik.com/en/product/nc3fbv2-da
neutrik xlr b
0
4
4
Connector_Audio
Jack_XLR_Neutrik_NC3FBV2-SW_Vertical
B Series, 3 pole female XLR receptacle, switching contacts, grounding: separate ground contact to mating connector shell and front panel, vertical PCB mount, https://www.neutrik.com/en/product/nc3fbv2-sw
neutrik xlr b
0
7
7
Connector_Audio
Jack_XLR_Neutrik_NC3FBV2_Vertical
B Series, 3 pole female XLR receptacle, grounding: separate ground contact to mating connector shell and front panel, vertical PCB mount, https://www.neutrik.com/en/product/nc3fbv2
neutrik xlr b
0
4
4
Connector_Audio
Jack_XLR_Neutrik_NC3MAAH-0_Horizontal
AA Series, 3 pole male XLR receptacle, grounding: ground contact connected to shell ground, but not to front panel and Pin 1, horizontal PCB mount, https://www.neutrik.com/en/product/nc3maah-0
neutrik xlr aa
0
4
4
Connector_Audio
Jack_XLR_Neutrik_NC3MAAH-1_Horizontal
AA Series, 3 pole male XLR receptacle, grounding: mating connector shell to pin1 and front panel, horizontal PCB mount, https://www.neutrik.com/en/product/nc3maah-1
neutrik xlr aa
0
3
3
Connector_Audio
Jack_XLR_Neutrik_NC3MAAH_Horizontal
AA Series, 3 pole male XLR receptacle, grounding: separate ground contact to mating connector shell and front panel, horizontal PCB mount, https://www.neutrik.com/en/product/nc3maah
neutrik xlr aa
0
4
4
Connector_Audio
Jack_XLR_Neutrik_NC3MAAV-0_Vertical
AA Series, 3 pole male XLR receptacle, grounding: ground contact connected to shell ground, but not to front panel and Pin 1, vertical PCB mount, https://www.neutrik.com/en/product/nc3maav-0
neutrik xlr aa
0
4
4
Connector_Audio
Jack_XLR_Neutrik_NC3MAAV-1_Vertical
AA Series, 3 pole male XLR receptacle, grounding: mating connector shell to pin1 and front panel, vertical PCB mount, https://www.neutrik.com/en/product/nc3maav-1
neutrik xlr aa
0
3
3
Connector_Audio
Jack_XLR_Neutrik_NC3MAAV_Vertical
AA Series, 3 pole male XLR receptacle, grounding: separate ground contact to mating connector shell and front panel, vertical PCB mount, https://www.neutrik.com/en/product/nc3maav
neutrik xlr aa
0
4
4
Connector_Audio
Jack_XLR_Neutrik_NC3MAFH-PH_Horizontal
A Series, Chassis connector H female (A series layout), mates with Phoenix MSTB2,5/3-ST, horizontal PCB mount, https://www.neutrik.com/en/product/nc3mafh-ph
neutrik xlr a
0
3
3
Connector_Audio
Jack_XLR_Neutrik_NC3MAH-0_Horizontal
A Series, 3 pole male XLR receptacle, grounding: ground contact connected to shell ground, but not to front panel and Pin 1, horizontal PCB mount, https://www.neutrik.com/en/product/nc3mah-0
neutrik xlr a
0
4
4
Connector_Audio
Jack_XLR_Neutrik_NC3MAHL_Horizontal
A Series, 3 pole male XLR receptacle, grounding: separate ground contact to mating connector shell and front panel, lateral left PCB mount, https://www.neutrik.com/en/product/nc3mahl
neutrik xlr a
0
4
4
Connector_Audio
Jack_XLR_Neutrik_NC3MAHR_Horizontal
A Series, 3 pole male XLR receptacle, grounding: separate ground contact to mating connector shell and front panel, lateral right PCB mount, https://www.neutrik.com/en/product/nc3mahr
neutrik xlr a
0
4
4
Connector_Audio
Jack_XLR_Neutrik_NC3MAH_Horizontal
A Series, 3 pole male XLR receptacle, grounding: separate ground contact to mating connector shell and front panel, horizontal PCB mount, https://www.neutrik.com/en/product/nc3mah
neutrik xlr a
0
4
4
Connector_Audio
Jack_XLR_Neutrik_NC3MAMH-PH_Horizontal
A Series, Chassis connector Phoenix H male (A series layout), mates with Phoenix MSTB 2,5/3-ST, horizontal PCB mount, https://www.neutrik.com/en/product/nc3mamh-ph
neutrik xlr a
0
3
3
Connector_Audio
Jack_XLR_Neutrik_NC3MAV-0_Vertical
A Series, 3 pole male XLR receptacle, grounding: ground contact connected to shell ground, but not to front panel and Pin 1, vertical PCB mount, https://www.neutrik.com/en/product/nc3mav-0
neutrik xlr a
0
4
4
Connector_Audio
Jack_XLR_Neutrik_NC3MAV_Vertical
A Series, 3 pole male XLR receptacle, grounding: separate ground contact to mating connector shell and front panel, vertical PCB mount, https://www.neutrik.com/en/product/nc3mav
neutrik xlr a
0
4
4
Connector_Audio
Jack_XLR_Neutrik_NC3MBH-0_Horizontal
B Series, 3 pole male XLR receptacle, grounding: ground contact connected to shell ground, but not to front panel and Pin 1, steel retention lug, horizontal PCB mount, https://www.neutrik.com/en/product/nc3mbh-0
neutrik xlr b
0
4
4
Connector_Audio
Jack_XLR_Neutrik_NC3MBH-1_Horizontal
B Series, 3 pole male XLR receptacle, grounding: mating connector shell to pin1 and front panel, steel retention lug, horizontal PCB mount, https://www.neutrik.com/en/product/nc3mbh-1
neutrik xlr b
0
3
3
Connector_Audio
Jack_XLR_Neutrik_NC3MBH-B_Horizontal
B Series, 3 pole male XLR receptacle, grounding: separate ground contact to mating connector shell and front panel, steel retention lug, horizontal PCB mount, black chrome shell, https://www.neutrik.com/en/product/nc3mbh-b
neutrik xlr b
0
4
4
Connector_Audio
Jack_XLR_Neutrik_NC3MBH-E_Horizontal
B Series, 3 pole male XLR receptacle, grounding: separate ground contact to mating connector shell and front panel, steel retention lug, horizontal PCB mount, additional ground contacts, https://www.neutrik.com/en/product/nc3mbh-e
neutrik xlr b
0
4
4
Connector_Audio
Jack_XLR_Neutrik_NC3MBHL-B_Horizontal
B Series, 3 pole male XLR receptacle, grounding: separate ground contact to mating connector shell and front panel, steel retention lug, lateral left PCB mount, black chrome shell, https://www.neutrik.com/en/product/nc3mbhl-b
neutrik xlr b
0
4
4
Connector_Audio
Jack_XLR_Neutrik_NC3MBHL_Horizontal
B Series, 3 pole male XLR receptacle, grounding: separate ground contact to mating connector shell and front panel, steel retention lug, lateral left PCB mount, https://www.neutrik.com/en/product/nc3mbhl
neutrik xlr b
0
4
4
Connector_Audio
Jack_XLR_Neutrik_NC3MBHR-B_Horizontal
B Series, 3 pole male XLR receptacle, grounding: separate ground contact to mating connector shell and front panel, steel retention lug, lateral right PCB mount, black chrome shell, https://www.neutrik.com/en/product/nc3mbhr-b
neutrik xlr b
0
4
4
Connector_Audio
Jack_XLR_Neutrik_NC3MBHR_Horizontal
B Series, 3 pole male XLR receptacle, grounding: separate ground contact to mating connector shell and front panel, steel retention lug, lateral right PCB mount, https://www.neutrik.com/en/product/nc3mbhr
neutrik xlr b
0
4
4
Connector_Audio
Jack_XLR_Neutrik_NC3MBH_Horizontal
B Series, 3 pole male XLR receptacle, grounding: separate ground contact to mating connector shell and front panel, steel retention lug, horizontal PCB mount, https://www.neutrik.com/en/product/nc3mbh
neutrik xlr b
0
4
4
Connector_Audio
Jack_XLR_Neutrik_NC3MBV-0_Vertical
B Series, 3 pole male XLR receptacle, grounding: ground contact connected to shell ground, but not to front panel and Pin 1, steel retention lug, vertical PCB mount, https://www.neutrik.com/en/product/nc3mbv-0
neutrik xlr b
0
4
4
Connector_Audio
Jack_XLR_Neutrik_NC3MBV-1_Vertical
B Series, 3 pole male XLR receptacle, grounding: mating connector shell to pin1 and front panel, steel retention lug, vertical PCB mount, https://www.neutrik.com/en/product/nc3mbv-1
neutrik xlr b
0
3
3
Connector_Audio
Jack_XLR_Neutrik_NC3MBV-B_Vertical
B Series, 3 pole male XLR receptacle, grounding: separate ground contact to mating connector shell and front panel, steel retention lug, vertical PCB mount, black chrome shell, https://www.neutrik.com/en/product/nc3mbv-b
neutrik xlr b
0
4
4
Connector_Audio
Jack_XLR_Neutrik_NC3MBV-E_Vertical
B Series, 3 pole male XLR receptacle, grounding: separate ground contact to mating connector shell and front panel, steel retention lug, vertical PCB mount, additional ground contacts, https://www.neutrik.com/en/product/nc3mbv-e
neutrik xlr b
0
4
4
Connector_Audio
Jack_XLR_Neutrik_NC3MBV-SW_Vertical
B Series, 3 pole male XLR receptacle, switching contacts, grounding: separate ground contact to mating connector shell and front panel, vertical PCB mount, https://www.neutrik.com/en/product/nc3mbv-sw
neutrik xlr b
0
7
7
Connector_Audio
Jack_XLR_Neutrik_NC3MBV_Vertical
B Series, 3 pole male XLR receptacle, grounding: separate ground contact to mating connector shell and front panel, steel retention lug, vertical PCB mount, https://www.neutrik.com/en/product/nc3mbv
neutrik xlr b
0
4
4
Connector_Audio
Jack_XLR_Neutrik_NC4FAH-0_Horizontal
A Series, 4 pole female XLR receptacle, grounding: separate ground contact to mating connector shell and front panel, horizontal PCB mount, retention spring instead of latch, https://www.neutrik.com/en/product/nc4fah-0
neutrik xlr a
0
5
5
Connector_Audio
Jack_XLR_Neutrik_NC4FAH_Horizontal
A Series, 4 pole female XLR receptacle, grounding: separate ground contact to mating connector shell and front panel, horizontal PCB mount, https://www.neutrik.com/en/product/nc4fah
neutrik xlr a
0
5
5
Connector_Audio
Jack_XLR_Neutrik_NC4FAV-0_Vertical
A Series, 4 pole female XLR receptacle, grounding: separate ground contact to mating connector shell and front panel, vertical PCB mount, retention spring instead of latch, https://www.neutrik.com/en/product/nc4fav-0
neutrik xlr a
0
5
5
Connector_Audio
Jack_XLR_Neutrik_NC4FAV_Vertical
A Series, 4 pole female XLR receptacle, grounding: separate ground contact to mating connector shell and front panel, vertical PCB mount, https://www.neutrik.com/en/product/nc4fav
neutrik xlr a
0
5
5
Connector_Audio
Jack_XLR_Neutrik_NC4FBH_Horizontal
B Series, 4 pole female XLR receptacle, grounding: separate ground contact to mating connector shell and front panel, horizontal PCB mount, https://www.neutrik.com/en/product/nc4fbh
neutrik xlr b
0
5
5
Connector_Audio
Jack_XLR_Neutrik_NC4FBV_Vertical
B Series, 4 pole female XLR receptacle, grounding: separate ground contact to mating connector shell and front panel, vertical PCB mount, https://www.neutrik.com/en/product/nc4fbv
neutrik xlr b
0
5
5
Connector_Audio
Jack_XLR_Neutrik_NC4MAH_Horizontal
A Series, 4 pole male XLR receptacle, grounding: separate ground contact to mating connector shell and front panel, horizontal PCB mount, https://www.neutrik.com/en/product/nc4mah
neutrik xlr a
0
5
5
Connector_Audio
Jack_XLR_Neutrik_NC4MAV_Vertical
A Series, 4 pole male XLR receptacle, grounding: separate ground contact to mating connector shell and front panel, vertical PCB mount, https://www.neutrik.com/en/product/nc4mav
neutrik xlr a
0
5
5
Connector_Audio
Jack_XLR_Neutrik_NC4MBH_Horizontal
B Series, 4 pole male XLR receptacle, grounding: separate ground contact to mating connector shell and front panel, horizontal PCB mount, https://www.neutrik.com/en/product/nc4mbh
neutrik xlr b
0
5
5
Connector_Audio
Jack_XLR_Neutrik_NC4MBV_Vertical
B Series, 4 pole male XLR receptacle, grounding: separate ground contact to mating connector shell and front panel, vertical PCB mount, https://www.neutrik.com/en/product/nc4mbv
neutrik xlr b
0
5
5
Connector_Audio
Jack_XLR_Neutrik_NC5FAH-0_Horizontal
A Series, 5 pole female XLR receptacle, grounding: separate ground contact to mating connector shell and front panel, horizontal PCB mount, retention spring instead of latch, https://www.neutrik.com/en/product/nc5fah-0
neutrik xlr a
0
6
6
Connector_Audio
Jack_XLR_Neutrik_NC5FAH-DA_Horizontal
A Series, 5 pole female XLR receptacle, grounding: mating connector shell to pin1 and front panel, horizontal PCB mount, asymmetric push, https://www.neutrik.com/en/product/nc5fah-da
neutrik xlr a
0
6
6
Connector_Audio
Jack_XLR_Neutrik_NC5FAH_Horizontal
A Series, 5 pole female XLR receptacle, grounding: separate ground contact to mating connector shell and front panel, horizontal PCB mount, https://www.neutrik.com/en/product/nc5fah
neutrik xlr a
0
6
6
Connector_Audio
Jack_XLR_Neutrik_NC5FAV-DA_Vertical
A Series, 5 pole female XLR receptacle, grounding: mating connector shell to pin1 and front panel, horizontal PCB mount, asymmetric push, https://www.neutrik.com/en/product/nc5fav-da
neutrik xlr a
0
6
6
Connector_Audio
Jack_XLR_Neutrik_NC5FAV-SW_Vertical
A Series, 5 pole female XLR receptacle, switching contacts, grounding: separate ground contact to mating connector shell and front panel, vertical PCB mount, color coding possible, https://www.neutrik.com/en/product/nc5fav-sw
neutrik xlr a
0
9
9
Connector_Audio
Jack_XLR_Neutrik_NC5FAV_Vertical
A Series, 5 pole female XLR receptacle, grounding: separate ground contact to mating connector shell and front panel, vertical PCB mount, https://www.neutrik.com/en/product/nc5fav
neutrik xlr a
0
6
6
Connector_Audio
Jack_XLR_Neutrik_NC5FBH-B_Horizontal
B Series, 5 pole female XLR receptacle, grounding: separate ground contact to mating connector shell and front panel, horizontal PCB mount, black chrome shell, https://www.neutrik.com/en/product/nc5fbh-b
neutrik xlr b
0
6
6
Connector_Audio
Jack_XLR_Neutrik_NC5FBH_Horizontal
B Series, 5 pole female XLR receptacle, grounding: separate ground contact to mating connector shell and front panel, horizontal PCB mount, https://www.neutrik.com/en/product/nc5fbh
neutrik xlr b
0
6
6
Connector_Audio
Jack_XLR_Neutrik_NC5FBV-B_Vertical
B Series, 5 pole female XLR receptacle, grounding: separate ground contact to mating connector shell and front panel, vertical PCB mount, black chrome shell, https://www.neutrik.com/en/product/nc5fbv-b
neutrik xlr b
0
6
6
Connector_Audio
Jack_XLR_Neutrik_NC5FBV-SW_Vertical
B Series, 5 pole female XLR receptacle, switching contacts, grounding: separate ground contact to mating connector shell and front panel, vertical PCB mount, https://www.neutrik.com/en/product/nc5fbv-sw
neutrik xlr b
0
9
9
Connector_Audio
Jack_XLR_Neutrik_NC5FBV_Vertical
B Series, 5 pole female XLR receptacle, grounding: separate ground contact to mating connector shell and front panel, vertical PCB mount, https://www.neutrik.com/en/product/nc5fbv
neutrik xlr b
0
6
6
Connector_Audio
Jack_XLR_Neutrik_NC5MAH_Horizontal
A Series, 5 pole male XLR receptacle, grounding: separate ground contact to mating connector shell and front panel, horizontal PCB mount, https://www.neutrik.com/en/product/nc5mah
neutrik xlr a
0
6
6
Connector_Audio
Jack_XLR_Neutrik_NC5MAV-SW_Vertical
A Series, 5 pole male XLR receptacle, switching contacts, grounding: separate ground contact to mating connector shell and front panel, vertical PCB mount, https://www.neutrik.com/en/product/nc5mav-sw
neutrik xlr a
0
9
9
Connector_Audio
Jack_XLR_Neutrik_NC5MAV_Vertical
A Series, 5 pole male XLR receptacle, grounding: separate ground contact to mating connector shell and front panel, vertical PCB mount, https://www.neutrik.com/en/product/nc5mav
neutrik xlr a
0
6
6
Connector_Audio
Jack_XLR_Neutrik_NC5MBH-B_Horizontal
B Series, 5 pole male XLR receptacle, grounding: separate ground contact to mating connector shell and front panel, horizontal PCB mount, black chrome shell, https://www.neutrik.com/en/product/nc5mbh-b
neutrik xlr b
0
6
6
Connector_Audio
Jack_XLR_Neutrik_NC5MBH_Horizontal
B Series, 5 pole male XLR receptacle, grounding: separate ground contact to mating connector shell and front panel, horizontal PCB mount, https://www.neutrik.com/en/product/nc5mbh
neutrik xlr b
0
6
6
Connector_Audio
Jack_XLR_Neutrik_NC5MBV-B_Vertical
B Series, 5 pole male XLR receptacle, grounding: separate ground contact to mating connector shell and front panel, vertical PCB mount, black chrome shell, https://www.neutrik.com/en/product/nc5mbv-b
neutrik xlr b
0
6
6
Connector_Audio
Jack_XLR_Neutrik_NC5MBV-SW_Vertical
B Series, 5 pole male XLR receptacle, switching contacts, grounding: separate ground contact to mating connector shell and front panel, vertical PCB mount, https://www.neutrik.com/en/product/nc5mbv-sw
neutrik xlr b
0
9
9
Connector_Audio
Jack_XLR_Neutrik_NC5MBV_Vertical
B Series, 5 pole male XLR receptacle, grounding: separate ground contact to mating connector shell and front panel, vertical PCB mount, https://www.neutrik.com/en/product/nc5mbv
neutrik xlr b
0
6
6
Connector_Audio
Jack_speakON-6.35mm_Neutrik_NLJ2MD-H_Horizontal
speakON Combo, 2 pole combination of speakON socket and 6.35mm (1/4in) jack receptacle, horizontal pcb mount, https://www.neutrik.com/en/product/nlj2md-h
neutrik speakon combo
0
2
2
Connector_Audio
Jack_speakON-6.35mm_Neutrik_NLJ2MD-V_Vertical
speakON Combo, 2 pole combination of speakON socket and 6.35mm (1/4in) jack receptacle, vertical pcb mount, https://www.neutrik.com/en/product/nlj2md-v
neutrik speakon combo
0
2
2
Connector_Audio
Jack_speakON_Neutrik_NL2MD-H_Horizontal
speakON Chassis Connectors, 2 pole chassis connector, gray D-size flange, countersunk thru holes, horizontal PCB, https://www.neutrik.com/en/product/nl2md-h
neutrik speakon
0
2
2
Connector_Audio
Jack_speakON_Neutrik_NL2MD-V_Vertical
speakON Chassis Connectors, 2 pole chassis connector, black D-size flange, countersunk thru holes, vertical PCB mount, https://www.neutrik.com/en/product/nl2md-v
neutrik speakon
0
2
2
Connector_Audio
Jack_speakON_Neutrik_NL4MD-H-1_Horizontal
speakON Chassis Connectors, 4 pole chassis connector, black D-size flange, countersunk thru holes, horizontal PCB mount, https://www.neutrik.com/en/product/nl4md-h-1
neutrik speakon
0
4
4
Connector_Audio
Jack_speakON_Neutrik_NL4MD-H-2_Horizontal
speakON Chassis Connectors, 4 pole chassis connector, black D-size flange, mirrored self tapping screw holes (A-screw), horizontal PCB mount, https://www.neutrik.com/en/product/nl4md-h-2
neutrik speakon
0
4
4
Connector_Audio
Jack_speakON_Neutrik_NL4MD-H-3_Horizontal
speakON Chassis Connectors, 4 pole chassis connector, black D-size flange, self tapping screw holes (A-screw), horizontal PCB mount, https://www.neutrik.com/en/product/nl4md-h-3
neutrik speakon
0
4
4
Connector_Audio
Jack_speakON_Neutrik_NL4MD-H_Horizontal
speakON Chassis Connectors, 4 pole chassis connector, grey D-size flange, self tapping screw holes (A-screw), horizontal PCB mount, https://www.neutrik.com/en/product/nl4md-h
neutrik speakon
0
4
4
Connector_Audio
Jack_speakON_Neutrik_NL4MD-V-1_Vertical
speakON Chassis Connectors, 4 pole chassis connector, grey D-size flange, self tapping screw holes (A-screw), vertical PCB mount, https://www.neutrik.com/en/product/nl4md-v-1
neutrik speakon
0
4
4
Connector_Audio
Jack_speakON_Neutrik_NL4MD-V-2_Vertical
speakON Chassis Connectors, 4 pole chassis connector, black D-size flange, mirrored self tapping screw holes (A-screw), vertical PCB mount, https://www.neutrik.com/en/product/nl4md-v-2
neutrik speakon
0
4
4
Connector_Audio
Jack_speakON_Neutrik_NL4MD-V-R_Vertical
speakON Chassis Connectors, 4 pole chassis connector, red D-size flange, countersunk thru holes, vertical PCB mount, https://www.neutrik.com/en/product/nl4md-v-r
neutrik speakon
0
4
4
Connector_Audio
Jack_speakON_Neutrik_NL4MD-V-S_Vertical
speakON Chassis Connectors, 4 pole chassis connector, black D-size flange, switchable version of NL4MD-V with 8 vertical PCB contacts (4 switching contacts), https://www.neutrik.com/en/product/nl4md-v-s
neutrik speakon
0
8
8
Connector_Audio
Jack_speakON_Neutrik_NL4MD-V_Vertical
speakON Chassis Connectors, 4 pole chassis connector, black D-size flange, countersunk thru holes, vertical PCB mount, https://www.neutrik.com/en/product/nl4md-v
neutrik speakon
0
4
4
Connector_Audio
Jack_speakON_Neutrik_NL8MD-V-1_Vertical
speakON Chassis Connectors, 8 pole chassis connector, nickel metal square G-size flange, self tapping screw holes (A-screw), vertical PCB mount, https://www.neutrik.com/en/product/nl8md-v-1
neutrik speakon
0
8
8
Connector_Audio
Jack_speakON_Neutrik_NL8MD-V_Vertical
speakON Chassis Connectors, 8 pole chassis connector, nickel metal square G-size flange, countersunk thru holes, vertical PCB mount, https://www.neutrik.com/en/product/nl8md-v
neutrik speakon
0
8
8
Connector_Audio
Jack_speakON_Neutrik_NLT4MD-V_Vertical
STX Series, 4 pole male chassis connector, metal housing, vertical PCB mount,  self tapping screw holes (A-screw), https://www.neutrik.com/en/product/nlt4md-v
neutrik speakon stx
0
4
4
Connector_Audio
MiniXLR-5_Switchcraft_TRAPC_Horizontal
http://www.switchcraft.com/ProductSummary.aspx?Parent=620 http://www.switchcraft.com/Drawings/TRAPC_X-TRASM_X_SERIES_CD.PDF
THT Mini XLR 5Pin right angle
0
5
5
Connector_BarrelJack
BarrelJack_CLIFF_FC681465S_SMT_Horizontal
Surface-mount DC Barrel Jack, https://www.cliffuk.co.uk/products/dcconnectors/FC681465S.pdf
Power Jack SMT
0
4
3
Connector_BarrelJack
BarrelJack_CUI_PJ-036AH-SMT_Horizontal
Surface-mount DC Barrel Jack, http://www.cui.com/product/resource/pj-036ah-smt.pdf
Power Jack SMT
0
3
3
Connector_BarrelJack
BarrelJack_CUI_PJ-063AH_Horizontal
Barrel Jack, 2.0mm ID, 5.5mm OD, 24V, 8A, no switch, https://www.cui.com/product/resource/pj-063ah.pdf
barrel jack cui dc power
0
4
3
Connector_BarrelJack
BarrelJack_CUI_PJ-063AH_Horizontal_CircularHoles
Barrel Jack, 2.0mm ID, 5.5mm OD, 24V, 8A, no switch, https://www.cui.com/product/resource/pj-063ah.pdf
barrel jack cui dc power
0
4
3
Connector_BarrelJack
BarrelJack_CUI_PJ-102AH_Horizontal
Thin-pin DC Barrel Jack, https://cdn-shop.adafruit.com/datasheets/21mmdcjackDatasheet.pdf
Power Jack
0
3
3
Connector_BarrelJack
BarrelJack_GCT_DCJ200-10-A_Horizontal
Barrel jack connector (5.5 mm outer diameter, 2.05 inner diameter ), https://gct.co/files/drawings/dcj200-10.pdf
connector barrel jack
0
3
3
Connector_BarrelJack
BarrelJack_Horizontal
DC Barrel Jack
Power Jack
0
3
3
Connector_BarrelJack
BarrelJack_Kycon_KLDX-0202-xC_Horizontal
DC Barrel Jack 2mm or 2.5mm center pin, https://www.kycon.com/Pub_Eng_Draw/KLDX-0202-AC%20&%20BC.pdf
power jack 2mm 2.5mm KLDX-0202-BC KLDX-0202-AC
0
3
3
Connector_BarrelJack
BarrelJack_SwitchcraftConxall_RAPC10U_Horizontal
DC Power Jack, 13A, 24V, Panel Mount,Through-hole, https://www.switchcraft.com/Drawings/RAPC10U_CD.pdf
barreljack switchcraftconxall dc power
0
2
2
Connector_BarrelJack
BarrelJack_Wuerth_6941xx301002
Wuerth electronics barrel jack connector (5.5mm outher diameter, inner diameter 2.05mm or 2.55mm depending on exact order number), See: http://katalog.we-online.de/em/datasheet/6941xx301002.pdf
connector barrel jack
0
3
3
Connector_Card
CF-Card_3M_N7E50-A516xx-30
Compact Flash Card connector, polarization inverse (https://multimedia.3m.com/mws/media/22424O/3mtm-cf-card-header-type-i-low-profile-surface-mount-ts0747.pdf)
connector cf
0
54
50
Connector_Card
CF-Card_3M_N7E50-E516xx-30
Compact Flash Card connector, normal polarization (https://multimedia.3m.com/mws/media/22424O/3mtm-cf-card-header-type-i-low-profile-surface-mount-ts0747.pdf)
connector cf
0
54
50
Connector_Card
SD_Hirose_DM1AA_SF_PEJ82
SD, SMD, top-mount, push-push (https://www.hirose.com/product/document?clcode=CL0609-0004-8-82&productname=DM1AA-SF-PEJ(82)&series=DM1&documenttype=2DDrawing&lang=en&documentid=0000915301)
SD card connector
0
16
13
Connector_Card
SD_Kyocera_145638009211859+
SD Card Connector, Normal Type, Outer Tail, Without Ejector (https://global.kyocera.com/prdct/electro/product/pdf/5638.pdf)
sd card smt
0
13
13
Connector_Card
SD_Kyocera_145638009511859+
SD Card Connector, Normal Type, Outer Tail, Spring Eject Type (https://global.kyocera.com/prdct/electro/product/pdf/5638.pdf)
sd card smt
0
13
13
Connector_Card
SD_Kyocera_145638109211859+
SD Card Connector, Reverse Type, Outer Tail, Without Ejector (https://global.kyocera.com/prdct/electro/product/pdf/5638.pdf)
sd card smt
0
13
13
Connector_Card
SD_Kyocera_145638109511859+
SD Card Connector, Reverse Type, Outer Tail, Spring Eject Type (https://global.kyocera.com/prdct/electro/product/pdf/5638.pdf)
sd card smt
0
13
13
Connector_Card
SD_TE_2041021
SD card connector, top mount, SMT (http://www.te.com/commerce/DocumentDelivery/DDEController?Action=showdoc&DocId=Customer+Drawing%7F2041021%7FB%7Fpdf%7FEnglish%7FENG_CD_2041021_B_C_2041021_B.pdf%7F2041021-4)
sd card
0
15
12
Connector_Card
microSD_HC_Hirose_DM3AT-SF-PEJM5
Micro SD, SMD, right-angle, push-pull (https://www.hirose.com/product/en/download_file/key_name/DM3AT-SF-PEJM5/category/Drawing%20(2D)/doc_file_id/44099/?file_category_id=6&item_id=06090031000&is_series=)
Micro SD
0
14
11
Connector_Card
microSD_HC_Hirose_DM3BT-DSF-PEJS
Micro SD, SMD, reverse on-board, right-angle, push-pull (https://www.hirose.com/product/en/download_file/key_name/DM3BT-DSF-PEJS/category/Drawing%20(2D)/doc_file_id/44097/?file_category_id=6&item_id=06090029900&is_series=)
Micro SD
0
16
11
Connector_Card
microSD_HC_Hirose_DM3D-SF
Micro SD, SMD, right-angle, push-pull (https://media.digikey.com/PDF/Data%20Sheets/Hirose%20PDFs/DM3D-SF.pdf)
Micro SD
0
14
11
Connector_Card
microSD_HC_Molex_47219-2001
1.10mm Pitch microSD Card Connector, Hinge Type, https://www.molex.com/pdm_docs/sd/472192001_sd.pdf
Micro SD
0
12
9
Connector_Card
microSD_HC_Molex_104031-0811
1.10mm Pitch microSD Memory Card Connector, Surface Mount, Push-Pull Type, 1.42mm Height, with Detect Switch (https://www.molex.com/pdm_docs/sd/1040310811_sd.pdf)
microSD SD molex
0
14
11
Connector_Card
microSD_HC_Wuerth_693072010801
http://katalog.we-online.de/em/datasheet/693072010801.pdf
Micro SD Wuerth Wurth Würth
0
12
9
Connector_Card
microSIM_JAE_SF53S006VCBR2000
https://www.jae.com/z-en/pdf_download_exec.cfm?param=SJ115712.pdf
microSIM GSM Card
0
14
7
Connector_Coaxial
BNC_Amphenol_031-6575_Horizontal
dual independently isolated BNC plug (https://www.amphenolrf.com/downloads/dl/file/id/2980/product/644/031_6575_customer_drawing.pdf)
Dual BNC Amphenol Horizontal
0
6
4
Connector_Coaxial
BNC_Amphenol_B6252HB-NPP3G-50_Horizontal
http://www.farnell.com/datasheets/612848.pdf
BNC Amphenol Horizontal
0
4
2
Connector_Coaxial
BNC_PanelMountable_Vertical
Panel-mountable BNC connector mounted through PCB, vertical
BNC connector
0
2
2
Connector_Coaxial
BNC_TEConnectivity_1478035_Horizontal
BNC RF Interface, PCB mount 4 pin, Right Angle, Bayonet, 50Ohm, 4GHz, https://www.te.com/commerce/DocumentDelivery/DDEController?Action=showdoc&DocId=Customer+Drawing%7F1478035%7FB1%7Fpdf%7FEnglish%7FENG_CD_1478035_B1.pdf%7F1-1478035-0
BNC RF interface bayonet 50ohm
0
5
2
Connector_Coaxial
BNC_TEConnectivity_1478204_Vertical
BNC female PCB mount 4 pin straight chassis connector http://www.te.com/usa-en/product-1-1478204-0.html
BNC female PCB mount 4 pin straight chassis connector 
0
5
2
Connector_Coaxial
BNC_Win_364A2x95_Horizontal
Dual front isolated BNC plug (https://www.winconn.com/wp-content/uploads/364A2595.pdf)
Dual BNC Horizontal Isolated
0
6
3
Connector_Coaxial
CoaxialSwitch_Hirose_MS-156C3_Horizontal
Subminiature Coaxial Switch 1.35mm High, DC to 11GHz
Switch Coaxial RF
0
12
3
Connector_Coaxial
MMCX_Molex_73415-0961_Horizontal_0.8mm-PCB
Molex MMCX Horizontal Coaxial https://www.molex.com/pdm_docs/sd/734150961_sd.pdf
Molex MMCX Horizontal Coaxial
0
3
2
Connector_Coaxial
MMCX_Molex_73415-0961_Horizontal_1.0mm-PCB
Molex MMCX Horizontal Coaxial https://www.molex.com/pdm_docs/sd/734150961_sd.pdf
Molex MMCX Horizontal Coaxial
0
3
2
Connector_Coaxial
MMCX_Molex_73415-0961_Horizontal_1.6mm-PCB
Molex MMCX Horizontal Coaxial https://www.molex.com/pdm_docs/sd/734150961_sd.pdf
Molex MMCX Horizontal Coaxial
0
3
2
Connector_Coaxial
MMCX_Molex_73415-1471_Vertical
http://www.molex.com/pdm_docs/sd/734151471_sd.pdf
Molex MMCX Coaxial Connector 50 ohms Female Jack Vertical THT
0
5
2
Connector_Coaxial
SMA_Amphenol_901-143_Horizontal
 Amphenol RF 901-143 https://www.amphenolrf.com/library/download/link/link_id/585682
SMA THT Female Jack Horizontal
0
5
2
Connector_Coaxial
SMA_Amphenol_901-144_Vertical
https://www.amphenolrf.com/downloads/dl/file/id/7023/product/3103/901_144_customer_drawing.pdf
SMA THT Female Jack Vertical
0
5
2
Connector_Coaxial
SMA_Amphenol_132134-10_Vertical
https://www.amphenolrf.com/downloads/dl/file/id/4007/product/2974/132134_10_customer_drawing.pdf
SMA SMD Female Jack Vertical
0
3
2
Connector_Coaxial
SMA_Amphenol_132134-11_Vertical
https://www.amphenolrf.com/downloads/dl/file/id/3406/product/2975/132134_11_customer_drawing.pdf
SMA THT Female Jack Vertical ExtendedLegs
0
5
2
Connector_Coaxial
SMA_Amphenol_132134-14_Vertical
https://www.amphenolrf.com/downloads/dl/file/id/1793/product/2976/132134_14_customer_drawing.pdf
SMA THT Female Jack Vertical ExtendedLegs
0
5
2
Connector_Coaxial
SMA_Amphenol_132134-16_Vertical
https://www.amphenolrf.com/downloads/dl/file/id/1141/product/2978/132134_16_customer_drawing.pdf
SMA THT Female Jack Vertical ExtendedLegs
0
5
2
Connector_Coaxial
SMA_Amphenol_132134_Vertical
https://www.amphenolrf.com/downloads/dl/file/id/2187/product/2843/132134_customer_drawing.pdf
SMA THT Female Jack Vertical ExtendedLegs
0
5
2
Connector_Coaxial
SMA_Amphenol_132203-12_Horizontal
https://www.amphenolrf.com/media/downloads/1769/132203-12.pdf
SMA THT Female Jack Horizontal
0
5
2
Connector_Coaxial
SMA_Amphenol_132289_EdgeMount
http://www.amphenolrf.com/132289.html
SMA
0
5
2
Connector_Coaxial
SMA_Amphenol_132291-12_Vertical
https://www.amphenolrf.com/downloads/dl/file/id/1688/product/3020/132291_12_customer_drawing.pdf
SMA THT Female Jack Vertical Bulkhead
0
5
2
Connector_Coaxial
SMA_Amphenol_132291_Vertical
https://www.amphenolrf.com/downloads/dl/file/id/3222/product/2918/132291_customer_drawing.pdf
SMA THT Female Jack Vertical Bulkhead
0
5
2
Connector_Coaxial
SMA_Molex_73251-1153_EdgeMount_Horizontal
Molex SMA RF Connectors, Edge Mount, (http://www.molex.com/pdm_docs/sd/732511150_sd.pdf)
sma edge
0
11
2
Connector_Coaxial
SMA_Molex_73251-2120_EdgeMount_Horizontal
Molex SMA RF Connector, Edge Mount, (http://www.molex.com/pdm_docs/sd/732512120_sd.pdf)
sma edge
0
11
2
Connector_Coaxial
SMA_Molex_73251-2200_Horizontal
https://www.molex.com/webdocs/datasheets/pdf/en-us/0732512200_RF_COAX_CONNECTORS.pdf
SMA THT Female Jack Horizontal
0
5
2
Connector_Coaxial
SMA_Samtec_SMA-J-P-X-ST-EM1_EdgeMount
Connector SMA, 0Hz to 20GHz, 50Ohm, Edge Mount (http://suddendocs.samtec.com/prints/sma-j-p-x-st-em1-mkt.pdf)
SMA Straight Samtec Edge Mount
0
5
2
Connector_Coaxial
SMA_Wurth_60312002114503_Vertical
https://www.we-online.de/katalog/datasheet/60312002114503.pdf
SMA THT Female Jack Vertical ExtendedLegs
0
5
2
Connector_Coaxial
SMB_Jack_Vertical
SMB pcb mounting jack
SMB Jack  Striaght
0
5
2
Connector_Coaxial
U.FL_Hirose_U.FL-R-SMT-1_Vertical
Hirose U.FL Coaxial https://www.hirose.com/product/en/products/U.FL/U.FL-R-SMT-1%2810%29/
Hirose U.FL Coaxial
0
3
2
Connector_Coaxial
U.FL_Molex_MCRF_73412-0110_Vertical
Molex Microcoaxial RF Connectors (MCRF), mates Hirose U.FL, (http://www.molex.com/pdm_docs/sd/734120110_sd.pdf)
mcrf hirose ufl u.fl microcoaxial
0
4
2
Connector_DIN
DIN41612_B2_2x8_Female_Vertical_THT
DIN41612 connector, type B/2, Vertical, 2 rows 16 pins wide, https://www.erni-x-press.com/de/downloads/kataloge/englische_kataloge/erni-din41612-iec60603-2-e.pdf
DIN 41612 IEC 60603 B/2
0
16
16
Connector_DIN
DIN41612_B2_2x8_Male_Horizontal_THT
DIN41612 connector, type B/2, Horizontal, 2 rows 16 pins wide, https://www.erni-x-press.com/de/downloads/kataloge/englische_kataloge/erni-din41612-iec60603-2-e.pdf
DIN 41612 IEC 60603 B/2
0
16
16
Connector_DIN
DIN41612_B2_2x16_Female_Vertical_THT
DIN41612 connector, type B/2, Vertical, 2 rows 16 pins wide, https://www.erni-x-press.com/de/downloads/kataloge/englische_kataloge/erni-din41612-iec60603-2-e.pdf
DIN 41612 IEC 60603 B/2
0
32
32
Connector_DIN
DIN41612_B2_2x16_Male_Horizontal_THT
DIN41612 connector, type B/2, Horizontal, 2 rows 16 pins wide, https://www.erni-x-press.com/de/downloads/kataloge/englische_kataloge/erni-din41612-iec60603-2-e.pdf
DIN 41612 IEC 60603 B/2
0
32
32
Connector_DIN
DIN41612_B3_2x5_Female_Vertical_THT
DIN41612 connector, type B/3, Vertical, 2 rows 10 pins wide, https://www.erni-x-press.com/de/downloads/kataloge/englische_kataloge/erni-din41612-iec60603-2-e.pdf
DIN 41612 IEC 60603 B/3
0
10
10
Connector_DIN
DIN41612_B3_2x5_Male_Horizontal_THT
DIN41612 connector, type B/3, Horizontal, 2 rows 10 pins wide, https://www.erni-x-press.com/de/downloads/kataloge/englische_kataloge/erni-din41612-iec60603-2-e.pdf
DIN 41612 IEC 60603 B/3
0
10
10
Connector_DIN
DIN41612_B3_2x10_Female_Vertical_THT
DIN41612 connector, type B/3, Vertical, 2 rows 10 pins wide, https://www.erni-x-press.com/de/downloads/kataloge/englische_kataloge/erni-din41612-iec60603-2-e.pdf
DIN 41612 IEC 60603 B/3
0
20
20
Connector_DIN
DIN41612_B3_2x10_Male_Horizontal_THT
DIN41612 connector, type B/3, Horizontal, 2 rows 10 pins wide, https://www.erni-x-press.com/de/downloads/kataloge/englische_kataloge/erni-din41612-iec60603-2-e.pdf
DIN 41612 IEC 60603 B/3
0
20
20
Connector_DIN
DIN41612_B_1x32_Female_Vertical_THT
DIN41612 connector, type B, Vertical, 2 rows 32 pins wide, https://www.erni-x-press.com/de/downloads/kataloge/englische_kataloge/erni-din41612-iec60603-2-e.pdf
DIN 41612 IEC 60603 B
0
32
32
Connector_DIN
DIN41612_B_1x32_Male_Horizontal_THT
DIN41612 connector, type B, Horizontal, 2 rows 32 pins wide, https://www.erni-x-press.com/de/downloads/kataloge/englische_kataloge/erni-din41612-iec60603-2-e.pdf
DIN 41612 IEC 60603 B
0
32
32
Connector_DIN
DIN41612_B_2x16_Female_Vertical_THT
DIN41612 connector, type B, Vertical, 2 rows 32 pins wide, https://www.erni-x-press.com/de/downloads/kataloge/englische_kataloge/erni-din41612-iec60603-2-e.pdf
DIN 41612 IEC 60603 B
0
32
32
Connector_DIN
DIN41612_B_2x16_Male_Horizontal_THT
DIN41612 connector, type B, Horizontal, 2 rows 32 pins wide, https://www.erni-x-press.com/de/downloads/kataloge/englische_kataloge/erni-din41612-iec60603-2-e.pdf
DIN 41612 IEC 60603 B
0
32
32
Connector_DIN
DIN41612_B_2x32_Female_Vertical_THT
DIN41612 connector, type B, Vertical, 2 rows 32 pins wide, https://www.erni-x-press.com/de/downloads/kataloge/englische_kataloge/erni-din41612-iec60603-2-e.pdf
DIN 41612 IEC 60603 B
0
64
64
Connector_DIN
DIN41612_B_2x32_Male_Horizontal_THT
DIN41612 connector, type B, Horizontal, 2 rows 32 pins wide, https://www.erni-x-press.com/de/downloads/kataloge/englische_kataloge/erni-din41612-iec60603-2-e.pdf
DIN 41612 IEC 60603 B
0
64
64
Connector_DIN
DIN41612_C2_2x16_Female_Vertical_THT
DIN41612 connector, type C/2, Vertical, 3 rows 16 pins wide, https://www.erni-x-press.com/de/downloads/kataloge/englische_kataloge/erni-din41612-iec60603-2-e.pdf
DIN 41612 IEC 60603 C/2
0
32
32
Connector_DIN
DIN41612_C2_2x16_Male_Horizontal_THT
DIN41612 connector, type C/2, Horizontal, 3 rows 16 pins wide, https://www.erni-x-press.com/de/downloads/kataloge/englische_kataloge/erni-din41612-iec60603-2-e.pdf
DIN 41612 IEC 60603 C/2
0
32
32
Connector_DIN
DIN41612_C2_3x16_Female_Vertical_THT
DIN41612 connector, type C/2, Vertical, 3 rows 16 pins wide, https://www.erni-x-press.com/de/downloads/kataloge/englische_kataloge/erni-din41612-iec60603-2-e.pdf
DIN 41612 IEC 60603 C/2
0
48
48
Connector_DIN
DIN41612_C2_3x16_Male_Horizontal_THT
DIN41612 connector, type C/2, Horizontal, 3 rows 16 pins wide, https://www.erni-x-press.com/de/downloads/kataloge/englische_kataloge/erni-din41612-iec60603-2-e.pdf
DIN 41612 IEC 60603 C/2
0
48
48
Connector_DIN
DIN41612_C3_2x10_Female_Vertical_THT
DIN41612 connector, type C/3, Vertical, 3 rows 10 pins wide, https://www.erni-x-press.com/de/downloads/kataloge/englische_kataloge/erni-din41612-iec60603-2-e.pdf
DIN 41612 IEC 60603 C/3
0
20
20
Connector_DIN
DIN41612_C3_2x10_Male_Horizontal_THT
DIN41612 connector, type C/3, Horizontal, 3 rows 10 pins wide, https://www.erni-x-press.com/de/downloads/kataloge/englische_kataloge/erni-din41612-iec60603-2-e.pdf
DIN 41612 IEC 60603 C/3
0
20
20
Connector_DIN
DIN41612_C3_3x10_Female_Vertical_THT
DIN41612 connector, type C/3, Vertical, 3 rows 10 pins wide, https://www.erni-x-press.com/de/downloads/kataloge/englische_kataloge/erni-din41612-iec60603-2-e.pdf
DIN 41612 IEC 60603 C/3
0
30
30
Connector_DIN
DIN41612_C3_3x10_Male_Horizontal_THT
DIN41612 connector, type C/3, Horizontal, 3 rows 10 pins wide, https://www.erni-x-press.com/de/downloads/kataloge/englische_kataloge/erni-din41612-iec60603-2-e.pdf
DIN 41612 IEC 60603 C/3
0
30
30
Connector_DIN
DIN41612_C_1x32_Female_Vertical_THT
DIN41612 connector, type C, Vertical, 3 rows 32 pins wide, https://www.erni-x-press.com/de/downloads/kataloge/englische_kataloge/erni-din41612-iec60603-2-e.pdf
DIN 41612 IEC 60603 C
0
32
32
Connector_DIN
DIN41612_C_1x32_Male_Horizontal_THT
DIN41612 connector, type C, Horizontal, 3 rows 32 pins wide, https://www.erni-x-press.com/de/downloads/kataloge/englische_kataloge/erni-din41612-iec60603-2-e.pdf
DIN 41612 IEC 60603 C
0
32
32
Connector_DIN
DIN41612_C_2x16_Female_Vertical_THT
DIN41612 connector, type C, Vertical, 3 rows 32 pins wide, https://www.erni-x-press.com/de/downloads/kataloge/englische_kataloge/erni-din41612-iec60603-2-e.pdf
DIN 41612 IEC 60603 C
0
32
32
Connector_DIN
DIN41612_C_2x16_Male_Horizontal_THT
DIN41612 connector, type C, Horizontal, 3 rows 32 pins wide, https://www.erni-x-press.com/de/downloads/kataloge/englische_kataloge/erni-din41612-iec60603-2-e.pdf
DIN 41612 IEC 60603 C
0
32
32
Connector_DIN
DIN41612_C_2x32_Female_Vertical_THT
DIN41612 connector, type C, Vertical, 3 rows 32 pins wide, https://www.erni-x-press.com/de/downloads/kataloge/englische_kataloge/erni-din41612-iec60603-2-e.pdf
DIN 41612 IEC 60603 C
0
64
64
Connector_DIN
DIN41612_C_2x32_Male_Horizontal_THT
DIN41612 connector, type C, Horizontal, 3 rows 32 pins wide, https://www.erni-x-press.com/de/downloads/kataloge/englische_kataloge/erni-din41612-iec60603-2-e.pdf
DIN 41612 IEC 60603 C
0
64
64
Connector_DIN
DIN41612_C_3x16_Female_Vertical_THT
DIN41612 connector, type C, Vertical, 3 rows 32 pins wide, https://www.erni-x-press.com/de/downloads/kataloge/englische_kataloge/erni-din41612-iec60603-2-e.pdf
DIN 41612 IEC 60603 C
0
48
48
Connector_DIN
DIN41612_C_3x16_Male_Horizontal_THT
DIN41612 connector, type C, Horizontal, 3 rows 32 pins wide, https://www.erni-x-press.com/de/downloads/kataloge/englische_kataloge/erni-din41612-iec60603-2-e.pdf
DIN 41612 IEC 60603 C
0
48
48
Connector_DIN
DIN41612_C_3x32_Female_Vertical_THT
DIN41612 connector, type C, Vertical, 3 rows 32 pins wide, https://www.erni-x-press.com/de/downloads/kataloge/englische_kataloge/erni-din41612-iec60603-2-e.pdf
DIN 41612 IEC 60603 C
0
96
96
Connector_DIN
DIN41612_C_3x32_Male_Horizontal_THT
DIN41612 connector, type C, Horizontal, 3 rows 32 pins wide, https://www.erni-x-press.com/de/downloads/kataloge/englische_kataloge/erni-din41612-iec60603-2-e.pdf
DIN 41612 IEC 60603 C
0
96
96
Connector_DIN
DIN41612_D_2x8_Female_Vertical_THT
DIN41612 connector, type D, Vertical, 3 rows 32 pins wide, https://www.erni-x-press.com/de/downloads/kataloge/englische_kataloge/erni-din41612-iec60603-2-e.pdf
DIN 41612 IEC 60603 D
0
16
16
Connector_DIN
DIN41612_D_2x8_Male_Horizontal_THT
DIN41612 connector, type D, Horizontal, 3 rows 32 pins wide, https://www.erni-x-press.com/de/downloads/kataloge/englische_kataloge/erni-din41612-iec60603-2-e.pdf
DIN 41612 IEC 60603 D
0
16
16
Connector_DIN
DIN41612_D_2x16_Female_Vertical_THT
DIN41612 connector, type D, Vertical, 3 rows 32 pins wide, https://www.erni-x-press.com/de/downloads/kataloge/englische_kataloge/erni-din41612-iec60603-2-e.pdf
DIN 41612 IEC 60603 D
0
32
32
Connector_DIN
DIN41612_D_2x16_Male_Horizontal_THT
DIN41612 connector, type D, Horizontal, 3 rows 32 pins wide, https://www.erni-x-press.com/de/downloads/kataloge/englische_kataloge/erni-din41612-iec60603-2-e.pdf
DIN 41612 IEC 60603 D
0
32
32
Connector_DIN
DIN41612_E_2x16_Female_Vertical_THT
DIN41612 connector, type E, Vertical, 5 rows 32 pins wide, https://www.erni-x-press.com/de/downloads/kataloge/englische_kataloge/erni-din41612-iec60603-2-e.pdf
DIN 41612 IEC 60603 E
0
32
32
Connector_DIN
DIN41612_E_2x16_Male_Horizontal_THT
DIN41612 connector, type E, Horizontal, 5 rows 32 pins wide, https://www.erni-x-press.com/de/downloads/kataloge/englische_kataloge/erni-din41612-iec60603-2-e.pdf
DIN 41612 IEC 60603 E
0
32
32
Connector_DIN
DIN41612_E_2x16_RowsAC_Female_Vertical_THT
DIN41612 connector, type E, Vertical, 5 rows 32 pins wide, https://www.erni-x-press.com/de/downloads/kataloge/englische_kataloge/erni-din41612-iec60603-2-e.pdf
DIN 41612 IEC 60603 E
0
32
32
Connector_DIN
DIN41612_E_2x16_RowsAC_Male_Horizontal_THT
DIN41612 connector, type E, Horizontal, 5 rows 32 pins wide, https://www.erni-x-press.com/de/downloads/kataloge/englische_kataloge/erni-din41612-iec60603-2-e.pdf
DIN 41612 IEC 60603 E
0
32
32
Connector_DIN
DIN41612_E_3x16_Female_Vertical_THT
DIN41612 connector, type E, Vertical, 5 rows 32 pins wide, https://www.erni-x-press.com/de/downloads/kataloge/englische_kataloge/erni-din41612-iec60603-2-e.pdf
DIN 41612 IEC 60603 E
0
48
48
Connector_DIN
DIN41612_E_3x16_Male_Horizontal_THT
DIN41612 connector, type E, Horizontal, 5 rows 32 pins wide, https://www.erni-x-press.com/de/downloads/kataloge/englische_kataloge/erni-din41612-iec60603-2-e.pdf
DIN 41612 IEC 60603 E
0
48
48
Connector_DIN
DIN41612_F_2x16_Female_Vertical_THT
DIN41612 connector, type F, Vertical, 3 rows 32 pins wide, https://www.erni-x-press.com/de/downloads/kataloge/englische_kataloge/erni-din41612-iec60603-2-e.pdf
DIN 41612 IEC 60603 F
0
32
32
Connector_DIN
DIN41612_F_2x16_Male_Horizontal_THT
DIN41612 connector, type F, Horizontal, 3 rows 32 pins wide, https://www.erni-x-press.com/de/downloads/kataloge/englische_kataloge/erni-din41612-iec60603-2-e.pdf
DIN 41612 IEC 60603 F
0
32
32
Connector_DIN
DIN41612_F_2x16_RowsZD_Female_Vertical_THT
DIN41612 connector, type F, Vertical, 3 rows 32 pins wide, https://www.erni-x-press.com/de/downloads/kataloge/englische_kataloge/erni-din41612-iec60603-2-e.pdf
DIN 41612 IEC 60603 F
0
32
32
Connector_DIN
DIN41612_F_2x16_RowsZD_Male_Horizontal_THT
DIN41612 connector, type F, Horizontal, 3 rows 32 pins wide, https://www.erni-x-press.com/de/downloads/kataloge/englische_kataloge/erni-din41612-iec60603-2-e.pdf
DIN 41612 IEC 60603 F
0
32
32
Connector_DIN
DIN41612_F_3x16_Female_Vertical_THT
DIN41612 connector, type F, Vertical, 3 rows 32 pins wide, https://www.erni-x-press.com/de/downloads/kataloge/englische_kataloge/erni-din41612-iec60603-2-e.pdf
DIN 41612 IEC 60603 F
0
48
48
Connector_DIN
DIN41612_F_3x16_Male_Horizontal_THT
DIN41612 connector, type F, Horizontal, 3 rows 32 pins wide, https://www.erni-x-press.com/de/downloads/kataloge/englische_kataloge/erni-din41612-iec60603-2-e.pdf
DIN 41612 IEC 60603 F
0
48
48
Connector_DIN
DIN41612_Q2_2x16_Male_Horizontal_THT
DIN41612 connector, type Q/2, Horizontal, 2 rows 16 pins wide, https://www.erni-x-press.com/de/downloads/kataloge/englische_kataloge/erni-din41612-iec60603-2-e.pdf
DIN 41612 IEC 60603 Q/2
0
32
32
Connector_DIN
DIN41612_Q2_2x16_Male_Vertical_THT
DIN41612 connector, type Q/2, Vertical, 2 rows 16 pins wide, https://www.erni-x-press.com/de/downloads/kataloge/englische_kataloge/erni-din41612-iec60603-2-e.pdf
DIN 41612 IEC 60603 Q/2
0
32
32
Connector_DIN
DIN41612_Q3_2x10_Male_Horizontal_THT
DIN41612 connector, type Q/3, Horizontal, 2 rows 10 pins wide, https://www.erni-x-press.com/de/downloads/kataloge/englische_kataloge/erni-din41612-iec60603-2-e.pdf
DIN 41612 IEC 60603 Q/3
0
20
20
Connector_DIN
DIN41612_Q3_2x10_Male_Vertical_THT
DIN41612 connector, type Q/3, Vertical, 2 rows 10 pins wide, https://www.erni-x-press.com/de/downloads/kataloge/englische_kataloge/erni-din41612-iec60603-2-e.pdf
DIN 41612 IEC 60603 Q/3
0
20
20
Connector_DIN
DIN41612_Q_2x32_Male_Horizontal_THT
DIN41612 connector, type Q, Horizontal, 2 rows 32 pins wide, https://www.erni-x-press.com/de/downloads/kataloge/englische_kataloge/erni-din41612-iec60603-2-e.pdf
DIN 41612 IEC 60603 Q
0
64
64
Connector_DIN
DIN41612_Q_2x32_Male_Vertical_THT
DIN41612 connector, type Q, Vertical, 2 rows 32 pins wide, https://www.erni-x-press.com/de/downloads/kataloge/englische_kataloge/erni-din41612-iec60603-2-e.pdf
DIN 41612 IEC 60603 Q
0
64
64
Connector_DIN
DIN41612_R2_2x16_Male_Horizontal_THT
DIN41612 connector, type R/2, Horizontal, 3 rows 16 pins wide, https://www.erni-x-press.com/de/downloads/kataloge/englische_kataloge/erni-din41612-iec60603-2-e.pdf
DIN 41612 IEC 60603 R/2
0
32
32
Connector_DIN
DIN41612_R2_2x16_Male_Vertical_THT
DIN41612 connector, type R/2, Vertical, 3 rows 16 pins wide, https://www.erni-x-press.com/de/downloads/kataloge/englische_kataloge/erni-din41612-iec60603-2-e.pdf
DIN 41612 IEC 60603 R/2
0
32
32
Connector_DIN
DIN41612_R2_3x16_Male_Horizontal_THT
DIN41612 connector, type R/2, Horizontal, 3 rows 16 pins wide, https://www.erni-x-press.com/de/downloads/kataloge/englische_kataloge/erni-din41612-iec60603-2-e.pdf
DIN 41612 IEC 60603 R/2
0
48
48
Connector_DIN
DIN41612_R2_3x16_Male_Vertical_THT
DIN41612 connector, type R/2, Vertical, 3 rows 16 pins wide, https://www.erni-x-press.com/de/downloads/kataloge/englische_kataloge/erni-din41612-iec60603-2-e.pdf
DIN 41612 IEC 60603 R/2
0
48
48
Connector_DIN
DIN41612_R3_2x10_Male_Horizontal_THT
DIN41612 connector, type R/3, Horizontal, 3 rows 10 pins wide, https://www.erni-x-press.com/de/downloads/kataloge/englische_kataloge/erni-din41612-iec60603-2-e.pdf
DIN 41612 IEC 60603 R/3
0
20
20
Connector_DIN
DIN41612_R3_2x10_Male_Vertical_THT
DIN41612 connector, type R/3, Vertical, 3 rows 10 pins wide, https://www.erni-x-press.com/de/downloads/kataloge/englische_kataloge/erni-din41612-iec60603-2-e.pdf
DIN 41612 IEC 60603 R/3
0
20
20
Connector_DIN
DIN41612_R3_3x10_Male_Horizontal_THT
DIN41612 connector, type R/3, Horizontal, 3 rows 10 pins wide, https://www.erni-x-press.com/de/downloads/kataloge/englische_kataloge/erni-din41612-iec60603-2-e.pdf
DIN 41612 IEC 60603 R/3
0
30
30
Connector_DIN
DIN41612_R3_3x10_Male_Vertical_THT
DIN41612 connector, type R/3, Vertical, 3 rows 10 pins wide, https://www.erni-x-press.com/de/downloads/kataloge/englische_kataloge/erni-din41612-iec60603-2-e.pdf
DIN 41612 IEC 60603 R/3
0
30
30
Connector_DIN
DIN41612_R_1x32_Male_Horizontal_THT
DIN41612 connector, type R, Horizontal, 3 rows 32 pins wide, https://www.erni-x-press.com/de/downloads/kataloge/englische_kataloge/erni-din41612-iec60603-2-e.pdf
DIN 41612 IEC 60603 R
0
32
32
Connector_DIN
DIN41612_R_1x32_Male_Vertical_THT
DIN41612 connector, type R, Vertical, 3 rows 32 pins wide, https://www.erni-x-press.com/de/downloads/kataloge/englische_kataloge/erni-din41612-iec60603-2-e.pdf
DIN 41612 IEC 60603 R
0
32
32
Connector_DIN
DIN41612_R_2x16_Male_Horizontal_THT
DIN41612 connector, type R, Horizontal, 3 rows 32 pins wide, https://www.erni-x-press.com/de/downloads/kataloge/englische_kataloge/erni-din41612-iec60603-2-e.pdf
DIN 41612 IEC 60603 R
0
32
32
Connector_DIN
DIN41612_R_2x16_Male_Vertical_THT
DIN41612 connector, type R, Vertical, 3 rows 32 pins wide, https://www.erni-x-press.com/de/downloads/kataloge/englische_kataloge/erni-din41612-iec60603-2-e.pdf
DIN 41612 IEC 60603 R
0
32
32
Connector_DIN
DIN41612_R_2x32_Male_Horizontal_THT
DIN41612 connector, type R, Horizontal, 3 rows 32 pins wide, https://www.erni-x-press.com/de/downloads/kataloge/englische_kataloge/erni-din41612-iec60603-2-e.pdf
DIN 41612 IEC 60603 R
0
64
64
Connector_DIN
DIN41612_R_2x32_Male_Vertical_THT
DIN41612 connector, type R, Vertical, 3 rows 32 pins wide, https://www.erni-x-press.com/de/downloads/kataloge/englische_kataloge/erni-din41612-iec60603-2-e.pdf
DIN 41612 IEC 60603 R
0
64
64
Connector_DIN
DIN41612_R_3x16_Male_Horizontal_THT
DIN41612 connector, type R, Horizontal, 3 rows 32 pins wide, https://www.erni-x-press.com/de/downloads/kataloge/englische_kataloge/erni-din41612-iec60603-2-e.pdf
DIN 41612 IEC 60603 R
0
48
48
Connector_DIN
DIN41612_R_3x16_Male_Vertical_THT
DIN41612 connector, type R, Vertical, 3 rows 32 pins wide, https://www.erni-x-press.com/de/downloads/kataloge/englische_kataloge/erni-din41612-iec60603-2-e.pdf
DIN 41612 IEC 60603 R
0
48
48
Connector_DIN
DIN41612_R_3x32_Male_Horizontal_THT
DIN41612 connector, type R, Horizontal, 3 rows 32 pins wide, https://www.erni-x-press.com/de/downloads/kataloge/englische_kataloge/erni-din41612-iec60603-2-e.pdf
DIN 41612 IEC 60603 R
0
96
96
Connector_DIN
DIN41612_R_3x32_Male_Vertical_THT
DIN41612 connector, type R, Vertical, 3 rows 32 pins wide, https://www.erni-x-press.com/de/downloads/kataloge/englische_kataloge/erni-din41612-iec60603-2-e.pdf
DIN 41612 IEC 60603 R
0
96
96
Connector_Dsub
DSUB-9_Female_EdgeMount_P2.77mm
9-pin D-Sub connector, solder-cups edge-mounted, female, x-pin-pitch 2.77mm, distance of mounting holes 25mm, see https://disti-assets.s3.amazonaws.com/tonar/files/datasheets/16730.pdf
9-pin D-Sub connector edge mount solder cup female x-pin-pitch 2.77mm mounting holes distance 25mm
0
9
9
Connector_Dsub
DSUB-9_Female_Horizontal_P2.77x2.54mm_EdgePinOffset9.40mm
9-pin D-Sub connector, horizontal/angled (90 deg), THT-mount, female, pitch 2.77x2.54mm, pin-PCB-offset 9.4mm, see http://docs-europe.electrocomponents.com/webdocs/1585/0900766b81585df2.pdf
9-pin D-Sub connector horizontal angled 90deg THT female pitch 2.77x2.54mm pin-PCB-offset 9.4mm
0
9
9
Connector_Dsub
DSUB-9_Female_Horizontal_P2.77x2.84mm_EdgePinOffset4.94mm_Housed_MountingHolesOffset7.48mm
9-pin D-Sub connector, horizontal/angled (90 deg), THT-mount, female, pitch 2.77x2.84mm, pin-PCB-offset 4.9399999999999995mm, distance of mounting holes 25mm, distance of mounting holes to PCB edge 7.4799999999999995mm, see https://disti-assets.s3.amazonaws.com/tonar/files/datasheets/16730.pdf
9-pin D-Sub connector horizontal angled 90deg THT female pitch 2.77x2.84mm pin-PCB-offset 4.9399999999999995mm mounting-holes-distance 25mm mounting-hole-offset 25mm
0
11
10
Connector_Dsub
DSUB-9_Female_Horizontal_P2.77x2.84mm_EdgePinOffset7.70mm_Housed_MountingHolesOffset9.12mm
9-pin D-Sub connector, horizontal/angled (90 deg), THT-mount, female, pitch 2.77x2.84mm, pin-PCB-offset 7.699999999999999mm, distance of mounting holes 25mm, distance of mounting holes to PCB edge 9.12mm, see https://disti-assets.s3.amazonaws.com/tonar/files/datasheets/16730.pdf
9-pin D-Sub connector horizontal angled 90deg THT female pitch 2.77x2.84mm pin-PCB-offset 7.699999999999999mm mounting-holes-distance 25mm mounting-hole-offset 25mm
0
11
10
Connector_Dsub
DSUB-9_Female_Horizontal_P2.77x2.84mm_EdgePinOffset9.40mm
9-pin D-Sub connector, horizontal/angled (90 deg), THT-mount, female, pitch 2.77x2.84mm, pin-PCB-offset 9.4mm, see http://docs-europe.electrocomponents.com/webdocs/1585/0900766b81585df2.pdf
9-pin D-Sub connector horizontal angled 90deg THT female pitch 2.77x2.84mm pin-PCB-offset 9.4mm
0
9
9
Connector_Dsub
DSUB-9_Female_Horizontal_P2.77x2.84mm_EdgePinOffset9.90mm_Housed_MountingHolesOffset11.32mm
9-pin D-Sub connector, horizontal/angled (90 deg), THT-mount, female, pitch 2.77x2.84mm, pin-PCB-offset 9.9mm, distance of mounting holes 25mm, distance of mounting holes to PCB edge 11.32mm, see https://disti-assets.s3.amazonaws.com/tonar/files/datasheets/16730.pdf
9-pin D-Sub connector horizontal angled 90deg THT female pitch 2.77x2.84mm pin-PCB-offset 9.9mm mounting-holes-distance 25mm mounting-hole-offset 25mm
0
11
10
Connector_Dsub
DSUB-9_Female_Horizontal_P2.77x2.84mm_EdgePinOffset14.56mm_Housed_MountingHolesOffset8.20mm
9-pin D-Sub connector, horizontal/angled (90 deg), THT-mount, female, pitch 2.77x2.84mm, pin-PCB-offset 14.56mm, distance of mounting holes 25mm, distance of mounting holes to PCB edge 8.2mm, see https://disti-assets.s3.amazonaws.com/tonar/files/datasheets/16730.pdf
9-pin D-Sub connector horizontal angled 90deg THT female pitch 2.77x2.84mm pin-PCB-offset 14.56mm mounting-holes-distance 25mm mounting-hole-offset 25mm
0
11
10
Connector_Dsub
DSUB-9_Female_Horizontal_P2.77x2.84mm_EdgePinOffset14.56mm_Housed_MountingHolesOffset15.98mm
9-pin D-Sub connector, horizontal/angled (90 deg), THT-mount, female, pitch 2.77x2.84mm, pin-PCB-offset 14.56mm, distance of mounting holes 25mm, distance of mounting holes to PCB edge 15.979999999999999mm, see https://disti-assets.s3.amazonaws.com/tonar/files/datasheets/16730.pdf
9-pin D-Sub connector horizontal angled 90deg THT female pitch 2.77x2.84mm pin-PCB-offset 14.56mm mounting-holes-distance 25mm mounting-hole-offset 25mm
0
11
10
Connector_Dsub
DSUB-9_Female_Vertical_P2.77x2.84mm
9-pin D-Sub connector, straight/vertical, THT-mount, female, pitch 2.77x2.84mm, distance of mounting holes 25mm, see https://disti-assets.s3.amazonaws.com/tonar/files/datasheets/16730.pdf
9-pin D-Sub connector straight vertical THT female pitch 2.77x2.84mm mounting holes distance 25mm
0
9
9
Connector_Dsub
DSUB-9_Female_Vertical_P2.77x2.84mm_MountingHoles
9-pin D-Sub connector, straight/vertical, THT-mount, female, pitch 2.77x2.84mm, distance of mounting holes 25mm, see https://disti-assets.s3.amazonaws.com/tonar/files/datasheets/16730.pdf
9-pin D-Sub connector straight vertical THT female pitch 2.77x2.84mm mounting holes distance 25mm
0
11
10
Connector_Dsub
DSUB-9_Male_EdgeMount_P2.77mm
9-pin D-Sub connector, solder-cups edge-mounted, male, x-pin-pitch 2.77mm, distance of mounting holes 25mm, see https://disti-assets.s3.amazonaws.com/tonar/files/datasheets/16730.pdf
9-pin D-Sub connector edge mount solder cup male x-pin-pitch 2.77mm mounting holes distance 25mm
0
9
9
Connector_Dsub
DSUB-9_Male_Horizontal_P2.77x2.54mm_EdgePinOffset9.40mm
9-pin D-Sub connector, horizontal/angled (90 deg), THT-mount, male, pitch 2.77x2.54mm, pin-PCB-offset 9.4mm, see http://docs-europe.electrocomponents.com/webdocs/1585/0900766b81585df2.pdf
9-pin D-Sub connector horizontal angled 90deg THT male pitch 2.77x2.54mm pin-PCB-offset 9.4mm
0
9
9
Connector_Dsub
DSUB-9_Male_Horizontal_P2.77x2.84mm_EdgePinOffset4.94mm_Housed_MountingHolesOffset7.48mm
9-pin D-Sub connector, horizontal/angled (90 deg), THT-mount, male, pitch 2.77x2.84mm, pin-PCB-offset 4.9399999999999995mm, distance of mounting holes 25mm, distance of mounting holes to PCB edge 7.4799999999999995mm, see https://disti-assets.s3.amazonaws.com/tonar/files/datasheets/16730.pdf
9-pin D-Sub connector horizontal angled 90deg THT male pitch 2.77x2.84mm pin-PCB-offset 4.9399999999999995mm mounting-holes-distance 25mm mounting-hole-offset 25mm
0
11
10
Connector_Dsub
DSUB-9_Male_Horizontal_P2.77x2.84mm_EdgePinOffset7.70mm_Housed_MountingHolesOffset9.12mm
9-pin D-Sub connector, horizontal/angled (90 deg), THT-mount, male, pitch 2.77x2.84mm, pin-PCB-offset 7.699999999999999mm, distance of mounting holes 25mm, distance of mounting holes to PCB edge 9.12mm, see https://disti-assets.s3.amazonaws.com/tonar/files/datasheets/16730.pdf
9-pin D-Sub connector horizontal angled 90deg THT male pitch 2.77x2.84mm pin-PCB-offset 7.699999999999999mm mounting-holes-distance 25mm mounting-hole-offset 25mm
0
11
10
Connector_Dsub
DSUB-9_Male_Horizontal_P2.77x2.84mm_EdgePinOffset9.40mm
9-pin D-Sub connector, horizontal/angled (90 deg), THT-mount, male, pitch 2.77x2.84mm, pin-PCB-offset 9.4mm, see http://docs-europe.electrocomponents.com/webdocs/1585/0900766b81585df2.pdf
9-pin D-Sub connector horizontal angled 90deg THT male pitch 2.77x2.84mm pin-PCB-offset 9.4mm
0
9
9
Connector_Dsub
DSUB-9_Male_Horizontal_P2.77x2.84mm_EdgePinOffset9.90mm_Housed_MountingHolesOffset11.32mm
9-pin D-Sub connector, horizontal/angled (90 deg), THT-mount, male, pitch 2.77x2.84mm, pin-PCB-offset 9.9mm, distance of mounting holes 25mm, distance of mounting holes to PCB edge 11.32mm, see https://disti-assets.s3.amazonaws.com/tonar/files/datasheets/16730.pdf
9-pin D-Sub connector horizontal angled 90deg THT male pitch 2.77x2.84mm pin-PCB-offset 9.9mm mounting-holes-distance 25mm mounting-hole-offset 25mm
0
11
10
Connector_Dsub
DSUB-9_Male_Horizontal_P2.77x2.84mm_EdgePinOffset14.56mm_Housed_MountingHolesOffset8.20mm
9-pin D-Sub connector, horizontal/angled (90 deg), THT-mount, male, pitch 2.77x2.84mm, pin-PCB-offset 14.56mm, distance of mounting holes 25mm, distance of mounting holes to PCB edge 8.2mm, see https://disti-assets.s3.amazonaws.com/tonar/files/datasheets/16730.pdf
9-pin D-Sub connector horizontal angled 90deg THT male pitch 2.77x2.84mm pin-PCB-offset 14.56mm mounting-holes-distance 25mm mounting-hole-offset 25mm
0
11
10
Connector_Dsub
DSUB-9_Male_Horizontal_P2.77x2.84mm_EdgePinOffset14.56mm_Housed_MountingHolesOffset15.98mm
9-pin D-Sub connector, horizontal/angled (90 deg), THT-mount, male, pitch 2.77x2.84mm, pin-PCB-offset 14.56mm, distance of mounting holes 25mm, distance of mounting holes to PCB edge 15.979999999999999mm, see https://disti-assets.s3.amazonaws.com/tonar/files/datasheets/16730.pdf
9-pin D-Sub connector horizontal angled 90deg THT male pitch 2.77x2.84mm pin-PCB-offset 14.56mm mounting-holes-distance 25mm mounting-hole-offset 25mm
0
11
10
Connector_Dsub
DSUB-9_Male_Vertical_P2.77x2.84mm
9-pin D-Sub connector, straight/vertical, THT-mount, male, pitch 2.77x2.84mm, distance of mounting holes 25mm, see https://disti-assets.s3.amazonaws.com/tonar/files/datasheets/16730.pdf
9-pin D-Sub connector straight vertical THT male pitch 2.77x2.84mm mounting holes distance 25mm
0
9
9
Connector_Dsub
DSUB-9_Male_Vertical_P2.77x2.84mm_MountingHoles
9-pin D-Sub connector, straight/vertical, THT-mount, male, pitch 2.77x2.84mm, distance of mounting holes 25mm, see https://disti-assets.s3.amazonaws.com/tonar/files/datasheets/16730.pdf
9-pin D-Sub connector straight vertical THT male pitch 2.77x2.84mm mounting holes distance 25mm
0
11
10
Connector_Dsub
DSUB-15-HD_Female_Horizontal_P2.29x1.98mm_EdgePinOffset3.03mm_Housed_MountingHolesOffset4.94mm
15-pin D-Sub connector, horizontal/angled (90 deg), THT-mount, female, pitch 2.29x1.98mm, pin-PCB-offset 3.0300000000000002mm, distance of mounting holes 25mm, distance of mounting holes to PCB edge 4.9399999999999995mm, see https://disti-assets.s3.amazonaws.com/tonar/files/datasheets/16730.pdf
15-pin D-Sub connector horizontal angled 90deg THT female pitch 2.29x1.98mm pin-PCB-offset 3.0300000000000002mm mounting-holes-distance 25mm mounting-hole-offset 25mm
0
17
16
Connector_Dsub
DSUB-15-HD_Female_Horizontal_P2.29x1.98mm_EdgePinOffset8.35mm_Housed_MountingHolesOffset10.89mm
15-pin D-Sub connector, horizontal/angled (90 deg), THT-mount, female, pitch 2.29x1.98mm, pin-PCB-offset 8.35mm, distance of mounting holes 25mm, distance of mounting holes to PCB edge 10.889999999999999mm, see https://disti-assets.s3.amazonaws.com/tonar/files/datasheets/16730.pdf
15-pin D-Sub connector horizontal angled 90deg THT female pitch 2.29x1.98mm pin-PCB-offset 8.35mm mounting-holes-distance 25mm mounting-hole-offset 25mm
0
17
16
Connector_Dsub
DSUB-15-HD_Female_Horizontal_P2.29x1.98mm_EdgePinOffset9.40mm
15-pin D-Sub connector, horizontal/angled (90 deg), THT-mount, female, pitch 2.29x1.98mm, pin-PCB-offset 9.4mm, see http://docs-europe.electrocomponents.com/webdocs/1585/0900766b81585df2.pdf
15-pin D-Sub connector horizontal angled 90deg THT female pitch 2.29x1.98mm pin-PCB-offset 9.4mm
0
15
15
Connector_Dsub
DSUB-15-HD_Female_Horizontal_P2.29x2.54mm_EdgePinOffset9.40mm
15-pin D-Sub connector, horizontal/angled (90 deg), THT-mount, female, pitch 2.29x2.54mm, pin-PCB-offset 9.4mm, see http://docs-europe.electrocomponents.com/webdocs/1585/0900766b81585df2.pdf
15-pin D-Sub connector horizontal angled 90deg THT female pitch 2.29x2.54mm pin-PCB-offset 9.4mm
0
15
15
Connector_Dsub
DSUB-15-HD_Female_Vertical_P2.29x1.98mm_MountingHoles
15-pin D-Sub connector, straight/vertical, THT-mount, female, pitch 2.29x1.98mm, distance of mounting holes 25mm, see https://disti-assets.s3.amazonaws.com/tonar/files/datasheets/16730.pdf
15-pin D-Sub connector straight vertical THT female pitch 2.29x1.98mm mounting holes distance 25mm
0
17
16
Connector_Dsub
DSUB-15-HD_Male_Horizontal_P2.29x1.98mm_EdgePinOffset3.03mm_Housed_MountingHolesOffset4.94mm
15-pin D-Sub connector, horizontal/angled (90 deg), THT-mount, male, pitch 2.29x1.98mm, pin-PCB-offset 3.0300000000000002mm, distance of mounting holes 25mm, distance of mounting holes to PCB edge 4.9399999999999995mm, see https://disti-assets.s3.amazonaws.com/tonar/files/datasheets/16730.pdf
15-pin D-Sub connector horizontal angled 90deg THT male pitch 2.29x1.98mm pin-PCB-offset 3.0300000000000002mm mounting-holes-distance 25mm mounting-hole-offset 25mm
0
17
16
Connector_Dsub
DSUB-15-HD_Male_Horizontal_P2.29x1.98mm_EdgePinOffset8.35mm_Housed_MountingHolesOffset10.89mm
15-pin D-Sub connector, horizontal/angled (90 deg), THT-mount, male, pitch 2.29x1.98mm, pin-PCB-offset 8.35mm, distance of mounting holes 25mm, distance of mounting holes to PCB edge 10.889999999999999mm, see https://disti-assets.s3.amazonaws.com/tonar/files/datasheets/16730.pdf
15-pin D-Sub connector horizontal angled 90deg THT male pitch 2.29x1.98mm pin-PCB-offset 8.35mm mounting-holes-distance 25mm mounting-hole-offset 25mm
0
17
16
Connector_Dsub
DSUB-15-HD_Male_Horizontal_P2.29x1.98mm_EdgePinOffset9.40mm
15-pin D-Sub connector, horizontal/angled (90 deg), THT-mount, male, pitch 2.29x1.98mm, pin-PCB-offset 9.4mm, see http://docs-europe.electrocomponents.com/webdocs/1585/0900766b81585df2.pdf
15-pin D-Sub connector horizontal angled 90deg THT male pitch 2.29x1.98mm pin-PCB-offset 9.4mm
0
15
15
Connector_Dsub
DSUB-15-HD_Male_Horizontal_P2.29x2.54mm_EdgePinOffset9.40mm
15-pin D-Sub connector, horizontal/angled (90 deg), THT-mount, male, pitch 2.29x2.54mm, pin-PCB-offset 9.4mm, see http://docs-europe.electrocomponents.com/webdocs/1585/0900766b81585df2.pdf
15-pin D-Sub connector horizontal angled 90deg THT male pitch 2.29x2.54mm pin-PCB-offset 9.4mm
0
15
15
Connector_Dsub
DSUB-15-HD_Male_Vertical_P2.29x1.98mm_MountingHoles
15-pin D-Sub connector, straight/vertical, THT-mount, male, pitch 2.29x1.98mm, distance of mounting holes 25mm, see https://disti-assets.s3.amazonaws.com/tonar/files/datasheets/16730.pdf
15-pin D-Sub connector straight vertical THT male pitch 2.29x1.98mm mounting holes distance 25mm
0
17
16
Connector_Dsub
DSUB-15_Female_EdgeMount_P2.77mm
15-pin D-Sub connector, solder-cups edge-mounted, female, x-pin-pitch 2.77mm, distance of mounting holes 33.3mm, see https://disti-assets.s3.amazonaws.com/tonar/files/datasheets/16730.pdf
15-pin D-Sub connector edge mount solder cup female x-pin-pitch 2.77mm mounting holes distance 33.3mm
0
15
15
Connector_Dsub
DSUB-15_Female_Horizontal_P2.77x2.54mm_EdgePinOffset9.40mm
15-pin D-Sub connector, horizontal/angled (90 deg), THT-mount, female, pitch 2.77x2.54mm, pin-PCB-offset 9.4mm, see http://docs-europe.electrocomponents.com/webdocs/1585/0900766b81585df2.pdf
15-pin D-Sub connector horizontal angled 90deg THT female pitch 2.77x2.54mm pin-PCB-offset 9.4mm
0
15
15
Connector_Dsub
DSUB-15_Female_Horizontal_P2.77x2.84mm_EdgePinOffset4.94mm_Housed_MountingHolesOffset7.48mm
15-pin D-Sub connector, horizontal/angled (90 deg), THT-mount, female, pitch 2.77x2.84mm, pin-PCB-offset 4.9399999999999995mm, distance of mounting holes 33.3mm, distance of mounting holes to PCB edge 7.4799999999999995mm, see https://disti-assets.s3.amazonaws.com/tonar/files/datasheets/16730.pdf
15-pin D-Sub connector horizontal angled 90deg THT female pitch 2.77x2.84mm pin-PCB-offset 4.9399999999999995mm mounting-holes-distance 33.3mm mounting-hole-offset 33.3mm
0
17
16
Connector_Dsub
DSUB-15_Female_Horizontal_P2.77x2.84mm_EdgePinOffset7.70mm_Housed_MountingHolesOffset9.12mm
15-pin D-Sub connector, horizontal/angled (90 deg), THT-mount, female, pitch 2.77x2.84mm, pin-PCB-offset 7.699999999999999mm, distance of mounting holes 33.3mm, distance of mounting holes to PCB edge 9.12mm, see https://disti-assets.s3.amazonaws.com/tonar/files/datasheets/16730.pdf
15-pin D-Sub connector horizontal angled 90deg THT female pitch 2.77x2.84mm pin-PCB-offset 7.699999999999999mm mounting-holes-distance 33.3mm mounting-hole-offset 33.3mm
0
17
16
Connector_Dsub
DSUB-15_Female_Horizontal_P2.77x2.84mm_EdgePinOffset9.40mm
15-pin D-Sub connector, horizontal/angled (90 deg), THT-mount, female, pitch 2.77x2.84mm, pin-PCB-offset 9.4mm, see http://docs-europe.electrocomponents.com/webdocs/1585/0900766b81585df2.pdf
15-pin D-Sub connector horizontal angled 90deg THT female pitch 2.77x2.84mm pin-PCB-offset 9.4mm
0
15
15
Connector_Dsub
DSUB-15_Female_Horizontal_P2.77x2.84mm_EdgePinOffset9.90mm_Housed_MountingHolesOffset11.32mm
15-pin D-Sub connector, horizontal/angled (90 deg), THT-mount, female, pitch 2.77x2.84mm, pin-PCB-offset 9.9mm, distance of mounting holes 33.3mm, distance of mounting holes to PCB edge 11.32mm, see https://disti-assets.s3.amazonaws.com/tonar/files/datasheets/16730.pdf
15-pin D-Sub connector horizontal angled 90deg THT female pitch 2.77x2.84mm pin-PCB-offset 9.9mm mounting-holes-distance 33.3mm mounting-hole-offset 33.3mm
0
17
16
Connector_Dsub
DSUB-15_Female_Horizontal_P2.77x2.84mm_EdgePinOffset14.56mm_Housed_MountingHolesOffset8.20mm
15-pin D-Sub connector, horizontal/angled (90 deg), THT-mount, female, pitch 2.77x2.84mm, pin-PCB-offset 14.56mm, distance of mounting holes 33.3mm, distance of mounting holes to PCB edge 8.2mm, see https://disti-assets.s3.amazonaws.com/tonar/files/datasheets/16730.pdf
15-pin D-Sub connector horizontal angled 90deg THT female pitch 2.77x2.84mm pin-PCB-offset 14.56mm mounting-holes-distance 33.3mm mounting-hole-offset 33.3mm
0
17
16
Connector_Dsub
DSUB-15_Female_Horizontal_P2.77x2.84mm_EdgePinOffset14.56mm_Housed_MountingHolesOffset15.98mm
15-pin D-Sub connector, horizontal/angled (90 deg), THT-mount, female, pitch 2.77x2.84mm, pin-PCB-offset 14.56mm, distance of mounting holes 33.3mm, distance of mounting holes to PCB edge 15.979999999999999mm, see https://disti-assets.s3.amazonaws.com/tonar/files/datasheets/16730.pdf
15-pin D-Sub connector horizontal angled 90deg THT female pitch 2.77x2.84mm pin-PCB-offset 14.56mm mounting-holes-distance 33.3mm mounting-hole-offset 33.3mm
0
17
16
Connector_Dsub
DSUB-15_Female_Vertical_P2.77x2.84mm
15-pin D-Sub connector, straight/vertical, THT-mount, female, pitch 2.77x2.84mm, distance of mounting holes 33.3mm, see https://disti-assets.s3.amazonaws.com/tonar/files/datasheets/16730.pdf
15-pin D-Sub connector straight vertical THT female pitch 2.77x2.84mm mounting holes distance 33.3mm
0
15
15
Connector_Dsub
DSUB-15_Female_Vertical_P2.77x2.84mm_MountingHoles
15-pin D-Sub connector, straight/vertical, THT-mount, female, pitch 2.77x2.84mm, distance of mounting holes 33.3mm, see https://disti-assets.s3.amazonaws.com/tonar/files/datasheets/16730.pdf
15-pin D-Sub connector straight vertical THT female pitch 2.77x2.84mm mounting holes distance 33.3mm
0
17
16
Connector_Dsub
DSUB-15_Male_EdgeMount_P2.77mm
15-pin D-Sub connector, solder-cups edge-mounted, male, x-pin-pitch 2.77mm, distance of mounting holes 33.3mm, see https://disti-assets.s3.amazonaws.com/tonar/files/datasheets/16730.pdf
15-pin D-Sub connector edge mount solder cup male x-pin-pitch 2.77mm mounting holes distance 33.3mm
0
15
15
Connector_Dsub
DSUB-15_Male_Horizontal_P2.77x2.54mm_EdgePinOffset9.40mm
15-pin D-Sub connector, horizontal/angled (90 deg), THT-mount, male, pitch 2.77x2.54mm, pin-PCB-offset 9.4mm, see http://docs-europe.electrocomponents.com/webdocs/1585/0900766b81585df2.pdf
15-pin D-Sub connector horizontal angled 90deg THT male pitch 2.77x2.54mm pin-PCB-offset 9.4mm
0
15
15
Connector_Dsub
DSUB-15_Male_Horizontal_P2.77x2.84mm_EdgePinOffset4.94mm_Housed_MountingHolesOffset7.48mm
15-pin D-Sub connector, horizontal/angled (90 deg), THT-mount, male, pitch 2.77x2.84mm, pin-PCB-offset 4.9399999999999995mm, distance of mounting holes 33.3mm, distance of mounting holes to PCB edge 7.4799999999999995mm, see https://disti-assets.s3.amazonaws.com/tonar/files/datasheets/16730.pdf
15-pin D-Sub connector horizontal angled 90deg THT male pitch 2.77x2.84mm pin-PCB-offset 4.9399999999999995mm mounting-holes-distance 33.3mm mounting-hole-offset 33.3mm
0
17
16
Connector_Dsub
DSUB-15_Male_Horizontal_P2.77x2.84mm_EdgePinOffset7.70mm_Housed_MountingHolesOffset9.12mm
15-pin D-Sub connector, horizontal/angled (90 deg), THT-mount, male, pitch 2.77x2.84mm, pin-PCB-offset 7.699999999999999mm, distance of mounting holes 33.3mm, distance of mounting holes to PCB edge 9.12mm, see https://disti-assets.s3.amazonaws.com/tonar/files/datasheets/16730.pdf
15-pin D-Sub connector horizontal angled 90deg THT male pitch 2.77x2.84mm pin-PCB-offset 7.699999999999999mm mounting-holes-distance 33.3mm mounting-hole-offset 33.3mm
0
17
16
Connector_Dsub
DSUB-15_Male_Horizontal_P2.77x2.84mm_EdgePinOffset9.40mm
15-pin D-Sub connector, horizontal/angled (90 deg), THT-mount, male, pitch 2.77x2.84mm, pin-PCB-offset 9.4mm, see http://docs-europe.electrocomponents.com/webdocs/1585/0900766b81585df2.pdf
15-pin D-Sub connector horizontal angled 90deg THT male pitch 2.77x2.84mm pin-PCB-offset 9.4mm
0
15
15
Connector_Dsub
DSUB-15_Male_Horizontal_P2.77x2.84mm_EdgePinOffset9.90mm_Housed_MountingHolesOffset11.32mm
15-pin D-Sub connector, horizontal/angled (90 deg), THT-mount, male, pitch 2.77x2.84mm, pin-PCB-offset 9.9mm, distance of mounting holes 33.3mm, distance of mounting holes to PCB edge 11.32mm, see https://disti-assets.s3.amazonaws.com/tonar/files/datasheets/16730.pdf
15-pin D-Sub connector horizontal angled 90deg THT male pitch 2.77x2.84mm pin-PCB-offset 9.9mm mounting-holes-distance 33.3mm mounting-hole-offset 33.3mm
0
17
16
Connector_Dsub
DSUB-15_Male_Horizontal_P2.77x2.84mm_EdgePinOffset14.56mm_Housed_MountingHolesOffset8.20mm
15-pin D-Sub connector, horizontal/angled (90 deg), THT-mount, male, pitch 2.77x2.84mm, pin-PCB-offset 14.56mm, distance of mounting holes 33.3mm, distance of mounting holes to PCB edge 8.2mm, see https://disti-assets.s3.amazonaws.com/tonar/files/datasheets/16730.pdf
15-pin D-Sub connector horizontal angled 90deg THT male pitch 2.77x2.84mm pin-PCB-offset 14.56mm mounting-holes-distance 33.3mm mounting-hole-offset 33.3mm
0
17
16
Connector_Dsub
DSUB-15_Male_Horizontal_P2.77x2.84mm_EdgePinOffset14.56mm_Housed_MountingHolesOffset15.98mm
15-pin D-Sub connector, horizontal/angled (90 deg), THT-mount, male, pitch 2.77x2.84mm, pin-PCB-offset 14.56mm, distance of mounting holes 33.3mm, distance of mounting holes to PCB edge 15.979999999999999mm, see https://disti-assets.s3.amazonaws.com/tonar/files/datasheets/16730.pdf
15-pin D-Sub connector horizontal angled 90deg THT male pitch 2.77x2.84mm pin-PCB-offset 14.56mm mounting-holes-distance 33.3mm mounting-hole-offset 33.3mm
0
17
16
Connector_Dsub
DSUB-15_Male_Vertical_P2.77x2.84mm
15-pin D-Sub connector, straight/vertical, THT-mount, male, pitch 2.77x2.84mm, distance of mounting holes 33.3mm, see https://disti-assets.s3.amazonaws.com/tonar/files/datasheets/16730.pdf
15-pin D-Sub connector straight vertical THT male pitch 2.77x2.84mm mounting holes distance 33.3mm
0
15
15
Connector_Dsub
DSUB-15_Male_Vertical_P2.77x2.84mm_MountingHoles
15-pin D-Sub connector, straight/vertical, THT-mount, male, pitch 2.77x2.84mm, distance of mounting holes 33.3mm, see https://disti-assets.s3.amazonaws.com/tonar/files/datasheets/16730.pdf
15-pin D-Sub connector straight vertical THT male pitch 2.77x2.84mm mounting holes distance 33.3mm
0
17
16
Connector_Dsub
DSUB-25_Female_EdgeMount_P2.77mm
25-pin D-Sub connector, solder-cups edge-mounted, female, x-pin-pitch 2.77mm, distance of mounting holes 47.1mm, see https://disti-assets.s3.amazonaws.com/tonar/files/datasheets/16730.pdf
25-pin D-Sub connector edge mount solder cup female x-pin-pitch 2.77mm mounting holes distance 47.1mm
0
25
25
Connector_Dsub
DSUB-25_Female_Horizontal_P2.77x2.54mm_EdgePinOffset9.40mm
25-pin D-Sub connector, horizontal/angled (90 deg), THT-mount, female, pitch 2.77x2.54mm, pin-PCB-offset 9.4mm, see http://docs-europe.electrocomponents.com/webdocs/1585/0900766b81585df2.pdf
25-pin D-Sub connector horizontal angled 90deg THT female pitch 2.77x2.54mm pin-PCB-offset 9.4mm
0
25
25
Connector_Dsub
DSUB-25_Female_Horizontal_P2.77x2.84mm_EdgePinOffset4.94mm_Housed_MountingHolesOffset7.48mm
25-pin D-Sub connector, horizontal/angled (90 deg), THT-mount, female, pitch 2.77x2.84mm, pin-PCB-offset 4.9399999999999995mm, distance of mounting holes 47.1mm, distance of mounting holes to PCB edge 7.4799999999999995mm, see https://disti-assets.s3.amazonaws.com/tonar/files/datasheets/16730.pdf
25-pin D-Sub connector horizontal angled 90deg THT female pitch 2.77x2.84mm pin-PCB-offset 4.9399999999999995mm mounting-holes-distance 47.1mm mounting-hole-offset 47.1mm
0
27
26
Connector_Dsub
DSUB-25_Female_Horizontal_P2.77x2.84mm_EdgePinOffset7.70mm_Housed_MountingHolesOffset9.12mm
25-pin D-Sub connector, horizontal/angled (90 deg), THT-mount, female, pitch 2.77x2.84mm, pin-PCB-offset 7.699999999999999mm, distance of mounting holes 47.1mm, distance of mounting holes to PCB edge 9.12mm, see https://disti-assets.s3.amazonaws.com/tonar/files/datasheets/16730.pdf
25-pin D-Sub connector horizontal angled 90deg THT female pitch 2.77x2.84mm pin-PCB-offset 7.699999999999999mm mounting-holes-distance 47.1mm mounting-hole-offset 47.1mm
0
27
26
Connector_Dsub
DSUB-25_Female_Horizontal_P2.77x2.84mm_EdgePinOffset9.40mm
25-pin D-Sub connector, horizontal/angled (90 deg), THT-mount, female, pitch 2.77x2.84mm, pin-PCB-offset 9.4mm, see http://docs-europe.electrocomponents.com/webdocs/1585/0900766b81585df2.pdf
25-pin D-Sub connector horizontal angled 90deg THT female pitch 2.77x2.84mm pin-PCB-offset 9.4mm
0
25
25
Connector_Dsub
DSUB-25_Female_Horizontal_P2.77x2.84mm_EdgePinOffset9.90mm_Housed_MountingHolesOffset11.32mm
25-pin D-Sub connector, horizontal/angled (90 deg), THT-mount, female, pitch 2.77x2.84mm, pin-PCB-offset 9.9mm, distance of mounting holes 47.1mm, distance of mounting holes to PCB edge 11.32mm, see https://disti-assets.s3.amazonaws.com/tonar/files/datasheets/16730.pdf
25-pin D-Sub connector horizontal angled 90deg THT female pitch 2.77x2.84mm pin-PCB-offset 9.9mm mounting-holes-distance 47.1mm mounting-hole-offset 47.1mm
0
27
26
Connector_Dsub
DSUB-25_Female_Horizontal_P2.77x2.84mm_EdgePinOffset14.56mm_Housed_MountingHolesOffset8.20mm
25-pin D-Sub connector, horizontal/angled (90 deg), THT-mount, female, pitch 2.77x2.84mm, pin-PCB-offset 14.56mm, distance of mounting holes 47.1mm, distance of mounting holes to PCB edge 8.2mm, see https://disti-assets.s3.amazonaws.com/tonar/files/datasheets/16730.pdf
25-pin D-Sub connector horizontal angled 90deg THT female pitch 2.77x2.84mm pin-PCB-offset 14.56mm mounting-holes-distance 47.1mm mounting-hole-offset 47.1mm
0
27
26
Connector_Dsub
DSUB-25_Female_Horizontal_P2.77x2.84mm_EdgePinOffset14.56mm_Housed_MountingHolesOffset15.98mm
25-pin D-Sub connector, horizontal/angled (90 deg), THT-mount, female, pitch 2.77x2.84mm, pin-PCB-offset 14.56mm, distance of mounting holes 47.1mm, distance of mounting holes to PCB edge 15.979999999999999mm, see https://disti-assets.s3.amazonaws.com/tonar/files/datasheets/16730.pdf
25-pin D-Sub connector horizontal angled 90deg THT female pitch 2.77x2.84mm pin-PCB-offset 14.56mm mounting-holes-distance 47.1mm mounting-hole-offset 47.1mm
0
27
26
Connector_Dsub
DSUB-25_Female_Vertical_P2.77x2.84mm
25-pin D-Sub connector, straight/vertical, THT-mount, female, pitch 2.77x2.84mm, distance of mounting holes 47.1mm, see https://disti-assets.s3.amazonaws.com/tonar/files/datasheets/16730.pdf
25-pin D-Sub connector straight vertical THT female pitch 2.77x2.84mm mounting holes distance 47.1mm
0
25
25
Connector_Dsub
DSUB-25_Female_Vertical_P2.77x2.84mm_MountingHoles
25-pin D-Sub connector, straight/vertical, THT-mount, female, pitch 2.77x2.84mm, distance of mounting holes 47.1mm, see https://disti-assets.s3.amazonaws.com/tonar/files/datasheets/16730.pdf
25-pin D-Sub connector straight vertical THT female pitch 2.77x2.84mm mounting holes distance 47.1mm
0
27
26
Connector_Dsub
DSUB-25_Male_EdgeMount_P2.77mm
25-pin D-Sub connector, solder-cups edge-mounted, male, x-pin-pitch 2.77mm, distance of mounting holes 47.1mm, see https://disti-assets.s3.amazonaws.com/tonar/files/datasheets/16730.pdf
25-pin D-Sub connector edge mount solder cup male x-pin-pitch 2.77mm mounting holes distance 47.1mm
0
25
25
Connector_Dsub
DSUB-25_Male_Horizontal_P2.77x2.54mm_EdgePinOffset9.40mm
25-pin D-Sub connector, horizontal/angled (90 deg), THT-mount, male, pitch 2.77x2.54mm, pin-PCB-offset 9.4mm, see http://docs-europe.electrocomponents.com/webdocs/1585/0900766b81585df2.pdf
25-pin D-Sub connector horizontal angled 90deg THT male pitch 2.77x2.54mm pin-PCB-offset 9.4mm
0
25
25
Connector_Dsub
DSUB-25_Male_Horizontal_P2.77x2.84mm_EdgePinOffset4.94mm_Housed_MountingHolesOffset7.48mm
25-pin D-Sub connector, horizontal/angled (90 deg), THT-mount, male, pitch 2.77x2.84mm, pin-PCB-offset 4.9399999999999995mm, distance of mounting holes 47.1mm, distance of mounting holes to PCB edge 7.4799999999999995mm, see https://disti-assets.s3.amazonaws.com/tonar/files/datasheets/16730.pdf
25-pin D-Sub connector horizontal angled 90deg THT male pitch 2.77x2.84mm pin-PCB-offset 4.9399999999999995mm mounting-holes-distance 47.1mm mounting-hole-offset 47.1mm
0
27
26
Connector_Dsub
DSUB-25_Male_Horizontal_P2.77x2.84mm_EdgePinOffset7.70mm_Housed_MountingHolesOffset9.12mm
25-pin D-Sub connector, horizontal/angled (90 deg), THT-mount, male, pitch 2.77x2.84mm, pin-PCB-offset 7.699999999999999mm, distance of mounting holes 47.1mm, distance of mounting holes to PCB edge 9.12mm, see https://disti-assets.s3.amazonaws.com/tonar/files/datasheets/16730.pdf
25-pin D-Sub connector horizontal angled 90deg THT male pitch 2.77x2.84mm pin-PCB-offset 7.699999999999999mm mounting-holes-distance 47.1mm mounting-hole-offset 47.1mm
0
27
26
Connector_Dsub
DSUB-25_Male_Horizontal_P2.77x2.84mm_EdgePinOffset9.40mm
25-pin D-Sub connector, horizontal/angled (90 deg), THT-mount, male, pitch 2.77x2.84mm, pin-PCB-offset 9.4mm, see http://docs-europe.electrocomponents.com/webdocs/1585/0900766b81585df2.pdf
25-pin D-Sub connector horizontal angled 90deg THT male pitch 2.77x2.84mm pin-PCB-offset 9.4mm
0
25
25
Connector_Dsub
DSUB-25_Male_Horizontal_P2.77x2.84mm_EdgePinOffset9.90mm_Housed_MountingHolesOffset11.32mm
25-pin D-Sub connector, horizontal/angled (90 deg), THT-mount, male, pitch 2.77x2.84mm, pin-PCB-offset 9.9mm, distance of mounting holes 47.1mm, distance of mounting holes to PCB edge 11.32mm, see https://disti-assets.s3.amazonaws.com/tonar/files/datasheets/16730.pdf
25-pin D-Sub connector horizontal angled 90deg THT male pitch 2.77x2.84mm pin-PCB-offset 9.9mm mounting-holes-distance 47.1mm mounting-hole-offset 47.1mm
0
27
26
Connector_Dsub
DSUB-25_Male_Horizontal_P2.77x2.84mm_EdgePinOffset14.56mm_Housed_MountingHolesOffset8.20mm
25-pin D-Sub connector, horizontal/angled (90 deg), THT-mount, male, pitch 2.77x2.84mm, pin-PCB-offset 14.56mm, distance of mounting holes 47.1mm, distance of mounting holes to PCB edge 8.2mm, see https://disti-assets.s3.amazonaws.com/tonar/files/datasheets/16730.pdf
25-pin D-Sub connector horizontal angled 90deg THT male pitch 2.77x2.84mm pin-PCB-offset 14.56mm mounting-holes-distance 47.1mm mounting-hole-offset 47.1mm
0
27
26
Connector_Dsub
DSUB-25_Male_Horizontal_P2.77x2.84mm_EdgePinOffset14.56mm_Housed_MountingHolesOffset15.98mm
25-pin D-Sub connector, horizontal/angled (90 deg), THT-mount, male, pitch 2.77x2.84mm, pin-PCB-offset 14.56mm, distance of mounting holes 47.1mm, distance of mounting holes to PCB edge 15.979999999999999mm, see https://disti-assets.s3.amazonaws.com/tonar/files/datasheets/16730.pdf
25-pin D-Sub connector horizontal angled 90deg THT male pitch 2.77x2.84mm pin-PCB-offset 14.56mm mounting-holes-distance 47.1mm mounting-hole-offset 47.1mm
0
27
26
Connector_Dsub
DSUB-25_Male_Vertical_P2.77x2.84mm
25-pin D-Sub connector, straight/vertical, THT-mount, male, pitch 2.77x2.84mm, distance of mounting holes 47.1mm, see https://disti-assets.s3.amazonaws.com/tonar/files/datasheets/16730.pdf
25-pin D-Sub connector straight vertical THT male pitch 2.77x2.84mm mounting holes distance 47.1mm
0
25
25
Connector_Dsub
DSUB-25_Male_Vertical_P2.77x2.84mm_MountingHoles
25-pin D-Sub connector, straight/vertical, THT-mount, male, pitch 2.77x2.84mm, distance of mounting holes 47.1mm, see https://disti-assets.s3.amazonaws.com/tonar/files/datasheets/16730.pdf
25-pin D-Sub connector straight vertical THT male pitch 2.77x2.84mm mounting holes distance 47.1mm
0
27
26
Connector_Dsub
DSUB-26-HD_Female_Horizontal_P2.29x1.98mm_EdgePinOffset3.03mm_Housed_MountingHolesOffset4.94mm
26-pin D-Sub connector, horizontal/angled (90 deg), THT-mount, female, pitch 2.29x1.98mm, pin-PCB-offset 3.0300000000000002mm, distance of mounting holes 33.3mm, distance of mounting holes to PCB edge 4.9399999999999995mm, see https://disti-assets.s3.amazonaws.com/tonar/files/datasheets/16730.pdf
26-pin D-Sub connector horizontal angled 90deg THT female pitch 2.29x1.98mm pin-PCB-offset 3.0300000000000002mm mounting-holes-distance 33.3mm mounting-hole-offset 33.3mm
0
28
27
Connector_Dsub
DSUB-26-HD_Female_Horizontal_P2.29x1.98mm_EdgePinOffset8.35mm_Housed_MountingHolesOffset10.89mm
26-pin D-Sub connector, horizontal/angled (90 deg), THT-mount, female, pitch 2.29x1.98mm, pin-PCB-offset 8.35mm, distance of mounting holes 33.3mm, distance of mounting holes to PCB edge 10.889999999999999mm, see https://disti-assets.s3.amazonaws.com/tonar/files/datasheets/16730.pdf
26-pin D-Sub connector horizontal angled 90deg THT female pitch 2.29x1.98mm pin-PCB-offset 8.35mm mounting-holes-distance 33.3mm mounting-hole-offset 33.3mm
0
28
27
Connector_Dsub
DSUB-26-HD_Female_Horizontal_P2.29x1.98mm_EdgePinOffset9.40mm
26-pin D-Sub connector, horizontal/angled (90 deg), THT-mount, female, pitch 2.29x1.98mm, pin-PCB-offset 9.4mm, see http://docs-europe.electrocomponents.com/webdocs/1585/0900766b81585df2.pdf
26-pin D-Sub connector horizontal angled 90deg THT female pitch 2.29x1.98mm pin-PCB-offset 9.4mm
0
26
26
Connector_Dsub
DSUB-26-HD_Female_Horizontal_P2.29x2.54mm_EdgePinOffset9.40mm
26-pin D-Sub connector, horizontal/angled (90 deg), THT-mount, female, pitch 2.29x2.54mm, pin-PCB-offset 9.4mm, see http://docs-europe.electrocomponents.com/webdocs/1585/0900766b81585df2.pdf
26-pin D-Sub connector horizontal angled 90deg THT female pitch 2.29x2.54mm pin-PCB-offset 9.4mm
0
26
26
Connector_Dsub
DSUB-26-HD_Female_Vertical_P2.29x1.98mm_MountingHoles
26-pin D-Sub connector, straight/vertical, THT-mount, female, pitch 2.29x1.98mm, distance of mounting holes 33.3mm, see https://disti-assets.s3.amazonaws.com/tonar/files/datasheets/16730.pdf
26-pin D-Sub connector straight vertical THT female pitch 2.29x1.98mm mounting holes distance 33.3mm
0
28
27
Connector_Dsub
DSUB-26-HD_Male_Horizontal_P2.29x1.98mm_EdgePinOffset3.03mm_Housed_MountingHolesOffset4.94mm
26-pin D-Sub connector, horizontal/angled (90 deg), THT-mount, male, pitch 2.29x1.98mm, pin-PCB-offset 3.0300000000000002mm, distance of mounting holes 33.3mm, distance of mounting holes to PCB edge 4.9399999999999995mm, see https://disti-assets.s3.amazonaws.com/tonar/files/datasheets/16730.pdf
26-pin D-Sub connector horizontal angled 90deg THT male pitch 2.29x1.98mm pin-PCB-offset 3.0300000000000002mm mounting-holes-distance 33.3mm mounting-hole-offset 33.3mm
0
28
27
Connector_Dsub
DSUB-26-HD_Male_Horizontal_P2.29x1.98mm_EdgePinOffset8.35mm_Housed_MountingHolesOffset10.89mm
26-pin D-Sub connector, horizontal/angled (90 deg), THT-mount, male, pitch 2.29x1.98mm, pin-PCB-offset 8.35mm, distance of mounting holes 33.3mm, distance of mounting holes to PCB edge 10.889999999999999mm, see https://disti-assets.s3.amazonaws.com/tonar/files/datasheets/16730.pdf
26-pin D-Sub connector horizontal angled 90deg THT male pitch 2.29x1.98mm pin-PCB-offset 8.35mm mounting-holes-distance 33.3mm mounting-hole-offset 33.3mm
0
28
27
Connector_Dsub
DSUB-26-HD_Male_Horizontal_P2.29x1.98mm_EdgePinOffset9.40mm
26-pin D-Sub connector, horizontal/angled (90 deg), THT-mount, male, pitch 2.29x1.98mm, pin-PCB-offset 9.4mm, see http://docs-europe.electrocomponents.com/webdocs/1585/0900766b81585df2.pdf
26-pin D-Sub connector horizontal angled 90deg THT male pitch 2.29x1.98mm pin-PCB-offset 9.4mm
0
26
26
Connector_Dsub
DSUB-26-HD_Male_Horizontal_P2.29x2.54mm_EdgePinOffset9.40mm
26-pin D-Sub connector, horizontal/angled (90 deg), THT-mount, male, pitch 2.29x2.54mm, pin-PCB-offset 9.4mm, see http://docs-europe.electrocomponents.com/webdocs/1585/0900766b81585df2.pdf
26-pin D-Sub connector horizontal angled 90deg THT male pitch 2.29x2.54mm pin-PCB-offset 9.4mm
0
26
26
Connector_Dsub
DSUB-26-HD_Male_Vertical_P2.29x1.98mm_MountingHoles
26-pin D-Sub connector, straight/vertical, THT-mount, male, pitch 2.29x1.98mm, distance of mounting holes 33.3mm, see https://disti-assets.s3.amazonaws.com/tonar/files/datasheets/16730.pdf
26-pin D-Sub connector straight vertical THT male pitch 2.29x1.98mm mounting holes distance 33.3mm
0
28
27
Connector_Dsub
DSUB-37_Female_EdgeMount_P2.77mm
37-pin D-Sub connector, solder-cups edge-mounted, female, x-pin-pitch 2.77mm, distance of mounting holes 63.5mm, see https://disti-assets.s3.amazonaws.com/tonar/files/datasheets/16730.pdf
37-pin D-Sub connector edge mount solder cup female x-pin-pitch 2.77mm mounting holes distance 63.5mm
0
37
37
Connector_Dsub
DSUB-37_Female_Horizontal_P2.77x2.54mm_EdgePinOffset9.40mm
37-pin D-Sub connector, horizontal/angled (90 deg), THT-mount, female, pitch 2.77x2.54mm, pin-PCB-offset 9.4mm, see http://docs-europe.electrocomponents.com/webdocs/1585/0900766b81585df2.pdf
37-pin D-Sub connector horizontal angled 90deg THT female pitch 2.77x2.54mm pin-PCB-offset 9.4mm
0
37
37
Connector_Dsub
DSUB-37_Female_Horizontal_P2.77x2.84mm_EdgePinOffset4.94mm_Housed_MountingHolesOffset7.48mm
37-pin D-Sub connector, horizontal/angled (90 deg), THT-mount, female, pitch 2.77x2.84mm, pin-PCB-offset 4.9399999999999995mm, distance of mounting holes 63.5mm, distance of mounting holes to PCB edge 7.4799999999999995mm, see https://disti-assets.s3.amazonaws.com/tonar/files/datasheets/16730.pdf
37-pin D-Sub connector horizontal angled 90deg THT female pitch 2.77x2.84mm pin-PCB-offset 4.9399999999999995mm mounting-holes-distance 63.5mm mounting-hole-offset 63.5mm
0
39
38
Connector_Dsub
DSUB-37_Female_Horizontal_P2.77x2.84mm_EdgePinOffset7.70mm_Housed_MountingHolesOffset9.12mm
37-pin D-Sub connector, horizontal/angled (90 deg), THT-mount, female, pitch 2.77x2.84mm, pin-PCB-offset 7.699999999999999mm, distance of mounting holes 63.5mm, distance of mounting holes to PCB edge 9.12mm, see https://disti-assets.s3.amazonaws.com/tonar/files/datasheets/16730.pdf
37-pin D-Sub connector horizontal angled 90deg THT female pitch 2.77x2.84mm pin-PCB-offset 7.699999999999999mm mounting-holes-distance 63.5mm mounting-hole-offset 63.5mm
0
39
38
Connector_Dsub
DSUB-37_Female_Horizontal_P2.77x2.84mm_EdgePinOffset9.40mm
37-pin D-Sub connector, horizontal/angled (90 deg), THT-mount, female, pitch 2.77x2.84mm, pin-PCB-offset 9.4mm, see http://docs-europe.electrocomponents.com/webdocs/1585/0900766b81585df2.pdf
37-pin D-Sub connector horizontal angled 90deg THT female pitch 2.77x2.84mm pin-PCB-offset 9.4mm
0
37
37
Connector_Dsub
DSUB-37_Female_Horizontal_P2.77x2.84mm_EdgePinOffset9.90mm_Housed_MountingHolesOffset11.32mm
37-pin D-Sub connector, horizontal/angled (90 deg), THT-mount, female, pitch 2.77x2.84mm, pin-PCB-offset 9.9mm, distance of mounting holes 63.5mm, distance of mounting holes to PCB edge 11.32mm, see https://disti-assets.s3.amazonaws.com/tonar/files/datasheets/16730.pdf
37-pin D-Sub connector horizontal angled 90deg THT female pitch 2.77x2.84mm pin-PCB-offset 9.9mm mounting-holes-distance 63.5mm mounting-hole-offset 63.5mm
0
39
38
Connector_Dsub
DSUB-37_Female_Horizontal_P2.77x2.84mm_EdgePinOffset14.56mm_Housed_MountingHolesOffset8.20mm
37-pin D-Sub connector, horizontal/angled (90 deg), THT-mount, female, pitch 2.77x2.84mm, pin-PCB-offset 14.56mm, distance of mounting holes 63.5mm, distance of mounting holes to PCB edge 8.2mm, see https://disti-assets.s3.amazonaws.com/tonar/files/datasheets/16730.pdf
37-pin D-Sub connector horizontal angled 90deg THT female pitch 2.77x2.84mm pin-PCB-offset 14.56mm mounting-holes-distance 63.5mm mounting-hole-offset 63.5mm
0
39
38
Connector_Dsub
DSUB-37_Female_Horizontal_P2.77x2.84mm_EdgePinOffset14.56mm_Housed_MountingHolesOffset15.98mm
37-pin D-Sub connector, horizontal/angled (90 deg), THT-mount, female, pitch 2.77x2.84mm, pin-PCB-offset 14.56mm, distance of mounting holes 63.5mm, distance of mounting holes to PCB edge 15.979999999999999mm, see https://disti-assets.s3.amazonaws.com/tonar/files/datasheets/16730.pdf
37-pin D-Sub connector horizontal angled 90deg THT female pitch 2.77x2.84mm pin-PCB-offset 14.56mm mounting-holes-distance 63.5mm mounting-hole-offset 63.5mm
0
39
38
Connector_Dsub
DSUB-37_Female_Vertical_P2.77x2.84mm
37-pin D-Sub connector, straight/vertical, THT-mount, female, pitch 2.77x2.84mm, distance of mounting holes 63.5mm, see https://disti-assets.s3.amazonaws.com/tonar/files/datasheets/16730.pdf
37-pin D-Sub connector straight vertical THT female pitch 2.77x2.84mm mounting holes distance 63.5mm
0
37
37
Connector_Dsub
DSUB-37_Female_Vertical_P2.77x2.84mm_MountingHoles
37-pin D-Sub connector, straight/vertical, THT-mount, female, pitch 2.77x2.84mm, distance of mounting holes 63.5mm, see https://disti-assets.s3.amazonaws.com/tonar/files/datasheets/16730.pdf
37-pin D-Sub connector straight vertical THT female pitch 2.77x2.84mm mounting holes distance 63.5mm
0
39
38
Connector_Dsub
DSUB-37_Male_EdgeMount_P2.77mm
37-pin D-Sub connector, solder-cups edge-mounted, male, x-pin-pitch 2.77mm, distance of mounting holes 63.5mm, see https://disti-assets.s3.amazonaws.com/tonar/files/datasheets/16730.pdf
37-pin D-Sub connector edge mount solder cup male x-pin-pitch 2.77mm mounting holes distance 63.5mm
0
37
37
Connector_Dsub
DSUB-37_Male_Horizontal_P2.77x2.54mm_EdgePinOffset9.40mm
37-pin D-Sub connector, horizontal/angled (90 deg), THT-mount, male, pitch 2.77x2.54mm, pin-PCB-offset 9.4mm, see http://docs-europe.electrocomponents.com/webdocs/1585/0900766b81585df2.pdf
37-pin D-Sub connector horizontal angled 90deg THT male pitch 2.77x2.54mm pin-PCB-offset 9.4mm
0
37
37
Connector_Dsub
DSUB-37_Male_Horizontal_P2.77x2.84mm_EdgePinOffset4.94mm_Housed_MountingHolesOffset7.48mm
37-pin D-Sub connector, horizontal/angled (90 deg), THT-mount, male, pitch 2.77x2.84mm, pin-PCB-offset 4.9399999999999995mm, distance of mounting holes 63.5mm, distance of mounting holes to PCB edge 7.4799999999999995mm, see https://disti-assets.s3.amazonaws.com/tonar/files/datasheets/16730.pdf
37-pin D-Sub connector horizontal angled 90deg THT male pitch 2.77x2.84mm pin-PCB-offset 4.9399999999999995mm mounting-holes-distance 63.5mm mounting-hole-offset 63.5mm
0
39
38
Connector_Dsub
DSUB-37_Male_Horizontal_P2.77x2.84mm_EdgePinOffset7.70mm_Housed_MountingHolesOffset9.12mm
37-pin D-Sub connector, horizontal/angled (90 deg), THT-mount, male, pitch 2.77x2.84mm, pin-PCB-offset 7.699999999999999mm, distance of mounting holes 63.5mm, distance of mounting holes to PCB edge 9.12mm, see https://disti-assets.s3.amazonaws.com/tonar/files/datasheets/16730.pdf
37-pin D-Sub connector horizontal angled 90deg THT male pitch 2.77x2.84mm pin-PCB-offset 7.699999999999999mm mounting-holes-distance 63.5mm mounting-hole-offset 63.5mm
0
39
38
Connector_Dsub
DSUB-37_Male_Horizontal_P2.77x2.84mm_EdgePinOffset9.40mm
37-pin D-Sub connector, horizontal/angled (90 deg), THT-mount, male, pitch 2.77x2.84mm, pin-PCB-offset 9.4mm, see http://docs-europe.electrocomponents.com/webdocs/1585/0900766b81585df2.pdf
37-pin D-Sub connector horizontal angled 90deg THT male pitch 2.77x2.84mm pin-PCB-offset 9.4mm
0
37
37
Connector_Dsub
DSUB-37_Male_Horizontal_P2.77x2.84mm_EdgePinOffset9.90mm_Housed_MountingHolesOffset11.32mm
37-pin D-Sub connector, horizontal/angled (90 deg), THT-mount, male, pitch 2.77x2.84mm, pin-PCB-offset 9.9mm, distance of mounting holes 63.5mm, distance of mounting holes to PCB edge 11.32mm, see https://disti-assets.s3.amazonaws.com/tonar/files/datasheets/16730.pdf
37-pin D-Sub connector horizontal angled 90deg THT male pitch 2.77x2.84mm pin-PCB-offset 9.9mm mounting-holes-distance 63.5mm mounting-hole-offset 63.5mm
0
39
38
Connector_Dsub
DSUB-37_Male_Horizontal_P2.77x2.84mm_EdgePinOffset14.56mm_Housed_MountingHolesOffset8.20mm
37-pin D-Sub connector, horizontal/angled (90 deg), THT-mount, male, pitch 2.77x2.84mm, pin-PCB-offset 14.56mm, distance of mounting holes 63.5mm, distance of mounting holes to PCB edge 8.2mm, see https://disti-assets.s3.amazonaws.com/tonar/files/datasheets/16730.pdf
37-pin D-Sub connector horizontal angled 90deg THT male pitch 2.77x2.84mm pin-PCB-offset 14.56mm mounting-holes-distance 63.5mm mounting-hole-offset 63.5mm
0
39
38
Connector_Dsub
DSUB-37_Male_Horizontal_P2.77x2.84mm_EdgePinOffset14.56mm_Housed_MountingHolesOffset15.98mm
37-pin D-Sub connector, horizontal/angled (90 deg), THT-mount, male, pitch 2.77x2.84mm, pin-PCB-offset 14.56mm, distance of mounting holes 63.5mm, distance of mounting holes to PCB edge 15.979999999999999mm, see https://disti-assets.s3.amazonaws.com/tonar/files/datasheets/16730.pdf
37-pin D-Sub connector horizontal angled 90deg THT male pitch 2.77x2.84mm pin-PCB-offset 14.56mm mounting-holes-distance 63.5mm mounting-hole-offset 63.5mm
0
39
38
Connector_Dsub
DSUB-37_Male_Vertical_P2.77x2.84mm
37-pin D-Sub connector, straight/vertical, THT-mount, male, pitch 2.77x2.84mm, distance of mounting holes 63.5mm, see https://disti-assets.s3.amazonaws.com/tonar/files/datasheets/16730.pdf
37-pin D-Sub connector straight vertical THT male pitch 2.77x2.84mm mounting holes distance 63.5mm
0
37
37
Connector_Dsub
DSUB-37_Male_Vertical_P2.77x2.84mm_MountingHoles
37-pin D-Sub connector, straight/vertical, THT-mount, male, pitch 2.77x2.84mm, distance of mounting holes 63.5mm, see https://disti-assets.s3.amazonaws.com/tonar/files/datasheets/16730.pdf
37-pin D-Sub connector straight vertical THT male pitch 2.77x2.84mm mounting holes distance 63.5mm
0
39
38
Connector_Dsub
DSUB-44-HD_Female_Horizontal_P2.29x1.98mm_EdgePinOffset3.03mm_Housed_MountingHolesOffset4.94mm
44-pin D-Sub connector, horizontal/angled (90 deg), THT-mount, female, pitch 2.29x1.98mm, pin-PCB-offset 3.0300000000000002mm, distance of mounting holes 47.1mm, distance of mounting holes to PCB edge 4.9399999999999995mm, see https://disti-assets.s3.amazonaws.com/tonar/files/datasheets/16730.pdf
44-pin D-Sub connector horizontal angled 90deg THT female pitch 2.29x1.98mm pin-PCB-offset 3.0300000000000002mm mounting-holes-distance 47.1mm mounting-hole-offset 47.1mm
0
46
45
Connector_Dsub
DSUB-44-HD_Female_Horizontal_P2.29x1.98mm_EdgePinOffset8.35mm_Housed_MountingHolesOffset10.89mm
44-pin D-Sub connector, horizontal/angled (90 deg), THT-mount, female, pitch 2.29x1.98mm, pin-PCB-offset 8.35mm, distance of mounting holes 47.1mm, distance of mounting holes to PCB edge 10.889999999999999mm, see https://disti-assets.s3.amazonaws.com/tonar/files/datasheets/16730.pdf
44-pin D-Sub connector horizontal angled 90deg THT female pitch 2.29x1.98mm pin-PCB-offset 8.35mm mounting-holes-distance 47.1mm mounting-hole-offset 47.1mm
0
46
45
Connector_Dsub
DSUB-44-HD_Female_Horizontal_P2.29x1.98mm_EdgePinOffset9.40mm
44-pin D-Sub connector, horizontal/angled (90 deg), THT-mount, female, pitch 2.29x1.98mm, pin-PCB-offset 9.4mm, see http://docs-europe.electrocomponents.com/webdocs/1585/0900766b81585df2.pdf
44-pin D-Sub connector horizontal angled 90deg THT female pitch 2.29x1.98mm pin-PCB-offset 9.4mm
0
44
44
Connector_Dsub
DSUB-44-HD_Female_Horizontal_P2.29x2.54mm_EdgePinOffset9.40mm
44-pin D-Sub connector, horizontal/angled (90 deg), THT-mount, female, pitch 2.29x2.54mm, pin-PCB-offset 9.4mm, see http://docs-europe.electrocomponents.com/webdocs/1585/0900766b81585df2.pdf
44-pin D-Sub connector horizontal angled 90deg THT female pitch 2.29x2.54mm pin-PCB-offset 9.4mm
0
44
44
Connector_Dsub
DSUB-44-HD_Female_Vertical_P2.29x1.98mm_MountingHoles
44-pin D-Sub connector, straight/vertical, THT-mount, female, pitch 2.29x1.98mm, distance of mounting holes 47.1mm, see https://disti-assets.s3.amazonaws.com/tonar/files/datasheets/16730.pdf
44-pin D-Sub connector straight vertical THT female pitch 2.29x1.98mm mounting holes distance 47.1mm
0
46
45
Connector_Dsub
DSUB-44-HD_Male_Horizontal_P2.29x1.98mm_EdgePinOffset3.03mm_Housed_MountingHolesOffset4.94mm
44-pin D-Sub connector, horizontal/angled (90 deg), THT-mount, male, pitch 2.29x1.98mm, pin-PCB-offset 3.0300000000000002mm, distance of mounting holes 47.1mm, distance of mounting holes to PCB edge 4.9399999999999995mm, see https://disti-assets.s3.amazonaws.com/tonar/files/datasheets/16730.pdf
44-pin D-Sub connector horizontal angled 90deg THT male pitch 2.29x1.98mm pin-PCB-offset 3.0300000000000002mm mounting-holes-distance 47.1mm mounting-hole-offset 47.1mm
0
46
45
Connector_Dsub
DSUB-44-HD_Male_Horizontal_P2.29x1.98mm_EdgePinOffset8.35mm_Housed_MountingHolesOffset10.89mm
44-pin D-Sub connector, horizontal/angled (90 deg), THT-mount, male, pitch 2.29x1.98mm, pin-PCB-offset 8.35mm, distance of mounting holes 47.1mm, distance of mounting holes to PCB edge 10.889999999999999mm, see https://disti-assets.s3.amazonaws.com/tonar/files/datasheets/16730.pdf
44-pin D-Sub connector horizontal angled 90deg THT male pitch 2.29x1.98mm pin-PCB-offset 8.35mm mounting-holes-distance 47.1mm mounting-hole-offset 47.1mm
0
46
45
Connector_Dsub
DSUB-44-HD_Male_Horizontal_P2.29x1.98mm_EdgePinOffset9.40mm
44-pin D-Sub connector, horizontal/angled (90 deg), THT-mount, male, pitch 2.29x1.98mm, pin-PCB-offset 9.4mm, see http://docs-europe.electrocomponents.com/webdocs/1585/0900766b81585df2.pdf
44-pin D-Sub connector horizontal angled 90deg THT male pitch 2.29x1.98mm pin-PCB-offset 9.4mm
0
44
44
Connector_Dsub
DSUB-44-HD_Male_Horizontal_P2.29x2.54mm_EdgePinOffset9.40mm
44-pin D-Sub connector, horizontal/angled (90 deg), THT-mount, male, pitch 2.29x2.54mm, pin-PCB-offset 9.4mm, see http://docs-europe.electrocomponents.com/webdocs/1585/0900766b81585df2.pdf
44-pin D-Sub connector horizontal angled 90deg THT male pitch 2.29x2.54mm pin-PCB-offset 9.4mm
0
44
44
Connector_Dsub
DSUB-44-HD_Male_Vertical_P2.29x1.98mm_MountingHoles
44-pin D-Sub connector, straight/vertical, THT-mount, male, pitch 2.29x1.98mm, distance of mounting holes 47.1mm, see https://disti-assets.s3.amazonaws.com/tonar/files/datasheets/16730.pdf
44-pin D-Sub connector straight vertical THT male pitch 2.29x1.98mm mounting holes distance 47.1mm
0
46
45
Connector_Dsub
DSUB-62-HD_Female_Horizontal_P2.41x1.98mm_EdgePinOffset3.03mm_Housed_MountingHolesOffset4.94mm
62-pin D-Sub connector, horizontal/angled (90 deg), THT-mount, female, pitch 2.41x1.98mm, pin-PCB-offset 3.0300000000000002mm, distance of mounting holes 63.5mm, distance of mounting holes to PCB edge 4.9399999999999995mm, see https://disti-assets.s3.amazonaws.com/tonar/files/datasheets/16730.pdf
62-pin D-Sub connector horizontal angled 90deg THT female pitch 2.41x1.98mm pin-PCB-offset 3.0300000000000002mm mounting-holes-distance 63.5mm mounting-hole-offset 63.5mm
0
64
63
Connector_Dsub
DSUB-62-HD_Female_Horizontal_P2.41x1.98mm_EdgePinOffset8.35mm_Housed_MountingHolesOffset10.89mm
62-pin D-Sub connector, horizontal/angled (90 deg), THT-mount, female, pitch 2.41x1.98mm, pin-PCB-offset 8.35mm, distance of mounting holes 63.5mm, distance of mounting holes to PCB edge 10.889999999999999mm, see https://disti-assets.s3.amazonaws.com/tonar/files/datasheets/16730.pdf
62-pin D-Sub connector horizontal angled 90deg THT female pitch 2.41x1.98mm pin-PCB-offset 8.35mm mounting-holes-distance 63.5mm mounting-hole-offset 63.5mm
0
64
63
Connector_Dsub
DSUB-62-HD_Female_Horizontal_P2.41x1.98mm_EdgePinOffset9.40mm
62-pin D-Sub connector, horizontal/angled (90 deg), THT-mount, female, pitch 2.41x1.98mm, pin-PCB-offset 9.4mm, see http://docs-europe.electrocomponents.com/webdocs/1585/0900766b81585df2.pdf
62-pin D-Sub connector horizontal angled 90deg THT female pitch 2.41x1.98mm pin-PCB-offset 9.4mm
0
62
62
Connector_Dsub
DSUB-62-HD_Female_Horizontal_P2.41x2.54mm_EdgePinOffset9.40mm
62-pin D-Sub connector, horizontal/angled (90 deg), THT-mount, female, pitch 2.41x2.54mm, pin-PCB-offset 9.4mm, see http://docs-europe.electrocomponents.com/webdocs/1585/0900766b81585df2.pdf
62-pin D-Sub connector horizontal angled 90deg THT female pitch 2.41x2.54mm pin-PCB-offset 9.4mm
0
62
62
Connector_Dsub
DSUB-62-HD_Female_Vertical_P2.41x1.98mm_MountingHoles
62-pin D-Sub connector, straight/vertical, THT-mount, female, pitch 2.41x1.98mm, distance of mounting holes 63.5mm, see https://disti-assets.s3.amazonaws.com/tonar/files/datasheets/16730.pdf
62-pin D-Sub connector straight vertical THT female pitch 2.41x1.98mm mounting holes distance 63.5mm
0
64
63
Connector_Dsub
DSUB-62-HD_Male_Horizontal_P2.41x1.98mm_EdgePinOffset3.03mm_Housed_MountingHolesOffset4.94mm
62-pin D-Sub connector, horizontal/angled (90 deg), THT-mount, male, pitch 2.41x1.98mm, pin-PCB-offset 3.0300000000000002mm, distance of mounting holes 63.5mm, distance of mounting holes to PCB edge 4.9399999999999995mm, see https://disti-assets.s3.amazonaws.com/tonar/files/datasheets/16730.pdf
62-pin D-Sub connector horizontal angled 90deg THT male pitch 2.41x1.98mm pin-PCB-offset 3.0300000000000002mm mounting-holes-distance 63.5mm mounting-hole-offset 63.5mm
0
64
63
Connector_Dsub
DSUB-62-HD_Male_Horizontal_P2.41x1.98mm_EdgePinOffset8.35mm_Housed_MountingHolesOffset10.89mm
62-pin D-Sub connector, horizontal/angled (90 deg), THT-mount, male, pitch 2.41x1.98mm, pin-PCB-offset 8.35mm, distance of mounting holes 63.5mm, distance of mounting holes to PCB edge 10.889999999999999mm, see https://disti-assets.s3.amazonaws.com/tonar/files/datasheets/16730.pdf
62-pin D-Sub connector horizontal angled 90deg THT male pitch 2.41x1.98mm pin-PCB-offset 8.35mm mounting-holes-distance 63.5mm mounting-hole-offset 63.5mm
0
64
63
Connector_Dsub
DSUB-62-HD_Male_Horizontal_P2.41x1.98mm_EdgePinOffset9.40mm
62-pin D-Sub connector, horizontal/angled (90 deg), THT-mount, male, pitch 2.41x1.98mm, pin-PCB-offset 9.4mm, see http://docs-europe.electrocomponents.com/webdocs/1585/0900766b81585df2.pdf
62-pin D-Sub connector horizontal angled 90deg THT male pitch 2.41x1.98mm pin-PCB-offset 9.4mm
0
62
62
Connector_Dsub
DSUB-62-HD_Male_Horizontal_P2.41x2.54mm_EdgePinOffset9.40mm
62-pin D-Sub connector, horizontal/angled (90 deg), THT-mount, male, pitch 2.41x2.54mm, pin-PCB-offset 9.4mm, see http://docs-europe.electrocomponents.com/webdocs/1585/0900766b81585df2.pdf
62-pin D-Sub connector horizontal angled 90deg THT male pitch 2.41x2.54mm pin-PCB-offset 9.4mm
0
62
62
Connector_Dsub
DSUB-62-HD_Male_Vertical_P2.41x1.98mm_MountingHoles
62-pin D-Sub connector, straight/vertical, THT-mount, male, pitch 2.41x1.98mm, distance of mounting holes 63.5mm, see https://disti-assets.s3.amazonaws.com/tonar/files/datasheets/16730.pdf
62-pin D-Sub connector straight vertical THT male pitch 2.41x1.98mm mounting holes distance 63.5mm
0
64
63
Connector_FFC-FPC
Hirose_FH12-6S-0.5SH_1x06-1MP_P0.50mm_Horizontal
Hirose FH12, FFC/FPC connector, FH12-6S-0.5SH, 6 Pins per row (https://www.hirose.com/product/en/products/FH12/FH12-24S-0.5SH(55)/), generated with kicad-footprint-generator
connector Hirose FH12 horizontal
0
8
7
Connector_FFC-FPC
Hirose_FH12-8S-0.5SH_1x08-1MP_P0.50mm_Horizontal
Hirose FH12, FFC/FPC connector, FH12-8S-0.5SH, 8 Pins per row (https://www.hirose.com/product/en/products/FH12/FH12-24S-0.5SH(55)/), generated with kicad-footprint-generator
connector Hirose FH12 horizontal
0
10
9
Connector_FFC-FPC
Hirose_FH12-10S-0.5SH_1x10-1MP_P0.50mm_Horizontal
Hirose FH12, FFC/FPC connector, FH12-10S-0.5SH, 10 Pins per row (https://www.hirose.com/product/en/products/FH12/FH12-24S-0.5SH(55)/), generated with kicad-footprint-generator
connector Hirose FH12 horizontal
0
12
11
Connector_FFC-FPC
Hirose_FH12-11S-0.5SH_1x11-1MP_P0.50mm_Horizontal
Hirose FH12, FFC/FPC connector, FH12-11S-0.5SH, 11 Pins per row (https://www.hirose.com/product/en/products/FH12/FH12-24S-0.5SH(55)/), generated with kicad-footprint-generator
connector Hirose FH12 horizontal
0
13
12
Connector_FFC-FPC
Hirose_FH12-12S-0.5SH_1x12-1MP_P0.50mm_Horizontal
Hirose FH12, FFC/FPC connector, FH12-12S-0.5SH, 12 Pins per row (https://www.hirose.com/product/en/products/FH12/FH12-24S-0.5SH(55)/), generated with kicad-footprint-generator
connector Hirose FH12 horizontal
0
14
13
Connector_FFC-FPC
Hirose_FH12-13S-0.5SH_1x13-1MP_P0.50mm_Horizontal
Hirose FH12, FFC/FPC connector, FH12-13S-0.5SH, 13 Pins per row (https://www.hirose.com/product/en/products/FH12/FH12-24S-0.5SH(55)/), generated with kicad-footprint-generator
connector Hirose FH12 horizontal
0
15
14
Connector_FFC-FPC
Hirose_FH12-14S-0.5SH_1x14-1MP_P0.50mm_Horizontal
Hirose FH12, FFC/FPC connector, FH12-14S-0.5SH, 14 Pins per row (https://www.hirose.com/product/en/products/FH12/FH12-24S-0.5SH(55)/), generated with kicad-footprint-generator
connector Hirose FH12 horizontal
0
16
15
Connector_FFC-FPC
Hirose_FH12-15S-0.5SH_1x15-1MP_P0.50mm_Horizontal
Hirose FH12, FFC/FPC connector, FH12-15S-0.5SH, 15 Pins per row (https://www.hirose.com/product/en/products/FH12/FH12-24S-0.5SH(55)/), generated with kicad-footprint-generator
connector Hirose FH12 horizontal
0
17
16
Connector_FFC-FPC
Hirose_FH12-16S-0.5SH_1x16-1MP_P0.50mm_Horizontal
Hirose FH12, FFC/FPC connector, FH12-16S-0.5SH, 16 Pins per row (https://www.hirose.com/product/en/products/FH12/FH12-24S-0.5SH(55)/), generated with kicad-footprint-generator
connector Hirose FH12 horizontal
0
18
17
Connector_FFC-FPC
Hirose_FH12-17S-0.5SH_1x17-1MP_P0.50mm_Horizontal
Hirose FH12, FFC/FPC connector, FH12-17S-0.5SH, 17 Pins per row (https://www.hirose.com/product/en/products/FH12/FH12-24S-0.5SH(55)/), generated with kicad-footprint-generator
connector Hirose FH12 horizontal
0
19
18
Connector_FFC-FPC
Hirose_FH12-18S-0.5SH_1x18-1MP_P0.50mm_Horizontal
Hirose FH12, FFC/FPC connector, FH12-18S-0.5SH, 18 Pins per row (https://www.hirose.com/product/en/products/FH12/FH12-24S-0.5SH(55)/), generated with kicad-footprint-generator
connector Hirose FH12 horizontal
0
20
19
Connector_FFC-FPC
Hirose_FH12-19S-0.5SH_1x19-1MP_P0.50mm_Horizontal
Hirose FH12, FFC/FPC connector, FH12-19S-0.5SH, 19 Pins per row (https://www.hirose.com/product/en/products/FH12/FH12-24S-0.5SH(55)/), generated with kicad-footprint-generator
connector Hirose FH12 horizontal
0
21
20
Connector_FFC-FPC
Hirose_FH12-20S-0.5SH_1x20-1MP_P0.50mm_Horizontal
Hirose FH12, FFC/FPC connector, FH12-20S-0.5SH, 20 Pins per row (https://www.hirose.com/product/en/products/FH12/FH12-24S-0.5SH(55)/), generated with kicad-footprint-generator
connector Hirose FH12 horizontal
0
22
21
Connector_FFC-FPC
Hirose_FH12-22S-0.5SH_1x22-1MP_P0.50mm_Horizontal
Hirose FH12, FFC/FPC connector, FH12-22S-0.5SH, 22 Pins per row (https://www.hirose.com/product/en/products/FH12/FH12-24S-0.5SH(55)/), generated with kicad-footprint-generator
connector Hirose FH12 horizontal
0
24
23
Connector_FFC-FPC
Hirose_FH12-24S-0.5SH_1x24-1MP_P0.50mm_Horizontal
Hirose FH12, FFC/FPC connector, FH12-24S-0.5SH, 24 Pins per row (https://www.hirose.com/product/en/products/FH12/FH12-24S-0.5SH(55)/), generated with kicad-footprint-generator
connector Hirose FH12 horizontal
0
26
25
Connector_FFC-FPC
Hirose_FH12-25S-0.5SH_1x25-1MP_P0.50mm_Horizontal
Hirose FH12, FFC/FPC connector, FH12-25S-0.5SH, 25 Pins per row (https://www.hirose.com/product/en/products/FH12/FH12-24S-0.5SH(55)/), generated with kicad-footprint-generator
connector Hirose FH12 horizontal
0
27
26
Connector_FFC-FPC
Hirose_FH12-26S-0.5SH_1x26-1MP_P0.50mm_Horizontal
Hirose FH12, FFC/FPC connector, FH12-26S-0.5SH, 26 Pins per row (https://www.hirose.com/product/en/products/FH12/FH12-24S-0.5SH(55)/), generated with kicad-footprint-generator
connector Hirose FH12 horizontal
0
28
27
Connector_FFC-FPC
Hirose_FH12-28S-0.5SH_1x28-1MP_P0.50mm_Horizontal
Hirose FH12, FFC/FPC connector, FH12-28S-0.5SH, 28 Pins per row (https://www.hirose.com/product/en/products/FH12/FH12-24S-0.5SH(55)/), generated with kicad-footprint-generator
connector Hirose FH12 horizontal
0
30
29
Connector_FFC-FPC
Hirose_FH12-30S-0.5SH_1x30-1MP_P0.50mm_Horizontal
Hirose FH12, FFC/FPC connector, FH12-30S-0.5SH, 30 Pins per row (https://www.hirose.com/product/en/products/FH12/FH12-24S-0.5SH(55)/), generated with kicad-footprint-generator
connector Hirose FH12 horizontal
0
32
31
Connector_FFC-FPC
Hirose_FH12-32S-0.5SH_1x32-1MP_P0.50mm_Horizontal
Hirose FH12, FFC/FPC connector, FH12-32S-0.5SH, 32 Pins per row (https://www.hirose.com/product/en/products/FH12/FH12-24S-0.5SH(55)/), generated with kicad-footprint-generator
connector Hirose FH12 horizontal
0
34
33
Connector_FFC-FPC
Hirose_FH12-33S-0.5SH_1x33-1MP_P0.50mm_Horizontal
Hirose FH12, FFC/FPC connector, FH12-33S-0.5SH, 33 Pins per row (https://www.hirose.com/product/en/products/FH12/FH12-24S-0.5SH(55)/), generated with kicad-footprint-generator
connector Hirose FH12 horizontal
0
35
34
Connector_FFC-FPC
Hirose_FH12-34S-0.5SH_1x34-1MP_P0.50mm_Horizontal
Hirose FH12, FFC/FPC connector, FH12-34S-0.5SH, 34 Pins per row (https://www.hirose.com/product/en/products/FH12/FH12-24S-0.5SH(55)/), generated with kicad-footprint-generator
connector Hirose FH12 horizontal
0
36
35
Connector_FFC-FPC
Hirose_FH12-35S-0.5SH_1x35-1MP_P0.50mm_Horizontal
Hirose FH12, FFC/FPC connector, FH12-35S-0.5SH, 35 Pins per row (https://www.hirose.com/product/en/products/FH12/FH12-24S-0.5SH(55)/), generated with kicad-footprint-generator
connector Hirose FH12 horizontal
0
37
36
Connector_FFC-FPC
Hirose_FH12-36S-0.5SH_1x36-1MP_P0.50mm_Horizontal
Hirose FH12, FFC/FPC connector, FH12-36S-0.5SH, 36 Pins per row (https://www.hirose.com/product/en/products/FH12/FH12-24S-0.5SH(55)/), generated with kicad-footprint-generator
connector Hirose FH12 horizontal
0
38
37
Connector_FFC-FPC
Hirose_FH12-40S-0.5SH_1x40-1MP_P0.50mm_Horizontal
Hirose FH12, FFC/FPC connector, FH12-40S-0.5SH, 40 Pins per row (https://www.hirose.com/product/en/products/FH12/FH12-24S-0.5SH(55)/), generated with kicad-footprint-generator
connector Hirose FH12 horizontal
0
42
41
Connector_FFC-FPC
Hirose_FH12-45S-0.5SH_1x45-1MP_P0.50mm_Horizontal
Hirose FH12, FFC/FPC connector, FH12-45S-0.5SH, 45 Pins per row (https://www.hirose.com/product/en/products/FH12/FH12-24S-0.5SH(55)/), generated with kicad-footprint-generator
connector Hirose FH12 horizontal
0
47
46
Connector_FFC-FPC
Hirose_FH12-50S-0.5SH_1x50-1MP_P0.50mm_Horizontal
Hirose FH12, FFC/FPC connector, FH12-50S-0.5SH, 50 Pins per row (https://www.hirose.com/product/en/products/FH12/FH12-24S-0.5SH(55)/), generated with kicad-footprint-generator
connector Hirose FH12 horizontal
0
52
51
Connector_FFC-FPC
Hirose_FH12-53S-0.5SH_1x53-1MP_P0.50mm_Horizontal
Hirose FH12, FFC/FPC connector, FH12-53S-0.5SH, 53 Pins per row (https://www.hirose.com/product/en/products/FH12/FH12-24S-0.5SH(55)/), generated with kicad-footprint-generator
connector Hirose FH12 horizontal
0
55
54
Connector_FFC-FPC
Hirose_FH41-30S-0.5SH_1x30_1MP_1SH_P0.5mm_Horizontal
Hirose FH41, FFC/FPC connector, FH41-30S-0.5SH, 30 Pins per row (https://www.hirose.com/fr/product/document?clcode=CL0580-2218-5-05&productname=FH41-30S-0.5SH(05)&series=FH41&documenttype=2DDrawing&lang=fr&documentid=0001001704)
connector Hirose FH41 horizontal
0
38
32
Connector_FFC-FPC
JAE_FF0825SA1_2Rows-25Pins_P0.40mm_Horizontal
Molex JAE 0.2mm pitch, 1mm overall height FFC/FPC connector, FF0825SA1, 25 Circuits (http://www.jae.com/z-en/pdf_download_exec.cfm?param=SJ108178.pdf), generated with kicad-footprint-generator
connector JAE  top entry
0
25
25
Connector_FFC-FPC
JAE_FF0829SA1_2Rows-29Pins_P0.40mm_Horizontal
Molex JAE 0.2mm pitch, 1mm overall height FFC/FPC connector, FF0829SA1, 29 Circuits (http://www.jae.com/z-en/pdf_download_exec.cfm?param=SJ108178.pdf), generated with kicad-footprint-generator
connector JAE  top entry
0
29
29
Connector_FFC-FPC
JAE_FF0841SA1_2Rows-41Pins_P0.40mm_Horizontal
Molex JAE 0.2mm pitch, 1mm overall height FFC/FPC connector, FF0841SA1, 41 Circuits (http://www.jae.com/z-en/pdf_download_exec.cfm?param=SJ108178.pdf), generated with kicad-footprint-generator
connector JAE  top entry
0
41
41
Connector_FFC-FPC
JAE_FF0851SA1_2Rows-51Pins_P0.40mm_Horizontal
Molex JAE 0.2mm pitch, 1mm overall height FFC/FPC connector, FF0851SA1, 51 Circuits (http://www.jae.com/z-en/pdf_download_exec.cfm?param=SJ108178.pdf), generated with kicad-footprint-generator
connector JAE  top entry
0
51
51
Connector_FFC-FPC
JAE_FF0871SA1_2Rows-71Pins_P0.40mm_Horizontal
Molex JAE 0.2mm pitch, 1mm overall height FFC/FPC connector, FF0871SA1, 71 Circuits (http://www.jae.com/z-en/pdf_download_exec.cfm?param=SJ108178.pdf), generated with kicad-footprint-generator
connector JAE  top entry
0
71
71
Connector_FFC-FPC
JAE_FF0881SA1_2Rows-81Pins_P0.40mm_Horizontal
Molex JAE 0.2mm pitch, 1mm overall height FFC/FPC connector, FF0881SA1, 81 Circuits (http://www.jae.com/z-en/pdf_download_exec.cfm?param=SJ108178.pdf), generated with kicad-footprint-generator
connector JAE  top entry
0
81
81
Connector_FFC-FPC
Jushuo_AFC07-S06FCA-00_1x6-1MP_P0.50_Horizontal
Jushuo AFC07, FFC/FPC connector, AFC07-S06FCA-00, 6 Pins per row (https://datasheet.lcsc.com/lcsc/1811040204_JUSHUO-AFC07-S32FCC-00_C11061.pdf)
connector jushuo horizontal
0
8
7
Connector_FFC-FPC
Jushuo_AFC07-S24FCA-00_1x24-1MP_P0.50_Horizontal
Jushuo AFC07, FFC/FPC connector, AFC07-S24FCA-00, 24 Pins per row (https://datasheet.lcsc.com/lcsc/1811040204_JUSHUO-AFC07-S32FCC-00_C11061.pdf)
connector jushuo horizontal
0
26
25
Connector_FFC-FPC
Molex_52559-3652_2x18-1MP_P0.5mm_Vertical
Molex 0.50mm Pitch Easy-On Type FFC/FPC, 52559-3652, 36 Circuits (https://www.molex.com/pdm_docs/sd/525593652_sd.pdf)
connector Molex top entry
0
40
37
Connector_FFC-FPC
Molex_54132-5033_1x50-1MP_P0.5mm_Horizontal
Molex FFC/FPC connector, 50 bottom-side contacts, 0.5mm pitch, 2.0mm height, https://www.molex.com/pdm_docs/sd/541325033_sd.pdf
FFC FPC
0
54
51
Connector_FFC-FPC
Molex_54548-1071_1x10-1MP_P0.5mm_Horizontal
Molex FFC/FPC connector, 10 bottom-side contacts, 0.5mm pitch, 1.2mm height, https://www.molex.com/pdm_docs/sd/545481071_sd.pdf
FFC FPC connector
0
12
11
Connector_FFC-FPC
Molex_200528-0040_1x04-1MP_P1.00mm_Horizontal
Molex Molex 1.00mm Pitch Easy-On BackFlip, Right-Angle, Bottom Contact FFC/FPC, 200528-0040, 4 Circuits (https://www.molex.com/pdm_docs/sd/2005280040_sd.pdf), generated with kicad-footprint-generator
connector Molex  top entry
0
6
5
Connector_FFC-FPC
Molex_200528-0050_1x05-1MP_P1.00mm_Horizontal
Molex Molex 1.00mm Pitch Easy-On BackFlip, Right-Angle, Bottom Contact FFC/FPC, 200528-0050, 5 Circuits (https://www.molex.com/pdm_docs/sd/2005280050_sd.pdf), generated with kicad-footprint-generator
connector Molex  top entry
0
7
6
Connector_FFC-FPC
Molex_200528-0060_1x06-1MP_P1.00mm_Horizontal
Molex Molex 1.00mm Pitch Easy-On BackFlip, Right-Angle, Bottom Contact FFC/FPC, 200528-0060, 6 Circuits (https://www.molex.com/pdm_docs/sd/2005280060_sd.pdf), generated with kicad-footprint-generator
connector Molex  top entry
0
8
7
Connector_FFC-FPC
Molex_200528-0070_1x07-1MP_P1.00mm_Horizontal
Molex Molex 1.00mm Pitch Easy-On BackFlip, Right-Angle, Bottom Contact FFC/FPC, 200528-0070, 7 Circuits (https://www.molex.com/pdm_docs/sd/2005280070_sd.pdf), generated with kicad-footprint-generator
connector Molex  top entry
0
9
8
Connector_FFC-FPC
Molex_200528-0080_1x08-1MP_P1.00mm_Horizontal
Molex Molex 1.00mm Pitch Easy-On BackFlip, Right-Angle, Bottom Contact FFC/FPC, 200528-0080, 8 Circuits (https://www.molex.com/pdm_docs/sd/2005280080_sd.pdf), generated with kicad-footprint-generator
connector Molex  top entry
0
10
9
Connector_FFC-FPC
Molex_200528-0090_1x09-1MP_P1.00mm_Horizontal
Molex Molex 1.00mm Pitch Easy-On BackFlip, Right-Angle, Bottom Contact FFC/FPC, 200528-0090, 9 Circuits (https://www.molex.com/pdm_docs/sd/2005280090_sd.pdf), generated with kicad-footprint-generator
connector Molex  top entry
0
11
10
Connector_FFC-FPC
Molex_200528-0100_1x10-1MP_P1.00mm_Horizontal
Molex Molex 1.00mm Pitch Easy-On BackFlip, Right-Angle, Bottom Contact FFC/FPC, 200528-0100, 10 Circuits (https://www.molex.com/pdm_docs/sd/2005280100_sd.pdf), generated with kicad-footprint-generator
connector Molex  top entry
0
12
11
Connector_FFC-FPC
Molex_200528-0110_1x11-1MP_P1.00mm_Horizontal
Molex Molex 1.00mm Pitch Easy-On BackFlip, Right-Angle, Bottom Contact FFC/FPC, 200528-0110, 11 Circuits (https://www.molex.com/pdm_docs/sd/2005280110_sd.pdf), generated with kicad-footprint-generator
connector Molex  top entry
0
13
12
Connector_FFC-FPC
Molex_200528-0120_1x12-1MP_P1.00mm_Horizontal
Molex Molex 1.00mm Pitch Easy-On BackFlip, Right-Angle, Bottom Contact FFC/FPC, 200528-0120, 12 Circuits (https://www.molex.com/pdm_docs/sd/2005280120_sd.pdf), generated with kicad-footprint-generator
connector Molex  top entry
0
14
13
Connector_FFC-FPC
Molex_200528-0130_1x13-1MP_P1.00mm_Horizontal
Molex Molex 1.00mm Pitch Easy-On BackFlip, Right-Angle, Bottom Contact FFC/FPC, 200528-0130, 13 Circuits (https://www.molex.com/pdm_docs/sd/2005280130_sd.pdf), generated with kicad-footprint-generator
connector Molex  top entry
0
15
14
Connector_FFC-FPC
Molex_200528-0140_1x14-1MP_P1.00mm_Horizontal
Molex Molex 1.00mm Pitch Easy-On BackFlip, Right-Angle, Bottom Contact FFC/FPC, 200528-0140, 14 Circuits (https://www.molex.com/pdm_docs/sd/2005280140_sd.pdf), generated with kicad-footprint-generator
connector Molex  top entry
0
16
15
Connector_FFC-FPC
Molex_200528-0150_1x15-1MP_P1.00mm_Horizontal
Molex Molex 1.00mm Pitch Easy-On BackFlip, Right-Angle, Bottom Contact FFC/FPC, 200528-0150, 15 Circuits (https://www.molex.com/pdm_docs/sd/2005280150_sd.pdf), generated with kicad-footprint-generator
connector Molex  top entry
0
17
16
Connector_FFC-FPC
Molex_200528-0160_1x16-1MP_P1.00mm_Horizontal
Molex Molex 1.00mm Pitch Easy-On BackFlip, Right-Angle, Bottom Contact FFC/FPC, 200528-0160, 16 Circuits (https://www.molex.com/pdm_docs/sd/2005280160_sd.pdf), generated with kicad-footprint-generator
connector Molex  top entry
0
18
17
Connector_FFC-FPC
Molex_200528-0170_1x17-1MP_P1.00mm_Horizontal
Molex Molex 1.00mm Pitch Easy-On BackFlip, Right-Angle, Bottom Contact FFC/FPC, 200528-0170, 17 Circuits (https://www.molex.com/pdm_docs/sd/2005280170_sd.pdf), generated with kicad-footprint-generator
connector Molex  top entry
0
19
18
Connector_FFC-FPC
Molex_200528-0180_1x18-1MP_P1.00mm_Horizontal
Molex Molex 1.00mm Pitch Easy-On BackFlip, Right-Angle, Bottom Contact FFC/FPC, 200528-0180, 18 Circuits (https://www.molex.com/pdm_docs/sd/2005280180_sd.pdf), generated with kicad-footprint-generator
connector Molex  top entry
0
20
19
Connector_FFC-FPC
Molex_200528-0190_1x19-1MP_P1.00mm_Horizontal
Molex Molex 1.00mm Pitch Easy-On BackFlip, Right-Angle, Bottom Contact FFC/FPC, 200528-0190, 19 Circuits (https://www.molex.com/pdm_docs/sd/2005280190_sd.pdf), generated with kicad-footprint-generator
connector Molex  top entry
0
21
20
Connector_FFC-FPC
Molex_200528-0200_1x20-1MP_P1.00mm_Horizontal
Molex Molex 1.00mm Pitch Easy-On BackFlip, Right-Angle, Bottom Contact FFC/FPC, 200528-0200, 20 Circuits (https://www.molex.com/pdm_docs/sd/2005280200_sd.pdf), generated with kicad-footprint-generator
connector Molex  top entry
0
22
21
Connector_FFC-FPC
Molex_200528-0210_1x21-1MP_P1.00mm_Horizontal
Molex Molex 1.00mm Pitch Easy-On BackFlip, Right-Angle, Bottom Contact FFC/FPC, 200528-0210, 21 Circuits (https://www.molex.com/pdm_docs/sd/2005280210_sd.pdf), generated with kicad-footprint-generator
connector Molex  top entry
0
23
22
Connector_FFC-FPC
Molex_200528-0220_1x22-1MP_P1.00mm_Horizontal
Molex Molex 1.00mm Pitch Easy-On BackFlip, Right-Angle, Bottom Contact FFC/FPC, 200528-0220, 22 Circuits (https://www.molex.com/pdm_docs/sd/2005280220_sd.pdf), generated with kicad-footprint-generator
connector Molex  top entry
0
24
23
Connector_FFC-FPC
Molex_200528-0230_1x23-1MP_P1.00mm_Horizontal
Molex Molex 1.00mm Pitch Easy-On BackFlip, Right-Angle, Bottom Contact FFC/FPC, 200528-0230, 23 Circuits (https://www.molex.com/pdm_docs/sd/2005280230_sd.pdf), generated with kicad-footprint-generator
connector Molex  top entry
0
25
24
Connector_FFC-FPC
Molex_200528-0240_1x24-1MP_P1.00mm_Horizontal
Molex Molex 1.00mm Pitch Easy-On BackFlip, Right-Angle, Bottom Contact FFC/FPC, 200528-0240, 24 Circuits (https://www.molex.com/pdm_docs/sd/2005280240_sd.pdf), generated with kicad-footprint-generator
connector Molex  top entry
0
26
25
Connector_FFC-FPC
Molex_200528-0250_1x25-1MP_P1.00mm_Horizontal
Molex Molex 1.00mm Pitch Easy-On BackFlip, Right-Angle, Bottom Contact FFC/FPC, 200528-0250, 25 Circuits (https://www.molex.com/pdm_docs/sd/2005280250_sd.pdf), generated with kicad-footprint-generator
connector Molex  top entry
0
27
26
Connector_FFC-FPC
Molex_200528-0260_1x26-1MP_P1.00mm_Horizontal
Molex Molex 1.00mm Pitch Easy-On BackFlip, Right-Angle, Bottom Contact FFC/FPC, 200528-0260, 26 Circuits (https://www.molex.com/pdm_docs/sd/2005280260_sd.pdf), generated with kicad-footprint-generator
connector Molex  top entry
0
28
27
Connector_FFC-FPC
Molex_200528-0270_1x27-1MP_P1.00mm_Horizontal
Molex Molex 1.00mm Pitch Easy-On BackFlip, Right-Angle, Bottom Contact FFC/FPC, 200528-0270, 27 Circuits (https://www.molex.com/pdm_docs/sd/2005280270_sd.pdf), generated with kicad-footprint-generator
connector Molex  top entry
0
29
28
Connector_FFC-FPC
Molex_200528-0280_1x28-1MP_P1.00mm_Horizontal
Molex Molex 1.00mm Pitch Easy-On BackFlip, Right-Angle, Bottom Contact FFC/FPC, 200528-0280, 28 Circuits (https://www.molex.com/pdm_docs/sd/2005280280_sd.pdf), generated with kicad-footprint-generator
connector Molex  top entry
0
30
29
Connector_FFC-FPC
Molex_200528-0290_1x29-1MP_P1.00mm_Horizontal
Molex Molex 1.00mm Pitch Easy-On BackFlip, Right-Angle, Bottom Contact FFC/FPC, 200528-0290, 29 Circuits (https://www.molex.com/pdm_docs/sd/2005280290_sd.pdf), generated with kicad-footprint-generator
connector Molex  top entry
0
31
30
Connector_FFC-FPC
Molex_200528-0300_1x30-1MP_P1.00mm_Horizontal
Molex Molex 1.00mm Pitch Easy-On BackFlip, Right-Angle, Bottom Contact FFC/FPC, 200528-0300, 30 Circuits (https://www.molex.com/pdm_docs/sd/2005280300_sd.pdf), generated with kicad-footprint-generator
connector Molex  top entry
0
32
31
Connector_FFC-FPC
Molex_502231-1500_1x15-1SH_P0.5mm_Vertical
Molex 0.50mm Pitch Easy-On Type FFC/FPC Connector, For LVDS, 6.05mm Height, Vertical, Surface Mount, ZIF, 15 Circuits (https://www.molex.com/pdm_docs/sd/5022311500_sd.pdf)
molex FFC/FPC connector Pitch 0.5mm vertical
0
17
16
Connector_FFC-FPC
Molex_502231-2400_1x24-1SH_P0.5mm_Vertical
Molex 0.50mm Pitch Easy-On Type FFC/FPC Connector, For LVDS, 6.05mm Height, Vertical, Surface Mount, ZIF, 24 Circuits (https://www.molex.com/pdm_docs/sd/5022312400_sd.pdf)
molex FFC/FPC connector Pitch 0.5mm vertical
0
26
25
Connector_FFC-FPC
Molex_502231-3300_1x33-1SH_P0.5mm_Vertical
Molex 0.50mm Pitch Easy-On Type FFC/FPC Connector, For LVDS, 6.05mm Height, Vertical, Surface Mount, ZIF, 33 Circuits (https://www.molex.com/pdm_docs/sd/5022313300_sd.pdf)
molex FFC/FPC connector Pitch 0.5mm vertical
0
36
34
Connector_FFC-FPC
Molex_502244-1530_1x15-1MP_P0.5mm_Horizontal
Molex 0.50mm Pitch Easy-On Type FFC/FPC Connector, For LVDS, 2.33mm Height, Right Angle, Surface Mount, ZIF, Bottom Contact Style, 15 Circuits (http://www.molex.com/pdm_docs/sd/5022441530_sd.pdf)
molex FFC/FPC connector Pitch 0.5mm right angle
0
19
16
Connector_FFC-FPC
Molex_502244-2430_1x24-1MP_P0.5mm_Horizontal
Molex 0.50mm Pitch Easy-On Type FFC/FPC Connector, For LVDS, 2.33mm Height, Right Angle, Surface Mount, ZIF, Bottom Contact Style, 24 Circuits (http://www.molex.com/pdm_docs/sd/5022441530_sd.pdf)
molex FFC/FPC connector Pitch 0.5mm right angle
0
28
25
Connector_FFC-FPC
Molex_502244-3330_1x33-1MP_P0.5mm_Horizontal
Molex 0.50mm Pitch Easy-On Type FFC/FPC Connector, For LVDS, 2.33mm Height, Right Angle, Surface Mount, ZIF, Bottom Contact Style, 33 Circuits (http://www.molex.com/pdm_docs/sd/5022441530_sd.pdf)
molex FFC/FPC connector Pitch 0.5mm right angle
0
39
34
Connector_FFC-FPC
Molex_502250-1791_2Rows-17Pins-1MP_P0.60mm_Horizontal
Molex Molex 0.30mm Pitch Easy-On BackFlip Type FFC/FPC, 502250-1791, 17 Circuits (http://www.molex.com/pdm_docs/sd/5022501791_sd.pdf), generated with kicad-footprint-generator
connector Molex  top entry
0
19
18
Connector_FFC-FPC
Molex_502250-2191_2Rows-21Pins-1MP_P0.60mm_Horizontal
Molex Molex 0.30mm Pitch Easy-On BackFlip Type FFC/FPC, 502250-2191, 21 Circuits (http://www.molex.com/pdm_docs/sd/5022502191_sd.pdf), generated with kicad-footprint-generator
connector Molex  top entry
0
23
22
Connector_FFC-FPC
Molex_502250-2391_2Rows-23Pins-1MP_P0.60mm_Horizontal
Molex Molex 0.30mm Pitch Easy-On BackFlip Type FFC/FPC, 502250-2391, 23 Circuits (http://www.molex.com/pdm_docs/sd/5022502391_sd.pdf), generated with kicad-footprint-generator
connector Molex  top entry
0
25
24
Connector_FFC-FPC
Molex_502250-2791_2Rows-27Pins-1MP_P0.60mm_Horizontal
Molex Molex 0.30mm Pitch Easy-On BackFlip Type FFC/FPC, 502250-2791, 27 Circuits (http://www.molex.com/pdm_docs/sd/5022502791_sd.pdf), generated with kicad-footprint-generator
connector Molex  top entry
0
29
28
Connector_FFC-FPC
Molex_502250-3391_2Rows-33Pins-1MP_P0.60mm_Horizontal
Molex Molex 0.30mm Pitch Easy-On BackFlip Type FFC/FPC, 502250-3391, 33 Circuits (http://www.molex.com/pdm_docs/sd/5022503391_sd.pdf), generated with kicad-footprint-generator
connector Molex  top entry
0
35
34
Connector_FFC-FPC
Molex_502250-3591_2Rows-35Pins-1MP_P0.60mm_Horizontal
Molex Molex 0.30mm Pitch Easy-On BackFlip Type FFC/FPC, 502250-3591, 35 Circuits (http://www.molex.com/pdm_docs/sd/5022503591_sd.pdf), generated with kicad-footprint-generator
connector Molex  top entry
0
37
36
Connector_FFC-FPC
Molex_502250-3991_2Rows-39Pins-1MP_P0.60mm_Horizontal
Molex Molex 0.30mm Pitch Easy-On BackFlip Type FFC/FPC, 502250-3991, 39 Circuits (http://www.molex.com/pdm_docs/sd/5022503991_sd.pdf), generated with kicad-footprint-generator
connector Molex  top entry
0
41
40
Connector_FFC-FPC
Molex_502250-4191_2Rows-41Pins-1MP_P0.60mm_Horizontal
Molex Molex 0.30mm Pitch Easy-On BackFlip Type FFC/FPC, 502250-4191, 41 Circuits (http://www.molex.com/pdm_docs/sd/5022504191_sd.pdf), generated with kicad-footprint-generator
connector Molex  top entry
0
43
42
Connector_FFC-FPC
Molex_502250-5191_2Rows-51Pins-1MP_P0.60mm_Horizontal
Molex Molex 0.30mm Pitch Easy-On BackFlip Type FFC/FPC, 502250-5191, 51 Circuits (http://www.molex.com/pdm_docs/sd/5022505191_sd.pdf), generated with kicad-footprint-generator
connector Molex  top entry
0
53
52
Connector_FFC-FPC
Omron_XF2M-4015-1A_1x40-1MP_P0.5mm_Horizontal
Omron FPC connector, 40 top-side contacts, 0.5mm pitch, SMT, https://omronfs.omron.com/en_US/ecb/products/pdf/en-xf2m.pdf
omron fpc xf2m
0
42
41
Connector_FFC-FPC
TE_0-1734839-5_1x05-1MP_P0.5mm_Horizontal
TE FPC connector, 05 top-side contacts, 0.5mm pitch, SMT, https://www.te.com/commerce/DocumentDelivery/DDEController?Action=showdoc&DocId=Customer+Drawing%7F1734839%7FC%7Fpdf%7FEnglish%7FENG_CD_1734839_C_C_1734839.pdf%7F4-1734839-0
te fpc 1734839
0
7
6
Connector_FFC-FPC
TE_0-1734839-6_1x06-1MP_P0.5mm_Horizontal
TE FPC connector, 06 top-side contacts, 0.5mm pitch, SMT, https://www.te.com/commerce/DocumentDelivery/DDEController?Action=showdoc&DocId=Customer+Drawing%7F1734839%7FC%7Fpdf%7FEnglish%7FENG_CD_1734839_C_C_1734839.pdf%7F4-1734839-0
te fpc 1734839
0
8
7
Connector_FFC-FPC
TE_0-1734839-7_1x07-1MP_P0.5mm_Horizontal
TE FPC connector, 07 top-side contacts, 0.5mm pitch, SMT, https://www.te.com/commerce/DocumentDelivery/DDEController?Action=showdoc&DocId=Customer+Drawing%7F1734839%7FC%7Fpdf%7FEnglish%7FENG_CD_1734839_C_C_1734839.pdf%7F4-1734839-0
te fpc 1734839
0
9
8
Connector_FFC-FPC
TE_0-1734839-8_1x08-1MP_P0.5mm_Horizontal
TE FPC connector, 08 top-side contacts, 0.5mm pitch, SMT, https://www.te.com/commerce/DocumentDelivery/DDEController?Action=showdoc&DocId=Customer+Drawing%7F1734839%7FC%7Fpdf%7FEnglish%7FENG_CD_1734839_C_C_1734839.pdf%7F4-1734839-0
te fpc 1734839
0
10
9
Connector_FFC-FPC
TE_0-1734839-9_1x09-1MP_P0.5mm_Horizontal
TE FPC connector, 09 top-side contacts, 0.5mm pitch, SMT, https://www.te.com/commerce/DocumentDelivery/DDEController?Action=showdoc&DocId=Customer+Drawing%7F1734839%7FC%7Fpdf%7FEnglish%7FENG_CD_1734839_C_C_1734839.pdf%7F4-1734839-0
te fpc 1734839
0
11
10
Connector_FFC-FPC
TE_1-84952-0_1x10-1MP_P1.0mm_Horizontal
TE FPC connector, 10 bottom-side contacts, 1.0mm pitch, 1.0mm height, SMT, http://www.te.com/commerce/DocumentDelivery/DDEController?Action=srchrtrv&DocNm=84952&DocType=Customer+Drawing&DocLang=English&DocFormat=pdf&PartCntxt=84952-4
te fpc 84952
0
12
11
Connector_FFC-FPC
TE_1-84952-1_1x11-1MP_P1.0mm_Horizontal
TE FPC connector, 11 bottom-side contacts, 1.0mm pitch, 1.0mm height, SMT, http://www.te.com/commerce/DocumentDelivery/DDEController?Action=srchrtrv&DocNm=84952&DocType=Customer+Drawing&DocLang=English&DocFormat=pdf&PartCntxt=84952-4
te fpc 84952
0
13
12
Connector_FFC-FPC
TE_1-84952-2_1x12-1MP_P1.0mm_Horizontal
TE FPC connector, 12 bottom-side contacts, 1.0mm pitch, 1.0mm height, SMT, http://www.te.com/commerce/DocumentDelivery/DDEController?Action=srchrtrv&DocNm=84952&DocType=Customer+Drawing&DocLang=English&DocFormat=pdf&PartCntxt=84952-4
te fpc 84952
0
14
13
Connector_FFC-FPC
TE_1-84952-3_1x13-1MP_P1.0mm_Horizontal
TE FPC connector, 13 bottom-side contacts, 1.0mm pitch, 1.0mm height, SMT, http://www.te.com/commerce/DocumentDelivery/DDEController?Action=srchrtrv&DocNm=84952&DocType=Customer+Drawing&DocLang=English&DocFormat=pdf&PartCntxt=84952-4
te fpc 84952
0
15
14
Connector_FFC-FPC
TE_1-84952-4_1x14-1MP_P1.0mm_Horizontal
TE FPC connector, 14 bottom-side contacts, 1.0mm pitch, 1.0mm height, SMT, http://www.te.com/commerce/DocumentDelivery/DDEController?Action=srchrtrv&DocNm=84952&DocType=Customer+Drawing&DocLang=English&DocFormat=pdf&PartCntxt=84952-4
te fpc 84952
0
16
15
Connector_FFC-FPC
TE_1-84952-5_1x15-1MP_P1.0mm_Horizontal
TE FPC connector, 15 bottom-side contacts, 1.0mm pitch, 1.0mm height, SMT, http://www.te.com/commerce/DocumentDelivery/DDEController?Action=srchrtrv&DocNm=84952&DocType=Customer+Drawing&DocLang=English&DocFormat=pdf&PartCntxt=84952-4
te fpc 84952
0
17
16
Connector_FFC-FPC
TE_1-84952-6_1x16-1MP_P1.0mm_Horizontal
TE FPC connector, 16 bottom-side contacts, 1.0mm pitch, 1.0mm height, SMT, http://www.te.com/commerce/DocumentDelivery/DDEController?Action=srchrtrv&DocNm=84952&DocType=Customer+Drawing&DocLang=English&DocFormat=pdf&PartCntxt=84952-4
te fpc 84952
0
18
17
Connector_FFC-FPC
TE_1-84952-7_1x17-1MP_P1.0mm_Horizontal
TE FPC connector, 17 bottom-side contacts, 1.0mm pitch, 1.0mm height, SMT, http://www.te.com/commerce/DocumentDelivery/DDEController?Action=srchrtrv&DocNm=84952&DocType=Customer+Drawing&DocLang=English&DocFormat=pdf&PartCntxt=84952-4
te fpc 84952
0
19
18
Connector_FFC-FPC
TE_1-84952-8_1x18-1MP_P1.0mm_Horizontal
TE FPC connector, 18 bottom-side contacts, 1.0mm pitch, 1.0mm height, SMT, http://www.te.com/commerce/DocumentDelivery/DDEController?Action=srchrtrv&DocNm=84952&DocType=Customer+Drawing&DocLang=English&DocFormat=pdf&PartCntxt=84952-4
te fpc 84952
0
20
19
Connector_FFC-FPC
TE_1-84952-9_1x19-1MP_P1.0mm_Horizontal
TE FPC connector, 19 bottom-side contacts, 1.0mm pitch, 1.0mm height, SMT, http://www.te.com/commerce/DocumentDelivery/DDEController?Action=srchrtrv&DocNm=84952&DocType=Customer+Drawing&DocLang=English&DocFormat=pdf&PartCntxt=84952-4
te fpc 84952
0
21
20
Connector_FFC-FPC
TE_1-84953-0_1x10-1MP_P1.0mm_Horizontal
TE FPC connector, 10 top-side contacts, 1.0mm pitch, 1.0mm height, SMT, http://www.te.com/commerce/DocumentDelivery/DDEController?Action=srchrtrv&DocNm=84953&DocType=Customer+Drawing&DocLang=English&DocFormat=pdf&PartCntxt=84953-4
te fpc 84953
0
12
11
Connector_FFC-FPC
TE_1-84953-1_1x11-1MP_P1.0mm_Horizontal
TE FPC connector, 11 top-side contacts, 1.0mm pitch, 1.0mm height, SMT, http://www.te.com/commerce/DocumentDelivery/DDEController?Action=srchrtrv&DocNm=84953&DocType=Customer+Drawing&DocLang=English&DocFormat=pdf&PartCntxt=84953-4
te fpc 84953
0
13
12
Connector_FFC-FPC
TE_1-84953-2_1x12-1MP_P1.0mm_Horizontal
TE FPC connector, 12 top-side contacts, 1.0mm pitch, 1.0mm height, SMT, http://www.te.com/commerce/DocumentDelivery/DDEController?Action=srchrtrv&DocNm=84953&DocType=Customer+Drawing&DocLang=English&DocFormat=pdf&PartCntxt=84953-4
te fpc 84953
0
14
13
Connector_FFC-FPC
TE_1-84953-3_1x13-1MP_P1.0mm_Horizontal
TE FPC connector, 13 top-side contacts, 1.0mm pitch, 1.0mm height, SMT, http://www.te.com/commerce/DocumentDelivery/DDEController?Action=srchrtrv&DocNm=84953&DocType=Customer+Drawing&DocLang=English&DocFormat=pdf&PartCntxt=84953-4
te fpc 84953
0
15
14
Connector_FFC-FPC
TE_1-84953-4_1x14-1MP_P1.0mm_Horizontal
TE FPC connector, 14 top-side contacts, 1.0mm pitch, 1.0mm height, SMT, http://www.te.com/commerce/DocumentDelivery/DDEController?Action=srchrtrv&DocNm=84953&DocType=Customer+Drawing&DocLang=English&DocFormat=pdf&PartCntxt=84953-4
te fpc 84953
0
16
15
Connector_FFC-FPC
TE_1-84953-5_1x15-1MP_P1.0mm_Horizontal
TE FPC connector, 15 top-side contacts, 1.0mm pitch, 1.0mm height, SMT, http://www.te.com/commerce/DocumentDelivery/DDEController?Action=srchrtrv&DocNm=84953&DocType=Customer+Drawing&DocLang=English&DocFormat=pdf&PartCntxt=84953-4
te fpc 84953
0
17
16
Connector_FFC-FPC
TE_1-84953-6_1x16-1MP_P1.0mm_Horizontal
TE FPC connector, 16 top-side contacts, 1.0mm pitch, 1.0mm height, SMT, http://www.te.com/commerce/DocumentDelivery/DDEController?Action=srchrtrv&DocNm=84953&DocType=Customer+Drawing&DocLang=English&DocFormat=pdf&PartCntxt=84953-4
te fpc 84953
0
18
17
Connector_FFC-FPC
TE_1-84953-7_1x17-1MP_P1.0mm_Horizontal
TE FPC connector, 17 top-side contacts, 1.0mm pitch, 1.0mm height, SMT, http://www.te.com/commerce/DocumentDelivery/DDEController?Action=srchrtrv&DocNm=84953&DocType=Customer+Drawing&DocLang=English&DocFormat=pdf&PartCntxt=84953-4
te fpc 84953
0
19
18
Connector_FFC-FPC
TE_1-84953-8_1x18-1MP_P1.0mm_Horizontal
TE FPC connector, 18 top-side contacts, 1.0mm pitch, 1.0mm height, SMT, http://www.te.com/commerce/DocumentDelivery/DDEController?Action=srchrtrv&DocNm=84953&DocType=Customer+Drawing&DocLang=English&DocFormat=pdf&PartCntxt=84953-4
te fpc 84953
0
20
19
Connector_FFC-FPC
TE_1-84953-9_1x19-1MP_P1.0mm_Horizontal
TE FPC connector, 19 top-side contacts, 1.0mm pitch, 1.0mm height, SMT, http://www.te.com/commerce/DocumentDelivery/DDEController?Action=srchrtrv&DocNm=84953&DocType=Customer+Drawing&DocLang=English&DocFormat=pdf&PartCntxt=84953-4
te fpc 84953
0
21
20
Connector_FFC-FPC
TE_1-1734839-0_1x10-1MP_P0.5mm_Horizontal
TE FPC connector, 10 top-side contacts, 0.5mm pitch, SMT, https://www.te.com/commerce/DocumentDelivery/DDEController?Action=showdoc&DocId=Customer+Drawing%7F1734839%7FC%7Fpdf%7FEnglish%7FENG_CD_1734839_C_C_1734839.pdf%7F4-1734839-0
te fpc 1734839
0
12
11
Connector_FFC-FPC
TE_1-1734839-1_1x11-1MP_P0.5mm_Horizontal
TE FPC connector, 11 top-side contacts, 0.5mm pitch, SMT, https://www.te.com/commerce/DocumentDelivery/DDEController?Action=showdoc&DocId=Customer+Drawing%7F1734839%7FC%7Fpdf%7FEnglish%7FENG_CD_1734839_C_C_1734839.pdf%7F4-1734839-0
te fpc 1734839
0
13
12
Connector_FFC-FPC
TE_1-1734839-2_1x12-1MP_P0.5mm_Horizontal
TE FPC connector, 12 top-side contacts, 0.5mm pitch, SMT, https://www.te.com/commerce/DocumentDelivery/DDEController?Action=showdoc&DocId=Customer+Drawing%7F1734839%7FC%7Fpdf%7FEnglish%7FENG_CD_1734839_C_C_1734839.pdf%7F4-1734839-0
te fpc 1734839
0
14
13
Connector_FFC-FPC
TE_1-1734839-3_1x13-1MP_P0.5mm_Horizontal
TE FPC connector, 13 top-side contacts, 0.5mm pitch, SMT, https://www.te.com/commerce/DocumentDelivery/DDEController?Action=showdoc&DocId=Customer+Drawing%7F1734839%7FC%7Fpdf%7FEnglish%7FENG_CD_1734839_C_C_1734839.pdf%7F4-1734839-0
te fpc 1734839
0
15
14
Connector_FFC-FPC
TE_1-1734839-4_1x14-1MP_P0.5mm_Horizontal
TE FPC connector, 14 top-side contacts, 0.5mm pitch, SMT, https://www.te.com/commerce/DocumentDelivery/DDEController?Action=showdoc&DocId=Customer+Drawing%7F1734839%7FC%7Fpdf%7FEnglish%7FENG_CD_1734839_C_C_1734839.pdf%7F4-1734839-0
te fpc 1734839
0
16
15
Connector_FFC-FPC
TE_1-1734839-5_1x15-1MP_P0.5mm_Horizontal
TE FPC connector, 15 top-side contacts, 0.5mm pitch, SMT, https://www.te.com/commerce/DocumentDelivery/DDEController?Action=showdoc&DocId=Customer+Drawing%7F1734839%7FC%7Fpdf%7FEnglish%7FENG_CD_1734839_C_C_1734839.pdf%7F4-1734839-0
te fpc 1734839
0
17
16
Connector_FFC-FPC
TE_1-1734839-6_1x16-1MP_P0.5mm_Horizontal
TE FPC connector, 16 top-side contacts, 0.5mm pitch, SMT, https://www.te.com/commerce/DocumentDelivery/DDEController?Action=showdoc&DocId=Customer+Drawing%7F1734839%7FC%7Fpdf%7FEnglish%7FENG_CD_1734839_C_C_1734839.pdf%7F4-1734839-0
te fpc 1734839
0
18
17
Connector_FFC-FPC
TE_1-1734839-7_1x17-1MP_P0.5mm_Horizontal
TE FPC connector, 17 top-side contacts, 0.5mm pitch, SMT, https://www.te.com/commerce/DocumentDelivery/DDEController?Action=showdoc&DocId=Customer+Drawing%7F1734839%7FC%7Fpdf%7FEnglish%7FENG_CD_1734839_C_C_1734839.pdf%7F4-1734839-0
te fpc 1734839
0
19
18
Connector_FFC-FPC
TE_1-1734839-8_1x18-1MP_P0.5mm_Horizontal
TE FPC connector, 18 top-side contacts, 0.5mm pitch, SMT, https://www.te.com/commerce/DocumentDelivery/DDEController?Action=showdoc&DocId=Customer+Drawing%7F1734839%7FC%7Fpdf%7FEnglish%7FENG_CD_1734839_C_C_1734839.pdf%7F4-1734839-0
te fpc 1734839
0
20
19
Connector_FFC-FPC
TE_1-1734839-9_1x19-1MP_P0.5mm_Horizontal
TE FPC connector, 19 top-side contacts, 0.5mm pitch, SMT, https://www.te.com/commerce/DocumentDelivery/DDEController?Action=showdoc&DocId=Customer+Drawing%7F1734839%7FC%7Fpdf%7FEnglish%7FENG_CD_1734839_C_C_1734839.pdf%7F4-1734839-0
te fpc 1734839
0
21
20
Connector_FFC-FPC
TE_2-84952-0_1x20-1MP_P1.0mm_Horizontal
TE FPC connector, 20 bottom-side contacts, 1.0mm pitch, 1.0mm height, SMT, http://www.te.com/commerce/DocumentDelivery/DDEController?Action=srchrtrv&DocNm=84952&DocType=Customer+Drawing&DocLang=English&DocFormat=pdf&PartCntxt=84952-4
te fpc 84952
0
22
21
Connector_FFC-FPC
TE_2-84952-1_1x21-1MP_P1.0mm_Horizontal
TE FPC connector, 21 bottom-side contacts, 1.0mm pitch, 1.0mm height, SMT, http://www.te.com/commerce/DocumentDelivery/DDEController?Action=srchrtrv&DocNm=84952&DocType=Customer+Drawing&DocLang=English&DocFormat=pdf&PartCntxt=84952-4
te fpc 84952
0
23
22
Connector_FFC-FPC
TE_2-84952-2_1x22-1MP_P1.0mm_Horizontal
TE FPC connector, 22 bottom-side contacts, 1.0mm pitch, 1.0mm height, SMT, http://www.te.com/commerce/DocumentDelivery/DDEController?Action=srchrtrv&DocNm=84952&DocType=Customer+Drawing&DocLang=English&DocFormat=pdf&PartCntxt=84952-4
te fpc 84952
0
24
23
Connector_FFC-FPC
TE_2-84952-3_1x23-1MP_P1.0mm_Horizontal
TE FPC connector, 23 bottom-side contacts, 1.0mm pitch, 1.0mm height, SMT, http://www.te.com/commerce/DocumentDelivery/DDEController?Action=srchrtrv&DocNm=84952&DocType=Customer+Drawing&DocLang=English&DocFormat=pdf&PartCntxt=84952-4
te fpc 84952
0
25
24
Connector_FFC-FPC
TE_2-84952-4_1x24-1MP_P1.0mm_Horizontal
TE FPC connector, 24 bottom-side contacts, 1.0mm pitch, 1.0mm height, SMT, http://www.te.com/commerce/DocumentDelivery/DDEController?Action=srchrtrv&DocNm=84952&DocType=Customer+Drawing&DocLang=English&DocFormat=pdf&PartCntxt=84952-4
te fpc 84952
0
26
25
Connector_FFC-FPC
TE_2-84952-5_1x25-1MP_P1.0mm_Horizontal
TE FPC connector, 25 bottom-side contacts, 1.0mm pitch, 1.0mm height, SMT, http://www.te.com/commerce/DocumentDelivery/DDEController?Action=srchrtrv&DocNm=84952&DocType=Customer+Drawing&DocLang=English&DocFormat=pdf&PartCntxt=84952-4
te fpc 84952
0
27
26
Connector_FFC-FPC
TE_2-84952-6_1x26-1MP_P1.0mm_Horizontal
TE FPC connector, 26 bottom-side contacts, 1.0mm pitch, 1.0mm height, SMT, http://www.te.com/commerce/DocumentDelivery/DDEController?Action=srchrtrv&DocNm=84952&DocType=Customer+Drawing&DocLang=English&DocFormat=pdf&PartCntxt=84952-4
te fpc 84952
0
28
27
Connector_FFC-FPC
TE_2-84952-7_1x27-1MP_P1.0mm_Horizontal
TE FPC connector, 27 bottom-side contacts, 1.0mm pitch, 1.0mm height, SMT, http://www.te.com/commerce/DocumentDelivery/DDEController?Action=srchrtrv&DocNm=84952&DocType=Customer+Drawing&DocLang=English&DocFormat=pdf&PartCntxt=84952-4
te fpc 84952
0
29
28
Connector_FFC-FPC
TE_2-84952-8_1x28-1MP_P1.0mm_Horizontal
TE FPC connector, 28 bottom-side contacts, 1.0mm pitch, 1.0mm height, SMT, http://www.te.com/commerce/DocumentDelivery/DDEController?Action=srchrtrv&DocNm=84952&DocType=Customer+Drawing&DocLang=English&DocFormat=pdf&PartCntxt=84952-4
te fpc 84952
0
30
29
Connector_FFC-FPC
TE_2-84952-9_1x29-1MP_P1.0mm_Horizontal
TE FPC connector, 29 bottom-side contacts, 1.0mm pitch, 1.0mm height, SMT, http://www.te.com/commerce/DocumentDelivery/DDEController?Action=srchrtrv&DocNm=84952&DocType=Customer+Drawing&DocLang=English&DocFormat=pdf&PartCntxt=84952-4
te fpc 84952
0
31
30
Connector_FFC-FPC
TE_2-84953-0_1x20-1MP_P1.0mm_Horizontal
TE FPC connector, 20 top-side contacts, 1.0mm pitch, 1.0mm height, SMT, http://www.te.com/commerce/DocumentDelivery/DDEController?Action=srchrtrv&DocNm=84953&DocType=Customer+Drawing&DocLang=English&DocFormat=pdf&PartCntxt=84953-4
te fpc 84953
0
22
21
Connector_FFC-FPC
TE_2-84953-1_1x21-1MP_P1.0mm_Horizontal
TE FPC connector, 21 top-side contacts, 1.0mm pitch, 1.0mm height, SMT, http://www.te.com/commerce/DocumentDelivery/DDEController?Action=srchrtrv&DocNm=84953&DocType=Customer+Drawing&DocLang=English&DocFormat=pdf&PartCntxt=84953-4
te fpc 84953
0
23
22
Connector_FFC-FPC
TE_2-84953-2_1x22-1MP_P1.0mm_Horizontal
TE FPC connector, 22 top-side contacts, 1.0mm pitch, 1.0mm height, SMT, http://www.te.com/commerce/DocumentDelivery/DDEController?Action=srchrtrv&DocNm=84953&DocType=Customer+Drawing&DocLang=English&DocFormat=pdf&PartCntxt=84953-4
te fpc 84953
0
24
23
Connector_FFC-FPC
TE_2-84953-3_1x23-1MP_P1.0mm_Horizontal
TE FPC connector, 23 top-side contacts, 1.0mm pitch, 1.0mm height, SMT, http://www.te.com/commerce/DocumentDelivery/DDEController?Action=srchrtrv&DocNm=84953&DocType=Customer+Drawing&DocLang=English&DocFormat=pdf&PartCntxt=84953-4
te fpc 84953
0
25
24
Connector_FFC-FPC
TE_2-84953-4_1x24-1MP_P1.0mm_Horizontal
TE FPC connector, 24 top-side contacts, 1.0mm pitch, 1.0mm height, SMT, http://www.te.com/commerce/DocumentDelivery/DDEController?Action=srchrtrv&DocNm=84953&DocType=Customer+Drawing&DocLang=English&DocFormat=pdf&PartCntxt=84953-4
te fpc 84953
0
26
25
Connector_FFC-FPC
TE_2-84953-5_1x25-1MP_P1.0mm_Horizontal
TE FPC connector, 25 top-side contacts, 1.0mm pitch, 1.0mm height, SMT, http://www.te.com/commerce/DocumentDelivery/DDEController?Action=srchrtrv&DocNm=84953&DocType=Customer+Drawing&DocLang=English&DocFormat=pdf&PartCntxt=84953-4
te fpc 84953
0
27
26
Connector_FFC-FPC
TE_2-84953-6_1x26-1MP_P1.0mm_Horizontal
TE FPC connector, 26 top-side contacts, 1.0mm pitch, 1.0mm height, SMT, http://www.te.com/commerce/DocumentDelivery/DDEController?Action=srchrtrv&DocNm=84953&DocType=Customer+Drawing&DocLang=English&DocFormat=pdf&PartCntxt=84953-4
te fpc 84953
0
28
27
Connector_FFC-FPC
TE_2-84953-7_1x27-1MP_P1.0mm_Horizontal
TE FPC connector, 27 top-side contacts, 1.0mm pitch, 1.0mm height, SMT, http://www.te.com/commerce/DocumentDelivery/DDEController?Action=srchrtrv&DocNm=84953&DocType=Customer+Drawing&DocLang=English&DocFormat=pdf&PartCntxt=84953-4
te fpc 84953
0
29
28
Connector_FFC-FPC
TE_2-84953-8_1x28-1MP_P1.0mm_Horizontal
TE FPC connector, 28 top-side contacts, 1.0mm pitch, 1.0mm height, SMT, http://www.te.com/commerce/DocumentDelivery/DDEController?Action=srchrtrv&DocNm=84953&DocType=Customer+Drawing&DocLang=English&DocFormat=pdf&PartCntxt=84953-4
te fpc 84953
0
30
29
Connector_FFC-FPC
TE_2-84953-9_1x29-1MP_P1.0mm_Horizontal
TE FPC connector, 29 top-side contacts, 1.0mm pitch, 1.0mm height, SMT, http://www.te.com/commerce/DocumentDelivery/DDEController?Action=srchrtrv&DocNm=84953&DocType=Customer+Drawing&DocLang=English&DocFormat=pdf&PartCntxt=84953-4
te fpc 84953
0
31
30
Connector_FFC-FPC
TE_2-1734839-0_1x20-1MP_P0.5mm_Horizontal
TE FPC connector, 20 top-side contacts, 0.5mm pitch, SMT, https://www.te.com/commerce/DocumentDelivery/DDEController?Action=showdoc&DocId=Customer+Drawing%7F1734839%7FC%7Fpdf%7FEnglish%7FENG_CD_1734839_C_C_1734839.pdf%7F4-1734839-0
te fpc 1734839
0
22
21
Connector_FFC-FPC
TE_2-1734839-1_1x21-1MP_P0.5mm_Horizontal
TE FPC connector, 21 top-side contacts, 0.5mm pitch, SMT, https://www.te.com/commerce/DocumentDelivery/DDEController?Action=showdoc&DocId=Customer+Drawing%7F1734839%7FC%7Fpdf%7FEnglish%7FENG_CD_1734839_C_C_1734839.pdf%7F4-1734839-0
te fpc 1734839
0
23
22
Connector_FFC-FPC
TE_2-1734839-2_1x22-1MP_P0.5mm_Horizontal
TE FPC connector, 22 top-side contacts, 0.5mm pitch, SMT, https://www.te.com/commerce/DocumentDelivery/DDEController?Action=showdoc&DocId=Customer+Drawing%7F1734839%7FC%7Fpdf%7FEnglish%7FENG_CD_1734839_C_C_1734839.pdf%7F4-1734839-0
te fpc 1734839
0
24
23
Connector_FFC-FPC
TE_2-1734839-3_1x23-1MP_P0.5mm_Horizontal
TE FPC connector, 23 top-side contacts, 0.5mm pitch, SMT, https://www.te.com/commerce/DocumentDelivery/DDEController?Action=showdoc&DocId=Customer+Drawing%7F1734839%7FC%7Fpdf%7FEnglish%7FENG_CD_1734839_C_C_1734839.pdf%7F4-1734839-0
te fpc 1734839
0
25
24
Connector_FFC-FPC
TE_2-1734839-4_1x24-1MP_P0.5mm_Horizontal
TE FPC connector, 24 top-side contacts, 0.5mm pitch, SMT, https://www.te.com/commerce/DocumentDelivery/DDEController?Action=showdoc&DocId=Customer+Drawing%7F1734839%7FC%7Fpdf%7FEnglish%7FENG_CD_1734839_C_C_1734839.pdf%7F4-1734839-0
te fpc 1734839
0
26
25
Connector_FFC-FPC
TE_2-1734839-5_1x25-1MP_P0.5mm_Horizontal
TE FPC connector, 25 top-side contacts, 0.5mm pitch, SMT, https://www.te.com/commerce/DocumentDelivery/DDEController?Action=showdoc&DocId=Customer+Drawing%7F1734839%7FC%7Fpdf%7FEnglish%7FENG_CD_1734839_C_C_1734839.pdf%7F4-1734839-0
te fpc 1734839
0
27
26
Connector_FFC-FPC
TE_2-1734839-6_1x26-1MP_P0.5mm_Horizontal
TE FPC connector, 26 top-side contacts, 0.5mm pitch, SMT, https://www.te.com/commerce/DocumentDelivery/DDEController?Action=showdoc&DocId=Customer+Drawing%7F1734839%7FC%7Fpdf%7FEnglish%7FENG_CD_1734839_C_C_1734839.pdf%7F4-1734839-0
te fpc 1734839
0
28
27
Connector_FFC-FPC
TE_2-1734839-7_1x27-1MP_P0.5mm_Horizontal
TE FPC connector, 27 top-side contacts, 0.5mm pitch, SMT, https://www.te.com/commerce/DocumentDelivery/DDEController?Action=showdoc&DocId=Customer+Drawing%7F1734839%7FC%7Fpdf%7FEnglish%7FENG_CD_1734839_C_C_1734839.pdf%7F4-1734839-0
te fpc 1734839
0
29
28
Connector_FFC-FPC
TE_2-1734839-8_1x28-1MP_P0.5mm_Horizontal
TE FPC connector, 28 top-side contacts, 0.5mm pitch, SMT, https://www.te.com/commerce/DocumentDelivery/DDEController?Action=showdoc&DocId=Customer+Drawing%7F1734839%7FC%7Fpdf%7FEnglish%7FENG_CD_1734839_C_C_1734839.pdf%7F4-1734839-0
te fpc 1734839
0
30
29
Connector_FFC-FPC
TE_2-1734839-9_1x29-1MP_P0.5mm_Horizontal
TE FPC connector, 29 top-side contacts, 0.5mm pitch, SMT, https://www.te.com/commerce/DocumentDelivery/DDEController?Action=showdoc&DocId=Customer+Drawing%7F1734839%7FC%7Fpdf%7FEnglish%7FENG_CD_1734839_C_C_1734839.pdf%7F4-1734839-0
te fpc 1734839
0
31
30
Connector_FFC-FPC
TE_3-84952-0_1x30-1MP_P1.0mm_Horizontal
TE FPC connector, 30 bottom-side contacts, 1.0mm pitch, 1.0mm height, SMT, http://www.te.com/commerce/DocumentDelivery/DDEController?Action=srchrtrv&DocNm=84952&DocType=Customer+Drawing&DocLang=English&DocFormat=pdf&PartCntxt=84952-4
te fpc 84952
0
32
31
Connector_FFC-FPC
TE_3-84953-0_1x30-1MP_P1.0mm_Horizontal
TE FPC connector, 30 top-side contacts, 1.0mm pitch, 1.0mm height, SMT, http://www.te.com/commerce/DocumentDelivery/DDEController?Action=srchrtrv&DocNm=84953&DocType=Customer+Drawing&DocLang=English&DocFormat=pdf&PartCntxt=84953-4
te fpc 84953
0
32
31
Connector_FFC-FPC
TE_3-1734839-0_1x30-1MP_P0.5mm_Horizontal
TE FPC connector, 30 top-side contacts, 0.5mm pitch, SMT, https://www.te.com/commerce/DocumentDelivery/DDEController?Action=showdoc&DocId=Customer+Drawing%7F1734839%7FC%7Fpdf%7FEnglish%7FENG_CD_1734839_C_C_1734839.pdf%7F4-1734839-0
te fpc 1734839
0
32
31
Connector_FFC-FPC
TE_3-1734839-1_1x31-1MP_P0.5mm_Horizontal
TE FPC connector, 31 top-side contacts, 0.5mm pitch, SMT, https://www.te.com/commerce/DocumentDelivery/DDEController?Action=showdoc&DocId=Customer+Drawing%7F1734839%7FC%7Fpdf%7FEnglish%7FENG_CD_1734839_C_C_1734839.pdf%7F4-1734839-0
te fpc 1734839
0
33
32
Connector_FFC-FPC
TE_3-1734839-2_1x32-1MP_P0.5mm_Horizontal
TE FPC connector, 32 top-side contacts, 0.5mm pitch, SMT, https://www.te.com/commerce/DocumentDelivery/DDEController?Action=showdoc&DocId=Customer+Drawing%7F1734839%7FC%7Fpdf%7FEnglish%7FENG_CD_1734839_C_C_1734839.pdf%7F4-1734839-0
te fpc 1734839
0
34
33
Connector_FFC-FPC
TE_3-1734839-3_1x33-1MP_P0.5mm_Horizontal
TE FPC connector, 33 top-side contacts, 0.5mm pitch, SMT, https://www.te.com/commerce/DocumentDelivery/DDEController?Action=showdoc&DocId=Customer+Drawing%7F1734839%7FC%7Fpdf%7FEnglish%7FENG_CD_1734839_C_C_1734839.pdf%7F4-1734839-0
te fpc 1734839
0
35
34
Connector_FFC-FPC
TE_3-1734839-4_1x34-1MP_P0.5mm_Horizontal
TE FPC connector, 34 top-side contacts, 0.5mm pitch, SMT, https://www.te.com/commerce/DocumentDelivery/DDEController?Action=showdoc&DocId=Customer+Drawing%7F1734839%7FC%7Fpdf%7FEnglish%7FENG_CD_1734839_C_C_1734839.pdf%7F4-1734839-0
te fpc 1734839
0
36
35
Connector_FFC-FPC
TE_3-1734839-5_1x35-1MP_P0.5mm_Horizontal
TE FPC connector, 35 top-side contacts, 0.5mm pitch, SMT, https://www.te.com/commerce/DocumentDelivery/DDEController?Action=showdoc&DocId=Customer+Drawing%7F1734839%7FC%7Fpdf%7FEnglish%7FENG_CD_1734839_C_C_1734839.pdf%7F4-1734839-0
te fpc 1734839
0
37
36
Connector_FFC-FPC
TE_3-1734839-6_1x36-1MP_P0.5mm_Horizontal
TE FPC connector, 36 top-side contacts, 0.5mm pitch, SMT, https://www.te.com/commerce/DocumentDelivery/DDEController?Action=showdoc&DocId=Customer+Drawing%7F1734839%7FC%7Fpdf%7FEnglish%7FENG_CD_1734839_C_C_1734839.pdf%7F4-1734839-0
te fpc 1734839
0
38
37
Connector_FFC-FPC
TE_3-1734839-7_1x37-1MP_P0.5mm_Horizontal
TE FPC connector, 37 top-side contacts, 0.5mm pitch, SMT, https://www.te.com/commerce/DocumentDelivery/DDEController?Action=showdoc&DocId=Customer+Drawing%7F1734839%7FC%7Fpdf%7FEnglish%7FENG_CD_1734839_C_C_1734839.pdf%7F4-1734839-0
te fpc 1734839
0
39
38
Connector_FFC-FPC
TE_3-1734839-8_1x38-1MP_P0.5mm_Horizontal
TE FPC connector, 38 top-side contacts, 0.5mm pitch, SMT, https://www.te.com/commerce/DocumentDelivery/DDEController?Action=showdoc&DocId=Customer+Drawing%7F1734839%7FC%7Fpdf%7FEnglish%7FENG_CD_1734839_C_C_1734839.pdf%7F4-1734839-0
te fpc 1734839
0
40
39
Connector_FFC-FPC
TE_3-1734839-9_1x39-1MP_P0.5mm_Horizontal
TE FPC connector, 39 top-side contacts, 0.5mm pitch, SMT, https://www.te.com/commerce/DocumentDelivery/DDEController?Action=showdoc&DocId=Customer+Drawing%7F1734839%7FC%7Fpdf%7FEnglish%7FENG_CD_1734839_C_C_1734839.pdf%7F4-1734839-0
te fpc 1734839
0
41
40
Connector_FFC-FPC
TE_4-1734839-0_1x40-1MP_P0.5mm_Horizontal
TE FPC connector, 40 top-side contacts, 0.5mm pitch, SMT, https://www.te.com/commerce/DocumentDelivery/DDEController?Action=showdoc&DocId=Customer+Drawing%7F1734839%7FC%7Fpdf%7FEnglish%7FENG_CD_1734839_C_C_1734839.pdf%7F4-1734839-0
te fpc 1734839
0
42
41
Connector_FFC-FPC
TE_4-1734839-1_1x41-1MP_P0.5mm_Horizontal
TE FPC connector, 41 top-side contacts, 0.5mm pitch, SMT, https://www.te.com/commerce/DocumentDelivery/DDEController?Action=showdoc&DocId=Customer+Drawing%7F1734839%7FC%7Fpdf%7FEnglish%7FENG_CD_1734839_C_C_1734839.pdf%7F4-1734839-0
te fpc 1734839
0
43
42
Connector_FFC-FPC
TE_4-1734839-2_1x42-1MP_P0.5mm_Horizontal
TE FPC connector, 42 top-side contacts, 0.5mm pitch, SMT, https://www.te.com/commerce/DocumentDelivery/DDEController?Action=showdoc&DocId=Customer+Drawing%7F1734839%7FC%7Fpdf%7FEnglish%7FENG_CD_1734839_C_C_1734839.pdf%7F4-1734839-0
te fpc 1734839
0
44
43
Connector_FFC-FPC
TE_4-1734839-3_1x43-1MP_P0.5mm_Horizontal
TE FPC connector, 43 top-side contacts, 0.5mm pitch, SMT, https://www.te.com/commerce/DocumentDelivery/DDEController?Action=showdoc&DocId=Customer+Drawing%7F1734839%7FC%7Fpdf%7FEnglish%7FENG_CD_1734839_C_C_1734839.pdf%7F4-1734839-0
te fpc 1734839
0
45
44
Connector_FFC-FPC
TE_4-1734839-4_1x44-1MP_P0.5mm_Horizontal
TE FPC connector, 44 top-side contacts, 0.5mm pitch, SMT, https://www.te.com/commerce/DocumentDelivery/DDEController?Action=showdoc&DocId=Customer+Drawing%7F1734839%7FC%7Fpdf%7FEnglish%7FENG_CD_1734839_C_C_1734839.pdf%7F4-1734839-0
te fpc 1734839
0
46
45
Connector_FFC-FPC
TE_4-1734839-5_1x45-1MP_P0.5mm_Horizontal
TE FPC connector, 45 top-side contacts, 0.5mm pitch, SMT, https://www.te.com/commerce/DocumentDelivery/DDEController?Action=showdoc&DocId=Customer+Drawing%7F1734839%7FC%7Fpdf%7FEnglish%7FENG_CD_1734839_C_C_1734839.pdf%7F4-1734839-0
te fpc 1734839
0
47
46
Connector_FFC-FPC
TE_4-1734839-6_1x46-1MP_P0.5mm_Horizontal
TE FPC connector, 46 top-side contacts, 0.5mm pitch, SMT, https://www.te.com/commerce/DocumentDelivery/DDEController?Action=showdoc&DocId=Customer+Drawing%7F1734839%7FC%7Fpdf%7FEnglish%7FENG_CD_1734839_C_C_1734839.pdf%7F4-1734839-0
te fpc 1734839
0
48
47
Connector_FFC-FPC
TE_4-1734839-7_1x47-1MP_P0.5mm_Horizontal
TE FPC connector, 47 top-side contacts, 0.5mm pitch, SMT, https://www.te.com/commerce/DocumentDelivery/DDEController?Action=showdoc&DocId=Customer+Drawing%7F1734839%7FC%7Fpdf%7FEnglish%7FENG_CD_1734839_C_C_1734839.pdf%7F4-1734839-0
te fpc 1734839
0
49
48
Connector_FFC-FPC
TE_4-1734839-8_1x48-1MP_P0.5mm_Horizontal
TE FPC connector, 48 top-side contacts, 0.5mm pitch, SMT, https://www.te.com/commerce/DocumentDelivery/DDEController?Action=showdoc&DocId=Customer+Drawing%7F1734839%7FC%7Fpdf%7FEnglish%7FENG_CD_1734839_C_C_1734839.pdf%7F4-1734839-0
te fpc 1734839
0
50
49
Connector_FFC-FPC
TE_4-1734839-9_1x49-1MP_P0.5mm_Horizontal
TE FPC connector, 49 top-side contacts, 0.5mm pitch, SMT, https://www.te.com/commerce/DocumentDelivery/DDEController?Action=showdoc&DocId=Customer+Drawing%7F1734839%7FC%7Fpdf%7FEnglish%7FENG_CD_1734839_C_C_1734839.pdf%7F4-1734839-0
te fpc 1734839
0
51
50
Connector_FFC-FPC
TE_5-1734839-0_1x50-1MP_P0.5mm_Horizontal
TE FPC connector, 50 top-side contacts, 0.5mm pitch, SMT, https://www.te.com/commerce/DocumentDelivery/DDEController?Action=showdoc&DocId=Customer+Drawing%7F1734839%7FC%7Fpdf%7FEnglish%7FENG_CD_1734839_C_C_1734839.pdf%7F4-1734839-0
te fpc 1734839
0
52
51
Connector_FFC-FPC
TE_84952-4_1x04-1MP_P1.0mm_Horizontal
TE FPC connector, 04 bottom-side contacts, 1.0mm pitch, 1.0mm height, SMT, http://www.te.com/commerce/DocumentDelivery/DDEController?Action=srchrtrv&DocNm=84952&DocType=Customer+Drawing&DocLang=English&DocFormat=pdf&PartCntxt=84952-4
te fpc 84952
0
6
5
Connector_FFC-FPC
TE_84952-5_1x05-1MP_P1.0mm_Horizontal
TE FPC connector, 05 bottom-side contacts, 1.0mm pitch, 1.0mm height, SMT, http://www.te.com/commerce/DocumentDelivery/DDEController?Action=srchrtrv&DocNm=84952&DocType=Customer+Drawing&DocLang=English&DocFormat=pdf&PartCntxt=84952-4
te fpc 84952
0
7
6
Connector_FFC-FPC
TE_84952-6_1x06-1MP_P1.0mm_Horizontal
TE FPC connector, 06 bottom-side contacts, 1.0mm pitch, 1.0mm height, SMT, http://www.te.com/commerce/DocumentDelivery/DDEController?Action=srchrtrv&DocNm=84952&DocType=Customer+Drawing&DocLang=English&DocFormat=pdf&PartCntxt=84952-4
te fpc 84952
0
8
7
Connector_FFC-FPC
TE_84952-7_1x07-1MP_P1.0mm_Horizontal
TE FPC connector, 07 bottom-side contacts, 1.0mm pitch, 1.0mm height, SMT, http://www.te.com/commerce/DocumentDelivery/DDEController?Action=srchrtrv&DocNm=84952&DocType=Customer+Drawing&DocLang=English&DocFormat=pdf&PartCntxt=84952-4
te fpc 84952
0
9
8
Connector_FFC-FPC
TE_84952-8_1x08-1MP_P1.0mm_Horizontal
TE FPC connector, 08 bottom-side contacts, 1.0mm pitch, 1.0mm height, SMT, http://www.te.com/commerce/DocumentDelivery/DDEController?Action=srchrtrv&DocNm=84952&DocType=Customer+Drawing&DocLang=English&DocFormat=pdf&PartCntxt=84952-4
te fpc 84952
0
10
9
Connector_FFC-FPC
TE_84952-9_1x09-1MP_P1.0mm_Horizontal
TE FPC connector, 09 bottom-side contacts, 1.0mm pitch, 1.0mm height, SMT, http://www.te.com/commerce/DocumentDelivery/DDEController?Action=srchrtrv&DocNm=84952&DocType=Customer+Drawing&DocLang=English&DocFormat=pdf&PartCntxt=84952-4
te fpc 84952
0
11
10
Connector_FFC-FPC
TE_84953-4_1x04-1MP_P1.0mm_Horizontal
TE FPC connector, 04 top-side contacts, 1.0mm pitch, 1.0mm height, SMT, http://www.te.com/commerce/DocumentDelivery/DDEController?Action=srchrtrv&DocNm=84953&DocType=Customer+Drawing&DocLang=English&DocFormat=pdf&PartCntxt=84953-4
te fpc 84953
0
6
5
Connector_FFC-FPC
TE_84953-5_1x05-1MP_P1.0mm_Horizontal
TE FPC connector, 05 top-side contacts, 1.0mm pitch, 1.0mm height, SMT, http://www.te.com/commerce/DocumentDelivery/DDEController?Action=srchrtrv&DocNm=84953&DocType=Customer+Drawing&DocLang=English&DocFormat=pdf&PartCntxt=84953-4
te fpc 84953
0
7
6
Connector_FFC-FPC
TE_84953-6_1x06-1MP_P1.0mm_Horizontal
TE FPC connector, 06 top-side contacts, 1.0mm pitch, 1.0mm height, SMT, http://www.te.com/commerce/DocumentDelivery/DDEController?Action=srchrtrv&DocNm=84953&DocType=Customer+Drawing&DocLang=English&DocFormat=pdf&PartCntxt=84953-4
te fpc 84953
0
8
7
Connector_FFC-FPC
TE_84953-7_1x07-1MP_P1.0mm_Horizontal
TE FPC connector, 07 top-side contacts, 1.0mm pitch, 1.0mm height, SMT, http://www.te.com/commerce/DocumentDelivery/DDEController?Action=srchrtrv&DocNm=84953&DocType=Customer+Drawing&DocLang=English&DocFormat=pdf&PartCntxt=84953-4
te fpc 84953
0
9
8
Connector_FFC-FPC
TE_84953-8_1x08-1MP_P1.0mm_Horizontal
TE FPC connector, 08 top-side contacts, 1.0mm pitch, 1.0mm height, SMT, http://www.te.com/commerce/DocumentDelivery/DDEController?Action=srchrtrv&DocNm=84953&DocType=Customer+Drawing&DocLang=English&DocFormat=pdf&PartCntxt=84953-4
te fpc 84953
0
10
9
Connector_FFC-FPC
TE_84953-9_1x09-1MP_P1.0mm_Horizontal
TE FPC connector, 09 top-side contacts, 1.0mm pitch, 1.0mm height, SMT, http://www.te.com/commerce/DocumentDelivery/DDEController?Action=srchrtrv&DocNm=84953&DocType=Customer+Drawing&DocLang=English&DocFormat=pdf&PartCntxt=84953-4
te fpc 84953
0
11
10
Connector_FFC-FPC
Wuerth_68611214422_1x12-1MP_P1.0mm_Horizontal
http://katalog.we-online.de/em/datasheet/68611214422.pdf
Wuerth FPC 68611214422 connector 12 bottom-side contacts 1.0mm pitch 1.0mm height SMT
0
14
13
Connector_HDMI
HDMI_A_Contact_Technology_HDMI-19APL2_Horizontal
HDMI Contact Technology Type A http://www.contactswitch.com/en/download.aspx?id=1449
HDMI Contact Technology Type A
0
23
20
Connector_HDMI
HDMI_A_Kycon_KDMIX-SL1-NS-WS-B15_VerticalRightAngle
HDMI, Type A, Kycon KDMIX-SL1-NS-WS-B15, Vertical Right Angle, http://www.kycon.com/Pub_Eng_Draw/KDMIX-SL1-NS-WS-B15.pdf
hdmi type a
0
23
20
Connector_HDMI
HDMI_A_Molex_208658-1001_Horizontal
HDMI Molex Type A https://www.molex.com/pdm_docs/sd/2086581001_sd.pdf
HDMI Molex Type A
0
23
20
Connector_HDMI
HDMI_Micro-D_Molex_46765-0x01
HDMI, Micro, Type D, SMD, 0.4mm pitch, 19 ckt, right angle (http://www.molex.com/pdm_docs/sd/467651301_sd.pdf)
hdmi micro type d right angle smd
0
23
20
Connector_HDMI
HDMI_Micro-D_Molex_46765-1x01
HDMI, Micro, Type D, THT, 0.4mm pitch, 19 ckt, right angle (http://www.molex.com/pdm_docs/sd/467651301_sd.pdf)
hdmi micro type d right angle tht
0
23
20
Connector_HDMI
HDMI_Micro-D_Molex_46765-2x0x
HDMI, Micro, Type D, THT/SMD hybrid, 0.4mm pitch, 19 ckt, right angle (http://www.molex.com/pdm_docs/sd/467651301_sd.pdf)
hdmi micro type d right angle tht smd hybrid 
0
23
20
Connector_Harting
Harting_har-flexicon_14110213001xxx_1x02-MP_P2.54mm_Vertical
Harting har-flexicon series connector, 14110213001xxx (https://b2b.harting.com/files/download/PRD/PDF_TS/1411XX13001XXX_100228421DRW046C.pdf), generated with kicad-footprint-generator
connector Harting har-flexicon vertical
0
4
3
Connector_Harting
Harting_har-flexicon_14110213002xxx_1x02-MP_P2.54mm_Horizontal
Harting har-flexicon series connector, 14110213002xxx (https://b2b.harting.com/files/download/PRD/PDF_TS/1411XX13002XXX_100228421DRW035C.pdf), generated with kicad-footprint-generator
connector Harting har-flexicon horizontal
0
4
3
Connector_Harting
Harting_har-flexicon_14110213010xxx_1x02-MP_P2.54mm_Horizontal
Harting har-flexicon series connector, 14110213010xxx (https://b2b.harting.com/files/download/PRD/PDF_TS/1411XX13010XXX_100228421DRW063C.pdf), generated with kicad-footprint-generator
connector Harting har-flexicon horizontal
0
4
3
Connector_Harting
Harting_har-flexicon_14110313001xxx_1x03-MP_P2.54mm_Vertical
Harting har-flexicon series connector, 14110313001xxx (https://b2b.harting.com/files/download/PRD/PDF_TS/1411XX13001XXX_100228421DRW046C.pdf), generated with kicad-footprint-generator
connector Harting har-flexicon vertical
0
5
4
Connector_Harting
Harting_har-flexicon_14110313002xxx_1x03-MP_P2.54mm_Horizontal
Harting har-flexicon series connector, 14110313002xxx (https://b2b.harting.com/files/download/PRD/PDF_TS/1411XX13002XXX_100228421DRW035C.pdf), generated with kicad-footprint-generator
connector Harting har-flexicon horizontal
0
5
4
Connector_Harting
Harting_har-flexicon_14110313010xxx_1x03-MP_P2.54mm_Horizontal
Harting har-flexicon series connector, 14110313010xxx (https://b2b.harting.com/files/download/PRD/PDF_TS/1411XX13010XXX_100228421DRW063C.pdf), generated with kicad-footprint-generator
connector Harting har-flexicon horizontal
0
5
4
Connector_Harting
Harting_har-flexicon_14110413001xxx_1x04-MP_P2.54mm_Vertical
Harting har-flexicon series connector, 14110413001xxx (https://b2b.harting.com/files/download/PRD/PDF_TS/1411XX13001XXX_100228421DRW046C.pdf), generated with kicad-footprint-generator
connector Harting har-flexicon vertical
0
6
5
Connector_Harting
Harting_har-flexicon_14110413002xxx_1x04-MP_P2.54mm_Horizontal
Harting har-flexicon series connector, 14110413002xxx (https://b2b.harting.com/files/download/PRD/PDF_TS/1411XX13002XXX_100228421DRW035C.pdf), generated with kicad-footprint-generator
connector Harting har-flexicon horizontal
0
6
5
Connector_Harting
Harting_har-flexicon_14110413010xxx_1x04-MP_P2.54mm_Horizontal
Harting har-flexicon series connector, 14110413010xxx (https://b2b.harting.com/files/download/PRD/PDF_TS/1411XX13010XXX_100228421DRW063C.pdf), generated with kicad-footprint-generator
connector Harting har-flexicon horizontal
0
6
5
Connector_Harting
Harting_har-flexicon_14110513001xxx_1x05-MP_P2.54mm_Vertical
Harting har-flexicon series connector, 14110513001xxx (https://b2b.harting.com/files/download/PRD/PDF_TS/1411XX13001XXX_100228421DRW046C.pdf), generated with kicad-footprint-generator
connector Harting har-flexicon vertical
0
7
6
Connector_Harting
Harting_har-flexicon_14110513002xxx_1x05-MP_P2.54mm_Horizontal
Harting har-flexicon series connector, 14110513002xxx (https://b2b.harting.com/files/download/PRD/PDF_TS/1411XX13002XXX_100228421DRW035C.pdf), generated with kicad-footprint-generator
connector Harting har-flexicon horizontal
0
7
6
Connector_Harting
Harting_har-flexicon_14110513010xxx_1x05-MP_P2.54mm_Horizontal
Harting har-flexicon series connector, 14110513010xxx (https://b2b.harting.com/files/download/PRD/PDF_TS/1411XX13010XXX_100228421DRW063C.pdf), generated with kicad-footprint-generator
connector Harting har-flexicon horizontal
0
7
6
Connector_Harting
Harting_har-flexicon_14110613001xxx_1x06-MP_P2.54mm_Vertical
Harting har-flexicon series connector, 14110613001xxx (https://b2b.harting.com/files/download/PRD/PDF_TS/1411XX13001XXX_100228421DRW046C.pdf), generated with kicad-footprint-generator
connector Harting har-flexicon vertical
0
8
7
Connector_Harting
Harting_har-flexicon_14110613002xxx_1x06-MP_P2.54mm_Horizontal
Harting har-flexicon series connector, 14110613002xxx (https://b2b.harting.com/files/download/PRD/PDF_TS/1411XX13002XXX_100228421DRW035C.pdf), generated with kicad-footprint-generator
connector Harting har-flexicon horizontal
0
8
7
Connector_Harting
Harting_har-flexicon_14110613010xxx_1x06-MP_P2.54mm_Horizontal
Harting har-flexicon series connector, 14110613010xxx (https://b2b.harting.com/files/download/PRD/PDF_TS/1411XX13010XXX_100228421DRW063C.pdf), generated with kicad-footprint-generator
connector Harting har-flexicon horizontal
0
8
7
Connector_Harting
Harting_har-flexicon_14110713001xxx_1x07-MP_P2.54mm_Vertical
Harting har-flexicon series connector, 14110713001xxx (https://b2b.harting.com/files/download/PRD/PDF_TS/1411XX13001XXX_100228421DRW046C.pdf), generated with kicad-footprint-generator
connector Harting har-flexicon vertical
0
9
8
Connector_Harting
Harting_har-flexicon_14110713002xxx_1x07-MP_P2.54mm_Horizontal
Harting har-flexicon series connector, 14110713002xxx (https://b2b.harting.com/files/download/PRD/PDF_TS/1411XX13002XXX_100228421DRW035C.pdf), generated with kicad-footprint-generator
connector Harting har-flexicon horizontal
0
9
8
Connector_Harting
Harting_har-flexicon_14110713010xxx_1x07-MP_P2.54mm_Horizontal
Harting har-flexicon series connector, 14110713010xxx (https://b2b.harting.com/files/download/PRD/PDF_TS/1411XX13010XXX_100228421DRW063C.pdf), generated with kicad-footprint-generator
connector Harting har-flexicon horizontal
0
9
8
Connector_Harting
Harting_har-flexicon_14110813001xxx_1x08-MP_P2.54mm_Vertical
Harting har-flexicon series connector, 14110813001xxx (https://b2b.harting.com/files/download/PRD/PDF_TS/1411XX13001XXX_100228421DRW046C.pdf), generated with kicad-footprint-generator
connector Harting har-flexicon vertical
0
10
9
Connector_Harting
Harting_har-flexicon_14110813002xxx_1x08-MP_P2.54mm_Horizontal
Harting har-flexicon series connector, 14110813002xxx (https://b2b.harting.com/files/download/PRD/PDF_TS/1411XX13002XXX_100228421DRW035C.pdf), generated with kicad-footprint-generator
connector Harting har-flexicon horizontal
0
10
9
Connector_Harting
Harting_har-flexicon_14110813010xxx_1x08-MP_P2.54mm_Horizontal
Harting har-flexicon series connector, 14110813010xxx (https://b2b.harting.com/files/download/PRD/PDF_TS/1411XX13010XXX_100228421DRW063C.pdf), generated with kicad-footprint-generator
connector Harting har-flexicon horizontal
0
10
9
Connector_Harting
Harting_har-flexicon_14110913001xxx_1x09-MP_P2.54mm_Vertical
Harting har-flexicon series connector, 14110913001xxx (https://b2b.harting.com/files/download/PRD/PDF_TS/1411XX13001XXX_100228421DRW046C.pdf), generated with kicad-footprint-generator
connector Harting har-flexicon vertical
0
11
10
Connector_Harting
Harting_har-flexicon_14110913002xxx_1x09-MP_P2.54mm_Horizontal
Harting har-flexicon series connector, 14110913002xxx (https://b2b.harting.com/files/download/PRD/PDF_TS/1411XX13002XXX_100228421DRW035C.pdf), generated with kicad-footprint-generator
connector Harting har-flexicon horizontal
0
11
10
Connector_Harting
Harting_har-flexicon_14110913010xxx_1x09-MP_P2.54mm_Horizontal
Harting har-flexicon series connector, 14110913010xxx (https://b2b.harting.com/files/download/PRD/PDF_TS/1411XX13010XXX_100228421DRW063C.pdf), generated with kicad-footprint-generator
connector Harting har-flexicon horizontal
0
11
10
Connector_Harting
Harting_har-flexicon_14111013001xxx_1x10-MP_P2.54mm_Vertical
Harting har-flexicon series connector, 14111013001xxx (https://b2b.harting.com/files/download/PRD/PDF_TS/1411XX13001XXX_100228421DRW046C.pdf), generated with kicad-footprint-generator
connector Harting har-flexicon vertical
0
12
11
Connector_Harting
Harting_har-flexicon_14111013002xxx_1x10-MP_P2.54mm_Horizontal
Harting har-flexicon series connector, 14111013002xxx (https://b2b.harting.com/files/download/PRD/PDF_TS/1411XX13002XXX_100228421DRW035C.pdf), generated with kicad-footprint-generator
connector Harting har-flexicon horizontal
0
12
11
Connector_Harting
Harting_har-flexicon_14111013010xxx_1x10-MP_P2.54mm_Horizontal
Harting har-flexicon series connector, 14111013010xxx (https://b2b.harting.com/files/download/PRD/PDF_TS/1411XX13010XXX_100228421DRW063C.pdf), generated with kicad-footprint-generator
connector Harting har-flexicon horizontal
0
12
11
Connector_Harting
Harting_har-flexicon_14111113001xxx_1x11-MP_P2.54mm_Vertical
Harting har-flexicon series connector, 14111113001xxx (https://b2b.harting.com/files/download/PRD/PDF_TS/1411XX13001XXX_100228421DRW046C.pdf), generated with kicad-footprint-generator
connector Harting har-flexicon vertical
0
13
12
Connector_Harting
Harting_har-flexicon_14111113002xxx_1x11-MP_P2.54mm_Horizontal
Harting har-flexicon series connector, 14111113002xxx (https://b2b.harting.com/files/download/PRD/PDF_TS/1411XX13002XXX_100228421DRW035C.pdf), generated with kicad-footprint-generator
connector Harting har-flexicon horizontal
0
13
12
Connector_Harting
Harting_har-flexicon_14111113010xxx_1x11-MP_P2.54mm_Horizontal
Harting har-flexicon series connector, 14111113010xxx (https://b2b.harting.com/files/download/PRD/PDF_TS/1411XX13010XXX_100228421DRW063C.pdf), generated with kicad-footprint-generator
connector Harting har-flexicon horizontal
0
13
12
Connector_Harting
Harting_har-flexicon_14111213001xxx_1x12-MP_P2.54mm_Vertical
Harting har-flexicon series connector, 14111213001xxx (https://b2b.harting.com/files/download/PRD/PDF_TS/1411XX13001XXX_100228421DRW046C.pdf), generated with kicad-footprint-generator
connector Harting har-flexicon vertical
0
14
13
Connector_Harting
Harting_har-flexicon_14111213002xxx_1x12-MP_P2.54mm_Horizontal
Harting har-flexicon series connector, 14111213002xxx (https://b2b.harting.com/files/download/PRD/PDF_TS/1411XX13002XXX_100228421DRW035C.pdf), generated with kicad-footprint-generator
connector Harting har-flexicon horizontal
0
14
13
Connector_Harting
Harting_har-flexicon_14111213010xxx_1x12-MP_P2.54mm_Horizontal
Harting har-flexicon series connector, 14111213010xxx (https://b2b.harting.com/files/download/PRD/PDF_TS/1411XX13010XXX_100228421DRW063C.pdf), generated with kicad-footprint-generator
connector Harting har-flexicon horizontal
0
14
13
Connector_Harwin
Harwin_Gecko-G125-FVX0605L0X_2x03_P1.25mm_Vertical
Harwin Gecko Connector, 6 pins, dual row female, vertical entry, PN:G125-FVX0605L0X
connector harwin gecko
0
6
6
Connector_Harwin
Harwin_Gecko-G125-FVX1005L0X_2x05_P1.25mm_Vertical
Harwin Gecko Connector, 10 pins, dual row female, vertical entry, PN:G125-FVX1005L0X
connector harwin gecko
0
10
10
Connector_Harwin
Harwin_Gecko-G125-FVX1205L0X_2x06_P1.25mm_Vertical
Harwin Gecko Connector, 12 pins, dual row female, vertical entry, PN:G125-FVX1205L0X
connector harwin gecko
0
12
12
Connector_Harwin
Harwin_Gecko-G125-FVX1605L0X_2x08_P1.25mm_Vertical
Harwin Gecko Connector, 16 pins, dual row female, vertical entry, PN:G125-FVX1605L0X
connector harwin gecko
0
16
16
Connector_Harwin
Harwin_Gecko-G125-FVX2005L0X_2x10_P1.25mm_Vertical
Harwin Gecko Connector, 20 pins, dual row female, vertical entry, PN:G125-FVX2005L0X
connector harwin gecko
0
20
20
Connector_Harwin
Harwin_Gecko-G125-FVX2605L0X_2x13_P1.25mm_Vertical
Harwin Gecko Connector, 26 pins, dual row female, vertical entry, PN:G125-FVX2605L0X
connector harwin gecko
0
26
26
Connector_Harwin
Harwin_Gecko-G125-FVX3405L0X_2x17_P1.25mm_Vertical
Harwin Gecko Connector, 34 pins, dual row female, vertical entry, PN:G125-FVX3405L0X
connector harwin gecko
0
34
34
Connector_Harwin
Harwin_Gecko-G125-FVX5005L0X_2x25_P1.25mm_Vertical
Harwin Gecko Connector, 50 pins, dual row female, vertical entry, PN:G125-FVX5005L0X
connector harwin gecko
0
50
50
Connector_Harwin
Harwin_Gecko-G125-MVX0605L0X_2x03_P1.25mm_Vertical
Harwin Gecko Connector, 6 pins, dual row male, vertical entry, no latches, PN:G125-MVX0605L0X
connector harwin gecko
0
6
6
Connector_Harwin
Harwin_Gecko-G125-MVX0605L1X_2x03_P1.25mm_Vertical
Harwin Gecko Connector, 6 pins, dual row male, vertical entry, with latches, PN:G125-MVX0605L1X
connector harwin gecko
0
6
6
Connector_Harwin
Harwin_Gecko-G125-MVX1005L0X_2x05_P1.25mm_Vertical
Harwin Gecko Connector, 10 pins, dual row male, vertical entry, no latches, PN:G125-MVX1005L0X
connector harwin gecko
0
10
10
Connector_Harwin
Harwin_Gecko-G125-MVX1005L1X_2x05_P1.25mm_Vertical
Harwin Gecko Connector, 10 pins, dual row male, vertical entry, with latches, PN:G125-MVX1005L1X
connector harwin gecko
0
10
10
Connector_Harwin
Harwin_Gecko-G125-MVX1205L0X_2x06_P1.25mm_Vertical
Harwin Gecko Connector, 12 pins, dual row male, vertical entry, no latches, PN:G125-MVX1205L0X
connector harwin gecko
0
12
12
Connector_Harwin
Harwin_Gecko-G125-MVX1205L1X_2x06_P1.25mm_Vertical
Harwin Gecko Connector, 12 pins, dual row male, vertical entry, with latches, PN:G125-MVX1205L1X
connector harwin gecko
0
12
12
Connector_Harwin
Harwin_Gecko-G125-MVX1605L0X_2x08_P1.25mm_Vertical
Harwin Gecko Connector, 16 pins, dual row male, vertical entry, no latches, PN:G125-MVX1605L0X
connector harwin gecko
0
16
16
Connector_Harwin
Harwin_Gecko-G125-MVX1605L1X_2x08_P1.25mm_Vertical
Harwin Gecko Connector, 16 pins, dual row male, vertical entry, with latches, PN:G125-MVX1605L1X
connector harwin gecko
0
16
16
Connector_Harwin
Harwin_Gecko-G125-MVX2005L0X_2x10_P1.25mm_Vertical
Harwin Gecko Connector, 20 pins, dual row male, vertical entry, no latches, PN:G125-MVX2005L0X
connector harwin gecko
0
20
20
Connector_Harwin
Harwin_Gecko-G125-MVX2005L1X_2x10_P1.25mm_Vertical
Harwin Gecko Connector, 20 pins, dual row male, vertical entry, with latches, PN:G125-MVX2005L1X
connector harwin gecko
0
20
20
Connector_Harwin
Harwin_Gecko-G125-MVX2605L0X_2x13_P1.25mm_Vertical
Harwin Gecko Connector, 26 pins, dual row male, vertical entry, no latches, PN:G125-MVX2605L0X
connector harwin gecko
0
26
26
Connector_Harwin
Harwin_Gecko-G125-MVX2605L1X_2x13_P1.25mm_Vertical
Harwin Gecko Connector, 26 pins, dual row male, vertical entry, with latches, PN:G125-MVX2605L1X
connector harwin gecko
0
26
26
Connector_Harwin
Harwin_Gecko-G125-MVX3405L0X_2x17_P1.25mm_Vertical
Harwin Gecko Connector, 34 pins, dual row male, vertical entry, no latches, PN:G125-MVX3405L0X
connector harwin gecko
0
34
34
Connector_Harwin
Harwin_Gecko-G125-MVX3405L1X_2x17_P1.25mm_Vertical
Harwin Gecko Connector, 34 pins, dual row male, vertical entry, with latches, PN:G125-MVX3405L1X
connector harwin gecko
0
34
34
Connector_Harwin
Harwin_Gecko-G125-MVX5005L0X_2x25_P1.25mm_Vertical
Harwin Gecko Connector, 50 pins, dual row male, vertical entry, no latches, PN:G125-MVX5005L0X
connector harwin gecko
0
50
50
Connector_Harwin
Harwin_Gecko-G125-MVX5005L1X_2x25_P1.25mm_Vertical
Harwin Gecko Connector, 50 pins, dual row male, vertical entry, with latches, PN:G125-MVX5005L1X
connector harwin gecko
0
50
50
Connector_Harwin
Harwin_LTek-Male_02_P2.00mm_Vertical
Harwin LTek Connector, 2 pins, single row male, vertical entry
connector harwin ltek M80
0
2
2
Connector_Harwin
Harwin_LTek-Male_02_P2.00mm_Vertical_StrainRelief
Harwin LTek Connector, 2 pins, single row male, vertical entry, strain relief clip
connector harwin ltek M80
0
6
2
Connector_Harwin
Harwin_LTek-Male_2x02_P2.00mm_Vertical
Harwin LTek Connector, 4 pins, single row male, vertical entry
connector harwin ltek M80
0
4
4
Connector_Harwin
Harwin_LTek-Male_2x02_P2.00mm_Vertical_StrainRelief
Harwin LTek Connector, 4 pins, single row male, vertical entry, strain relief clip
connector harwin ltek M80
0
8
4
Connector_Harwin
Harwin_LTek-Male_2x03_P2.00mm_Vertical
Harwin LTek Connector, 6 pins, single row male, vertical entry
connector harwin ltek M80
0
6
6
Connector_Harwin
Harwin_LTek-Male_2x03_P2.00mm_Vertical_StrainRelief
Harwin LTek Connector, 6 pins, single row male, vertical entry, strain relief clip
connector harwin ltek M80
0
10
6
Connector_Harwin
Harwin_LTek-Male_2x04_P2.00mm_Vertical
Harwin LTek Connector, 8 pins, single row male, vertical entry
connector harwin ltek M80
0
8
8
Connector_Harwin
Harwin_LTek-Male_2x04_P2.00mm_Vertical_StrainRelief
Harwin LTek Connector, 8 pins, single row male, vertical entry, strain relief clip
connector harwin ltek M80
0
12
8
Connector_Harwin
Harwin_LTek-Male_2x05_P2.00mm_Vertical
Harwin LTek Connector, 10 pins, single row male, vertical entry
connector harwin ltek M80
0
10
10
Connector_Harwin
Harwin_LTek-Male_2x05_P2.00mm_Vertical_StrainRelief
Harwin LTek Connector, 10 pins, single row male, vertical entry, strain relief clip
connector harwin ltek M80
0
14
10
Connector_Harwin
Harwin_LTek-Male_2x06_P2.00mm_Vertical
Harwin LTek Connector, 12 pins, single row male, vertical entry
connector harwin ltek M80
0
12
12
Connector_Harwin
Harwin_LTek-Male_2x06_P2.00mm_Vertical_StrainRelief
Harwin LTek Connector, 12 pins, single row male, vertical entry, strain relief clip
connector harwin ltek M80
0
16
12
Connector_Harwin
Harwin_LTek-Male_2x07_P2.00mm_Vertical
Harwin LTek Connector, 14 pins, single row male, vertical entry
connector harwin ltek M80
0
14
14
Connector_Harwin
Harwin_LTek-Male_2x07_P2.00mm_Vertical_StrainRelief
Harwin LTek Connector, 14 pins, single row male, vertical entry, strain relief clip
connector harwin ltek M80
0
18
14
Connector_Harwin
Harwin_LTek-Male_2x08_P2.00mm_Vertical
Harwin LTek Connector, 16 pins, single row male, vertical entry
connector harwin ltek M80
0
16
16
Connector_Harwin
Harwin_LTek-Male_2x08_P2.00mm_Vertical_StrainRelief
Harwin LTek Connector, 16 pins, single row male, vertical entry, strain relief clip
connector harwin ltek M80
0
20
16
Connector_Harwin
Harwin_LTek-Male_2x09_P2.00mm_Vertical
Harwin LTek Connector, 18 pins, single row male, vertical entry
connector harwin ltek M80
0
18
18
Connector_Harwin
Harwin_LTek-Male_2x09_P2.00mm_Vertical_StrainRelief
Harwin LTek Connector, 18 pins, single row male, vertical entry, strain relief clip
connector harwin ltek M80
0
22
18
Connector_Harwin
Harwin_LTek-Male_2x10_P2.00mm_Vertical
Harwin LTek Connector, 20 pins, single row male, vertical entry
connector harwin ltek M80
0
20
20
Connector_Harwin
Harwin_LTek-Male_2x10_P2.00mm_Vertical_StrainRelief
Harwin LTek Connector, 20 pins, single row male, vertical entry, strain relief clip
connector harwin ltek M80
0
24
20
Connector_Harwin
Harwin_LTek-Male_2x13_P2.00mm_Vertical
Harwin LTek Connector, 26 pins, single row male, vertical entry
connector harwin ltek M80
0
26
26
Connector_Harwin
Harwin_LTek-Male_2x13_P2.00mm_Vertical_StrainRelief
Harwin LTek Connector, 26 pins, single row male, vertical entry, strain relief clip
connector harwin ltek M80
0
30
26
Connector_Harwin
Harwin_LTek-Male_2x17_P2.00mm_Vertical
Harwin LTek Connector, 34 pins, single row male, vertical entry
connector harwin ltek M80
0
34
34
Connector_Harwin
Harwin_LTek-Male_2x17_P2.00mm_Vertical_StrainRelief
Harwin LTek Connector, 34 pins, single row male, vertical entry, strain relief clip
connector harwin ltek M80
0
38
34
Connector_Harwin
Harwin_LTek-Male_2x22_P2.00mm_Vertical
Harwin LTek Connector, 44 pins, single row male, vertical entry
connector harwin ltek M80
0
44
44
Connector_Harwin
Harwin_LTek-Male_2x22_P2.00mm_Vertical_StrainRelief
Harwin LTek Connector, 44 pins, single row male, vertical entry, strain relief clip
connector harwin ltek M80
0
48
44
Connector_Harwin
Harwin_LTek-Male_03_P2.00mm_Vertical
Harwin LTek Connector, 3 pins, single row male, vertical entry
connector harwin ltek M80
0
3
3
Connector_Harwin
Harwin_LTek-Male_03_P2.00mm_Vertical_StrainRelief
Harwin LTek Connector, 3 pins, single row male, vertical entry, strain relief clip
connector harwin ltek M80
0
7
3
Connector_Harwin
Harwin_LTek-Male_04_P2.00mm_Vertical
Harwin LTek Connector, 4 pins, single row male, vertical entry
connector harwin ltek M80
0
4
4
Connector_Harwin
Harwin_LTek-Male_04_P2.00mm_Vertical_StrainRelief
Harwin LTek Connector, 4 pins, single row male, vertical entry, strain relief clip
connector harwin ltek M80
0
8
4
Connector_Harwin
Harwin_LTek-Male_05_P2.00mm_Vertical
Harwin LTek Connector, 5 pins, single row male, vertical entry
connector harwin ltek M80
0
5
5
Connector_Harwin
Harwin_LTek-Male_05_P2.00mm_Vertical_StrainRelief
Harwin LTek Connector, 5 pins, single row male, vertical entry, strain relief clip
connector harwin ltek M80
0
9
5
Connector_Harwin
Harwin_LTek-Male_06_P2.00mm_Vertical
Harwin LTek Connector, 6 pins, single row male, vertical entry
connector harwin ltek M80
0
6
6
Connector_Harwin
Harwin_LTek-Male_06_P2.00mm_Vertical_StrainRelief
Harwin LTek Connector, 6 pins, single row male, vertical entry, strain relief clip
connector harwin ltek M80
0
10
6
Connector_Harwin
Harwin_LTek-Male_07_P2.00mm_Vertical
Harwin LTek Connector, 7 pins, single row male, vertical entry
connector harwin ltek M80
0
7
7
Connector_Harwin
Harwin_LTek-Male_07_P2.00mm_Vertical_StrainRelief
Harwin LTek Connector, 7 pins, single row male, vertical entry, strain relief clip
connector harwin ltek M80
0
11
7
Connector_Harwin
Harwin_LTek-Male_17_P2.00mm_Vertical
Harwin LTek Connector, 17 pins, single row male, vertical entry
connector harwin ltek M80
0
17
17
Connector_Harwin
Harwin_LTek-Male_17_P2.00mm_Vertical_StrainRelief
Harwin LTek Connector, 17 pins, single row male, vertical entry, strain relief clip
connector harwin ltek M80
0
21
17
Connector_Harwin
Harwin_LTek-Male_22_P2.00mm_Vertical
Harwin LTek Connector, 22 pins, single row male, vertical entry
connector harwin ltek M80
0
22
22
Connector_Harwin
Harwin_LTek-Male_22_P2.00mm_Vertical_StrainRelief
Harwin LTek Connector, 22 pins, single row male, vertical entry, strain relief clip
connector harwin ltek M80
0
26
22
Connector_Harwin
Harwin_M20-89003xx_1x03_P2.54mm_Horizontal
Harwin Male Horizontal Surface Mount Single Row 2.54mm (0.1 inch) Pitch PCB Connector, M20-89003xx, 3 Pins per row (https://cdn.harwin.com/pdfs/M20-890.pdf), generated with kicad-footprint-generator
connector Harwin M20-890 horizontal
0
4
3
Connector_Harwin
Harwin_M20-89004xx_1x04_P2.54mm_Horizontal
Harwin Male Horizontal Surface Mount Single Row 2.54mm (0.1 inch) Pitch PCB Connector, M20-89004xx, 4 Pins per row (https://cdn.harwin.com/pdfs/M20-890.pdf), generated with kicad-footprint-generator
connector Harwin M20-890 horizontal
0
5
4
Connector_Harwin
Harwin_M20-89005xx_1x05_P2.54mm_Horizontal
Harwin Male Horizontal Surface Mount Single Row 2.54mm (0.1 inch) Pitch PCB Connector, M20-89005xx, 5 Pins per row (https://cdn.harwin.com/pdfs/M20-890.pdf), generated with kicad-footprint-generator
connector Harwin M20-890 horizontal
0
6
5
Connector_Harwin
Harwin_M20-89006xx_1x06_P2.54mm_Horizontal
Harwin Male Horizontal Surface Mount Single Row 2.54mm (0.1 inch) Pitch PCB Connector, M20-89006xx, 6 Pins per row (https://cdn.harwin.com/pdfs/M20-890.pdf), generated with kicad-footprint-generator
connector Harwin M20-890 horizontal
0
7
6
Connector_Harwin
Harwin_M20-89007xx_1x07_P2.54mm_Horizontal
Harwin Male Horizontal Surface Mount Single Row 2.54mm (0.1 inch) Pitch PCB Connector, M20-89007xx, 7 Pins per row (https://cdn.harwin.com/pdfs/M20-890.pdf), generated with kicad-footprint-generator
connector Harwin M20-890 horizontal
0
8
7
Connector_Harwin
Harwin_M20-89008xx_1x08_P2.54mm_Horizontal
Harwin Male Horizontal Surface Mount Single Row 2.54mm (0.1 inch) Pitch PCB Connector, M20-89008xx, 8 Pins per row (https://cdn.harwin.com/pdfs/M20-890.pdf), generated with kicad-footprint-generator
connector Harwin M20-890 horizontal
0
9
8
Connector_Harwin
Harwin_M20-89009xx_1x09_P2.54mm_Horizontal
Harwin Male Horizontal Surface Mount Single Row 2.54mm (0.1 inch) Pitch PCB Connector, M20-89009xx, 9 Pins per row (https://cdn.harwin.com/pdfs/M20-890.pdf), generated with kicad-footprint-generator
connector Harwin M20-890 horizontal
0
10
9
Connector_Harwin
Harwin_M20-89010xx_1x10_P2.54mm_Horizontal
Harwin Male Horizontal Surface Mount Single Row 2.54mm (0.1 inch) Pitch PCB Connector, M20-89010xx, 10 Pins per row (https://cdn.harwin.com/pdfs/M20-890.pdf), generated with kicad-footprint-generator
connector Harwin M20-890 horizontal
0
11
10
Connector_Harwin
Harwin_M20-89011xx_1x11_P2.54mm_Horizontal
Harwin Male Horizontal Surface Mount Single Row 2.54mm (0.1 inch) Pitch PCB Connector, M20-89011xx, 11 Pins per row (https://cdn.harwin.com/pdfs/M20-890.pdf), generated with kicad-footprint-generator
connector Harwin M20-890 horizontal
0
12
11
Connector_Harwin
Harwin_M20-89012xx_1x12_P2.54mm_Horizontal
Harwin Male Horizontal Surface Mount Single Row 2.54mm (0.1 inch) Pitch PCB Connector, M20-89012xx, 12 Pins per row (https://cdn.harwin.com/pdfs/M20-890.pdf), generated with kicad-footprint-generator
connector Harwin M20-890 horizontal
0
13
12
Connector_Harwin
Harwin_M20-89013xx_1x13_P2.54mm_Horizontal
Harwin Male Horizontal Surface Mount Single Row 2.54mm (0.1 inch) Pitch PCB Connector, M20-89013xx, 13 Pins per row (https://cdn.harwin.com/pdfs/M20-890.pdf), generated with kicad-footprint-generator
connector Harwin M20-890 horizontal
0
14
13
Connector_Harwin
Harwin_M20-89014xx_1x14_P2.54mm_Horizontal
Harwin Male Horizontal Surface Mount Single Row 2.54mm (0.1 inch) Pitch PCB Connector, M20-89014xx, 14 Pins per row (https://cdn.harwin.com/pdfs/M20-890.pdf), generated with kicad-footprint-generator
connector Harwin M20-890 horizontal
0
15
14
Connector_Harwin
Harwin_M20-89015xx_1x15_P2.54mm_Horizontal
Harwin Male Horizontal Surface Mount Single Row 2.54mm (0.1 inch) Pitch PCB Connector, M20-89015xx, 15 Pins per row (https://cdn.harwin.com/pdfs/M20-890.pdf), generated with kicad-footprint-generator
connector Harwin M20-890 horizontal
0
16
15
Connector_Harwin
Harwin_M20-89016xx_1x16_P2.54mm_Horizontal
Harwin Male Horizontal Surface Mount Single Row 2.54mm (0.1 inch) Pitch PCB Connector, M20-89016xx, 16 Pins per row (https://cdn.harwin.com/pdfs/M20-890.pdf), generated with kicad-footprint-generator
connector Harwin M20-890 horizontal
0
17
16
Connector_Harwin
Harwin_M20-89017xx_1x17_P2.54mm_Horizontal
Harwin Male Horizontal Surface Mount Single Row 2.54mm (0.1 inch) Pitch PCB Connector, M20-89017xx, 17 Pins per row (https://cdn.harwin.com/pdfs/M20-890.pdf), generated with kicad-footprint-generator
connector Harwin M20-890 horizontal
0
18
17
Connector_Harwin
Harwin_M20-89018xx_1x18_P2.54mm_Horizontal
Harwin Male Horizontal Surface Mount Single Row 2.54mm (0.1 inch) Pitch PCB Connector, M20-89018xx, 18 Pins per row (https://cdn.harwin.com/pdfs/M20-890.pdf), generated with kicad-footprint-generator
connector Harwin M20-890 horizontal
0
19
18
Connector_Harwin
Harwin_M20-89019xx_1x19_P2.54mm_Horizontal
Harwin Male Horizontal Surface Mount Single Row 2.54mm (0.1 inch) Pitch PCB Connector, M20-89019xx, 19 Pins per row (https://cdn.harwin.com/pdfs/M20-890.pdf), generated with kicad-footprint-generator
connector Harwin M20-890 horizontal
0
20
19
Connector_Harwin
Harwin_M20-89020xx_1x20_P2.54mm_Horizontal
Harwin Male Horizontal Surface Mount Single Row 2.54mm (0.1 inch) Pitch PCB Connector, M20-89020xx, 20 Pins per row (https://cdn.harwin.com/pdfs/M20-890.pdf), generated with kicad-footprint-generator
connector Harwin M20-890 horizontal
0
21
20
Connector_Harwin
Harwin_M20-7810245_2x02_P2.54mm_Vertical
Harwin Female Vertical Surface Mount Double Row 2.54mm (0.1 inch) Pitch PCB Connector, M20-7810245, 2 Pins per row (https://cdn.harwin.com/pdfs/M20-781.pdf), generated with kicad-footprint-generator
connector Harwin M20 side entry
0
4
4
Connector_Harwin
Harwin_M20-7810345_2x03_P2.54mm_Vertical
Harwin Female Vertical Surface Mount Double Row 2.54mm (0.1 inch) Pitch PCB Connector, M20-7810345, 3 Pins per row (https://cdn.harwin.com/pdfs/M20-781.pdf), generated with kicad-footprint-generator
connector Harwin M20 side entry
0
6
6
Connector_Harwin
Harwin_M20-7810445_2x04_P2.54mm_Vertical
Harwin Female Vertical Surface Mount Double Row 2.54mm (0.1 inch) Pitch PCB Connector, M20-7810445, 4 Pins per row (https://cdn.harwin.com/pdfs/M20-781.pdf), generated with kicad-footprint-generator
connector Harwin M20 side entry
0
8
8
Connector_Harwin
Harwin_M20-7810545_2x05_P2.54mm_Vertical
Harwin Female Vertical Surface Mount Double Row 2.54mm (0.1 inch) Pitch PCB Connector, M20-7810545, 5 Pins per row (https://cdn.harwin.com/pdfs/M20-781.pdf), generated with kicad-footprint-generator
connector Harwin M20 side entry
0
10
10
Connector_Harwin
Harwin_M20-7810645_2x06_P2.54mm_Vertical
Harwin Female Vertical Surface Mount Double Row 2.54mm (0.1 inch) Pitch PCB Connector, M20-7810645, 6 Pins per row (https://cdn.harwin.com/pdfs/M20-781.pdf), generated with kicad-footprint-generator
connector Harwin M20 side entry
0
12
12
Connector_Harwin
Harwin_M20-7810745_2x07_P2.54mm_Vertical
Harwin Female Vertical Surface Mount Double Row 2.54mm (0.1 inch) Pitch PCB Connector, M20-7810745, 7 Pins per row (https://cdn.harwin.com/pdfs/M20-781.pdf), generated with kicad-footprint-generator
connector Harwin M20 side entry
0
14
14
Connector_Harwin
Harwin_M20-7810845_2x08_P2.54mm_Vertical
Harwin Female Vertical Surface Mount Double Row 2.54mm (0.1 inch) Pitch PCB Connector, M20-7810845, 8 Pins per row (https://cdn.harwin.com/pdfs/M20-781.pdf), generated with kicad-footprint-generator
connector Harwin M20 side entry
0
16
16
Connector_Harwin
Harwin_M20-7810945_2x09_P2.54mm_Vertical
Harwin Female Vertical Surface Mount Double Row 2.54mm (0.1 inch) Pitch PCB Connector, M20-7810945, 9 Pins per row (https://cdn.harwin.com/pdfs/M20-781.pdf), generated with kicad-footprint-generator
connector Harwin M20 side entry
0
18
18
Connector_Harwin
Harwin_M20-7811045_2x10_P2.54mm_Vertical
Harwin Female Vertical Surface Mount Double Row 2.54mm (0.1 inch) Pitch PCB Connector, M20-7811045, 10 Pins per row (https://cdn.harwin.com/pdfs/M20-781.pdf), generated with kicad-footprint-generator
connector Harwin M20 side entry
0
20
20
Connector_Harwin
Harwin_M20-7811245_2x12_P2.54mm_Vertical
Harwin Female Vertical Surface Mount Double Row 2.54mm (0.1 inch) Pitch PCB Connector, M20-7811245, 12 Pins per row (https://cdn.harwin.com/pdfs/M20-781.pdf), generated with kicad-footprint-generator
connector Harwin M20 side entry
0
24
24
Connector_Harwin
Harwin_M20-7811545_2x15_P2.54mm_Vertical
Harwin Female Vertical Surface Mount Double Row 2.54mm (0.1 inch) Pitch PCB Connector, M20-7811545, 15 Pins per row (https://cdn.harwin.com/pdfs/M20-781.pdf), generated with kicad-footprint-generator
connector Harwin M20 side entry
0
30
30
Connector_Harwin
Harwin_M20-7812045_2x20_P2.54mm_Vertical
Harwin Female Vertical Surface Mount Double Row 2.54mm (0.1 inch) Pitch PCB Connector, M20-7812045, 20 Pins per row (https://cdn.harwin.com/pdfs/M20-781.pdf), generated with kicad-footprint-generator
connector Harwin M20 side entry
0
40
40
Connector_Hirose
Hirose_BM24_BM24-40DP-2-0.35V_2x20_P0.35mm_PowerPin2_Vertical
Hirose BM24 series connector, BM24-40DP/2-0.35V (https://www.hirose.com/product/en/download_file/key_name/BM24/category/Catalog/doc_file_id/47680/?file_category_id=4&item_id=50&is_series=1)
connector Hirose  BM24 40pin header
0
44
42
Connector_Hirose
Hirose_BM24_BM24-40DS-2-0.35V_2x20_P0.35mm_PowerPin2_Vertical
Hirose BM24 series connector, BM24-40DS/2-0.35V (https://www.hirose.com/product/en/download_file/key_name/BM24/category/Catalog/doc_file_id/47680/?file_category_id=4&item_id=50&is_series=1)
connector Hirose 40pin receptacle vertical
0
42
42
Connector_Hirose
Hirose_DF3EA-02P-2H_1x02-1MP_P2.00mm_Horizontal
Hirose  series connector, DF3EA-02P-2H (https://www.hirose.com/product/document?clcode=CL0543-0332-0-51&productname=DF3EA-5P-2H(51)&series=DF3&documenttype=2DDrawing&lang=en&documentid=0001163317), generated with kicad-footprint-generator
connector Hirose  top entry
0
4
3
Connector_Hirose
Hirose_DF3EA-03P-2H_1x03-1MP_P2.00mm_Horizontal
Hirose  series connector, DF3EA-03P-2H (https://www.hirose.com/product/document?clcode=CL0543-0332-0-51&productname=DF3EA-5P-2H(51)&series=DF3&documenttype=2DDrawing&lang=en&documentid=0001163317), generated with kicad-footprint-generator
connector Hirose  top entry
0
5
4
Connector_Hirose
Hirose_DF3EA-04P-2H_1x04-1MP_P2.00mm_Horizontal
Hirose  series connector, DF3EA-04P-2H (https://www.hirose.com/product/document?clcode=CL0543-0332-0-51&productname=DF3EA-5P-2H(51)&series=DF3&documenttype=2DDrawing&lang=en&documentid=0001163317), generated with kicad-footprint-generator
connector Hirose  top entry
0
6
5
Connector_Hirose
Hirose_DF3EA-05P-2H_1x05-1MP_P2.00mm_Horizontal
Hirose  series connector, DF3EA-05P-2H (https://www.hirose.com/product/document?clcode=CL0543-0332-0-51&productname=DF3EA-5P-2H(51)&series=DF3&documenttype=2DDrawing&lang=en&documentid=0001163317), generated with kicad-footprint-generator
connector Hirose  top entry
0
7
6
Connector_Hirose
Hirose_DF3EA-06P-2H_1x06-1MP_P2.00mm_Horizontal
Hirose  series connector, DF3EA-06P-2H (https://www.hirose.com/product/document?clcode=CL0543-0332-0-51&productname=DF3EA-5P-2H(51)&series=DF3&documenttype=2DDrawing&lang=en&documentid=0001163317), generated with kicad-footprint-generator
connector Hirose  top entry
0
8
7
Connector_Hirose
Hirose_DF3EA-07P-2H_1x07-1MP_P2.00mm_Horizontal
Hirose  series connector, DF3EA-07P-2H (https://www.hirose.com/product/document?clcode=CL0543-0332-0-51&productname=DF3EA-5P-2H(51)&series=DF3&documenttype=2DDrawing&lang=en&documentid=0001163317), generated with kicad-footprint-generator
connector Hirose  top entry
0
9
8
Connector_Hirose
Hirose_DF3EA-08P-2H_1x08-1MP_P2.00mm_Horizontal
Hirose  series connector, DF3EA-08P-2H (https://www.hirose.com/product/document?clcode=CL0543-0332-0-51&productname=DF3EA-5P-2H(51)&series=DF3&documenttype=2DDrawing&lang=en&documentid=0001163317), generated with kicad-footprint-generator
connector Hirose  top entry
0
10
9
Connector_Hirose
Hirose_DF3EA-09P-2H_1x09-1MP_P2.00mm_Horizontal
Hirose  series connector, DF3EA-09P-2H (https://www.hirose.com/product/document?clcode=CL0543-0332-0-51&productname=DF3EA-5P-2H(51)&series=DF3&documenttype=2DDrawing&lang=en&documentid=0001163317), generated with kicad-footprint-generator
connector Hirose  top entry
0
11
10
Connector_Hirose
Hirose_DF3EA-10P-2H_1x10-1MP_P2.00mm_Horizontal
Hirose  series connector, DF3EA-10P-2H (https://www.hirose.com/product/document?clcode=CL0543-0332-0-51&productname=DF3EA-5P-2H(51)&series=DF3&documenttype=2DDrawing&lang=en&documentid=0001163317), generated with kicad-footprint-generator
connector Hirose  top entry
0
12
11
Connector_Hirose
Hirose_DF3EA-11P-2H_1x11-1MP_P2.00mm_Horizontal
Hirose  series connector, DF3EA-11P-2H (https://www.hirose.com/product/document?clcode=CL0543-0332-0-51&productname=DF3EA-5P-2H(51)&series=DF3&documenttype=2DDrawing&lang=en&documentid=0001163317), generated with kicad-footprint-generator
connector Hirose  top entry
0
13
12
Connector_Hirose
Hirose_DF3EA-12P-2H_1x12-1MP_P2.00mm_Horizontal
Hirose  series connector, DF3EA-12P-2H (https://www.hirose.com/product/document?clcode=CL0543-0332-0-51&productname=DF3EA-5P-2H(51)&series=DF3&documenttype=2DDrawing&lang=en&documentid=0001163317), generated with kicad-footprint-generator
connector Hirose  top entry
0
14
13
Connector_Hirose
Hirose_DF3EA-13P-2H_1x13-1MP_P2.00mm_Horizontal
Hirose  series connector, DF3EA-13P-2H (https://www.hirose.com/product/document?clcode=CL0543-0332-0-51&productname=DF3EA-5P-2H(51)&series=DF3&documenttype=2DDrawing&lang=en&documentid=0001163317), generated with kicad-footprint-generator
connector Hirose  top entry
0
15
14
Connector_Hirose
Hirose_DF3EA-14P-2H_1x14-1MP_P2.00mm_Horizontal
Hirose  series connector, DF3EA-14P-2H (https://www.hirose.com/product/document?clcode=CL0543-0332-0-51&productname=DF3EA-5P-2H(51)&series=DF3&documenttype=2DDrawing&lang=en&documentid=0001163317), generated with kicad-footprint-generator
connector Hirose  top entry
0
16
15
Connector_Hirose
Hirose_DF3EA-15P-2H_1x15-1MP_P2.00mm_Horizontal
Hirose  series connector, DF3EA-15P-2H (https://www.hirose.com/product/document?clcode=CL0543-0332-0-51&productname=DF3EA-5P-2H(51)&series=DF3&documenttype=2DDrawing&lang=en&documentid=0001163317), generated with kicad-footprint-generator
connector Hirose  top entry
0
17
16
Connector_Hirose
Hirose_DF11-4DP-2DSA_2x02_P2.00mm_Vertical
Hirose DF11 through hole, DF11-4DP-2DSA, 2 Pins per row (https://www.hirose.com/product/document?clcode=&productname=&series=DF11&documenttype=Catalog&lang=en&documentid=D31688_en), generated with kicad-footprint-generator
connector Hirose DF11 vertical
0
4
4
Connector_Hirose
Hirose_DF11-6DP-2DSA_2x03_P2.00mm_Vertical
Hirose DF11 through hole, DF11-6DP-2DSA, 3 Pins per row (https://www.hirose.com/product/document?clcode=&productname=&series=DF11&documenttype=Catalog&lang=en&documentid=D31688_en), generated with kicad-footprint-generator
connector Hirose DF11 vertical
0
6
6
Connector_Hirose
Hirose_DF11-8DP-2DSA_2x04_P2.00mm_Vertical
Hirose DF11 through hole, DF11-8DP-2DSA, 4 Pins per row (https://www.hirose.com/product/document?clcode=&productname=&series=DF11&documenttype=Catalog&lang=en&documentid=D31688_en), generated with kicad-footprint-generator
connector Hirose DF11 vertical
0
8
8
Connector_Hirose
Hirose_DF11-10DP-2DSA_2x05_P2.00mm_Vertical
Hirose DF11 through hole, DF11-10DP-2DSA, 5 Pins per row (https://www.hirose.com/product/document?clcode=&productname=&series=DF11&documenttype=Catalog&lang=en&documentid=D31688_en), generated with kicad-footprint-generator
connector Hirose DF11 vertical
0
10
10
Connector_Hirose
Hirose_DF11-12DP-2DSA_2x06_P2.00mm_Vertical
Hirose DF11 through hole, DF11-12DP-2DSA, 6 Pins per row (https://www.hirose.com/product/document?clcode=&productname=&series=DF11&documenttype=Catalog&lang=en&documentid=D31688_en), generated with kicad-footprint-generator
connector Hirose DF11 vertical
0
12
12
Connector_Hirose
Hirose_DF11-14DP-2DSA_2x07_P2.00mm_Vertical
Hirose DF11 through hole, DF11-14DP-2DSA, 7 Pins per row (https://www.hirose.com/product/document?clcode=&productname=&series=DF11&documenttype=Catalog&lang=en&documentid=D31688_en), generated with kicad-footprint-generator
connector Hirose DF11 vertical
0
14
14
Connector_Hirose
Hirose_DF11-16DP-2DSA_2x08_P2.00mm_Vertical
Hirose DF11 through hole, DF11-16DP-2DSA, 8 Pins per row (https://www.hirose.com/product/document?clcode=&productname=&series=DF11&documenttype=Catalog&lang=en&documentid=D31688_en), generated with kicad-footprint-generator
connector Hirose DF11 vertical
0
16
16
Connector_Hirose
Hirose_DF11-18DP-2DSA_2x09_P2.00mm_Vertical
Hirose DF11 through hole, DF11-18DP-2DSA, 9 Pins per row (https://www.hirose.com/product/document?clcode=&productname=&series=DF11&documenttype=Catalog&lang=en&documentid=D31688_en), generated with kicad-footprint-generator
connector Hirose DF11 vertical
0
18
18
Connector_Hirose
Hirose_DF11-20DP-2DSA_2x10_P2.00mm_Vertical
Hirose DF11 through hole, DF11-20DP-2DSA, 10 Pins per row (https://www.hirose.com/product/document?clcode=&productname=&series=DF11&documenttype=Catalog&lang=en&documentid=D31688_en), generated with kicad-footprint-generator
connector Hirose DF11 vertical
0
20
20
Connector_Hirose
Hirose_DF11-22DP-2DSA_2x11_P2.00mm_Vertical
Hirose DF11 through hole, DF11-22DP-2DSA, 11 Pins per row (https://www.hirose.com/product/document?clcode=&productname=&series=DF11&documenttype=Catalog&lang=en&documentid=D31688_en), generated with kicad-footprint-generator
connector Hirose DF11 vertical
0
22
22
Connector_Hirose
Hirose_DF11-24DP-2DSA_2x12_P2.00mm_Vertical
Hirose DF11 through hole, DF11-24DP-2DSA, 12 Pins per row (https://www.hirose.com/product/document?clcode=&productname=&series=DF11&documenttype=Catalog&lang=en&documentid=D31688_en), generated with kicad-footprint-generator
connector Hirose DF11 vertical
0
24
24
Connector_Hirose
Hirose_DF11-26DP-2DSA_2x13_P2.00mm_Vertical
Hirose DF11 through hole, DF11-26DP-2DSA, 13 Pins per row (https://www.hirose.com/product/document?clcode=&productname=&series=DF11&documenttype=Catalog&lang=en&documentid=D31688_en), generated with kicad-footprint-generator
connector Hirose DF11 vertical
0
26
26
Connector_Hirose
Hirose_DF11-28DP-2DSA_2x14_P2.00mm_Vertical
Hirose DF11 through hole, DF11-28DP-2DSA, 14 Pins per row (https://www.hirose.com/product/document?clcode=&productname=&series=DF11&documenttype=Catalog&lang=en&documentid=D31688_en), generated with kicad-footprint-generator
connector Hirose DF11 vertical
0
28
28
Connector_Hirose
Hirose_DF11-30DP-2DSA_2x15_P2.00mm_Vertical
Hirose DF11 through hole, DF11-30DP-2DSA, 15 Pins per row (https://www.hirose.com/product/document?clcode=&productname=&series=DF11&documenttype=Catalog&lang=en&documentid=D31688_en), generated with kicad-footprint-generator
connector Hirose DF11 vertical
0
30
30
Connector_Hirose
Hirose_DF11-32DP-2DSA_2x16_P2.00mm_Vertical
Hirose DF11 through hole, DF11-32DP-2DSA, 16 Pins per row (https://www.hirose.com/product/document?clcode=&productname=&series=DF11&documenttype=Catalog&lang=en&documentid=D31688_en), generated with kicad-footprint-generator
connector Hirose DF11 vertical
0
32
32
Connector_Hirose
Hirose_DF12_DF12C3.0-10DS-0.5V_2x05_P0.50mm_Vertical
Hirose DF12C SMD, DF12C3.0-10DS-0.5V, 10 Pins per row (https://www.hirose.com/product/document?clcode=CL0537-0694-9-81&productname=DF12C(3.0)-50DS-0.5V(81)&series=DF12&documenttype=2DDrawing&lang=en&documentid=0000994748), generated with kicad-footprint-generator
connector Hirose DF12 vertical
0
20
10
Connector_Hirose
Hirose_DF12_DF12C3.0-14DS-0.5V_2x07_P0.50mm_Vertical
Hirose DF12C SMD, DF12C3.0-14DS-0.5V, 14 Pins per row (https://www.hirose.com/product/document?clcode=CL0537-0694-9-81&productname=DF12C(3.0)-50DS-0.5V(81)&series=DF12&documenttype=2DDrawing&lang=en&documentid=0000994748), generated with kicad-footprint-generator
connector Hirose DF12 vertical
0
28
14
Connector_Hirose
Hirose_DF12_DF12C3.0-20DS-0.5V_2x10_P0.50mm_Vertical
Hirose DF12C SMD, DF12C3.0-20DS-0.5V, 20 Pins per row (https://www.hirose.com/product/document?clcode=CL0537-0694-9-81&productname=DF12C(3.0)-50DS-0.5V(81)&series=DF12&documenttype=2DDrawing&lang=en&documentid=0000994748), generated with kicad-footprint-generator
connector Hirose DF12 vertical
0
40
20
Connector_Hirose
Hirose_DF12_DF12C3.0-30DS-0.5V_2x15_P0.50mm_Vertical
Hirose DF12C SMD, DF12C3.0-30DS-0.5V, 30 Pins per row (https://www.hirose.com/product/document?clcode=CL0537-0694-9-81&productname=DF12C(3.0)-50DS-0.5V(81)&series=DF12&documenttype=2DDrawing&lang=en&documentid=0000994748), generated with kicad-footprint-generator
connector Hirose DF12 vertical
0
60
30
Connector_Hirose
Hirose_DF12_DF12C3.0-32DS-0.5V_2x16_P0.50mm_Vertical
Hirose DF12C SMD, DF12C3.0-32DS-0.5V, 32 Pins per row (https://www.hirose.com/product/document?clcode=CL0537-0694-9-81&productname=DF12C(3.0)-50DS-0.5V(81)&series=DF12&documenttype=2DDrawing&lang=en&documentid=0000994748), generated with kicad-footprint-generator
connector Hirose DF12 vertical
0
64
32
Connector_Hirose
Hirose_DF12_DF12C3.0-36DS-0.5V_2x18_P0.50mm_Vertical
Hirose DF12C SMD, DF12C3.0-36DS-0.5V, 36 Pins per row (https://www.hirose.com/product/document?clcode=CL0537-0694-9-81&productname=DF12C(3.0)-50DS-0.5V(81)&series=DF12&documenttype=2DDrawing&lang=en&documentid=0000994748), generated with kicad-footprint-generator
connector Hirose DF12 vertical
0
72
36
Connector_Hirose
Hirose_DF12_DF12C3.0-40DS-0.5V_2x20_P0.50mm_Vertical
Hirose DF12C SMD, DF12C3.0-40DS-0.5V, 40 Pins per row (https://www.hirose.com/product/document?clcode=CL0537-0694-9-81&productname=DF12C(3.0)-50DS-0.5V(81)&series=DF12&documenttype=2DDrawing&lang=en&documentid=0000994748), generated with kicad-footprint-generator
connector Hirose DF12 vertical
0
80
40
Connector_Hirose
Hirose_DF12_DF12C3.0-50DS-0.5V_2x25_P0.50mm_Vertical
Hirose DF12C SMD, DF12C3.0-50DS-0.5V, 50 Pins per row (https://www.hirose.com/product/document?clcode=CL0537-0694-9-81&productname=DF12C(3.0)-50DS-0.5V(81)&series=DF12&documenttype=2DDrawing&lang=en&documentid=0000994748), generated with kicad-footprint-generator
connector Hirose DF12 vertical
0
100
50
Connector_Hirose
Hirose_DF12_DF12C3.0-60DS-0.5V_2x30_P0.50mm_Vertical
Hirose DF12C SMD, DF12C3.0-60DS-0.5V, 60 Pins per row (https://www.hirose.com/product/document?clcode=CL0537-0694-9-81&productname=DF12C(3.0)-50DS-0.5V(81)&series=DF12&documenttype=2DDrawing&lang=en&documentid=0000994748), generated with kicad-footprint-generator
connector Hirose DF12 vertical
0
120
60
Connector_Hirose
Hirose_DF12_DF12E3.0-10DP-0.5V_2x05_P0.50mm_Vertical
Hirose DF12E SMD, DF12E3.0-10DP-0.5V, 10 Pins per row (https://www.hirose.com/product/document?clcode=CL0537-0834-6-81&productname=DF12E(3.0)-50DP-0.5V(81)&series=DF12&documenttype=2DDrawing&lang=en&documentid=0000992393), generated with kicad-footprint-generator
connector Hirose DF12 vertical
0
20
10
Connector_Hirose
Hirose_DF12_DF12E3.0-14DP-0.5V_2x07_P0.50mm_Vertical
Hirose DF12E SMD, DF12E3.0-14DP-0.5V, 14 Pins per row (https://www.hirose.com/product/document?clcode=CL0537-0834-6-81&productname=DF12E(3.0)-50DP-0.5V(81)&series=DF12&documenttype=2DDrawing&lang=en&documentid=0000992393), generated with kicad-footprint-generator
connector Hirose DF12 vertical
0
28
14
Connector_Hirose
Hirose_DF12_DF12E3.0-20DP-0.5V_2x10_P0.50mm_Vertical
Hirose DF12E SMD, DF12E3.0-20DP-0.5V, 20 Pins per row (https://www.hirose.com/product/document?clcode=CL0537-0834-6-81&productname=DF12E(3.0)-50DP-0.5V(81)&series=DF12&documenttype=2DDrawing&lang=en&documentid=0000992393), generated with kicad-footprint-generator
connector Hirose DF12 vertical
0
40
20
Connector_Hirose
Hirose_DF12_DF12E3.0-30DP-0.5V_2x15_P0.50mm_Vertical
Hirose DF12E SMD, DF12E3.0-30DP-0.5V, 30 Pins per row (https://www.hirose.com/product/document?clcode=CL0537-0834-6-81&productname=DF12E(3.0)-50DP-0.5V(81)&series=DF12&documenttype=2DDrawing&lang=en&documentid=0000992393), generated with kicad-footprint-generator
connector Hirose DF12 vertical
0
60
30
Connector_Hirose
Hirose_DF12_DF12E3.0-32DP-0.5V_2x16_P0.50mm_Vertical
Hirose DF12E SMD, DF12E3.0-32DP-0.5V, 32 Pins per row (https://www.hirose.com/product/document?clcode=CL0537-0834-6-81&productname=DF12E(3.0)-50DP-0.5V(81)&series=DF12&documenttype=2DDrawing&lang=en&documentid=0000992393), generated with kicad-footprint-generator
connector Hirose DF12 vertical
0
64
32
Connector_Hirose
Hirose_DF12_DF12E3.0-36DP-0.5V_2x18_P0.50mm_Vertical
Hirose DF12E SMD, DF12E3.0-36DP-0.5V, 36 Pins per row (https://www.hirose.com/product/document?clcode=CL0537-0834-6-81&productname=DF12E(3.0)-50DP-0.5V(81)&series=DF12&documenttype=2DDrawing&lang=en&documentid=0000992393), generated with kicad-footprint-generator
connector Hirose DF12 vertical
0
72
36
Connector_Hirose
Hirose_DF12_DF12E3.0-40DP-0.5V_2x20_P0.50mm_Vertical
Hirose DF12E SMD, DF12E3.0-40DP-0.5V, 40 Pins per row (https://www.hirose.com/product/document?clcode=CL0537-0834-6-81&productname=DF12E(3.0)-50DP-0.5V(81)&series=DF12&documenttype=2DDrawing&lang=en&documentid=0000992393), generated with kicad-footprint-generator
connector Hirose DF12 vertical
0
80
40
Connector_Hirose
Hirose_DF12_DF12E3.0-50DP-0.5V_2x25_P0.50mm_Vertical
Hirose DF12E SMD, DF12E3.0-50DP-0.5V, 50 Pins per row (https://www.hirose.com/product/document?clcode=CL0537-0834-6-81&productname=DF12E(3.0)-50DP-0.5V(81)&series=DF12&documenttype=2DDrawing&lang=en&documentid=0000992393), generated with kicad-footprint-generator
connector Hirose DF12 vertical
0
100
50
Connector_Hirose
Hirose_DF12_DF12E3.0-60DP-0.5V_2x30_P0.50mm_Vertical
Hirose DF12E SMD, DF12E3.0-60DP-0.5V, 60 Pins per row (https://www.hirose.com/product/document?clcode=CL0537-0834-6-81&productname=DF12E(3.0)-50DP-0.5V(81)&series=DF12&documenttype=2DDrawing&lang=en&documentid=0000992393), generated with kicad-footprint-generator
connector Hirose DF12 vertical
0
120
60
Connector_Hirose
Hirose_DF12_DF12E3.0-80DP-0.5V_2x40_P0.50mm_Vertical
Hirose DF12E SMD, DF12E3.0-80DP-0.5V, 80 Pins per row (https://www.hirose.com/product/document?clcode=CL0537-0834-6-81&productname=DF12E(3.0)-50DP-0.5V(81)&series=DF12&documenttype=2DDrawing&lang=en&documentid=0000992393), generated with kicad-footprint-generator
connector Hirose DF12 vertical
0
160
80
Connector_Hirose
Hirose_DF13-02P-1.25DSA_1x02_P1.25mm_Vertical
Hirose DF13 through hole, DF13-02P-1.25DSA, 2 Pins per row (https://www.hirose.com/product/en/products/DF13/DF13-2P-1.25DSA%2850%29/), generated with kicad-footprint-generator
connector Hirose DF13 vertical
0
2
2
Connector_Hirose
Hirose_DF13-02P-1.25DS_1x02_P1.25mm_Horizontal
Hirose DF13 through hole, DF13-02P-1.25DS, 2 Pins per row (https://www.hirose.com/product/en/products/DF13/DF13-4P-1.25DS%2820%29/), generated with kicad-footprint-generator
connector Hirose DF13 horizontal
0
2
2
Connector_Hirose
Hirose_DF13-03P-1.25DSA_1x03_P1.25mm_Vertical
Hirose DF13 through hole, DF13-03P-1.25DSA, 3 Pins per row (https://www.hirose.com/product/en/products/DF13/DF13-2P-1.25DSA%2850%29/), generated with kicad-footprint-generator
connector Hirose DF13 vertical
0
3
3
Connector_Hirose
Hirose_DF13-03P-1.25DS_1x03_P1.25mm_Horizontal
Hirose DF13 through hole, DF13-03P-1.25DS, 3 Pins per row (https://www.hirose.com/product/en/products/DF13/DF13-4P-1.25DS%2820%29/), generated with kicad-footprint-generator
connector Hirose DF13 horizontal
0
3
3
Connector_Hirose
Hirose_DF13-04P-1.25DSA_1x04_P1.25mm_Vertical
Hirose DF13 through hole, DF13-04P-1.25DSA, 4 Pins per row (https://www.hirose.com/product/en/products/DF13/DF13-2P-1.25DSA%2850%29/), generated with kicad-footprint-generator
connector Hirose DF13 vertical
0
4
4
Connector_Hirose
Hirose_DF13-04P-1.25DS_1x04_P1.25mm_Horizontal
Hirose DF13 through hole, DF13-04P-1.25DS, 4 Pins per row (https://www.hirose.com/product/en/products/DF13/DF13-4P-1.25DS%2820%29/), generated with kicad-footprint-generator
connector Hirose DF13 horizontal
0
4
4
Connector_Hirose
Hirose_DF13-05P-1.25DSA_1x05_P1.25mm_Vertical
Hirose DF13 through hole, DF13-05P-1.25DSA, 5 Pins per row (https://www.hirose.com/product/en/products/DF13/DF13-2P-1.25DSA%2850%29/), generated with kicad-footprint-generator
connector Hirose DF13 vertical
0
5
5
Connector_Hirose
Hirose_DF13-05P-1.25DS_1x05_P1.25mm_Horizontal
Hirose DF13 through hole, DF13-05P-1.25DS, 5 Pins per row (https://www.hirose.com/product/en/products/DF13/DF13-4P-1.25DS%2820%29/), generated with kicad-footprint-generator
connector Hirose DF13 horizontal
0
5
5
Connector_Hirose
Hirose_DF13-06P-1.25DSA_1x06_P1.25mm_Vertical
Hirose DF13 through hole, DF13-06P-1.25DSA, 6 Pins per row (https://www.hirose.com/product/en/products/DF13/DF13-2P-1.25DSA%2850%29/), generated with kicad-footprint-generator
connector Hirose DF13 vertical
0
6
6
Connector_Hirose
Hirose_DF13-06P-1.25DS_1x06_P1.25mm_Horizontal
Hirose DF13 through hole, DF13-06P-1.25DS, 6 Pins per row (https://www.hirose.com/product/en/products/DF13/DF13-4P-1.25DS%2820%29/), generated with kicad-footprint-generator
connector Hirose DF13 horizontal
0
6
6
Connector_Hirose
Hirose_DF13-07P-1.25DSA_1x07_P1.25mm_Vertical
Hirose DF13 through hole, DF13-07P-1.25DSA, 7 Pins per row (https://www.hirose.com/product/en/products/DF13/DF13-2P-1.25DSA%2850%29/), generated with kicad-footprint-generator
connector Hirose DF13 vertical
0
7
7
Connector_Hirose
Hirose_DF13-07P-1.25DS_1x07_P1.25mm_Horizontal
Hirose DF13 through hole, DF13-07P-1.25DS, 7 Pins per row (https://www.hirose.com/product/en/products/DF13/DF13-4P-1.25DS%2820%29/), generated with kicad-footprint-generator
connector Hirose DF13 horizontal
0
7
7
Connector_Hirose
Hirose_DF13-08P-1.25DSA_1x08_P1.25mm_Vertical
Hirose DF13 through hole, DF13-08P-1.25DSA, 8 Pins per row (https://www.hirose.com/product/en/products/DF13/DF13-2P-1.25DSA%2850%29/), generated with kicad-footprint-generator
connector Hirose DF13 vertical
0
8
8
Connector_Hirose
Hirose_DF13-08P-1.25DS_1x08_P1.25mm_Horizontal
Hirose DF13 through hole, DF13-08P-1.25DS, 8 Pins per row (https://www.hirose.com/product/en/products/DF13/DF13-4P-1.25DS%2820%29/), generated with kicad-footprint-generator
connector Hirose DF13 horizontal
0
8
8
Connector_Hirose
Hirose_DF13-09P-1.25DSA_1x09_P1.25mm_Vertical
Hirose DF13 through hole, DF13-09P-1.25DSA, 9 Pins per row (https://www.hirose.com/product/en/products/DF13/DF13-2P-1.25DSA%2850%29/), generated with kicad-footprint-generator
connector Hirose DF13 vertical
0
9
9
Connector_Hirose
Hirose_DF13-09P-1.25DS_1x09_P1.25mm_Horizontal
Hirose DF13 through hole, DF13-09P-1.25DS, 9 Pins per row (https://www.hirose.com/product/en/products/DF13/DF13-4P-1.25DS%2820%29/), generated with kicad-footprint-generator
connector Hirose DF13 horizontal
0
9
9
Connector_Hirose
Hirose_DF13-10P-1.25DSA_1x10_P1.25mm_Vertical
Hirose DF13 through hole, DF13-10P-1.25DSA, 10 Pins per row (https://www.hirose.com/product/en/products/DF13/DF13-2P-1.25DSA%2850%29/), generated with kicad-footprint-generator
connector Hirose DF13 vertical
0
10
10
Connector_Hirose
Hirose_DF13-10P-1.25DS_1x10_P1.25mm_Horizontal
Hirose DF13 through hole, DF13-10P-1.25DS, 10 Pins per row (https://www.hirose.com/product/en/products/DF13/DF13-4P-1.25DS%2820%29/), generated with kicad-footprint-generator
connector Hirose DF13 horizontal
0
10
10
Connector_Hirose
Hirose_DF13-11P-1.25DSA_1x11_P1.25mm_Vertical
Hirose DF13 through hole, DF13-11P-1.25DSA, 11 Pins per row (https://www.hirose.com/product/en/products/DF13/DF13-2P-1.25DSA%2850%29/), generated with kicad-footprint-generator
connector Hirose DF13 vertical
0
11
11
Connector_Hirose
Hirose_DF13-11P-1.25DS_1x11_P1.25mm_Horizontal
Hirose DF13 through hole, DF13-11P-1.25DS, 11 Pins per row (https://www.hirose.com/product/en/products/DF13/DF13-4P-1.25DS%2820%29/), generated with kicad-footprint-generator
connector Hirose DF13 horizontal
0
11
11
Connector_Hirose
Hirose_DF13-12P-1.25DSA_1x12_P1.25mm_Vertical
Hirose DF13 through hole, DF13-12P-1.25DSA, 12 Pins per row (https://www.hirose.com/product/en/products/DF13/DF13-2P-1.25DSA%2850%29/), generated with kicad-footprint-generator
connector Hirose DF13 vertical
0
12
12
Connector_Hirose
Hirose_DF13-12P-1.25DS_1x12_P1.25mm_Horizontal
Hirose DF13 through hole, DF13-12P-1.25DS, 12 Pins per row (https://www.hirose.com/product/en/products/DF13/DF13-4P-1.25DS%2820%29/), generated with kicad-footprint-generator
connector Hirose DF13 horizontal
0
12
12
Connector_Hirose
Hirose_DF13-13P-1.25DSA_1x13_P1.25mm_Vertical
Hirose DF13 through hole, DF13-13P-1.25DSA, 13 Pins per row (https://www.hirose.com/product/en/products/DF13/DF13-2P-1.25DSA%2850%29/), generated with kicad-footprint-generator
connector Hirose DF13 vertical
0
13
13
Connector_Hirose
Hirose_DF13-14P-1.25DSA_1x14_P1.25mm_Vertical
Hirose DF13 through hole, DF13-14P-1.25DSA, 14 Pins per row (https://www.hirose.com/product/en/products/DF13/DF13-2P-1.25DSA%2850%29/), generated with kicad-footprint-generator
connector Hirose DF13 vertical
0
14
14
Connector_Hirose
Hirose_DF13-14P-1.25DS_1x14_P1.25mm_Horizontal
Hirose DF13 through hole, DF13-14P-1.25DS, 14 Pins per row (https://www.hirose.com/product/en/products/DF13/DF13-4P-1.25DS%2820%29/), generated with kicad-footprint-generator
connector Hirose DF13 horizontal
0
14
14
Connector_Hirose
Hirose_DF13-15P-1.25DSA_1x15_P1.25mm_Vertical
Hirose DF13 through hole, DF13-15P-1.25DSA, 15 Pins per row (https://www.hirose.com/product/en/products/DF13/DF13-2P-1.25DSA%2850%29/), generated with kicad-footprint-generator
connector Hirose DF13 vertical
0
15
15
Connector_Hirose
Hirose_DF13-15P-1.25DS_1x15_P1.25mm_Horizontal
Hirose DF13 through hole, DF13-15P-1.25DS, 15 Pins per row (https://www.hirose.com/product/en/products/DF13/DF13-4P-1.25DS%2820%29/), generated with kicad-footprint-generator
connector Hirose DF13 horizontal
0
15
15
Connector_Hirose
Hirose_DF13C_CL535-0402-2-51_1x02-1MP_P1.25mm_Vertical
Hirose DF13C SMD, CL535-0402-2-51, 2 Pins per row (https://www.hirose.com/product/en/products/DF13/DF13C-10P-1.25V%2851%29/), generated with kicad-footprint-generator
connector Hirose DF13C vertical
0
4
3
Connector_Hirose
Hirose_DF13C_CL535-0403-5-51_1x03-1MP_P1.25mm_Vertical
Hirose DF13C SMD, CL535-0403-5-51, 3 Pins per row (https://www.hirose.com/product/en/products/DF13/DF13C-10P-1.25V%2851%29/), generated with kicad-footprint-generator
connector Hirose DF13C vertical
0
5
4
Connector_Hirose
Hirose_DF13C_CL535-0404-8-51_1x04-1MP_P1.25mm_Vertical
Hirose DF13C SMD, CL535-0404-8-51, 4 Pins per row (https://www.hirose.com/product/en/products/DF13/DF13C-10P-1.25V%2851%29/), generated with kicad-footprint-generator
connector Hirose DF13C vertical
0
6
5
Connector_Hirose
Hirose_DF13C_CL535-0405-0-51_1x05-1MP_P1.25mm_Vertical
Hirose DF13C SMD, CL535-0405-0-51, 5 Pins per row (https://www.hirose.com/product/en/products/DF13/DF13C-10P-1.25V%2851%29/), generated with kicad-footprint-generator
connector Hirose DF13C vertical
0
7
6
Connector_Hirose
Hirose_DF13C_CL535-0406-3-51_1x06-1MP_P1.25mm_Vertical
Hirose DF13C SMD, CL535-0406-3-51, 6 Pins per row (https://www.hirose.com/product/en/products/DF13/DF13C-10P-1.25V%2851%29/), generated with kicad-footprint-generator
connector Hirose DF13C vertical
0
8
7
Connector_Hirose
Hirose_DF13C_CL535-0407-6-51_1x07-1MP_P1.25mm_Vertical
Hirose DF13C SMD, CL535-0407-6-51, 7 Pins per row (https://www.hirose.com/product/en/products/DF13/DF13C-10P-1.25V%2851%29/), generated with kicad-footprint-generator
connector Hirose DF13C vertical
0
9
8
Connector_Hirose
Hirose_DF13C_CL535-0408-9-51_1x08-1MP_P1.25mm_Vertical
Hirose DF13C SMD, CL535-0408-9-51, 8 Pins per row (https://www.hirose.com/product/en/products/DF13/DF13C-10P-1.25V%2851%29/), generated with kicad-footprint-generator
connector Hirose DF13C vertical
0
10
9
Connector_Hirose
Hirose_DF13C_CL535-0409-1-51_1x09-1MP_P1.25mm_Vertical
Hirose DF13C SMD, CL535-0409-1-51, 9 Pins per row (https://www.hirose.com/product/en/products/DF13/DF13C-10P-1.25V%2851%29/), generated with kicad-footprint-generator
connector Hirose DF13C vertical
0
11
10
Connector_Hirose
Hirose_DF13C_CL535-0410-4-51_1x10-1MP_P1.25mm_Vertical
Hirose DF13C SMD, CL535-0410-4-51, 10 Pins per row (https://www.hirose.com/product/en/products/DF13/DF13C-10P-1.25V%2851%29/), generated with kicad-footprint-generator
connector Hirose DF13C vertical
0
12
11
Connector_Hirose
Hirose_DF13C_CL535-0411-3-51_1x11-1MP_P1.25mm_Vertical
Hirose DF13C SMD, CL535-0411-3-51, 11 Pins per row (https://www.hirose.com/product/en/products/DF13/DF13C-10P-1.25V%2851%29/), generated with kicad-footprint-generator
connector Hirose DF13C vertical
0
13
12
Connector_Hirose
Hirose_DF13C_CL535-0412-6-51_1x12-1MP_P1.25mm_Vertical
Hirose DF13C SMD, CL535-0412-6-51, 12 Pins per row (https://www.hirose.com/product/en/products/DF13/DF13C-10P-1.25V%2851%29/), generated with kicad-footprint-generator
connector Hirose DF13C vertical
0
14
13
Connector_Hirose
Hirose_DF13C_CL535-0414-1-51_1x14-1MP_P1.25mm_Vertical
Hirose DF13C SMD, CL535-0414-1-51, 14 Pins per row (https://www.hirose.com/product/en/products/DF13/DF13C-10P-1.25V%2851%29/), generated with kicad-footprint-generator
connector Hirose DF13C vertical
0
16
15
Connector_Hirose
Hirose_DF13C_CL535-0415-4-51_1x15-1MP_P1.25mm_Vertical
Hirose DF13C SMD, CL535-0415-4-51, 15 Pins per row (https://www.hirose.com/product/en/products/DF13/DF13C-10P-1.25V%2851%29/), generated with kicad-footprint-generator
connector Hirose DF13C vertical
0
17
16
Connector_Hirose
Hirose_DF52-2S-0.8H_1x02-1MP_P0.80mm_Horizontal
Hirose  series connector, DF52-2S-0.8H (https://www.hirose.com/product/en/products/DF52/DF52-3S-0.8H%2821%29/), generated with kicad-footprint-generator
connector Hirose  top entry
0
4
3
Connector_Hirose
Hirose_DF52-3S-0.8H_1x03-1MP_P0.80mm_Horizontal
Hirose  series connector, DF52-3S-0.8H (https://www.hirose.com/product/en/products/DF52/DF52-3S-0.8H%2821%29/), generated with kicad-footprint-generator
connector Hirose  top entry
0
5
4
Connector_Hirose
Hirose_DF52-4S-0.8H_1x04-1MP_P0.80mm_Horizontal
Hirose  series connector, DF52-4S-0.8H (https://www.hirose.com/product/en/products/DF52/DF52-3S-0.8H%2821%29/), generated with kicad-footprint-generator
connector Hirose  top entry
0
6
5
Connector_Hirose
Hirose_DF52-5S-0.8H_1x05-1MP_P0.80mm_Horizontal
Hirose  series connector, DF52-5S-0.8H (https://www.hirose.com/product/en/products/DF52/DF52-3S-0.8H%2821%29/), generated with kicad-footprint-generator
connector Hirose  top entry
0
7
6
Connector_Hirose
Hirose_DF52-6S-0.8H_1x06-1MP_P0.80mm_Horizontal
Hirose  series connector, DF52-6S-0.8H (https://www.hirose.com/product/en/products/DF52/DF52-3S-0.8H%2821%29/), generated with kicad-footprint-generator
connector Hirose  top entry
0
8
7
Connector_Hirose
Hirose_DF52-7S-0.8H_1x07-1MP_P0.80mm_Horizontal
Hirose  series connector, DF52-7S-0.8H (https://www.hirose.com/product/en/products/DF52/DF52-3S-0.8H%2821%29/), generated with kicad-footprint-generator
connector Hirose  top entry
0
9
8
Connector_Hirose
Hirose_DF52-8S-0.8H_1x08-1MP_P0.80mm_Horizontal
Hirose  series connector, DF52-8S-0.8H (https://www.hirose.com/product/en/products/DF52/DF52-3S-0.8H%2821%29/), generated with kicad-footprint-generator
connector Hirose  top entry
0
10
9
Connector_Hirose
Hirose_DF52-9S-0.8H_1x09-1MP_P0.80mm_Horizontal
Hirose  series connector, DF52-9S-0.8H (https://www.hirose.com/product/en/products/DF52/DF52-3S-0.8H%2821%29/), generated with kicad-footprint-generator
connector Hirose  top entry
0
11
10
Connector_Hirose
Hirose_DF52-10S-0.8H_1x10-1MP_P0.80mm_Horizontal
Hirose  series connector, DF52-10S-0.8H (https://www.hirose.com/product/en/products/DF52/DF52-3S-0.8H%2821%29/), generated with kicad-footprint-generator
connector Hirose  top entry
0
12
11
Connector_Hirose
Hirose_DF52-11S-0.8H_1x11-1MP_P0.80mm_Horizontal
Hirose  series connector, DF52-11S-0.8H (https://www.hirose.com/product/en/products/DF52/DF52-3S-0.8H%2821%29/), generated with kicad-footprint-generator
connector Hirose  top entry
0
13
12
Connector_Hirose
Hirose_DF52-12S-0.8H_1x12-1MP_P0.80mm_Horizontal
Hirose  series connector, DF52-12S-0.8H (https://www.hirose.com/product/en/products/DF52/DF52-3S-0.8H%2821%29/), generated with kicad-footprint-generator
connector Hirose  top entry
0
14
13
Connector_Hirose
Hirose_DF52-14S-0.8H_1x14-1MP_P0.80mm_Horizontal
Hirose  series connector, DF52-14S-0.8H (https://www.hirose.com/product/en/products/DF52/DF52-3S-0.8H%2821%29/), generated with kicad-footprint-generator
connector Hirose  top entry
0
16
15
Connector_Hirose
Hirose_DF52-15S-0.8H_1x15-1MP_P0.80mm_Horizontal
Hirose  series connector, DF52-15S-0.8H (https://www.hirose.com/product/en/products/DF52/DF52-3S-0.8H%2821%29/), generated with kicad-footprint-generator
connector Hirose  top entry
0
17
16
Connector_Hirose
Hirose_DF63-5P-3.96DSA_1x05_P3.96mm_Vertical
Hirose DF63 through hole, DF63-5P-3.96DSA, 5 Pins per row (https://www.hirose.com/product/en/products/DF63/), generated with kicad-footprint-generator
connector Hirose DF63 vertical
0
5
5
Connector_Hirose
Hirose_DF63-6P-3.96DSA_1x06_P3.96mm_Vertical
Hirose DF63 through hole, DF63-6P-3.96DSA, 6 Pins per row (https://www.hirose.com/product/en/products/DF63/), generated with kicad-footprint-generator
connector Hirose DF63 vertical
0
6
6
Connector_Hirose
Hirose_DF63M-1P-3.96DSA_1x01_P3.96mm_Vertical
Hirose DF63 through hole, DF63M-1P-3.96DSA, 1 Pins per row (https://www.hirose.com/product/en/products/DF63/), generated with kicad-footprint-generator
connector Hirose DF63 vertical
0
1
1
Connector_Hirose
Hirose_DF63M-2P-3.96DSA_1x02_P3.96mm_Vertical
Hirose DF63 through hole, DF63M-2P-3.96DSA, 2 Pins per row (https://www.hirose.com/product/en/products/DF63/), generated with kicad-footprint-generator
connector Hirose DF63 vertical
0
2
2
Connector_Hirose
Hirose_DF63M-3P-3.96DSA_1x03_P3.96mm_Vertical
Hirose DF63 through hole, DF63M-3P-3.96DSA, 3 Pins per row (https://www.hirose.com/product/en/products/DF63/), generated with kicad-footprint-generator
connector Hirose DF63 vertical
0
3
3
Connector_Hirose
Hirose_DF63M-4P-3.96DSA_1x04_P3.96mm_Vertical
Hirose DF63 through hole, DF63M-4P-3.96DSA, 4 Pins per row (https://www.hirose.com/product/en/products/DF63/), generated with kicad-footprint-generator
connector Hirose DF63 vertical
0
4
4
Connector_Hirose
Hirose_DF63R-1P-3.96DSA_1x01_P3.96mm_Vertical
Hirose DF63 through hole, DF63R-1P-3.96DSA, 1 Pins per row (https://www.hirose.com/product/en/products/DF63/), generated with kicad-footprint-generator
connector Hirose DF63 vertical
0
1
1
Connector_Hirose
Hirose_DF63R-2P-3.96DSA_1x02_P3.96mm_Vertical
Hirose DF63 through hole, DF63R-2P-3.96DSA, 2 Pins per row (https://www.hirose.com/product/en/products/DF63/), generated with kicad-footprint-generator
connector Hirose DF63 vertical
0
2
2
Connector_Hirose
Hirose_DF63R-3P-3.96DSA_1x03_P3.96mm_Vertical
Hirose DF63 through hole, DF63R-3P-3.96DSA, 3 Pins per row (https://www.hirose.com/product/en/products/DF63/), generated with kicad-footprint-generator
connector Hirose DF63 vertical
0
3
3
Connector_Hirose
Hirose_DF63R-4P-3.96DSA_1x04_P3.96mm_Vertical
Hirose DF63 through hole, DF63R-4P-3.96DSA, 4 Pins per row (https://www.hirose.com/product/en/products/DF63/), generated with kicad-footprint-generator
connector Hirose DF63 vertical
0
4
4
Connector_Hirose
Hirose_DF63R-5P-3.96DSA_1x05_P3.96mm_Vertical
Hirose DF63 through hole, DF63R-5P-3.96DSA, 5 Pins per row (https://www.hirose.com/product/en/products/DF63/), generated with kicad-footprint-generator
connector Hirose DF63 vertical
0
5
5
Connector_IDC
IDC-Header_2x03_P2.54mm_Horizontal
Through hole IDC box header, 2x03, 2.54mm pitch, DIN 41651 / IEC 60603-13, double rows, https://docs.google.com/spreadsheets/d/16SsEcesNF15N3Lb4niX7dcUr-NY5_MFPQhobNuNppn4/edit#gid=0
Through hole horizontal IDC box header THT 2x03 2.54mm double row
0
6
6
Connector_IDC
IDC-Header_2x03_P2.54mm_Vertical
Through hole IDC box header, 2x03, 2.54mm pitch, DIN 41651 / IEC 60603-13, double rows, https://docs.google.com/spreadsheets/d/16SsEcesNF15N3Lb4niX7dcUr-NY5_MFPQhobNuNppn4/edit#gid=0
Through hole vertical IDC box header THT 2x03 2.54mm double row
0
6
6
Connector_IDC
IDC-Header_2x04_P2.54mm_Horizontal
Through hole IDC box header, 2x04, 2.54mm pitch, DIN 41651 / IEC 60603-13, double rows, https://docs.google.com/spreadsheets/d/16SsEcesNF15N3Lb4niX7dcUr-NY5_MFPQhobNuNppn4/edit#gid=0
Through hole horizontal IDC box header THT 2x04 2.54mm double row
0
8
8
Connector_IDC
IDC-Header_2x04_P2.54mm_Vertical
Through hole IDC box header, 2x04, 2.54mm pitch, DIN 41651 / IEC 60603-13, double rows, https://docs.google.com/spreadsheets/d/16SsEcesNF15N3Lb4niX7dcUr-NY5_MFPQhobNuNppn4/edit#gid=0
Through hole vertical IDC box header THT 2x04 2.54mm double row
0
8
8
Connector_IDC
IDC-Header_2x05-1MP_P2.54mm_Latch6.5mm_Vertical
Through hole IDC header, 2x05, 2.54mm pitch, DIN 41651 / IEC 60603-13, double rows, 6.5mm latches, mounting holes, https://docs.google.com/spreadsheets/d/16SsEcesNF15N3Lb4niX7dcUr-NY5_MFPQhobNuNppn4/edit#gid=0
Through hole vertical IDC header THT 2x05 2.54mm double row
0
12
11
Connector_IDC
IDC-Header_2x05-1MP_P2.54mm_Latch9.5mm_Vertical
Through hole IDC header, 2x05, 2.54mm pitch, DIN 41651 / IEC 60603-13, double rows, 9.5mm latches, mounting holes, https://docs.google.com/spreadsheets/d/16SsEcesNF15N3Lb4niX7dcUr-NY5_MFPQhobNuNppn4/edit#gid=0
Through hole vertical IDC header THT 2x05 2.54mm double row
0
12
11
Connector_IDC
IDC-Header_2x05-1MP_P2.54mm_Latch12.0mm_Vertical
Through hole IDC header, 2x05, 2.54mm pitch, DIN 41651 / IEC 60603-13, double rows, 12.0mm latches, mounting holes, https://docs.google.com/spreadsheets/d/16SsEcesNF15N3Lb4niX7dcUr-NY5_MFPQhobNuNppn4/edit#gid=0
Through hole vertical IDC header THT 2x05 2.54mm double row
0
12
11
Connector_IDC
IDC-Header_2x05-1MP_P2.54mm_Latch_Horizontal
Through hole IDC header, 2x05, 2.54mm pitch, DIN 41651 / IEC 60603-13, double rows latches, mounting holes, https://docs.google.com/spreadsheets/d/16SsEcesNF15N3Lb4niX7dcUr-NY5_MFPQhobNuNppn4/edit#gid=0
Through hole horizontal IDC header THT 2x05 2.54mm double row
0
12
11
Connector_IDC
IDC-Header_2x05-1MP_P2.54mm_Latch_Vertical
Through hole IDC header, 2x05, 2.54mm pitch, DIN 41651 / IEC 60603-13, double rows latches, mounting holes, https://docs.google.com/spreadsheets/d/16SsEcesNF15N3Lb4niX7dcUr-NY5_MFPQhobNuNppn4/edit#gid=0
Through hole vertical IDC header THT 2x05 2.54mm double row
0
12
11
Connector_IDC
IDC-Header_2x05_P2.54mm_Horizontal
Through hole IDC box header, 2x05, 2.54mm pitch, DIN 41651 / IEC 60603-13, double rows, https://docs.google.com/spreadsheets/d/16SsEcesNF15N3Lb4niX7dcUr-NY5_MFPQhobNuNppn4/edit#gid=0
Through hole horizontal IDC box header THT 2x05 2.54mm double row
0
10
10
Connector_IDC
IDC-Header_2x05_P2.54mm_Latch6.5mm_Vertical
Through hole IDC header, 2x05, 2.54mm pitch, DIN 41651 / IEC 60603-13, double rows, 6.5mm latches, https://docs.google.com/spreadsheets/d/16SsEcesNF15N3Lb4niX7dcUr-NY5_MFPQhobNuNppn4/edit#gid=0
Through hole vertical IDC header THT 2x05 2.54mm double row
0
10
10
Connector_IDC
IDC-Header_2x05_P2.54mm_Latch9.5mm_Vertical
Through hole IDC header, 2x05, 2.54mm pitch, DIN 41651 / IEC 60603-13, double rows, 9.5mm latches, https://docs.google.com/spreadsheets/d/16SsEcesNF15N3Lb4niX7dcUr-NY5_MFPQhobNuNppn4/edit#gid=0
Through hole vertical IDC header THT 2x05 2.54mm double row
0
10
10
Connector_IDC
IDC-Header_2x05_P2.54mm_Latch12.0mm_Vertical
Through hole IDC header, 2x05, 2.54mm pitch, DIN 41651 / IEC 60603-13, double rows, 12.0mm latches, https://docs.google.com/spreadsheets/d/16SsEcesNF15N3Lb4niX7dcUr-NY5_MFPQhobNuNppn4/edit#gid=0
Through hole vertical IDC header THT 2x05 2.54mm double row
0
10
10
Connector_IDC
IDC-Header_2x05_P2.54mm_Latch_Horizontal
Through hole IDC header, 2x05, 2.54mm pitch, DIN 41651 / IEC 60603-13, double rows latches, https://docs.google.com/spreadsheets/d/16SsEcesNF15N3Lb4niX7dcUr-NY5_MFPQhobNuNppn4/edit#gid=0
Through hole horizontal IDC header THT 2x05 2.54mm double row
0
10
10
Connector_IDC
IDC-Header_2x05_P2.54mm_Latch_Vertical
Through hole IDC header, 2x05, 2.54mm pitch, DIN 41651 / IEC 60603-13, double rows latches, https://docs.google.com/spreadsheets/d/16SsEcesNF15N3Lb4niX7dcUr-NY5_MFPQhobNuNppn4/edit#gid=0
Through hole vertical IDC header THT 2x05 2.54mm double row
0
10
10
Connector_IDC
IDC-Header_2x05_P2.54mm_Vertical
Through hole IDC box header, 2x05, 2.54mm pitch, DIN 41651 / IEC 60603-13, double rows, https://docs.google.com/spreadsheets/d/16SsEcesNF15N3Lb4niX7dcUr-NY5_MFPQhobNuNppn4/edit#gid=0
Through hole vertical IDC box header THT 2x05 2.54mm double row
0
10
10
Connector_IDC
IDC-Header_2x06-1MP_P2.54mm_Latch6.5mm_Vertical
Through hole IDC header, 2x06, 2.54mm pitch, DIN 41651 / IEC 60603-13, double rows, 6.5mm latches, mounting holes, https://docs.google.com/spreadsheets/d/16SsEcesNF15N3Lb4niX7dcUr-NY5_MFPQhobNuNppn4/edit#gid=0
Through hole vertical IDC header THT 2x06 2.54mm double row
0
14
13
Connector_IDC
IDC-Header_2x06-1MP_P2.54mm_Latch9.5mm_Vertical
Through hole IDC header, 2x06, 2.54mm pitch, DIN 41651 / IEC 60603-13, double rows, 9.5mm latches, mounting holes, https://docs.google.com/spreadsheets/d/16SsEcesNF15N3Lb4niX7dcUr-NY5_MFPQhobNuNppn4/edit#gid=0
Through hole vertical IDC header THT 2x06 2.54mm double row
0
14
13
Connector_IDC
IDC-Header_2x06-1MP_P2.54mm_Latch12.0mm_Vertical
Through hole IDC header, 2x06, 2.54mm pitch, DIN 41651 / IEC 60603-13, double rows, 12.0mm latches, mounting holes, https://docs.google.com/spreadsheets/d/16SsEcesNF15N3Lb4niX7dcUr-NY5_MFPQhobNuNppn4/edit#gid=0
Through hole vertical IDC header THT 2x06 2.54mm double row
0
14
13
Connector_IDC
IDC-Header_2x06-1MP_P2.54mm_Latch_Horizontal
Through hole IDC header, 2x06, 2.54mm pitch, DIN 41651 / IEC 60603-13, double rows latches, mounting holes, https://docs.google.com/spreadsheets/d/16SsEcesNF15N3Lb4niX7dcUr-NY5_MFPQhobNuNppn4/edit#gid=0
Through hole horizontal IDC header THT 2x06 2.54mm double row
0
14
13
Connector_IDC
IDC-Header_2x06-1MP_P2.54mm_Latch_Vertical
Through hole IDC header, 2x06, 2.54mm pitch, DIN 41651 / IEC 60603-13, double rows latches, mounting holes, https://docs.google.com/spreadsheets/d/16SsEcesNF15N3Lb4niX7dcUr-NY5_MFPQhobNuNppn4/edit#gid=0
Through hole vertical IDC header THT 2x06 2.54mm double row
0
14
13
Connector_IDC
IDC-Header_2x06_P2.54mm_Horizontal
Through hole IDC box header, 2x06, 2.54mm pitch, DIN 41651 / IEC 60603-13, double rows, https://docs.google.com/spreadsheets/d/16SsEcesNF15N3Lb4niX7dcUr-NY5_MFPQhobNuNppn4/edit#gid=0
Through hole horizontal IDC box header THT 2x06 2.54mm double row
0
12
12
Connector_IDC
IDC-Header_2x06_P2.54mm_Latch6.5mm_Vertical
Through hole IDC header, 2x06, 2.54mm pitch, DIN 41651 / IEC 60603-13, double rows, 6.5mm latches, https://docs.google.com/spreadsheets/d/16SsEcesNF15N3Lb4niX7dcUr-NY5_MFPQhobNuNppn4/edit#gid=0
Through hole vertical IDC header THT 2x06 2.54mm double row
0
12
12
Connector_IDC
IDC-Header_2x06_P2.54mm_Latch9.5mm_Vertical
Through hole IDC header, 2x06, 2.54mm pitch, DIN 41651 / IEC 60603-13, double rows, 9.5mm latches, https://docs.google.com/spreadsheets/d/16SsEcesNF15N3Lb4niX7dcUr-NY5_MFPQhobNuNppn4/edit#gid=0
Through hole vertical IDC header THT 2x06 2.54mm double row
0
12
12
Connector_IDC
IDC-Header_2x06_P2.54mm_Latch12.0mm_Vertical
Through hole IDC header, 2x06, 2.54mm pitch, DIN 41651 / IEC 60603-13, double rows, 12.0mm latches, https://docs.google.com/spreadsheets/d/16SsEcesNF15N3Lb4niX7dcUr-NY5_MFPQhobNuNppn4/edit#gid=0
Through hole vertical IDC header THT 2x06 2.54mm double row
0
12
12
Connector_IDC
IDC-Header_2x06_P2.54mm_Latch_Horizontal
Through hole IDC header, 2x06, 2.54mm pitch, DIN 41651 / IEC 60603-13, double rows latches, https://docs.google.com/spreadsheets/d/16SsEcesNF15N3Lb4niX7dcUr-NY5_MFPQhobNuNppn4/edit#gid=0
Through hole horizontal IDC header THT 2x06 2.54mm double row
0
12
12
Connector_IDC
IDC-Header_2x06_P2.54mm_Latch_Vertical
Through hole IDC header, 2x06, 2.54mm pitch, DIN 41651 / IEC 60603-13, double rows latches, https://docs.google.com/spreadsheets/d/16SsEcesNF15N3Lb4niX7dcUr-NY5_MFPQhobNuNppn4/edit#gid=0
Through hole vertical IDC header THT 2x06 2.54mm double row
0
12
12
Connector_IDC
IDC-Header_2x06_P2.54mm_Vertical
Through hole IDC box header, 2x06, 2.54mm pitch, DIN 41651 / IEC 60603-13, double rows, https://docs.google.com/spreadsheets/d/16SsEcesNF15N3Lb4niX7dcUr-NY5_MFPQhobNuNppn4/edit#gid=0
Through hole vertical IDC box header THT 2x06 2.54mm double row
0
12
12
Connector_IDC
IDC-Header_2x07-1MP_P2.54mm_Latch6.5mm_Vertical
Through hole IDC header, 2x07, 2.54mm pitch, DIN 41651 / IEC 60603-13, double rows, 6.5mm latches, mounting holes, https://docs.google.com/spreadsheets/d/16SsEcesNF15N3Lb4niX7dcUr-NY5_MFPQhobNuNppn4/edit#gid=0
Through hole vertical IDC header THT 2x07 2.54mm double row
0
16
15
Connector_IDC
IDC-Header_2x07-1MP_P2.54mm_Latch9.5mm_Vertical
Through hole IDC header, 2x07, 2.54mm pitch, DIN 41651 / IEC 60603-13, double rows, 9.5mm latches, mounting holes, https://docs.google.com/spreadsheets/d/16SsEcesNF15N3Lb4niX7dcUr-NY5_MFPQhobNuNppn4/edit#gid=0
Through hole vertical IDC header THT 2x07 2.54mm double row
0
16
15
Connector_IDC
IDC-Header_2x07-1MP_P2.54mm_Latch12.0mm_Vertical
Through hole IDC header, 2x07, 2.54mm pitch, DIN 41651 / IEC 60603-13, double rows, 12.0mm latches, mounting holes, https://docs.google.com/spreadsheets/d/16SsEcesNF15N3Lb4niX7dcUr-NY5_MFPQhobNuNppn4/edit#gid=0
Through hole vertical IDC header THT 2x07 2.54mm double row
0
16
15
Connector_IDC
IDC-Header_2x07-1MP_P2.54mm_Latch_Horizontal
Through hole IDC header, 2x07, 2.54mm pitch, DIN 41651 / IEC 60603-13, double rows latches, mounting holes, https://docs.google.com/spreadsheets/d/16SsEcesNF15N3Lb4niX7dcUr-NY5_MFPQhobNuNppn4/edit#gid=0
Through hole horizontal IDC header THT 2x07 2.54mm double row
0
16
15
Connector_IDC
IDC-Header_2x07-1MP_P2.54mm_Latch_Vertical
Through hole IDC header, 2x07, 2.54mm pitch, DIN 41651 / IEC 60603-13, double rows latches, mounting holes, https://docs.google.com/spreadsheets/d/16SsEcesNF15N3Lb4niX7dcUr-NY5_MFPQhobNuNppn4/edit#gid=0
Through hole vertical IDC header THT 2x07 2.54mm double row
0
16
15
Connector_IDC
IDC-Header_2x07_P2.54mm_Horizontal
Through hole IDC box header, 2x07, 2.54mm pitch, DIN 41651 / IEC 60603-13, double rows, https://docs.google.com/spreadsheets/d/16SsEcesNF15N3Lb4niX7dcUr-NY5_MFPQhobNuNppn4/edit#gid=0
Through hole horizontal IDC box header THT 2x07 2.54mm double row
0
14
14
Connector_IDC
IDC-Header_2x07_P2.54mm_Horizontal_Lock
Connector IDC Locked, 10 contacts, compatible header: PANCON HE10 (Series 50, (https://www.reboul.fr/storage/00003af6.pdf)
connector idc locked
0
16
14
Connector_IDC
IDC-Header_2x07_P2.54mm_Latch6.5mm_Vertical
Through hole IDC header, 2x07, 2.54mm pitch, DIN 41651 / IEC 60603-13, double rows, 6.5mm latches, https://docs.google.com/spreadsheets/d/16SsEcesNF15N3Lb4niX7dcUr-NY5_MFPQhobNuNppn4/edit#gid=0
Through hole vertical IDC header THT 2x07 2.54mm double row
0
14
14
Connector_IDC
IDC-Header_2x07_P2.54mm_Latch9.5mm_Vertical
Through hole IDC header, 2x07, 2.54mm pitch, DIN 41651 / IEC 60603-13, double rows, 9.5mm latches, https://docs.google.com/spreadsheets/d/16SsEcesNF15N3Lb4niX7dcUr-NY5_MFPQhobNuNppn4/edit#gid=0
Through hole vertical IDC header THT 2x07 2.54mm double row
0
14
14
Connector_IDC
IDC-Header_2x07_P2.54mm_Latch12.0mm_Vertical
Through hole IDC header, 2x07, 2.54mm pitch, DIN 41651 / IEC 60603-13, double rows, 12.0mm latches, https://docs.google.com/spreadsheets/d/16SsEcesNF15N3Lb4niX7dcUr-NY5_MFPQhobNuNppn4/edit#gid=0
Through hole vertical IDC header THT 2x07 2.54mm double row
0
14
14
Connector_IDC
IDC-Header_2x07_P2.54mm_Latch_Horizontal
Through hole IDC header, 2x07, 2.54mm pitch, DIN 41651 / IEC 60603-13, double rows latches, https://docs.google.com/spreadsheets/d/16SsEcesNF15N3Lb4niX7dcUr-NY5_MFPQhobNuNppn4/edit#gid=0
Through hole horizontal IDC header THT 2x07 2.54mm double row
0
14
14
Connector_IDC
IDC-Header_2x07_P2.54mm_Latch_Vertical
Through hole IDC header, 2x07, 2.54mm pitch, DIN 41651 / IEC 60603-13, double rows latches, https://docs.google.com/spreadsheets/d/16SsEcesNF15N3Lb4niX7dcUr-NY5_MFPQhobNuNppn4/edit#gid=0
Through hole vertical IDC header THT 2x07 2.54mm double row
0
14
14
Connector_IDC
IDC-Header_2x07_P2.54mm_Vertical
Through hole IDC box header, 2x07, 2.54mm pitch, DIN 41651 / IEC 60603-13, double rows, https://docs.google.com/spreadsheets/d/16SsEcesNF15N3Lb4niX7dcUr-NY5_MFPQhobNuNppn4/edit#gid=0
Through hole vertical IDC box header THT 2x07 2.54mm double row
0
14
14
Connector_IDC
IDC-Header_2x08-1MP_P2.54mm_Latch6.5mm_Vertical
Through hole IDC header, 2x08, 2.54mm pitch, DIN 41651 / IEC 60603-13, double rows, 6.5mm latches, mounting holes, https://docs.google.com/spreadsheets/d/16SsEcesNF15N3Lb4niX7dcUr-NY5_MFPQhobNuNppn4/edit#gid=0
Through hole vertical IDC header THT 2x08 2.54mm double row
0
18
17
Connector_IDC
IDC-Header_2x08-1MP_P2.54mm_Latch9.5mm_Vertical
Through hole IDC header, 2x08, 2.54mm pitch, DIN 41651 / IEC 60603-13, double rows, 9.5mm latches, mounting holes, https://docs.google.com/spreadsheets/d/16SsEcesNF15N3Lb4niX7dcUr-NY5_MFPQhobNuNppn4/edit#gid=0
Through hole vertical IDC header THT 2x08 2.54mm double row
0
18
17
Connector_IDC
IDC-Header_2x08-1MP_P2.54mm_Latch12.0mm_Vertical
Through hole IDC header, 2x08, 2.54mm pitch, DIN 41651 / IEC 60603-13, double rows, 12.0mm latches, mounting holes, https://docs.google.com/spreadsheets/d/16SsEcesNF15N3Lb4niX7dcUr-NY5_MFPQhobNuNppn4/edit#gid=0
Through hole vertical IDC header THT 2x08 2.54mm double row
0
18
17
Connector_IDC
IDC-Header_2x08-1MP_P2.54mm_Latch_Horizontal
Through hole IDC header, 2x08, 2.54mm pitch, DIN 41651 / IEC 60603-13, double rows latches, mounting holes, https://docs.google.com/spreadsheets/d/16SsEcesNF15N3Lb4niX7dcUr-NY5_MFPQhobNuNppn4/edit#gid=0
Through hole horizontal IDC header THT 2x08 2.54mm double row
0
18
17
Connector_IDC
IDC-Header_2x08-1MP_P2.54mm_Latch_Vertical
Through hole IDC header, 2x08, 2.54mm pitch, DIN 41651 / IEC 60603-13, double rows latches, mounting holes, https://docs.google.com/spreadsheets/d/16SsEcesNF15N3Lb4niX7dcUr-NY5_MFPQhobNuNppn4/edit#gid=0
Through hole vertical IDC header THT 2x08 2.54mm double row
0
18
17
Connector_IDC
IDC-Header_2x08_P2.54mm_Horizontal
Through hole IDC box header, 2x08, 2.54mm pitch, DIN 41651 / IEC 60603-13, double rows, https://docs.google.com/spreadsheets/d/16SsEcesNF15N3Lb4niX7dcUr-NY5_MFPQhobNuNppn4/edit#gid=0
Through hole horizontal IDC box header THT 2x08 2.54mm double row
0
16
16
Connector_IDC
IDC-Header_2x08_P2.54mm_Latch6.5mm_Vertical
Through hole IDC header, 2x08, 2.54mm pitch, DIN 41651 / IEC 60603-13, double rows, 6.5mm latches, https://docs.google.com/spreadsheets/d/16SsEcesNF15N3Lb4niX7dcUr-NY5_MFPQhobNuNppn4/edit#gid=0
Through hole vertical IDC header THT 2x08 2.54mm double row
0
16
16
Connector_IDC
IDC-Header_2x08_P2.54mm_Latch9.5mm_Vertical
Through hole IDC header, 2x08, 2.54mm pitch, DIN 41651 / IEC 60603-13, double rows, 9.5mm latches, https://docs.google.com/spreadsheets/d/16SsEcesNF15N3Lb4niX7dcUr-NY5_MFPQhobNuNppn4/edit#gid=0
Through hole vertical IDC header THT 2x08 2.54mm double row
0
16
16
Connector_IDC
IDC-Header_2x08_P2.54mm_Latch12.0mm_Vertical
Through hole IDC header, 2x08, 2.54mm pitch, DIN 41651 / IEC 60603-13, double rows, 12.0mm latches, https://docs.google.com/spreadsheets/d/16SsEcesNF15N3Lb4niX7dcUr-NY5_MFPQhobNuNppn4/edit#gid=0
Through hole vertical IDC header THT 2x08 2.54mm double row
0
16
16
Connector_IDC
IDC-Header_2x08_P2.54mm_Latch_Horizontal
Through hole IDC header, 2x08, 2.54mm pitch, DIN 41651 / IEC 60603-13, double rows latches, https://docs.google.com/spreadsheets/d/16SsEcesNF15N3Lb4niX7dcUr-NY5_MFPQhobNuNppn4/edit#gid=0
Through hole horizontal IDC header THT 2x08 2.54mm double row
0
16
16
Connector_IDC
IDC-Header_2x08_P2.54mm_Latch_Vertical
Through hole IDC header, 2x08, 2.54mm pitch, DIN 41651 / IEC 60603-13, double rows latches, https://docs.google.com/spreadsheets/d/16SsEcesNF15N3Lb4niX7dcUr-NY5_MFPQhobNuNppn4/edit#gid=0
Through hole vertical IDC header THT 2x08 2.54mm double row
0
16
16
Connector_IDC
IDC-Header_2x08_P2.54mm_Vertical
Through hole IDC box header, 2x08, 2.54mm pitch, DIN 41651 / IEC 60603-13, double rows, https://docs.google.com/spreadsheets/d/16SsEcesNF15N3Lb4niX7dcUr-NY5_MFPQhobNuNppn4/edit#gid=0
Through hole vertical IDC box header THT 2x08 2.54mm double row
0
16
16
Connector_IDC
IDC-Header_2x10-1MP_P2.54mm_Latch6.5mm_Vertical
Through hole IDC header, 2x10, 2.54mm pitch, DIN 41651 / IEC 60603-13, double rows, 6.5mm latches, mounting holes, https://docs.google.com/spreadsheets/d/16SsEcesNF15N3Lb4niX7dcUr-NY5_MFPQhobNuNppn4/edit#gid=0
Through hole vertical IDC header THT 2x10 2.54mm double row
0
22
21
Connector_IDC
IDC-Header_2x10-1MP_P2.54mm_Latch9.5mm_Vertical
Through hole IDC header, 2x10, 2.54mm pitch, DIN 41651 / IEC 60603-13, double rows, 9.5mm latches, mounting holes, https://docs.google.com/spreadsheets/d/16SsEcesNF15N3Lb4niX7dcUr-NY5_MFPQhobNuNppn4/edit#gid=0
Through hole vertical IDC header THT 2x10 2.54mm double row
0
22
21
Connector_IDC
IDC-Header_2x10-1MP_P2.54mm_Latch12.0mm_Vertical
Through hole IDC header, 2x10, 2.54mm pitch, DIN 41651 / IEC 60603-13, double rows, 12.0mm latches, mounting holes, https://docs.google.com/spreadsheets/d/16SsEcesNF15N3Lb4niX7dcUr-NY5_MFPQhobNuNppn4/edit#gid=0
Through hole vertical IDC header THT 2x10 2.54mm double row
0
22
21
Connector_IDC
IDC-Header_2x10-1MP_P2.54mm_Latch_Horizontal
Through hole IDC header, 2x10, 2.54mm pitch, DIN 41651 / IEC 60603-13, double rows latches, mounting holes, https://docs.google.com/spreadsheets/d/16SsEcesNF15N3Lb4niX7dcUr-NY5_MFPQhobNuNppn4/edit#gid=0
Through hole horizontal IDC header THT 2x10 2.54mm double row
0
22
21
Connector_IDC
IDC-Header_2x10-1MP_P2.54mm_Latch_Vertical
Through hole IDC header, 2x10, 2.54mm pitch, DIN 41651 / IEC 60603-13, double rows latches, mounting holes, https://docs.google.com/spreadsheets/d/16SsEcesNF15N3Lb4niX7dcUr-NY5_MFPQhobNuNppn4/edit#gid=0
Through hole vertical IDC header THT 2x10 2.54mm double row
0
22
21
Connector_IDC
IDC-Header_2x10_P2.54mm_Horizontal
Through hole IDC box header, 2x10, 2.54mm pitch, DIN 41651 / IEC 60603-13, double rows, https://docs.google.com/spreadsheets/d/16SsEcesNF15N3Lb4niX7dcUr-NY5_MFPQhobNuNppn4/edit#gid=0
Through hole horizontal IDC box header THT 2x10 2.54mm double row
0
20
20
Connector_IDC
IDC-Header_2x10_P2.54mm_Latch6.5mm_Vertical
Through hole IDC header, 2x10, 2.54mm pitch, DIN 41651 / IEC 60603-13, double rows, 6.5mm latches, https://docs.google.com/spreadsheets/d/16SsEcesNF15N3Lb4niX7dcUr-NY5_MFPQhobNuNppn4/edit#gid=0
Through hole vertical IDC header THT 2x10 2.54mm double row
0
20
20
Connector_IDC
IDC-Header_2x10_P2.54mm_Latch9.5mm_Vertical
Through hole IDC header, 2x10, 2.54mm pitch, DIN 41651 / IEC 60603-13, double rows, 9.5mm latches, https://docs.google.com/spreadsheets/d/16SsEcesNF15N3Lb4niX7dcUr-NY5_MFPQhobNuNppn4/edit#gid=0
Through hole vertical IDC header THT 2x10 2.54mm double row
0
20
20
Connector_IDC
IDC-Header_2x10_P2.54mm_Latch12.0mm_Vertical
Through hole IDC header, 2x10, 2.54mm pitch, DIN 41651 / IEC 60603-13, double rows, 12.0mm latches, https://docs.google.com/spreadsheets/d/16SsEcesNF15N3Lb4niX7dcUr-NY5_MFPQhobNuNppn4/edit#gid=0
Through hole vertical IDC header THT 2x10 2.54mm double row
0
20
20
Connector_IDC
IDC-Header_2x10_P2.54mm_Latch_Horizontal
Through hole IDC header, 2x10, 2.54mm pitch, DIN 41651 / IEC 60603-13, double rows latches, https://docs.google.com/spreadsheets/d/16SsEcesNF15N3Lb4niX7dcUr-NY5_MFPQhobNuNppn4/edit#gid=0
Through hole horizontal IDC header THT 2x10 2.54mm double row
0
20
20
Connector_IDC
IDC-Header_2x10_P2.54mm_Latch_Vertical
Through hole IDC header, 2x10, 2.54mm pitch, DIN 41651 / IEC 60603-13, double rows latches, https://docs.google.com/spreadsheets/d/16SsEcesNF15N3Lb4niX7dcUr-NY5_MFPQhobNuNppn4/edit#gid=0
Through hole vertical IDC header THT 2x10 2.54mm double row
0
20
20
Connector_IDC
IDC-Header_2x10_P2.54mm_Vertical
Through hole IDC box header, 2x10, 2.54mm pitch, DIN 41651 / IEC 60603-13, double rows, https://docs.google.com/spreadsheets/d/16SsEcesNF15N3Lb4niX7dcUr-NY5_MFPQhobNuNppn4/edit#gid=0
Through hole vertical IDC box header THT 2x10 2.54mm double row
0
20
20
Connector_IDC
IDC-Header_2x12-1MP_P2.54mm_Latch6.5mm_Vertical
Through hole IDC header, 2x12, 2.54mm pitch, DIN 41651 / IEC 60603-13, double rows, 6.5mm latches, mounting holes, https://docs.google.com/spreadsheets/d/16SsEcesNF15N3Lb4niX7dcUr-NY5_MFPQhobNuNppn4/edit#gid=0
Through hole vertical IDC header THT 2x12 2.54mm double row
0
26
25
Connector_IDC
IDC-Header_2x12-1MP_P2.54mm_Latch9.5mm_Vertical
Through hole IDC header, 2x12, 2.54mm pitch, DIN 41651 / IEC 60603-13, double rows, 9.5mm latches, mounting holes, https://docs.google.com/spreadsheets/d/16SsEcesNF15N3Lb4niX7dcUr-NY5_MFPQhobNuNppn4/edit#gid=0
Through hole vertical IDC header THT 2x12 2.54mm double row
0
26
25
Connector_IDC
IDC-Header_2x12-1MP_P2.54mm_Latch12.0mm_Vertical
Through hole IDC header, 2x12, 2.54mm pitch, DIN 41651 / IEC 60603-13, double rows, 12.0mm latches, mounting holes, https://docs.google.com/spreadsheets/d/16SsEcesNF15N3Lb4niX7dcUr-NY5_MFPQhobNuNppn4/edit#gid=0
Through hole vertical IDC header THT 2x12 2.54mm double row
0
26
25
Connector_IDC
IDC-Header_2x12-1MP_P2.54mm_Latch_Horizontal
Through hole IDC header, 2x12, 2.54mm pitch, DIN 41651 / IEC 60603-13, double rows latches, mounting holes, https://docs.google.com/spreadsheets/d/16SsEcesNF15N3Lb4niX7dcUr-NY5_MFPQhobNuNppn4/edit#gid=0
Through hole horizontal IDC header THT 2x12 2.54mm double row
0
26
25
Connector_IDC
IDC-Header_2x12-1MP_P2.54mm_Latch_Vertical
Through hole IDC header, 2x12, 2.54mm pitch, DIN 41651 / IEC 60603-13, double rows latches, mounting holes, https://docs.google.com/spreadsheets/d/16SsEcesNF15N3Lb4niX7dcUr-NY5_MFPQhobNuNppn4/edit#gid=0
Through hole vertical IDC header THT 2x12 2.54mm double row
0
26
25
Connector_IDC
IDC-Header_2x12_P2.54mm_Horizontal
Through hole IDC box header, 2x12, 2.54mm pitch, DIN 41651 / IEC 60603-13, double rows, https://docs.google.com/spreadsheets/d/16SsEcesNF15N3Lb4niX7dcUr-NY5_MFPQhobNuNppn4/edit#gid=0
Through hole horizontal IDC box header THT 2x12 2.54mm double row
0
24
24
Connector_IDC
IDC-Header_2x12_P2.54mm_Latch6.5mm_Vertical
Through hole IDC header, 2x12, 2.54mm pitch, DIN 41651 / IEC 60603-13, double rows, 6.5mm latches, https://docs.google.com/spreadsheets/d/16SsEcesNF15N3Lb4niX7dcUr-NY5_MFPQhobNuNppn4/edit#gid=0
Through hole vertical IDC header THT 2x12 2.54mm double row
0
24
24
Connector_IDC
IDC-Header_2x12_P2.54mm_Latch9.5mm_Vertical
Through hole IDC header, 2x12, 2.54mm pitch, DIN 41651 / IEC 60603-13, double rows, 9.5mm latches, https://docs.google.com/spreadsheets/d/16SsEcesNF15N3Lb4niX7dcUr-NY5_MFPQhobNuNppn4/edit#gid=0
Through hole vertical IDC header THT 2x12 2.54mm double row
0
24
24
Connector_IDC
IDC-Header_2x12_P2.54mm_Latch12.0mm_Vertical
Through hole IDC header, 2x12, 2.54mm pitch, DIN 41651 / IEC 60603-13, double rows, 12.0mm latches, https://docs.google.com/spreadsheets/d/16SsEcesNF15N3Lb4niX7dcUr-NY5_MFPQhobNuNppn4/edit#gid=0
Through hole vertical IDC header THT 2x12 2.54mm double row
0
24
24
Connector_IDC
IDC-Header_2x12_P2.54mm_Latch_Horizontal
Through hole IDC header, 2x12, 2.54mm pitch, DIN 41651 / IEC 60603-13, double rows latches, https://docs.google.com/spreadsheets/d/16SsEcesNF15N3Lb4niX7dcUr-NY5_MFPQhobNuNppn4/edit#gid=0
Through hole horizontal IDC header THT 2x12 2.54mm double row
0
24
24
Connector_IDC
IDC-Header_2x12_P2.54mm_Latch_Vertical
Through hole IDC header, 2x12, 2.54mm pitch, DIN 41651 / IEC 60603-13, double rows latches, https://docs.google.com/spreadsheets/d/16SsEcesNF15N3Lb4niX7dcUr-NY5_MFPQhobNuNppn4/edit#gid=0
Through hole vertical IDC header THT 2x12 2.54mm double row
0
24
24
Connector_IDC
IDC-Header_2x12_P2.54mm_Vertical
Through hole IDC box header, 2x12, 2.54mm pitch, DIN 41651 / IEC 60603-13, double rows, https://docs.google.com/spreadsheets/d/16SsEcesNF15N3Lb4niX7dcUr-NY5_MFPQhobNuNppn4/edit#gid=0
Through hole vertical IDC box header THT 2x12 2.54mm double row
0
24
24
Connector_IDC
IDC-Header_2x13-1MP_P2.54mm_Latch6.5mm_Vertical
Through hole IDC header, 2x13, 2.54mm pitch, DIN 41651 / IEC 60603-13, double rows, 6.5mm latches, mounting holes, https://docs.google.com/spreadsheets/d/16SsEcesNF15N3Lb4niX7dcUr-NY5_MFPQhobNuNppn4/edit#gid=0
Through hole vertical IDC header THT 2x13 2.54mm double row
0
28
27
Connector_IDC
IDC-Header_2x13-1MP_P2.54mm_Latch9.5mm_Vertical
Through hole IDC header, 2x13, 2.54mm pitch, DIN 41651 / IEC 60603-13, double rows, 9.5mm latches, mounting holes, https://docs.google.com/spreadsheets/d/16SsEcesNF15N3Lb4niX7dcUr-NY5_MFPQhobNuNppn4/edit#gid=0
Through hole vertical IDC header THT 2x13 2.54mm double row
0
28
27
Connector_IDC
IDC-Header_2x13-1MP_P2.54mm_Latch12.0mm_Vertical
Through hole IDC header, 2x13, 2.54mm pitch, DIN 41651 / IEC 60603-13, double rows, 12.0mm latches, mounting holes, https://docs.google.com/spreadsheets/d/16SsEcesNF15N3Lb4niX7dcUr-NY5_MFPQhobNuNppn4/edit#gid=0
Through hole vertical IDC header THT 2x13 2.54mm double row
0
28
27
Connector_IDC
IDC-Header_2x13-1MP_P2.54mm_Latch_Horizontal
Through hole IDC header, 2x13, 2.54mm pitch, DIN 41651 / IEC 60603-13, double rows latches, mounting holes, https://docs.google.com/spreadsheets/d/16SsEcesNF15N3Lb4niX7dcUr-NY5_MFPQhobNuNppn4/edit#gid=0
Through hole horizontal IDC header THT 2x13 2.54mm double row
0
28
27
Connector_IDC
IDC-Header_2x13-1MP_P2.54mm_Latch_Vertical
Through hole IDC header, 2x13, 2.54mm pitch, DIN 41651 / IEC 60603-13, double rows latches, mounting holes, https://docs.google.com/spreadsheets/d/16SsEcesNF15N3Lb4niX7dcUr-NY5_MFPQhobNuNppn4/edit#gid=0
Through hole vertical IDC header THT 2x13 2.54mm double row
0
28
27
Connector_IDC
IDC-Header_2x13_P2.54mm_Horizontal
Through hole IDC box header, 2x13, 2.54mm pitch, DIN 41651 / IEC 60603-13, double rows, https://docs.google.com/spreadsheets/d/16SsEcesNF15N3Lb4niX7dcUr-NY5_MFPQhobNuNppn4/edit#gid=0
Through hole horizontal IDC box header THT 2x13 2.54mm double row
0
26
26
Connector_IDC
IDC-Header_2x13_P2.54mm_Latch6.5mm_Vertical
Through hole IDC header, 2x13, 2.54mm pitch, DIN 41651 / IEC 60603-13, double rows, 6.5mm latches, https://docs.google.com/spreadsheets/d/16SsEcesNF15N3Lb4niX7dcUr-NY5_MFPQhobNuNppn4/edit#gid=0
Through hole vertical IDC header THT 2x13 2.54mm double row
0
26
26
Connector_IDC
IDC-Header_2x13_P2.54mm_Latch9.5mm_Vertical
Through hole IDC header, 2x13, 2.54mm pitch, DIN 41651 / IEC 60603-13, double rows, 9.5mm latches, https://docs.google.com/spreadsheets/d/16SsEcesNF15N3Lb4niX7dcUr-NY5_MFPQhobNuNppn4/edit#gid=0
Through hole vertical IDC header THT 2x13 2.54mm double row
0
26
26
Connector_IDC
IDC-Header_2x13_P2.54mm_Latch12.0mm_Vertical
Through hole IDC header, 2x13, 2.54mm pitch, DIN 41651 / IEC 60603-13, double rows, 12.0mm latches, https://docs.google.com/spreadsheets/d/16SsEcesNF15N3Lb4niX7dcUr-NY5_MFPQhobNuNppn4/edit#gid=0
Through hole vertical IDC header THT 2x13 2.54mm double row
0
26
26
Connector_IDC
IDC-Header_2x13_P2.54mm_Latch_Horizontal
Through hole IDC header, 2x13, 2.54mm pitch, DIN 41651 / IEC 60603-13, double rows latches, https://docs.google.com/spreadsheets/d/16SsEcesNF15N3Lb4niX7dcUr-NY5_MFPQhobNuNppn4/edit#gid=0
Through hole horizontal IDC header THT 2x13 2.54mm double row
0
26
26
Connector_IDC
IDC-Header_2x13_P2.54mm_Latch_Vertical
Through hole IDC header, 2x13, 2.54mm pitch, DIN 41651 / IEC 60603-13, double rows latches, https://docs.google.com/spreadsheets/d/16SsEcesNF15N3Lb4niX7dcUr-NY5_MFPQhobNuNppn4/edit#gid=0
Through hole vertical IDC header THT 2x13 2.54mm double row
0
26
26
Connector_IDC
IDC-Header_2x13_P2.54mm_Vertical
Through hole IDC box header, 2x13, 2.54mm pitch, DIN 41651 / IEC 60603-13, double rows, https://docs.google.com/spreadsheets/d/16SsEcesNF15N3Lb4niX7dcUr-NY5_MFPQhobNuNppn4/edit#gid=0
Through hole vertical IDC box header THT 2x13 2.54mm double row
0
26
26
Connector_IDC
IDC-Header_2x15-1MP_P2.54mm_Latch6.5mm_Vertical
Through hole IDC header, 2x15, 2.54mm pitch, DIN 41651 / IEC 60603-13, double rows, 6.5mm latches, mounting holes, https://docs.google.com/spreadsheets/d/16SsEcesNF15N3Lb4niX7dcUr-NY5_MFPQhobNuNppn4/edit#gid=0
Through hole vertical IDC header THT 2x15 2.54mm double row
0
32
31
Connector_IDC
IDC-Header_2x15-1MP_P2.54mm_Latch9.5mm_Vertical
Through hole IDC header, 2x15, 2.54mm pitch, DIN 41651 / IEC 60603-13, double rows, 9.5mm latches, mounting holes, https://docs.google.com/spreadsheets/d/16SsEcesNF15N3Lb4niX7dcUr-NY5_MFPQhobNuNppn4/edit#gid=0
Through hole vertical IDC header THT 2x15 2.54mm double row
0
32
31
Connector_IDC
IDC-Header_2x15-1MP_P2.54mm_Latch12.0mm_Vertical
Through hole IDC header, 2x15, 2.54mm pitch, DIN 41651 / IEC 60603-13, double rows, 12.0mm latches, mounting holes, https://docs.google.com/spreadsheets/d/16SsEcesNF15N3Lb4niX7dcUr-NY5_MFPQhobNuNppn4/edit#gid=0
Through hole vertical IDC header THT 2x15 2.54mm double row
0
32
31
Connector_IDC
IDC-Header_2x15-1MP_P2.54mm_Latch_Horizontal
Through hole IDC header, 2x15, 2.54mm pitch, DIN 41651 / IEC 60603-13, double rows latches, mounting holes, https://docs.google.com/spreadsheets/d/16SsEcesNF15N3Lb4niX7dcUr-NY5_MFPQhobNuNppn4/edit#gid=0
Through hole horizontal IDC header THT 2x15 2.54mm double row
0
32
31
Connector_IDC
IDC-Header_2x15-1MP_P2.54mm_Latch_Vertical
Through hole IDC header, 2x15, 2.54mm pitch, DIN 41651 / IEC 60603-13, double rows latches, mounting holes, https://docs.google.com/spreadsheets/d/16SsEcesNF15N3Lb4niX7dcUr-NY5_MFPQhobNuNppn4/edit#gid=0
Through hole vertical IDC header THT 2x15 2.54mm double row
0
32
31
Connector_IDC
IDC-Header_2x15_P2.54mm_Horizontal
Through hole IDC box header, 2x15, 2.54mm pitch, DIN 41651 / IEC 60603-13, double rows, https://docs.google.com/spreadsheets/d/16SsEcesNF15N3Lb4niX7dcUr-NY5_MFPQhobNuNppn4/edit#gid=0
Through hole horizontal IDC box header THT 2x15 2.54mm double row
0
30
30
Connector_IDC
IDC-Header_2x15_P2.54mm_Latch6.5mm_Vertical
Through hole IDC header, 2x15, 2.54mm pitch, DIN 41651 / IEC 60603-13, double rows, 6.5mm latches, https://docs.google.com/spreadsheets/d/16SsEcesNF15N3Lb4niX7dcUr-NY5_MFPQhobNuNppn4/edit#gid=0
Through hole vertical IDC header THT 2x15 2.54mm double row
0
30
30
Connector_IDC
IDC-Header_2x15_P2.54mm_Latch9.5mm_Vertical
Through hole IDC header, 2x15, 2.54mm pitch, DIN 41651 / IEC 60603-13, double rows, 9.5mm latches, https://docs.google.com/spreadsheets/d/16SsEcesNF15N3Lb4niX7dcUr-NY5_MFPQhobNuNppn4/edit#gid=0
Through hole vertical IDC header THT 2x15 2.54mm double row
0
30
30
Connector_IDC
IDC-Header_2x15_P2.54mm_Latch12.0mm_Vertical
Through hole IDC header, 2x15, 2.54mm pitch, DIN 41651 / IEC 60603-13, double rows, 12.0mm latches, https://docs.google.com/spreadsheets/d/16SsEcesNF15N3Lb4niX7dcUr-NY5_MFPQhobNuNppn4/edit#gid=0
Through hole vertical IDC header THT 2x15 2.54mm double row
0
30
30
Connector_IDC
IDC-Header_2x15_P2.54mm_Latch_Horizontal
Through hole IDC header, 2x15, 2.54mm pitch, DIN 41651 / IEC 60603-13, double rows latches, https://docs.google.com/spreadsheets/d/16SsEcesNF15N3Lb4niX7dcUr-NY5_MFPQhobNuNppn4/edit#gid=0
Through hole horizontal IDC header THT 2x15 2.54mm double row
0
30
30
Connector_IDC
IDC-Header_2x15_P2.54mm_Latch_Vertical
Through hole IDC header, 2x15, 2.54mm pitch, DIN 41651 / IEC 60603-13, double rows latches, https://docs.google.com/spreadsheets/d/16SsEcesNF15N3Lb4niX7dcUr-NY5_MFPQhobNuNppn4/edit#gid=0
Through hole vertical IDC header THT 2x15 2.54mm double row
0
30
30
Connector_IDC
IDC-Header_2x15_P2.54mm_Vertical
Through hole IDC box header, 2x15, 2.54mm pitch, DIN 41651 / IEC 60603-13, double rows, https://docs.google.com/spreadsheets/d/16SsEcesNF15N3Lb4niX7dcUr-NY5_MFPQhobNuNppn4/edit#gid=0
Through hole vertical IDC box header THT 2x15 2.54mm double row
0
30
30
Connector_IDC
IDC-Header_2x17-1MP_P2.54mm_Latch6.5mm_Vertical
Through hole IDC header, 2x17, 2.54mm pitch, DIN 41651 / IEC 60603-13, double rows, 6.5mm latches, mounting holes, https://docs.google.com/spreadsheets/d/16SsEcesNF15N3Lb4niX7dcUr-NY5_MFPQhobNuNppn4/edit#gid=0
Through hole vertical IDC header THT 2x17 2.54mm double row
0
36
35
Connector_IDC
IDC-Header_2x17-1MP_P2.54mm_Latch9.5mm_Vertical
Through hole IDC header, 2x17, 2.54mm pitch, DIN 41651 / IEC 60603-13, double rows, 9.5mm latches, mounting holes, https://docs.google.com/spreadsheets/d/16SsEcesNF15N3Lb4niX7dcUr-NY5_MFPQhobNuNppn4/edit#gid=0
Through hole vertical IDC header THT 2x17 2.54mm double row
0
36
35
Connector_IDC
IDC-Header_2x17-1MP_P2.54mm_Latch12.0mm_Vertical
Through hole IDC header, 2x17, 2.54mm pitch, DIN 41651 / IEC 60603-13, double rows, 12.0mm latches, mounting holes, https://docs.google.com/spreadsheets/d/16SsEcesNF15N3Lb4niX7dcUr-NY5_MFPQhobNuNppn4/edit#gid=0
Through hole vertical IDC header THT 2x17 2.54mm double row
0
36
35
Connector_IDC
IDC-Header_2x17-1MP_P2.54mm_Latch_Horizontal
Through hole IDC header, 2x17, 2.54mm pitch, DIN 41651 / IEC 60603-13, double rows latches, mounting holes, https://docs.google.com/spreadsheets/d/16SsEcesNF15N3Lb4niX7dcUr-NY5_MFPQhobNuNppn4/edit#gid=0
Through hole horizontal IDC header THT 2x17 2.54mm double row
0
36
35
Connector_IDC
IDC-Header_2x17-1MP_P2.54mm_Latch_Vertical
Through hole IDC header, 2x17, 2.54mm pitch, DIN 41651 / IEC 60603-13, double rows latches, mounting holes, https://docs.google.com/spreadsheets/d/16SsEcesNF15N3Lb4niX7dcUr-NY5_MFPQhobNuNppn4/edit#gid=0
Through hole vertical IDC header THT 2x17 2.54mm double row
0
36
35
Connector_IDC
IDC-Header_2x17_P2.54mm_Horizontal
Through hole IDC box header, 2x17, 2.54mm pitch, DIN 41651 / IEC 60603-13, double rows, https://docs.google.com/spreadsheets/d/16SsEcesNF15N3Lb4niX7dcUr-NY5_MFPQhobNuNppn4/edit#gid=0
Through hole horizontal IDC box header THT 2x17 2.54mm double row
0
34
34
Connector_IDC
IDC-Header_2x17_P2.54mm_Latch6.5mm_Vertical
Through hole IDC header, 2x17, 2.54mm pitch, DIN 41651 / IEC 60603-13, double rows, 6.5mm latches, https://docs.google.com/spreadsheets/d/16SsEcesNF15N3Lb4niX7dcUr-NY5_MFPQhobNuNppn4/edit#gid=0
Through hole vertical IDC header THT 2x17 2.54mm double row
0
34
34
Connector_IDC
IDC-Header_2x17_P2.54mm_Latch9.5mm_Vertical
Through hole IDC header, 2x17, 2.54mm pitch, DIN 41651 / IEC 60603-13, double rows, 9.5mm latches, https://docs.google.com/spreadsheets/d/16SsEcesNF15N3Lb4niX7dcUr-NY5_MFPQhobNuNppn4/edit#gid=0
Through hole vertical IDC header THT 2x17 2.54mm double row
0
34
34
Connector_IDC
IDC-Header_2x17_P2.54mm_Latch12.0mm_Vertical
Through hole IDC header, 2x17, 2.54mm pitch, DIN 41651 / IEC 60603-13, double rows, 12.0mm latches, https://docs.google.com/spreadsheets/d/16SsEcesNF15N3Lb4niX7dcUr-NY5_MFPQhobNuNppn4/edit#gid=0
Through hole vertical IDC header THT 2x17 2.54mm double row
0
34
34
Connector_IDC
IDC-Header_2x17_P2.54mm_Latch_Horizontal
Through hole IDC header, 2x17, 2.54mm pitch, DIN 41651 / IEC 60603-13, double rows latches, https://docs.google.com/spreadsheets/d/16SsEcesNF15N3Lb4niX7dcUr-NY5_MFPQhobNuNppn4/edit#gid=0
Through hole horizontal IDC header THT 2x17 2.54mm double row
0
34
34
Connector_IDC
IDC-Header_2x17_P2.54mm_Latch_Vertical
Through hole IDC header, 2x17, 2.54mm pitch, DIN 41651 / IEC 60603-13, double rows latches, https://docs.google.com/spreadsheets/d/16SsEcesNF15N3Lb4niX7dcUr-NY5_MFPQhobNuNppn4/edit#gid=0
Through hole vertical IDC header THT 2x17 2.54mm double row
0
34
34
Connector_IDC
IDC-Header_2x17_P2.54mm_Vertical
Through hole IDC box header, 2x17, 2.54mm pitch, DIN 41651 / IEC 60603-13, double rows, https://docs.google.com/spreadsheets/d/16SsEcesNF15N3Lb4niX7dcUr-NY5_MFPQhobNuNppn4/edit#gid=0
Through hole vertical IDC box header THT 2x17 2.54mm double row
0
34
34
Connector_IDC
IDC-Header_2x20-1MP_P2.54mm_Latch6.5mm_Vertical
Through hole IDC header, 2x20, 2.54mm pitch, DIN 41651 / IEC 60603-13, double rows, 6.5mm latches, mounting holes, https://docs.google.com/spreadsheets/d/16SsEcesNF15N3Lb4niX7dcUr-NY5_MFPQhobNuNppn4/edit#gid=0
Through hole vertical IDC header THT 2x20 2.54mm double row
0
42
41
Connector_IDC
IDC-Header_2x20-1MP_P2.54mm_Latch9.5mm_Vertical
Through hole IDC header, 2x20, 2.54mm pitch, DIN 41651 / IEC 60603-13, double rows, 9.5mm latches, mounting holes, https://docs.google.com/spreadsheets/d/16SsEcesNF15N3Lb4niX7dcUr-NY5_MFPQhobNuNppn4/edit#gid=0
Through hole vertical IDC header THT 2x20 2.54mm double row
0
42
41
Connector_IDC
IDC-Header_2x20-1MP_P2.54mm_Latch12.0mm_Vertical
Through hole IDC header, 2x20, 2.54mm pitch, DIN 41651 / IEC 60603-13, double rows, 12.0mm latches, mounting holes, https://docs.google.com/spreadsheets/d/16SsEcesNF15N3Lb4niX7dcUr-NY5_MFPQhobNuNppn4/edit#gid=0
Through hole vertical IDC header THT 2x20 2.54mm double row
0
42
41
Connector_IDC
IDC-Header_2x20-1MP_P2.54mm_Latch_Horizontal
Through hole IDC header, 2x20, 2.54mm pitch, DIN 41651 / IEC 60603-13, double rows latches, mounting holes, https://docs.google.com/spreadsheets/d/16SsEcesNF15N3Lb4niX7dcUr-NY5_MFPQhobNuNppn4/edit#gid=0
Through hole horizontal IDC header THT 2x20 2.54mm double row
0
42
41
Connector_IDC
IDC-Header_2x20-1MP_P2.54mm_Latch_Vertical
Through hole IDC header, 2x20, 2.54mm pitch, DIN 41651 / IEC 60603-13, double rows latches, mounting holes, https://docs.google.com/spreadsheets/d/16SsEcesNF15N3Lb4niX7dcUr-NY5_MFPQhobNuNppn4/edit#gid=0
Through hole vertical IDC header THT 2x20 2.54mm double row
0
42
41
Connector_IDC
IDC-Header_2x20_P2.54mm_Horizontal
Through hole IDC box header, 2x20, 2.54mm pitch, DIN 41651 / IEC 60603-13, double rows, https://docs.google.com/spreadsheets/d/16SsEcesNF15N3Lb4niX7dcUr-NY5_MFPQhobNuNppn4/edit#gid=0
Through hole horizontal IDC box header THT 2x20 2.54mm double row
0
40
40
Connector_IDC
IDC-Header_2x20_P2.54mm_Latch6.5mm_Vertical
Through hole IDC header, 2x20, 2.54mm pitch, DIN 41651 / IEC 60603-13, double rows, 6.5mm latches, https://docs.google.com/spreadsheets/d/16SsEcesNF15N3Lb4niX7dcUr-NY5_MFPQhobNuNppn4/edit#gid=0
Through hole vertical IDC header THT 2x20 2.54mm double row
0
40
40
Connector_IDC
IDC-Header_2x20_P2.54mm_Latch9.5mm_Vertical
Through hole IDC header, 2x20, 2.54mm pitch, DIN 41651 / IEC 60603-13, double rows, 9.5mm latches, https://docs.google.com/spreadsheets/d/16SsEcesNF15N3Lb4niX7dcUr-NY5_MFPQhobNuNppn4/edit#gid=0
Through hole vertical IDC header THT 2x20 2.54mm double row
0
40
40
Connector_IDC
IDC-Header_2x20_P2.54mm_Latch12.0mm_Vertical
Through hole IDC header, 2x20, 2.54mm pitch, DIN 41651 / IEC 60603-13, double rows, 12.0mm latches, https://docs.google.com/spreadsheets/d/16SsEcesNF15N3Lb4niX7dcUr-NY5_MFPQhobNuNppn4/edit#gid=0
Through hole vertical IDC header THT 2x20 2.54mm double row
0
40
40
Connector_IDC
IDC-Header_2x20_P2.54mm_Latch_Horizontal
Through hole IDC header, 2x20, 2.54mm pitch, DIN 41651 / IEC 60603-13, double rows latches, https://docs.google.com/spreadsheets/d/16SsEcesNF15N3Lb4niX7dcUr-NY5_MFPQhobNuNppn4/edit#gid=0
Through hole horizontal IDC header THT 2x20 2.54mm double row
0
40
40
Connector_IDC
IDC-Header_2x20_P2.54mm_Latch_Vertical
Through hole IDC header, 2x20, 2.54mm pitch, DIN 41651 / IEC 60603-13, double rows latches, https://docs.google.com/spreadsheets/d/16SsEcesNF15N3Lb4niX7dcUr-NY5_MFPQhobNuNppn4/edit#gid=0
Through hole vertical IDC header THT 2x20 2.54mm double row
0
40
40
Connector_IDC
IDC-Header_2x20_P2.54mm_Vertical
Through hole IDC box header, 2x20, 2.54mm pitch, DIN 41651 / IEC 60603-13, double rows, https://docs.google.com/spreadsheets/d/16SsEcesNF15N3Lb4niX7dcUr-NY5_MFPQhobNuNppn4/edit#gid=0
Through hole vertical IDC box header THT 2x20 2.54mm double row
0
40
40
Connector_IDC
IDC-Header_2x25-1MP_P2.54mm_Latch6.5mm_Vertical
Through hole IDC header, 2x25, 2.54mm pitch, DIN 41651 / IEC 60603-13, double rows, 6.5mm latches, mounting holes, https://docs.google.com/spreadsheets/d/16SsEcesNF15N3Lb4niX7dcUr-NY5_MFPQhobNuNppn4/edit#gid=0
Through hole vertical IDC header THT 2x25 2.54mm double row
0
52
51
Connector_IDC
IDC-Header_2x25-1MP_P2.54mm_Latch9.5mm_Vertical
Through hole IDC header, 2x25, 2.54mm pitch, DIN 41651 / IEC 60603-13, double rows, 9.5mm latches, mounting holes, https://docs.google.com/spreadsheets/d/16SsEcesNF15N3Lb4niX7dcUr-NY5_MFPQhobNuNppn4/edit#gid=0
Through hole vertical IDC header THT 2x25 2.54mm double row
0
52
51
Connector_IDC
IDC-Header_2x25-1MP_P2.54mm_Latch12.0mm_Vertical
Through hole IDC header, 2x25, 2.54mm pitch, DIN 41651 / IEC 60603-13, double rows, 12.0mm latches, mounting holes, https://docs.google.com/spreadsheets/d/16SsEcesNF15N3Lb4niX7dcUr-NY5_MFPQhobNuNppn4/edit#gid=0
Through hole vertical IDC header THT 2x25 2.54mm double row
0
52
51
Connector_IDC
IDC-Header_2x25-1MP_P2.54mm_Latch_Horizontal
Through hole IDC header, 2x25, 2.54mm pitch, DIN 41651 / IEC 60603-13, double rows latches, mounting holes, https://docs.google.com/spreadsheets/d/16SsEcesNF15N3Lb4niX7dcUr-NY5_MFPQhobNuNppn4/edit#gid=0
Through hole horizontal IDC header THT 2x25 2.54mm double row
0
52
51
Connector_IDC
IDC-Header_2x25-1MP_P2.54mm_Latch_Vertical
Through hole IDC header, 2x25, 2.54mm pitch, DIN 41651 / IEC 60603-13, double rows latches, mounting holes, https://docs.google.com/spreadsheets/d/16SsEcesNF15N3Lb4niX7dcUr-NY5_MFPQhobNuNppn4/edit#gid=0
Through hole vertical IDC header THT 2x25 2.54mm double row
0
52
51
Connector_IDC
IDC-Header_2x25_P2.54mm_Horizontal
Through hole IDC box header, 2x25, 2.54mm pitch, DIN 41651 / IEC 60603-13, double rows, https://docs.google.com/spreadsheets/d/16SsEcesNF15N3Lb4niX7dcUr-NY5_MFPQhobNuNppn4/edit#gid=0
Through hole horizontal IDC box header THT 2x25 2.54mm double row
0
50
50
Connector_IDC
IDC-Header_2x25_P2.54mm_Latch6.5mm_Vertical
Through hole IDC header, 2x25, 2.54mm pitch, DIN 41651 / IEC 60603-13, double rows, 6.5mm latches, https://docs.google.com/spreadsheets/d/16SsEcesNF15N3Lb4niX7dcUr-NY5_MFPQhobNuNppn4/edit#gid=0
Through hole vertical IDC header THT 2x25 2.54mm double row
0
50
50
Connector_IDC
IDC-Header_2x25_P2.54mm_Latch9.5mm_Vertical
Through hole IDC header, 2x25, 2.54mm pitch, DIN 41651 / IEC 60603-13, double rows, 9.5mm latches, https://docs.google.com/spreadsheets/d/16SsEcesNF15N3Lb4niX7dcUr-NY5_MFPQhobNuNppn4/edit#gid=0
Through hole vertical IDC header THT 2x25 2.54mm double row
0
50
50
Connector_IDC
IDC-Header_2x25_P2.54mm_Latch12.0mm_Vertical
Through hole IDC header, 2x25, 2.54mm pitch, DIN 41651 / IEC 60603-13, double rows, 12.0mm latches, https://docs.google.com/spreadsheets/d/16SsEcesNF15N3Lb4niX7dcUr-NY5_MFPQhobNuNppn4/edit#gid=0
Through hole vertical IDC header THT 2x25 2.54mm double row
0
50
50
Connector_IDC
IDC-Header_2x25_P2.54mm_Latch_Horizontal
Through hole IDC header, 2x25, 2.54mm pitch, DIN 41651 / IEC 60603-13, double rows latches, https://docs.google.com/spreadsheets/d/16SsEcesNF15N3Lb4niX7dcUr-NY5_MFPQhobNuNppn4/edit#gid=0
Through hole horizontal IDC header THT 2x25 2.54mm double row
0
50
50
Connector_IDC
IDC-Header_2x25_P2.54mm_Latch_Vertical
Through hole IDC header, 2x25, 2.54mm pitch, DIN 41651 / IEC 60603-13, double rows latches, https://docs.google.com/spreadsheets/d/16SsEcesNF15N3Lb4niX7dcUr-NY5_MFPQhobNuNppn4/edit#gid=0
Through hole vertical IDC header THT 2x25 2.54mm double row
0
50
50
Connector_IDC
IDC-Header_2x25_P2.54mm_Vertical
Through hole IDC box header, 2x25, 2.54mm pitch, DIN 41651 / IEC 60603-13, double rows, https://docs.google.com/spreadsheets/d/16SsEcesNF15N3Lb4niX7dcUr-NY5_MFPQhobNuNppn4/edit#gid=0
Through hole vertical IDC box header THT 2x25 2.54mm double row
0
50
50
Connector_IDC
IDC-Header_2x30-1MP_P2.54mm_Latch6.5mm_Vertical
Through hole IDC header, 2x30, 2.54mm pitch, DIN 41651 / IEC 60603-13, double rows, 6.5mm latches, mounting holes, https://docs.google.com/spreadsheets/d/16SsEcesNF15N3Lb4niX7dcUr-NY5_MFPQhobNuNppn4/edit#gid=0
Through hole vertical IDC header THT 2x30 2.54mm double row
0
62
61
Connector_IDC
IDC-Header_2x30-1MP_P2.54mm_Latch9.5mm_Vertical
Through hole IDC header, 2x30, 2.54mm pitch, DIN 41651 / IEC 60603-13, double rows, 9.5mm latches, mounting holes, https://docs.google.com/spreadsheets/d/16SsEcesNF15N3Lb4niX7dcUr-NY5_MFPQhobNuNppn4/edit#gid=0
Through hole vertical IDC header THT 2x30 2.54mm double row
0
62
61
Connector_IDC
IDC-Header_2x30-1MP_P2.54mm_Latch12.0mm_Vertical
Through hole IDC header, 2x30, 2.54mm pitch, DIN 41651 / IEC 60603-13, double rows, 12.0mm latches, mounting holes, https://docs.google.com/spreadsheets/d/16SsEcesNF15N3Lb4niX7dcUr-NY5_MFPQhobNuNppn4/edit#gid=0
Through hole vertical IDC header THT 2x30 2.54mm double row
0
62
61
Connector_IDC
IDC-Header_2x30-1MP_P2.54mm_Latch_Horizontal
Through hole IDC header, 2x30, 2.54mm pitch, DIN 41651 / IEC 60603-13, double rows latches, mounting holes, https://docs.google.com/spreadsheets/d/16SsEcesNF15N3Lb4niX7dcUr-NY5_MFPQhobNuNppn4/edit#gid=0
Through hole horizontal IDC header THT 2x30 2.54mm double row
0
62
61
Connector_IDC
IDC-Header_2x30-1MP_P2.54mm_Latch_Vertical
Through hole IDC header, 2x30, 2.54mm pitch, DIN 41651 / IEC 60603-13, double rows latches, mounting holes, https://docs.google.com/spreadsheets/d/16SsEcesNF15N3Lb4niX7dcUr-NY5_MFPQhobNuNppn4/edit#gid=0
Through hole vertical IDC header THT 2x30 2.54mm double row
0
62
61
Connector_IDC
IDC-Header_2x30_P2.54mm_Horizontal
Through hole IDC box header, 2x30, 2.54mm pitch, DIN 41651 / IEC 60603-13, double rows, https://docs.google.com/spreadsheets/d/16SsEcesNF15N3Lb4niX7dcUr-NY5_MFPQhobNuNppn4/edit#gid=0
Through hole horizontal IDC box header THT 2x30 2.54mm double row
0
60
60
Connector_IDC
IDC-Header_2x30_P2.54mm_Latch6.5mm_Vertical
Through hole IDC header, 2x30, 2.54mm pitch, DIN 41651 / IEC 60603-13, double rows, 6.5mm latches, https://docs.google.com/spreadsheets/d/16SsEcesNF15N3Lb4niX7dcUr-NY5_MFPQhobNuNppn4/edit#gid=0
Through hole vertical IDC header THT 2x30 2.54mm double row
0
60
60
Connector_IDC
IDC-Header_2x30_P2.54mm_Latch9.5mm_Vertical
Through hole IDC header, 2x30, 2.54mm pitch, DIN 41651 / IEC 60603-13, double rows, 9.5mm latches, https://docs.google.com/spreadsheets/d/16SsEcesNF15N3Lb4niX7dcUr-NY5_MFPQhobNuNppn4/edit#gid=0
Through hole vertical IDC header THT 2x30 2.54mm double row
0
60
60
Connector_IDC
IDC-Header_2x30_P2.54mm_Latch12.0mm_Vertical
Through hole IDC header, 2x30, 2.54mm pitch, DIN 41651 / IEC 60603-13, double rows, 12.0mm latches, https://docs.google.com/spreadsheets/d/16SsEcesNF15N3Lb4niX7dcUr-NY5_MFPQhobNuNppn4/edit#gid=0
Through hole vertical IDC header THT 2x30 2.54mm double row
0
60
60
Connector_IDC
IDC-Header_2x30_P2.54mm_Latch_Horizontal
Through hole IDC header, 2x30, 2.54mm pitch, DIN 41651 / IEC 60603-13, double rows latches, https://docs.google.com/spreadsheets/d/16SsEcesNF15N3Lb4niX7dcUr-NY5_MFPQhobNuNppn4/edit#gid=0
Through hole horizontal IDC header THT 2x30 2.54mm double row
0
60
60
Connector_IDC
IDC-Header_2x30_P2.54mm_Latch_Vertical
Through hole IDC header, 2x30, 2.54mm pitch, DIN 41651 / IEC 60603-13, double rows latches, https://docs.google.com/spreadsheets/d/16SsEcesNF15N3Lb4niX7dcUr-NY5_MFPQhobNuNppn4/edit#gid=0
Through hole vertical IDC header THT 2x30 2.54mm double row
0
60
60
Connector_IDC
IDC-Header_2x30_P2.54mm_Vertical
Through hole IDC box header, 2x30, 2.54mm pitch, DIN 41651 / IEC 60603-13, double rows, https://docs.google.com/spreadsheets/d/16SsEcesNF15N3Lb4niX7dcUr-NY5_MFPQhobNuNppn4/edit#gid=0
Through hole vertical IDC box header THT 2x30 2.54mm double row
0
60
60
Connector_IDC
IDC-Header_2x32-1MP_P2.54mm_Latch6.5mm_Vertical
Through hole IDC header, 2x32, 2.54mm pitch, DIN 41651 / IEC 60603-13, double rows, 6.5mm latches, mounting holes, https://docs.google.com/spreadsheets/d/16SsEcesNF15N3Lb4niX7dcUr-NY5_MFPQhobNuNppn4/edit#gid=0
Through hole vertical IDC header THT 2x32 2.54mm double row
0
66
65
Connector_IDC
IDC-Header_2x32-1MP_P2.54mm_Latch9.5mm_Vertical
Through hole IDC header, 2x32, 2.54mm pitch, DIN 41651 / IEC 60603-13, double rows, 9.5mm latches, mounting holes, https://docs.google.com/spreadsheets/d/16SsEcesNF15N3Lb4niX7dcUr-NY5_MFPQhobNuNppn4/edit#gid=0
Through hole vertical IDC header THT 2x32 2.54mm double row
0
66
65
Connector_IDC
IDC-Header_2x32-1MP_P2.54mm_Latch12.0mm_Vertical
Through hole IDC header, 2x32, 2.54mm pitch, DIN 41651 / IEC 60603-13, double rows, 12.0mm latches, mounting holes, https://docs.google.com/spreadsheets/d/16SsEcesNF15N3Lb4niX7dcUr-NY5_MFPQhobNuNppn4/edit#gid=0
Through hole vertical IDC header THT 2x32 2.54mm double row
0
66
65
Connector_IDC
IDC-Header_2x32-1MP_P2.54mm_Latch_Horizontal
Through hole IDC header, 2x32, 2.54mm pitch, DIN 41651 / IEC 60603-13, double rows latches, mounting holes, https://docs.google.com/spreadsheets/d/16SsEcesNF15N3Lb4niX7dcUr-NY5_MFPQhobNuNppn4/edit#gid=0
Through hole horizontal IDC header THT 2x32 2.54mm double row
0
66
65
Connector_IDC
IDC-Header_2x32-1MP_P2.54mm_Latch_Vertical
Through hole IDC header, 2x32, 2.54mm pitch, DIN 41651 / IEC 60603-13, double rows latches, mounting holes, https://docs.google.com/spreadsheets/d/16SsEcesNF15N3Lb4niX7dcUr-NY5_MFPQhobNuNppn4/edit#gid=0
Through hole vertical IDC header THT 2x32 2.54mm double row
0
66
65
Connector_IDC
IDC-Header_2x32_P2.54mm_Horizontal
Through hole IDC box header, 2x32, 2.54mm pitch, DIN 41651 / IEC 60603-13, double rows, https://docs.google.com/spreadsheets/d/16SsEcesNF15N3Lb4niX7dcUr-NY5_MFPQhobNuNppn4/edit#gid=0
Through hole horizontal IDC box header THT 2x32 2.54mm double row
0
64
64
Connector_IDC
IDC-Header_2x32_P2.54mm_Latch6.5mm_Vertical
Through hole IDC header, 2x32, 2.54mm pitch, DIN 41651 / IEC 60603-13, double rows, 6.5mm latches, https://docs.google.com/spreadsheets/d/16SsEcesNF15N3Lb4niX7dcUr-NY5_MFPQhobNuNppn4/edit#gid=0
Through hole vertical IDC header THT 2x32 2.54mm double row
0
64
64
Connector_IDC
IDC-Header_2x32_P2.54mm_Latch9.5mm_Vertical
Through hole IDC header, 2x32, 2.54mm pitch, DIN 41651 / IEC 60603-13, double rows, 9.5mm latches, https://docs.google.com/spreadsheets/d/16SsEcesNF15N3Lb4niX7dcUr-NY5_MFPQhobNuNppn4/edit#gid=0
Through hole vertical IDC header THT 2x32 2.54mm double row
0
64
64
Connector_IDC
IDC-Header_2x32_P2.54mm_Latch12.0mm_Vertical
Through hole IDC header, 2x32, 2.54mm pitch, DIN 41651 / IEC 60603-13, double rows, 12.0mm latches, https://docs.google.com/spreadsheets/d/16SsEcesNF15N3Lb4niX7dcUr-NY5_MFPQhobNuNppn4/edit#gid=0
Through hole vertical IDC header THT 2x32 2.54mm double row
0
64
64
Connector_IDC
IDC-Header_2x32_P2.54mm_Latch_Horizontal
Through hole IDC header, 2x32, 2.54mm pitch, DIN 41651 / IEC 60603-13, double rows latches, https://docs.google.com/spreadsheets/d/16SsEcesNF15N3Lb4niX7dcUr-NY5_MFPQhobNuNppn4/edit#gid=0
Through hole horizontal IDC header THT 2x32 2.54mm double row
0
64
64
Connector_IDC
IDC-Header_2x32_P2.54mm_Latch_Vertical
Through hole IDC header, 2x32, 2.54mm pitch, DIN 41651 / IEC 60603-13, double rows latches, https://docs.google.com/spreadsheets/d/16SsEcesNF15N3Lb4niX7dcUr-NY5_MFPQhobNuNppn4/edit#gid=0
Through hole vertical IDC header THT 2x32 2.54mm double row
0
64
64
Connector_IDC
IDC-Header_2x32_P2.54mm_Vertical
Through hole IDC box header, 2x32, 2.54mm pitch, DIN 41651 / IEC 60603-13, double rows, https://docs.google.com/spreadsheets/d/16SsEcesNF15N3Lb4niX7dcUr-NY5_MFPQhobNuNppn4/edit#gid=0
Through hole vertical IDC box header THT 2x32 2.54mm double row
0
64
64
Connector_JAE
JAE_LY20-4P-DLT1_2x02_P2.00mm_Horizontal
Molex LY 20 series connector, LY20-4P-DLT1, 2 Circuits (http://www.jae.com/z-en/pdf_download_exec.cfm?param=SJ038187.pdf), generated with kicad-footprint-generator
connector JAE  top entry
0
4
4
Connector_JAE
JAE_LY20-4P-DT1_2x02_P2.00mm_Vertical
Molex LY 20 series connector, LY20-4P-DT1, 2 Circuits (http://www.jae.com/z-en/pdf_download_exec.cfm?param=SJ103130.pdf), generated with kicad-footprint-generator
connector JAE  side entry
0
4
4
Connector_JAE
JAE_LY20-6P-DLT1_2x03_P2.00mm_Horizontal
Molex LY 20 series connector, LY20-6P-DLT1, 3 Circuits (http://www.jae.com/z-en/pdf_download_exec.cfm?param=SJ038187.pdf), generated with kicad-footprint-generator
connector JAE  top entry
0
6
6
Connector_JAE
JAE_LY20-6P-DT1_2x03_P2.00mm_Vertical
Molex LY 20 series connector, LY20-6P-DT1, 3 Circuits (http://www.jae.com/z-en/pdf_download_exec.cfm?param=SJ103130.pdf), generated with kicad-footprint-generator
connector JAE  side entry
0
6
6
Connector_JAE
JAE_LY20-8P-DLT1_2x04_P2.00mm_Horizontal
Molex LY 20 series connector, LY20-8P-DLT1, 4 Circuits (http://www.jae.com/z-en/pdf_download_exec.cfm?param=SJ038187.pdf), generated with kicad-footprint-generator
connector JAE  top entry
0
8
8
Connector_JAE
JAE_LY20-8P-DT1_2x04_P2.00mm_Vertical
Molex LY 20 series connector, LY20-8P-DT1, 4 Circuits (http://www.jae.com/z-en/pdf_download_exec.cfm?param=SJ103130.pdf), generated with kicad-footprint-generator
connector JAE  side entry
0
8
8
Connector_JAE
JAE_LY20-10P-DLT1_2x05_P2.00mm_Horizontal
Molex LY 20 series connector, LY20-10P-DLT1, 5 Circuits (http://www.jae.com/z-en/pdf_download_exec.cfm?param=SJ038187.pdf), generated with kicad-footprint-generator
connector JAE  top entry
0
10
10
Connector_JAE
JAE_LY20-10P-DT1_2x05_P2.00mm_Vertical
Molex LY 20 series connector, LY20-10P-DT1, 5 Circuits (http://www.jae.com/z-en/pdf_download_exec.cfm?param=SJ103130.pdf), generated with kicad-footprint-generator
connector JAE  side entry
0
10
10
Connector_JAE
JAE_LY20-12P-DLT1_2x06_P2.00mm_Horizontal
Molex LY 20 series connector, LY20-12P-DLT1, 6 Circuits (http://www.jae.com/z-en/pdf_download_exec.cfm?param=SJ038187.pdf), generated with kicad-footprint-generator
connector JAE  top entry
0
12
12
Connector_JAE
JAE_LY20-12P-DT1_2x06_P2.00mm_Vertical
Molex LY 20 series connector, LY20-12P-DT1, 6 Circuits (http://www.jae.com/z-en/pdf_download_exec.cfm?param=SJ103130.pdf), generated with kicad-footprint-generator
connector JAE  side entry
0
12
12
Connector_JAE
JAE_LY20-14P-DLT1_2x07_P2.00mm_Horizontal
Molex LY 20 series connector, LY20-14P-DLT1, 7 Circuits (http://www.jae.com/z-en/pdf_download_exec.cfm?param=SJ038187.pdf), generated with kicad-footprint-generator
connector JAE  top entry
0
14
14
Connector_JAE
JAE_LY20-14P-DT1_2x07_P2.00mm_Vertical
Molex LY 20 series connector, LY20-14P-DT1, 7 Circuits (http://www.jae.com/z-en/pdf_download_exec.cfm?param=SJ103130.pdf), generated with kicad-footprint-generator
connector JAE  side entry
0
14
14
Connector_JAE
JAE_LY20-16P-DLT1_2x08_P2.00mm_Horizontal
Molex LY 20 series connector, LY20-16P-DLT1, 8 Circuits (http://www.jae.com/z-en/pdf_download_exec.cfm?param=SJ038187.pdf), generated with kicad-footprint-generator
connector JAE  top entry
0
16
16
Connector_JAE
JAE_LY20-16P-DT1_2x08_P2.00mm_Vertical
Molex LY 20 series connector, LY20-16P-DT1, 8 Circuits (http://www.jae.com/z-en/pdf_download_exec.cfm?param=SJ103130.pdf), generated with kicad-footprint-generator
connector JAE  side entry
0
16
16
Connector_JAE
JAE_LY20-18P-DLT1_2x09_P2.00mm_Horizontal
Molex LY 20 series connector, LY20-18P-DLT1, 9 Circuits (http://www.jae.com/z-en/pdf_download_exec.cfm?param=SJ038187.pdf), generated with kicad-footprint-generator
connector JAE  top entry
0
18
18
Connector_JAE
JAE_LY20-18P-DT1_2x09_P2.00mm_Vertical
Molex LY 20 series connector, LY20-18P-DT1, 9 Circuits (http://www.jae.com/z-en/pdf_download_exec.cfm?param=SJ103130.pdf), generated with kicad-footprint-generator
connector JAE  side entry
0
18
18
Connector_JAE
JAE_LY20-20P-DLT1_2x10_P2.00mm_Horizontal
Molex LY 20 series connector, LY20-20P-DLT1, 10 Circuits (http://www.jae.com/z-en/pdf_download_exec.cfm?param=SJ038187.pdf), generated with kicad-footprint-generator
connector JAE  top entry
0
20
20
Connector_JAE
JAE_LY20-20P-DT1_2x10_P2.00mm_Vertical
Molex LY 20 series connector, LY20-20P-DT1, 10 Circuits (http://www.jae.com/z-en/pdf_download_exec.cfm?param=SJ103130.pdf), generated with kicad-footprint-generator
connector JAE  side entry
0
20
20
Connector_JAE
JAE_LY20-22P-DLT1_2x11_P2.00mm_Horizontal
Molex LY 20 series connector, LY20-22P-DLT1, 11 Circuits (http://www.jae.com/z-en/pdf_download_exec.cfm?param=SJ038187.pdf), generated with kicad-footprint-generator
connector JAE  top entry
0
22
22
Connector_JAE
JAE_LY20-22P-DT1_2x11_P2.00mm_Vertical
Molex LY 20 series connector, LY20-22P-DT1, 11 Circuits (http://www.jae.com/z-en/pdf_download_exec.cfm?param=SJ103130.pdf), generated with kicad-footprint-generator
connector JAE  side entry
0
22
22
Connector_JAE
JAE_LY20-24P-DLT1_2x12_P2.00mm_Horizontal
Molex LY 20 series connector, LY20-24P-DLT1, 12 Circuits (http://www.jae.com/z-en/pdf_download_exec.cfm?param=SJ038187.pdf), generated with kicad-footprint-generator
connector JAE  top entry
0
24
24
Connector_JAE
JAE_LY20-24P-DT1_2x12_P2.00mm_Vertical
Molex LY 20 series connector, LY20-24P-DT1, 12 Circuits (http://www.jae.com/z-en/pdf_download_exec.cfm?param=SJ103130.pdf), generated with kicad-footprint-generator
connector JAE  side entry
0
24
24
Connector_JAE
JAE_LY20-26P-DLT1_2x13_P2.00mm_Horizontal
Molex LY 20 series connector, LY20-26P-DLT1, 13 Circuits (http://www.jae.com/z-en/pdf_download_exec.cfm?param=SJ038187.pdf), generated with kicad-footprint-generator
connector JAE  top entry
0
26
26
Connector_JAE
JAE_LY20-26P-DT1_2x13_P2.00mm_Vertical
Molex LY 20 series connector, LY20-26P-DT1, 13 Circuits (http://www.jae.com/z-en/pdf_download_exec.cfm?param=SJ103130.pdf), generated with kicad-footprint-generator
connector JAE  side entry
0
26
26
Connector_JAE
JAE_LY20-28P-DLT1_2x14_P2.00mm_Horizontal
Molex LY 20 series connector, LY20-28P-DLT1, 14 Circuits (http://www.jae.com/z-en/pdf_download_exec.cfm?param=SJ038187.pdf), generated with kicad-footprint-generator
connector JAE  top entry
0
28
28
Connector_JAE
JAE_LY20-28P-DT1_2x14_P2.00mm_Vertical
Molex LY 20 series connector, LY20-28P-DT1, 14 Circuits (http://www.jae.com/z-en/pdf_download_exec.cfm?param=SJ103130.pdf), generated with kicad-footprint-generator
connector JAE  side entry
0
28
28
Connector_JAE
JAE_LY20-30P-DLT1_2x15_P2.00mm_Horizontal
Molex LY 20 series connector, LY20-30P-DLT1, 15 Circuits (http://www.jae.com/z-en/pdf_download_exec.cfm?param=SJ038187.pdf), generated with kicad-footprint-generator
connector JAE  top entry
0
30
30
Connector_JAE
JAE_LY20-30P-DT1_2x15_P2.00mm_Vertical
Molex LY 20 series connector, LY20-30P-DT1, 15 Circuits (http://www.jae.com/z-en/pdf_download_exec.cfm?param=SJ103130.pdf), generated with kicad-footprint-generator
connector JAE  side entry
0
30
30
Connector_JAE
JAE_LY20-32P-DLT1_2x16_P2.00mm_Horizontal
Molex LY 20 series connector, LY20-32P-DLT1, 16 Circuits (http://www.jae.com/z-en/pdf_download_exec.cfm?param=SJ038187.pdf), generated with kicad-footprint-generator
connector JAE  top entry
0
32
32
Connector_JAE
JAE_LY20-32P-DT1_2x16_P2.00mm_Vertical
Molex LY 20 series connector, LY20-32P-DT1, 16 Circuits (http://www.jae.com/z-en/pdf_download_exec.cfm?param=SJ103130.pdf), generated with kicad-footprint-generator
connector JAE  side entry
0
32
32
Connector_JAE
JAE_LY20-34P-DLT1_2x17_P2.00mm_Horizontal
Molex LY 20 series connector, LY20-34P-DLT1, 17 Circuits (http://www.jae.com/z-en/pdf_download_exec.cfm?param=SJ038187.pdf), generated with kicad-footprint-generator
connector JAE  top entry
0
34
34
Connector_JAE
JAE_LY20-34P-DT1_2x17_P2.00mm_Vertical
Molex LY 20 series connector, LY20-34P-DT1, 17 Circuits (http://www.jae.com/z-en/pdf_download_exec.cfm?param=SJ103130.pdf), generated with kicad-footprint-generator
connector JAE  side entry
0
34
34
Connector_JAE
JAE_LY20-36P-DLT1_2x18_P2.00mm_Horizontal
Molex LY 20 series connector, LY20-36P-DLT1, 18 Circuits (http://www.jae.com/z-en/pdf_download_exec.cfm?param=SJ038187.pdf), generated with kicad-footprint-generator
connector JAE  top entry
0
36
36
Connector_JAE
JAE_LY20-36P-DT1_2x18_P2.00mm_Vertical
Molex LY 20 series connector, LY20-36P-DT1, 18 Circuits (http://www.jae.com/z-en/pdf_download_exec.cfm?param=SJ103130.pdf), generated with kicad-footprint-generator
connector JAE  side entry
0
36
36
Connector_JAE
JAE_LY20-38P-DLT1_2x19_P2.00mm_Horizontal
Molex LY 20 series connector, LY20-38P-DLT1, 19 Circuits (http://www.jae.com/z-en/pdf_download_exec.cfm?param=SJ038187.pdf), generated with kicad-footprint-generator
connector JAE  top entry
0
38
38
Connector_JAE
JAE_LY20-38P-DT1_2x19_P2.00mm_Vertical
Molex LY 20 series connector, LY20-38P-DT1, 19 Circuits (http://www.jae.com/z-en/pdf_download_exec.cfm?param=SJ103130.pdf), generated with kicad-footprint-generator
connector JAE  side entry
0
38
38
Connector_JAE
JAE_LY20-40P-DLT1_2x20_P2.00mm_Horizontal
Molex LY 20 series connector, LY20-40P-DLT1, 20 Circuits (http://www.jae.com/z-en/pdf_download_exec.cfm?param=SJ038187.pdf), generated with kicad-footprint-generator
connector JAE  top entry
0
40
40
Connector_JAE
JAE_LY20-40P-DT1_2x20_P2.00mm_Vertical
Molex LY 20 series connector, LY20-40P-DT1, 20 Circuits (http://www.jae.com/z-en/pdf_download_exec.cfm?param=SJ103130.pdf), generated with kicad-footprint-generator
connector JAE  side entry
0
40
40
Connector_JAE
JAE_LY20-42P-DLT1_2x21_P2.00mm_Horizontal
Molex LY 20 series connector, LY20-42P-DLT1, 21 Circuits (http://www.jae.com/z-en/pdf_download_exec.cfm?param=SJ038187.pdf), generated with kicad-footprint-generator
connector JAE  top entry
0
42
42
Connector_JAE
JAE_LY20-42P-DT1_2x21_P2.00mm_Vertical
Molex LY 20 series connector, LY20-42P-DT1, 21 Circuits (http://www.jae.com/z-en/pdf_download_exec.cfm?param=SJ103130.pdf), generated with kicad-footprint-generator
connector JAE  side entry
0
42
42
Connector_JAE
JAE_LY20-44P-DLT1_2x22_P2.00mm_Horizontal
Molex LY 20 series connector, LY20-44P-DLT1, 22 Circuits (http://www.jae.com/z-en/pdf_download_exec.cfm?param=SJ038187.pdf), generated with kicad-footprint-generator
connector JAE  top entry
0
44
44
Connector_JAE
JAE_LY20-44P-DT1_2x22_P2.00mm_Vertical
Molex LY 20 series connector, LY20-44P-DT1, 22 Circuits (http://www.jae.com/z-en/pdf_download_exec.cfm?param=SJ103130.pdf), generated with kicad-footprint-generator
connector JAE  side entry
0
44
44
Connector_JAE
JAE_MM70-314-310B1
http://www.heilind.com/marketing/documents/jae/JAE_MM70.pdf
connector JAE MXM
0
280
279
Connector_JAE
JAE_SIM_Card_SF72S006
SIM Card, Push-Push, https://www.jae.com/direct/topics/topics_file_download/topics_id=68892&ext_no=06&index=0&_lang=en&v=202003111511468456809
SIM Card with Detect Switch
0
18
9
Connector_JST
JST_ACH_BM01B-ACHSS-A-GAN-ETF_1x01-1MP_P1.20mm_Vertical
JST ACH series connector, BM01B-ACHSS-A-GAN-ETF (http://www.jst-mfg.com/product/pdf/eng/eACH.pdf), generated with kicad-footprint-generator
connector JST ACH vertical
0
3
2
Connector_JST
JST_ACH_BM02B-ACHSS-GAN-ETF_1x02-1MP_P1.20mm_Vertical
JST ACH series connector, BM02B-ACHSS-GAN-ETF (http://www.jst-mfg.com/product/pdf/eng/eACH.pdf), generated with kicad-footprint-generator
connector JST ACH vertical
0
4
3
Connector_JST
JST_ACH_BM03B-ACHSS-GAN-ETF_1x03-1MP_P1.20mm_Vertical
JST ACH series connector, BM03B-ACHSS-GAN-ETF (http://www.jst-mfg.com/product/pdf/eng/eACH.pdf), generated with kicad-footprint-generator
connector JST ACH vertical
0
5
4
Connector_JST
JST_ACH_BM04B-ACHSS-A-GAN-ETF_1x04-1MP_P1.20mm_Vertical
JST ACH series connector, BM04B-ACHSS-A-GAN-ETF (http://www.jst-mfg.com/product/pdf/eng/eACH.pdf), generated with kicad-footprint-generator
connector JST ACH vertical
0
6
5
Connector_JST
JST_ACH_BM05B-ACHSS-A-GAN-ETF_1x05-1MP_P1.20mm_Vertical
JST ACH series connector, BM05B-ACHSS-A-GAN-ETF (http://www.jst-mfg.com/product/pdf/eng/eACH.pdf), generated with kicad-footprint-generator
connector JST ACH vertical
0
7
6
Connector_JST
JST_AUH_BM03B-AUHKS-GA-TB_1x03-1MP_P1.50mm_Vertical
JST AUH series connector, BM03B-AUHKS-GA-TB (http://www.jst-mfg.com/product/pdf/eng/eAUH.pdf), generated with kicad-footprint-generator
connector JST AUH side entry
0
5
4
Connector_JST
JST_AUH_BM05B-AUHKS-GA-TB_1x05-1MP_P1.50mm_Vertical
JST AUH series connector, BM05B-AUHKS-GA-TB (http://www.jst-mfg.com/product/pdf/eng/eAUH.pdf), generated with kicad-footprint-generator
connector JST AUH side entry
0
7
6
Connector_JST
JST_EH_B2B-EH-A_1x02_P2.50mm_Vertical
JST EH series connector, B2B-EH-A (http://www.jst-mfg.com/product/pdf/eng/eEH.pdf), generated with kicad-footprint-generator
connector JST EH vertical
0
2
2
Connector_JST
JST_EH_B3B-EH-A_1x03_P2.50mm_Vertical
JST EH series connector, B3B-EH-A (http://www.jst-mfg.com/product/pdf/eng/eEH.pdf), generated with kicad-footprint-generator
connector JST EH vertical
0
3
3
Connector_JST
JST_EH_B4B-EH-A_1x04_P2.50mm_Vertical
JST EH series connector, B4B-EH-A (http://www.jst-mfg.com/product/pdf/eng/eEH.pdf), generated with kicad-footprint-generator
connector JST EH vertical
0
4
4
Connector_JST
JST_EH_B5B-EH-A_1x05_P2.50mm_Vertical
JST EH series connector, B5B-EH-A (http://www.jst-mfg.com/product/pdf/eng/eEH.pdf), generated with kicad-footprint-generator
connector JST EH vertical
0
5
5
Connector_JST
JST_EH_B6B-EH-A_1x06_P2.50mm_Vertical
JST EH series connector, B6B-EH-A (http://www.jst-mfg.com/product/pdf/eng/eEH.pdf), generated with kicad-footprint-generator
connector JST EH vertical
0
6
6
Connector_JST
JST_EH_B7B-EH-A_1x07_P2.50mm_Vertical
JST EH series connector, B7B-EH-A (http://www.jst-mfg.com/product/pdf/eng/eEH.pdf), generated with kicad-footprint-generator
connector JST EH vertical
0
7
7
Connector_JST
JST_EH_B8B-EH-A_1x08_P2.50mm_Vertical
JST EH series connector, B8B-EH-A (http://www.jst-mfg.com/product/pdf/eng/eEH.pdf), generated with kicad-footprint-generator
connector JST EH vertical
0
8
8
Connector_JST
JST_EH_B9B-EH-A_1x09_P2.50mm_Vertical
JST EH series connector, B9B-EH-A (http://www.jst-mfg.com/product/pdf/eng/eEH.pdf), generated with kicad-footprint-generator
connector JST EH vertical
0
9
9
Connector_JST
JST_EH_B10B-EH-A_1x10_P2.50mm_Vertical
JST EH series connector, B10B-EH-A (http://www.jst-mfg.com/product/pdf/eng/eEH.pdf), generated with kicad-footprint-generator
connector JST EH side entry
0
10
10
Connector_JST
JST_EH_B11B-EH-A_1x11_P2.50mm_Vertical
JST EH series connector, B11B-EH-A (http://www.jst-mfg.com/product/pdf/eng/eEH.pdf), generated with kicad-footprint-generator
connector JST EH side entry
0
11
11
Connector_JST
JST_EH_B12B-EH-A_1x12_P2.50mm_Vertical
JST EH series connector, B12B-EH-A (http://www.jst-mfg.com/product/pdf/eng/eEH.pdf), generated with kicad-footprint-generator
connector JST EH side entry
0
12
12
Connector_JST
JST_EH_B13B-EH-A_1x13_P2.50mm_Vertical
JST EH series connector, B13B-EH-A (http://www.jst-mfg.com/product/pdf/eng/eEH.pdf), generated with kicad-footprint-generator
connector JST EH side entry
0
13
13
Connector_JST
JST_EH_B14B-EH-A_1x14_P2.50mm_Vertical
JST EH series connector, B14B-EH-A (http://www.jst-mfg.com/product/pdf/eng/eEH.pdf), generated with kicad-footprint-generator
connector JST EH side entry
0
14
14
Connector_JST
JST_EH_B15B-EH-A_1x15_P2.50mm_Vertical
JST EH series connector, B15B-EH-A (http://www.jst-mfg.com/product/pdf/eng/eEH.pdf), generated with kicad-footprint-generator
connector JST EH side entry
0
15
15
Connector_JST
JST_EH_S2B-EH_1x02_P2.50mm_Horizontal
JST EH series connector, S2B-EH (http://www.jst-mfg.com/product/pdf/eng/eEH.pdf), generated with kicad-footprint-generator
connector JST EH horizontal
0
2
2
Connector_JST
JST_EH_S3B-EH_1x03_P2.50mm_Horizontal
JST EH series connector, S3B-EH (http://www.jst-mfg.com/product/pdf/eng/eEH.pdf), generated with kicad-footprint-generator
connector JST EH horizontal
0
3
3
Connector_JST
JST_EH_S4B-EH_1x04_P2.50mm_Horizontal
JST EH series connector, S4B-EH (http://www.jst-mfg.com/product/pdf/eng/eEH.pdf), generated with kicad-footprint-generator
connector JST EH horizontal
0
4
4
Connector_JST
JST_EH_S5B-EH_1x05_P2.50mm_Horizontal
JST EH series connector, S5B-EH (http://www.jst-mfg.com/product/pdf/eng/eEH.pdf), generated with kicad-footprint-generator
connector JST EH horizontal
0
5
5
Connector_JST
JST_EH_S6B-EH_1x06_P2.50mm_Horizontal
JST EH series connector, S6B-EH (http://www.jst-mfg.com/product/pdf/eng/eEH.pdf), generated with kicad-footprint-generator
connector JST EH horizontal
0
6
6
Connector_JST
JST_EH_S7B-EH_1x07_P2.50mm_Horizontal
JST EH series connector, S7B-EH (http://www.jst-mfg.com/product/pdf/eng/eEH.pdf), generated with kicad-footprint-generator
connector JST EH horizontal
0
7
7
Connector_JST
JST_EH_S8B-EH_1x08_P2.50mm_Horizontal
JST EH series connector, S8B-EH (http://www.jst-mfg.com/product/pdf/eng/eEH.pdf), generated with kicad-footprint-generator
connector JST EH horizontal
0
8
8
Connector_JST
JST_EH_S9B-EH_1x09_P2.50mm_Horizontal
JST EH series connector, S9B-EH (http://www.jst-mfg.com/product/pdf/eng/eEH.pdf), generated with kicad-footprint-generator
connector JST EH horizontal
0
9
9
Connector_JST
JST_EH_S10B-EH_1x10_P2.50mm_Horizontal
JST EH series connector, S10B-EH (http://www.jst-mfg.com/product/pdf/eng/eEH.pdf), generated with kicad-footprint-generator
connector JST EH top entry
0
10
10
Connector_JST
JST_EH_S11B-EH_1x11_P2.50mm_Horizontal
JST EH series connector, S11B-EH (http://www.jst-mfg.com/product/pdf/eng/eEH.pdf), generated with kicad-footprint-generator
connector JST EH top entry
0
11
11
Connector_JST
JST_EH_S12B-EH_1x12_P2.50mm_Horizontal
JST EH series connector, S12B-EH (http://www.jst-mfg.com/product/pdf/eng/eEH.pdf), generated with kicad-footprint-generator
connector JST EH top entry
0
12
12
Connector_JST
JST_EH_S13B-EH_1x13_P2.50mm_Horizontal
JST EH series connector, S13B-EH (http://www.jst-mfg.com/product/pdf/eng/eEH.pdf), generated with kicad-footprint-generator
connector JST EH top entry
0
13
13
Connector_JST
JST_EH_S14B-EH_1x14_P2.50mm_Horizontal
JST EH series connector, S14B-EH (http://www.jst-mfg.com/product/pdf/eng/eEH.pdf), generated with kicad-footprint-generator
connector JST EH top entry
0
14
14
Connector_JST
JST_EH_S15B-EH_1x15_P2.50mm_Horizontal
JST EH series connector, S15B-EH (http://www.jst-mfg.com/product/pdf/eng/eEH.pdf), generated with kicad-footprint-generator
connector JST EH top entry
0
15
15
Connector_JST
JST_GH_BM02B-GHS-TBT_1x02-1MP_P1.25mm_Vertical
JST GH series connector, BM02B-GHS-TBT (http://www.jst-mfg.com/product/pdf/eng/eGH.pdf), generated with kicad-footprint-generator
connector JST GH side entry
0
4
3
Connector_JST
JST_GH_BM03B-GHS-TBT_1x03-1MP_P1.25mm_Vertical
JST GH series connector, BM03B-GHS-TBT (http://www.jst-mfg.com/product/pdf/eng/eGH.pdf), generated with kicad-footprint-generator
connector JST GH side entry
0
5
4
Connector_JST
JST_GH_BM04B-GHS-TBT_1x04-1MP_P1.25mm_Vertical
JST GH series connector, BM04B-GHS-TBT (http://www.jst-mfg.com/product/pdf/eng/eGH.pdf), generated with kicad-footprint-generator
connector JST GH side entry
0
6
5
Connector_JST
JST_GH_BM05B-GHS-TBT_1x05-1MP_P1.25mm_Vertical
JST GH series connector, BM05B-GHS-TBT (http://www.jst-mfg.com/product/pdf/eng/eGH.pdf), generated with kicad-footprint-generator
connector JST GH side entry
0
7
6
Connector_JST
JST_GH_BM06B-GHS-TBT_1x06-1MP_P1.25mm_Vertical
JST GH series connector, BM06B-GHS-TBT (http://www.jst-mfg.com/product/pdf/eng/eGH.pdf), generated with kicad-footprint-generator
connector JST GH side entry
0
8
7
Connector_JST
JST_GH_BM07B-GHS-TBT_1x07-1MP_P1.25mm_Vertical
JST GH series connector, BM07B-GHS-TBT (http://www.jst-mfg.com/product/pdf/eng/eGH.pdf), generated with kicad-footprint-generator
connector JST GH side entry
0
9
8
Connector_JST
JST_GH_BM08B-GHS-TBT_1x08-1MP_P1.25mm_Vertical
JST GH series connector, BM08B-GHS-TBT (http://www.jst-mfg.com/product/pdf/eng/eGH.pdf), generated with kicad-footprint-generator
connector JST GH side entry
0
10
9
Connector_JST
JST_GH_BM09B-GHS-TBT_1x09-1MP_P1.25mm_Vertical
JST GH series connector, BM09B-GHS-TBT (http://www.jst-mfg.com/product/pdf/eng/eGH.pdf), generated with kicad-footprint-generator
connector JST GH side entry
0
11
10
Connector_JST
JST_GH_BM10B-GHS-TBT_1x10-1MP_P1.25mm_Vertical
JST GH series connector, BM10B-GHS-TBT (http://www.jst-mfg.com/product/pdf/eng/eGH.pdf), generated with kicad-footprint-generator
connector JST GH side entry
0
12
11
Connector_JST
JST_GH_BM11B-GHS-TBT_1x11-1MP_P1.25mm_Vertical
JST GH series connector, BM11B-GHS-TBT (http://www.jst-mfg.com/product/pdf/eng/eGH.pdf), generated with kicad-footprint-generator
connector JST GH side entry
0
13
12
Connector_JST
JST_GH_BM12B-GHS-TBT_1x12-1MP_P1.25mm_Vertical
JST GH series connector, BM12B-GHS-TBT (http://www.jst-mfg.com/product/pdf/eng/eGH.pdf), generated with kicad-footprint-generator
connector JST GH side entry
0
14
13
Connector_JST
JST_GH_BM13B-GHS-TBT_1x13-1MP_P1.25mm_Vertical
JST GH series connector, BM13B-GHS-TBT (http://www.jst-mfg.com/product/pdf/eng/eGH.pdf), generated with kicad-footprint-generator
connector JST GH side entry
0
15
14
Connector_JST
JST_GH_BM14B-GHS-TBT_1x14-1MP_P1.25mm_Vertical
JST GH series connector, BM14B-GHS-TBT (http://www.jst-mfg.com/product/pdf/eng/eGH.pdf), generated with kicad-footprint-generator
connector JST GH side entry
0
16
15
Connector_JST
JST_GH_BM15B-GHS-TBT_1x15-1MP_P1.25mm_Vertical
JST GH series connector, BM15B-GHS-TBT (http://www.jst-mfg.com/product/pdf/eng/eGH.pdf), generated with kicad-footprint-generator
connector JST GH side entry
0
17
16
Connector_JST
JST_GH_SM02B-GHS-TB_1x02-1MP_P1.25mm_Horizontal
JST GH series connector, SM02B-GHS-TB (http://www.jst-mfg.com/product/pdf/eng/eGH.pdf), generated with kicad-footprint-generator
connector JST GH top entry
0
4
3
Connector_JST
JST_GH_SM03B-GHS-TB_1x03-1MP_P1.25mm_Horizontal
JST GH series connector, SM03B-GHS-TB (http://www.jst-mfg.com/product/pdf/eng/eGH.pdf), generated with kicad-footprint-generator
connector JST GH top entry
0
5
4
Connector_JST
JST_GH_SM04B-GHS-TB_1x04-1MP_P1.25mm_Horizontal
JST GH series connector, SM04B-GHS-TB (http://www.jst-mfg.com/product/pdf/eng/eGH.pdf), generated with kicad-footprint-generator
connector JST GH top entry
0
6
5
Connector_JST
JST_GH_SM05B-GHS-TB_1x05-1MP_P1.25mm_Horizontal
JST GH series connector, SM05B-GHS-TB (http://www.jst-mfg.com/product/pdf/eng/eGH.pdf), generated with kicad-footprint-generator
connector JST GH top entry
0
7
6
Connector_JST
JST_GH_SM06B-GHS-TB_1x06-1MP_P1.25mm_Horizontal
JST GH series connector, SM06B-GHS-TB (http://www.jst-mfg.com/product/pdf/eng/eGH.pdf), generated with kicad-footprint-generator
connector JST GH top entry
0
8
7
Connector_JST
JST_GH_SM07B-GHS-TB_1x07-1MP_P1.25mm_Horizontal
JST GH series connector, SM07B-GHS-TB (http://www.jst-mfg.com/product/pdf/eng/eGH.pdf), generated with kicad-footprint-generator
connector JST GH top entry
0
9
8
Connector_JST
JST_GH_SM08B-GHS-TB_1x08-1MP_P1.25mm_Horizontal
JST GH series connector, SM08B-GHS-TB (http://www.jst-mfg.com/product/pdf/eng/eGH.pdf), generated with kicad-footprint-generator
connector JST GH top entry
0
10
9
Connector_JST
JST_GH_SM09B-GHS-TB_1x09-1MP_P1.25mm_Horizontal
JST GH series connector, SM09B-GHS-TB (http://www.jst-mfg.com/product/pdf/eng/eGH.pdf), generated with kicad-footprint-generator
connector JST GH top entry
0
11
10
Connector_JST
JST_GH_SM10B-GHS-TB_1x10-1MP_P1.25mm_Horizontal
JST GH series connector, SM10B-GHS-TB (http://www.jst-mfg.com/product/pdf/eng/eGH.pdf), generated with kicad-footprint-generator
connector JST GH top entry
0
12
11
Connector_JST
JST_GH_SM11B-GHS-TB_1x11-1MP_P1.25mm_Horizontal
JST GH series connector, SM11B-GHS-TB (http://www.jst-mfg.com/product/pdf/eng/eGH.pdf), generated with kicad-footprint-generator
connector JST GH top entry
0
13
12
Connector_JST
JST_GH_SM12B-GHS-TB_1x12-1MP_P1.25mm_Horizontal
JST GH series connector, SM12B-GHS-TB (http://www.jst-mfg.com/product/pdf/eng/eGH.pdf), generated with kicad-footprint-generator
connector JST GH top entry
0
14
13
Connector_JST
JST_GH_SM13B-GHS-TB_1x13-1MP_P1.25mm_Horizontal
JST GH series connector, SM13B-GHS-TB (http://www.jst-mfg.com/product/pdf/eng/eGH.pdf), generated with kicad-footprint-generator
connector JST GH top entry
0
15
14
Connector_JST
JST_GH_SM14B-GHS-TB_1x14-1MP_P1.25mm_Horizontal
JST GH series connector, SM14B-GHS-TB (http://www.jst-mfg.com/product/pdf/eng/eGH.pdf), generated with kicad-footprint-generator
connector JST GH top entry
0
16
15
Connector_JST
JST_GH_SM15B-GHS-TB_1x15-1MP_P1.25mm_Horizontal
JST GH series connector, SM15B-GHS-TB (http://www.jst-mfg.com/product/pdf/eng/eGH.pdf), generated with kicad-footprint-generator
connector JST GH top entry
0
17
16
Connector_JST
JST_J2100_B06B-J21DK-GGXR_2x03_P2.50x4.00mm_Vertical
JST J2100 series connector, B06B-J21DK-GGXR (http://www.jst-mfg.com/product/pdf/eng/eJFA-J2000.pdf), generated with kicad-footprint-generator
connector JST J2100 vertical
0
8
6
Connector_JST
JST_J2100_B08B-J21DK-GGXR_2x04_P2.50x4.00mm_Vertical
JST J2100 series connector, B08B-J21DK-GGXR (http://www.jst-mfg.com/product/pdf/eng/eJFA-J2000.pdf), generated with kicad-footprint-generator
connector JST J2100 vertical
0
10
8
Connector_JST
JST_J2100_B10B-J21DK-GGXR_2x05_P2.50x4.00mm_Vertical
JST J2100 series connector, B10B-J21DK-GGXR (http://www.jst-mfg.com/product/pdf/eng/eJFA-J2000.pdf), generated with kicad-footprint-generator
connector JST J2100 vertical
0
12
10
Connector_JST
JST_J2100_B12B-J21DK-GGXR_2x06_P2.50x4.00mm_Vertical
JST J2100 series connector, B12B-J21DK-GGXR (http://www.jst-mfg.com/product/pdf/eng/eJFA-J2000.pdf), generated with kicad-footprint-generator
connector JST J2100 vertical
0
14
12
Connector_JST
JST_J2100_B16B-J21DK-GGXR_2x08_P2.50x4.00mm_Vertical
JST J2100 series connector, B16B-J21DK-GGXR (http://www.jst-mfg.com/product/pdf/eng/eJFA-J2000.pdf), generated with kicad-footprint-generator
connector JST J2100 vertical
0
18
16
Connector_JST
JST_J2100_B20B-J21DK-GGXR_2x10_P2.50x4.00mm_Vertical
JST J2100 series connector, B20B-J21DK-GGXR (http://www.jst-mfg.com/product/pdf/eng/eJFA-J2000.pdf), generated with kicad-footprint-generator
connector JST J2100 vertical
0
22
20
Connector_JST
JST_J2100_S06B-J21DK-GGXR_2x03_P2.50mm_Horizontal
JST J2100 series connector, S06B-J21DK-GGXR (http://www.jst-mfg.com/product/pdf/eng/eJFA-J2000.pdf), generated with kicad-footprint-generator
connector JST J2100 horizontal
0
7
6
Connector_JST
JST_J2100_S08B-J21DK-GGXR_2x04_P2.50mm_Horizontal
JST J2100 series connector, S08B-J21DK-GGXR (http://www.jst-mfg.com/product/pdf/eng/eJFA-J2000.pdf), generated with kicad-footprint-generator
connector JST J2100 horizontal
0
10
8
Connector_JST
JST_J2100_S10B-J21DK-GGXR_2x05_P2.50mm_Horizontal
JST J2100 series connector, S10B-J21DK-GGXR (http://www.jst-mfg.com/product/pdf/eng/eJFA-J2000.pdf), generated with kicad-footprint-generator
connector JST J2100 horizontal
0
12
10
Connector_JST
JST_J2100_S12B-J21DK-GGXR_2x06_P2.50mm_Horizontal
JST J2100 series connector, S12B-J21DK-GGXR (http://www.jst-mfg.com/product/pdf/eng/eJFA-J2000.pdf), generated with kicad-footprint-generator
connector JST J2100 horizontal
0
14
12
Connector_JST
JST_J2100_S16B-J21DK-GGXR_2x08_P2.50mm_Horizontal
JST J2100 series connector, S16B-J21DK-GGXR (http://www.jst-mfg.com/product/pdf/eng/eJFA-J2000.pdf), generated with kicad-footprint-generator
connector JST J2100 horizontal
0
18
16
Connector_JST
JST_J2100_S20B-J21DK-GGXR_2x10_P2.50mm_Horizontal
JST J2100 series connector, S20B-J21DK-GGXR (http://www.jst-mfg.com/product/pdf/eng/eJFA-J2000.pdf), generated with kicad-footprint-generator
connector JST J2100 horizontal
0
22
20
Connector_JST
JST_JWPF_B02B-JWPF-SK-R_1x02_P2.00mm_Vertical
JST JWPF series connector, B02B-JWPF-SK-R (http://www.jst-mfg.com/product/pdf/eng/eJWPF1.pdf), generated with kicad-footprint-generator
connector JST JWPF side entry
0
2
2
Connector_JST
JST_JWPF_B03B-JWPF-SK-R_1x03_P2.00mm_Vertical
JST JWPF series connector, B03B-JWPF-SK-R (http://www.jst-mfg.com/product/pdf/eng/eJWPF1.pdf), generated with kicad-footprint-generator
connector JST JWPF side entry
0
3
3
Connector_JST
JST_JWPF_B04B-JWPF-SK-R_1x04_P2.00mm_Vertical
JST JWPF series connector, B04B-JWPF-SK-R (http://www.jst-mfg.com/product/pdf/eng/eJWPF1.pdf), generated with kicad-footprint-generator
connector JST JWPF side entry
0
4
4
Connector_JST
JST_JWPF_B06B-JWPF-SK-R_2x03_P2.00mm_Vertical
JST JWPF series connector, B06B-JWPF-SK-R (http://www.jst-mfg.com/product/pdf/eng/eJWPF1.pdf), generated with kicad-footprint-generator
connector JST JWPF side entry
0
6
6
Connector_JST
JST_JWPF_B08B-JWPF-SK-R_2x04_P2.00mm_Vertical
JST JWPF series connector, B08B-JWPF-SK-R (http://www.jst-mfg.com/product/pdf/eng/eJWPF1.pdf), generated with kicad-footprint-generator
connector JST JWPF side entry
0
8
8
Connector_JST
JST_LEA_SM02B-LEASS-TF_1x02-1MP_P4.20mm_Horizontal
JST LEA series connector, SM02B-LEASS-TF (http://www.jst-mfg.com/product/pdf/eng/eLEA.pdf), generated with kicad-footprint-generator
connector JST LEA top entry
0
4
3
Connector_JST
JST_NV_B02P-NV_1x02_P5.00mm_Vertical
JST NV series connector, B02P-NV (http://www.jst-mfg.com/product/pdf/eng/eNV.pdf), generated with kicad-footprint-generator
connector JST NV side entry
0
2
2
Connector_JST
JST_NV_B03P-NV_1x03_P5.00mm_Vertical
JST NV series connector, B03P-NV (http://www.jst-mfg.com/product/pdf/eng/eNV.pdf), generated with kicad-footprint-generator
connector JST NV side entry
0
3
3
Connector_JST
JST_NV_B04P-NV_1x04_P5.00mm_Vertical
JST NV series connector, B04P-NV (http://www.jst-mfg.com/product/pdf/eng/eNV.pdf), generated with kicad-footprint-generator
connector JST NV side entry
0
4
4
Connector_JST
JST_PHD_B8B-PHDSS_2x04_P2.00mm_Vertical
JST PHD series connector, B8B-PHDSS (http://www.jst-mfg.com/product/pdf/eng/ePHD.pdf), generated with kicad-footprint-generator
connector JST PHD vertical
0
8
8
Connector_JST
JST_PHD_B10B-PHDSS_2x05_P2.00mm_Vertical
JST PHD series connector, B10B-PHDSS (http://www.jst-mfg.com/product/pdf/eng/ePHD.pdf), generated with kicad-footprint-generator
connector JST PHD vertical
0
10
10
Connector_JST
JST_PHD_B12B-PHDSS_2x06_P2.00mm_Vertical
JST PHD series connector, B12B-PHDSS (http://www.jst-mfg.com/product/pdf/eng/ePHD.pdf), generated with kicad-footprint-generator
connector JST PHD vertical
0
12
12
Connector_JST
JST_PHD_B14B-PHDSS_2x07_P2.00mm_Vertical
JST PHD series connector, B14B-PHDSS (http://www.jst-mfg.com/product/pdf/eng/ePHD.pdf), generated with kicad-footprint-generator
connector JST PHD vertical
0
14
14
Connector_JST
JST_PHD_B16B-PHDSS_2x08_P2.00mm_Vertical
JST PHD series connector, B16B-PHDSS (http://www.jst-mfg.com/product/pdf/eng/ePHD.pdf), generated with kicad-footprint-generator
connector JST PHD vertical
0
16
16
Connector_JST
JST_PHD_B18B-PHDSS_2x09_P2.00mm_Vertical
JST PHD series connector, B18B-PHDSS (http://www.jst-mfg.com/product/pdf/eng/ePHD.pdf), generated with kicad-footprint-generator
connector JST PHD vertical
0
18
18
Connector_JST
JST_PHD_B20B-PHDSS_2x10_P2.00mm_Vertical
JST PHD series connector, B20B-PHDSS (http://www.jst-mfg.com/product/pdf/eng/ePHD.pdf), generated with kicad-footprint-generator
connector JST PHD vertical
0
20
20
Connector_JST
JST_PHD_B22B-PHDSS_2x11_P2.00mm_Vertical
JST PHD series connector, B22B-PHDSS (http://www.jst-mfg.com/product/pdf/eng/ePHD.pdf), generated with kicad-footprint-generator
connector JST PHD vertical
0
22
22
Connector_JST
JST_PHD_B24B-PHDSS_2x12_P2.00mm_Vertical
JST PHD series connector, B24B-PHDSS (http://www.jst-mfg.com/product/pdf/eng/ePHD.pdf), generated with kicad-footprint-generator
connector JST PHD vertical
0
24
24
Connector_JST
JST_PHD_B26B-PHDSS_2x13_P2.00mm_Vertical
JST PHD series connector, B26B-PHDSS (http://www.jst-mfg.com/product/pdf/eng/ePHD.pdf), generated with kicad-footprint-generator
connector JST PHD vertical
0
26
26
Connector_JST
JST_PHD_B28B-PHDSS_2x14_P2.00mm_Vertical
JST PHD series connector, B28B-PHDSS (http://www.jst-mfg.com/product/pdf/eng/ePHD.pdf), generated with kicad-footprint-generator
connector JST PHD vertical
0
28
28
Connector_JST
JST_PHD_B30B-PHDSS_2x15_P2.00mm_Vertical
JST PHD series connector, B30B-PHDSS (http://www.jst-mfg.com/product/pdf/eng/ePHD.pdf), generated with kicad-footprint-generator
connector JST PHD vertical
0
30
30
Connector_JST
JST_PHD_B32B-PHDSS_2x16_P2.00mm_Vertical
JST PHD series connector, B32B-PHDSS (http://www.jst-mfg.com/product/pdf/eng/ePHD.pdf), generated with kicad-footprint-generator
connector JST PHD vertical
0
32
32
Connector_JST
JST_PHD_B34B-PHDSS_2x17_P2.00mm_Vertical
JST PHD series connector, B34B-PHDSS (http://www.jst-mfg.com/product/pdf/eng/ePHD.pdf), generated with kicad-footprint-generator
connector JST PHD vertical
0
34
34
Connector_JST
JST_PHD_S8B-PHDSS_2x04_P2.00mm_Horizontal
JST PHD series connector, S8B-PHDSS (http://www.jst-mfg.com/product/pdf/eng/ePHD.pdf), generated with kicad-footprint-generator
connector JST PHD horizontal
0
8
8
Connector_JST
JST_PHD_S10B-PHDSS_2x05_P2.00mm_Horizontal
JST PHD series connector, S10B-PHDSS (http://www.jst-mfg.com/product/pdf/eng/ePHD.pdf), generated with kicad-footprint-generator
connector JST PHD horizontal
0
10
10
Connector_JST
JST_PHD_S12B-PHDSS_2x06_P2.00mm_Horizontal
JST PHD series connector, S12B-PHDSS (http://www.jst-mfg.com/product/pdf/eng/ePHD.pdf), generated with kicad-footprint-generator
connector JST PHD horizontal
0
12
12
Connector_JST
JST_PHD_S14B-PHDSS_2x07_P2.00mm_Horizontal
JST PHD series connector, S14B-PHDSS (http://www.jst-mfg.com/product/pdf/eng/ePHD.pdf), generated with kicad-footprint-generator
connector JST PHD horizontal
0
14
14
Connector_JST
JST_PHD_S16B-PHDSS_2x08_P2.00mm_Horizontal
JST PHD series connector, S16B-PHDSS (http://www.jst-mfg.com/product/pdf/eng/ePHD.pdf), generated with kicad-footprint-generator
connector JST PHD horizontal
0
16
16
Connector_JST
JST_PHD_S18B-PHDSS_2x09_P2.00mm_Horizontal
JST PHD series connector, S18B-PHDSS (http://www.jst-mfg.com/product/pdf/eng/ePHD.pdf), generated with kicad-footprint-generator
connector JST PHD horizontal
0
18
18
Connector_JST
JST_PHD_S20B-PHDSS_2x10_P2.00mm_Horizontal
JST PHD series connector, S20B-PHDSS (http://www.jst-mfg.com/product/pdf/eng/ePHD.pdf), generated with kicad-footprint-generator
connector JST PHD horizontal
0
20
20
Connector_JST
JST_PHD_S22B-PHDSS_2x11_P2.00mm_Horizontal
JST PHD series connector, S22B-PHDSS (http://www.jst-mfg.com/product/pdf/eng/ePHD.pdf), generated with kicad-footprint-generator
connector JST PHD horizontal
0
22
22
Connector_JST
JST_PHD_S24B-PHDSS_2x12_P2.00mm_Horizontal
JST PHD series connector, S24B-PHDSS (http://www.jst-mfg.com/product/pdf/eng/ePHD.pdf), generated with kicad-footprint-generator
connector JST PHD horizontal
0
24
24
Connector_JST
JST_PHD_S26B-PHDSS_2x13_P2.00mm_Horizontal
JST PHD series connector, S26B-PHDSS (http://www.jst-mfg.com/product/pdf/eng/ePHD.pdf), generated with kicad-footprint-generator
connector JST PHD horizontal
0
26
26
Connector_JST
JST_PHD_S28B-PHDSS_2x14_P2.00mm_Horizontal
JST PHD series connector, S28B-PHDSS (http://www.jst-mfg.com/product/pdf/eng/ePHD.pdf), generated with kicad-footprint-generator
connector JST PHD horizontal
0
28
28
Connector_JST
JST_PHD_S30B-PHDSS_2x15_P2.00mm_Horizontal
JST PHD series connector, S30B-PHDSS (http://www.jst-mfg.com/product/pdf/eng/ePHD.pdf), generated with kicad-footprint-generator
connector JST PHD horizontal
0
30
30
Connector_JST
JST_PHD_S32B-PHDSS_2x16_P2.00mm_Horizontal
JST PHD series connector, S32B-PHDSS (http://www.jst-mfg.com/product/pdf/eng/ePHD.pdf), generated with kicad-footprint-generator
connector JST PHD horizontal
0
32
32
Connector_JST
JST_PHD_S34B-PHDSS_2x17_P2.00mm_Horizontal
JST PHD series connector, S34B-PHDSS (http://www.jst-mfg.com/product/pdf/eng/ePHD.pdf), generated with kicad-footprint-generator
connector JST PHD horizontal
0
34
34
Connector_JST
JST_PH_B2B-PH-K_1x02_P2.00mm_Vertical
JST PH series connector, B2B-PH-K (http://www.jst-mfg.com/product/pdf/eng/ePH.pdf), generated with kicad-footprint-generator
connector JST PH side entry
0
2
2
Connector_JST
JST_PH_B2B-PH-SM4-TB_1x02-1MP_P2.00mm_Vertical
JST PH series connector, B2B-PH-SM4-TB (http://www.jst-mfg.com/product/pdf/eng/ePH.pdf), generated with kicad-footprint-generator
connector JST PH side entry
0
4
3
Connector_JST
JST_PH_B3B-PH-K_1x03_P2.00mm_Vertical
JST PH series connector, B3B-PH-K (http://www.jst-mfg.com/product/pdf/eng/ePH.pdf), generated with kicad-footprint-generator
connector JST PH side entry
0
3
3
Connector_JST
JST_PH_B3B-PH-SM4-TB_1x03-1MP_P2.00mm_Vertical
JST PH series connector, B3B-PH-SM4-TB (http://www.jst-mfg.com/product/pdf/eng/ePH.pdf), generated with kicad-footprint-generator
connector JST PH side entry
0
5
4
Connector_JST
JST_PH_B4B-PH-K_1x04_P2.00mm_Vertical
JST PH series connector, B4B-PH-K (http://www.jst-mfg.com/product/pdf/eng/ePH.pdf), generated with kicad-footprint-generator
connector JST PH side entry
0
4
4
Connector_JST
JST_PH_B4B-PH-SM4-TB_1x04-1MP_P2.00mm_Vertical
JST PH series connector, B4B-PH-SM4-TB (http://www.jst-mfg.com/product/pdf/eng/ePH.pdf), generated with kicad-footprint-generator
connector JST PH side entry
0
6
5
Connector_JST
JST_PH_B5B-PH-K_1x05_P2.00mm_Vertical
JST PH series connector, B5B-PH-K (http://www.jst-mfg.com/product/pdf/eng/ePH.pdf), generated with kicad-footprint-generator
connector JST PH side entry
0
5
5
Connector_JST
JST_PH_B5B-PH-SM4-TB_1x05-1MP_P2.00mm_Vertical
JST PH series connector, B5B-PH-SM4-TB (http://www.jst-mfg.com/product/pdf/eng/ePH.pdf), generated with kicad-footprint-generator
connector JST PH side entry
0
7
6
Connector_JST
JST_PH_B6B-PH-K_1x06_P2.00mm_Vertical
JST PH series connector, B6B-PH-K (http://www.jst-mfg.com/product/pdf/eng/ePH.pdf), generated with kicad-footprint-generator
connector JST PH side entry
0
6
6
Connector_JST
JST_PH_B6B-PH-SM4-TB_1x06-1MP_P2.00mm_Vertical
JST PH series connector, B6B-PH-SM4-TB (http://www.jst-mfg.com/product/pdf/eng/ePH.pdf), generated with kicad-footprint-generator
connector JST PH side entry
0
8
7
Connector_JST
JST_PH_B7B-PH-K_1x07_P2.00mm_Vertical
JST PH series connector, B7B-PH-K (http://www.jst-mfg.com/product/pdf/eng/ePH.pdf), generated with kicad-footprint-generator
connector JST PH side entry
0
7
7
Connector_JST
JST_PH_B7B-PH-SM4-TB_1x07-1MP_P2.00mm_Vertical
JST PH series connector, B7B-PH-SM4-TB (http://www.jst-mfg.com/product/pdf/eng/ePH.pdf), generated with kicad-footprint-generator
connector JST PH side entry
0
9
8
Connector_JST
JST_PH_B8B-PH-K_1x08_P2.00mm_Vertical
JST PH series connector, B8B-PH-K (http://www.jst-mfg.com/product/pdf/eng/ePH.pdf), generated with kicad-footprint-generator
connector JST PH side entry
0
8
8
Connector_JST
JST_PH_B8B-PH-SM4-TB_1x08-1MP_P2.00mm_Vertical
JST PH series connector, B8B-PH-SM4-TB (http://www.jst-mfg.com/product/pdf/eng/ePH.pdf), generated with kicad-footprint-generator
connector JST PH side entry
0
10
9
Connector_JST
JST_PH_B9B-PH-K_1x09_P2.00mm_Vertical
JST PH series connector, B9B-PH-K (http://www.jst-mfg.com/product/pdf/eng/ePH.pdf), generated with kicad-footprint-generator
connector JST PH side entry
0
9
9
Connector_JST
JST_PH_B9B-PH-SM4-TB_1x09-1MP_P2.00mm_Vertical
JST PH series connector, B9B-PH-SM4-TB (http://www.jst-mfg.com/product/pdf/eng/ePH.pdf), generated with kicad-footprint-generator
connector JST PH side entry
0
11
10
Connector_JST
JST_PH_B10B-PH-K_1x10_P2.00mm_Vertical
JST PH series connector, B10B-PH-K (http://www.jst-mfg.com/product/pdf/eng/ePH.pdf), generated with kicad-footprint-generator
connector JST PH side entry
0
10
10
Connector_JST
JST_PH_B10B-PH-SM4-TB_1x10-1MP_P2.00mm_Vertical
JST PH series connector, B10B-PH-SM4-TB (http://www.jst-mfg.com/product/pdf/eng/ePH.pdf), generated with kicad-footprint-generator
connector JST PH side entry
0
12
11
Connector_JST
JST_PH_B11B-PH-K_1x11_P2.00mm_Vertical
JST PH series connector, B11B-PH-K (http://www.jst-mfg.com/product/pdf/eng/ePH.pdf), generated with kicad-footprint-generator
connector JST PH side entry
0
11
11
Connector_JST
JST_PH_B11B-PH-SM4-TB_1x11-1MP_P2.00mm_Vertical
JST PH series connector, B11B-PH-SM4-TB (http://www.jst-mfg.com/product/pdf/eng/ePH.pdf), generated with kicad-footprint-generator
connector JST PH side entry
0
13
12
Connector_JST
JST_PH_B12B-PH-K_1x12_P2.00mm_Vertical
JST PH series connector, B12B-PH-K (http://www.jst-mfg.com/product/pdf/eng/ePH.pdf), generated with kicad-footprint-generator
connector JST PH side entry
0
12
12
Connector_JST
JST_PH_B12B-PH-SM4-TB_1x12-1MP_P2.00mm_Vertical
JST PH series connector, B12B-PH-SM4-TB (http://www.jst-mfg.com/product/pdf/eng/ePH.pdf), generated with kicad-footprint-generator
connector JST PH side entry
0
14
13
Connector_JST
JST_PH_B13B-PH-K_1x13_P2.00mm_Vertical
JST PH series connector, B13B-PH-K (http://www.jst-mfg.com/product/pdf/eng/ePH.pdf), generated with kicad-footprint-generator
connector JST PH side entry
0
13
13
Connector_JST
JST_PH_B13B-PH-SM4-TB_1x13-1MP_P2.00mm_Vertical
JST PH series connector, B13B-PH-SM4-TB (http://www.jst-mfg.com/product/pdf/eng/ePH.pdf), generated with kicad-footprint-generator
connector JST PH side entry
0
15
14
Connector_JST
JST_PH_B14B-PH-K_1x14_P2.00mm_Vertical
JST PH series connector, B14B-PH-K (http://www.jst-mfg.com/product/pdf/eng/ePH.pdf), generated with kicad-footprint-generator
connector JST PH side entry
0
14
14
Connector_JST
JST_PH_B14B-PH-SM4-TB_1x14-1MP_P2.00mm_Vertical
JST PH series connector, B14B-PH-SM4-TB (http://www.jst-mfg.com/product/pdf/eng/ePH.pdf), generated with kicad-footprint-generator
connector JST PH side entry
0
16
15
Connector_JST
JST_PH_B15B-PH-K_1x15_P2.00mm_Vertical
JST PH series connector, B15B-PH-K (http://www.jst-mfg.com/product/pdf/eng/ePH.pdf), generated with kicad-footprint-generator
connector JST PH side entry
0
15
15
Connector_JST
JST_PH_B15B-PH-SM4-TB_1x15-1MP_P2.00mm_Vertical
JST PH series connector, B15B-PH-SM4-TB (http://www.jst-mfg.com/product/pdf/eng/ePH.pdf), generated with kicad-footprint-generator
connector JST PH side entry
0
17
16
Connector_JST
JST_PH_B16B-PH-K_1x16_P2.00mm_Vertical
JST PH series connector, B16B-PH-K (http://www.jst-mfg.com/product/pdf/eng/ePH.pdf), generated with kicad-footprint-generator
connector JST PH side entry
0
16
16
Connector_JST
JST_PH_B16B-PH-SM4-TB_1x16-1MP_P2.00mm_Vertical
JST PH series connector, B16B-PH-SM4-TB (http://www.jst-mfg.com/product/pdf/eng/ePH.pdf), generated with kicad-footprint-generator
connector JST PH side entry
0
18
17
Connector_JST
JST_PH_S2B-PH-K_1x02_P2.00mm_Horizontal
JST PH series connector, S2B-PH-K (http://www.jst-mfg.com/product/pdf/eng/ePH.pdf), generated with kicad-footprint-generator
connector JST PH top entry
0
2
2
Connector_JST
JST_PH_S2B-PH-SM4-TB_1x02-1MP_P2.00mm_Horizontal
JST PH series connector, S2B-PH-SM4-TB (http://www.jst-mfg.com/product/pdf/eng/ePH.pdf), generated with kicad-footprint-generator
connector JST PH top entry
0
4
3
Connector_JST
JST_PH_S3B-PH-K_1x03_P2.00mm_Horizontal
JST PH series connector, S3B-PH-K (http://www.jst-mfg.com/product/pdf/eng/ePH.pdf), generated with kicad-footprint-generator
connector JST PH top entry
0
3
3
Connector_JST
JST_PH_S3B-PH-SM4-TB_1x03-1MP_P2.00mm_Horizontal
JST PH series connector, S3B-PH-SM4-TB (http://www.jst-mfg.com/product/pdf/eng/ePH.pdf), generated with kicad-footprint-generator
connector JST PH top entry
0
5
4
Connector_JST
JST_PH_S4B-PH-K_1x04_P2.00mm_Horizontal
JST PH series connector, S4B-PH-K (http://www.jst-mfg.com/product/pdf/eng/ePH.pdf), generated with kicad-footprint-generator
connector JST PH top entry
0
4
4
Connector_JST
JST_PH_S4B-PH-SM4-TB_1x04-1MP_P2.00mm_Horizontal
JST PH series connector, S4B-PH-SM4-TB (http://www.jst-mfg.com/product/pdf/eng/ePH.pdf), generated with kicad-footprint-generator
connector JST PH top entry
0
6
5
Connector_JST
JST_PH_S5B-PH-K_1x05_P2.00mm_Horizontal
JST PH series connector, S5B-PH-K (http://www.jst-mfg.com/product/pdf/eng/ePH.pdf), generated with kicad-footprint-generator
connector JST PH top entry
0
5
5
Connector_JST
JST_PH_S5B-PH-SM4-TB_1x05-1MP_P2.00mm_Horizontal
JST PH series connector, S5B-PH-SM4-TB (http://www.jst-mfg.com/product/pdf/eng/ePH.pdf), generated with kicad-footprint-generator
connector JST PH top entry
0
7
6
Connector_JST
JST_PH_S6B-PH-K_1x06_P2.00mm_Horizontal
JST PH series connector, S6B-PH-K (http://www.jst-mfg.com/product/pdf/eng/ePH.pdf), generated with kicad-footprint-generator
connector JST PH top entry
0
6
6
Connector_JST
JST_PH_S6B-PH-SM4-TB_1x06-1MP_P2.00mm_Horizontal
JST PH series connector, S6B-PH-SM4-TB (http://www.jst-mfg.com/product/pdf/eng/ePH.pdf), generated with kicad-footprint-generator
connector JST PH top entry
0
8
7
Connector_JST
JST_PH_S7B-PH-K_1x07_P2.00mm_Horizontal
JST PH series connector, S7B-PH-K (http://www.jst-mfg.com/product/pdf/eng/ePH.pdf), generated with kicad-footprint-generator
connector JST PH top entry
0
7
7
Connector_JST
JST_PH_S7B-PH-SM4-TB_1x07-1MP_P2.00mm_Horizontal
JST PH series connector, S7B-PH-SM4-TB (http://www.jst-mfg.com/product/pdf/eng/ePH.pdf), generated with kicad-footprint-generator
connector JST PH top entry
0
9
8
Connector_JST
JST_PH_S8B-PH-K_1x08_P2.00mm_Horizontal
JST PH series connector, S8B-PH-K (http://www.jst-mfg.com/product/pdf/eng/ePH.pdf), generated with kicad-footprint-generator
connector JST PH top entry
0
8
8
Connector_JST
JST_PH_S8B-PH-SM4-TB_1x08-1MP_P2.00mm_Horizontal
JST PH series connector, S8B-PH-SM4-TB (http://www.jst-mfg.com/product/pdf/eng/ePH.pdf), generated with kicad-footprint-generator
connector JST PH top entry
0
10
9
Connector_JST
JST_PH_S9B-PH-K_1x09_P2.00mm_Horizontal
JST PH series connector, S9B-PH-K (http://www.jst-mfg.com/product/pdf/eng/ePH.pdf), generated with kicad-footprint-generator
connector JST PH top entry
0
9
9
Connector_JST
JST_PH_S9B-PH-SM4-TB_1x09-1MP_P2.00mm_Horizontal
JST PH series connector, S9B-PH-SM4-TB (http://www.jst-mfg.com/product/pdf/eng/ePH.pdf), generated with kicad-footprint-generator
connector JST PH top entry
0
11
10
Connector_JST
JST_PH_S10B-PH-K_1x10_P2.00mm_Horizontal
JST PH series connector, S10B-PH-K (http://www.jst-mfg.com/product/pdf/eng/ePH.pdf), generated with kicad-footprint-generator
connector JST PH top entry
0
10
10
Connector_JST
JST_PH_S10B-PH-SM4-TB_1x10-1MP_P2.00mm_Horizontal
JST PH series connector, S10B-PH-SM4-TB (http://www.jst-mfg.com/product/pdf/eng/ePH.pdf), generated with kicad-footprint-generator
connector JST PH top entry
0
12
11
Connector_JST
JST_PH_S11B-PH-K_1x11_P2.00mm_Horizontal
JST PH series connector, S11B-PH-K (http://www.jst-mfg.com/product/pdf/eng/ePH.pdf), generated with kicad-footprint-generator
connector JST PH top entry
0
11
11
Connector_JST
JST_PH_S11B-PH-SM4-TB_1x11-1MP_P2.00mm_Horizontal
JST PH series connector, S11B-PH-SM4-TB (http://www.jst-mfg.com/product/pdf/eng/ePH.pdf), generated with kicad-footprint-generator
connector JST PH top entry
0
13
12
Connector_JST
JST_PH_S12B-PH-K_1x12_P2.00mm_Horizontal
JST PH series connector, S12B-PH-K (http://www.jst-mfg.com/product/pdf/eng/ePH.pdf), generated with kicad-footprint-generator
connector JST PH top entry
0
12
12
Connector_JST
JST_PH_S12B-PH-SM4-TB_1x12-1MP_P2.00mm_Horizontal
JST PH series connector, S12B-PH-SM4-TB (http://www.jst-mfg.com/product/pdf/eng/ePH.pdf), generated with kicad-footprint-generator
connector JST PH top entry
0
14
13
Connector_JST
JST_PH_S13B-PH-K_1x13_P2.00mm_Horizontal
JST PH series connector, S13B-PH-K (http://www.jst-mfg.com/product/pdf/eng/ePH.pdf), generated with kicad-footprint-generator
connector JST PH top entry
0
13
13
Connector_JST
JST_PH_S13B-PH-SM4-TB_1x13-1MP_P2.00mm_Horizontal
JST PH series connector, S13B-PH-SM4-TB (http://www.jst-mfg.com/product/pdf/eng/ePH.pdf), generated with kicad-footprint-generator
connector JST PH top entry
0
15
14
Connector_JST
JST_PH_S14B-PH-K_1x14_P2.00mm_Horizontal
JST PH series connector, S14B-PH-K (http://www.jst-mfg.com/product/pdf/eng/ePH.pdf), generated with kicad-footprint-generator
connector JST PH top entry
0
14
14
Connector_JST
JST_PH_S14B-PH-SM4-TB_1x14-1MP_P2.00mm_Horizontal
JST PH series connector, S14B-PH-SM4-TB (http://www.jst-mfg.com/product/pdf/eng/ePH.pdf), generated with kicad-footprint-generator
connector JST PH top entry
0
16
15
Connector_JST
JST_PH_S15B-PH-K_1x15_P2.00mm_Horizontal
JST PH series connector, S15B-PH-K (http://www.jst-mfg.com/product/pdf/eng/ePH.pdf), generated with kicad-footprint-generator
connector JST PH top entry
0
15
15
Connector_JST
JST_PH_S15B-PH-SM4-TB_1x15-1MP_P2.00mm_Horizontal
JST PH series connector, S15B-PH-SM4-TB (http://www.jst-mfg.com/product/pdf/eng/ePH.pdf), generated with kicad-footprint-generator
connector JST PH top entry
0
17
16
Connector_JST
JST_PH_S16B-PH-K_1x16_P2.00mm_Horizontal
JST PH series connector, S16B-PH-K (http://www.jst-mfg.com/product/pdf/eng/ePH.pdf), generated with kicad-footprint-generator
connector JST PH top entry
0
16
16
Connector_JST
JST_PUD_B08B-PUDSS_2x04_P2.00mm_Vertical
JST PUD series connector, B08B-PUDSS (http://www.jst-mfg.com/product/pdf/eng/ePUD.pdf), generated with kicad-footprint-generator
connector JST PUD side entry
0
8
8
Connector_JST
JST_PUD_B10B-PUDSS_2x05_P2.00mm_Vertical
JST PUD series connector, B10B-PUDSS (http://www.jst-mfg.com/product/pdf/eng/ePUD.pdf), generated with kicad-footprint-generator
connector JST PUD side entry
0
10
10
Connector_JST
JST_PUD_B12B-PUDSS_2x06_P2.00mm_Vertical
JST PUD series connector, B12B-PUDSS (http://www.jst-mfg.com/product/pdf/eng/ePUD.pdf), generated with kicad-footprint-generator
connector JST PUD side entry
0
12
12
Connector_JST
JST_PUD_B14B-PUDSS_2x07_P2.00mm_Vertical
JST PUD series connector, B14B-PUDSS (http://www.jst-mfg.com/product/pdf/eng/ePUD.pdf), generated with kicad-footprint-generator
connector JST PUD side entry
0
14
14
Connector_JST
JST_PUD_B16B-PUDSS_2x08_P2.00mm_Vertical
JST PUD series connector, B16B-PUDSS (http://www.jst-mfg.com/product/pdf/eng/ePUD.pdf), generated with kicad-footprint-generator
connector JST PUD side entry
0
16
16
Connector_JST
JST_PUD_B18B-PUDSS_2x09_P2.00mm_Vertical
JST PUD series connector, B18B-PUDSS (http://www.jst-mfg.com/product/pdf/eng/ePUD.pdf), generated with kicad-footprint-generator
connector JST PUD side entry
0
18
18
Connector_JST
JST_PUD_B20B-PUDSS_2x10_P2.00mm_Vertical
JST PUD series connector, B20B-PUDSS (http://www.jst-mfg.com/product/pdf/eng/ePUD.pdf), generated with kicad-footprint-generator
connector JST PUD side entry
0
20
20
Connector_JST
JST_PUD_B22B-PUDSS_2x11_P2.00mm_Vertical
JST PUD series connector, B22B-PUDSS (http://www.jst-mfg.com/product/pdf/eng/ePUD.pdf), generated with kicad-footprint-generator
connector JST PUD side entry
0
22
22
Connector_JST
JST_PUD_B24B-PUDSS_2x12_P2.00mm_Vertical
JST PUD series connector, B24B-PUDSS (http://www.jst-mfg.com/product/pdf/eng/ePUD.pdf), generated with kicad-footprint-generator
connector JST PUD side entry
0
24
24
Connector_JST
JST_PUD_B26B-PUDSS_2x13_P2.00mm_Vertical
JST PUD series connector, B26B-PUDSS (http://www.jst-mfg.com/product/pdf/eng/ePUD.pdf), generated with kicad-footprint-generator
connector JST PUD side entry
0
26
26
Connector_JST
JST_PUD_B28B-PUDSS_2x14_P2.00mm_Vertical
JST PUD series connector, B28B-PUDSS (http://www.jst-mfg.com/product/pdf/eng/ePUD.pdf), generated with kicad-footprint-generator
connector JST PUD side entry
0
28
28
Connector_JST
JST_PUD_B30B-PUDSS_2x15_P2.00mm_Vertical
JST PUD series connector, B30B-PUDSS (http://www.jst-mfg.com/product/pdf/eng/ePUD.pdf), generated with kicad-footprint-generator
connector JST PUD side entry
0
30
30
Connector_JST
JST_PUD_B32B-PUDSS_2x16_P2.00mm_Vertical
JST PUD series connector, B32B-PUDSS (http://www.jst-mfg.com/product/pdf/eng/ePUD.pdf), generated with kicad-footprint-generator
connector JST PUD side entry
0
32
32
Connector_JST
JST_PUD_B34B-PUDSS_2x17_P2.00mm_Vertical
JST PUD series connector, B34B-PUDSS (http://www.jst-mfg.com/product/pdf/eng/ePUD.pdf), generated with kicad-footprint-generator
connector JST PUD side entry
0
34
34
Connector_JST
JST_PUD_B36B-PUDSS_2x18_P2.00mm_Vertical
JST PUD series connector, B36B-PUDSS (http://www.jst-mfg.com/product/pdf/eng/ePUD.pdf), generated with kicad-footprint-generator
connector JST PUD side entry
0
36
36
Connector_JST
JST_PUD_B38B-PUDSS_2x19_P2.00mm_Vertical
JST PUD series connector, B38B-PUDSS (http://www.jst-mfg.com/product/pdf/eng/ePUD.pdf), generated with kicad-footprint-generator
connector JST PUD side entry
0
38
38
Connector_JST
JST_PUD_B40B-PUDSS_2x20_P2.00mm_Vertical
JST PUD series connector, B40B-PUDSS (http://www.jst-mfg.com/product/pdf/eng/ePUD.pdf), generated with kicad-footprint-generator
connector JST PUD side entry
0
40
40
Connector_JST
JST_PUD_S08B-PUDSS-1_2x04_P2.00mm_Horizontal
JST PUD series connector, S08B-PUDSS-1 (http://www.jst-mfg.com/product/pdf/eng/ePUD.pdf), generated with kicad-footprint-generator
connector JST PUD top entry
0
8
8
Connector_JST
JST_PUD_S10B-PUDSS-1_2x05_P2.00mm_Horizontal
JST PUD series connector, S10B-PUDSS-1 (http://www.jst-mfg.com/product/pdf/eng/ePUD.pdf), generated with kicad-footprint-generator
connector JST PUD top entry
0
10
10
Connector_JST
JST_PUD_S12B-PUDSS-1_2x06_P2.00mm_Horizontal
JST PUD series connector, S12B-PUDSS-1 (http://www.jst-mfg.com/product/pdf/eng/ePUD.pdf), generated with kicad-footprint-generator
connector JST PUD top entry
0
12
12
Connector_JST
JST_PUD_S14B-PUDSS-1_2x07_P2.00mm_Horizontal
JST PUD series connector, S14B-PUDSS-1 (http://www.jst-mfg.com/product/pdf/eng/ePUD.pdf), generated with kicad-footprint-generator
connector JST PUD top entry
0
14
14
Connector_JST
JST_PUD_S16B-PUDSS-1_2x08_P2.00mm_Horizontal
JST PUD series connector, S16B-PUDSS-1 (http://www.jst-mfg.com/product/pdf/eng/ePUD.pdf), generated with kicad-footprint-generator
connector JST PUD top entry
0
16
16
Connector_JST
JST_PUD_S18B-PUDSS-1_2x09_P2.00mm_Horizontal
JST PUD series connector, S18B-PUDSS-1 (http://www.jst-mfg.com/product/pdf/eng/ePUD.pdf), generated with kicad-footprint-generator
connector JST PUD top entry
0
18
18
Connector_JST
JST_PUD_S20B-PUDSS-1_2x10_P2.00mm_Horizontal
JST PUD series connector, S20B-PUDSS-1 (http://www.jst-mfg.com/product/pdf/eng/ePUD.pdf), generated with kicad-footprint-generator
connector JST PUD top entry
0
20
20
Connector_JST
JST_PUD_S22B-PUDSS-1_2x11_P2.00mm_Horizontal
JST PUD series connector, S22B-PUDSS-1 (http://www.jst-mfg.com/product/pdf/eng/ePUD.pdf), generated with kicad-footprint-generator
connector JST PUD top entry
0
22
22
Connector_JST
JST_PUD_S24B-PUDSS-1_2x12_P2.00mm_Horizontal
JST PUD series connector, S24B-PUDSS-1 (http://www.jst-mfg.com/product/pdf/eng/ePUD.pdf), generated with kicad-footprint-generator
connector JST PUD top entry
0
24
24
Connector_JST
JST_PUD_S26B-PUDSS-1_2x13_P2.00mm_Horizontal
JST PUD series connector, S26B-PUDSS-1 (http://www.jst-mfg.com/product/pdf/eng/ePUD.pdf), generated with kicad-footprint-generator
connector JST PUD top entry
0
26
26
Connector_JST
JST_PUD_S28B-PUDSS-1_2x14_P2.00mm_Horizontal
JST PUD series connector, S28B-PUDSS-1 (http://www.jst-mfg.com/product/pdf/eng/ePUD.pdf), generated with kicad-footprint-generator
connector JST PUD top entry
0
28
28
Connector_JST
JST_PUD_S30B-PUDSS-1_2x15_P2.00mm_Horizontal
JST PUD series connector, S30B-PUDSS-1 (http://www.jst-mfg.com/product/pdf/eng/ePUD.pdf), generated with kicad-footprint-generator
connector JST PUD top entry
0
30
30
Connector_JST
JST_PUD_S32B-PUDSS-1_2x16_P2.00mm_Horizontal
JST PUD series connector, S32B-PUDSS-1 (http://www.jst-mfg.com/product/pdf/eng/ePUD.pdf), generated with kicad-footprint-generator
connector JST PUD top entry
0
32
32
Connector_JST
JST_PUD_S34B-PUDSS-1_2x17_P2.00mm_Horizontal
JST PUD series connector, S34B-PUDSS-1 (http://www.jst-mfg.com/product/pdf/eng/ePUD.pdf), generated with kicad-footprint-generator
connector JST PUD top entry
0
34
34
Connector_JST
JST_PUD_S36B-PUDSS-1_2x18_P2.00mm_Horizontal
JST PUD series connector, S36B-PUDSS-1 (http://www.jst-mfg.com/product/pdf/eng/ePUD.pdf), generated with kicad-footprint-generator
connector JST PUD top entry
0
36
36
Connector_JST
JST_PUD_S38B-PUDSS-1_2x19_P2.00mm_Horizontal
JST PUD series connector, S38B-PUDSS-1 (http://www.jst-mfg.com/product/pdf/eng/ePUD.pdf), generated with kicad-footprint-generator
connector JST PUD top entry
0
38
38
Connector_JST
JST_PUD_S40B-PUDSS-1_2x20_P2.00mm_Horizontal
JST PUD series connector, S40B-PUDSS-1 (http://www.jst-mfg.com/product/pdf/eng/ePUD.pdf), generated with kicad-footprint-generator
connector JST PUD top entry
0
40
40
Connector_JST
JST_SFH_SM02B-SFHRS-TF_1x02-1MP_P4.20mm_Horizontal
JST SFH series connector, SM02B-SFHRS-TF (http://www.jst-mfg.com/product/pdf/eng/eSFH.pdf), generated with kicad-footprint-generator
connector JST SFH horizontal
0
4
3
Connector_JST
JST_SHL_SM02B-SHLS-TF_1x02-1MP_P1.00mm_Horizontal
JST SHL series connector, SM02B-SHLS-TF (http://www.jst-mfg.com/product/pdf/eng/eSHL.pdf), generated with kicad-footprint-generator
connector JST SHL top entry
0
4
3
Connector_JST
JST_SHL_SM05B-SHLS-TF_1x05-1MP_P1.00mm_Horizontal
JST SHL series connector, SM05B-SHLS-TF (http://www.jst-mfg.com/product/pdf/eng/eSHL.pdf), generated with kicad-footprint-generator
connector JST SHL top entry
0
7
6
Connector_JST
JST_SHL_SM06B-SHLS-TF_1x06-1MP_P1.00mm_Horizontal
JST SHL series connector, SM06B-SHLS-TF (http://www.jst-mfg.com/product/pdf/eng/eSHL.pdf), generated with kicad-footprint-generator
connector JST SHL top entry
0
8
7
Connector_JST
JST_SHL_SM07B-SHLS-TF_1x07-1MP_P1.00mm_Horizontal
JST SHL series connector, SM07B-SHLS-TF (http://www.jst-mfg.com/product/pdf/eng/eSHL.pdf), generated with kicad-footprint-generator
connector JST SHL top entry
0
9
8
Connector_JST
JST_SHL_SM08B-SHLS-TF_1x08-1MP_P1.00mm_Horizontal
JST SHL series connector, SM08B-SHLS-TF (http://www.jst-mfg.com/product/pdf/eng/eSHL.pdf), generated with kicad-footprint-generator
connector JST SHL top entry
0
10
9
Connector_JST
JST_SHL_SM10B-SHLS-TF_1x10-1MP_P1.00mm_Horizontal
JST SHL series connector, SM10B-SHLS-TF (http://www.jst-mfg.com/product/pdf/eng/eSHL.pdf), generated with kicad-footprint-generator
connector JST SHL top entry
0
12
11
Connector_JST
JST_SHL_SM11B-SHLS-TF_1x11-1MP_P1.00mm_Horizontal
JST SHL series connector, SM11B-SHLS-TF (http://www.jst-mfg.com/product/pdf/eng/eSHL.pdf), generated with kicad-footprint-generator
connector JST SHL top entry
0
13
12
Connector_JST
JST_SHL_SM12B-SHLS-TF_1x12-1MP_P1.00mm_Horizontal
JST SHL series connector, SM12B-SHLS-TF (http://www.jst-mfg.com/product/pdf/eng/eSHL.pdf), generated with kicad-footprint-generator
connector JST SHL top entry
0
14
13
Connector_JST
JST_SHL_SM14B-SHLS-TF_1x14-1MP_P1.00mm_Horizontal
JST SHL series connector, SM14B-SHLS-TF (http://www.jst-mfg.com/product/pdf/eng/eSHL.pdf), generated with kicad-footprint-generator
connector JST SHL top entry
0
16
15
Connector_JST
JST_SHL_SM16B-SHLS-TF_1x16-1MP_P1.00mm_Horizontal
JST SHL series connector, SM16B-SHLS-TF (http://www.jst-mfg.com/product/pdf/eng/eSHL.pdf), generated with kicad-footprint-generator
connector JST SHL top entry
0
18
17
Connector_JST
JST_SHL_SM20B-SHLS-TF_1x20-1MP_P1.00mm_Horizontal
JST SHL series connector, SM20B-SHLS-TF (http://www.jst-mfg.com/product/pdf/eng/eSHL.pdf), generated with kicad-footprint-generator
connector JST SHL top entry
0
22
21
Connector_JST
JST_SHL_SM22B-SHLS-TF_1x22-1MP_P1.00mm_Horizontal
JST SHL series connector, SM22B-SHLS-TF (http://www.jst-mfg.com/product/pdf/eng/eSHL.pdf), generated with kicad-footprint-generator
connector JST SHL top entry
0
24
23
Connector_JST
JST_SHL_SM26B-SHLS-TF_1x26-1MP_P1.00mm_Horizontal
JST SHL series connector, SM26B-SHLS-TF (http://www.jst-mfg.com/product/pdf/eng/eSHL.pdf), generated with kicad-footprint-generator
connector JST SHL top entry
0
28
27
Connector_JST
JST_SHL_SM30B-SHLS-TF_1x30-1MP_P1.00mm_Horizontal
JST SHL series connector, SM30B-SHLS-TF (http://www.jst-mfg.com/product/pdf/eng/eSHL.pdf), generated with kicad-footprint-generator
connector JST SHL top entry
0
32
31
Connector_JST
JST_SH_BM02B-SRSS-TB_1x02-1MP_P1.00mm_Vertical
JST SH series connector, BM02B-SRSS-TB (http://www.jst-mfg.com/product/pdf/eng/eSH.pdf), generated with kicad-footprint-generator
connector JST SH side entry
0
4
3
Connector_JST
JST_SH_BM03B-SRSS-TB_1x03-1MP_P1.00mm_Vertical
JST SH series connector, BM03B-SRSS-TB (http://www.jst-mfg.com/product/pdf/eng/eSH.pdf), generated with kicad-footprint-generator
connector JST SH side entry
0
5
4
Connector_JST
JST_SH_BM04B-SRSS-TB_1x04-1MP_P1.00mm_Vertical
JST SH series connector, BM04B-SRSS-TB (http://www.jst-mfg.com/product/pdf/eng/eSH.pdf), generated with kicad-footprint-generator
connector JST SH side entry
0
6
5
Connector_JST
JST_SH_BM05B-SRSS-TB_1x05-1MP_P1.00mm_Vertical
JST SH series connector, BM05B-SRSS-TB (http://www.jst-mfg.com/product/pdf/eng/eSH.pdf), generated with kicad-footprint-generator
connector JST SH side entry
0
7
6
Connector_JST
JST_SH_BM06B-SRSS-TB_1x06-1MP_P1.00mm_Vertical
JST SH series connector, BM06B-SRSS-TB (http://www.jst-mfg.com/product/pdf/eng/eSH.pdf), generated with kicad-footprint-generator
connector JST SH side entry
0
8
7
Connector_JST
JST_SH_BM07B-SRSS-TB_1x07-1MP_P1.00mm_Vertical
JST SH series connector, BM07B-SRSS-TB (http://www.jst-mfg.com/product/pdf/eng/eSH.pdf), generated with kicad-footprint-generator
connector JST SH side entry
0
9
8
Connector_JST
JST_SH_BM08B-SRSS-TB_1x08-1MP_P1.00mm_Vertical
JST SH series connector, BM08B-SRSS-TB (http://www.jst-mfg.com/product/pdf/eng/eSH.pdf), generated with kicad-footprint-generator
connector JST SH side entry
0
10
9
Connector_JST
JST_SH_BM09B-SRSS-TB_1x09-1MP_P1.00mm_Vertical
JST SH series connector, BM09B-SRSS-TB (http://www.jst-mfg.com/product/pdf/eng/eSH.pdf), generated with kicad-footprint-generator
connector JST SH side entry
0
11
10
Connector_JST
JST_SH_BM10B-SRSS-TB_1x10-1MP_P1.00mm_Vertical
JST SH series connector, BM10B-SRSS-TB (http://www.jst-mfg.com/product/pdf/eng/eSH.pdf), generated with kicad-footprint-generator
connector JST SH side entry
0
12
11
Connector_JST
JST_SH_BM11B-SRSS-TB_1x11-1MP_P1.00mm_Vertical
JST SH series connector, BM11B-SRSS-TB (http://www.jst-mfg.com/product/pdf/eng/eSH.pdf), generated with kicad-footprint-generator
connector JST SH side entry
0
13
12
Connector_JST
JST_SH_BM12B-SRSS-TB_1x12-1MP_P1.00mm_Vertical
JST SH series connector, BM12B-SRSS-TB (http://www.jst-mfg.com/product/pdf/eng/eSH.pdf), generated with kicad-footprint-generator
connector JST SH side entry
0
14
13
Connector_JST
JST_SH_BM13B-SRSS-TB_1x13-1MP_P1.00mm_Vertical
JST SH series connector, BM13B-SRSS-TB (http://www.jst-mfg.com/product/pdf/eng/eSH.pdf), generated with kicad-footprint-generator
connector JST SH side entry
0
15
14
Connector_JST
JST_SH_BM14B-SRSS-TB_1x14-1MP_P1.00mm_Vertical
JST SH series connector, BM14B-SRSS-TB (http://www.jst-mfg.com/product/pdf/eng/eSH.pdf), generated with kicad-footprint-generator
connector JST SH side entry
0
16
15
Connector_JST
JST_SH_BM15B-SRSS-TB_1x15-1MP_P1.00mm_Vertical
JST SH series connector, BM15B-SRSS-TB (http://www.jst-mfg.com/product/pdf/eng/eSH.pdf), generated with kicad-footprint-generator
connector JST SH side entry
0
17
16
Connector_JST
JST_SH_SM02B-SRSS-TB_1x02-1MP_P1.00mm_Horizontal
JST SH series connector, SM02B-SRSS-TB (http://www.jst-mfg.com/product/pdf/eng/eSH.pdf), generated with kicad-footprint-generator
connector JST SH top entry
0
4
3
Connector_JST
JST_SH_SM03B-SRSS-TB_1x03-1MP_P1.00mm_Horizontal
JST SH series connector, SM03B-SRSS-TB (http://www.jst-mfg.com/product/pdf/eng/eSH.pdf), generated with kicad-footprint-generator
connector JST SH top entry
0
5
4
Connector_JST
JST_SH_SM04B-SRSS-TB_1x04-1MP_P1.00mm_Horizontal
JST SH series connector, SM04B-SRSS-TB (http://www.jst-mfg.com/product/pdf/eng/eSH.pdf), generated with kicad-footprint-generator
connector JST SH top entry
0
6
5
Connector_JST
JST_SH_SM05B-SRSS-TB_1x05-1MP_P1.00mm_Horizontal
JST SH series connector, SM05B-SRSS-TB (http://www.jst-mfg.com/product/pdf/eng/eSH.pdf), generated with kicad-footprint-generator
connector JST SH top entry
0
7
6
Connector_JST
JST_SH_SM06B-SRSS-TB_1x06-1MP_P1.00mm_Horizontal
JST SH series connector, SM06B-SRSS-TB (http://www.jst-mfg.com/product/pdf/eng/eSH.pdf), generated with kicad-footprint-generator
connector JST SH top entry
0
8
7
Connector_JST
JST_SH_SM07B-SRSS-TB_1x07-1MP_P1.00mm_Horizontal
JST SH series connector, SM07B-SRSS-TB (http://www.jst-mfg.com/product/pdf/eng/eSH.pdf), generated with kicad-footprint-generator
connector JST SH top entry
0
9
8
Connector_JST
JST_SH_SM08B-SRSS-TB_1x08-1MP_P1.00mm_Horizontal
JST SH series connector, SM08B-SRSS-TB (http://www.jst-mfg.com/product/pdf/eng/eSH.pdf), generated with kicad-footprint-generator
connector JST SH top entry
0
10
9
Connector_JST
JST_SH_SM09B-SRSS-TB_1x09-1MP_P1.00mm_Horizontal
JST SH series connector, SM09B-SRSS-TB (http://www.jst-mfg.com/product/pdf/eng/eSH.pdf), generated with kicad-footprint-generator
connector JST SH top entry
0
11
10
Connector_JST
JST_SH_SM10B-SRSS-TB_1x10-1MP_P1.00mm_Horizontal
JST SH series connector, SM10B-SRSS-TB (http://www.jst-mfg.com/product/pdf/eng/eSH.pdf), generated with kicad-footprint-generator
connector JST SH top entry
0
12
11
Connector_JST
JST_SH_SM11B-SRSS-TB_1x11-1MP_P1.00mm_Horizontal
JST SH series connector, SM11B-SRSS-TB (http://www.jst-mfg.com/product/pdf/eng/eSH.pdf), generated with kicad-footprint-generator
connector JST SH top entry
0
13
12
Connector_JST
JST_SH_SM12B-SRSS-TB_1x12-1MP_P1.00mm_Horizontal
JST SH series connector, SM12B-SRSS-TB (http://www.jst-mfg.com/product/pdf/eng/eSH.pdf), generated with kicad-footprint-generator
connector JST SH top entry
0
14
13
Connector_JST
JST_SH_SM13B-SRSS-TB_1x13-1MP_P1.00mm_Horizontal
JST SH series connector, SM13B-SRSS-TB (http://www.jst-mfg.com/product/pdf/eng/eSH.pdf), generated with kicad-footprint-generator
connector JST SH top entry
0
15
14
Connector_JST
JST_SH_SM14B-SRSS-TB_1x14-1MP_P1.00mm_Horizontal
JST SH series connector, SM14B-SRSS-TB (http://www.jst-mfg.com/product/pdf/eng/eSH.pdf), generated with kicad-footprint-generator
connector JST SH top entry
0
16
15
Connector_JST
JST_SH_SM15B-SRSS-TB_1x15-1MP_P1.00mm_Horizontal
JST SH series connector, SM15B-SRSS-TB (http://www.jst-mfg.com/product/pdf/eng/eSH.pdf), generated with kicad-footprint-generator
connector JST SH top entry
0
17
16
Connector_JST
JST_SH_SM20B-SRSS-TB_1x20-1MP_P1.00mm_Horizontal
JST SH series connector, SM20B-SRSS-TB (http://www.jst-mfg.com/product/pdf/eng/eSH.pdf), generated with kicad-footprint-generator
connector JST SH top entry
0
22
21
Connector_JST
JST_SUR_BM02B-SURS-TF_1x02-1MP_P0.80mm_Vertical
JST SUR series connector, BM02B-SURS-TF (http://www.jst-mfg.com/product/pdf/eng/eSUR.pdf), generated with kicad-footprint-generator
connector JST SUR side entry
0
4
3
Connector_JST
JST_SUR_BM03B-SURS-TF_1x03-1MP_P0.80mm_Vertical
JST SUR series connector, BM03B-SURS-TF (http://www.jst-mfg.com/product/pdf/eng/eSUR.pdf), generated with kicad-footprint-generator
connector JST SUR side entry
0
5
4
Connector_JST
JST_SUR_BM04B-SURS-TF_1x04-1MP_P0.80mm_Vertical
JST SUR series connector, BM04B-SURS-TF (http://www.jst-mfg.com/product/pdf/eng/eSUR.pdf), generated with kicad-footprint-generator
connector JST SUR side entry
0
6
5
Connector_JST
JST_SUR_BM05B-SURS-TF_1x05-1MP_P0.80mm_Vertical
JST SUR series connector, BM05B-SURS-TF (http://www.jst-mfg.com/product/pdf/eng/eSUR.pdf), generated with kicad-footprint-generator
connector JST SUR side entry
0
7
6
Connector_JST
JST_SUR_BM06B-SURS-TF_1x06-1MP_P0.80mm_Vertical
JST SUR series connector, BM06B-SURS-TF (http://www.jst-mfg.com/product/pdf/eng/eSUR.pdf), generated with kicad-footprint-generator
connector JST SUR side entry
0
8
7
Connector_JST
JST_SUR_BM08B-SURS-TF_1x08-1MP_P0.80mm_Vertical
JST SUR series connector, BM08B-SURS-TF (http://www.jst-mfg.com/product/pdf/eng/eSUR.pdf), generated with kicad-footprint-generator
connector JST SUR side entry
0
10
9
Connector_JST
JST_SUR_BM10B-SURS-TF_1x10-1MP_P0.80mm_Vertical
JST SUR series connector, BM10B-SURS-TF (http://www.jst-mfg.com/product/pdf/eng/eSUR.pdf), generated with kicad-footprint-generator
connector JST SUR side entry
0
12
11
Connector_JST
JST_SUR_BM12B-SURS-TF_1x12-1MP_P0.80mm_Vertical
JST SUR series connector, BM12B-SURS-TF (http://www.jst-mfg.com/product/pdf/eng/eSUR.pdf), generated with kicad-footprint-generator
connector JST SUR side entry
0
14
13
Connector_JST
JST_SUR_BM14B-SURS-TF_1x14-1MP_P0.80mm_Vertical
JST SUR series connector, BM14B-SURS-TF (http://www.jst-mfg.com/product/pdf/eng/eSUR.pdf), generated with kicad-footprint-generator
connector JST SUR side entry
0
16
15
Connector_JST
JST_SUR_BM15B-SURS-TF_1x15-1MP_P0.80mm_Vertical
JST SUR series connector, BM15B-SURS-TF (http://www.jst-mfg.com/product/pdf/eng/eSUR.pdf), generated with kicad-footprint-generator
connector JST SUR side entry
0
17
16
Connector_JST
JST_SUR_BM16B-SURS-TF_1x16-1MP_P0.80mm_Vertical
JST SUR series connector, BM16B-SURS-TF (http://www.jst-mfg.com/product/pdf/eng/eSUR.pdf), generated with kicad-footprint-generator
connector JST SUR side entry
0
18
17
Connector_JST
JST_SUR_BM17B-SURS-TF_1x17-1MP_P0.80mm_Vertical
JST SUR series connector, BM17B-SURS-TF (http://www.jst-mfg.com/product/pdf/eng/eSUR.pdf), generated with kicad-footprint-generator
connector JST SUR side entry
0
19
18
Connector_JST
JST_SUR_BM20B-SURS-TF_1x20-1MP_P0.80mm_Vertical
JST SUR series connector, BM20B-SURS-TF (http://www.jst-mfg.com/product/pdf/eng/eSUR.pdf), generated with kicad-footprint-generator
connector JST SUR side entry
0
22
21
Connector_JST
JST_SUR_SM02B-SURS-TF_1x02-1MP_P0.80mm_Horizontal
JST SUR series connector, SM02B-SURS-TF (http://www.jst-mfg.com/product/pdf/eng/eSUR.pdf), generated with kicad-footprint-generator
connector JST SUR top entry
0
4
3
Connector_JST
JST_SUR_SM03B-SURS-TF_1x03-1MP_P0.80mm_Horizontal
JST SUR series connector, SM03B-SURS-TF (http://www.jst-mfg.com/product/pdf/eng/eSUR.pdf), generated with kicad-footprint-generator
connector JST SUR top entry
0
5
4
Connector_JST
JST_SUR_SM04B-SURS-TF_1x04-1MP_P0.80mm_Horizontal
JST SUR series connector, SM04B-SURS-TF (http://www.jst-mfg.com/product/pdf/eng/eSUR.pdf), generated with kicad-footprint-generator
connector JST SUR top entry
0
6
5
Connector_JST
JST_SUR_SM05B-SURS-TF_1x05-1MP_P0.80mm_Horizontal
JST SUR series connector, SM05B-SURS-TF (http://www.jst-mfg.com/product/pdf/eng/eSUR.pdf), generated with kicad-footprint-generator
connector JST SUR top entry
0
7
6
Connector_JST
JST_SUR_SM06B-SURS-TF_1x06-1MP_P0.80mm_Horizontal
JST SUR series connector, SM06B-SURS-TF (http://www.jst-mfg.com/product/pdf/eng/eSUR.pdf), generated with kicad-footprint-generator
connector JST SUR top entry
0
8
7
Connector_JST
JST_SUR_SM08B-SURS-TF_1x08-1MP_P0.80mm_Horizontal
JST SUR series connector, SM08B-SURS-TF (http://www.jst-mfg.com/product/pdf/eng/eSUR.pdf), generated with kicad-footprint-generator
connector JST SUR top entry
0
10
9
Connector_JST
JST_SUR_SM10B-SURS-TF_1x10-1MP_P0.80mm_Horizontal
JST SUR series connector, SM10B-SURS-TF (http://www.jst-mfg.com/product/pdf/eng/eSUR.pdf), generated with kicad-footprint-generator
connector JST SUR top entry
0
12
11
Connector_JST
JST_SUR_SM12B-SURS-TF_1x12-1MP_P0.80mm_Horizontal
JST SUR series connector, SM12B-SURS-TF (http://www.jst-mfg.com/product/pdf/eng/eSUR.pdf), generated with kicad-footprint-generator
connector JST SUR top entry
0
14
13
Connector_JST
JST_SUR_SM14B-SURS-TF_1x14-1MP_P0.80mm_Horizontal
JST SUR series connector, SM14B-SURS-TF (http://www.jst-mfg.com/product/pdf/eng/eSUR.pdf), generated with kicad-footprint-generator
connector JST SUR top entry
0
16
15
Connector_JST
JST_SUR_SM15B-SURS-TF_1x15-1MP_P0.80mm_Horizontal
JST SUR series connector, SM15B-SURS-TF (http://www.jst-mfg.com/product/pdf/eng/eSUR.pdf), generated with kicad-footprint-generator
connector JST SUR top entry
0
17
16
Connector_JST
JST_SUR_SM16B-SURS-TF_1x16-1MP_P0.80mm_Horizontal
JST SUR series connector, SM16B-SURS-TF (http://www.jst-mfg.com/product/pdf/eng/eSUR.pdf), generated with kicad-footprint-generator
connector JST SUR top entry
0
18
17
Connector_JST
JST_SUR_SM17B-SURS-TF_1x17-1MP_P0.80mm_Horizontal
JST SUR series connector, SM17B-SURS-TF (http://www.jst-mfg.com/product/pdf/eng/eSUR.pdf), generated with kicad-footprint-generator
connector JST SUR top entry
0
19
18
Connector_JST
JST_SUR_SM20B-SURS-TF_1x20-1MP_P0.80mm_Horizontal
JST SUR series connector, SM20B-SURS-TF (http://www.jst-mfg.com/product/pdf/eng/eSUR.pdf), generated with kicad-footprint-generator
connector JST SUR top entry
0
22
21
Connector_JST
JST_SUR_SM22B-SURS-TF_1x22-1MP_P0.80mm_Horizontal
JST SUR series connector, SM22B-SURS-TF (http://www.jst-mfg.com/product/pdf/eng/eSUR.pdf), generated with kicad-footprint-generator
connector JST SUR top entry
0
24
23
Connector_JST
JST_VH_B2P-VH-B_1x02_P3.96mm_Vertical
JST VH PBT series connector, B2P-VH-B (http://www.jst-mfg.com/product/pdf/eng/eVH.pdf), generated with kicad-footprint-generator
connector JST VH vertical
0
2
2
Connector_JST
JST_VH_B2P-VH-FB-B_1x02_P3.96mm_Vertical
JST VH series connector, B2P-VH-FB-B, shrouded (http://www.jst-mfg.com/product/pdf/eng/eVH.pdf),  generated with kicad-footprint-generator
connector JST VH side entry
0
2
2
Connector_JST
JST_VH_B2P-VH_1x02_P3.96mm_Vertical
JST VH series connector, B2P-VH (http://www.jst-mfg.com/product/pdf/eng/eVH.pdf), generated with kicad-footprint-generator
connector JST VH vertical
0
2
2
Connector_JST
JST_VH_B2P3-VH_1x02_P7.92mm_Vertical
JST VH series connector, B2P3-VH (http://www.jst-mfg.com/product/pdf/eng/eVH.pdf), generated with kicad-footprint-generator
connector JST VH vertical
0
2
2
Connector_JST
JST_VH_B2PS-VH_1x02_P3.96mm_Horizontal
JST VH series connector, B2PS-VH (http://www.jst-mfg.com/product/pdf/eng/eVH.pdf), generated with kicad-footprint-generator
connector JST VH top entry
0
2
2
Connector_JST
JST_VH_B3P-VH-B_1x03_P3.96mm_Vertical
JST VH PBT series connector, B3P-VH-B (http://www.jst-mfg.com/product/pdf/eng/eVH.pdf), generated with kicad-footprint-generator
connector JST VH vertical
0
3
3
Connector_JST
JST_VH_B3P-VH-FB-B_1x03_P3.96mm_Vertical
JST VH series connector, B3P-VH-FB-B, shrouded (http://www.jst-mfg.com/product/pdf/eng/eVH.pdf),  generated with kicad-footprint-generator
connector JST VH side entry
0
3
3
Connector_JST
JST_VH_B3P-VH_1x03_P3.96mm_Vertical
JST VH series connector, B3P-VH (http://www.jst-mfg.com/product/pdf/eng/eVH.pdf), generated with kicad-footprint-generator
connector JST VH vertical
0
3
3
Connector_JST
JST_VH_B3PS-VH_1x03_P3.96mm_Horizontal
JST VH series connector, B3PS-VH (http://www.jst-mfg.com/product/pdf/eng/eVH.pdf), generated with kicad-footprint-generator
connector JST VH top entry
0
3
3
Connector_JST
JST_VH_B4P-VH-B_1x04_P3.96mm_Vertical
JST VH PBT series connector, B4P-VH-B (http://www.jst-mfg.com/product/pdf/eng/eVH.pdf), generated with kicad-footprint-generator
connector JST VH vertical
0
4
4
Connector_JST
JST_VH_B4P-VH-FB-B_1x04_P3.96mm_Vertical
JST VH series connector, B4P-VH-FB-B, shrouded (http://www.jst-mfg.com/product/pdf/eng/eVH.pdf),  generated with kicad-footprint-generator
connector JST VH side entry
0
4
4
Connector_JST
JST_VH_B4P-VH_1x04_P3.96mm_Vertical
JST VH series connector, B4P-VH (http://www.jst-mfg.com/product/pdf/eng/eVH.pdf), generated with kicad-footprint-generator
connector JST VH vertical
0
4
4
Connector_JST
JST_VH_B4PS-VH_1x04_P3.96mm_Horizontal
JST VH series connector, B4PS-VH (http://www.jst-mfg.com/product/pdf/eng/eVH.pdf), generated with kicad-footprint-generator
connector JST VH top entry
0
4
4
Connector_JST
JST_VH_B5P-VH-B_1x05_P3.96mm_Vertical
JST VH PBT series connector, B5P-VH-B (http://www.jst-mfg.com/product/pdf/eng/eVH.pdf), generated with kicad-footprint-generator
connector JST VH vertical
0
5
5
Connector_JST
JST_VH_B5P-VH-FB-B_1x05_P3.96mm_Vertical
JST VH series connector, B5P-VH-FB-B, shrouded (http://www.jst-mfg.com/product/pdf/eng/eVH.pdf),  generated with kicad-footprint-generator
connector JST VH side entry
0
5
5
Connector_JST
JST_VH_B5P-VH_1x05_P3.96mm_Vertical
JST VH series connector, B5P-VH (http://www.jst-mfg.com/product/pdf/eng/eVH.pdf), generated with kicad-footprint-generator
connector JST VH vertical
0
5
5
Connector_JST
JST_VH_B5PS-VH_1x05_P3.96mm_Horizontal
JST VH series connector, B5PS-VH (http://www.jst-mfg.com/product/pdf/eng/eVH.pdf), generated with kicad-footprint-generator
connector JST VH top entry
0
5
5
Connector_JST
JST_VH_B6P-VH-B_1x06_P3.96mm_Vertical
JST VH PBT series connector, B6P-VH-B (http://www.jst-mfg.com/product/pdf/eng/eVH.pdf), generated with kicad-footprint-generator
connector JST VH vertical
0
6
6
Connector_JST
JST_VH_B6P-VH-FB-B_1x06_P3.96mm_Vertical
JST VH series connector, B6P-VH-FB-B, shrouded (http://www.jst-mfg.com/product/pdf/eng/eVH.pdf),  generated with kicad-footprint-generator
connector JST VH side entry
0
6
6
Connector_JST
JST_VH_B6P-VH_1x06_P3.96mm_Vertical
JST VH series connector, B6P-VH (http://www.jst-mfg.com/product/pdf/eng/eVH.pdf), generated with kicad-footprint-generator
connector JST VH vertical
0
6
6
Connector_JST
JST_VH_B6PS-VH_1x06_P3.96mm_Horizontal
JST VH series connector, B6PS-VH (http://www.jst-mfg.com/product/pdf/eng/eVH.pdf), generated with kicad-footprint-generator
connector JST VH top entry
0
6
6
Connector_JST
JST_VH_B7P-VH-B_1x07_P3.96mm_Vertical
JST VH PBT series connector, B7P-VH-B (http://www.jst-mfg.com/product/pdf/eng/eVH.pdf), generated with kicad-footprint-generator
connector JST VH vertical
0
7
7
Connector_JST
JST_VH_B7P-VH-FB-B_1x07_P3.96mm_Vertical
JST VH series connector, B7P-VH-FB-B, shrouded (http://www.jst-mfg.com/product/pdf/eng/eVH.pdf),  generated with kicad-footprint-generator
connector JST VH side entry
0
7
7
Connector_JST
JST_VH_B7P-VH_1x07_P3.96mm_Vertical
JST VH series connector, B7P-VH (http://www.jst-mfg.com/product/pdf/eng/eVH.pdf), generated with kicad-footprint-generator
connector JST VH vertical
0
7
7
Connector_JST
JST_VH_B7PS-VH_1x07_P3.96mm_Horizontal
JST VH series connector, B7PS-VH (http://www.jst-mfg.com/product/pdf/eng/eVH.pdf), generated with kicad-footprint-generator
connector JST VH top entry
0
7
7
Connector_JST
JST_VH_B8P-VH-B_1x08_P3.96mm_Vertical
JST VH PBT series connector, B8P-VH-B (http://www.jst-mfg.com/product/pdf/eng/eVH.pdf), generated with kicad-footprint-generator
connector JST VH vertical
0
8
8
Connector_JST
JST_VH_B8P-VH-FB-B_1x08_P3.96mm_Vertical
JST VH series connector, B8P-VH-FB-B, shrouded (http://www.jst-mfg.com/product/pdf/eng/eVH.pdf),  generated with kicad-footprint-generator
connector JST VH side entry
0
8
8
Connector_JST
JST_VH_B8P-VH_1x08_P3.96mm_Vertical
JST VH series connector, B8P-VH (http://www.jst-mfg.com/product/pdf/eng/eVH.pdf), generated with kicad-footprint-generator
connector JST VH vertical
0
8
8
Connector_JST
JST_VH_B8PS-VH_1x08_P3.96mm_Horizontal
JST VH series connector, B8PS-VH (http://www.jst-mfg.com/product/pdf/eng/eVH.pdf), generated with kicad-footprint-generator
connector JST VH top entry
0
8
8
Connector_JST
JST_VH_B9P-VH-B_1x09_P3.96mm_Vertical
JST VH PBT series connector, B9P-VH-B (http://www.jst-mfg.com/product/pdf/eng/eVH.pdf), generated with kicad-footprint-generator
connector JST VH vertical
0
9
9
Connector_JST
JST_VH_B9P-VH-FB-B_1x09_P3.96mm_Vertical
JST VH series connector, B9P-VH-FB-B, shrouded (http://www.jst-mfg.com/product/pdf/eng/eVH.pdf),  generated with kicad-footprint-generator
connector JST VH side entry
0
9
9
Connector_JST
JST_VH_B9P-VH_1x09_P3.96mm_Vertical
JST VH series connector, B9P-VH (http://www.jst-mfg.com/product/pdf/eng/eVH.pdf), generated with kicad-footprint-generator
connector JST VH vertical
0
9
9
Connector_JST
JST_VH_B9PS-VH_1x09_P3.96mm_Horizontal
JST VH series connector, B9PS-VH (http://www.jst-mfg.com/product/pdf/eng/eVH.pdf), generated with kicad-footprint-generator
connector JST VH top entry
0
9
9
Connector_JST
JST_VH_B10P-VH-B_1x10_P3.96mm_Vertical
JST VH PBT series connector, B10P-VH-B (http://www.jst-mfg.com/product/pdf/eng/eVH.pdf), generated with kicad-footprint-generator
connector JST VH vertical
0
10
10
Connector_JST
JST_VH_B10P-VH-FB-B_1x10_P3.96mm_Vertical
JST VH series connector, B10P-VH-FB-B, shrouded (http://www.jst-mfg.com/product/pdf/eng/eVH.pdf),  generated with kicad-footprint-generator
connector JST VH side entry
0
10
10
Connector_JST
JST_VH_B10P-VH_1x10_P3.96mm_Vertical
JST VH series connector, B10P-VH (http://www.jst-mfg.com/product/pdf/eng/eVH.pdf), generated with kicad-footprint-generator
connector JST VH vertical
0
10
10
Connector_JST
JST_VH_B10PS-VH_1x10_P3.96mm_Horizontal
JST VH series connector, B10PS-VH (http://www.jst-mfg.com/product/pdf/eng/eVH.pdf), generated with kicad-footprint-generator
connector JST VH top entry
0
10
10
Connector_JST
JST_VH_B11P-VH-B_1x11_P3.96mm_Vertical
JST VH PBT series connector, B11P-VH-B (http://www.jst-mfg.com/product/pdf/eng/eVH.pdf), generated with kicad-footprint-generator
connector JST VH vertical
0
11
11
Connector_JST
JST_VH_S2P-VH_1x02_P3.96mm_Horizontal
JST VH series connector, S2P-VH (http://www.jst-mfg.com/product/pdf/eng/eVH.pdf), generated with kicad-footprint-generator
connector JST VH top entry
0
2
2
Connector_JST
JST_VH_S3P-VH_1x03_P3.96mm_Horizontal
JST VH series connector, S3P-VH (http://www.jst-mfg.com/product/pdf/eng/eVH.pdf), generated with kicad-footprint-generator
connector JST VH top entry
0
3
3
Connector_JST
JST_VH_S4P-VH_1x04_P3.96mm_Horizontal
JST VH series connector, S4P-VH (http://www.jst-mfg.com/product/pdf/eng/eVH.pdf), generated with kicad-footprint-generator
connector JST VH top entry
0
4
4
Connector_JST
JST_VH_S5P-VH_1x05_P3.96mm_Horizontal
JST VH series connector, S5P-VH (http://www.jst-mfg.com/product/pdf/eng/eVH.pdf), generated with kicad-footprint-generator
connector JST VH top entry
0
5
5
Connector_JST
JST_VH_S6P-VH_1x06_P3.96mm_Horizontal
JST VH series connector, S6P-VH (http://www.jst-mfg.com/product/pdf/eng/eVH.pdf), generated with kicad-footprint-generator
connector JST VH top entry
0
6
6
Connector_JST
JST_VH_S7P-VH_1x07_P3.96mm_Horizontal
JST VH series connector, S7P-VH (http://www.jst-mfg.com/product/pdf/eng/eVH.pdf), generated with kicad-footprint-generator
connector JST VH top entry
0
7
7
Connector_JST
JST_XAG_SM05B-XAGKS-BN-TB_1x05-1MP_P2.50mm_Horizontal
JST XAG series connector, SM05B-XAGKS-BN-TB (http://www.jst-mfg.com/product/pdf/eng/eXAG.pdf), generated with kicad-footprint-generator
connector JST XAG top entry
0
7
6
Connector_JST
JST_XA_B02B-XASK-1-A_1x02_P2.50mm_Vertical
JST XA series connector, B02B-XASK-1-A (http://www.jst-mfg.com/product/pdf/eng/eXA1.pdf), generated with kicad-footprint-generator
connector JST XA vertical boss
0
2
2
Connector_JST
JST_XA_B02B-XASK-1_1x02_P2.50mm_Vertical
JST XA series connector, B02B-XASK-1 (http://www.jst-mfg.com/product/pdf/eng/eXA1.pdf), generated with kicad-footprint-generator
connector JST XA vertical
0
2
2
Connector_JST
JST_XA_B03B-XASK-1-A_1x03_P2.50mm_Vertical
JST XA series connector, B03B-XASK-1-A (http://www.jst-mfg.com/product/pdf/eng/eXA1.pdf), generated with kicad-footprint-generator
connector JST XA vertical boss
0
3
3
Connector_JST
JST_XA_B03B-XASK-1_1x03_P2.50mm_Vertical
JST XA series connector, B03B-XASK-1 (http://www.jst-mfg.com/product/pdf/eng/eXA1.pdf), generated with kicad-footprint-generator
connector JST XA vertical
0
3
3
Connector_JST
JST_XA_B04B-XASK-1-A_1x04_P2.50mm_Vertical
JST XA series connector, B04B-XASK-1-A (http://www.jst-mfg.com/product/pdf/eng/eXA1.pdf), generated with kicad-footprint-generator
connector JST XA vertical boss
0
4
4
Connector_JST
JST_XA_B04B-XASK-1_1x04_P2.50mm_Vertical
JST XA series connector, B04B-XASK-1 (http://www.jst-mfg.com/product/pdf/eng/eXA1.pdf), generated with kicad-footprint-generator
connector JST XA vertical
0
4
4
Connector_JST
JST_XA_B05B-XASK-1-A_1x05_P2.50mm_Vertical
JST XA series connector, B05B-XASK-1-A (http://www.jst-mfg.com/product/pdf/eng/eXA1.pdf), generated with kicad-footprint-generator
connector JST XA vertical boss
0
5
5
Connector_JST
JST_XA_B05B-XASK-1_1x05_P2.50mm_Vertical
JST XA series connector, B05B-XASK-1 (http://www.jst-mfg.com/product/pdf/eng/eXA1.pdf), generated with kicad-footprint-generator
connector JST XA vertical
0
5
5
Connector_JST
JST_XA_B06B-XASK-1-A_1x06_P2.50mm_Vertical
JST XA series connector, B06B-XASK-1-A (http://www.jst-mfg.com/product/pdf/eng/eXA1.pdf), generated with kicad-footprint-generator
connector JST XA vertical boss
0
6
6
Connector_JST
JST_XA_B06B-XASK-1_1x06_P2.50mm_Vertical
JST XA series connector, B06B-XASK-1 (http://www.jst-mfg.com/product/pdf/eng/eXA1.pdf), generated with kicad-footprint-generator
connector JST XA vertical
0
6
6
Connector_JST
JST_XA_B07B-XASK-1-A_1x07_P2.50mm_Vertical
JST XA series connector, B07B-XASK-1-A (http://www.jst-mfg.com/product/pdf/eng/eXA1.pdf), generated with kicad-footprint-generator
connector JST XA vertical boss
0
7
7
Connector_JST
JST_XA_B07B-XASK-1_1x07_P2.50mm_Vertical
JST XA series connector, B07B-XASK-1 (http://www.jst-mfg.com/product/pdf/eng/eXA1.pdf), generated with kicad-footprint-generator
connector JST XA vertical
0
7
7
Connector_JST
JST_XA_B08B-XASK-1-A_1x08_P2.50mm_Vertical
JST XA series connector, B08B-XASK-1-A (http://www.jst-mfg.com/product/pdf/eng/eXA1.pdf), generated with kicad-footprint-generator
connector JST XA vertical boss
0
8
8
Connector_JST
JST_XA_B08B-XASK-1_1x08_P2.50mm_Vertical
JST XA series connector, B08B-XASK-1 (http://www.jst-mfg.com/product/pdf/eng/eXA1.pdf), generated with kicad-footprint-generator
connector JST XA vertical
0
8
8
Connector_JST
JST_XA_B09B-XASK-1-A_1x09_P2.50mm_Vertical
JST XA series connector, B09B-XASK-1-A (http://www.jst-mfg.com/product/pdf/eng/eXA1.pdf), generated with kicad-footprint-generator
connector JST XA vertical boss
0
9
9
Connector_JST
JST_XA_B09B-XASK-1_1x09_P2.50mm_Vertical
JST XA series connector, B09B-XASK-1 (http://www.jst-mfg.com/product/pdf/eng/eXA1.pdf), generated with kicad-footprint-generator
connector JST XA vertical
0
9
9
Connector_JST
JST_XA_B10B-XASK-1-A_1x10_P2.50mm_Vertical
JST XA series connector, B10B-XASK-1-A (http://www.jst-mfg.com/product/pdf/eng/eXA1.pdf), generated with kicad-footprint-generator
connector JST XA vertical boss
0
10
10
Connector_JST
JST_XA_B10B-XASK-1_1x10_P2.50mm_Vertical
JST XA series connector, B10B-XASK-1 (http://www.jst-mfg.com/product/pdf/eng/eXA1.pdf), generated with kicad-footprint-generator
connector JST XA vertical
0
10
10
Connector_JST
JST_XA_B11B-XASK-1-A_1x11_P2.50mm_Vertical
JST XA series connector, B11B-XASK-1-A (http://www.jst-mfg.com/product/pdf/eng/eXA1.pdf), generated with kicad-footprint-generator
connector JST XA vertical boss
0
11
11
Connector_JST
JST_XA_B11B-XASK-1_1x11_P2.50mm_Vertical
JST XA series connector, B11B-XASK-1 (http://www.jst-mfg.com/product/pdf/eng/eXA1.pdf), generated with kicad-footprint-generator
connector JST XA vertical
0
11
11
Connector_JST
JST_XA_B12B-XASK-1-A_1x12_P2.50mm_Vertical
JST XA series connector, B12B-XASK-1-A (http://www.jst-mfg.com/product/pdf/eng/eXA1.pdf), generated with kicad-footprint-generator
connector JST XA vertical boss
0
12
12
Connector_JST
JST_XA_B12B-XASK-1_1x12_P2.50mm_Vertical
JST XA series connector, B12B-XASK-1 (http://www.jst-mfg.com/product/pdf/eng/eXA1.pdf), generated with kicad-footprint-generator
connector JST XA vertical
0
12
12
Connector_JST
JST_XA_B13B-XASK-1-A_1x13_P2.50mm_Vertical
JST XA series connector, B13B-XASK-1-A (http://www.jst-mfg.com/product/pdf/eng/eXA1.pdf), generated with kicad-footprint-generator
connector JST XA vertical boss
0
13
13
Connector_JST
JST_XA_B13B-XASK-1_1x13_P2.50mm_Vertical
JST XA series connector, B13B-XASK-1 (http://www.jst-mfg.com/product/pdf/eng/eXA1.pdf), generated with kicad-footprint-generator
connector JST XA vertical
0
13
13
Connector_JST
JST_XA_B14B-XASK-1-A_1x14_P2.50mm_Vertical
JST XA series connector, B14B-XASK-1-A (http://www.jst-mfg.com/product/pdf/eng/eXA1.pdf), generated with kicad-footprint-generator
connector JST XA vertical boss
0
14
14
Connector_JST
JST_XA_B14B-XASK-1_1x14_P2.50mm_Vertical
JST XA series connector, B14B-XASK-1 (http://www.jst-mfg.com/product/pdf/eng/eXA1.pdf), generated with kicad-footprint-generator
connector JST XA vertical
0
14
14
Connector_JST
JST_XA_B15B-XASK-1-A_1x15_P2.50mm_Vertical
JST XA series connector, B15B-XASK-1-A (http://www.jst-mfg.com/product/pdf/eng/eXA1.pdf), generated with kicad-footprint-generator
connector JST XA vertical boss
0
15
15
Connector_JST
JST_XA_B15B-XASK-1_1x15_P2.50mm_Vertical
JST XA series connector, B15B-XASK-1 (http://www.jst-mfg.com/product/pdf/eng/eXA1.pdf), generated with kicad-footprint-generator
connector JST XA vertical
0
15
15
Connector_JST
JST_XA_B18B-XASK-1_1x18_P2.50mm_Vertical
JST XA series connector, B18B-XASK-1 (http://www.jst-mfg.com/product/pdf/eng/eXA1.pdf), generated with kicad-footprint-generator
connector JST XA vertical
0
18
18
Connector_JST
JST_XA_B20B-XASK-1-A_1x20_P2.50mm_Vertical
JST XA series connector, B20B-XASK-1-A (http://www.jst-mfg.com/product/pdf/eng/eXA1.pdf), generated with kicad-footprint-generator
connector JST XA vertical boss
0
20
20
Connector_JST
JST_XA_B20B-XASK-1_1x20_P2.50mm_Vertical
JST XA series connector, B20B-XASK-1 (http://www.jst-mfg.com/product/pdf/eng/eXA1.pdf), generated with kicad-footprint-generator
connector JST XA vertical
0
20
20
Connector_JST
JST_XA_S02B-XASK-1N-BN_1x02_P2.50mm_Horizontal
JST XA series connector, S02B-XASK-1N-BN (http://www.jst-mfg.com/product/pdf/eng/eXA1.pdf), generated with kicad-footprint-generator
connector JST XA horizontal
0
2
2
Connector_JST
JST_XA_S02B-XASK-1_1x02_P2.50mm_Horizontal
JST XA series connector, S02B-XASK-1 (http://www.jst-mfg.com/product/pdf/eng/eXA1.pdf), generated with kicad-footprint-generator
connector JST XA horizontal hook
0
2
2
Connector_JST
JST_XA_S03B-XASK-1N-BN_1x03_P2.50mm_Horizontal
JST XA series connector, S03B-XASK-1N-BN (http://www.jst-mfg.com/product/pdf/eng/eXA1.pdf), generated with kicad-footprint-generator
connector JST XA horizontal
0
3
3
Connector_JST
JST_XA_S03B-XASK-1_1x03_P2.50mm_Horizontal
JST XA series connector, S03B-XASK-1 (http://www.jst-mfg.com/product/pdf/eng/eXA1.pdf), generated with kicad-footprint-generator
connector JST XA horizontal hook
0
3
3
Connector_JST
JST_XA_S04B-XASK-1N-BN_1x04_P2.50mm_Horizontal
JST XA series connector, S04B-XASK-1N-BN (http://www.jst-mfg.com/product/pdf/eng/eXA1.pdf), generated with kicad-footprint-generator
connector JST XA horizontal
0
4
4
Connector_JST
JST_XA_S04B-XASK-1_1x04_P2.50mm_Horizontal
JST XA series connector, S04B-XASK-1 (http://www.jst-mfg.com/product/pdf/eng/eXA1.pdf), generated with kicad-footprint-generator
connector JST XA horizontal hook
0
4
4
Connector_JST
JST_XA_S05B-XASK-1N-BN_1x05_P2.50mm_Horizontal
JST XA series connector, S05B-XASK-1N-BN (http://www.jst-mfg.com/product/pdf/eng/eXA1.pdf), generated with kicad-footprint-generator
connector JST XA horizontal
0
5
5
Connector_JST
JST_XA_S05B-XASK-1_1x05_P2.50mm_Horizontal
JST XA series connector, S05B-XASK-1 (http://www.jst-mfg.com/product/pdf/eng/eXA1.pdf), generated with kicad-footprint-generator
connector JST XA horizontal hook
0
5
5
Connector_JST
JST_XA_S06B-XASK-1N-BN_1x06_P2.50mm_Horizontal
JST XA series connector, S06B-XASK-1N-BN (http://www.jst-mfg.com/product/pdf/eng/eXA1.pdf), generated with kicad-footprint-generator
connector JST XA horizontal
0
6
6
Connector_JST
JST_XA_S06B-XASK-1_1x06_P2.50mm_Horizontal
JST XA series connector, S06B-XASK-1 (http://www.jst-mfg.com/product/pdf/eng/eXA1.pdf), generated with kicad-footprint-generator
connector JST XA horizontal hook
0
6
6
Connector_JST
JST_XA_S07B-XASK-1N-BN_1x07_P2.50mm_Horizontal
JST XA series connector, S07B-XASK-1N-BN (http://www.jst-mfg.com/product/pdf/eng/eXA1.pdf), generated with kicad-footprint-generator
connector JST XA horizontal
0
7
7
Connector_JST
JST_XA_S07B-XASK-1_1x07_P2.50mm_Horizontal
JST XA series connector, S07B-XASK-1 (http://www.jst-mfg.com/product/pdf/eng/eXA1.pdf), generated with kicad-footprint-generator
connector JST XA horizontal hook
0
7
7
Connector_JST
JST_XA_S08B-XASK-1N-BN_1x08_P2.50mm_Horizontal
JST XA series connector, S08B-XASK-1N-BN (http://www.jst-mfg.com/product/pdf/eng/eXA1.pdf), generated with kicad-footprint-generator
connector JST XA horizontal
0
8
8
Connector_JST
JST_XA_S08B-XASK-1_1x08_P2.50mm_Horizontal
JST XA series connector, S08B-XASK-1 (http://www.jst-mfg.com/product/pdf/eng/eXA1.pdf), generated with kicad-footprint-generator
connector JST XA horizontal hook
0
8
8
Connector_JST
JST_XA_S09B-XASK-1N-BN_1x09_P2.50mm_Horizontal
JST XA series connector, S09B-XASK-1N-BN (http://www.jst-mfg.com/product/pdf/eng/eXA1.pdf), generated with kicad-footprint-generator
connector JST XA horizontal
0
9
9
Connector_JST
JST_XA_S09B-XASK-1_1x09_P2.50mm_Horizontal
JST XA series connector, S09B-XASK-1 (http://www.jst-mfg.com/product/pdf/eng/eXA1.pdf), generated with kicad-footprint-generator
connector JST XA horizontal hook
0
9
9
Connector_JST
JST_XA_S10B-XASK-1N-BN_1x10_P2.50mm_Horizontal
JST XA series connector, S10B-XASK-1N-BN (http://www.jst-mfg.com/product/pdf/eng/eXA1.pdf), generated with kicad-footprint-generator
connector JST XA horizontal
0
10
10
Connector_JST
JST_XA_S10B-XASK-1_1x10_P2.50mm_Horizontal
JST XA series connector, S10B-XASK-1 (http://www.jst-mfg.com/product/pdf/eng/eXA1.pdf), generated with kicad-footprint-generator
connector JST XA horizontal hook
0
10
10
Connector_JST
JST_XA_S11B-XASK-1N-BN_1x11_P2.50mm_Horizontal
JST XA series connector, S11B-XASK-1N-BN (http://www.jst-mfg.com/product/pdf/eng/eXA1.pdf), generated with kicad-footprint-generator
connector JST XA horizontal
0
11
11
Connector_JST
JST_XA_S11B-XASK-1_1x11_P2.50mm_Horizontal
JST XA series connector, S11B-XASK-1 (http://www.jst-mfg.com/product/pdf/eng/eXA1.pdf), generated with kicad-footprint-generator
connector JST XA horizontal hook
0
11
11
Connector_JST
JST_XA_S12B-XASK-1N-BN_1x12_P2.50mm_Horizontal
JST XA series connector, S12B-XASK-1N-BN (http://www.jst-mfg.com/product/pdf/eng/eXA1.pdf), generated with kicad-footprint-generator
connector JST XA horizontal
0
12
12
Connector_JST
JST_XA_S12B-XASK-1_1x12_P2.50mm_Horizontal
JST XA series connector, S12B-XASK-1 (http://www.jst-mfg.com/product/pdf/eng/eXA1.pdf), generated with kicad-footprint-generator
connector JST XA horizontal hook
0
12
12
Connector_JST
JST_XA_S13B-XASK-1N-BN_1x13_P2.50mm_Horizontal
JST XA series connector, S13B-XASK-1N-BN (http://www.jst-mfg.com/product/pdf/eng/eXA1.pdf), generated with kicad-footprint-generator
connector JST XA horizontal
0
13
13
Connector_JST
JST_XA_S13B-XASK-1_1x13_P2.50mm_Horizontal
JST XA series connector, S13B-XASK-1 (http://www.jst-mfg.com/product/pdf/eng/eXA1.pdf), generated with kicad-footprint-generator
connector JST XA horizontal hook
0
13
13
Connector_JST
JST_XA_S14B-XASK-1N-BN_1x14_P2.50mm_Horizontal
JST XA series connector, S14B-XASK-1N-BN (http://www.jst-mfg.com/product/pdf/eng/eXA1.pdf), generated with kicad-footprint-generator
connector JST XA horizontal
0
14
14
Connector_JST
JST_XA_S14B-XASK-1_1x14_P2.50mm_Horizontal
JST XA series connector, S14B-XASK-1 (http://www.jst-mfg.com/product/pdf/eng/eXA1.pdf), generated with kicad-footprint-generator
connector JST XA horizontal hook
0
14
14
Connector_JST
JST_XH_B1B-XH-AM_1x01_P2.50mm_Vertical
JST XH series connector, B1B-XH-AM, with boss (http://www.jst-mfg.com/product/pdf/eng/eXH.pdf), generated with kicad-footprint-generator
connector JST XH vertical boss
0
1
1
Connector_JST
JST_XH_B2B-XH-AM_1x02_P2.50mm_Vertical
JST XH series connector, B2B-XH-AM, with boss (http://www.jst-mfg.com/product/pdf/eng/eXH.pdf), generated with kicad-footprint-generator
connector JST XH vertical boss
0
2
2
Connector_JST
JST_XH_B2B-XH-A_1x02_P2.50mm_Vertical
JST XH series connector, B2B-XH-A (http://www.jst-mfg.com/product/pdf/eng/eXH.pdf), generated with kicad-footprint-generator
connector JST XH vertical
0
2
2
Connector_JST
JST_XH_B3B-XH-AM_1x03_P2.50mm_Vertical
JST XH series connector, B3B-XH-AM, with boss (http://www.jst-mfg.com/product/pdf/eng/eXH.pdf), generated with kicad-footprint-generator
connector JST XH vertical boss
0
3
3
Connector_JST
JST_XH_B3B-XH-A_1x03_P2.50mm_Vertical
JST XH series connector, B3B-XH-A (http://www.jst-mfg.com/product/pdf/eng/eXH.pdf), generated with kicad-footprint-generator
connector JST XH vertical
0
3
3
Connector_JST
JST_XH_B4B-XH-AM_1x04_P2.50mm_Vertical
JST XH series connector, B4B-XH-AM, with boss (http://www.jst-mfg.com/product/pdf/eng/eXH.pdf), generated with kicad-footprint-generator
connector JST XH vertical boss
0
4
4
Connector_JST
JST_XH_B4B-XH-A_1x04_P2.50mm_Vertical
JST XH series connector, B4B-XH-A (http://www.jst-mfg.com/product/pdf/eng/eXH.pdf), generated with kicad-footprint-generator
connector JST XH vertical
0
4
4
Connector_JST
JST_XH_B5B-XH-AM_1x05_P2.50mm_Vertical
JST XH series connector, B5B-XH-AM, with boss (http://www.jst-mfg.com/product/pdf/eng/eXH.pdf), generated with kicad-footprint-generator
connector JST XH vertical boss
0
5
5
Connector_JST
JST_XH_B5B-XH-A_1x05_P2.50mm_Vertical
JST XH series connector, B5B-XH-A (http://www.jst-mfg.com/product/pdf/eng/eXH.pdf), generated with kicad-footprint-generator
connector JST XH vertical
0
5
5
Connector_JST
JST_XH_B6B-XH-AM_1x06_P2.50mm_Vertical
JST XH series connector, B6B-XH-AM, with boss (http://www.jst-mfg.com/product/pdf/eng/eXH.pdf), generated with kicad-footprint-generator
connector JST XH vertical boss
0
6
6
Connector_JST
JST_XH_B6B-XH-A_1x06_P2.50mm_Vertical
JST XH series connector, B6B-XH-A (http://www.jst-mfg.com/product/pdf/eng/eXH.pdf), generated with kicad-footprint-generator
connector JST XH vertical
0
6
6
Connector_JST
JST_XH_B7B-XH-AM_1x07_P2.50mm_Vertical
JST XH series connector, B7B-XH-AM, with boss (http://www.jst-mfg.com/product/pdf/eng/eXH.pdf), generated with kicad-footprint-generator
connector JST XH vertical boss
0
7
7
Connector_JST
JST_XH_B7B-XH-A_1x07_P2.50mm_Vertical
JST XH series connector, B7B-XH-A (http://www.jst-mfg.com/product/pdf/eng/eXH.pdf), generated with kicad-footprint-generator
connector JST XH vertical
0
7
7
Connector_JST
JST_XH_B8B-XH-AM_1x08_P2.50mm_Vertical
JST XH series connector, B8B-XH-AM, with boss (http://www.jst-mfg.com/product/pdf/eng/eXH.pdf), generated with kicad-footprint-generator
connector JST XH vertical boss
0
8
8
Connector_JST
JST_XH_B8B-XH-A_1x08_P2.50mm_Vertical
JST XH series connector, B8B-XH-A (http://www.jst-mfg.com/product/pdf/eng/eXH.pdf), generated with kicad-footprint-generator
connector JST XH vertical
0
8
8
Connector_JST
JST_XH_B9B-XH-AM_1x09_P2.50mm_Vertical
JST XH series connector, B9B-XH-AM, with boss (http://www.jst-mfg.com/product/pdf/eng/eXH.pdf), generated with kicad-footprint-generator
connector JST XH vertical boss
0
9
9
Connector_JST
JST_XH_B9B-XH-A_1x09_P2.50mm_Vertical
JST XH series connector, B9B-XH-A (http://www.jst-mfg.com/product/pdf/eng/eXH.pdf), generated with kicad-footprint-generator
connector JST XH vertical
0
9
9
Connector_JST
JST_XH_B10B-XH-AM_1x10_P2.50mm_Vertical
JST XH series connector, B10B-XH-AM, with boss (http://www.jst-mfg.com/product/pdf/eng/eXH.pdf), generated with kicad-footprint-generator
connector JST XH side entry boss
0
10
10
Connector_JST
JST_XH_B10B-XH-A_1x10_P2.50mm_Vertical
JST XH series connector, B10B-XH-A (http://www.jst-mfg.com/product/pdf/eng/eXH.pdf), generated with kicad-footprint-generator
connector JST XH side entry
0
10
10
Connector_JST
JST_XH_B11B-XH-A_1x11_P2.50mm_Vertical
JST XH series connector, B11B-XH-A (http://www.jst-mfg.com/product/pdf/eng/eXH.pdf), generated with kicad-footprint-generator
connector JST XH side entry
0
11
11
Connector_JST
JST_XH_B12B-XH-AM_1x12_P2.50mm_Vertical
JST XH series connector, B12B-XH-AM, with boss (http://www.jst-mfg.com/product/pdf/eng/eXH.pdf), generated with kicad-footprint-generator
connector JST XH side entry boss
0
12
12
Connector_JST
JST_XH_B12B-XH-A_1x12_P2.50mm_Vertical
JST XH series connector, B12B-XH-A (http://www.jst-mfg.com/product/pdf/eng/eXH.pdf), generated with kicad-footprint-generator
connector JST XH side entry
0
12
12
Connector_JST
JST_XH_B13B-XH-A_1x13_P2.50mm_Vertical
JST XH series connector, B13B-XH-A (http://www.jst-mfg.com/product/pdf/eng/eXH.pdf), generated with kicad-footprint-generator
connector JST XH side entry
0
13
13
Connector_JST
JST_XH_B14B-XH-A_1x14_P2.50mm_Vertical
JST XH series connector, B14B-XH-A (http://www.jst-mfg.com/product/pdf/eng/eXH.pdf), generated with kicad-footprint-generator
connector JST XH side entry
0
14
14
Connector_JST
JST_XH_B15B-XH-A_1x15_P2.50mm_Vertical
JST XH series connector, B15B-XH-A (http://www.jst-mfg.com/product/pdf/eng/eXH.pdf), generated with kicad-footprint-generator
connector JST XH side entry
0
15
15
Connector_JST
JST_XH_B16B-XH-A_1x16_P2.50mm_Vertical
JST XH series connector, B16B-XH-A (http://www.jst-mfg.com/product/pdf/eng/eXH.pdf), generated with kicad-footprint-generator
connector JST XH side entry
0
16
16
Connector_JST
JST_XH_B20B-XH-A_1x20_P2.50mm_Vertical
JST XH series connector, B20B-XH-A (http://www.jst-mfg.com/product/pdf/eng/eXH.pdf), generated with kicad-footprint-generator
connector JST XH side entry
0
20
20
Connector_JST
JST_XH_S2B-XH-A-1_1x02_P2.50mm_Horizontal
JST XH series connector, S2B-XH-A-1 (http://www.jst-mfg.com/product/pdf/eng/eXH.pdf), generated with kicad-footprint-generator
connector JST XH horizontal
0
2
2
Connector_JST
JST_XH_S2B-XH-A_1x02_P2.50mm_Horizontal
JST XH series connector, S2B-XH-A (http://www.jst-mfg.com/product/pdf/eng/eXH.pdf), generated with kicad-footprint-generator
connector JST XH horizontal
0
2
2
Connector_JST
JST_XH_S3B-XH-A-1_1x03_P2.50mm_Horizontal
JST XH series connector, S3B-XH-A-1 (http://www.jst-mfg.com/product/pdf/eng/eXH.pdf), generated with kicad-footprint-generator
connector JST XH horizontal
0
3
3
Connector_JST
JST_XH_S3B-XH-A_1x03_P2.50mm_Horizontal
JST XH series connector, S3B-XH-A (http://www.jst-mfg.com/product/pdf/eng/eXH.pdf), generated with kicad-footprint-generator
connector JST XH horizontal
0
3
3
Connector_JST
JST_XH_S4B-XH-A-1_1x04_P2.50mm_Horizontal
JST XH series connector, S4B-XH-A-1 (http://www.jst-mfg.com/product/pdf/eng/eXH.pdf), generated with kicad-footprint-generator
connector JST XH horizontal
0
4
4
Connector_JST
JST_XH_S4B-XH-A_1x04_P2.50mm_Horizontal
JST XH series connector, S4B-XH-A (http://www.jst-mfg.com/product/pdf/eng/eXH.pdf), generated with kicad-footprint-generator
connector JST XH horizontal
0
4
4
Connector_JST
JST_XH_S5B-XH-A-1_1x05_P2.50mm_Horizontal
JST XH series connector, S5B-XH-A-1 (http://www.jst-mfg.com/product/pdf/eng/eXH.pdf), generated with kicad-footprint-generator
connector JST XH horizontal
0
5
5
Connector_JST
JST_XH_S5B-XH-A_1x05_P2.50mm_Horizontal
JST XH series connector, S5B-XH-A (http://www.jst-mfg.com/product/pdf/eng/eXH.pdf), generated with kicad-footprint-generator
connector JST XH horizontal
0
5
5
Connector_JST
JST_XH_S6B-XH-A-1_1x06_P2.50mm_Horizontal
JST XH series connector, S6B-XH-A-1 (http://www.jst-mfg.com/product/pdf/eng/eXH.pdf), generated with kicad-footprint-generator
connector JST XH horizontal
0
6
6
Connector_JST
JST_XH_S6B-XH-A_1x06_P2.50mm_Horizontal
JST XH series connector, S6B-XH-A (http://www.jst-mfg.com/product/pdf/eng/eXH.pdf), generated with kicad-footprint-generator
connector JST XH horizontal
0
6
6
Connector_JST
JST_XH_S7B-XH-A-1_1x07_P2.50mm_Horizontal
JST XH series connector, S7B-XH-A-1 (http://www.jst-mfg.com/product/pdf/eng/eXH.pdf), generated with kicad-footprint-generator
connector JST XH horizontal
0
7
7
Connector_JST
JST_XH_S7B-XH-A_1x07_P2.50mm_Horizontal
JST XH series connector, S7B-XH-A (http://www.jst-mfg.com/product/pdf/eng/eXH.pdf), generated with kicad-footprint-generator
connector JST XH horizontal
0
7
7
Connector_JST
JST_XH_S8B-XH-A-1_1x08_P2.50mm_Horizontal
JST XH series connector, S8B-XH-A-1 (http://www.jst-mfg.com/product/pdf/eng/eXH.pdf), generated with kicad-footprint-generator
connector JST XH horizontal
0
8
8
Connector_JST
JST_XH_S8B-XH-A_1x08_P2.50mm_Horizontal
JST XH series connector, S8B-XH-A (http://www.jst-mfg.com/product/pdf/eng/eXH.pdf), generated with kicad-footprint-generator
connector JST XH horizontal
0
8
8
Connector_JST
JST_XH_S9B-XH-A-1_1x09_P2.50mm_Horizontal
JST XH series connector, S9B-XH-A-1 (http://www.jst-mfg.com/product/pdf/eng/eXH.pdf), generated with kicad-footprint-generator
connector JST XH horizontal
0
9
9
Connector_JST
JST_XH_S9B-XH-A_1x09_P2.50mm_Horizontal
JST XH series connector, S9B-XH-A (http://www.jst-mfg.com/product/pdf/eng/eXH.pdf), generated with kicad-footprint-generator
connector JST XH horizontal
0
9
9
Connector_JST
JST_XH_S10B-XH-A-1_1x10_P2.50mm_Horizontal
JST XH series connector, S10B-XH-A-1 (http://www.jst-mfg.com/product/pdf/eng/eXH.pdf), generated with kicad-footprint-generator
connector JST XH top entry
0
10
10
Connector_JST
JST_XH_S10B-XH-A_1x10_P2.50mm_Horizontal
JST XH series connector, S10B-XH-A (http://www.jst-mfg.com/product/pdf/eng/eXH.pdf), generated with kicad-footprint-generator
connector JST XH top entry
0
10
10
Connector_JST
JST_XH_S11B-XH-A-1_1x11_P2.50mm_Horizontal
JST XH series connector, S11B-XH-A-1 (http://www.jst-mfg.com/product/pdf/eng/eXH.pdf), generated with kicad-footprint-generator
connector JST XH top entry
0
11
11
Connector_JST
JST_XH_S11B-XH-A_1x11_P2.50mm_Horizontal
JST XH series connector, S11B-XH-A (http://www.jst-mfg.com/product/pdf/eng/eXH.pdf), generated with kicad-footprint-generator
connector JST XH top entry
0
11
11
Connector_JST
JST_XH_S12B-XH-A-1_1x12_P2.50mm_Horizontal
JST XH series connector, S12B-XH-A-1 (http://www.jst-mfg.com/product/pdf/eng/eXH.pdf), generated with kicad-footprint-generator
connector JST XH top entry
0
12
12
Connector_JST
JST_XH_S12B-XH-A_1x12_P2.50mm_Horizontal
JST XH series connector, S12B-XH-A (http://www.jst-mfg.com/product/pdf/eng/eXH.pdf), generated with kicad-footprint-generator
connector JST XH top entry
0
12
12
Connector_JST
JST_XH_S13B-XH-A-1_1x13_P2.50mm_Horizontal
JST XH series connector, S13B-XH-A-1 (http://www.jst-mfg.com/product/pdf/eng/eXH.pdf), generated with kicad-footprint-generator
connector JST XH top entry
0
13
13
Connector_JST
JST_XH_S13B-XH-A_1x13_P2.50mm_Horizontal
JST XH series connector, S13B-XH-A (http://www.jst-mfg.com/product/pdf/eng/eXH.pdf), generated with kicad-footprint-generator
connector JST XH top entry
0
13
13
Connector_JST
JST_XH_S14B-XH-A-1_1x14_P2.50mm_Horizontal
JST XH series connector, S14B-XH-A-1 (http://www.jst-mfg.com/product/pdf/eng/eXH.pdf), generated with kicad-footprint-generator
connector JST XH top entry
0
14
14
Connector_JST
JST_XH_S14B-XH-A_1x14_P2.50mm_Horizontal
JST XH series connector, S14B-XH-A (http://www.jst-mfg.com/product/pdf/eng/eXH.pdf), generated with kicad-footprint-generator
connector JST XH top entry
0
14
14
Connector_JST
JST_XH_S15B-XH-A-1_1x15_P2.50mm_Horizontal
JST XH series connector, S15B-XH-A-1 (http://www.jst-mfg.com/product/pdf/eng/eXH.pdf), generated with kicad-footprint-generator
connector JST XH top entry
0
15
15
Connector_JST
JST_XH_S15B-XH-A_1x15_P2.50mm_Horizontal
JST XH series connector, S15B-XH-A (http://www.jst-mfg.com/product/pdf/eng/eXH.pdf), generated with kicad-footprint-generator
connector JST XH top entry
0
15
15
Connector_JST
JST_XH_S16B-XH-A_1x16_P2.50mm_Horizontal
JST XH series connector, S16B-XH-A (http://www.jst-mfg.com/product/pdf/eng/eXH.pdf), generated with kicad-footprint-generator
connector JST XH top entry
0
16
16
Connector_JST
JST_ZE_B02B-ZESK-1D_1x02_P1.50mm_Vertical
JST ZE series connector, B02B-ZESK-1D, with boss (http://www.jst-mfg.com/product/pdf/eng/eZE.pdf), generated with kicad-footprint-generator
connector JST ZE side entry boss
0
2
2
Connector_JST
JST_ZE_B03B-ZESK-1D_1x03_P1.50mm_Vertical
JST ZE series connector, B03B-ZESK-1D, with boss (http://www.jst-mfg.com/product/pdf/eng/eZE.pdf), generated with kicad-footprint-generator
connector JST ZE side entry boss
0
3
3
Connector_JST
JST_ZE_B03B-ZESK-D_1x03_P1.50mm_Vertical
JST ZE series connector, B03B-ZESK-D (http://www.jst-mfg.com/product/pdf/eng/eZE.pdf), generated with kicad-footprint-generator
connector JST ZE side entry
0
3
3
Connector_JST
JST_ZE_B04B-ZESK-1D_1x04_P1.50mm_Vertical
JST ZE series connector, B04B-ZESK-1D, with boss (http://www.jst-mfg.com/product/pdf/eng/eZE.pdf), generated with kicad-footprint-generator
connector JST ZE side entry boss
0
4
4
Connector_JST
JST_ZE_B04B-ZESK-D_1x04_P1.50mm_Vertical
JST ZE series connector, B04B-ZESK-D (http://www.jst-mfg.com/product/pdf/eng/eZE.pdf), generated with kicad-footprint-generator
connector JST ZE side entry
0
4
4
Connector_JST
JST_ZE_B05B-ZESK-1D_1x05_P1.50mm_Vertical
JST ZE series connector, B05B-ZESK-1D, with boss (http://www.jst-mfg.com/product/pdf/eng/eZE.pdf), generated with kicad-footprint-generator
connector JST ZE side entry boss
0
5
5
Connector_JST
JST_ZE_B05B-ZESK-D_1x05_P1.50mm_Vertical
JST ZE series connector, B05B-ZESK-D (http://www.jst-mfg.com/product/pdf/eng/eZE.pdf), generated with kicad-footprint-generator
connector JST ZE side entry
0
5
5
Connector_JST
JST_ZE_B06B-ZESK-1D_1x06_P1.50mm_Vertical
JST ZE series connector, B06B-ZESK-1D, with boss (http://www.jst-mfg.com/product/pdf/eng/eZE.pdf), generated with kicad-footprint-generator
connector JST ZE side entry boss
0
6
6
Connector_JST
JST_ZE_B06B-ZESK-D_1x06_P1.50mm_Vertical
JST ZE series connector, B06B-ZESK-D (http://www.jst-mfg.com/product/pdf/eng/eZE.pdf), generated with kicad-footprint-generator
connector JST ZE side entry
0
6
6
Connector_JST
JST_ZE_B07B-ZESK-1D_1x07_P1.50mm_Vertical
JST ZE series connector, B07B-ZESK-1D, with boss (http://www.jst-mfg.com/product/pdf/eng/eZE.pdf), generated with kicad-footprint-generator
connector JST ZE side entry boss
0
7
7
Connector_JST
JST_ZE_B07B-ZESK-D_1x07_P1.50mm_Vertical
JST ZE series connector, B07B-ZESK-D (http://www.jst-mfg.com/product/pdf/eng/eZE.pdf), generated with kicad-footprint-generator
connector JST ZE side entry
0
7
7
Connector_JST
JST_ZE_B08B-ZESK-1D_1x08_P1.50mm_Vertical
JST ZE series connector, B08B-ZESK-1D, with boss (http://www.jst-mfg.com/product/pdf/eng/eZE.pdf), generated with kicad-footprint-generator
connector JST ZE side entry boss
0
8
8
Connector_JST
JST_ZE_B08B-ZESK-D_1x08_P1.50mm_Vertical
JST ZE series connector, B08B-ZESK-D (http://www.jst-mfg.com/product/pdf/eng/eZE.pdf), generated with kicad-footprint-generator
connector JST ZE side entry
0
8
8
Connector_JST
JST_ZE_B09B-ZESK-1D_1x09_P1.50mm_Vertical
JST ZE series connector, B09B-ZESK-1D, with boss (http://www.jst-mfg.com/product/pdf/eng/eZE.pdf), generated with kicad-footprint-generator
connector JST ZE side entry boss
0
9
9
Connector_JST
JST_ZE_B09B-ZESK-D_1x09_P1.50mm_Vertical
JST ZE series connector, B09B-ZESK-D (http://www.jst-mfg.com/product/pdf/eng/eZE.pdf), generated with kicad-footprint-generator
connector JST ZE side entry
0
9
9
Connector_JST
JST_ZE_B10B-ZESK-1D_1x10_P1.50mm_Vertical
JST ZE series connector, B10B-ZESK-1D, with boss (http://www.jst-mfg.com/product/pdf/eng/eZE.pdf), generated with kicad-footprint-generator
connector JST ZE side entry boss
0
10
10
Connector_JST
JST_ZE_B10B-ZESK-D_1x10_P1.50mm_Vertical
JST ZE series connector, B10B-ZESK-D (http://www.jst-mfg.com/product/pdf/eng/eZE.pdf), generated with kicad-footprint-generator
connector JST ZE side entry
0
10
10
Connector_JST
JST_ZE_B11B-ZESK-1D_1x11_P1.50mm_Vertical
JST ZE series connector, B11B-ZESK-1D, with boss (http://www.jst-mfg.com/product/pdf/eng/eZE.pdf), generated with kicad-footprint-generator
connector JST ZE side entry boss
0
11
11
Connector_JST
JST_ZE_B11B-ZESK-D_1x11_P1.50mm_Vertical
JST ZE series connector, B11B-ZESK-D (http://www.jst-mfg.com/product/pdf/eng/eZE.pdf), generated with kicad-footprint-generator
connector JST ZE side entry
0
11
11
Connector_JST
JST_ZE_B12B-ZESK-1D_1x12_P1.50mm_Vertical
JST ZE series connector, B12B-ZESK-1D, with boss (http://www.jst-mfg.com/product/pdf/eng/eZE.pdf), generated with kicad-footprint-generator
connector JST ZE side entry boss
0
12
12
Connector_JST
JST_ZE_B12B-ZESK-D_1x12_P1.50mm_Vertical
JST ZE series connector, B12B-ZESK-D (http://www.jst-mfg.com/product/pdf/eng/eZE.pdf), generated with kicad-footprint-generator
connector JST ZE side entry
0
12
12
Connector_JST
JST_ZE_B13B-ZESK-1D_1x13_P1.50mm_Vertical
JST ZE series connector, B13B-ZESK-1D, with boss (http://www.jst-mfg.com/product/pdf/eng/eZE.pdf), generated with kicad-footprint-generator
connector JST ZE side entry boss
0
13
13
Connector_JST
JST_ZE_B13B-ZESK-D_1x13_P1.50mm_Vertical
JST ZE series connector, B13B-ZESK-D (http://www.jst-mfg.com/product/pdf/eng/eZE.pdf), generated with kicad-footprint-generator
connector JST ZE side entry
0
13
13
Connector_JST
JST_ZE_B14B-ZESK-1D_1x14_P1.50mm_Vertical
JST ZE series connector, B14B-ZESK-1D, with boss (http://www.jst-mfg.com/product/pdf/eng/eZE.pdf), generated with kicad-footprint-generator
connector JST ZE side entry boss
0
14
14
Connector_JST
JST_ZE_B14B-ZESK-D_1x14_P1.50mm_Vertical
JST ZE series connector, B14B-ZESK-D (http://www.jst-mfg.com/product/pdf/eng/eZE.pdf), generated with kicad-footprint-generator
connector JST ZE side entry
0
14
14
Connector_JST
JST_ZE_B15B-ZESK-1D_1x15_P1.50mm_Vertical
JST ZE series connector, B15B-ZESK-1D, with boss (http://www.jst-mfg.com/product/pdf/eng/eZE.pdf), generated with kicad-footprint-generator
connector JST ZE side entry boss
0
15
15
Connector_JST
JST_ZE_B15B-ZESK-D_1x15_P1.50mm_Vertical
JST ZE series connector, B15B-ZESK-D (http://www.jst-mfg.com/product/pdf/eng/eZE.pdf), generated with kicad-footprint-generator
connector JST ZE side entry
0
15
15
Connector_JST
JST_ZE_B16B-ZESK-1D_1x16_P1.50mm_Vertical
JST ZE series connector, B16B-ZESK-1D, with boss (http://www.jst-mfg.com/product/pdf/eng/eZE.pdf), generated with kicad-footprint-generator
connector JST ZE side entry boss
0
16
16
Connector_JST
JST_ZE_B16B-ZESK-D_1x16_P1.50mm_Vertical
JST ZE series connector, B16B-ZESK-D (http://www.jst-mfg.com/product/pdf/eng/eZE.pdf), generated with kicad-footprint-generator
connector JST ZE side entry
0
16
16
Connector_JST
JST_ZE_BM02B-ZESS-TBT_1x02-1MP_P1.50mm_Vertical
JST ZE series connector, BM02B-ZESS-TBT (http://www.jst-mfg.com/product/pdf/eng/eZE.pdf), generated with kicad-footprint-generator
connector JST ZE vertical
0
4
3
Connector_JST
JST_ZE_BM03B-ZESS-TBT_1x03-1MP_P1.50mm_Vertical
JST ZE series connector, BM03B-ZESS-TBT (http://www.jst-mfg.com/product/pdf/eng/eZE.pdf), generated with kicad-footprint-generator
connector JST ZE vertical
0
5
4
Connector_JST
JST_ZE_BM04B-ZESS-TBT_1x04-1MP_P1.50mm_Vertical
JST ZE series connector, BM04B-ZESS-TBT (http://www.jst-mfg.com/product/pdf/eng/eZE.pdf), generated with kicad-footprint-generator
connector JST ZE vertical
0
6
5
Connector_JST
JST_ZE_BM05B-ZESS-TBT_1x05-1MP_P1.50mm_Vertical
JST ZE series connector, BM05B-ZESS-TBT (http://www.jst-mfg.com/product/pdf/eng/eZE.pdf), generated with kicad-footprint-generator
connector JST ZE vertical
0
7
6
Connector_JST
JST_ZE_BM06B-ZESS-TBT_1x06-1MP_P1.50mm_Vertical
JST ZE series connector, BM06B-ZESS-TBT (http://www.jst-mfg.com/product/pdf/eng/eZE.pdf), generated with kicad-footprint-generator
connector JST ZE vertical
0
8
7
Connector_JST
JST_ZE_BM07B-ZESS-TBT_1x07-1MP_P1.50mm_Vertical
JST ZE series connector, BM07B-ZESS-TBT (http://www.jst-mfg.com/product/pdf/eng/eZE.pdf), generated with kicad-footprint-generator
connector JST ZE vertical
0
9
8
Connector_JST
JST_ZE_BM08B-ZESS-TBT_1x08-1MP_P1.50mm_Vertical
JST ZE series connector, BM08B-ZESS-TBT (http://www.jst-mfg.com/product/pdf/eng/eZE.pdf), generated with kicad-footprint-generator
connector JST ZE vertical
0
10
9
Connector_JST
JST_ZE_BM09B-ZESS-TBT_1x09-1MP_P1.50mm_Vertical
JST ZE series connector, BM09B-ZESS-TBT (http://www.jst-mfg.com/product/pdf/eng/eZE.pdf), generated with kicad-footprint-generator
connector JST ZE vertical
0
11
10
Connector_JST
JST_ZE_BM10B-ZESS-TBT_1x10-1MP_P1.50mm_Vertical
JST ZE series connector, BM10B-ZESS-TBT (http://www.jst-mfg.com/product/pdf/eng/eZE.pdf), generated with kicad-footprint-generator
connector JST ZE vertical
0
12
11
Connector_JST
JST_ZE_BM11B-ZESS-TBT_1x11-1MP_P1.50mm_Vertical
JST ZE series connector, BM11B-ZESS-TBT (http://www.jst-mfg.com/product/pdf/eng/eZE.pdf), generated with kicad-footprint-generator
connector JST ZE vertical
0
13
12
Connector_JST
JST_ZE_BM12B-ZESS-TBT_1x12-1MP_P1.50mm_Vertical
JST ZE series connector, BM12B-ZESS-TBT (http://www.jst-mfg.com/product/pdf/eng/eZE.pdf), generated with kicad-footprint-generator
connector JST ZE vertical
0
14
13
Connector_JST
JST_ZE_BM13B-ZESS-TBT_1x13-1MP_P1.50mm_Vertical
JST ZE series connector, BM13B-ZESS-TBT (http://www.jst-mfg.com/product/pdf/eng/eZE.pdf), generated with kicad-footprint-generator
connector JST ZE vertical
0
15
14
Connector_JST
JST_ZE_BM14B-ZESS-TBT_1x14-1MP_P1.50mm_Vertical
JST ZE series connector, BM14B-ZESS-TBT (http://www.jst-mfg.com/product/pdf/eng/eZE.pdf), generated with kicad-footprint-generator
connector JST ZE vertical
0
16
15
Connector_JST
JST_ZE_BM15B-ZESS-TBT_1x15-1MP_P1.50mm_Vertical
JST ZE series connector, BM15B-ZESS-TBT (http://www.jst-mfg.com/product/pdf/eng/eZE.pdf), generated with kicad-footprint-generator
connector JST ZE vertical
0
17
16
Connector_JST
JST_ZE_BM16B-ZESS-TBT_1x16-1MP_P1.50mm_Vertical
JST ZE series connector, BM16B-ZESS-TBT (http://www.jst-mfg.com/product/pdf/eng/eZE.pdf), generated with kicad-footprint-generator
connector JST ZE vertical
0
18
17
Connector_JST
JST_ZE_S02B-ZESK-2D_1x02_P1.50mm_Horizontal
JST ZE series connector, S02B-ZESK-2D (http://www.jst-mfg.com/product/pdf/eng/eZE.pdf), generated with kicad-footprint-generator
connector JST ZE top entry
0
2
2
Connector_JST
JST_ZE_S03B-ZESK-2D_1x03_P1.50mm_Horizontal
JST ZE series connector, S03B-ZESK-2D (http://www.jst-mfg.com/product/pdf/eng/eZE.pdf), generated with kicad-footprint-generator
connector JST ZE top entry
0
3
3
Connector_JST
JST_ZE_S04B-ZESK-2D_1x04_P1.50mm_Horizontal
JST ZE series connector, S04B-ZESK-2D (http://www.jst-mfg.com/product/pdf/eng/eZE.pdf), generated with kicad-footprint-generator
connector JST ZE top entry
0
4
4
Connector_JST
JST_ZE_S05B-ZESK-2D_1x05_P1.50mm_Horizontal
JST ZE series connector, S05B-ZESK-2D (http://www.jst-mfg.com/product/pdf/eng/eZE.pdf), generated with kicad-footprint-generator
connector JST ZE top entry
0
5
5
Connector_JST
JST_ZE_S06B-ZESK-2D_1x06_P1.50mm_Horizontal
JST ZE series connector, S06B-ZESK-2D (http://www.jst-mfg.com/product/pdf/eng/eZE.pdf), generated with kicad-footprint-generator
connector JST ZE top entry
0
6
6
Connector_JST
JST_ZE_S07B-ZESK-2D_1x07_P1.50mm_Horizontal
JST ZE series connector, S07B-ZESK-2D (http://www.jst-mfg.com/product/pdf/eng/eZE.pdf), generated with kicad-footprint-generator
connector JST ZE top entry
0
7
7
Connector_JST
JST_ZE_S08B-ZESK-2D_1x08_P1.50mm_Horizontal
JST ZE series connector, S08B-ZESK-2D (http://www.jst-mfg.com/product/pdf/eng/eZE.pdf), generated with kicad-footprint-generator
connector JST ZE top entry
0
8
8
Connector_JST
JST_ZE_S09B-ZESK-2D_1x09_P1.50mm_Horizontal
JST ZE series connector, S09B-ZESK-2D (http://www.jst-mfg.com/product/pdf/eng/eZE.pdf), generated with kicad-footprint-generator
connector JST ZE top entry
0
9
9
Connector_JST
JST_ZE_S10B-ZESK-2D_1x10_P1.50mm_Horizontal
JST ZE series connector, S10B-ZESK-2D (http://www.jst-mfg.com/product/pdf/eng/eZE.pdf), generated with kicad-footprint-generator
connector JST ZE top entry
0
10
10
Connector_JST
JST_ZE_S11B-ZESK-2D_1x11_P1.50mm_Horizontal
JST ZE series connector, S11B-ZESK-2D (http://www.jst-mfg.com/product/pdf/eng/eZE.pdf), generated with kicad-footprint-generator
connector JST ZE top entry
0
11
11
Connector_JST
JST_ZE_S12B-ZESK-2D_1x12_P1.50mm_Horizontal
JST ZE series connector, S12B-ZESK-2D (http://www.jst-mfg.com/product/pdf/eng/eZE.pdf), generated with kicad-footprint-generator
connector JST ZE top entry
0
12
12
Connector_JST
JST_ZE_S13B-ZESK-2D_1x13_P1.50mm_Horizontal
JST ZE series connector, S13B-ZESK-2D (http://www.jst-mfg.com/product/pdf/eng/eZE.pdf), generated with kicad-footprint-generator
connector JST ZE top entry
0
13
13
Connector_JST
JST_ZE_S14B-ZESK-2D_1x14_P1.50mm_Horizontal
JST ZE series connector, S14B-ZESK-2D (http://www.jst-mfg.com/product/pdf/eng/eZE.pdf), generated with kicad-footprint-generator
connector JST ZE top entry
0
14
14
Connector_JST
JST_ZE_S15B-ZESK-2D_1x15_P1.50mm_Horizontal
JST ZE series connector, S15B-ZESK-2D (http://www.jst-mfg.com/product/pdf/eng/eZE.pdf), generated with kicad-footprint-generator
connector JST ZE top entry
0
15
15
Connector_JST
JST_ZE_S16B-ZESK-2D_1x16_P1.50mm_Horizontal
JST ZE series connector, S16B-ZESK-2D (http://www.jst-mfg.com/product/pdf/eng/eZE.pdf), generated with kicad-footprint-generator
connector JST ZE top entry
0
16
16
Connector_JST
JST_ZE_SM02B-ZESS-TB_1x02-1MP_P1.50mm_Horizontal
JST ZE series connector, SM02B-ZESS-TB (http://www.jst-mfg.com/product/pdf/eng/eZE.pdf), generated with kicad-footprint-generator
connector JST ZE horizontal
0
4
3
Connector_JST
JST_ZE_SM03B-ZESS-TB_1x03-1MP_P1.50mm_Horizontal
JST ZE series connector, SM03B-ZESS-TB (http://www.jst-mfg.com/product/pdf/eng/eZE.pdf), generated with kicad-footprint-generator
connector JST ZE horizontal
0
5
4
Connector_JST
JST_ZE_SM04B-ZESS-TB_1x04-1MP_P1.50mm_Horizontal
JST ZE series connector, SM04B-ZESS-TB (http://www.jst-mfg.com/product/pdf/eng/eZE.pdf), generated with kicad-footprint-generator
connector JST ZE horizontal
0
6
5
Connector_JST
JST_ZE_SM05B-ZESS-TB_1x05-1MP_P1.50mm_Horizontal
JST ZE series connector, SM05B-ZESS-TB (http://www.jst-mfg.com/product/pdf/eng/eZE.pdf), generated with kicad-footprint-generator
connector JST ZE horizontal
0
7
6
Connector_JST
JST_ZE_SM06B-ZESS-TB_1x06-1MP_P1.50mm_Horizontal
JST ZE series connector, SM06B-ZESS-TB (http://www.jst-mfg.com/product/pdf/eng/eZE.pdf), generated with kicad-footprint-generator
connector JST ZE horizontal
0
8
7
Connector_JST
JST_ZE_SM07B-ZESS-TB_1x07-1MP_P1.50mm_Horizontal
JST ZE series connector, SM07B-ZESS-TB (http://www.jst-mfg.com/product/pdf/eng/eZE.pdf), generated with kicad-footprint-generator
connector JST ZE horizontal
0
9
8
Connector_JST
JST_ZE_SM08B-ZESS-TB_1x08-1MP_P1.50mm_Horizontal
JST ZE series connector, SM08B-ZESS-TB (http://www.jst-mfg.com/product/pdf/eng/eZE.pdf), generated with kicad-footprint-generator
connector JST ZE horizontal
0
10
9
Connector_JST
JST_ZE_SM09B-ZESS-TB_1x09-1MP_P1.50mm_Horizontal
JST ZE series connector, SM09B-ZESS-TB (http://www.jst-mfg.com/product/pdf/eng/eZE.pdf), generated with kicad-footprint-generator
connector JST ZE horizontal
0
11
10
Connector_JST
JST_ZE_SM10B-ZESS-TB_1x10-1MP_P1.50mm_Horizontal
JST ZE series connector, SM10B-ZESS-TB (http://www.jst-mfg.com/product/pdf/eng/eZE.pdf), generated with kicad-footprint-generator
connector JST ZE horizontal
0
12
11
Connector_JST
JST_ZE_SM11B-ZESS-TB_1x11-1MP_P1.50mm_Horizontal
JST ZE series connector, SM11B-ZESS-TB (http://www.jst-mfg.com/product/pdf/eng/eZE.pdf), generated with kicad-footprint-generator
connector JST ZE horizontal
0
13
12
Connector_JST
JST_ZE_SM12B-ZESS-TB_1x12-1MP_P1.50mm_Horizontal
JST ZE series connector, SM12B-ZESS-TB (http://www.jst-mfg.com/product/pdf/eng/eZE.pdf), generated with kicad-footprint-generator
connector JST ZE horizontal
0
14
13
Connector_JST
JST_ZE_SM13B-ZESS-TB_1x13-1MP_P1.50mm_Horizontal
JST ZE series connector, SM13B-ZESS-TB (http://www.jst-mfg.com/product/pdf/eng/eZE.pdf), generated with kicad-footprint-generator
connector JST ZE horizontal
0
15
14
Connector_JST
JST_ZE_SM14B-ZESS-TB_1x14-1MP_P1.50mm_Horizontal
JST ZE series connector, SM14B-ZESS-TB (http://www.jst-mfg.com/product/pdf/eng/eZE.pdf), generated with kicad-footprint-generator
connector JST ZE horizontal
0
16
15
Connector_JST
JST_ZE_SM15B-ZESS-TB_1x15-1MP_P1.50mm_Horizontal
JST ZE series connector, SM15B-ZESS-TB (http://www.jst-mfg.com/product/pdf/eng/eZE.pdf), generated with kicad-footprint-generator
connector JST ZE horizontal
0
17
16
Connector_JST
JST_ZE_SM16B-ZESS-TB_1x16-1MP_P1.50mm_Horizontal
JST ZE series connector, SM16B-ZESS-TB (http://www.jst-mfg.com/product/pdf/eng/eZE.pdf), generated with kicad-footprint-generator
connector JST ZE horizontal
0
18
17
Connector_PCBEdge
4UCON_10156_2x40_P1.27mm_Socket_Horizontal
4UCON 10156 Card edge socket with 80 contacts (40 each side), through-hole, http://www.4uconnector.com/online/object/4udrawing/10156.pdf
4UCON 10156 Card edge socket with 80 contacts
0
80
80
Connector_PCBEdge
BUS_AT
AT ISA 16 bits Bus Edge Connector
BUS ISA AT Edge connector
0
98
98
Connector_PCBEdge
BUS_PCI
PCI bus Edge Connector
PCI bus Edge Connector
0
240
120
Connector_PCBEdge
BUS_PCI_Express_Mini
Mini-PCI Express bus connector (https://s3.amazonaws.com/fit-iot/download/facet-cards/documents/PCI_Express_miniCard_Electromechanical_specs_rev1.2.pdf#page=11)
mini pcie
0
54
53
Connector_PCBEdge
BUS_PCI_Express_Mini_Dual
Mini-PCI Express bus connector full size with dual clips (https://s3.amazonaws.com/fit-iot/download/facet-cards/documents/PCI_Express_miniCard_Electromechanical_specs_rev1.2.pdf#page=28)
mini pcie
0
54
53
Connector_PCBEdge
BUS_PCI_Express_Mini_Full
Mini-PCI Express bus connector full size with clips (https://s3.amazonaws.com/fit-iot/download/facet-cards/documents/PCI_Express_miniCard_Electromechanical_specs_rev1.2.pdf#page=24)
mini pcie
0
54
53
Connector_PCBEdge
BUS_PCI_Express_Mini_Half
Mini-PCI Express bus connector half size with clips (https://s3.amazonaws.com/fit-iot/download/facet-cards/documents/PCI_Express_miniCard_Electromechanical_specs_rev1.2.pdf#page=25)
mini pcie
0
54
53
Connector_PCBEdge
BUS_PCIexpress_x1
PCIexpress Bus Edge Connector x1 http://www.ritrontek.com/uploadfile/2016/1026/20161026105231124.pdf#page=70
PCIe
0
36
36
Connector_PCBEdge
BUS_PCIexpress_x4
PCIexpress Bus Edge Connector x1 http://www.ritrontek.com/uploadfile/2016/1026/20161026105231124.pdf#page=70
PCIe
0
64
64
Connector_PCBEdge
BUS_PCIexpress_x8
PCIexpress Bus Edge Connector x1 http://www.ritrontek.com/uploadfile/2016/1026/20161026105231124.pdf#page=70
PCIe
0
98
98
Connector_PCBEdge
BUS_PCIexpress_x16
PCIexpress Bus Edge Connector x1 http://www.ritrontek.com/uploadfile/2016/1026/20161026105231124.pdf#page=70
PCIe
0
164
164
Connector_PCBEdge
Samtec_MECF-05-0_-L-DV_2x05_P1.27mm_Polarized_Edge
Highspeed card edge connector for PCB's with 05 contacts (polarized)
conn samtec card-edge high-speed
0
8
8
Connector_PCBEdge
Samtec_MECF-05-0_-NP-L-DV_2x05_P1.27mm_Edge
Highspeed card edge connector for PCB's with 05 contacts (not polarized)
conn samtec card-edge high-speed
0
10
10
Connector_PCBEdge
Samtec_MECF-05-01-L-DV-WT_2x05_P1.27mm_Polarized_Socket_Horizontal
Highspeed card edge connector for 1.6mm PCB's with 05 contacts (polarized)
conn samtec card-edge high-speed
0
10
8
Connector_PCBEdge
Samtec_MECF-05-01-L-DV_2x05_P1.27mm_Polarized_Socket_Horizontal
Highspeed card edge connector for 1.6mm PCB's with 05 contacts (polarized)
conn samtec card-edge high-speed
0
8
8
Connector_PCBEdge
Samtec_MECF-05-01-NP-L-DV-WT_2x05_P1.27mm_Socket_Horizontal
Highspeed card edge connector for 1.6mm PCB's with 05 contacts (not polarized)
conn samtec card-edge high-speed
0
12
10
Connector_PCBEdge
Samtec_MECF-05-01-NP-L-DV_2x05_P1.27mm_Socket_Horizontal
Highspeed card edge connector for 1.6mm PCB's with 05 contacts (not polarized)
conn samtec card-edge high-speed
0
10
10
Connector_PCBEdge
Samtec_MECF-05-02-L-DV-WT_2x05_P1.27mm_Polarized_Socket_Horizontal
Highspeed card edge connector for 2.4mm PCB's with 05 contacts (polarized)
conn samtec card-edge high-speed
0
10
8
Connector_PCBEdge
Samtec_MECF-05-02-L-DV_2x05_P1.27mm_Polarized_Socket_Horizontal
Highspeed card edge connector for 2.4mm PCB's with 05 contacts (polarized)
conn samtec card-edge high-speed
0
8
8
Connector_PCBEdge
Samtec_MECF-05-02-NP-L-DV-WT_2x05_P1.27mm_Socket_Horizontal
Highspeed card edge connector for 2.4mm PCB's with 05 contacts (not polarized)
conn samtec card-edge high-speed
0
12
10
Connector_PCBEdge
Samtec_MECF-05-02-NP-L-DV_2x05_P1.27mm_Socket_Horizontal
Highspeed card edge connector for 2.4mm PCB's with 05 contacts (not polarized)
conn samtec card-edge high-speed
0
10
10
Connector_PCBEdge
Samtec_MECF-08-0_-L-DV_2x08_P1.27mm_Polarized_Edge
Highspeed card edge connector for PCB's with 08 contacts (polarized)
conn samtec card-edge high-speed
0
14
14
Connector_PCBEdge
Samtec_MECF-08-0_-NP-L-DV_2x08_P1.27mm_Edge
Highspeed card edge connector for PCB's with 08 contacts (not polarized)
conn samtec card-edge high-speed
0
16
16
Connector_PCBEdge
Samtec_MECF-08-01-L-DV-WT_2x08_P1.27mm_Polarized_Socket_Horizontal
Highspeed card edge connector for 1.6mm PCB's with 08 contacts (polarized)
conn samtec card-edge high-speed
0
16
14
Connector_PCBEdge
Samtec_MECF-08-01-L-DV_2x08_P1.27mm_Polarized_Socket_Horizontal
Highspeed card edge connector for 1.6mm PCB's with 08 contacts (polarized)
conn samtec card-edge high-speed
0
14
14
Connector_PCBEdge
Samtec_MECF-08-01-NP-L-DV-WT_2x08_P1.27mm_Socket_Horizontal
Highspeed card edge connector for 1.6mm PCB's with 08 contacts (not polarized)
conn samtec card-edge high-speed
0
18
16
Connector_PCBEdge
Samtec_MECF-08-01-NP-L-DV_2x08_P1.27mm_Socket_Horizontal
Highspeed card edge connector for 1.6mm PCB's with 08 contacts (not polarized)
conn samtec card-edge high-speed
0
16
16
Connector_PCBEdge
Samtec_MECF-08-02-L-DV-WT_2x08_P1.27mm_Polarized_Socket_Horizontal
Highspeed card edge connector for 2.4mm PCB's with 08 contacts (polarized)
conn samtec card-edge high-speed
0
16
14
Connector_PCBEdge
Samtec_MECF-08-02-L-DV_2x08_P1.27mm_Polarized_Socket_Horizontal
Highspeed card edge connector for 2.4mm PCB's with 08 contacts (polarized)
conn samtec card-edge high-speed
0
14
14
Connector_PCBEdge
Samtec_MECF-08-02-NP-L-DV-WT_2x08_P1.27mm_Socket_Horizontal
Highspeed card edge connector for 2.4mm PCB's with 08 contacts (not polarized)
conn samtec card-edge high-speed
0
18
16
Connector_PCBEdge
Samtec_MECF-08-02-NP-L-DV_2x08_P1.27mm_Socket_Horizontal
Highspeed card edge connector for 2.4mm PCB's with 08 contacts (not polarized)
conn samtec card-edge high-speed
0
16
16
Connector_PCBEdge
Samtec_MECF-20-0_-L-DV_2x20_P1.27mm_Polarized_Edge
Highspeed card edge connector for PCB's with 20 contacts (polarized)
conn samtec card-edge high-speed
0
38
38
Connector_PCBEdge
Samtec_MECF-20-0_-NP-L-DV_2x20_P1.27mm_Edge
Highspeed card edge connector for PCB's with 20 contacts (not polarized)
conn samtec card-edge high-speed
0
40
40
Connector_PCBEdge
Samtec_MECF-20-01-L-DV-WT_2x20_P1.27mm_Polarized_Socket_Horizontal
Highspeed card edge connector for 1.6mm PCB's with 20 contacts (polarized)
conn samtec card-edge high-speed
0
40
38
Connector_PCBEdge
Samtec_MECF-20-01-L-DV_2x20_P1.27mm_Polarized_Socket_Horizontal
Highspeed card edge connector for 1.6mm PCB's with 20 contacts (polarized)
conn samtec card-edge high-speed
0
38
38
Connector_PCBEdge
Samtec_MECF-20-01-NP-L-DV-WT_2x20_P1.27mm_Socket_Horizontal
Highspeed card edge connector for 1.6mm PCB's with 20 contacts (not polarized)
conn samtec card-edge high-speed
0
42
40
Connector_PCBEdge
Samtec_MECF-20-01-NP-L-DV_2x20_P1.27mm_Socket_Horizontal
Highspeed card edge connector for 1.6mm PCB's with 20 contacts (not polarized)
conn samtec card-edge high-speed
0
40
40
Connector_PCBEdge
Samtec_MECF-20-02-L-DV-WT_2x20_P1.27mm_Polarized_Socket_Horizontal
Highspeed card edge connector for 2.4mm PCB's with 20 contacts (polarized)
conn samtec card-edge high-speed
0
40
38
Connector_PCBEdge
Samtec_MECF-20-02-L-DV_2x20_P1.27mm_Polarized_Socket_Horizontal
Highspeed card edge connector for 2.4mm PCB's with 20 contacts (polarized)
conn samtec card-edge high-speed
0
38
38
Connector_PCBEdge
Samtec_MECF-20-02-NP-L-DV-WT_2x20_P1.27mm_Socket_Horizontal
Highspeed card edge connector for 2.4mm PCB's with 20 contacts (not polarized)
conn samtec card-edge high-speed
0
42
40
Connector_PCBEdge
Samtec_MECF-20-02-NP-L-DV_2x20_P1.27mm_Socket_Horizontal
Highspeed card edge connector for 2.4mm PCB's with 20 contacts (not polarized)
conn samtec card-edge high-speed
0
40
40
Connector_PCBEdge
Samtec_MECF-30-0_-L-DV_2x30_P1.27mm_Polarized_Edge
Highspeed card edge connector for PCB's with 30 contacts (polarized)
conn samtec card-edge high-speed
0
58
58
Connector_PCBEdge
Samtec_MECF-30-0_-NP-L-DV_2x30_P1.27mm_Edge
Highspeed card edge connector for PCB's with 30 contacts (not polarized)
conn samtec card-edge high-speed
0
60
60
Connector_PCBEdge
Samtec_MECF-30-01-L-DV-WT_2x30_P1.27mm_Polarized_Socket_Horizontal
Highspeed card edge connector for 1.6mm PCB's with 30 contacts (polarized)
conn samtec card-edge high-speed
0
60
58
Connector_PCBEdge
Samtec_MECF-30-01-L-DV_2x30_P1.27mm_Polarized_Socket_Horizontal
Highspeed card edge connector for 1.6mm PCB's with 30 contacts (polarized)
conn samtec card-edge high-speed
0
58
58
Connector_PCBEdge
Samtec_MECF-30-01-NP-L-DV-WT_2x30_P1.27mm_Socket_Horizontal
Highspeed card edge connector for 1.6mm PCB's with 30 contacts (not polarized)
conn samtec card-edge high-speed
0
62
60
Connector_PCBEdge
Samtec_MECF-30-01-NP-L-DV_2x30_P1.27mm_Socket_Horizontal
Highspeed card edge connector for 1.6mm PCB's with 30 contacts (not polarized)
conn samtec card-edge high-speed
0
60
60
Connector_PCBEdge
Samtec_MECF-30-02-L-DV-WT_2x30_P1.27mm_Polarized_Socket_Horizontal
Highspeed card edge connector for 2.4mm PCB's with 30 contacts (polarized)
conn samtec card-edge high-speed
0
60
58
Connector_PCBEdge
Samtec_MECF-30-02-L-DV_2x30_P1.27mm_Polarized_Socket_Horizontal
Highspeed card edge connector for 2.4mm PCB's with 30 contacts (polarized)
conn samtec card-edge high-speed
0
58
58
Connector_PCBEdge
Samtec_MECF-30-02-NP-L-DV-WT_2x30_P1.27mm_Socket_Horizontal
Highspeed card edge connector for 2.4mm PCB's with 30 contacts (not polarized)
conn samtec card-edge high-speed
0
62
60
Connector_PCBEdge
Samtec_MECF-30-02-NP-L-DV_2x30_P1.27mm_Socket_Horizontal
Highspeed card edge connector for 2.4mm PCB's with 30 contacts (not polarized)
conn samtec card-edge high-speed
0
60
60
Connector_PCBEdge
Samtec_MECF-40-0_-L-DV_2x40_P1.27mm_Polarized_Edge
Highspeed card edge connector for PCB's with 40 contacts (polarized)
conn samtec card-edge high-speed
0
78
78
Connector_PCBEdge
Samtec_MECF-40-0_-NP-L-DV_2x40_P1.27mm_Edge
Highspeed card edge connector for PCB's with 40 contacts (not polarized)
conn samtec card-edge high-speed
0
80
80
Connector_PCBEdge
Samtec_MECF-40-01-L-DV-WT_2x40_P1.27mm_Polarized_Socket_Horizontal
Highspeed card edge connector for 1.6mm PCB's with 40 contacts (polarized)
conn samtec card-edge high-speed
0
80
78
Connector_PCBEdge
Samtec_MECF-40-01-L-DV_2x40_P1.27mm_Polarized_Socket_Horizontal
Highspeed card edge connector for 1.6mm PCB's with 40 contacts (polarized)
conn samtec card-edge high-speed
0
78
78
Connector_PCBEdge
Samtec_MECF-40-01-NP-L-DV-WT_2x40_P1.27mm_Socket_Horizontal
Highspeed card edge connector for 1.6mm PCB's with 40 contacts (not polarized)
conn samtec card-edge high-speed
0
82
80
Connector_PCBEdge
Samtec_MECF-40-01-NP-L-DV_2x40_P1.27mm_Socket_Horizontal
Highspeed card edge connector for 1.6mm PCB's with 40 contacts (not polarized)
conn samtec card-edge high-speed
0
80
80
Connector_PCBEdge
Samtec_MECF-40-02-L-DV-WT_2x40_P1.27mm_Polarized_Socket_Horizontal
Highspeed card edge connector for 2.4mm PCB's with 40 contacts (polarized)
conn samtec card-edge high-speed
0
80
78
Connector_PCBEdge
Samtec_MECF-40-02-L-DV_2x40_P1.27mm_Polarized_Socket_Horizontal
Highspeed card edge connector for 2.4mm PCB's with 40 contacts (polarized)
conn samtec card-edge high-speed
0
78
78
Connector_PCBEdge
Samtec_MECF-40-02-NP-L-DV-WT_2x40_P1.27mm_Socket_Horizontal
Highspeed card edge connector for 2.4mm PCB's with 40 contacts (not polarized)
conn samtec card-edge high-speed
0
82
80
Connector_PCBEdge
Samtec_MECF-40-02-NP-L-DV_2x40_P1.27mm_Socket_Horizontal
Highspeed card edge connector for 2.4mm PCB's with 40 contacts (not polarized)
conn samtec card-edge high-speed
0
80
80
Connector_PCBEdge
Samtec_MECF-50-0_-L-DV_2x50_P1.27mm_Polarized_Edge
Highspeed card edge connector for PCB's with 50 contacts (polarized)
conn samtec card-edge high-speed
0
98
98
Connector_PCBEdge
Samtec_MECF-50-0_-NP-L-DV_2x50_P1.27mm_Edge
Highspeed card edge connector for PCB's with 50 contacts (not polarized)
conn samtec card-edge high-speed
0
100
100
Connector_PCBEdge
Samtec_MECF-50-01-L-DV-WT_2x50_P1.27mm_Polarized_Socket_Horizontal
Highspeed card edge connector for 1.6mm PCB's with 50 contacts (polarized)
conn samtec card-edge high-speed
0
100
98
Connector_PCBEdge
Samtec_MECF-50-01-L-DV_2x50_P1.27mm_Polarized_Socket_Horizontal
Highspeed card edge connector for 1.6mm PCB's with 50 contacts (polarized)
conn samtec card-edge high-speed
0
98
98
Connector_PCBEdge
Samtec_MECF-50-01-NP-L-DV-WT_2x50_P1.27mm_Socket_Horizontal
Highspeed card edge connector for 1.6mm PCB's with 50 contacts (not polarized)
conn samtec card-edge high-speed
0
102
100
Connector_PCBEdge
Samtec_MECF-50-01-NP-L-DV_2x50_P1.27mm_Socket_Horizontal
Highspeed card edge connector for 1.6mm PCB's with 50 contacts (not polarized)
conn samtec card-edge high-speed
0
100
100
Connector_PCBEdge
Samtec_MECF-50-02-L-DV-WT_2x50_P1.27mm_Polarized_Socket_Horizontal
Highspeed card edge connector for 2.4mm PCB's with 50 contacts (polarized)
conn samtec card-edge high-speed
0
100
98
Connector_PCBEdge
Samtec_MECF-50-02-L-DV_2x50_P1.27mm_Polarized_Socket_Horizontal
Highspeed card edge connector for 2.4mm PCB's with 50 contacts (polarized)
conn samtec card-edge high-speed
0
98
98
Connector_PCBEdge
Samtec_MECF-50-02-NP-L-DV-WT_2x50_P1.27mm_Socket_Horizontal
Highspeed card edge connector for 2.4mm PCB's with 50 contacts (not polarized)
conn samtec card-edge high-speed
0
102
100
Connector_PCBEdge
Samtec_MECF-50-02-NP-L-DV_2x50_P1.27mm_Socket_Horizontal
Highspeed card edge connector for 2.4mm PCB's with 50 contacts (not polarized)
conn samtec card-edge high-speed
0
100
100
Connector_PCBEdge
Samtec_MECF-60-0_-L-DV_2x60_P1.27mm_Polarized_Edge
Highspeed card edge connector for PCB's with 60 contacts (polarized)
conn samtec card-edge high-speed
0
116
116
Connector_PCBEdge
Samtec_MECF-60-0_-NP-L-DV_2x60_P1.27mm_Edge
Highspeed card edge connector for PCB's with 60 contacts (not polarized)
conn samtec card-edge high-speed
0
120
120
Connector_PCBEdge
Samtec_MECF-60-01-L-DV-WT_2x60_P1.27mm_Polarized_Socket_Horizontal
Highspeed card edge connector for 1.6mm PCB's with 60 contacts (polarized)
conn samtec card-edge high-speed
0
118
116
Connector_PCBEdge
Samtec_MECF-60-01-L-DV_2x60_P1.27mm_Polarized_Socket_Horizontal
Highspeed card edge connector for 1.6mm PCB's with 60 contacts (polarized)
conn samtec card-edge high-speed
0
116
116
Connector_PCBEdge
Samtec_MECF-60-01-NP-L-DV-WT_2x60_P1.27mm_Socket_Horizontal
Highspeed card edge connector for 1.6mm PCB's with 60 contacts (not polarized)
conn samtec card-edge high-speed
0
122
120
Connector_PCBEdge
Samtec_MECF-60-01-NP-L-DV_2x60_P1.27mm_Socket_Horizontal
Highspeed card edge connector for 1.6mm PCB's with 60 contacts (not polarized)
conn samtec card-edge high-speed
0
120
120
Connector_PCBEdge
Samtec_MECF-60-02-L-DV-WT_2x60_P1.27mm_Polarized_Socket_Horizontal
Highspeed card edge connector for 2.4mm PCB's with 60 contacts (polarized)
conn samtec card-edge high-speed
0
118
116
Connector_PCBEdge
Samtec_MECF-60-02-L-DV_2x60_P1.27mm_Polarized_Socket_Horizontal
Highspeed card edge connector for 2.4mm PCB's with 60 contacts (polarized)
conn samtec card-edge high-speed
0
116
116
Connector_PCBEdge
Samtec_MECF-60-02-NP-L-DV-WT_2x60_P1.27mm_Socket_Horizontal
Highspeed card edge connector for 2.4mm PCB's with 60 contacts (not polarized)
conn samtec card-edge high-speed
0
122
120
Connector_PCBEdge
Samtec_MECF-60-02-NP-L-DV_2x60_P1.27mm_Socket_Horizontal
Highspeed card edge connector for 2.4mm PCB's with 60 contacts (not polarized)
conn samtec card-edge high-speed
0
120
120
Connector_PCBEdge
Samtec_MECF-70-0_-L-DV_2x70_P1.27mm_Polarized_Edge
Highspeed card edge connector for PCB's with 70 contacts (polarized)
conn samtec card-edge high-speed
0
136
136
Connector_PCBEdge
Samtec_MECF-70-0_-NP-L-DV_2x70_P1.27mm_Edge
Highspeed card edge connector for PCB's with 70 contacts (not polarized)
conn samtec card-edge high-speed
0
140
140
Connector_PCBEdge
Samtec_MECF-70-01-L-DV-WT_2x70_P1.27mm_Polarized_Socket_Horizontal
Highspeed card edge connector for 1.6mm PCB's with 70 contacts (polarized)
conn samtec card-edge high-speed
0
138
136
Connector_PCBEdge
Samtec_MECF-70-01-L-DV_2x70_P1.27mm_Polarized_Socket_Horizontal
Highspeed card edge connector for 1.6mm PCB's with 70 contacts (polarized)
conn samtec card-edge high-speed
0
136
136
Connector_PCBEdge
Samtec_MECF-70-01-NP-L-DV-WT_2x70_P1.27mm_Socket_Horizontal
Highspeed card edge connector for 1.6mm PCB's with 70 contacts (not polarized)
conn samtec card-edge high-speed
0
142
140
Connector_PCBEdge
Samtec_MECF-70-01-NP-L-DV_2x70_P1.27mm_Socket_Horizontal
Highspeed card edge connector for 1.6mm PCB's with 70 contacts (not polarized)
conn samtec card-edge high-speed
0
140
140
Connector_PCBEdge
Samtec_MECF-70-02-L-DV-WT_2x70_P1.27mm_Polarized_Socket_Horizontal
Highspeed card edge connector for 2.4mm PCB's with 70 contacts (polarized)
conn samtec card-edge high-speed
0
138
136
Connector_PCBEdge
Samtec_MECF-70-02-L-DV_2x70_P1.27mm_Polarized_Socket_Horizontal
Highspeed card edge connector for 2.4mm PCB's with 70 contacts (polarized)
conn samtec card-edge high-speed
0
136
136
Connector_PCBEdge
Samtec_MECF-70-02-NP-L-DV-WT_2x70_P1.27mm_Socket_Horizontal
Highspeed card edge connector for 2.4mm PCB's with 70 contacts (not polarized)
conn samtec card-edge high-speed
0
142
140
Connector_PCBEdge
Samtec_MECF-70-02-NP-L-DV_2x70_P1.27mm_Socket_Horizontal
Highspeed card edge connector for 2.4mm PCB's with 70 contacts (not polarized)
conn samtec card-edge high-speed
0
140
140
Connector_PCBEdge
molex_EDGELOCK_2-CKT
https://www.molex.com/pdm_docs/sd/2008900106_sd.pdf
Connector PCBEdge molex EDGELOCK
0
2
2
Connector_PCBEdge
molex_EDGELOCK_4-CKT
https://www.molex.com/pdm_docs/sd/2008900106_sd.pdf
Connector PCBEdge molex EDGELOCK
0
4
4
Connector_PCBEdge
molex_EDGELOCK_6-CKT
https://www.molex.com/pdm_docs/sd/2008900106_sd.pdf
Connector PCBEdge molex EDGELOCK
0
6
6
Connector_PCBEdge
molex_EDGELOCK_8-CKT
https://www.molex.com/pdm_docs/sd/2008900106_sd.pdf
Connector PCBEdge molex EDGELOCK
0
8
8
Connector_Phoenix_GMSTB
PhoenixContact_GMSTBA_2,5_2-G-7,62_1x02_P7.62mm_Horizontal
Generic Phoenix Contact connector footprint for: GMSTBA_2,5/2-G-7,62; number of pins: 02; pin pitch: 7.62mm; Angled || order number: 1766233 12A 630V
phoenix_contact connector GMSTBA_01x02_G_7.62mm
0
2
2
Connector_Phoenix_GMSTB
PhoenixContact_GMSTBA_2,5_2-G_1x02_P7.50mm_Horizontal
Generic Phoenix Contact connector footprint for: GMSTBA_2,5/2-G; number of pins: 02; pin pitch: 7.50mm; Angled || order number: 1766343 12A 630V
phoenix_contact connector GMSTBA_01x02_G_7.50mm
0
2
2
Connector_Phoenix_GMSTB
PhoenixContact_GMSTBA_2,5_3-G-7,62_1x03_P7.62mm_Horizontal
Generic Phoenix Contact connector footprint for: GMSTBA_2,5/3-G-7,62; number of pins: 03; pin pitch: 7.62mm; Angled || order number: 1766246 12A 630V
phoenix_contact connector GMSTBA_01x03_G_7.62mm
0
3
3
Connector_Phoenix_GMSTB
PhoenixContact_GMSTBA_2,5_3-G_1x03_P7.50mm_Horizontal
Generic Phoenix Contact connector footprint for: GMSTBA_2,5/3-G; number of pins: 03; pin pitch: 7.50mm; Angled || order number: 1766356 12A 630V
phoenix_contact connector GMSTBA_01x03_G_7.50mm
0
3
3
Connector_Phoenix_GMSTB
PhoenixContact_GMSTBA_2,5_4-G-7,62_1x04_P7.62mm_Horizontal
Generic Phoenix Contact connector footprint for: GMSTBA_2,5/4-G-7,62; number of pins: 04; pin pitch: 7.62mm; Angled || order number: 1766259 12A 630V
phoenix_contact connector GMSTBA_01x04_G_7.62mm
0
4
4
Connector_Phoenix_GMSTB
PhoenixContact_GMSTBA_2,5_4-G_1x04_P7.50mm_Horizontal
Generic Phoenix Contact connector footprint for: GMSTBA_2,5/4-G; number of pins: 04; pin pitch: 7.50mm; Angled || order number: 1766369 12A 630V
phoenix_contact connector GMSTBA_01x04_G_7.50mm
0
4
4
Connector_Phoenix_GMSTB
PhoenixContact_GMSTBA_2,5_5-G-7,62_1x05_P7.62mm_Horizontal
Generic Phoenix Contact connector footprint for: GMSTBA_2,5/5-G-7,62; number of pins: 05; pin pitch: 7.62mm; Angled || order number: 1766262 12A 630V
phoenix_contact connector GMSTBA_01x05_G_7.62mm
0
5
5
Connector_Phoenix_GMSTB
PhoenixContact_GMSTBA_2,5_5-G_1x05_P7.50mm_Horizontal
Generic Phoenix Contact connector footprint for: GMSTBA_2,5/5-G; number of pins: 05; pin pitch: 7.50mm; Angled || order number: 1766372 12A 630V
phoenix_contact connector GMSTBA_01x05_G_7.50mm
0
5
5
Connector_Phoenix_GMSTB
PhoenixContact_GMSTBA_2,5_6-G-7,62_1x06_P7.62mm_Horizontal
Generic Phoenix Contact connector footprint for: GMSTBA_2,5/6-G-7,62; number of pins: 06; pin pitch: 7.62mm; Angled || order number: 1766275 12A 630V
phoenix_contact connector GMSTBA_01x06_G_7.62mm
0
6
6
Connector_Phoenix_GMSTB
PhoenixContact_GMSTBA_2,5_6-G_1x06_P7.50mm_Horizontal
Generic Phoenix Contact connector footprint for: GMSTBA_2,5/6-G; number of pins: 06; pin pitch: 7.50mm; Angled || order number: 1766385 12A 630V
phoenix_contact connector GMSTBA_01x06_G_7.50mm
0
6
6
Connector_Phoenix_GMSTB
PhoenixContact_GMSTBA_2,5_7-G-7,62_1x07_P7.62mm_Horizontal
Generic Phoenix Contact connector footprint for: GMSTBA_2,5/7-G-7,62; number of pins: 07; pin pitch: 7.62mm; Angled || order number: 1766288 12A 630V
phoenix_contact connector GMSTBA_01x07_G_7.62mm
0
7
7
Connector_Phoenix_GMSTB
PhoenixContact_GMSTBA_2,5_7-G_1x07_P7.50mm_Horizontal
Generic Phoenix Contact connector footprint for: GMSTBA_2,5/7-G; number of pins: 07; pin pitch: 7.50mm; Angled || order number: 1766398 12A 630V
phoenix_contact connector GMSTBA_01x07_G_7.50mm
0
7
7
Connector_Phoenix_GMSTB
PhoenixContact_GMSTBA_2,5_8-G-7,62_1x08_P7.62mm_Horizontal
Generic Phoenix Contact connector footprint for: GMSTBA_2,5/8-G-7,62; number of pins: 08; pin pitch: 7.62mm; Angled || order number: 1766291 12A 630V
phoenix_contact connector GMSTBA_01x08_G_7.62mm
0
8
8
Connector_Phoenix_GMSTB
PhoenixContact_GMSTBA_2,5_8-G_1x08_P7.50mm_Horizontal
Generic Phoenix Contact connector footprint for: GMSTBA_2,5/8-G; number of pins: 08; pin pitch: 7.50mm; Angled || order number: 1766408 12A 630V
phoenix_contact connector GMSTBA_01x08_G_7.50mm
0
8
8
Connector_Phoenix_GMSTB
PhoenixContact_GMSTBA_2,5_9-G-7,62_1x09_P7.62mm_Horizontal
Generic Phoenix Contact connector footprint for: GMSTBA_2,5/9-G-7,62; number of pins: 09; pin pitch: 7.62mm; Angled || order number: 1766301 12A 630V
phoenix_contact connector GMSTBA_01x09_G_7.62mm
0
9
9
Connector_Phoenix_GMSTB
PhoenixContact_GMSTBA_2,5_9-G_1x09_P7.50mm_Horizontal
Generic Phoenix Contact connector footprint for: GMSTBA_2,5/9-G; number of pins: 09; pin pitch: 7.50mm; Angled || order number: 1766411 12A 630V
phoenix_contact connector GMSTBA_01x09_G_7.50mm
0
9
9
Connector_Phoenix_GMSTB
PhoenixContact_GMSTBA_2,5_10-G-7,62_1x10_P7.62mm_Horizontal
Generic Phoenix Contact connector footprint for: GMSTBA_2,5/10-G-7,62; number of pins: 10; pin pitch: 7.62mm; Angled || order number: 1766314 12A 630V
phoenix_contact connector GMSTBA_01x10_G_7.62mm
0
10
10
Connector_Phoenix_GMSTB
PhoenixContact_GMSTBA_2,5_10-G_1x10_P7.50mm_Horizontal
Generic Phoenix Contact connector footprint for: GMSTBA_2,5/10-G; number of pins: 10; pin pitch: 7.50mm; Angled || order number: 1766424 12A 630V
phoenix_contact connector GMSTBA_01x10_G_7.50mm
0
10
10
Connector_Phoenix_GMSTB
PhoenixContact_GMSTBA_2,5_11-G-7,62_1x11_P7.62mm_Horizontal
Generic Phoenix Contact connector footprint for: GMSTBA_2,5/11-G-7,62; number of pins: 11; pin pitch: 7.62mm; Angled || order number: 1766327 12A 630V
phoenix_contact connector GMSTBA_01x11_G_7.62mm
0
11
11
Connector_Phoenix_GMSTB
PhoenixContact_GMSTBA_2,5_11-G_1x11_P7.50mm_Horizontal
Generic Phoenix Contact connector footprint for: GMSTBA_2,5/11-G; number of pins: 11; pin pitch: 7.50mm; Angled || order number: 1766437 12A 630V
phoenix_contact connector GMSTBA_01x11_G_7.50mm
0
11
11
Connector_Phoenix_GMSTB
PhoenixContact_GMSTBA_2,5_12-G-7,62_1x12_P7.62mm_Horizontal
Generic Phoenix Contact connector footprint for: GMSTBA_2,5/12-G-7,62; number of pins: 12; pin pitch: 7.62mm; Angled || order number: 1766330 12A 630V
phoenix_contact connector GMSTBA_01x12_G_7.62mm
0
12
12
Connector_Phoenix_GMSTB
PhoenixContact_GMSTBA_2,5_12-G_1x12_P7.50mm_Horizontal
Generic Phoenix Contact connector footprint for: GMSTBA_2,5/12-G; number of pins: 12; pin pitch: 7.50mm; Angled || order number: 1766440 12A 630V
phoenix_contact connector GMSTBA_01x12_G_7.50mm
0
12
12
Connector_Phoenix_GMSTB
PhoenixContact_GMSTBVA_2,5_2-G-7,62_1x02_P7.62mm_Vertical
Generic Phoenix Contact connector footprint for: GMSTBVA_2,5/2-G-7,62; number of pins: 02; pin pitch: 7.62mm; Vertical || order number: 1766770 12A 630V
phoenix_contact connector GMSTBVA_01x02_G_7.62mm
0
2
2
Connector_Phoenix_GMSTB
PhoenixContact_GMSTBVA_2,5_2-G_1x02_P7.50mm_Vertical
Generic Phoenix Contact connector footprint for: GMSTBVA_2,5/2-G; number of pins: 02; pin pitch: 7.50mm; Vertical || order number: 1766660 12A 630V
phoenix_contact connector GMSTBVA_01x02_G_7.50mm
0
2
2
Connector_Phoenix_GMSTB
PhoenixContact_GMSTBVA_2,5_3-G-7,62_1x03_P7.62mm_Vertical
Generic Phoenix Contact connector footprint for: GMSTBVA_2,5/3-G-7,62; number of pins: 03; pin pitch: 7.62mm; Vertical || order number: 1766783 12A 630V
phoenix_contact connector GMSTBVA_01x03_G_7.62mm
0
3
3
Connector_Phoenix_GMSTB
PhoenixContact_GMSTBVA_2,5_3-G_1x03_P7.50mm_Vertical
Generic Phoenix Contact connector footprint for: GMSTBVA_2,5/3-G; number of pins: 03; pin pitch: 7.50mm; Vertical || order number: 1766673 12A 630V
phoenix_contact connector GMSTBVA_01x03_G_7.50mm
0
3
3
Connector_Phoenix_GMSTB
PhoenixContact_GMSTBVA_2,5_4-G-7,62_1x04_P7.62mm_Vertical
Generic Phoenix Contact connector footprint for: GMSTBVA_2,5/4-G-7,62; number of pins: 04; pin pitch: 7.62mm; Vertical || order number: 1766796 12A 630V
phoenix_contact connector GMSTBVA_01x04_G_7.62mm
0
4
4
Connector_Phoenix_GMSTB
PhoenixContact_GMSTBVA_2,5_4-G_1x04_P7.50mm_Vertical
Generic Phoenix Contact connector footprint for: GMSTBVA_2,5/4-G; number of pins: 04; pin pitch: 7.50mm; Vertical || order number: 1766686 12A 630V
phoenix_contact connector GMSTBVA_01x04_G_7.50mm
0
4
4
Connector_Phoenix_GMSTB
PhoenixContact_GMSTBVA_2,5_5-G-7,62_1x05_P7.62mm_Vertical
Generic Phoenix Contact connector footprint for: GMSTBVA_2,5/5-G-7,62; number of pins: 05; pin pitch: 7.62mm; Vertical || order number: 1766806 12A 630V
phoenix_contact connector GMSTBVA_01x05_G_7.62mm
0
5
5
Connector_Phoenix_GMSTB
PhoenixContact_GMSTBVA_2,5_5-G_1x05_P7.50mm_Vertical
Generic Phoenix Contact connector footprint for: GMSTBVA_2,5/5-G; number of pins: 05; pin pitch: 7.50mm; Vertical || order number: 1766699 12A 630V
phoenix_contact connector GMSTBVA_01x05_G_7.50mm
0
5
5
Connector_Phoenix_GMSTB
PhoenixContact_GMSTBVA_2,5_6-G-7,62_1x06_P7.62mm_Vertical
Generic Phoenix Contact connector footprint for: GMSTBVA_2,5/6-G-7,62; number of pins: 06; pin pitch: 7.62mm; Vertical || order number: 1766819 12A 630V
phoenix_contact connector GMSTBVA_01x06_G_7.62mm
0
6
6
Connector_Phoenix_GMSTB
PhoenixContact_GMSTBVA_2,5_6-G_1x06_P7.50mm_Vertical
Generic Phoenix Contact connector footprint for: GMSTBVA_2,5/6-G; number of pins: 06; pin pitch: 7.50mm; Vertical || order number: 1766709 12A 630V
phoenix_contact connector GMSTBVA_01x06_G_7.50mm
0
6
6
Connector_Phoenix_GMSTB
PhoenixContact_GMSTBVA_2,5_7-G-7,62_1x07_P7.62mm_Vertical
Generic Phoenix Contact connector footprint for: GMSTBVA_2,5/7-G-7,62; number of pins: 07; pin pitch: 7.62mm; Vertical || order number: 1766822 12A 630V
phoenix_contact connector GMSTBVA_01x07_G_7.62mm
0
7
7
Connector_Phoenix_GMSTB
PhoenixContact_GMSTBVA_2,5_7-G_1x07_P7.50mm_Vertical
Generic Phoenix Contact connector footprint for: GMSTBVA_2,5/7-G; number of pins: 07; pin pitch: 7.50mm; Vertical || order number: 1766712 12A 630V
phoenix_contact connector GMSTBVA_01x07_G_7.50mm
0
7
7
Connector_Phoenix_GMSTB
PhoenixContact_GMSTBVA_2,5_8-G-7,62_1x08_P7.62mm_Vertical
Generic Phoenix Contact connector footprint for: GMSTBVA_2,5/8-G-7,62; number of pins: 08; pin pitch: 7.62mm; Vertical || order number: 1766835 12A 630V
phoenix_contact connector GMSTBVA_01x08_G_7.62mm
0
8
8
Connector_Phoenix_GMSTB
PhoenixContact_GMSTBVA_2,5_8-G_1x08_P7.50mm_Vertical
Generic Phoenix Contact connector footprint for: GMSTBVA_2,5/8-G; number of pins: 08; pin pitch: 7.50mm; Vertical || order number: 1766725 12A 630V
phoenix_contact connector GMSTBVA_01x08_G_7.50mm
0
8
8
Connector_Phoenix_GMSTB
PhoenixContact_GMSTBVA_2,5_9-G-7,62_1x09_P7.62mm_Vertical
Generic Phoenix Contact connector footprint for: GMSTBVA_2,5/9-G-7,62; number of pins: 09; pin pitch: 7.62mm; Vertical || order number: 1766848 12A 630V
phoenix_contact connector GMSTBVA_01x09_G_7.62mm
0
9
9
Connector_Phoenix_GMSTB
PhoenixContact_GMSTBVA_2,5_9-G_1x09_P7.50mm_Vertical
Generic Phoenix Contact connector footprint for: GMSTBVA_2,5/9-G; number of pins: 09; pin pitch: 7.50mm; Vertical || order number: 1766738 12A 630V
phoenix_contact connector GMSTBVA_01x09_G_7.50mm
0
9
9
Connector_Phoenix_GMSTB
PhoenixContact_GMSTBVA_2,5_10-G-7,62_1x10_P7.62mm_Vertical
Generic Phoenix Contact connector footprint for: GMSTBVA_2,5/10-G-7,62; number of pins: 10; pin pitch: 7.62mm; Vertical || order number: 1766851 12A 630V
phoenix_contact connector GMSTBVA_01x10_G_7.62mm
0
10
10
Connector_Phoenix_GMSTB
PhoenixContact_GMSTBVA_2,5_10-G_1x10_P7.50mm_Vertical
Generic Phoenix Contact connector footprint for: GMSTBVA_2,5/10-G; number of pins: 10; pin pitch: 7.50mm; Vertical || order number: 1766741 12A 630V
phoenix_contact connector GMSTBVA_01x10_G_7.50mm
0
10
10
Connector_Phoenix_GMSTB
PhoenixContact_GMSTBVA_2,5_11-G-7,62_1x11_P7.62mm_Vertical
Generic Phoenix Contact connector footprint for: GMSTBVA_2,5/11-G-7,62; number of pins: 11; pin pitch: 7.62mm; Vertical || order number: 1766864 12A 630V
phoenix_contact connector GMSTBVA_01x11_G_7.62mm
0
11
11
Connector_Phoenix_GMSTB
PhoenixContact_GMSTBVA_2,5_11-G_1x11_P7.50mm_Vertical
Generic Phoenix Contact connector footprint for: GMSTBVA_2,5/11-G; number of pins: 11; pin pitch: 7.50mm; Vertical || order number: 1766754 12A 630V
phoenix_contact connector GMSTBVA_01x11_G_7.50mm
0
11
11
Connector_Phoenix_GMSTB
PhoenixContact_GMSTBVA_2,5_12-G-7,62_1x12_P7.62mm_Vertical
Generic Phoenix Contact connector footprint for: GMSTBVA_2,5/12-G-7,62; number of pins: 12; pin pitch: 7.62mm; Vertical || order number: 1766877 12A 630V
phoenix_contact connector GMSTBVA_01x12_G_7.62mm
0
12
12
Connector_Phoenix_GMSTB
PhoenixContact_GMSTBVA_2,5_12-G_1x12_P7.50mm_Vertical
Generic Phoenix Contact connector footprint for: GMSTBVA_2,5/12-G; number of pins: 12; pin pitch: 7.50mm; Vertical || order number: 1766767 12A 630V
phoenix_contact connector GMSTBVA_01x12_G_7.50mm
0
12
12
Connector_Phoenix_GMSTB
PhoenixContact_GMSTBV_2,5_2-GF-7,62_1x02_P7.62mm_Vertical_ThreadedFlange
Generic Phoenix Contact connector footprint for: GMSTBV_2,5/2-GF-7,62; number of pins: 02; pin pitch: 7.62mm; Vertical; threaded flange || order number: 1829154 12A 630V
phoenix_contact connector GMSTBV_01x02_GF_7.62mm
0
2
2
Connector_Phoenix_GMSTB
PhoenixContact_GMSTBV_2,5_2-GF-7,62_1x02_P7.62mm_Vertical_ThreadedFlange_MountHole
Generic Phoenix Contact connector footprint for: GMSTBV_2,5/2-GF-7,62; number of pins: 02; pin pitch: 7.62mm; Vertical; threaded flange; footprint includes mount hole for mounting screw: ISO 1481-ST 2.2x6.5 C or ISO 7049-ST 2.2x6.5 C (http://www.fasteners.eu/standards/ISO/7049/) || order number: 1829154 12A 630V
phoenix_contact connector GMSTBV_01x02_GF_7.62mm_MH
0
2
2
Connector_Phoenix_GMSTB
PhoenixContact_GMSTBV_2,5_3-GF-7,62_1x03_P7.62mm_Vertical_ThreadedFlange
Generic Phoenix Contact connector footprint for: GMSTBV_2,5/3-GF-7,62; number of pins: 03; pin pitch: 7.62mm; Vertical; threaded flange || order number: 1829167 12A 630V
phoenix_contact connector GMSTBV_01x03_GF_7.62mm
0
3
3
Connector_Phoenix_GMSTB
PhoenixContact_GMSTBV_2,5_3-GF-7,62_1x03_P7.62mm_Vertical_ThreadedFlange_MountHole
Generic Phoenix Contact connector footprint for: GMSTBV_2,5/3-GF-7,62; number of pins: 03; pin pitch: 7.62mm; Vertical; threaded flange; footprint includes mount hole for mounting screw: ISO 1481-ST 2.2x6.5 C or ISO 7049-ST 2.2x6.5 C (http://www.fasteners.eu/standards/ISO/7049/) || order number: 1829167 12A 630V
phoenix_contact connector GMSTBV_01x03_GF_7.62mm_MH
0
3
3
Connector_Phoenix_GMSTB
PhoenixContact_GMSTBV_2,5_4-GF-7,62_1x04_P7.62mm_Vertical_ThreadedFlange
Generic Phoenix Contact connector footprint for: GMSTBV_2,5/4-GF-7,62; number of pins: 04; pin pitch: 7.62mm; Vertical; threaded flange || order number: 1829170 12A 630V
phoenix_contact connector GMSTBV_01x04_GF_7.62mm
0
4
4
Connector_Phoenix_GMSTB
PhoenixContact_GMSTBV_2,5_4-GF-7,62_1x04_P7.62mm_Vertical_ThreadedFlange_MountHole
Generic Phoenix Contact connector footprint for: GMSTBV_2,5/4-GF-7,62; number of pins: 04; pin pitch: 7.62mm; Vertical; threaded flange; footprint includes mount hole for mounting screw: ISO 1481-ST 2.2x6.5 C or ISO 7049-ST 2.2x6.5 C (http://www.fasteners.eu/standards/ISO/7049/) || order number: 1829170 12A 630V
phoenix_contact connector GMSTBV_01x04_GF_7.62mm_MH
0
4
4
Connector_Phoenix_GMSTB
PhoenixContact_GMSTBV_2,5_5-GF-7,62_1x05_P7.62mm_Vertical_ThreadedFlange
Generic Phoenix Contact connector footprint for: GMSTBV_2,5/5-GF-7,62; number of pins: 05; pin pitch: 7.62mm; Vertical; threaded flange || order number: 1829183 12A 630V
phoenix_contact connector GMSTBV_01x05_GF_7.62mm
0
5
5
Connector_Phoenix_GMSTB
PhoenixContact_GMSTBV_2,5_5-GF-7,62_1x05_P7.62mm_Vertical_ThreadedFlange_MountHole
Generic Phoenix Contact connector footprint for: GMSTBV_2,5/5-GF-7,62; number of pins: 05; pin pitch: 7.62mm; Vertical; threaded flange; footprint includes mount hole for mounting screw: ISO 1481-ST 2.2x6.5 C or ISO 7049-ST 2.2x6.5 C (http://www.fasteners.eu/standards/ISO/7049/) || order number: 1829183 12A 630V
phoenix_contact connector GMSTBV_01x05_GF_7.62mm_MH
0
5
5
Connector_Phoenix_GMSTB
PhoenixContact_GMSTBV_2,5_6-GF-7,62_1x06_P7.62mm_Vertical_ThreadedFlange
Generic Phoenix Contact connector footprint for: GMSTBV_2,5/6-GF-7,62; number of pins: 06; pin pitch: 7.62mm; Vertical; threaded flange || order number: 1829196 12A 630V
phoenix_contact connector GMSTBV_01x06_GF_7.62mm
0
6
6
Connector_Phoenix_GMSTB
PhoenixContact_GMSTBV_2,5_6-GF-7,62_1x06_P7.62mm_Vertical_ThreadedFlange_MountHole
Generic Phoenix Contact connector footprint for: GMSTBV_2,5/6-GF-7,62; number of pins: 06; pin pitch: 7.62mm; Vertical; threaded flange; footprint includes mount hole for mounting screw: ISO 1481-ST 2.2x6.5 C or ISO 7049-ST 2.2x6.5 C (http://www.fasteners.eu/standards/ISO/7049/) || order number: 1829196 12A 630V
phoenix_contact connector GMSTBV_01x06_GF_7.62mm_MH
0
6
6
Connector_Phoenix_GMSTB
PhoenixContact_GMSTBV_2,5_7-GF-7,62_1x07_P7.62mm_Vertical_ThreadedFlange
Generic Phoenix Contact connector footprint for: GMSTBV_2,5/7-GF-7,62; number of pins: 07; pin pitch: 7.62mm; Vertical; threaded flange || order number: 1829206 12A 630V
phoenix_contact connector GMSTBV_01x07_GF_7.62mm
0
7
7
Connector_Phoenix_GMSTB
PhoenixContact_GMSTBV_2,5_7-GF-7,62_1x07_P7.62mm_Vertical_ThreadedFlange_MountHole
Generic Phoenix Contact connector footprint for: GMSTBV_2,5/7-GF-7,62; number of pins: 07; pin pitch: 7.62mm; Vertical; threaded flange; footprint includes mount hole for mounting screw: ISO 1481-ST 2.2x6.5 C or ISO 7049-ST 2.2x6.5 C (http://www.fasteners.eu/standards/ISO/7049/) || order number: 1829206 12A 630V
phoenix_contact connector GMSTBV_01x07_GF_7.62mm_MH
0
7
7
Connector_Phoenix_GMSTB
PhoenixContact_GMSTBV_2,5_8-GF-7,62_1x08_P7.62mm_Vertical_ThreadedFlange
Generic Phoenix Contact connector footprint for: GMSTBV_2,5/8-GF-7,62; number of pins: 08; pin pitch: 7.62mm; Vertical; threaded flange || order number: 1829219 12A 630V
phoenix_contact connector GMSTBV_01x08_GF_7.62mm
0
8
8
Connector_Phoenix_GMSTB
PhoenixContact_GMSTBV_2,5_8-GF-7,62_1x08_P7.62mm_Vertical_ThreadedFlange_MountHole
Generic Phoenix Contact connector footprint for: GMSTBV_2,5/8-GF-7,62; number of pins: 08; pin pitch: 7.62mm; Vertical; threaded flange; footprint includes mount hole for mounting screw: ISO 1481-ST 2.2x6.5 C or ISO 7049-ST 2.2x6.5 C (http://www.fasteners.eu/standards/ISO/7049/) || order number: 1829219 12A 630V
phoenix_contact connector GMSTBV_01x08_GF_7.62mm_MH
0
8
8
Connector_Phoenix_GMSTB
PhoenixContact_GMSTBV_2,5_9-GF-7,62_1x09_P7.62mm_Vertical_ThreadedFlange
Generic Phoenix Contact connector footprint for: GMSTBV_2,5/9-GF-7,62; number of pins: 09; pin pitch: 7.62mm; Vertical; threaded flange || order number: 1829222 12A 630V
phoenix_contact connector GMSTBV_01x09_GF_7.62mm
0
9
9
Connector_Phoenix_GMSTB
PhoenixContact_GMSTBV_2,5_9-GF-7,62_1x09_P7.62mm_Vertical_ThreadedFlange_MountHole
Generic Phoenix Contact connector footprint for: GMSTBV_2,5/9-GF-7,62; number of pins: 09; pin pitch: 7.62mm; Vertical; threaded flange; footprint includes mount hole for mounting screw: ISO 1481-ST 2.2x6.5 C or ISO 7049-ST 2.2x6.5 C (http://www.fasteners.eu/standards/ISO/7049/) || order number: 1829222 12A 630V
phoenix_contact connector GMSTBV_01x09_GF_7.62mm_MH
0
9
9
Connector_Phoenix_GMSTB
PhoenixContact_GMSTBV_2,5_10-GF-7,62_1x10_P7.62mm_Vertical_ThreadedFlange
Generic Phoenix Contact connector footprint for: GMSTBV_2,5/10-GF-7,62; number of pins: 10; pin pitch: 7.62mm; Vertical; threaded flange || order number: 1829235 12A 630V
phoenix_contact connector GMSTBV_01x10_GF_7.62mm
0
10
10
Connector_Phoenix_GMSTB
PhoenixContact_GMSTBV_2,5_10-GF-7,62_1x10_P7.62mm_Vertical_ThreadedFlange_MountHole
Generic Phoenix Contact connector footprint for: GMSTBV_2,5/10-GF-7,62; number of pins: 10; pin pitch: 7.62mm; Vertical; threaded flange; footprint includes mount hole for mounting screw: ISO 1481-ST 2.2x6.5 C or ISO 7049-ST 2.2x6.5 C (http://www.fasteners.eu/standards/ISO/7049/) || order number: 1829235 12A 630V
phoenix_contact connector GMSTBV_01x10_GF_7.62mm_MH
0
10
10
Connector_Phoenix_GMSTB
PhoenixContact_GMSTBV_2,5_11-GF-7,62_1x11_P7.62mm_Vertical_ThreadedFlange
Generic Phoenix Contact connector footprint for: GMSTBV_2,5/11-GF-7,62; number of pins: 11; pin pitch: 7.62mm; Vertical; threaded flange || order number: 1829248 12A 630V
phoenix_contact connector GMSTBV_01x11_GF_7.62mm
0
11
11
Connector_Phoenix_GMSTB
PhoenixContact_GMSTBV_2,5_11-GF-7,62_1x11_P7.62mm_Vertical_ThreadedFlange_MountHole
Generic Phoenix Contact connector footprint for: GMSTBV_2,5/11-GF-7,62; number of pins: 11; pin pitch: 7.62mm; Vertical; threaded flange; footprint includes mount hole for mounting screw: ISO 1481-ST 2.2x6.5 C or ISO 7049-ST 2.2x6.5 C (http://www.fasteners.eu/standards/ISO/7049/) || order number: 1829248 12A 630V
phoenix_contact connector GMSTBV_01x11_GF_7.62mm_MH
0
11
11
Connector_Phoenix_GMSTB
PhoenixContact_GMSTBV_2,5_12-GF-7,62_1x12_P7.62mm_Vertical_ThreadedFlange
Generic Phoenix Contact connector footprint for: GMSTBV_2,5/12-GF-7,62; number of pins: 12; pin pitch: 7.62mm; Vertical; threaded flange || order number: 1829251 12A 630V
phoenix_contact connector GMSTBV_01x12_GF_7.62mm
0
12
12
Connector_Phoenix_GMSTB
PhoenixContact_GMSTBV_2,5_12-GF-7,62_1x12_P7.62mm_Vertical_ThreadedFlange_MountHole
Generic Phoenix Contact connector footprint for: GMSTBV_2,5/12-GF-7,62; number of pins: 12; pin pitch: 7.62mm; Vertical; threaded flange; footprint includes mount hole for mounting screw: ISO 1481-ST 2.2x6.5 C or ISO 7049-ST 2.2x6.5 C (http://www.fasteners.eu/standards/ISO/7049/) || order number: 1829251 12A 630V
phoenix_contact connector GMSTBV_01x12_GF_7.62mm_MH
0
12
12
Connector_Phoenix_GMSTB
PhoenixContact_GMSTB_2,5_2-GF-7,62_1x02_P7.62mm_Horizontal_ThreadedFlange
Generic Phoenix Contact connector footprint for: GMSTB_2,5/2-GF-7,62; number of pins: 02; pin pitch: 7.62mm; Angled; threaded flange || order number: 1806229 12A 630V
phoenix_contact connector GMSTB_01x02_GF_7.62mm
0
2
2
Connector_Phoenix_GMSTB
PhoenixContact_GMSTB_2,5_2-GF-7,62_1x02_P7.62mm_Horizontal_ThreadedFlange_MountHole
Generic Phoenix Contact connector footprint for: GMSTB_2,5/2-GF-7,62; number of pins: 02; pin pitch: 7.62mm; Angled; threaded flange; footprint includes mount hole for mounting screw: ISO 1481-ST 2.2x6.5 C or ISO 7049-ST 2.2x6.5 C (http://www.fasteners.eu/standards/ISO/7049/) || order number: 1806229 12A 630V
phoenix_contact connector GMSTB_01x02_GF_7.62mm_MH
0
2
2
Connector_Phoenix_GMSTB
PhoenixContact_GMSTB_2,5_3-GF-7,62_1x03_P7.62mm_Horizontal_ThreadedFlange
Generic Phoenix Contact connector footprint for: GMSTB_2,5/3-GF-7,62; number of pins: 03; pin pitch: 7.62mm; Angled; threaded flange || order number: 1806232 12A 630V
phoenix_contact connector GMSTB_01x03_GF_7.62mm
0
3
3
Connector_Phoenix_GMSTB
PhoenixContact_GMSTB_2,5_3-GF-7,62_1x03_P7.62mm_Horizontal_ThreadedFlange_MountHole
Generic Phoenix Contact connector footprint for: GMSTB_2,5/3-GF-7,62; number of pins: 03; pin pitch: 7.62mm; Angled; threaded flange; footprint includes mount hole for mounting screw: ISO 1481-ST 2.2x6.5 C or ISO 7049-ST 2.2x6.5 C (http://www.fasteners.eu/standards/ISO/7049/) || order number: 1806232 12A 630V
phoenix_contact connector GMSTB_01x03_GF_7.62mm_MH
0
3
3
Connector_Phoenix_GMSTB
PhoenixContact_GMSTB_2,5_4-GF-7,62_1x04_P7.62mm_Horizontal_ThreadedFlange
Generic Phoenix Contact connector footprint for: GMSTB_2,5/4-GF-7,62; number of pins: 04; pin pitch: 7.62mm; Angled; threaded flange || order number: 1806245 12A 630V
phoenix_contact connector GMSTB_01x04_GF_7.62mm
0
4
4
Connector_Phoenix_GMSTB
PhoenixContact_GMSTB_2,5_4-GF-7,62_1x04_P7.62mm_Horizontal_ThreadedFlange_MountHole
Generic Phoenix Contact connector footprint for: GMSTB_2,5/4-GF-7,62; number of pins: 04; pin pitch: 7.62mm; Angled; threaded flange; footprint includes mount hole for mounting screw: ISO 1481-ST 2.2x6.5 C or ISO 7049-ST 2.2x6.5 C (http://www.fasteners.eu/standards/ISO/7049/) || order number: 1806245 12A 630V
phoenix_contact connector GMSTB_01x04_GF_7.62mm_MH
0
4
4
Connector_Phoenix_GMSTB
PhoenixContact_GMSTB_2,5_5-GF-7,62_1x05_P7.62mm_Horizontal_ThreadedFlange
Generic Phoenix Contact connector footprint for: GMSTB_2,5/5-GF-7,62; number of pins: 05; pin pitch: 7.62mm; Angled; threaded flange || order number: 1806258 12A 630V
phoenix_contact connector GMSTB_01x05_GF_7.62mm
0
5
5
Connector_Phoenix_GMSTB
PhoenixContact_GMSTB_2,5_5-GF-7,62_1x05_P7.62mm_Horizontal_ThreadedFlange_MountHole
Generic Phoenix Contact connector footprint for: GMSTB_2,5/5-GF-7,62; number of pins: 05; pin pitch: 7.62mm; Angled; threaded flange; footprint includes mount hole for mounting screw: ISO 1481-ST 2.2x6.5 C or ISO 7049-ST 2.2x6.5 C (http://www.fasteners.eu/standards/ISO/7049/) || order number: 1806258 12A 630V
phoenix_contact connector GMSTB_01x05_GF_7.62mm_MH
0
5
5
Connector_Phoenix_GMSTB
PhoenixContact_GMSTB_2,5_6-GF-7,62_1x06_P7.62mm_Horizontal_ThreadedFlange
Generic Phoenix Contact connector footprint for: GMSTB_2,5/6-GF-7,62; number of pins: 06; pin pitch: 7.62mm; Angled; threaded flange || order number: 1806261 12A 630V
phoenix_contact connector GMSTB_01x06_GF_7.62mm
0
6
6
Connector_Phoenix_GMSTB
PhoenixContact_GMSTB_2,5_6-GF-7,62_1x06_P7.62mm_Horizontal_ThreadedFlange_MountHole
Generic Phoenix Contact connector footprint for: GMSTB_2,5/6-GF-7,62; number of pins: 06; pin pitch: 7.62mm; Angled; threaded flange; footprint includes mount hole for mounting screw: ISO 1481-ST 2.2x6.5 C or ISO 7049-ST 2.2x6.5 C (http://www.fasteners.eu/standards/ISO/7049/) || order number: 1806261 12A 630V
phoenix_contact connector GMSTB_01x06_GF_7.62mm_MH
0
6
6
Connector_Phoenix_GMSTB
PhoenixContact_GMSTB_2,5_7-GF-7,62_1x07_P7.62mm_Horizontal_ThreadedFlange
Generic Phoenix Contact connector footprint for: GMSTB_2,5/7-GF-7,62; number of pins: 07; pin pitch: 7.62mm; Angled; threaded flange || order number: 1806274 12A 630V
phoenix_contact connector GMSTB_01x07_GF_7.62mm
0
7
7
Connector_Phoenix_GMSTB
PhoenixContact_GMSTB_2,5_7-GF-7,62_1x07_P7.62mm_Horizontal_ThreadedFlange_MountHole
Generic Phoenix Contact connector footprint for: GMSTB_2,5/7-GF-7,62; number of pins: 07; pin pitch: 7.62mm; Angled; threaded flange; footprint includes mount hole for mounting screw: ISO 1481-ST 2.2x6.5 C or ISO 7049-ST 2.2x6.5 C (http://www.fasteners.eu/standards/ISO/7049/) || order number: 1806274 12A 630V
phoenix_contact connector GMSTB_01x07_GF_7.62mm_MH
0
7
7
Connector_Phoenix_GMSTB
PhoenixContact_GMSTB_2,5_8-GF-7,62_1x08_P7.62mm_Horizontal_ThreadedFlange
Generic Phoenix Contact connector footprint for: GMSTB_2,5/8-GF-7,62; number of pins: 08; pin pitch: 7.62mm; Angled; threaded flange || order number: 1806287 12A 630V
phoenix_contact connector GMSTB_01x08_GF_7.62mm
0
8
8
Connector_Phoenix_GMSTB
PhoenixContact_GMSTB_2,5_8-GF-7,62_1x08_P7.62mm_Horizontal_ThreadedFlange_MountHole
Generic Phoenix Contact connector footprint for: GMSTB_2,5/8-GF-7,62; number of pins: 08; pin pitch: 7.62mm; Angled; threaded flange; footprint includes mount hole for mounting screw: ISO 1481-ST 2.2x6.5 C or ISO 7049-ST 2.2x6.5 C (http://www.fasteners.eu/standards/ISO/7049/) || order number: 1806287 12A 630V
phoenix_contact connector GMSTB_01x08_GF_7.62mm_MH
0
8
8
Connector_Phoenix_GMSTB
PhoenixContact_GMSTB_2,5_9-GF-7,62_1x09_P7.62mm_Horizontal_ThreadedFlange
Generic Phoenix Contact connector footprint for: GMSTB_2,5/9-GF-7,62; number of pins: 09; pin pitch: 7.62mm; Angled; threaded flange || order number: 1806290 12A 630V
phoenix_contact connector GMSTB_01x09_GF_7.62mm
0
9
9
Connector_Phoenix_GMSTB
PhoenixContact_GMSTB_2,5_9-GF-7,62_1x09_P7.62mm_Horizontal_ThreadedFlange_MountHole
Generic Phoenix Contact connector footprint for: GMSTB_2,5/9-GF-7,62; number of pins: 09; pin pitch: 7.62mm; Angled; threaded flange; footprint includes mount hole for mounting screw: ISO 1481-ST 2.2x6.5 C or ISO 7049-ST 2.2x6.5 C (http://www.fasteners.eu/standards/ISO/7049/) || order number: 1806290 12A 630V
phoenix_contact connector GMSTB_01x09_GF_7.62mm_MH
0
9
9
Connector_Phoenix_GMSTB
PhoenixContact_GMSTB_2,5_10-GF-7,62_1x10_P7.62mm_Horizontal_ThreadedFlange
Generic Phoenix Contact connector footprint for: GMSTB_2,5/10-GF-7,62; number of pins: 10; pin pitch: 7.62mm; Angled; threaded flange || order number: 1806300 12A 630V
phoenix_contact connector GMSTB_01x10_GF_7.62mm
0
10
10
Connector_Phoenix_GMSTB
PhoenixContact_GMSTB_2,5_10-GF-7,62_1x10_P7.62mm_Horizontal_ThreadedFlange_MountHole
Generic Phoenix Contact connector footprint for: GMSTB_2,5/10-GF-7,62; number of pins: 10; pin pitch: 7.62mm; Angled; threaded flange; footprint includes mount hole for mounting screw: ISO 1481-ST 2.2x6.5 C or ISO 7049-ST 2.2x6.5 C (http://www.fasteners.eu/standards/ISO/7049/) || order number: 1806300 12A 630V
phoenix_contact connector GMSTB_01x10_GF_7.62mm_MH
0
10
10
Connector_Phoenix_GMSTB
PhoenixContact_GMSTB_2,5_11-GF-7,62_1x11_P7.62mm_Horizontal_ThreadedFlange
Generic Phoenix Contact connector footprint for: GMSTB_2,5/11-GF-7,62; number of pins: 11; pin pitch: 7.62mm; Angled; threaded flange || order number: 1806313 12A 630V
phoenix_contact connector GMSTB_01x11_GF_7.62mm
0
11
11
Connector_Phoenix_GMSTB
PhoenixContact_GMSTB_2,5_11-GF-7,62_1x11_P7.62mm_Horizontal_ThreadedFlange_MountHole
Generic Phoenix Contact connector footprint for: GMSTB_2,5/11-GF-7,62; number of pins: 11; pin pitch: 7.62mm; Angled; threaded flange; footprint includes mount hole for mounting screw: ISO 1481-ST 2.2x6.5 C or ISO 7049-ST 2.2x6.5 C (http://www.fasteners.eu/standards/ISO/7049/) || order number: 1806313 12A 630V
phoenix_contact connector GMSTB_01x11_GF_7.62mm_MH
0
11
11
Connector_Phoenix_GMSTB
PhoenixContact_GMSTB_2,5_12-GF-7,62_1x12_P7.62mm_Horizontal_ThreadedFlange
Generic Phoenix Contact connector footprint for: GMSTB_2,5/12-GF-7,62; number of pins: 12; pin pitch: 7.62mm; Angled; threaded flange || order number: 1806326 12A 630V
phoenix_contact connector GMSTB_01x12_GF_7.62mm
0
12
12
Connector_Phoenix_GMSTB
PhoenixContact_GMSTB_2,5_12-GF-7,62_1x12_P7.62mm_Horizontal_ThreadedFlange_MountHole
Generic Phoenix Contact connector footprint for: GMSTB_2,5/12-GF-7,62; number of pins: 12; pin pitch: 7.62mm; Angled; threaded flange; footprint includes mount hole for mounting screw: ISO 1481-ST 2.2x6.5 C or ISO 7049-ST 2.2x6.5 C (http://www.fasteners.eu/standards/ISO/7049/) || order number: 1806326 12A 630V
phoenix_contact connector GMSTB_01x12_GF_7.62mm_MH
0
12
12
Connector_Phoenix_MC
PhoenixContact_MCV_1,5_2-G-3.5_1x02_P3.50mm_Vertical
Generic Phoenix Contact connector footprint for: MCV_1,5/2-G-3.5; number of pins: 02; pin pitch: 3.50mm; Vertical || order number: 1843606 8A 160V
phoenix_contact connector MCV_01x02_G_3.5mm
0
2
2
Connector_Phoenix_MC
PhoenixContact_MCV_1,5_2-G-3.81_1x02_P3.81mm_Vertical
Generic Phoenix Contact connector footprint for: MCV_1,5/2-G-3.81; number of pins: 02; pin pitch: 3.81mm; Vertical || order number: 1803426 8A 160V
phoenix_contact connector MCV_01x02_G_3.81mm
0
2
2
Connector_Phoenix_MC
PhoenixContact_MCV_1,5_2-GF-3.5_1x02_P3.50mm_Vertical_ThreadedFlange
Generic Phoenix Contact connector footprint for: MCV_1,5/2-GF-3.5; number of pins: 02; pin pitch: 3.50mm; Vertical; threaded flange || order number: 1843224 8A 160V
phoenix_contact connector MCV_01x02_GF_3.5mm
0
2
2
Connector_Phoenix_MC
PhoenixContact_MCV_1,5_2-GF-3.5_1x02_P3.50mm_Vertical_ThreadedFlange_MountHole
Generic Phoenix Contact connector footprint for: MCV_1,5/2-GF-3.5; number of pins: 02; pin pitch: 3.50mm; Vertical; threaded flange; footprint includes mount hole for mounting screw: ISO 1481-ST 2.2x4.5 C or ISO 7049-ST 2.2x4.5 C (http://www.fasteners.eu/standards/ISO/7049/) || order number: 1843224 8A 160V
phoenix_contact connector MCV_01x02_GF_3.5mm_MH
0
2
2
Connector_Phoenix_MC
PhoenixContact_MCV_1,5_2-GF-3.81_1x02_P3.81mm_Vertical_ThreadedFlange
Generic Phoenix Contact connector footprint for: MCV_1,5/2-GF-3.81; number of pins: 02; pin pitch: 3.81mm; Vertical; threaded flange || order number: 1830596 8A 160V
phoenix_contact connector MCV_01x02_GF_3.81mm
0
2
2
Connector_Phoenix_MC
PhoenixContact_MCV_1,5_2-GF-3.81_1x02_P3.81mm_Vertical_ThreadedFlange_MountHole
Generic Phoenix Contact connector footprint for: MCV_1,5/2-GF-3.81; number of pins: 02; pin pitch: 3.81mm; Vertical; threaded flange; footprint includes mount hole for mounting screw: ISO 1481-ST 2.2x4.5 C or ISO 7049-ST 2.2x4.5 C (http://www.fasteners.eu/standards/ISO/7049/) || order number: 1830596 8A 160V
phoenix_contact connector MCV_01x02_GF_3.81mm_MH
0
2
2
Connector_Phoenix_MC
PhoenixContact_MCV_1,5_3-G-3.5_1x03_P3.50mm_Vertical
Generic Phoenix Contact connector footprint for: MCV_1,5/3-G-3.5; number of pins: 03; pin pitch: 3.50mm; Vertical || order number: 1843619 8A 160V
phoenix_contact connector MCV_01x03_G_3.5mm
0
3
3
Connector_Phoenix_MC
PhoenixContact_MCV_1,5_3-G-3.81_1x03_P3.81mm_Vertical
Generic Phoenix Contact connector footprint for: MCV_1,5/3-G-3.81; number of pins: 03; pin pitch: 3.81mm; Vertical || order number: 1803439 8A 160V
phoenix_contact connector MCV_01x03_G_3.81mm
0
3
3
Connector_Phoenix_MC
PhoenixContact_MCV_1,5_3-GF-3.5_1x03_P3.50mm_Vertical_ThreadedFlange
Generic Phoenix Contact connector footprint for: MCV_1,5/3-GF-3.5; number of pins: 03; pin pitch: 3.50mm; Vertical; threaded flange || order number: 1843237 8A 160V
phoenix_contact connector MCV_01x03_GF_3.5mm
0
3
3
Connector_Phoenix_MC
PhoenixContact_MCV_1,5_3-GF-3.5_1x03_P3.50mm_Vertical_ThreadedFlange_MountHole
Generic Phoenix Contact connector footprint for: MCV_1,5/3-GF-3.5; number of pins: 03; pin pitch: 3.50mm; Vertical; threaded flange; footprint includes mount hole for mounting screw: ISO 1481-ST 2.2x4.5 C or ISO 7049-ST 2.2x4.5 C (http://www.fasteners.eu/standards/ISO/7049/) || order number: 1843237 8A 160V
phoenix_contact connector MCV_01x03_GF_3.5mm_MH
0
3
3
Connector_Phoenix_MC
PhoenixContact_MCV_1,5_3-GF-3.81_1x03_P3.81mm_Vertical_ThreadedFlange
Generic Phoenix Contact connector footprint for: MCV_1,5/3-GF-3.81; number of pins: 03; pin pitch: 3.81mm; Vertical; threaded flange || order number: 1830606 8A 160V
phoenix_contact connector MCV_01x03_GF_3.81mm
0
3
3
Connector_Phoenix_MC
PhoenixContact_MCV_1,5_3-GF-3.81_1x03_P3.81mm_Vertical_ThreadedFlange_MountHole
Generic Phoenix Contact connector footprint for: MCV_1,5/3-GF-3.81; number of pins: 03; pin pitch: 3.81mm; Vertical; threaded flange; footprint includes mount hole for mounting screw: ISO 1481-ST 2.2x4.5 C or ISO 7049-ST 2.2x4.5 C (http://www.fasteners.eu/standards/ISO/7049/) || order number: 1830606 8A 160V
phoenix_contact connector MCV_01x03_GF_3.81mm_MH
0
3
3
Connector_Phoenix_MC
PhoenixContact_MCV_1,5_4-G-3.5_1x04_P3.50mm_Vertical
Generic Phoenix Contact connector footprint for: MCV_1,5/4-G-3.5; number of pins: 04; pin pitch: 3.50mm; Vertical || order number: 1843622 8A 160V
phoenix_contact connector MCV_01x04_G_3.5mm
0
4
4
Connector_Phoenix_MC
PhoenixContact_MCV_1,5_4-G-3.81_1x04_P3.81mm_Vertical
Generic Phoenix Contact connector footprint for: MCV_1,5/4-G-3.81; number of pins: 04; pin pitch: 3.81mm; Vertical || order number: 1803442 8A 160V
phoenix_contact connector MCV_01x04_G_3.81mm
0
4
4
Connector_Phoenix_MC
PhoenixContact_MCV_1,5_4-GF-3.5_1x04_P3.50mm_Vertical_ThreadedFlange
Generic Phoenix Contact connector footprint for: MCV_1,5/4-GF-3.5; number of pins: 04; pin pitch: 3.50mm; Vertical; threaded flange || order number: 1843240 8A 160V
phoenix_contact connector MCV_01x04_GF_3.5mm
0
4
4
Connector_Phoenix_MC
PhoenixContact_MCV_1,5_4-GF-3.5_1x04_P3.50mm_Vertical_ThreadedFlange_MountHole
Generic Phoenix Contact connector footprint for: MCV_1,5/4-GF-3.5; number of pins: 04; pin pitch: 3.50mm; Vertical; threaded flange; footprint includes mount hole for mounting screw: ISO 1481-ST 2.2x4.5 C or ISO 7049-ST 2.2x4.5 C (http://www.fasteners.eu/standards/ISO/7049/) || order number: 1843240 8A 160V
phoenix_contact connector MCV_01x04_GF_3.5mm_MH
0
4
4
Connector_Phoenix_MC
PhoenixContact_MCV_1,5_4-GF-3.81_1x04_P3.81mm_Vertical_ThreadedFlange
Generic Phoenix Contact connector footprint for: MCV_1,5/4-GF-3.81; number of pins: 04; pin pitch: 3.81mm; Vertical; threaded flange || order number: 1830619 8A 160V
phoenix_contact connector MCV_01x04_GF_3.81mm
0
4
4
Connector_Phoenix_MC
PhoenixContact_MCV_1,5_4-GF-3.81_1x04_P3.81mm_Vertical_ThreadedFlange_MountHole
Generic Phoenix Contact connector footprint for: MCV_1,5/4-GF-3.81; number of pins: 04; pin pitch: 3.81mm; Vertical; threaded flange; footprint includes mount hole for mounting screw: ISO 1481-ST 2.2x4.5 C or ISO 7049-ST 2.2x4.5 C (http://www.fasteners.eu/standards/ISO/7049/) || order number: 1830619 8A 160V
phoenix_contact connector MCV_01x04_GF_3.81mm_MH
0
4
4
Connector_Phoenix_MC
PhoenixContact_MCV_1,5_5-G-3.5_1x05_P3.50mm_Vertical
Generic Phoenix Contact connector footprint for: MCV_1,5/5-G-3.5; number of pins: 05; pin pitch: 3.50mm; Vertical || order number: 1843635 8A 160V
phoenix_contact connector MCV_01x05_G_3.5mm
0
5
5
Connector_Phoenix_MC
PhoenixContact_MCV_1,5_5-G-3.81_1x05_P3.81mm_Vertical
Generic Phoenix Contact connector footprint for: MCV_1,5/5-G-3.81; number of pins: 05; pin pitch: 3.81mm; Vertical || order number: 1803455 8A 160V
phoenix_contact connector MCV_01x05_G_3.81mm
0
5
5
Connector_Phoenix_MC
PhoenixContact_MCV_1,5_5-GF-3.5_1x05_P3.50mm_Vertical_ThreadedFlange
Generic Phoenix Contact connector footprint for: MCV_1,5/5-GF-3.5; number of pins: 05; pin pitch: 3.50mm; Vertical; threaded flange || order number: 1843253 8A 160V
phoenix_contact connector MCV_01x05_GF_3.5mm
0
5
5
Connector_Phoenix_MC
PhoenixContact_MCV_1,5_5-GF-3.5_1x05_P3.50mm_Vertical_ThreadedFlange_MountHole
Generic Phoenix Contact connector footprint for: MCV_1,5/5-GF-3.5; number of pins: 05; pin pitch: 3.50mm; Vertical; threaded flange; footprint includes mount hole for mounting screw: ISO 1481-ST 2.2x4.5 C or ISO 7049-ST 2.2x4.5 C (http://www.fasteners.eu/standards/ISO/7049/) || order number: 1843253 8A 160V
phoenix_contact connector MCV_01x05_GF_3.5mm_MH
0
5
5
Connector_Phoenix_MC
PhoenixContact_MCV_1,5_5-GF-3.81_1x05_P3.81mm_Vertical_ThreadedFlange
Generic Phoenix Contact connector footprint for: MCV_1,5/5-GF-3.81; number of pins: 05; pin pitch: 3.81mm; Vertical; threaded flange || order number: 1830622 8A 160V
phoenix_contact connector MCV_01x05_GF_3.81mm
0
5
5
Connector_Phoenix_MC
PhoenixContact_MCV_1,5_5-GF-3.81_1x05_P3.81mm_Vertical_ThreadedFlange_MountHole
Generic Phoenix Contact connector footprint for: MCV_1,5/5-GF-3.81; number of pins: 05; pin pitch: 3.81mm; Vertical; threaded flange; footprint includes mount hole for mounting screw: ISO 1481-ST 2.2x4.5 C or ISO 7049-ST 2.2x4.5 C (http://www.fasteners.eu/standards/ISO/7049/) || order number: 1830622 8A 160V
phoenix_contact connector MCV_01x05_GF_3.81mm_MH
0
5
5
Connector_Phoenix_MC
PhoenixContact_MCV_1,5_6-G-3.5_1x06_P3.50mm_Vertical
Generic Phoenix Contact connector footprint for: MCV_1,5/6-G-3.5; number of pins: 06; pin pitch: 3.50mm; Vertical || order number: 1843648 8A 160V
phoenix_contact connector MCV_01x06_G_3.5mm
0
6
6
Connector_Phoenix_MC
PhoenixContact_MCV_1,5_6-G-3.81_1x06_P3.81mm_Vertical
Generic Phoenix Contact connector footprint for: MCV_1,5/6-G-3.81; number of pins: 06; pin pitch: 3.81mm; Vertical || order number: 1803468 8A 160V
phoenix_contact connector MCV_01x06_G_3.81mm
0
6
6
Connector_Phoenix_MC
PhoenixContact_MCV_1,5_6-GF-3.5_1x06_P3.50mm_Vertical_ThreadedFlange
Generic Phoenix Contact connector footprint for: MCV_1,5/6-GF-3.5; number of pins: 06; pin pitch: 3.50mm; Vertical; threaded flange || order number: 1843266 8A 160V
phoenix_contact connector MCV_01x06_GF_3.5mm
0
6
6
Connector_Phoenix_MC
PhoenixContact_MCV_1,5_6-GF-3.5_1x06_P3.50mm_Vertical_ThreadedFlange_MountHole
Generic Phoenix Contact connector footprint for: MCV_1,5/6-GF-3.5; number of pins: 06; pin pitch: 3.50mm; Vertical; threaded flange; footprint includes mount hole for mounting screw: ISO 1481-ST 2.2x4.5 C or ISO 7049-ST 2.2x4.5 C (http://www.fasteners.eu/standards/ISO/7049/) || order number: 1843266 8A 160V
phoenix_contact connector MCV_01x06_GF_3.5mm_MH
0
6
6
Connector_Phoenix_MC
PhoenixContact_MCV_1,5_6-GF-3.81_1x06_P3.81mm_Vertical_ThreadedFlange
Generic Phoenix Contact connector footprint for: MCV_1,5/6-GF-3.81; number of pins: 06; pin pitch: 3.81mm; Vertical; threaded flange || order number: 1830635 8A 160V
phoenix_contact connector MCV_01x06_GF_3.81mm
0
6
6
Connector_Phoenix_MC
PhoenixContact_MCV_1,5_6-GF-3.81_1x06_P3.81mm_Vertical_ThreadedFlange_MountHole
Generic Phoenix Contact connector footprint for: MCV_1,5/6-GF-3.81; number of pins: 06; pin pitch: 3.81mm; Vertical; threaded flange; footprint includes mount hole for mounting screw: ISO 1481-ST 2.2x4.5 C or ISO 7049-ST 2.2x4.5 C (http://www.fasteners.eu/standards/ISO/7049/) || order number: 1830635 8A 160V
phoenix_contact connector MCV_01x06_GF_3.81mm_MH
0
6
6
Connector_Phoenix_MC
PhoenixContact_MCV_1,5_7-G-3.5_1x07_P3.50mm_Vertical
Generic Phoenix Contact connector footprint for: MCV_1,5/7-G-3.5; number of pins: 07; pin pitch: 3.50mm; Vertical || order number: 1843651 8A 160V
phoenix_contact connector MCV_01x07_G_3.5mm
0
7
7
Connector_Phoenix_MC
PhoenixContact_MCV_1,5_7-G-3.81_1x07_P3.81mm_Vertical
Generic Phoenix Contact connector footprint for: MCV_1,5/7-G-3.81; number of pins: 07; pin pitch: 3.81mm; Vertical || order number: 1803471 8A 160V
phoenix_contact connector MCV_01x07_G_3.81mm
0
7
7
Connector_Phoenix_MC
PhoenixContact_MCV_1,5_7-GF-3.5_1x07_P3.50mm_Vertical_ThreadedFlange
Generic Phoenix Contact connector footprint for: MCV_1,5/7-GF-3.5; number of pins: 07; pin pitch: 3.50mm; Vertical; threaded flange || order number: 1843279 8A 160V
phoenix_contact connector MCV_01x07_GF_3.5mm
0
7
7
Connector_Phoenix_MC
PhoenixContact_MCV_1,5_7-GF-3.5_1x07_P3.50mm_Vertical_ThreadedFlange_MountHole
Generic Phoenix Contact connector footprint for: MCV_1,5/7-GF-3.5; number of pins: 07; pin pitch: 3.50mm; Vertical; threaded flange; footprint includes mount hole for mounting screw: ISO 1481-ST 2.2x4.5 C or ISO 7049-ST 2.2x4.5 C (http://www.fasteners.eu/standards/ISO/7049/) || order number: 1843279 8A 160V
phoenix_contact connector MCV_01x07_GF_3.5mm_MH
0
7
7
Connector_Phoenix_MC
PhoenixContact_MCV_1,5_7-GF-3.81_1x07_P3.81mm_Vertical_ThreadedFlange
Generic Phoenix Contact connector footprint for: MCV_1,5/7-GF-3.81; number of pins: 07; pin pitch: 3.81mm; Vertical; threaded flange || order number: 1830648 8A 160V
phoenix_contact connector MCV_01x07_GF_3.81mm
0
7
7
Connector_Phoenix_MC
PhoenixContact_MCV_1,5_7-GF-3.81_1x07_P3.81mm_Vertical_ThreadedFlange_MountHole
Generic Phoenix Contact connector footprint for: MCV_1,5/7-GF-3.81; number of pins: 07; pin pitch: 3.81mm; Vertical; threaded flange; footprint includes mount hole for mounting screw: ISO 1481-ST 2.2x4.5 C or ISO 7049-ST 2.2x4.5 C (http://www.fasteners.eu/standards/ISO/7049/) || order number: 1830648 8A 160V
phoenix_contact connector MCV_01x07_GF_3.81mm_MH
0
7
7
Connector_Phoenix_MC
PhoenixContact_MCV_1,5_8-G-3.5_1x08_P3.50mm_Vertical
Generic Phoenix Contact connector footprint for: MCV_1,5/8-G-3.5; number of pins: 08; pin pitch: 3.50mm; Vertical || order number: 1843664 8A 160V
phoenix_contact connector MCV_01x08_G_3.5mm
0
8
8
Connector_Phoenix_MC
PhoenixContact_MCV_1,5_8-G-3.81_1x08_P3.81mm_Vertical
Generic Phoenix Contact connector footprint for: MCV_1,5/8-G-3.81; number of pins: 08; pin pitch: 3.81mm; Vertical || order number: 1803484 8A 160V
phoenix_contact connector MCV_01x08_G_3.81mm
0
8
8
Connector_Phoenix_MC
PhoenixContact_MCV_1,5_8-GF-3.5_1x08_P3.50mm_Vertical_ThreadedFlange
Generic Phoenix Contact connector footprint for: MCV_1,5/8-GF-3.5; number of pins: 08; pin pitch: 3.50mm; Vertical; threaded flange || order number: 1843282 8A 160V
phoenix_contact connector MCV_01x08_GF_3.5mm
0
8
8
Connector_Phoenix_MC
PhoenixContact_MCV_1,5_8-GF-3.5_1x08_P3.50mm_Vertical_ThreadedFlange_MountHole
Generic Phoenix Contact connector footprint for: MCV_1,5/8-GF-3.5; number of pins: 08; pin pitch: 3.50mm; Vertical; threaded flange; footprint includes mount hole for mounting screw: ISO 1481-ST 2.2x4.5 C or ISO 7049-ST 2.2x4.5 C (http://www.fasteners.eu/standards/ISO/7049/) || order number: 1843282 8A 160V
phoenix_contact connector MCV_01x08_GF_3.5mm_MH
0
8
8
Connector_Phoenix_MC
PhoenixContact_MCV_1,5_8-GF-3.81_1x08_P3.81mm_Vertical_ThreadedFlange
Generic Phoenix Contact connector footprint for: MCV_1,5/8-GF-3.81; number of pins: 08; pin pitch: 3.81mm; Vertical; threaded flange || order number: 1830651 8A 160V
phoenix_contact connector MCV_01x08_GF_3.81mm
0
8
8
Connector_Phoenix_MC
PhoenixContact_MCV_1,5_8-GF-3.81_1x08_P3.81mm_Vertical_ThreadedFlange_MountHole
Generic Phoenix Contact connector footprint for: MCV_1,5/8-GF-3.81; number of pins: 08; pin pitch: 3.81mm; Vertical; threaded flange; footprint includes mount hole for mounting screw: ISO 1481-ST 2.2x4.5 C or ISO 7049-ST 2.2x4.5 C (http://www.fasteners.eu/standards/ISO/7049/) || order number: 1830651 8A 160V
phoenix_contact connector MCV_01x08_GF_3.81mm_MH
0
8
8
Connector_Phoenix_MC
PhoenixContact_MCV_1,5_9-G-3.5_1x09_P3.50mm_Vertical
Generic Phoenix Contact connector footprint for: MCV_1,5/9-G-3.5; number of pins: 09; pin pitch: 3.50mm; Vertical || order number: 1843677 8A 160V
phoenix_contact connector MCV_01x09_G_3.5mm
0
9
9
Connector_Phoenix_MC
PhoenixContact_MCV_1,5_9-G-3.81_1x09_P3.81mm_Vertical
Generic Phoenix Contact connector footprint for: MCV_1,5/9-G-3.81; number of pins: 09; pin pitch: 3.81mm; Vertical || order number: 1803497 8A 160V
phoenix_contact connector MCV_01x09_G_3.81mm
0
9
9
Connector_Phoenix_MC
PhoenixContact_MCV_1,5_9-GF-3.5_1x09_P3.50mm_Vertical_ThreadedFlange
Generic Phoenix Contact connector footprint for: MCV_1,5/9-GF-3.5; number of pins: 09; pin pitch: 3.50mm; Vertical; threaded flange || order number: 1843295 8A 160V
phoenix_contact connector MCV_01x09_GF_3.5mm
0
9
9
Connector_Phoenix_MC
PhoenixContact_MCV_1,5_9-GF-3.5_1x09_P3.50mm_Vertical_ThreadedFlange_MountHole
Generic Phoenix Contact connector footprint for: MCV_1,5/9-GF-3.5; number of pins: 09; pin pitch: 3.50mm; Vertical; threaded flange; footprint includes mount hole for mounting screw: ISO 1481-ST 2.2x4.5 C or ISO 7049-ST 2.2x4.5 C (http://www.fasteners.eu/standards/ISO/7049/) || order number: 1843295 8A 160V
phoenix_contact connector MCV_01x09_GF_3.5mm_MH
0
9
9
Connector_Phoenix_MC
PhoenixContact_MCV_1,5_9-GF-3.81_1x09_P3.81mm_Vertical_ThreadedFlange
Generic Phoenix Contact connector footprint for: MCV_1,5/9-GF-3.81; number of pins: 09; pin pitch: 3.81mm; Vertical; threaded flange || order number: 1830664 8A 160V
phoenix_contact connector MCV_01x09_GF_3.81mm
0
9
9
Connector_Phoenix_MC
PhoenixContact_MCV_1,5_9-GF-3.81_1x09_P3.81mm_Vertical_ThreadedFlange_MountHole
Generic Phoenix Contact connector footprint for: MCV_1,5/9-GF-3.81; number of pins: 09; pin pitch: 3.81mm; Vertical; threaded flange; footprint includes mount hole for mounting screw: ISO 1481-ST 2.2x4.5 C or ISO 7049-ST 2.2x4.5 C (http://www.fasteners.eu/standards/ISO/7049/) || order number: 1830664 8A 160V
phoenix_contact connector MCV_01x09_GF_3.81mm_MH
0
9
9
Connector_Phoenix_MC
PhoenixContact_MCV_1,5_10-G-3.5_1x10_P3.50mm_Vertical
Generic Phoenix Contact connector footprint for: MCV_1,5/10-G-3.5; number of pins: 10; pin pitch: 3.50mm; Vertical || order number: 1843680 8A 160V
phoenix_contact connector MCV_01x10_G_3.5mm
0
10
10
Connector_Phoenix_MC
PhoenixContact_MCV_1,5_10-G-3.81_1x10_P3.81mm_Vertical
Generic Phoenix Contact connector footprint for: MCV_1,5/10-G-3.81; number of pins: 10; pin pitch: 3.81mm; Vertical || order number: 1803507 8A 160V
phoenix_contact connector MCV_01x10_G_3.81mm
0
10
10
Connector_Phoenix_MC
PhoenixContact_MCV_1,5_10-GF-3.5_1x10_P3.50mm_Vertical_ThreadedFlange
Generic Phoenix Contact connector footprint for: MCV_1,5/10-GF-3.5; number of pins: 10; pin pitch: 3.50mm; Vertical; threaded flange || order number: 1843305 8A 160V
phoenix_contact connector MCV_01x10_GF_3.5mm
0
10
10
Connector_Phoenix_MC
PhoenixContact_MCV_1,5_10-GF-3.5_1x10_P3.50mm_Vertical_ThreadedFlange_MountHole
Generic Phoenix Contact connector footprint for: MCV_1,5/10-GF-3.5; number of pins: 10; pin pitch: 3.50mm; Vertical; threaded flange; footprint includes mount hole for mounting screw: ISO 1481-ST 2.2x4.5 C or ISO 7049-ST 2.2x4.5 C (http://www.fasteners.eu/standards/ISO/7049/) || order number: 1843305 8A 160V
phoenix_contact connector MCV_01x10_GF_3.5mm_MH
0
10
10
Connector_Phoenix_MC
PhoenixContact_MCV_1,5_10-GF-3.81_1x10_P3.81mm_Vertical_ThreadedFlange
Generic Phoenix Contact connector footprint for: MCV_1,5/10-GF-3.81; number of pins: 10; pin pitch: 3.81mm; Vertical; threaded flange || order number: 1830677 8A 160V
phoenix_contact connector MCV_01x10_GF_3.81mm
0
10
10
Connector_Phoenix_MC
PhoenixContact_MCV_1,5_10-GF-3.81_1x10_P3.81mm_Vertical_ThreadedFlange_MountHole
Generic Phoenix Contact connector footprint for: MCV_1,5/10-GF-3.81; number of pins: 10; pin pitch: 3.81mm; Vertical; threaded flange; footprint includes mount hole for mounting screw: ISO 1481-ST 2.2x4.5 C or ISO 7049-ST 2.2x4.5 C (http://www.fasteners.eu/standards/ISO/7049/) || order number: 1830677 8A 160V
phoenix_contact connector MCV_01x10_GF_3.81mm_MH
0
10
10
Connector_Phoenix_MC
PhoenixContact_MCV_1,5_11-G-3.5_1x11_P3.50mm_Vertical
Generic Phoenix Contact connector footprint for: MCV_1,5/11-G-3.5; number of pins: 11; pin pitch: 3.50mm; Vertical || order number: 1843693 8A 160V
phoenix_contact connector MCV_01x11_G_3.5mm
0
11
11
Connector_Phoenix_MC
PhoenixContact_MCV_1,5_11-G-3.81_1x11_P3.81mm_Vertical
Generic Phoenix Contact connector footprint for: MCV_1,5/11-G-3.81; number of pins: 11; pin pitch: 3.81mm; Vertical || order number: 1803510 8A 160V
phoenix_contact connector MCV_01x11_G_3.81mm
0
11
11
Connector_Phoenix_MC
PhoenixContact_MCV_1,5_11-GF-3.5_1x11_P3.50mm_Vertical_ThreadedFlange
Generic Phoenix Contact connector footprint for: MCV_1,5/11-GF-3.5; number of pins: 11; pin pitch: 3.50mm; Vertical; threaded flange || order number: 1843318 8A 160V
phoenix_contact connector MCV_01x11_GF_3.5mm
0
11
11
Connector_Phoenix_MC
PhoenixContact_MCV_1,5_11-GF-3.5_1x11_P3.50mm_Vertical_ThreadedFlange_MountHole
Generic Phoenix Contact connector footprint for: MCV_1,5/11-GF-3.5; number of pins: 11; pin pitch: 3.50mm; Vertical; threaded flange; footprint includes mount hole for mounting screw: ISO 1481-ST 2.2x4.5 C or ISO 7049-ST 2.2x4.5 C (http://www.fasteners.eu/standards/ISO/7049/) || order number: 1843318 8A 160V
phoenix_contact connector MCV_01x11_GF_3.5mm_MH
0
11
11
Connector_Phoenix_MC
PhoenixContact_MCV_1,5_11-GF-3.81_1x11_P3.81mm_Vertical_ThreadedFlange
Generic Phoenix Contact connector footprint for: MCV_1,5/11-GF-3.81; number of pins: 11; pin pitch: 3.81mm; Vertical; threaded flange || order number: 1830680 8A 160V
phoenix_contact connector MCV_01x11_GF_3.81mm
0
11
11
Connector_Phoenix_MC
PhoenixContact_MCV_1,5_11-GF-3.81_1x11_P3.81mm_Vertical_ThreadedFlange_MountHole
Generic Phoenix Contact connector footprint for: MCV_1,5/11-GF-3.81; number of pins: 11; pin pitch: 3.81mm; Vertical; threaded flange; footprint includes mount hole for mounting screw: ISO 1481-ST 2.2x4.5 C or ISO 7049-ST 2.2x4.5 C (http://www.fasteners.eu/standards/ISO/7049/) || order number: 1830680 8A 160V
phoenix_contact connector MCV_01x11_GF_3.81mm_MH
0
11
11
Connector_Phoenix_MC
PhoenixContact_MCV_1,5_12-G-3.5_1x12_P3.50mm_Vertical
Generic Phoenix Contact connector footprint for: MCV_1,5/12-G-3.5; number of pins: 12; pin pitch: 3.50mm; Vertical || order number: 1843703 8A 160V
phoenix_contact connector MCV_01x12_G_3.5mm
0
12
12
Connector_Phoenix_MC
PhoenixContact_MCV_1,5_12-G-3.81_1x12_P3.81mm_Vertical
Generic Phoenix Contact connector footprint for: MCV_1,5/12-G-3.81; number of pins: 12; pin pitch: 3.81mm; Vertical || order number: 1803523 8A 160V
phoenix_contact connector MCV_01x12_G_3.81mm
0
12
12
Connector_Phoenix_MC
PhoenixContact_MCV_1,5_12-GF-3.5_1x12_P3.50mm_Vertical_ThreadedFlange
Generic Phoenix Contact connector footprint for: MCV_1,5/12-GF-3.5; number of pins: 12; pin pitch: 3.50mm; Vertical; threaded flange || order number: 1843321 8A 160V
phoenix_contact connector MCV_01x12_GF_3.5mm
0
12
12
Connector_Phoenix_MC
PhoenixContact_MCV_1,5_12-GF-3.5_1x12_P3.50mm_Vertical_ThreadedFlange_MountHole
Generic Phoenix Contact connector footprint for: MCV_1,5/12-GF-3.5; number of pins: 12; pin pitch: 3.50mm; Vertical; threaded flange; footprint includes mount hole for mounting screw: ISO 1481-ST 2.2x4.5 C or ISO 7049-ST 2.2x4.5 C (http://www.fasteners.eu/standards/ISO/7049/) || order number: 1843321 8A 160V
phoenix_contact connector MCV_01x12_GF_3.5mm_MH
0
12
12
Connector_Phoenix_MC
PhoenixContact_MCV_1,5_12-GF-3.81_1x12_P3.81mm_Vertical_ThreadedFlange
Generic Phoenix Contact connector footprint for: MCV_1,5/12-GF-3.81; number of pins: 12; pin pitch: 3.81mm; Vertical; threaded flange || order number: 1830693 8A 160V
phoenix_contact connector MCV_01x12_GF_3.81mm
0
12
12
Connector_Phoenix_MC
PhoenixContact_MCV_1,5_12-GF-3.81_1x12_P3.81mm_Vertical_ThreadedFlange_MountHole
Generic Phoenix Contact connector footprint for: MCV_1,5/12-GF-3.81; number of pins: 12; pin pitch: 3.81mm; Vertical; threaded flange; footprint includes mount hole for mounting screw: ISO 1481-ST 2.2x4.5 C or ISO 7049-ST 2.2x4.5 C (http://www.fasteners.eu/standards/ISO/7049/) || order number: 1830693 8A 160V
phoenix_contact connector MCV_01x12_GF_3.81mm_MH
0
12
12
Connector_Phoenix_MC
PhoenixContact_MCV_1,5_13-G-3.5_1x13_P3.50mm_Vertical
Generic Phoenix Contact connector footprint for: MCV_1,5/13-G-3.5; number of pins: 13; pin pitch: 3.50mm; Vertical || order number: 1843716 8A 160V
phoenix_contact connector MCV_01x13_G_3.5mm
0
13
13
Connector_Phoenix_MC
PhoenixContact_MCV_1,5_13-G-3.81_1x13_P3.81mm_Vertical
Generic Phoenix Contact connector footprint for: MCV_1,5/13-G-3.81; number of pins: 13; pin pitch: 3.81mm; Vertical || order number: 1803536 8A 160V
phoenix_contact connector MCV_01x13_G_3.81mm
0
13
13
Connector_Phoenix_MC
PhoenixContact_MCV_1,5_13-GF-3.5_1x13_P3.50mm_Vertical_ThreadedFlange
Generic Phoenix Contact connector footprint for: MCV_1,5/13-GF-3.5; number of pins: 13; pin pitch: 3.50mm; Vertical; threaded flange || order number: 1843334 8A 160V
phoenix_contact connector MCV_01x13_GF_3.5mm
0
13
13
Connector_Phoenix_MC
PhoenixContact_MCV_1,5_13-GF-3.5_1x13_P3.50mm_Vertical_ThreadedFlange_MountHole
Generic Phoenix Contact connector footprint for: MCV_1,5/13-GF-3.5; number of pins: 13; pin pitch: 3.50mm; Vertical; threaded flange; footprint includes mount hole for mounting screw: ISO 1481-ST 2.2x4.5 C or ISO 7049-ST 2.2x4.5 C (http://www.fasteners.eu/standards/ISO/7049/) || order number: 1843334 8A 160V
phoenix_contact connector MCV_01x13_GF_3.5mm_MH
0
13
13
Connector_Phoenix_MC
PhoenixContact_MCV_1,5_13-GF-3.81_1x13_P3.81mm_Vertical_ThreadedFlange
Generic Phoenix Contact connector footprint for: MCV_1,5/13-GF-3.81; number of pins: 13; pin pitch: 3.81mm; Vertical; threaded flange || order number: 1830703 8A 160V
phoenix_contact connector MCV_01x13_GF_3.81mm
0
13
13
Connector_Phoenix_MC
PhoenixContact_MCV_1,5_13-GF-3.81_1x13_P3.81mm_Vertical_ThreadedFlange_MountHole
Generic Phoenix Contact connector footprint for: MCV_1,5/13-GF-3.81; number of pins: 13; pin pitch: 3.81mm; Vertical; threaded flange; footprint includes mount hole for mounting screw: ISO 1481-ST 2.2x4.5 C or ISO 7049-ST 2.2x4.5 C (http://www.fasteners.eu/standards/ISO/7049/) || order number: 1830703 8A 160V
phoenix_contact connector MCV_01x13_GF_3.81mm_MH
0
13
13
Connector_Phoenix_MC
PhoenixContact_MCV_1,5_14-G-3.5_1x14_P3.50mm_Vertical
Generic Phoenix Contact connector footprint for: MCV_1,5/14-G-3.5; number of pins: 14; pin pitch: 3.50mm; Vertical || order number: 1843729 8A 160V
phoenix_contact connector MCV_01x14_G_3.5mm
0
14
14
Connector_Phoenix_MC
PhoenixContact_MCV_1,5_14-G-3.81_1x14_P3.81mm_Vertical
Generic Phoenix Contact connector footprint for: MCV_1,5/14-G-3.81; number of pins: 14; pin pitch: 3.81mm; Vertical || order number: 1803549 8A 160V
phoenix_contact connector MCV_01x14_G_3.81mm
0
14
14
Connector_Phoenix_MC
PhoenixContact_MCV_1,5_14-GF-3.5_1x14_P3.50mm_Vertical_ThreadedFlange
Generic Phoenix Contact connector footprint for: MCV_1,5/14-GF-3.5; number of pins: 14; pin pitch: 3.50mm; Vertical; threaded flange || order number: 1843347 8A 160V
phoenix_contact connector MCV_01x14_GF_3.5mm
0
14
14
Connector_Phoenix_MC
PhoenixContact_MCV_1,5_14-GF-3.5_1x14_P3.50mm_Vertical_ThreadedFlange_MountHole
Generic Phoenix Contact connector footprint for: MCV_1,5/14-GF-3.5; number of pins: 14; pin pitch: 3.50mm; Vertical; threaded flange; footprint includes mount hole for mounting screw: ISO 1481-ST 2.2x4.5 C or ISO 7049-ST 2.2x4.5 C (http://www.fasteners.eu/standards/ISO/7049/) || order number: 1843347 8A 160V
phoenix_contact connector MCV_01x14_GF_3.5mm_MH
0
14
14
Connector_Phoenix_MC
PhoenixContact_MCV_1,5_14-GF-3.81_1x14_P3.81mm_Vertical_ThreadedFlange
Generic Phoenix Contact connector footprint for: MCV_1,5/14-GF-3.81; number of pins: 14; pin pitch: 3.81mm; Vertical; threaded flange || order number: 1830716 8A 160V
phoenix_contact connector MCV_01x14_GF_3.81mm
0
14
14
Connector_Phoenix_MC
PhoenixContact_MCV_1,5_14-GF-3.81_1x14_P3.81mm_Vertical_ThreadedFlange_MountHole
Generic Phoenix Contact connector footprint for: MCV_1,5/14-GF-3.81; number of pins: 14; pin pitch: 3.81mm; Vertical; threaded flange; footprint includes mount hole for mounting screw: ISO 1481-ST 2.2x4.5 C or ISO 7049-ST 2.2x4.5 C (http://www.fasteners.eu/standards/ISO/7049/) || order number: 1830716 8A 160V
phoenix_contact connector MCV_01x14_GF_3.81mm_MH
0
14
14
Connector_Phoenix_MC
PhoenixContact_MCV_1,5_15-G-3.5_1x15_P3.50mm_Vertical
Generic Phoenix Contact connector footprint for: MCV_1,5/15-G-3.5; number of pins: 15; pin pitch: 3.50mm; Vertical || order number: 1843732 8A 160V
phoenix_contact connector MCV_01x15_G_3.5mm
0
15
15
Connector_Phoenix_MC
PhoenixContact_MCV_1,5_15-G-3.81_1x15_P3.81mm_Vertical
Generic Phoenix Contact connector footprint for: MCV_1,5/15-G-3.81; number of pins: 15; pin pitch: 3.81mm; Vertical || order number: 1803552 8A 160V
phoenix_contact connector MCV_01x15_G_3.81mm
0
15
15
Connector_Phoenix_MC
PhoenixContact_MCV_1,5_15-GF-3.5_1x15_P3.50mm_Vertical_ThreadedFlange
Generic Phoenix Contact connector footprint for: MCV_1,5/15-GF-3.5; number of pins: 15; pin pitch: 3.50mm; Vertical; threaded flange || order number: 1843350 8A 160V
phoenix_contact connector MCV_01x15_GF_3.5mm
0
15
15
Connector_Phoenix_MC
PhoenixContact_MCV_1,5_15-GF-3.5_1x15_P3.50mm_Vertical_ThreadedFlange_MountHole
Generic Phoenix Contact connector footprint for: MCV_1,5/15-GF-3.5; number of pins: 15; pin pitch: 3.50mm; Vertical; threaded flange; footprint includes mount hole for mounting screw: ISO 1481-ST 2.2x4.5 C or ISO 7049-ST 2.2x4.5 C (http://www.fasteners.eu/standards/ISO/7049/) || order number: 1843350 8A 160V
phoenix_contact connector MCV_01x15_GF_3.5mm_MH
0
15
15
Connector_Phoenix_MC
PhoenixContact_MCV_1,5_15-GF-3.81_1x15_P3.81mm_Vertical_ThreadedFlange
Generic Phoenix Contact connector footprint for: MCV_1,5/15-GF-3.81; number of pins: 15; pin pitch: 3.81mm; Vertical; threaded flange || order number: 1830729 8A 160V
phoenix_contact connector MCV_01x15_GF_3.81mm
0
15
15
Connector_Phoenix_MC
PhoenixContact_MCV_1,5_15-GF-3.81_1x15_P3.81mm_Vertical_ThreadedFlange_MountHole
Generic Phoenix Contact connector footprint for: MCV_1,5/15-GF-3.81; number of pins: 15; pin pitch: 3.81mm; Vertical; threaded flange; footprint includes mount hole for mounting screw: ISO 1481-ST 2.2x4.5 C or ISO 7049-ST 2.2x4.5 C (http://www.fasteners.eu/standards/ISO/7049/) || order number: 1830729 8A 160V
phoenix_contact connector MCV_01x15_GF_3.81mm_MH
0
15
15
Connector_Phoenix_MC
PhoenixContact_MCV_1,5_16-G-3.5_1x16_P3.50mm_Vertical
Generic Phoenix Contact connector footprint for: MCV_1,5/16-G-3.5; number of pins: 16; pin pitch: 3.50mm; Vertical || order number: 1843745 8A 160V
phoenix_contact connector MCV_01x16_G_3.5mm
0
16
16
Connector_Phoenix_MC
PhoenixContact_MCV_1,5_16-G-3.81_1x16_P3.81mm_Vertical
Generic Phoenix Contact connector footprint for: MCV_1,5/16-G-3.81; number of pins: 16; pin pitch: 3.81mm; Vertical || order number: 1803565 8A 160V
phoenix_contact connector MCV_01x16_G_3.81mm
0
16
16
Connector_Phoenix_MC
PhoenixContact_MCV_1,5_16-GF-3.5_1x16_P3.50mm_Vertical_ThreadedFlange
Generic Phoenix Contact connector footprint for: MCV_1,5/16-GF-3.5; number of pins: 16; pin pitch: 3.50mm; Vertical; threaded flange || order number: 1843363 8A 160V
phoenix_contact connector MCV_01x16_GF_3.5mm
0
16
16
Connector_Phoenix_MC
PhoenixContact_MCV_1,5_16-GF-3.5_1x16_P3.50mm_Vertical_ThreadedFlange_MountHole
Generic Phoenix Contact connector footprint for: MCV_1,5/16-GF-3.5; number of pins: 16; pin pitch: 3.50mm; Vertical; threaded flange; footprint includes mount hole for mounting screw: ISO 1481-ST 2.2x4.5 C or ISO 7049-ST 2.2x4.5 C (http://www.fasteners.eu/standards/ISO/7049/) || order number: 1843363 8A 160V
phoenix_contact connector MCV_01x16_GF_3.5mm_MH
0
16
16
Connector_Phoenix_MC
PhoenixContact_MCV_1,5_16-GF-3.81_1x16_P3.81mm_Vertical_ThreadedFlange
Generic Phoenix Contact connector footprint for: MCV_1,5/16-GF-3.81; number of pins: 16; pin pitch: 3.81mm; Vertical; threaded flange || order number: 1830732 8A 160V
phoenix_contact connector MCV_01x16_GF_3.81mm
0
16
16
Connector_Phoenix_MC
PhoenixContact_MCV_1,5_16-GF-3.81_1x16_P3.81mm_Vertical_ThreadedFlange_MountHole
Generic Phoenix Contact connector footprint for: MCV_1,5/16-GF-3.81; number of pins: 16; pin pitch: 3.81mm; Vertical; threaded flange; footprint includes mount hole for mounting screw: ISO 1481-ST 2.2x4.5 C or ISO 7049-ST 2.2x4.5 C (http://www.fasteners.eu/standards/ISO/7049/) || order number: 1830732 8A 160V
phoenix_contact connector MCV_01x16_GF_3.81mm_MH
0
16
16
Connector_Phoenix_MC
PhoenixContact_MC_1,5_2-G-3.5_1x02_P3.50mm_Horizontal
Generic Phoenix Contact connector footprint for: MC_1,5/2-G-3.5; number of pins: 02; pin pitch: 3.50mm; Angled || order number: 1844210 8A 160V
phoenix_contact connector MC_01x02_G_3.5mm
0
2
2
Connector_Phoenix_MC
PhoenixContact_MC_1,5_2-G-3.81_1x02_P3.81mm_Horizontal
Generic Phoenix Contact connector footprint for: MC_1,5/2-G-3.81; number of pins: 02; pin pitch: 3.81mm; Angled || order number: 1803277 8A 160V
phoenix_contact connector MC_01x02_G_3.81mm
0
2
2
Connector_Phoenix_MC
PhoenixContact_MC_1,5_2-GF-3.5_1x02_P3.50mm_Horizontal_ThreadedFlange
Generic Phoenix Contact connector footprint for: MC_1,5/2-GF-3.5; number of pins: 02; pin pitch: 3.50mm; Angled; threaded flange || order number: 1843790 8A 160V
phoenix_contact connector MC_01x02_GF_3.5mm
0
2
2
Connector_Phoenix_MC
PhoenixContact_MC_1,5_2-GF-3.5_1x02_P3.50mm_Horizontal_ThreadedFlange_MountHole
Generic Phoenix Contact connector footprint for: MC_1,5/2-GF-3.5; number of pins: 02; pin pitch: 3.50mm; Angled; threaded flange; footprint includes mount hole for mounting screw: ISO 1481-ST 2.2x4.5 C or ISO 7049-ST 2.2x4.5 C (http://www.fasteners.eu/standards/ISO/7049/) || order number: 1843790 8A 160V
phoenix_contact connector MC_01x02_GF_3.5mm_MH
0
2
2
Connector_Phoenix_MC
PhoenixContact_MC_1,5_2-GF-3.81_1x02_P3.81mm_Horizontal_ThreadedFlange
Generic Phoenix Contact connector footprint for: MC_1,5/2-GF-3.81; number of pins: 02; pin pitch: 3.81mm; Angled; threaded flange || order number: 1827868 8A 160V
phoenix_contact connector MC_01x02_GF_3.81mm
0
2
2
Connector_Phoenix_MC
PhoenixContact_MC_1,5_2-GF-3.81_1x02_P3.81mm_Horizontal_ThreadedFlange_MountHole
Generic Phoenix Contact connector footprint for: MC_1,5/2-GF-3.81; number of pins: 02; pin pitch: 3.81mm; Angled; threaded flange; footprint includes mount hole for mounting screw: ISO 1481-ST 2.2x4.5 C or ISO 7049-ST 2.2x4.5 C (http://www.fasteners.eu/standards/ISO/7049/) || order number: 1827868 8A 160V
phoenix_contact connector MC_01x02_GF_3.81mm_MH
0
2
2
Connector_Phoenix_MC
PhoenixContact_MC_1,5_3-G-3.5_1x03_P3.50mm_Horizontal
Generic Phoenix Contact connector footprint for: MC_1,5/3-G-3.5; number of pins: 03; pin pitch: 3.50mm; Angled || order number: 1844223 8A 160V
phoenix_contact connector MC_01x03_G_3.5mm
0
3
3
Connector_Phoenix_MC
PhoenixContact_MC_1,5_3-G-3.81_1x03_P3.81mm_Horizontal
Generic Phoenix Contact connector footprint for: MC_1,5/3-G-3.81; number of pins: 03; pin pitch: 3.81mm; Angled || order number: 1803280 8A 160V
phoenix_contact connector MC_01x03_G_3.81mm
0
3
3
Connector_Phoenix_MC
PhoenixContact_MC_1,5_3-GF-3.5_1x03_P3.50mm_Horizontal_ThreadedFlange
Generic Phoenix Contact connector footprint for: MC_1,5/3-GF-3.5; number of pins: 03; pin pitch: 3.50mm; Angled; threaded flange || order number: 1843800 8A 160V
phoenix_contact connector MC_01x03_GF_3.5mm
0
3
3
Connector_Phoenix_MC
PhoenixContact_MC_1,5_3-GF-3.5_1x03_P3.50mm_Horizontal_ThreadedFlange_MountHole
Generic Phoenix Contact connector footprint for: MC_1,5/3-GF-3.5; number of pins: 03; pin pitch: 3.50mm; Angled; threaded flange; footprint includes mount hole for mounting screw: ISO 1481-ST 2.2x4.5 C or ISO 7049-ST 2.2x4.5 C (http://www.fasteners.eu/standards/ISO/7049/) || order number: 1843800 8A 160V
phoenix_contact connector MC_01x03_GF_3.5mm_MH
0
3
3
Connector_Phoenix_MC
PhoenixContact_MC_1,5_3-GF-3.81_1x03_P3.81mm_Horizontal_ThreadedFlange
Generic Phoenix Contact connector footprint for: MC_1,5/3-GF-3.81; number of pins: 03; pin pitch: 3.81mm; Angled; threaded flange || order number: 1827871 8A 160V
phoenix_contact connector MC_01x03_GF_3.81mm
0
3
3
Connector_Phoenix_MC
PhoenixContact_MC_1,5_3-GF-3.81_1x03_P3.81mm_Horizontal_ThreadedFlange_MountHole
Generic Phoenix Contact connector footprint for: MC_1,5/3-GF-3.81; number of pins: 03; pin pitch: 3.81mm; Angled; threaded flange; footprint includes mount hole for mounting screw: ISO 1481-ST 2.2x4.5 C or ISO 7049-ST 2.2x4.5 C (http://www.fasteners.eu/standards/ISO/7049/) || order number: 1827871 8A 160V
phoenix_contact connector MC_01x03_GF_3.81mm_MH
0
3
3
Connector_Phoenix_MC
PhoenixContact_MC_1,5_4-G-3.5_1x04_P3.50mm_Horizontal
Generic Phoenix Contact connector footprint for: MC_1,5/4-G-3.5; number of pins: 04; pin pitch: 3.50mm; Angled || order number: 1844236 8A 160V
phoenix_contact connector MC_01x04_G_3.5mm
0
4
4
Connector_Phoenix_MC
PhoenixContact_MC_1,5_4-G-3.81_1x04_P3.81mm_Horizontal
Generic Phoenix Contact connector footprint for: MC_1,5/4-G-3.81; number of pins: 04; pin pitch: 3.81mm; Angled || order number: 1803293 8A 160V
phoenix_contact connector MC_01x04_G_3.81mm
0
4
4
Connector_Phoenix_MC
PhoenixContact_MC_1,5_4-GF-3.5_1x04_P3.50mm_Horizontal_ThreadedFlange
Generic Phoenix Contact connector footprint for: MC_1,5/4-GF-3.5; number of pins: 04; pin pitch: 3.50mm; Angled; threaded flange || order number: 1843813 8A 160V
phoenix_contact connector MC_01x04_GF_3.5mm
0
4
4
Connector_Phoenix_MC
PhoenixContact_MC_1,5_4-GF-3.5_1x04_P3.50mm_Horizontal_ThreadedFlange_MountHole
Generic Phoenix Contact connector footprint for: MC_1,5/4-GF-3.5; number of pins: 04; pin pitch: 3.50mm; Angled; threaded flange; footprint includes mount hole for mounting screw: ISO 1481-ST 2.2x4.5 C or ISO 7049-ST 2.2x4.5 C (http://www.fasteners.eu/standards/ISO/7049/) || order number: 1843813 8A 160V
phoenix_contact connector MC_01x04_GF_3.5mm_MH
0
4
4
Connector_Phoenix_MC
PhoenixContact_MC_1,5_4-GF-3.81_1x04_P3.81mm_Horizontal_ThreadedFlange
Generic Phoenix Contact connector footprint for: MC_1,5/4-GF-3.81; number of pins: 04; pin pitch: 3.81mm; Angled; threaded flange || order number: 1827884 8A 160V
phoenix_contact connector MC_01x04_GF_3.81mm
0
4
4
Connector_Phoenix_MC
PhoenixContact_MC_1,5_4-GF-3.81_1x04_P3.81mm_Horizontal_ThreadedFlange_MountHole
Generic Phoenix Contact connector footprint for: MC_1,5/4-GF-3.81; number of pins: 04; pin pitch: 3.81mm; Angled; threaded flange; footprint includes mount hole for mounting screw: ISO 1481-ST 2.2x4.5 C or ISO 7049-ST 2.2x4.5 C (http://www.fasteners.eu/standards/ISO/7049/) || order number: 1827884 8A 160V
phoenix_contact connector MC_01x04_GF_3.81mm_MH
0
4
4
Connector_Phoenix_MC
PhoenixContact_MC_1,5_5-G-3.5_1x05_P3.50mm_Horizontal
Generic Phoenix Contact connector footprint for: MC_1,5/5-G-3.5; number of pins: 05; pin pitch: 3.50mm; Angled || order number: 1844249 8A 160V
phoenix_contact connector MC_01x05_G_3.5mm
0
5
5
Connector_Phoenix_MC
PhoenixContact_MC_1,5_5-G-3.81_1x05_P3.81mm_Horizontal
Generic Phoenix Contact connector footprint for: MC_1,5/5-G-3.81; number of pins: 05; pin pitch: 3.81mm; Angled || order number: 1803303 8A 160V
phoenix_contact connector MC_01x05_G_3.81mm
0
5
5
Connector_Phoenix_MC
PhoenixContact_MC_1,5_5-GF-3.5_1x05_P3.50mm_Horizontal_ThreadedFlange
Generic Phoenix Contact connector footprint for: MC_1,5/5-GF-3.5; number of pins: 05; pin pitch: 3.50mm; Angled; threaded flange || order number: 1843826 8A 160V
phoenix_contact connector MC_01x05_GF_3.5mm
0
5
5
Connector_Phoenix_MC
PhoenixContact_MC_1,5_5-GF-3.5_1x05_P3.50mm_Horizontal_ThreadedFlange_MountHole
Generic Phoenix Contact connector footprint for: MC_1,5/5-GF-3.5; number of pins: 05; pin pitch: 3.50mm; Angled; threaded flange; footprint includes mount hole for mounting screw: ISO 1481-ST 2.2x4.5 C or ISO 7049-ST 2.2x4.5 C (http://www.fasteners.eu/standards/ISO/7049/) || order number: 1843826 8A 160V
phoenix_contact connector MC_01x05_GF_3.5mm_MH
0
5
5
Connector_Phoenix_MC
PhoenixContact_MC_1,5_5-GF-3.81_1x05_P3.81mm_Horizontal_ThreadedFlange
Generic Phoenix Contact connector footprint for: MC_1,5/5-GF-3.81; number of pins: 05; pin pitch: 3.81mm; Angled; threaded flange || order number: 1827897 8A 160V
phoenix_contact connector MC_01x05_GF_3.81mm
0
5
5
Connector_Phoenix_MC
PhoenixContact_MC_1,5_5-GF-3.81_1x05_P3.81mm_Horizontal_ThreadedFlange_MountHole
Generic Phoenix Contact connector footprint for: MC_1,5/5-GF-3.81; number of pins: 05; pin pitch: 3.81mm; Angled; threaded flange; footprint includes mount hole for mounting screw: ISO 1481-ST 2.2x4.5 C or ISO 7049-ST 2.2x4.5 C (http://www.fasteners.eu/standards/ISO/7049/) || order number: 1827897 8A 160V
phoenix_contact connector MC_01x05_GF_3.81mm_MH
0
5
5
Connector_Phoenix_MC
PhoenixContact_MC_1,5_6-G-3.5_1x06_P3.50mm_Horizontal
Generic Phoenix Contact connector footprint for: MC_1,5/6-G-3.5; number of pins: 06; pin pitch: 3.50mm; Angled || order number: 1844252 8A 160V
phoenix_contact connector MC_01x06_G_3.5mm
0
6
6
Connector_Phoenix_MC
PhoenixContact_MC_1,5_6-G-3.81_1x06_P3.81mm_Horizontal
Generic Phoenix Contact connector footprint for: MC_1,5/6-G-3.81; number of pins: 06; pin pitch: 3.81mm; Angled || order number: 1803316 8A 160V
phoenix_contact connector MC_01x06_G_3.81mm
0
6
6
Connector_Phoenix_MC
PhoenixContact_MC_1,5_6-GF-3.5_1x06_P3.50mm_Horizontal_ThreadedFlange
Generic Phoenix Contact connector footprint for: MC_1,5/6-GF-3.5; number of pins: 06; pin pitch: 3.50mm; Angled; threaded flange || order number: 1843839 8A 160V
phoenix_contact connector MC_01x06_GF_3.5mm
0
6
6
Connector_Phoenix_MC
PhoenixContact_MC_1,5_6-GF-3.5_1x06_P3.50mm_Horizontal_ThreadedFlange_MountHole
Generic Phoenix Contact connector footprint for: MC_1,5/6-GF-3.5; number of pins: 06; pin pitch: 3.50mm; Angled; threaded flange; footprint includes mount hole for mounting screw: ISO 1481-ST 2.2x4.5 C or ISO 7049-ST 2.2x4.5 C (http://www.fasteners.eu/standards/ISO/7049/) || order number: 1843839 8A 160V
phoenix_contact connector MC_01x06_GF_3.5mm_MH
0
6
6
Connector_Phoenix_MC
PhoenixContact_MC_1,5_6-GF-3.81_1x06_P3.81mm_Horizontal_ThreadedFlange
Generic Phoenix Contact connector footprint for: MC_1,5/6-GF-3.81; number of pins: 06; pin pitch: 3.81mm; Angled; threaded flange || order number: 1827907 8A 160V
phoenix_contact connector MC_01x06_GF_3.81mm
0
6
6
Connector_Phoenix_MC
PhoenixContact_MC_1,5_6-GF-3.81_1x06_P3.81mm_Horizontal_ThreadedFlange_MountHole
Generic Phoenix Contact connector footprint for: MC_1,5/6-GF-3.81; number of pins: 06; pin pitch: 3.81mm; Angled; threaded flange; footprint includes mount hole for mounting screw: ISO 1481-ST 2.2x4.5 C or ISO 7049-ST 2.2x4.5 C (http://www.fasteners.eu/standards/ISO/7049/) || order number: 1827907 8A 160V
phoenix_contact connector MC_01x06_GF_3.81mm_MH
0
6
6
Connector_Phoenix_MC
PhoenixContact_MC_1,5_7-G-3.5_1x07_P3.50mm_Horizontal
Generic Phoenix Contact connector footprint for: MC_1,5/7-G-3.5; number of pins: 07; pin pitch: 3.50mm; Angled || order number: 1844265 8A 160V
phoenix_contact connector MC_01x07_G_3.5mm
0
7
7
Connector_Phoenix_MC
PhoenixContact_MC_1,5_7-G-3.81_1x07_P3.81mm_Horizontal
Generic Phoenix Contact connector footprint for: MC_1,5/7-G-3.81; number of pins: 07; pin pitch: 3.81mm; Angled || order number: 1803329 8A 160V
phoenix_contact connector MC_01x07_G_3.81mm
0
7
7
Connector_Phoenix_MC
PhoenixContact_MC_1,5_7-GF-3.5_1x07_P3.50mm_Horizontal_ThreadedFlange
Generic Phoenix Contact connector footprint for: MC_1,5/7-GF-3.5; number of pins: 07; pin pitch: 3.50mm; Angled; threaded flange || order number: 1843842 8A 160V
phoenix_contact connector MC_01x07_GF_3.5mm
0
7
7
Connector_Phoenix_MC
PhoenixContact_MC_1,5_7-GF-3.5_1x07_P3.50mm_Horizontal_ThreadedFlange_MountHole
Generic Phoenix Contact connector footprint for: MC_1,5/7-GF-3.5; number of pins: 07; pin pitch: 3.50mm; Angled; threaded flange; footprint includes mount hole for mounting screw: ISO 1481-ST 2.2x4.5 C or ISO 7049-ST 2.2x4.5 C (http://www.fasteners.eu/standards/ISO/7049/) || order number: 1843842 8A 160V
phoenix_contact connector MC_01x07_GF_3.5mm_MH
0
7
7
Connector_Phoenix_MC
PhoenixContact_MC_1,5_7-GF-3.81_1x07_P3.81mm_Horizontal_ThreadedFlange
Generic Phoenix Contact connector footprint for: MC_1,5/7-GF-3.81; number of pins: 07; pin pitch: 3.81mm; Angled; threaded flange || order number: 1827910 8A 160V
phoenix_contact connector MC_01x07_GF_3.81mm
0
7
7
Connector_Phoenix_MC
PhoenixContact_MC_1,5_7-GF-3.81_1x07_P3.81mm_Horizontal_ThreadedFlange_MountHole
Generic Phoenix Contact connector footprint for: MC_1,5/7-GF-3.81; number of pins: 07; pin pitch: 3.81mm; Angled; threaded flange; footprint includes mount hole for mounting screw: ISO 1481-ST 2.2x4.5 C or ISO 7049-ST 2.2x4.5 C (http://www.fasteners.eu/standards/ISO/7049/) || order number: 1827910 8A 160V
phoenix_contact connector MC_01x07_GF_3.81mm_MH
0
7
7
Connector_Phoenix_MC
PhoenixContact_MC_1,5_8-G-3.5_1x08_P3.50mm_Horizontal
Generic Phoenix Contact connector footprint for: MC_1,5/8-G-3.5; number of pins: 08; pin pitch: 3.50mm; Angled || order number: 1844278 8A 160V
phoenix_contact connector MC_01x08_G_3.5mm
0
8
8
Connector_Phoenix_MC
PhoenixContact_MC_1,5_8-G-3.81_1x08_P3.81mm_Horizontal
Generic Phoenix Contact connector footprint for: MC_1,5/8-G-3.81; number of pins: 08; pin pitch: 3.81mm; Angled || order number: 1803332 8A 160V
phoenix_contact connector MC_01x08_G_3.81mm
0
8
8
Connector_Phoenix_MC
PhoenixContact_MC_1,5_8-GF-3.5_1x08_P3.50mm_Horizontal_ThreadedFlange
Generic Phoenix Contact connector footprint for: MC_1,5/8-GF-3.5; number of pins: 08; pin pitch: 3.50mm; Angled; threaded flange || order number: 1843855 8A 160V
phoenix_contact connector MC_01x08_GF_3.5mm
0
8
8
Connector_Phoenix_MC
PhoenixContact_MC_1,5_8-GF-3.5_1x08_P3.50mm_Horizontal_ThreadedFlange_MountHole
Generic Phoenix Contact connector footprint for: MC_1,5/8-GF-3.5; number of pins: 08; pin pitch: 3.50mm; Angled; threaded flange; footprint includes mount hole for mounting screw: ISO 1481-ST 2.2x4.5 C or ISO 7049-ST 2.2x4.5 C (http://www.fasteners.eu/standards/ISO/7049/) || order number: 1843855 8A 160V
phoenix_contact connector MC_01x08_GF_3.5mm_MH
0
8
8
Connector_Phoenix_MC
PhoenixContact_MC_1,5_8-GF-3.81_1x08_P3.81mm_Horizontal_ThreadedFlange
Generic Phoenix Contact connector footprint for: MC_1,5/8-GF-3.81; number of pins: 08; pin pitch: 3.81mm; Angled; threaded flange || order number: 1827923 8A 160V
phoenix_contact connector MC_01x08_GF_3.81mm
0
8
8
Connector_Phoenix_MC
PhoenixContact_MC_1,5_8-GF-3.81_1x08_P3.81mm_Horizontal_ThreadedFlange_MountHole
Generic Phoenix Contact connector footprint for: MC_1,5/8-GF-3.81; number of pins: 08; pin pitch: 3.81mm; Angled; threaded flange; footprint includes mount hole for mounting screw: ISO 1481-ST 2.2x4.5 C or ISO 7049-ST 2.2x4.5 C (http://www.fasteners.eu/standards/ISO/7049/) || order number: 1827923 8A 160V
phoenix_contact connector MC_01x08_GF_3.81mm_MH
0
8
8
Connector_Phoenix_MC
PhoenixContact_MC_1,5_9-G-3.5_1x09_P3.50mm_Horizontal
Generic Phoenix Contact connector footprint for: MC_1,5/9-G-3.5; number of pins: 09; pin pitch: 3.50mm; Angled || order number: 1844281 8A 160V
phoenix_contact connector MC_01x09_G_3.5mm
0
9
9
Connector_Phoenix_MC
PhoenixContact_MC_1,5_9-G-3.81_1x09_P3.81mm_Horizontal
Generic Phoenix Contact connector footprint for: MC_1,5/9-G-3.81; number of pins: 09; pin pitch: 3.81mm; Angled || order number: 1803345 8A 160V
phoenix_contact connector MC_01x09_G_3.81mm
0
9
9
Connector_Phoenix_MC
PhoenixContact_MC_1,5_9-GF-3.5_1x09_P3.50mm_Horizontal_ThreadedFlange
Generic Phoenix Contact connector footprint for: MC_1,5/9-GF-3.5; number of pins: 09; pin pitch: 3.50mm; Angled; threaded flange || order number: 1843868 8A 160V
phoenix_contact connector MC_01x09_GF_3.5mm
0
9
9
Connector_Phoenix_MC
PhoenixContact_MC_1,5_9-GF-3.5_1x09_P3.50mm_Horizontal_ThreadedFlange_MountHole
Generic Phoenix Contact connector footprint for: MC_1,5/9-GF-3.5; number of pins: 09; pin pitch: 3.50mm; Angled; threaded flange; footprint includes mount hole for mounting screw: ISO 1481-ST 2.2x4.5 C or ISO 7049-ST 2.2x4.5 C (http://www.fasteners.eu/standards/ISO/7049/) || order number: 1843868 8A 160V
phoenix_contact connector MC_01x09_GF_3.5mm_MH
0
9
9
Connector_Phoenix_MC
PhoenixContact_MC_1,5_9-GF-3.81_1x09_P3.81mm_Horizontal_ThreadedFlange
Generic Phoenix Contact connector footprint for: MC_1,5/9-GF-3.81; number of pins: 09; pin pitch: 3.81mm; Angled; threaded flange || order number: 1827936 8A 160V
phoenix_contact connector MC_01x09_GF_3.81mm
0
9
9
Connector_Phoenix_MC
PhoenixContact_MC_1,5_9-GF-3.81_1x09_P3.81mm_Horizontal_ThreadedFlange_MountHole
Generic Phoenix Contact connector footprint for: MC_1,5/9-GF-3.81; number of pins: 09; pin pitch: 3.81mm; Angled; threaded flange; footprint includes mount hole for mounting screw: ISO 1481-ST 2.2x4.5 C or ISO 7049-ST 2.2x4.5 C (http://www.fasteners.eu/standards/ISO/7049/) || order number: 1827936 8A 160V
phoenix_contact connector MC_01x09_GF_3.81mm_MH
0
9
9
Connector_Phoenix_MC
PhoenixContact_MC_1,5_10-G-3.5_1x10_P3.50mm_Horizontal
Generic Phoenix Contact connector footprint for: MC_1,5/10-G-3.5; number of pins: 10; pin pitch: 3.50mm; Angled || order number: 1844294 8A 160V
phoenix_contact connector MC_01x10_G_3.5mm
0
10
10
Connector_Phoenix_MC
PhoenixContact_MC_1,5_10-G-3.81_1x10_P3.81mm_Horizontal
Generic Phoenix Contact connector footprint for: MC_1,5/10-G-3.81; number of pins: 10; pin pitch: 3.81mm; Angled || order number: 1803358 8A 160V
phoenix_contact connector MC_01x10_G_3.81mm
0
10
10
Connector_Phoenix_MC
PhoenixContact_MC_1,5_10-GF-3.5_1x10_P3.50mm_Horizontal_ThreadedFlange
Generic Phoenix Contact connector footprint for: MC_1,5/10-GF-3.5; number of pins: 10; pin pitch: 3.50mm; Angled; threaded flange || order number: 1843871 8A 160V
phoenix_contact connector MC_01x10_GF_3.5mm
0
10
10
Connector_Phoenix_MC
PhoenixContact_MC_1,5_10-GF-3.5_1x10_P3.50mm_Horizontal_ThreadedFlange_MountHole
Generic Phoenix Contact connector footprint for: MC_1,5/10-GF-3.5; number of pins: 10; pin pitch: 3.50mm; Angled; threaded flange; footprint includes mount hole for mounting screw: ISO 1481-ST 2.2x4.5 C or ISO 7049-ST 2.2x4.5 C (http://www.fasteners.eu/standards/ISO/7049/) || order number: 1843871 8A 160V
phoenix_contact connector MC_01x10_GF_3.5mm_MH
0
10
10
Connector_Phoenix_MC
PhoenixContact_MC_1,5_10-GF-3.81_1x10_P3.81mm_Horizontal_ThreadedFlange
Generic Phoenix Contact connector footprint for: MC_1,5/10-GF-3.81; number of pins: 10; pin pitch: 3.81mm; Angled; threaded flange || order number: 1827949 8A 160V
phoenix_contact connector MC_01x10_GF_3.81mm
0
10
10
Connector_Phoenix_MC
PhoenixContact_MC_1,5_10-GF-3.81_1x10_P3.81mm_Horizontal_ThreadedFlange_MountHole
Generic Phoenix Contact connector footprint for: MC_1,5/10-GF-3.81; number of pins: 10; pin pitch: 3.81mm; Angled; threaded flange; footprint includes mount hole for mounting screw: ISO 1481-ST 2.2x4.5 C or ISO 7049-ST 2.2x4.5 C (http://www.fasteners.eu/standards/ISO/7049/) || order number: 1827949 8A 160V
phoenix_contact connector MC_01x10_GF_3.81mm_MH
0
10
10
Connector_Phoenix_MC
PhoenixContact_MC_1,5_11-G-3.5_1x11_P3.50mm_Horizontal
Generic Phoenix Contact connector footprint for: MC_1,5/11-G-3.5; number of pins: 11; pin pitch: 3.50mm; Angled || order number: 1844304 8A 160V
phoenix_contact connector MC_01x11_G_3.5mm
0
11
11
Connector_Phoenix_MC
PhoenixContact_MC_1,5_11-G-3.81_1x11_P3.81mm_Horizontal
Generic Phoenix Contact connector footprint for: MC_1,5/11-G-3.81; number of pins: 11; pin pitch: 3.81mm; Angled || order number: 1803361 8A 160V
phoenix_contact connector MC_01x11_G_3.81mm
0
11
11
Connector_Phoenix_MC
PhoenixContact_MC_1,5_11-GF-3.5_1x11_P3.50mm_Horizontal_ThreadedFlange
Generic Phoenix Contact connector footprint for: MC_1,5/11-GF-3.5; number of pins: 11; pin pitch: 3.50mm; Angled; threaded flange || order number: 1843884 8A 160V
phoenix_contact connector MC_01x11_GF_3.5mm
0
11
11
Connector_Phoenix_MC
PhoenixContact_MC_1,5_11-GF-3.5_1x11_P3.50mm_Horizontal_ThreadedFlange_MountHole
Generic Phoenix Contact connector footprint for: MC_1,5/11-GF-3.5; number of pins: 11; pin pitch: 3.50mm; Angled; threaded flange; footprint includes mount hole for mounting screw: ISO 1481-ST 2.2x4.5 C or ISO 7049-ST 2.2x4.5 C (http://www.fasteners.eu/standards/ISO/7049/) || order number: 1843884 8A 160V
phoenix_contact connector MC_01x11_GF_3.5mm_MH
0
11
11
Connector_Phoenix_MC
PhoenixContact_MC_1,5_11-GF-3.81_1x11_P3.81mm_Horizontal_ThreadedFlange
Generic Phoenix Contact connector footprint for: MC_1,5/11-GF-3.81; number of pins: 11; pin pitch: 3.81mm; Angled; threaded flange || order number: 1827952 8A 160V
phoenix_contact connector MC_01x11_GF_3.81mm
0
11
11
Connector_Phoenix_MC
PhoenixContact_MC_1,5_11-GF-3.81_1x11_P3.81mm_Horizontal_ThreadedFlange_MountHole
Generic Phoenix Contact connector footprint for: MC_1,5/11-GF-3.81; number of pins: 11; pin pitch: 3.81mm; Angled; threaded flange; footprint includes mount hole for mounting screw: ISO 1481-ST 2.2x4.5 C or ISO 7049-ST 2.2x4.5 C (http://www.fasteners.eu/standards/ISO/7049/) || order number: 1827952 8A 160V
phoenix_contact connector MC_01x11_GF_3.81mm_MH
0
11
11
Connector_Phoenix_MC
PhoenixContact_MC_1,5_12-G-3.5_1x12_P3.50mm_Horizontal
Generic Phoenix Contact connector footprint for: MC_1,5/12-G-3.5; number of pins: 12; pin pitch: 3.50mm; Angled || order number: 1844317 8A 160V
phoenix_contact connector MC_01x12_G_3.5mm
0
12
12
Connector_Phoenix_MC
PhoenixContact_MC_1,5_12-G-3.81_1x12_P3.81mm_Horizontal
Generic Phoenix Contact connector footprint for: MC_1,5/12-G-3.81; number of pins: 12; pin pitch: 3.81mm; Angled || order number: 1803374 8A 160V
phoenix_contact connector MC_01x12_G_3.81mm
0
12
12
Connector_Phoenix_MC
PhoenixContact_MC_1,5_12-GF-3.5_1x12_P3.50mm_Horizontal_ThreadedFlange
Generic Phoenix Contact connector footprint for: MC_1,5/12-GF-3.5; number of pins: 12; pin pitch: 3.50mm; Angled; threaded flange || order number: 1843897 8A 160V
phoenix_contact connector MC_01x12_GF_3.5mm
0
12
12
Connector_Phoenix_MC
PhoenixContact_MC_1,5_12-GF-3.5_1x12_P3.50mm_Horizontal_ThreadedFlange_MountHole
Generic Phoenix Contact connector footprint for: MC_1,5/12-GF-3.5; number of pins: 12; pin pitch: 3.50mm; Angled; threaded flange; footprint includes mount hole for mounting screw: ISO 1481-ST 2.2x4.5 C or ISO 7049-ST 2.2x4.5 C (http://www.fasteners.eu/standards/ISO/7049/) || order number: 1843897 8A 160V
phoenix_contact connector MC_01x12_GF_3.5mm_MH
0
12
12
Connector_Phoenix_MC
PhoenixContact_MC_1,5_12-GF-3.81_1x12_P3.81mm_Horizontal_ThreadedFlange
Generic Phoenix Contact connector footprint for: MC_1,5/12-GF-3.81; number of pins: 12; pin pitch: 3.81mm; Angled; threaded flange || order number: 1827965 8A 160V
phoenix_contact connector MC_01x12_GF_3.81mm
0
12
12
Connector_Phoenix_MC
PhoenixContact_MC_1,5_12-GF-3.81_1x12_P3.81mm_Horizontal_ThreadedFlange_MountHole
Generic Phoenix Contact connector footprint for: MC_1,5/12-GF-3.81; number of pins: 12; pin pitch: 3.81mm; Angled; threaded flange; footprint includes mount hole for mounting screw: ISO 1481-ST 2.2x4.5 C or ISO 7049-ST 2.2x4.5 C (http://www.fasteners.eu/standards/ISO/7049/) || order number: 1827965 8A 160V
phoenix_contact connector MC_01x12_GF_3.81mm_MH
0
12
12
Connector_Phoenix_MC
PhoenixContact_MC_1,5_13-G-3.5_1x13_P3.50mm_Horizontal
Generic Phoenix Contact connector footprint for: MC_1,5/13-G-3.5; number of pins: 13; pin pitch: 3.50mm; Angled || order number: 1844320 8A 160V
phoenix_contact connector MC_01x13_G_3.5mm
0
13
13
Connector_Phoenix_MC
PhoenixContact_MC_1,5_13-G-3.81_1x13_P3.81mm_Horizontal
Generic Phoenix Contact connector footprint for: MC_1,5/13-G-3.81; number of pins: 13; pin pitch: 3.81mm; Angled || order number: 1803387 8A 160V
phoenix_contact connector MC_01x13_G_3.81mm
0
13
13
Connector_Phoenix_MC
PhoenixContact_MC_1,5_13-GF-3.5_1x13_P3.50mm_Horizontal_ThreadedFlange
Generic Phoenix Contact connector footprint for: MC_1,5/13-GF-3.5; number of pins: 13; pin pitch: 3.50mm; Angled; threaded flange || order number: 1843907 8A 160V
phoenix_contact connector MC_01x13_GF_3.5mm
0
13
13
Connector_Phoenix_MC
PhoenixContact_MC_1,5_13-GF-3.5_1x13_P3.50mm_Horizontal_ThreadedFlange_MountHole
Generic Phoenix Contact connector footprint for: MC_1,5/13-GF-3.5; number of pins: 13; pin pitch: 3.50mm; Angled; threaded flange; footprint includes mount hole for mounting screw: ISO 1481-ST 2.2x4.5 C or ISO 7049-ST 2.2x4.5 C (http://www.fasteners.eu/standards/ISO/7049/) || order number: 1843907 8A 160V
phoenix_contact connector MC_01x13_GF_3.5mm_MH
0
13
13
Connector_Phoenix_MC
PhoenixContact_MC_1,5_13-GF-3.81_1x13_P3.81mm_Horizontal_ThreadedFlange
Generic Phoenix Contact connector footprint for: MC_1,5/13-GF-3.81; number of pins: 13; pin pitch: 3.81mm; Angled; threaded flange || order number: 1827978 8A 160V
phoenix_contact connector MC_01x13_GF_3.81mm
0
13
13
Connector_Phoenix_MC
PhoenixContact_MC_1,5_13-GF-3.81_1x13_P3.81mm_Horizontal_ThreadedFlange_MountHole
Generic Phoenix Contact connector footprint for: MC_1,5/13-GF-3.81; number of pins: 13; pin pitch: 3.81mm; Angled; threaded flange; footprint includes mount hole for mounting screw: ISO 1481-ST 2.2x4.5 C or ISO 7049-ST 2.2x4.5 C (http://www.fasteners.eu/standards/ISO/7049/) || order number: 1827978 8A 160V
phoenix_contact connector MC_01x13_GF_3.81mm_MH
0
13
13
Connector_Phoenix_MC
PhoenixContact_MC_1,5_14-G-3.5_1x14_P3.50mm_Horizontal
Generic Phoenix Contact connector footprint for: MC_1,5/14-G-3.5; number of pins: 14; pin pitch: 3.50mm; Angled || order number: 1844333 8A 160V
phoenix_contact connector MC_01x14_G_3.5mm
0
14
14
Connector_Phoenix_MC
PhoenixContact_MC_1,5_14-G-3.81_1x14_P3.81mm_Horizontal
Generic Phoenix Contact connector footprint for: MC_1,5/14-G-3.81; number of pins: 14; pin pitch: 3.81mm; Angled || order number: 1803390 8A 160V
phoenix_contact connector MC_01x14_G_3.81mm
0
14
14
Connector_Phoenix_MC
PhoenixContact_MC_1,5_14-GF-3.5_1x14_P3.50mm_Horizontal_ThreadedFlange
Generic Phoenix Contact connector footprint for: MC_1,5/14-GF-3.5; number of pins: 14; pin pitch: 3.50mm; Angled; threaded flange || order number: 1843910 8A 160V
phoenix_contact connector MC_01x14_GF_3.5mm
0
14
14
Connector_Phoenix_MC
PhoenixContact_MC_1,5_14-GF-3.5_1x14_P3.50mm_Horizontal_ThreadedFlange_MountHole
Generic Phoenix Contact connector footprint for: MC_1,5/14-GF-3.5; number of pins: 14; pin pitch: 3.50mm; Angled; threaded flange; footprint includes mount hole for mounting screw: ISO 1481-ST 2.2x4.5 C or ISO 7049-ST 2.2x4.5 C (http://www.fasteners.eu/standards/ISO/7049/) || order number: 1843910 8A 160V
phoenix_contact connector MC_01x14_GF_3.5mm_MH
0
14
14
Connector_Phoenix_MC
PhoenixContact_MC_1,5_14-GF-3.81_1x14_P3.81mm_Horizontal_ThreadedFlange
Generic Phoenix Contact connector footprint for: MC_1,5/14-GF-3.81; number of pins: 14; pin pitch: 3.81mm; Angled; threaded flange || order number: 1827981 8A 160V
phoenix_contact connector MC_01x14_GF_3.81mm
0
14
14
Connector_Phoenix_MC
PhoenixContact_MC_1,5_14-GF-3.81_1x14_P3.81mm_Horizontal_ThreadedFlange_MountHole
Generic Phoenix Contact connector footprint for: MC_1,5/14-GF-3.81; number of pins: 14; pin pitch: 3.81mm; Angled; threaded flange; footprint includes mount hole for mounting screw: ISO 1481-ST 2.2x4.5 C or ISO 7049-ST 2.2x4.5 C (http://www.fasteners.eu/standards/ISO/7049/) || order number: 1827981 8A 160V
phoenix_contact connector MC_01x14_GF_3.81mm_MH
0
14
14
Connector_Phoenix_MC
PhoenixContact_MC_1,5_15-G-3.5_1x15_P3.50mm_Horizontal
Generic Phoenix Contact connector footprint for: MC_1,5/15-G-3.5; number of pins: 15; pin pitch: 3.50mm; Angled || order number: 1844346 8A 160V
phoenix_contact connector MC_01x15_G_3.5mm
0
15
15
Connector_Phoenix_MC
PhoenixContact_MC_1,5_15-G-3.81_1x15_P3.81mm_Horizontal
Generic Phoenix Contact connector footprint for: MC_1,5/15-G-3.81; number of pins: 15; pin pitch: 3.81mm; Angled || order number: 1803400 8A 160V
phoenix_contact connector MC_01x15_G_3.81mm
0
15
15
Connector_Phoenix_MC
PhoenixContact_MC_1,5_15-GF-3.5_1x15_P3.50mm_Horizontal_ThreadedFlange
Generic Phoenix Contact connector footprint for: MC_1,5/15-GF-3.5; number of pins: 15; pin pitch: 3.50mm; Angled; threaded flange || order number: 1843923 8A 160V
phoenix_contact connector MC_01x15_GF_3.5mm
0
15
15
Connector_Phoenix_MC
PhoenixContact_MC_1,5_15-GF-3.5_1x15_P3.50mm_Horizontal_ThreadedFlange_MountHole
Generic Phoenix Contact connector footprint for: MC_1,5/15-GF-3.5; number of pins: 15; pin pitch: 3.50mm; Angled; threaded flange; footprint includes mount hole for mounting screw: ISO 1481-ST 2.2x4.5 C or ISO 7049-ST 2.2x4.5 C (http://www.fasteners.eu/standards/ISO/7049/) || order number: 1843923 8A 160V
phoenix_contact connector MC_01x15_GF_3.5mm_MH
0
15
15
Connector_Phoenix_MC
PhoenixContact_MC_1,5_15-GF-3.81_1x15_P3.81mm_Horizontal_ThreadedFlange
Generic Phoenix Contact connector footprint for: MC_1,5/15-GF-3.81; number of pins: 15; pin pitch: 3.81mm; Angled; threaded flange || order number: 1827994 8A 160V
phoenix_contact connector MC_01x15_GF_3.81mm
0
15
15
Connector_Phoenix_MC
PhoenixContact_MC_1,5_15-GF-3.81_1x15_P3.81mm_Horizontal_ThreadedFlange_MountHole
Generic Phoenix Contact connector footprint for: MC_1,5/15-GF-3.81; number of pins: 15; pin pitch: 3.81mm; Angled; threaded flange; footprint includes mount hole for mounting screw: ISO 1481-ST 2.2x4.5 C or ISO 7049-ST 2.2x4.5 C (http://www.fasteners.eu/standards/ISO/7049/) || order number: 1827994 8A 160V
phoenix_contact connector MC_01x15_GF_3.81mm_MH
0
15
15
Connector_Phoenix_MC
PhoenixContact_MC_1,5_16-G-3.5_1x16_P3.50mm_Horizontal
Generic Phoenix Contact connector footprint for: MC_1,5/16-G-3.5; number of pins: 16; pin pitch: 3.50mm; Angled || order number: 1844359 8A 160V
phoenix_contact connector MC_01x16_G_3.5mm
0
16
16
Connector_Phoenix_MC
PhoenixContact_MC_1,5_16-G-3.81_1x16_P3.81mm_Horizontal
Generic Phoenix Contact connector footprint for: MC_1,5/16-G-3.81; number of pins: 16; pin pitch: 3.81mm; Angled || order number: 1803413 8A 160V
phoenix_contact connector MC_01x16_G_3.81mm
0
16
16
Connector_Phoenix_MC
PhoenixContact_MC_1,5_16-GF-3.5_1x16_P3.50mm_Horizontal_ThreadedFlange
Generic Phoenix Contact connector footprint for: MC_1,5/16-GF-3.5; number of pins: 16; pin pitch: 3.50mm; Angled; threaded flange || order number: 1843936 8A 160V
phoenix_contact connector MC_01x16_GF_3.5mm
0
16
16
Connector_Phoenix_MC
PhoenixContact_MC_1,5_16-GF-3.5_1x16_P3.50mm_Horizontal_ThreadedFlange_MountHole
Generic Phoenix Contact connector footprint for: MC_1,5/16-GF-3.5; number of pins: 16; pin pitch: 3.50mm; Angled; threaded flange; footprint includes mount hole for mounting screw: ISO 1481-ST 2.2x4.5 C or ISO 7049-ST 2.2x4.5 C (http://www.fasteners.eu/standards/ISO/7049/) || order number: 1843936 8A 160V
phoenix_contact connector MC_01x16_GF_3.5mm_MH
0
16
16
Connector_Phoenix_MC
PhoenixContact_MC_1,5_16-GF-3.81_1x16_P3.81mm_Horizontal_ThreadedFlange
Generic Phoenix Contact connector footprint for: MC_1,5/16-GF-3.81; number of pins: 16; pin pitch: 3.81mm; Angled; threaded flange || order number: 1828003 8A 160V
phoenix_contact connector MC_01x16_GF_3.81mm
0
16
16
Connector_Phoenix_MC
PhoenixContact_MC_1,5_16-GF-3.81_1x16_P3.81mm_Horizontal_ThreadedFlange_MountHole
Generic Phoenix Contact connector footprint for: MC_1,5/16-GF-3.81; number of pins: 16; pin pitch: 3.81mm; Angled; threaded flange; footprint includes mount hole for mounting screw: ISO 1481-ST 2.2x4.5 C or ISO 7049-ST 2.2x4.5 C (http://www.fasteners.eu/standards/ISO/7049/) || order number: 1828003 8A 160V
phoenix_contact connector MC_01x16_GF_3.81mm_MH
0
16
16
Connector_Phoenix_MC_HighVoltage
PhoenixContact_MCV_1,5_2-G-5.08_1x02_P5.08mm_Vertical
Generic Phoenix Contact connector footprint for: MCV_1,5/2-G-5.08; number of pins: 02; pin pitch: 5.08mm; Vertical || order number: 1836299 8A 320V
phoenix_contact connector MCV_01x02_G_5.08mm
0
2
2
Connector_Phoenix_MC_HighVoltage
PhoenixContact_MCV_1,5_2-GF-5.08_1x02_P5.08mm_Vertical_ThreadedFlange
Generic Phoenix Contact connector footprint for: MCV_1,5/2-GF-5.08; number of pins: 02; pin pitch: 5.08mm; Vertical; threaded flange || order number: 1847615 8A 320V
phoenix_contact connector MCV_01x02_GF_5.08mm
0
2
2
Connector_Phoenix_MC_HighVoltage
PhoenixContact_MCV_1,5_2-GF-5.08_1x02_P5.08mm_Vertical_ThreadedFlange_MountHole
Generic Phoenix Contact connector footprint for: MCV_1,5/2-GF-5.08; number of pins: 02; pin pitch: 5.08mm; Vertical; threaded flange; footprint includes mount hole for mounting screw: ISO 1481-ST 2.2x4.5 C or ISO 7049-ST 2.2x4.5 C (http://www.fasteners.eu/standards/ISO/7049/) || order number: 1847615 8A 320V
phoenix_contact connector MCV_01x02_GF_5.08mm_MH
0
2
2
Connector_Phoenix_MC_HighVoltage
PhoenixContact_MCV_1,5_3-G-5.08_1x03_P5.08mm_Vertical
Generic Phoenix Contact connector footprint for: MCV_1,5/3-G-5.08; number of pins: 03; pin pitch: 5.08mm; Vertical || order number: 1836309 8A 320V
phoenix_contact connector MCV_01x03_G_5.08mm
0
3
3
Connector_Phoenix_MC_HighVoltage
PhoenixContact_MCV_1,5_3-GF-5.08_1x03_P5.08mm_Vertical_ThreadedFlange
Generic Phoenix Contact connector footprint for: MCV_1,5/3-GF-5.08; number of pins: 03; pin pitch: 5.08mm; Vertical; threaded flange || order number: 1847628 8A 320V
phoenix_contact connector MCV_01x03_GF_5.08mm
0
3
3
Connector_Phoenix_MC_HighVoltage
PhoenixContact_MCV_1,5_3-GF-5.08_1x03_P5.08mm_Vertical_ThreadedFlange_MountHole
Generic Phoenix Contact connector footprint for: MCV_1,5/3-GF-5.08; number of pins: 03; pin pitch: 5.08mm; Vertical; threaded flange; footprint includes mount hole for mounting screw: ISO 1481-ST 2.2x4.5 C or ISO 7049-ST 2.2x4.5 C (http://www.fasteners.eu/standards/ISO/7049/) || order number: 1847628 8A 320V
phoenix_contact connector MCV_01x03_GF_5.08mm_MH
0
3
3
Connector_Phoenix_MC_HighVoltage
PhoenixContact_MCV_1,5_4-G-5.08_1x04_P5.08mm_Vertical
Generic Phoenix Contact connector footprint for: MCV_1,5/4-G-5.08; number of pins: 04; pin pitch: 5.08mm; Vertical || order number: 1836312 8A 320V
phoenix_contact connector MCV_01x04_G_5.08mm
0
4
4
Connector_Phoenix_MC_HighVoltage
PhoenixContact_MCV_1,5_4-GF-5.08_1x04_P5.08mm_Vertical_ThreadedFlange
Generic Phoenix Contact connector footprint for: MCV_1,5/4-GF-5.08; number of pins: 04; pin pitch: 5.08mm; Vertical; threaded flange || order number: 1847631 8A 320V
phoenix_contact connector MCV_01x04_GF_5.08mm
0
4
4
Connector_Phoenix_MC_HighVoltage
PhoenixContact_MCV_1,5_4-GF-5.08_1x04_P5.08mm_Vertical_ThreadedFlange_MountHole
Generic Phoenix Contact connector footprint for: MCV_1,5/4-GF-5.08; number of pins: 04; pin pitch: 5.08mm; Vertical; threaded flange; footprint includes mount hole for mounting screw: ISO 1481-ST 2.2x4.5 C or ISO 7049-ST 2.2x4.5 C (http://www.fasteners.eu/standards/ISO/7049/) || order number: 1847631 8A 320V
phoenix_contact connector MCV_01x04_GF_5.08mm_MH
0
4
4
Connector_Phoenix_MC_HighVoltage
PhoenixContact_MCV_1,5_5-G-5.08_1x05_P5.08mm_Vertical
Generic Phoenix Contact connector footprint for: MCV_1,5/5-G-5.08; number of pins: 05; pin pitch: 5.08mm; Vertical || order number: 1836325 8A 320V
phoenix_contact connector MCV_01x05_G_5.08mm
0
5
5
Connector_Phoenix_MC_HighVoltage
PhoenixContact_MCV_1,5_5-GF-5.08_1x05_P5.08mm_Vertical_ThreadedFlange
Generic Phoenix Contact connector footprint for: MCV_1,5/5-GF-5.08; number of pins: 05; pin pitch: 5.08mm; Vertical; threaded flange || order number: 1847644 8A 320V
phoenix_contact connector MCV_01x05_GF_5.08mm
0
5
5
Connector_Phoenix_MC_HighVoltage
PhoenixContact_MCV_1,5_5-GF-5.08_1x05_P5.08mm_Vertical_ThreadedFlange_MountHole
Generic Phoenix Contact connector footprint for: MCV_1,5/5-GF-5.08; number of pins: 05; pin pitch: 5.08mm; Vertical; threaded flange; footprint includes mount hole for mounting screw: ISO 1481-ST 2.2x4.5 C or ISO 7049-ST 2.2x4.5 C (http://www.fasteners.eu/standards/ISO/7049/) || order number: 1847644 8A 320V
phoenix_contact connector MCV_01x05_GF_5.08mm_MH
0
5
5
Connector_Phoenix_MC_HighVoltage
PhoenixContact_MCV_1,5_6-G-5.08_1x06_P5.08mm_Vertical
Generic Phoenix Contact connector footprint for: MCV_1,5/6-G-5.08; number of pins: 06; pin pitch: 5.08mm; Vertical || order number: 1836338 8A 320V
phoenix_contact connector MCV_01x06_G_5.08mm
0
6
6
Connector_Phoenix_MC_HighVoltage
PhoenixContact_MCV_1,5_6-GF-5.08_1x06_P5.08mm_Vertical_ThreadedFlange
Generic Phoenix Contact connector footprint for: MCV_1,5/6-GF-5.08; number of pins: 06; pin pitch: 5.08mm; Vertical; threaded flange || order number: 1847657 8A 320V
phoenix_contact connector MCV_01x06_GF_5.08mm
0
6
6
Connector_Phoenix_MC_HighVoltage
PhoenixContact_MCV_1,5_6-GF-5.08_1x06_P5.08mm_Vertical_ThreadedFlange_MountHole
Generic Phoenix Contact connector footprint for: MCV_1,5/6-GF-5.08; number of pins: 06; pin pitch: 5.08mm; Vertical; threaded flange; footprint includes mount hole for mounting screw: ISO 1481-ST 2.2x4.5 C or ISO 7049-ST 2.2x4.5 C (http://www.fasteners.eu/standards/ISO/7049/) || order number: 1847657 8A 320V
phoenix_contact connector MCV_01x06_GF_5.08mm_MH
0
6
6
Connector_Phoenix_MC_HighVoltage
PhoenixContact_MCV_1,5_7-G-5.08_1x07_P5.08mm_Vertical
Generic Phoenix Contact connector footprint for: MCV_1,5/7-G-5.08; number of pins: 07; pin pitch: 5.08mm; Vertical || order number: 1836341 8A 320V
phoenix_contact connector MCV_01x07_G_5.08mm
0
7
7
Connector_Phoenix_MC_HighVoltage
PhoenixContact_MCV_1,5_7-GF-5.08_1x07_P5.08mm_Vertical_ThreadedFlange
Generic Phoenix Contact connector footprint for: MCV_1,5/7-GF-5.08; number of pins: 07; pin pitch: 5.08mm; Vertical; threaded flange || order number: 1847660 8A 320V
phoenix_contact connector MCV_01x07_GF_5.08mm
0
7
7
Connector_Phoenix_MC_HighVoltage
PhoenixContact_MCV_1,5_7-GF-5.08_1x07_P5.08mm_Vertical_ThreadedFlange_MountHole
Generic Phoenix Contact connector footprint for: MCV_1,5/7-GF-5.08; number of pins: 07; pin pitch: 5.08mm; Vertical; threaded flange; footprint includes mount hole for mounting screw: ISO 1481-ST 2.2x4.5 C or ISO 7049-ST 2.2x4.5 C (http://www.fasteners.eu/standards/ISO/7049/) || order number: 1847660 8A 320V
phoenix_contact connector MCV_01x07_GF_5.08mm_MH
0
7
7
Connector_Phoenix_MC_HighVoltage
PhoenixContact_MCV_1,5_8-G-5.08_1x08_P5.08mm_Vertical
Generic Phoenix Contact connector footprint for: MCV_1,5/8-G-5.08; number of pins: 08; pin pitch: 5.08mm; Vertical || order number: 1836354 8A 320V
phoenix_contact connector MCV_01x08_G_5.08mm
0
8
8
Connector_Phoenix_MC_HighVoltage
PhoenixContact_MCV_1,5_8-GF-5.08_1x08_P5.08mm_Vertical_ThreadedFlange
Generic Phoenix Contact connector footprint for: MCV_1,5/8-GF-5.08; number of pins: 08; pin pitch: 5.08mm; Vertical; threaded flange || order number: 1847673 8A 320V
phoenix_contact connector MCV_01x08_GF_5.08mm
0
8
8
Connector_Phoenix_MC_HighVoltage
PhoenixContact_MCV_1,5_8-GF-5.08_1x08_P5.08mm_Vertical_ThreadedFlange_MountHole
Generic Phoenix Contact connector footprint for: MCV_1,5/8-GF-5.08; number of pins: 08; pin pitch: 5.08mm; Vertical; threaded flange; footprint includes mount hole for mounting screw: ISO 1481-ST 2.2x4.5 C or ISO 7049-ST 2.2x4.5 C (http://www.fasteners.eu/standards/ISO/7049/) || order number: 1847673 8A 320V
phoenix_contact connector MCV_01x08_GF_5.08mm_MH
0
8
8
Connector_Phoenix_MC_HighVoltage
PhoenixContact_MCV_1,5_9-G-5.08_1x09_P5.08mm_Vertical
Generic Phoenix Contact connector footprint for: MCV_1,5/9-G-5.08; number of pins: 09; pin pitch: 5.08mm; Vertical || order number: 1836367 8A 320V
phoenix_contact connector MCV_01x09_G_5.08mm
0
9
9
Connector_Phoenix_MC_HighVoltage
PhoenixContact_MCV_1,5_9-GF-5.08_1x09_P5.08mm_Vertical_ThreadedFlange
Generic Phoenix Contact connector footprint for: MCV_1,5/9-GF-5.08; number of pins: 09; pin pitch: 5.08mm; Vertical; threaded flange || order number: 1847686 8A 320V
phoenix_contact connector MCV_01x09_GF_5.08mm
0
9
9
Connector_Phoenix_MC_HighVoltage
PhoenixContact_MCV_1,5_9-GF-5.08_1x09_P5.08mm_Vertical_ThreadedFlange_MountHole
Generic Phoenix Contact connector footprint for: MCV_1,5/9-GF-5.08; number of pins: 09; pin pitch: 5.08mm; Vertical; threaded flange; footprint includes mount hole for mounting screw: ISO 1481-ST 2.2x4.5 C or ISO 7049-ST 2.2x4.5 C (http://www.fasteners.eu/standards/ISO/7049/) || order number: 1847686 8A 320V
phoenix_contact connector MCV_01x09_GF_5.08mm_MH
0
9
9
Connector_Phoenix_MC_HighVoltage
PhoenixContact_MCV_1,5_10-G-5.08_1x10_P5.08mm_Vertical
Generic Phoenix Contact connector footprint for: MCV_1,5/10-G-5.08; number of pins: 10; pin pitch: 5.08mm; Vertical || order number: 1836370 8A 320V
phoenix_contact connector MCV_01x10_G_5.08mm
0
10
10
Connector_Phoenix_MC_HighVoltage
PhoenixContact_MCV_1,5_10-GF-5.08_1x10_P5.08mm_Vertical_ThreadedFlange
Generic Phoenix Contact connector footprint for: MCV_1,5/10-GF-5.08; number of pins: 10; pin pitch: 5.08mm; Vertical; threaded flange || order number: 1847699 8A 320V
phoenix_contact connector MCV_01x10_GF_5.08mm
0
10
10
Connector_Phoenix_MC_HighVoltage
PhoenixContact_MCV_1,5_10-GF-5.08_1x10_P5.08mm_Vertical_ThreadedFlange_MountHole
Generic Phoenix Contact connector footprint for: MCV_1,5/10-GF-5.08; number of pins: 10; pin pitch: 5.08mm; Vertical; threaded flange; footprint includes mount hole for mounting screw: ISO 1481-ST 2.2x4.5 C or ISO 7049-ST 2.2x4.5 C (http://www.fasteners.eu/standards/ISO/7049/) || order number: 1847699 8A 320V
phoenix_contact connector MCV_01x10_GF_5.08mm_MH
0
10
10
Connector_Phoenix_MC_HighVoltage
PhoenixContact_MCV_1,5_11-G-5.08_1x11_P5.08mm_Vertical
Generic Phoenix Contact connector footprint for: MCV_1,5/11-G-5.08; number of pins: 11; pin pitch: 5.08mm; Vertical || order number: 1836383 8A 320V
phoenix_contact connector MCV_01x11_G_5.08mm
0
11
11
Connector_Phoenix_MC_HighVoltage
PhoenixContact_MCV_1,5_11-GF-5.08_1x11_P5.08mm_Vertical_ThreadedFlange
Generic Phoenix Contact connector footprint for: MCV_1,5/11-GF-5.08; number of pins: 11; pin pitch: 5.08mm; Vertical; threaded flange || order number: 1847709 8A 320V
phoenix_contact connector MCV_01x11_GF_5.08mm
0
11
11
Connector_Phoenix_MC_HighVoltage
PhoenixContact_MCV_1,5_11-GF-5.08_1x11_P5.08mm_Vertical_ThreadedFlange_MountHole
Generic Phoenix Contact connector footprint for: MCV_1,5/11-GF-5.08; number of pins: 11; pin pitch: 5.08mm; Vertical; threaded flange; footprint includes mount hole for mounting screw: ISO 1481-ST 2.2x4.5 C or ISO 7049-ST 2.2x4.5 C (http://www.fasteners.eu/standards/ISO/7049/) || order number: 1847709 8A 320V
phoenix_contact connector MCV_01x11_GF_5.08mm_MH
0
11
11
Connector_Phoenix_MC_HighVoltage
PhoenixContact_MCV_1,5_12-G-5.08_1x12_P5.08mm_Vertical
Generic Phoenix Contact connector footprint for: MCV_1,5/12-G-5.08; number of pins: 12; pin pitch: 5.08mm; Vertical || order number: 1836396 8A 320V
phoenix_contact connector MCV_01x12_G_5.08mm
0
12
12
Connector_Phoenix_MC_HighVoltage
PhoenixContact_MCV_1,5_12-GF-5.08_1x12_P5.08mm_Vertical_ThreadedFlange
Generic Phoenix Contact connector footprint for: MCV_1,5/12-GF-5.08; number of pins: 12; pin pitch: 5.08mm; Vertical; threaded flange || order number: 1847712 8A 320V
phoenix_contact connector MCV_01x12_GF_5.08mm
0
12
12
Connector_Phoenix_MC_HighVoltage
PhoenixContact_MCV_1,5_12-GF-5.08_1x12_P5.08mm_Vertical_ThreadedFlange_MountHole
Generic Phoenix Contact connector footprint for: MCV_1,5/12-GF-5.08; number of pins: 12; pin pitch: 5.08mm; Vertical; threaded flange; footprint includes mount hole for mounting screw: ISO 1481-ST 2.2x4.5 C or ISO 7049-ST 2.2x4.5 C (http://www.fasteners.eu/standards/ISO/7049/) || order number: 1847712 8A 320V
phoenix_contact connector MCV_01x12_GF_5.08mm_MH
0
12
12
Connector_Phoenix_MC_HighVoltage
PhoenixContact_MC_1,5_2-G-5.08_1x02_P5.08mm_Horizontal
Generic Phoenix Contact connector footprint for: MC_1,5/2-G-5.08; number of pins: 02; pin pitch: 5.08mm; Angled || order number: 1836189 8A 320V
phoenix_contact connector MC_01x02_G_5.08mm
0
2
2
Connector_Phoenix_MC_HighVoltage
PhoenixContact_MC_1,5_2-GF-5.08_1x02_P5.08mm_Horizontal_ThreadedFlange
Generic Phoenix Contact connector footprint for: MC_1,5/2-GF-5.08; number of pins: 02; pin pitch: 5.08mm; Angled; threaded flange || order number: 1847466 8A 320V
phoenix_contact connector MC_01x02_GF_5.08mm
0
2
2
Connector_Phoenix_MC_HighVoltage
PhoenixContact_MC_1,5_2-GF-5.08_1x02_P5.08mm_Horizontal_ThreadedFlange_MountHole
Generic Phoenix Contact connector footprint for: MC_1,5/2-GF-5.08; number of pins: 02; pin pitch: 5.08mm; Angled; threaded flange; footprint includes mount hole for mounting screw: ISO 1481-ST 2.2x4.5 C or ISO 7049-ST 2.2x4.5 C (http://www.fasteners.eu/standards/ISO/7049/) || order number: 1847466 8A 320V
phoenix_contact connector MC_01x02_GF_5.08mm_MH
0
2
2
Connector_Phoenix_MC_HighVoltage
PhoenixContact_MC_1,5_3-G-5.08_1x03_P5.08mm_Horizontal
Generic Phoenix Contact connector footprint for: MC_1,5/3-G-5.08; number of pins: 03; pin pitch: 5.08mm; Angled || order number: 1836192 8A 320V
phoenix_contact connector MC_01x03_G_5.08mm
0
3
3
Connector_Phoenix_MC_HighVoltage
PhoenixContact_MC_1,5_3-GF-5.08_1x03_P5.08mm_Horizontal_ThreadedFlange
Generic Phoenix Contact connector footprint for: MC_1,5/3-GF-5.08; number of pins: 03; pin pitch: 5.08mm; Angled; threaded flange || order number: 1847479 8A 320V
phoenix_contact connector MC_01x03_GF_5.08mm
0
3
3
Connector_Phoenix_MC_HighVoltage
PhoenixContact_MC_1,5_3-GF-5.08_1x03_P5.08mm_Horizontal_ThreadedFlange_MountHole
Generic Phoenix Contact connector footprint for: MC_1,5/3-GF-5.08; number of pins: 03; pin pitch: 5.08mm; Angled; threaded flange; footprint includes mount hole for mounting screw: ISO 1481-ST 2.2x4.5 C or ISO 7049-ST 2.2x4.5 C (http://www.fasteners.eu/standards/ISO/7049/) || order number: 1847479 8A 320V
phoenix_contact connector MC_01x03_GF_5.08mm_MH
0
3
3
Connector_Phoenix_MC_HighVoltage
PhoenixContact_MC_1,5_4-G-5.08_1x04_P5.08mm_Horizontal
Generic Phoenix Contact connector footprint for: MC_1,5/4-G-5.08; number of pins: 04; pin pitch: 5.08mm; Angled || order number: 1836202 8A 320V
phoenix_contact connector MC_01x04_G_5.08mm
0
4
4
Connector_Phoenix_MC_HighVoltage
PhoenixContact_MC_1,5_4-GF-5.08_1x04_P5.08mm_Horizontal_ThreadedFlange
Generic Phoenix Contact connector footprint for: MC_1,5/4-GF-5.08; number of pins: 04; pin pitch: 5.08mm; Angled; threaded flange || order number: 1847482 8A 320V
phoenix_contact connector MC_01x04_GF_5.08mm
0
4
4
Connector_Phoenix_MC_HighVoltage
PhoenixContact_MC_1,5_4-GF-5.08_1x04_P5.08mm_Horizontal_ThreadedFlange_MountHole
Generic Phoenix Contact connector footprint for: MC_1,5/4-GF-5.08; number of pins: 04; pin pitch: 5.08mm; Angled; threaded flange; footprint includes mount hole for mounting screw: ISO 1481-ST 2.2x4.5 C or ISO 7049-ST 2.2x4.5 C (http://www.fasteners.eu/standards/ISO/7049/) || order number: 1847482 8A 320V
phoenix_contact connector MC_01x04_GF_5.08mm_MH
0
4
4
Connector_Phoenix_MC_HighVoltage
PhoenixContact_MC_1,5_5-G-5.08_1x05_P5.08mm_Horizontal
Generic Phoenix Contact connector footprint for: MC_1,5/5-G-5.08; number of pins: 05; pin pitch: 5.08mm; Angled || order number: 1836215 8A 320V
phoenix_contact connector MC_01x05_G_5.08mm
0
5
5
Connector_Phoenix_MC_HighVoltage
PhoenixContact_MC_1,5_5-GF-5.08_1x05_P5.08mm_Horizontal_ThreadedFlange
Generic Phoenix Contact connector footprint for: MC_1,5/5-GF-5.08; number of pins: 05; pin pitch: 5.08mm; Angled; threaded flange || order number: 1847495 8A 320V
phoenix_contact connector MC_01x05_GF_5.08mm
0
5
5
Connector_Phoenix_MC_HighVoltage
PhoenixContact_MC_1,5_5-GF-5.08_1x05_P5.08mm_Horizontal_ThreadedFlange_MountHole
Generic Phoenix Contact connector footprint for: MC_1,5/5-GF-5.08; number of pins: 05; pin pitch: 5.08mm; Angled; threaded flange; footprint includes mount hole for mounting screw: ISO 1481-ST 2.2x4.5 C or ISO 7049-ST 2.2x4.5 C (http://www.fasteners.eu/standards/ISO/7049/) || order number: 1847495 8A 320V
phoenix_contact connector MC_01x05_GF_5.08mm_MH
0
5
5
Connector_Phoenix_MC_HighVoltage
PhoenixContact_MC_1,5_6-G-5.08_1x06_P5.08mm_Horizontal
Generic Phoenix Contact connector footprint for: MC_1,5/6-G-5.08; number of pins: 06; pin pitch: 5.08mm; Angled || order number: 1836228 8A 320V
phoenix_contact connector MC_01x06_G_5.08mm
0
6
6
Connector_Phoenix_MC_HighVoltage
PhoenixContact_MC_1,5_6-GF-5.08_1x06_P5.08mm_Horizontal_ThreadedFlange
Generic Phoenix Contact connector footprint for: MC_1,5/6-GF-5.08; number of pins: 06; pin pitch: 5.08mm; Angled; threaded flange || order number: 1847505 8A 320V
phoenix_contact connector MC_01x06_GF_5.08mm
0
6
6
Connector_Phoenix_MC_HighVoltage
PhoenixContact_MC_1,5_6-GF-5.08_1x06_P5.08mm_Horizontal_ThreadedFlange_MountHole
Generic Phoenix Contact connector footprint for: MC_1,5/6-GF-5.08; number of pins: 06; pin pitch: 5.08mm; Angled; threaded flange; footprint includes mount hole for mounting screw: ISO 1481-ST 2.2x4.5 C or ISO 7049-ST 2.2x4.5 C (http://www.fasteners.eu/standards/ISO/7049/) || order number: 1847505 8A 320V
phoenix_contact connector MC_01x06_GF_5.08mm_MH
0
6
6
Connector_Phoenix_MC_HighVoltage
PhoenixContact_MC_1,5_7-G-5.08_1x07_P5.08mm_Horizontal
Generic Phoenix Contact connector footprint for: MC_1,5/7-G-5.08; number of pins: 07; pin pitch: 5.08mm; Angled || order number: 1836231 8A 320V
phoenix_contact connector MC_01x07_G_5.08mm
0
7
7
Connector_Phoenix_MC_HighVoltage
PhoenixContact_MC_1,5_7-GF-5.08_1x07_P5.08mm_Horizontal_ThreadedFlange
Generic Phoenix Contact connector footprint for: MC_1,5/7-GF-5.08; number of pins: 07; pin pitch: 5.08mm; Angled; threaded flange || order number: 1847518 8A 320V
phoenix_contact connector MC_01x07_GF_5.08mm
0
7
7
Connector_Phoenix_MC_HighVoltage
PhoenixContact_MC_1,5_7-GF-5.08_1x07_P5.08mm_Horizontal_ThreadedFlange_MountHole
Generic Phoenix Contact connector footprint for: MC_1,5/7-GF-5.08; number of pins: 07; pin pitch: 5.08mm; Angled; threaded flange; footprint includes mount hole for mounting screw: ISO 1481-ST 2.2x4.5 C or ISO 7049-ST 2.2x4.5 C (http://www.fasteners.eu/standards/ISO/7049/) || order number: 1847518 8A 320V
phoenix_contact connector MC_01x07_GF_5.08mm_MH
0
7
7
Connector_Phoenix_MC_HighVoltage
PhoenixContact_MC_1,5_8-G-5.08_1x08_P5.08mm_Horizontal
Generic Phoenix Contact connector footprint for: MC_1,5/8-G-5.08; number of pins: 08; pin pitch: 5.08mm; Angled || order number: 1836244 8A 320V
phoenix_contact connector MC_01x08_G_5.08mm
0
8
8
Connector_Phoenix_MC_HighVoltage
PhoenixContact_MC_1,5_8-GF-5.08_1x08_P5.08mm_Horizontal_ThreadedFlange
Generic Phoenix Contact connector footprint for: MC_1,5/8-GF-5.08; number of pins: 08; pin pitch: 5.08mm; Angled; threaded flange || order number: 1847521 8A 320V
phoenix_contact connector MC_01x08_GF_5.08mm
0
8
8
Connector_Phoenix_MC_HighVoltage
PhoenixContact_MC_1,5_8-GF-5.08_1x08_P5.08mm_Horizontal_ThreadedFlange_MountHole
Generic Phoenix Contact connector footprint for: MC_1,5/8-GF-5.08; number of pins: 08; pin pitch: 5.08mm; Angled; threaded flange; footprint includes mount hole for mounting screw: ISO 1481-ST 2.2x4.5 C or ISO 7049-ST 2.2x4.5 C (http://www.fasteners.eu/standards/ISO/7049/) || order number: 1847521 8A 320V
phoenix_contact connector MC_01x08_GF_5.08mm_MH
0
8
8
Connector_Phoenix_MC_HighVoltage
PhoenixContact_MC_1,5_9-G-5.08_1x09_P5.08mm_Horizontal
Generic Phoenix Contact connector footprint for: MC_1,5/9-G-5.08; number of pins: 09; pin pitch: 5.08mm; Angled || order number: 1836257 8A 320V
phoenix_contact connector MC_01x09_G_5.08mm
0
9
9
Connector_Phoenix_MC_HighVoltage
PhoenixContact_MC_1,5_9-GF-5.08_1x09_P5.08mm_Horizontal_ThreadedFlange
Generic Phoenix Contact connector footprint for: MC_1,5/9-GF-5.08; number of pins: 09; pin pitch: 5.08mm; Angled; threaded flange || order number: 1847534 8A 320V
phoenix_contact connector MC_01x09_GF_5.08mm
0
9
9
Connector_Phoenix_MC_HighVoltage
PhoenixContact_MC_1,5_9-GF-5.08_1x09_P5.08mm_Horizontal_ThreadedFlange_MountHole
Generic Phoenix Contact connector footprint for: MC_1,5/9-GF-5.08; number of pins: 09; pin pitch: 5.08mm; Angled; threaded flange; footprint includes mount hole for mounting screw: ISO 1481-ST 2.2x4.5 C or ISO 7049-ST 2.2x4.5 C (http://www.fasteners.eu/standards/ISO/7049/) || order number: 1847534 8A 320V
phoenix_contact connector MC_01x09_GF_5.08mm_MH
0
9
9
Connector_Phoenix_MC_HighVoltage
PhoenixContact_MC_1,5_10-G-5.08_1x10_P5.08mm_Horizontal
Generic Phoenix Contact connector footprint for: MC_1,5/10-G-5.08; number of pins: 10; pin pitch: 5.08mm; Angled || order number: 1836260 8A 320V
phoenix_contact connector MC_01x10_G_5.08mm
0
10
10
Connector_Phoenix_MC_HighVoltage
PhoenixContact_MC_1,5_10-GF-5.08_1x10_P5.08mm_Horizontal_ThreadedFlange
Generic Phoenix Contact connector footprint for: MC_1,5/10-GF-5.08; number of pins: 10; pin pitch: 5.08mm; Angled; threaded flange || order number: 1847547 8A 320V
phoenix_contact connector MC_01x10_GF_5.08mm
0
10
10
Connector_Phoenix_MC_HighVoltage
PhoenixContact_MC_1,5_10-GF-5.08_1x10_P5.08mm_Horizontal_ThreadedFlange_MountHole
Generic Phoenix Contact connector footprint for: MC_1,5/10-GF-5.08; number of pins: 10; pin pitch: 5.08mm; Angled; threaded flange; footprint includes mount hole for mounting screw: ISO 1481-ST 2.2x4.5 C or ISO 7049-ST 2.2x4.5 C (http://www.fasteners.eu/standards/ISO/7049/) || order number: 1847547 8A 320V
phoenix_contact connector MC_01x10_GF_5.08mm_MH
0
10
10
Connector_Phoenix_MC_HighVoltage
PhoenixContact_MC_1,5_11-G-5.08_1x11_P5.08mm_Horizontal
Generic Phoenix Contact connector footprint for: MC_1,5/11-G-5.08; number of pins: 11; pin pitch: 5.08mm; Angled || order number: 1836273 8A 320V
phoenix_contact connector MC_01x11_G_5.08mm
0
11
11
Connector_Phoenix_MC_HighVoltage
PhoenixContact_MC_1,5_11-GF-5.08_1x11_P5.08mm_Horizontal_ThreadedFlange
Generic Phoenix Contact connector footprint for: MC_1,5/11-GF-5.08; number of pins: 11; pin pitch: 5.08mm; Angled; threaded flange || order number: 1847550 8A 320V
phoenix_contact connector MC_01x11_GF_5.08mm
0
11
11
Connector_Phoenix_MC_HighVoltage
PhoenixContact_MC_1,5_11-GF-5.08_1x11_P5.08mm_Horizontal_ThreadedFlange_MountHole
Generic Phoenix Contact connector footprint for: MC_1,5/11-GF-5.08; number of pins: 11; pin pitch: 5.08mm; Angled; threaded flange; footprint includes mount hole for mounting screw: ISO 1481-ST 2.2x4.5 C or ISO 7049-ST 2.2x4.5 C (http://www.fasteners.eu/standards/ISO/7049/) || order number: 1847550 8A 320V
phoenix_contact connector MC_01x11_GF_5.08mm_MH
0
11
11
Connector_Phoenix_MC_HighVoltage
PhoenixContact_MC_1,5_12-G-5.08_1x12_P5.08mm_Horizontal
Generic Phoenix Contact connector footprint for: MC_1,5/12-G-5.08; number of pins: 12; pin pitch: 5.08mm; Angled || order number: 1836286 8A 320V
phoenix_contact connector MC_01x12_G_5.08mm
0
12
12
Connector_Phoenix_MC_HighVoltage
PhoenixContact_MC_1,5_12-GF-5.08_1x12_P5.08mm_Horizontal_ThreadedFlange
Generic Phoenix Contact connector footprint for: MC_1,5/12-GF-5.08; number of pins: 12; pin pitch: 5.08mm; Angled; threaded flange || order number: 1847563 8A 320V
phoenix_contact connector MC_01x12_GF_5.08mm
0
12
12
Connector_Phoenix_MC_HighVoltage
PhoenixContact_MC_1,5_12-GF-5.08_1x12_P5.08mm_Horizontal_ThreadedFlange_MountHole
Generic Phoenix Contact connector footprint for: MC_1,5/12-GF-5.08; number of pins: 12; pin pitch: 5.08mm; Angled; threaded flange; footprint includes mount hole for mounting screw: ISO 1481-ST 2.2x4.5 C or ISO 7049-ST 2.2x4.5 C (http://www.fasteners.eu/standards/ISO/7049/) || order number: 1847563 8A 320V
phoenix_contact connector MC_01x12_GF_5.08mm_MH
0
12
12
Connector_Phoenix_MSTB
PhoenixContact_MSTBA_2,5_2-G-5,08_1x02_P5.08mm_Horizontal
Generic Phoenix Contact connector footprint for: MSTBA_2,5/2-G-5,08; number of pins: 02; pin pitch: 5.08mm; Angled || order number: 1757242 12A || order number: 1923869 16A (HC)
phoenix_contact connector MSTBA_01x02_G_5.08mm
0
2
2
Connector_Phoenix_MSTB
PhoenixContact_MSTBA_2,5_2-G_1x02_P5.00mm_Horizontal
Generic Phoenix Contact connector footprint for: MSTBA_2,5/2-G; number of pins: 02; pin pitch: 5.00mm; Angled || order number: 1757475 12A || order number: 1923759 16A (HC)
phoenix_contact connector MSTBA_01x02_G_5.00mm
0
2
2
Connector_Phoenix_MSTB
PhoenixContact_MSTBA_2,5_3-G-5,08_1x03_P5.08mm_Horizontal
Generic Phoenix Contact connector footprint for: MSTBA_2,5/3-G-5,08; number of pins: 03; pin pitch: 5.08mm; Angled || order number: 1757255 12A || order number: 1923872 16A (HC)
phoenix_contact connector MSTBA_01x03_G_5.08mm
0
3
3
Connector_Phoenix_MSTB
PhoenixContact_MSTBA_2,5_3-G_1x03_P5.00mm_Horizontal
Generic Phoenix Contact connector footprint for: MSTBA_2,5/3-G; number of pins: 03; pin pitch: 5.00mm; Angled || order number: 1757488 12A || order number: 1923762 16A (HC)
phoenix_contact connector MSTBA_01x03_G_5.00mm
0
3
3
Connector_Phoenix_MSTB
PhoenixContact_MSTBA_2,5_4-G-5,08_1x04_P5.08mm_Horizontal
Generic Phoenix Contact connector footprint for: MSTBA_2,5/4-G-5,08; number of pins: 04; pin pitch: 5.08mm; Angled || order number: 1757268 12A || order number: 1923885 16A (HC)
phoenix_contact connector MSTBA_01x04_G_5.08mm
0
4
4
Connector_Phoenix_MSTB
PhoenixContact_MSTBA_2,5_4-G_1x04_P5.00mm_Horizontal
Generic Phoenix Contact connector footprint for: MSTBA_2,5/4-G; number of pins: 04; pin pitch: 5.00mm; Angled || order number: 1757491 12A || order number: 1923775 16A (HC)
phoenix_contact connector MSTBA_01x04_G_5.00mm
0
4
4
Connector_Phoenix_MSTB
PhoenixContact_MSTBA_2,5_5-G-5,08_1x05_P5.08mm_Horizontal
Generic Phoenix Contact connector footprint for: MSTBA_2,5/5-G-5,08; number of pins: 05; pin pitch: 5.08mm; Angled || order number: 1757271 12A || order number: 1923898 16A (HC)
phoenix_contact connector MSTBA_01x05_G_5.08mm
0
5
5
Connector_Phoenix_MSTB
PhoenixContact_MSTBA_2,5_5-G_1x05_P5.00mm_Horizontal
Generic Phoenix Contact connector footprint for: MSTBA_2,5/5-G; number of pins: 05; pin pitch: 5.00mm; Angled || order number: 1757501 12A || order number: 1923788 16A (HC)
phoenix_contact connector MSTBA_01x05_G_5.00mm
0
5
5
Connector_Phoenix_MSTB
PhoenixContact_MSTBA_2,5_6-G-5,08_1x06_P5.08mm_Horizontal
Generic Phoenix Contact connector footprint for: MSTBA_2,5/6-G-5,08; number of pins: 06; pin pitch: 5.08mm; Angled || order number: 1757284 12A || order number: 1923908 16A (HC)
phoenix_contact connector MSTBA_01x06_G_5.08mm
0
6
6
Connector_Phoenix_MSTB
PhoenixContact_MSTBA_2,5_6-G_1x06_P5.00mm_Horizontal
Generic Phoenix Contact connector footprint for: MSTBA_2,5/6-G; number of pins: 06; pin pitch: 5.00mm; Angled || order number: 1757514 12A || order number: 1923791 16A (HC)
phoenix_contact connector MSTBA_01x06_G_5.00mm
0
6
6
Connector_Phoenix_MSTB
PhoenixContact_MSTBA_2,5_7-G-5,08_1x07_P5.08mm_Horizontal
Generic Phoenix Contact connector footprint for: MSTBA_2,5/7-G-5,08; number of pins: 07; pin pitch: 5.08mm; Angled || order number: 1757297 12A || order number: 1923911 16A (HC)
phoenix_contact connector MSTBA_01x07_G_5.08mm
0
7
7
Connector_Phoenix_MSTB
PhoenixContact_MSTBA_2,5_7-G_1x07_P5.00mm_Horizontal
Generic Phoenix Contact connector footprint for: MSTBA_2,5/7-G; number of pins: 07; pin pitch: 5.00mm; Angled || order number: 1757493 12A || order number: 1923801 16A (HC)
phoenix_contact connector MSTBA_01x07_G_5.00mm
0
7
7
Connector_Phoenix_MSTB
PhoenixContact_MSTBA_2,5_8-G-5,08_1x08_P5.08mm_Horizontal
Generic Phoenix Contact connector footprint for: MSTBA_2,5/8-G-5,08; number of pins: 08; pin pitch: 5.08mm; Angled || order number: 1757307 12A || order number: 1923924 16A (HC)
phoenix_contact connector MSTBA_01x08_G_5.08mm
0
8
8
Connector_Phoenix_MSTB
PhoenixContact_MSTBA_2,5_8-G_1x08_P5.00mm_Horizontal
Generic Phoenix Contact connector footprint for: MSTBA_2,5/8-G; number of pins: 08; pin pitch: 5.00mm; Angled || order number: 1757527 12A || order number: 1923814 16A (HC)
phoenix_contact connector MSTBA_01x08_G_5.00mm
0
8
8
Connector_Phoenix_MSTB
PhoenixContact_MSTBA_2,5_9-G-5,08_1x09_P5.08mm_Horizontal
Generic Phoenix Contact connector footprint for: MSTBA_2,5/9-G-5,08; number of pins: 09; pin pitch: 5.08mm; Angled || order number: 1757310 12A || order number: 1923937 16A (HC)
phoenix_contact connector MSTBA_01x09_G_5.08mm
0
9
9
Connector_Phoenix_MSTB
PhoenixContact_MSTBA_2,5_9-G_1x09_P5.00mm_Horizontal
Generic Phoenix Contact connector footprint for: MSTBA_2,5/9-G; number of pins: 09; pin pitch: 5.00mm; Angled || order number: 1757530 12A || order number: 1923827 16A (HC)
phoenix_contact connector MSTBA_01x09_G_5.00mm
0
9
9
Connector_Phoenix_MSTB
PhoenixContact_MSTBA_2,5_10-G-5,08_1x10_P5.08mm_Horizontal
Generic Phoenix Contact connector footprint for: MSTBA_2,5/10-G-5,08; number of pins: 10; pin pitch: 5.08mm; Angled || order number: 1757323 12A || order number: 1923940 16A (HC)
phoenix_contact connector MSTBA_01x10_G_5.08mm
0
10
10
Connector_Phoenix_MSTB
PhoenixContact_MSTBA_2,5_10-G_1x10_P5.00mm_Horizontal
Generic Phoenix Contact connector footprint for: MSTBA_2,5/10-G; number of pins: 10; pin pitch: 5.00mm; Angled || order number: 1757543 12A || order number: 1923830 16A (HC)
phoenix_contact connector MSTBA_01x10_G_5.00mm
0
10
10
Connector_Phoenix_MSTB
PhoenixContact_MSTBA_2,5_11-G-5,08_1x11_P5.08mm_Horizontal
Generic Phoenix Contact connector footprint for: MSTBA_2,5/11-G-5,08; number of pins: 11; pin pitch: 5.08mm; Angled || order number: 1757336 12A || order number: 1923953 16A (HC)
phoenix_contact connector MSTBA_01x11_G_5.08mm
0
11
11
Connector_Phoenix_MSTB
PhoenixContact_MSTBA_2,5_11-G_1x11_P5.00mm_Horizontal
Generic Phoenix Contact connector footprint for: MSTBA_2,5/11-G; number of pins: 11; pin pitch: 5.00mm; Angled || order number: 1757556 12A || order number: 1923843 16A (HC)
phoenix_contact connector MSTBA_01x11_G_5.00mm
0
11
11
Connector_Phoenix_MSTB
PhoenixContact_MSTBA_2,5_12-G-5,08_1x12_P5.08mm_Horizontal
Generic Phoenix Contact connector footprint for: MSTBA_2,5/12-G-5,08; number of pins: 12; pin pitch: 5.08mm; Angled || order number: 1757349 12A || order number: 1923966 16A (HC)
phoenix_contact connector MSTBA_01x12_G_5.08mm
0
12
12
Connector_Phoenix_MSTB
PhoenixContact_MSTBA_2,5_12-G_1x12_P5.00mm_Horizontal
Generic Phoenix Contact connector footprint for: MSTBA_2,5/12-G; number of pins: 12; pin pitch: 5.00mm; Angled || order number: 1757569 12A || order number: 1923856 16A (HC)
phoenix_contact connector MSTBA_01x12_G_5.00mm
0
12
12
Connector_Phoenix_MSTB
PhoenixContact_MSTBA_2,5_13-G-5,08_1x13_P5.08mm_Horizontal
Generic Phoenix Contact connector footprint for: MSTBA_2,5/13-G-5,08; number of pins: 13; pin pitch: 5.08mm; Angled || order number: 1757352 12A
phoenix_contact connector MSTBA_01x13_G_5.08mm
0
13
13
Connector_Phoenix_MSTB
PhoenixContact_MSTBA_2,5_13-G_1x13_P5.00mm_Horizontal
Generic Phoenix Contact connector footprint for: MSTBA_2,5/13-G; number of pins: 13; pin pitch: 5.00mm; Angled || order number: 1757572 12A
phoenix_contact connector MSTBA_01x13_G_5.00mm
0
13
13
Connector_Phoenix_MSTB
PhoenixContact_MSTBA_2,5_14-G-5,08_1x14_P5.08mm_Horizontal
Generic Phoenix Contact connector footprint for: MSTBA_2,5/14-G-5,08; number of pins: 14; pin pitch: 5.08mm; Angled || order number: 1757365 12A
phoenix_contact connector MSTBA_01x14_G_5.08mm
0
14
14
Connector_Phoenix_MSTB
PhoenixContact_MSTBA_2,5_14-G_1x14_P5.00mm_Horizontal
Generic Phoenix Contact connector footprint for: MSTBA_2,5/14-G; number of pins: 14; pin pitch: 5.00mm; Angled || order number: 1757585 12A
phoenix_contact connector MSTBA_01x14_G_5.00mm
0
14
14
Connector_Phoenix_MSTB
PhoenixContact_MSTBA_2,5_15-G-5,08_1x15_P5.08mm_Horizontal
Generic Phoenix Contact connector footprint for: MSTBA_2,5/15-G-5,08; number of pins: 15; pin pitch: 5.08mm; Angled || order number: 1757378 12A
phoenix_contact connector MSTBA_01x15_G_5.08mm
0
15
15
Connector_Phoenix_MSTB
PhoenixContact_MSTBA_2,5_15-G_1x15_P5.00mm_Horizontal
Generic Phoenix Contact connector footprint for: MSTBA_2,5/15-G; number of pins: 15; pin pitch: 5.00mm; Angled || order number: 1757598 12A
phoenix_contact connector MSTBA_01x15_G_5.00mm
0
15
15
Connector_Phoenix_MSTB
PhoenixContact_MSTBA_2,5_16-G-5,08_1x16_P5.08mm_Horizontal
Generic Phoenix Contact connector footprint for: MSTBA_2,5/16-G-5,08; number of pins: 16; pin pitch: 5.08mm; Angled || order number: 1757381 12A
phoenix_contact connector MSTBA_01x16_G_5.08mm
0
16
16
Connector_Phoenix_MSTB
PhoenixContact_MSTBA_2,5_16-G_1x16_P5.00mm_Horizontal
Generic Phoenix Contact connector footprint for: MSTBA_2,5/16-G; number of pins: 16; pin pitch: 5.00mm; Angled || order number: 1757608 12A
phoenix_contact connector MSTBA_01x16_G_5.00mm
0
16
16
Connector_Phoenix_MSTB
PhoenixContact_MSTBVA_2,5_2-G-5,08_1x02_P5.08mm_Vertical
Generic Phoenix Contact connector footprint for: MSTBVA_2,5/2-G-5,08; number of pins: 02; pin pitch: 5.08mm; Vertical || order number: 1755736 12A || order number: 1924305 16A (HC)
phoenix_contact connector MSTBVA_01x02_G_5.08mm
0
2
2
Connector_Phoenix_MSTB
PhoenixContact_MSTBVA_2,5_2-G_1x02_P5.00mm_Vertical
Generic Phoenix Contact connector footprint for: MSTBVA_2,5/2-G; number of pins: 02; pin pitch: 5.00mm; Vertical || order number: 1755516 12A || order number: 1924198 16A (HC)
phoenix_contact connector MSTBVA_01x02_G_5.00mm
0
2
2
Connector_Phoenix_MSTB
PhoenixContact_MSTBVA_2,5_3-G-5,08_1x03_P5.08mm_Vertical
Generic Phoenix Contact connector footprint for: MSTBVA_2,5/3-G-5,08; number of pins: 03; pin pitch: 5.08mm; Vertical || order number: 1755749 12A || order number: 1924318 16A (HC)
phoenix_contact connector MSTBVA_01x03_G_5.08mm
0
3
3
Connector_Phoenix_MSTB
PhoenixContact_MSTBVA_2,5_3-G_1x03_P5.00mm_Vertical
Generic Phoenix Contact connector footprint for: MSTBVA_2,5/3-G; number of pins: 03; pin pitch: 5.00mm; Vertical || order number: 1755529 12A || order number: 1924208 16A (HC)
phoenix_contact connector MSTBVA_01x03_G_5.00mm
0
3
3
Connector_Phoenix_MSTB
PhoenixContact_MSTBVA_2,5_4-G-5,08_1x04_P5.08mm_Vertical
Generic Phoenix Contact connector footprint for: MSTBVA_2,5/4-G-5,08; number of pins: 04; pin pitch: 5.08mm; Vertical || order number: 1755752 12A || order number: 1924321 16A (HC)
phoenix_contact connector MSTBVA_01x04_G_5.08mm
0
4
4
Connector_Phoenix_MSTB
PhoenixContact_MSTBVA_2,5_4-G_1x04_P5.00mm_Vertical
Generic Phoenix Contact connector footprint for: MSTBVA_2,5/4-G; number of pins: 04; pin pitch: 5.00mm; Vertical || order number: 1755532 12A || order number: 1924211 16A (HC)
phoenix_contact connector MSTBVA_01x04_G_5.00mm
0
4
4
Connector_Phoenix_MSTB
PhoenixContact_MSTBVA_2,5_5-G-5,08_1x05_P5.08mm_Vertical
Generic Phoenix Contact connector footprint for: MSTBVA_2,5/5-G-5,08; number of pins: 05; pin pitch: 5.08mm; Vertical || order number: 1755765 12A || order number: 1924334 16A (HC)
phoenix_contact connector MSTBVA_01x05_G_5.08mm
0
5
5
Connector_Phoenix_MSTB
PhoenixContact_MSTBVA_2,5_5-G_1x05_P5.00mm_Vertical
Generic Phoenix Contact connector footprint for: MSTBVA_2,5/5-G; number of pins: 05; pin pitch: 5.00mm; Vertical || order number: 1755545 12A || order number: 1924224 16A (HC)
phoenix_contact connector MSTBVA_01x05_G_5.00mm
0
5
5
Connector_Phoenix_MSTB
PhoenixContact_MSTBVA_2,5_6-G-5,08_1x06_P5.08mm_Vertical
Generic Phoenix Contact connector footprint for: MSTBVA_2,5/6-G-5,08; number of pins: 06; pin pitch: 5.08mm; Vertical || order number: 1755778 12A || order number: 1924347 16A (HC)
phoenix_contact connector MSTBVA_01x06_G_5.08mm
0
6
6
Connector_Phoenix_MSTB
PhoenixContact_MSTBVA_2,5_6-G_1x06_P5.00mm_Vertical
Generic Phoenix Contact connector footprint for: MSTBVA_2,5/6-G; number of pins: 06; pin pitch: 5.00mm; Vertical || order number: 1755558 12A || order number: 1924237 16A (HC)
phoenix_contact connector MSTBVA_01x06_G_5.00mm
0
6
6
Connector_Phoenix_MSTB
PhoenixContact_MSTBVA_2,5_7-G-5,08_1x07_P5.08mm_Vertical
Generic Phoenix Contact connector footprint for: MSTBVA_2,5/7-G-5,08; number of pins: 07; pin pitch: 5.08mm; Vertical || order number: 1755781 12A || order number: 1924350 16A (HC)
phoenix_contact connector MSTBVA_01x07_G_5.08mm
0
7
7
Connector_Phoenix_MSTB
PhoenixContact_MSTBVA_2,5_7-G_1x07_P5.00mm_Vertical
Generic Phoenix Contact connector footprint for: MSTBVA_2,5/7-G; number of pins: 07; pin pitch: 5.00mm; Vertical || order number: 1755561 12A || order number: 1924240 16A (HC)
phoenix_contact connector MSTBVA_01x07_G_5.00mm
0
7
7
Connector_Phoenix_MSTB
PhoenixContact_MSTBVA_2,5_8-G-5,08_1x08_P5.08mm_Vertical
Generic Phoenix Contact connector footprint for: MSTBVA_2,5/8-G-5,08; number of pins: 08; pin pitch: 5.08mm; Vertical || order number: 1755794 12A || order number: 1924363 16A (HC)
phoenix_contact connector MSTBVA_01x08_G_5.08mm
0
8
8
Connector_Phoenix_MSTB
PhoenixContact_MSTBVA_2,5_8-G_1x08_P5.00mm_Vertical
Generic Phoenix Contact connector footprint for: MSTBVA_2,5/8-G; number of pins: 08; pin pitch: 5.00mm; Vertical || order number: 1755574 12A || order number: 1924253 16A (HC)
phoenix_contact connector MSTBVA_01x08_G_5.00mm
0
8
8
Connector_Phoenix_MSTB
PhoenixContact_MSTBVA_2,5_9-G-5,08_1x09_P5.08mm_Vertical
Generic Phoenix Contact connector footprint for: MSTBVA_2,5/9-G-5,08; number of pins: 09; pin pitch: 5.08mm; Vertical || order number: 1755804 12A || order number: 1924376 16A (HC)
phoenix_contact connector MSTBVA_01x09_G_5.08mm
0
9
9
Connector_Phoenix_MSTB
PhoenixContact_MSTBVA_2,5_9-G_1x09_P5.00mm_Vertical
Generic Phoenix Contact connector footprint for: MSTBVA_2,5/9-G; number of pins: 09; pin pitch: 5.00mm; Vertical || order number: 1755587 12A || order number: 1924266 16A (HC)
phoenix_contact connector MSTBVA_01x09_G_5.00mm
0
9
9
Connector_Phoenix_MSTB
PhoenixContact_MSTBVA_2,5_10-G-5,08_1x10_P5.08mm_Vertical
Generic Phoenix Contact connector footprint for: MSTBVA_2,5/10-G-5,08; number of pins: 10; pin pitch: 5.08mm; Vertical || order number: 1755817 12A || order number: 1924389 16A (HC)
phoenix_contact connector MSTBVA_01x10_G_5.08mm
0
10
10
Connector_Phoenix_MSTB
PhoenixContact_MSTBVA_2,5_10-G_1x10_P5.00mm_Vertical
Generic Phoenix Contact connector footprint for: MSTBVA_2,5/10-G; number of pins: 10; pin pitch: 5.00mm; Vertical || order number: 1755503 12A || order number: 1924279 16A (HC)
phoenix_contact connector MSTBVA_01x10_G_5.00mm
0
10
10
Connector_Phoenix_MSTB
PhoenixContact_MSTBVA_2,5_11-G-5,08_1x11_P5.08mm_Vertical
Generic Phoenix Contact connector footprint for: MSTBVA_2,5/11-G-5,08; number of pins: 11; pin pitch: 5.08mm; Vertical || order number: 1755820 12A || order number: 1924392 16A (HC)
phoenix_contact connector MSTBVA_01x11_G_5.08mm
0
11
11
Connector_Phoenix_MSTB
PhoenixContact_MSTBVA_2,5_11-G_1x11_P5.00mm_Vertical
Generic Phoenix Contact connector footprint for: MSTBVA_2,5/11-G; number of pins: 11; pin pitch: 5.00mm; Vertical || order number: 1755590 12A || order number: 1924282 16A (HC)
phoenix_contact connector MSTBVA_01x11_G_5.00mm
0
11
11
Connector_Phoenix_MSTB
PhoenixContact_MSTBVA_2,5_12-G-5,08_1x12_P5.08mm_Vertical
Generic Phoenix Contact connector footprint for: MSTBVA_2,5/12-G-5,08; number of pins: 12; pin pitch: 5.08mm; Vertical || order number: 1755833 12A || order number: 1924402 16A (HC)
phoenix_contact connector MSTBVA_01x12_G_5.08mm
0
12
12
Connector_Phoenix_MSTB
PhoenixContact_MSTBVA_2,5_12-G_1x12_P5.00mm_Vertical
Generic Phoenix Contact connector footprint for: MSTBVA_2,5/12-G; number of pins: 12; pin pitch: 5.00mm; Vertical || order number: 1755600 12A || order number: 1924295 16A (HC)
phoenix_contact connector MSTBVA_01x12_G_5.00mm
0
12
12
Connector_Phoenix_MSTB
PhoenixContact_MSTBVA_2,5_13-G-5,08_1x13_P5.08mm_Vertical
Generic Phoenix Contact connector footprint for: MSTBVA_2,5/13-G-5,08; number of pins: 13; pin pitch: 5.08mm; Vertical || order number: 1755846 12A
phoenix_contact connector MSTBVA_01x13_G_5.08mm
0
13
13
Connector_Phoenix_MSTB
PhoenixContact_MSTBVA_2,5_13-G_1x13_P5.00mm_Vertical
Generic Phoenix Contact connector footprint for: MSTBVA_2,5/13-G; number of pins: 13; pin pitch: 5.00mm; Vertical || order number: 1755613 12A
phoenix_contact connector MSTBVA_01x13_G_5.00mm
0
13
13
Connector_Phoenix_MSTB
PhoenixContact_MSTBVA_2,5_14-G-5,08_1x14_P5.08mm_Vertical
Generic Phoenix Contact connector footprint for: MSTBVA_2,5/14-G-5,08; number of pins: 14; pin pitch: 5.08mm; Vertical || order number: 1755859 12A
phoenix_contact connector MSTBVA_01x14_G_5.08mm
0
14
14
Connector_Phoenix_MSTB
PhoenixContact_MSTBVA_2,5_14-G_1x14_P5.00mm_Vertical
Generic Phoenix Contact connector footprint for: MSTBVA_2,5/14-G; number of pins: 14; pin pitch: 5.00mm; Vertical || order number: 1755626 12A
phoenix_contact connector MSTBVA_01x14_G_5.00mm
0
14
14
Connector_Phoenix_MSTB
PhoenixContact_MSTBVA_2,5_15-G-5,08_1x15_P5.08mm_Vertical
Generic Phoenix Contact connector footprint for: MSTBVA_2,5/15-G-5,08; number of pins: 15; pin pitch: 5.08mm; Vertical || order number: 1755862 12A
phoenix_contact connector MSTBVA_01x15_G_5.08mm
0
15
15
Connector_Phoenix_MSTB
PhoenixContact_MSTBVA_2,5_15-G_1x15_P5.00mm_Vertical
Generic Phoenix Contact connector footprint for: MSTBVA_2,5/15-G; number of pins: 15; pin pitch: 5.00mm; Vertical || order number: 1755639 12A
phoenix_contact connector MSTBVA_01x15_G_5.00mm
0
15
15
Connector_Phoenix_MSTB
PhoenixContact_MSTBVA_2,5_16-G-5,08_1x16_P5.08mm_Vertical
Generic Phoenix Contact connector footprint for: MSTBVA_2,5/16-G-5,08; number of pins: 16; pin pitch: 5.08mm; Vertical || order number: 1755875 12A
phoenix_contact connector MSTBVA_01x16_G_5.08mm
0
16
16
Connector_Phoenix_MSTB
PhoenixContact_MSTBVA_2,5_16-G_1x16_P5.00mm_Vertical
Generic Phoenix Contact connector footprint for: MSTBVA_2,5/16-G; number of pins: 16; pin pitch: 5.00mm; Vertical || order number: 1755642 12A
phoenix_contact connector MSTBVA_01x16_G_5.00mm
0
16
16
Connector_Phoenix_MSTB
PhoenixContact_MSTBV_2,5_2-GF-5,08_1x02_P5.08mm_Vertical_ThreadedFlange
Generic Phoenix Contact connector footprint for: MSTBV_2,5/2-GF-5,08; number of pins: 02; pin pitch: 5.08mm; Vertical; threaded flange || order number: 1777073 12A || order number: 1924525 16A (HC)
phoenix_contact connector MSTBV_01x02_GF_5.08mm
0
2
2
Connector_Phoenix_MSTB
PhoenixContact_MSTBV_2,5_2-GF-5,08_1x02_P5.08mm_Vertical_ThreadedFlange_MountHole
Generic Phoenix Contact connector footprint for: MSTBV_2,5/2-GF-5,08; number of pins: 02; pin pitch: 5.08mm; Vertical; threaded flange; footprint includes mount hole for mounting screw: ISO 1481-ST 2.2x6.5 C or ISO 7049-ST 2.2x6.5 C (http://www.fasteners.eu/standards/ISO/7049/) || order number: 1777073 12A || order number: 1924525 16A (HC)
phoenix_contact connector MSTBV_01x02_GF_5.08mm_MH
0
2
2
Connector_Phoenix_MSTB
PhoenixContact_MSTBV_2,5_2-GF_1x02_P5.00mm_Vertical_ThreadedFlange
Generic Phoenix Contact connector footprint for: MSTBV_2,5/2-GF; number of pins: 02; pin pitch: 5.00mm; Vertical; threaded flange || order number: 1776883 12A || order number: 1924415 16A (HC)
phoenix_contact connector MSTBV_01x02_GF_5.00mm
0
2
2
Connector_Phoenix_MSTB
PhoenixContact_MSTBV_2,5_2-GF_1x02_P5.00mm_Vertical_ThreadedFlange_MountHole
Generic Phoenix Contact connector footprint for: MSTBV_2,5/2-GF; number of pins: 02; pin pitch: 5.00mm; Vertical; threaded flange; footprint includes mount hole for mounting screw: ISO 1481-ST 2.2x6.5 C or ISO 7049-ST 2.2x6.5 C (http://www.fasteners.eu/standards/ISO/7049/) || order number: 1776883 12A || order number: 1924415 16A (HC)
phoenix_contact connector MSTBV_01x02_GF_5.00mm_MH
0
2
2
Connector_Phoenix_MSTB
PhoenixContact_MSTBV_2,5_3-GF-5,08_1x03_P5.08mm_Vertical_ThreadedFlange
Generic Phoenix Contact connector footprint for: MSTBV_2,5/3-GF-5,08; number of pins: 03; pin pitch: 5.08mm; Vertical; threaded flange || order number: 1777086 12A || order number: 1924538 16A (HC)
phoenix_contact connector MSTBV_01x03_GF_5.08mm
0
3
3
Connector_Phoenix_MSTB
PhoenixContact_MSTBV_2,5_3-GF-5,08_1x03_P5.08mm_Vertical_ThreadedFlange_MountHole
Generic Phoenix Contact connector footprint for: MSTBV_2,5/3-GF-5,08; number of pins: 03; pin pitch: 5.08mm; Vertical; threaded flange; footprint includes mount hole for mounting screw: ISO 1481-ST 2.2x6.5 C or ISO 7049-ST 2.2x6.5 C (http://www.fasteners.eu/standards/ISO/7049/) || order number: 1777086 12A || order number: 1924538 16A (HC)
phoenix_contact connector MSTBV_01x03_GF_5.08mm_MH
0
3
3
Connector_Phoenix_MSTB
PhoenixContact_MSTBV_2,5_3-GF_1x03_P5.00mm_Vertical_ThreadedFlange
Generic Phoenix Contact connector footprint for: MSTBV_2,5/3-GF; number of pins: 03; pin pitch: 5.00mm; Vertical; threaded flange || order number: 1776896 12A || order number: 1924428 16A (HC)
phoenix_contact connector MSTBV_01x03_GF_5.00mm
0
3
3
Connector_Phoenix_MSTB
PhoenixContact_MSTBV_2,5_3-GF_1x03_P5.00mm_Vertical_ThreadedFlange_MountHole
Generic Phoenix Contact connector footprint for: MSTBV_2,5/3-GF; number of pins: 03; pin pitch: 5.00mm; Vertical; threaded flange; footprint includes mount hole for mounting screw: ISO 1481-ST 2.2x6.5 C or ISO 7049-ST 2.2x6.5 C (http://www.fasteners.eu/standards/ISO/7049/) || order number: 1776896 12A || order number: 1924428 16A (HC)
phoenix_contact connector MSTBV_01x03_GF_5.00mm_MH
0
3
3
Connector_Phoenix_MSTB
PhoenixContact_MSTBV_2,5_4-GF-5,08_1x04_P5.08mm_Vertical_ThreadedFlange
Generic Phoenix Contact connector footprint for: MSTBV_2,5/4-GF-5,08; number of pins: 04; pin pitch: 5.08mm; Vertical; threaded flange || order number: 1777099 12A || order number: 1924541 16A (HC)
phoenix_contact connector MSTBV_01x04_GF_5.08mm
0
4
4
Connector_Phoenix_MSTB
PhoenixContact_MSTBV_2,5_4-GF-5,08_1x04_P5.08mm_Vertical_ThreadedFlange_MountHole
Generic Phoenix Contact connector footprint for: MSTBV_2,5/4-GF-5,08; number of pins: 04; pin pitch: 5.08mm; Vertical; threaded flange; footprint includes mount hole for mounting screw: ISO 1481-ST 2.2x6.5 C or ISO 7049-ST 2.2x6.5 C (http://www.fasteners.eu/standards/ISO/7049/) || order number: 1777099 12A || order number: 1924541 16A (HC)
phoenix_contact connector MSTBV_01x04_GF_5.08mm_MH
0
4
4
Connector_Phoenix_MSTB
PhoenixContact_MSTBV_2,5_4-GF_1x04_P5.00mm_Vertical_ThreadedFlange
Generic Phoenix Contact connector footprint for: MSTBV_2,5/4-GF; number of pins: 04; pin pitch: 5.00mm; Vertical; threaded flange || order number: 1776906 12A || order number: 1924431 16A (HC)
phoenix_contact connector MSTBV_01x04_GF_5.00mm
0
4
4
Connector_Phoenix_MSTB
PhoenixContact_MSTBV_2,5_4-GF_1x04_P5.00mm_Vertical_ThreadedFlange_MountHole
Generic Phoenix Contact connector footprint for: MSTBV_2,5/4-GF; number of pins: 04; pin pitch: 5.00mm; Vertical; threaded flange; footprint includes mount hole for mounting screw: ISO 1481-ST 2.2x6.5 C or ISO 7049-ST 2.2x6.5 C (http://www.fasteners.eu/standards/ISO/7049/) || order number: 1776906 12A || order number: 1924431 16A (HC)
phoenix_contact connector MSTBV_01x04_GF_5.00mm_MH
0
4
4
Connector_Phoenix_MSTB
PhoenixContact_MSTBV_2,5_5-GF-5,08_1x05_P5.08mm_Vertical_ThreadedFlange
Generic Phoenix Contact connector footprint for: MSTBV_2,5/5-GF-5,08; number of pins: 05; pin pitch: 5.08mm; Vertical; threaded flange || order number: 1777109 12A || order number: 1924554 16A (HC)
phoenix_contact connector MSTBV_01x05_GF_5.08mm
0
5
5
Connector_Phoenix_MSTB
PhoenixContact_MSTBV_2,5_5-GF-5,08_1x05_P5.08mm_Vertical_ThreadedFlange_MountHole
Generic Phoenix Contact connector footprint for: MSTBV_2,5/5-GF-5,08; number of pins: 05; pin pitch: 5.08mm; Vertical; threaded flange; footprint includes mount hole for mounting screw: ISO 1481-ST 2.2x6.5 C or ISO 7049-ST 2.2x6.5 C (http://www.fasteners.eu/standards/ISO/7049/) || order number: 1777109 12A || order number: 1924554 16A (HC)
phoenix_contact connector MSTBV_01x05_GF_5.08mm_MH
0
5
5
Connector_Phoenix_MSTB
PhoenixContact_MSTBV_2,5_5-GF_1x05_P5.00mm_Vertical_ThreadedFlange
Generic Phoenix Contact connector footprint for: MSTBV_2,5/5-GF; number of pins: 05; pin pitch: 5.00mm; Vertical; threaded flange || order number: 1776919 12A || order number: 1924444 16A (HC)
phoenix_contact connector MSTBV_01x05_GF_5.00mm
0
5
5
Connector_Phoenix_MSTB
PhoenixContact_MSTBV_2,5_5-GF_1x05_P5.00mm_Vertical_ThreadedFlange_MountHole
Generic Phoenix Contact connector footprint for: MSTBV_2,5/5-GF; number of pins: 05; pin pitch: 5.00mm; Vertical; threaded flange; footprint includes mount hole for mounting screw: ISO 1481-ST 2.2x6.5 C or ISO 7049-ST 2.2x6.5 C (http://www.fasteners.eu/standards/ISO/7049/) || order number: 1776919 12A || order number: 1924444 16A (HC)
phoenix_contact connector MSTBV_01x05_GF_5.00mm_MH
0
5
5
Connector_Phoenix_MSTB
PhoenixContact_MSTBV_2,5_6-GF-5,08_1x06_P5.08mm_Vertical_ThreadedFlange
Generic Phoenix Contact connector footprint for: MSTBV_2,5/6-GF-5,08; number of pins: 06; pin pitch: 5.08mm; Vertical; threaded flange || order number: 1777112 12A || order number: 1924567 16A (HC)
phoenix_contact connector MSTBV_01x06_GF_5.08mm
0
6
6
Connector_Phoenix_MSTB
PhoenixContact_MSTBV_2,5_6-GF-5,08_1x06_P5.08mm_Vertical_ThreadedFlange_MountHole
Generic Phoenix Contact connector footprint for: MSTBV_2,5/6-GF-5,08; number of pins: 06; pin pitch: 5.08mm; Vertical; threaded flange; footprint includes mount hole for mounting screw: ISO 1481-ST 2.2x6.5 C or ISO 7049-ST 2.2x6.5 C (http://www.fasteners.eu/standards/ISO/7049/) || order number: 1777112 12A || order number: 1924567 16A (HC)
phoenix_contact connector MSTBV_01x06_GF_5.08mm_MH
0
6
6
Connector_Phoenix_MSTB
PhoenixContact_MSTBV_2,5_6-GF_1x06_P5.00mm_Vertical_ThreadedFlange
Generic Phoenix Contact connector footprint for: MSTBV_2,5/6-GF; number of pins: 06; pin pitch: 5.00mm; Vertical; threaded flange || order number: 1776922 12A || order number: 1924457 16A (HC)
phoenix_contact connector MSTBV_01x06_GF_5.00mm
0
6
6
Connector_Phoenix_MSTB
PhoenixContact_MSTBV_2,5_6-GF_1x06_P5.00mm_Vertical_ThreadedFlange_MountHole
Generic Phoenix Contact connector footprint for: MSTBV_2,5/6-GF; number of pins: 06; pin pitch: 5.00mm; Vertical; threaded flange; footprint includes mount hole for mounting screw: ISO 1481-ST 2.2x6.5 C or ISO 7049-ST 2.2x6.5 C (http://www.fasteners.eu/standards/ISO/7049/) || order number: 1776922 12A || order number: 1924457 16A (HC)
phoenix_contact connector MSTBV_01x06_GF_5.00mm_MH
0
6
6
Connector_Phoenix_MSTB
PhoenixContact_MSTBV_2,5_7-GF-5,08_1x07_P5.08mm_Vertical_ThreadedFlange
Generic Phoenix Contact connector footprint for: MSTBV_2,5/7-GF-5,08; number of pins: 07; pin pitch: 5.08mm; Vertical; threaded flange || order number: 1777125 12A || order number: 1924570 16A (HC)
phoenix_contact connector MSTBV_01x07_GF_5.08mm
0
7
7
Connector_Phoenix_MSTB
PhoenixContact_MSTBV_2,5_7-GF-5,08_1x07_P5.08mm_Vertical_ThreadedFlange_MountHole
Generic Phoenix Contact connector footprint for: MSTBV_2,5/7-GF-5,08; number of pins: 07; pin pitch: 5.08mm; Vertical; threaded flange; footprint includes mount hole for mounting screw: ISO 1481-ST 2.2x6.5 C or ISO 7049-ST 2.2x6.5 C (http://www.fasteners.eu/standards/ISO/7049/) || order number: 1777125 12A || order number: 1924570 16A (HC)
phoenix_contact connector MSTBV_01x07_GF_5.08mm_MH
0
7
7
Connector_Phoenix_MSTB
PhoenixContact_MSTBV_2,5_7-GF_1x07_P5.00mm_Vertical_ThreadedFlange
Generic Phoenix Contact connector footprint for: MSTBV_2,5/7-GF; number of pins: 07; pin pitch: 5.00mm; Vertical; threaded flange || order number: 1776935 12A || order number: 1924460 16A (HC)
phoenix_contact connector MSTBV_01x07_GF_5.00mm
0
7
7
Connector_Phoenix_MSTB
PhoenixContact_MSTBV_2,5_7-GF_1x07_P5.00mm_Vertical_ThreadedFlange_MountHole
Generic Phoenix Contact connector footprint for: MSTBV_2,5/7-GF; number of pins: 07; pin pitch: 5.00mm; Vertical; threaded flange; footprint includes mount hole for mounting screw: ISO 1481-ST 2.2x6.5 C or ISO 7049-ST 2.2x6.5 C (http://www.fasteners.eu/standards/ISO/7049/) || order number: 1776935 12A || order number: 1924460 16A (HC)
phoenix_contact connector MSTBV_01x07_GF_5.00mm_MH
0
7
7
Connector_Phoenix_MSTB
PhoenixContact_MSTBV_2,5_8-GF-5,08_1x08_P5.08mm_Vertical_ThreadedFlange
Generic Phoenix Contact connector footprint for: MSTBV_2,5/8-GF-5,08; number of pins: 08; pin pitch: 5.08mm; Vertical; threaded flange || order number: 1777138 12A || order number: 1924583 16A (HC)
phoenix_contact connector MSTBV_01x08_GF_5.08mm
0
8
8
Connector_Phoenix_MSTB
PhoenixContact_MSTBV_2,5_8-GF-5,08_1x08_P5.08mm_Vertical_ThreadedFlange_MountHole
Generic Phoenix Contact connector footprint for: MSTBV_2,5/8-GF-5,08; number of pins: 08; pin pitch: 5.08mm; Vertical; threaded flange; footprint includes mount hole for mounting screw: ISO 1481-ST 2.2x6.5 C or ISO 7049-ST 2.2x6.5 C (http://www.fasteners.eu/standards/ISO/7049/) || order number: 1777138 12A || order number: 1924583 16A (HC)
phoenix_contact connector MSTBV_01x08_GF_5.08mm_MH
0
8
8
Connector_Phoenix_MSTB
PhoenixContact_MSTBV_2,5_8-GF_1x08_P5.00mm_Vertical_ThreadedFlange
Generic Phoenix Contact connector footprint for: MSTBV_2,5/8-GF; number of pins: 08; pin pitch: 5.00mm; Vertical; threaded flange || order number: 1776948 12A || order number: 1924473 16A (HC)
phoenix_contact connector MSTBV_01x08_GF_5.00mm
0
8
8
Connector_Phoenix_MSTB
PhoenixContact_MSTBV_2,5_8-GF_1x08_P5.00mm_Vertical_ThreadedFlange_MountHole
Generic Phoenix Contact connector footprint for: MSTBV_2,5/8-GF; number of pins: 08; pin pitch: 5.00mm; Vertical; threaded flange; footprint includes mount hole for mounting screw: ISO 1481-ST 2.2x6.5 C or ISO 7049-ST 2.2x6.5 C (http://www.fasteners.eu/standards/ISO/7049/) || order number: 1776948 12A || order number: 1924473 16A (HC)
phoenix_contact connector MSTBV_01x08_GF_5.00mm_MH
0
8
8
Connector_Phoenix_MSTB
PhoenixContact_MSTBV_2,5_9-GF-5,08_1x09_P5.08mm_Vertical_ThreadedFlange
Generic Phoenix Contact connector footprint for: MSTBV_2,5/9-GF-5,08; number of pins: 09; pin pitch: 5.08mm; Vertical; threaded flange || order number: 1777141 12A || order number: 1924596 16A (HC)
phoenix_contact connector MSTBV_01x09_GF_5.08mm
0
9
9
Connector_Phoenix_MSTB
PhoenixContact_MSTBV_2,5_9-GF-5,08_1x09_P5.08mm_Vertical_ThreadedFlange_MountHole
Generic Phoenix Contact connector footprint for: MSTBV_2,5/9-GF-5,08; number of pins: 09; pin pitch: 5.08mm; Vertical; threaded flange; footprint includes mount hole for mounting screw: ISO 1481-ST 2.2x6.5 C or ISO 7049-ST 2.2x6.5 C (http://www.fasteners.eu/standards/ISO/7049/) || order number: 1777141 12A || order number: 1924596 16A (HC)
phoenix_contact connector MSTBV_01x09_GF_5.08mm_MH
0
9
9
Connector_Phoenix_MSTB
PhoenixContact_MSTBV_2,5_9-GF_1x09_P5.00mm_Vertical_ThreadedFlange
Generic Phoenix Contact connector footprint for: MSTBV_2,5/9-GF; number of pins: 09; pin pitch: 5.00mm; Vertical; threaded flange || order number: 1776951 12A || order number: 1924486 16A (HC)
phoenix_contact connector MSTBV_01x09_GF_5.00mm
0
9
9
Connector_Phoenix_MSTB
PhoenixContact_MSTBV_2,5_9-GF_1x09_P5.00mm_Vertical_ThreadedFlange_MountHole
Generic Phoenix Contact connector footprint for: MSTBV_2,5/9-GF; number of pins: 09; pin pitch: 5.00mm; Vertical; threaded flange; footprint includes mount hole for mounting screw: ISO 1481-ST 2.2x6.5 C or ISO 7049-ST 2.2x6.5 C (http://www.fasteners.eu/standards/ISO/7049/) || order number: 1776951 12A || order number: 1924486 16A (HC)
phoenix_contact connector MSTBV_01x09_GF_5.00mm_MH
0
9
9
Connector_Phoenix_MSTB
PhoenixContact_MSTBV_2,5_10-GF-5,08_1x10_P5.08mm_Vertical_ThreadedFlange
Generic Phoenix Contact connector footprint for: MSTBV_2,5/10-GF-5,08; number of pins: 10; pin pitch: 5.08mm; Vertical; threaded flange || order number: 1777154 12A || order number: 1924606 16A (HC)
phoenix_contact connector MSTBV_01x10_GF_5.08mm
0
10
10
Connector_Phoenix_MSTB
PhoenixContact_MSTBV_2,5_10-GF-5,08_1x10_P5.08mm_Vertical_ThreadedFlange_MountHole
Generic Phoenix Contact connector footprint for: MSTBV_2,5/10-GF-5,08; number of pins: 10; pin pitch: 5.08mm; Vertical; threaded flange; footprint includes mount hole for mounting screw: ISO 1481-ST 2.2x6.5 C or ISO 7049-ST 2.2x6.5 C (http://www.fasteners.eu/standards/ISO/7049/) || order number: 1777154 12A || order number: 1924606 16A (HC)
phoenix_contact connector MSTBV_01x10_GF_5.08mm_MH
0
10
10
Connector_Phoenix_MSTB
PhoenixContact_MSTBV_2,5_10-GF_1x10_P5.00mm_Vertical_ThreadedFlange
Generic Phoenix Contact connector footprint for: MSTBV_2,5/10-GF; number of pins: 10; pin pitch: 5.00mm; Vertical; threaded flange || order number: 1776964 12A || order number: 1924499 16A (HC)
phoenix_contact connector MSTBV_01x10_GF_5.00mm
0
10
10
Connector_Phoenix_MSTB
PhoenixContact_MSTBV_2,5_10-GF_1x10_P5.00mm_Vertical_ThreadedFlange_MountHole
Generic Phoenix Contact connector footprint for: MSTBV_2,5/10-GF; number of pins: 10; pin pitch: 5.00mm; Vertical; threaded flange; footprint includes mount hole for mounting screw: ISO 1481-ST 2.2x6.5 C or ISO 7049-ST 2.2x6.5 C (http://www.fasteners.eu/standards/ISO/7049/) || order number: 1776964 12A || order number: 1924499 16A (HC)
phoenix_contact connector MSTBV_01x10_GF_5.00mm_MH
0
10
10
Connector_Phoenix_MSTB
PhoenixContact_MSTBV_2,5_11-GF-5,08_1x11_P5.08mm_Vertical_ThreadedFlange
Generic Phoenix Contact connector footprint for: MSTBV_2,5/11-GF-5,08; number of pins: 11; pin pitch: 5.08mm; Vertical; threaded flange || order number: 1777167 12A || order number: 1924619 16A (HC)
phoenix_contact connector MSTBV_01x11_GF_5.08mm
0
11
11
Connector_Phoenix_MSTB
PhoenixContact_MSTBV_2,5_11-GF-5,08_1x11_P5.08mm_Vertical_ThreadedFlange_MountHole
Generic Phoenix Contact connector footprint for: MSTBV_2,5/11-GF-5,08; number of pins: 11; pin pitch: 5.08mm; Vertical; threaded flange; footprint includes mount hole for mounting screw: ISO 1481-ST 2.2x6.5 C or ISO 7049-ST 2.2x6.5 C (http://www.fasteners.eu/standards/ISO/7049/) || order number: 1777167 12A || order number: 1924619 16A (HC)
phoenix_contact connector MSTBV_01x11_GF_5.08mm_MH
0
11
11
Connector_Phoenix_MSTB
PhoenixContact_MSTBV_2,5_11-GF_1x11_P5.00mm_Vertical_ThreadedFlange
Generic Phoenix Contact connector footprint for: MSTBV_2,5/11-GF; number of pins: 11; pin pitch: 5.00mm; Vertical; threaded flange || order number: 1776977 12A || order number: 1924509 16A (HC)
phoenix_contact connector MSTBV_01x11_GF_5.00mm
0
11
11
Connector_Phoenix_MSTB
PhoenixContact_MSTBV_2,5_11-GF_1x11_P5.00mm_Vertical_ThreadedFlange_MountHole
Generic Phoenix Contact connector footprint for: MSTBV_2,5/11-GF; number of pins: 11; pin pitch: 5.00mm; Vertical; threaded flange; footprint includes mount hole for mounting screw: ISO 1481-ST 2.2x6.5 C or ISO 7049-ST 2.2x6.5 C (http://www.fasteners.eu/standards/ISO/7049/) || order number: 1776977 12A || order number: 1924509 16A (HC)
phoenix_contact connector MSTBV_01x11_GF_5.00mm_MH
0
11
11
Connector_Phoenix_MSTB
PhoenixContact_MSTBV_2,5_12-GF-5,08_1x12_P5.08mm_Vertical_ThreadedFlange
Generic Phoenix Contact connector footprint for: MSTBV_2,5/12-GF-5,08; number of pins: 12; pin pitch: 5.08mm; Vertical; threaded flange || order number: 1777170 12A || order number: 1924622 16A (HC)
phoenix_contact connector MSTBV_01x12_GF_5.08mm
0
12
12
Connector_Phoenix_MSTB
PhoenixContact_MSTBV_2,5_12-GF-5,08_1x12_P5.08mm_Vertical_ThreadedFlange_MountHole
Generic Phoenix Contact connector footprint for: MSTBV_2,5/12-GF-5,08; number of pins: 12; pin pitch: 5.08mm; Vertical; threaded flange; footprint includes mount hole for mounting screw: ISO 1481-ST 2.2x6.5 C or ISO 7049-ST 2.2x6.5 C (http://www.fasteners.eu/standards/ISO/7049/) || order number: 1777170 12A || order number: 1924622 16A (HC)
phoenix_contact connector MSTBV_01x12_GF_5.08mm_MH
0
12
12
Connector_Phoenix_MSTB
PhoenixContact_MSTBV_2,5_12-GF_1x12_P5.00mm_Vertical_ThreadedFlange
Generic Phoenix Contact connector footprint for: MSTBV_2,5/12-GF; number of pins: 12; pin pitch: 5.00mm; Vertical; threaded flange || order number: 1776980 12A || order number: 1924512 16A (HC)
phoenix_contact connector MSTBV_01x12_GF_5.00mm
0
12
12
Connector_Phoenix_MSTB
PhoenixContact_MSTBV_2,5_12-GF_1x12_P5.00mm_Vertical_ThreadedFlange_MountHole
Generic Phoenix Contact connector footprint for: MSTBV_2,5/12-GF; number of pins: 12; pin pitch: 5.00mm; Vertical; threaded flange; footprint includes mount hole for mounting screw: ISO 1481-ST 2.2x6.5 C or ISO 7049-ST 2.2x6.5 C (http://www.fasteners.eu/standards/ISO/7049/) || order number: 1776980 12A || order number: 1924512 16A (HC)
phoenix_contact connector MSTBV_01x12_GF_5.00mm_MH
0
12
12
Connector_Phoenix_MSTB
PhoenixContact_MSTBV_2,5_13-GF-5,08_1x13_P5.08mm_Vertical_ThreadedFlange
Generic Phoenix Contact connector footprint for: MSTBV_2,5/13-GF-5,08; number of pins: 13; pin pitch: 5.08mm; Vertical; threaded flange || order number: 1777183 12A
phoenix_contact connector MSTBV_01x13_GF_5.08mm
0
13
13
Connector_Phoenix_MSTB
PhoenixContact_MSTBV_2,5_13-GF-5,08_1x13_P5.08mm_Vertical_ThreadedFlange_MountHole
Generic Phoenix Contact connector footprint for: MSTBV_2,5/13-GF-5,08; number of pins: 13; pin pitch: 5.08mm; Vertical; threaded flange; footprint includes mount hole for mounting screw: ISO 1481-ST 2.2x6.5 C or ISO 7049-ST 2.2x6.5 C (http://www.fasteners.eu/standards/ISO/7049/) || order number: 1777183 12A
phoenix_contact connector MSTBV_01x13_GF_5.08mm_MH
0
13
13
Connector_Phoenix_MSTB
PhoenixContact_MSTBV_2,5_13-GF_1x13_P5.00mm_Vertical_ThreadedFlange
Generic Phoenix Contact connector footprint for: MSTBV_2,5/13-GF; number of pins: 13; pin pitch: 5.00mm; Vertical; threaded flange || order number: 1776993 12A
phoenix_contact connector MSTBV_01x13_GF_5.00mm
0
13
13
Connector_Phoenix_MSTB
PhoenixContact_MSTBV_2,5_13-GF_1x13_P5.00mm_Vertical_ThreadedFlange_MountHole
Generic Phoenix Contact connector footprint for: MSTBV_2,5/13-GF; number of pins: 13; pin pitch: 5.00mm; Vertical; threaded flange; footprint includes mount hole for mounting screw: ISO 1481-ST 2.2x6.5 C or ISO 7049-ST 2.2x6.5 C (http://www.fasteners.eu/standards/ISO/7049/) || order number: 1776993 12A
phoenix_contact connector MSTBV_01x13_GF_5.00mm_MH
0
13
13
Connector_Phoenix_MSTB
PhoenixContact_MSTBV_2,5_14-GF-5,08_1x14_P5.08mm_Vertical_ThreadedFlange
Generic Phoenix Contact connector footprint for: MSTBV_2,5/14-GF-5,08; number of pins: 14; pin pitch: 5.08mm; Vertical; threaded flange || order number: 1777196 12A
phoenix_contact connector MSTBV_01x14_GF_5.08mm
0
14
14
Connector_Phoenix_MSTB
PhoenixContact_MSTBV_2,5_14-GF-5,08_1x14_P5.08mm_Vertical_ThreadedFlange_MountHole
Generic Phoenix Contact connector footprint for: MSTBV_2,5/14-GF-5,08; number of pins: 14; pin pitch: 5.08mm; Vertical; threaded flange; footprint includes mount hole for mounting screw: ISO 1481-ST 2.2x6.5 C or ISO 7049-ST 2.2x6.5 C (http://www.fasteners.eu/standards/ISO/7049/) || order number: 1777196 12A
phoenix_contact connector MSTBV_01x14_GF_5.08mm_MH
0
14
14
Connector_Phoenix_MSTB
PhoenixContact_MSTBV_2,5_14-GF_1x14_P5.00mm_Vertical_ThreadedFlange
Generic Phoenix Contact connector footprint for: MSTBV_2,5/14-GF; number of pins: 14; pin pitch: 5.00mm; Vertical; threaded flange || order number: 1776002 12A
phoenix_contact connector MSTBV_01x14_GF_5.00mm
0
14
14
Connector_Phoenix_MSTB
PhoenixContact_MSTBV_2,5_14-GF_1x14_P5.00mm_Vertical_ThreadedFlange_MountHole
Generic Phoenix Contact connector footprint for: MSTBV_2,5/14-GF; number of pins: 14; pin pitch: 5.00mm; Vertical; threaded flange; footprint includes mount hole for mounting screw: ISO 1481-ST 2.2x6.5 C or ISO 7049-ST 2.2x6.5 C (http://www.fasteners.eu/standards/ISO/7049/) || order number: 1776002 12A
phoenix_contact connector MSTBV_01x14_GF_5.00mm_MH
0
14
14
Connector_Phoenix_MSTB
PhoenixContact_MSTBV_2,5_15-GF-5,08_1x15_P5.08mm_Vertical_ThreadedFlange
Generic Phoenix Contact connector footprint for: MSTBV_2,5/15-GF-5,08; number of pins: 15; pin pitch: 5.08mm; Vertical; threaded flange || order number: 1777206 12A
phoenix_contact connector MSTBV_01x15_GF_5.08mm
0
15
15
Connector_Phoenix_MSTB
PhoenixContact_MSTBV_2,5_15-GF-5,08_1x15_P5.08mm_Vertical_ThreadedFlange_MountHole
Generic Phoenix Contact connector footprint for: MSTBV_2,5/15-GF-5,08; number of pins: 15; pin pitch: 5.08mm; Vertical; threaded flange; footprint includes mount hole for mounting screw: ISO 1481-ST 2.2x6.5 C or ISO 7049-ST 2.2x6.5 C (http://www.fasteners.eu/standards/ISO/7049/) || order number: 1777206 12A
phoenix_contact connector MSTBV_01x15_GF_5.08mm_MH
0
15
15
Connector_Phoenix_MSTB
PhoenixContact_MSTBV_2,5_15-GF_1x15_P5.00mm_Vertical_ThreadedFlange
Generic Phoenix Contact connector footprint for: MSTBV_2,5/15-GF; number of pins: 15; pin pitch: 5.00mm; Vertical; threaded flange || order number: 1776015 12A
phoenix_contact connector MSTBV_01x15_GF_5.00mm
0
15
15
Connector_Phoenix_MSTB
PhoenixContact_MSTBV_2,5_15-GF_1x15_P5.00mm_Vertical_ThreadedFlange_MountHole
Generic Phoenix Contact connector footprint for: MSTBV_2,5/15-GF; number of pins: 15; pin pitch: 5.00mm; Vertical; threaded flange; footprint includes mount hole for mounting screw: ISO 1481-ST 2.2x6.5 C or ISO 7049-ST 2.2x6.5 C (http://www.fasteners.eu/standards/ISO/7049/) || order number: 1776015 12A
phoenix_contact connector MSTBV_01x15_GF_5.00mm_MH
0
15
15
Connector_Phoenix_MSTB
PhoenixContact_MSTBV_2,5_16-GF-5,08_1x16_P5.08mm_Vertical_ThreadedFlange
Generic Phoenix Contact connector footprint for: MSTBV_2,5/16-GF-5,08; number of pins: 16; pin pitch: 5.08mm; Vertical; threaded flange || order number: 1777219 12A
phoenix_contact connector MSTBV_01x16_GF_5.08mm
0
16
16
Connector_Phoenix_MSTB
PhoenixContact_MSTBV_2,5_16-GF-5,08_1x16_P5.08mm_Vertical_ThreadedFlange_MountHole
Generic Phoenix Contact connector footprint for: MSTBV_2,5/16-GF-5,08; number of pins: 16; pin pitch: 5.08mm; Vertical; threaded flange; footprint includes mount hole for mounting screw: ISO 1481-ST 2.2x6.5 C or ISO 7049-ST 2.2x6.5 C (http://www.fasteners.eu/standards/ISO/7049/) || order number: 1777219 12A
phoenix_contact connector MSTBV_01x16_GF_5.08mm_MH
0
16
16
Connector_Phoenix_MSTB
PhoenixContact_MSTBV_2,5_16-GF_1x16_P5.00mm_Vertical_ThreadedFlange
Generic Phoenix Contact connector footprint for: MSTBV_2,5/16-GF; number of pins: 16; pin pitch: 5.00mm; Vertical; threaded flange || order number: 1776028 12A
phoenix_contact connector MSTBV_01x16_GF_5.00mm
0
16
16
Connector_Phoenix_MSTB
PhoenixContact_MSTBV_2,5_16-GF_1x16_P5.00mm_Vertical_ThreadedFlange_MountHole
Generic Phoenix Contact connector footprint for: MSTBV_2,5/16-GF; number of pins: 16; pin pitch: 5.00mm; Vertical; threaded flange; footprint includes mount hole for mounting screw: ISO 1481-ST 2.2x6.5 C or ISO 7049-ST 2.2x6.5 C (http://www.fasteners.eu/standards/ISO/7049/) || order number: 1776028 12A
phoenix_contact connector MSTBV_01x16_GF_5.00mm_MH
0
16
16
Connector_Phoenix_MSTB
PhoenixContact_MSTB_2,5_2-GF-5,08_1x02_P5.08mm_Horizontal_ThreadedFlange
Generic Phoenix Contact connector footprint for: MSTB_2,5/2-GF-5,08; number of pins: 02; pin pitch: 5.08mm; Angled; threaded flange || order number: 1776508 12A || order number: 1924088 16A (HC)
phoenix_contact connector MSTB_01x02_GF_5.08mm
0
2
2
Connector_Phoenix_MSTB
PhoenixContact_MSTB_2,5_2-GF-5,08_1x02_P5.08mm_Horizontal_ThreadedFlange_MountHole
Generic Phoenix Contact connector footprint for: MSTB_2,5/2-GF-5,08; number of pins: 02; pin pitch: 5.08mm; Angled; threaded flange; footprint includes mount hole for mounting screw: ISO 1481-ST 2.2x6.5 C or ISO 7049-ST 2.2x6.5 C (http://www.fasteners.eu/standards/ISO/7049/) || order number: 1776508 12A || order number: 1924088 16A (HC)
phoenix_contact connector MSTB_01x02_GF_5.08mm_MH
0
2
2
Connector_Phoenix_MSTB
PhoenixContact_MSTB_2,5_2-GF_1x02_P5.00mm_Horizontal_ThreadedFlange
Generic Phoenix Contact connector footprint for: MSTB_2,5/2-GF; number of pins: 02; pin pitch: 5.00mm; Angled; threaded flange || order number: 1776692 12A || order number: 1923979 16A (HC)
phoenix_contact connector MSTB_01x02_GF_5.00mm
0
2
2
Connector_Phoenix_MSTB
PhoenixContact_MSTB_2,5_2-GF_1x02_P5.00mm_Horizontal_ThreadedFlange_MountHole
Generic Phoenix Contact connector footprint for: MSTB_2,5/2-GF; number of pins: 02; pin pitch: 5.00mm; Angled; threaded flange; footprint includes mount hole for mounting screw: ISO 1481-ST 2.2x6.5 C or ISO 7049-ST 2.2x6.5 C (http://www.fasteners.eu/standards/ISO/7049/) || order number: 1776692 12A || order number: 1923979 16A (HC)
phoenix_contact connector MSTB_01x02_GF_5.00mm_MH
0
2
2
Connector_Phoenix_MSTB
PhoenixContact_MSTB_2,5_3-GF-5,08_1x03_P5.08mm_Horizontal_ThreadedFlange
Generic Phoenix Contact connector footprint for: MSTB_2,5/3-GF-5,08; number of pins: 03; pin pitch: 5.08mm; Angled; threaded flange || order number: 1776511 12A || order number: 1924091 16A (HC)
phoenix_contact connector MSTB_01x03_GF_5.08mm
0
3
3
Connector_Phoenix_MSTB
PhoenixContact_MSTB_2,5_3-GF-5,08_1x03_P5.08mm_Horizontal_ThreadedFlange_MountHole
Generic Phoenix Contact connector footprint for: MSTB_2,5/3-GF-5,08; number of pins: 03; pin pitch: 5.08mm; Angled; threaded flange; footprint includes mount hole for mounting screw: ISO 1481-ST 2.2x6.5 C or ISO 7049-ST 2.2x6.5 C (http://www.fasteners.eu/standards/ISO/7049/) || order number: 1776511 12A || order number: 1924091 16A (HC)
phoenix_contact connector MSTB_01x03_GF_5.08mm_MH
0
3
3
Connector_Phoenix_MSTB
PhoenixContact_MSTB_2,5_3-GF_1x03_P5.00mm_Horizontal_ThreadedFlange
Generic Phoenix Contact connector footprint for: MSTB_2,5/3-GF; number of pins: 03; pin pitch: 5.00mm; Angled; threaded flange || order number: 1776702 12A || order number: 1923982 16A (HC)
phoenix_contact connector MSTB_01x03_GF_5.00mm
0
3
3
Connector_Phoenix_MSTB
PhoenixContact_MSTB_2,5_3-GF_1x03_P5.00mm_Horizontal_ThreadedFlange_MountHole
Generic Phoenix Contact connector footprint for: MSTB_2,5/3-GF; number of pins: 03; pin pitch: 5.00mm; Angled; threaded flange; footprint includes mount hole for mounting screw: ISO 1481-ST 2.2x6.5 C or ISO 7049-ST 2.2x6.5 C (http://www.fasteners.eu/standards/ISO/7049/) || order number: 1776702 12A || order number: 1923982 16A (HC)
phoenix_contact connector MSTB_01x03_GF_5.00mm_MH
0
3
3
Connector_Phoenix_MSTB
PhoenixContact_MSTB_2,5_4-GF-5,08_1x04_P5.08mm_Horizontal_ThreadedFlange
Generic Phoenix Contact connector footprint for: MSTB_2,5/4-GF-5,08; number of pins: 04; pin pitch: 5.08mm; Angled; threaded flange || order number: 1776524 12A || order number: 1924101 16A (HC)
phoenix_contact connector MSTB_01x04_GF_5.08mm
0
4
4
Connector_Phoenix_MSTB
PhoenixContact_MSTB_2,5_4-GF-5,08_1x04_P5.08mm_Horizontal_ThreadedFlange_MountHole
Generic Phoenix Contact connector footprint for: MSTB_2,5/4-GF-5,08; number of pins: 04; pin pitch: 5.08mm; Angled; threaded flange; footprint includes mount hole for mounting screw: ISO 1481-ST 2.2x6.5 C or ISO 7049-ST 2.2x6.5 C (http://www.fasteners.eu/standards/ISO/7049/) || order number: 1776524 12A || order number: 1924101 16A (HC)
phoenix_contact connector MSTB_01x04_GF_5.08mm_MH
0
4
4
Connector_Phoenix_MSTB
PhoenixContact_MSTB_2,5_4-GF_1x04_P5.00mm_Horizontal_ThreadedFlange
Generic Phoenix Contact connector footprint for: MSTB_2,5/4-GF; number of pins: 04; pin pitch: 5.00mm; Angled; threaded flange || order number: 1776715 12A || order number: 1923995 16A (HC)
phoenix_contact connector MSTB_01x04_GF_5.00mm
0
4
4
Connector_Phoenix_MSTB
PhoenixContact_MSTB_2,5_4-GF_1x04_P5.00mm_Horizontal_ThreadedFlange_MountHole
Generic Phoenix Contact connector footprint for: MSTB_2,5/4-GF; number of pins: 04; pin pitch: 5.00mm; Angled; threaded flange; footprint includes mount hole for mounting screw: ISO 1481-ST 2.2x6.5 C or ISO 7049-ST 2.2x6.5 C (http://www.fasteners.eu/standards/ISO/7049/) || order number: 1776715 12A || order number: 1923995 16A (HC)
phoenix_contact connector MSTB_01x04_GF_5.00mm_MH
0
4
4
Connector_Phoenix_MSTB
PhoenixContact_MSTB_2,5_5-GF-5,08_1x05_P5.08mm_Horizontal_ThreadedFlange
Generic Phoenix Contact connector footprint for: MSTB_2,5/5-GF-5,08; number of pins: 05; pin pitch: 5.08mm; Angled; threaded flange || order number: 1776537 12A || order number: 1924114 16A (HC)
phoenix_contact connector MSTB_01x05_GF_5.08mm
0
5
5
Connector_Phoenix_MSTB
PhoenixContact_MSTB_2,5_5-GF-5,08_1x05_P5.08mm_Horizontal_ThreadedFlange_MountHole
Generic Phoenix Contact connector footprint for: MSTB_2,5/5-GF-5,08; number of pins: 05; pin pitch: 5.08mm; Angled; threaded flange; footprint includes mount hole for mounting screw: ISO 1481-ST 2.2x6.5 C or ISO 7049-ST 2.2x6.5 C (http://www.fasteners.eu/standards/ISO/7049/) || order number: 1776537 12A || order number: 1924114 16A (HC)
phoenix_contact connector MSTB_01x05_GF_5.08mm_MH
0
5
5
Connector_Phoenix_MSTB
PhoenixContact_MSTB_2,5_5-GF_1x05_P5.00mm_Horizontal_ThreadedFlange
Generic Phoenix Contact connector footprint for: MSTB_2,5/5-GF; number of pins: 05; pin pitch: 5.00mm; Angled; threaded flange || order number: 1776728 12A || order number: 1924004 16A (HC)
phoenix_contact connector MSTB_01x05_GF_5.00mm
0
5
5
Connector_Phoenix_MSTB
PhoenixContact_MSTB_2,5_5-GF_1x05_P5.00mm_Horizontal_ThreadedFlange_MountHole
Generic Phoenix Contact connector footprint for: MSTB_2,5/5-GF; number of pins: 05; pin pitch: 5.00mm; Angled; threaded flange; footprint includes mount hole for mounting screw: ISO 1481-ST 2.2x6.5 C or ISO 7049-ST 2.2x6.5 C (http://www.fasteners.eu/standards/ISO/7049/) || order number: 1776728 12A || order number: 1924004 16A (HC)
phoenix_contact connector MSTB_01x05_GF_5.00mm_MH
0
5
5
Connector_Phoenix_MSTB
PhoenixContact_MSTB_2,5_6-GF-5,08_1x06_P5.08mm_Horizontal_ThreadedFlange
Generic Phoenix Contact connector footprint for: MSTB_2,5/6-GF-5,08; number of pins: 06; pin pitch: 5.08mm; Angled; threaded flange || order number: 1776540 12A || order number: 1924127 16A (HC)
phoenix_contact connector MSTB_01x06_GF_5.08mm
0
6
6
Connector_Phoenix_MSTB
PhoenixContact_MSTB_2,5_6-GF-5,08_1x06_P5.08mm_Horizontal_ThreadedFlange_MountHole
Generic Phoenix Contact connector footprint for: MSTB_2,5/6-GF-5,08; number of pins: 06; pin pitch: 5.08mm; Angled; threaded flange; footprint includes mount hole for mounting screw: ISO 1481-ST 2.2x6.5 C or ISO 7049-ST 2.2x6.5 C (http://www.fasteners.eu/standards/ISO/7049/) || order number: 1776540 12A || order number: 1924127 16A (HC)
phoenix_contact connector MSTB_01x06_GF_5.08mm_MH
0
6
6
Connector_Phoenix_MSTB
PhoenixContact_MSTB_2,5_6-GF_1x06_P5.00mm_Horizontal_ThreadedFlange
Generic Phoenix Contact connector footprint for: MSTB_2,5/6-GF; number of pins: 06; pin pitch: 5.00mm; Angled; threaded flange || order number: 1776731 12A || order number: 1924017 16A (HC)
phoenix_contact connector MSTB_01x06_GF_5.00mm
0
6
6
Connector_Phoenix_MSTB
PhoenixContact_MSTB_2,5_6-GF_1x06_P5.00mm_Horizontal_ThreadedFlange_MountHole
Generic Phoenix Contact connector footprint for: MSTB_2,5/6-GF; number of pins: 06; pin pitch: 5.00mm; Angled; threaded flange; footprint includes mount hole for mounting screw: ISO 1481-ST 2.2x6.5 C or ISO 7049-ST 2.2x6.5 C (http://www.fasteners.eu/standards/ISO/7049/) || order number: 1776731 12A || order number: 1924017 16A (HC)
phoenix_contact connector MSTB_01x06_GF_5.00mm_MH
0
6
6
Connector_Phoenix_MSTB
PhoenixContact_MSTB_2,5_7-GF-5,08_1x07_P5.08mm_Horizontal_ThreadedFlange
Generic Phoenix Contact connector footprint for: MSTB_2,5/7-GF-5,08; number of pins: 07; pin pitch: 5.08mm; Angled; threaded flange || order number: 1776553 12A || order number: 1924130 16A (HC)
phoenix_contact connector MSTB_01x07_GF_5.08mm
0
7
7
Connector_Phoenix_MSTB
PhoenixContact_MSTB_2,5_7-GF-5,08_1x07_P5.08mm_Horizontal_ThreadedFlange_MountHole
Generic Phoenix Contact connector footprint for: MSTB_2,5/7-GF-5,08; number of pins: 07; pin pitch: 5.08mm; Angled; threaded flange; footprint includes mount hole for mounting screw: ISO 1481-ST 2.2x6.5 C or ISO 7049-ST 2.2x6.5 C (http://www.fasteners.eu/standards/ISO/7049/) || order number: 1776553 12A || order number: 1924130 16A (HC)
phoenix_contact connector MSTB_01x07_GF_5.08mm_MH
0
7
7
Connector_Phoenix_MSTB
PhoenixContact_MSTB_2,5_7-GF_1x07_P5.00mm_Horizontal_ThreadedFlange
Generic Phoenix Contact connector footprint for: MSTB_2,5/7-GF; number of pins: 07; pin pitch: 5.00mm; Angled; threaded flange || order number: 1776744 12A || order number: 1924020 16A (HC)
phoenix_contact connector MSTB_01x07_GF_5.00mm
0
7
7
Connector_Phoenix_MSTB
PhoenixContact_MSTB_2,5_7-GF_1x07_P5.00mm_Horizontal_ThreadedFlange_MountHole
Generic Phoenix Contact connector footprint for: MSTB_2,5/7-GF; number of pins: 07; pin pitch: 5.00mm; Angled; threaded flange; footprint includes mount hole for mounting screw: ISO 1481-ST 2.2x6.5 C or ISO 7049-ST 2.2x6.5 C (http://www.fasteners.eu/standards/ISO/7049/) || order number: 1776744 12A || order number: 1924020 16A (HC)
phoenix_contact connector MSTB_01x07_GF_5.00mm_MH
0
7
7
Connector_Phoenix_MSTB
PhoenixContact_MSTB_2,5_8-GF-5,08_1x08_P5.08mm_Horizontal_ThreadedFlange
Generic Phoenix Contact connector footprint for: MSTB_2,5/8-GF-5,08; number of pins: 08; pin pitch: 5.08mm; Angled; threaded flange || order number: 1776566 12A || order number: 1924143 16A (HC)
phoenix_contact connector MSTB_01x08_GF_5.08mm
0
8
8
Connector_Phoenix_MSTB
PhoenixContact_MSTB_2,5_8-GF-5,08_1x08_P5.08mm_Horizontal_ThreadedFlange_MountHole
Generic Phoenix Contact connector footprint for: MSTB_2,5/8-GF-5,08; number of pins: 08; pin pitch: 5.08mm; Angled; threaded flange; footprint includes mount hole for mounting screw: ISO 1481-ST 2.2x6.5 C or ISO 7049-ST 2.2x6.5 C (http://www.fasteners.eu/standards/ISO/7049/) || order number: 1776566 12A || order number: 1924143 16A (HC)
phoenix_contact connector MSTB_01x08_GF_5.08mm_MH
0
8
8
Connector_Phoenix_MSTB
PhoenixContact_MSTB_2,5_8-GF_1x08_P5.00mm_Horizontal_ThreadedFlange
Generic Phoenix Contact connector footprint for: MSTB_2,5/8-GF; number of pins: 08; pin pitch: 5.00mm; Angled; threaded flange || order number: 1776757 12A || order number: 1924033 16A (HC)
phoenix_contact connector MSTB_01x08_GF_5.00mm
0
8
8
Connector_Phoenix_MSTB
PhoenixContact_MSTB_2,5_8-GF_1x08_P5.00mm_Horizontal_ThreadedFlange_MountHole
Generic Phoenix Contact connector footprint for: MSTB_2,5/8-GF; number of pins: 08; pin pitch: 5.00mm; Angled; threaded flange; footprint includes mount hole for mounting screw: ISO 1481-ST 2.2x6.5 C or ISO 7049-ST 2.2x6.5 C (http://www.fasteners.eu/standards/ISO/7049/) || order number: 1776757 12A || order number: 1924033 16A (HC)
phoenix_contact connector MSTB_01x08_GF_5.00mm_MH
0
8
8
Connector_Phoenix_MSTB
PhoenixContact_MSTB_2,5_9-GF-5,08_1x09_P5.08mm_Horizontal_ThreadedFlange
Generic Phoenix Contact connector footprint for: MSTB_2,5/9-GF-5,08; number of pins: 09; pin pitch: 5.08mm; Angled; threaded flange || order number: 1776579 12A || order number: 1924156 16A (HC)
phoenix_contact connector MSTB_01x09_GF_5.08mm
0
9
9
Connector_Phoenix_MSTB
PhoenixContact_MSTB_2,5_9-GF-5,08_1x09_P5.08mm_Horizontal_ThreadedFlange_MountHole
Generic Phoenix Contact connector footprint for: MSTB_2,5/9-GF-5,08; number of pins: 09; pin pitch: 5.08mm; Angled; threaded flange; footprint includes mount hole for mounting screw: ISO 1481-ST 2.2x6.5 C or ISO 7049-ST 2.2x6.5 C (http://www.fasteners.eu/standards/ISO/7049/) || order number: 1776579 12A || order number: 1924156 16A (HC)
phoenix_contact connector MSTB_01x09_GF_5.08mm_MH
0
9
9
Connector_Phoenix_MSTB
PhoenixContact_MSTB_2,5_9-GF_1x09_P5.00mm_Horizontal_ThreadedFlange
Generic Phoenix Contact connector footprint for: MSTB_2,5/9-GF; number of pins: 09; pin pitch: 5.00mm; Angled; threaded flange || order number: 1776760 12A || order number: 1924046 16A (HC)
phoenix_contact connector MSTB_01x09_GF_5.00mm
0
9
9
Connector_Phoenix_MSTB
PhoenixContact_MSTB_2,5_9-GF_1x09_P5.00mm_Horizontal_ThreadedFlange_MountHole
Generic Phoenix Contact connector footprint for: MSTB_2,5/9-GF; number of pins: 09; pin pitch: 5.00mm; Angled; threaded flange; footprint includes mount hole for mounting screw: ISO 1481-ST 2.2x6.5 C or ISO 7049-ST 2.2x6.5 C (http://www.fasteners.eu/standards/ISO/7049/) || order number: 1776760 12A || order number: 1924046 16A (HC)
phoenix_contact connector MSTB_01x09_GF_5.00mm_MH
0
9
9
Connector_Phoenix_MSTB
PhoenixContact_MSTB_2,5_10-GF-5,08_1x10_P5.08mm_Horizontal_ThreadedFlange
Generic Phoenix Contact connector footprint for: MSTB_2,5/10-GF-5,08; number of pins: 10; pin pitch: 5.08mm; Angled; threaded flange || order number: 1776582 12A || order number: 1924169 16A (HC)
phoenix_contact connector MSTB_01x10_GF_5.08mm
0
10
10
Connector_Phoenix_MSTB
PhoenixContact_MSTB_2,5_10-GF-5,08_1x10_P5.08mm_Horizontal_ThreadedFlange_MountHole
Generic Phoenix Contact connector footprint for: MSTB_2,5/10-GF-5,08; number of pins: 10; pin pitch: 5.08mm; Angled; threaded flange; footprint includes mount hole for mounting screw: ISO 1481-ST 2.2x6.5 C or ISO 7049-ST 2.2x6.5 C (http://www.fasteners.eu/standards/ISO/7049/) || order number: 1776582 12A || order number: 1924169 16A (HC)
phoenix_contact connector MSTB_01x10_GF_5.08mm_MH
0
10
10
Connector_Phoenix_MSTB
PhoenixContact_MSTB_2,5_10-GF_1x10_P5.00mm_Horizontal_ThreadedFlange
Generic Phoenix Contact connector footprint for: MSTB_2,5/10-GF; number of pins: 10; pin pitch: 5.00mm; Angled; threaded flange || order number: 1776773 12A || order number: 1924059 16A (HC)
phoenix_contact connector MSTB_01x10_GF_5.00mm
0
10
10
Connector_Phoenix_MSTB
PhoenixContact_MSTB_2,5_10-GF_1x10_P5.00mm_Horizontal_ThreadedFlange_MountHole
Generic Phoenix Contact connector footprint for: MSTB_2,5/10-GF; number of pins: 10; pin pitch: 5.00mm; Angled; threaded flange; footprint includes mount hole for mounting screw: ISO 1481-ST 2.2x6.5 C or ISO 7049-ST 2.2x6.5 C (http://www.fasteners.eu/standards/ISO/7049/) || order number: 1776773 12A || order number: 1924059 16A (HC)
phoenix_contact connector MSTB_01x10_GF_5.00mm_MH
0
10
10
Connector_Phoenix_MSTB
PhoenixContact_MSTB_2,5_11-GF-5,08_1x11_P5.08mm_Horizontal_ThreadedFlange
Generic Phoenix Contact connector footprint for: MSTB_2,5/11-GF-5,08; number of pins: 11; pin pitch: 5.08mm; Angled; threaded flange || order number: 1776595 12A || order number: 1924172 16A (HC)
phoenix_contact connector MSTB_01x11_GF_5.08mm
0
11
11
Connector_Phoenix_MSTB
PhoenixContact_MSTB_2,5_11-GF-5,08_1x11_P5.08mm_Horizontal_ThreadedFlange_MountHole
Generic Phoenix Contact connector footprint for: MSTB_2,5/11-GF-5,08; number of pins: 11; pin pitch: 5.08mm; Angled; threaded flange; footprint includes mount hole for mounting screw: ISO 1481-ST 2.2x6.5 C or ISO 7049-ST 2.2x6.5 C (http://www.fasteners.eu/standards/ISO/7049/) || order number: 1776595 12A || order number: 1924172 16A (HC)
phoenix_contact connector MSTB_01x11_GF_5.08mm_MH
0
11
11
Connector_Phoenix_MSTB
PhoenixContact_MSTB_2,5_11-GF_1x11_P5.00mm_Horizontal_ThreadedFlange
Generic Phoenix Contact connector footprint for: MSTB_2,5/11-GF; number of pins: 11; pin pitch: 5.00mm; Angled; threaded flange || order number: 1776786 12A || order number: 1924062 16A (HC)
phoenix_contact connector MSTB_01x11_GF_5.00mm
0
11
11
Connector_Phoenix_MSTB
PhoenixContact_MSTB_2,5_11-GF_1x11_P5.00mm_Horizontal_ThreadedFlange_MountHole
Generic Phoenix Contact connector footprint for: MSTB_2,5/11-GF; number of pins: 11; pin pitch: 5.00mm; Angled; threaded flange; footprint includes mount hole for mounting screw: ISO 1481-ST 2.2x6.5 C or ISO 7049-ST 2.2x6.5 C (http://www.fasteners.eu/standards/ISO/7049/) || order number: 1776786 12A || order number: 1924062 16A (HC)
phoenix_contact connector MSTB_01x11_GF_5.00mm_MH
0
11
11
Connector_Phoenix_MSTB
PhoenixContact_MSTB_2,5_12-GF-5,08_1x12_P5.08mm_Horizontal_ThreadedFlange
Generic Phoenix Contact connector footprint for: MSTB_2,5/12-GF-5,08; number of pins: 12; pin pitch: 5.08mm; Angled; threaded flange || order number: 1776605 12A || order number: 1924185 16A (HC)
phoenix_contact connector MSTB_01x12_GF_5.08mm
0
12
12
Connector_Phoenix_MSTB
PhoenixContact_MSTB_2,5_12-GF-5,08_1x12_P5.08mm_Horizontal_ThreadedFlange_MountHole
Generic Phoenix Contact connector footprint for: MSTB_2,5/12-GF-5,08; number of pins: 12; pin pitch: 5.08mm; Angled; threaded flange; footprint includes mount hole for mounting screw: ISO 1481-ST 2.2x6.5 C or ISO 7049-ST 2.2x6.5 C (http://www.fasteners.eu/standards/ISO/7049/) || order number: 1776605 12A || order number: 1924185 16A (HC)
phoenix_contact connector MSTB_01x12_GF_5.08mm_MH
0
12
12
Connector_Phoenix_MSTB
PhoenixContact_MSTB_2,5_12-GF_1x12_P5.00mm_Horizontal_ThreadedFlange
Generic Phoenix Contact connector footprint for: MSTB_2,5/12-GF; number of pins: 12; pin pitch: 5.00mm; Angled; threaded flange || order number: 1776799 12A || order number: 1924075 16A (HC)
phoenix_contact connector MSTB_01x12_GF_5.00mm
0
12
12
Connector_Phoenix_MSTB
PhoenixContact_MSTB_2,5_12-GF_1x12_P5.00mm_Horizontal_ThreadedFlange_MountHole
Generic Phoenix Contact connector footprint for: MSTB_2,5/12-GF; number of pins: 12; pin pitch: 5.00mm; Angled; threaded flange; footprint includes mount hole for mounting screw: ISO 1481-ST 2.2x6.5 C or ISO 7049-ST 2.2x6.5 C (http://www.fasteners.eu/standards/ISO/7049/) || order number: 1776799 12A || order number: 1924075 16A (HC)
phoenix_contact connector MSTB_01x12_GF_5.00mm_MH
0
12
12
Connector_Phoenix_MSTB
PhoenixContact_MSTB_2,5_13-GF-5,08_1x13_P5.08mm_Horizontal_ThreadedFlange
Generic Phoenix Contact connector footprint for: MSTB_2,5/13-GF-5,08; number of pins: 13; pin pitch: 5.08mm; Angled; threaded flange || order number: 1776618 12A
phoenix_contact connector MSTB_01x13_GF_5.08mm
0
13
13
Connector_Phoenix_MSTB
PhoenixContact_MSTB_2,5_13-GF-5,08_1x13_P5.08mm_Horizontal_ThreadedFlange_MountHole
Generic Phoenix Contact connector footprint for: MSTB_2,5/13-GF-5,08; number of pins: 13; pin pitch: 5.08mm; Angled; threaded flange; footprint includes mount hole for mounting screw: ISO 1481-ST 2.2x6.5 C or ISO 7049-ST 2.2x6.5 C (http://www.fasteners.eu/standards/ISO/7049/) || order number: 1776618 12A
phoenix_contact connector MSTB_01x13_GF_5.08mm_MH
0
13
13
Connector_Phoenix_MSTB
PhoenixContact_MSTB_2,5_13-GF_1x13_P5.00mm_Horizontal_ThreadedFlange
Generic Phoenix Contact connector footprint for: MSTB_2,5/13-GF; number of pins: 13; pin pitch: 5.00mm; Angled; threaded flange || order number: 1776809 12A
phoenix_contact connector MSTB_01x13_GF_5.00mm
0
13
13
Connector_Phoenix_MSTB
PhoenixContact_MSTB_2,5_13-GF_1x13_P5.00mm_Horizontal_ThreadedFlange_MountHole
Generic Phoenix Contact connector footprint for: MSTB_2,5/13-GF; number of pins: 13; pin pitch: 5.00mm; Angled; threaded flange; footprint includes mount hole for mounting screw: ISO 1481-ST 2.2x6.5 C or ISO 7049-ST 2.2x6.5 C (http://www.fasteners.eu/standards/ISO/7049/) || order number: 1776809 12A
phoenix_contact connector MSTB_01x13_GF_5.00mm_MH
0
13
13
Connector_Phoenix_MSTB
PhoenixContact_MSTB_2,5_14-GF-5,08_1x14_P5.08mm_Horizontal_ThreadedFlange
Generic Phoenix Contact connector footprint for: MSTB_2,5/14-GF-5,08; number of pins: 14; pin pitch: 5.08mm; Angled; threaded flange || order number: 1776621 12A
phoenix_contact connector MSTB_01x14_GF_5.08mm
0
14
14
Connector_Phoenix_MSTB
PhoenixContact_MSTB_2,5_14-GF-5,08_1x14_P5.08mm_Horizontal_ThreadedFlange_MountHole
Generic Phoenix Contact connector footprint for: MSTB_2,5/14-GF-5,08; number of pins: 14; pin pitch: 5.08mm; Angled; threaded flange; footprint includes mount hole for mounting screw: ISO 1481-ST 2.2x6.5 C or ISO 7049-ST 2.2x6.5 C (http://www.fasteners.eu/standards/ISO/7049/) || order number: 1776621 12A
phoenix_contact connector MSTB_01x14_GF_5.08mm_MH
0
14
14
Connector_Phoenix_MSTB
PhoenixContact_MSTB_2,5_14-GF_1x14_P5.00mm_Horizontal_ThreadedFlange
Generic Phoenix Contact connector footprint for: MSTB_2,5/14-GF; number of pins: 14; pin pitch: 5.00mm; Angled; threaded flange || order number: 1776812 12A
phoenix_contact connector MSTB_01x14_GF_5.00mm
0
14
14
Connector_Phoenix_MSTB
PhoenixContact_MSTB_2,5_14-GF_1x14_P5.00mm_Horizontal_ThreadedFlange_MountHole
Generic Phoenix Contact connector footprint for: MSTB_2,5/14-GF; number of pins: 14; pin pitch: 5.00mm; Angled; threaded flange; footprint includes mount hole for mounting screw: ISO 1481-ST 2.2x6.5 C or ISO 7049-ST 2.2x6.5 C (http://www.fasteners.eu/standards/ISO/7049/) || order number: 1776812 12A
phoenix_contact connector MSTB_01x14_GF_5.00mm_MH
0
14
14
Connector_Phoenix_MSTB
PhoenixContact_MSTB_2,5_15-GF-5,08_1x15_P5.08mm_Horizontal_ThreadedFlange
Generic Phoenix Contact connector footprint for: MSTB_2,5/15-GF-5,08; number of pins: 15; pin pitch: 5.08mm; Angled; threaded flange || order number: 1776634 12A
phoenix_contact connector MSTB_01x15_GF_5.08mm
0
15
15
Connector_Phoenix_MSTB
PhoenixContact_MSTB_2,5_15-GF-5,08_1x15_P5.08mm_Horizontal_ThreadedFlange_MountHole
Generic Phoenix Contact connector footprint for: MSTB_2,5/15-GF-5,08; number of pins: 15; pin pitch: 5.08mm; Angled; threaded flange; footprint includes mount hole for mounting screw: ISO 1481-ST 2.2x6.5 C or ISO 7049-ST 2.2x6.5 C (http://www.fasteners.eu/standards/ISO/7049/) || order number: 1776634 12A
phoenix_contact connector MSTB_01x15_GF_5.08mm_MH
0
15
15
Connector_Phoenix_MSTB
PhoenixContact_MSTB_2,5_15-GF_1x15_P5.00mm_Horizontal_ThreadedFlange
Generic Phoenix Contact connector footprint for: MSTB_2,5/15-GF; number of pins: 15; pin pitch: 5.00mm; Angled; threaded flange || order number: 1776825 12A
phoenix_contact connector MSTB_01x15_GF_5.00mm
0
15
15
Connector_Phoenix_MSTB
PhoenixContact_MSTB_2,5_15-GF_1x15_P5.00mm_Horizontal_ThreadedFlange_MountHole
Generic Phoenix Contact connector footprint for: MSTB_2,5/15-GF; number of pins: 15; pin pitch: 5.00mm; Angled; threaded flange; footprint includes mount hole for mounting screw: ISO 1481-ST 2.2x6.5 C or ISO 7049-ST 2.2x6.5 C (http://www.fasteners.eu/standards/ISO/7049/) || order number: 1776825 12A
phoenix_contact connector MSTB_01x15_GF_5.00mm_MH
0
15
15
Connector_Phoenix_MSTB
PhoenixContact_MSTB_2,5_16-GF-5,08_1x16_P5.08mm_Horizontal_ThreadedFlange
Generic Phoenix Contact connector footprint for: MSTB_2,5/16-GF-5,08; number of pins: 16; pin pitch: 5.08mm; Angled; threaded flange || order number: 1776647 12A
phoenix_contact connector MSTB_01x16_GF_5.08mm
0
16
16
Connector_Phoenix_MSTB
PhoenixContact_MSTB_2,5_16-GF-5,08_1x16_P5.08mm_Horizontal_ThreadedFlange_MountHole
Generic Phoenix Contact connector footprint for: MSTB_2,5/16-GF-5,08; number of pins: 16; pin pitch: 5.08mm; Angled; threaded flange; footprint includes mount hole for mounting screw: ISO 1481-ST 2.2x6.5 C or ISO 7049-ST 2.2x6.5 C (http://www.fasteners.eu/standards/ISO/7049/) || order number: 1776647 12A
phoenix_contact connector MSTB_01x16_GF_5.08mm_MH
0
16
16
Connector_Phoenix_MSTB
PhoenixContact_MSTB_2,5_16-GF_1x16_P5.00mm_Horizontal_ThreadedFlange
Generic Phoenix Contact connector footprint for: MSTB_2,5/16-GF; number of pins: 16; pin pitch: 5.00mm; Angled; threaded flange || order number: 1776838 12A
phoenix_contact connector MSTB_01x16_GF_5.00mm
0
16
16
Connector_Phoenix_MSTB
PhoenixContact_MSTB_2,5_16-GF_1x16_P5.00mm_Horizontal_ThreadedFlange_MountHole
Generic Phoenix Contact connector footprint for: MSTB_2,5/16-GF; number of pins: 16; pin pitch: 5.00mm; Angled; threaded flange; footprint includes mount hole for mounting screw: ISO 1481-ST 2.2x6.5 C or ISO 7049-ST 2.2x6.5 C (http://www.fasteners.eu/standards/ISO/7049/) || order number: 1776838 12A
phoenix_contact connector MSTB_01x16_GF_5.00mm_MH
0
16
16
Connector_Pin
Pin_D0.7mm_L6.5mm_W1.8mm_FlatFork
solder Pin_ with flat fork, hole diameter 0.7mm, length 6.5mm, width 1.8mm
solder Pin_ with flat fork
0
1
1
Connector_Pin
Pin_D0.9mm_L10.0mm_W2.4mm_FlatFork
solder Pin_ with flat fork, hole diameter 0.9mm, length 10.0mm, width 2.4mm
solder Pin_ with flat fork
0
1
1
Connector_Pin
Pin_D1.0mm_L10.0mm
solder Pin_ diameter 1.0mm, hole diameter 1.0mm (press fit), length 10.0mm
solder Pin_ press fit
0
1
1
Connector_Pin
Pin_D1.0mm_L10.0mm_LooseFit
solder Pin_ diameter 1.0mm, hole diameter 1.2mm (loose fit), length 10.0mm
solder Pin_ loose fit
0
1
1
Connector_Pin
Pin_D1.1mm_L8.5mm_W2.5mm_FlatFork
solder Pin_ with flat fork, hole diameter 1.1mm, length 8.5mm, width 2.5mm
solder Pin_ with flat fork
0
1
1
Connector_Pin
Pin_D1.1mm_L10.2mm_W3.5mm_Flat
solder Pin_ with flat with hole, hole diameter 1.1mm, length 10.2mm, width 3.5mm
solder Pin_ with flat fork
0
1
1
Connector_Pin
Pin_D1.2mm_L10.2mm_W2.9mm_FlatFork
solder Pin_ with flat with fork, hole diameter 1.2mm, length 11.3mm, width 3.0mm
solder Pin_ with flat fork
0
1
1
Connector_Pin
Pin_D1.2mm_L11.3mm_W3.0mm_Flat
solder Pin_ with flat with hole, hole diameter 1.2mm, length 11.3mm, width 3.0mm
solder Pin_ with flat fork
0
1
1
Connector_Pin
Pin_D1.3mm_L10.0mm_W3.5mm_Flat
solder Pin_ with flat with hole, hole diameter 1.3mm, length 10.0mm, width 3.5mm, e.g. Ettinger 13.13.865, https://katalog.ettinger.de/#p=434
solder Pin_ with flat fork
0
1
1
Connector_Pin
Pin_D1.3mm_L11.0mm
solder Pin_ diameter 1.3mm, hole diameter 1.3mm, length 11.0mm
solder Pin_ pressfit
0
1
1
Connector_Pin
Pin_D1.3mm_L11.0mm_LooseFit
solder Pin_ diameter 1.3mm, hole diameter 1.5mm (loose fit), length 11.0mm
solder Pin_ loose fit
0
1
1
Connector_Pin
Pin_D1.3mm_L11.3mm_W2.8mm_Flat
solder Pin_ with flat with hole, hole diameter 1.3mm, length 11.3mm, width 2.8mm
solder Pin_ with flat fork
0
1
1
Connector_Pin
Pin_D1.4mm_L8.5mm_W2.8mm_FlatFork
solder Pin_ with flat with fork, hole diameter 1.4mm, length 8.5mm, width 2.8mm, e.g. Ettinger 13.13.890, https://katalog.ettinger.de/#p=434
solder Pin_ with flat fork
0
1
1
Connector_PinHeader_1.00mm
PinHeader_1x01_P1.00mm_Horizontal
Through hole angled pin header, 1x01, 1.00mm pitch, 2.0mm pin length, single row
Through hole angled pin header THT 1x01 1.00mm single row
0
1
1
Connector_PinHeader_1.00mm
PinHeader_1x01_P1.00mm_Vertical
Through hole straight pin header, 1x01, 1.00mm pitch, single row
Through hole pin header THT 1x01 1.00mm single row
0
1
1
Connector_PinHeader_1.00mm
PinHeader_1x02_P1.00mm_Horizontal
Through hole angled pin header, 1x02, 1.00mm pitch, 2.0mm pin length, single row
Through hole angled pin header THT 1x02 1.00mm single row
0
2
2
Connector_PinHeader_1.00mm
PinHeader_1x02_P1.00mm_Vertical
Through hole straight pin header, 1x02, 1.00mm pitch, single row
Through hole pin header THT 1x02 1.00mm single row
0
2
2
Connector_PinHeader_1.00mm
PinHeader_1x02_P1.00mm_Vertical_SMD_Pin1Left
surface-mounted straight pin header, 1x02, 1.00mm pitch, single row, style 1 (pin 1 left)
Surface mounted pin header SMD 1x02 1.00mm single row style1 pin1 left
0
2
2
Connector_PinHeader_1.00mm
PinHeader_1x02_P1.00mm_Vertical_SMD_Pin1Right
surface-mounted straight pin header, 1x02, 1.00mm pitch, single row, style 2 (pin 1 right)
Surface mounted pin header SMD 1x02 1.00mm single row style2 pin1 right
0
2
2
Connector_PinHeader_1.00mm
PinHeader_1x03_P1.00mm_Horizontal
Through hole angled pin header, 1x03, 1.00mm pitch, 2.0mm pin length, single row
Through hole angled pin header THT 1x03 1.00mm single row
0
3
3
Connector_PinHeader_1.00mm
PinHeader_1x03_P1.00mm_Vertical
Through hole straight pin header, 1x03, 1.00mm pitch, single row
Through hole pin header THT 1x03 1.00mm single row
0
3
3
Connector_PinHeader_1.00mm
PinHeader_1x03_P1.00mm_Vertical_SMD_Pin1Left
surface-mounted straight pin header, 1x03, 1.00mm pitch, single row, style 1 (pin 1 left)
Surface mounted pin header SMD 1x03 1.00mm single row style1 pin1 left
0
3
3
Connector_PinHeader_1.00mm
PinHeader_1x03_P1.00mm_Vertical_SMD_Pin1Right
surface-mounted straight pin header, 1x03, 1.00mm pitch, single row, style 2 (pin 1 right)
Surface mounted pin header SMD 1x03 1.00mm single row style2 pin1 right
0
3
3
Connector_PinHeader_1.00mm
PinHeader_1x04_P1.00mm_Horizontal
Through hole angled pin header, 1x04, 1.00mm pitch, 2.0mm pin length, single row
Through hole angled pin header THT 1x04 1.00mm single row
0
4
4
Connector_PinHeader_1.00mm
PinHeader_1x04_P1.00mm_Vertical
Through hole straight pin header, 1x04, 1.00mm pitch, single row
Through hole pin header THT 1x04 1.00mm single row
0
4
4
Connector_PinHeader_1.00mm
PinHeader_1x04_P1.00mm_Vertical_SMD_Pin1Left
surface-mounted straight pin header, 1x04, 1.00mm pitch, single row, style 1 (pin 1 left)
Surface mounted pin header SMD 1x04 1.00mm single row style1 pin1 left
0
4
4
Connector_PinHeader_1.00mm
PinHeader_1x04_P1.00mm_Vertical_SMD_Pin1Right
surface-mounted straight pin header, 1x04, 1.00mm pitch, single row, style 2 (pin 1 right)
Surface mounted pin header SMD 1x04 1.00mm single row style2 pin1 right
0
4
4
Connector_PinHeader_1.00mm
PinHeader_1x05_P1.00mm_Horizontal
Through hole angled pin header, 1x05, 1.00mm pitch, 2.0mm pin length, single row
Through hole angled pin header THT 1x05 1.00mm single row
0
5
5
Connector_PinHeader_1.00mm
PinHeader_1x05_P1.00mm_Vertical
Through hole straight pin header, 1x05, 1.00mm pitch, single row
Through hole pin header THT 1x05 1.00mm single row
0
5
5
Connector_PinHeader_1.00mm
PinHeader_1x05_P1.00mm_Vertical_SMD_Pin1Left
surface-mounted straight pin header, 1x05, 1.00mm pitch, single row, style 1 (pin 1 left)
Surface mounted pin header SMD 1x05 1.00mm single row style1 pin1 left
0
5
5
Connector_PinHeader_1.00mm
PinHeader_1x05_P1.00mm_Vertical_SMD_Pin1Right
surface-mounted straight pin header, 1x05, 1.00mm pitch, single row, style 2 (pin 1 right)
Surface mounted pin header SMD 1x05 1.00mm single row style2 pin1 right
0
5
5
Connector_PinHeader_1.00mm
PinHeader_1x06_P1.00mm_Horizontal
Through hole angled pin header, 1x06, 1.00mm pitch, 2.0mm pin length, single row
Through hole angled pin header THT 1x06 1.00mm single row
0
6
6
Connector_PinHeader_1.00mm
PinHeader_1x06_P1.00mm_Vertical
Through hole straight pin header, 1x06, 1.00mm pitch, single row
Through hole pin header THT 1x06 1.00mm single row
0
6
6
Connector_PinHeader_1.00mm
PinHeader_1x06_P1.00mm_Vertical_SMD_Pin1Left
surface-mounted straight pin header, 1x06, 1.00mm pitch, single row, style 1 (pin 1 left)
Surface mounted pin header SMD 1x06 1.00mm single row style1 pin1 left
0
6
6
Connector_PinHeader_1.00mm
PinHeader_1x06_P1.00mm_Vertical_SMD_Pin1Right
surface-mounted straight pin header, 1x06, 1.00mm pitch, single row, style 2 (pin 1 right)
Surface mounted pin header SMD 1x06 1.00mm single row style2 pin1 right
0
6
6
Connector_PinHeader_1.00mm
PinHeader_1x07_P1.00mm_Horizontal
Through hole angled pin header, 1x07, 1.00mm pitch, 2.0mm pin length, single row
Through hole angled pin header THT 1x07 1.00mm single row
0
7
7
Connector_PinHeader_1.00mm
PinHeader_1x07_P1.00mm_Vertical
Through hole straight pin header, 1x07, 1.00mm pitch, single row
Through hole pin header THT 1x07 1.00mm single row
0
7
7
Connector_PinHeader_1.00mm
PinHeader_1x07_P1.00mm_Vertical_SMD_Pin1Left
surface-mounted straight pin header, 1x07, 1.00mm pitch, single row, style 1 (pin 1 left)
Surface mounted pin header SMD 1x07 1.00mm single row style1 pin1 left
0
7
7
Connector_PinHeader_1.00mm
PinHeader_1x07_P1.00mm_Vertical_SMD_Pin1Right
surface-mounted straight pin header, 1x07, 1.00mm pitch, single row, style 2 (pin 1 right)
Surface mounted pin header SMD 1x07 1.00mm single row style2 pin1 right
0
7
7
Connector_PinHeader_1.00mm
PinHeader_1x08_P1.00mm_Horizontal
Through hole angled pin header, 1x08, 1.00mm pitch, 2.0mm pin length, single row
Through hole angled pin header THT 1x08 1.00mm single row
0
8
8
Connector_PinHeader_1.00mm
PinHeader_1x08_P1.00mm_Vertical
Through hole straight pin header, 1x08, 1.00mm pitch, single row
Through hole pin header THT 1x08 1.00mm single row
0
8
8
Connector_PinHeader_1.00mm
PinHeader_1x08_P1.00mm_Vertical_SMD_Pin1Left
surface-mounted straight pin header, 1x08, 1.00mm pitch, single row, style 1 (pin 1 left)
Surface mounted pin header SMD 1x08 1.00mm single row style1 pin1 left
0
8
8
Connector_PinHeader_1.00mm
PinHeader_1x08_P1.00mm_Vertical_SMD_Pin1Right
surface-mounted straight pin header, 1x08, 1.00mm pitch, single row, style 2 (pin 1 right)
Surface mounted pin header SMD 1x08 1.00mm single row style2 pin1 right
0
8
8
Connector_PinHeader_1.00mm
PinHeader_1x09_P1.00mm_Horizontal
Through hole angled pin header, 1x09, 1.00mm pitch, 2.0mm pin length, single row
Through hole angled pin header THT 1x09 1.00mm single row
0
9
9
Connector_PinHeader_1.00mm
PinHeader_1x09_P1.00mm_Vertical
Through hole straight pin header, 1x09, 1.00mm pitch, single row
Through hole pin header THT 1x09 1.00mm single row
0
9
9
Connector_PinHeader_1.00mm
PinHeader_1x09_P1.00mm_Vertical_SMD_Pin1Left
surface-mounted straight pin header, 1x09, 1.00mm pitch, single row, style 1 (pin 1 left)
Surface mounted pin header SMD 1x09 1.00mm single row style1 pin1 left
0
9
9
Connector_PinHeader_1.00mm
PinHeader_1x09_P1.00mm_Vertical_SMD_Pin1Right
surface-mounted straight pin header, 1x09, 1.00mm pitch, single row, style 2 (pin 1 right)
Surface mounted pin header SMD 1x09 1.00mm single row style2 pin1 right
0
9
9
Connector_PinHeader_1.00mm
PinHeader_1x10_P1.00mm_Horizontal
Through hole angled pin header, 1x10, 1.00mm pitch, 2.0mm pin length, single row
Through hole angled pin header THT 1x10 1.00mm single row
0
10
10
Connector_PinHeader_1.00mm
PinHeader_1x10_P1.00mm_Vertical
Through hole straight pin header, 1x10, 1.00mm pitch, single row
Through hole pin header THT 1x10 1.00mm single row
0
10
10
Connector_PinHeader_1.00mm
PinHeader_1x10_P1.00mm_Vertical_SMD_Pin1Left
surface-mounted straight pin header, 1x10, 1.00mm pitch, single row, style 1 (pin 1 left)
Surface mounted pin header SMD 1x10 1.00mm single row style1 pin1 left
0
10
10
Connector_PinHeader_1.00mm
PinHeader_1x10_P1.00mm_Vertical_SMD_Pin1Right
surface-mounted straight pin header, 1x10, 1.00mm pitch, single row, style 2 (pin 1 right)
Surface mounted pin header SMD 1x10 1.00mm single row style2 pin1 right
0
10
10
Connector_PinHeader_1.00mm
PinHeader_1x11_P1.00mm_Horizontal
Through hole angled pin header, 1x11, 1.00mm pitch, 2.0mm pin length, single row
Through hole angled pin header THT 1x11 1.00mm single row
0
11
11
Connector_PinHeader_1.00mm
PinHeader_1x11_P1.00mm_Vertical
Through hole straight pin header, 1x11, 1.00mm pitch, single row
Through hole pin header THT 1x11 1.00mm single row
0
11
11
Connector_PinHeader_1.00mm
PinHeader_1x11_P1.00mm_Vertical_SMD_Pin1Left
surface-mounted straight pin header, 1x11, 1.00mm pitch, single row, style 1 (pin 1 left)
Surface mounted pin header SMD 1x11 1.00mm single row style1 pin1 left
0
11
11
Connector_PinHeader_1.00mm
PinHeader_1x11_P1.00mm_Vertical_SMD_Pin1Right
surface-mounted straight pin header, 1x11, 1.00mm pitch, single row, style 2 (pin 1 right)
Surface mounted pin header SMD 1x11 1.00mm single row style2 pin1 right
0
11
11
Connector_PinHeader_1.00mm
PinHeader_1x12_P1.00mm_Horizontal
Through hole angled pin header, 1x12, 1.00mm pitch, 2.0mm pin length, single row
Through hole angled pin header THT 1x12 1.00mm single row
0
12
12
Connector_PinHeader_1.00mm
PinHeader_1x12_P1.00mm_Vertical
Through hole straight pin header, 1x12, 1.00mm pitch, single row
Through hole pin header THT 1x12 1.00mm single row
0
12
12
Connector_PinHeader_1.00mm
PinHeader_1x12_P1.00mm_Vertical_SMD_Pin1Left
surface-mounted straight pin header, 1x12, 1.00mm pitch, single row, style 1 (pin 1 left)
Surface mounted pin header SMD 1x12 1.00mm single row style1 pin1 left
0
12
12
Connector_PinHeader_1.00mm
PinHeader_1x12_P1.00mm_Vertical_SMD_Pin1Right
surface-mounted straight pin header, 1x12, 1.00mm pitch, single row, style 2 (pin 1 right)
Surface mounted pin header SMD 1x12 1.00mm single row style2 pin1 right
0
12
12
Connector_PinHeader_1.00mm
PinHeader_1x13_P1.00mm_Horizontal
Through hole angled pin header, 1x13, 1.00mm pitch, 2.0mm pin length, single row
Through hole angled pin header THT 1x13 1.00mm single row
0
13
13
Connector_PinHeader_1.00mm
PinHeader_1x13_P1.00mm_Vertical
Through hole straight pin header, 1x13, 1.00mm pitch, single row
Through hole pin header THT 1x13 1.00mm single row
0
13
13
Connector_PinHeader_1.00mm
PinHeader_1x13_P1.00mm_Vertical_SMD_Pin1Left
surface-mounted straight pin header, 1x13, 1.00mm pitch, single row, style 1 (pin 1 left)
Surface mounted pin header SMD 1x13 1.00mm single row style1 pin1 left
0
13
13
Connector_PinHeader_1.00mm
PinHeader_1x13_P1.00mm_Vertical_SMD_Pin1Right
surface-mounted straight pin header, 1x13, 1.00mm pitch, single row, style 2 (pin 1 right)
Surface mounted pin header SMD 1x13 1.00mm single row style2 pin1 right
0
13
13
Connector_PinHeader_1.00mm
PinHeader_1x14_P1.00mm_Horizontal
Through hole angled pin header, 1x14, 1.00mm pitch, 2.0mm pin length, single row
Through hole angled pin header THT 1x14 1.00mm single row
0
14
14
Connector_PinHeader_1.00mm
PinHeader_1x14_P1.00mm_Vertical
Through hole straight pin header, 1x14, 1.00mm pitch, single row
Through hole pin header THT 1x14 1.00mm single row
0
14
14
Connector_PinHeader_1.00mm
PinHeader_1x14_P1.00mm_Vertical_SMD_Pin1Left
surface-mounted straight pin header, 1x14, 1.00mm pitch, single row, style 1 (pin 1 left)
Surface mounted pin header SMD 1x14 1.00mm single row style1 pin1 left
0
14
14
Connector_PinHeader_1.00mm
PinHeader_1x14_P1.00mm_Vertical_SMD_Pin1Right
surface-mounted straight pin header, 1x14, 1.00mm pitch, single row, style 2 (pin 1 right)
Surface mounted pin header SMD 1x14 1.00mm single row style2 pin1 right
0
14
14
Connector_PinHeader_1.00mm
PinHeader_1x15_P1.00mm_Horizontal
Through hole angled pin header, 1x15, 1.00mm pitch, 2.0mm pin length, single row
Through hole angled pin header THT 1x15 1.00mm single row
0
15
15
Connector_PinHeader_1.00mm
PinHeader_1x15_P1.00mm_Vertical
Through hole straight pin header, 1x15, 1.00mm pitch, single row
Through hole pin header THT 1x15 1.00mm single row
0
15
15
Connector_PinHeader_1.00mm
PinHeader_1x15_P1.00mm_Vertical_SMD_Pin1Left
surface-mounted straight pin header, 1x15, 1.00mm pitch, single row, style 1 (pin 1 left)
Surface mounted pin header SMD 1x15 1.00mm single row style1 pin1 left
0
15
15
Connector_PinHeader_1.00mm
PinHeader_1x15_P1.00mm_Vertical_SMD_Pin1Right
surface-mounted straight pin header, 1x15, 1.00mm pitch, single row, style 2 (pin 1 right)
Surface mounted pin header SMD 1x15 1.00mm single row style2 pin1 right
0
15
15
Connector_PinHeader_1.00mm
PinHeader_1x16_P1.00mm_Horizontal
Through hole angled pin header, 1x16, 1.00mm pitch, 2.0mm pin length, single row
Through hole angled pin header THT 1x16 1.00mm single row
0
16
16
Connector_PinHeader_1.00mm
PinHeader_1x16_P1.00mm_Vertical
Through hole straight pin header, 1x16, 1.00mm pitch, single row
Through hole pin header THT 1x16 1.00mm single row
0
16
16
Connector_PinHeader_1.00mm
PinHeader_1x16_P1.00mm_Vertical_SMD_Pin1Left
surface-mounted straight pin header, 1x16, 1.00mm pitch, single row, style 1 (pin 1 left)
Surface mounted pin header SMD 1x16 1.00mm single row style1 pin1 left
0
16
16
Connector_PinHeader_1.00mm
PinHeader_1x16_P1.00mm_Vertical_SMD_Pin1Right
surface-mounted straight pin header, 1x16, 1.00mm pitch, single row, style 2 (pin 1 right)
Surface mounted pin header SMD 1x16 1.00mm single row style2 pin1 right
0
16
16
Connector_PinHeader_1.00mm
PinHeader_1x17_P1.00mm_Horizontal
Through hole angled pin header, 1x17, 1.00mm pitch, 2.0mm pin length, single row
Through hole angled pin header THT 1x17 1.00mm single row
0
17
17
Connector_PinHeader_1.00mm
PinHeader_1x17_P1.00mm_Vertical
Through hole straight pin header, 1x17, 1.00mm pitch, single row
Through hole pin header THT 1x17 1.00mm single row
0
17
17
Connector_PinHeader_1.00mm
PinHeader_1x17_P1.00mm_Vertical_SMD_Pin1Left
surface-mounted straight pin header, 1x17, 1.00mm pitch, single row, style 1 (pin 1 left)
Surface mounted pin header SMD 1x17 1.00mm single row style1 pin1 left
0
17
17
Connector_PinHeader_1.00mm
PinHeader_1x17_P1.00mm_Vertical_SMD_Pin1Right
surface-mounted straight pin header, 1x17, 1.00mm pitch, single row, style 2 (pin 1 right)
Surface mounted pin header SMD 1x17 1.00mm single row style2 pin1 right
0
17
17
Connector_PinHeader_1.00mm
PinHeader_1x18_P1.00mm_Horizontal
Through hole angled pin header, 1x18, 1.00mm pitch, 2.0mm pin length, single row
Through hole angled pin header THT 1x18 1.00mm single row
0
18
18
Connector_PinHeader_1.00mm
PinHeader_1x18_P1.00mm_Vertical
Through hole straight pin header, 1x18, 1.00mm pitch, single row
Through hole pin header THT 1x18 1.00mm single row
0
18
18
Connector_PinHeader_1.00mm
PinHeader_1x18_P1.00mm_Vertical_SMD_Pin1Left
surface-mounted straight pin header, 1x18, 1.00mm pitch, single row, style 1 (pin 1 left)
Surface mounted pin header SMD 1x18 1.00mm single row style1 pin1 left
0
18
18
Connector_PinHeader_1.00mm
PinHeader_1x18_P1.00mm_Vertical_SMD_Pin1Right
surface-mounted straight pin header, 1x18, 1.00mm pitch, single row, style 2 (pin 1 right)
Surface mounted pin header SMD 1x18 1.00mm single row style2 pin1 right
0
18
18
Connector_PinHeader_1.00mm
PinHeader_1x19_P1.00mm_Horizontal
Through hole angled pin header, 1x19, 1.00mm pitch, 2.0mm pin length, single row
Through hole angled pin header THT 1x19 1.00mm single row
0
19
19
Connector_PinHeader_1.00mm
PinHeader_1x19_P1.00mm_Vertical
Through hole straight pin header, 1x19, 1.00mm pitch, single row
Through hole pin header THT 1x19 1.00mm single row
0
19
19
Connector_PinHeader_1.00mm
PinHeader_1x19_P1.00mm_Vertical_SMD_Pin1Left
surface-mounted straight pin header, 1x19, 1.00mm pitch, single row, style 1 (pin 1 left)
Surface mounted pin header SMD 1x19 1.00mm single row style1 pin1 left
0
19
19
Connector_PinHeader_1.00mm
PinHeader_1x19_P1.00mm_Vertical_SMD_Pin1Right
surface-mounted straight pin header, 1x19, 1.00mm pitch, single row, style 2 (pin 1 right)
Surface mounted pin header SMD 1x19 1.00mm single row style2 pin1 right
0
19
19
Connector_PinHeader_1.00mm
PinHeader_1x20_P1.00mm_Horizontal
Through hole angled pin header, 1x20, 1.00mm pitch, 2.0mm pin length, single row
Through hole angled pin header THT 1x20 1.00mm single row
0
20
20
Connector_PinHeader_1.00mm
PinHeader_1x20_P1.00mm_Vertical
Through hole straight pin header, 1x20, 1.00mm pitch, single row
Through hole pin header THT 1x20 1.00mm single row
0
20
20
Connector_PinHeader_1.00mm
PinHeader_1x20_P1.00mm_Vertical_SMD_Pin1Left
surface-mounted straight pin header, 1x20, 1.00mm pitch, single row, style 1 (pin 1 left)
Surface mounted pin header SMD 1x20 1.00mm single row style1 pin1 left
0
20
20
Connector_PinHeader_1.00mm
PinHeader_1x20_P1.00mm_Vertical_SMD_Pin1Right
surface-mounted straight pin header, 1x20, 1.00mm pitch, single row, style 2 (pin 1 right)
Surface mounted pin header SMD 1x20 1.00mm single row style2 pin1 right
0
20
20
Connector_PinHeader_1.00mm
PinHeader_1x21_P1.00mm_Horizontal
Through hole angled pin header, 1x21, 1.00mm pitch, 2.0mm pin length, single row
Through hole angled pin header THT 1x21 1.00mm single row
0
21
21
Connector_PinHeader_1.00mm
PinHeader_1x21_P1.00mm_Vertical
Through hole straight pin header, 1x21, 1.00mm pitch, single row
Through hole pin header THT 1x21 1.00mm single row
0
21
21
Connector_PinHeader_1.00mm
PinHeader_1x21_P1.00mm_Vertical_SMD_Pin1Left
surface-mounted straight pin header, 1x21, 1.00mm pitch, single row, style 1 (pin 1 left)
Surface mounted pin header SMD 1x21 1.00mm single row style1 pin1 left
0
21
21
Connector_PinHeader_1.00mm
PinHeader_1x21_P1.00mm_Vertical_SMD_Pin1Right
surface-mounted straight pin header, 1x21, 1.00mm pitch, single row, style 2 (pin 1 right)
Surface mounted pin header SMD 1x21 1.00mm single row style2 pin1 right
0
21
21
Connector_PinHeader_1.00mm
PinHeader_1x22_P1.00mm_Horizontal
Through hole angled pin header, 1x22, 1.00mm pitch, 2.0mm pin length, single row
Through hole angled pin header THT 1x22 1.00mm single row
0
22
22
Connector_PinHeader_1.00mm
PinHeader_1x22_P1.00mm_Vertical
Through hole straight pin header, 1x22, 1.00mm pitch, single row
Through hole pin header THT 1x22 1.00mm single row
0
22
22
Connector_PinHeader_1.00mm
PinHeader_1x22_P1.00mm_Vertical_SMD_Pin1Left
surface-mounted straight pin header, 1x22, 1.00mm pitch, single row, style 1 (pin 1 left)
Surface mounted pin header SMD 1x22 1.00mm single row style1 pin1 left
0
22
22
Connector_PinHeader_1.00mm
PinHeader_1x22_P1.00mm_Vertical_SMD_Pin1Right
surface-mounted straight pin header, 1x22, 1.00mm pitch, single row, style 2 (pin 1 right)
Surface mounted pin header SMD 1x22 1.00mm single row style2 pin1 right
0
22
22
Connector_PinHeader_1.00mm
PinHeader_1x23_P1.00mm_Horizontal
Through hole angled pin header, 1x23, 1.00mm pitch, 2.0mm pin length, single row
Through hole angled pin header THT 1x23 1.00mm single row
0
23
23
Connector_PinHeader_1.00mm
PinHeader_1x23_P1.00mm_Vertical
Through hole straight pin header, 1x23, 1.00mm pitch, single row
Through hole pin header THT 1x23 1.00mm single row
0
23
23
Connector_PinHeader_1.00mm
PinHeader_1x23_P1.00mm_Vertical_SMD_Pin1Left
surface-mounted straight pin header, 1x23, 1.00mm pitch, single row, style 1 (pin 1 left)
Surface mounted pin header SMD 1x23 1.00mm single row style1 pin1 left
0
23
23
Connector_PinHeader_1.00mm
PinHeader_1x23_P1.00mm_Vertical_SMD_Pin1Right
surface-mounted straight pin header, 1x23, 1.00mm pitch, single row, style 2 (pin 1 right)
Surface mounted pin header SMD 1x23 1.00mm single row style2 pin1 right
0
23
23
Connector_PinHeader_1.00mm
PinHeader_1x24_P1.00mm_Horizontal
Through hole angled pin header, 1x24, 1.00mm pitch, 2.0mm pin length, single row
Through hole angled pin header THT 1x24 1.00mm single row
0
24
24
Connector_PinHeader_1.00mm
PinHeader_1x24_P1.00mm_Vertical
Through hole straight pin header, 1x24, 1.00mm pitch, single row
Through hole pin header THT 1x24 1.00mm single row
0
24
24
Connector_PinHeader_1.00mm
PinHeader_1x24_P1.00mm_Vertical_SMD_Pin1Left
surface-mounted straight pin header, 1x24, 1.00mm pitch, single row, style 1 (pin 1 left)
Surface mounted pin header SMD 1x24 1.00mm single row style1 pin1 left
0
24
24
Connector_PinHeader_1.00mm
PinHeader_1x24_P1.00mm_Vertical_SMD_Pin1Right
surface-mounted straight pin header, 1x24, 1.00mm pitch, single row, style 2 (pin 1 right)
Surface mounted pin header SMD 1x24 1.00mm single row style2 pin1 right
0
24
24
Connector_PinHeader_1.00mm
PinHeader_1x25_P1.00mm_Horizontal
Through hole angled pin header, 1x25, 1.00mm pitch, 2.0mm pin length, single row
Through hole angled pin header THT 1x25 1.00mm single row
0
25
25
Connector_PinHeader_1.00mm
PinHeader_1x25_P1.00mm_Vertical
Through hole straight pin header, 1x25, 1.00mm pitch, single row
Through hole pin header THT 1x25 1.00mm single row
0
25
25
Connector_PinHeader_1.00mm
PinHeader_1x25_P1.00mm_Vertical_SMD_Pin1Left
surface-mounted straight pin header, 1x25, 1.00mm pitch, single row, style 1 (pin 1 left)
Surface mounted pin header SMD 1x25 1.00mm single row style1 pin1 left
0
25
25
Connector_PinHeader_1.00mm
PinHeader_1x25_P1.00mm_Vertical_SMD_Pin1Right
surface-mounted straight pin header, 1x25, 1.00mm pitch, single row, style 2 (pin 1 right)
Surface mounted pin header SMD 1x25 1.00mm single row style2 pin1 right
0
25
25
Connector_PinHeader_1.00mm
PinHeader_1x26_P1.00mm_Horizontal
Through hole angled pin header, 1x26, 1.00mm pitch, 2.0mm pin length, single row
Through hole angled pin header THT 1x26 1.00mm single row
0
26
26
Connector_PinHeader_1.00mm
PinHeader_1x26_P1.00mm_Vertical
Through hole straight pin header, 1x26, 1.00mm pitch, single row
Through hole pin header THT 1x26 1.00mm single row
0
26
26
Connector_PinHeader_1.00mm
PinHeader_1x26_P1.00mm_Vertical_SMD_Pin1Left
surface-mounted straight pin header, 1x26, 1.00mm pitch, single row, style 1 (pin 1 left)
Surface mounted pin header SMD 1x26 1.00mm single row style1 pin1 left
0
26
26
Connector_PinHeader_1.00mm
PinHeader_1x26_P1.00mm_Vertical_SMD_Pin1Right
surface-mounted straight pin header, 1x26, 1.00mm pitch, single row, style 2 (pin 1 right)
Surface mounted pin header SMD 1x26 1.00mm single row style2 pin1 right
0
26
26
Connector_PinHeader_1.00mm
PinHeader_1x27_P1.00mm_Horizontal
Through hole angled pin header, 1x27, 1.00mm pitch, 2.0mm pin length, single row
Through hole angled pin header THT 1x27 1.00mm single row
0
27
27
Connector_PinHeader_1.00mm
PinHeader_1x27_P1.00mm_Vertical
Through hole straight pin header, 1x27, 1.00mm pitch, single row
Through hole pin header THT 1x27 1.00mm single row
0
27
27
Connector_PinHeader_1.00mm
PinHeader_1x27_P1.00mm_Vertical_SMD_Pin1Left
surface-mounted straight pin header, 1x27, 1.00mm pitch, single row, style 1 (pin 1 left)
Surface mounted pin header SMD 1x27 1.00mm single row style1 pin1 left
0
27
27
Connector_PinHeader_1.00mm
PinHeader_1x27_P1.00mm_Vertical_SMD_Pin1Right
surface-mounted straight pin header, 1x27, 1.00mm pitch, single row, style 2 (pin 1 right)
Surface mounted pin header SMD 1x27 1.00mm single row style2 pin1 right
0
27
27
Connector_PinHeader_1.00mm
PinHeader_1x28_P1.00mm_Horizontal
Through hole angled pin header, 1x28, 1.00mm pitch, 2.0mm pin length, single row
Through hole angled pin header THT 1x28 1.00mm single row
0
28
28
Connector_PinHeader_1.00mm
PinHeader_1x28_P1.00mm_Vertical
Through hole straight pin header, 1x28, 1.00mm pitch, single row
Through hole pin header THT 1x28 1.00mm single row
0
28
28
Connector_PinHeader_1.00mm
PinHeader_1x28_P1.00mm_Vertical_SMD_Pin1Left
surface-mounted straight pin header, 1x28, 1.00mm pitch, single row, style 1 (pin 1 left)
Surface mounted pin header SMD 1x28 1.00mm single row style1 pin1 left
0
28
28
Connector_PinHeader_1.00mm
PinHeader_1x28_P1.00mm_Vertical_SMD_Pin1Right
surface-mounted straight pin header, 1x28, 1.00mm pitch, single row, style 2 (pin 1 right)
Surface mounted pin header SMD 1x28 1.00mm single row style2 pin1 right
0
28
28
Connector_PinHeader_1.00mm
PinHeader_1x29_P1.00mm_Horizontal
Through hole angled pin header, 1x29, 1.00mm pitch, 2.0mm pin length, single row
Through hole angled pin header THT 1x29 1.00mm single row
0
29
29
Connector_PinHeader_1.00mm
PinHeader_1x29_P1.00mm_Vertical
Through hole straight pin header, 1x29, 1.00mm pitch, single row
Through hole pin header THT 1x29 1.00mm single row
0
29
29
Connector_PinHeader_1.00mm
PinHeader_1x29_P1.00mm_Vertical_SMD_Pin1Left
surface-mounted straight pin header, 1x29, 1.00mm pitch, single row, style 1 (pin 1 left)
Surface mounted pin header SMD 1x29 1.00mm single row style1 pin1 left
0
29
29
Connector_PinHeader_1.00mm
PinHeader_1x29_P1.00mm_Vertical_SMD_Pin1Right
surface-mounted straight pin header, 1x29, 1.00mm pitch, single row, style 2 (pin 1 right)
Surface mounted pin header SMD 1x29 1.00mm single row style2 pin1 right
0
29
29
Connector_PinHeader_1.00mm
PinHeader_1x30_P1.00mm_Horizontal
Through hole angled pin header, 1x30, 1.00mm pitch, 2.0mm pin length, single row
Through hole angled pin header THT 1x30 1.00mm single row
0
30
30
Connector_PinHeader_1.00mm
PinHeader_1x30_P1.00mm_Vertical
Through hole straight pin header, 1x30, 1.00mm pitch, single row
Through hole pin header THT 1x30 1.00mm single row
0
30
30
Connector_PinHeader_1.00mm
PinHeader_1x30_P1.00mm_Vertical_SMD_Pin1Left
surface-mounted straight pin header, 1x30, 1.00mm pitch, single row, style 1 (pin 1 left)
Surface mounted pin header SMD 1x30 1.00mm single row style1 pin1 left
0
30
30
Connector_PinHeader_1.00mm
PinHeader_1x30_P1.00mm_Vertical_SMD_Pin1Right
surface-mounted straight pin header, 1x30, 1.00mm pitch, single row, style 2 (pin 1 right)
Surface mounted pin header SMD 1x30 1.00mm single row style2 pin1 right
0
30
30
Connector_PinHeader_1.00mm
PinHeader_1x31_P1.00mm_Horizontal
Through hole angled pin header, 1x31, 1.00mm pitch, 2.0mm pin length, single row
Through hole angled pin header THT 1x31 1.00mm single row
0
31
31
Connector_PinHeader_1.00mm
PinHeader_1x31_P1.00mm_Vertical
Through hole straight pin header, 1x31, 1.00mm pitch, single row
Through hole pin header THT 1x31 1.00mm single row
0
31
31
Connector_PinHeader_1.00mm
PinHeader_1x31_P1.00mm_Vertical_SMD_Pin1Left
surface-mounted straight pin header, 1x31, 1.00mm pitch, single row, style 1 (pin 1 left)
Surface mounted pin header SMD 1x31 1.00mm single row style1 pin1 left
0
31
31
Connector_PinHeader_1.00mm
PinHeader_1x31_P1.00mm_Vertical_SMD_Pin1Right
surface-mounted straight pin header, 1x31, 1.00mm pitch, single row, style 2 (pin 1 right)
Surface mounted pin header SMD 1x31 1.00mm single row style2 pin1 right
0
31
31
Connector_PinHeader_1.00mm
PinHeader_1x32_P1.00mm_Horizontal
Through hole angled pin header, 1x32, 1.00mm pitch, 2.0mm pin length, single row
Through hole angled pin header THT 1x32 1.00mm single row
0
32
32
Connector_PinHeader_1.00mm
PinHeader_1x32_P1.00mm_Vertical
Through hole straight pin header, 1x32, 1.00mm pitch, single row
Through hole pin header THT 1x32 1.00mm single row
0
32
32
Connector_PinHeader_1.00mm
PinHeader_1x32_P1.00mm_Vertical_SMD_Pin1Left
surface-mounted straight pin header, 1x32, 1.00mm pitch, single row, style 1 (pin 1 left)
Surface mounted pin header SMD 1x32 1.00mm single row style1 pin1 left
0
32
32
Connector_PinHeader_1.00mm
PinHeader_1x32_P1.00mm_Vertical_SMD_Pin1Right
surface-mounted straight pin header, 1x32, 1.00mm pitch, single row, style 2 (pin 1 right)
Surface mounted pin header SMD 1x32 1.00mm single row style2 pin1 right
0
32
32
Connector_PinHeader_1.00mm
PinHeader_1x33_P1.00mm_Horizontal
Through hole angled pin header, 1x33, 1.00mm pitch, 2.0mm pin length, single row
Through hole angled pin header THT 1x33 1.00mm single row
0
33
33
Connector_PinHeader_1.00mm
PinHeader_1x33_P1.00mm_Vertical
Through hole straight pin header, 1x33, 1.00mm pitch, single row
Through hole pin header THT 1x33 1.00mm single row
0
33
33
Connector_PinHeader_1.00mm
PinHeader_1x33_P1.00mm_Vertical_SMD_Pin1Left
surface-mounted straight pin header, 1x33, 1.00mm pitch, single row, style 1 (pin 1 left)
Surface mounted pin header SMD 1x33 1.00mm single row style1 pin1 left
0
33
33
Connector_PinHeader_1.00mm
PinHeader_1x33_P1.00mm_Vertical_SMD_Pin1Right
surface-mounted straight pin header, 1x33, 1.00mm pitch, single row, style 2 (pin 1 right)
Surface mounted pin header SMD 1x33 1.00mm single row style2 pin1 right
0
33
33
Connector_PinHeader_1.00mm
PinHeader_1x34_P1.00mm_Horizontal
Through hole angled pin header, 1x34, 1.00mm pitch, 2.0mm pin length, single row
Through hole angled pin header THT 1x34 1.00mm single row
0
34
34
Connector_PinHeader_1.00mm
PinHeader_1x34_P1.00mm_Vertical
Through hole straight pin header, 1x34, 1.00mm pitch, single row
Through hole pin header THT 1x34 1.00mm single row
0
34
34
Connector_PinHeader_1.00mm
PinHeader_1x34_P1.00mm_Vertical_SMD_Pin1Left
surface-mounted straight pin header, 1x34, 1.00mm pitch, single row, style 1 (pin 1 left)
Surface mounted pin header SMD 1x34 1.00mm single row style1 pin1 left
0
34
34
Connector_PinHeader_1.00mm
PinHeader_1x34_P1.00mm_Vertical_SMD_Pin1Right
surface-mounted straight pin header, 1x34, 1.00mm pitch, single row, style 2 (pin 1 right)
Surface mounted pin header SMD 1x34 1.00mm single row style2 pin1 right
0
34
34
Connector_PinHeader_1.00mm
PinHeader_1x35_P1.00mm_Horizontal
Through hole angled pin header, 1x35, 1.00mm pitch, 2.0mm pin length, single row
Through hole angled pin header THT 1x35 1.00mm single row
0
35
35
Connector_PinHeader_1.00mm
PinHeader_1x35_P1.00mm_Vertical
Through hole straight pin header, 1x35, 1.00mm pitch, single row
Through hole pin header THT 1x35 1.00mm single row
0
35
35
Connector_PinHeader_1.00mm
PinHeader_1x35_P1.00mm_Vertical_SMD_Pin1Left
surface-mounted straight pin header, 1x35, 1.00mm pitch, single row, style 1 (pin 1 left)
Surface mounted pin header SMD 1x35 1.00mm single row style1 pin1 left
0
35
35
Connector_PinHeader_1.00mm
PinHeader_1x35_P1.00mm_Vertical_SMD_Pin1Right
surface-mounted straight pin header, 1x35, 1.00mm pitch, single row, style 2 (pin 1 right)
Surface mounted pin header SMD 1x35 1.00mm single row style2 pin1 right
0
35
35
Connector_PinHeader_1.00mm
PinHeader_1x36_P1.00mm_Horizontal
Through hole angled pin header, 1x36, 1.00mm pitch, 2.0mm pin length, single row
Through hole angled pin header THT 1x36 1.00mm single row
0
36
36
Connector_PinHeader_1.00mm
PinHeader_1x36_P1.00mm_Vertical
Through hole straight pin header, 1x36, 1.00mm pitch, single row
Through hole pin header THT 1x36 1.00mm single row
0
36
36
Connector_PinHeader_1.00mm
PinHeader_1x36_P1.00mm_Vertical_SMD_Pin1Left
surface-mounted straight pin header, 1x36, 1.00mm pitch, single row, style 1 (pin 1 left)
Surface mounted pin header SMD 1x36 1.00mm single row style1 pin1 left
0
36
36
Connector_PinHeader_1.00mm
PinHeader_1x36_P1.00mm_Vertical_SMD_Pin1Right
surface-mounted straight pin header, 1x36, 1.00mm pitch, single row, style 2 (pin 1 right)
Surface mounted pin header SMD 1x36 1.00mm single row style2 pin1 right
0
36
36
Connector_PinHeader_1.00mm
PinHeader_1x37_P1.00mm_Horizontal
Through hole angled pin header, 1x37, 1.00mm pitch, 2.0mm pin length, single row
Through hole angled pin header THT 1x37 1.00mm single row
0
37
37
Connector_PinHeader_1.00mm
PinHeader_1x37_P1.00mm_Vertical
Through hole straight pin header, 1x37, 1.00mm pitch, single row
Through hole pin header THT 1x37 1.00mm single row
0
37
37
Connector_PinHeader_1.00mm
PinHeader_1x37_P1.00mm_Vertical_SMD_Pin1Left
surface-mounted straight pin header, 1x37, 1.00mm pitch, single row, style 1 (pin 1 left)
Surface mounted pin header SMD 1x37 1.00mm single row style1 pin1 left
0
37
37
Connector_PinHeader_1.00mm
PinHeader_1x37_P1.00mm_Vertical_SMD_Pin1Right
surface-mounted straight pin header, 1x37, 1.00mm pitch, single row, style 2 (pin 1 right)
Surface mounted pin header SMD 1x37 1.00mm single row style2 pin1 right
0
37
37
Connector_PinHeader_1.00mm
PinHeader_1x38_P1.00mm_Horizontal
Through hole angled pin header, 1x38, 1.00mm pitch, 2.0mm pin length, single row
Through hole angled pin header THT 1x38 1.00mm single row
0
38
38
Connector_PinHeader_1.00mm
PinHeader_1x38_P1.00mm_Vertical
Through hole straight pin header, 1x38, 1.00mm pitch, single row
Through hole pin header THT 1x38 1.00mm single row
0
38
38
Connector_PinHeader_1.00mm
PinHeader_1x38_P1.00mm_Vertical_SMD_Pin1Left
surface-mounted straight pin header, 1x38, 1.00mm pitch, single row, style 1 (pin 1 left)
Surface mounted pin header SMD 1x38 1.00mm single row style1 pin1 left
0
38
38
Connector_PinHeader_1.00mm
PinHeader_1x38_P1.00mm_Vertical_SMD_Pin1Right
surface-mounted straight pin header, 1x38, 1.00mm pitch, single row, style 2 (pin 1 right)
Surface mounted pin header SMD 1x38 1.00mm single row style2 pin1 right
0
38
38
Connector_PinHeader_1.00mm
PinHeader_1x39_P1.00mm_Horizontal
Through hole angled pin header, 1x39, 1.00mm pitch, 2.0mm pin length, single row
Through hole angled pin header THT 1x39 1.00mm single row
0
39
39
Connector_PinHeader_1.00mm
PinHeader_1x39_P1.00mm_Vertical
Through hole straight pin header, 1x39, 1.00mm pitch, single row
Through hole pin header THT 1x39 1.00mm single row
0
39
39
Connector_PinHeader_1.00mm
PinHeader_1x39_P1.00mm_Vertical_SMD_Pin1Left
surface-mounted straight pin header, 1x39, 1.00mm pitch, single row, style 1 (pin 1 left)
Surface mounted pin header SMD 1x39 1.00mm single row style1 pin1 left
0
39
39
Connector_PinHeader_1.00mm
PinHeader_1x39_P1.00mm_Vertical_SMD_Pin1Right
surface-mounted straight pin header, 1x39, 1.00mm pitch, single row, style 2 (pin 1 right)
Surface mounted pin header SMD 1x39 1.00mm single row style2 pin1 right
0
39
39
Connector_PinHeader_1.00mm
PinHeader_1x40_P1.00mm_Horizontal
Through hole angled pin header, 1x40, 1.00mm pitch, 2.0mm pin length, single row
Through hole angled pin header THT 1x40 1.00mm single row
0
40
40
Connector_PinHeader_1.00mm
PinHeader_1x40_P1.00mm_Vertical
Through hole straight pin header, 1x40, 1.00mm pitch, single row
Through hole pin header THT 1x40 1.00mm single row
0
40
40
Connector_PinHeader_1.00mm
PinHeader_1x40_P1.00mm_Vertical_SMD_Pin1Left
surface-mounted straight pin header, 1x40, 1.00mm pitch, single row, style 1 (pin 1 left)
Surface mounted pin header SMD 1x40 1.00mm single row style1 pin1 left
0
40
40
Connector_PinHeader_1.00mm
PinHeader_1x40_P1.00mm_Vertical_SMD_Pin1Right
surface-mounted straight pin header, 1x40, 1.00mm pitch, single row, style 2 (pin 1 right)
Surface mounted pin header SMD 1x40 1.00mm single row style2 pin1 right
0
40
40
Connector_PinHeader_1.00mm
PinHeader_2x01_P1.00mm_Horizontal
Through hole angled pin header, 2x01, 1.00mm pitch, 2.0mm pin length, double rows
Through hole angled pin header THT 2x01 1.00mm double row
0
2
2
Connector_PinHeader_1.00mm
PinHeader_2x01_P1.00mm_Vertical
Through hole straight pin header, 2x01, 1.00mm pitch, double rows
Through hole pin header THT 2x01 1.00mm double row
0
2
2
Connector_PinHeader_1.00mm
PinHeader_2x01_P1.00mm_Vertical_SMD
surface-mounted straight pin header, 2x01, 1.00mm pitch, double rows
Surface mounted pin header SMD 2x01 1.00mm double row
0
2
2
Connector_PinHeader_1.00mm
PinHeader_2x02_P1.00mm_Horizontal
Through hole angled pin header, 2x02, 1.00mm pitch, 2.0mm pin length, double rows
Through hole angled pin header THT 2x02 1.00mm double row
0
4
4
Connector_PinHeader_1.00mm
PinHeader_2x02_P1.00mm_Vertical
Through hole straight pin header, 2x02, 1.00mm pitch, double rows
Through hole pin header THT 2x02 1.00mm double row
0
4
4
Connector_PinHeader_1.00mm
PinHeader_2x02_P1.00mm_Vertical_SMD
surface-mounted straight pin header, 2x02, 1.00mm pitch, double rows
Surface mounted pin header SMD 2x02 1.00mm double row
0
4
4
Connector_PinHeader_1.00mm
PinHeader_2x03_P1.00mm_Horizontal
Through hole angled pin header, 2x03, 1.00mm pitch, 2.0mm pin length, double rows
Through hole angled pin header THT 2x03 1.00mm double row
0
6
6
Connector_PinHeader_1.00mm
PinHeader_2x03_P1.00mm_Vertical
Through hole straight pin header, 2x03, 1.00mm pitch, double rows
Through hole pin header THT 2x03 1.00mm double row
0
6
6
Connector_PinHeader_1.00mm
PinHeader_2x03_P1.00mm_Vertical_SMD
surface-mounted straight pin header, 2x03, 1.00mm pitch, double rows
Surface mounted pin header SMD 2x03 1.00mm double row
0
6
6
Connector_PinHeader_1.00mm
PinHeader_2x04_P1.00mm_Horizontal
Through hole angled pin header, 2x04, 1.00mm pitch, 2.0mm pin length, double rows
Through hole angled pin header THT 2x04 1.00mm double row
0
8
8
Connector_PinHeader_1.00mm
PinHeader_2x04_P1.00mm_Vertical
Through hole straight pin header, 2x04, 1.00mm pitch, double rows
Through hole pin header THT 2x04 1.00mm double row
0
8
8
Connector_PinHeader_1.00mm
PinHeader_2x04_P1.00mm_Vertical_SMD
surface-mounted straight pin header, 2x04, 1.00mm pitch, double rows
Surface mounted pin header SMD 2x04 1.00mm double row
0
8
8
Connector_PinHeader_1.00mm
PinHeader_2x05_P1.00mm_Horizontal
Through hole angled pin header, 2x05, 1.00mm pitch, 2.0mm pin length, double rows
Through hole angled pin header THT 2x05 1.00mm double row
0
10
10
Connector_PinHeader_1.00mm
PinHeader_2x05_P1.00mm_Vertical
Through hole straight pin header, 2x05, 1.00mm pitch, double rows
Through hole pin header THT 2x05 1.00mm double row
0
10
10
Connector_PinHeader_1.00mm
PinHeader_2x05_P1.00mm_Vertical_SMD
surface-mounted straight pin header, 2x05, 1.00mm pitch, double rows
Surface mounted pin header SMD 2x05 1.00mm double row
0
10
10
Connector_PinHeader_1.00mm
PinHeader_2x06_P1.00mm_Horizontal
Through hole angled pin header, 2x06, 1.00mm pitch, 2.0mm pin length, double rows
Through hole angled pin header THT 2x06 1.00mm double row
0
12
12
Connector_PinHeader_1.00mm
PinHeader_2x06_P1.00mm_Vertical
Through hole straight pin header, 2x06, 1.00mm pitch, double rows
Through hole pin header THT 2x06 1.00mm double row
0
12
12
Connector_PinHeader_1.00mm
PinHeader_2x06_P1.00mm_Vertical_SMD
surface-mounted straight pin header, 2x06, 1.00mm pitch, double rows
Surface mounted pin header SMD 2x06 1.00mm double row
0
12
12
Connector_PinHeader_1.00mm
PinHeader_2x07_P1.00mm_Horizontal
Through hole angled pin header, 2x07, 1.00mm pitch, 2.0mm pin length, double rows
Through hole angled pin header THT 2x07 1.00mm double row
0
14
14
Connector_PinHeader_1.00mm
PinHeader_2x07_P1.00mm_Vertical
Through hole straight pin header, 2x07, 1.00mm pitch, double rows
Through hole pin header THT 2x07 1.00mm double row
0
14
14
Connector_PinHeader_1.00mm
PinHeader_2x07_P1.00mm_Vertical_SMD
surface-mounted straight pin header, 2x07, 1.00mm pitch, double rows
Surface mounted pin header SMD 2x07 1.00mm double row
0
14
14
Connector_PinHeader_1.00mm
PinHeader_2x08_P1.00mm_Horizontal
Through hole angled pin header, 2x08, 1.00mm pitch, 2.0mm pin length, double rows
Through hole angled pin header THT 2x08 1.00mm double row
0
16
16
Connector_PinHeader_1.00mm
PinHeader_2x08_P1.00mm_Vertical
Through hole straight pin header, 2x08, 1.00mm pitch, double rows
Through hole pin header THT 2x08 1.00mm double row
0
16
16
Connector_PinHeader_1.00mm
PinHeader_2x08_P1.00mm_Vertical_SMD
surface-mounted straight pin header, 2x08, 1.00mm pitch, double rows
Surface mounted pin header SMD 2x08 1.00mm double row
0
16
16
Connector_PinHeader_1.00mm
PinHeader_2x09_P1.00mm_Horizontal
Through hole angled pin header, 2x09, 1.00mm pitch, 2.0mm pin length, double rows
Through hole angled pin header THT 2x09 1.00mm double row
0
18
18
Connector_PinHeader_1.00mm
PinHeader_2x09_P1.00mm_Vertical
Through hole straight pin header, 2x09, 1.00mm pitch, double rows
Through hole pin header THT 2x09 1.00mm double row
0
18
18
Connector_PinHeader_1.00mm
PinHeader_2x09_P1.00mm_Vertical_SMD
surface-mounted straight pin header, 2x09, 1.00mm pitch, double rows
Surface mounted pin header SMD 2x09 1.00mm double row
0
18
18
Connector_PinHeader_1.00mm
PinHeader_2x10_P1.00mm_Horizontal
Through hole angled pin header, 2x10, 1.00mm pitch, 2.0mm pin length, double rows
Through hole angled pin header THT 2x10 1.00mm double row
0
20
20
Connector_PinHeader_1.00mm
PinHeader_2x10_P1.00mm_Vertical
Through hole straight pin header, 2x10, 1.00mm pitch, double rows
Through hole pin header THT 2x10 1.00mm double row
0
20
20
Connector_PinHeader_1.00mm
PinHeader_2x10_P1.00mm_Vertical_SMD
surface-mounted straight pin header, 2x10, 1.00mm pitch, double rows
Surface mounted pin header SMD 2x10 1.00mm double row
0
20
20
Connector_PinHeader_1.00mm
PinHeader_2x11_P1.00mm_Horizontal
Through hole angled pin header, 2x11, 1.00mm pitch, 2.0mm pin length, double rows
Through hole angled pin header THT 2x11 1.00mm double row
0
22
22
Connector_PinHeader_1.00mm
PinHeader_2x11_P1.00mm_Vertical
Through hole straight pin header, 2x11, 1.00mm pitch, double rows
Through hole pin header THT 2x11 1.00mm double row
0
22
22
Connector_PinHeader_1.00mm
PinHeader_2x11_P1.00mm_Vertical_SMD
surface-mounted straight pin header, 2x11, 1.00mm pitch, double rows
Surface mounted pin header SMD 2x11 1.00mm double row
0
22
22
Connector_PinHeader_1.00mm
PinHeader_2x12_P1.00mm_Horizontal
Through hole angled pin header, 2x12, 1.00mm pitch, 2.0mm pin length, double rows
Through hole angled pin header THT 2x12 1.00mm double row
0
24
24
Connector_PinHeader_1.00mm
PinHeader_2x12_P1.00mm_Vertical
Through hole straight pin header, 2x12, 1.00mm pitch, double rows
Through hole pin header THT 2x12 1.00mm double row
0
24
24
Connector_PinHeader_1.00mm
PinHeader_2x12_P1.00mm_Vertical_SMD
surface-mounted straight pin header, 2x12, 1.00mm pitch, double rows
Surface mounted pin header SMD 2x12 1.00mm double row
0
24
24
Connector_PinHeader_1.00mm
PinHeader_2x13_P1.00mm_Horizontal
Through hole angled pin header, 2x13, 1.00mm pitch, 2.0mm pin length, double rows
Through hole angled pin header THT 2x13 1.00mm double row
0
26
26
Connector_PinHeader_1.00mm
PinHeader_2x13_P1.00mm_Vertical
Through hole straight pin header, 2x13, 1.00mm pitch, double rows
Through hole pin header THT 2x13 1.00mm double row
0
26
26
Connector_PinHeader_1.00mm
PinHeader_2x13_P1.00mm_Vertical_SMD
surface-mounted straight pin header, 2x13, 1.00mm pitch, double rows
Surface mounted pin header SMD 2x13 1.00mm double row
0
26
26
Connector_PinHeader_1.00mm
PinHeader_2x14_P1.00mm_Horizontal
Through hole angled pin header, 2x14, 1.00mm pitch, 2.0mm pin length, double rows
Through hole angled pin header THT 2x14 1.00mm double row
0
28
28
Connector_PinHeader_1.00mm
PinHeader_2x14_P1.00mm_Vertical
Through hole straight pin header, 2x14, 1.00mm pitch, double rows
Through hole pin header THT 2x14 1.00mm double row
0
28
28
Connector_PinHeader_1.00mm
PinHeader_2x14_P1.00mm_Vertical_SMD
surface-mounted straight pin header, 2x14, 1.00mm pitch, double rows
Surface mounted pin header SMD 2x14 1.00mm double row
0
28
28
Connector_PinHeader_1.00mm
PinHeader_2x15_P1.00mm_Horizontal
Through hole angled pin header, 2x15, 1.00mm pitch, 2.0mm pin length, double rows
Through hole angled pin header THT 2x15 1.00mm double row
0
30
30
Connector_PinHeader_1.00mm
PinHeader_2x15_P1.00mm_Vertical
Through hole straight pin header, 2x15, 1.00mm pitch, double rows
Through hole pin header THT 2x15 1.00mm double row
0
30
30
Connector_PinHeader_1.00mm
PinHeader_2x15_P1.00mm_Vertical_SMD
surface-mounted straight pin header, 2x15, 1.00mm pitch, double rows
Surface mounted pin header SMD 2x15 1.00mm double row
0
30
30
Connector_PinHeader_1.00mm
PinHeader_2x16_P1.00mm_Horizontal
Through hole angled pin header, 2x16, 1.00mm pitch, 2.0mm pin length, double rows
Through hole angled pin header THT 2x16 1.00mm double row
0
32
32
Connector_PinHeader_1.00mm
PinHeader_2x16_P1.00mm_Vertical
Through hole straight pin header, 2x16, 1.00mm pitch, double rows
Through hole pin header THT 2x16 1.00mm double row
0
32
32
Connector_PinHeader_1.00mm
PinHeader_2x16_P1.00mm_Vertical_SMD
surface-mounted straight pin header, 2x16, 1.00mm pitch, double rows
Surface mounted pin header SMD 2x16 1.00mm double row
0
32
32
Connector_PinHeader_1.00mm
PinHeader_2x17_P1.00mm_Horizontal
Through hole angled pin header, 2x17, 1.00mm pitch, 2.0mm pin length, double rows
Through hole angled pin header THT 2x17 1.00mm double row
0
34
34
Connector_PinHeader_1.00mm
PinHeader_2x17_P1.00mm_Vertical
Through hole straight pin header, 2x17, 1.00mm pitch, double rows
Through hole pin header THT 2x17 1.00mm double row
0
34
34
Connector_PinHeader_1.00mm
PinHeader_2x17_P1.00mm_Vertical_SMD
surface-mounted straight pin header, 2x17, 1.00mm pitch, double rows
Surface mounted pin header SMD 2x17 1.00mm double row
0
34
34
Connector_PinHeader_1.00mm
PinHeader_2x18_P1.00mm_Horizontal
Through hole angled pin header, 2x18, 1.00mm pitch, 2.0mm pin length, double rows
Through hole angled pin header THT 2x18 1.00mm double row
0
36
36
Connector_PinHeader_1.00mm
PinHeader_2x18_P1.00mm_Vertical
Through hole straight pin header, 2x18, 1.00mm pitch, double rows
Through hole pin header THT 2x18 1.00mm double row
0
36
36
Connector_PinHeader_1.00mm
PinHeader_2x18_P1.00mm_Vertical_SMD
surface-mounted straight pin header, 2x18, 1.00mm pitch, double rows
Surface mounted pin header SMD 2x18 1.00mm double row
0
36
36
Connector_PinHeader_1.00mm
PinHeader_2x19_P1.00mm_Horizontal
Through hole angled pin header, 2x19, 1.00mm pitch, 2.0mm pin length, double rows
Through hole angled pin header THT 2x19 1.00mm double row
0
38
38
Connector_PinHeader_1.00mm
PinHeader_2x19_P1.00mm_Vertical
Through hole straight pin header, 2x19, 1.00mm pitch, double rows
Through hole pin header THT 2x19 1.00mm double row
0
38
38
Connector_PinHeader_1.00mm
PinHeader_2x19_P1.00mm_Vertical_SMD
surface-mounted straight pin header, 2x19, 1.00mm pitch, double rows
Surface mounted pin header SMD 2x19 1.00mm double row
0
38
38
Connector_PinHeader_1.00mm
PinHeader_2x20_P1.00mm_Horizontal
Through hole angled pin header, 2x20, 1.00mm pitch, 2.0mm pin length, double rows
Through hole angled pin header THT 2x20 1.00mm double row
0
40
40
Connector_PinHeader_1.00mm
PinHeader_2x20_P1.00mm_Vertical
Through hole straight pin header, 2x20, 1.00mm pitch, double rows
Through hole pin header THT 2x20 1.00mm double row
0
40
40
Connector_PinHeader_1.00mm
PinHeader_2x20_P1.00mm_Vertical_SMD
surface-mounted straight pin header, 2x20, 1.00mm pitch, double rows
Surface mounted pin header SMD 2x20 1.00mm double row
0
40
40
Connector_PinHeader_1.00mm
PinHeader_2x21_P1.00mm_Horizontal
Through hole angled pin header, 2x21, 1.00mm pitch, 2.0mm pin length, double rows
Through hole angled pin header THT 2x21 1.00mm double row
0
42
42
Connector_PinHeader_1.00mm
PinHeader_2x21_P1.00mm_Vertical
Through hole straight pin header, 2x21, 1.00mm pitch, double rows
Through hole pin header THT 2x21 1.00mm double row
0
42
42
Connector_PinHeader_1.00mm
PinHeader_2x21_P1.00mm_Vertical_SMD
surface-mounted straight pin header, 2x21, 1.00mm pitch, double rows
Surface mounted pin header SMD 2x21 1.00mm double row
0
42
42
Connector_PinHeader_1.00mm
PinHeader_2x22_P1.00mm_Horizontal
Through hole angled pin header, 2x22, 1.00mm pitch, 2.0mm pin length, double rows
Through hole angled pin header THT 2x22 1.00mm double row
0
44
44
Connector_PinHeader_1.00mm
PinHeader_2x22_P1.00mm_Vertical
Through hole straight pin header, 2x22, 1.00mm pitch, double rows
Through hole pin header THT 2x22 1.00mm double row
0
44
44
Connector_PinHeader_1.00mm
PinHeader_2x22_P1.00mm_Vertical_SMD
surface-mounted straight pin header, 2x22, 1.00mm pitch, double rows
Surface mounted pin header SMD 2x22 1.00mm double row
0
44
44
Connector_PinHeader_1.00mm
PinHeader_2x23_P1.00mm_Horizontal
Through hole angled pin header, 2x23, 1.00mm pitch, 2.0mm pin length, double rows
Through hole angled pin header THT 2x23 1.00mm double row
0
46
46
Connector_PinHeader_1.00mm
PinHeader_2x23_P1.00mm_Vertical
Through hole straight pin header, 2x23, 1.00mm pitch, double rows
Through hole pin header THT 2x23 1.00mm double row
0
46
46
Connector_PinHeader_1.00mm
PinHeader_2x23_P1.00mm_Vertical_SMD
surface-mounted straight pin header, 2x23, 1.00mm pitch, double rows
Surface mounted pin header SMD 2x23 1.00mm double row
0
46
46
Connector_PinHeader_1.00mm
PinHeader_2x24_P1.00mm_Horizontal
Through hole angled pin header, 2x24, 1.00mm pitch, 2.0mm pin length, double rows
Through hole angled pin header THT 2x24 1.00mm double row
0
48
48
Connector_PinHeader_1.00mm
PinHeader_2x24_P1.00mm_Vertical
Through hole straight pin header, 2x24, 1.00mm pitch, double rows
Through hole pin header THT 2x24 1.00mm double row
0
48
48
Connector_PinHeader_1.00mm
PinHeader_2x24_P1.00mm_Vertical_SMD
surface-mounted straight pin header, 2x24, 1.00mm pitch, double rows
Surface mounted pin header SMD 2x24 1.00mm double row
0
48
48
Connector_PinHeader_1.00mm
PinHeader_2x25_P1.00mm_Horizontal
Through hole angled pin header, 2x25, 1.00mm pitch, 2.0mm pin length, double rows
Through hole angled pin header THT 2x25 1.00mm double row
0
50
50
Connector_PinHeader_1.00mm
PinHeader_2x25_P1.00mm_Vertical
Through hole straight pin header, 2x25, 1.00mm pitch, double rows
Through hole pin header THT 2x25 1.00mm double row
0
50
50
Connector_PinHeader_1.00mm
PinHeader_2x25_P1.00mm_Vertical_SMD
surface-mounted straight pin header, 2x25, 1.00mm pitch, double rows
Surface mounted pin header SMD 2x25 1.00mm double row
0
50
50
Connector_PinHeader_1.00mm
PinHeader_2x26_P1.00mm_Horizontal
Through hole angled pin header, 2x26, 1.00mm pitch, 2.0mm pin length, double rows
Through hole angled pin header THT 2x26 1.00mm double row
0
52
52
Connector_PinHeader_1.00mm
PinHeader_2x26_P1.00mm_Vertical
Through hole straight pin header, 2x26, 1.00mm pitch, double rows
Through hole pin header THT 2x26 1.00mm double row
0
52
52
Connector_PinHeader_1.00mm
PinHeader_2x26_P1.00mm_Vertical_SMD
surface-mounted straight pin header, 2x26, 1.00mm pitch, double rows
Surface mounted pin header SMD 2x26 1.00mm double row
0
52
52
Connector_PinHeader_1.00mm
PinHeader_2x27_P1.00mm_Horizontal
Through hole angled pin header, 2x27, 1.00mm pitch, 2.0mm pin length, double rows
Through hole angled pin header THT 2x27 1.00mm double row
0
54
54
Connector_PinHeader_1.00mm
PinHeader_2x27_P1.00mm_Vertical
Through hole straight pin header, 2x27, 1.00mm pitch, double rows
Through hole pin header THT 2x27 1.00mm double row
0
54
54
Connector_PinHeader_1.00mm
PinHeader_2x27_P1.00mm_Vertical_SMD
surface-mounted straight pin header, 2x27, 1.00mm pitch, double rows
Surface mounted pin header SMD 2x27 1.00mm double row
0
54
54
Connector_PinHeader_1.00mm
PinHeader_2x28_P1.00mm_Horizontal
Through hole angled pin header, 2x28, 1.00mm pitch, 2.0mm pin length, double rows
Through hole angled pin header THT 2x28 1.00mm double row
0
56
56
Connector_PinHeader_1.00mm
PinHeader_2x28_P1.00mm_Vertical
Through hole straight pin header, 2x28, 1.00mm pitch, double rows
Through hole pin header THT 2x28 1.00mm double row
0
56
56
Connector_PinHeader_1.00mm
PinHeader_2x28_P1.00mm_Vertical_SMD
surface-mounted straight pin header, 2x28, 1.00mm pitch, double rows
Surface mounted pin header SMD 2x28 1.00mm double row
0
56
56
Connector_PinHeader_1.00mm
PinHeader_2x29_P1.00mm_Horizontal
Through hole angled pin header, 2x29, 1.00mm pitch, 2.0mm pin length, double rows
Through hole angled pin header THT 2x29 1.00mm double row
0
58
58
Connector_PinHeader_1.00mm
PinHeader_2x29_P1.00mm_Vertical
Through hole straight pin header, 2x29, 1.00mm pitch, double rows
Through hole pin header THT 2x29 1.00mm double row
0
58
58
Connector_PinHeader_1.00mm
PinHeader_2x29_P1.00mm_Vertical_SMD
surface-mounted straight pin header, 2x29, 1.00mm pitch, double rows
Surface mounted pin header SMD 2x29 1.00mm double row
0
58
58
Connector_PinHeader_1.00mm
PinHeader_2x30_P1.00mm_Horizontal
Through hole angled pin header, 2x30, 1.00mm pitch, 2.0mm pin length, double rows
Through hole angled pin header THT 2x30 1.00mm double row
0
60
60
Connector_PinHeader_1.00mm
PinHeader_2x30_P1.00mm_Vertical
Through hole straight pin header, 2x30, 1.00mm pitch, double rows
Through hole pin header THT 2x30 1.00mm double row
0
60
60
Connector_PinHeader_1.00mm
PinHeader_2x30_P1.00mm_Vertical_SMD
surface-mounted straight pin header, 2x30, 1.00mm pitch, double rows
Surface mounted pin header SMD 2x30 1.00mm double row
0
60
60
Connector_PinHeader_1.00mm
PinHeader_2x31_P1.00mm_Horizontal
Through hole angled pin header, 2x31, 1.00mm pitch, 2.0mm pin length, double rows
Through hole angled pin header THT 2x31 1.00mm double row
0
62
62
Connector_PinHeader_1.00mm
PinHeader_2x31_P1.00mm_Vertical
Through hole straight pin header, 2x31, 1.00mm pitch, double rows
Through hole pin header THT 2x31 1.00mm double row
0
62
62
Connector_PinHeader_1.00mm
PinHeader_2x31_P1.00mm_Vertical_SMD
surface-mounted straight pin header, 2x31, 1.00mm pitch, double rows
Surface mounted pin header SMD 2x31 1.00mm double row
0
62
62
Connector_PinHeader_1.00mm
PinHeader_2x32_P1.00mm_Horizontal
Through hole angled pin header, 2x32, 1.00mm pitch, 2.0mm pin length, double rows
Through hole angled pin header THT 2x32 1.00mm double row
0
64
64
Connector_PinHeader_1.00mm
PinHeader_2x32_P1.00mm_Vertical
Through hole straight pin header, 2x32, 1.00mm pitch, double rows
Through hole pin header THT 2x32 1.00mm double row
0
64
64
Connector_PinHeader_1.00mm
PinHeader_2x32_P1.00mm_Vertical_SMD
surface-mounted straight pin header, 2x32, 1.00mm pitch, double rows
Surface mounted pin header SMD 2x32 1.00mm double row
0
64
64
Connector_PinHeader_1.00mm
PinHeader_2x33_P1.00mm_Horizontal
Through hole angled pin header, 2x33, 1.00mm pitch, 2.0mm pin length, double rows
Through hole angled pin header THT 2x33 1.00mm double row
0
66
66
Connector_PinHeader_1.00mm
PinHeader_2x33_P1.00mm_Vertical
Through hole straight pin header, 2x33, 1.00mm pitch, double rows
Through hole pin header THT 2x33 1.00mm double row
0
66
66
Connector_PinHeader_1.00mm
PinHeader_2x33_P1.00mm_Vertical_SMD
surface-mounted straight pin header, 2x33, 1.00mm pitch, double rows
Surface mounted pin header SMD 2x33 1.00mm double row
0
66
66
Connector_PinHeader_1.00mm
PinHeader_2x34_P1.00mm_Horizontal
Through hole angled pin header, 2x34, 1.00mm pitch, 2.0mm pin length, double rows
Through hole angled pin header THT 2x34 1.00mm double row
0
68
68
Connector_PinHeader_1.00mm
PinHeader_2x34_P1.00mm_Vertical
Through hole straight pin header, 2x34, 1.00mm pitch, double rows
Through hole pin header THT 2x34 1.00mm double row
0
68
68
Connector_PinHeader_1.00mm
PinHeader_2x34_P1.00mm_Vertical_SMD
surface-mounted straight pin header, 2x34, 1.00mm pitch, double rows
Surface mounted pin header SMD 2x34 1.00mm double row
0
68
68
Connector_PinHeader_1.00mm
PinHeader_2x35_P1.00mm_Horizontal
Through hole angled pin header, 2x35, 1.00mm pitch, 2.0mm pin length, double rows
Through hole angled pin header THT 2x35 1.00mm double row
0
70
70
Connector_PinHeader_1.00mm
PinHeader_2x35_P1.00mm_Vertical
Through hole straight pin header, 2x35, 1.00mm pitch, double rows
Through hole pin header THT 2x35 1.00mm double row
0
70
70
Connector_PinHeader_1.00mm
PinHeader_2x35_P1.00mm_Vertical_SMD
surface-mounted straight pin header, 2x35, 1.00mm pitch, double rows
Surface mounted pin header SMD 2x35 1.00mm double row
0
70
70
Connector_PinHeader_1.00mm
PinHeader_2x36_P1.00mm_Horizontal
Through hole angled pin header, 2x36, 1.00mm pitch, 2.0mm pin length, double rows
Through hole angled pin header THT 2x36 1.00mm double row
0
72
72
Connector_PinHeader_1.00mm
PinHeader_2x36_P1.00mm_Vertical
Through hole straight pin header, 2x36, 1.00mm pitch, double rows
Through hole pin header THT 2x36 1.00mm double row
0
72
72
Connector_PinHeader_1.00mm
PinHeader_2x36_P1.00mm_Vertical_SMD
surface-mounted straight pin header, 2x36, 1.00mm pitch, double rows
Surface mounted pin header SMD 2x36 1.00mm double row
0
72
72
Connector_PinHeader_1.00mm
PinHeader_2x37_P1.00mm_Horizontal
Through hole angled pin header, 2x37, 1.00mm pitch, 2.0mm pin length, double rows
Through hole angled pin header THT 2x37 1.00mm double row
0
74
74
Connector_PinHeader_1.00mm
PinHeader_2x37_P1.00mm_Vertical
Through hole straight pin header, 2x37, 1.00mm pitch, double rows
Through hole pin header THT 2x37 1.00mm double row
0
74
74
Connector_PinHeader_1.00mm
PinHeader_2x37_P1.00mm_Vertical_SMD
surface-mounted straight pin header, 2x37, 1.00mm pitch, double rows
Surface mounted pin header SMD 2x37 1.00mm double row
0
74
74
Connector_PinHeader_1.00mm
PinHeader_2x38_P1.00mm_Horizontal
Through hole angled pin header, 2x38, 1.00mm pitch, 2.0mm pin length, double rows
Through hole angled pin header THT 2x38 1.00mm double row
0
76
76
Connector_PinHeader_1.00mm
PinHeader_2x38_P1.00mm_Vertical
Through hole straight pin header, 2x38, 1.00mm pitch, double rows
Through hole pin header THT 2x38 1.00mm double row
0
76
76
Connector_PinHeader_1.00mm
PinHeader_2x38_P1.00mm_Vertical_SMD
surface-mounted straight pin header, 2x38, 1.00mm pitch, double rows
Surface mounted pin header SMD 2x38 1.00mm double row
0
76
76
Connector_PinHeader_1.00mm
PinHeader_2x39_P1.00mm_Horizontal
Through hole angled pin header, 2x39, 1.00mm pitch, 2.0mm pin length, double rows
Through hole angled pin header THT 2x39 1.00mm double row
0
78
78
Connector_PinHeader_1.00mm
PinHeader_2x39_P1.00mm_Vertical
Through hole straight pin header, 2x39, 1.00mm pitch, double rows
Through hole pin header THT 2x39 1.00mm double row
0
78
78
Connector_PinHeader_1.00mm
PinHeader_2x39_P1.00mm_Vertical_SMD
surface-mounted straight pin header, 2x39, 1.00mm pitch, double rows
Surface mounted pin header SMD 2x39 1.00mm double row
0
78
78
Connector_PinHeader_1.00mm
PinHeader_2x40_P1.00mm_Horizontal
Through hole angled pin header, 2x40, 1.00mm pitch, 2.0mm pin length, double rows
Through hole angled pin header THT 2x40 1.00mm double row
0
80
80
Connector_PinHeader_1.00mm
PinHeader_2x40_P1.00mm_Vertical
Through hole straight pin header, 2x40, 1.00mm pitch, double rows
Through hole pin header THT 2x40 1.00mm double row
0
80
80
Connector_PinHeader_1.00mm
PinHeader_2x40_P1.00mm_Vertical_SMD
surface-mounted straight pin header, 2x40, 1.00mm pitch, double rows
Surface mounted pin header SMD 2x40 1.00mm double row
0
80
80
Connector_PinSocket_1.00mm
PinSocket_1x02_P1.00mm_Vertical
Through hole straight socket strip, 1x02, 1.00mm pitch, single row (https://gct.co/files/drawings/bc065.pdf), script generated
Through hole socket strip THT 1x02 1.00mm single row
0
2
2
Connector_PinSocket_1.00mm
PinSocket_1x02_P1.00mm_Vertical_SMD_Pin1Left
surface-mounted straight socket strip, 1x02, 1.00mm pitch, single row, style 1 (pin 1 left) (https://gct.co/files/drawings/bc070.pdf), script generated
Surface mounted socket strip SMD 1x02 1.00mm single row style1 pin1 left
0
2
2
Connector_PinSocket_1.00mm
PinSocket_1x02_P1.00mm_Vertical_SMD_Pin1Right
surface-mounted straight socket strip, 1x02, 1.00mm pitch, single row, style 2 (pin 1 right) (https://gct.co/files/drawings/bc070.pdf), script generated
Surface mounted socket strip SMD 1x02 1.00mm single row style2 pin1 right
0
2
2
Connector_PinSocket_1.00mm
PinSocket_1x03_P1.00mm_Vertical
Through hole straight socket strip, 1x03, 1.00mm pitch, single row (https://gct.co/files/drawings/bc065.pdf), script generated
Through hole socket strip THT 1x03 1.00mm single row
0
3
3
Connector_PinSocket_1.00mm
PinSocket_1x03_P1.00mm_Vertical_SMD_Pin1Left
surface-mounted straight socket strip, 1x03, 1.00mm pitch, single row, style 1 (pin 1 left) (https://gct.co/files/drawings/bc070.pdf), script generated
Surface mounted socket strip SMD 1x03 1.00mm single row style1 pin1 left
0
3
3
Connector_PinSocket_1.00mm
PinSocket_1x03_P1.00mm_Vertical_SMD_Pin1Right
surface-mounted straight socket strip, 1x03, 1.00mm pitch, single row, style 2 (pin 1 right) (https://gct.co/files/drawings/bc070.pdf), script generated
Surface mounted socket strip SMD 1x03 1.00mm single row style2 pin1 right
0
3
3
Connector_PinSocket_1.00mm
PinSocket_1x04_P1.00mm_Vertical
Through hole straight socket strip, 1x04, 1.00mm pitch, single row (https://gct.co/files/drawings/bc065.pdf), script generated
Through hole socket strip THT 1x04 1.00mm single row
0
4
4
Connector_PinSocket_1.00mm
PinSocket_1x04_P1.00mm_Vertical_SMD_Pin1Left
surface-mounted straight socket strip, 1x04, 1.00mm pitch, single row, style 1 (pin 1 left) (https://gct.co/files/drawings/bc070.pdf), script generated
Surface mounted socket strip SMD 1x04 1.00mm single row style1 pin1 left
0
4
4
Connector_PinSocket_1.00mm
PinSocket_1x04_P1.00mm_Vertical_SMD_Pin1Right
surface-mounted straight socket strip, 1x04, 1.00mm pitch, single row, style 2 (pin 1 right) (https://gct.co/files/drawings/bc070.pdf), script generated
Surface mounted socket strip SMD 1x04 1.00mm single row style2 pin1 right
0
4
4
Connector_PinSocket_1.00mm
PinSocket_1x05_P1.00mm_Vertical
Through hole straight socket strip, 1x05, 1.00mm pitch, single row (https://gct.co/files/drawings/bc065.pdf), script generated
Through hole socket strip THT 1x05 1.00mm single row
0
5
5
Connector_PinSocket_1.00mm
PinSocket_1x05_P1.00mm_Vertical_SMD_Pin1Left
surface-mounted straight socket strip, 1x05, 1.00mm pitch, single row, style 1 (pin 1 left) (https://gct.co/files/drawings/bc070.pdf), script generated
Surface mounted socket strip SMD 1x05 1.00mm single row style1 pin1 left
0
5
5
Connector_PinSocket_1.00mm
PinSocket_1x05_P1.00mm_Vertical_SMD_Pin1Right
surface-mounted straight socket strip, 1x05, 1.00mm pitch, single row, style 2 (pin 1 right) (https://gct.co/files/drawings/bc070.pdf), script generated
Surface mounted socket strip SMD 1x05 1.00mm single row style2 pin1 right
0
5
5
Connector_PinSocket_1.00mm
PinSocket_1x06_P1.00mm_Vertical
Through hole straight socket strip, 1x06, 1.00mm pitch, single row (https://gct.co/files/drawings/bc065.pdf), script generated
Through hole socket strip THT 1x06 1.00mm single row
0
6
6
Connector_PinSocket_1.00mm
PinSocket_1x06_P1.00mm_Vertical_SMD_Pin1Left
surface-mounted straight socket strip, 1x06, 1.00mm pitch, single row, style 1 (pin 1 left) (https://gct.co/files/drawings/bc070.pdf), script generated
Surface mounted socket strip SMD 1x06 1.00mm single row style1 pin1 left
0
6
6
Connector_PinSocket_1.00mm
PinSocket_1x06_P1.00mm_Vertical_SMD_Pin1Right
surface-mounted straight socket strip, 1x06, 1.00mm pitch, single row, style 2 (pin 1 right) (https://gct.co/files/drawings/bc070.pdf), script generated
Surface mounted socket strip SMD 1x06 1.00mm single row style2 pin1 right
0
6
6
Connector_PinSocket_1.00mm
PinSocket_1x07_P1.00mm_Vertical
Through hole straight socket strip, 1x07, 1.00mm pitch, single row (https://gct.co/files/drawings/bc065.pdf), script generated
Through hole socket strip THT 1x07 1.00mm single row
0
7
7
Connector_PinSocket_1.00mm
PinSocket_1x07_P1.00mm_Vertical_SMD_Pin1Left
surface-mounted straight socket strip, 1x07, 1.00mm pitch, single row, style 1 (pin 1 left) (https://gct.co/files/drawings/bc070.pdf), script generated
Surface mounted socket strip SMD 1x07 1.00mm single row style1 pin1 left
0
7
7
Connector_PinSocket_1.00mm
PinSocket_1x07_P1.00mm_Vertical_SMD_Pin1Right
surface-mounted straight socket strip, 1x07, 1.00mm pitch, single row, style 2 (pin 1 right) (https://gct.co/files/drawings/bc070.pdf), script generated
Surface mounted socket strip SMD 1x07 1.00mm single row style2 pin1 right
0
7
7
Connector_PinSocket_1.00mm
PinSocket_1x08_P1.00mm_Vertical
Through hole straight socket strip, 1x08, 1.00mm pitch, single row (https://gct.co/files/drawings/bc065.pdf), script generated
Through hole socket strip THT 1x08 1.00mm single row
0
8
8
Connector_PinSocket_1.00mm
PinSocket_1x08_P1.00mm_Vertical_SMD_Pin1Left
surface-mounted straight socket strip, 1x08, 1.00mm pitch, single row, style 1 (pin 1 left) (https://gct.co/files/drawings/bc070.pdf), script generated
Surface mounted socket strip SMD 1x08 1.00mm single row style1 pin1 left
0
8
8
Connector_PinSocket_1.00mm
PinSocket_1x08_P1.00mm_Vertical_SMD_Pin1Right
surface-mounted straight socket strip, 1x08, 1.00mm pitch, single row, style 2 (pin 1 right) (https://gct.co/files/drawings/bc070.pdf), script generated
Surface mounted socket strip SMD 1x08 1.00mm single row style2 pin1 right
0
8
8
Connector_PinSocket_1.00mm
PinSocket_1x09_P1.00mm_Vertical
Through hole straight socket strip, 1x09, 1.00mm pitch, single row (https://gct.co/files/drawings/bc065.pdf), script generated
Through hole socket strip THT 1x09 1.00mm single row
0
9
9
Connector_PinSocket_1.00mm
PinSocket_1x09_P1.00mm_Vertical_SMD_Pin1Left
surface-mounted straight socket strip, 1x09, 1.00mm pitch, single row, style 1 (pin 1 left) (https://gct.co/files/drawings/bc070.pdf), script generated
Surface mounted socket strip SMD 1x09 1.00mm single row style1 pin1 left
0
9
9
Connector_PinSocket_1.00mm
PinSocket_1x09_P1.00mm_Vertical_SMD_Pin1Right
surface-mounted straight socket strip, 1x09, 1.00mm pitch, single row, style 2 (pin 1 right) (https://gct.co/files/drawings/bc070.pdf), script generated
Surface mounted socket strip SMD 1x09 1.00mm single row style2 pin1 right
0
9
9
Connector_PinSocket_1.00mm
PinSocket_1x10_P1.00mm_Vertical
Through hole straight socket strip, 1x10, 1.00mm pitch, single row (https://gct.co/files/drawings/bc065.pdf), script generated
Through hole socket strip THT 1x10 1.00mm single row
0
10
10
Connector_PinSocket_1.00mm
PinSocket_1x10_P1.00mm_Vertical_SMD_Pin1Left
surface-mounted straight socket strip, 1x10, 1.00mm pitch, single row, style 1 (pin 1 left) (https://gct.co/files/drawings/bc070.pdf), script generated
Surface mounted socket strip SMD 1x10 1.00mm single row style1 pin1 left
0
10
10
Connector_PinSocket_1.00mm
PinSocket_1x10_P1.00mm_Vertical_SMD_Pin1Right
surface-mounted straight socket strip, 1x10, 1.00mm pitch, single row, style 2 (pin 1 right) (https://gct.co/files/drawings/bc070.pdf), script generated
Surface mounted socket strip SMD 1x10 1.00mm single row style2 pin1 right
0
10
10
Connector_PinSocket_1.00mm
PinSocket_1x11_P1.00mm_Vertical
Through hole straight socket strip, 1x11, 1.00mm pitch, single row (https://gct.co/files/drawings/bc065.pdf), script generated
Through hole socket strip THT 1x11 1.00mm single row
0
11
11
Connector_PinSocket_1.00mm
PinSocket_1x11_P1.00mm_Vertical_SMD_Pin1Left
surface-mounted straight socket strip, 1x11, 1.00mm pitch, single row, style 1 (pin 1 left) (https://gct.co/files/drawings/bc070.pdf), script generated
Surface mounted socket strip SMD 1x11 1.00mm single row style1 pin1 left
0
11
11
Connector_PinSocket_1.00mm
PinSocket_1x11_P1.00mm_Vertical_SMD_Pin1Right
surface-mounted straight socket strip, 1x11, 1.00mm pitch, single row, style 2 (pin 1 right) (https://gct.co/files/drawings/bc070.pdf), script generated
Surface mounted socket strip SMD 1x11 1.00mm single row style2 pin1 right
0
11
11
Connector_PinSocket_1.00mm
PinSocket_1x12_P1.00mm_Vertical
Through hole straight socket strip, 1x12, 1.00mm pitch, single row (https://gct.co/files/drawings/bc065.pdf), script generated
Through hole socket strip THT 1x12 1.00mm single row
0
12
12
Connector_PinSocket_1.00mm
PinSocket_1x12_P1.00mm_Vertical_SMD_Pin1Left
surface-mounted straight socket strip, 1x12, 1.00mm pitch, single row, style 1 (pin 1 left) (https://gct.co/files/drawings/bc070.pdf), script generated
Surface mounted socket strip SMD 1x12 1.00mm single row style1 pin1 left
0
12
12
Connector_PinSocket_1.00mm
PinSocket_1x12_P1.00mm_Vertical_SMD_Pin1Right
surface-mounted straight socket strip, 1x12, 1.00mm pitch, single row, style 2 (pin 1 right) (https://gct.co/files/drawings/bc070.pdf), script generated
Surface mounted socket strip SMD 1x12 1.00mm single row style2 pin1 right
0
12
12
Connector_PinSocket_1.00mm
PinSocket_1x13_P1.00mm_Vertical
Through hole straight socket strip, 1x13, 1.00mm pitch, single row (https://gct.co/files/drawings/bc065.pdf), script generated
Through hole socket strip THT 1x13 1.00mm single row
0
13
13
Connector_PinSocket_1.00mm
PinSocket_1x13_P1.00mm_Vertical_SMD_Pin1Left
surface-mounted straight socket strip, 1x13, 1.00mm pitch, single row, style 1 (pin 1 left) (https://gct.co/files/drawings/bc070.pdf), script generated
Surface mounted socket strip SMD 1x13 1.00mm single row style1 pin1 left
0
13
13
Connector_PinSocket_1.00mm
PinSocket_1x13_P1.00mm_Vertical_SMD_Pin1Right
surface-mounted straight socket strip, 1x13, 1.00mm pitch, single row, style 2 (pin 1 right) (https://gct.co/files/drawings/bc070.pdf), script generated
Surface mounted socket strip SMD 1x13 1.00mm single row style2 pin1 right
0
13
13
Connector_PinSocket_1.00mm
PinSocket_1x14_P1.00mm_Vertical
Through hole straight socket strip, 1x14, 1.00mm pitch, single row (https://gct.co/files/drawings/bc065.pdf), script generated
Through hole socket strip THT 1x14 1.00mm single row
0
14
14
Connector_PinSocket_1.00mm
PinSocket_1x14_P1.00mm_Vertical_SMD_Pin1Left
surface-mounted straight socket strip, 1x14, 1.00mm pitch, single row, style 1 (pin 1 left) (https://gct.co/files/drawings/bc070.pdf), script generated
Surface mounted socket strip SMD 1x14 1.00mm single row style1 pin1 left
0
14
14
Connector_PinSocket_1.00mm
PinSocket_1x14_P1.00mm_Vertical_SMD_Pin1Right
surface-mounted straight socket strip, 1x14, 1.00mm pitch, single row, style 2 (pin 1 right) (https://gct.co/files/drawings/bc070.pdf), script generated
Surface mounted socket strip SMD 1x14 1.00mm single row style2 pin1 right
0
14
14
Connector_PinSocket_1.00mm
PinSocket_1x15_P1.00mm_Vertical
Through hole straight socket strip, 1x15, 1.00mm pitch, single row (https://gct.co/files/drawings/bc065.pdf), script generated
Through hole socket strip THT 1x15 1.00mm single row
0
15
15
Connector_PinSocket_1.00mm
PinSocket_1x15_P1.00mm_Vertical_SMD_Pin1Left
surface-mounted straight socket strip, 1x15, 1.00mm pitch, single row, style 1 (pin 1 left) (https://gct.co/files/drawings/bc070.pdf), script generated
Surface mounted socket strip SMD 1x15 1.00mm single row style1 pin1 left
0
15
15
Connector_PinSocket_1.00mm
PinSocket_1x15_P1.00mm_Vertical_SMD_Pin1Right
surface-mounted straight socket strip, 1x15, 1.00mm pitch, single row, style 2 (pin 1 right) (https://gct.co/files/drawings/bc070.pdf), script generated
Surface mounted socket strip SMD 1x15 1.00mm single row style2 pin1 right
0
15
15
Connector_PinSocket_1.00mm
PinSocket_1x16_P1.00mm_Vertical
Through hole straight socket strip, 1x16, 1.00mm pitch, single row (https://gct.co/files/drawings/bc065.pdf), script generated
Through hole socket strip THT 1x16 1.00mm single row
0
16
16
Connector_PinSocket_1.00mm
PinSocket_1x16_P1.00mm_Vertical_SMD_Pin1Left
surface-mounted straight socket strip, 1x16, 1.00mm pitch, single row, style 1 (pin 1 left) (https://gct.co/files/drawings/bc070.pdf), script generated
Surface mounted socket strip SMD 1x16 1.00mm single row style1 pin1 left
0
16
16
Connector_PinSocket_1.00mm
PinSocket_1x16_P1.00mm_Vertical_SMD_Pin1Right
surface-mounted straight socket strip, 1x16, 1.00mm pitch, single row, style 2 (pin 1 right) (https://gct.co/files/drawings/bc070.pdf), script generated
Surface mounted socket strip SMD 1x16 1.00mm single row style2 pin1 right
0
16
16
Connector_PinSocket_1.00mm
PinSocket_1x17_P1.00mm_Vertical
Through hole straight socket strip, 1x17, 1.00mm pitch, single row (https://gct.co/files/drawings/bc065.pdf), script generated
Through hole socket strip THT 1x17 1.00mm single row
0
17
17
Connector_PinSocket_1.00mm
PinSocket_1x17_P1.00mm_Vertical_SMD_Pin1Left
surface-mounted straight socket strip, 1x17, 1.00mm pitch, single row, style 1 (pin 1 left) (https://gct.co/files/drawings/bc070.pdf), script generated
Surface mounted socket strip SMD 1x17 1.00mm single row style1 pin1 left
0
17
17
Connector_PinSocket_1.00mm
PinSocket_1x17_P1.00mm_Vertical_SMD_Pin1Right
surface-mounted straight socket strip, 1x17, 1.00mm pitch, single row, style 2 (pin 1 right) (https://gct.co/files/drawings/bc070.pdf), script generated
Surface mounted socket strip SMD 1x17 1.00mm single row style2 pin1 right
0
17
17
Connector_PinSocket_1.00mm
PinSocket_1x18_P1.00mm_Vertical
Through hole straight socket strip, 1x18, 1.00mm pitch, single row (https://gct.co/files/drawings/bc065.pdf), script generated
Through hole socket strip THT 1x18 1.00mm single row
0
18
18
Connector_PinSocket_1.00mm
PinSocket_1x18_P1.00mm_Vertical_SMD_Pin1Left
surface-mounted straight socket strip, 1x18, 1.00mm pitch, single row, style 1 (pin 1 left) (https://gct.co/files/drawings/bc070.pdf), script generated
Surface mounted socket strip SMD 1x18 1.00mm single row style1 pin1 left
0
18
18
Connector_PinSocket_1.00mm
PinSocket_1x18_P1.00mm_Vertical_SMD_Pin1Right
surface-mounted straight socket strip, 1x18, 1.00mm pitch, single row, style 2 (pin 1 right) (https://gct.co/files/drawings/bc070.pdf), script generated
Surface mounted socket strip SMD 1x18 1.00mm single row style2 pin1 right
0
18
18
Connector_PinSocket_1.00mm
PinSocket_1x19_P1.00mm_Vertical
Through hole straight socket strip, 1x19, 1.00mm pitch, single row (https://gct.co/files/drawings/bc065.pdf), script generated
Through hole socket strip THT 1x19 1.00mm single row
0
19
19
Connector_PinSocket_1.00mm
PinSocket_1x19_P1.00mm_Vertical_SMD_Pin1Left
surface-mounted straight socket strip, 1x19, 1.00mm pitch, single row, style 1 (pin 1 left) (https://gct.co/files/drawings/bc070.pdf), script generated
Surface mounted socket strip SMD 1x19 1.00mm single row style1 pin1 left
0
19
19
Connector_PinSocket_1.00mm
PinSocket_1x19_P1.00mm_Vertical_SMD_Pin1Right
surface-mounted straight socket strip, 1x19, 1.00mm pitch, single row, style 2 (pin 1 right) (https://gct.co/files/drawings/bc070.pdf), script generated
Surface mounted socket strip SMD 1x19 1.00mm single row style2 pin1 right
0
19
19
Connector_PinSocket_1.00mm
PinSocket_1x20_P1.00mm_Vertical
Through hole straight socket strip, 1x20, 1.00mm pitch, single row (https://gct.co/files/drawings/bc065.pdf), script generated
Through hole socket strip THT 1x20 1.00mm single row
0
20
20
Connector_PinSocket_1.00mm
PinSocket_1x20_P1.00mm_Vertical_SMD_Pin1Left
surface-mounted straight socket strip, 1x20, 1.00mm pitch, single row, style 1 (pin 1 left) (https://gct.co/files/drawings/bc070.pdf), script generated
Surface mounted socket strip SMD 1x20 1.00mm single row style1 pin1 left
0
20
20
Connector_PinSocket_1.00mm
PinSocket_1x20_P1.00mm_Vertical_SMD_Pin1Right
surface-mounted straight socket strip, 1x20, 1.00mm pitch, single row, style 2 (pin 1 right) (https://gct.co/files/drawings/bc070.pdf), script generated
Surface mounted socket strip SMD 1x20 1.00mm single row style2 pin1 right
0
20
20
Connector_PinSocket_1.00mm
PinSocket_1x21_P1.00mm_Vertical
Through hole straight socket strip, 1x21, 1.00mm pitch, single row (https://gct.co/files/drawings/bc065.pdf), script generated
Through hole socket strip THT 1x21 1.00mm single row
0
21
21
Connector_PinSocket_1.00mm
PinSocket_1x21_P1.00mm_Vertical_SMD_Pin1Left
surface-mounted straight socket strip, 1x21, 1.00mm pitch, single row, style 1 (pin 1 left) (https://gct.co/files/drawings/bc070.pdf), script generated
Surface mounted socket strip SMD 1x21 1.00mm single row style1 pin1 left
0
21
21
Connector_PinSocket_1.00mm
PinSocket_1x21_P1.00mm_Vertical_SMD_Pin1Right
surface-mounted straight socket strip, 1x21, 1.00mm pitch, single row, style 2 (pin 1 right) (https://gct.co/files/drawings/bc070.pdf), script generated
Surface mounted socket strip SMD 1x21 1.00mm single row style2 pin1 right
0
21
21
Connector_PinSocket_1.00mm
PinSocket_1x22_P1.00mm_Vertical
Through hole straight socket strip, 1x22, 1.00mm pitch, single row (https://gct.co/files/drawings/bc065.pdf), script generated
Through hole socket strip THT 1x22 1.00mm single row
0
22
22
Connector_PinSocket_1.00mm
PinSocket_1x22_P1.00mm_Vertical_SMD_Pin1Left
surface-mounted straight socket strip, 1x22, 1.00mm pitch, single row, style 1 (pin 1 left) (https://gct.co/files/drawings/bc070.pdf), script generated
Surface mounted socket strip SMD 1x22 1.00mm single row style1 pin1 left
0
22
22
Connector_PinSocket_1.00mm
PinSocket_1x22_P1.00mm_Vertical_SMD_Pin1Right
surface-mounted straight socket strip, 1x22, 1.00mm pitch, single row, style 2 (pin 1 right) (https://gct.co/files/drawings/bc070.pdf), script generated
Surface mounted socket strip SMD 1x22 1.00mm single row style2 pin1 right
0
22
22
Connector_PinSocket_1.00mm
PinSocket_1x23_P1.00mm_Vertical
Through hole straight socket strip, 1x23, 1.00mm pitch, single row (https://gct.co/files/drawings/bc065.pdf), script generated
Through hole socket strip THT 1x23 1.00mm single row
0
23
23
Connector_PinSocket_1.00mm
PinSocket_1x23_P1.00mm_Vertical_SMD_Pin1Left
surface-mounted straight socket strip, 1x23, 1.00mm pitch, single row, style 1 (pin 1 left) (https://gct.co/files/drawings/bc070.pdf), script generated
Surface mounted socket strip SMD 1x23 1.00mm single row style1 pin1 left
0
23
23
Connector_PinSocket_1.00mm
PinSocket_1x23_P1.00mm_Vertical_SMD_Pin1Right
surface-mounted straight socket strip, 1x23, 1.00mm pitch, single row, style 2 (pin 1 right) (https://gct.co/files/drawings/bc070.pdf), script generated
Surface mounted socket strip SMD 1x23 1.00mm single row style2 pin1 right
0
23
23
Connector_PinSocket_1.00mm
PinSocket_1x24_P1.00mm_Vertical
Through hole straight socket strip, 1x24, 1.00mm pitch, single row (https://gct.co/files/drawings/bc065.pdf), script generated
Through hole socket strip THT 1x24 1.00mm single row
0
24
24
Connector_PinSocket_1.00mm
PinSocket_1x24_P1.00mm_Vertical_SMD_Pin1Left
surface-mounted straight socket strip, 1x24, 1.00mm pitch, single row, style 1 (pin 1 left) (https://gct.co/files/drawings/bc070.pdf), script generated
Surface mounted socket strip SMD 1x24 1.00mm single row style1 pin1 left
0
24
24
Connector_PinSocket_1.00mm
PinSocket_1x24_P1.00mm_Vertical_SMD_Pin1Right
surface-mounted straight socket strip, 1x24, 1.00mm pitch, single row, style 2 (pin 1 right) (https://gct.co/files/drawings/bc070.pdf), script generated
Surface mounted socket strip SMD 1x24 1.00mm single row style2 pin1 right
0
24
24
Connector_PinSocket_1.00mm
PinSocket_1x25_P1.00mm_Vertical
Through hole straight socket strip, 1x25, 1.00mm pitch, single row (https://gct.co/files/drawings/bc065.pdf), script generated
Through hole socket strip THT 1x25 1.00mm single row
0
25
25
Connector_PinSocket_1.00mm
PinSocket_1x25_P1.00mm_Vertical_SMD_Pin1Left
surface-mounted straight socket strip, 1x25, 1.00mm pitch, single row, style 1 (pin 1 left) (https://gct.co/files/drawings/bc070.pdf), script generated
Surface mounted socket strip SMD 1x25 1.00mm single row style1 pin1 left
0
25
25
Connector_PinSocket_1.00mm
PinSocket_1x25_P1.00mm_Vertical_SMD_Pin1Right
surface-mounted straight socket strip, 1x25, 1.00mm pitch, single row, style 2 (pin 1 right) (https://gct.co/files/drawings/bc070.pdf), script generated
Surface mounted socket strip SMD 1x25 1.00mm single row style2 pin1 right
0
25
25
Connector_PinSocket_1.00mm
PinSocket_1x26_P1.00mm_Vertical
Through hole straight socket strip, 1x26, 1.00mm pitch, single row (https://gct.co/files/drawings/bc065.pdf), script generated
Through hole socket strip THT 1x26 1.00mm single row
0
26
26
Connector_PinSocket_1.00mm
PinSocket_1x26_P1.00mm_Vertical_SMD_Pin1Left
surface-mounted straight socket strip, 1x26, 1.00mm pitch, single row, style 1 (pin 1 left) (https://gct.co/files/drawings/bc070.pdf), script generated
Surface mounted socket strip SMD 1x26 1.00mm single row style1 pin1 left
0
26
26
Connector_PinSocket_1.00mm
PinSocket_1x26_P1.00mm_Vertical_SMD_Pin1Right
surface-mounted straight socket strip, 1x26, 1.00mm pitch, single row, style 2 (pin 1 right) (https://gct.co/files/drawings/bc070.pdf), script generated
Surface mounted socket strip SMD 1x26 1.00mm single row style2 pin1 right
0
26
26
Connector_PinSocket_1.00mm
PinSocket_1x27_P1.00mm_Vertical
Through hole straight socket strip, 1x27, 1.00mm pitch, single row (https://gct.co/files/drawings/bc065.pdf), script generated
Through hole socket strip THT 1x27 1.00mm single row
0
27
27
Connector_PinSocket_1.00mm
PinSocket_1x27_P1.00mm_Vertical_SMD_Pin1Left
surface-mounted straight socket strip, 1x27, 1.00mm pitch, single row, style 1 (pin 1 left) (https://gct.co/files/drawings/bc070.pdf), script generated
Surface mounted socket strip SMD 1x27 1.00mm single row style1 pin1 left
0
27
27
Connector_PinSocket_1.00mm
PinSocket_1x27_P1.00mm_Vertical_SMD_Pin1Right
surface-mounted straight socket strip, 1x27, 1.00mm pitch, single row, style 2 (pin 1 right) (https://gct.co/files/drawings/bc070.pdf), script generated
Surface mounted socket strip SMD 1x27 1.00mm single row style2 pin1 right
0
27
27
Connector_PinSocket_1.00mm
PinSocket_1x28_P1.00mm_Vertical
Through hole straight socket strip, 1x28, 1.00mm pitch, single row (https://gct.co/files/drawings/bc065.pdf), script generated
Through hole socket strip THT 1x28 1.00mm single row
0
28
28
Connector_PinSocket_1.00mm
PinSocket_1x28_P1.00mm_Vertical_SMD_Pin1Left
surface-mounted straight socket strip, 1x28, 1.00mm pitch, single row, style 1 (pin 1 left) (https://gct.co/files/drawings/bc070.pdf), script generated
Surface mounted socket strip SMD 1x28 1.00mm single row style1 pin1 left
0
28
28
Connector_PinSocket_1.00mm
PinSocket_1x28_P1.00mm_Vertical_SMD_Pin1Right
surface-mounted straight socket strip, 1x28, 1.00mm pitch, single row, style 2 (pin 1 right) (https://gct.co/files/drawings/bc070.pdf), script generated
Surface mounted socket strip SMD 1x28 1.00mm single row style2 pin1 right
0
28
28
Connector_PinSocket_1.00mm
PinSocket_1x29_P1.00mm_Vertical
Through hole straight socket strip, 1x29, 1.00mm pitch, single row (https://gct.co/files/drawings/bc065.pdf), script generated
Through hole socket strip THT 1x29 1.00mm single row
0
29
29
Connector_PinSocket_1.00mm
PinSocket_1x29_P1.00mm_Vertical_SMD_Pin1Left
surface-mounted straight socket strip, 1x29, 1.00mm pitch, single row, style 1 (pin 1 left) (https://gct.co/files/drawings/bc070.pdf), script generated
Surface mounted socket strip SMD 1x29 1.00mm single row style1 pin1 left
0
29
29
Connector_PinSocket_1.00mm
PinSocket_1x29_P1.00mm_Vertical_SMD_Pin1Right
surface-mounted straight socket strip, 1x29, 1.00mm pitch, single row, style 2 (pin 1 right) (https://gct.co/files/drawings/bc070.pdf), script generated
Surface mounted socket strip SMD 1x29 1.00mm single row style2 pin1 right
0
29
29
Connector_PinSocket_1.00mm
PinSocket_1x30_P1.00mm_Vertical
Through hole straight socket strip, 1x30, 1.00mm pitch, single row (https://gct.co/files/drawings/bc065.pdf), script generated
Through hole socket strip THT 1x30 1.00mm single row
0
30
30
Connector_PinSocket_1.00mm
PinSocket_1x30_P1.00mm_Vertical_SMD_Pin1Left
surface-mounted straight socket strip, 1x30, 1.00mm pitch, single row, style 1 (pin 1 left) (https://gct.co/files/drawings/bc070.pdf), script generated
Surface mounted socket strip SMD 1x30 1.00mm single row style1 pin1 left
0
30
30
Connector_PinSocket_1.00mm
PinSocket_1x30_P1.00mm_Vertical_SMD_Pin1Right
surface-mounted straight socket strip, 1x30, 1.00mm pitch, single row, style 2 (pin 1 right) (https://gct.co/files/drawings/bc070.pdf), script generated
Surface mounted socket strip SMD 1x30 1.00mm single row style2 pin1 right
0
30
30
Connector_PinSocket_1.00mm
PinSocket_1x31_P1.00mm_Vertical
Through hole straight socket strip, 1x31, 1.00mm pitch, single row (https://gct.co/files/drawings/bc065.pdf), script generated
Through hole socket strip THT 1x31 1.00mm single row
0
31
31
Connector_PinSocket_1.00mm
PinSocket_1x31_P1.00mm_Vertical_SMD_Pin1Left
surface-mounted straight socket strip, 1x31, 1.00mm pitch, single row, style 1 (pin 1 left) (https://gct.co/files/drawings/bc070.pdf), script generated
Surface mounted socket strip SMD 1x31 1.00mm single row style1 pin1 left
0
31
31
Connector_PinSocket_1.00mm
PinSocket_1x31_P1.00mm_Vertical_SMD_Pin1Right
surface-mounted straight socket strip, 1x31, 1.00mm pitch, single row, style 2 (pin 1 right) (https://gct.co/files/drawings/bc070.pdf), script generated
Surface mounted socket strip SMD 1x31 1.00mm single row style2 pin1 right
0
31
31
Connector_PinSocket_1.00mm
PinSocket_1x32_P1.00mm_Vertical
Through hole straight socket strip, 1x32, 1.00mm pitch, single row (https://gct.co/files/drawings/bc065.pdf), script generated
Through hole socket strip THT 1x32 1.00mm single row
0
32
32
Connector_PinSocket_1.00mm
PinSocket_1x32_P1.00mm_Vertical_SMD_Pin1Left
surface-mounted straight socket strip, 1x32, 1.00mm pitch, single row, style 1 (pin 1 left) (https://gct.co/files/drawings/bc070.pdf), script generated
Surface mounted socket strip SMD 1x32 1.00mm single row style1 pin1 left
0
32
32
Connector_PinSocket_1.00mm
PinSocket_1x32_P1.00mm_Vertical_SMD_Pin1Right
surface-mounted straight socket strip, 1x32, 1.00mm pitch, single row, style 2 (pin 1 right) (https://gct.co/files/drawings/bc070.pdf), script generated
Surface mounted socket strip SMD 1x32 1.00mm single row style2 pin1 right
0
32
32
Connector_PinSocket_1.00mm
PinSocket_1x33_P1.00mm_Vertical
Through hole straight socket strip, 1x33, 1.00mm pitch, single row (https://gct.co/files/drawings/bc065.pdf), script generated
Through hole socket strip THT 1x33 1.00mm single row
0
33
33
Connector_PinSocket_1.00mm
PinSocket_1x33_P1.00mm_Vertical_SMD_Pin1Left
surface-mounted straight socket strip, 1x33, 1.00mm pitch, single row, style 1 (pin 1 left) (https://gct.co/files/drawings/bc070.pdf), script generated
Surface mounted socket strip SMD 1x33 1.00mm single row style1 pin1 left
0
33
33
Connector_PinSocket_1.00mm
PinSocket_1x33_P1.00mm_Vertical_SMD_Pin1Right
surface-mounted straight socket strip, 1x33, 1.00mm pitch, single row, style 2 (pin 1 right) (https://gct.co/files/drawings/bc070.pdf), script generated
Surface mounted socket strip SMD 1x33 1.00mm single row style2 pin1 right
0
33
33
Connector_PinSocket_1.00mm
PinSocket_1x34_P1.00mm_Vertical
Through hole straight socket strip, 1x34, 1.00mm pitch, single row (https://gct.co/files/drawings/bc065.pdf), script generated
Through hole socket strip THT 1x34 1.00mm single row
0
34
34
Connector_PinSocket_1.00mm
PinSocket_1x34_P1.00mm_Vertical_SMD_Pin1Left
surface-mounted straight socket strip, 1x34, 1.00mm pitch, single row, style 1 (pin 1 left) (https://gct.co/files/drawings/bc070.pdf), script generated
Surface mounted socket strip SMD 1x34 1.00mm single row style1 pin1 left
0
34
34
Connector_PinSocket_1.00mm
PinSocket_1x34_P1.00mm_Vertical_SMD_Pin1Right
surface-mounted straight socket strip, 1x34, 1.00mm pitch, single row, style 2 (pin 1 right) (https://gct.co/files/drawings/bc070.pdf), script generated
Surface mounted socket strip SMD 1x34 1.00mm single row style2 pin1 right
0
34
34
Connector_PinSocket_1.00mm
PinSocket_1x35_P1.00mm_Vertical
Through hole straight socket strip, 1x35, 1.00mm pitch, single row (https://gct.co/files/drawings/bc065.pdf), script generated
Through hole socket strip THT 1x35 1.00mm single row
0
35
35
Connector_PinSocket_1.00mm
PinSocket_1x35_P1.00mm_Vertical_SMD_Pin1Left
surface-mounted straight socket strip, 1x35, 1.00mm pitch, single row, style 1 (pin 1 left) (https://gct.co/files/drawings/bc070.pdf), script generated
Surface mounted socket strip SMD 1x35 1.00mm single row style1 pin1 left
0
35
35
Connector_PinSocket_1.00mm
PinSocket_1x35_P1.00mm_Vertical_SMD_Pin1Right
surface-mounted straight socket strip, 1x35, 1.00mm pitch, single row, style 2 (pin 1 right) (https://gct.co/files/drawings/bc070.pdf), script generated
Surface mounted socket strip SMD 1x35 1.00mm single row style2 pin1 right
0
35
35
Connector_PinSocket_1.00mm
PinSocket_1x36_P1.00mm_Vertical
Through hole straight socket strip, 1x36, 1.00mm pitch, single row (https://gct.co/files/drawings/bc065.pdf), script generated
Through hole socket strip THT 1x36 1.00mm single row
0
36
36
Connector_PinSocket_1.00mm
PinSocket_1x36_P1.00mm_Vertical_SMD_Pin1Left
surface-mounted straight socket strip, 1x36, 1.00mm pitch, single row, style 1 (pin 1 left) (https://gct.co/files/drawings/bc070.pdf), script generated
Surface mounted socket strip SMD 1x36 1.00mm single row style1 pin1 left
0
36
36
Connector_PinSocket_1.00mm
PinSocket_1x36_P1.00mm_Vertical_SMD_Pin1Right
surface-mounted straight socket strip, 1x36, 1.00mm pitch, single row, style 2 (pin 1 right) (https://gct.co/files/drawings/bc070.pdf), script generated
Surface mounted socket strip SMD 1x36 1.00mm single row style2 pin1 right
0
36
36
Connector_PinSocket_1.00mm
PinSocket_1x37_P1.00mm_Vertical
Through hole straight socket strip, 1x37, 1.00mm pitch, single row (https://gct.co/files/drawings/bc065.pdf), script generated
Through hole socket strip THT 1x37 1.00mm single row
0
37
37
Connector_PinSocket_1.00mm
PinSocket_1x37_P1.00mm_Vertical_SMD_Pin1Left
surface-mounted straight socket strip, 1x37, 1.00mm pitch, single row, style 1 (pin 1 left) (https://gct.co/files/drawings/bc070.pdf), script generated
Surface mounted socket strip SMD 1x37 1.00mm single row style1 pin1 left
0
37
37
Connector_PinSocket_1.00mm
PinSocket_1x37_P1.00mm_Vertical_SMD_Pin1Right
surface-mounted straight socket strip, 1x37, 1.00mm pitch, single row, style 2 (pin 1 right) (https://gct.co/files/drawings/bc070.pdf), script generated
Surface mounted socket strip SMD 1x37 1.00mm single row style2 pin1 right
0
37
37
Connector_PinSocket_1.00mm
PinSocket_1x38_P1.00mm_Vertical
Through hole straight socket strip, 1x38, 1.00mm pitch, single row (https://gct.co/files/drawings/bc065.pdf), script generated
Through hole socket strip THT 1x38 1.00mm single row
0
38
38
Connector_PinSocket_1.00mm
PinSocket_1x38_P1.00mm_Vertical_SMD_Pin1Left
surface-mounted straight socket strip, 1x38, 1.00mm pitch, single row, style 1 (pin 1 left) (https://gct.co/files/drawings/bc070.pdf), script generated
Surface mounted socket strip SMD 1x38 1.00mm single row style1 pin1 left
0
38
38
Connector_PinSocket_1.00mm
PinSocket_1x38_P1.00mm_Vertical_SMD_Pin1Right
surface-mounted straight socket strip, 1x38, 1.00mm pitch, single row, style 2 (pin 1 right) (https://gct.co/files/drawings/bc070.pdf), script generated
Surface mounted socket strip SMD 1x38 1.00mm single row style2 pin1 right
0
38
38
Connector_PinSocket_1.00mm
PinSocket_1x39_P1.00mm_Vertical
Through hole straight socket strip, 1x39, 1.00mm pitch, single row (https://gct.co/files/drawings/bc065.pdf), script generated
Through hole socket strip THT 1x39 1.00mm single row
0
39
39
Connector_PinSocket_1.00mm
PinSocket_1x39_P1.00mm_Vertical_SMD_Pin1Left
surface-mounted straight socket strip, 1x39, 1.00mm pitch, single row, style 1 (pin 1 left) (https://gct.co/files/drawings/bc070.pdf), script generated
Surface mounted socket strip SMD 1x39 1.00mm single row style1 pin1 left
0
39
39
Connector_PinSocket_1.00mm
PinSocket_1x39_P1.00mm_Vertical_SMD_Pin1Right
surface-mounted straight socket strip, 1x39, 1.00mm pitch, single row, style 2 (pin 1 right) (https://gct.co/files/drawings/bc070.pdf), script generated
Surface mounted socket strip SMD 1x39 1.00mm single row style2 pin1 right
0
39
39
Connector_PinSocket_1.00mm
PinSocket_1x40_P1.00mm_Vertical
Through hole straight socket strip, 1x40, 1.00mm pitch, single row (https://gct.co/files/drawings/bc065.pdf), script generated
Through hole socket strip THT 1x40 1.00mm single row
0
40
40
Connector_PinSocket_1.00mm
PinSocket_1x40_P1.00mm_Vertical_SMD_Pin1Left
surface-mounted straight socket strip, 1x40, 1.00mm pitch, single row, style 1 (pin 1 left) (https://gct.co/files/drawings/bc070.pdf), script generated
Surface mounted socket strip SMD 1x40 1.00mm single row style1 pin1 left
0
40
40
Connector_PinSocket_1.00mm
PinSocket_1x40_P1.00mm_Vertical_SMD_Pin1Right
surface-mounted straight socket strip, 1x40, 1.00mm pitch, single row, style 2 (pin 1 right) (https://gct.co/files/drawings/bc070.pdf), script generated
Surface mounted socket strip SMD 1x40 1.00mm single row style2 pin1 right
0
40
40
Connector_PinSocket_1.00mm
PinSocket_2x02_P1.00mm_Vertical_SMD
surface-mounted straight socket strip, 2x02, 1.00mm pitch, double cols (https://gct.co/files/drawings/bc085.pdf), script generated
Surface mounted socket strip SMD 2x02 1.00mm double row
0
4
4
Connector_PinSocket_1.00mm
PinSocket_2x03_P1.00mm_Vertical_SMD
surface-mounted straight socket strip, 2x03, 1.00mm pitch, double cols (https://gct.co/files/drawings/bc085.pdf), script generated
Surface mounted socket strip SMD 2x03 1.00mm double row
0
6
6
Connector_PinSocket_1.00mm
PinSocket_2x04_P1.00mm_Vertical_SMD
surface-mounted straight socket strip, 2x04, 1.00mm pitch, double cols (https://gct.co/files/drawings/bc085.pdf), script generated
Surface mounted socket strip SMD 2x04 1.00mm double row
0
8
8
Connector_PinSocket_1.00mm
PinSocket_2x05_P1.00mm_Vertical_SMD
surface-mounted straight socket strip, 2x05, 1.00mm pitch, double cols (https://gct.co/files/drawings/bc085.pdf), script generated
Surface mounted socket strip SMD 2x05 1.00mm double row
0
10
10
Connector_PinSocket_1.00mm
PinSocket_2x06_P1.00mm_Vertical_SMD
surface-mounted straight socket strip, 2x06, 1.00mm pitch, double cols (https://gct.co/files/drawings/bc085.pdf), script generated
Surface mounted socket strip SMD 2x06 1.00mm double row
0
12
12
Connector_PinSocket_1.00mm
PinSocket_2x07_P1.00mm_Vertical_SMD
surface-mounted straight socket strip, 2x07, 1.00mm pitch, double cols (https://gct.co/files/drawings/bc085.pdf), script generated
Surface mounted socket strip SMD 2x07 1.00mm double row
0
14
14
Connector_PinSocket_1.00mm
PinSocket_2x08_P1.00mm_Vertical_SMD
surface-mounted straight socket strip, 2x08, 1.00mm pitch, double cols (https://gct.co/files/drawings/bc085.pdf), script generated
Surface mounted socket strip SMD 2x08 1.00mm double row
0
16
16
Connector_PinSocket_1.00mm
PinSocket_2x09_P1.00mm_Vertical_SMD
surface-mounted straight socket strip, 2x09, 1.00mm pitch, double cols (https://gct.co/files/drawings/bc085.pdf), script generated
Surface mounted socket strip SMD 2x09 1.00mm double row
0
18
18
Connector_PinSocket_1.00mm
PinSocket_2x10_P1.00mm_Vertical_SMD
surface-mounted straight socket strip, 2x10, 1.00mm pitch, double cols (https://gct.co/files/drawings/bc085.pdf), script generated
Surface mounted socket strip SMD 2x10 1.00mm double row
0
20
20
Connector_PinSocket_1.00mm
PinSocket_2x11_P1.00mm_Vertical_SMD
surface-mounted straight socket strip, 2x11, 1.00mm pitch, double cols (https://gct.co/files/drawings/bc085.pdf), script generated
Surface mounted socket strip SMD 2x11 1.00mm double row
0
22
22
Connector_PinSocket_1.00mm
PinSocket_2x12_P1.00mm_Vertical_SMD
surface-mounted straight socket strip, 2x12, 1.00mm pitch, double cols (https://gct.co/files/drawings/bc085.pdf), script generated
Surface mounted socket strip SMD 2x12 1.00mm double row
0
24
24
Connector_PinSocket_1.00mm
PinSocket_2x13_P1.00mm_Vertical_SMD
surface-mounted straight socket strip, 2x13, 1.00mm pitch, double cols (https://gct.co/files/drawings/bc085.pdf), script generated
Surface mounted socket strip SMD 2x13 1.00mm double row
0
26
26
Connector_PinSocket_1.00mm
PinSocket_2x14_P1.00mm_Vertical_SMD
surface-mounted straight socket strip, 2x14, 1.00mm pitch, double cols (https://gct.co/files/drawings/bc085.pdf), script generated
Surface mounted socket strip SMD 2x14 1.00mm double row
0
28
28
Connector_PinSocket_1.00mm
PinSocket_2x15_P1.00mm_Vertical_SMD
surface-mounted straight socket strip, 2x15, 1.00mm pitch, double cols (https://gct.co/files/drawings/bc085.pdf), script generated
Surface mounted socket strip SMD 2x15 1.00mm double row
0
30
30
Connector_PinSocket_1.00mm
PinSocket_2x16_P1.00mm_Vertical_SMD
surface-mounted straight socket strip, 2x16, 1.00mm pitch, double cols (https://gct.co/files/drawings/bc085.pdf), script generated
Surface mounted socket strip SMD 2x16 1.00mm double row
0
32
32
Connector_PinSocket_1.00mm
PinSocket_2x17_P1.00mm_Vertical_SMD
surface-mounted straight socket strip, 2x17, 1.00mm pitch, double cols (https://gct.co/files/drawings/bc085.pdf), script generated
Surface mounted socket strip SMD 2x17 1.00mm double row
0
34
34
Connector_PinSocket_1.00mm
PinSocket_2x18_P1.00mm_Vertical_SMD
surface-mounted straight socket strip, 2x18, 1.00mm pitch, double cols (https://gct.co/files/drawings/bc085.pdf), script generated
Surface mounted socket strip SMD 2x18 1.00mm double row
0
36
36
Connector_PinSocket_1.00mm
PinSocket_2x19_P1.00mm_Vertical_SMD
surface-mounted straight socket strip, 2x19, 1.00mm pitch, double cols (https://gct.co/files/drawings/bc085.pdf), script generated
Surface mounted socket strip SMD 2x19 1.00mm double row
0
38
38
Connector_PinSocket_1.00mm
PinSocket_2x20_P1.00mm_Vertical_SMD
surface-mounted straight socket strip, 2x20, 1.00mm pitch, double cols (https://gct.co/files/drawings/bc085.pdf), script generated
Surface mounted socket strip SMD 2x20 1.00mm double row
0
40
40
Connector_PinSocket_1.00mm
PinSocket_2x21_P1.00mm_Vertical_SMD
surface-mounted straight socket strip, 2x21, 1.00mm pitch, double cols (https://gct.co/files/drawings/bc085.pdf), script generated
Surface mounted socket strip SMD 2x21 1.00mm double row
0
42
42
Connector_PinSocket_1.00mm
PinSocket_2x22_P1.00mm_Vertical_SMD
surface-mounted straight socket strip, 2x22, 1.00mm pitch, double cols (https://gct.co/files/drawings/bc085.pdf), script generated
Surface mounted socket strip SMD 2x22 1.00mm double row
0
44
44
Connector_PinSocket_1.00mm
PinSocket_2x23_P1.00mm_Vertical_SMD
surface-mounted straight socket strip, 2x23, 1.00mm pitch, double cols (https://gct.co/files/drawings/bc085.pdf), script generated
Surface mounted socket strip SMD 2x23 1.00mm double row
0
46
46
Connector_PinSocket_1.00mm
PinSocket_2x24_P1.00mm_Vertical_SMD
surface-mounted straight socket strip, 2x24, 1.00mm pitch, double cols (https://gct.co/files/drawings/bc085.pdf), script generated
Surface mounted socket strip SMD 2x24 1.00mm double row
0
48
48
Connector_PinSocket_1.00mm
PinSocket_2x25_P1.00mm_Vertical_SMD
surface-mounted straight socket strip, 2x25, 1.00mm pitch, double cols (https://gct.co/files/drawings/bc085.pdf), script generated
Surface mounted socket strip SMD 2x25 1.00mm double row
0
50
50
Connector_PinSocket_1.00mm
PinSocket_2x26_P1.00mm_Vertical_SMD
surface-mounted straight socket strip, 2x26, 1.00mm pitch, double cols (https://gct.co/files/drawings/bc085.pdf), script generated
Surface mounted socket strip SMD 2x26 1.00mm double row
0
52
52
Connector_PinSocket_1.00mm
PinSocket_2x27_P1.00mm_Vertical_SMD
surface-mounted straight socket strip, 2x27, 1.00mm pitch, double cols (https://gct.co/files/drawings/bc085.pdf), script generated
Surface mounted socket strip SMD 2x27 1.00mm double row
0
54
54
Connector_PinSocket_1.00mm
PinSocket_2x28_P1.00mm_Vertical_SMD
surface-mounted straight socket strip, 2x28, 1.00mm pitch, double cols (https://gct.co/files/drawings/bc085.pdf), script generated
Surface mounted socket strip SMD 2x28 1.00mm double row
0
56
56
Connector_PinSocket_1.00mm
PinSocket_2x29_P1.00mm_Vertical_SMD
surface-mounted straight socket strip, 2x29, 1.00mm pitch, double cols (https://gct.co/files/drawings/bc085.pdf), script generated
Surface mounted socket strip SMD 2x29 1.00mm double row
0
58
58
Connector_PinSocket_1.00mm
PinSocket_2x30_P1.00mm_Vertical_SMD
surface-mounted straight socket strip, 2x30, 1.00mm pitch, double cols (https://gct.co/files/drawings/bc085.pdf), script generated
Surface mounted socket strip SMD 2x30 1.00mm double row
0
60
60
Connector_PinSocket_1.00mm
PinSocket_2x31_P1.00mm_Vertical_SMD
surface-mounted straight socket strip, 2x31, 1.00mm pitch, double cols (https://gct.co/files/drawings/bc085.pdf), script generated
Surface mounted socket strip SMD 2x31 1.00mm double row
0
62
62
Connector_PinSocket_1.00mm
PinSocket_2x32_P1.00mm_Vertical_SMD
surface-mounted straight socket strip, 2x32, 1.00mm pitch, double cols (https://gct.co/files/drawings/bc085.pdf), script generated
Surface mounted socket strip SMD 2x32 1.00mm double row
0
64
64
Connector_PinSocket_1.00mm
PinSocket_2x33_P1.00mm_Vertical_SMD
surface-mounted straight socket strip, 2x33, 1.00mm pitch, double cols (https://gct.co/files/drawings/bc085.pdf), script generated
Surface mounted socket strip SMD 2x33 1.00mm double row
0
66
66
Connector_PinSocket_1.00mm
PinSocket_2x34_P1.00mm_Vertical_SMD
surface-mounted straight socket strip, 2x34, 1.00mm pitch, double cols (https://gct.co/files/drawings/bc085.pdf), script generated
Surface mounted socket strip SMD 2x34 1.00mm double row
0
68
68
Connector_PinSocket_1.00mm
PinSocket_2x35_P1.00mm_Vertical_SMD
surface-mounted straight socket strip, 2x35, 1.00mm pitch, double cols (https://gct.co/files/drawings/bc085.pdf), script generated
Surface mounted socket strip SMD 2x35 1.00mm double row
0
70
70
Connector_PinSocket_1.00mm
PinSocket_2x36_P1.00mm_Vertical_SMD
surface-mounted straight socket strip, 2x36, 1.00mm pitch, double cols (https://gct.co/files/drawings/bc085.pdf), script generated
Surface mounted socket strip SMD 2x36 1.00mm double row
0
72
72
Connector_PinSocket_1.00mm
PinSocket_2x37_P1.00mm_Vertical_SMD
surface-mounted straight socket strip, 2x37, 1.00mm pitch, double cols (https://gct.co/files/drawings/bc085.pdf), script generated
Surface mounted socket strip SMD 2x37 1.00mm double row
0
74
74
Connector_PinSocket_1.00mm
PinSocket_2x38_P1.00mm_Vertical_SMD
surface-mounted straight socket strip, 2x38, 1.00mm pitch, double cols (https://gct.co/files/drawings/bc085.pdf), script generated
Surface mounted socket strip SMD 2x38 1.00mm double row
0
76
76
Connector_PinSocket_1.00mm
PinSocket_2x39_P1.00mm_Vertical_SMD
surface-mounted straight socket strip, 2x39, 1.00mm pitch, double cols (https://gct.co/files/drawings/bc085.pdf), script generated
Surface mounted socket strip SMD 2x39 1.00mm double row
0
78
78
Connector_PinSocket_1.00mm
PinSocket_2x40_P1.00mm_Vertical_SMD
surface-mounted straight socket strip, 2x40, 1.00mm pitch, double cols (https://gct.co/files/drawings/bc085.pdf), script generated
Surface mounted socket strip SMD 2x40 1.00mm double row
0
80
80
