(footprint "avia8" (version 20211014) (generator pcbnew)
  (layer "F.Cu")
  (tedit 0)
  (attr through_hole)
  (fp_text reference "J**" (at -0.0508 -4.4196 unlocked) (layer "F.SilkS")
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 5c0f5c5d-0ccc-456a-b4f2-7db923ad772d)
  )
  (fp_text value "avia8" (at 0.0254 4.2926 unlocked) (layer "F.Fab")
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp b0de5e5b-2e3a-495d-934e-fd6d1f4aa4bc)
  )
  (pad "" np_thru_hole circle (at -8.382 -5.2832) (size 2.8 2.8) (drill 2.4) (layers F&B.Cu *.Mask) (tstamp 6ffd00c9-b1bb-4ed4-957d-60b558aa3bc5))
  (pad "" np_thru_hole circle (at 7.5184 -1.27) (size 2.5 2.5) (drill 2.2) (layers F&B.Cu *.Mask) (tstamp 717a3aab-c7d0-41a7-a947-124cdc15809d))
  (pad "" np_thru_hole circle (at -7.5184 -1.27) (size 2.5 2.5) (drill 2.2) (layers F&B.Cu *.Mask) (tstamp 8f61b0ea-6d20-4de0-9f22-fbb4743a3d7b))
  (pad "" np_thru_hole circle (at 8.382 -5.2832) (size 2.8 2.8) (drill 2.4) (layers F&B.Cu *.Mask) (tstamp dfc0d0e3-be08-4aa6-8e1f-39e0ab1e4019))
  (pad "1" thru_hole circle (at -2.0828 -2.54) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask) (tstamp a290e8ea-f822-4093-9e4f-a338ca6ae887))
  (pad "2" thru_hole circle (at 0 -2.54) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask) (tstamp 4df73996-63b7-4ad5-97da-b8f4f16eb06b))
  (pad "3" thru_hole circle (at 2.0828 -2.54) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask) (tstamp a88a7649-35cb-4897-868f-145142579c64))
  (pad "4" thru_hole circle (at -2.7178 0) (size 2 2) (drill 1) (layers *.Cu *.Mask) (tstamp 1bba5922-d2f5-4ed3-baf0-cf5c4408e749))
  (pad "5" thru_hole circle (at 0 0) (size 2 2) (drill 1) (layers *.Cu *.Mask) (tstamp 7073db79-9e61-4ebf-899e-6e592af72912))
  (pad "6" thru_hole circle (at 2.7178 0) (size 2 2) (drill 1) (layers *.Cu *.Mask) (tstamp feb15ff2-c2e0-4b94-b228-7ebcb3058498))
  (pad "7" thru_hole circle (at -1.4986 2.54) (size 2 2) (drill 1) (layers *.Cu *.Mask) (tstamp 15d3b23e-0672-4051-96ab-4a6768fc6e71))
  (pad "8" thru_hole circle (at 1.4986 2.54) (size 2 2) (drill 1) (layers *.Cu *.Mask) (tstamp 285e9ea3-5a1e-4fc8-8a9d-b70542acd227))
)
