Cmp-Mod V01 Created by CvPcb (2013-feb-26)-stable date = Сб 27 дек 2014 18:49:59

BeginCmp
TimeStamp = /53576FC3;
Reference = C8;
ValeurCmp = 0.33u;
IdModule  = SM0805;
EndCmp

BeginCmp
TimeStamp = /53576FB6;
Reference = C9;
ValeurCmp = 0.1u;
IdModule  = SM0805;
EndCmp

BeginCmp
TimeStamp = /5357821E;
Reference = C10;
ValeurCmp = 1u;
IdModule  = SM0805;
EndCmp

BeginCmp
TimeStamp = /5357750C;
Reference = C12;
ValeurCmp = 47u;
IdModule  = SM1206POL;
EndCmp

BeginCmp
TimeStamp = /54759E36;
Reference = DA1;
ValeurCmp = NX3L4051-HX;
IdModule  = HXQFN16;
EndCmp

BeginCmp
TimeStamp = /5475A2C1;
Reference = DA2;
ValeurCmp = NX3L4051-HX;
IdModule  = HXQFN16;
EndCmp

BeginCmp
TimeStamp = /5475A2C7;
Reference = DA3;
ValeurCmp = NX3L4051-HX;
IdModule  = HXQFN16;
EndCmp

BeginCmp
TimeStamp = /53577523;
Reference = L1;
ValeurCmp = BMB2A0300AN1;
IdModule  = SM0805;
EndCmp

BeginCmp
TimeStamp = /53579853;
Reference = P1;
ValeurCmp = контакт 1;
IdModule  = SIL-8;
EndCmp

BeginCmp
TimeStamp = /5475974D;
Reference = P2;
ValeurCmp = контакт 2a;
IdModule  = SIL-8;
EndCmp

BeginCmp
TimeStamp = /5475975B;
Reference = P3;
ValeurCmp = контакт 2б;
IdModule  = SIL-8;
EndCmp

BeginCmp
TimeStamp = /5357BA72;
Reference = P4;
ValeurCmp = MCU;
IdModule  = SIL-8;
EndCmp

BeginCmp
TimeStamp = /5357ABB4;
Reference = P6;
ValeurCmp = 5V;
IdModule  = SIL-2;
EndCmp

BeginCmp
TimeStamp = /53579396;
Reference = R1;
ValeurCmp = 10k;
IdModule  = SM0603;
EndCmp

BeginCmp
TimeStamp = /535793A8;
Reference = R2;
ValeurCmp = 10k;
IdModule  = SM0603;
EndCmp

BeginCmp
TimeStamp = /5357C8F8;
Reference = R3;
ValeurCmp = 47k;
IdModule  = SM0603;
EndCmp

BeginCmp
TimeStamp = /53562118;
Reference = R4;
ValeurCmp = 1k 0.1% (RT0805BRB071KL);
IdModule  = SM0805;
EndCmp

BeginCmp
TimeStamp = /547C0DD9;
Reference = R5;
ValeurCmp = 1k 0.1% (RT0805BRB071KL);
IdModule  = SM0805;
EndCmp

BeginCmp
TimeStamp = /547C0DE4;
Reference = R6;
ValeurCmp = 1k 0.1% (RT0805BRB071KL);
IdModule  = SM0805;
EndCmp

BeginCmp
TimeStamp = /547C0DEA;
Reference = R7;
ValeurCmp = 1k 0.1% (RT0805BRB071KL);
IdModule  = SM0805;
EndCmp

BeginCmp
TimeStamp = /547C0DF0;
Reference = R8;
ValeurCmp = 1k 0.1% (RT0805BRB071KL);
IdModule  = SM0805;
EndCmp

BeginCmp
TimeStamp = /524D62C1;
Reference = U4;
ValeurCmp = AD7794/7795;
IdModule  = SSOP24;
EndCmp

BeginCmp
TimeStamp = /535787B7;
Reference = U5;
ValeurCmp = LM1117-33;
IdModule  = SOT223;
EndCmp

BeginCmp
TimeStamp = /549EDA1E;
Reference = X1;
ValeurCmp = GND_CONNECTOR;
IdModule  = GND_connector;
EndCmp

EndListe
