(module VIA (layer F.Cu) (tedit 5D2D6442)
  (fp_text reference "" (at 0 0.5) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text value VIA (at 0 -1.5) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (pad ~ thru_hole circle (at 0 0) (size 1.5 1.5) (drill 0.6) (layers *.Cu)
    (clearance 0.2) (zone_connect 1))
)
