(export (version D)
  (design
    (source /home/eddy/Docs/SAO/BTA/MIRROR_CONTROL_termo/Project/kicad/multiplexer/multiplexer.sch)
    (date "Ср 16 май 2018 21:15:06")
    (tool "Eeschema 4.0.7")
    (sheet (number 1) (name /) (tstamps /)
      (title_block
        (title)
        (company)
        (rev)
        (date)
        (source multiplexer.sch)
        (comment (number 1) (value ""))
        (comment (number 2) (value ""))
        (comment (number 3) (value ""))
        (comment (number 4) (value ""))))
    (sheet (number 2) (name "/Block 1/") (tstamps /0000BB11/)
      (title_block
        (title)
        (company)
        (rev)
        (date)
        (source 8chblock.sch)
        (comment (number 1) (value ""))
        (comment (number 2) (value ""))
        (comment (number 3) (value ""))
        (comment (number 4) (value ""))))
    (sheet (number 3) (name "/Block 2/") (tstamps /0000BB22/)
      (title_block
        (title)
        (company)
        (rev)
        (date)
        (source 8chblock.sch)
        (comment (number 1) (value ""))
        (comment (number 2) (value ""))
        (comment (number 3) (value ""))
        (comment (number 4) (value ""))))
    (sheet (number 4) (name "/Block 3/") (tstamps /0000BB33/)
      (title_block
        (title)
        (company)
        (rev)
        (date)
        (source 8chblock.sch)
        (comment (number 1) (value ""))
        (comment (number 2) (value ""))
        (comment (number 3) (value ""))
        (comment (number 4) (value ""))))
    (sheet (number 5) (name "/Block 4/") (tstamps /0000BB44/)
      (title_block
        (title)
        (company)
        (rev)
        (date)
        (source 8chblock.sch)
        (comment (number 1) (value ""))
        (comment (number 2) (value ""))
        (comment (number 3) (value ""))
        (comment (number 4) (value ""))))
    (sheet (number 6) (name "/Block 5/") (tstamps /0000BB55/)
      (title_block
        (title)
        (company)
        (rev)
        (date)
        (source 8chblock.sch)
        (comment (number 1) (value ""))
        (comment (number 2) (value ""))
        (comment (number 3) (value ""))
        (comment (number 4) (value ""))))
    (sheet (number 7) (name "/Block 6/") (tstamps /0000BB66/)
      (title_block
        (title)
        (company)
        (rev)
        (date)
        (source 8chblock.sch)
        (comment (number 1) (value ""))
        (comment (number 2) (value ""))
        (comment (number 3) (value ""))
        (comment (number 4) (value "")))))
  (components
    (comp (ref J1)
      (value "5V in")
      (footprint TerminalBlock.pretty:TerminalBlock_bornier-2_P5.08mm)
      (libsource (lib Connector) (part Screw_Terminal_01x02))
      (sheetpath (names /) (tstamps /))
      (tstamp 5AFC0F3D))
    (comp (ref U1)
      (value 74HC4051)
      (footprint Package_SO.pretty:SOIC-16_3.9x9.9mm_P1.27mm)
      (libsource (lib 74xx) (part 74HC4051))
      (sheetpath (names /) (tstamps /))
      (tstamp 5AFC26B8))
    (comp (ref C1.1)
      (value 0.1)
      (footprint Capacitor_SMD.pretty:C_0805_2012Metric_Pad1.29x1.40mm_HandSolder)
      (libsource (lib Device) (part C))
      (sheetpath (names /) (tstamps /))
      (tstamp 5AFC41A4))
    (comp (ref C1.2)
      (value 0.1)
      (footprint Capacitor_SMD.pretty:C_0805_2012Metric_Pad1.29x1.40mm_HandSolder)
      (libsource (lib Device) (part C))
      (sheetpath (names /) (tstamps /))
      (tstamp 5AFC4777))
    (comp (ref C1.3)
      (value 0.1)
      (footprint Capacitor_SMD.pretty:C_0805_2012Metric_Pad1.29x1.40mm_HandSolder)
      (libsource (lib Device) (part C))
      (sheetpath (names /) (tstamps /))
      (tstamp 5AFC47BD))
    (comp (ref C1.4)
      (value 0.1)
      (footprint Capacitor_SMD.pretty:C_0805_2012Metric_Pad1.29x1.40mm_HandSolder)
      (libsource (lib Device) (part C))
      (sheetpath (names /) (tstamps /))
      (tstamp 5AFC48A0))
    (comp (ref C1.5)
      (value 0.1)
      (footprint Capacitor_SMD.pretty:C_0805_2012Metric_Pad1.29x1.40mm_HandSolder)
      (libsource (lib Device) (part C))
      (sheetpath (names /) (tstamps /))
      (tstamp 5AFC48A6))
    (comp (ref C1.6)
      (value 0.1)
      (footprint Capacitor_SMD.pretty:C_0805_2012Metric_Pad1.29x1.40mm_HandSolder)
      (libsource (lib Device) (part C))
      (sheetpath (names /) (tstamps /))
      (tstamp 5AFC48AC))
    (comp (ref C2)
      (value 0.1)
      (footprint Capacitor_SMD.pretty:C_0805_2012Metric_Pad1.29x1.40mm_HandSolder)
      (libsource (lib Device) (part C))
      (sheetpath (names /) (tstamps /))
      (tstamp 5AFC48DA))
    (comp (ref J2)
      (value I2C_IN)
      (footprint Connector_PinHeader_2.54mm.pretty:PinHeader_1x03_P2.54mm_Vertical)
      (libsource (lib Connector) (part Conn_01x03_Male))
      (sheetpath (names /) (tstamps /))
      (tstamp 5AFC95E7))
    (comp (ref U2)
      (value LM1117-3.3)
      (footprint Package_TO_SOT_SMD.pretty:SOT-223-3_TabPin2)
      (libsource (lib Regulator_Linear) (part LM1117-3.3))
      (sheetpath (names /) (tstamps /))
      (tstamp 5AFCC18D))
    (comp (ref C9)
      (value 47u)
      (footprint Capacitor_Tantalum_SMD.pretty:CP_EIA-3216-18_Kemet-A_Pad1.53x1.40mm_HandSolder)
      (libsource (lib Device) (part CP))
      (sheetpath (names /) (tstamps /))
      (tstamp 5AFCD1B0))
    (comp (ref J3)
      (value ADDR)
      (footprint Connector_PinHeader_2.54mm.pretty:PinHeader_1x06_P2.54mm_Vertical)
      (libsource (lib Connector) (part Conn_01x06_Male))
      (sheetpath (names /) (tstamps /))
      (tstamp 5AFCFEDA))
    (comp (ref C8)
      (value 0.1)
      (footprint Capacitor_SMD.pretty:C_0805_2012Metric_Pad1.29x1.40mm_HandSolder)
      (libsource (lib Device) (part C))
      (sheetpath (names /) (tstamps /))
      (tstamp 5AFC88A9))
    (comp (ref U3.1)
      (value 74HC4051)
      (footprint Package_SO.pretty:SOIC-16_3.9x9.9mm_P1.27mm)
      (libsource (lib 74xx) (part 74HC4051))
      (sheetpath (names "/Block 1/") (tstamps /0000BB11/))
      (tstamp 5AFC50F9))
    (comp (ref R1.1)
      (value 47k)
      (footprint Resistor_SMD.pretty:R_0805_2012Metric_Pad1.29x1.40mm_HandSolder)
      (libsource (lib Device) (part R))
      (sheetpath (names "/Block 1/") (tstamps /0000BB11/))
      (tstamp 5AFC5111))
    (comp (ref J3.1)
      (value SDA/SCL)
      (footprint mylib:8pair)
      (libsource (lib Connector_Generic) (part Conn_02x08_Top_Bottom))
      (sheetpath (names "/Block 1/") (tstamps /0000BB11/))
      (tstamp 5AFC511E))
    (comp (ref R4.1)
      (value 4k7)
      (footprint Resistor_SMD.pretty:R_0805_2012Metric_Pad1.29x1.40mm_HandSolder)
      (libsource (lib Device) (part R))
      (sheetpath (names "/Block 1/") (tstamps /0000BB11/))
      (tstamp 5AFC513F))
    (comp (ref R6.1)
      (value 4k7)
      (footprint Resistor_SMD.pretty:R_0805_2012Metric_Pad1.29x1.40mm_HandSolder)
      (libsource (lib Device) (part R))
      (sheetpath (names "/Block 1/") (tstamps /0000BB11/))
      (tstamp 5AFC5146))
    (comp (ref R2.1)
      (value 4k7)
      (footprint Resistor_SMD.pretty:R_0805_2012Metric_Pad1.29x1.40mm_HandSolder)
      (libsource (lib Device) (part R))
      (sheetpath (names "/Block 1/") (tstamps /0000BB11/))
      (tstamp 5AFC514D))
    (comp (ref R7.1)
      (value 4k7)
      (footprint Resistor_SMD.pretty:R_0805_2012Metric_Pad1.29x1.40mm_HandSolder)
      (libsource (lib Device) (part R))
      (sheetpath (names "/Block 1/") (tstamps /0000BB11/))
      (tstamp 5AFC5154))
    (comp (ref R5.1)
      (value 4k7)
      (footprint Resistor_SMD.pretty:R_0805_2012Metric_Pad1.29x1.40mm_HandSolder)
      (libsource (lib Device) (part R))
      (sheetpath (names "/Block 1/") (tstamps /0000BB11/))
      (tstamp 5AFC515B))
    (comp (ref R3.1)
      (value 4k7)
      (footprint Resistor_SMD.pretty:R_0805_2012Metric_Pad1.29x1.40mm_HandSolder)
      (libsource (lib Device) (part R))
      (sheetpath (names "/Block 1/") (tstamps /0000BB11/))
      (tstamp 5AFC5162))
    (comp (ref R8.1)
      (value 4k7)
      (footprint Resistor_SMD.pretty:R_0805_2012Metric_Pad1.29x1.40mm_HandSolder)
      (libsource (lib Device) (part R))
      (sheetpath (names "/Block 1/") (tstamps /0000BB11/))
      (tstamp 5AFC5169))
    (comp (ref R9.1)
      (value 4k7)
      (footprint Resistor_SMD.pretty:R_0805_2012Metric_Pad1.29x1.40mm_HandSolder)
      (libsource (lib Device) (part R))
      (sheetpath (names "/Block 1/") (tstamps /0000BB11/))
      (tstamp 5AFC5170))
    (comp (ref U3.2)
      (value 74HC4051)
      (footprint Package_SO.pretty:SOIC-16_3.9x9.9mm_P1.27mm)
      (libsource (lib 74xx) (part 74HC4051))
      (sheetpath (names "/Block 2/") (tstamps /0000BB22/))
      (tstamp 5AFC50F9))
    (comp (ref R1.2)
      (value 47k)
      (footprint Resistor_SMD.pretty:R_0805_2012Metric_Pad1.29x1.40mm_HandSolder)
      (libsource (lib Device) (part R))
      (sheetpath (names "/Block 2/") (tstamps /0000BB22/))
      (tstamp 5AFC5111))
    (comp (ref J3.2)
      (value SDA/SCL)
      (footprint mylib:8pair)
      (libsource (lib Connector_Generic) (part Conn_02x08_Top_Bottom))
      (sheetpath (names "/Block 2/") (tstamps /0000BB22/))
      (tstamp 5AFC511E))
    (comp (ref R4.2)
      (value 4k7)
      (footprint Resistor_SMD.pretty:R_0805_2012Metric_Pad1.29x1.40mm_HandSolder)
      (libsource (lib Device) (part R))
      (sheetpath (names "/Block 2/") (tstamps /0000BB22/))
      (tstamp 5AFC513F))
    (comp (ref R6.2)
      (value 4k7)
      (footprint Resistor_SMD.pretty:R_0805_2012Metric_Pad1.29x1.40mm_HandSolder)
      (libsource (lib Device) (part R))
      (sheetpath (names "/Block 2/") (tstamps /0000BB22/))
      (tstamp 5AFC5146))
    (comp (ref R2.2)
      (value 4k7)
      (footprint Resistor_SMD.pretty:R_0805_2012Metric_Pad1.29x1.40mm_HandSolder)
      (libsource (lib Device) (part R))
      (sheetpath (names "/Block 2/") (tstamps /0000BB22/))
      (tstamp 5AFC514D))
    (comp (ref R7.2)
      (value 4k7)
      (footprint Resistor_SMD.pretty:R_0805_2012Metric_Pad1.29x1.40mm_HandSolder)
      (libsource (lib Device) (part R))
      (sheetpath (names "/Block 2/") (tstamps /0000BB22/))
      (tstamp 5AFC5154))
    (comp (ref R5.2)
      (value 4k7)
      (footprint Resistor_SMD.pretty:R_0805_2012Metric_Pad1.29x1.40mm_HandSolder)
      (libsource (lib Device) (part R))
      (sheetpath (names "/Block 2/") (tstamps /0000BB22/))
      (tstamp 5AFC515B))
    (comp (ref R3.2)
      (value 4k7)
      (footprint Resistor_SMD.pretty:R_0805_2012Metric_Pad1.29x1.40mm_HandSolder)
      (libsource (lib Device) (part R))
      (sheetpath (names "/Block 2/") (tstamps /0000BB22/))
      (tstamp 5AFC5162))
    (comp (ref R8.2)
      (value 4k7)
      (footprint Resistor_SMD.pretty:R_0805_2012Metric_Pad1.29x1.40mm_HandSolder)
      (libsource (lib Device) (part R))
      (sheetpath (names "/Block 2/") (tstamps /0000BB22/))
      (tstamp 5AFC5169))
    (comp (ref R9.2)
      (value 4k7)
      (footprint Resistor_SMD.pretty:R_0805_2012Metric_Pad1.29x1.40mm_HandSolder)
      (libsource (lib Device) (part R))
      (sheetpath (names "/Block 2/") (tstamps /0000BB22/))
      (tstamp 5AFC5170))
    (comp (ref U3.3)
      (value 74HC4051)
      (footprint Package_SO.pretty:SOIC-16_3.9x9.9mm_P1.27mm)
      (libsource (lib 74xx) (part 74HC4051))
      (sheetpath (names "/Block 3/") (tstamps /0000BB33/))
      (tstamp 5AFC50F9))
    (comp (ref R1.3)
      (value 47k)
      (footprint Resistor_SMD.pretty:R_0805_2012Metric_Pad1.29x1.40mm_HandSolder)
      (libsource (lib Device) (part R))
      (sheetpath (names "/Block 3/") (tstamps /0000BB33/))
      (tstamp 5AFC5111))
    (comp (ref J3.3)
      (value SDA/SCL)
      (footprint mylib:8pair)
      (libsource (lib Connector_Generic) (part Conn_02x08_Top_Bottom))
      (sheetpath (names "/Block 3/") (tstamps /0000BB33/))
      (tstamp 5AFC511E))
    (comp (ref R4.3)
      (value 4k7)
      (footprint Resistor_SMD.pretty:R_0805_2012Metric_Pad1.29x1.40mm_HandSolder)
      (libsource (lib Device) (part R))
      (sheetpath (names "/Block 3/") (tstamps /0000BB33/))
      (tstamp 5AFC513F))
    (comp (ref R6.3)
      (value 4k7)
      (footprint Resistor_SMD.pretty:R_0805_2012Metric_Pad1.29x1.40mm_HandSolder)
      (libsource (lib Device) (part R))
      (sheetpath (names "/Block 3/") (tstamps /0000BB33/))
      (tstamp 5AFC5146))
    (comp (ref R2.3)
      (value 4k7)
      (footprint Resistor_SMD.pretty:R_0805_2012Metric_Pad1.29x1.40mm_HandSolder)
      (libsource (lib Device) (part R))
      (sheetpath (names "/Block 3/") (tstamps /0000BB33/))
      (tstamp 5AFC514D))
    (comp (ref R7.3)
      (value 4k7)
      (footprint Resistor_SMD.pretty:R_0805_2012Metric_Pad1.29x1.40mm_HandSolder)
      (libsource (lib Device) (part R))
      (sheetpath (names "/Block 3/") (tstamps /0000BB33/))
      (tstamp 5AFC5154))
    (comp (ref R5.3)
      (value 4k7)
      (footprint Resistor_SMD.pretty:R_0805_2012Metric_Pad1.29x1.40mm_HandSolder)
      (libsource (lib Device) (part R))
      (sheetpath (names "/Block 3/") (tstamps /0000BB33/))
      (tstamp 5AFC515B))
    (comp (ref R3.3)
      (value 4k7)
      (footprint Resistor_SMD.pretty:R_0805_2012Metric_Pad1.29x1.40mm_HandSolder)
      (libsource (lib Device) (part R))
      (sheetpath (names "/Block 3/") (tstamps /0000BB33/))
      (tstamp 5AFC5162))
    (comp (ref R8.3)
      (value 4k7)
      (footprint Resistor_SMD.pretty:R_0805_2012Metric_Pad1.29x1.40mm_HandSolder)
      (libsource (lib Device) (part R))
      (sheetpath (names "/Block 3/") (tstamps /0000BB33/))
      (tstamp 5AFC5169))
    (comp (ref R9.3)
      (value 4k7)
      (footprint Resistor_SMD.pretty:R_0805_2012Metric_Pad1.29x1.40mm_HandSolder)
      (libsource (lib Device) (part R))
      (sheetpath (names "/Block 3/") (tstamps /0000BB33/))
      (tstamp 5AFC5170))
    (comp (ref U3.4)
      (value 74HC4051)
      (footprint Package_SO.pretty:SOIC-16_3.9x9.9mm_P1.27mm)
      (libsource (lib 74xx) (part 74HC4051))
      (sheetpath (names "/Block 4/") (tstamps /0000BB44/))
      (tstamp 5AFC50F9))
    (comp (ref R1.4)
      (value 47k)
      (footprint Resistor_SMD.pretty:R_0805_2012Metric_Pad1.29x1.40mm_HandSolder)
      (libsource (lib Device) (part R))
      (sheetpath (names "/Block 4/") (tstamps /0000BB44/))
      (tstamp 5AFC5111))
    (comp (ref J3.4)
      (value SDA/SCL)
      (footprint mylib:8pair)
      (libsource (lib Connector_Generic) (part Conn_02x08_Top_Bottom))
      (sheetpath (names "/Block 4/") (tstamps /0000BB44/))
      (tstamp 5AFC511E))
    (comp (ref R4.4)
      (value 4k7)
      (footprint Resistor_SMD.pretty:R_0805_2012Metric_Pad1.29x1.40mm_HandSolder)
      (libsource (lib Device) (part R))
      (sheetpath (names "/Block 4/") (tstamps /0000BB44/))
      (tstamp 5AFC513F))
    (comp (ref R6.4)
      (value 4k7)
      (footprint Resistor_SMD.pretty:R_0805_2012Metric_Pad1.29x1.40mm_HandSolder)
      (libsource (lib Device) (part R))
      (sheetpath (names "/Block 4/") (tstamps /0000BB44/))
      (tstamp 5AFC5146))
    (comp (ref R2.4)
      (value 4k7)
      (footprint Resistor_SMD.pretty:R_0805_2012Metric_Pad1.29x1.40mm_HandSolder)
      (libsource (lib Device) (part R))
      (sheetpath (names "/Block 4/") (tstamps /0000BB44/))
      (tstamp 5AFC514D))
    (comp (ref R7.4)
      (value 4k7)
      (footprint Resistor_SMD.pretty:R_0805_2012Metric_Pad1.29x1.40mm_HandSolder)
      (libsource (lib Device) (part R))
      (sheetpath (names "/Block 4/") (tstamps /0000BB44/))
      (tstamp 5AFC5154))
    (comp (ref R5.4)
      (value 4k7)
      (footprint Resistor_SMD.pretty:R_0805_2012Metric_Pad1.29x1.40mm_HandSolder)
      (libsource (lib Device) (part R))
      (sheetpath (names "/Block 4/") (tstamps /0000BB44/))
      (tstamp 5AFC515B))
    (comp (ref R3.4)
      (value 4k7)
      (footprint Resistor_SMD.pretty:R_0805_2012Metric_Pad1.29x1.40mm_HandSolder)
      (libsource (lib Device) (part R))
      (sheetpath (names "/Block 4/") (tstamps /0000BB44/))
      (tstamp 5AFC5162))
    (comp (ref R8.4)
      (value 4k7)
      (footprint Resistor_SMD.pretty:R_0805_2012Metric_Pad1.29x1.40mm_HandSolder)
      (libsource (lib Device) (part R))
      (sheetpath (names "/Block 4/") (tstamps /0000BB44/))
      (tstamp 5AFC5169))
    (comp (ref R9.4)
      (value 4k7)
      (footprint Resistor_SMD.pretty:R_0805_2012Metric_Pad1.29x1.40mm_HandSolder)
      (libsource (lib Device) (part R))
      (sheetpath (names "/Block 4/") (tstamps /0000BB44/))
      (tstamp 5AFC5170))
    (comp (ref U3.5)
      (value 74HC4051)
      (footprint Package_SO.pretty:SOIC-16_3.9x9.9mm_P1.27mm)
      (libsource (lib 74xx) (part 74HC4051))
      (sheetpath (names "/Block 5/") (tstamps /0000BB55/))
      (tstamp 5AFC50F9))
    (comp (ref R1.5)
      (value 47k)
      (footprint Resistor_SMD.pretty:R_0805_2012Metric_Pad1.29x1.40mm_HandSolder)
      (libsource (lib Device) (part R))
      (sheetpath (names "/Block 5/") (tstamps /0000BB55/))
      (tstamp 5AFC5111))
    (comp (ref J3.5)
      (value SDA/SCL)
      (footprint mylib:8pair)
      (libsource (lib Connector_Generic) (part Conn_02x08_Top_Bottom))
      (sheetpath (names "/Block 5/") (tstamps /0000BB55/))
      (tstamp 5AFC511E))
    (comp (ref R4.5)
      (value 4k7)
      (footprint Resistor_SMD.pretty:R_0805_2012Metric_Pad1.29x1.40mm_HandSolder)
      (libsource (lib Device) (part R))
      (sheetpath (names "/Block 5/") (tstamps /0000BB55/))
      (tstamp 5AFC513F))
    (comp (ref R6.5)
      (value 4k7)
      (footprint Resistor_SMD.pretty:R_0805_2012Metric_Pad1.29x1.40mm_HandSolder)
      (libsource (lib Device) (part R))
      (sheetpath (names "/Block 5/") (tstamps /0000BB55/))
      (tstamp 5AFC5146))
    (comp (ref R2.5)
      (value 4k7)
      (footprint Resistor_SMD.pretty:R_0805_2012Metric_Pad1.29x1.40mm_HandSolder)
      (libsource (lib Device) (part R))
      (sheetpath (names "/Block 5/") (tstamps /0000BB55/))
      (tstamp 5AFC514D))
    (comp (ref R7.5)
      (value 4k7)
      (footprint Resistor_SMD.pretty:R_0805_2012Metric_Pad1.29x1.40mm_HandSolder)
      (libsource (lib Device) (part R))
      (sheetpath (names "/Block 5/") (tstamps /0000BB55/))
      (tstamp 5AFC5154))
    (comp (ref R5.5)
      (value 4k7)
      (footprint Resistor_SMD.pretty:R_0805_2012Metric_Pad1.29x1.40mm_HandSolder)
      (libsource (lib Device) (part R))
      (sheetpath (names "/Block 5/") (tstamps /0000BB55/))
      (tstamp 5AFC515B))
    (comp (ref R3.5)
      (value 4k7)
      (footprint Resistor_SMD.pretty:R_0805_2012Metric_Pad1.29x1.40mm_HandSolder)
      (libsource (lib Device) (part R))
      (sheetpath (names "/Block 5/") (tstamps /0000BB55/))
      (tstamp 5AFC5162))
    (comp (ref R8.5)
      (value 4k7)
      (footprint Resistor_SMD.pretty:R_0805_2012Metric_Pad1.29x1.40mm_HandSolder)
      (libsource (lib Device) (part R))
      (sheetpath (names "/Block 5/") (tstamps /0000BB55/))
      (tstamp 5AFC5169))
    (comp (ref R9.5)
      (value 4k7)
      (footprint Resistor_SMD.pretty:R_0805_2012Metric_Pad1.29x1.40mm_HandSolder)
      (libsource (lib Device) (part R))
      (sheetpath (names "/Block 5/") (tstamps /0000BB55/))
      (tstamp 5AFC5170))
    (comp (ref U3.6)
      (value 74HC4051)
      (footprint Package_SO.pretty:SOIC-16_3.9x9.9mm_P1.27mm)
      (libsource (lib 74xx) (part 74HC4051))
      (sheetpath (names "/Block 6/") (tstamps /0000BB66/))
      (tstamp 5AFC50F9))
    (comp (ref R1.6)
      (value 47k)
      (footprint Resistor_SMD.pretty:R_0805_2012Metric_Pad1.29x1.40mm_HandSolder)
      (libsource (lib Device) (part R))
      (sheetpath (names "/Block 6/") (tstamps /0000BB66/))
      (tstamp 5AFC5111))
    (comp (ref J3.6)
      (value SDA/SCL)
      (footprint mylib:8pair)
      (libsource (lib Connector_Generic) (part Conn_02x08_Top_Bottom))
      (sheetpath (names "/Block 6/") (tstamps /0000BB66/))
      (tstamp 5AFC511E))
    (comp (ref R4.6)
      (value 4k7)
      (footprint Resistor_SMD.pretty:R_0805_2012Metric_Pad1.29x1.40mm_HandSolder)
      (libsource (lib Device) (part R))
      (sheetpath (names "/Block 6/") (tstamps /0000BB66/))
      (tstamp 5AFC513F))
    (comp (ref R6.6)
      (value 4k7)
      (footprint Resistor_SMD.pretty:R_0805_2012Metric_Pad1.29x1.40mm_HandSolder)
      (libsource (lib Device) (part R))
      (sheetpath (names "/Block 6/") (tstamps /0000BB66/))
      (tstamp 5AFC5146))
    (comp (ref R2.6)
      (value 4k7)
      (footprint Resistor_SMD.pretty:R_0805_2012Metric_Pad1.29x1.40mm_HandSolder)
      (libsource (lib Device) (part R))
      (sheetpath (names "/Block 6/") (tstamps /0000BB66/))
      (tstamp 5AFC514D))
    (comp (ref R7.6)
      (value 4k7)
      (footprint Resistor_SMD.pretty:R_0805_2012Metric_Pad1.29x1.40mm_HandSolder)
      (libsource (lib Device) (part R))
      (sheetpath (names "/Block 6/") (tstamps /0000BB66/))
      (tstamp 5AFC5154))
    (comp (ref R5.6)
      (value 4k7)
      (footprint Resistor_SMD.pretty:R_0805_2012Metric_Pad1.29x1.40mm_HandSolder)
      (libsource (lib Device) (part R))
      (sheetpath (names "/Block 6/") (tstamps /0000BB66/))
      (tstamp 5AFC515B))
    (comp (ref R3.6)
      (value 4k7)
      (footprint Resistor_SMD.pretty:R_0805_2012Metric_Pad1.29x1.40mm_HandSolder)
      (libsource (lib Device) (part R))
      (sheetpath (names "/Block 6/") (tstamps /0000BB66/))
      (tstamp 5AFC5162))
    (comp (ref R8.6)
      (value 4k7)
      (footprint Resistor_SMD.pretty:R_0805_2012Metric_Pad1.29x1.40mm_HandSolder)
      (libsource (lib Device) (part R))
      (sheetpath (names "/Block 6/") (tstamps /0000BB66/))
      (tstamp 5AFC5169))
    (comp (ref R9.6)
      (value 4k7)
      (footprint Resistor_SMD.pretty:R_0805_2012Metric_Pad1.29x1.40mm_HandSolder)
      (libsource (lib Device) (part R))
      (sheetpath (names "/Block 6/") (tstamps /0000BB66/))
      (tstamp 5AFC5170)))
  (libparts
    (libpart (lib 74xx) (part 74HC4051)
      (aliases
        (alias 74HCT4051))
      (footprints
        (fp DIP*W7.62mm*)
        (fp SOIC*3.9x9.9mm*P1.27mm*)
        (fp SOIC*5.3x10.2mm*P1.27mm*)
        (fp TSSOP*4.4x5mm*P0.65mm*))
      (fields
        (field (name Reference) U)
        (field (name Value) 74HC4051))
      (pins
        (pin (num 1) (name A4) (type passive))
        (pin (num 2) (name A6) (type passive))
        (pin (num 3) (name A) (type passive))
        (pin (num 4) (name A7) (type passive))
        (pin (num 5) (name A5) (type passive))
        (pin (num 6) (name ~E) (type input))
        (pin (num 7) (name VEE) (type power_in))
        (pin (num 8) (name GND) (type power_in))
        (pin (num 9) (name S2) (type input))
        (pin (num 10) (name S1) (type input))
        (pin (num 11) (name S0) (type input))
        (pin (num 12) (name A3) (type passive))
        (pin (num 13) (name A0) (type passive))
        (pin (num 14) (name A1) (type passive))
        (pin (num 15) (name A2) (type passive))
        (pin (num 16) (name VCC) (type power_in))))
    (libpart (lib Device) (part C)
      (footprints
        (fp C_*))
      (fields
        (field (name Reference) C)
        (field (name Value) C))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib Device) (part CP)
      (footprints
        (fp CP_*))
      (fields
        (field (name Reference) C)
        (field (name Value) CP))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib Connector) (part Conn_01x03_Male)
      (footprints
        (fp Connector*:*_1x??_*))
      (fields
        (field (name Reference) J)
        (field (name Value) Conn_01x03_Male))
      (pins
        (pin (num 1) (name Pin_1) (type passive))
        (pin (num 2) (name Pin_2) (type passive))
        (pin (num 3) (name Pin_3) (type passive))))
    (libpart (lib Connector) (part Conn_01x06_Male)
      (footprints
        (fp Connector*:*_1x??_*))
      (fields
        (field (name Reference) J)
        (field (name Value) Conn_01x06_Male))
      (pins
        (pin (num 1) (name Pin_1) (type passive))
        (pin (num 2) (name Pin_2) (type passive))
        (pin (num 3) (name Pin_3) (type passive))
        (pin (num 4) (name Pin_4) (type passive))
        (pin (num 5) (name Pin_5) (type passive))
        (pin (num 6) (name Pin_6) (type passive))))
    (libpart (lib Connector_Generic) (part Conn_02x08_Top_Bottom)
      (footprints
        (fp Connector*:*_2x??_*))
      (fields
        (field (name Reference) J)
        (field (name Value) Conn_02x08_Top_Bottom))
      (pins
        (pin (num 1) (name Pin_1) (type passive))
        (pin (num 2) (name Pin_2) (type passive))
        (pin (num 3) (name Pin_3) (type passive))
        (pin (num 4) (name Pin_4) (type passive))
        (pin (num 5) (name Pin_5) (type passive))
        (pin (num 6) (name Pin_6) (type passive))
        (pin (num 7) (name Pin_7) (type passive))
        (pin (num 8) (name Pin_8) (type passive))
        (pin (num 9) (name Pin_9) (type passive))
        (pin (num 10) (name Pin_10) (type passive))
        (pin (num 11) (name Pin_11) (type passive))
        (pin (num 12) (name Pin_12) (type passive))
        (pin (num 13) (name Pin_13) (type passive))
        (pin (num 14) (name Pin_14) (type passive))
        (pin (num 15) (name Pin_15) (type passive))
        (pin (num 16) (name Pin_16) (type passive))))
    (libpart (lib Regulator_Linear) (part LM1117-1.8)
      (aliases
        (alias LM1117-2.5)
        (alias LM1117-3.3)
        (alias LM1117-5.0)
        (alias TLV1117-15)
        (alias TLV1117-18)
        (alias TLV1117-25)
        (alias TLV1117-33)
        (alias TLV1117-50))
      (footprints
        (fp SOT?223*)
        (fp TO?263*)
        (fp TO?252*)
        (fp TO?220*))
      (fields
        (field (name Reference) U)
        (field (name Value) LM1117-1.8))
      (pins
        (pin (num 1) (name GND) (type power_in))
        (pin (num 2) (name VO) (type power_out))
        (pin (num 3) (name VI) (type power_in))))
    (libpart (lib Device) (part R)
      (footprints
        (fp R_*))
      (fields
        (field (name Reference) R)
        (field (name Value) R))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib Connector) (part Screw_Terminal_01x02)
      (footprints
        (fp TerminalBlock*:*))
      (fields
        (field (name Reference) J)
        (field (name Value) Screw_Terminal_01x02))
      (pins
        (pin (num 1) (name Pin_1) (type passive))
        (pin (num 2) (name Pin_2) (type passive)))))
  (libraries
    (library (logical 74xx)
      (uri /usr/share/kicad/kicad-symbols/74xx.lib))
    (library (logical Device)
      (uri /usr/share/kicad/kicad-symbols/Device.lib))
    (library (logical Connector)
      (uri /usr/share/kicad/kicad-symbols/Connector.lib))
    (library (logical Connector_Generic)
      (uri /usr/share/kicad/kicad-symbols/Connector_Generic.lib))
    (library (logical Regulator_Linear)
      (uri /usr/share/kicad/kicad-symbols/Regulator_Linear.lib)))
  (nets
    (net (code 1) (name /ADDR1)
      (node (ref U3.2) (pin 10))
      (node (ref J3) (pin 2))
      (node (ref U3.6) (pin 10))
      (node (ref U3.1) (pin 10))
      (node (ref U3.4) (pin 10))
      (node (ref U3.3) (pin 10))
      (node (ref U3.5) (pin 10)))
    (net (code 2) (name /MUL3)
      (node (ref R1.4) (pin 1))
      (node (ref U3.4) (pin 6))
      (node (ref U1) (pin 12)))
    (net (code 3) (name /ADDR0)
      (node (ref U3.5) (pin 11))
      (node (ref U3.4) (pin 11))
      (node (ref J3) (pin 1))
      (node (ref U3.6) (pin 11))
      (node (ref U3.1) (pin 11))
      (node (ref U3.2) (pin 11))
      (node (ref U3.3) (pin 11)))
    (net (code 4) (name /I2C_SDA)
      (node (ref J2) (pin 1))
      (node (ref U3.1) (pin 3))
      (node (ref U3.2) (pin 3))
      (node (ref U3.4) (pin 3))
      (node (ref U3.3) (pin 3))
      (node (ref U3.5) (pin 3))
      (node (ref U3.6) (pin 3)))
    (net (code 5) (name /MUL5)
      (node (ref U3.6) (pin 6))
      (node (ref U1) (pin 5))
      (node (ref R1.6) (pin 1)))
    (net (code 6) (name /ADDR2)
      (node (ref U3.1) (pin 9))
      (node (ref U3.3) (pin 9))
      (node (ref U3.6) (pin 9))
      (node (ref U3.2) (pin 9))
      (node (ref U3.4) (pin 9))
      (node (ref U3.5) (pin 9))
      (node (ref J3) (pin 3)))
    (net (code 7) (name /I2C_SCL)
      (node (ref J3.1) (pin 15))
      (node (ref J3.1) (pin 16))
      (node (ref J3.6) (pin 14))
      (node (ref J3.6) (pin 15))
      (node (ref J3.6) (pin 16))
      (node (ref J3.2) (pin 9))
      (node (ref J2) (pin 2))
      (node (ref J3.6) (pin 11))
      (node (ref J3.6) (pin 12))
      (node (ref J3.1) (pin 9))
      (node (ref J3.1) (pin 10))
      (node (ref J3.1) (pin 14))
      (node (ref J3.6) (pin 10))
      (node (ref J3.6) (pin 13))
      (node (ref J3.1) (pin 12))
      (node (ref J3.1) (pin 11))
      (node (ref J3.1) (pin 13))
      (node (ref J3.5) (pin 15))
      (node (ref J3.5) (pin 10))
      (node (ref J3.5) (pin 12))
      (node (ref J3.5) (pin 13))
      (node (ref J3.5) (pin 14))
      (node (ref J3.4) (pin 9))
      (node (ref J3.4) (pin 11))
      (node (ref J3.5) (pin 16))
      (node (ref J3.4) (pin 15))
      (node (ref J3.5) (pin 9))
      (node (ref J3.4) (pin 16))
      (node (ref J3.4) (pin 14))
      (node (ref J3.4) (pin 13))
      (node (ref J3.4) (pin 12))
      (node (ref J3.4) (pin 10))
      (node (ref J3.5) (pin 11))
      (node (ref J3.2) (pin 15))
      (node (ref J3.2) (pin 16))
      (node (ref J3.2) (pin 14))
      (node (ref J3.2) (pin 13))
      (node (ref J3.2) (pin 12))
      (node (ref J3.2) (pin 10))
      (node (ref J3.2) (pin 11))
      (node (ref J3.6) (pin 9))
      (node (ref J3.3) (pin 9))
      (node (ref J3.3) (pin 10))
      (node (ref J3.3) (pin 12))
      (node (ref J3.3) (pin 11))
      (node (ref J3.3) (pin 13))
      (node (ref J3.3) (pin 14))
      (node (ref J3.3) (pin 15))
      (node (ref J3.3) (pin 16)))
    (net (code 8) (name +5V)
      (node (ref R1.5) (pin 2))
      (node (ref U3.5) (pin 16))
      (node (ref U3.4) (pin 16))
      (node (ref U3.1) (pin 16))
      (node (ref C1.1) (pin 1))
      (node (ref U3.6) (pin 16))
      (node (ref R1.1) (pin 2))
      (node (ref C1.6) (pin 1))
      (node (ref U2) (pin 3))
      (node (ref U3.3) (pin 16))
      (node (ref C1.2) (pin 1))
      (node (ref C1.5) (pin 1))
      (node (ref U1) (pin 16))
      (node (ref R1.6) (pin 2))
      (node (ref C8) (pin 1))
      (node (ref C2) (pin 1))
      (node (ref R1.4) (pin 2))
      (node (ref J1) (pin 2))
      (node (ref C1.3) (pin 1))
      (node (ref U3.2) (pin 16))
      (node (ref C1.4) (pin 1))
      (node (ref R1.2) (pin 2))
      (node (ref R1.3) (pin 2)))
    (net (code 9) (name GND)
      (node (ref U3.3) (pin 8))
      (node (ref U3.2) (pin 7))
      (node (ref U3.2) (pin 8))
      (node (ref U1) (pin 8))
      (node (ref C1.4) (pin 2))
      (node (ref U3.6) (pin 8))
      (node (ref U3.6) (pin 7))
      (node (ref C1.3) (pin 2))
      (node (ref C1.2) (pin 2))
      (node (ref U3.5) (pin 8))
      (node (ref U3.3) (pin 7))
      (node (ref C2) (pin 2))
      (node (ref C1.6) (pin 2))
      (node (ref C8) (pin 2))
      (node (ref C9) (pin 2))
      (node (ref U2) (pin 1))
      (node (ref J1) (pin 1))
      (node (ref C1.5) (pin 2))
      (node (ref J2) (pin 3))
      (node (ref U1) (pin 3))
      (node (ref U3.1) (pin 8))
      (node (ref U3.1) (pin 7))
      (node (ref U3.4) (pin 7))
      (node (ref U3.4) (pin 8))
      (node (ref U1) (pin 6))
      (node (ref U1) (pin 7))
      (node (ref C1.1) (pin 2))
      (node (ref U3.5) (pin 7)))
    (net (code 10) (name /MUL1)
      (node (ref U1) (pin 14))
      (node (ref R1.2) (pin 1))
      (node (ref U3.2) (pin 6)))
    (net (code 11) (name +3V3)
      (node (ref R6.5) (pin 1))
      (node (ref R4.4) (pin 1))
      (node (ref R4.5) (pin 1))
      (node (ref R6.4) (pin 1))
      (node (ref R2.6) (pin 1))
      (node (ref R7.6) (pin 1))
      (node (ref R5.6) (pin 1))
      (node (ref R3.6) (pin 1))
      (node (ref R9.5) (pin 1))
      (node (ref R8.5) (pin 1))
      (node (ref R3.5) (pin 1))
      (node (ref R5.5) (pin 1))
      (node (ref R7.5) (pin 1))
      (node (ref R2.5) (pin 1))
      (node (ref R7.4) (pin 1))
      (node (ref R2.4) (pin 1))
      (node (ref R5.4) (pin 1))
      (node (ref R6.3) (pin 1))
      (node (ref R4.3) (pin 1))
      (node (ref R8.6) (pin 1))
      (node (ref R9.6) (pin 1))
      (node (ref R9.4) (pin 1))
      (node (ref R8.4) (pin 1))
      (node (ref R3.4) (pin 1))
      (node (ref R8.1) (pin 1))
      (node (ref R6.2) (pin 1))
      (node (ref R6.1) (pin 1))
      (node (ref R4.1) (pin 1))
      (node (ref R9.1) (pin 1))
      (node (ref R2.2) (pin 1))
      (node (ref R7.2) (pin 1))
      (node (ref R5.2) (pin 1))
      (node (ref R3.1) (pin 1))
      (node (ref R3.2) (pin 1))
      (node (ref R8.2) (pin 1))
      (node (ref R5.1) (pin 1))
      (node (ref R9.2) (pin 1))
      (node (ref R7.1) (pin 1))
      (node (ref R2.1) (pin 1))
      (node (ref C9) (pin 1))
      (node (ref R6.6) (pin 1))
      (node (ref R8.3) (pin 1))
      (node (ref R2.3) (pin 1))
      (node (ref R7.3) (pin 1))
      (node (ref R5.3) (pin 1))
      (node (ref R3.3) (pin 1))
      (node (ref R4.6) (pin 1))
      (node (ref R9.3) (pin 1))
      (node (ref R4.2) (pin 1))
      (node (ref U2) (pin 2)))
    (net (code 12) (name /MUL2)
      (node (ref R1.3) (pin 1))
      (node (ref U1) (pin 15))
      (node (ref U3.3) (pin 6)))
    (net (code 13) (name /MUL4)
      (node (ref U3.5) (pin 6))
      (node (ref R1.5) (pin 1))
      (node (ref U1) (pin 1)))
    (net (code 14) (name /ADDR3)
      (node (ref U1) (pin 11))
      (node (ref J3) (pin 4)))
    (net (code 15) (name /ADDR4)
      (node (ref J3) (pin 5))
      (node (ref U1) (pin 10)))
    (net (code 16) (name /ADDR5)
      (node (ref J3) (pin 6))
      (node (ref U1) (pin 9)))
    (net (code 17) (name /MUL0)
      (node (ref R1.1) (pin 1))
      (node (ref U3.1) (pin 6))
      (node (ref U1) (pin 13)))
    (net (code 18) (name "Net-(U1-Pad4)")
      (node (ref U1) (pin 4)))
    (net (code 19) (name "Net-(U1-Pad2)")
      (node (ref U1) (pin 2)))
    (net (code 20) (name "/Block 1/CH6")
      (node (ref J3.1) (pin 5))
      (node (ref R6.1) (pin 2))
      (node (ref U3.1) (pin 2)))
    (net (code 21) (name "/Block 1/CH7")
      (node (ref U3.1) (pin 4))
      (node (ref R5.1) (pin 2))
      (node (ref J3.1) (pin 4)))
    (net (code 22) (name "/Block 1/CH5")
      (node (ref J3.1) (pin 3))
      (node (ref R4.1) (pin 2))
      (node (ref U3.1) (pin 5)))
    (net (code 23) (name "/Block 1/CH3")
      (node (ref J3.1) (pin 1))
      (node (ref U3.1) (pin 12))
      (node (ref R2.1) (pin 2)))
    (net (code 24) (name "/Block 1/CH4")
      (node (ref J3.1) (pin 6))
      (node (ref R7.1) (pin 2))
      (node (ref U3.1) (pin 1)))
    (net (code 25) (name "/Block 1/CH2")
      (node (ref J3.1) (pin 8))
      (node (ref U3.1) (pin 15))
      (node (ref R8.1) (pin 2)))
    (net (code 26) (name "/Block 1/CH0")
      (node (ref U3.1) (pin 13))
      (node (ref R3.1) (pin 2))
      (node (ref J3.1) (pin 2)))
    (net (code 27) (name "/Block 1/CH1")
      (node (ref R9.1) (pin 2))
      (node (ref J3.1) (pin 7))
      (node (ref U3.1) (pin 14)))
    (net (code 28) (name "/Block 2/CH4")
      (node (ref U3.2) (pin 1))
      (node (ref J3.2) (pin 6))
      (node (ref R7.2) (pin 2)))
    (net (code 29) (name "/Block 2/CH6")
      (node (ref U3.2) (pin 2))
      (node (ref J3.2) (pin 5))
      (node (ref R6.2) (pin 2)))
    (net (code 30) (name "/Block 2/CH7")
      (node (ref R5.2) (pin 2))
      (node (ref J3.2) (pin 4))
      (node (ref U3.2) (pin 4)))
    (net (code 31) (name "/Block 2/CH5")
      (node (ref R4.2) (pin 2))
      (node (ref J3.2) (pin 3))
      (node (ref U3.2) (pin 5)))
    (net (code 32) (name "/Block 2/CH3")
      (node (ref U3.2) (pin 12))
      (node (ref J3.2) (pin 1))
      (node (ref R2.2) (pin 2)))
    (net (code 33) (name "/Block 2/CH0")
      (node (ref U3.2) (pin 13))
      (node (ref R3.2) (pin 2))
      (node (ref J3.2) (pin 2)))
    (net (code 34) (name "/Block 2/CH1")
      (node (ref U3.2) (pin 14))
      (node (ref R9.2) (pin 2))
      (node (ref J3.2) (pin 7)))
    (net (code 35) (name "/Block 2/CH2")
      (node (ref J3.2) (pin 8))
      (node (ref R8.2) (pin 2))
      (node (ref U3.2) (pin 15)))
    (net (code 36) (name "/Block 3/CH6")
      (node (ref U3.3) (pin 2))
      (node (ref J3.3) (pin 5))
      (node (ref R6.3) (pin 2)))
    (net (code 37) (name "/Block 3/CH7")
      (node (ref J3.3) (pin 4))
      (node (ref U3.3) (pin 4))
      (node (ref R5.3) (pin 2)))
    (net (code 38) (name "/Block 3/CH5")
      (node (ref R4.3) (pin 2))
      (node (ref J3.3) (pin 3))
      (node (ref U3.3) (pin 5)))
    (net (code 39) (name "/Block 3/CH3")
      (node (ref U3.3) (pin 12))
      (node (ref J3.3) (pin 1))
      (node (ref R2.3) (pin 2)))
    (net (code 40) (name "/Block 3/CH4")
      (node (ref J3.3) (pin 6))
      (node (ref U3.3) (pin 1))
      (node (ref R7.3) (pin 2)))
    (net (code 41) (name "/Block 3/CH0")
      (node (ref R3.3) (pin 2))
      (node (ref J3.3) (pin 2))
      (node (ref U3.3) (pin 13)))
    (net (code 42) (name "/Block 3/CH1")
      (node (ref J3.3) (pin 7))
      (node (ref R9.3) (pin 2))
      (node (ref U3.3) (pin 14)))
    (net (code 43) (name "/Block 3/CH2")
      (node (ref U3.3) (pin 15))
      (node (ref R8.3) (pin 2))
      (node (ref J3.3) (pin 8)))
    (net (code 44) (name "/Block 4/CH4")
      (node (ref U3.4) (pin 1))
      (node (ref R7.4) (pin 2))
      (node (ref J3.4) (pin 6)))
    (net (code 45) (name "/Block 4/CH6")
      (node (ref R6.4) (pin 2))
      (node (ref J3.4) (pin 5))
      (node (ref U3.4) (pin 2)))
    (net (code 46) (name "/Block 4/CH7")
      (node (ref J3.4) (pin 4))
      (node (ref R5.4) (pin 2))
      (node (ref U3.4) (pin 4)))
    (net (code 47) (name "/Block 4/CH5")
      (node (ref U3.4) (pin 5))
      (node (ref R4.4) (pin 2))
      (node (ref J3.4) (pin 3)))
    (net (code 48) (name "/Block 4/CH3")
      (node (ref J3.4) (pin 1))
      (node (ref R2.4) (pin 2))
      (node (ref U3.4) (pin 12)))
    (net (code 49) (name "/Block 4/CH0")
      (node (ref R3.4) (pin 2))
      (node (ref J3.4) (pin 2))
      (node (ref U3.4) (pin 13)))
    (net (code 50) (name "/Block 4/CH1")
      (node (ref R9.4) (pin 2))
      (node (ref U3.4) (pin 14))
      (node (ref J3.4) (pin 7)))
    (net (code 51) (name "/Block 4/CH2")
      (node (ref R8.4) (pin 2))
      (node (ref U3.4) (pin 15))
      (node (ref J3.4) (pin 8)))
    (net (code 52) (name "/Block 5/CH4")
      (node (ref U3.5) (pin 1))
      (node (ref R7.5) (pin 2))
      (node (ref J3.5) (pin 6)))
    (net (code 53) (name "/Block 5/CH6")
      (node (ref J3.5) (pin 5))
      (node (ref U3.5) (pin 2))
      (node (ref R6.5) (pin 2)))
    (net (code 54) (name "/Block 5/CH7")
      (node (ref J3.5) (pin 4))
      (node (ref R5.5) (pin 2))
      (node (ref U3.5) (pin 4)))
    (net (code 55) (name "/Block 5/CH5")
      (node (ref R4.5) (pin 2))
      (node (ref U3.5) (pin 5))
      (node (ref J3.5) (pin 3)))
    (net (code 56) (name "/Block 5/CH3")
      (node (ref J3.5) (pin 1))
      (node (ref R2.5) (pin 2))
      (node (ref U3.5) (pin 12)))
    (net (code 57) (name "/Block 5/CH0")
      (node (ref J3.5) (pin 2))
      (node (ref R3.5) (pin 2))
      (node (ref U3.5) (pin 13)))
    (net (code 58) (name "/Block 5/CH1")
      (node (ref J3.5) (pin 7))
      (node (ref U3.5) (pin 14))
      (node (ref R9.5) (pin 2)))
    (net (code 59) (name "/Block 5/CH2")
      (node (ref R8.5) (pin 2))
      (node (ref J3.5) (pin 8))
      (node (ref U3.5) (pin 15)))
    (net (code 60) (name "/Block 6/CH4")
      (node (ref R7.6) (pin 2))
      (node (ref U3.6) (pin 1))
      (node (ref J3.6) (pin 6)))
    (net (code 61) (name "/Block 6/CH6")
      (node (ref J3.6) (pin 5))
      (node (ref U3.6) (pin 2))
      (node (ref R6.6) (pin 2)))
    (net (code 62) (name "/Block 6/CH7")
      (node (ref R5.6) (pin 2))
      (node (ref U3.6) (pin 4))
      (node (ref J3.6) (pin 4)))
    (net (code 63) (name "/Block 6/CH5")
      (node (ref R4.6) (pin 2))
      (node (ref J3.6) (pin 3))
      (node (ref U3.6) (pin 5)))
    (net (code 64) (name "/Block 6/CH3")
      (node (ref J3.6) (pin 1))
      (node (ref R2.6) (pin 2))
      (node (ref U3.6) (pin 12)))
    (net (code 65) (name "/Block 6/CH0")
      (node (ref U3.6) (pin 13))
      (node (ref J3.6) (pin 2))
      (node (ref R3.6) (pin 2)))
    (net (code 66) (name "/Block 6/CH1")
      (node (ref R9.6) (pin 2))
      (node (ref U3.6) (pin 14))
      (node (ref J3.6) (pin 7)))
    (net (code 67) (name "/Block 6/CH2")
      (node (ref R8.6) (pin 2))
      (node (ref U3.6) (pin 15))
      (node (ref J3.6) (pin 8)))))