(export (version D)
  (design
    (source /tmp/kicad/tsys01.sch)
    (date "Ср 31 май 2017 08:29:04")
    (tool "Eeschema 4.0.6")
    (sheet (number 1) (name /) (tstamps /)
      (title_block
        (title)
        (company)
        (rev)
        (date)
        (source tsys01.sch)
        (comment (number 1) (value ""))
        (comment (number 2) (value ""))
        (comment (number 3) (value ""))
        (comment (number 4) (value "")))))
  (components
    (comp (ref U1)
      (value TSYS01)
      (footprint QFN-16-1EP_4x4mm_Pitch0.65mm)
      (libsource (lib tsys01) (part TSYS01))
      (sheetpath (names /) (tstamps /))
      (tstamp 58B8439D))
    (comp (ref C1)
      (value 100n)
      (footprint Capacitors_SMD.pretty:C_0603)
      (libsource (lib device) (part C))
      (sheetpath (names /) (tstamps /))
      (tstamp 58B85507))
    (comp (ref R1)
      (value 4k7)
      (footprint Resistors_SMD.pretty:R_0603)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 58B85A14))
    (comp (ref R2)
      (value 4k7)
      (footprint Resistors_SMD.pretty:R_0603)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 58B85BA0))
    (comp (ref P1)
      (value CONN_01X04)
      (footprint my_footprints:SMD_conn_4x2.5mm)
      (libsource (lib conn) (part CONN_01X04))
      (sheetpath (names /) (tstamps /))
      (tstamp 58B85ED6))
    (comp (ref Hole1)
      (value "Hole 3mm")
      (footprint my_footprints:Hole_3mm)
      (libsource (lib conn) (part CONN_01X01))
      (sheetpath (names /) (tstamps /))
      (tstamp 592E54A8))
    (comp (ref Hole2)
      (value "Hole 3mm")
      (footprint my_footprints:Hole_3mm)
      (libsource (lib conn) (part CONN_01X01))
      (sheetpath (names /) (tstamps /))
      (tstamp 592E5682)))
  (libparts
    (libpart (lib device) (part C)
      (description "Unpolarized capacitor")
      (footprints
        (fp C_*))
      (fields
        (field (name Reference) C)
        (field (name Value) C))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib conn) (part CONN_01X01)
      (description "Connector, single row, 01x01, pin header")
      (footprints
        (fp Pin_Header_Straight_1X*)
        (fp Pin_Header_Angled_1X*)
        (fp Socket_Strip_Straight_1X*)
        (fp Socket_Strip_Angled_1X*))
      (fields
        (field (name Reference) J)
        (field (name Value) CONN_01X01))
      (pins
        (pin (num 1) (name P1) (type passive))))
    (libpart (lib conn) (part CONN_01X04)
      (description "Connector, single row, 01x04, pin header")
      (footprints
        (fp Pin_Header_Straight_1X*)
        (fp Pin_Header_Angled_1X*)
        (fp Socket_Strip_Straight_1X*)
        (fp Socket_Strip_Angled_1X*))
      (fields
        (field (name Reference) J)
        (field (name Value) CONN_01X04))
      (pins
        (pin (num 1) (name P1) (type passive))
        (pin (num 2) (name P2) (type passive))
        (pin (num 3) (name P3) (type passive))
        (pin (num 4) (name P4) (type passive))))
    (libpart (lib device) (part R)
      (description Resistor)
      (footprints
        (fp R_*)
        (fp R_*))
      (fields
        (field (name Reference) R)
        (field (name Value) R))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib tsys01) (part TSYS01)
      (fields
        (field (name Reference) U)
        (field (name Value) TSYS01))
      (pins
        (pin (num 1) (name VSS) (type power_in))
        (pin (num 2) (name CSB) (type input))
        (pin (num 3) (name SCLK/SCL) (type input))
        (pin (num 4) (name SDI/SDA) (type input))
        (pin (num 5) (name SDO) (type input))
        (pin (num 6) (name NC6) (type NotConnected))
        (pin (num 9) (name NC) (type NotConnected))
        (pin (num 10) (name A) (type input))
        (pin (num 11) (name B) (type input))
        (pin (num 12) (name NC) (type NotConnected))
        (pin (num 13) (name NC) (type NotConnected))
        (pin (num 14) (name NC) (type NotConnected))
        (pin (num 15) (name VDD) (type power_in))
        (pin (num 16) (name PS) (type input))
        (pin (num 17) (name PAD) (type input))
        (pin (num NC) (name 7) (type NotConnected)))))
  (libraries
    (library (logical device)
      (uri /usr/share/kicad/library/device.lib))
    (library (logical conn)
      (uri /usr/share/kicad/library/conn.lib))
    (library (logical tsys01)
      (uri tsys01.lib)))
  (nets
    (net (code 1) (name "Net-(P1-Pad3)")
      (node (ref U1) (pin 4))
      (node (ref P1) (pin 3)))
    (net (code 2) (name "Net-(R1-Pad2)")
      (node (ref R1) (pin 2))
      (node (ref R2) (pin 2))
      (node (ref U1) (pin 2)))
    (net (code 3) (name VDD)
      (node (ref P1) (pin 4))
      (node (ref C1) (pin 2))
      (node (ref U1) (pin 16))
      (node (ref U1) (pin 15))
      (node (ref R1) (pin 1)))
    (net (code 4) (name GND)
      (node (ref C1) (pin 1))
      (node (ref U1) (pin 1))
      (node (ref R2) (pin 1))
      (node (ref P1) (pin 1)))
    (net (code 5) (name "Net-(P1-Pad2)")
      (node (ref U1) (pin 3))
      (node (ref P1) (pin 2)))
    (net (code 6) (name "Net-(U1-Pad5)")
      (node (ref U1) (pin 5)))
    (net (code 7) (name "Net-(U1-Pad17)")
      (node (ref U1) (pin 17)))
    (net (code 8) (name "Net-(Hole1-Pad1)")
      (node (ref Hole1) (pin 1)))
    (net (code 9) (name "Net-(Hole2-Pad1)")
      (node (ref Hole2) (pin 1)))
    (net (code 11) (name "Net-(U1-Pad6)")
      (node (ref U1) (pin 6)))
    (net (code 12) (name "Net-(U1-Pad9)")
      (node (ref U1) (pin 9)))
    (net (code 13) (name "Net-(U1-Pad10)")
      (node (ref U1) (pin 11))
      (node (ref U1) (pin 10)))
    (net (code 14) (name "Net-(U1-Pad12)")
      (node (ref U1) (pin 12)))
    (net (code 15) (name "Net-(U1-Pad13)")
      (node (ref U1) (pin 13)))
    (net (code 16) (name "Net-(U1-Pad14)")
      (node (ref U1) (pin 14)))
    (net (code 17) (name "Net-(U1-PadNC)")
      (node (ref U1) (pin NC)))))