182832195481432
Connector_Dsub
DSUB-9_Female_EdgeMount_P2.77mm
9-pin D-Sub connector, solder-cups edge-mounted, female, x-pin-pitch 2.77mm, distance of mounting holes 25mm, see https://disti-assets.s3.amazonaws.com/tonar/files/datasheets/16730.pdf
9-pin D-Sub connector edge mount solder cup female x-pin-pitch 2.77mm mounting holes distance 25mm
0
9
9
Connector_Dsub
DSUB-9_Female_Horizontal_P2.77x2.54mm_EdgePinOffset9.40mm
9-pin D-Sub connector, horizontal/angled (90 deg), THT-mount, female, pitch 2.77x2.54mm, pin-PCB-offset 9.4mm, see http://docs-europe.electrocomponents.com/webdocs/1585/0900766b81585df2.pdf
9-pin D-Sub connector horizontal angled 90deg THT female pitch 2.77x2.54mm pin-PCB-offset 9.4mm
0
9
9
Connector_Dsub
DSUB-9_Female_Horizontal_P2.77x2.84mm_EdgePinOffset4.94mm_Housed_MountingHolesOffset7.48mm
9-pin D-Sub connector, horizontal/angled (90 deg), THT-mount, female, pitch 2.77x2.84mm, pin-PCB-offset 4.9399999999999995mm, distance of mounting holes 25mm, distance of mounting holes to PCB edge 7.4799999999999995mm, see https://disti-assets.s3.amazonaws.com/tonar/files/datasheets/16730.pdf
9-pin D-Sub connector horizontal angled 90deg THT female pitch 2.77x2.84mm pin-PCB-offset 4.9399999999999995mm mounting-holes-distance 25mm mounting-hole-offset 25mm
0
11
10
Connector_Dsub
DSUB-9_Female_Horizontal_P2.77x2.84mm_EdgePinOffset7.70mm_Housed_MountingHolesOffset9.12mm
9-pin D-Sub connector, horizontal/angled (90 deg), THT-mount, female, pitch 2.77x2.84mm, pin-PCB-offset 7.699999999999999mm, distance of mounting holes 25mm, distance of mounting holes to PCB edge 9.12mm, see https://disti-assets.s3.amazonaws.com/tonar/files/datasheets/16730.pdf
9-pin D-Sub connector horizontal angled 90deg THT female pitch 2.77x2.84mm pin-PCB-offset 7.699999999999999mm mounting-holes-distance 25mm mounting-hole-offset 25mm
0
11
10
Connector_Dsub
DSUB-9_Female_Horizontal_P2.77x2.84mm_EdgePinOffset9.40mm
9-pin D-Sub connector, horizontal/angled (90 deg), THT-mount, female, pitch 2.77x2.84mm, pin-PCB-offset 9.4mm, see http://docs-europe.electrocomponents.com/webdocs/1585/0900766b81585df2.pdf
9-pin D-Sub connector horizontal angled 90deg THT female pitch 2.77x2.84mm pin-PCB-offset 9.4mm
0
9
9
Connector_Dsub
DSUB-9_Female_Horizontal_P2.77x2.84mm_EdgePinOffset9.90mm_Housed_MountingHolesOffset11.32mm
9-pin D-Sub connector, horizontal/angled (90 deg), THT-mount, female, pitch 2.77x2.84mm, pin-PCB-offset 9.9mm, distance of mounting holes 25mm, distance of mounting holes to PCB edge 11.32mm, see https://disti-assets.s3.amazonaws.com/tonar/files/datasheets/16730.pdf
9-pin D-Sub connector horizontal angled 90deg THT female pitch 2.77x2.84mm pin-PCB-offset 9.9mm mounting-holes-distance 25mm mounting-hole-offset 25mm
0
11
10
Connector_Dsub
DSUB-9_Female_Horizontal_P2.77x2.84mm_EdgePinOffset14.56mm_Housed_MountingHolesOffset8.20mm
9-pin D-Sub connector, horizontal/angled (90 deg), THT-mount, female, pitch 2.77x2.84mm, pin-PCB-offset 14.56mm, distance of mounting holes 25mm, distance of mounting holes to PCB edge 8.2mm, see https://disti-assets.s3.amazonaws.com/tonar/files/datasheets/16730.pdf
9-pin D-Sub connector horizontal angled 90deg THT female pitch 2.77x2.84mm pin-PCB-offset 14.56mm mounting-holes-distance 25mm mounting-hole-offset 25mm
0
11
10
Connector_Dsub
DSUB-9_Female_Horizontal_P2.77x2.84mm_EdgePinOffset14.56mm_Housed_MountingHolesOffset15.98mm
9-pin D-Sub connector, horizontal/angled (90 deg), THT-mount, female, pitch 2.77x2.84mm, pin-PCB-offset 14.56mm, distance of mounting holes 25mm, distance of mounting holes to PCB edge 15.979999999999999mm, see https://disti-assets.s3.amazonaws.com/tonar/files/datasheets/16730.pdf
9-pin D-Sub connector horizontal angled 90deg THT female pitch 2.77x2.84mm pin-PCB-offset 14.56mm mounting-holes-distance 25mm mounting-hole-offset 25mm
0
11
10
Connector_Dsub
DSUB-9_Female_Vertical_P2.77x2.84mm
9-pin D-Sub connector, straight/vertical, THT-mount, female, pitch 2.77x2.84mm, distance of mounting holes 25mm, see https://disti-assets.s3.amazonaws.com/tonar/files/datasheets/16730.pdf
9-pin D-Sub connector straight vertical THT female pitch 2.77x2.84mm mounting holes distance 25mm
0
9
9
Connector_Dsub
DSUB-9_Female_Vertical_P2.77x2.84mm_MountingHoles
9-pin D-Sub connector, straight/vertical, THT-mount, female, pitch 2.77x2.84mm, distance of mounting holes 25mm, see https://disti-assets.s3.amazonaws.com/tonar/files/datasheets/16730.pdf
9-pin D-Sub connector straight vertical THT female pitch 2.77x2.84mm mounting holes distance 25mm
0
11
10
Connector_Dsub
DSUB-9_Male_EdgeMount_P2.77mm
9-pin D-Sub connector, solder-cups edge-mounted, male, x-pin-pitch 2.77mm, distance of mounting holes 25mm, see https://disti-assets.s3.amazonaws.com/tonar/files/datasheets/16730.pdf
9-pin D-Sub connector edge mount solder cup male x-pin-pitch 2.77mm mounting holes distance 25mm
0
9
9
Connector_Dsub
DSUB-9_Male_Horizontal_P2.77x2.54mm_EdgePinOffset9.40mm
9-pin D-Sub connector, horizontal/angled (90 deg), THT-mount, male, pitch 2.77x2.54mm, pin-PCB-offset 9.4mm, see http://docs-europe.electrocomponents.com/webdocs/1585/0900766b81585df2.pdf
9-pin D-Sub connector horizontal angled 90deg THT male pitch 2.77x2.54mm pin-PCB-offset 9.4mm
0
9
9
Connector_Dsub
DSUB-9_Male_Horizontal_P2.77x2.84mm_EdgePinOffset4.94mm_Housed_MountingHolesOffset7.48mm
9-pin D-Sub connector, horizontal/angled (90 deg), THT-mount, male, pitch 2.77x2.84mm, pin-PCB-offset 4.9399999999999995mm, distance of mounting holes 25mm, distance of mounting holes to PCB edge 7.4799999999999995mm, see https://disti-assets.s3.amazonaws.com/tonar/files/datasheets/16730.pdf
9-pin D-Sub connector horizontal angled 90deg THT male pitch 2.77x2.84mm pin-PCB-offset 4.9399999999999995mm mounting-holes-distance 25mm mounting-hole-offset 25mm
0
11
10
Connector_Dsub
DSUB-9_Male_Horizontal_P2.77x2.84mm_EdgePinOffset7.70mm_Housed_MountingHolesOffset9.12mm
9-pin D-Sub connector, horizontal/angled (90 deg), THT-mount, male, pitch 2.77x2.84mm, pin-PCB-offset 7.699999999999999mm, distance of mounting holes 25mm, distance of mounting holes to PCB edge 9.12mm, see https://disti-assets.s3.amazonaws.com/tonar/files/datasheets/16730.pdf
9-pin D-Sub connector horizontal angled 90deg THT male pitch 2.77x2.84mm pin-PCB-offset 7.699999999999999mm mounting-holes-distance 25mm mounting-hole-offset 25mm
0
11
10
Connector_Dsub
DSUB-9_Male_Horizontal_P2.77x2.84mm_EdgePinOffset9.40mm
9-pin D-Sub connector, horizontal/angled (90 deg), THT-mount, male, pitch 2.77x2.84mm, pin-PCB-offset 9.4mm, see http://docs-europe.electrocomponents.com/webdocs/1585/0900766b81585df2.pdf
9-pin D-Sub connector horizontal angled 90deg THT male pitch 2.77x2.84mm pin-PCB-offset 9.4mm
0
9
9
Connector_Dsub
DSUB-9_Male_Horizontal_P2.77x2.84mm_EdgePinOffset9.90mm_Housed_MountingHolesOffset11.32mm
9-pin D-Sub connector, horizontal/angled (90 deg), THT-mount, male, pitch 2.77x2.84mm, pin-PCB-offset 9.9mm, distance of mounting holes 25mm, distance of mounting holes to PCB edge 11.32mm, see https://disti-assets.s3.amazonaws.com/tonar/files/datasheets/16730.pdf
9-pin D-Sub connector horizontal angled 90deg THT male pitch 2.77x2.84mm pin-PCB-offset 9.9mm mounting-holes-distance 25mm mounting-hole-offset 25mm
0
11
10
Connector_Dsub
DSUB-9_Male_Horizontal_P2.77x2.84mm_EdgePinOffset14.56mm_Housed_MountingHolesOffset8.20mm
9-pin D-Sub connector, horizontal/angled (90 deg), THT-mount, male, pitch 2.77x2.84mm, pin-PCB-offset 14.56mm, distance of mounting holes 25mm, distance of mounting holes to PCB edge 8.2mm, see https://disti-assets.s3.amazonaws.com/tonar/files/datasheets/16730.pdf
9-pin D-Sub connector horizontal angled 90deg THT male pitch 2.77x2.84mm pin-PCB-offset 14.56mm mounting-holes-distance 25mm mounting-hole-offset 25mm
0
11
10
Connector_Dsub
DSUB-9_Male_Horizontal_P2.77x2.84mm_EdgePinOffset14.56mm_Housed_MountingHolesOffset15.98mm
9-pin D-Sub connector, horizontal/angled (90 deg), THT-mount, male, pitch 2.77x2.84mm, pin-PCB-offset 14.56mm, distance of mounting holes 25mm, distance of mounting holes to PCB edge 15.979999999999999mm, see https://disti-assets.s3.amazonaws.com/tonar/files/datasheets/16730.pdf
9-pin D-Sub connector horizontal angled 90deg THT male pitch 2.77x2.84mm pin-PCB-offset 14.56mm mounting-holes-distance 25mm mounting-hole-offset 25mm
0
11
10
Connector_Dsub
DSUB-9_Male_Vertical_P2.77x2.84mm
9-pin D-Sub connector, straight/vertical, THT-mount, male, pitch 2.77x2.84mm, distance of mounting holes 25mm, see https://disti-assets.s3.amazonaws.com/tonar/files/datasheets/16730.pdf
9-pin D-Sub connector straight vertical THT male pitch 2.77x2.84mm mounting holes distance 25mm
0
9
9
Connector_Dsub
DSUB-9_Male_Vertical_P2.77x2.84mm_MountingHoles
9-pin D-Sub connector, straight/vertical, THT-mount, male, pitch 2.77x2.84mm, distance of mounting holes 25mm, see https://disti-assets.s3.amazonaws.com/tonar/files/datasheets/16730.pdf
9-pin D-Sub connector straight vertical THT male pitch 2.77x2.84mm mounting holes distance 25mm
0
11
10
Connector_Dsub
DSUB-15-HD_Female_Horizontal_P2.29x1.98mm_EdgePinOffset3.03mm_Housed_MountingHolesOffset4.94mm
15-pin D-Sub connector, horizontal/angled (90 deg), THT-mount, female, pitch 2.29x1.98mm, pin-PCB-offset 3.0300000000000002mm, distance of mounting holes 25mm, distance of mounting holes to PCB edge 4.9399999999999995mm, see https://disti-assets.s3.amazonaws.com/tonar/files/datasheets/16730.pdf
15-pin D-Sub connector horizontal angled 90deg THT female pitch 2.29x1.98mm pin-PCB-offset 3.0300000000000002mm mounting-holes-distance 25mm mounting-hole-offset 25mm
0
17
16
Connector_Dsub
DSUB-15-HD_Female_Horizontal_P2.29x1.98mm_EdgePinOffset8.35mm_Housed_MountingHolesOffset10.89mm
15-pin D-Sub connector, horizontal/angled (90 deg), THT-mount, female, pitch 2.29x1.98mm, pin-PCB-offset 8.35mm, distance of mounting holes 25mm, distance of mounting holes to PCB edge 10.889999999999999mm, see https://disti-assets.s3.amazonaws.com/tonar/files/datasheets/16730.pdf
15-pin D-Sub connector horizontal angled 90deg THT female pitch 2.29x1.98mm pin-PCB-offset 8.35mm mounting-holes-distance 25mm mounting-hole-offset 25mm
0
17
16
Connector_Dsub
DSUB-15-HD_Female_Horizontal_P2.29x1.98mm_EdgePinOffset9.40mm
15-pin D-Sub connector, horizontal/angled (90 deg), THT-mount, female, pitch 2.29x1.98mm, pin-PCB-offset 9.4mm, see http://docs-europe.electrocomponents.com/webdocs/1585/0900766b81585df2.pdf
15-pin D-Sub connector horizontal angled 90deg THT female pitch 2.29x1.98mm pin-PCB-offset 9.4mm
0
15
15
Connector_Dsub
DSUB-15-HD_Female_Horizontal_P2.29x2.54mm_EdgePinOffset9.40mm
15-pin D-Sub connector, horizontal/angled (90 deg), THT-mount, female, pitch 2.29x2.54mm, pin-PCB-offset 9.4mm, see http://docs-europe.electrocomponents.com/webdocs/1585/0900766b81585df2.pdf
15-pin D-Sub connector horizontal angled 90deg THT female pitch 2.29x2.54mm pin-PCB-offset 9.4mm
0
15
15
Connector_Dsub
DSUB-15-HD_Female_Vertical_P2.29x1.98mm_MountingHoles
15-pin D-Sub connector, straight/vertical, THT-mount, female, pitch 2.29x1.98mm, distance of mounting holes 25mm, see https://disti-assets.s3.amazonaws.com/tonar/files/datasheets/16730.pdf
15-pin D-Sub connector straight vertical THT female pitch 2.29x1.98mm mounting holes distance 25mm
0
17
16
Connector_Dsub
DSUB-15-HD_Male_Horizontal_P2.29x1.98mm_EdgePinOffset3.03mm_Housed_MountingHolesOffset4.94mm
15-pin D-Sub connector, horizontal/angled (90 deg), THT-mount, male, pitch 2.29x1.98mm, pin-PCB-offset 3.0300000000000002mm, distance of mounting holes 25mm, distance of mounting holes to PCB edge 4.9399999999999995mm, see https://disti-assets.s3.amazonaws.com/tonar/files/datasheets/16730.pdf
15-pin D-Sub connector horizontal angled 90deg THT male pitch 2.29x1.98mm pin-PCB-offset 3.0300000000000002mm mounting-holes-distance 25mm mounting-hole-offset 25mm
0
17
16
Connector_Dsub
DSUB-15-HD_Male_Horizontal_P2.29x1.98mm_EdgePinOffset8.35mm_Housed_MountingHolesOffset10.89mm
15-pin D-Sub connector, horizontal/angled (90 deg), THT-mount, male, pitch 2.29x1.98mm, pin-PCB-offset 8.35mm, distance of mounting holes 25mm, distance of mounting holes to PCB edge 10.889999999999999mm, see https://disti-assets.s3.amazonaws.com/tonar/files/datasheets/16730.pdf
15-pin D-Sub connector horizontal angled 90deg THT male pitch 2.29x1.98mm pin-PCB-offset 8.35mm mounting-holes-distance 25mm mounting-hole-offset 25mm
0
17
16
Connector_Dsub
DSUB-15-HD_Male_Horizontal_P2.29x1.98mm_EdgePinOffset9.40mm
15-pin D-Sub connector, horizontal/angled (90 deg), THT-mount, male, pitch 2.29x1.98mm, pin-PCB-offset 9.4mm, see http://docs-europe.electrocomponents.com/webdocs/1585/0900766b81585df2.pdf
15-pin D-Sub connector horizontal angled 90deg THT male pitch 2.29x1.98mm pin-PCB-offset 9.4mm
0
15
15
Connector_Dsub
DSUB-15-HD_Male_Horizontal_P2.29x2.54mm_EdgePinOffset9.40mm
15-pin D-Sub connector, horizontal/angled (90 deg), THT-mount, male, pitch 2.29x2.54mm, pin-PCB-offset 9.4mm, see http://docs-europe.electrocomponents.com/webdocs/1585/0900766b81585df2.pdf
15-pin D-Sub connector horizontal angled 90deg THT male pitch 2.29x2.54mm pin-PCB-offset 9.4mm
0
15
15
Connector_Dsub
DSUB-15-HD_Male_Vertical_P2.29x1.98mm_MountingHoles
15-pin D-Sub connector, straight/vertical, THT-mount, male, pitch 2.29x1.98mm, distance of mounting holes 25mm, see https://disti-assets.s3.amazonaws.com/tonar/files/datasheets/16730.pdf
15-pin D-Sub connector straight vertical THT male pitch 2.29x1.98mm mounting holes distance 25mm
0
17
16
Connector_Dsub
DSUB-15_Female_EdgeMount_P2.77mm
15-pin D-Sub connector, solder-cups edge-mounted, female, x-pin-pitch 2.77mm, distance of mounting holes 33.3mm, see https://disti-assets.s3.amazonaws.com/tonar/files/datasheets/16730.pdf
15-pin D-Sub connector edge mount solder cup female x-pin-pitch 2.77mm mounting holes distance 33.3mm
0
15
15
Connector_Dsub
DSUB-15_Female_Horizontal_P2.77x2.54mm_EdgePinOffset9.40mm
15-pin D-Sub connector, horizontal/angled (90 deg), THT-mount, female, pitch 2.77x2.54mm, pin-PCB-offset 9.4mm, see http://docs-europe.electrocomponents.com/webdocs/1585/0900766b81585df2.pdf
15-pin D-Sub connector horizontal angled 90deg THT female pitch 2.77x2.54mm pin-PCB-offset 9.4mm
0
15
15
Connector_Dsub
DSUB-15_Female_Horizontal_P2.77x2.84mm_EdgePinOffset4.94mm_Housed_MountingHolesOffset7.48mm
15-pin D-Sub connector, horizontal/angled (90 deg), THT-mount, female, pitch 2.77x2.84mm, pin-PCB-offset 4.9399999999999995mm, distance of mounting holes 33.3mm, distance of mounting holes to PCB edge 7.4799999999999995mm, see https://disti-assets.s3.amazonaws.com/tonar/files/datasheets/16730.pdf
15-pin D-Sub connector horizontal angled 90deg THT female pitch 2.77x2.84mm pin-PCB-offset 4.9399999999999995mm mounting-holes-distance 33.3mm mounting-hole-offset 33.3mm
0
17
16
Connector_Dsub
DSUB-15_Female_Horizontal_P2.77x2.84mm_EdgePinOffset7.70mm_Housed_MountingHolesOffset9.12mm
15-pin D-Sub connector, horizontal/angled (90 deg), THT-mount, female, pitch 2.77x2.84mm, pin-PCB-offset 7.699999999999999mm, distance of mounting holes 33.3mm, distance of mounting holes to PCB edge 9.12mm, see https://disti-assets.s3.amazonaws.com/tonar/files/datasheets/16730.pdf
15-pin D-Sub connector horizontal angled 90deg THT female pitch 2.77x2.84mm pin-PCB-offset 7.699999999999999mm mounting-holes-distance 33.3mm mounting-hole-offset 33.3mm
0
17
16
Connector_Dsub
DSUB-15_Female_Horizontal_P2.77x2.84mm_EdgePinOffset9.40mm
15-pin D-Sub connector, horizontal/angled (90 deg), THT-mount, female, pitch 2.77x2.84mm, pin-PCB-offset 9.4mm, see http://docs-europe.electrocomponents.com/webdocs/1585/0900766b81585df2.pdf
15-pin D-Sub connector horizontal angled 90deg THT female pitch 2.77x2.84mm pin-PCB-offset 9.4mm
0
15
15
Connector_Dsub
DSUB-15_Female_Horizontal_P2.77x2.84mm_EdgePinOffset9.90mm_Housed_MountingHolesOffset11.32mm
15-pin D-Sub connector, horizontal/angled (90 deg), THT-mount, female, pitch 2.77x2.84mm, pin-PCB-offset 9.9mm, distance of mounting holes 33.3mm, distance of mounting holes to PCB edge 11.32mm, see https://disti-assets.s3.amazonaws.com/tonar/files/datasheets/16730.pdf
15-pin D-Sub connector horizontal angled 90deg THT female pitch 2.77x2.84mm pin-PCB-offset 9.9mm mounting-holes-distance 33.3mm mounting-hole-offset 33.3mm
0
17
16
Connector_Dsub
DSUB-15_Female_Horizontal_P2.77x2.84mm_EdgePinOffset14.56mm_Housed_MountingHolesOffset8.20mm
15-pin D-Sub connector, horizontal/angled (90 deg), THT-mount, female, pitch 2.77x2.84mm, pin-PCB-offset 14.56mm, distance of mounting holes 33.3mm, distance of mounting holes to PCB edge 8.2mm, see https://disti-assets.s3.amazonaws.com/tonar/files/datasheets/16730.pdf
15-pin D-Sub connector horizontal angled 90deg THT female pitch 2.77x2.84mm pin-PCB-offset 14.56mm mounting-holes-distance 33.3mm mounting-hole-offset 33.3mm
0
17
16
Connector_Dsub
DSUB-15_Female_Horizontal_P2.77x2.84mm_EdgePinOffset14.56mm_Housed_MountingHolesOffset15.98mm
15-pin D-Sub connector, horizontal/angled (90 deg), THT-mount, female, pitch 2.77x2.84mm, pin-PCB-offset 14.56mm, distance of mounting holes 33.3mm, distance of mounting holes to PCB edge 15.979999999999999mm, see https://disti-assets.s3.amazonaws.com/tonar/files/datasheets/16730.pdf
15-pin D-Sub connector horizontal angled 90deg THT female pitch 2.77x2.84mm pin-PCB-offset 14.56mm mounting-holes-distance 33.3mm mounting-hole-offset 33.3mm
0
17
16
Connector_Dsub
DSUB-15_Female_Vertical_P2.77x2.84mm
15-pin D-Sub connector, straight/vertical, THT-mount, female, pitch 2.77x2.84mm, distance of mounting holes 33.3mm, see https://disti-assets.s3.amazonaws.com/tonar/files/datasheets/16730.pdf
15-pin D-Sub connector straight vertical THT female pitch 2.77x2.84mm mounting holes distance 33.3mm
0
15
15
Connector_Dsub
DSUB-15_Female_Vertical_P2.77x2.84mm_MountingHoles
15-pin D-Sub connector, straight/vertical, THT-mount, female, pitch 2.77x2.84mm, distance of mounting holes 33.3mm, see https://disti-assets.s3.amazonaws.com/tonar/files/datasheets/16730.pdf
15-pin D-Sub connector straight vertical THT female pitch 2.77x2.84mm mounting holes distance 33.3mm
0
17
16
Connector_Dsub
DSUB-15_Male_EdgeMount_P2.77mm
15-pin D-Sub connector, solder-cups edge-mounted, male, x-pin-pitch 2.77mm, distance of mounting holes 33.3mm, see https://disti-assets.s3.amazonaws.com/tonar/files/datasheets/16730.pdf
15-pin D-Sub connector edge mount solder cup male x-pin-pitch 2.77mm mounting holes distance 33.3mm
0
15
15
Connector_Dsub
DSUB-15_Male_Horizontal_P2.77x2.54mm_EdgePinOffset9.40mm
15-pin D-Sub connector, horizontal/angled (90 deg), THT-mount, male, pitch 2.77x2.54mm, pin-PCB-offset 9.4mm, see http://docs-europe.electrocomponents.com/webdocs/1585/0900766b81585df2.pdf
15-pin D-Sub connector horizontal angled 90deg THT male pitch 2.77x2.54mm pin-PCB-offset 9.4mm
0
15
15
Connector_Dsub
DSUB-15_Male_Horizontal_P2.77x2.84mm_EdgePinOffset4.94mm_Housed_MountingHolesOffset7.48mm
15-pin D-Sub connector, horizontal/angled (90 deg), THT-mount, male, pitch 2.77x2.84mm, pin-PCB-offset 4.9399999999999995mm, distance of mounting holes 33.3mm, distance of mounting holes to PCB edge 7.4799999999999995mm, see https://disti-assets.s3.amazonaws.com/tonar/files/datasheets/16730.pdf
15-pin D-Sub connector horizontal angled 90deg THT male pitch 2.77x2.84mm pin-PCB-offset 4.9399999999999995mm mounting-holes-distance 33.3mm mounting-hole-offset 33.3mm
0
17
16
Connector_Dsub
DSUB-15_Male_Horizontal_P2.77x2.84mm_EdgePinOffset7.70mm_Housed_MountingHolesOffset9.12mm
15-pin D-Sub connector, horizontal/angled (90 deg), THT-mount, male, pitch 2.77x2.84mm, pin-PCB-offset 7.699999999999999mm, distance of mounting holes 33.3mm, distance of mounting holes to PCB edge 9.12mm, see https://disti-assets.s3.amazonaws.com/tonar/files/datasheets/16730.pdf
15-pin D-Sub connector horizontal angled 90deg THT male pitch 2.77x2.84mm pin-PCB-offset 7.699999999999999mm mounting-holes-distance 33.3mm mounting-hole-offset 33.3mm
0
17
16
Connector_Dsub
DSUB-15_Male_Horizontal_P2.77x2.84mm_EdgePinOffset9.40mm
15-pin D-Sub connector, horizontal/angled (90 deg), THT-mount, male, pitch 2.77x2.84mm, pin-PCB-offset 9.4mm, see http://docs-europe.electrocomponents.com/webdocs/1585/0900766b81585df2.pdf
15-pin D-Sub connector horizontal angled 90deg THT male pitch 2.77x2.84mm pin-PCB-offset 9.4mm
0
15
15
Connector_Dsub
DSUB-15_Male_Horizontal_P2.77x2.84mm_EdgePinOffset9.90mm_Housed_MountingHolesOffset11.32mm
15-pin D-Sub connector, horizontal/angled (90 deg), THT-mount, male, pitch 2.77x2.84mm, pin-PCB-offset 9.9mm, distance of mounting holes 33.3mm, distance of mounting holes to PCB edge 11.32mm, see https://disti-assets.s3.amazonaws.com/tonar/files/datasheets/16730.pdf
15-pin D-Sub connector horizontal angled 90deg THT male pitch 2.77x2.84mm pin-PCB-offset 9.9mm mounting-holes-distance 33.3mm mounting-hole-offset 33.3mm
0
17
16
Connector_Dsub
DSUB-15_Male_Horizontal_P2.77x2.84mm_EdgePinOffset14.56mm_Housed_MountingHolesOffset8.20mm
15-pin D-Sub connector, horizontal/angled (90 deg), THT-mount, male, pitch 2.77x2.84mm, pin-PCB-offset 14.56mm, distance of mounting holes 33.3mm, distance of mounting holes to PCB edge 8.2mm, see https://disti-assets.s3.amazonaws.com/tonar/files/datasheets/16730.pdf
15-pin D-Sub connector horizontal angled 90deg THT male pitch 2.77x2.84mm pin-PCB-offset 14.56mm mounting-holes-distance 33.3mm mounting-hole-offset 33.3mm
0
17
16
Connector_Dsub
DSUB-15_Male_Horizontal_P2.77x2.84mm_EdgePinOffset14.56mm_Housed_MountingHolesOffset15.98mm
15-pin D-Sub connector, horizontal/angled (90 deg), THT-mount, male, pitch 2.77x2.84mm, pin-PCB-offset 14.56mm, distance of mounting holes 33.3mm, distance of mounting holes to PCB edge 15.979999999999999mm, see https://disti-assets.s3.amazonaws.com/tonar/files/datasheets/16730.pdf
15-pin D-Sub connector horizontal angled 90deg THT male pitch 2.77x2.84mm pin-PCB-offset 14.56mm mounting-holes-distance 33.3mm mounting-hole-offset 33.3mm
0
17
16
Connector_Dsub
DSUB-15_Male_Vertical_P2.77x2.84mm
15-pin D-Sub connector, straight/vertical, THT-mount, male, pitch 2.77x2.84mm, distance of mounting holes 33.3mm, see https://disti-assets.s3.amazonaws.com/tonar/files/datasheets/16730.pdf
15-pin D-Sub connector straight vertical THT male pitch 2.77x2.84mm mounting holes distance 33.3mm
0
15
15
Connector_Dsub
DSUB-15_Male_Vertical_P2.77x2.84mm_MountingHoles
15-pin D-Sub connector, straight/vertical, THT-mount, male, pitch 2.77x2.84mm, distance of mounting holes 33.3mm, see https://disti-assets.s3.amazonaws.com/tonar/files/datasheets/16730.pdf
15-pin D-Sub connector straight vertical THT male pitch 2.77x2.84mm mounting holes distance 33.3mm
0
17
16
Connector_Dsub
DSUB-25_Female_EdgeMount_P2.77mm
25-pin D-Sub connector, solder-cups edge-mounted, female, x-pin-pitch 2.77mm, distance of mounting holes 47.1mm, see https://disti-assets.s3.amazonaws.com/tonar/files/datasheets/16730.pdf
25-pin D-Sub connector edge mount solder cup female x-pin-pitch 2.77mm mounting holes distance 47.1mm
0
25
25
Connector_Dsub
DSUB-25_Female_Horizontal_P2.77x2.54mm_EdgePinOffset9.40mm
25-pin D-Sub connector, horizontal/angled (90 deg), THT-mount, female, pitch 2.77x2.54mm, pin-PCB-offset 9.4mm, see http://docs-europe.electrocomponents.com/webdocs/1585/0900766b81585df2.pdf
25-pin D-Sub connector horizontal angled 90deg THT female pitch 2.77x2.54mm pin-PCB-offset 9.4mm
0
25
25
Connector_Dsub
DSUB-25_Female_Horizontal_P2.77x2.84mm_EdgePinOffset4.94mm_Housed_MountingHolesOffset7.48mm
25-pin D-Sub connector, horizontal/angled (90 deg), THT-mount, female, pitch 2.77x2.84mm, pin-PCB-offset 4.9399999999999995mm, distance of mounting holes 47.1mm, distance of mounting holes to PCB edge 7.4799999999999995mm, see https://disti-assets.s3.amazonaws.com/tonar/files/datasheets/16730.pdf
25-pin D-Sub connector horizontal angled 90deg THT female pitch 2.77x2.84mm pin-PCB-offset 4.9399999999999995mm mounting-holes-distance 47.1mm mounting-hole-offset 47.1mm
0
27
26
Connector_Dsub
DSUB-25_Female_Horizontal_P2.77x2.84mm_EdgePinOffset7.70mm_Housed_MountingHolesOffset9.12mm
25-pin D-Sub connector, horizontal/angled (90 deg), THT-mount, female, pitch 2.77x2.84mm, pin-PCB-offset 7.699999999999999mm, distance of mounting holes 47.1mm, distance of mounting holes to PCB edge 9.12mm, see https://disti-assets.s3.amazonaws.com/tonar/files/datasheets/16730.pdf
25-pin D-Sub connector horizontal angled 90deg THT female pitch 2.77x2.84mm pin-PCB-offset 7.699999999999999mm mounting-holes-distance 47.1mm mounting-hole-offset 47.1mm
0
27
26
Connector_Dsub
DSUB-25_Female_Horizontal_P2.77x2.84mm_EdgePinOffset9.40mm
25-pin D-Sub connector, horizontal/angled (90 deg), THT-mount, female, pitch 2.77x2.84mm, pin-PCB-offset 9.4mm, see http://docs-europe.electrocomponents.com/webdocs/1585/0900766b81585df2.pdf
25-pin D-Sub connector horizontal angled 90deg THT female pitch 2.77x2.84mm pin-PCB-offset 9.4mm
0
25
25
Connector_Dsub
DSUB-25_Female_Horizontal_P2.77x2.84mm_EdgePinOffset9.90mm_Housed_MountingHolesOffset11.32mm
25-pin D-Sub connector, horizontal/angled (90 deg), THT-mount, female, pitch 2.77x2.84mm, pin-PCB-offset 9.9mm, distance of mounting holes 47.1mm, distance of mounting holes to PCB edge 11.32mm, see https://disti-assets.s3.amazonaws.com/tonar/files/datasheets/16730.pdf
25-pin D-Sub connector horizontal angled 90deg THT female pitch 2.77x2.84mm pin-PCB-offset 9.9mm mounting-holes-distance 47.1mm mounting-hole-offset 47.1mm
0
27
26
Connector_Dsub
DSUB-25_Female_Horizontal_P2.77x2.84mm_EdgePinOffset14.56mm_Housed_MountingHolesOffset8.20mm
25-pin D-Sub connector, horizontal/angled (90 deg), THT-mount, female, pitch 2.77x2.84mm, pin-PCB-offset 14.56mm, distance of mounting holes 47.1mm, distance of mounting holes to PCB edge 8.2mm, see https://disti-assets.s3.amazonaws.com/tonar/files/datasheets/16730.pdf
25-pin D-Sub connector horizontal angled 90deg THT female pitch 2.77x2.84mm pin-PCB-offset 14.56mm mounting-holes-distance 47.1mm mounting-hole-offset 47.1mm
0
27
26
Connector_Dsub
DSUB-25_Female_Horizontal_P2.77x2.84mm_EdgePinOffset14.56mm_Housed_MountingHolesOffset15.98mm
25-pin D-Sub connector, horizontal/angled (90 deg), THT-mount, female, pitch 2.77x2.84mm, pin-PCB-offset 14.56mm, distance of mounting holes 47.1mm, distance of mounting holes to PCB edge 15.979999999999999mm, see https://disti-assets.s3.amazonaws.com/tonar/files/datasheets/16730.pdf
25-pin D-Sub connector horizontal angled 90deg THT female pitch 2.77x2.84mm pin-PCB-offset 14.56mm mounting-holes-distance 47.1mm mounting-hole-offset 47.1mm
0
27
26
Connector_Dsub
DSUB-25_Female_Vertical_P2.77x2.84mm
25-pin D-Sub connector, straight/vertical, THT-mount, female, pitch 2.77x2.84mm, distance of mounting holes 47.1mm, see https://disti-assets.s3.amazonaws.com/tonar/files/datasheets/16730.pdf
25-pin D-Sub connector straight vertical THT female pitch 2.77x2.84mm mounting holes distance 47.1mm
0
25
25
Connector_Dsub
DSUB-25_Female_Vertical_P2.77x2.84mm_MountingHoles
25-pin D-Sub connector, straight/vertical, THT-mount, female, pitch 2.77x2.84mm, distance of mounting holes 47.1mm, see https://disti-assets.s3.amazonaws.com/tonar/files/datasheets/16730.pdf
25-pin D-Sub connector straight vertical THT female pitch 2.77x2.84mm mounting holes distance 47.1mm
0
27
26
Connector_Dsub
DSUB-25_Male_EdgeMount_P2.77mm
25-pin D-Sub connector, solder-cups edge-mounted, male, x-pin-pitch 2.77mm, distance of mounting holes 47.1mm, see https://disti-assets.s3.amazonaws.com/tonar/files/datasheets/16730.pdf
25-pin D-Sub connector edge mount solder cup male x-pin-pitch 2.77mm mounting holes distance 47.1mm
0
25
25
Connector_Dsub
DSUB-25_Male_Horizontal_P2.77x2.54mm_EdgePinOffset9.40mm
25-pin D-Sub connector, horizontal/angled (90 deg), THT-mount, male, pitch 2.77x2.54mm, pin-PCB-offset 9.4mm, see http://docs-europe.electrocomponents.com/webdocs/1585/0900766b81585df2.pdf
25-pin D-Sub connector horizontal angled 90deg THT male pitch 2.77x2.54mm pin-PCB-offset 9.4mm
0
25
25
Connector_Dsub
DSUB-25_Male_Horizontal_P2.77x2.84mm_EdgePinOffset4.94mm_Housed_MountingHolesOffset7.48mm
25-pin D-Sub connector, horizontal/angled (90 deg), THT-mount, male, pitch 2.77x2.84mm, pin-PCB-offset 4.9399999999999995mm, distance of mounting holes 47.1mm, distance of mounting holes to PCB edge 7.4799999999999995mm, see https://disti-assets.s3.amazonaws.com/tonar/files/datasheets/16730.pdf
25-pin D-Sub connector horizontal angled 90deg THT male pitch 2.77x2.84mm pin-PCB-offset 4.9399999999999995mm mounting-holes-distance 47.1mm mounting-hole-offset 47.1mm
0
27
26
Connector_Dsub
DSUB-25_Male_Horizontal_P2.77x2.84mm_EdgePinOffset7.70mm_Housed_MountingHolesOffset9.12mm
25-pin D-Sub connector, horizontal/angled (90 deg), THT-mount, male, pitch 2.77x2.84mm, pin-PCB-offset 7.699999999999999mm, distance of mounting holes 47.1mm, distance of mounting holes to PCB edge 9.12mm, see https://disti-assets.s3.amazonaws.com/tonar/files/datasheets/16730.pdf
25-pin D-Sub connector horizontal angled 90deg THT male pitch 2.77x2.84mm pin-PCB-offset 7.699999999999999mm mounting-holes-distance 47.1mm mounting-hole-offset 47.1mm
0
27
26
Connector_Dsub
DSUB-25_Male_Horizontal_P2.77x2.84mm_EdgePinOffset9.40mm
25-pin D-Sub connector, horizontal/angled (90 deg), THT-mount, male, pitch 2.77x2.84mm, pin-PCB-offset 9.4mm, see http://docs-europe.electrocomponents.com/webdocs/1585/0900766b81585df2.pdf
25-pin D-Sub connector horizontal angled 90deg THT male pitch 2.77x2.84mm pin-PCB-offset 9.4mm
0
25
25
Connector_Dsub
DSUB-25_Male_Horizontal_P2.77x2.84mm_EdgePinOffset9.90mm_Housed_MountingHolesOffset11.32mm
25-pin D-Sub connector, horizontal/angled (90 deg), THT-mount, male, pitch 2.77x2.84mm, pin-PCB-offset 9.9mm, distance of mounting holes 47.1mm, distance of mounting holes to PCB edge 11.32mm, see https://disti-assets.s3.amazonaws.com/tonar/files/datasheets/16730.pdf
25-pin D-Sub connector horizontal angled 90deg THT male pitch 2.77x2.84mm pin-PCB-offset 9.9mm mounting-holes-distance 47.1mm mounting-hole-offset 47.1mm
0
27
26
Connector_Dsub
DSUB-25_Male_Horizontal_P2.77x2.84mm_EdgePinOffset14.56mm_Housed_MountingHolesOffset8.20mm
25-pin D-Sub connector, horizontal/angled (90 deg), THT-mount, male, pitch 2.77x2.84mm, pin-PCB-offset 14.56mm, distance of mounting holes 47.1mm, distance of mounting holes to PCB edge 8.2mm, see https://disti-assets.s3.amazonaws.com/tonar/files/datasheets/16730.pdf
25-pin D-Sub connector horizontal angled 90deg THT male pitch 2.77x2.84mm pin-PCB-offset 14.56mm mounting-holes-distance 47.1mm mounting-hole-offset 47.1mm
0
27
26
Connector_Dsub
DSUB-25_Male_Horizontal_P2.77x2.84mm_EdgePinOffset14.56mm_Housed_MountingHolesOffset15.98mm
25-pin D-Sub connector, horizontal/angled (90 deg), THT-mount, male, pitch 2.77x2.84mm, pin-PCB-offset 14.56mm, distance of mounting holes 47.1mm, distance of mounting holes to PCB edge 15.979999999999999mm, see https://disti-assets.s3.amazonaws.com/tonar/files/datasheets/16730.pdf
25-pin D-Sub connector horizontal angled 90deg THT male pitch 2.77x2.84mm pin-PCB-offset 14.56mm mounting-holes-distance 47.1mm mounting-hole-offset 47.1mm
0
27
26
Connector_Dsub
DSUB-25_Male_Vertical_P2.77x2.84mm
25-pin D-Sub connector, straight/vertical, THT-mount, male, pitch 2.77x2.84mm, distance of mounting holes 47.1mm, see https://disti-assets.s3.amazonaws.com/tonar/files/datasheets/16730.pdf
25-pin D-Sub connector straight vertical THT male pitch 2.77x2.84mm mounting holes distance 47.1mm
0
25
25
Connector_Dsub
DSUB-25_Male_Vertical_P2.77x2.84mm_MountingHoles
25-pin D-Sub connector, straight/vertical, THT-mount, male, pitch 2.77x2.84mm, distance of mounting holes 47.1mm, see https://disti-assets.s3.amazonaws.com/tonar/files/datasheets/16730.pdf
25-pin D-Sub connector straight vertical THT male pitch 2.77x2.84mm mounting holes distance 47.1mm
0
27
26
Connector_Dsub
DSUB-26-HD_Female_Horizontal_P2.29x1.98mm_EdgePinOffset3.03mm_Housed_MountingHolesOffset4.94mm
26-pin D-Sub connector, horizontal/angled (90 deg), THT-mount, female, pitch 2.29x1.98mm, pin-PCB-offset 3.0300000000000002mm, distance of mounting holes 33.3mm, distance of mounting holes to PCB edge 4.9399999999999995mm, see https://disti-assets.s3.amazonaws.com/tonar/files/datasheets/16730.pdf
26-pin D-Sub connector horizontal angled 90deg THT female pitch 2.29x1.98mm pin-PCB-offset 3.0300000000000002mm mounting-holes-distance 33.3mm mounting-hole-offset 33.3mm
0
28
27
Connector_Dsub
DSUB-26-HD_Female_Horizontal_P2.29x1.98mm_EdgePinOffset8.35mm_Housed_MountingHolesOffset10.89mm
26-pin D-Sub connector, horizontal/angled (90 deg), THT-mount, female, pitch 2.29x1.98mm, pin-PCB-offset 8.35mm, distance of mounting holes 33.3mm, distance of mounting holes to PCB edge 10.889999999999999mm, see https://disti-assets.s3.amazonaws.com/tonar/files/datasheets/16730.pdf
26-pin D-Sub connector horizontal angled 90deg THT female pitch 2.29x1.98mm pin-PCB-offset 8.35mm mounting-holes-distance 33.3mm mounting-hole-offset 33.3mm
0
28
27
Connector_Dsub
DSUB-26-HD_Female_Horizontal_P2.29x1.98mm_EdgePinOffset9.40mm
26-pin D-Sub connector, horizontal/angled (90 deg), THT-mount, female, pitch 2.29x1.98mm, pin-PCB-offset 9.4mm, see http://docs-europe.electrocomponents.com/webdocs/1585/0900766b81585df2.pdf
26-pin D-Sub connector horizontal angled 90deg THT female pitch 2.29x1.98mm pin-PCB-offset 9.4mm
0
26
26
Connector_Dsub
DSUB-26-HD_Female_Horizontal_P2.29x2.54mm_EdgePinOffset9.40mm
26-pin D-Sub connector, horizontal/angled (90 deg), THT-mount, female, pitch 2.29x2.54mm, pin-PCB-offset 9.4mm, see http://docs-europe.electrocomponents.com/webdocs/1585/0900766b81585df2.pdf
26-pin D-Sub connector horizontal angled 90deg THT female pitch 2.29x2.54mm pin-PCB-offset 9.4mm
0
26
26
Connector_Dsub
DSUB-26-HD_Female_Vertical_P2.29x1.98mm_MountingHoles
26-pin D-Sub connector, straight/vertical, THT-mount, female, pitch 2.29x1.98mm, distance of mounting holes 33.3mm, see https://disti-assets.s3.amazonaws.com/tonar/files/datasheets/16730.pdf
26-pin D-Sub connector straight vertical THT female pitch 2.29x1.98mm mounting holes distance 33.3mm
0
28
27
Connector_Dsub
DSUB-26-HD_Male_Horizontal_P2.29x1.98mm_EdgePinOffset3.03mm_Housed_MountingHolesOffset4.94mm
26-pin D-Sub connector, horizontal/angled (90 deg), THT-mount, male, pitch 2.29x1.98mm, pin-PCB-offset 3.0300000000000002mm, distance of mounting holes 33.3mm, distance of mounting holes to PCB edge 4.9399999999999995mm, see https://disti-assets.s3.amazonaws.com/tonar/files/datasheets/16730.pdf
26-pin D-Sub connector horizontal angled 90deg THT male pitch 2.29x1.98mm pin-PCB-offset 3.0300000000000002mm mounting-holes-distance 33.3mm mounting-hole-offset 33.3mm
0
28
27
Connector_Dsub
DSUB-26-HD_Male_Horizontal_P2.29x1.98mm_EdgePinOffset8.35mm_Housed_MountingHolesOffset10.89mm
26-pin D-Sub connector, horizontal/angled (90 deg), THT-mount, male, pitch 2.29x1.98mm, pin-PCB-offset 8.35mm, distance of mounting holes 33.3mm, distance of mounting holes to PCB edge 10.889999999999999mm, see https://disti-assets.s3.amazonaws.com/tonar/files/datasheets/16730.pdf
26-pin D-Sub connector horizontal angled 90deg THT male pitch 2.29x1.98mm pin-PCB-offset 8.35mm mounting-holes-distance 33.3mm mounting-hole-offset 33.3mm
0
28
27
Connector_Dsub
DSUB-26-HD_Male_Horizontal_P2.29x1.98mm_EdgePinOffset9.40mm
26-pin D-Sub connector, horizontal/angled (90 deg), THT-mount, male, pitch 2.29x1.98mm, pin-PCB-offset 9.4mm, see http://docs-europe.electrocomponents.com/webdocs/1585/0900766b81585df2.pdf
26-pin D-Sub connector horizontal angled 90deg THT male pitch 2.29x1.98mm pin-PCB-offset 9.4mm
0
26
26
Connector_Dsub
DSUB-26-HD_Male_Horizontal_P2.29x2.54mm_EdgePinOffset9.40mm
26-pin D-Sub connector, horizontal/angled (90 deg), THT-mount, male, pitch 2.29x2.54mm, pin-PCB-offset 9.4mm, see http://docs-europe.electrocomponents.com/webdocs/1585/0900766b81585df2.pdf
26-pin D-Sub connector horizontal angled 90deg THT male pitch 2.29x2.54mm pin-PCB-offset 9.4mm
0
26
26
Connector_Dsub
DSUB-26-HD_Male_Vertical_P2.29x1.98mm_MountingHoles
26-pin D-Sub connector, straight/vertical, THT-mount, male, pitch 2.29x1.98mm, distance of mounting holes 33.3mm, see https://disti-assets.s3.amazonaws.com/tonar/files/datasheets/16730.pdf
26-pin D-Sub connector straight vertical THT male pitch 2.29x1.98mm mounting holes distance 33.3mm
0
28
27
Connector_Dsub
DSUB-37_Female_EdgeMount_P2.77mm
37-pin D-Sub connector, solder-cups edge-mounted, female, x-pin-pitch 2.77mm, distance of mounting holes 63.5mm, see https://disti-assets.s3.amazonaws.com/tonar/files/datasheets/16730.pdf
37-pin D-Sub connector edge mount solder cup female x-pin-pitch 2.77mm mounting holes distance 63.5mm
0
37
37
Connector_Dsub
DSUB-37_Female_Horizontal_P2.77x2.54mm_EdgePinOffset9.40mm
37-pin D-Sub connector, horizontal/angled (90 deg), THT-mount, female, pitch 2.77x2.54mm, pin-PCB-offset 9.4mm, see http://docs-europe.electrocomponents.com/webdocs/1585/0900766b81585df2.pdf
37-pin D-Sub connector horizontal angled 90deg THT female pitch 2.77x2.54mm pin-PCB-offset 9.4mm
0
37
37
Connector_Dsub
DSUB-37_Female_Horizontal_P2.77x2.84mm_EdgePinOffset4.94mm_Housed_MountingHolesOffset7.48mm
37-pin D-Sub connector, horizontal/angled (90 deg), THT-mount, female, pitch 2.77x2.84mm, pin-PCB-offset 4.9399999999999995mm, distance of mounting holes 63.5mm, distance of mounting holes to PCB edge 7.4799999999999995mm, see https://disti-assets.s3.amazonaws.com/tonar/files/datasheets/16730.pdf
37-pin D-Sub connector horizontal angled 90deg THT female pitch 2.77x2.84mm pin-PCB-offset 4.9399999999999995mm mounting-holes-distance 63.5mm mounting-hole-offset 63.5mm
0
39
38
Connector_Dsub
DSUB-37_Female_Horizontal_P2.77x2.84mm_EdgePinOffset7.70mm_Housed_MountingHolesOffset9.12mm
37-pin D-Sub connector, horizontal/angled (90 deg), THT-mount, female, pitch 2.77x2.84mm, pin-PCB-offset 7.699999999999999mm, distance of mounting holes 63.5mm, distance of mounting holes to PCB edge 9.12mm, see https://disti-assets.s3.amazonaws.com/tonar/files/datasheets/16730.pdf
37-pin D-Sub connector horizontal angled 90deg THT female pitch 2.77x2.84mm pin-PCB-offset 7.699999999999999mm mounting-holes-distance 63.5mm mounting-hole-offset 63.5mm
0
39
38
Connector_Dsub
DSUB-37_Female_Horizontal_P2.77x2.84mm_EdgePinOffset9.40mm
37-pin D-Sub connector, horizontal/angled (90 deg), THT-mount, female, pitch 2.77x2.84mm, pin-PCB-offset 9.4mm, see http://docs-europe.electrocomponents.com/webdocs/1585/0900766b81585df2.pdf
37-pin D-Sub connector horizontal angled 90deg THT female pitch 2.77x2.84mm pin-PCB-offset 9.4mm
0
37
37
Connector_Dsub
DSUB-37_Female_Horizontal_P2.77x2.84mm_EdgePinOffset9.90mm_Housed_MountingHolesOffset11.32mm
37-pin D-Sub connector, horizontal/angled (90 deg), THT-mount, female, pitch 2.77x2.84mm, pin-PCB-offset 9.9mm, distance of mounting holes 63.5mm, distance of mounting holes to PCB edge 11.32mm, see https://disti-assets.s3.amazonaws.com/tonar/files/datasheets/16730.pdf
37-pin D-Sub connector horizontal angled 90deg THT female pitch 2.77x2.84mm pin-PCB-offset 9.9mm mounting-holes-distance 63.5mm mounting-hole-offset 63.5mm
0
39
38
Connector_Dsub
DSUB-37_Female_Horizontal_P2.77x2.84mm_EdgePinOffset14.56mm_Housed_MountingHolesOffset8.20mm
37-pin D-Sub connector, horizontal/angled (90 deg), THT-mount, female, pitch 2.77x2.84mm, pin-PCB-offset 14.56mm, distance of mounting holes 63.5mm, distance of mounting holes to PCB edge 8.2mm, see https://disti-assets.s3.amazonaws.com/tonar/files/datasheets/16730.pdf
37-pin D-Sub connector horizontal angled 90deg THT female pitch 2.77x2.84mm pin-PCB-offset 14.56mm mounting-holes-distance 63.5mm mounting-hole-offset 63.5mm
0
39
38
Connector_Dsub
DSUB-37_Female_Horizontal_P2.77x2.84mm_EdgePinOffset14.56mm_Housed_MountingHolesOffset15.98mm
37-pin D-Sub connector, horizontal/angled (90 deg), THT-mount, female, pitch 2.77x2.84mm, pin-PCB-offset 14.56mm, distance of mounting holes 63.5mm, distance of mounting holes to PCB edge 15.979999999999999mm, see https://disti-assets.s3.amazonaws.com/tonar/files/datasheets/16730.pdf
37-pin D-Sub connector horizontal angled 90deg THT female pitch 2.77x2.84mm pin-PCB-offset 14.56mm mounting-holes-distance 63.5mm mounting-hole-offset 63.5mm
0
39
38
Connector_Dsub
DSUB-37_Female_Vertical_P2.77x2.84mm
37-pin D-Sub connector, straight/vertical, THT-mount, female, pitch 2.77x2.84mm, distance of mounting holes 63.5mm, see https://disti-assets.s3.amazonaws.com/tonar/files/datasheets/16730.pdf
37-pin D-Sub connector straight vertical THT female pitch 2.77x2.84mm mounting holes distance 63.5mm
0
37
37
Connector_Dsub
DSUB-37_Female_Vertical_P2.77x2.84mm_MountingHoles
37-pin D-Sub connector, straight/vertical, THT-mount, female, pitch 2.77x2.84mm, distance of mounting holes 63.5mm, see https://disti-assets.s3.amazonaws.com/tonar/files/datasheets/16730.pdf
37-pin D-Sub connector straight vertical THT female pitch 2.77x2.84mm mounting holes distance 63.5mm
0
39
38
Connector_Dsub
DSUB-37_Male_EdgeMount_P2.77mm
37-pin D-Sub connector, solder-cups edge-mounted, male, x-pin-pitch 2.77mm, distance of mounting holes 63.5mm, see https://disti-assets.s3.amazonaws.com/tonar/files/datasheets/16730.pdf
37-pin D-Sub connector edge mount solder cup male x-pin-pitch 2.77mm mounting holes distance 63.5mm
0
37
37
Connector_Dsub
DSUB-37_Male_Horizontal_P2.77x2.54mm_EdgePinOffset9.40mm
37-pin D-Sub connector, horizontal/angled (90 deg), THT-mount, male, pitch 2.77x2.54mm, pin-PCB-offset 9.4mm, see http://docs-europe.electrocomponents.com/webdocs/1585/0900766b81585df2.pdf
37-pin D-Sub connector horizontal angled 90deg THT male pitch 2.77x2.54mm pin-PCB-offset 9.4mm
0
37
37
Connector_Dsub
DSUB-37_Male_Horizontal_P2.77x2.84mm_EdgePinOffset4.94mm_Housed_MountingHolesOffset7.48mm
37-pin D-Sub connector, horizontal/angled (90 deg), THT-mount, male, pitch 2.77x2.84mm, pin-PCB-offset 4.9399999999999995mm, distance of mounting holes 63.5mm, distance of mounting holes to PCB edge 7.4799999999999995mm, see https://disti-assets.s3.amazonaws.com/tonar/files/datasheets/16730.pdf
37-pin D-Sub connector horizontal angled 90deg THT male pitch 2.77x2.84mm pin-PCB-offset 4.9399999999999995mm mounting-holes-distance 63.5mm mounting-hole-offset 63.5mm
0
39
38
Connector_Dsub
DSUB-37_Male_Horizontal_P2.77x2.84mm_EdgePinOffset7.70mm_Housed_MountingHolesOffset9.12mm
37-pin D-Sub connector, horizontal/angled (90 deg), THT-mount, male, pitch 2.77x2.84mm, pin-PCB-offset 7.699999999999999mm, distance of mounting holes 63.5mm, distance of mounting holes to PCB edge 9.12mm, see https://disti-assets.s3.amazonaws.com/tonar/files/datasheets/16730.pdf
37-pin D-Sub connector horizontal angled 90deg THT male pitch 2.77x2.84mm pin-PCB-offset 7.699999999999999mm mounting-holes-distance 63.5mm mounting-hole-offset 63.5mm
0
39
38
Connector_Dsub
DSUB-37_Male_Horizontal_P2.77x2.84mm_EdgePinOffset9.40mm
37-pin D-Sub connector, horizontal/angled (90 deg), THT-mount, male, pitch 2.77x2.84mm, pin-PCB-offset 9.4mm, see http://docs-europe.electrocomponents.com/webdocs/1585/0900766b81585df2.pdf
37-pin D-Sub connector horizontal angled 90deg THT male pitch 2.77x2.84mm pin-PCB-offset 9.4mm
0
37
37
Connector_Dsub
DSUB-37_Male_Horizontal_P2.77x2.84mm_EdgePinOffset9.90mm_Housed_MountingHolesOffset11.32mm
37-pin D-Sub connector, horizontal/angled (90 deg), THT-mount, male, pitch 2.77x2.84mm, pin-PCB-offset 9.9mm, distance of mounting holes 63.5mm, distance of mounting holes to PCB edge 11.32mm, see https://disti-assets.s3.amazonaws.com/tonar/files/datasheets/16730.pdf
37-pin D-Sub connector horizontal angled 90deg THT male pitch 2.77x2.84mm pin-PCB-offset 9.9mm mounting-holes-distance 63.5mm mounting-hole-offset 63.5mm
0
39
38
Connector_Dsub
DSUB-37_Male_Horizontal_P2.77x2.84mm_EdgePinOffset14.56mm_Housed_MountingHolesOffset8.20mm
37-pin D-Sub connector, horizontal/angled (90 deg), THT-mount, male, pitch 2.77x2.84mm, pin-PCB-offset 14.56mm, distance of mounting holes 63.5mm, distance of mounting holes to PCB edge 8.2mm, see https://disti-assets.s3.amazonaws.com/tonar/files/datasheets/16730.pdf
37-pin D-Sub connector horizontal angled 90deg THT male pitch 2.77x2.84mm pin-PCB-offset 14.56mm mounting-holes-distance 63.5mm mounting-hole-offset 63.5mm
0
39
38
Connector_Dsub
DSUB-37_Male_Horizontal_P2.77x2.84mm_EdgePinOffset14.56mm_Housed_MountingHolesOffset15.98mm
37-pin D-Sub connector, horizontal/angled (90 deg), THT-mount, male, pitch 2.77x2.84mm, pin-PCB-offset 14.56mm, distance of mounting holes 63.5mm, distance of mounting holes to PCB edge 15.979999999999999mm, see https://disti-assets.s3.amazonaws.com/tonar/files/datasheets/16730.pdf
37-pin D-Sub connector horizontal angled 90deg THT male pitch 2.77x2.84mm pin-PCB-offset 14.56mm mounting-holes-distance 63.5mm mounting-hole-offset 63.5mm
0
39
38
Connector_Dsub
DSUB-37_Male_Vertical_P2.77x2.84mm
37-pin D-Sub connector, straight/vertical, THT-mount, male, pitch 2.77x2.84mm, distance of mounting holes 63.5mm, see https://disti-assets.s3.amazonaws.com/tonar/files/datasheets/16730.pdf
37-pin D-Sub connector straight vertical THT male pitch 2.77x2.84mm mounting holes distance 63.5mm
0
37
37
Connector_Dsub
DSUB-37_Male_Vertical_P2.77x2.84mm_MountingHoles
37-pin D-Sub connector, straight/vertical, THT-mount, male, pitch 2.77x2.84mm, distance of mounting holes 63.5mm, see https://disti-assets.s3.amazonaws.com/tonar/files/datasheets/16730.pdf
37-pin D-Sub connector straight vertical THT male pitch 2.77x2.84mm mounting holes distance 63.5mm
0
39
38
Connector_Dsub
DSUB-44-HD_Female_Horizontal_P2.29x1.98mm_EdgePinOffset3.03mm_Housed_MountingHolesOffset4.94mm
44-pin D-Sub connector, horizontal/angled (90 deg), THT-mount, female, pitch 2.29x1.98mm, pin-PCB-offset 3.0300000000000002mm, distance of mounting holes 47.1mm, distance of mounting holes to PCB edge 4.9399999999999995mm, see https://disti-assets.s3.amazonaws.com/tonar/files/datasheets/16730.pdf
44-pin D-Sub connector horizontal angled 90deg THT female pitch 2.29x1.98mm pin-PCB-offset 3.0300000000000002mm mounting-holes-distance 47.1mm mounting-hole-offset 47.1mm
0
46
45
Connector_Dsub
DSUB-44-HD_Female_Horizontal_P2.29x1.98mm_EdgePinOffset8.35mm_Housed_MountingHolesOffset10.89mm
44-pin D-Sub connector, horizontal/angled (90 deg), THT-mount, female, pitch 2.29x1.98mm, pin-PCB-offset 8.35mm, distance of mounting holes 47.1mm, distance of mounting holes to PCB edge 10.889999999999999mm, see https://disti-assets.s3.amazonaws.com/tonar/files/datasheets/16730.pdf
44-pin D-Sub connector horizontal angled 90deg THT female pitch 2.29x1.98mm pin-PCB-offset 8.35mm mounting-holes-distance 47.1mm mounting-hole-offset 47.1mm
0
46
45
Connector_Dsub
DSUB-44-HD_Female_Horizontal_P2.29x1.98mm_EdgePinOffset9.40mm
44-pin D-Sub connector, horizontal/angled (90 deg), THT-mount, female, pitch 2.29x1.98mm, pin-PCB-offset 9.4mm, see http://docs-europe.electrocomponents.com/webdocs/1585/0900766b81585df2.pdf
44-pin D-Sub connector horizontal angled 90deg THT female pitch 2.29x1.98mm pin-PCB-offset 9.4mm
0
44
44
Connector_Dsub
DSUB-44-HD_Female_Horizontal_P2.29x2.54mm_EdgePinOffset9.40mm
44-pin D-Sub connector, horizontal/angled (90 deg), THT-mount, female, pitch 2.29x2.54mm, pin-PCB-offset 9.4mm, see http://docs-europe.electrocomponents.com/webdocs/1585/0900766b81585df2.pdf
44-pin D-Sub connector horizontal angled 90deg THT female pitch 2.29x2.54mm pin-PCB-offset 9.4mm
0
44
44
Connector_Dsub
DSUB-44-HD_Female_Vertical_P2.29x1.98mm_MountingHoles
44-pin D-Sub connector, straight/vertical, THT-mount, female, pitch 2.29x1.98mm, distance of mounting holes 47.1mm, see https://disti-assets.s3.amazonaws.com/tonar/files/datasheets/16730.pdf
44-pin D-Sub connector straight vertical THT female pitch 2.29x1.98mm mounting holes distance 47.1mm
0
46
45
Connector_Dsub
DSUB-44-HD_Male_Horizontal_P2.29x1.98mm_EdgePinOffset3.03mm_Housed_MountingHolesOffset4.94mm
44-pin D-Sub connector, horizontal/angled (90 deg), THT-mount, male, pitch 2.29x1.98mm, pin-PCB-offset 3.0300000000000002mm, distance of mounting holes 47.1mm, distance of mounting holes to PCB edge 4.9399999999999995mm, see https://disti-assets.s3.amazonaws.com/tonar/files/datasheets/16730.pdf
44-pin D-Sub connector horizontal angled 90deg THT male pitch 2.29x1.98mm pin-PCB-offset 3.0300000000000002mm mounting-holes-distance 47.1mm mounting-hole-offset 47.1mm
0
46
45
Connector_Dsub
DSUB-44-HD_Male_Horizontal_P2.29x1.98mm_EdgePinOffset8.35mm_Housed_MountingHolesOffset10.89mm
44-pin D-Sub connector, horizontal/angled (90 deg), THT-mount, male, pitch 2.29x1.98mm, pin-PCB-offset 8.35mm, distance of mounting holes 47.1mm, distance of mounting holes to PCB edge 10.889999999999999mm, see https://disti-assets.s3.amazonaws.com/tonar/files/datasheets/16730.pdf
44-pin D-Sub connector horizontal angled 90deg THT male pitch 2.29x1.98mm pin-PCB-offset 8.35mm mounting-holes-distance 47.1mm mounting-hole-offset 47.1mm
0
46
45
Connector_Dsub
DSUB-44-HD_Male_Horizontal_P2.29x1.98mm_EdgePinOffset9.40mm
44-pin D-Sub connector, horizontal/angled (90 deg), THT-mount, male, pitch 2.29x1.98mm, pin-PCB-offset 9.4mm, see http://docs-europe.electrocomponents.com/webdocs/1585/0900766b81585df2.pdf
44-pin D-Sub connector horizontal angled 90deg THT male pitch 2.29x1.98mm pin-PCB-offset 9.4mm
0
44
44
Connector_Dsub
DSUB-44-HD_Male_Horizontal_P2.29x2.54mm_EdgePinOffset9.40mm
44-pin D-Sub connector, horizontal/angled (90 deg), THT-mount, male, pitch 2.29x2.54mm, pin-PCB-offset 9.4mm, see http://docs-europe.electrocomponents.com/webdocs/1585/0900766b81585df2.pdf
44-pin D-Sub connector horizontal angled 90deg THT male pitch 2.29x2.54mm pin-PCB-offset 9.4mm
0
44
44
Connector_Dsub
DSUB-44-HD_Male_Vertical_P2.29x1.98mm_MountingHoles
44-pin D-Sub connector, straight/vertical, THT-mount, male, pitch 2.29x1.98mm, distance of mounting holes 47.1mm, see https://disti-assets.s3.amazonaws.com/tonar/files/datasheets/16730.pdf
44-pin D-Sub connector straight vertical THT male pitch 2.29x1.98mm mounting holes distance 47.1mm
0
46
45
Connector_Dsub
DSUB-62-HD_Female_Horizontal_P2.41x1.98mm_EdgePinOffset3.03mm_Housed_MountingHolesOffset4.94mm
62-pin D-Sub connector, horizontal/angled (90 deg), THT-mount, female, pitch 2.41x1.98mm, pin-PCB-offset 3.0300000000000002mm, distance of mounting holes 63.5mm, distance of mounting holes to PCB edge 4.9399999999999995mm, see https://disti-assets.s3.amazonaws.com/tonar/files/datasheets/16730.pdf
62-pin D-Sub connector horizontal angled 90deg THT female pitch 2.41x1.98mm pin-PCB-offset 3.0300000000000002mm mounting-holes-distance 63.5mm mounting-hole-offset 63.5mm
0
64
63
Connector_Dsub
DSUB-62-HD_Female_Horizontal_P2.41x1.98mm_EdgePinOffset8.35mm_Housed_MountingHolesOffset10.89mm
62-pin D-Sub connector, horizontal/angled (90 deg), THT-mount, female, pitch 2.41x1.98mm, pin-PCB-offset 8.35mm, distance of mounting holes 63.5mm, distance of mounting holes to PCB edge 10.889999999999999mm, see https://disti-assets.s3.amazonaws.com/tonar/files/datasheets/16730.pdf
62-pin D-Sub connector horizontal angled 90deg THT female pitch 2.41x1.98mm pin-PCB-offset 8.35mm mounting-holes-distance 63.5mm mounting-hole-offset 63.5mm
0
64
63
Connector_Dsub
DSUB-62-HD_Female_Horizontal_P2.41x1.98mm_EdgePinOffset9.40mm
62-pin D-Sub connector, horizontal/angled (90 deg), THT-mount, female, pitch 2.41x1.98mm, pin-PCB-offset 9.4mm, see http://docs-europe.electrocomponents.com/webdocs/1585/0900766b81585df2.pdf
62-pin D-Sub connector horizontal angled 90deg THT female pitch 2.41x1.98mm pin-PCB-offset 9.4mm
0
62
62
Connector_Dsub
DSUB-62-HD_Female_Horizontal_P2.41x2.54mm_EdgePinOffset9.40mm
62-pin D-Sub connector, horizontal/angled (90 deg), THT-mount, female, pitch 2.41x2.54mm, pin-PCB-offset 9.4mm, see http://docs-europe.electrocomponents.com/webdocs/1585/0900766b81585df2.pdf
62-pin D-Sub connector horizontal angled 90deg THT female pitch 2.41x2.54mm pin-PCB-offset 9.4mm
0
62
62
Connector_Dsub
DSUB-62-HD_Female_Vertical_P2.41x1.98mm_MountingHoles
62-pin D-Sub connector, straight/vertical, THT-mount, female, pitch 2.41x1.98mm, distance of mounting holes 63.5mm, see https://disti-assets.s3.amazonaws.com/tonar/files/datasheets/16730.pdf
62-pin D-Sub connector straight vertical THT female pitch 2.41x1.98mm mounting holes distance 63.5mm
0
64
63
Connector_Dsub
DSUB-62-HD_Male_Horizontal_P2.41x1.98mm_EdgePinOffset3.03mm_Housed_MountingHolesOffset4.94mm
62-pin D-Sub connector, horizontal/angled (90 deg), THT-mount, male, pitch 2.41x1.98mm, pin-PCB-offset 3.0300000000000002mm, distance of mounting holes 63.5mm, distance of mounting holes to PCB edge 4.9399999999999995mm, see https://disti-assets.s3.amazonaws.com/tonar/files/datasheets/16730.pdf
62-pin D-Sub connector horizontal angled 90deg THT male pitch 2.41x1.98mm pin-PCB-offset 3.0300000000000002mm mounting-holes-distance 63.5mm mounting-hole-offset 63.5mm
0
64
63
Connector_Dsub
DSUB-62-HD_Male_Horizontal_P2.41x1.98mm_EdgePinOffset8.35mm_Housed_MountingHolesOffset10.89mm
62-pin D-Sub connector, horizontal/angled (90 deg), THT-mount, male, pitch 2.41x1.98mm, pin-PCB-offset 8.35mm, distance of mounting holes 63.5mm, distance of mounting holes to PCB edge 10.889999999999999mm, see https://disti-assets.s3.amazonaws.com/tonar/files/datasheets/16730.pdf
62-pin D-Sub connector horizontal angled 90deg THT male pitch 2.41x1.98mm pin-PCB-offset 8.35mm mounting-holes-distance 63.5mm mounting-hole-offset 63.5mm
0
64
63
Connector_Dsub
DSUB-62-HD_Male_Horizontal_P2.41x1.98mm_EdgePinOffset9.40mm
62-pin D-Sub connector, horizontal/angled (90 deg), THT-mount, male, pitch 2.41x1.98mm, pin-PCB-offset 9.4mm, see http://docs-europe.electrocomponents.com/webdocs/1585/0900766b81585df2.pdf
62-pin D-Sub connector horizontal angled 90deg THT male pitch 2.41x1.98mm pin-PCB-offset 9.4mm
0
62
62
Connector_Dsub
DSUB-62-HD_Male_Horizontal_P2.41x2.54mm_EdgePinOffset9.40mm
62-pin D-Sub connector, horizontal/angled (90 deg), THT-mount, male, pitch 2.41x2.54mm, pin-PCB-offset 9.4mm, see http://docs-europe.electrocomponents.com/webdocs/1585/0900766b81585df2.pdf
62-pin D-Sub connector horizontal angled 90deg THT male pitch 2.41x2.54mm pin-PCB-offset 9.4mm
0
62
62
Connector_Dsub
DSUB-62-HD_Male_Vertical_P2.41x1.98mm_MountingHoles
62-pin D-Sub connector, straight/vertical, THT-mount, male, pitch 2.41x1.98mm, distance of mounting holes 63.5mm, see https://disti-assets.s3.amazonaws.com/tonar/files/datasheets/16730.pdf
62-pin D-Sub connector straight vertical THT male pitch 2.41x1.98mm mounting holes distance 63.5mm
0
64
63
